{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"POWERLINKV5_20160108113846"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"14.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"POWERLINK"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2010]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2010-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2011-01-01"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":1405}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":164}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":1569}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2010 Version: 5"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":53},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":109},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":2},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":142},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":1405},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":1405}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":1711},null,{"$f":"SUM($P$46:$P$65)","v":1405}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation",null,null,"2016-01-08T11:38:46"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":8243,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[1,"POWERLINKV5_20151103074515","2010-01-02T19:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED",null,"System Normal Constraint","PLANNED",0]
[2,"POWERLINKV5_20151103074515","2010-01-02T19:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3,"POWERLINKV5_20151103074515","2010-01-03T09:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.87," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4,"POWERLINKV5_20151103074515","2010-01-03T09:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.58," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5,"POWERLINKV5_20151103074515","2010-01-03T09:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.44," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6,"POWERLINKV5_20151103074515","2010-01-03T10:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.13," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7,"POWERLINKV5_20151103074515","2010-01-03T10:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.02," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8,"POWERLINKV5_20151103074515","2010-01-03T10:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.53," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[9,"POWERLINKV5_20151103074515","2010-01-03T10:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.18," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[10,"POWERLINKV5_20151103074515","2010-01-03T10:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.38," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[11,"POWERLINKV5_20151103074515","2010-01-03T10:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.24," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[12,"POWERLINKV5_20151103074515","2010-01-03T11:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[13,"POWERLINKV5_20151103074515","2010-01-03T11:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,233.16," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[14,"POWERLINKV5_20151103074515","2010-01-03T11:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.91," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[15,"POWERLINKV5_20151103074515","2010-01-03T11:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.37," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[16,"POWERLINKV5_20151103074515","2010-01-03T11:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.96," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[17,"POWERLINKV5_20151103074515","2010-01-03T11:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.96," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[18,"POWERLINKV5_20151103074515","2010-01-03T11:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.3," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[19,"POWERLINKV5_20151103074515","2010-01-03T11:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.44," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[20,"POWERLINKV5_20151103074515","2010-01-03T11:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[21,"POWERLINKV5_20151103074515","2010-01-03T11:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[22,"POWERLINKV5_20151103074515","2010-01-03T11:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.91," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[23,"POWERLINKV5_20151103074515","2010-01-03T11:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.88," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[24,"POWERLINKV5_20151103074515","2010-01-03T12:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.87," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[25,"POWERLINKV5_20151103074515","2010-01-03T12:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.44," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[26,"POWERLINKV5_20151103074515","2010-01-03T12:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.64," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[27,"POWERLINKV5_20151103074515","2010-01-03T12:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.61," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[28,"POWERLINKV5_20151103074515","2010-01-03T12:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.86," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[29,"POWERLINKV5_20151103074515","2010-01-03T12:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,18.87," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[30,"POWERLINKV5_20151103074515","2010-01-03T12:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[31,"POWERLINKV5_20151103074515","2010-01-03T12:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.84," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[32,"POWERLINKV5_20151103074515","2010-01-03T13:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[33,"POWERLINKV5_20151103074515","2010-01-03T13:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.19," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[34,"POWERLINKV5_20151103074515","2010-01-03T13:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.6," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[35,"POWERLINKV5_20151103074515","2010-01-03T13:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,18.68," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[36,"POWERLINKV5_20151103074515","2010-01-03T13:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.72," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[37,"POWERLINKV5_20151103074515","2010-01-03T13:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.14," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[38,"POWERLINKV5_20151103074515","2010-01-03T13:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.15," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[39,"POWERLINKV5_20151103074515","2010-01-03T13:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.37," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[40,"POWERLINKV5_20151103074515","2010-01-03T13:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.14," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[41,"POWERLINKV5_20151103074515","2010-01-03T13:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,18.690000000000001," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[42,"POWERLINKV5_20151103074515","2010-01-03T13:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,18.48," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[43,"POWERLINKV5_20151103074515","2010-01-03T14:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.36," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[44,"POWERLINKV5_20151103074515","2010-01-03T14:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.37," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[45,"POWERLINKV5_20151103074515","2010-01-03T14:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.35," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[46,"POWERLINKV5_20151103074515","2010-01-03T14:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.92," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[47,"POWERLINKV5_20151103074515","2010-01-03T14:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.18," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[48,"POWERLINKV5_20151103074515","2010-01-03T14:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[49,"POWERLINKV5_20151103074515","2010-01-03T14:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,18.75," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[50,"POWERLINKV5_20151103074515","2010-01-03T14:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,19.12," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[51,"POWERLINKV5_20151103074515","2010-01-03T14:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.9," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[52,"POWERLINKV5_20151103074515","2010-01-03T14:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.36," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[53,"POWERLINKV5_20151103074515","2010-01-03T14:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.13," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[54,"POWERLINKV5_20151103074515","2010-01-03T15:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.68," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[55,"POWERLINKV5_20151103074515","2010-01-03T15:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.69," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[56,"POWERLINKV5_20151103074515","2010-01-03T15:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[57,"POWERLINKV5_20151103074515","2010-01-03T15:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.22," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[58,"POWERLINKV5_20151103074515","2010-01-03T15:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[59,"POWERLINKV5_20151103074515","2010-01-03T15:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.27," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[60,"POWERLINKV5_20151103074515","2010-01-03T15:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,19.7," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[61,"POWERLINKV5_20151103074515","2010-01-03T15:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,19.7," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[62,"POWERLINKV5_20151103074515","2010-01-03T16:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,19.510000000000002," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[63,"POWERLINKV5_20151103074515","2010-01-03T16:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.36," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[64,"POWERLINKV5_20151103074515","2010-01-03T16:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.27," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[65,"POWERLINKV5_20151103074515","2010-01-03T16:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.22," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[66,"POWERLINKV5_20151103074515","2010-01-03T16:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[67,"POWERLINKV5_20151103074515","2010-01-03T16:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,19.670000000000002," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[68,"POWERLINKV5_20151103074515","2010-01-03T16:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,27.14," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[69,"POWERLINKV5_20151103074515","2010-01-03T16:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.24," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[70,"POWERLINKV5_20151103074515","2010-01-03T16:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.25," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[71,"POWERLINKV5_20151103074515","2010-01-03T16:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.46," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[72,"POWERLINKV5_20151103074515","2010-01-03T18:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.08," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[73,"POWERLINKV5_20151103074515","2010-01-03T18:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.02," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[74,"POWERLINKV5_20151103074515","2010-01-03T18:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.41," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[75,"POWERLINKV5_20151103074515","2010-01-03T18:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.42," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[76,"POWERLINKV5_20151103074515","2010-01-03T19:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.5," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[77,"POWERLINKV5_20151103074515","2010-01-04T09:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.94," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[78,"POWERLINKV5_20151103074515","2010-01-04T09:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[79,"POWERLINKV5_20151103074515","2010-01-04T09:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.02," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[80,"POWERLINKV5_20151103074515","2010-01-04T09:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.65," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[81,"POWERLINKV5_20151103074515","2010-01-04T09:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.44," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[82,"POWERLINKV5_20151103074515","2010-01-04T09:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.01," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[83,"POWERLINKV5_20151103074515","2010-01-04T09:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.2," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[84,"POWERLINKV5_20151103074515","2010-01-04T09:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.46," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[85,"POWERLINKV5_20151103074515","2010-01-04T10:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.31," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[86,"POWERLINKV5_20151103074515","2010-01-04T11:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[87,"POWERLINKV5_20151103074515","2010-01-04T11:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[88,"POWERLINKV5_20151103074515","2010-01-04T11:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.27," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[89,"POWERLINKV5_20151103074515","2010-01-04T12:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.38," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[90,"POWERLINKV5_20151103074515","2010-01-04T12:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.58," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[91,"POWERLINKV5_20151103074515","2010-01-04T12:10:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[92,"POWERLINKV5_20151103074515","2010-01-04T13:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[93,"POWERLINKV5_20151103074515","2010-01-04T15:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.24," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[94,"POWERLINKV5_20151103074515","2010-01-04T15:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.54," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[95,"POWERLINKV5_20151103074515","2010-01-04T15:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.58," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[96,"POWERLINKV5_20151103074515","2010-01-04T15:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[97,"POWERLINKV5_20151103074515","2010-01-04T15:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[98,"POWERLINKV5_20151103074515","2010-01-04T15:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[99,"POWERLINKV5_20151103074515","2010-01-04T15:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[100,"POWERLINKV5_20151103074515","2010-01-04T15:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.96," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[101,"POWERLINKV5_20151103074515","2010-01-04T16:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.06," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[102,"POWERLINKV5_20151103074515","2010-01-04T16:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.16," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[103,"POWERLINKV5_20151103074515","2010-01-04T16:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[104,"POWERLINKV5_20151103074515","2010-01-04T16:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.96," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[105,"POWERLINKV5_20151103074515","2010-01-04T16:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[106,"POWERLINKV5_20151103074515","2010-01-04T16:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.62," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[107,"POWERLINKV5_20151103074515","2010-01-04T16:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.25," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[108,"POWERLINKV5_20151103074515","2010-01-04T16:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.04," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[109,"POWERLINKV5_20151103074515","2010-01-04T16:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.06," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[110,"POWERLINKV5_20151103074515","2010-01-04T16:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.8," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[111,"POWERLINKV5_20151103074515","2010-01-04T17:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.06," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[112,"POWERLINKV5_20151103074515","2010-01-09T10:30:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,22.64,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[113,"POWERLINKV5_20151103074515","2010-01-09T10:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,17.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[114,"POWERLINKV5_20151103074515","2010-01-09T10:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,16.54,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[115,"POWERLINKV5_20151103074515","2010-01-09T10:45:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,27.51,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[116,"POWERLINKV5_20151103074515","2010-01-09T10:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,22.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[117,"POWERLINKV5_20151103074515","2010-01-09T10:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,21.73,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[118,"POWERLINKV5_20151103074515","2010-01-09T11:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,21.15,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[119,"POWERLINKV5_20151103074515","2010-01-09T11:20:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,11.48,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[120,"POWERLINKV5_20151103074515","2010-01-09T11:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,12.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[121,"POWERLINKV5_20151103074515","2010-01-09T11:30:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,12.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[122,"POWERLINKV5_20151103074515","2010-01-09T11:40:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,10.81,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[123,"POWERLINKV5_20151103074515","2010-01-09T11:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,16.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[124,"POWERLINKV5_20151103074515","2010-01-09T11:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,18.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[125,"POWERLINKV5_20151103074515","2010-01-09T12:00:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,41.55,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[126,"POWERLINKV5_20151103074515","2010-01-09T14:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,12.51,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[127,"POWERLINKV5_20151103074515","2010-01-09T14:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,19.14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[128,"POWERLINKV5_20151103074515","2010-01-09T14:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,14.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[129,"POWERLINKV5_20151103074515","2010-01-09T14:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,24.68,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[130,"POWERLINKV5_20151103074515","2010-01-09T14:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,23.63,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[131,"POWERLINKV5_20151103074515","2010-01-09T14:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,20.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[132,"POWERLINKV5_20151103074515","2010-01-09T14:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,21.45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[133,"POWERLINKV5_20151103074515","2010-01-09T14:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,19.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[134,"POWERLINKV5_20151103074515","2010-01-09T14:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,21.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[135,"POWERLINKV5_20151103074515","2010-01-09T14:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,18.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[136,"POWERLINKV5_20151103074515","2010-01-09T15:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,19.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[137,"POWERLINKV5_20151103074515","2010-01-09T15:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,27.19,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[138,"POWERLINKV5_20151103074515","2010-01-09T15:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,26.12,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[139,"POWERLINKV5_20151103074515","2010-01-09T15:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,28.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[140,"POWERLINKV5_20151103074515","2010-01-09T15:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,49.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[141,"POWERLINKV5_20151103074515","2010-01-09T15:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,47.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[142,"POWERLINKV5_20151103074515","2010-01-09T15:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,51.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[143,"POWERLINKV5_20151103074515","2010-01-09T15:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,64.760000000000005,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[144,"POWERLINKV5_20151103074515","2010-01-09T16:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,46.82,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[145,"POWERLINKV5_20151103074515","2010-01-09T16:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,64.760000000000005,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[146,"POWERLINKV5_20151103074515","2010-01-09T16:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,41.66,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[147,"POWERLINKV5_20151103074515","2010-01-09T16:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,23.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[148,"POWERLINKV5_20151103074515","2010-01-09T17:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,56.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[149,"POWERLINKV5_20151103074515","2010-01-09T17:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-01-30",1,57.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[150,"POWERLINKV5_20151103074515","2010-01-09T17:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,48.52,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[151,"POWERLINKV5_20151103074515","2010-01-09T17:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,50.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[152,"POWERLINKV5_20151103074515","2010-01-09T17:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,49.83,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[153,"POWERLINKV5_20151103074515","2010-01-09T17:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,49.82,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[154,"POWERLINKV5_20151103074515","2010-01-09T17:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,23.37,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[155,"POWERLINKV5_20151103074515","2010-01-09T17:40:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,36.11,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[156,"POWERLINKV5_20151103074515","2010-01-09T17:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,20.69,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[157,"POWERLINKV5_20151103074515","2010-01-09T17:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,22.07,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[158,"POWERLINKV5_20151103074515","2010-01-09T17:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,25.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[159,"POWERLINKV5_20151103074515","2010-01-09T18:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,23.79,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[160,"POWERLINKV5_20151103074515","2010-01-09T18:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,26.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[161,"POWERLINKV5_20151103074515","2010-01-09T18:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,28.66,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[162,"POWERLINKV5_20151103074515","2010-01-09T18:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,25.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[163,"POWERLINKV5_20151103074515","2010-01-09T18:20:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,37.44,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[164,"POWERLINKV5_20151103074515","2010-01-09T18:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,21.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[165,"POWERLINKV5_20151103074515","2010-01-09T18:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,22.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[166,"POWERLINKV5_20151103074515","2010-01-09T18:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,25.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[167,"POWERLINKV5_20151103074515","2010-01-09T18:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,20.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[168,"POWERLINKV5_20151103074515","2010-01-09T18:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,18.93,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[169,"POWERLINKV5_20151103074515","2010-01-09T18:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,17.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[170,"POWERLINKV5_20151103074515","2010-01-09T19:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,10.14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[171,"POWERLINKV5_20151103074515","2010-01-09T19:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,21.83,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[172,"POWERLINKV5_20151103074515","2010-01-09T19:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,21.05,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[173,"POWERLINKV5_20151103074515","2010-01-09T19:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,20.95,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[174,"POWERLINKV5_20151103074515","2010-01-10T11:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,10.19,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[175,"POWERLINKV5_20151103074515","2010-01-10T11:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,11.72,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[176,"POWERLINKV5_20151103074515","2010-01-10T11:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-01-30",1,10.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[177,"POWERLINKV5_20151103074515","2010-01-12T05:40:00","Q>N_NIL_8L_8M","Q-NIL_8L_8M","2008-01-18",1,16.059999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[178,"POWERLINKV5_20151103074515","2010-01-16T19:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.78," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[179,"POWERLINKV5_20151103074515","2010-01-16T19:35:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,493.7,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[180,"POWERLINKV5_20151103074515","2010-01-16T19:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,16.010000000000002," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[181,"POWERLINKV5_20151103074515","2010-01-16T19:40:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,488.17,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[182,"POWERLINKV5_20151103074515","2010-01-16T19:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.51," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[183,"POWERLINKV5_20151103074515","2010-01-16T19:45:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,493.6,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[184,"POWERLINKV5_20151103074515","2010-01-16T19:50:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,493.94,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[185,"POWERLINKV5_20151103074515","2010-01-16T19:55:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,200000,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[186,"POWERLINKV5_20151103074515","2010-01-16T19:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,15.97," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[187,"POWERLINKV5_20151103074515","2010-01-16T19:55:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[188,"POWERLINKV5_20151103074515","2010-01-16T19:55:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[189,"POWERLINKV5_20151103074515","2010-01-16T20:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,16.04," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[190,"POWERLINKV5_20151103074515","2010-01-16T20:00:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[191,"POWERLINKV5_20151103074515","2010-01-16T20:00:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[192,"POWERLINKV5_20151103074515","2010-01-16T20:05:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[193,"POWERLINKV5_20151103074515","2010-01-16T20:10:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,496.22,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[194,"POWERLINKV5_20151103074515","2010-01-16T20:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,16.34," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[195,"POWERLINKV5_20151103074515","2010-01-16T20:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.24," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[196,"POWERLINKV5_20151103074515","2010-01-16T20:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.02," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[197,"POWERLINKV5_20151103074515","2010-01-17T05:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.42," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[198,"POWERLINKV5_20151103074515","2010-01-17T05:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[199,"POWERLINKV5_20151103074515","2010-01-17T05:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[200,"POWERLINKV5_20151103074515","2010-01-17T05:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.47," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[201,"POWERLINKV5_20151103074515","2010-01-17T05:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[202,"POWERLINKV5_20151103074515","2010-01-17T07:35:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,459.69,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[203,"POWERLINKV5_20151103074515","2010-01-17T07:40:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[204,"POWERLINKV5_20151103074515","2010-01-17T07:45:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[205,"POWERLINKV5_20151103074515","2010-01-17T08:40:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[206,"POWERLINKV5_20151103074515","2010-01-17T08:45:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[207,"POWERLINKV5_20151103074515","2010-01-17T12:20:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,1783.86,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[208,"POWERLINKV5_20151103074515","2010-01-17T12:40:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[209,"POWERLINKV5_20151103074515","2010-01-17T12:45:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[210,"POWERLINKV5_20151103074515","2010-01-17T12:45:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[211,"POWERLINKV5_20151103074515","2010-01-17T12:50:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[212,"POWERLINKV5_20151103074515","2010-01-17T12:50:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[213,"POWERLINKV5_20151103074515","2010-01-17T12:55:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[214,"POWERLINKV5_20151103074515","2010-01-17T13:00:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[215,"POWERLINKV5_20151103074515","2010-01-17T13:00:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[216,"POWERLINKV5_20151103074515","2010-01-17T13:05:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[217,"POWERLINKV5_20151103074515","2010-01-17T13:10:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[218,"POWERLINKV5_20151103074515","2010-01-17T13:15:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,76698.05,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[219,"POWERLINKV5_20151103074515","2010-01-17T13:15:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[220,"POWERLINKV5_20151103074515","2010-01-17T13:20:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,76696.75,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[221,"POWERLINKV5_20151103074515","2010-01-17T13:20:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[222,"POWERLINKV5_20151103074515","2010-01-17T13:25:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[223,"POWERLINKV5_20151103074515","2010-01-17T13:30:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[224,"POWERLINKV5_20151103074515","2010-01-17T13:35:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[225,"POWERLINKV5_20151103074515","2010-01-17T13:40:00","Q^FNQ_-030","Q-H13RS_SVC","2009-01-17",1,200000,"Nominated offset = -30MW, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","OUTAGE","OTHER","Ross SVC","REGULATED","INCLUDED","Unplanned outage of H013 Ross SVC following a fault, refer to AFW Q10S/0211.","UNPLANNED",1]
[226,"POWERLINKV5_20151103074515","2010-01-17T17:35:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,1762.93,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[227,"POWERLINKV5_20151103074515","2010-01-17T17:45:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,1759.71,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[228,"POWERLINKV5_20151103074515","2010-01-17T17:50:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,1757.81,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[229,"POWERLINKV5_20151103074515","2010-01-17T17:55:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,200000,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[230,"POWERLINKV5_20151103074515","2010-01-17T17:55:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[231,"POWERLINKV5_20151103074515","2010-01-17T17:55:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[232,"POWERLINKV5_20151103074515","2010-01-17T17:55:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[233,"POWERLINKV5_20151103074515","2010-01-17T18:00:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,200000,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[234,"POWERLINKV5_20151103074515","2010-01-17T18:00:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[235,"POWERLINKV5_20151103074515","2010-01-17T18:00:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[236,"POWERLINKV5_20151103074515","2010-01-17T18:00:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[237,"POWERLINKV5_20151103074515","2010-01-17T18:05:00","Q^NIL_FNQ","Q-NIL","2009-01-17",1,200000,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[238,"POWERLINKV5_20151103074515","2010-01-17T18:05:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[239,"POWERLINKV5_20151103074515","2010-01-17T18:05:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[240,"POWERLINKV5_20151103074515","2010-01-17T18:05:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[241,"POWERLINKV5_20151103074515","2010-01-17T18:10:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,4216.3599999999997,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[242,"POWERLINKV5_20151103074515","2010-01-17T18:15:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,4226.91,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[243,"POWERLINKV5_20151103074515","2010-01-17T18:20:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,4226.91,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[244,"POWERLINKV5_20151103074515","2010-01-17T18:25:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,13516.09,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[245,"POWERLINKV5_20151103074515","2010-01-17T18:30:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,13516.13,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[246,"POWERLINKV5_20151103074515","2010-01-17T18:55:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,3130.03,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[247,"POWERLINKV5_20151103074515","2010-01-17T19:00:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,3130.03,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[248,"POWERLINKV5_20151103074515","2010-01-17T19:05:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-01-03",2,4226.91,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[249,"POWERLINKV5_20151103074515","2010-01-17T19:15:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[250,"POWERLINKV5_20151103074515","2010-01-17T19:20:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[251,"POWERLINKV5_20151103074515","2010-01-17T19:25:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[252,"POWERLINKV5_20151103074515","2010-01-17T19:30:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[253,"POWERLINKV5_20151103074515","2010-01-18T08:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.55," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[254,"POWERLINKV5_20151103074515","2010-01-18T08:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11033.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[255,"POWERLINKV5_20151103074515","2010-01-18T08:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,27.16," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[256,"POWERLINKV5_20151103074515","2010-01-18T08:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.54," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[257,"POWERLINKV5_20151103074515","2010-01-18T09:15:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[258,"POWERLINKV5_20151103074515","2010-01-18T09:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.65," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[259,"POWERLINKV5_20151103074515","2010-01-18T09:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,15.48," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[260,"POWERLINKV5_20151103074515","2010-01-18T09:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,15.64," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[261,"POWERLINKV5_20151103074515","2010-01-18T09:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,15.12," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[262,"POWERLINKV5_20151103074515","2010-01-18T09:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,27.41," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[263,"POWERLINKV5_20151103074515","2010-01-18T09:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,236.78," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[264,"POWERLINKV5_20151103074515","2010-01-18T09:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,237.93," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[265,"POWERLINKV5_20151103074515","2010-01-18T09:55:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,237.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[266,"POWERLINKV5_20151103074515","2010-01-18T10:00:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,239.61," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[267,"POWERLINKV5_20151103074515","2010-01-18T10:05:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,14.4," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[268,"POWERLINKV5_20151103074515","2010-01-18T15:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,200000,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[269,"POWERLINKV5_20151103074515","2010-01-18T15:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,200000,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[270,"POWERLINKV5_20151103074515","2010-01-18T15:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,200000,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[271,"POWERLINKV5_20151103074515","2010-01-18T15:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,200000,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[272,"POWERLINKV5_20151103074515","2010-01-18T19:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[273,"POWERLINKV5_20151103074515","2010-01-18T19:20:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[274,"POWERLINKV5_20151103074515","2010-01-18T19:25:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[275,"POWERLINKV5_20151103074515","2010-01-19T11:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[276,"POWERLINKV5_20151103074515","2010-01-19T11:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[277,"POWERLINKV5_20151103074515","2010-01-19T11:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[278,"POWERLINKV5_20151103074515","2010-01-19T11:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[279,"POWERLINKV5_20151103074515","2010-01-19T12:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[280,"POWERLINKV5_20151103074515","2010-01-19T12:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[281,"POWERLINKV5_20151103074515","2010-01-19T12:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.6500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[282,"POWERLINKV5_20151103074515","2010-01-19T12:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[283,"POWERLINKV5_20151103074515","2010-01-19T12:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[284,"POWERLINKV5_20151103074515","2010-01-19T12:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.6099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[285,"POWERLINKV5_20151103074515","2010-01-19T12:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[286,"POWERLINKV5_20151103074515","2010-01-19T12:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[287,"POWERLINKV5_20151103074515","2010-01-19T12:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[288,"POWERLINKV5_20151103074515","2010-01-19T12:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.5999999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[289,"POWERLINKV5_20151103074515","2010-01-19T12:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[290,"POWERLINKV5_20151103074515","2010-01-19T12:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[291,"POWERLINKV5_20151103074515","2010-01-19T13:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[292,"POWERLINKV5_20151103074515","2010-01-19T13:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.1500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[293,"POWERLINKV5_20151103074515","2010-01-19T13:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[294,"POWERLINKV5_20151103074515","2010-01-19T13:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[295,"POWERLINKV5_20151103074515","2010-01-19T13:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[296,"POWERLINKV5_20151103074515","2010-01-19T13:20:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,13.08," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[297,"POWERLINKV5_20151103074515","2010-01-19T13:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[298,"POWERLINKV5_20151103074515","2010-01-19T13:25:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,12.86," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[299,"POWERLINKV5_20151103074515","2010-01-19T13:30:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.94," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[300,"POWERLINKV5_20151103074515","2010-01-19T13:35:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.15," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[301,"POWERLINKV5_20151103074515","2010-01-19T13:45:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.08," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[302,"POWERLINKV5_20151103074515","2010-01-19T13:50:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,11.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[303,"POWERLINKV5_20151103074515","2010-01-19T17:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[304,"POWERLINKV5_20151103074515","2010-01-19T17:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.37,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[305,"POWERLINKV5_20151103074515","2010-01-19T17:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[306,"POWERLINKV5_20151103074515","2010-01-19T17:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[307,"POWERLINKV5_20151103074515","2010-01-19T18:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[308,"POWERLINKV5_20151103074515","2010-01-19T18:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[309,"POWERLINKV5_20151103074515","2010-01-19T18:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[310,"POWERLINKV5_20151103074515","2010-01-19T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[311,"POWERLINKV5_20151103074515","2010-01-19T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[312,"POWERLINKV5_20151103074515","2010-01-19T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[313,"POWERLINKV5_20151103074515","2010-01-19T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[314,"POWERLINKV5_20151103074515","2010-01-19T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[315,"POWERLINKV5_20151103074515","2010-01-19T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[316,"POWERLINKV5_20151103074515","2010-01-19T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[317,"POWERLINKV5_20151103074515","2010-01-19T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[318,"POWERLINKV5_20151103074515","2010-01-19T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.37,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[319,"POWERLINKV5_20151103074515","2010-01-19T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[320,"POWERLINKV5_20151103074515","2010-01-19T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[321,"POWERLINKV5_20151103074515","2010-01-19T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[322,"POWERLINKV5_20151103074515","2010-01-19T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[323,"POWERLINKV5_20151103074515","2010-01-19T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[324,"POWERLINKV5_20151103074515","2010-01-19T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[325,"POWERLINKV5_20151103074515","2010-01-19T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[326,"POWERLINKV5_20151103074515","2010-01-19T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[327,"POWERLINKV5_20151103074515","2010-01-19T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[328,"POWERLINKV5_20151103074515","2010-01-19T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[329,"POWERLINKV5_20151103074515","2010-01-20","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[330,"POWERLINKV5_20151103074515","2010-01-20T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[331,"POWERLINKV5_20151103074515","2010-01-20T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[332,"POWERLINKV5_20151103074515","2010-01-20T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[333,"POWERLINKV5_20151103074515","2010-01-20T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[334,"POWERLINKV5_20151103074515","2010-01-20T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.26,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[335,"POWERLINKV5_20151103074515","2010-01-20T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[336,"POWERLINKV5_20151103074515","2010-01-20T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[337,"POWERLINKV5_20151103074515","2010-01-20T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[338,"POWERLINKV5_20151103074515","2010-01-20T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.82,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[339,"POWERLINKV5_20151103074515","2010-01-20T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[340,"POWERLINKV5_20151103074515","2010-01-20T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[341,"POWERLINKV5_20151103074515","2010-01-20T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[342,"POWERLINKV5_20151103074515","2010-01-20T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[343,"POWERLINKV5_20151103074515","2010-01-20T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[344,"POWERLINKV5_20151103074515","2010-01-20T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[345,"POWERLINKV5_20151103074515","2010-01-20T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[346,"POWERLINKV5_20151103074515","2010-01-20T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[347,"POWERLINKV5_20151103074515","2010-01-20T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[348,"POWERLINKV5_20151103074515","2010-01-20T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[349,"POWERLINKV5_20151103074515","2010-01-20T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[350,"POWERLINKV5_20151103074515","2010-01-20T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[351,"POWERLINKV5_20151103074515","2010-01-20T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[352,"POWERLINKV5_20151103074515","2010-01-20T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[353,"POWERLINKV5_20151103074515","2010-01-20T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[354,"POWERLINKV5_20151103074515","2010-01-20T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[355,"POWERLINKV5_20151103074515","2010-01-20T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[356,"POWERLINKV5_20151103074515","2010-01-20T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[357,"POWERLINKV5_20151103074515","2010-01-20T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[358,"POWERLINKV5_20151103074515","2010-01-20T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[359,"POWERLINKV5_20151103074515","2010-01-20T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[360,"POWERLINKV5_20151103074515","2010-01-20T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.82,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[361,"POWERLINKV5_20151103074515","2010-01-20T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[362,"POWERLINKV5_20151103074515","2010-01-20T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[363,"POWERLINKV5_20151103074515","2010-01-20T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[364,"POWERLINKV5_20151103074515","2010-01-20T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[365,"POWERLINKV5_20151103074515","2010-01-20T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[366,"POWERLINKV5_20151103074515","2010-01-20T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[367,"POWERLINKV5_20151103074515","2010-01-20T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[368,"POWERLINKV5_20151103074515","2010-01-20T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[369,"POWERLINKV5_20151103074515","2010-01-20T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[370,"POWERLINKV5_20151103074515","2010-01-20T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1008.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[371,"POWERLINKV5_20151103074515","2010-01-20T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1008.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[372,"POWERLINKV5_20151103074515","2010-01-20T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[373,"POWERLINKV5_20151103074515","2010-01-20T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[374,"POWERLINKV5_20151103074515","2010-01-20T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[375,"POWERLINKV5_20151103074515","2010-01-20T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[376,"POWERLINKV5_20151103074515","2010-01-20T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[377,"POWERLINKV5_20151103074515","2010-01-20T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[378,"POWERLINKV5_20151103074515","2010-01-20T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[379,"POWERLINKV5_20151103074515","2010-01-20T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[380,"POWERLINKV5_20151103074515","2010-01-20T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[381,"POWERLINKV5_20151103074515","2010-01-20T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[382,"POWERLINKV5_20151103074515","2010-01-20T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[383,"POWERLINKV5_20151103074515","2010-01-20T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[384,"POWERLINKV5_20151103074515","2010-01-20T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[385,"POWERLINKV5_20151103074515","2010-01-20T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[386,"POWERLINKV5_20151103074515","2010-01-20T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[387,"POWERLINKV5_20151103074515","2010-01-20T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[388,"POWERLINKV5_20151103074515","2010-01-20T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[389,"POWERLINKV5_20151103074515","2010-01-20T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[390,"POWERLINKV5_20151103074515","2010-01-20T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[391,"POWERLINKV5_20151103074515","2010-01-20T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[392,"POWERLINKV5_20151103074515","2010-01-20T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[393,"POWERLINKV5_20151103074515","2010-01-20T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[394,"POWERLINKV5_20151103074515","2010-01-20T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[395,"POWERLINKV5_20151103074515","2010-01-20T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[396,"POWERLINKV5_20151103074515","2010-01-20T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[397,"POWERLINKV5_20151103074515","2010-01-20T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[398,"POWERLINKV5_20151103074515","2010-01-20T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[399,"POWERLINKV5_20151103074515","2010-01-20T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[400,"POWERLINKV5_20151103074515","2010-01-20T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[401,"POWERLINKV5_20151103074515","2010-01-20T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[402,"POWERLINKV5_20151103074515","2010-01-20T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[403,"POWERLINKV5_20151103074515","2010-01-20T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[404,"POWERLINKV5_20151103074515","2010-01-20T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[405,"POWERLINKV5_20151103074515","2010-01-20T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[406,"POWERLINKV5_20151103074515","2010-01-20T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[407,"POWERLINKV5_20151103074515","2010-01-20T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.66,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[408,"POWERLINKV5_20151103074515","2010-01-20T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[409,"POWERLINKV5_20151103074515","2010-01-20T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[410,"POWERLINKV5_20151103074515","2010-01-20T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[411,"POWERLINKV5_20151103074515","2010-01-20T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[412,"POWERLINKV5_20151103074515","2010-01-20T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[413,"POWERLINKV5_20151103074515","2010-01-20T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[414,"POWERLINKV5_20151103074515","2010-01-20T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[415,"POWERLINKV5_20151103074515","2010-01-20T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[416,"POWERLINKV5_20151103074515","2010-01-20T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[417,"POWERLINKV5_20151103074515","2010-01-20T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[418,"POWERLINKV5_20151103074515","2010-01-20T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[419,"POWERLINKV5_20151103074515","2010-01-20T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[420,"POWERLINKV5_20151103074515","2010-01-20T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[421,"POWERLINKV5_20151103074515","2010-01-20T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[422,"POWERLINKV5_20151103074515","2010-01-20T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[423,"POWERLINKV5_20151103074515","2010-01-20T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[424,"POWERLINKV5_20151103074515","2010-01-20T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[425,"POWERLINKV5_20151103074515","2010-01-20T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[426,"POWERLINKV5_20151103074515","2010-01-20T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[427,"POWERLINKV5_20151103074515","2010-01-20T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[428,"POWERLINKV5_20151103074515","2010-01-21","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[429,"POWERLINKV5_20151103074515","2010-01-21T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[430,"POWERLINKV5_20151103074515","2010-01-21T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[431,"POWERLINKV5_20151103074515","2010-01-21T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[432,"POWERLINKV5_20151103074515","2010-01-21T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[433,"POWERLINKV5_20151103074515","2010-01-21T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[434,"POWERLINKV5_20151103074515","2010-01-21T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[435,"POWERLINKV5_20151103074515","2010-01-21T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[436,"POWERLINKV5_20151103074515","2010-01-21T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[437,"POWERLINKV5_20151103074515","2010-01-21T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[438,"POWERLINKV5_20151103074515","2010-01-21T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.37,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[439,"POWERLINKV5_20151103074515","2010-01-21T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[440,"POWERLINKV5_20151103074515","2010-01-21T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[441,"POWERLINKV5_20151103074515","2010-01-21T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[442,"POWERLINKV5_20151103074515","2010-01-21T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[443,"POWERLINKV5_20151103074515","2010-01-21T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[444,"POWERLINKV5_20151103074515","2010-01-21T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[445,"POWERLINKV5_20151103074515","2010-01-21T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.34,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[446,"POWERLINKV5_20151103074515","2010-01-21T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[447,"POWERLINKV5_20151103074515","2010-01-21T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[448,"POWERLINKV5_20151103074515","2010-01-21T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[449,"POWERLINKV5_20151103074515","2010-01-21T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[450,"POWERLINKV5_20151103074515","2010-01-21T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[451,"POWERLINKV5_20151103074515","2010-01-21T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[452,"POWERLINKV5_20151103074515","2010-01-21T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[453,"POWERLINKV5_20151103074515","2010-01-21T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[454,"POWERLINKV5_20151103074515","2010-01-21T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[455,"POWERLINKV5_20151103074515","2010-01-21T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[456,"POWERLINKV5_20151103074515","2010-01-21T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[457,"POWERLINKV5_20151103074515","2010-01-21T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[458,"POWERLINKV5_20151103074515","2010-01-21T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[459,"POWERLINKV5_20151103074515","2010-01-21T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[460,"POWERLINKV5_20151103074515","2010-01-21T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[461,"POWERLINKV5_20151103074515","2010-01-21T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[462,"POWERLINKV5_20151103074515","2010-01-21T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[463,"POWERLINKV5_20151103074515","2010-01-21T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[464,"POWERLINKV5_20151103074515","2010-01-21T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[465,"POWERLINKV5_20151103074515","2010-01-21T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[466,"POWERLINKV5_20151103074515","2010-01-21T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[467,"POWERLINKV5_20151103074515","2010-01-21T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[468,"POWERLINKV5_20151103074515","2010-01-21T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[469,"POWERLINKV5_20151103074515","2010-01-21T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[470,"POWERLINKV5_20151103074515","2010-01-21T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[471,"POWERLINKV5_20151103074515","2010-01-21T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[472,"POWERLINKV5_20151103074515","2010-01-21T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1012.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[473,"POWERLINKV5_20151103074515","2010-01-21T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[474,"POWERLINKV5_20151103074515","2010-01-21T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[475,"POWERLINKV5_20151103074515","2010-01-21T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[476,"POWERLINKV5_20151103074515","2010-01-21T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[477,"POWERLINKV5_20151103074515","2010-01-21T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[478,"POWERLINKV5_20151103074515","2010-01-21T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[479,"POWERLINKV5_20151103074515","2010-01-21T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[480,"POWERLINKV5_20151103074515","2010-01-21T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[481,"POWERLINKV5_20151103074515","2010-01-21T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.26,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[482,"POWERLINKV5_20151103074515","2010-01-21T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[483,"POWERLINKV5_20151103074515","2010-01-21T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[484,"POWERLINKV5_20151103074515","2010-01-21T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[485,"POWERLINKV5_20151103074515","2010-01-21T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[486,"POWERLINKV5_20151103074515","2010-01-21T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[487,"POWERLINKV5_20151103074515","2010-01-21T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[488,"POWERLINKV5_20151103074515","2010-01-21T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[489,"POWERLINKV5_20151103074515","2010-01-21T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[490,"POWERLINKV5_20151103074515","2010-01-21T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[491,"POWERLINKV5_20151103074515","2010-01-21T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[492,"POWERLINKV5_20151103074515","2010-01-21T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[493,"POWERLINKV5_20151103074515","2010-01-21T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[494,"POWERLINKV5_20151103074515","2010-01-21T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[495,"POWERLINKV5_20151103074515","2010-01-21T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[496,"POWERLINKV5_20151103074515","2010-01-21T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[497,"POWERLINKV5_20151103074515","2010-01-21T11:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.4100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[498,"POWERLINKV5_20151103074515","2010-01-21T11:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1036.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[499,"POWERLINKV5_20151103074515","2010-01-21T11:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[500,"POWERLINKV5_20151103074515","2010-01-21T11:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1045.26,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[501,"POWERLINKV5_20151103074515","2010-01-21T11:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[502,"POWERLINKV5_20151103074515","2010-01-21T11:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[503,"POWERLINKV5_20151103074515","2010-01-21T11:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[504,"POWERLINKV5_20151103074515","2010-01-21T11:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[505,"POWERLINKV5_20151103074515","2010-01-21T11:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[506,"POWERLINKV5_20151103074515","2010-01-21T11:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1046.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[507,"POWERLINKV5_20151103074515","2010-01-21T11:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1049.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[508,"POWERLINKV5_20151103074515","2010-01-21T11:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1047.82,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[509,"POWERLINKV5_20151103074515","2010-01-21T12:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1072.6600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[510,"POWERLINKV5_20151103074515","2010-01-21T12:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1132.3599999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[511,"POWERLINKV5_20151103074515","2010-01-21T12:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1096.9100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[512,"POWERLINKV5_20151103074515","2010-01-21T12:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1127.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[513,"POWERLINKV5_20151103074515","2010-01-21T12:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1116.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[514,"POWERLINKV5_20151103074515","2010-01-21T12:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1087.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[515,"POWERLINKV5_20151103074515","2010-01-21T12:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1092.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[516,"POWERLINKV5_20151103074515","2010-01-21T12:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1089.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[517,"POWERLINKV5_20151103074515","2010-01-21T12:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1093.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[518,"POWERLINKV5_20151103074515","2010-01-21T12:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1110.6500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[519,"POWERLINKV5_20151103074515","2010-01-21T12:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1092.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[520,"POWERLINKV5_20151103074515","2010-01-21T12:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1120.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[521,"POWERLINKV5_20151103074515","2010-01-21T13:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1091.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[522,"POWERLINKV5_20151103074515","2010-01-21T13:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1092.69,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[523,"POWERLINKV5_20151103074515","2010-01-21T13:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1094.1300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[524,"POWERLINKV5_20151103074515","2010-01-21T13:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1094.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[525,"POWERLINKV5_20151103074515","2010-01-21T13:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1094.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[526,"POWERLINKV5_20151103074515","2010-01-21T13:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1094.0899999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[527,"POWERLINKV5_20151103074515","2010-01-21T13:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1125.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[528,"POWERLINKV5_20151103074515","2010-01-21T13:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1095.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[529,"POWERLINKV5_20151103074515","2010-01-21T13:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1128.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[530,"POWERLINKV5_20151103074515","2010-01-21T13:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1101.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[531,"POWERLINKV5_20151103074515","2010-01-21T13:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1132.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[532,"POWERLINKV5_20151103074515","2010-01-21T13:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1130.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[533,"POWERLINKV5_20151103074515","2010-01-21T14:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1097.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[534,"POWERLINKV5_20151103074515","2010-01-21T14:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1096.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[535,"POWERLINKV5_20151103074515","2010-01-21T14:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1098.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[536,"POWERLINKV5_20151103074515","2010-01-21T14:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1095.26,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[537,"POWERLINKV5_20151103074515","2010-01-21T14:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1096.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[538,"POWERLINKV5_20151103074515","2010-01-21T14:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1096.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[539,"POWERLINKV5_20151103074515","2010-01-21T14:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1096.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[540,"POWERLINKV5_20151103074515","2010-01-21T14:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1092.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[541,"POWERLINKV5_20151103074515","2010-01-21T14:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1101.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[542,"POWERLINKV5_20151103074515","2010-01-21T15:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,10915.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[543,"POWERLINKV5_20151103074515","2010-01-21T15:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1279.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[544,"POWERLINKV5_20151103074515","2010-01-21T15:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1088.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[545,"POWERLINKV5_20151103074515","2010-01-21T16:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[546,"POWERLINKV5_20151103074515","2010-01-21T16:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.1600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[547,"POWERLINKV5_20151103074515","2010-01-21T16:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[548,"POWERLINKV5_20151103074515","2010-01-21T16:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1069.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[549,"POWERLINKV5_20151103074515","2010-01-21T16:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1087.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[550,"POWERLINKV5_20151103074515","2010-01-21T16:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[551,"POWERLINKV5_20151103074515","2010-01-21T16:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[552,"POWERLINKV5_20151103074515","2010-01-21T16:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1034.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[553,"POWERLINKV5_20151103074515","2010-01-21T16:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.8399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[554,"POWERLINKV5_20151103074515","2010-01-21T17:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[555,"POWERLINKV5_20151103074515","2010-01-21T17:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1051.1400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[556,"POWERLINKV5_20151103074515","2010-01-21T17:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1088.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[557,"POWERLINKV5_20151103074515","2010-01-21T17:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1088.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[558,"POWERLINKV5_20151103074515","2010-01-21T17:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[559,"POWERLINKV5_20151103074515","2010-01-21T17:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[560,"POWERLINKV5_20151103074515","2010-01-21T17:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[561,"POWERLINKV5_20151103074515","2010-01-21T17:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[562,"POWERLINKV5_20151103074515","2010-01-21T17:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[563,"POWERLINKV5_20151103074515","2010-01-21T17:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1036.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[564,"POWERLINKV5_20151103074515","2010-01-21T17:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[565,"POWERLINKV5_20151103074515","2010-01-21T17:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.76,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[566,"POWERLINKV5_20151103074515","2010-01-21T18:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[567,"POWERLINKV5_20151103074515","2010-01-21T18:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1098.3800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[568,"POWERLINKV5_20151103074515","2010-01-21T18:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1053.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[569,"POWERLINKV5_20151103074515","2010-01-21T18:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1059.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[570,"POWERLINKV5_20151103074515","2010-01-21T18:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1095.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[571,"POWERLINKV5_20151103074515","2010-01-21T18:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1053.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[572,"POWERLINKV5_20151103074515","2010-01-21T18:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1047.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[573,"POWERLINKV5_20151103074515","2010-01-21T18:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1059.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[574,"POWERLINKV5_20151103074515","2010-01-21T18:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1053.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[575,"POWERLINKV5_20151103074515","2010-01-21T18:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1046.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[576,"POWERLINKV5_20151103074515","2010-01-21T18:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[577,"POWERLINKV5_20151103074515","2010-01-21T18:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.5899999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[578,"POWERLINKV5_20151103074515","2010-01-21T19:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[579,"POWERLINKV5_20151103074515","2010-01-21T19:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[580,"POWERLINKV5_20151103074515","2010-01-21T19:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1046.0999999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[581,"POWERLINKV5_20151103074515","2010-01-21T19:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.6300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[582,"POWERLINKV5_20151103074515","2010-01-21T19:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1046.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[583,"POWERLINKV5_20151103074515","2010-01-21T19:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1045.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[584,"POWERLINKV5_20151103074515","2010-01-21T19:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[585,"POWERLINKV5_20151103074515","2010-01-21T19:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1048.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[586,"POWERLINKV5_20151103074515","2010-01-21T19:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1056,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[587,"POWERLINKV5_20151103074515","2010-01-21T19:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1048.8800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[588,"POWERLINKV5_20151103074515","2010-01-21T19:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1045.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[589,"POWERLINKV5_20151103074515","2010-01-21T19:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.1199999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[590,"POWERLINKV5_20151103074515","2010-01-21T20:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[591,"POWERLINKV5_20151103074515","2010-01-21T20:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1056.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[592,"POWERLINKV5_20151103074515","2010-01-21T20:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1053.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[593,"POWERLINKV5_20151103074515","2010-01-21T20:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1046.3900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[594,"POWERLINKV5_20151103074515","2010-01-21T20:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[595,"POWERLINKV5_20151103074515","2010-01-21T20:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[596,"POWERLINKV5_20151103074515","2010-01-21T20:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[597,"POWERLINKV5_20151103074515","2010-01-21T20:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[598,"POWERLINKV5_20151103074515","2010-01-21T20:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.3499999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[599,"POWERLINKV5_20151103074515","2010-01-21T20:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[600,"POWERLINKV5_20151103074515","2010-01-21T20:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1034.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[601,"POWERLINKV5_20151103074515","2010-01-21T20:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.6099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[602,"POWERLINKV5_20151103074515","2010-01-21T21:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[603,"POWERLINKV5_20151103074515","2010-01-21T21:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[604,"POWERLINKV5_20151103074515","2010-01-21T21:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[605,"POWERLINKV5_20151103074515","2010-01-21T21:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[606,"POWERLINKV5_20151103074515","2010-01-21T21:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[607,"POWERLINKV5_20151103074515","2010-01-21T21:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1034.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[608,"POWERLINKV5_20151103074515","2010-01-21T21:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[609,"POWERLINKV5_20151103074515","2010-01-21T21:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[610,"POWERLINKV5_20151103074515","2010-01-21T21:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.6500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[611,"POWERLINKV5_20151103074515","2010-01-21T21:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.6300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[612,"POWERLINKV5_20151103074515","2010-01-21T21:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[613,"POWERLINKV5_20151103074515","2010-01-21T21:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[614,"POWERLINKV5_20151103074515","2010-01-21T22:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[615,"POWERLINKV5_20151103074515","2010-01-21T22:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[616,"POWERLINKV5_20151103074515","2010-01-21T22:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[617,"POWERLINKV5_20151103074515","2010-01-21T22:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[618,"POWERLINKV5_20151103074515","2010-01-21T22:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.3399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[619,"POWERLINKV5_20151103074515","2010-01-21T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[620,"POWERLINKV5_20151103074515","2010-01-21T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[621,"POWERLINKV5_20151103074515","2010-01-21T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[622,"POWERLINKV5_20151103074515","2010-01-21T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[623,"POWERLINKV5_20151103074515","2010-01-21T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[624,"POWERLINKV5_20151103074515","2010-01-21T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[625,"POWERLINKV5_20151103074515","2010-01-21T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[626,"POWERLINKV5_20151103074515","2010-01-21T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[627,"POWERLINKV5_20151103074515","2010-01-21T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[628,"POWERLINKV5_20151103074515","2010-01-21T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[629,"POWERLINKV5_20151103074515","2010-01-21T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[630,"POWERLINKV5_20151103074515","2010-01-21T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[631,"POWERLINKV5_20151103074515","2010-01-21T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[632,"POWERLINKV5_20151103074515","2010-01-21T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[633,"POWERLINKV5_20151103074515","2010-01-21T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[634,"POWERLINKV5_20151103074515","2010-01-21T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[635,"POWERLINKV5_20151103074515","2010-01-21T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[636,"POWERLINKV5_20151103074515","2010-01-21T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[637,"POWERLINKV5_20151103074515","2010-01-21T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[638,"POWERLINKV5_20151103074515","2010-01-22","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[639,"POWERLINKV5_20151103074515","2010-01-22T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[640,"POWERLINKV5_20151103074515","2010-01-22T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[641,"POWERLINKV5_20151103074515","2010-01-22T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[642,"POWERLINKV5_20151103074515","2010-01-22T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.76,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[643,"POWERLINKV5_20151103074515","2010-01-22T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[644,"POWERLINKV5_20151103074515","2010-01-22T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[645,"POWERLINKV5_20151103074515","2010-01-22T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[646,"POWERLINKV5_20151103074515","2010-01-22T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.3900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[647,"POWERLINKV5_20151103074515","2010-01-22T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[648,"POWERLINKV5_20151103074515","2010-01-22T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[649,"POWERLINKV5_20151103074515","2010-01-22T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[650,"POWERLINKV5_20151103074515","2010-01-22T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[651,"POWERLINKV5_20151103074515","2010-01-22T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[652,"POWERLINKV5_20151103074515","2010-01-22T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[653,"POWERLINKV5_20151103074515","2010-01-22T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[654,"POWERLINKV5_20151103074515","2010-01-22T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[655,"POWERLINKV5_20151103074515","2010-01-22T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[656,"POWERLINKV5_20151103074515","2010-01-22T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[657,"POWERLINKV5_20151103074515","2010-01-22T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.66,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[658,"POWERLINKV5_20151103074515","2010-01-22T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[659,"POWERLINKV5_20151103074515","2010-01-22T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[660,"POWERLINKV5_20151103074515","2010-01-22T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.36,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[661,"POWERLINKV5_20151103074515","2010-01-22T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[662,"POWERLINKV5_20151103074515","2010-01-22T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[663,"POWERLINKV5_20151103074515","2010-01-22T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[664,"POWERLINKV5_20151103074515","2010-01-22T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[665,"POWERLINKV5_20151103074515","2010-01-22T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.36,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[666,"POWERLINKV5_20151103074515","2010-01-22T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[667,"POWERLINKV5_20151103074515","2010-01-22T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[668,"POWERLINKV5_20151103074515","2010-01-22T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[669,"POWERLINKV5_20151103074515","2010-01-22T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[670,"POWERLINKV5_20151103074515","2010-01-22T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[671,"POWERLINKV5_20151103074515","2010-01-22T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[672,"POWERLINKV5_20151103074515","2010-01-22T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[673,"POWERLINKV5_20151103074515","2010-01-22T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[674,"POWERLINKV5_20151103074515","2010-01-22T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[675,"POWERLINKV5_20151103074515","2010-01-22T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[676,"POWERLINKV5_20151103074515","2010-01-22T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[677,"POWERLINKV5_20151103074515","2010-01-22T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[678,"POWERLINKV5_20151103074515","2010-01-22T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[679,"POWERLINKV5_20151103074515","2010-01-22T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[680,"POWERLINKV5_20151103074515","2010-01-22T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[681,"POWERLINKV5_20151103074515","2010-01-22T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[682,"POWERLINKV5_20151103074515","2010-01-22T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[683,"POWERLINKV5_20151103074515","2010-01-22T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[684,"POWERLINKV5_20151103074515","2010-01-22T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[685,"POWERLINKV5_20151103074515","2010-01-22T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[686,"POWERLINKV5_20151103074515","2010-01-22T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[687,"POWERLINKV5_20151103074515","2010-01-22T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[688,"POWERLINKV5_20151103074515","2010-01-22T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[689,"POWERLINKV5_20151103074515","2010-01-22T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[690,"POWERLINKV5_20151103074515","2010-01-22T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[691,"POWERLINKV5_20151103074515","2010-01-22T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[692,"POWERLINKV5_20151103074515","2010-01-22T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[693,"POWERLINKV5_20151103074515","2010-01-22T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[694,"POWERLINKV5_20151103074515","2010-01-22T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[695,"POWERLINKV5_20151103074515","2010-01-22T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[696,"POWERLINKV5_20151103074515","2010-01-22T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[697,"POWERLINKV5_20151103074515","2010-01-22T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[698,"POWERLINKV5_20151103074515","2010-01-22T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[699,"POWERLINKV5_20151103074515","2010-01-22T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[700,"POWERLINKV5_20151103074515","2010-01-22T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[701,"POWERLINKV5_20151103074515","2010-01-22T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[702,"POWERLINKV5_20151103074515","2010-01-22T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[703,"POWERLINKV5_20151103074515","2010-01-22T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[704,"POWERLINKV5_20151103074515","2010-01-22T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[705,"POWERLINKV5_20151103074515","2010-01-22T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[706,"POWERLINKV5_20151103074515","2010-01-22T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[707,"POWERLINKV5_20151103074515","2010-01-22T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[708,"POWERLINKV5_20151103074515","2010-01-22T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[709,"POWERLINKV5_20151103074515","2010-01-22T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[710,"POWERLINKV5_20151103074515","2010-01-22T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[711,"POWERLINKV5_20151103074515","2010-01-22T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[712,"POWERLINKV5_20151103074515","2010-01-22T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[713,"POWERLINKV5_20151103074515","2010-01-22T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[714,"POWERLINKV5_20151103074515","2010-01-22T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[715,"POWERLINKV5_20151103074515","2010-01-22T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[716,"POWERLINKV5_20151103074515","2010-01-22T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[717,"POWERLINKV5_20151103074515","2010-01-22T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[718,"POWERLINKV5_20151103074515","2010-01-22T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[719,"POWERLINKV5_20151103074515","2010-01-22T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[720,"POWERLINKV5_20151103074515","2010-01-22T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[721,"POWERLINKV5_20151103074515","2010-01-22T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[722,"POWERLINKV5_20151103074515","2010-01-22T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.6500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[723,"POWERLINKV5_20151103074515","2010-01-22T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[724,"POWERLINKV5_20151103074515","2010-01-22T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[725,"POWERLINKV5_20151103074515","2010-01-22T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[726,"POWERLINKV5_20151103074515","2010-01-22T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[727,"POWERLINKV5_20151103074515","2010-01-22T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[728,"POWERLINKV5_20151103074515","2010-01-22T07:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[729,"POWERLINKV5_20151103074515","2010-01-22T07:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[730,"POWERLINKV5_20151103074515","2010-01-22T07:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[731,"POWERLINKV5_20151103074515","2010-01-22T07:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.3900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[732,"POWERLINKV5_20151103074515","2010-01-22T07:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.8399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[733,"POWERLINKV5_20151103074515","2010-01-22T07:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[734,"POWERLINKV5_20151103074515","2010-01-22T08:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.3800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[735,"POWERLINKV5_20151103074515","2010-01-22T08:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[736,"POWERLINKV5_20151103074515","2010-01-22T08:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[737,"POWERLINKV5_20151103074515","2010-01-22T08:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[738,"POWERLINKV5_20151103074515","2010-01-22T08:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[739,"POWERLINKV5_20151103074515","2010-01-22T08:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[740,"POWERLINKV5_20151103074515","2010-01-22T08:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[741,"POWERLINKV5_20151103074515","2010-01-22T08:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[742,"POWERLINKV5_20151103074515","2010-01-22T08:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[743,"POWERLINKV5_20151103074515","2010-01-22T08:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[744,"POWERLINKV5_20151103074515","2010-01-22T08:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.8399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[745,"POWERLINKV5_20151103074515","2010-01-22T08:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[746,"POWERLINKV5_20151103074515","2010-01-22T09:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[747,"POWERLINKV5_20151103074515","2010-01-22T09:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[748,"POWERLINKV5_20151103074515","2010-01-22T09:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[749,"POWERLINKV5_20151103074515","2010-01-22T09:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[750,"POWERLINKV5_20151103074515","2010-01-22T09:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[751,"POWERLINKV5_20151103074515","2010-01-22T09:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[752,"POWERLINKV5_20151103074515","2010-01-22T09:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[753,"POWERLINKV5_20151103074515","2010-01-22T09:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[754,"POWERLINKV5_20151103074515","2010-01-22T09:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[755,"POWERLINKV5_20151103074515","2010-01-22T09:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[756,"POWERLINKV5_20151103074515","2010-01-22T09:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1042.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[757,"POWERLINKV5_20151103074515","2010-01-22T09:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[758,"POWERLINKV5_20151103074515","2010-01-22T10:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.1600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[759,"POWERLINKV5_20151103074515","2010-01-22T10:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[760,"POWERLINKV5_20151103074515","2010-01-22T10:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[761,"POWERLINKV5_20151103074515","2010-01-22T10:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.4100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[762,"POWERLINKV5_20151103074515","2010-01-22T10:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[763,"POWERLINKV5_20151103074515","2010-01-22T10:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.6600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[764,"POWERLINKV5_20151103074515","2010-01-22T10:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.9100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[765,"POWERLINKV5_20151103074515","2010-01-22T10:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.3900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[766,"POWERLINKV5_20151103074515","2010-01-22T10:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1041.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[767,"POWERLINKV5_20151103074515","2010-01-22T10:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[768,"POWERLINKV5_20151103074515","2010-01-22T10:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[769,"POWERLINKV5_20151103074515","2010-01-22T10:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.9000000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[770,"POWERLINKV5_20151103074515","2010-01-22T11:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1040.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[771,"POWERLINKV5_20151103074515","2010-01-22T11:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[772,"POWERLINKV5_20151103074515","2010-01-22T11:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[773,"POWERLINKV5_20151103074515","2010-01-22T11:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[774,"POWERLINKV5_20151103074515","2010-01-22T11:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[775,"POWERLINKV5_20151103074515","2010-01-22T11:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[776,"POWERLINKV5_20151103074515","2010-01-22T11:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[777,"POWERLINKV5_20151103074515","2010-01-22T11:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[778,"POWERLINKV5_20151103074515","2010-01-22T11:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[779,"POWERLINKV5_20151103074515","2010-01-22T11:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[780,"POWERLINKV5_20151103074515","2010-01-22T11:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[781,"POWERLINKV5_20151103074515","2010-01-22T11:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[782,"POWERLINKV5_20151103074515","2010-01-22T12:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[783,"POWERLINKV5_20151103074515","2010-01-22T12:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1087.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[784,"POWERLINKV5_20151103074515","2010-01-22T12:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[785,"POWERLINKV5_20151103074515","2010-01-22T12:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[786,"POWERLINKV5_20151103074515","2010-01-22T12:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[787,"POWERLINKV5_20151103074515","2010-01-22T12:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[788,"POWERLINKV5_20151103074515","2010-01-22T12:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[789,"POWERLINKV5_20151103074515","2010-01-22T12:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[790,"POWERLINKV5_20151103074515","2010-01-22T12:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[791,"POWERLINKV5_20151103074515","2010-01-22T17:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[792,"POWERLINKV5_20151103074515","2010-01-22T17:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[793,"POWERLINKV5_20151103074515","2010-01-22T17:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[794,"POWERLINKV5_20151103074515","2010-01-22T17:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[795,"POWERLINKV5_20151103074515","2010-01-22T17:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[796,"POWERLINKV5_20151103074515","2010-01-22T17:45:00","QNTE_ROC","Q-NIL","2006-01-27",1,17.28,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[797,"POWERLINKV5_20151103074515","2010-01-22T17:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[798,"POWERLINKV5_20151103074515","2010-01-22T18:30:00","QNTE_ROC","Q-NIL","2006-01-27",1,18.89,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[799,"POWERLINKV5_20151103074515","2010-01-22T18:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[800,"POWERLINKV5_20151103074515","2010-01-22T19:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.27,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[801,"POWERLINKV5_20151103074515","2010-01-22T19:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.6199999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[802,"POWERLINKV5_20151103074515","2010-01-22T19:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[803,"POWERLINKV5_20151103074515","2010-01-22T19:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[804,"POWERLINKV5_20151103074515","2010-01-22T19:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1088.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[805,"POWERLINKV5_20151103074515","2010-01-22T19:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1049.8900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[806,"POWERLINKV5_20151103074515","2010-01-22T19:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1044.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[807,"POWERLINKV5_20151103074515","2010-01-22T19:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[808,"POWERLINKV5_20151103074515","2010-01-22T19:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[809,"POWERLINKV5_20151103074515","2010-01-22T20:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[810,"POWERLINKV5_20151103074515","2010-01-22T20:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1049.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[811,"POWERLINKV5_20151103074515","2010-01-22T20:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.5899999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[812,"POWERLINKV5_20151103074515","2010-01-22T20:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[813,"POWERLINKV5_20151103074515","2010-01-22T20:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1043.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[814,"POWERLINKV5_20151103074515","2010-01-22T20:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[815,"POWERLINKV5_20151103074515","2010-01-22T20:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[816,"POWERLINKV5_20151103074515","2010-01-22T20:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1036.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[817,"POWERLINKV5_20151103074515","2010-01-22T20:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[818,"POWERLINKV5_20151103074515","2010-01-22T20:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[819,"POWERLINKV5_20151103074515","2010-01-22T20:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.8599999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[820,"POWERLINKV5_20151103074515","2010-01-22T20:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1036.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[821,"POWERLINKV5_20151103074515","2010-01-22T21:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[822,"POWERLINKV5_20151103074515","2010-01-22T21:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[823,"POWERLINKV5_20151103074515","2010-01-22T21:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[824,"POWERLINKV5_20151103074515","2010-01-22T21:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[825,"POWERLINKV5_20151103074515","2010-01-22T21:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[826,"POWERLINKV5_20151103074515","2010-01-22T21:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1034.8800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[827,"POWERLINKV5_20151103074515","2010-01-22T21:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1035.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[828,"POWERLINKV5_20151103074515","2010-01-22T21:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[829,"POWERLINKV5_20151103074515","2010-01-22T21:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[830,"POWERLINKV5_20151103074515","2010-01-22T21:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[831,"POWERLINKV5_20151103074515","2010-01-22T21:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.5999999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[832,"POWERLINKV5_20151103074515","2010-01-22T21:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[833,"POWERLINKV5_20151103074515","2010-01-22T22:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.96,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[834,"POWERLINKV5_20151103074515","2010-01-22T22:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[835,"POWERLINKV5_20151103074515","2010-01-22T22:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.69,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[836,"POWERLINKV5_20151103074515","2010-01-22T22:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1034.3800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[837,"POWERLINKV5_20151103074515","2010-01-22T22:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1033.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[838,"POWERLINKV5_20151103074515","2010-01-22T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[839,"POWERLINKV5_20151103074515","2010-01-22T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[840,"POWERLINKV5_20151103074515","2010-01-22T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1032.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[841,"POWERLINKV5_20151103074515","2010-01-22T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[842,"POWERLINKV5_20151103074515","2010-01-22T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.9000000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[843,"POWERLINKV5_20151103074515","2010-01-22T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.3699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[844,"POWERLINKV5_20151103074515","2010-01-22T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[845,"POWERLINKV5_20151103074515","2010-01-22T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[846,"POWERLINKV5_20151103074515","2010-01-22T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[847,"POWERLINKV5_20151103074515","2010-01-22T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[848,"POWERLINKV5_20151103074515","2010-01-22T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[849,"POWERLINKV5_20151103074515","2010-01-22T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[850,"POWERLINKV5_20151103074515","2010-01-22T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[851,"POWERLINKV5_20151103074515","2010-01-22T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[852,"POWERLINKV5_20151103074515","2010-01-22T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[853,"POWERLINKV5_20151103074515","2010-01-22T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[854,"POWERLINKV5_20151103074515","2010-01-22T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.1300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[855,"POWERLINKV5_20151103074515","2010-01-22T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[856,"POWERLINKV5_20151103074515","2010-01-22T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[857,"POWERLINKV5_20151103074515","2010-01-23","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[858,"POWERLINKV5_20151103074515","2010-01-23T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.1300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[859,"POWERLINKV5_20151103074515","2010-01-23T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[860,"POWERLINKV5_20151103074515","2010-01-23T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[861,"POWERLINKV5_20151103074515","2010-01-23T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[862,"POWERLINKV5_20151103074515","2010-01-23T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[863,"POWERLINKV5_20151103074515","2010-01-23T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[864,"POWERLINKV5_20151103074515","2010-01-23T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[865,"POWERLINKV5_20151103074515","2010-01-23T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3499999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[866,"POWERLINKV5_20151103074515","2010-01-23T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[867,"POWERLINKV5_20151103074515","2010-01-23T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[868,"POWERLINKV5_20151103074515","2010-01-23T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[869,"POWERLINKV5_20151103074515","2010-01-23T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[870,"POWERLINKV5_20151103074515","2010-01-23T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[871,"POWERLINKV5_20151103074515","2010-01-23T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[872,"POWERLINKV5_20151103074515","2010-01-23T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[873,"POWERLINKV5_20151103074515","2010-01-23T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[874,"POWERLINKV5_20151103074515","2010-01-23T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[875,"POWERLINKV5_20151103074515","2010-01-23T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[876,"POWERLINKV5_20151103074515","2010-01-23T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[877,"POWERLINKV5_20151103074515","2010-01-23T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[878,"POWERLINKV5_20151103074515","2010-01-23T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[879,"POWERLINKV5_20151103074515","2010-01-23T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[880,"POWERLINKV5_20151103074515","2010-01-23T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[881,"POWERLINKV5_20151103074515","2010-01-23T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[882,"POWERLINKV5_20151103074515","2010-01-23T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.37,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[883,"POWERLINKV5_20151103074515","2010-01-23T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[884,"POWERLINKV5_20151103074515","2010-01-23T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[885,"POWERLINKV5_20151103074515","2010-01-23T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[886,"POWERLINKV5_20151103074515","2010-01-23T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[887,"POWERLINKV5_20151103074515","2010-01-23T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[888,"POWERLINKV5_20151103074515","2010-01-23T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.39,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[889,"POWERLINKV5_20151103074515","2010-01-23T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[890,"POWERLINKV5_20151103074515","2010-01-23T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[891,"POWERLINKV5_20151103074515","2010-01-23T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.4,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[892,"POWERLINKV5_20151103074515","2010-01-23T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[893,"POWERLINKV5_20151103074515","2010-01-23T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[894,"POWERLINKV5_20151103074515","2010-01-23T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[895,"POWERLINKV5_20151103074515","2010-01-23T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[896,"POWERLINKV5_20151103074515","2010-01-23T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[897,"POWERLINKV5_20151103074515","2010-01-23T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[898,"POWERLINKV5_20151103074515","2010-01-23T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[899,"POWERLINKV5_20151103074515","2010-01-23T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[900,"POWERLINKV5_20151103074515","2010-01-23T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[901,"POWERLINKV5_20151103074515","2010-01-23T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[902,"POWERLINKV5_20151103074515","2010-01-23T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[903,"POWERLINKV5_20151103074515","2010-01-23T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[904,"POWERLINKV5_20151103074515","2010-01-23T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[905,"POWERLINKV5_20151103074515","2010-01-23T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.91,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[906,"POWERLINKV5_20151103074515","2010-01-23T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[907,"POWERLINKV5_20151103074515","2010-01-23T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[908,"POWERLINKV5_20151103074515","2010-01-23T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[909,"POWERLINKV5_20151103074515","2010-01-23T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[910,"POWERLINKV5_20151103074515","2010-01-23T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[911,"POWERLINKV5_20151103074515","2010-01-23T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[912,"POWERLINKV5_20151103074515","2010-01-23T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[913,"POWERLINKV5_20151103074515","2010-01-23T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[914,"POWERLINKV5_20151103074515","2010-01-23T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[915,"POWERLINKV5_20151103074515","2010-01-23T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[916,"POWERLINKV5_20151103074515","2010-01-23T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[917,"POWERLINKV5_20151103074515","2010-01-23T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[918,"POWERLINKV5_20151103074515","2010-01-23T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[919,"POWERLINKV5_20151103074515","2010-01-23T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[920,"POWERLINKV5_20151103074515","2010-01-23T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[921,"POWERLINKV5_20151103074515","2010-01-23T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[922,"POWERLINKV5_20151103074515","2010-01-23T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[923,"POWERLINKV5_20151103074515","2010-01-23T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[924,"POWERLINKV5_20151103074515","2010-01-23T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[925,"POWERLINKV5_20151103074515","2010-01-23T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[926,"POWERLINKV5_20151103074515","2010-01-23T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[927,"POWERLINKV5_20151103074515","2010-01-23T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[928,"POWERLINKV5_20151103074515","2010-01-23T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[929,"POWERLINKV5_20151103074515","2010-01-23T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[930,"POWERLINKV5_20151103074515","2010-01-23T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[931,"POWERLINKV5_20151103074515","2010-01-23T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[932,"POWERLINKV5_20151103074515","2010-01-23T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[933,"POWERLINKV5_20151103074515","2010-01-23T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[934,"POWERLINKV5_20151103074515","2010-01-23T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[935,"POWERLINKV5_20151103074515","2010-01-23T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[936,"POWERLINKV5_20151103074515","2010-01-23T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[937,"POWERLINKV5_20151103074515","2010-01-23T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[938,"POWERLINKV5_20151103074515","2010-01-23T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[939,"POWERLINKV5_20151103074515","2010-01-23T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[940,"POWERLINKV5_20151103074515","2010-01-23T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[941,"POWERLINKV5_20151103074515","2010-01-23T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[942,"POWERLINKV5_20151103074515","2010-01-23T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[943,"POWERLINKV5_20151103074515","2010-01-23T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[944,"POWERLINKV5_20151103074515","2010-01-23T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[945,"POWERLINKV5_20151103074515","2010-01-23T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[946,"POWERLINKV5_20151103074515","2010-01-23T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[947,"POWERLINKV5_20151103074515","2010-01-23T07:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[948,"POWERLINKV5_20151103074515","2010-01-23T07:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[949,"POWERLINKV5_20151103074515","2010-01-23T07:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[950,"POWERLINKV5_20151103074515","2010-01-23T07:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[951,"POWERLINKV5_20151103074515","2010-01-23T07:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[952,"POWERLINKV5_20151103074515","2010-01-23T07:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[953,"POWERLINKV5_20151103074515","2010-01-23T08:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[954,"POWERLINKV5_20151103074515","2010-01-23T08:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.1300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[955,"POWERLINKV5_20151103074515","2010-01-23T08:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[956,"POWERLINKV5_20151103074515","2010-01-23T08:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[957,"POWERLINKV5_20151103074515","2010-01-23T08:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[958,"POWERLINKV5_20151103074515","2010-01-23T08:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[959,"POWERLINKV5_20151103074515","2010-01-23T08:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[960,"POWERLINKV5_20151103074515","2010-01-23T08:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[961,"POWERLINKV5_20151103074515","2010-01-23T08:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.1099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[962,"POWERLINKV5_20151103074515","2010-01-23T08:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.5899999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[963,"POWERLINKV5_20151103074515","2010-01-23T08:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[964,"POWERLINKV5_20151103074515","2010-01-23T08:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[965,"POWERLINKV5_20151103074515","2010-01-23T09:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[966,"POWERLINKV5_20151103074515","2010-01-23T09:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[967,"POWERLINKV5_20151103074515","2010-01-23T09:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[968,"POWERLINKV5_20151103074515","2010-01-23T09:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[969,"POWERLINKV5_20151103074515","2010-01-23T09:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[970,"POWERLINKV5_20151103074515","2010-01-23T09:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[971,"POWERLINKV5_20151103074515","2010-01-23T09:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[972,"POWERLINKV5_20151103074515","2010-01-23T09:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1039.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[973,"POWERLINKV5_20151103074515","2010-01-23T09:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1036.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[974,"POWERLINKV5_20151103074515","2010-01-23T09:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[975,"POWERLINKV5_20151103074515","2010-01-23T09:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[976,"POWERLINKV5_20151103074515","2010-01-23T09:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1038.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[977,"POWERLINKV5_20151103074515","2010-01-23T10:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1037.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[978,"POWERLINKV5_20151103074515","2010-01-23T10:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.9000000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[979,"POWERLINKV5_20151103074515","2010-01-23T10:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[980,"POWERLINKV5_20151103074515","2010-01-23T10:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.1600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[981,"POWERLINKV5_20151103074515","2010-01-23T10:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[982,"POWERLINKV5_20151103074515","2010-01-23T10:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[983,"POWERLINKV5_20151103074515","2010-01-23T10:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[984,"POWERLINKV5_20151103074515","2010-01-23T10:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[985,"POWERLINKV5_20151103074515","2010-01-23T10:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.36,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[986,"POWERLINKV5_20151103074515","2010-01-23T10:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[987,"POWERLINKV5_20151103074515","2010-01-23T10:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1008.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[988,"POWERLINKV5_20151103074515","2010-01-23T10:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1005.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[989,"POWERLINKV5_20151103074515","2010-01-23T11:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1012.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[990,"POWERLINKV5_20151103074515","2010-01-23T11:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1008.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[991,"POWERLINKV5_20151103074515","2010-01-23T11:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1009.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[992,"POWERLINKV5_20151103074515","2010-01-23T11:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1010.39,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[993,"POWERLINKV5_20151103074515","2010-01-23T11:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[994,"POWERLINKV5_20151103074515","2010-01-23T11:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[995,"POWERLINKV5_20151103074515","2010-01-23T11:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[996,"POWERLINKV5_20151103074515","2010-01-23T11:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[997,"POWERLINKV5_20151103074515","2010-01-23T11:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[998,"POWERLINKV5_20151103074515","2010-01-23T11:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[999,"POWERLINKV5_20151103074515","2010-01-23T11:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1014.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1000,"POWERLINKV5_20151103074515","2010-01-23T11:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1001,"POWERLINKV5_20151103074515","2010-01-23T12:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1002,"POWERLINKV5_20151103074515","2010-01-23T12:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1003,"POWERLINKV5_20151103074515","2010-01-23T12:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1004,"POWERLINKV5_20151103074515","2010-01-23T12:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1005,"POWERLINKV5_20151103074515","2010-01-23T12:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1006,"POWERLINKV5_20151103074515","2010-01-23T12:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1007,"POWERLINKV5_20151103074515","2010-01-23T12:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1008,"POWERLINKV5_20151103074515","2010-01-23T14:50:00","QNTE_ROC","Q-NIL","2006-01-27",1,131.11000000000001,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1009,"POWERLINKV5_20151103074515","2010-01-23T19:35:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,501.57,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1010,"POWERLINKV5_20151103074515","2010-01-23T19:40:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,501.75,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1011,"POWERLINKV5_20151103074515","2010-01-23T19:45:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1012,"POWERLINKV5_20151103074515","2010-01-23T20:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1013,"POWERLINKV5_20151103074515","2010-01-23T20:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1014,"POWERLINKV5_20151103074515","2010-01-23T20:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.1600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1015,"POWERLINKV5_20151103074515","2010-01-23T20:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1016,"POWERLINKV5_20151103074515","2010-01-23T20:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1017,"POWERLINKV5_20151103074515","2010-01-23T20:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1018,"POWERLINKV5_20151103074515","2010-01-23T20:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1019,"POWERLINKV5_20151103074515","2010-01-23T20:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1020,"POWERLINKV5_20151103074515","2010-01-23T20:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1021,"POWERLINKV5_20151103074515","2010-01-23T20:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1022,"POWERLINKV5_20151103074515","2010-01-23T21:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1023,"POWERLINKV5_20151103074515","2010-01-23T21:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1024,"POWERLINKV5_20151103074515","2010-01-23T21:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1025,"POWERLINKV5_20151103074515","2010-01-23T21:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1026,"POWERLINKV5_20151103074515","2010-01-23T21:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1027,"POWERLINKV5_20151103074515","2010-01-23T21:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1028,"POWERLINKV5_20151103074515","2010-01-23T21:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1029,"POWERLINKV5_20151103074515","2010-01-23T21:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1030,"POWERLINKV5_20151103074515","2010-01-23T21:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1031,"POWERLINKV5_20151103074515","2010-01-23T21:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1032,"POWERLINKV5_20151103074515","2010-01-23T21:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1033,"POWERLINKV5_20151103074515","2010-01-23T21:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1034,"POWERLINKV5_20151103074515","2010-01-23T22:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1035,"POWERLINKV5_20151103074515","2010-01-23T22:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1036,"POWERLINKV5_20151103074515","2010-01-23T22:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1037,"POWERLINKV5_20151103074515","2010-01-23T22:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1038,"POWERLINKV5_20151103074515","2010-01-23T22:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.69,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1039,"POWERLINKV5_20151103074515","2010-01-23T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1040,"POWERLINKV5_20151103074515","2010-01-23T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1041,"POWERLINKV5_20151103074515","2010-01-23T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1042,"POWERLINKV5_20151103074515","2010-01-23T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1043,"POWERLINKV5_20151103074515","2010-01-23T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.34,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1044,"POWERLINKV5_20151103074515","2010-01-23T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1045,"POWERLINKV5_20151103074515","2010-01-23T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1046,"POWERLINKV5_20151103074515","2010-01-23T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1047,"POWERLINKV5_20151103074515","2010-01-23T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1048,"POWERLINKV5_20151103074515","2010-01-23T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.9100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1049,"POWERLINKV5_20151103074515","2010-01-23T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.6300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1050,"POWERLINKV5_20151103074515","2010-01-23T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1051,"POWERLINKV5_20151103074515","2010-01-23T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.96,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1052,"POWERLINKV5_20151103074515","2010-01-23T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1053,"POWERLINKV5_20151103074515","2010-01-23T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1054,"POWERLINKV5_20151103074515","2010-01-23T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1055,"POWERLINKV5_20151103074515","2010-01-23T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1056,"POWERLINKV5_20151103074515","2010-01-23T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1057,"POWERLINKV5_20151103074515","2010-01-23T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1058,"POWERLINKV5_20151103074515","2010-01-24","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1059,"POWERLINKV5_20151103074515","2010-01-24T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1060,"POWERLINKV5_20151103074515","2010-01-24T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1061,"POWERLINKV5_20151103074515","2010-01-24T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1062,"POWERLINKV5_20151103074515","2010-01-24T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1063,"POWERLINKV5_20151103074515","2010-01-24T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1064,"POWERLINKV5_20151103074515","2010-01-24T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1065,"POWERLINKV5_20151103074515","2010-01-24T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1066,"POWERLINKV5_20151103074515","2010-01-24T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.67,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1067,"POWERLINKV5_20151103074515","2010-01-24T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1068,"POWERLINKV5_20151103074515","2010-01-24T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.81,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1069,"POWERLINKV5_20151103074515","2010-01-24T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1070,"POWERLINKV5_20151103074515","2010-01-24T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1071,"POWERLINKV5_20151103074515","2010-01-24T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1072,"POWERLINKV5_20151103074515","2010-01-24T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1073,"POWERLINKV5_20151103074515","2010-01-24T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1074,"POWERLINKV5_20151103074515","2010-01-24T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1075,"POWERLINKV5_20151103074515","2010-01-24T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1076,"POWERLINKV5_20151103074515","2010-01-24T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1077,"POWERLINKV5_20151103074515","2010-01-24T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1078,"POWERLINKV5_20151103074515","2010-01-24T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1079,"POWERLINKV5_20151103074515","2010-01-24T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1080,"POWERLINKV5_20151103074515","2010-01-24T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1081,"POWERLINKV5_20151103074515","2010-01-24T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1082,"POWERLINKV5_20151103074515","2010-01-24T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1083,"POWERLINKV5_20151103074515","2010-01-24T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1084,"POWERLINKV5_20151103074515","2010-01-24T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1085,"POWERLINKV5_20151103074515","2010-01-24T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1086,"POWERLINKV5_20151103074515","2010-01-24T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1087,"POWERLINKV5_20151103074515","2010-01-24T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.37,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1088,"POWERLINKV5_20151103074515","2010-01-24T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1089,"POWERLINKV5_20151103074515","2010-01-24T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1090,"POWERLINKV5_20151103074515","2010-01-24T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1091,"POWERLINKV5_20151103074515","2010-01-24T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1092,"POWERLINKV5_20151103074515","2010-01-24T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1093,"POWERLINKV5_20151103074515","2010-01-24T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1094,"POWERLINKV5_20151103074515","2010-01-24T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1095,"POWERLINKV5_20151103074515","2010-01-24T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.27,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1096,"POWERLINKV5_20151103074515","2010-01-24T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1097,"POWERLINKV5_20151103074515","2010-01-24T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1098,"POWERLINKV5_20151103074515","2010-01-24T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1099,"POWERLINKV5_20151103074515","2010-01-24T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1100,"POWERLINKV5_20151103074515","2010-01-24T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1101,"POWERLINKV5_20151103074515","2010-01-24T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1102,"POWERLINKV5_20151103074515","2010-01-24T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1103,"POWERLINKV5_20151103074515","2010-01-24T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1104,"POWERLINKV5_20151103074515","2010-01-24T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1105,"POWERLINKV5_20151103074515","2010-01-24T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1106,"POWERLINKV5_20151103074515","2010-01-24T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1107,"POWERLINKV5_20151103074515","2010-01-24T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1108,"POWERLINKV5_20151103074515","2010-01-24T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1109,"POWERLINKV5_20151103074515","2010-01-24T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1110,"POWERLINKV5_20151103074515","2010-01-24T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1111,"POWERLINKV5_20151103074515","2010-01-24T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1112,"POWERLINKV5_20151103074515","2010-01-24T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1113,"POWERLINKV5_20151103074515","2010-01-24T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1114,"POWERLINKV5_20151103074515","2010-01-24T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1115,"POWERLINKV5_20151103074515","2010-01-24T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1116,"POWERLINKV5_20151103074515","2010-01-24T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1117,"POWERLINKV5_20151103074515","2010-01-24T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1118,"POWERLINKV5_20151103074515","2010-01-24T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1119,"POWERLINKV5_20151103074515","2010-01-24T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1120,"POWERLINKV5_20151103074515","2010-01-24T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1121,"POWERLINKV5_20151103074515","2010-01-24T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1122,"POWERLINKV5_20151103074515","2010-01-24T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1123,"POWERLINKV5_20151103074515","2010-01-24T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1124,"POWERLINKV5_20151103074515","2010-01-24T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1125,"POWERLINKV5_20151103074515","2010-01-24T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1126,"POWERLINKV5_20151103074515","2010-01-24T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1127,"POWERLINKV5_20151103074515","2010-01-24T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1128,"POWERLINKV5_20151103074515","2010-01-24T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1129,"POWERLINKV5_20151103074515","2010-01-24T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1130,"POWERLINKV5_20151103074515","2010-01-24T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1131,"POWERLINKV5_20151103074515","2010-01-24T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1132,"POWERLINKV5_20151103074515","2010-01-24T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1133,"POWERLINKV5_20151103074515","2010-01-24T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1134,"POWERLINKV5_20151103074515","2010-01-24T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1135,"POWERLINKV5_20151103074515","2010-01-24T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1136,"POWERLINKV5_20151103074515","2010-01-24T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.29,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1137,"POWERLINKV5_20151103074515","2010-01-24T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1138,"POWERLINKV5_20151103074515","2010-01-24T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1139,"POWERLINKV5_20151103074515","2010-01-24T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1140,"POWERLINKV5_20151103074515","2010-01-24T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1141,"POWERLINKV5_20151103074515","2010-01-24T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1142,"POWERLINKV5_20151103074515","2010-01-24T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1143,"POWERLINKV5_20151103074515","2010-01-24T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1144,"POWERLINKV5_20151103074515","2010-01-24T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1145,"POWERLINKV5_20151103074515","2010-01-24T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1146,"POWERLINKV5_20151103074515","2010-01-24T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1147,"POWERLINKV5_20151103074515","2010-01-24T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1148,"POWERLINKV5_20151103074515","2010-01-24T07:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1149,"POWERLINKV5_20151103074515","2010-01-24T07:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1150,"POWERLINKV5_20151103074515","2010-01-24T07:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1151,"POWERLINKV5_20151103074515","2010-01-24T07:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1152,"POWERLINKV5_20151103074515","2010-01-24T07:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1153,"POWERLINKV5_20151103074515","2010-01-24T07:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1154,"POWERLINKV5_20151103074515","2010-01-24T08:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1155,"POWERLINKV5_20151103074515","2010-01-24T08:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1156,"POWERLINKV5_20151103074515","2010-01-24T08:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1157,"POWERLINKV5_20151103074515","2010-01-24T08:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1158,"POWERLINKV5_20151103074515","2010-01-24T08:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1159,"POWERLINKV5_20151103074515","2010-01-24T08:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1160,"POWERLINKV5_20151103074515","2010-01-24T08:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1161,"POWERLINKV5_20151103074515","2010-01-24T08:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1162,"POWERLINKV5_20151103074515","2010-01-24T08:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1163,"POWERLINKV5_20151103074515","2010-01-24T08:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1164,"POWERLINKV5_20151103074515","2010-01-24T08:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1165,"POWERLINKV5_20151103074515","2010-01-24T08:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1166,"POWERLINKV5_20151103074515","2010-01-24T09:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.35,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1167,"POWERLINKV5_20151103074515","2010-01-24T09:00:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,6285.32,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1168,"POWERLINKV5_20151103074515","2010-01-24T09:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1169,"POWERLINKV5_20151103074515","2010-01-24T09:05:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-01-03",2,200000,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1170,"POWERLINKV5_20151103074515","2010-01-24T09:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1171,"POWERLINKV5_20151103074515","2010-01-24T09:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1172,"POWERLINKV5_20151103074515","2010-01-24T09:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1173,"POWERLINKV5_20151103074515","2010-01-24T09:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1174,"POWERLINKV5_20151103074515","2010-01-24T09:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1175,"POWERLINKV5_20151103074515","2010-01-24T09:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.1,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1176,"POWERLINKV5_20151103074515","2010-01-24T09:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1177,"POWERLINKV5_20151103074515","2010-01-24T09:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1178,"POWERLINKV5_20151103074515","2010-01-24T09:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1179,"POWERLINKV5_20151103074515","2010-01-24T09:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1180,"POWERLINKV5_20151103074515","2010-01-24T10:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1181,"POWERLINKV5_20151103074515","2010-01-24T10:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1182,"POWERLINKV5_20151103074515","2010-01-24T10:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.4,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1183,"POWERLINKV5_20151103074515","2010-01-24T10:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.4,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1184,"POWERLINKV5_20151103074515","2010-01-24T10:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1185,"POWERLINKV5_20151103074515","2010-01-24T10:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1186,"POWERLINKV5_20151103074515","2010-01-24T10:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1187,"POWERLINKV5_20151103074515","2010-01-24T10:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1188,"POWERLINKV5_20151103074515","2010-01-24T10:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1189,"POWERLINKV5_20151103074515","2010-01-24T10:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1190,"POWERLINKV5_20151103074515","2010-01-24T10:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1191,"POWERLINKV5_20151103074515","2010-01-24T10:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1192,"POWERLINKV5_20151103074515","2010-01-24T11:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1193,"POWERLINKV5_20151103074515","2010-01-24T11:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1194,"POWERLINKV5_20151103074515","2010-01-24T11:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1195,"POWERLINKV5_20151103074515","2010-01-24T11:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1196,"POWERLINKV5_20151103074515","2010-01-24T11:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1197,"POWERLINKV5_20151103074515","2010-01-24T11:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1198,"POWERLINKV5_20151103074515","2010-01-24T11:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1199,"POWERLINKV5_20151103074515","2010-01-24T11:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1200,"POWERLINKV5_20151103074515","2010-01-24T20:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1201,"POWERLINKV5_20151103074515","2010-01-24T20:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1202,"POWERLINKV5_20151103074515","2010-01-24T21:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1203,"POWERLINKV5_20151103074515","2010-01-24T21:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1204,"POWERLINKV5_20151103074515","2010-01-24T21:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1205,"POWERLINKV5_20151103074515","2010-01-24T21:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1206,"POWERLINKV5_20151103074515","2010-01-24T21:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1207,"POWERLINKV5_20151103074515","2010-01-24T21:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1208,"POWERLINKV5_20151103074515","2010-01-24T21:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.66,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1209,"POWERLINKV5_20151103074515","2010-01-24T21:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1210,"POWERLINKV5_20151103074515","2010-01-24T21:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1211,"POWERLINKV5_20151103074515","2010-01-24T21:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1212,"POWERLINKV5_20151103074515","2010-01-24T21:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1213,"POWERLINKV5_20151103074515","2010-01-24T21:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1214,"POWERLINKV5_20151103074515","2010-01-24T22:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1215,"POWERLINKV5_20151103074515","2010-01-24T22:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.8599999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1216,"POWERLINKV5_20151103074515","2010-01-24T22:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1217,"POWERLINKV5_20151103074515","2010-01-24T22:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1218,"POWERLINKV5_20151103074515","2010-01-24T22:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1219,"POWERLINKV5_20151103074515","2010-01-24T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1220,"POWERLINKV5_20151103074515","2010-01-24T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1221,"POWERLINKV5_20151103074515","2010-01-24T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1222,"POWERLINKV5_20151103074515","2010-01-24T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1223,"POWERLINKV5_20151103074515","2010-01-24T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1224,"POWERLINKV5_20151103074515","2010-01-24T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1225,"POWERLINKV5_20151103074515","2010-01-24T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1226,"POWERLINKV5_20151103074515","2010-01-24T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1227,"POWERLINKV5_20151103074515","2010-01-24T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1228,"POWERLINKV5_20151103074515","2010-01-24T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1229,"POWERLINKV5_20151103074515","2010-01-24T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1230,"POWERLINKV5_20151103074515","2010-01-24T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1231,"POWERLINKV5_20151103074515","2010-01-24T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1232,"POWERLINKV5_20151103074515","2010-01-24T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1233,"POWERLINKV5_20151103074515","2010-01-24T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1234,"POWERLINKV5_20151103074515","2010-01-24T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1235,"POWERLINKV5_20151103074515","2010-01-24T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1236,"POWERLINKV5_20151103074515","2010-01-24T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.28,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1237,"POWERLINKV5_20151103074515","2010-01-24T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1238,"POWERLINKV5_20151103074515","2010-01-25","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1239,"POWERLINKV5_20151103074515","2010-01-25T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.35,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1240,"POWERLINKV5_20151103074515","2010-01-25T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1241,"POWERLINKV5_20151103074515","2010-01-25T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1242,"POWERLINKV5_20151103074515","2010-01-25T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1243,"POWERLINKV5_20151103074515","2010-01-25T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1244,"POWERLINKV5_20151103074515","2010-01-25T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.36,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1245,"POWERLINKV5_20151103074515","2010-01-25T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1246,"POWERLINKV5_20151103074515","2010-01-25T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1247,"POWERLINKV5_20151103074515","2010-01-25T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1248,"POWERLINKV5_20151103074515","2010-01-25T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1249,"POWERLINKV5_20151103074515","2010-01-25T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1250,"POWERLINKV5_20151103074515","2010-01-25T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1251,"POWERLINKV5_20151103074515","2010-01-25T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1252,"POWERLINKV5_20151103074515","2010-01-25T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.34,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1253,"POWERLINKV5_20151103074515","2010-01-25T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1254,"POWERLINKV5_20151103074515","2010-01-25T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1255,"POWERLINKV5_20151103074515","2010-01-25T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1256,"POWERLINKV5_20151103074515","2010-01-25T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1257,"POWERLINKV5_20151103074515","2010-01-25T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1258,"POWERLINKV5_20151103074515","2010-01-25T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1259,"POWERLINKV5_20151103074515","2010-01-25T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1260,"POWERLINKV5_20151103074515","2010-01-25T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.94,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1261,"POWERLINKV5_20151103074515","2010-01-25T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1262,"POWERLINKV5_20151103074515","2010-01-25T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1263,"POWERLINKV5_20151103074515","2010-01-25T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1264,"POWERLINKV5_20151103074515","2010-01-25T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1265,"POWERLINKV5_20151103074515","2010-01-25T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1266,"POWERLINKV5_20151103074515","2010-01-25T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1267,"POWERLINKV5_20151103074515","2010-01-25T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1268,"POWERLINKV5_20151103074515","2010-01-25T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1269,"POWERLINKV5_20151103074515","2010-01-25T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1270,"POWERLINKV5_20151103074515","2010-01-25T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1271,"POWERLINKV5_20151103074515","2010-01-25T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1272,"POWERLINKV5_20151103074515","2010-01-25T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1273,"POWERLINKV5_20151103074515","2010-01-25T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1274,"POWERLINKV5_20151103074515","2010-01-25T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1275,"POWERLINKV5_20151103074515","2010-01-25T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1276,"POWERLINKV5_20151103074515","2010-01-25T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1277,"POWERLINKV5_20151103074515","2010-01-25T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1278,"POWERLINKV5_20151103074515","2010-01-25T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1279,"POWERLINKV5_20151103074515","2010-01-25T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.62,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1280,"POWERLINKV5_20151103074515","2010-01-25T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1013.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1281,"POWERLINKV5_20151103074515","2010-01-25T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1011.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1282,"POWERLINKV5_20151103074515","2010-01-25T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1012.4,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1283,"POWERLINKV5_20151103074515","2010-01-25T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1284,"POWERLINKV5_20151103074515","2010-01-25T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.46,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1285,"POWERLINKV5_20151103074515","2010-01-25T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1286,"POWERLINKV5_20151103074515","2010-01-25T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1287,"POWERLINKV5_20151103074515","2010-01-25T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1015.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1288,"POWERLINKV5_20151103074515","2010-01-25T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.12,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1289,"POWERLINKV5_20151103074515","2010-01-25T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1290,"POWERLINKV5_20151103074515","2010-01-25T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1291,"POWERLINKV5_20151103074515","2010-01-25T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1292,"POWERLINKV5_20151103074515","2010-01-25T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1293,"POWERLINKV5_20151103074515","2010-01-25T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1294,"POWERLINKV5_20151103074515","2010-01-25T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1295,"POWERLINKV5_20151103074515","2010-01-25T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1296,"POWERLINKV5_20151103074515","2010-01-25T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.69,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1297,"POWERLINKV5_20151103074515","2010-01-25T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.69,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1298,"POWERLINKV5_20151103074515","2010-01-25T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1299,"POWERLINKV5_20151103074515","2010-01-25T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1300,"POWERLINKV5_20151103074515","2010-01-25T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.08,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1301,"POWERLINKV5_20151103074515","2010-01-25T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1302,"POWERLINKV5_20151103074515","2010-01-25T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1303,"POWERLINKV5_20151103074515","2010-01-25T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1304,"POWERLINKV5_20151103074515","2010-01-25T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.93,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1305,"POWERLINKV5_20151103074515","2010-01-25T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.76,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1306,"POWERLINKV5_20151103074515","2010-01-25T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1307,"POWERLINKV5_20151103074515","2010-01-25T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1308,"POWERLINKV5_20151103074515","2010-01-25T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1309,"POWERLINKV5_20151103074515","2010-01-25T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1310,"POWERLINKV5_20151103074515","2010-01-25T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1311,"POWERLINKV5_20151103074515","2010-01-25T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1312,"POWERLINKV5_20151103074515","2010-01-25T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1313,"POWERLINKV5_20151103074515","2010-01-25T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1314,"POWERLINKV5_20151103074515","2010-01-25T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1315,"POWERLINKV5_20151103074515","2010-01-25T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1316,"POWERLINKV5_20151103074515","2010-01-25T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1317,"POWERLINKV5_20151103074515","2010-01-25T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1318,"POWERLINKV5_20151103074515","2010-01-25T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1319,"POWERLINKV5_20151103074515","2010-01-25T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.52,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1320,"POWERLINKV5_20151103074515","2010-01-25T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1321,"POWERLINKV5_20151103074515","2010-01-25T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.54,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1322,"POWERLINKV5_20151103074515","2010-01-25T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1323,"POWERLINKV5_20151103074515","2010-01-25T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.73,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1324,"POWERLINKV5_20151103074515","2010-01-25T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1325,"POWERLINKV5_20151103074515","2010-01-25T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.23,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1326,"POWERLINKV5_20151103074515","2010-01-25T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.89,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1327,"POWERLINKV5_20151103074515","2010-01-25T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1328,"POWERLINKV5_20151103074515","2010-01-25T07:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1329,"POWERLINKV5_20151103074515","2010-01-25T07:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1330,"POWERLINKV5_20151103074515","2010-01-25T07:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1331,"POWERLINKV5_20151103074515","2010-01-25T07:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1332,"POWERLINKV5_20151103074515","2010-01-25T07:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1333,"POWERLINKV5_20151103074515","2010-01-25T07:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1334,"POWERLINKV5_20151103074515","2010-01-25T08:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1335,"POWERLINKV5_20151103074515","2010-01-25T08:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.53,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1336,"POWERLINKV5_20151103074515","2010-01-25T08:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.1500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1337,"POWERLINKV5_20151103074515","2010-01-25T08:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1338,"POWERLINKV5_20151103074515","2010-01-25T08:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1339,"POWERLINKV5_20151103074515","2010-01-25T08:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1340,"POWERLINKV5_20151103074515","2010-01-25T08:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1341,"POWERLINKV5_20151103074515","2010-01-25T08:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.4000000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1342,"POWERLINKV5_20151103074515","2010-01-25T08:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1343,"POWERLINKV5_20151103074515","2010-01-25T08:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.4100000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1344,"POWERLINKV5_20151103074515","2010-01-25T08:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1026.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1345,"POWERLINKV5_20151103074515","2010-01-25T08:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1027.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1346,"POWERLINKV5_20151103074515","2010-01-25T09:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1347,"POWERLINKV5_20151103074515","2010-01-25T09:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1348,"POWERLINKV5_20151103074515","2010-01-25T09:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1349,"POWERLINKV5_20151103074515","2010-01-25T09:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1350,"POWERLINKV5_20151103074515","2010-01-25T09:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1351,"POWERLINKV5_20151103074515","2010-01-25T09:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1352,"POWERLINKV5_20151103074515","2010-01-25T09:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1031.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1353,"POWERLINKV5_20151103074515","2010-01-25T09:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.6099999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1354,"POWERLINKV5_20151103074515","2010-01-25T09:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1355,"POWERLINKV5_20151103074515","2010-01-25T09:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1356,"POWERLINKV5_20151103074515","2010-01-25T09:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1357,"POWERLINKV5_20151103074515","2010-01-25T09:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1358,"POWERLINKV5_20151103074515","2010-01-25T21:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1359,"POWERLINKV5_20151103074515","2010-01-25T21:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1030.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1360,"POWERLINKV5_20151103074515","2010-01-25T21:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1361,"POWERLINKV5_20151103074515","2010-01-25T21:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1362,"POWERLINKV5_20151103074515","2010-01-25T21:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.61,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1363,"POWERLINKV5_20151103074515","2010-01-25T21:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.1500000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1364,"POWERLINKV5_20151103074515","2010-01-25T21:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1365,"POWERLINKV5_20151103074515","2010-01-25T21:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1366,"POWERLINKV5_20151103074515","2010-01-25T21:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1367,"POWERLINKV5_20151103074515","2010-01-25T22:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1368,"POWERLINKV5_20151103074515","2010-01-25T22:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.3399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1369,"POWERLINKV5_20151103074515","2010-01-25T22:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1370,"POWERLINKV5_20151103074515","2010-01-25T22:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1371,"POWERLINKV5_20151103074515","2010-01-25T22:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1372,"POWERLINKV5_20151103074515","2010-01-25T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1373,"POWERLINKV5_20151103074515","2010-01-25T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.0899999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1374,"POWERLINKV5_20151103074515","2010-01-25T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1375,"POWERLINKV5_20151103074515","2010-01-25T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1376,"POWERLINKV5_20151103074515","2010-01-25T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1377,"POWERLINKV5_20151103074515","2010-01-25T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.3,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1378,"POWERLINKV5_20151103074515","2010-01-25T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1379,"POWERLINKV5_20151103074515","2010-01-25T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1380,"POWERLINKV5_20151103074515","2010-01-25T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.8599999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1381,"POWERLINKV5_20151103074515","2010-01-25T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.6600000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1382,"POWERLINKV5_20151103074515","2010-01-25T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1028.44,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1383,"POWERLINKV5_20151103074515","2010-01-25T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.8599999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1384,"POWERLINKV5_20151103074515","2010-01-25T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8699999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1385,"POWERLINKV5_20151103074515","2010-01-25T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.31,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1386,"POWERLINKV5_20151103074515","2010-01-25T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1387,"POWERLINKV5_20151103074515","2010-01-25T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.71,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1388,"POWERLINKV5_20151103074515","2010-01-25T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1389,"POWERLINKV5_20151103074515","2010-01-25T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1390,"POWERLINKV5_20151103074515","2010-01-25T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1391,"POWERLINKV5_20151103074515","2010-01-26","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1392,"POWERLINKV5_20151103074515","2010-01-26T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1393,"POWERLINKV5_20151103074515","2010-01-26T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.96,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1394,"POWERLINKV5_20151103074515","2010-01-26T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.6,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1395,"POWERLINKV5_20151103074515","2010-01-26T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1396,"POWERLINKV5_20151103074515","2010-01-26T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1397,"POWERLINKV5_20151103074515","2010-01-26T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1398,"POWERLINKV5_20151103074515","2010-01-26T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1399,"POWERLINKV5_20151103074515","2010-01-26T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1400,"POWERLINKV5_20151103074515","2010-01-26T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.55,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1401,"POWERLINKV5_20151103074515","2010-01-26T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.56,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1402,"POWERLINKV5_20151103074515","2010-01-26T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1403,"POWERLINKV5_20151103074515","2010-01-26T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1404,"POWERLINKV5_20151103074515","2010-01-26T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1405,"POWERLINKV5_20151103074515","2010-01-26T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1406,"POWERLINKV5_20151103074515","2010-01-26T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1407,"POWERLINKV5_20151103074515","2010-01-26T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1408,"POWERLINKV5_20151103074515","2010-01-26T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1409,"POWERLINKV5_20151103074515","2010-01-26T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.22,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1410,"POWERLINKV5_20151103074515","2010-01-26T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1411,"POWERLINKV5_20151103074515","2010-01-26T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1412,"POWERLINKV5_20151103074515","2010-01-26T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1413,"POWERLINKV5_20151103074515","2010-01-26T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1414,"POWERLINKV5_20151103074515","2010-01-26T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1415,"POWERLINKV5_20151103074515","2010-01-26T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.34,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1416,"POWERLINKV5_20151103074515","2010-01-26T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1417,"POWERLINKV5_20151103074515","2010-01-26T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1418,"POWERLINKV5_20151103074515","2010-01-26T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1419,"POWERLINKV5_20151103074515","2010-01-26T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.04,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1420,"POWERLINKV5_20151103074515","2010-01-26T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1421,"POWERLINKV5_20151103074515","2010-01-26T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.59,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1422,"POWERLINKV5_20151103074515","2010-01-26T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1423,"POWERLINKV5_20151103074515","2010-01-26T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.21,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1424,"POWERLINKV5_20151103074515","2010-01-26T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1425,"POWERLINKV5_20151103074515","2010-01-26T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1426,"POWERLINKV5_20151103074515","2010-01-26T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1427,"POWERLINKV5_20151103074515","2010-01-26T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.74,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1428,"POWERLINKV5_20151103074515","2010-01-26T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1429,"POWERLINKV5_20151103074515","2010-01-26T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1430,"POWERLINKV5_20151103074515","2010-01-26T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1431,"POWERLINKV5_20151103074515","2010-01-26T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1432,"POWERLINKV5_20151103074515","2010-01-26T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1433,"POWERLINKV5_20151103074515","2010-01-26T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.19,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1434,"POWERLINKV5_20151103074515","2010-01-26T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1435,"POWERLINKV5_20151103074515","2010-01-26T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1436,"POWERLINKV5_20151103074515","2010-01-26T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1437,"POWERLINKV5_20151103074515","2010-01-26T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1438,"POWERLINKV5_20151103074515","2010-01-26T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1439,"POWERLINKV5_20151103074515","2010-01-26T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.11,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1440,"POWERLINKV5_20151103074515","2010-01-26T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1441,"POWERLINKV5_20151103074515","2010-01-26T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.75,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1442,"POWERLINKV5_20151103074515","2010-01-26T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.88,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1443,"POWERLINKV5_20151103074515","2010-01-26T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1444,"POWERLINKV5_20151103074515","2010-01-26T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1445,"POWERLINKV5_20151103074515","2010-01-26T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1446,"POWERLINKV5_20151103074515","2010-01-26T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.17,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1447,"POWERLINKV5_20151103074515","2010-01-26T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1448,"POWERLINKV5_20151103074515","2010-01-26T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1449,"POWERLINKV5_20151103074515","2010-01-26T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.16,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1450,"POWERLINKV5_20151103074515","2010-01-26T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1451,"POWERLINKV5_20151103074515","2010-01-26T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1452,"POWERLINKV5_20151103074515","2010-01-26T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.87,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1453,"POWERLINKV5_20151103074515","2010-01-26T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.26,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1454,"POWERLINKV5_20151103074515","2010-01-26T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.2,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1455,"POWERLINKV5_20151103074515","2010-01-26T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1456,"POWERLINKV5_20151103074515","2010-01-26T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.01,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1457,"POWERLINKV5_20151103074515","2010-01-26T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1458,"POWERLINKV5_20151103074515","2010-01-26T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.72,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1459,"POWERLINKV5_20151103074515","2010-01-26T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1460,"POWERLINKV5_20151103074515","2010-01-26T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1461,"POWERLINKV5_20151103074515","2010-01-26T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.4,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1462,"POWERLINKV5_20151103074515","2010-01-26T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.45,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1463,"POWERLINKV5_20151103074515","2010-01-26T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1464,"POWERLINKV5_20151103074515","2010-01-26T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1016.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1465,"POWERLINKV5_20151103074515","2010-01-26T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1017.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1466,"POWERLINKV5_20151103074515","2010-01-26T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1467,"POWERLINKV5_20151103074515","2010-01-26T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1468,"POWERLINKV5_20151103074515","2010-01-26T06:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1469,"POWERLINKV5_20151103074515","2010-01-26T06:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1470,"POWERLINKV5_20151103074515","2010-01-26T06:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.07,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1471,"POWERLINKV5_20151103074515","2010-01-26T06:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1472,"POWERLINKV5_20151103074515","2010-01-26T06:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.13,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1473,"POWERLINKV5_20151103074515","2010-01-26T06:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1474,"POWERLINKV5_20151103074515","2010-01-26T06:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.06,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1475,"POWERLINKV5_20151103074515","2010-01-26T07:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.24,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1476,"POWERLINKV5_20151103074515","2010-01-26T07:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1477,"POWERLINKV5_20151103074515","2010-01-26T07:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1478,"POWERLINKV5_20151103074515","2010-01-26T07:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1479,"POWERLINKV5_20151103074515","2010-01-26T07:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.02,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1480,"POWERLINKV5_20151103074515","2010-01-26T07:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1481,"POWERLINKV5_20151103074515","2010-01-26T07:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1482,"POWERLINKV5_20151103074515","2010-01-26T22:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.8900000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1483,"POWERLINKV5_20151103074515","2010-01-26T22:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1484,"POWERLINKV5_20151103074515","2010-01-26T22:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1485,"POWERLINKV5_20151103074515","2010-01-26T22:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.6400000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1486,"POWERLINKV5_20151103074515","2010-01-26T22:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.6300000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1487,"POWERLINKV5_20151103074515","2010-01-26T22:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1029.42,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1488,"POWERLINKV5_20151103074515","2010-01-26T22:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1489,"POWERLINKV5_20151103074515","2010-01-26T23:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.39,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1490,"POWERLINKV5_20151103074515","2010-01-26T23:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1491,"POWERLINKV5_20151103074515","2010-01-26T23:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1025.1199999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1492,"POWERLINKV5_20151103074515","2010-01-26T23:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.8800000000001,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1493,"POWERLINKV5_20151103074515","2010-01-26T23:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1494,"POWERLINKV5_20151103074515","2010-01-26T23:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1495,"POWERLINKV5_20151103074515","2010-01-26T23:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1496,"POWERLINKV5_20151103074515","2010-01-26T23:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1497,"POWERLINKV5_20151103074515","2010-01-26T23:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1024.3399999999999,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1498,"POWERLINKV5_20151103074515","2010-01-26T23:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1499,"POWERLINKV5_20151103074515","2010-01-26T23:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1500,"POWERLINKV5_20151103074515","2010-01-26T23:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1501,"POWERLINKV5_20151103074515","2010-01-27","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1502,"POWERLINKV5_20151103074515","2010-01-27T00:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1503,"POWERLINKV5_20151103074515","2010-01-27T00:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1504,"POWERLINKV5_20151103074515","2010-01-27T00:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1505,"POWERLINKV5_20151103074515","2010-01-27T00:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.48,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1506,"POWERLINKV5_20151103074515","2010-01-27T00:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.57,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1507,"POWERLINKV5_20151103074515","2010-01-27T00:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.35,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1508,"POWERLINKV5_20151103074515","2010-01-27T00:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.92,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1509,"POWERLINKV5_20151103074515","2010-01-27T00:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.9,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1510,"POWERLINKV5_20151103074515","2010-01-27T00:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1511,"POWERLINKV5_20151103074515","2010-01-27T00:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1512,"POWERLINKV5_20151103074515","2010-01-27T00:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1513,"POWERLINKV5_20151103074515","2010-01-27T01:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1514,"POWERLINKV5_20151103074515","2010-01-27T01:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1515,"POWERLINKV5_20151103074515","2010-01-27T01:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1516,"POWERLINKV5_20151103074515","2010-01-27T01:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.64,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1517,"POWERLINKV5_20151103074515","2010-01-27T01:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.65,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1518,"POWERLINKV5_20151103074515","2010-01-27T01:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.43,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1519,"POWERLINKV5_20151103074515","2010-01-27T01:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1520,"POWERLINKV5_20151103074515","2010-01-27T01:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1521,"POWERLINKV5_20151103074515","2010-01-27T01:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.8,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1522,"POWERLINKV5_20151103074515","2010-01-27T01:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.95,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1523,"POWERLINKV5_20151103074515","2010-01-27T01:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1524,"POWERLINKV5_20151103074515","2010-01-27T01:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.09,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1525,"POWERLINKV5_20151103074515","2010-01-27T02:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.7,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1526,"POWERLINKV5_20151103074515","2010-01-27T02:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1527,"POWERLINKV5_20151103074515","2010-01-27T02:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1528,"POWERLINKV5_20151103074515","2010-01-27T02:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1529,"POWERLINKV5_20151103074515","2010-01-27T02:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1530,"POWERLINKV5_20151103074515","2010-01-27T02:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1531,"POWERLINKV5_20151103074515","2010-01-27T02:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1532,"POWERLINKV5_20151103074515","2010-01-27T02:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1533,"POWERLINKV5_20151103074515","2010-01-27T02:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1534,"POWERLINKV5_20151103074515","2010-01-27T02:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.15,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1535,"POWERLINKV5_20151103074515","2010-01-27T02:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1536,"POWERLINKV5_20151103074515","2010-01-27T02:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1537,"POWERLINKV5_20151103074515","2010-01-27T03:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.41,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1538,"POWERLINKV5_20151103074515","2010-01-27T03:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1539,"POWERLINKV5_20151103074515","2010-01-27T03:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.85,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1540,"POWERLINKV5_20151103074515","2010-01-27T03:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.05,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1541,"POWERLINKV5_20151103074515","2010-01-27T03:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1542,"POWERLINKV5_20151103074515","2010-01-27T03:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1543,"POWERLINKV5_20151103074515","2010-01-27T03:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.78,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1544,"POWERLINKV5_20151103074515","2010-01-27T03:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.84,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1545,"POWERLINKV5_20151103074515","2010-01-27T03:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.97,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1546,"POWERLINKV5_20151103074515","2010-01-27T03:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1547,"POWERLINKV5_20151103074515","2010-01-27T03:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1548,"POWERLINKV5_20151103074515","2010-01-27T03:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.83,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1549,"POWERLINKV5_20151103074515","2010-01-27T04:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.03,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1550,"POWERLINKV5_20151103074515","2010-01-27T04:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1018.98,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1551,"POWERLINKV5_20151103074515","2010-01-27T04:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.51,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1552,"POWERLINKV5_20151103074515","2010-01-27T04:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.5,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1553,"POWERLINKV5_20151103074515","2010-01-27T04:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.49,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1554,"POWERLINKV5_20151103074515","2010-01-27T04:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1555,"POWERLINKV5_20151103074515","2010-01-27T04:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1019.68,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1556,"POWERLINKV5_20151103074515","2010-01-27T04:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1557,"POWERLINKV5_20151103074515","2010-01-27T04:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1558,"POWERLINKV5_20151103074515","2010-01-27T04:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.33,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1559,"POWERLINKV5_20151103074515","2010-01-27T04:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.25,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1560,"POWERLINKV5_20151103074515","2010-01-27T04:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.18,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1561,"POWERLINKV5_20151103074515","2010-01-27T05:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1562,"POWERLINKV5_20151103074515","2010-01-27T05:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1563,"POWERLINKV5_20151103074515","2010-01-27T05:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1564,"POWERLINKV5_20151103074515","2010-01-27T05:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1565,"POWERLINKV5_20151103074515","2010-01-27T05:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.38,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1566,"POWERLINKV5_20151103074515","2010-01-27T05:25:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.47,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1567,"POWERLINKV5_20151103074515","2010-01-27T05:30:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1568,"POWERLINKV5_20151103074515","2010-01-27T05:35:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1569,"POWERLINKV5_20151103074515","2010-01-27T05:40:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.58,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1570,"POWERLINKV5_20151103074515","2010-01-27T05:45:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.77,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1571,"POWERLINKV5_20151103074515","2010-01-27T05:50:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.63,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1572,"POWERLINKV5_20151103074515","2010-01-27T05:55:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.79,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1573,"POWERLINKV5_20151103074515","2010-01-27T06:00:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1023.34,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1574,"POWERLINKV5_20151103074515","2010-01-27T06:05:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.14,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1575,"POWERLINKV5_20151103074515","2010-01-27T06:10:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1020.86,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1576,"POWERLINKV5_20151103074515","2010-01-27T06:15:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1021.99,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1577,"POWERLINKV5_20151103074515","2010-01-27T06:20:00","Q>NIL_CNTR_CNTR","Q-NIL","2010-01-15",1,1022.32,"Out= Nil, Ergon relay limit on Chinchilla to Tarong 132kV lines, for the contingent loss of a single Chinchilla to Tarong 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1578,"POWERLINKV5_20151103074515","2010-01-27T12:15:00","QNTE_ROC","Q-NIL","2006-01-27",1,199971.54,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1579,"POWERLINKV5_20151103074515","2010-01-28T13:05:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,31.67,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1580,"POWERLINKV5_20151103074515","2010-01-28T13:10:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,31.67,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1581,"POWERLINKV5_20151103074515","2010-01-28T13:15:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,30.75,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1582,"POWERLINKV5_20151103074515","2010-01-28T13:20:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,28.22,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1583,"POWERLINKV5_20151103074515","2010-01-28T13:25:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,31.67,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1584,"POWERLINKV5_20151103074515","2010-01-28T13:30:00","Q>MRTA","Q-NIL_MRTA","2007-01-14",1,28.22,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1585,"POWERLINKV5_20151103074515","2010-01-30T06:40:00","Q>>NIL_855_871","Q-NIL","2009-01-15",2,10.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1586,"POWERLINKV5_20151103074515","2010-01-31T17:15:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-6338.42,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1587,"POWERLINKV5_20151103074515","2010-01-31T17:20:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-6353.41,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1588,"POWERLINKV5_20151103074515","2010-01-31T19:30:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4229.57,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1589,"POWERLINKV5_20151103074515","2010-01-31T19:35:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4231.6899999999996,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1590,"POWERLINKV5_20151103074515","2010-01-31T19:40:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4229.59,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1591,"POWERLINKV5_20151103074515","2010-01-31T19:45:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4231.6899999999996,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1592,"POWERLINKV5_20151103074515","2010-01-31T19:50:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4228.6499999999996,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1593,"POWERLINKV5_20151103074515","2010-02-04T03:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.59,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1594,"POWERLINKV5_20151103074515","2010-02-04T03:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1595,"POWERLINKV5_20151103074515","2010-02-04T04:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.33,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1596,"POWERLINKV5_20151103074515","2010-02-04T19:15:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4218.78,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1597,"POWERLINKV5_20151103074515","2010-02-04T19:20:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4217.87,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1598,"POWERLINKV5_20151103074515","2010-02-04T19:25:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4229.3900000000003,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1599,"POWERLINKV5_20151103074515","2010-02-04T19:30:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-13514.98,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1600,"POWERLINKV5_20151103074515","2010-02-05T01:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1601,"POWERLINKV5_20151103074515","2010-02-05T01:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1602,"POWERLINKV5_20151103074515","2010-02-05T01:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1603,"POWERLINKV5_20151103074515","2010-02-05T03:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1604,"POWERLINKV5_20151103074515","2010-02-05T03:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.72,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1605,"POWERLINKV5_20151103074515","2010-02-05T03:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1606,"POWERLINKV5_20151103074515","2010-02-05T03:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1607,"POWERLINKV5_20151103074515","2010-02-05T03:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1608,"POWERLINKV5_20151103074515","2010-02-05T04:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.71,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1609,"POWERLINKV5_20151103074515","2010-02-05T04:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1610,"POWERLINKV5_20151103074515","2010-02-05T04:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.2,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1611,"POWERLINKV5_20151103074515","2010-02-05T11:55:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,10.77,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1612,"POWERLINKV5_20151103074515","2010-02-05T12:05:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.29,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1613,"POWERLINKV5_20151103074515","2010-02-05T12:10:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.66,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1614,"POWERLINKV5_20151103074515","2010-02-05T12:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.54,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1615,"POWERLINKV5_20151103074515","2010-02-05T12:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.89,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1616,"POWERLINKV5_20151103074515","2010-02-05T12:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,10.74,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1617,"POWERLINKV5_20151103074515","2010-02-05T12:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.46,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1618,"POWERLINKV5_20151103074515","2010-02-05T12:35:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.63,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1619,"POWERLINKV5_20151103074515","2010-02-05T12:45:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.54,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1620,"POWERLINKV5_20151103074515","2010-02-05T12:50:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,10.72,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1621,"POWERLINKV5_20151103074515","2010-02-05T12:55:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,12.06,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1622,"POWERLINKV5_20151103074515","2010-02-05T13:00:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.55,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1623,"POWERLINKV5_20151103074515","2010-02-05T13:05:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.59,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1624,"POWERLINKV5_20151103074515","2010-02-05T13:10:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,21.01,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1625,"POWERLINKV5_20151103074515","2010-02-05T13:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,12.45,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1626,"POWERLINKV5_20151103074515","2010-02-05T13:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.58,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1627,"POWERLINKV5_20151103074515","2010-02-05T13:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,11.56,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1628,"POWERLINKV5_20151103074515","2010-02-05T13:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,13.65,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1629,"POWERLINKV5_20151103074515","2010-02-05T13:40:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-05",2,12.93,"N-Q-MNSP1.ENERGY * -1 >= 125 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30139.","UNPLANNED",0]
[1630,"POWERLINKV5_20151103074515","2010-02-07T19:20:00","Q^NIL_FNQ","Q-NIL","2009-12-17",1,69653.600000000006,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1631,"POWERLINKV5_20151103074515","2010-02-07T19:45:00","Q^NIL_FNQ","Q-NIL","2009-12-17",1,69655,"Out=Nil, Far North Qld Voltage Stability limit for loss of either Chalumbin to Ross (857 or 858) 275kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1632,"POWERLINKV5_20151103074515","2010-02-07T20:10:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-3126.38,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1633,"POWERLINKV5_20151103074515","2010-02-07T20:15:00","Q>NIL_SMRS_CVCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-3119.87,"Out= Nil, avoid O/L T37 Collinsville Tee T177 King Creek to T193 Clare South (7128) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1634,"POWERLINKV5_20151103074515","2010-02-10T05:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.54,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1635,"POWERLINKV5_20151103074515","2010-02-11T04:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.25,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1636,"POWERLINKV5_20151103074515","2010-02-11T14:30:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-1143.28,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1637,"POWERLINKV5_20151103074515","2010-02-11T14:30:00","QNTE_ROC","Q-NIL","2006-12-27",1,-25.16,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1638,"POWERLINKV5_20151103074515","2010-02-11T14:35:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-1148.4000000000001,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1639,"POWERLINKV5_20151103074515","2010-02-11T14:35:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-21.79,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1640,"POWERLINKV5_20151103074515","2010-02-11T14:40:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-787.78,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1641,"POWERLINKV5_20151103074515","2010-02-11T14:45:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-834.46,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1642,"POWERLINKV5_20151103074515","2010-02-11T14:50:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-825.95,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1643,"POWERLINKV5_20151103074515","2010-02-11T14:55:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-833.69,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1644,"POWERLINKV5_20151103074515","2010-02-11T15:00:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-3125.26,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1645,"POWERLINKV5_20151103074515","2010-02-11T15:05:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-1059.78,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1646,"POWERLINKV5_20151103074515","2010-02-11T15:10:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-1172.8900000000001,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1647,"POWERLINKV5_20151103074515","2010-02-11T15:15:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-1053.94,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1648,"POWERLINKV5_20151103074515","2010-02-11T15:20:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-655.33000000000004,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1649,"POWERLINKV5_20151103074515","2010-02-11T15:25:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-655.89,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1650,"POWERLINKV5_20151103074515","2010-02-11T15:35:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-999.44,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1651,"POWERLINKV5_20151103074515","2010-02-11T15:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-68.349999999999994," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1652,"POWERLINKV5_20151103074515","2010-02-11T15:35:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-108.02,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1653,"POWERLINKV5_20151103074515","2010-02-11T15:40:00","#QLD1_E_20100211","#QLD1_E_20100211","2010-02-11",5,-317.58999999999997,"Multiple QLD1 LHS <= -50 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30310.","UNPLANNED",0]
[1654,"POWERLINKV5_20151103074515","2010-02-11T15:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-14.45," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1655,"POWERLINKV5_20151103074515","2010-02-12T05:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.26,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1656,"POWERLINKV5_20151103074515","2010-02-12T05:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1657,"POWERLINKV5_20151103074515","2010-02-12T05:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1658,"POWERLINKV5_20151103074515","2010-02-12T05:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.25,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1659,"POWERLINKV5_20151103074515","2010-02-12T11:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-492.92,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1660,"POWERLINKV5_20151103074515","2010-02-12T11:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-165.05,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1661,"POWERLINKV5_20151103074515","2010-02-12T11:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-139.54,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1662,"POWERLINKV5_20151103074515","2010-02-12T11:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-1165.27,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1663,"POWERLINKV5_20151103074515","2010-02-12T11:25:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-13.48,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1664,"POWERLINKV5_20151103074515","2010-02-12T11:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-1231.29,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1665,"POWERLINKV5_20151103074515","2010-02-12T11:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-1181,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1666,"POWERLINKV5_20151103074515","2010-02-12T11:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-915.61,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1667,"POWERLINKV5_20151103074515","2010-02-12T11:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-915.62,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1668,"POWERLINKV5_20151103074515","2010-02-12T11:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-839.66,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1669,"POWERLINKV5_20151103074515","2010-02-12T11:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-730.65,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1670,"POWERLINKV5_20151103074515","2010-02-12T12:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-414.38,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1671,"POWERLINKV5_20151103074515","2010-02-12T12:05:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-850.75,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1672,"POWERLINKV5_20151103074515","2010-02-12T12:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-937.08,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1673,"POWERLINKV5_20151103074515","2010-02-12T12:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-1012.29,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1674,"POWERLINKV5_20151103074515","2010-02-12T12:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-845.89,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1675,"POWERLINKV5_20151103074515","2010-02-12T12:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-839.93,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1676,"POWERLINKV5_20151103074515","2010-02-12T12:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-840.04,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1677,"POWERLINKV5_20151103074515","2010-02-12T12:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-447.8,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1678,"POWERLINKV5_20151103074515","2010-02-12T12:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-845.4,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1679,"POWERLINKV5_20151103074515","2010-02-12T12:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-181.58,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1680,"POWERLINKV5_20151103074515","2010-02-12T12:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-180.32,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1681,"POWERLINKV5_20151103074515","2010-02-12T12:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-145.94999999999999,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1682,"POWERLINKV5_20151103074515","2010-02-12T13:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-126.04,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1683,"POWERLINKV5_20151103074515","2010-02-12T13:05:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-134.26,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1684,"POWERLINKV5_20151103074515","2010-02-12T13:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-94.74,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1685,"POWERLINKV5_20151103074515","2010-02-12T13:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-115.97,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1686,"POWERLINKV5_20151103074515","2010-02-12T13:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-337.27,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1687,"POWERLINKV5_20151103074515","2010-02-12T13:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-95.1,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1688,"POWERLINKV5_20151103074515","2010-02-12T13:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-131.32,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1689,"POWERLINKV5_20151103074515","2010-02-12T13:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-83.82,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1690,"POWERLINKV5_20151103074515","2010-02-12T13:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-138.05000000000001,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1691,"POWERLINKV5_20151103074515","2010-02-12T13:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-77.349999999999994,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1692,"POWERLINKV5_20151103074515","2010-02-12T13:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-77.819999999999993,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1693,"POWERLINKV5_20151103074515","2010-02-12T13:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-171.15,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1694,"POWERLINKV5_20151103074515","2010-02-12T14:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-81.61,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1695,"POWERLINKV5_20151103074515","2010-02-12T14:05:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-598.38,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1696,"POWERLINKV5_20151103074515","2010-02-12T14:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-620.63,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1697,"POWERLINKV5_20151103074515","2010-02-12T14:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-728.64,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1698,"POWERLINKV5_20151103074515","2010-02-12T14:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-342.11,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1699,"POWERLINKV5_20151103074515","2010-02-12T14:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-130.74,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1700,"POWERLINKV5_20151103074515","2010-02-12T14:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-341.81,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1701,"POWERLINKV5_20151103074515","2010-02-12T14:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-381.56,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1702,"POWERLINKV5_20151103074515","2010-02-12T14:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-158.44999999999999,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1703,"POWERLINKV5_20151103074515","2010-02-12T14:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-90.68,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1704,"POWERLINKV5_20151103074515","2010-02-12T14:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-59.92,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1705,"POWERLINKV5_20151103074515","2010-02-12T14:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-28.07,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1706,"POWERLINKV5_20151103074515","2010-02-12T15:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-37.08,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1707,"POWERLINKV5_20151103074515","2010-02-12T15:05:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-85.86,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1708,"POWERLINKV5_20151103074515","2010-02-12T15:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-209.88,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1709,"POWERLINKV5_20151103074515","2010-02-12T15:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-68.75,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1710,"POWERLINKV5_20151103074515","2010-02-12T15:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-209.94,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1711,"POWERLINKV5_20151103074515","2010-02-12T15:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-64.510000000000005,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1712,"POWERLINKV5_20151103074515","2010-02-12T15:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-101.33,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1713,"POWERLINKV5_20151103074515","2010-02-12T15:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-73.17,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1714,"POWERLINKV5_20151103074515","2010-02-12T15:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-120.78,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1715,"POWERLINKV5_20151103074515","2010-02-12T15:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-67.17,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1716,"POWERLINKV5_20151103074515","2010-02-12T15:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-75.58,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1717,"POWERLINKV5_20151103074515","2010-02-12T15:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-85.72,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1718,"POWERLINKV5_20151103074515","2010-02-12T16:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-210.04,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1719,"POWERLINKV5_20151103074515","2010-02-12T16:05:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-211.2,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1720,"POWERLINKV5_20151103074515","2010-02-12T16:10:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-362.9,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1721,"POWERLINKV5_20151103074515","2010-02-12T16:15:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-405.77,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1722,"POWERLINKV5_20151103074515","2010-02-12T16:20:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-80.39,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1723,"POWERLINKV5_20151103074515","2010-02-12T16:25:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-341.18,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1724,"POWERLINKV5_20151103074515","2010-02-12T16:30:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-390.09,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1725,"POWERLINKV5_20151103074515","2010-02-12T16:35:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-389.96,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1726,"POWERLINKV5_20151103074515","2010-02-12T16:40:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-389.99,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1727,"POWERLINKV5_20151103074515","2010-02-12T16:45:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-744.1,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1728,"POWERLINKV5_20151103074515","2010-02-12T16:50:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-57.91,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1729,"POWERLINKV5_20151103074515","2010-02-12T16:55:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-14.58,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1730,"POWERLINKV5_20151103074515","2010-02-12T17:00:00","#QLD1_E_20100212","#QLD1_E_20100212","2010-02-12",4,-13.29,"Multiple QLD1 LHS <= 0 (Wt = 4)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due Negative Settlement Residues. Refer to Maket Notice 30333.","UNPLANNED",0]
[1731,"POWERLINKV5_20151103074515","2010-02-14T08:20:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76054.98,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1732,"POWERLINKV5_20151103074515","2010-02-14T08:25:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76049.97,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1733,"POWERLINKV5_20151103074515","2010-02-14T20:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-13.75," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1734,"POWERLINKV5_20151103074515","2010-02-15T09:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,17.670000000000002,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1735,"POWERLINKV5_20151103074515","2010-02-15T09:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.91," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1736,"POWERLINKV5_20151103074515","2010-02-15T09:35:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,23.88,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1737,"POWERLINKV5_20151103074515","2010-02-15T09:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-22.07," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1738,"POWERLINKV5_20151103074515","2010-02-15T09:40:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,12.86,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1739,"POWERLINKV5_20151103074515","2010-02-15T09:45:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,18.420000000000002,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1740,"POWERLINKV5_20151103074515","2010-02-15T09:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.91," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1741,"POWERLINKV5_20151103074515","2010-02-15T09:50:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.52,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1742,"POWERLINKV5_20151103074515","2010-02-15T09:55:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,12.22,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1743,"POWERLINKV5_20151103074515","2010-02-15T10:00:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.62,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1744,"POWERLINKV5_20151103074515","2010-02-15T10:05:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.83,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1745,"POWERLINKV5_20151103074515","2010-02-15T10:10:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.93,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1746,"POWERLINKV5_20151103074515","2010-02-15T10:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.48,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1747,"POWERLINKV5_20151103074515","2010-02-15T10:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.04,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1748,"POWERLINKV5_20151103074515","2010-02-15T10:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,12.56,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1749,"POWERLINKV5_20151103074515","2010-02-15T10:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,14.11,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1750,"POWERLINKV5_20151103074515","2010-02-15T10:35:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,13.76,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1751,"POWERLINKV5_20151103074515","2010-02-15T10:40:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,14.03,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1752,"POWERLINKV5_20151103074515","2010-02-15T10:45:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-02-15",3,12.81,"N-Q-MNSP1. * -1 >= 146 (Wt = 20)","OUTAGE","OTHER","Unknown","REGULATED","99","AEMO invoked constraint due to issues in NSW. Refer to Maket Notice 30382.","UNPLANNED",0]
[1753,"POWERLINKV5_20151103074515","2010-02-16T14:05:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75997.38,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1754,"POWERLINKV5_20151103074515","2010-02-17T22:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.059999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1755,"POWERLINKV5_20151103074515","2010-02-17T23:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1756,"POWERLINKV5_20151103074515","2010-02-17T23:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1757,"POWERLINKV5_20151103074515","2010-02-17T23:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.91,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1758,"POWERLINKV5_20151103074515","2010-02-17T23:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.88,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1759,"POWERLINKV5_20151103074515","2010-02-18","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.92,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1760,"POWERLINKV5_20151103074515","2010-02-18T00:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1761,"POWERLINKV5_20151103074515","2010-02-18T00:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1762,"POWERLINKV5_20151103074515","2010-02-18T00:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1763,"POWERLINKV5_20151103074515","2010-02-18T00:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.8,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1764,"POWERLINKV5_20151103074515","2010-02-18T00:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.809999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1765,"POWERLINKV5_20151103074515","2010-02-18T00:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.91,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1766,"POWERLINKV5_20151103074515","2010-02-18T00:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1767,"POWERLINKV5_20151103074515","2010-02-18T00:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.16,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1768,"POWERLINKV5_20151103074515","2010-02-18T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1769,"POWERLINKV5_20151103074515","2010-02-18T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.29,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1770,"POWERLINKV5_20151103074515","2010-02-18T01:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.27,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1771,"POWERLINKV5_20151103074515","2010-02-18T01:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.22,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1772,"POWERLINKV5_20151103074515","2010-02-18T01:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1773,"POWERLINKV5_20151103074515","2010-02-18T01:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.27,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1774,"POWERLINKV5_20151103074515","2010-02-18T01:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.420000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1775,"POWERLINKV5_20151103074515","2010-02-18T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1776,"POWERLINKV5_20151103074515","2010-02-18T01:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-18.420000000000002,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1777,"POWERLINKV5_20151103074515","2010-02-18T01:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.16,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1778,"POWERLINKV5_20151103074515","2010-02-18T02:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.05,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1779,"POWERLINKV5_20151103074515","2010-02-18T02:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.38,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1780,"POWERLINKV5_20151103074515","2010-02-18T02:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.19,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1781,"POWERLINKV5_20151103074515","2010-02-18T02:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1782,"POWERLINKV5_20151103074515","2010-02-18T02:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1783,"POWERLINKV5_20151103074515","2010-02-18T02:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.81,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1784,"POWERLINKV5_20151103074515","2010-02-18T02:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.92,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1785,"POWERLINKV5_20151103074515","2010-02-18T02:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.4,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1786,"POWERLINKV5_20151103074515","2010-02-18T02:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.05,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1787,"POWERLINKV5_20151103074515","2010-02-18T03:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1788,"POWERLINKV5_20151103074515","2010-02-18T03:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1789,"POWERLINKV5_20151103074515","2010-02-18T03:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.29,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1790,"POWERLINKV5_20151103074515","2010-02-18T03:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1791,"POWERLINKV5_20151103074515","2010-02-18T03:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.29,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1792,"POWERLINKV5_20151103074515","2010-02-18T03:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.91,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1793,"POWERLINKV5_20151103074515","2010-02-18T04:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.03,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1794,"POWERLINKV5_20151103074515","2010-02-18T04:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1795,"POWERLINKV5_20151103074515","2010-02-18T04:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.37,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1796,"POWERLINKV5_20151103074515","2010-02-18T04:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-19.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1797,"POWERLINKV5_20151103074515","2010-02-18T04:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.37,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1798,"POWERLINKV5_20151103074515","2010-02-18T04:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.13,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1799,"POWERLINKV5_20151103074515","2010-02-18T04:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.83,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1800,"POWERLINKV5_20151103074515","2010-02-18T04:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.85,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1801,"POWERLINKV5_20151103074515","2010-02-18T04:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.04,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1802,"POWERLINKV5_20151103074515","2010-02-18T04:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1803,"POWERLINKV5_20151103074515","2010-02-18T04:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.93,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1804,"POWERLINKV5_20151103074515","2010-02-18T04:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.29,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1805,"POWERLINKV5_20151103074515","2010-02-18T05:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1806,"POWERLINKV5_20151103074515","2010-02-18T05:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-27.75,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1807,"POWERLINKV5_20151103074515","2010-02-18T05:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.55,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1808,"POWERLINKV5_20151103074515","2010-02-19T04:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1809,"POWERLINKV5_20151103074515","2010-02-19T04:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.83,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1810,"POWERLINKV5_20151103074515","2010-02-19T12:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.27,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1811,"POWERLINKV5_20151103074515","2010-02-19T12:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.64,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1812,"POWERLINKV5_20151103074515","2010-02-19T13:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.1,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1813,"POWERLINKV5_20151103074515","2010-02-19T13:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.26,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1814,"POWERLINKV5_20151103074515","2010-02-19T13:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.44,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1815,"POWERLINKV5_20151103074515","2010-02-19T13:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.420000000000002,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1816,"POWERLINKV5_20151103074515","2010-02-19T13:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1817,"POWERLINKV5_20151103074515","2010-02-19T13:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1818,"POWERLINKV5_20151103074515","2010-02-19T13:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.33,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1819,"POWERLINKV5_20151103074515","2010-02-19T13:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1820,"POWERLINKV5_20151103074515","2010-02-19T13:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1821,"POWERLINKV5_20151103074515","2010-02-19T13:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.95,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1822,"POWERLINKV5_20151103074515","2010-02-19T13:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1823,"POWERLINKV5_20151103074515","2010-02-19T14:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1824,"POWERLINKV5_20151103074515","2010-02-19T14:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.37,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1825,"POWERLINKV5_20151103074515","2010-02-19T23:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1826,"POWERLINKV5_20151103074515","2010-02-20T00:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.26,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1827,"POWERLINKV5_20151103074515","2010-02-20T00:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1828,"POWERLINKV5_20151103074515","2010-02-20T01:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1829,"POWERLINKV5_20151103074515","2010-02-20T01:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.6,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1830,"POWERLINKV5_20151103074515","2010-02-20T01:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.3,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1831,"POWERLINKV5_20151103074515","2010-02-20T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1832,"POWERLINKV5_20151103074515","2010-02-20T04:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1833,"POWERLINKV5_20151103074515","2010-02-20T06:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1834,"POWERLINKV5_20151103074515","2010-02-20T06:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.05,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1835,"POWERLINKV5_20151103074515","2010-02-20T06:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1836,"POWERLINKV5_20151103074515","2010-02-20T19:35:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-504.45,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1837,"POWERLINKV5_20151103074515","2010-02-20T19:40:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-503.93,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1838,"POWERLINKV5_20151103074515","2010-02-21T14:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1839,"POWERLINKV5_20151103074515","2010-02-21T14:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1840,"POWERLINKV5_20151103074515","2010-02-21T19:05:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-4232.12,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1841,"POWERLINKV5_20151103074515","2010-02-22T05:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.19,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1842,"POWERLINKV5_20151103074515","2010-02-22T09:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1843,"POWERLINKV5_20151103074515","2010-02-22T09:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.94,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1844,"POWERLINKV5_20151103074515","2010-02-22T09:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1845,"POWERLINKV5_20151103074515","2010-02-22T09:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-16.100000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1846,"POWERLINKV5_20151103074515","2010-02-22T10:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1847,"POWERLINKV5_20151103074515","2010-02-22T10:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1848,"POWERLINKV5_20151103074515","2010-02-22T10:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1849,"POWERLINKV5_20151103074515","2010-02-22T10:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1850,"POWERLINKV5_20151103074515","2010-02-22T10:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.07,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1851,"POWERLINKV5_20151103074515","2010-02-22T17:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-40.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1852,"POWERLINKV5_20151103074515","2010-02-22T17:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-57.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1853,"POWERLINKV5_20151103074515","2010-02-22T17:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-47.92,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1854,"POWERLINKV5_20151103074515","2010-02-22T17:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-48.85,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1855,"POWERLINKV5_20151103074515","2010-02-22T17:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-47.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1856,"POWERLINKV5_20151103074515","2010-02-22T17:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-48.92,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1857,"POWERLINKV5_20151103074515","2010-02-22T17:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1858,"POWERLINKV5_20151103074515","2010-02-22T18:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-59.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1859,"POWERLINKV5_20151103074515","2010-02-22T18:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-27.48,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1860,"POWERLINKV5_20151103074515","2010-02-22T18:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.75,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1861,"POWERLINKV5_20151103074515","2010-02-22T18:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.83,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1862,"POWERLINKV5_20151103074515","2010-02-22T18:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.65,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1863,"POWERLINKV5_20151103074515","2010-02-22T18:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1864,"POWERLINKV5_20151103074515","2010-02-22T18:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1865,"POWERLINKV5_20151103074515","2010-02-22T18:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1866,"POWERLINKV5_20151103074515","2010-02-22T18:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.33,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1867,"POWERLINKV5_20151103074515","2010-02-22T18:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1868,"POWERLINKV5_20151103074515","2010-02-22T18:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1869,"POWERLINKV5_20151103074515","2010-02-22T19:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1870,"POWERLINKV5_20151103074515","2010-02-22T19:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1871,"POWERLINKV5_20151103074515","2010-02-22T19:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1872,"POWERLINKV5_20151103074515","2010-02-22T19:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1873,"POWERLINKV5_20151103074515","2010-02-22T19:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.5,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1874,"POWERLINKV5_20151103074515","2010-02-22T19:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1875,"POWERLINKV5_20151103074515","2010-02-22T19:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-21.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1876,"POWERLINKV5_20151103074515","2010-02-22T19:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.850000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1877,"POWERLINKV5_20151103074515","2010-02-22T19:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-24.79,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1878,"POWERLINKV5_20151103074515","2010-02-22T19:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-31.14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1879,"POWERLINKV5_20151103074515","2010-02-22T19:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1880,"POWERLINKV5_20151103074515","2010-02-22T19:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1881,"POWERLINKV5_20151103074515","2010-02-22T20:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1882,"POWERLINKV5_20151103074515","2010-02-22T20:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1883,"POWERLINKV5_20151103074515","2010-02-22T20:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.94,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1884,"POWERLINKV5_20151103074515","2010-02-22T21:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-17.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1885,"POWERLINKV5_20151103074515","2010-02-22T21:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1886,"POWERLINKV5_20151103074515","2010-02-22T22:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.440000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1887,"POWERLINKV5_20151103074515","2010-02-23T00:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.67,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1888,"POWERLINKV5_20151103074515","2010-02-23T00:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1889,"POWERLINKV5_20151103074515","2010-02-23T00:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1890,"POWERLINKV5_20151103074515","2010-02-23T00:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1891,"POWERLINKV5_20151103074515","2010-02-23T00:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1892,"POWERLINKV5_20151103074515","2010-02-23T00:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1893,"POWERLINKV5_20151103074515","2010-02-23T00:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1894,"POWERLINKV5_20151103074515","2010-02-23T01:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1895,"POWERLINKV5_20151103074515","2010-02-23T01:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-17.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1896,"POWERLINKV5_20151103074515","2010-02-23T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-27.68,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1897,"POWERLINKV5_20151103074515","2010-02-23T01:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1898,"POWERLINKV5_20151103074515","2010-02-23T01:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.25,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1899,"POWERLINKV5_20151103074515","2010-02-23T01:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.98,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1900,"POWERLINKV5_20151103074515","2010-02-23T01:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.98,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1901,"POWERLINKV5_20151103074515","2010-02-23T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.19,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1902,"POWERLINKV5_20151103074515","2010-02-23T01:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.1,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1903,"POWERLINKV5_20151103074515","2010-02-23T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1904,"POWERLINKV5_20151103074515","2010-02-23T01:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.43,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1905,"POWERLINKV5_20151103074515","2010-02-23T01:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1906,"POWERLINKV5_20151103074515","2010-02-23T02:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1907,"POWERLINKV5_20151103074515","2010-02-23T02:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.27,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1908,"POWERLINKV5_20151103074515","2010-02-23T02:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1909,"POWERLINKV5_20151103074515","2010-02-23T02:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.329999999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1910,"POWERLINKV5_20151103074515","2010-02-23T02:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.399999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1911,"POWERLINKV5_20151103074515","2010-02-23T02:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-18.399999999999999,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1912,"POWERLINKV5_20151103074515","2010-02-23T02:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1913,"POWERLINKV5_20151103074515","2010-02-23T02:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1914,"POWERLINKV5_20151103074515","2010-02-23T02:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.34,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1915,"POWERLINKV5_20151103074515","2010-02-23T02:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1916,"POWERLINKV5_20151103074515","2010-02-23T02:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1917,"POWERLINKV5_20151103074515","2010-02-23T02:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.399999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1918,"POWERLINKV5_20151103074515","2010-02-23T03:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1919,"POWERLINKV5_20151103074515","2010-02-23T03:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1920,"POWERLINKV5_20151103074515","2010-02-23T03:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1921,"POWERLINKV5_20151103074515","2010-02-23T03:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1922,"POWERLINKV5_20151103074515","2010-02-23T03:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.19,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1923,"POWERLINKV5_20151103074515","2010-02-23T03:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1924,"POWERLINKV5_20151103074515","2010-02-23T03:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.06,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1925,"POWERLINKV5_20151103074515","2010-02-23T03:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1926,"POWERLINKV5_20151103074515","2010-02-23T03:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1927,"POWERLINKV5_20151103074515","2010-02-23T03:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1928,"POWERLINKV5_20151103074515","2010-02-23T04:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.39,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1929,"POWERLINKV5_20151103074515","2010-02-23T04:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1930,"POWERLINKV5_20151103074515","2010-02-23T04:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1931,"POWERLINKV5_20151103074515","2010-02-23T04:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.72,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1932,"POWERLINKV5_20151103074515","2010-02-23T04:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.9,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1933,"POWERLINKV5_20151103074515","2010-02-23T04:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1934,"POWERLINKV5_20151103074515","2010-02-23T04:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.32,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1935,"POWERLINKV5_20151103074515","2010-02-23T04:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1936,"POWERLINKV5_20151103074515","2010-02-23T04:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1937,"POWERLINKV5_20151103074515","2010-02-23T04:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.17,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1938,"POWERLINKV5_20151103074515","2010-02-23T05:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.62,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1939,"POWERLINKV5_20151103074515","2010-02-23T06:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.4,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1940,"POWERLINKV5_20151103074515","2010-02-23T06:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1941,"POWERLINKV5_20151103074515","2010-02-23T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.190000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1942,"POWERLINKV5_20151103074515","2010-02-23T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-31.76,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1943,"POWERLINKV5_20151103074515","2010-02-23T06:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-28.7,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1944,"POWERLINKV5_20151103074515","2010-02-23T09:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-24.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1945,"POWERLINKV5_20151103074515","2010-02-23T09:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-20.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1946,"POWERLINKV5_20151103074515","2010-02-23T09:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1947,"POWERLINKV5_20151103074515","2010-02-27T19:15:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-459.07,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1948,"POWERLINKV5_20151103074515","2010-02-27T19:20:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-459.37,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1949,"POWERLINKV5_20151103074515","2010-02-27T19:25:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-459.08,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1950,"POWERLINKV5_20151103074515","2010-02-27T19:30:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-458.91,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1951,"POWERLINKV5_20151103074515","2010-02-27T19:35:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-458.91,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1952,"POWERLINKV5_20151103074515","2010-02-27T19:40:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76063.850000000006,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1953,"POWERLINKV5_20151103074515","2010-02-27T19:45:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76065.2,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1954,"POWERLINKV5_20151103074515","2010-02-28T08:50:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76062.91,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1955,"POWERLINKV5_20151103074515","2010-02-28T08:55:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76062.95,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1956,"POWERLINKV5_20151103074515","2010-03-01T09:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-11.09," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1957,"POWERLINKV5_20151103074515","2010-03-02T05:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1958,"POWERLINKV5_20151103074515","2010-03-03T19:00:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76017.89,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1959,"POWERLINKV5_20151103074515","2010-03-03T19:05:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-76015.94,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1960,"POWERLINKV5_20151103074515","2010-03-04T13:15:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75976.63,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1961,"POWERLINKV5_20151103074515","2010-03-04T13:20:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75969.919999999998,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1962,"POWERLINKV5_20151103074515","2010-03-04T13:25:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75973.81,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1963,"POWERLINKV5_20151103074515","2010-03-05T13:40:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75932.92,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1964,"POWERLINKV5_20151103074515","2010-03-05T13:45:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75914.03,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1965,"POWERLINKV5_20151103074515","2010-03-05T13:50:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75924.19,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1966,"POWERLINKV5_20151103074515","2010-03-05T19:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-23.75," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1967,"POWERLINKV5_20151103074515","2010-03-05T19:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-24.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1968,"POWERLINKV5_20151103074515","2010-03-05T19:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-20.100000000000001," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1969,"POWERLINKV5_20151103074515","2010-03-05T19:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-24.11," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1970,"POWERLINKV5_20151103074515","2010-03-06T19:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-52.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1971,"POWERLINKV5_20151103074515","2010-03-06T19:35:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-447.65,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1972,"POWERLINKV5_20151103074515","2010-03-06T19:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-38.82," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1973,"POWERLINKV5_20151103074515","2010-03-06T19:40:00","Q>NIL_SMRS_CRTVS2","Q-NIL_CN_132_CLOSED","2009-12-03",2,-460.75,"Out= Nil, avoid O/L T193 Clare South to T56 Townsville South (7131) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1974,"POWERLINKV5_20151103074515","2010-03-06T19:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-239.85," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1975,"POWERLINKV5_20151103074515","2010-03-06T19:45:00","Q>NIL_SMRS_CRTVS1","Q-NIL_CN_132_CLOSED","2009-12-03",2,-5062.3999999999996,"Out= Nil, avoid O/L T193 Clare South Tee T36 Invicta Mill to T56 Townsville South (7130) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1976,"POWERLINKV5_20151103074515","2010-03-06T19:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-12.21," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1977,"POWERLINKV5_20151103074515","2010-03-06T19:50:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-6364.67,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1978,"POWERLINKV5_20151103074515","2010-03-06T19:55:00","Q>NIL_SMRS_SMCR","Q-NIL_CN_132_CLOSED","2009-12-03",2,-6349.21,"Out= Nil, avoid O/L H35 Strathmore to T193 Clare South (7208) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1979,"POWERLINKV5_20151103074515","2010-03-06T20:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-12.02," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1980,"POWERLINKV5_20151103074515","2010-03-06T20:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-11.61," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1981,"POWERLINKV5_20151103074515","2010-03-06T20:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-26.7," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1982,"POWERLINKV5_20151103074515","2010-03-06T20:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1983,"POWERLINKV5_20151103074515","2010-03-06T20:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-12.78," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1984,"POWERLINKV5_20151103074515","2010-03-06T22:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1985,"POWERLINKV5_20151103074515","2010-03-07T06:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-19.39," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1986,"POWERLINKV5_20151103074515","2010-03-07T06:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-15.94," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1987,"POWERLINKV5_20151103074515","2010-03-07T06:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-15.56," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1988,"POWERLINKV5_20151103074515","2010-03-07T07:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-50.23," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1989,"POWERLINKV5_20151103074515","2010-03-07T07:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-47.48," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1990,"POWERLINKV5_20151103074515","2010-03-07T07:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-23.26," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1991,"POWERLINKV5_20151103074515","2010-03-07T08:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.4," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1992,"POWERLINKV5_20151103074515","2010-03-07T08:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-20.61," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1993,"POWERLINKV5_20151103074515","2010-03-07T08:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-21.93," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1994,"POWERLINKV5_20151103074515","2010-03-07T08:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-242.88," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1995,"POWERLINKV5_20151103074515","2010-03-07T08:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-60.63," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1996,"POWERLINKV5_20151103074515","2010-03-07T08:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-59.07," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1997,"POWERLINKV5_20151103074515","2010-03-07T08:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1998,"POWERLINKV5_20151103074515","2010-03-07T08:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-58.95," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1999,"POWERLINKV5_20151103074515","2010-03-07T09:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-25.78," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2001,"POWERLINKV5_20151103074515","2010-03-07T09:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-55.23," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2003,"POWERLINKV5_20151103074515","2010-03-07T09:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-242.25," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2006,"POWERLINKV5_20151103074515","2010-03-07T09:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-55.27," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2010,"POWERLINKV5_20151103074515","2010-03-07T10:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-63.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2013,"POWERLINKV5_20151103074515","2010-03-07T10:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-16.329999999999998," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2016,"POWERLINKV5_20151103074515","2010-03-07T10:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-254.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2017,"POWERLINKV5_20151103074515","2010-03-07T11:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-249.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2020,"POWERLINKV5_20151103074515","2010-03-07T11:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-11.52," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2023,"POWERLINKV5_20151103074515","2010-03-07T12:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.87," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2026,"POWERLINKV5_20151103074515","2010-03-07T12:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-58.97," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2029,"POWERLINKV5_20151103074515","2010-03-07T12:30:00","Q>NIL_SMRS_SMRS","Q-NIL_CN_132_CLOSED","2009-12-03",2,-75663.289999999994,"Out= Nil, avoid O/L on H35 Strathmore to H13 Ross (879) on trip of H35 Strathmore to H13 Ross (880), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2033,"POWERLINKV5_20151103074515","2010-03-07T12:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-58.42," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2036,"POWERLINKV5_20151103074515","2010-03-07T13:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-240.08," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2039,"POWERLINKV5_20151103074515","2010-03-07T13:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.74," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2040,"POWERLINKV5_20151103074515","2010-03-07T13:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.74," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2043,"POWERLINKV5_20151103074515","2010-03-07T13:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-262.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2046,"POWERLINKV5_20151103074515","2010-03-07T13:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-254.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2049,"POWERLINKV5_20151103074515","2010-03-07T14:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-24.72," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2052,"POWERLINKV5_20151103074515","2010-03-07T14:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-73.790000000000006," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2056,"POWERLINKV5_20151103074515","2010-03-07T14:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-65.66," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2059,"POWERLINKV5_20151103074515","2010-03-07T15:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-76.81," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2060,"POWERLINKV5_20151103074515","2010-03-07T15:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-63.58," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2063,"POWERLINKV5_20151103074515","2010-03-07T15:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-241.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2066,"POWERLINKV5_20151103074515","2010-03-07T15:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.74," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2069,"POWERLINKV5_20151103074515","2010-03-07T15:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-254.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2072,"POWERLINKV5_20151103074515","2010-03-07T16:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.75," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2075,"POWERLINKV5_20151103074515","2010-03-07T16:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-76.81," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2079,"POWERLINKV5_20151103074515","2010-03-07T16:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-261.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2082,"POWERLINKV5_20151103074515","2010-03-07T16:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-256.58999999999997," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2083,"POWERLINKV5_20151103074515","2010-03-07T16:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-69.13," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2086,"POWERLINKV5_20151103074515","2010-03-07T17:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-254.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2089,"POWERLINKV5_20151103074515","2010-03-07T17:20:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-265.58999999999997," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2092,"POWERLINKV5_20151103074515","2010-03-07T17:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-254.95," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2095,"POWERLINKV5_20151103074515","2010-03-07T17:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-239.46," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2098,"POWERLINKV5_20151103074515","2010-03-07T18:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-239.33," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2102,"POWERLINKV5_20151103074515","2010-03-07T18:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-10.32," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2105,"POWERLINKV5_20151103074515","2010-03-07T18:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-11.29," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2106,"POWERLINKV5_20151103074515","2010-03-07T18:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-62.82," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2110,"POWERLINKV5_20151103074515","2010-03-07T19:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-258.23," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2111,"POWERLINKV5_20151103074515","2010-03-07T19:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-77.680000000000007," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2115,"POWERLINKV5_20151103074515","2010-03-07T19:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-275.62," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2118,"POWERLINKV5_20151103074515","2010-03-07T19:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-274.99," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2122,"POWERLINKV5_20151103074515","2010-03-07T19:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-653.71," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2125,"POWERLINKV5_20151103074515","2010-03-07T20:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-26.63," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2128,"POWERLINKV5_20151103074515","2010-03-07T20:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.74," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2129,"POWERLINKV5_20151103074515","2010-03-07T20:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-253.25," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2133,"POWERLINKV5_20151103074515","2010-03-07T20:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-259.76," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2134,"POWERLINKV5_20151103074515","2010-03-07T21:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-21.03," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2138,"POWERLINKV5_20151103074515","2010-03-08T10:00:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-234.54," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2141,"POWERLINKV5_20151103074515","2010-03-08T10:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-32.71," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2145,"POWERLINKV5_20151103074515","2010-03-08T10:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-227.44," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2148,"POWERLINKV5_20151103074515","2010-03-08T10:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-231.69," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2151,"POWERLINKV5_20151103074515","2010-03-08T13:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-25.4," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2152,"POWERLINKV5_20151103074515","2010-03-08T13:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-58.25," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2156,"POWERLINKV5_20151103074515","2010-03-08T13:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-240.09," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2158,"POWERLINKV5_20151103074515","2010-03-08T13:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-388.69," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2161,"POWERLINKV5_20151103074515","2010-03-08T14:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-23.06," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2164,"POWERLINKV5_20151103074515","2010-03-08T14:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-489.92," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2168,"POWERLINKV5_20151103074515","2010-03-08T14:55:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-23," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2171,"POWERLINKV5_20151103074515","2010-03-08T15:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-30.24," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2174,"POWERLINKV5_20151103074515","2010-03-08T15:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-16.239999999999998," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2175,"POWERLINKV5_20151103074515","2010-03-08T16:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-26.31," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2179,"POWERLINKV5_20151103074515","2010-03-09T07:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-238.76," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2181,"POWERLINKV5_20151103074515","2010-03-09T12:55:00","Q>MRTA","Q-NIL_MRTA","2007-06-14",1,-21.13,"Out = NIL, OakeyPS constrained for continous rating of Middle-Ridge-Tangkam 110kV lines ","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2184,"POWERLINKV5_20151103074515","2010-03-11T00:20:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1015.45,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2187,"POWERLINKV5_20151103074515","2010-03-11T00:35:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1015.33,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2191,"POWERLINKV5_20151103074515","2010-03-11T00:55:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1011.47,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2194,"POWERLINKV5_20151103074515","2010-03-11T01:10:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1018.36,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2197,"POWERLINKV5_20151103074515","2010-03-11T01:25:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1008.7,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2198,"POWERLINKV5_20151103074515","2010-03-11T01:30:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1008.94,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2202,"POWERLINKV5_20151103074515","2010-03-11T01:50:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1010.3,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2204,"POWERLINKV5_20151103074515","2010-03-11T02:00:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1007,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2207,"POWERLINKV5_20151103074515","2010-03-11T02:15:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1015.18,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2210,"POWERLINKV5_20151103074515","2010-03-11T02:30:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1009.64,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2214,"POWERLINKV5_20151103074515","2010-03-11T02:50:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1009.99,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2217,"POWERLINKV5_20151103074515","2010-03-11T03:05:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1004.24,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2218,"POWERLINKV5_20151103074515","2010-03-11T03:10:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1005.5,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2221,"POWERLINKV5_20151103074515","2010-03-11T03:25:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1006.54,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2223,"POWERLINKV5_20151103074515","2010-03-11T03:35:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1009,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2227,"POWERLINKV5_20151103074515","2010-03-11T03:55:00","Q>NIL_TRCN_TRCN","Q-NIL","2009-11-09",1,-1008.94,"Out= Nil, Powerlink relay limit on Tarong to Chinchilla 132kV lines, for the contingent loss of a single Tarong to Chinchilla 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2230,"POWERLINKV5_20151103074515","2010-04-01T04:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2233,"POWERLINKV5_20151103074515","2010-04-01T04:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.31,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2237,"POWERLINKV5_20151103074515","2010-04-01T04:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.24,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2240,"POWERLINKV5_20151103074515","2010-04-01T05:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2241,"POWERLINKV5_20151103074515","2010-04-01T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2244,"POWERLINKV5_20151103074515","2010-04-01T05:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2246,"POWERLINKV5_20151103074515","2010-04-01T05:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2250,"POWERLINKV5_20151103074515","2010-04-01T05:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.51,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2253,"POWERLINKV5_20151103074515","2010-04-01T06:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2256,"POWERLINKV5_20151103074515","2010-04-01T06:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2260,"POWERLINKV5_20151103074515","2010-04-01T06:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2263,"POWERLINKV5_20151103074515","2010-04-01T07:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2264,"POWERLINKV5_20151103074515","2010-04-01T07:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2267,"POWERLINKV5_20151103074515","2010-04-01T08:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.68,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2269,"POWERLINKV5_20151103074515","2010-04-01T08:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2273,"POWERLINKV5_20151103074515","2010-04-01T09:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.09,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2276,"POWERLINKV5_20151103074515","2010-04-01T09:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.57,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2280,"POWERLINKV5_20151103074515","2010-04-01T10:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2283,"POWERLINKV5_20151103074515","2010-04-01T10:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2286,"POWERLINKV5_20151103074515","2010-04-01T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2287,"POWERLINKV5_20151103074515","2010-04-01T10:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2290,"POWERLINKV5_20151103074515","2010-04-01T10:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.98,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2292,"POWERLINKV5_20151103074515","2010-04-01T11:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2296,"POWERLINKV5_20151103074515","2010-04-01T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2299,"POWERLINKV5_20151103074515","2010-04-01T11:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2303,"POWERLINKV5_20151103074515","2010-04-01T11:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2306,"POWERLINKV5_20151103074515","2010-04-01T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.4,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2309,"POWERLINKV5_20151103074515","2010-04-01T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2311,"POWERLINKV5_20151103074515","2010-04-01T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2312,"POWERLINKV5_20151103074515","2010-04-01T12:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2316,"POWERLINKV5_20151103074515","2010-04-01T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.85,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2319,"POWERLINKV5_20151103074515","2010-04-01T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2322,"POWERLINKV5_20151103074515","2010-04-01T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2326,"POWERLINKV5_20151103074515","2010-04-01T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.07,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2329,"POWERLINKV5_20151103074515","2010-04-01T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2332,"POWERLINKV5_20151103074515","2010-04-01T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2334,"POWERLINKV5_20151103074515","2010-04-01T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2335,"POWERLINKV5_20151103074515","2010-04-01T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.31,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2339,"POWERLINKV5_20151103074515","2010-04-01T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2342,"POWERLINKV5_20151103074515","2010-04-01T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2345,"POWERLINKV5_20151103074515","2010-04-01T15:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-19.04," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2349,"POWERLINKV5_20151103074515","2010-04-01T15:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-240.4," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2352,"POWERLINKV5_20151103074515","2010-04-01T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2355,"POWERLINKV5_20151103074515","2010-04-01T15:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-105.49," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2357,"POWERLINKV5_20151103074515","2010-04-01T15:45:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-23.3," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2358,"POWERLINKV5_20151103074515","2010-04-01T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2362,"POWERLINKV5_20151103074515","2010-04-01T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.13,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2365,"POWERLINKV5_20151103074515","2010-04-01T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2368,"POWERLINKV5_20151103074515","2010-04-01T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2372,"POWERLINKV5_20151103074515","2010-04-01T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.7,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2375,"POWERLINKV5_20151103074515","2010-04-01T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.89,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2376,"POWERLINKV5_20151103074515","2010-04-01T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2380,"POWERLINKV5_20151103074515","2010-04-01T23:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2381,"POWERLINKV5_20151103074515","2010-04-01T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2385,"POWERLINKV5_20151103074515","2010-04-01T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.13,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2388,"POWERLINKV5_20151103074515","2010-04-02T00:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.51,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2391,"POWERLINKV5_20151103074515","2010-04-02T20:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2395,"POWERLINKV5_20151103074515","2010-04-02T20:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2398,"POWERLINKV5_20151103074515","2010-04-02T20:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2399,"POWERLINKV5_20151103074515","2010-04-02T20:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2403,"POWERLINKV5_20151103074515","2010-04-02T21:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2404,"POWERLINKV5_20151103074515","2010-04-02T21:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2408,"POWERLINKV5_20151103074515","2010-04-02T21:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.88,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2411,"POWERLINKV5_20151103074515","2010-04-02T21:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2415,"POWERLINKV5_20151103074515","2010-04-02T22:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2418,"POWERLINKV5_20151103074515","2010-04-02T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2421,"POWERLINKV5_20151103074515","2010-04-02T23:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2422,"POWERLINKV5_20151103074515","2010-04-02T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2424,"POWERLINKV5_20151103074515","2010-04-02T23:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.09,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2427,"POWERLINKV5_20151103074515","2010-04-02T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2431,"POWERLINKV5_20151103074515","2010-04-02T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2434,"POWERLINKV5_20151103074515","2010-04-03T00:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2438,"POWERLINKV5_20151103074515","2010-04-03T00:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2441,"POWERLINKV5_20151103074515","2010-04-03T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2444,"POWERLINKV5_20151103074515","2010-04-03T01:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2445,"POWERLINKV5_20151103074515","2010-04-03T01:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2447,"POWERLINKV5_20151103074515","2010-04-03T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2450,"POWERLINKV5_20151103074515","2010-04-03T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2454,"POWERLINKV5_20151103074515","2010-04-03T01:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2457,"POWERLINKV5_20151103074515","2010-04-03T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2461,"POWERLINKV5_20151103074515","2010-04-03T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2464,"POWERLINKV5_20151103074515","2010-04-03T02:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2467,"POWERLINKV5_20151103074515","2010-04-03T02:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2468,"POWERLINKV5_20151103074515","2010-04-03T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2470,"POWERLINKV5_20151103074515","2010-04-03T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2474,"POWERLINKV5_20151103074515","2010-04-03T03:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2477,"POWERLINKV5_20151103074515","2010-04-03T03:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2480,"POWERLINKV5_20151103074515","2010-04-03T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.75,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2484,"POWERLINKV5_20151103074515","2010-04-03T04:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2487,"POWERLINKV5_20151103074515","2010-04-03T04:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2490,"POWERLINKV5_20151103074515","2010-04-03T04:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2491,"POWERLINKV5_20151103074515","2010-04-03T04:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.35,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2493,"POWERLINKV5_20151103074515","2010-04-03T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2497,"POWERLINKV5_20151103074515","2010-04-03T05:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2500,"POWERLINKV5_20151103074515","2010-04-03T05:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2503,"POWERLINKV5_20151103074515","2010-04-03T05:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2507,"POWERLINKV5_20151103074515","2010-04-03T06:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2510,"POWERLINKV5_20151103074515","2010-04-03T06:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2512,"POWERLINKV5_20151103074515","2010-04-03T06:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2513,"POWERLINKV5_20151103074515","2010-04-03T06:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.85,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2516,"POWERLINKV5_20151103074515","2010-04-03T07:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.82,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2520,"POWERLINKV5_20151103074515","2010-04-03T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.8,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2523,"POWERLINKV5_20151103074515","2010-04-03T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2526,"POWERLINKV5_20151103074515","2010-04-03T07:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2530,"POWERLINKV5_20151103074515","2010-04-03T08:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2533,"POWERLINKV5_20151103074515","2010-04-03T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2535,"POWERLINKV5_20151103074515","2010-04-03T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2536,"POWERLINKV5_20151103074515","2010-04-03T08:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2539,"POWERLINKV5_20151103074515","2010-04-03T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2543,"POWERLINKV5_20151103074515","2010-04-03T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2546,"POWERLINKV5_20151103074515","2010-04-03T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.24,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2549,"POWERLINKV5_20151103074515","2010-04-04T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2553,"POWERLINKV5_20151103074515","2010-04-04T22:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.83,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2556,"POWERLINKV5_20151103074515","2010-04-04T22:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2558,"POWERLINKV5_20151103074515","2010-04-04T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.31,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2559,"POWERLINKV5_20151103074515","2010-04-04T22:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2562,"POWERLINKV5_20151103074515","2010-04-04T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2566,"POWERLINKV5_20151103074515","2010-04-04T23:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.7,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2569,"POWERLINKV5_20151103074515","2010-04-04T23:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2573,"POWERLINKV5_20151103074515","2010-04-05T00:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2576,"POWERLINKV5_20151103074515","2010-04-05T00:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2579,"POWERLINKV5_20151103074515","2010-04-05T00:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2581,"POWERLINKV5_20151103074515","2010-04-05T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2582,"POWERLINKV5_20151103074515","2010-04-05T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2585,"POWERLINKV5_20151103074515","2010-04-05T01:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2589,"POWERLINKV5_20151103074515","2010-04-05T01:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2592,"POWERLINKV5_20151103074515","2010-04-05T01:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2596,"POWERLINKV5_20151103074515","2010-04-05T02:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2599,"POWERLINKV5_20151103074515","2010-04-05T02:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2602,"POWERLINKV5_20151103074515","2010-04-05T02:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2604,"POWERLINKV5_20151103074515","2010-04-05T02:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2605,"POWERLINKV5_20151103074515","2010-04-05T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.35,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2608,"POWERLINKV5_20151103074515","2010-04-05T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2612,"POWERLINKV5_20151103074515","2010-04-05T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2615,"POWERLINKV5_20151103074515","2010-04-05T03:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2619,"POWERLINKV5_20151103074515","2010-04-05T03:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2622,"POWERLINKV5_20151103074515","2010-04-05T04:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1008.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2623,"POWERLINKV5_20151103074515","2010-04-05T04:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1008.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2625,"POWERLINKV5_20151103074515","2010-04-05T04:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2628,"POWERLINKV5_20151103074515","2010-04-05T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2632,"POWERLINKV5_20151103074515","2010-04-05T05:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2635,"POWERLINKV5_20151103074515","2010-04-05T05:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2638,"POWERLINKV5_20151103074515","2010-04-05T05:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2642,"POWERLINKV5_20151103074515","2010-04-05T05:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.78,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2645,"POWERLINKV5_20151103074515","2010-04-05T06:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2646,"POWERLINKV5_20151103074515","2010-04-05T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.55,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2648,"POWERLINKV5_20151103074515","2010-04-05T06:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2651,"POWERLINKV5_20151103074515","2010-04-05T06:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.27,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2655,"POWERLINKV5_20151103074515","2010-04-05T06:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2658,"POWERLINKV5_20151103074515","2010-04-05T07:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2661,"POWERLINKV5_20151103074515","2010-04-05T07:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.45,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2665,"POWERLINKV5_20151103074515","2010-04-05T08:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2668,"POWERLINKV5_20151103074515","2010-04-05T08:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2669,"POWERLINKV5_20151103074515","2010-04-05T08:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2671,"POWERLINKV5_20151103074515","2010-04-05T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.02,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2674,"POWERLINKV5_20151103074515","2010-04-05T08:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2678,"POWERLINKV5_20151103074515","2010-04-05T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2681,"POWERLINKV5_20151103074515","2010-04-05T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2684,"POWERLINKV5_20151103074515","2010-04-05T12:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2688,"POWERLINKV5_20151103074515","2010-04-05T12:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2691,"POWERLINKV5_20151103074515","2010-04-05T13:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2692,"POWERLINKV5_20151103074515","2010-04-05T13:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2694,"POWERLINKV5_20151103074515","2010-04-05T13:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2697,"POWERLINKV5_20151103074515","2010-04-05T22:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2701,"POWERLINKV5_20151103074515","2010-04-05T22:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2704,"POWERLINKV5_20151103074515","2010-04-05T22:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.48,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2707,"POWERLINKV5_20151103074515","2010-04-05T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2711,"POWERLINKV5_20151103074515","2010-04-05T23:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2714,"POWERLINKV5_20151103074515","2010-04-05T23:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2715,"POWERLINKV5_20151103074515","2010-04-05T23:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2717,"POWERLINKV5_20151103074515","2010-04-06","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.16,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2720,"POWERLINKV5_20151103074515","2010-04-06T00:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2724,"POWERLINKV5_20151103074515","2010-04-06T00:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2727,"POWERLINKV5_20151103074515","2010-04-06T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2731,"POWERLINKV5_20151103074515","2010-04-06T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.67,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2734,"POWERLINKV5_20151103074515","2010-04-06T01:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.75,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2736,"POWERLINKV5_20151103074515","2010-04-06T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2737,"POWERLINKV5_20151103074515","2010-04-06T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.739999999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2740,"POWERLINKV5_20151103074515","2010-04-06T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2743,"POWERLINKV5_20151103074515","2010-04-06T02:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2747,"POWERLINKV5_20151103074515","2010-04-06T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2750,"POWERLINKV5_20151103074515","2010-04-06T02:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2754,"POWERLINKV5_20151103074515","2010-04-06T02:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.47,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2757,"POWERLINKV5_20151103074515","2010-04-06T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2759,"POWERLINKV5_20151103074515","2010-04-06T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2760,"POWERLINKV5_20151103074515","2010-04-06T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.62,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2763,"POWERLINKV5_20151103074515","2010-04-06T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2766,"POWERLINKV5_20151103074515","2010-04-06T03:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2770,"POWERLINKV5_20151103074515","2010-04-06T04:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1009.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2773,"POWERLINKV5_20151103074515","2010-04-06T04:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1010.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2777,"POWERLINKV5_20151103074515","2010-04-06T04:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2780,"POWERLINKV5_20151103074515","2010-04-06T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2782,"POWERLINKV5_20151103074515","2010-04-06T05:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2783,"POWERLINKV5_20151103074515","2010-04-06T05:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2786,"POWERLINKV5_20151103074515","2010-04-06T05:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2790,"POWERLINKV5_20151103074515","2010-04-06T05:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.31,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2793,"POWERLINKV5_20151103074515","2010-04-06T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2796,"POWERLINKV5_20151103074515","2010-04-06T06:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2800,"POWERLINKV5_20151103074515","2010-04-06T06:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2803,"POWERLINKV5_20151103074515","2010-04-06T07:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.89,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2805,"POWERLINKV5_20151103074515","2010-04-06T07:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2806,"POWERLINKV5_20151103074515","2010-04-06T07:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2809,"POWERLINKV5_20151103074515","2010-04-06T07:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2813,"POWERLINKV5_20151103074515","2010-04-06T07:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2816,"POWERLINKV5_20151103074515","2010-04-07T01:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.08,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2819,"POWERLINKV5_20151103074515","2010-04-11T06:10:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-12.94,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2823,"POWERLINKV5_20151103074515","2010-04-11T06:30:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-16.8,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2824,"POWERLINKV5_20151103074515","2010-04-11T06:35:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-17,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2826,"POWERLINKV5_20151103074515","2010-04-11T06:45:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-16.75,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2829,"POWERLINKV5_20151103074515","2010-04-11T07:00:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-17.7,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2832,"POWERLINKV5_20151103074515","2010-04-11T07:15:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-20.81,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2836,"POWERLINKV5_20151103074515","2010-04-11T07:35:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-20,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2839,"POWERLINKV5_20151103074515","2010-04-11T07:50:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-20.25,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2842,"POWERLINKV5_20151103074515","2010-04-11T08:05:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-20.39,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2846,"POWERLINKV5_20151103074515","2010-04-11T08:25:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-21.59,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2847,"POWERLINKV5_20151103074515","2010-04-11T08:30:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-21.43,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2849,"POWERLINKV5_20151103074515","2010-04-11T08:40:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-21.93,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2852,"POWERLINKV5_20151103074515","2010-04-11T08:55:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-22.26,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2855,"POWERLINKV5_20151103074515","2010-04-11T09:10:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-22.27,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2859,"POWERLINKV5_20151103074515","2010-04-11T09:30:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-22.11,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2862,"POWERLINKV5_20151103074515","2010-04-11T09:45:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-22.8,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2865,"POWERLINKV5_20151103074515","2010-04-11T10:00:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-23.15,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2869,"POWERLINKV5_20151103074515","2010-04-11T10:20:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-24.65,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2870,"POWERLINKV5_20151103074515","2010-04-11T10:25:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-24.65,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2872,"POWERLINKV5_20151103074515","2010-04-11T10:35:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-24.38,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2875,"POWERLINKV5_20151103074515","2010-04-11T10:50:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-24.65,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2878,"POWERLINKV5_20151103074515","2010-04-11T11:05:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-26.37,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2882,"POWERLINKV5_20151103074515","2010-04-11T11:25:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-27.11,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2885,"POWERLINKV5_20151103074515","2010-04-11T11:40:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-28.34,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2889,"POWERLINKV5_20151103074515","2010-04-11T12:00:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-29.35,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2892,"POWERLINKV5_20151103074515","2010-04-11T12:15:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-32.51,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2893,"POWERLINKV5_20151103074515","2010-04-11T12:20:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-57.79,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2895,"POWERLINKV5_20151103074515","2010-04-11T12:30:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-33.22,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2898,"POWERLINKV5_20151103074515","2010-04-11T12:45:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-29.1,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2901,"POWERLINKV5_20151103074515","2010-04-11T13:00:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-57.79,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2905,"POWERLINKV5_20151103074515","2010-04-11T13:20:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-57.39,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2908,"POWERLINKV5_20151103074515","2010-04-11T13:35:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-144.29,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2912,"POWERLINKV5_20151103074515","2010-04-11T13:55:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-95.5,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2915,"POWERLINKV5_20151103074515","2010-04-11T14:10:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-95.5,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2916,"POWERLINKV5_20151103074515","2010-04-11T14:15:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-56.79,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2918,"POWERLINKV5_20151103074515","2010-04-11T14:25:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-29.3,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2921,"POWERLINKV5_20151103074515","2010-04-11T14:40:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-28,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2924,"POWERLINKV5_20151103074515","2010-04-11T14:55:00","Q>TV_TYP","Q-TV_TYP","2005-09-19",1,-24.39,"Out = 7241 Townsville - Townsville PS 132KV line orT145 Townsville PS SW'YD 132kV 2 bus.","OUTAGE","OTHER","Feeder 7241","NON-REGULATED","4","Planned and Scheduled Generator outage, refer to AFW Q09S/1813 ma dQ10S/0853.","PLANNED",0]
[2928,"POWERLINKV5_20151103074515","2010-04-12T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2931,"POWERLINKV5_20151103074515","2010-04-12T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2935,"POWERLINKV5_20151103074515","2010-04-12T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2937,"POWERLINKV5_20151103074515","2010-04-12T23:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2940,"POWERLINKV5_20151103074515","2010-04-13T00:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2941,"POWERLINKV5_20151103074515","2010-04-13T00:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2944,"POWERLINKV5_20151103074515","2010-04-13T00:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.51,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2948,"POWERLINKV5_20151103074515","2010-04-13T00:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2951,"POWERLINKV5_20151103074515","2010-04-13T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2954,"POWERLINKV5_20151103074515","2010-04-13T01:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2958,"POWERLINKV5_20151103074515","2010-04-13T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2960,"POWERLINKV5_20151103074515","2010-04-13T01:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2963,"POWERLINKV5_20151103074515","2010-04-13T02:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.88,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2964,"POWERLINKV5_20151103074515","2010-04-13T02:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2967,"POWERLINKV5_20151103074515","2010-04-13T02:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.02,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2971,"POWERLINKV5_20151103074515","2010-04-13T02:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2974,"POWERLINKV5_20151103074515","2010-04-13T08:40:00","Q>BCLC_CLWU_BCGL","Q-BCLC_811","2010-01-19",1,-10.08,"Out= Bouldercombe to Larcom Creek (811), avoid O/L Bouldercombe to Gladstone (812) on trip of Calvale to Wurdong (871), Feedback","OUTAGE","OTHER","Feeder 811","REGULATED","INCLUDED","Outage of Feeder 811, refer to AFW Q10S/0789.","PLANNED",1]
[2977,"POWERLINKV5_20151103074515","2010-04-15T00:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2981,"POWERLINKV5_20151103074515","2010-04-15T01:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2983,"POWERLINKV5_20151103074515","2010-04-15T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2984,"POWERLINKV5_20151103074515","2010-04-15T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2987,"POWERLINKV5_20151103074515","2010-04-15T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.35,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2990,"POWERLINKV5_20151103074515","2010-04-15T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.89,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2994,"POWERLINKV5_20151103074515","2010-04-15T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2997,"POWERLINKV5_20151103074515","2010-04-15T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3000,"POWERLINKV5_20151103074515","2010-04-15T02:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3004,"POWERLINKV5_20151103074515","2010-04-15T02:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3006,"POWERLINKV5_20151103074515","2010-04-15T03:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3007,"POWERLINKV5_20151103074515","2010-04-15T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3010,"POWERLINKV5_20151103074515","2010-04-15T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3013,"POWERLINKV5_20151103074515","2010-04-15T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3017,"POWERLINKV5_20151103074515","2010-04-15T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3020,"POWERLINKV5_20151103074515","2010-04-15T05:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3023,"POWERLINKV5_20151103074515","2010-04-15T05:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3025,"POWERLINKV5_20151103074515","2010-04-15T05:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3029,"POWERLINKV5_20151103074515","2010-04-15T06:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3030,"POWERLINKV5_20151103074515","2010-04-15T12:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3033,"POWERLINKV5_20151103074515","2010-04-15T12:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3036,"POWERLINKV5_20151103074515","2010-04-15T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3040,"POWERLINKV5_20151103074515","2010-04-15T12:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3043,"POWERLINKV5_20151103074515","2010-04-15T13:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3047,"POWERLINKV5_20151103074515","2010-04-15T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.85,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3048,"POWERLINKV5_20151103074515","2010-04-15T13:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.83,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3052,"POWERLINKV5_20151103074515","2010-04-15T13:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3053,"POWERLINKV5_20151103074515","2010-04-15T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3056,"POWERLINKV5_20151103074515","2010-04-15T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.64,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3059,"POWERLINKV5_20151103074515","2010-04-15T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3063,"POWERLINKV5_20151103074515","2010-04-15T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3066,"POWERLINKV5_20151103074515","2010-04-15T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.64,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3070,"POWERLINKV5_20151103074515","2010-04-15T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.8,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3071,"POWERLINKV5_20151103074515","2010-04-15T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3075,"POWERLINKV5_20151103074515","2010-04-15T15:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3076,"POWERLINKV5_20151103074515","2010-04-15T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3079,"POWERLINKV5_20151103074515","2010-04-15T16:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3083,"POWERLINKV5_20151103074515","2010-04-15T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3086,"POWERLINKV5_20151103074515","2010-04-15T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.8,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3089,"POWERLINKV5_20151103074515","2010-04-15T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3093,"POWERLINKV5_20151103074515","2010-04-15T17:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.78,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3094,"POWERLINKV5_20151103074515","2010-04-15T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3098,"POWERLINKV5_20151103074515","2010-04-15T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.13,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3099,"POWERLINKV5_20151103074515","2010-04-15T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3102,"POWERLINKV5_20151103074515","2010-04-15T18:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3106,"POWERLINKV5_20151103074515","2010-04-15T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1027.3800000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3109,"POWERLINKV5_20151103074515","2010-04-15T18:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3112,"POWERLINKV5_20151103074515","2010-04-15T18:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3116,"POWERLINKV5_20151103074515","2010-04-15T19:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3117,"POWERLINKV5_20151103074515","2010-04-15T19:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.45,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3121,"POWERLINKV5_20151103074515","2010-04-15T19:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3122,"POWERLINKV5_20151103074515","2010-04-15T19:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3125,"POWERLINKV5_20151103074515","2010-04-15T20:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.32,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3129,"POWERLINKV5_20151103074515","2010-04-15T20:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.61,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3132,"POWERLINKV5_20151103074515","2010-04-15T20:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3135,"POWERLINKV5_20151103074515","2010-04-15T20:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.88,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3138,"POWERLINKV5_20151103074515","2010-04-15T21:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3141,"POWERLINKV5_20151103074515","2010-04-15T21:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3142,"POWERLINKV5_20151103074515","2010-04-15T21:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3145,"POWERLINKV5_20151103074515","2010-04-15T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3148,"POWERLINKV5_20151103074515","2010-04-15T21:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3152,"POWERLINKV5_20151103074515","2010-04-15T22:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3155,"POWERLINKV5_20151103074515","2010-04-15T22:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3158,"POWERLINKV5_20151103074515","2010-04-15T22:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.16,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3161,"POWERLINKV5_20151103074515","2010-04-15T23:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3164,"POWERLINKV5_20151103074515","2010-04-15T23:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3165,"POWERLINKV5_20151103074515","2010-04-15T23:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3168,"POWERLINKV5_20151103074515","2010-04-15T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.82,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3171,"POWERLINKV5_20151103074515","2010-04-15T23:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3175,"POWERLINKV5_20151103074515","2010-04-16T00:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3178,"POWERLINKV5_20151103074515","2010-04-16T00:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3181,"POWERLINKV5_20151103074515","2010-04-16T00:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.309999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3184,"POWERLINKV5_20151103074515","2010-04-16T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3187,"POWERLINKV5_20151103074515","2010-04-16T01:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3188,"POWERLINKV5_20151103074515","2010-04-16T01:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3191,"POWERLINKV5_20151103074515","2010-04-16T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3194,"POWERLINKV5_20151103074515","2010-04-16T01:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3198,"POWERLINKV5_20151103074515","2010-04-16T01:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3201,"POWERLINKV5_20151103074515","2010-04-16T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3205,"POWERLINKV5_20151103074515","2010-04-16T01:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3207,"POWERLINKV5_20151103074515","2010-04-16T02:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3210,"POWERLINKV5_20151103074515","2010-04-16T02:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3211,"POWERLINKV5_20151103074515","2010-04-16T02:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3214,"POWERLINKV5_20151103074515","2010-04-16T02:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3217,"POWERLINKV5_20151103074515","2010-04-16T02:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3221,"POWERLINKV5_20151103074515","2010-04-16T02:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3224,"POWERLINKV5_20151103074515","2010-04-16T02:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3228,"POWERLINKV5_20151103074515","2010-04-16T03:00:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3230,"POWERLINKV5_20151103074515","2010-04-16T03:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3233,"POWERLINKV5_20151103074515","2010-04-16T03:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3234,"POWERLINKV5_20151103074515","2010-04-16T03:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3237,"POWERLINKV5_20151103074515","2010-04-16T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3241,"POWERLINKV5_20151103074515","2010-04-16T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3244,"POWERLINKV5_20151103074515","2010-04-16T03:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3247,"POWERLINKV5_20151103074515","2010-04-16T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3249,"POWERLINKV5_20151103074515","2010-04-16T04:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3253,"POWERLINKV5_20151103074515","2010-04-16T04:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1006.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3256,"POWERLINKV5_20151103074515","2010-04-16T04:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3257,"POWERLINKV5_20151103074515","2010-04-16T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1002.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3260,"POWERLINKV5_20151103074515","2010-04-16T04:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3264,"POWERLINKV5_20151103074515","2010-04-16T05:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.78,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3267,"POWERLINKV5_20151103074515","2010-04-16T05:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3270,"POWERLINKV5_20151103074515","2010-04-16T05:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3272,"POWERLINKV5_20151103074515","2010-04-16T05:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3276,"POWERLINKV5_20151103074515","2010-04-16T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.68,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3279,"POWERLINKV5_20151103074515","2010-04-16T10:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3280,"POWERLINKV5_20151103074515","2010-04-16T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3283,"POWERLINKV5_20151103074515","2010-04-16T10:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.19,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3287,"POWERLINKV5_20151103074515","2010-04-16T11:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3290,"POWERLINKV5_20151103074515","2010-04-16T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3293,"POWERLINKV5_20151103074515","2010-04-16T11:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.19,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3295,"POWERLINKV5_20151103074515","2010-04-16T11:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3299,"POWERLINKV5_20151103074515","2010-04-16T12:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.07,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3300,"POWERLINKV5_20151103074515","2010-04-16T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3303,"POWERLINKV5_20151103074515","2010-04-16T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3306,"POWERLINKV5_20151103074515","2010-04-16T12:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3310,"POWERLINKV5_20151103074515","2010-04-16T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3313,"POWERLINKV5_20151103074515","2010-04-16T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3316,"POWERLINKV5_20151103074515","2010-04-16T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3318,"POWERLINKV5_20151103074515","2010-04-16T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3322,"POWERLINKV5_20151103074515","2010-04-16T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.19,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3323,"POWERLINKV5_20151103074515","2010-04-16T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3326,"POWERLINKV5_20151103074515","2010-04-16T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3329,"POWERLINKV5_20151103074515","2010-04-16T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3333,"POWERLINKV5_20151103074515","2010-04-16T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3336,"POWERLINKV5_20151103074515","2010-04-16T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3339,"POWERLINKV5_20151103074515","2010-04-16T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3342,"POWERLINKV5_20151103074515","2010-04-16T15:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3345,"POWERLINKV5_20151103074515","2010-04-17T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3346,"POWERLINKV5_20151103074515","2010-04-17T01:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3349,"POWERLINKV5_20151103074515","2010-04-17T01:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3352,"POWERLINKV5_20151103074515","2010-04-17T01:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.92,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3356,"POWERLINKV5_20151103074515","2010-04-17T01:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3359,"POWERLINKV5_20151103074515","2010-04-17T02:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3362,"POWERLINKV5_20151103074515","2010-04-17T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.45,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3365,"POWERLINKV5_20151103074515","2010-04-17T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3368,"POWERLINKV5_20151103074515","2010-04-17T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3369,"POWERLINKV5_20151103074515","2010-04-17T03:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3372,"POWERLINKV5_20151103074515","2010-04-17T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3375,"POWERLINKV5_20151103074515","2010-04-17T03:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3379,"POWERLINKV5_20151103074515","2010-04-17T03:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3382,"POWERLINKV5_20151103074515","2010-04-17T04:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3385,"POWERLINKV5_20151103074515","2010-04-17T04:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3388,"POWERLINKV5_20151103074515","2010-04-17T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3391,"POWERLINKV5_20151103074515","2010-04-17T04:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3392,"POWERLINKV5_20151103074515","2010-04-17T05:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3395,"POWERLINKV5_20151103074515","2010-04-17T05:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3399,"POWERLINKV5_20151103074515","2010-04-17T05:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3402,"POWERLINKV5_20151103074515","2010-04-17T06:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.68,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3405,"POWERLINKV5_20151103074515","2010-04-17T19:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1028.6600000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3408,"POWERLINKV5_20151103074515","2010-04-17T19:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3411,"POWERLINKV5_20151103074515","2010-04-17T19:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3414,"POWERLINKV5_20151103074515","2010-04-17T20:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3415,"POWERLINKV5_20151103074515","2010-04-17T20:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.89,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3418,"POWERLINKV5_20151103074515","2010-04-17T20:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3422,"POWERLINKV5_20151103074515","2010-04-17T20:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3425,"POWERLINKV5_20151103074515","2010-04-17T21:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.06,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3428,"POWERLINKV5_20151103074515","2010-04-17T21:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3431,"POWERLINKV5_20151103074515","2010-04-17T21:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3434,"POWERLINKV5_20151103074515","2010-04-17T21:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.75,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3437,"POWERLINKV5_20151103074515","2010-04-17T22:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3438,"POWERLINKV5_20151103074515","2010-04-17T22:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3441,"POWERLINKV5_20151103074515","2010-04-17T22:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.32,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3445,"POWERLINKV5_20151103074515","2010-04-18T00:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3448,"POWERLINKV5_20151103074515","2010-04-18T00:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3450,"POWERLINKV5_20151103074515","2010-04-18T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3454,"POWERLINKV5_20151103074515","2010-04-18T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3457,"POWERLINKV5_20151103074515","2010-04-18T01:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3458,"POWERLINKV5_20151103074515","2010-04-18T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3461,"POWERLINKV5_20151103074515","2010-04-18T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3464,"POWERLINKV5_20151103074515","2010-04-18T02:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.62,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3468,"POWERLINKV5_20151103074515","2010-04-18T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.55,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3471,"POWERLINKV5_20151103074515","2010-04-18T02:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3473,"POWERLINKV5_20151103074515","2010-04-18T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3477,"POWERLINKV5_20151103074515","2010-04-18T03:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3480,"POWERLINKV5_20151103074515","2010-04-18T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3481,"POWERLINKV5_20151103074515","2010-04-18T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3484,"POWERLINKV5_20151103074515","2010-04-18T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3487,"POWERLINKV5_20151103074515","2010-04-18T03:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.75,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3491,"POWERLINKV5_20151103074515","2010-04-18T04:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3494,"POWERLINKV5_20151103074515","2010-04-18T04:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3496,"POWERLINKV5_20151103074515","2010-04-18T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3500,"POWERLINKV5_20151103074515","2010-04-18T05:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.61,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3503,"POWERLINKV5_20151103074515","2010-04-18T05:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3504,"POWERLINKV5_20151103074515","2010-04-18T05:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3507,"POWERLINKV5_20151103074515","2010-04-18T05:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.85,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3510,"POWERLINKV5_20151103074515","2010-04-18T05:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3514,"POWERLINKV5_20151103074515","2010-04-18T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3517,"POWERLINKV5_20151103074515","2010-04-18T06:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3519,"POWERLINKV5_20151103074515","2010-04-18T06:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3523,"POWERLINKV5_20151103074515","2010-04-18T06:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3526,"POWERLINKV5_20151103074515","2010-04-18T07:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3527,"POWERLINKV5_20151103074515","2010-04-18T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3530,"POWERLINKV5_20151103074515","2010-04-18T12:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3533,"POWERLINKV5_20151103074515","2010-04-18T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3537,"POWERLINKV5_20151103074515","2010-04-18T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3540,"POWERLINKV5_20151103074515","2010-04-18T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.88,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3543,"POWERLINKV5_20151103074515","2010-04-18T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.7,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3546,"POWERLINKV5_20151103074515","2010-04-18T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.55,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3549,"POWERLINKV5_20151103074515","2010-04-18T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.88,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3550,"POWERLINKV5_20151103074515","2010-04-18T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3553,"POWERLINKV5_20151103074515","2010-04-18T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3557,"POWERLINKV5_20151103074515","2010-04-18T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3560,"POWERLINKV5_20151103074515","2010-04-18T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3563,"POWERLINKV5_20151103074515","2010-04-18T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3566,"POWERLINKV5_20151103074515","2010-04-18T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3569,"POWERLINKV5_20151103074515","2010-04-18T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.85,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3572,"POWERLINKV5_20151103074515","2010-04-18T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.31,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3573,"POWERLINKV5_20151103074515","2010-04-18T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3576,"POWERLINKV5_20151103074515","2010-04-18T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3580,"POWERLINKV5_20151103074515","2010-04-18T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.83,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3583,"POWERLINKV5_20151103074515","2010-04-24T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-40387.870000000003,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3586,"POWERLINKV5_20151103074515","2010-04-24T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-40387.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3589,"POWERLINKV5_20151103074515","2010-04-24T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3592,"POWERLINKV5_20151103074515","2010-04-24T16:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3595,"POWERLINKV5_20151103074515","2010-04-24T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3596,"POWERLINKV5_20151103074515","2010-04-24T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3599,"POWERLINKV5_20151103074515","2010-04-24T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3603,"POWERLINKV5_20151103074515","2010-04-24T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.57,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3606,"POWERLINKV5_20151103074515","2010-04-24T17:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3609,"POWERLINKV5_20151103074515","2010-04-24T17:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.6300000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3612,"POWERLINKV5_20151103074515","2010-04-24T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.8800000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3615,"POWERLINKV5_20151103074515","2010-04-24T18:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1030.8699999999999,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3616,"POWERLINKV5_20151103074515","2010-04-24T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1029.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3619,"POWERLINKV5_20151103074515","2010-04-24T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.6400000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3622,"POWERLINKV5_20151103074515","2010-04-24T18:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1027.2,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3626,"POWERLINKV5_20151103074515","2010-04-24T19:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1032.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3629,"POWERLINKV5_20151103074515","2010-04-24T19:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3632,"POWERLINKV5_20151103074515","2010-04-24T19:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3635,"POWERLINKV5_20151103074515","2010-04-24T19:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3638,"POWERLINKV5_20151103074515","2010-04-24T20:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3639,"POWERLINKV5_20151103074515","2010-04-24T20:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3642,"POWERLINKV5_20151103074515","2010-04-24T20:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3645,"POWERLINKV5_20151103074515","2010-04-24T20:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3649,"POWERLINKV5_20151103074515","2010-04-24T20:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3651,"POWERLINKV5_20151103074515","2010-04-24T21:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.24,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3655,"POWERLINKV5_20151103074515","2010-04-24T21:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3658,"POWERLINKV5_20151103074515","2010-04-24T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3661,"POWERLINKV5_20151103074515","2010-04-24T21:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3662,"POWERLINKV5_20151103074515","2010-04-24T22:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3665,"POWERLINKV5_20151103074515","2010-04-24T22:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3668,"POWERLINKV5_20151103074515","2010-04-24T22:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.27,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3672,"POWERLINKV5_20151103074515","2010-04-24T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.47,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3674,"POWERLINKV5_20151103074515","2010-04-24T23:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3678,"POWERLINKV5_20151103074515","2010-04-24T23:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.62,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3681,"POWERLINKV5_20151103074515","2010-04-24T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3684,"POWERLINKV5_20151103074515","2010-04-24T23:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3685,"POWERLINKV5_20151103074515","2010-04-24T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3688,"POWERLINKV5_20151103074515","2010-04-25T00:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3691,"POWERLINKV5_20151103074515","2010-04-25T00:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3695,"POWERLINKV5_20151103074515","2010-04-25T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3697,"POWERLINKV5_20151103074515","2010-04-25T00:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3701,"POWERLINKV5_20151103074515","2010-04-25T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3704,"POWERLINKV5_20151103074515","2010-04-25T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3707,"POWERLINKV5_20151103074515","2010-04-25T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.6,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3708,"POWERLINKV5_20151103074515","2010-04-25T01:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3711,"POWERLINKV5_20151103074515","2010-04-25T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3715,"POWERLINKV5_20151103074515","2010-04-25T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3718,"POWERLINKV5_20151103074515","2010-04-25T02:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3720,"POWERLINKV5_20151103074515","2010-04-25T02:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3724,"POWERLINKV5_20151103074515","2010-04-25T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3727,"POWERLINKV5_20151103074515","2010-04-25T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3730,"POWERLINKV5_20151103074515","2010-04-25T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.27,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3731,"POWERLINKV5_20151103074515","2010-04-25T03:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.82,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3734,"POWERLINKV5_20151103074515","2010-04-25T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3738,"POWERLINKV5_20151103074515","2010-04-25T04:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3741,"POWERLINKV5_20151103074515","2010-04-25T04:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3743,"POWERLINKV5_20151103074515","2010-04-25T04:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3747,"POWERLINKV5_20151103074515","2010-04-25T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3750,"POWERLINKV5_20151103074515","2010-04-25T05:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.74,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3753,"POWERLINKV5_20151103074515","2010-04-25T05:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3754,"POWERLINKV5_20151103074515","2010-04-25T05:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.91,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3757,"POWERLINKV5_20151103074515","2010-04-25T05:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3761,"POWERLINKV5_20151103074515","2010-04-25T06:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3764,"POWERLINKV5_20151103074515","2010-04-25T06:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.67,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3766,"POWERLINKV5_20151103074515","2010-04-25T06:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3770,"POWERLINKV5_20151103074515","2010-04-25T07:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3773,"POWERLINKV5_20151103074515","2010-04-25T07:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.13,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3774,"POWERLINKV5_20151103074515","2010-04-25T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3777,"POWERLINKV5_20151103074515","2010-04-25T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3780,"POWERLINKV5_20151103074515","2010-04-25T07:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3784,"POWERLINKV5_20151103074515","2010-04-25T08:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.27,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3787,"POWERLINKV5_20151103074515","2010-04-25T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3789,"POWERLINKV5_20151103074515","2010-04-25T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3793,"POWERLINKV5_20151103074515","2010-04-25T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3796,"POWERLINKV5_20151103074515","2010-04-25T09:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3797,"POWERLINKV5_20151103074515","2010-04-25T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3800,"POWERLINKV5_20151103074515","2010-04-25T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3803,"POWERLINKV5_20151103074515","2010-04-25T09:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3807,"POWERLINKV5_20151103074515","2010-04-25T10:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3810,"POWERLINKV5_20151103074515","2010-04-25T10:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.45,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3813,"POWERLINKV5_20151103074515","2010-04-25T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3816,"POWERLINKV5_20151103074515","2010-04-25T10:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3819,"POWERLINKV5_20151103074515","2010-04-25T11:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3820,"POWERLINKV5_20151103074515","2010-04-25T11:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3823,"POWERLINKV5_20151103074515","2010-04-25T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3826,"POWERLINKV5_20151103074515","2010-04-25T11:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3830,"POWERLINKV5_20151103074515","2010-04-25T11:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.48,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3833,"POWERLINKV5_20151103074515","2010-04-25T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3836,"POWERLINKV5_20151103074515","2010-04-25T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.29,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3839,"POWERLINKV5_20151103074515","2010-04-25T12:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3842,"POWERLINKV5_20151103074515","2010-04-25T12:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.07,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3843,"POWERLINKV5_20151103074515","2010-04-25T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3846,"POWERLINKV5_20151103074515","2010-04-25T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3849,"POWERLINKV5_20151103074515","2010-04-25T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3852,"POWERLINKV5_20151103074515","2010-04-25T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3855,"POWERLINKV5_20151103074515","2010-04-25T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3859,"POWERLINKV5_20151103074515","2010-04-25T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3862,"POWERLINKV5_20151103074515","2010-04-25T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3865,"POWERLINKV5_20151103074515","2010-04-25T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3866,"POWERLINKV5_20151103074515","2010-04-25T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3869,"POWERLINKV5_20151103074515","2010-04-25T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3873,"POWERLINKV5_20151103074515","2010-04-25T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3875,"POWERLINKV5_20151103074515","2010-04-25T15:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3878,"POWERLINKV5_20151103074515","2010-04-25T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3882,"POWERLINKV5_20151103074515","2010-04-25T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3885,"POWERLINKV5_20151103074515","2010-04-25T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3888,"POWERLINKV5_20151103074515","2010-04-25T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.57,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3889,"POWERLINKV5_20151103074515","2010-04-25T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3892,"POWERLINKV5_20151103074515","2010-04-25T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.89,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3896,"POWERLINKV5_20151103074515","2010-04-25T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1027.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3898,"POWERLINKV5_20151103074515","2010-04-25T17:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1032.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3901,"POWERLINKV5_20151103074515","2010-04-25T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1040.94,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3905,"POWERLINKV5_20151103074515","2010-04-25T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1042.24,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3908,"POWERLINKV5_20151103074515","2010-04-25T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1055.51,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3909,"POWERLINKV5_20151103074515","2010-04-25T18:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1041.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3912,"POWERLINKV5_20151103074515","2010-04-25T18:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1041.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3915,"POWERLINKV5_20151103074515","2010-04-25T19:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1040.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3919,"POWERLINKV5_20151103074515","2010-04-25T19:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.8,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3921,"POWERLINKV5_20151103074515","2010-04-25T19:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3924,"POWERLINKV5_20151103074515","2010-04-25T19:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.35,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3928,"POWERLINKV5_20151103074515","2010-04-25T20:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3931,"POWERLINKV5_20151103074515","2010-04-25T20:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3932,"POWERLINKV5_20151103074515","2010-04-25T20:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3935,"POWERLINKV5_20151103074515","2010-04-25T20:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3938,"POWERLINKV5_20151103074515","2010-04-25T20:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3942,"POWERLINKV5_20151103074515","2010-04-25T21:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3944,"POWERLINKV5_20151103074515","2010-04-25T21:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3947,"POWERLINKV5_20151103074515","2010-04-25T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3951,"POWERLINKV5_20151103074515","2010-04-25T22:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3954,"POWERLINKV5_20151103074515","2010-04-25T22:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.21,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3955,"POWERLINKV5_20151103074515","2010-04-25T22:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3958,"POWERLINKV5_20151103074515","2010-04-25T22:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.09,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3961,"POWERLINKV5_20151103074515","2010-04-25T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.35,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3965,"POWERLINKV5_20151103074515","2010-04-25T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1027.3900000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3967,"POWERLINKV5_20151103074515","2010-04-25T23:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.44,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3971,"POWERLINKV5_20151103074515","2010-04-25T23:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.61,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3974,"POWERLINKV5_20151103074515","2010-04-25T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3977,"POWERLINKV5_20151103074515","2010-04-26T00:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.32,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3978,"POWERLINKV5_20151103074515","2010-04-26T00:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.32,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3981,"POWERLINKV5_20151103074515","2010-04-26T00:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3984,"POWERLINKV5_20151103074515","2010-04-26T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3988,"POWERLINKV5_20151103074515","2010-04-26T01:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3990,"POWERLINKV5_20151103074515","2010-04-26T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3994,"POWERLINKV5_20151103074515","2010-04-26T01:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.32,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3997,"POWERLINKV5_20151103074515","2010-04-26T01:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.82,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4000,"POWERLINKV5_20151103074515","2010-04-26T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.16,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4001,"POWERLINKV5_20151103074515","2010-04-26T02:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4004,"POWERLINKV5_20151103074515","2010-04-26T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4007,"POWERLINKV5_20151103074515","2010-04-26T02:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4011,"POWERLINKV5_20151103074515","2010-04-26T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4013,"POWERLINKV5_20151103074515","2010-04-26T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4017,"POWERLINKV5_20151103074515","2010-04-26T03:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4020,"POWERLINKV5_20151103074515","2010-04-26T03:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4023,"POWERLINKV5_20151103074515","2010-04-26T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4024,"POWERLINKV5_20151103074515","2010-04-26T04:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4027,"POWERLINKV5_20151103074515","2010-04-26T04:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4031,"POWERLINKV5_20151103074515","2010-04-26T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4034,"POWERLINKV5_20151103074515","2010-04-26T04:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4036,"POWERLINKV5_20151103074515","2010-04-26T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.13,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4040,"POWERLINKV5_20151103074515","2010-04-26T05:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4043,"POWERLINKV5_20151103074515","2010-04-26T05:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4046,"POWERLINKV5_20151103074515","2010-04-26T05:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4047,"POWERLINKV5_20151103074515","2010-04-26T06:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.46,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4050,"POWERLINKV5_20151103074515","2010-04-26T06:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4053,"POWERLINKV5_20151103074515","2010-04-26T06:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.47,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4056,"POWERLINKV5_20151103074515","2010-04-26T06:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4059,"POWERLINKV5_20151103074515","2010-04-26T07:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4063,"POWERLINKV5_20151103074515","2010-04-26T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4066,"POWERLINKV5_20151103074515","2010-04-26T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4067,"POWERLINKV5_20151103074515","2010-04-26T07:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.56,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4070,"POWERLINKV5_20151103074515","2010-04-26T07:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4073,"POWERLINKV5_20151103074515","2010-04-26T08:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4076,"POWERLINKV5_20151103074515","2010-04-26T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.63,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4079,"POWERLINKV5_20151103074515","2010-04-26T08:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4082,"POWERLINKV5_20151103074515","2010-04-26T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4086,"POWERLINKV5_20151103074515","2010-04-26T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4089,"POWERLINKV5_20151103074515","2010-04-26T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4090,"POWERLINKV5_20151103074515","2010-04-26T09:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4093,"POWERLINKV5_20151103074515","2010-04-26T09:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4096,"POWERLINKV5_20151103074515","2010-04-26T10:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4099,"POWERLINKV5_20151103074515","2010-04-26T10:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4102,"POWERLINKV5_20151103074515","2010-04-26T10:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4105,"POWERLINKV5_20151103074515","2010-04-26T10:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4109,"POWERLINKV5_20151103074515","2010-04-26T11:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.83,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4112,"POWERLINKV5_20151103074515","2010-04-26T11:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4113,"POWERLINKV5_20151103074515","2010-04-26T11:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.64,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4116,"POWERLINKV5_20151103074515","2010-04-26T11:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4119,"POWERLINKV5_20151103074515","2010-04-26T12:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.75,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4122,"POWERLINKV5_20151103074515","2010-04-26T12:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4125,"POWERLINKV5_20151103074515","2010-04-26T12:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.05,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4129,"POWERLINKV5_20151103074515","2010-04-26T12:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4132,"POWERLINKV5_20151103074515","2010-04-26T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4135,"POWERLINKV5_20151103074515","2010-04-26T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4136,"POWERLINKV5_20151103074515","2010-04-26T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.68,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4139,"POWERLINKV5_20151103074515","2010-04-26T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4142,"POWERLINKV5_20151103074515","2010-04-26T13:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4145,"POWERLINKV5_20151103074515","2010-04-26T14:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4148,"POWERLINKV5_20151103074515","2010-04-26T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.98,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4152,"POWERLINKV5_20151103074515","2010-04-26T14:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.97,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4155,"POWERLINKV5_20151103074515","2010-04-26T15:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4158,"POWERLINKV5_20151103074515","2010-04-26T15:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.07,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4159,"POWERLINKV5_20151103074515","2010-04-26T15:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4162,"POWERLINKV5_20151103074515","2010-04-26T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4166,"POWERLINKV5_20151103074515","2010-04-26T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4168,"POWERLINKV5_20151103074515","2010-04-26T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.1,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4171,"POWERLINKV5_20151103074515","2010-04-26T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4175,"POWERLINKV5_20151103074515","2010-04-26T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4178,"POWERLINKV5_20151103074515","2010-04-26T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4181,"POWERLINKV5_20151103074515","2010-04-26T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4182,"POWERLINKV5_20151103074515","2010-04-26T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.29,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4185,"POWERLINKV5_20151103074515","2010-04-26T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.6199999999999,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4189,"POWERLINKV5_20151103074515","2010-04-26T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.48,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4191,"POWERLINKV5_20151103074515","2010-04-26T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1029.8499999999999,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4194,"POWERLINKV5_20151103074515","2010-04-26T18:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1029.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4198,"POWERLINKV5_20151103074515","2010-04-26T18:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4201,"POWERLINKV5_20151103074515","2010-04-27T02:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4204,"POWERLINKV5_20151103074515","2010-04-27T03:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4205,"POWERLINKV5_20151103074515","2010-04-27T04:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.03,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4208,"POWERLINKV5_20151103074515","2010-04-28T09:40:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-12.68," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4212,"POWERLINKV5_20151103074515","2010-05-05T02:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4214,"POWERLINKV5_20151103074515","2010-05-05T12:20:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.92,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4217,"POWERLINKV5_20151103074515","2010-05-05T12:35:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.2,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4221,"POWERLINKV5_20151103074515","2010-05-05T12:55:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.16,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4224,"POWERLINKV5_20151103074515","2010-05-05T13:10:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.14,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4225,"POWERLINKV5_20151103074515","2010-05-05T13:15:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.14,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4228,"POWERLINKV5_20151103074515","2010-05-05T13:30:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1019.64,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon outage with Condamine Power Station, refer to NOS 10SW4745.","PLANNED",0]
[4231,"POWERLINKV5_20151103074515","2010-05-05T19:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-05-05",2,-10.62,"N-Q-MNSP1. * -1 <= 100 (Wt = 20)","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0921 and Market Notice 31683.","PLANNED",1]
[4235,"POWERLINKV5_20151103074515","2010-05-06T02:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.6,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4237,"POWERLINKV5_20151103074515","2010-05-07T01:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.97,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4240,"POWERLINKV5_20151103074515","2010-05-07T01:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4244,"POWERLINKV5_20151103074515","2010-05-08T01:35:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1018.59,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4247,"POWERLINKV5_20151103074515","2010-05-08T01:55:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1017.49,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4248,"POWERLINKV5_20151103074515","2010-05-08T02:00:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1018.09,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4251,"POWERLINKV5_20151103074515","2010-05-08T02:15:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1017.39,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4254,"POWERLINKV5_20151103074515","2010-05-08T04:05:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1013.71,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4257,"POWERLINKV5_20151103074515","2010-05-08T04:25:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1013.71,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4260,"POWERLINKV5_20151103074515","2010-05-08T11:25:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.38,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4263,"POWERLINKV5_20151103074515","2010-05-08T11:50:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.6,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4267,"POWERLINKV5_20151103074515","2010-05-08T12:10:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.45,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4270,"POWERLINKV5_20151103074515","2010-05-08T12:25:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.38,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4271,"POWERLINKV5_20151103074515","2010-05-08T12:30:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.38,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4274,"POWERLINKV5_20151103074515","2010-05-09T00:10:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.9,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4277,"POWERLINKV5_20151103074515","2010-05-09T00:30:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.42,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4280,"POWERLINKV5_20151103074515","2010-05-09T00:45:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.15,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4283,"POWERLINKV5_20151103074515","2010-05-09T01:00:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.1,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4287,"POWERLINKV5_20151103074515","2010-05-09T01:30:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.24,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4290,"POWERLINKV5_20151103074515","2010-05-09T02:05:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4293,"POWERLINKV5_20151103074515","2010-05-09T02:25:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4294,"POWERLINKV5_20151103074515","2010-05-09T02:30:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4297,"POWERLINKV5_20151103074515","2010-05-09T02:45:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4300,"POWERLINKV5_20151103074515","2010-05-09T03:00:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1018.38,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4303,"POWERLINKV5_20151103074515","2010-05-09T03:15:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.48,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4306,"POWERLINKV5_20151103074515","2010-05-09T03:45:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1018.59,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4310,"POWERLINKV5_20151103074515","2010-05-09T04:25:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1017.83,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4313,"POWERLINKV5_20151103074515","2010-05-09T05:00:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1018,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4316,"POWERLINKV5_20151103074515","2010-05-09T05:30:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.5,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4317,"POWERLINKV5_20151103074515","2010-05-09T05:35:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4320,"POWERLINKV5_20151103074515","2010-05-09T05:55:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1019.99,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4323,"POWERLINKV5_20151103074515","2010-05-09T10:00:00","Q>TR_TX4","Q-TR_TX4","2010-03-22",1,-1020.73,"Out= H18 Tarong 275/132 kV Tx #4, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1.","OUTAGE","OTHER","H018 Tarong 4T","REGULATED","INCLUDED","Planned outage of H018 Tarong 4T, refer to AFW Q10S/0006.","PLANNED",1]
[4326,"POWERLINKV5_20151103074515","2010-05-10T00:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4329,"POWERLINKV5_20151103074515","2010-05-10T00:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4333,"POWERLINKV5_20151103074515","2010-05-10T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4336,"POWERLINKV5_20151103074515","2010-05-10T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.24,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4339,"POWERLINKV5_20151103074515","2010-05-10T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4340,"POWERLINKV5_20151103074515","2010-05-10T01:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4343,"POWERLINKV5_20151103074515","2010-05-10T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4346,"POWERLINKV5_20151103074515","2010-05-10T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4349,"POWERLINKV5_20151103074515","2010-05-10T02:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4352,"POWERLINKV5_20151103074515","2010-05-10T02:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.87,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4356,"POWERLINKV5_20151103074515","2010-05-10T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.59,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4359,"POWERLINKV5_20151103074515","2010-05-10T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.3,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4362,"POWERLINKV5_20151103074515","2010-05-10T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4363,"POWERLINKV5_20151103074515","2010-05-10T03:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.02,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4367,"POWERLINKV5_20151103074515","2010-05-10T04:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4369,"POWERLINKV5_20151103074515","2010-05-10T04:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.71,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4372,"POWERLINKV5_20151103074515","2010-05-10T04:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.49,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4375,"POWERLINKV5_20151103074515","2010-05-10T04:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.37,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4379,"POWERLINKV5_20151103074515","2010-05-10T05:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.39,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4382,"POWERLINKV5_20151103074515","2010-05-10T07:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.52,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4383,"POWERLINKV5_20151103074515","2010-05-10T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4386,"POWERLINKV5_20151103074515","2010-05-10T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4390,"POWERLINKV5_20151103074515","2010-05-10T17:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.36,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4392,"POWERLINKV5_20151103074515","2010-05-10T17:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-18.38,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4395,"POWERLINKV5_20151103074515","2010-05-10T18:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.95,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4398,"POWERLINKV5_20151103074515","2010-05-10T18:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-11.96,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4402,"POWERLINKV5_20151103074515","2010-05-11T05:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4405,"POWERLINKV5_20151103074515","2010-05-11T17:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.86,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4406,"POWERLINKV5_20151103074515","2010-05-11T17:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-20.77,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4409,"POWERLINKV5_20151103074515","2010-05-11T17:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-20.04,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4413,"POWERLINKV5_20151103074515","2010-05-11T18:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.01,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4415,"POWERLINKV5_20151103074515","2010-05-11T18:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-11.33,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4418,"POWERLINKV5_20151103074515","2010-05-11T19:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-20.82,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4421,"POWERLINKV5_20151103074515","2010-05-11T19:35:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-16.059999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4425,"POWERLINKV5_20151103074515","2010-05-11T19:45:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-27.75,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4428,"POWERLINKV5_20151103074515","2010-05-11T19:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-19.670000000000002,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4429,"POWERLINKV5_20151103074515","2010-05-11T19:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.47,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4432,"POWERLINKV5_20151103074515","2010-05-11T20:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-12.48,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4436,"POWERLINKV5_20151103074515","2010-05-11T20:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-15.97,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4438,"POWERLINKV5_20151103074515","2010-05-11T20:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-15.07,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4441,"POWERLINKV5_20151103074515","2010-05-11T20:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.68,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4445,"POWERLINKV5_20151103074515","2010-05-11T20:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.34,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4448,"POWERLINKV5_20151103074515","2010-05-11T20:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-14.41,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4451,"POWERLINKV5_20151103074515","2010-05-11T20:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.98,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4452,"POWERLINKV5_20151103074515","2010-05-11T20:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-12.81,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4455,"POWERLINKV5_20151103074515","2010-05-11T21:00:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.43,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4459,"POWERLINKV5_20151103074515","2010-05-12T00:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.65,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4461,"POWERLINKV5_20151103074515","2010-05-12T01:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4464,"POWERLINKV5_20151103074515","2010-05-12T01:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.21,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4468,"POWERLINKV5_20151103074515","2010-05-12T01:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.91,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4471,"POWERLINKV5_20151103074515","2010-05-12T01:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.74,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4474,"POWERLINKV5_20151103074515","2010-05-12T03:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.18,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4475,"POWERLINKV5_20151103074515","2010-05-12T07:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.88,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4478,"POWERLINKV5_20151103074515","2010-05-12T07:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-11.16,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4481,"POWERLINKV5_20151103074515","2010-05-12T07:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-53.27,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4484,"POWERLINKV5_20151103074515","2010-05-12T07:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.51,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4487,"POWERLINKV5_20151103074515","2010-05-12T07:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.8,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4491,"POWERLINKV5_20151103074515","2010-05-12T07:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-43.32,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4494,"POWERLINKV5_20151103074515","2010-05-12T07:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-49.88,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4497,"POWERLINKV5_20151103074515","2010-05-12T09:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-40.799999999999997,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4498,"POWERLINKV5_20151103074515","2010-05-12T09:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-36.51,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4501,"POWERLINKV5_20151103074515","2010-05-12T09:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-43.43,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4504,"POWERLINKV5_20151103074515","2010-05-12T09:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-35.33,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4507,"POWERLINKV5_20151103074515","2010-05-12T17:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-10.37,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4510,"POWERLINKV5_20151103074515","2010-05-12T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-108.29,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4514,"POWERLINKV5_20151103074515","2010-05-12T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-104.11,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4517,"POWERLINKV5_20151103074515","2010-05-12T18:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-16.87,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4520,"POWERLINKV5_20151103074515","2010-05-12T18:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-22.92,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4521,"POWERLINKV5_20151103074515","2010-05-12T18:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-19.29,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4524,"POWERLINKV5_20151103074515","2010-05-12T18:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-60.83,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4527,"POWERLINKV5_20151103074515","2010-05-12T18:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-29.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4530,"POWERLINKV5_20151103074515","2010-05-12T18:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-69.55,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4533,"POWERLINKV5_20151103074515","2010-05-12T19:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.81,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4537,"POWERLINKV5_20151103074515","2010-05-12T19:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.6,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4540,"POWERLINKV5_20151103074515","2010-05-12T19:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-18.38,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4541,"POWERLINKV5_20151103074515","2010-05-12T19:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.760000000000002,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4544,"POWERLINKV5_20151103074515","2010-05-12T19:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-20.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4547,"POWERLINKV5_20151103074515","2010-05-12T20:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-46.59,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4550,"POWERLINKV5_20151103074515","2010-05-12T22:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-46.64,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4553,"POWERLINKV5_20151103074515","2010-05-12T22:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.07,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4556,"POWERLINKV5_20151103074515","2010-05-13T01:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.97,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4560,"POWERLINKV5_20151103074515","2010-05-13T01:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.55,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4563,"POWERLINKV5_20151103074515","2010-05-13T02:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4564,"POWERLINKV5_20151103074515","2010-05-13T02:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.24,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4568,"POWERLINKV5_20151103074515","2010-05-13T02:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4569,"POWERLINKV5_20151103074515","2010-05-13T02:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.7,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4573,"POWERLINKV5_20151103074515","2010-05-13T03:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.84,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4576,"POWERLINKV5_20151103074515","2010-05-13T03:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4580,"POWERLINKV5_20151103074515","2010-05-13T04:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.11,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4583,"POWERLINKV5_20151103074515","2010-05-13T04:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.31,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4586,"POWERLINKV5_20151103074515","2010-05-13T05:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.76,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4587,"POWERLINKV5_20151103074515","2010-05-13T06:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.44,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4591,"POWERLINKV5_20151103074515","2010-05-13T06:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.420000000000002,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4592,"POWERLINKV5_20151103074515","2010-05-13T06:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-57.1,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4596,"POWERLINKV5_20151103074515","2010-05-13T06:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-52.32,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4599,"POWERLINKV5_20151103074515","2010-05-13T07:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-60.13,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4603,"POWERLINKV5_20151103074515","2010-05-13T07:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-13.04,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4606,"POWERLINKV5_20151103074515","2010-05-13T08:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.44,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4609,"POWERLINKV5_20151103074515","2010-05-13T15:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-16.54," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4610,"POWERLINKV5_20151103074515","2010-05-13T17:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-10.119999999999999,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4614,"POWERLINKV5_20151103074515","2010-05-13T18:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-37.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4615,"POWERLINKV5_20151103074515","2010-05-13T18:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-46.31,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4619,"POWERLINKV5_20151103074515","2010-05-13T18:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-41.12,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4622,"POWERLINKV5_20151103074515","2010-05-13T18:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-44.57,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4626,"POWERLINKV5_20151103074515","2010-05-13T22:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.34,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4629,"POWERLINKV5_20151103074515","2010-05-14T01:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.97,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4632,"POWERLINKV5_20151103074515","2010-05-14T02:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.23,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4633,"POWERLINKV5_20151103074515","2010-05-14T02:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.24,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4637,"POWERLINKV5_20151103074515","2010-05-14T04:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.31,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4639,"POWERLINKV5_20151103074515","2010-05-14T04:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.420000000000002,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4642,"POWERLINKV5_20151103074515","2010-05-14T04:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.18,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4645,"POWERLINKV5_20151103074515","2010-05-14T06:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.67,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4649,"POWERLINKV5_20151103074515","2010-05-14T08:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-39.270000000000003,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4652,"POWERLINKV5_20151103074515","2010-05-14T08:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-42.78,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4655,"POWERLINKV5_20151103074515","2010-05-14T09:10:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-38.15,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4656,"POWERLINKV5_20151103074515","2010-05-14T09:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-39.85,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4660,"POWERLINKV5_20151103074515","2010-05-14T09:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-30.85,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4662,"POWERLINKV5_20151103074515","2010-05-14T09:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-28.97,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4665,"POWERLINKV5_20151103074515","2010-05-14T09:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-30.29,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4668,"POWERLINKV5_20151103074515","2010-05-14T09:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-11.98,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4672,"POWERLINKV5_20151103074515","2010-05-14T09:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-10",1,-11.13,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0922.","PLANNED",1]
[4675,"POWERLINKV5_20151103074515","2010-05-14T10:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.44,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4678,"POWERLINKV5_20151103074515","2010-05-14T12:10:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-13.31," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4679,"POWERLINKV5_20151103074515","2010-05-14T13:15:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-16.72," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4681,"POWERLINKV5_20151103074515","2010-05-14T17:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.01,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4685,"POWERLINKV5_20151103074515","2010-05-14T17:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-17.68,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4688,"POWERLINKV5_20151103074515","2010-05-14T18:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.66,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4691,"POWERLINKV5_20151103074515","2010-05-14T18:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-58.48,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4695,"POWERLINKV5_20151103074515","2010-05-14T18:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-24.01,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4698,"POWERLINKV5_20151103074515","2010-05-14T19:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.96,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4699,"POWERLINKV5_20151103074515","2010-05-14T19:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-24.27,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4702,"POWERLINKV5_20151103074515","2010-05-14T19:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.42,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4704,"POWERLINKV5_20151103074515","2010-05-14T19:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.21,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4708,"POWERLINKV5_20151103074515","2010-05-14T19:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.87,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4711,"POWERLINKV5_20151103074515","2010-05-14T20:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.190000000000001,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4714,"POWERLINKV5_20151103074515","2010-05-14T20:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-19.190000000000001,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4718,"POWERLINKV5_20151103074515","2010-05-14T20:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-30.34,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4721,"POWERLINKV5_20151103074515","2010-05-14T21:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.55,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4722,"POWERLINKV5_20151103074515","2010-05-14T21:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-54.82,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4725,"POWERLINKV5_20151103074515","2010-05-14T21:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.21,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4727,"POWERLINKV5_20151103074515","2010-05-14T21:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.79,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4731,"POWERLINKV5_20151103074515","2010-05-14T22:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-57.11,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4734,"POWERLINKV5_20151103074515","2010-05-14T22:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-58.35,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4738,"POWERLINKV5_20151103074515","2010-05-14T22:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.75,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4741,"POWERLINKV5_20151103074515","2010-05-14T23:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-56.02,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4744,"POWERLINKV5_20151103074515","2010-05-14T23:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.39,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4745,"POWERLINKV5_20151103074515","2010-05-14T23:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.93,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4748,"POWERLINKV5_20151103074515","2010-05-14T23:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-59.9,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4750,"POWERLINKV5_20151103074515","2010-05-15T00:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.24,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4754,"POWERLINKV5_20151103074515","2010-05-15T00:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.92,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4757,"POWERLINKV5_20151103074515","2010-05-15T00:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.89,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4761,"POWERLINKV5_20151103074515","2010-05-15T01:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.4,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4764,"POWERLINKV5_20151103074515","2010-05-15T01:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.78,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4767,"POWERLINKV5_20151103074515","2010-05-15T01:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.440000000000001,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4769,"POWERLINKV5_20151103074515","2010-05-15T01:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.66,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4770,"POWERLINKV5_20151103074515","2010-05-15T01:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.43,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4773,"POWERLINKV5_20151103074515","2010-05-15T02:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.18,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4777,"POWERLINKV5_20151103074515","2010-05-15T02:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.23,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4780,"POWERLINKV5_20151103074515","2010-05-15T03:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4784,"POWERLINKV5_20151103074515","2010-05-15T03:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-17.02,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4787,"POWERLINKV5_20151103074515","2010-05-15T04:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4790,"POWERLINKV5_20151103074515","2010-05-15T05:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.97,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4792,"POWERLINKV5_20151103074515","2010-05-15T06:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.79,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4793,"POWERLINKV5_20151103074515","2010-05-15T06:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.83,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4797,"POWERLINKV5_20151103074515","2010-05-15T08:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4800,"POWERLINKV5_20151103074515","2010-05-15T08:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.45,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4803,"POWERLINKV5_20151103074515","2010-05-15T08:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.9,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4807,"POWERLINKV5_20151103074515","2010-05-15T09:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-29.48,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4810,"POWERLINKV5_20151103074515","2010-05-15T09:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-29.92,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4813,"POWERLINKV5_20151103074515","2010-05-15T09:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-28.03,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4815,"POWERLINKV5_20151103074515","2010-05-15T09:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4816,"POWERLINKV5_20151103074515","2010-05-15T09:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-28.36,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4820,"POWERLINKV5_20151103074515","2010-05-15T10:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-28.67,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4823,"POWERLINKV5_20151103074515","2010-05-15T10:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-29.97,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4826,"POWERLINKV5_20151103074515","2010-05-15T10:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-48.07,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4830,"POWERLINKV5_20151103074515","2010-05-15T11:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.14,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4833,"POWERLINKV5_20151103074515","2010-05-15T11:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.47,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4834,"POWERLINKV5_20151103074515","2010-05-15T11:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.09,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4838,"POWERLINKV5_20151103074515","2010-05-15T12:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.1,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4839,"POWERLINKV5_20151103074515","2010-05-15T12:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.92,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4843,"POWERLINKV5_20151103074515","2010-05-15T18:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-24.68,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4846,"POWERLINKV5_20151103074515","2010-05-15T18:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4849,"POWERLINKV5_20151103074515","2010-05-15T19:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4853,"POWERLINKV5_20151103074515","2010-05-15T19:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.14,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4856,"POWERLINKV5_20151103074515","2010-05-15T19:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-26.04,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4857,"POWERLINKV5_20151103074515","2010-05-15T19:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-31.58,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4861,"POWERLINKV5_20151103074515","2010-05-15T20:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.99,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4862,"POWERLINKV5_20151103074515","2010-05-15T20:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-28.75,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4866,"POWERLINKV5_20151103074515","2010-05-15T20:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.59,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4869,"POWERLINKV5_20151103074515","2010-05-15T21:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.37,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4872,"POWERLINKV5_20151103074515","2010-05-16T01:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.3,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4876,"POWERLINKV5_20151103074515","2010-05-16T01:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.94,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4879,"POWERLINKV5_20151103074515","2010-05-16T02:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4880,"POWERLINKV5_20151103074515","2010-05-16T03:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.59,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4882,"POWERLINKV5_20151103074515","2010-05-16T04:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4885,"POWERLINKV5_20151103074515","2010-05-16T09:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.82,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4889,"POWERLINKV5_20151103074515","2010-05-16T09:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-33.72,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4892,"POWERLINKV5_20151103074515","2010-05-16T09:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-44.08,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4896,"POWERLINKV5_20151103074515","2010-05-16T09:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-32.96,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4899,"POWERLINKV5_20151103074515","2010-05-16T10:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-44.48,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4902,"POWERLINKV5_20151103074515","2010-05-16T10:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-29.72,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4903,"POWERLINKV5_20151103074515","2010-05-16T10:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.47,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4905,"POWERLINKV5_20151103074515","2010-05-16T10:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-12.51,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4908,"POWERLINKV5_20151103074515","2010-05-16T19:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.940000000000001,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4912,"POWERLINKV5_20151103074515","2010-05-16T20:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.94,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4915,"POWERLINKV5_20151103074515","2010-05-16T20:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.71,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4919,"POWERLINKV5_20151103074515","2010-05-16T20:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-17.809999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4922,"POWERLINKV5_20151103074515","2010-05-17T04:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.23,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4925,"POWERLINKV5_20151103074515","2010-05-17T06:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-54.36,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4926,"POWERLINKV5_20151103074515","2010-05-17T07:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-46.71,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4928,"POWERLINKV5_20151103074515","2010-05-17T08:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-68.09,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4931,"POWERLINKV5_20151103074515","2010-05-17T08:05:00","Q>>BCGL_BCLC_CLWU","Q-BCGL_812","2010-03-12",1,-15.84,"Out= Bouldercombe to Gladstone (812), avoid O/L Calvale to Wurdong (871) on trip of Bouldercombe to Larcom Creek (811), Feedback","OUTAGE","OTHER","Feeder 812","REGULATED","INCLUDED","Outage of Feeder 812, refer to AFW Q10S/0895.","PLANNED",1]
[4935,"POWERLINKV5_20151103074515","2010-05-17T08:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-68.42,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4938,"POWERLINKV5_20151103074515","2010-05-17T08:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-54.45,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4942,"POWERLINKV5_20151103074515","2010-05-17T08:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-91.07,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4945,"POWERLINKV5_20151103074515","2010-05-17T08:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-74.19,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4948,"POWERLINKV5_20151103074515","2010-05-17T08:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-54.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4949,"POWERLINKV5_20151103074515","2010-05-17T08:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-25.01,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4951,"POWERLINKV5_20151103074515","2010-05-17T08:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-18.89,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4955,"POWERLINKV5_20151103074515","2010-05-17T09:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.199999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4958,"POWERLINKV5_20151103074515","2010-05-17T09:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.42,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4961,"POWERLINKV5_20151103074515","2010-05-17T09:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-13.04,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4965,"POWERLINKV5_20151103074515","2010-05-17T09:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-17.64,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4968,"POWERLINKV5_20151103074515","2010-05-17T09:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4971,"POWERLINKV5_20151103074515","2010-05-17T09:45:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.19,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4972,"POWERLINKV5_20151103074515","2010-05-17T09:45:00","QNTE_ROC","Q-NIL","2006-12-27",1,-13.07,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4974,"POWERLINKV5_20151103074515","2010-05-17T09:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.44,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4978,"POWERLINKV5_20151103074515","2010-05-17T10:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.13,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4981,"POWERLINKV5_20151103074515","2010-05-17T10:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.17,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4984,"POWERLINKV5_20151103074515","2010-05-17T10:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-17.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4988,"POWERLINKV5_20151103074515","2010-05-17T10:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.46,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4991,"POWERLINKV5_20151103074515","2010-05-17T10:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.86,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4993,"POWERLINKV5_20151103074515","2010-05-17T10:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-21.37,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[4994,"POWERLINKV5_20151103074515","2010-05-17T10:45:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-13.45,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[4997,"POWERLINKV5_20151103074515","2010-05-17T10:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.74,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5001,"POWERLINKV5_20151103074515","2010-05-17T11:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5004,"POWERLINKV5_20151103074515","2010-05-17T11:10:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-17.61,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5007,"POWERLINKV5_20151103074515","2010-05-17T11:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.3,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5011,"POWERLINKV5_20151103074515","2010-05-17T11:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.52,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5014,"POWERLINKV5_20151103074515","2010-05-17T11:35:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-19.559999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5016,"POWERLINKV5_20151103074515","2010-05-17T11:40:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-12.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5017,"POWERLINKV5_20151103074515","2010-05-17T11:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5020,"POWERLINKV5_20151103074515","2010-05-17T11:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.61,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5024,"POWERLINKV5_20151103074515","2010-05-17T12:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.2,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5027,"POWERLINKV5_20151103074515","2010-05-17T12:10:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.07,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5030,"POWERLINKV5_20151103074515","2010-05-17T12:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.59,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5034,"POWERLINKV5_20151103074515","2010-05-17T12:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.36,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5037,"POWERLINKV5_20151103074515","2010-05-17T12:45:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-13.27,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5039,"POWERLINKV5_20151103074515","2010-05-17T12:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.81,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5040,"POWERLINKV5_20151103074515","2010-05-17T12:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.15,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5043,"POWERLINKV5_20151103074515","2010-05-17T13:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.35,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5047,"POWERLINKV5_20151103074515","2010-05-17T14:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.19,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5050,"POWERLINKV5_20151103074515","2010-05-17T14:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.51,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5054,"POWERLINKV5_20151103074515","2010-05-17T15:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.55,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5057,"POWERLINKV5_20151103074515","2010-05-17T15:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.44,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5060,"POWERLINKV5_20151103074515","2010-05-17T15:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.44,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5062,"POWERLINKV5_20151103074515","2010-05-17T16:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.95,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5063,"POWERLINKV5_20151103074515","2010-05-17T16:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.27,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5066,"POWERLINKV5_20151103074515","2010-05-17T16:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.41,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5070,"POWERLINKV5_20151103074515","2010-05-17T16:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.84,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5073,"POWERLINKV5_20151103074515","2010-05-17T16:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.59,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5077,"POWERLINKV5_20151103074515","2010-05-17T17:00:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-18.68,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5080,"POWERLINKV5_20151103074515","2010-05-17T17:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-20.82,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5081,"POWERLINKV5_20151103074515","2010-05-17T17:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.71,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5083,"POWERLINKV5_20151103074515","2010-05-17T17:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.510000000000002,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5086,"POWERLINKV5_20151103074515","2010-05-17T17:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-28.61,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5089,"POWERLINKV5_20151103074515","2010-05-17T17:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-49.5,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5093,"POWERLINKV5_20151103074515","2010-05-17T18:00:00","QNTE_ROC","Q-NIL","2006-12-27",1,-20.6,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5096,"POWERLINKV5_20151103074515","2010-05-17T18:10:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-77.45,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5100,"POWERLINKV5_20151103074515","2010-05-17T18:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-65.27,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5103,"POWERLINKV5_20151103074515","2010-05-17T18:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-81.67,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5104,"POWERLINKV5_20151103074515","2010-05-17T18:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-64.48,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5106,"POWERLINKV5_20151103074515","2010-05-17T18:35:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-65.88,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5109,"POWERLINKV5_20151103074515","2010-05-17T18:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-52.65,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5113,"POWERLINKV5_20151103074515","2010-05-17T18:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-55.49,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5116,"POWERLINKV5_20151103074515","2010-05-17T19:00:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-19.899999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5119,"POWERLINKV5_20151103074515","2010-05-17T19:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-52.46,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5123,"POWERLINKV5_20151103074515","2010-05-17T19:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-34.94,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5126,"POWERLINKV5_20151103074515","2010-05-17T19:25:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-26.76,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5127,"POWERLINKV5_20151103074515","2010-05-17T19:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-30.21,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5129,"POWERLINKV5_20151103074515","2010-05-17T19:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-37.130000000000003,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5132,"POWERLINKV5_20151103074515","2010-05-17T19:40:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-18.78,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5136,"POWERLINKV5_20151103074515","2010-05-17T19:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-17.46,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5139,"POWERLINKV5_20151103074515","2010-05-17T20:00:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-12.06,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5142,"POWERLINKV5_20151103074515","2010-05-17T20:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-28.74,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5146,"POWERLINKV5_20151103074515","2010-05-17T20:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.61,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5149,"POWERLINKV5_20151103074515","2010-05-17T20:25:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-23.7,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5150,"POWERLINKV5_20151103074515","2010-05-17T20:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.94,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5152,"POWERLINKV5_20151103074515","2010-05-17T20:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.5,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5155,"POWERLINKV5_20151103074515","2010-05-17T20:40:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-21.27,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5159,"POWERLINKV5_20151103074515","2010-05-17T20:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.36,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5162,"POWERLINKV5_20151103074515","2010-05-17T20:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.86,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5165,"POWERLINKV5_20151103074515","2010-05-17T21:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-11.21,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5169,"POWERLINKV5_20151103074515","2010-05-17T21:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.6,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5172,"POWERLINKV5_20151103074515","2010-05-17T21:40:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-12.52,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5173,"POWERLINKV5_20151103074515","2010-05-17T21:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.3,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5175,"POWERLINKV5_20151103074515","2010-05-17T21:55:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-17.87,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5178,"POWERLINKV5_20151103074515","2010-05-17T22:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.21,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5182,"POWERLINKV5_20151103074515","2010-05-17T22:15:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-20.52,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5185,"POWERLINKV5_20151103074515","2010-05-17T22:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.48,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5188,"POWERLINKV5_20151103074515","2010-05-17T22:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-30.02,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5192,"POWERLINKV5_20151103074515","2010-05-17T22:55:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-26.35,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5194,"POWERLINKV5_20151103074515","2010-05-17T23:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-19.809999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5195,"POWERLINKV5_20151103074515","2010-05-17T23:15:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-12.92,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5198,"POWERLINKV5_20151103074515","2010-05-17T23:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-23.04,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5201,"POWERLINKV5_20151103074515","2010-05-17T23:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.02,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5205,"POWERLINKV5_20151103074515","2010-05-18T00:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.05,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5208,"POWERLINKV5_20151103074515","2010-05-18T00:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.01,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5212,"POWERLINKV5_20151103074515","2010-05-18T01:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-26.25,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5215,"POWERLINKV5_20151103074515","2010-05-18T01:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-22.66,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5217,"POWERLINKV5_20151103074515","2010-05-18T01:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.39,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5218,"POWERLINKV5_20151103074515","2010-05-18T01:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.579999999999998,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5221,"POWERLINKV5_20151103074515","2010-05-18T01:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-23.01,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5224,"POWERLINKV5_20151103074515","2010-05-18T02:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-22.18,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5228,"POWERLINKV5_20151103074515","2010-05-18T02:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.329999999999998,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5231,"POWERLINKV5_20151103074515","2010-05-18T02:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.15,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5235,"POWERLINKV5_20151103074515","2010-05-18T04:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.31,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5238,"POWERLINKV5_20151103074515","2010-05-18T06:15:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,69.83,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5240,"POWERLINKV5_20151103074515","2010-05-18T06:25:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,69.599999999999994,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5241,"POWERLINKV5_20151103074515","2010-05-18T06:30:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,69.03,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5244,"POWERLINKV5_20151103074515","2010-05-18T06:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-50.34,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5248,"POWERLINKV5_20151103074515","2010-05-18T07:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-22.61,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5251,"POWERLINKV5_20151103074515","2010-05-18T08:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-18.45,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5254,"POWERLINKV5_20151103074515","2010-05-18T08:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-39.89,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5258,"POWERLINKV5_20151103074515","2010-05-18T08:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-21.79,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5261,"POWERLINKV5_20151103074515","2010-05-18T09:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.65,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5263,"POWERLINKV5_20151103074515","2010-05-18T10:15:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,415.61,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5264,"POWERLINKV5_20151103074515","2010-05-18T10:20:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,415.61,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5267,"POWERLINKV5_20151103074515","2010-05-18T10:55:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,415.41,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5271,"POWERLINKV5_20151103074515","2010-05-18T11:20:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,411.86,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5274,"POWERLINKV5_20151103074515","2010-05-18T11:35:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,412.14,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5277,"POWERLINKV5_20151103074515","2010-05-18T11:55:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,410.83,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5281,"POWERLINKV5_20151103074515","2010-05-18T12:15:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,411.95,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5282,"POWERLINKV5_20151103074515","2010-05-18T12:20:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,409.26,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5286,"POWERLINKV5_20151103074515","2010-05-18T13:05:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,411.95,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5287,"POWERLINKV5_20151103074515","2010-05-18T13:10:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,411.46,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5290,"POWERLINKV5_20151103074515","2010-05-18T13:25:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,411.95,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5294,"POWERLINKV5_20151103074515","2010-05-18T13:50:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,415.85,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5297,"POWERLINKV5_20151103074515","2010-05-18T14:10:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,412.51,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5300,"POWERLINKV5_20151103074515","2010-05-18T14:25:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,412.14,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5304,"POWERLINKV5_20151103074515","2010-05-18T16:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.42,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5305,"POWERLINKV5_20151103074515","2010-05-18T16:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.12,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5307,"POWERLINKV5_20151103074515","2010-05-18T17:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.75,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5310,"POWERLINKV5_20151103074515","2010-05-18T17:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-47.41,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5313,"POWERLINKV5_20151103074515","2010-05-18T17:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-19.22,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5317,"POWERLINKV5_20151103074515","2010-05-18T18:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-23.04,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5320,"POWERLINKV5_20151103074515","2010-05-18T18:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-21.45,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5323,"POWERLINKV5_20151103074515","2010-05-18T18:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-42.58,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5327,"POWERLINKV5_20151103074515","2010-05-18T18:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.16,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5328,"POWERLINKV5_20151103074515","2010-05-18T18:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-39.4,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5330,"POWERLINKV5_20151103074515","2010-05-18T18:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-30.92,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5333,"POWERLINKV5_20151103074515","2010-05-18T18:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-22.01,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5336,"POWERLINKV5_20151103074515","2010-05-18T19:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-33.19,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5340,"POWERLINKV5_20151103074515","2010-05-18T19:25:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,12.05,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5343,"POWERLINKV5_20151103074515","2010-05-18T19:55:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,71.39,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5346,"POWERLINKV5_20151103074515","2010-05-18T20:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.98,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5350,"POWERLINKV5_20151103074515","2010-05-18T20:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-25.03,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5351,"POWERLINKV5_20151103074515","2010-05-18T20:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-27.29,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5353,"POWERLINKV5_20151103074515","2010-05-18T20:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.02,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5356,"POWERLINKV5_20151103074515","2010-05-18T20:25:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-10.07,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5359,"POWERLINKV5_20151103074515","2010-05-18T20:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5363,"POWERLINKV5_20151103074515","2010-05-18T20:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-34.83,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5366,"POWERLINKV5_20151103074515","2010-05-18T20:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-25.77,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5370,"POWERLINKV5_20151103074515","2010-05-18T21:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-16.579999999999998,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5373,"POWERLINKV5_20151103074515","2010-05-18T22:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-77.28,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5374,"POWERLINKV5_20151103074515","2010-05-18T22:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-62.39,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5376,"POWERLINKV5_20151103074515","2010-05-18T22:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-32.880000000000003,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5379,"POWERLINKV5_20151103074515","2010-05-19T00:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.13,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5382,"POWERLINKV5_20151103074515","2010-05-19T01:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-15.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5386,"POWERLINKV5_20151103074515","2010-05-19T01:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-27.64,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5389,"POWERLINKV5_20151103074515","2010-05-19T02:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-22.25,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5393,"POWERLINKV5_20151103074515","2010-05-19T02:40:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.29,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5395,"POWERLINKV5_20151103074515","2010-05-19T03:00:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.24,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5398,"POWERLINKV5_20151103074515","2010-05-19T03:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.3,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5399,"POWERLINKV5_20151103074515","2010-05-19T03:30:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.3,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5402,"POWERLINKV5_20151103074515","2010-05-19T03:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.3,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5406,"POWERLINKV5_20151103074515","2010-05-19T04:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.3,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5409,"POWERLINKV5_20151103074515","2010-05-19T05:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.34,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5412,"POWERLINKV5_20151103074515","2010-05-19T06:20:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,72.48,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5416,"POWERLINKV5_20151103074515","2010-05-19T06:55:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,66.41,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5418,"POWERLINKV5_20151103074515","2010-05-19T07:00:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,65.67,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5421,"POWERLINKV5_20151103074515","2010-05-19T15:10:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,469.32,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5422,"POWERLINKV5_20151103074515","2010-05-19T15:15:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,469.32,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0116.","PLANNED",1]
[5425,"POWERLINKV5_20151103074515","2010-05-19T20:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.14,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5429,"POWERLINKV5_20151103074515","2010-05-19T22:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-11.45,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5432,"POWERLINKV5_20151103074515","2010-05-20T02:45:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.399999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5435,"POWERLINKV5_20151103074515","2010-05-20T04:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.26,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/0799.","PLANNED",1]
[5439,"POWERLINKV5_20151103074515","2010-05-20T17:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.84,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5441,"POWERLINKV5_20151103074515","2010-05-20T18:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.91,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5444,"POWERLINKV5_20151103074515","2010-05-20T19:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5445,"POWERLINKV5_20151103074515","2010-05-20T20:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-12.53,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5448,"POWERLINKV5_20151103074515","2010-05-20T20:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.55,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5452,"POWERLINKV5_20151103074515","2010-05-20T20:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-19.420000000000002,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5455,"POWERLINKV5_20151103074515","2010-05-20T20:30:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.51,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5458,"POWERLINKV5_20151103074515","2010-05-20T20:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.440000000000001,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5462,"POWERLINKV5_20151103074515","2010-05-20T20:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.61,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5464,"POWERLINKV5_20151103074515","2010-05-20T21:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.48,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5465,"POWERLINKV5_20151103074515","2010-05-20T21:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-10.48,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5468,"POWERLINKV5_20151103074515","2010-05-20T21:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.76,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5471,"POWERLINKV5_20151103074515","2010-05-20T22:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-16.010000000000002,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5475,"POWERLINKV5_20151103074515","2010-05-21T00:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-22.22,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5478,"POWERLINKV5_20151103074515","2010-05-21T00:55:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-14.97,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5481,"POWERLINKV5_20151103074515","2010-05-21T01:15:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-19.62,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5485,"POWERLINKV5_20151103074515","2010-05-21T01:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-22.17,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5487,"POWERLINKV5_20151103074515","2010-05-21T02:00:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-20.32,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5488,"POWERLINKV5_20151103074515","2010-05-21T02:05:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-15.88,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5491,"POWERLINKV5_20151103074515","2010-05-21T02:20:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-22.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5494,"POWERLINKV5_20151103074515","2010-05-21T02:35:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-20.32,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5498,"POWERLINKV5_20151103074515","2010-05-21T03:05:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-22.18,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5501,"POWERLINKV5_20151103074515","2010-05-21T03:20:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-20.239999999999998,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5504,"POWERLINKV5_20151103074515","2010-05-21T03:35:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-19.559999999999999,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5506,"POWERLINKV5_20151103074515","2010-05-21T03:50:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.14,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5510,"POWERLINKV5_20151103074515","2010-05-21T04:10:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.15,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5511,"POWERLINKV5_20151103074515","2010-05-21T04:15:00","Q:N_BCKTR_BI_POT","Q-BRTR_8814_8815","2006-02-17",1,-13.16,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on loss of Boyne Island Potline, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5514,"POWERLINKV5_20151103074515","2010-05-21T06:50:00","Q:N_BCKTR_BCK2L-G","Q-BRTR_8814_8815","2006-02-17",1,-15.07,"Outage=either 8814,or 8815, or 9901, or 9902, or a Braemar Tx,  limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, ( Offset -100MW )","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815, refer to AFW Q10S/1220.","PLANNED",1]
[5517,"POWERLINKV5_20151103074515","2010-05-21T06:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.39,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0923.","PLANNED",1]
[5521,"POWERLINKV5_20151103074515","2010-05-21T23:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.29,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5524,"POWERLINKV5_20151103074515","2010-05-21T23:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.95,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5528,"POWERLINKV5_20151103074515","2010-05-22T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-26.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5529,"POWERLINKV5_20151103074515","2010-05-22T01:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-20.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5533,"POWERLINKV5_20151103074515","2010-05-22T02:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5534,"POWERLINKV5_20151103074515","2010-05-22T02:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.25,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5537,"POWERLINKV5_20151103074515","2010-05-22T02:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.170000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5540,"POWERLINKV5_20151103074515","2010-05-22T02:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.600000000000001,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5544,"POWERLINKV5_20151103074515","2010-05-22T03:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.91,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5547,"POWERLINKV5_20151103074515","2010-05-22T04:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.5,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5551,"POWERLINKV5_20151103074515","2010-05-22T04:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.18,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5552,"POWERLINKV5_20151103074515","2010-05-22T04:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.989999999999998,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5556,"POWERLINKV5_20151103074515","2010-05-22T05:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.57,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5557,"POWERLINKV5_20151103074515","2010-05-22T06:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.99,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5560,"POWERLINKV5_20151103074515","2010-05-22T06:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.989999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5564,"POWERLINKV5_20151103074515","2010-05-22T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.14,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5567,"POWERLINKV5_20151103074515","2010-05-22T14:35:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-12.99," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5570,"POWERLINKV5_20151103074515","2010-05-22T17:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-26.13,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5574,"POWERLINKV5_20151103074515","2010-05-22T22:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.93,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5575,"POWERLINKV5_20151103074515","2010-05-22T22:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5579,"POWERLINKV5_20151103074515","2010-05-23T01:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.86,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5580,"POWERLINKV5_20151103074515","2010-05-23T01:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5583,"POWERLINKV5_20151103074515","2010-05-23T02:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-17.66,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5587,"POWERLINKV5_20151103074515","2010-05-23T03:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.56,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5590,"POWERLINKV5_20151103074515","2010-05-23T04:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5593,"POWERLINKV5_20151103074515","2010-05-23T05:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-16.100000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5596,"POWERLINKV5_20151103074515","2010-05-23T12:50:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-22.91," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5599,"POWERLINKV5_20151103074515","2010-05-23T13:05:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-22.46," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5602,"POWERLINKV5_20151103074515","2010-05-23T13:25:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-21.59," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5603,"POWERLINKV5_20151103074515","2010-05-23T13:30:00","Q>>NIL_855_871","Q-NIL","2009-12-15",2,-62.05," To prevent thermal overload on Calvale to Wurdong 275kV fdr 871 on trip of Calvale to Stanwell (855), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5606,"POWERLINKV5_20151103074515","2010-05-23T20:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-16.3,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5610,"POWERLINKV5_20151103074515","2010-05-23T20:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.69,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5613,"POWERLINKV5_20151103074515","2010-05-23T20:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5616,"POWERLINKV5_20151103074515","2010-05-24T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-31.05,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5619,"POWERLINKV5_20151103074515","2010-05-24T02:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.73,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5622,"POWERLINKV5_20151103074515","2010-05-24T03:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.920000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5623,"POWERLINKV5_20151103074515","2010-05-24T05:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-19.82,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5626,"POWERLINKV5_20151103074515","2010-05-24T05:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.86,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5629,"POWERLINKV5_20151103074515","2010-05-24T11:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-1162.1300000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5633,"POWERLINKV5_20151103074515","2010-05-24T19:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.62,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5636,"POWERLINKV5_20151103074515","2010-05-24T22:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5639,"POWERLINKV5_20151103074515","2010-05-24T22:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5642,"POWERLINKV5_20151103074515","2010-05-24T22:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.68,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5645,"POWERLINKV5_20151103074515","2010-05-24T23:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.57,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5646,"POWERLINKV5_20151103074515","2010-05-24T23:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.89,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5649,"POWERLINKV5_20151103074515","2010-05-24T23:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.6,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5652,"POWERLINKV5_20151103074515","2010-05-25T00:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.46,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5656,"POWERLINKV5_20151103074515","2010-05-25T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.11,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5659,"POWERLINKV5_20151103074515","2010-05-25T01:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.79,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5663,"POWERLINKV5_20151103074515","2010-05-25T01:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-24.19,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5665,"POWERLINKV5_20151103074515","2010-05-25T02:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.78,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5668,"POWERLINKV5_20151103074515","2010-05-25T02:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.18,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5669,"POWERLINKV5_20151103074515","2010-05-25T02:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.190000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5672,"POWERLINKV5_20151103074515","2010-05-25T03:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.190000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5675,"POWERLINKV5_20151103074515","2010-05-25T03:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.1,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5679,"POWERLINKV5_20151103074515","2010-05-25T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.649999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5682,"POWERLINKV5_20151103074515","2010-05-25T10:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.149999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5686,"POWERLINKV5_20151103074515","2010-05-25T10:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.05,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5688,"POWERLINKV5_20151103074515","2010-05-25T10:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5691,"POWERLINKV5_20151103074515","2010-05-25T10:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.670000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5692,"POWERLINKV5_20151103074515","2010-05-25T10:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5695,"POWERLINKV5_20151103074515","2010-05-25T11:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.26,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5698,"POWERLINKV5_20151103074515","2010-05-25T11:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5702,"POWERLINKV5_20151103074515","2010-05-25T11:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5705,"POWERLINKV5_20151103074515","2010-05-25T11:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.49,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5707,"POWERLINKV5_20151103074515","2010-05-25T12:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.75,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5711,"POWERLINKV5_20151103074515","2010-05-25T12:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5714,"POWERLINKV5_20151103074515","2010-05-25T12:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.059999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5715,"POWERLINKV5_20151103074515","2010-05-25T12:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.739999999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5718,"POWERLINKV5_20151103074515","2010-05-25T12:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.62,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5722,"POWERLINKV5_20151103074515","2010-05-25T13:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.69,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5725,"POWERLINKV5_20151103074515","2010-05-25T20:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.23,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5728,"POWERLINKV5_20151103074515","2010-05-25T20:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.83,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5730,"POWERLINKV5_20151103074515","2010-05-25T20:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5734,"POWERLINKV5_20151103074515","2010-05-25T20:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.34,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5737,"POWERLINKV5_20151103074515","2010-05-25T21:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.73,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5738,"POWERLINKV5_20151103074515","2010-05-25T21:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5741,"POWERLINKV5_20151103074515","2010-05-25T22:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.56,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5745,"POWERLINKV5_20151103074515","2010-05-25T22:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.56,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5748,"POWERLINKV5_20151103074515","2010-05-25T22:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5751,"POWERLINKV5_20151103074515","2010-05-25T22:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.26,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5753,"POWERLINKV5_20151103074515","2010-05-25T23:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.26,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5757,"POWERLINKV5_20151103074515","2010-05-25T23:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.45,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5760,"POWERLINKV5_20151103074515","2010-05-26T00:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.55,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5761,"POWERLINKV5_20151103074515","2010-05-26T00:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.05,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5764,"POWERLINKV5_20151103074515","2010-05-26T00:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5768,"POWERLINKV5_20151103074515","2010-05-26T02:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5771,"POWERLINKV5_20151103074515","2010-05-26T03:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.14,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5774,"POWERLINKV5_20151103074515","2010-05-26T04:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.9,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5776,"POWERLINKV5_20151103074515","2010-05-26T05:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.78,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5780,"POWERLINKV5_20151103074515","2010-05-26T08:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.02,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5781,"POWERLINKV5_20151103074515","2010-05-26T08:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.87,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5784,"POWERLINKV5_20151103074515","2010-05-26T09:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.44,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5787,"POWERLINKV5_20151103074515","2010-05-26T09:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.119999999999999,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5791,"POWERLINKV5_20151103074515","2010-05-26T11:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.210000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5794,"POWERLINKV5_20151103074515","2010-05-26T16:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5797,"POWERLINKV5_20151103074515","2010-05-26T17:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.32,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5800,"POWERLINKV5_20151103074515","2010-05-26T17:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.62,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5803,"POWERLINKV5_20151103074515","2010-05-26T18:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.59,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5804,"POWERLINKV5_20151103074515","2010-05-26T18:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.21,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5807,"POWERLINKV5_20151103074515","2010-05-26T19:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-20.38,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5810,"POWERLINKV5_20151103074515","2010-05-26T19:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-18.3,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5814,"POWERLINKV5_20151103074515","2010-05-26T19:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-21.77,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5817,"POWERLINKV5_20151103074515","2010-05-26T19:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.65,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5820,"POWERLINKV5_20151103074515","2010-05-26T19:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.64,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5823,"POWERLINKV5_20151103074515","2010-05-26T20:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-19.37,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5826,"POWERLINKV5_20151103074515","2010-05-26T20:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5827,"POWERLINKV5_20151103074515","2010-05-26T20:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.05,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5830,"POWERLINKV5_20151103074515","2010-05-26T20:25:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.61,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5833,"POWERLINKV5_20151103074515","2010-05-26T20:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.47,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5837,"POWERLINKV5_20151103074515","2010-05-26T20:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.739999999999998,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5840,"POWERLINKV5_20151103074515","2010-05-26T20:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.25,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5843,"POWERLINKV5_20151103074515","2010-05-26T20:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.11,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5846,"POWERLINKV5_20151103074515","2010-05-26T21:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.57,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5849,"POWERLINKV5_20151103074515","2010-05-26T21:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.46,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5850,"POWERLINKV5_20151103074515","2010-05-26T21:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.43,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5853,"POWERLINKV5_20151103074515","2010-05-26T21:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.3,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5856,"POWERLINKV5_20151103074515","2010-05-26T22:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.670000000000002,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5860,"POWERLINKV5_20151103074515","2010-05-26T23:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.58,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5863,"POWERLINKV5_20151103074515","2010-05-26T23:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5866,"POWERLINKV5_20151103074515","2010-05-26T23:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.63,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5869,"POWERLINKV5_20151103074515","2010-05-27T00:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.84,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5872,"POWERLINKV5_20151103074515","2010-05-27T00:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5873,"POWERLINKV5_20151103074515","2010-05-27T00:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.17,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5876,"POWERLINKV5_20151103074515","2010-05-27T01:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.02,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5880,"POWERLINKV5_20151103074515","2010-05-27T02:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.77,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5883,"POWERLINKV5_20151103074515","2010-05-27T02:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.100000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5886,"POWERLINKV5_20151103074515","2010-05-27T02:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5889,"POWERLINKV5_20151103074515","2010-05-27T03:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.15,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5892,"POWERLINKV5_20151103074515","2010-05-27T04:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.02,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5895,"POWERLINKV5_20151103074515","2010-05-27T08:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5896,"POWERLINKV5_20151103074515","2010-05-27T08:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.68,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5899,"POWERLINKV5_20151103074515","2010-05-27T09:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.47,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5903,"POWERLINKV5_20151103074515","2010-05-27T09:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.94,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5906,"POWERLINKV5_20151103074515","2010-05-27T09:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5908,"POWERLINKV5_20151103074515","2010-05-27T09:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5912,"POWERLINKV5_20151103074515","2010-05-27T10:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.809999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5915,"POWERLINKV5_20151103074515","2010-05-27T10:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-24.74,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5916,"POWERLINKV5_20151103074515","2010-05-27T10:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.55,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5919,"POWERLINKV5_20151103074515","2010-05-27T10:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-13.41,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5922,"POWERLINKV5_20151103074515","2010-05-27T10:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.28,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5926,"POWERLINKV5_20151103074515","2010-05-27T10:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5929,"POWERLINKV5_20151103074515","2010-05-27T11:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.43,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5931,"POWERLINKV5_20151103074515","2010-05-27T11:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5935,"POWERLINKV5_20151103074515","2010-05-27T11:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5938,"POWERLINKV5_20151103074515","2010-05-27T11:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.98,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5939,"POWERLINKV5_20151103074515","2010-05-27T11:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5942,"POWERLINKV5_20151103074515","2010-05-27T11:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.98,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5945,"POWERLINKV5_20151103074515","2010-05-27T11:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.71,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5949,"POWERLINKV5_20151103074515","2010-05-27T11:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.1,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5952,"POWERLINKV5_20151103074515","2010-05-27T12:00:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.78,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5954,"POWERLINKV5_20151103074515","2010-05-27T12:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.7,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5958,"POWERLINKV5_20151103074515","2010-05-27T12:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.05,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5961,"POWERLINKV5_20151103074515","2010-05-27T12:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5962,"POWERLINKV5_20151103074515","2010-05-27T12:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5965,"POWERLINKV5_20151103074515","2010-05-27T13:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.37,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5968,"POWERLINKV5_20151103074515","2010-05-27T13:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5972,"POWERLINKV5_20151103074515","2010-05-27T15:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.2,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5975,"POWERLINKV5_20151103074515","2010-05-27T16:15:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-17.989999999999998,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5977,"POWERLINKV5_20151103074515","2010-05-27T16:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.6,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5981,"POWERLINKV5_20151103074515","2010-05-27T16:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.88,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5984,"POWERLINKV5_20151103074515","2010-05-27T17:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.72,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5985,"POWERLINKV5_20151103074515","2010-05-27T17:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.7,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5988,"POWERLINKV5_20151103074515","2010-05-27T18:10:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.73,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5991,"POWERLINKV5_20151103074515","2010-05-27T19:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.6,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[5995,"POWERLINKV5_20151103074515","2010-05-27T19:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.34,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5998,"POWERLINKV5_20151103074515","2010-05-27T19:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-22.72,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6001,"POWERLINKV5_20151103074515","2010-05-27T19:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.1,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6004,"POWERLINKV5_20151103074515","2010-05-27T19:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.13,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6007,"POWERLINKV5_20151103074515","2010-05-27T19:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.010000000000002,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6008,"POWERLINKV5_20151103074515","2010-05-27T19:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.79,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6011,"POWERLINKV5_20151103074515","2010-05-27T19:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-15.28,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6014,"POWERLINKV5_20151103074515","2010-05-27T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6018,"POWERLINKV5_20151103074515","2010-05-27T20:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6021,"POWERLINKV5_20151103074515","2010-05-27T20:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-16.36,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6024,"POWERLINKV5_20151103074515","2010-05-27T20:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-22.64,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6027,"POWERLINKV5_20151103074515","2010-05-27T20:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-19.52,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6030,"POWERLINKV5_20151103074515","2010-05-27T20:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.15,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6031,"POWERLINKV5_20151103074515","2010-05-27T20:45:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-14.63,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6034,"POWERLINKV5_20151103074515","2010-05-27T20:55:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-22.31,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6038,"POWERLINKV5_20151103074515","2010-05-27T21:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.33,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6041,"POWERLINKV5_20151103074515","2010-05-27T22:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.53,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6044,"POWERLINKV5_20151103074515","2010-05-27T22:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.71,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6047,"POWERLINKV5_20151103074515","2010-05-27T23:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.28,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6050,"POWERLINKV5_20151103074515","2010-05-28T00:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6053,"POWERLINKV5_20151103074515","2010-05-28T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.13,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6054,"POWERLINKV5_20151103074515","2010-05-28T01:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.03,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6057,"POWERLINKV5_20151103074515","2010-05-28T02:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.95,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6061,"POWERLINKV5_20151103074515","2010-05-28T03:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.260000000000002,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6064,"POWERLINKV5_20151103074515","2010-05-28T03:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.86,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6067,"POWERLINKV5_20151103074515","2010-05-28T06:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6070,"POWERLINKV5_20151103074515","2010-05-28T08:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.73,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6073,"POWERLINKV5_20151103074515","2010-05-28T08:35:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.199999999999999,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6074,"POWERLINKV5_20151103074515","2010-05-28T08:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.41,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6077,"POWERLINKV5_20151103074515","2010-05-28T09:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6080,"POWERLINKV5_20151103074515","2010-05-28T09:20:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.42,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6084,"POWERLINKV5_20151103074515","2010-05-28T09:30:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-12.29,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6087,"POWERLINKV5_20151103074515","2010-05-28T09:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.18,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6090,"POWERLINKV5_20151103074515","2010-05-28T10:50:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.37,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0924.","PLANNED",1]
[6093,"POWERLINKV5_20151103074515","2010-05-29T03:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.8,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6096,"POWERLINKV5_20151103074515","2010-05-31T20:05:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-11.45,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0925.","PLANNED",1]
[6097,"POWERLINKV5_20151103074515","2010-06-02T20:40:00","Q>GBMU_GBMU_MDSPT","Q-GBMU_835_836","2010-05-17",2,-10.58,"Out= 835 or 836 Greenbank to Mudgeeraba 275kV line with parallel 110kV network closed, avoid O/L F907 Molendinar to Southport 110kV line on trip of remaining 835 or 836 Greenbank to Mudgeeraba 275kV line, Feedback","OUTAGE","OTHER","Feeder 836","REGULATED","INCLUDED","Planned outage of Feeder 836, refer to AFW Q10S/0925.","PLANNED",1]
[6100,"POWERLINKV5_20151103074515","2010-06-03T20:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6103,"POWERLINKV5_20151103074515","2010-06-03T20:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.79,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6107,"POWERLINKV5_20151103074515","2010-06-04T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6109,"POWERLINKV5_20151103074515","2010-06-04T20:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.87,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6112,"POWERLINKV5_20151103074515","2010-06-04T21:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6116,"POWERLINKV5_20151103074515","2010-06-04T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-57.06,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6119,"POWERLINKV5_20151103074515","2010-06-04T22:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6120,"POWERLINKV5_20151103074515","2010-06-04T22:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6123,"POWERLINKV5_20151103074515","2010-06-04T23:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-26.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6126,"POWERLINKV5_20151103074515","2010-06-04T23:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6130,"POWERLINKV5_20151103074515","2010-06-05T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.58,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6132,"POWERLINKV5_20151103074515","2010-06-05T08:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6136,"POWERLINKV5_20151103074515","2010-06-05T08:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-33.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6139,"POWERLINKV5_20151103074515","2010-06-05T08:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-61.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6142,"POWERLINKV5_20151103074515","2010-06-05T09:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-28.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6143,"POWERLINKV5_20151103074515","2010-06-05T09:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-60.71,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6146,"POWERLINKV5_20151103074515","2010-06-05T09:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-28.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6149,"POWERLINKV5_20151103074515","2010-06-05T09:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-47.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6153,"POWERLINKV5_20151103074515","2010-06-05T09:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-47.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6155,"POWERLINKV5_20151103074515","2010-06-05T10:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-25.1,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6159,"POWERLINKV5_20151103074515","2010-06-05T10:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6162,"POWERLINKV5_20151103074515","2010-06-05T10:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6165,"POWERLINKV5_20151103074515","2010-06-05T10:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6166,"POWERLINKV5_20151103074515","2010-06-05T11:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.65,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6169,"POWERLINKV5_20151103074515","2010-06-05T11:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.79,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6172,"POWERLINKV5_20151103074515","2010-06-05T11:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.58,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6176,"POWERLINKV5_20151103074515","2010-06-05T12:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.43,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6178,"POWERLINKV5_20151103074515","2010-06-05T12:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.029999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6182,"POWERLINKV5_20151103074515","2010-06-05T13:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.04,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6185,"POWERLINKV5_20151103074515","2010-06-05T14:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6188,"POWERLINKV5_20151103074515","2010-06-05T15:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.03,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6189,"POWERLINKV5_20151103074515","2010-06-05T15:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-77.17,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6192,"POWERLINKV5_20151103074515","2010-06-05T15:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-66.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6196,"POWERLINKV5_20151103074515","2010-06-05T15:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-76.45,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6199,"POWERLINKV5_20151103074515","2010-06-05T16:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-25.83,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6201,"POWERLINKV5_20151103074515","2010-06-05T16:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-27.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6205,"POWERLINKV5_20151103074515","2010-06-05T16:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6208,"POWERLINKV5_20151103074515","2010-06-05T16:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-63.31,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6211,"POWERLINKV5_20151103074515","2010-06-05T17:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-89.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6212,"POWERLINKV5_20151103074515","2010-06-05T17:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-170.37,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6215,"POWERLINKV5_20151103074515","2010-06-05T17:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-31.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6219,"POWERLINKV5_20151103074515","2010-06-05T18:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-31.31,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6222,"POWERLINKV5_20151103074515","2010-06-05T19:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6224,"POWERLINKV5_20151103074515","2010-06-05T19:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6228,"POWERLINKV5_20151103074515","2010-06-05T19:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6231,"POWERLINKV5_20151103074515","2010-06-05T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-21.86,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6232,"POWERLINKV5_20151103074515","2010-06-05T20:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6235,"POWERLINKV5_20151103074515","2010-06-05T20:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-59.76,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6238,"POWERLINKV5_20151103074515","2010-06-05T20:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-62.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6242,"POWERLINKV5_20151103074515","2010-06-05T21:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-45.83,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6245,"POWERLINKV5_20151103074515","2010-06-05T21:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-36.57,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6247,"POWERLINKV5_20151103074515","2010-06-05T21:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6251,"POWERLINKV5_20151103074515","2010-06-05T21:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.56,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6254,"POWERLINKV5_20151103074515","2010-06-05T22:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.559999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6255,"POWERLINKV5_20151103074515","2010-06-05T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.04,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6258,"POWERLINKV5_20151103074515","2010-06-05T22:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-61.59,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6261,"POWERLINKV5_20151103074515","2010-06-05T22:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-58.85,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6265,"POWERLINKV5_20151103074515","2010-06-05T23:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-48.45,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6268,"POWERLINKV5_20151103074515","2010-06-05T23:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-49.83,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6270,"POWERLINKV5_20151103074515","2010-06-05T23:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-49.19,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6274,"POWERLINKV5_20151103074515","2010-06-05T23:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-51.48,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6277,"POWERLINKV5_20151103074515","2010-06-06","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-37.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6278,"POWERLINKV5_20151103074515","2010-06-06T00:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.39,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6281,"POWERLINKV5_20151103074515","2010-06-06T00:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.99,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6284,"POWERLINKV5_20151103074515","2010-06-06T00:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.04,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6288,"POWERLINKV5_20151103074515","2010-06-06T01:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6291,"POWERLINKV5_20151103074515","2010-06-06T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6294,"POWERLINKV5_20151103074515","2010-06-06T02:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.43,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6297,"POWERLINKV5_20151103074515","2010-06-06T08:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6300,"POWERLINKV5_20151103074515","2010-06-06T08:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-18.559999999999999,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6301,"POWERLINKV5_20151103074515","2010-06-06T08:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.39,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6304,"POWERLINKV5_20151103074515","2010-06-06T09:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6307,"POWERLINKV5_20151103074515","2010-06-06T09:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-53.19,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6310,"POWERLINKV5_20151103074515","2010-06-06T09:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-60.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6313,"POWERLINKV5_20151103074515","2010-06-06T09:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-64.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6317,"POWERLINKV5_20151103074515","2010-06-06T10:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-60.66,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6320,"POWERLINKV5_20151103074515","2010-06-06T10:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-62.69,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6323,"POWERLINKV5_20151103074515","2010-06-06T10:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-61.22,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6324,"POWERLINKV5_20151103074515","2010-06-06T10:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-61.96,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6327,"POWERLINKV5_20151103074515","2010-06-06T11:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-62.4,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6331,"POWERLINKV5_20151103074515","2010-06-06T11:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-24.96,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6333,"POWERLINKV5_20151103074515","2010-06-06T11:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-23.85,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6336,"POWERLINKV5_20151103074515","2010-06-06T11:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-53.78,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6340,"POWERLINKV5_20151103074515","2010-06-06T12:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-30.42,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6343,"POWERLINKV5_20151103074515","2010-06-06T12:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-21.36,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6346,"POWERLINKV5_20151103074515","2010-06-06T12:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.55,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6347,"POWERLINKV5_20151103074515","2010-06-06T12:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.46,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6350,"POWERLINKV5_20151103074515","2010-06-06T13:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.11,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6354,"POWERLINKV5_20151103074515","2010-06-06T16:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6356,"POWERLINKV5_20151103074515","2010-06-06T16:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6359,"POWERLINKV5_20151103074515","2010-06-06T16:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.53,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6363,"POWERLINKV5_20151103074515","2010-06-06T19:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6366,"POWERLINKV5_20151103074515","2010-06-06T20:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-28.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6369,"POWERLINKV5_20151103074515","2010-06-06T21:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.67,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6370,"POWERLINKV5_20151103074515","2010-06-07T08:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.45,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6373,"POWERLINKV5_20151103074515","2010-06-07T09:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-31.32,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6377,"POWERLINKV5_20151103074515","2010-06-07T09:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6379,"POWERLINKV5_20151103074515","2010-06-07T09:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6382,"POWERLINKV5_20151103074515","2010-06-07T10:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6386,"POWERLINKV5_20151103074515","2010-06-07T10:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6389,"POWERLINKV5_20151103074515","2010-06-07T11:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.85,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6390,"POWERLINKV5_20151103074515","2010-06-07T11:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.64,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6393,"POWERLINKV5_20151103074515","2010-06-07T12:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6396,"POWERLINKV5_20151103074515","2010-06-07T12:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6400,"POWERLINKV5_20151103074515","2010-06-07T13:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6402,"POWERLINKV5_20151103074515","2010-06-07T13:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6405,"POWERLINKV5_20151103074515","2010-06-07T14:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.44,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6409,"POWERLINKV5_20151103074515","2010-06-07T16:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.06,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6412,"POWERLINKV5_20151103074515","2010-06-07T16:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.63,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6413,"POWERLINKV5_20151103074515","2010-06-07T17:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-31.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6416,"POWERLINKV5_20151103074515","2010-06-07T19:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-18.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6419,"POWERLINKV5_20151103074515","2010-06-07T20:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-24.27,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6423,"POWERLINKV5_20151103074515","2010-06-07T20:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.63,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6425,"POWERLINKV5_20151103074515","2010-06-07T20:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-25.79,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6428,"POWERLINKV5_20151103074515","2010-06-07T20:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-23.72,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6432,"POWERLINKV5_20151103074515","2010-06-07T21:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-39.479999999999997,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6435,"POWERLINKV5_20151103074515","2010-06-07T21:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.51,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6436,"POWERLINKV5_20151103074515","2010-06-07T21:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.02,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6439,"POWERLINKV5_20151103074515","2010-06-07T21:45:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-13.78,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6442,"POWERLINKV5_20151103074515","2010-06-07T22:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-60.92,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6446,"POWERLINKV5_20151103074515","2010-06-07T22:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.61,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6448,"POWERLINKV5_20151103074515","2010-06-07T23:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.5,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6452,"POWERLINKV5_20151103074515","2010-06-08T08:25:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-18.64,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6455,"POWERLINKV5_20151103074515","2010-06-08T08:40:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-13.08,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6458,"POWERLINKV5_20151103074515","2010-06-08T09:05:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-11.36,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6459,"POWERLINKV5_20151103074515","2010-06-08T09:10:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-10.99,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6462,"POWERLINKV5_20151103074515","2010-06-08T09:25:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-11.51,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6465,"POWERLINKV5_20151103074515","2010-06-08T09:40:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-11.9,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6469,"POWERLINKV5_20151103074515","2010-06-08T10:10:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-11.16,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6471,"POWERLINKV5_20151103074515","2010-06-08T10:25:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-10.33,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6475,"POWERLINKV5_20151103074515","2010-06-08T10:45:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-10.029999999999999,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6478,"POWERLINKV5_20151103074515","2010-06-08T11:00:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-10.039999999999999,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6481,"POWERLINKV5_20151103074515","2010-06-08T11:25:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-11.95,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6482,"POWERLINKV5_20151103074515","2010-06-08T11:35:00","CA_BPS_3B1F648C_01","CA_BPS_3B1F648C","2010-06-07",1,-10.15,"Constraint Automation, O/L 330KV_9902    @R2_BRAE for CTG LQOA on trip of 9901 R2_BRAE - R3_BULLI 330KV LINE.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Planned outage of Feeder 8814, refer to AFW Q10S/0806 and Market Notice 32061.","PLANNED",1]
[6485,"POWERLINKV5_20151103074515","2010-06-10T20:35:00","Q>>TRBR_BRBC","Q-TRBR","2010-06-10",1,-12.11,"Outage = 8814 or 8815 275kV feeder Tarong to Braemar, for trip of either 9901 or 9902 330kV feeder Braemar to Bulli Creek to prevent thermal O/L on remaining 9901 or 9902","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Unplanned outage of Feeder 8814, refer to Market Notice 32099.","UNPLANNED",1]
[6489,"POWERLINKV5_20151103074515","2010-06-10T21:30:00","Q>>TRBR_BRBC","Q-TRBR","2010-06-10",1,-12.82,"Outage = 8814 or 8815 275kV feeder Tarong to Braemar, for trip of either 9901 or 9902 330kV feeder Braemar to Bulli Creek to prevent thermal O/L on remaining 9901 or 9902","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Unplanned outage of Feeder 8814, refer to Market Notice 32099.","UNPLANNED",1]
[6492,"POWERLINKV5_20151103074515","2010-06-10T22:10:00","Q>>TRBR_BRBC","Q-TRBR","2010-06-10",1,-10.16,"Outage = 8814 or 8815 275kV feeder Tarong to Braemar, for trip of either 9901 or 9902 330kV feeder Braemar to Bulli Creek to prevent thermal O/L on remaining 9901 or 9902","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Unplanned outage of Feeder 8814, refer to Market Notice 32099.","UNPLANNED",1]
[6494,"POWERLINKV5_20151103074515","2010-06-10T22:25:00","Q>>TRBR_BRBC","Q-TRBR","2010-06-10",1,-10.25,"Outage = 8814 or 8815 275kV feeder Tarong to Braemar, for trip of either 9901 or 9902 330kV feeder Braemar to Bulli Creek to prevent thermal O/L on remaining 9901 or 9902","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Unplanned outage of Feeder 8814, refer to Market Notice 32099.","UNPLANNED",1]
[6498,"POWERLINKV5_20151103074515","2010-06-12T09:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-17.59,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6501,"POWERLINKV5_20151103074515","2010-06-12T20:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.68,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6504,"POWERLINKV5_20151103074515","2010-06-12T20:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.2,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6505,"POWERLINKV5_20151103074515","2010-06-12T20:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-19.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6508,"POWERLINKV5_20151103074515","2010-06-12T21:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.58,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6511,"POWERLINKV5_20151103074515","2010-06-12T21:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-21.55,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6514,"POWERLINKV5_20151103074515","2010-06-12T22:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.88,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6517,"POWERLINKV5_20151103074515","2010-06-12T22:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.07,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6521,"POWERLINKV5_20151103074515","2010-06-12T22:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.63,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6524,"POWERLINKV5_20151103074515","2010-06-14T05:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.42,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6527,"POWERLINKV5_20151103074515","2010-06-14T19:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.81,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6528,"POWERLINKV5_20151103074515","2010-06-14T19:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.07,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6531,"POWERLINKV5_20151103074515","2010-06-14T20:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.93,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6534,"POWERLINKV5_20151103074515","2010-06-14T20:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.739999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6537,"POWERLINKV5_20151103074515","2010-06-14T20:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6540,"POWERLINKV5_20151103074515","2010-06-14T20:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6544,"POWERLINKV5_20151103074515","2010-06-14T21:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-26.72,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6547,"POWERLINKV5_20151103074515","2010-06-14T21:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.100000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6548,"POWERLINKV5_20151103074515","2010-06-14T22:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6551,"POWERLINKV5_20151103074515","2010-06-14T22:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.82,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6554,"POWERLINKV5_20151103074515","2010-06-14T22:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.38,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6557,"POWERLINKV5_20151103074515","2010-06-14T23:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6560,"POWERLINKV5_20151103074515","2010-06-15T01:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.38,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6563,"POWERLINKV5_20151103074515","2010-06-15T01:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.73,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6567,"POWERLINKV5_20151103074515","2010-06-15T07:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.199999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6570,"POWERLINKV5_20151103074515","2010-06-15T20:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6571,"POWERLINKV5_20151103074515","2010-06-15T20:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.03,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6574,"POWERLINKV5_20151103074515","2010-06-15T20:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.12,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6577,"POWERLINKV5_20151103074515","2010-06-15T21:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.31,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6580,"POWERLINKV5_20151103074515","2010-06-16T10:40:00","QNTE_ROC","Q-NIL","2006-12-27",1,-10.17,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6583,"POWERLINKV5_20151103074515","2010-06-19T22:30:00","Q>>PWSP_WOSP_SPCE","Q-808_PARALLEL_CLOSE","2010-05-31",1,-15.04,"Out= 808 Palmwoods to South Pine 275kV line, avoid O/L 745/1 or 746/1 South Pine to Caboolture 110kV line on trip of 807 Woolooga to South Pine 275kV line, Feedback.","OUTAGE","OTHER","Feeder 808","REGULATED","INCLUDED","Outage of Feeder 808, refer to AFW Q10S/1399.","PLANNED",1]
[6586,"POWERLINKV5_20151103074515","2010-06-21T08:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6590,"POWERLINKV5_20151103074515","2010-06-21T08:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6593,"POWERLINKV5_20151103074515","2010-06-21T12:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6594,"POWERLINKV5_20151103074515","2010-06-21T12:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6597,"POWERLINKV5_20151103074515","2010-06-21T13:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.17,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6600,"POWERLINKV5_20151103074515","2010-06-21T14:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6603,"POWERLINKV5_20151103074515","2010-06-21T16:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6606,"POWERLINKV5_20151103074515","2010-06-21T16:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6610,"POWERLINKV5_20151103074515","2010-06-21T19:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6613,"POWERLINKV5_20151103074515","2010-06-21T20:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.49,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6616,"POWERLINKV5_20151103074515","2010-06-21T20:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-28.03,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6617,"POWERLINKV5_20151103074515","2010-06-21T20:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.309999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6620,"POWERLINKV5_20151103074515","2010-06-21T20:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.670000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6624,"POWERLINKV5_20151103074515","2010-06-21T20:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.54,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6626,"POWERLINKV5_20151103074515","2010-06-21T21:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6629,"POWERLINKV5_20151103074515","2010-06-21T21:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6633,"POWERLINKV5_20151103074515","2010-06-21T21:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6636,"POWERLINKV5_20151103074515","2010-06-21T22:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.66,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6639,"POWERLINKV5_20151103074515","2010-06-21T22:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.07,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6640,"POWERLINKV5_20151103074515","2010-06-21T22:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.36,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6643,"POWERLINKV5_20151103074515","2010-06-21T23:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.35,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6647,"POWERLINKV5_20151103074515","2010-06-21T23:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6649,"POWERLINKV5_20151103074515","2010-06-22T01:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.06,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6652,"POWERLINKV5_20151103074515","2010-06-22T01:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.68,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6656,"POWERLINKV5_20151103074515","2010-06-22T01:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6659,"POWERLINKV5_20151103074515","2010-06-22T07:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.8,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6662,"POWERLINKV5_20151103074515","2010-06-22T08:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6663,"POWERLINKV5_20151103074515","2010-06-22T08:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.73,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6666,"POWERLINKV5_20151103074515","2010-06-22T08:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.15,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6670,"POWERLINKV5_20151103074515","2010-06-22T08:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6672,"POWERLINKV5_20151103074515","2010-06-22T09:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.4,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6675,"POWERLINKV5_20151103074515","2010-06-22T09:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.86,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6679,"POWERLINKV5_20151103074515","2010-06-22T09:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.86,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6682,"POWERLINKV5_20151103074515","2010-06-22T09:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6685,"POWERLINKV5_20151103074515","2010-06-22T10:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6686,"POWERLINKV5_20151103074515","2010-06-22T10:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6689,"POWERLINKV5_20151103074515","2010-06-22T10:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6693,"POWERLINKV5_20151103074515","2010-06-22T11:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.4,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6695,"POWERLINKV5_20151103074515","2010-06-22T11:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.3,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6698,"POWERLINKV5_20151103074515","2010-06-22T11:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.25,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6702,"POWERLINKV5_20151103074515","2010-06-22T13:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.57,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6705,"POWERLINKV5_20151103074515","2010-06-22T13:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6706,"POWERLINKV5_20151103074515","2010-06-22T13:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.63,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6709,"POWERLINKV5_20151103074515","2010-06-22T14:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6712,"POWERLINKV5_20151103074515","2010-06-22T14:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6716,"POWERLINKV5_20151103074515","2010-06-22T16:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.57,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6718,"POWERLINKV5_20151103074515","2010-06-22T16:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6721,"POWERLINKV5_20151103074515","2010-06-22T17:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6725,"POWERLINKV5_20151103074515","2010-06-23T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.38,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6728,"POWERLINKV5_20151103074515","2010-06-25T21:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.47,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6729,"POWERLINKV5_20151103074515","2010-06-25T22:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.16,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6732,"POWERLINKV5_20151103074515","2010-06-25T22:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.47,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6735,"POWERLINKV5_20151103074515","2010-06-25T22:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.039999999999999,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6738,"POWERLINKV5_20151103074515","2010-06-26T01:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.01,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6741,"POWERLINKV5_20151103074515","2010-06-26T10:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.35,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6745,"POWERLINKV5_20151103074515","2010-06-26T10:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.89,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6748,"POWERLINKV5_20151103074515","2010-06-26T11:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.96,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6751,"POWERLINKV5_20151103074515","2010-06-26T11:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.68,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6752,"POWERLINKV5_20151103074515","2010-06-26T11:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.68,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6755,"POWERLINKV5_20151103074515","2010-06-26T11:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.06,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6758,"POWERLINKV5_20151103074515","2010-06-26T12:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.85,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6761,"POWERLINKV5_20151103074515","2010-06-26T12:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.16,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6764,"POWERLINKV5_20151103074515","2010-06-26T16:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.29,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6768,"POWERLINKV5_20151103074515","2010-06-26T17:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-17.96,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6771,"POWERLINKV5_20151103074515","2010-06-26T17:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.66,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6774,"POWERLINKV5_20151103074515","2010-06-26T17:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6775,"POWERLINKV5_20151103074515","2010-06-26T18:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-40.01,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6778,"POWERLINKV5_20151103074515","2010-06-26T18:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-49.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6781,"POWERLINKV5_20151103074515","2010-06-26T18:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-43.89,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6784,"POWERLINKV5_20151103074515","2010-06-26T19:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.3,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6787,"POWERLINKV5_20151103074515","2010-06-26T19:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-27.42,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6791,"POWERLINKV5_20151103074515","2010-06-26T20:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.13,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6794,"POWERLINKV5_20151103074515","2010-06-26T20:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6797,"POWERLINKV5_20151103074515","2010-06-26T20:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.68,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6798,"POWERLINKV5_20151103074515","2010-06-26T20:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.02,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6801,"POWERLINKV5_20151103074515","2010-06-26T20:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.85,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6804,"POWERLINKV5_20151103074515","2010-06-26T21:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.33,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6807,"POWERLINKV5_20151103074515","2010-06-26T21:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.35,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6810,"POWERLINKV5_20151103074515","2010-06-26T21:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.52,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6814,"POWERLINKV5_20151103074515","2010-06-26T22:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.03,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6817,"POWERLINKV5_20151103074515","2010-06-27T17:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6820,"POWERLINKV5_20151103074515","2010-06-27T17:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-57.97,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6821,"POWERLINKV5_20151103074515","2010-06-27T18:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.01,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6825,"POWERLINKV5_20151103074515","2010-06-27T19:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.89,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6827,"POWERLINKV5_20151103074515","2010-06-27T19:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.3,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6830,"POWERLINKV5_20151103074515","2010-06-27T19:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.44,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6833,"POWERLINKV5_20151103074515","2010-06-27T20:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.68,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6837,"POWERLINKV5_20151103074515","2010-06-28T14:05:00","Q_CPSA_72","Q-CLBCON_7355","2010-04-15",1,-1024.98,"Discretionary, Condamine PS =< 72MW","OUTAGE","OTHER","Condamine PS","REGULATED","3","Ergon and Condamine PS otuage","PLANNED",0]
[6840,"POWERLINKV5_20151103074515","2010-06-28T22:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.19,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6843,"POWERLINKV5_20151103074515","2010-06-29T10:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.87,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6844,"POWERLINKV5_20151103074515","2010-06-29T10:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6848,"POWERLINKV5_20151103074515","2010-07-01T00:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.54,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6850,"POWERLINKV5_20151103074515","2010-07-01T01:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6853,"POWERLINKV5_20151103074515","2010-07-01T01:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.67,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6856,"POWERLINKV5_20151103074515","2010-07-01T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.58,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6860,"POWERLINKV5_20151103074515","2010-07-01T01:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.29,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6863,"POWERLINKV5_20151103074515","2010-07-01T02:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.35,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6864,"POWERLINKV5_20151103074515","2010-07-01T02:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6867,"POWERLINKV5_20151103074515","2010-07-01T02:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.91,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6871,"POWERLINKV5_20151103074515","2010-07-01T03:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.87,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6873,"POWERLINKV5_20151103074515","2010-07-01T16:50:00","Q>>BCGL_CLWU_LCGL","Q-BCGL_812","2010-06-29",2,-16.420000000000002,"Out= Bouldercombe to Gladstone (812), avoid O/L Larcom Creek to Gladstone (8859) on trip of Calvale to Wurdong (871), Feedback","OUTAGE","OTHER","Feeder 812","REGULATED","INCLUDED","Outage of Feeder 812, refer to AFW Q10S/1486.","PLANNED",1]
[6876,"POWERLINKV5_20151103074515","2010-07-02T02:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.97,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6879,"POWERLINKV5_20151103074515","2010-07-02T22:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-21.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6883,"POWERLINKV5_20151103074515","2010-07-03T01:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.51,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6886,"POWERLINKV5_20151103074515","2010-07-03T16:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.75,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6887,"POWERLINKV5_20151103074515","2010-07-05T04:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.1,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6890,"POWERLINKV5_20151103074515","2010-07-06T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.02,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6894,"POWERLINKV5_20151103074515","2010-07-07T03:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6896,"POWERLINKV5_20151103074515","2010-07-07T09:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.79,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6899,"POWERLINKV5_20151103074515","2010-07-07T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6903,"POWERLINKV5_20151103074515","2010-07-07T22:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.26,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6906,"POWERLINKV5_20151103074515","2010-07-08T20:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6909,"POWERLINKV5_20151103074515","2010-07-09T02:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6910,"POWERLINKV5_20151103074515","2010-07-09T03:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.69,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6913,"POWERLINKV5_20151103074515","2010-07-10T03:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.3,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6917,"POWERLINKV5_20151103074515","2010-07-10T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.79,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6919,"POWERLINKV5_20151103074515","2010-07-10T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6922,"POWERLINKV5_20151103074515","2010-07-10T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6926,"POWERLINKV5_20151103074515","2010-07-15T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6929,"POWERLINKV5_20151103074515","2010-07-15T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-18.260000000000002,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6932,"POWERLINKV5_20151103074515","2010-07-16T11:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.18,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6933,"POWERLINKV5_20151103074515","2010-07-16T11:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6936,"POWERLINKV5_20151103074515","2010-07-16T12:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6938,"POWERLINKV5_20151103074515","2010-07-16T12:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6942,"POWERLINKV5_20151103074515","2010-07-16T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6945,"POWERLINKV5_20151103074515","2010-07-16T12:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6949,"POWERLINKV5_20151103074515","2010-07-16T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6952,"POWERLINKV5_20151103074515","2010-07-16T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6955,"POWERLINKV5_20151103074515","2010-07-16T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6956,"POWERLINKV5_20151103074515","2010-07-16T14:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6959,"POWERLINKV5_20151103074515","2010-07-16T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.62,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6962,"POWERLINKV5_20151103074515","2010-07-16T14:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6965,"POWERLINKV5_20151103074515","2010-07-16T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6968,"POWERLINKV5_20151103074515","2010-07-16T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6972,"POWERLINKV5_20151103074515","2010-07-16T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6975,"POWERLINKV5_20151103074515","2010-07-16T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6978,"POWERLINKV5_20151103074515","2010-07-16T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.14,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6979,"POWERLINKV5_20151103074515","2010-07-16T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6982,"POWERLINKV5_20151103074515","2010-07-16T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6985,"POWERLINKV5_20151103074515","2010-07-16T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6988,"POWERLINKV5_20151103074515","2010-07-16T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6991,"POWERLINKV5_20151103074515","2010-07-16T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.98,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6995,"POWERLINKV5_20151103074515","2010-07-16T23:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6998,"POWERLINKV5_20151103074515","2010-07-16T23:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6999,"POWERLINKV5_20151103074515","2010-07-16T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.01,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7002,"POWERLINKV5_20151103074515","2010-07-17T00:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7005,"POWERLINKV5_20151103074515","2010-07-17T00:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7008,"POWERLINKV5_20151103074515","2010-07-17T11:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7011,"POWERLINKV5_20151103074515","2010-07-17T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7014,"POWERLINKV5_20151103074515","2010-07-17T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7018,"POWERLINKV5_20151103074515","2010-07-17T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7021,"POWERLINKV5_20151103074515","2010-07-17T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.25,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7022,"POWERLINKV5_20151103074515","2010-07-17T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.79,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7026,"POWERLINKV5_20151103074515","2010-07-17T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7027,"POWERLINKV5_20151103074515","2010-07-17T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.5,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7031,"POWERLINKV5_20151103074515","2010-07-17T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7034,"POWERLINKV5_20151103074515","2010-07-17T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7037,"POWERLINKV5_20151103074515","2010-07-17T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7041,"POWERLINKV5_20151103074515","2010-07-17T14:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7044,"POWERLINKV5_20151103074515","2010-07-17T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.08,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7045,"POWERLINKV5_20151103074515","2010-07-17T15:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7049,"POWERLINKV5_20151103074515","2010-07-17T15:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7050,"POWERLINKV5_20151103074515","2010-07-17T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7054,"POWERLINKV5_20151103074515","2010-07-17T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7057,"POWERLINKV5_20151103074515","2010-07-17T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7061,"POWERLINKV5_20151103074515","2010-07-17T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7064,"POWERLINKV5_20151103074515","2010-07-17T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7067,"POWERLINKV5_20151103074515","2010-07-17T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.61,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7068,"POWERLINKV5_20151103074515","2010-07-17T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.95,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7072,"POWERLINKV5_20151103074515","2010-07-17T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7073,"POWERLINKV5_20151103074515","2010-07-17T17:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7077,"POWERLINKV5_20151103074515","2010-07-17T23:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1026.57,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7080,"POWERLINKV5_20151103074515","2010-07-17T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022.76,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7084,"POWERLINKV5_20151103074515","2010-07-18T00:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7087,"POWERLINKV5_20151103074515","2010-07-18T00:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7090,"POWERLINKV5_20151103074515","2010-07-18T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.17,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7091,"POWERLINKV5_20151103074515","2010-07-18T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.26,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7095,"POWERLINKV5_20151103074515","2010-07-18T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7096,"POWERLINKV5_20151103074515","2010-07-18T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.33,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7100,"POWERLINKV5_20151103074515","2010-07-18T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.7,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7103,"POWERLINKV5_20151103074515","2010-07-18T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1011.45,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7107,"POWERLINKV5_20151103074515","2010-07-18T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7110,"POWERLINKV5_20151103074515","2010-07-18T08:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.58,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7113,"POWERLINKV5_20151103074515","2010-07-18T09:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.64,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7114,"POWERLINKV5_20151103074515","2010-07-18T09:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7118,"POWERLINKV5_20151103074515","2010-07-18T10:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7120,"POWERLINKV5_20151103074515","2010-07-18T10:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7123,"POWERLINKV5_20151103074515","2010-07-18T10:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7126,"POWERLINKV5_20151103074515","2010-07-18T10:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7130,"POWERLINKV5_20151103074515","2010-07-18T11:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7133,"POWERLINKV5_20151103074515","2010-07-18T11:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.41,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7136,"POWERLINKV5_20151103074515","2010-07-18T11:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7137,"POWERLINKV5_20151103074515","2010-07-18T11:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7139,"POWERLINKV5_20151103074515","2010-07-18T12:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7143,"POWERLINKV5_20151103074515","2010-07-18T12:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.15,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7146,"POWERLINKV5_20151103074515","2010-07-18T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7149,"POWERLINKV5_20151103074515","2010-07-18T12:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.73,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7153,"POWERLINKV5_20151103074515","2010-07-18T13:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.92,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7156,"POWERLINKV5_20151103074515","2010-07-18T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7157,"POWERLINKV5_20151103074515","2010-07-18T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.61,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7160,"POWERLINKV5_20151103074515","2010-07-18T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7162,"POWERLINKV5_20151103074515","2010-07-18T13:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7166,"POWERLINKV5_20151103074515","2010-07-18T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7169,"POWERLINKV5_20151103074515","2010-07-18T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7172,"POWERLINKV5_20151103074515","2010-07-18T14:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.23,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7176,"POWERLINKV5_20151103074515","2010-07-18T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7179,"POWERLINKV5_20151103074515","2010-07-18T15:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.38,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7180,"POWERLINKV5_20151103074515","2010-07-18T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.96,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7183,"POWERLINKV5_20151103074515","2010-07-18T15:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7185,"POWERLINKV5_20151103074515","2010-07-18T15:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1019.84,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7189,"POWERLINKV5_20151103074515","2010-07-18T16:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.69,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7192,"POWERLINKV5_20151103074515","2010-07-18T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7195,"POWERLINKV5_20151103074515","2010-07-18T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.86,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7199,"POWERLINKV5_20151103074515","2010-07-18T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.48,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7202,"POWERLINKV5_20151103074515","2010-07-18T21:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7203,"POWERLINKV5_20151103074515","2010-07-18T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.12,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7206,"POWERLINKV5_20151103074515","2010-07-18T21:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7208,"POWERLINKV5_20151103074515","2010-07-18T22:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1023.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7212,"POWERLINKV5_20151103074515","2010-07-19T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.34,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7215,"POWERLINKV5_20151103074515","2010-07-19T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7219,"POWERLINKV5_20151103074515","2010-07-19T03:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.03,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7222,"POWERLINKV5_20151103074515","2010-07-19T03:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1015.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7225,"POWERLINKV5_20151103074515","2010-07-19T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.64,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7226,"POWERLINKV5_20151103074515","2010-07-19T04:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7229,"POWERLINKV5_20151103074515","2010-07-19T04:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.02,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7231,"POWERLINKV5_20151103074515","2010-07-19T19:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7235,"POWERLINKV5_20151103074515","2010-07-20T01:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.49,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7238,"POWERLINKV5_20151103074515","2010-07-20T06:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7242,"POWERLINKV5_20151103074515","2010-07-20T09:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.739999999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7245,"POWERLINKV5_20151103074515","2010-07-20T09:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7248,"POWERLINKV5_20151103074515","2010-07-20T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7250,"POWERLINKV5_20151103074515","2010-07-21T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.74,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7251,"POWERLINKV5_20151103074515","2010-07-21T02:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.79,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7254,"POWERLINKV5_20151103074515","2010-07-21T09:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.69,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7258,"POWERLINKV5_20151103074515","2010-07-21T10:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7261,"POWERLINKV5_20151103074515","2010-07-21T10:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.33,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7265,"POWERLINKV5_20151103074515","2010-07-22T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-25.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7268,"POWERLINKV5_20151103074515","2010-07-22T06:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7271,"POWERLINKV5_20151103074515","2010-07-22T12:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.99,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7273,"POWERLINKV5_20151103074515","2010-07-22T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7274,"POWERLINKV5_20151103074515","2010-07-23T01:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.71,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7278,"POWERLINKV5_20151103074515","2010-07-23T09:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.9,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7281,"POWERLINKV5_20151103074515","2010-07-23T09:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.88,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7284,"POWERLINKV5_20151103074515","2010-07-23T09:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.79,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7288,"POWERLINKV5_20151103074515","2010-07-23T21:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7291,"POWERLINKV5_20151103074515","2010-07-23T22:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-33.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7294,"POWERLINKV5_20151103074515","2010-07-23T22:30:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7296,"POWERLINKV5_20151103074515","2010-07-23T22:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-16.059999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7297,"POWERLINKV5_20151103074515","2010-07-23T22:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.03,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7301,"POWERLINKV5_20151103074515","2010-07-23T23:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.05,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7304,"POWERLINKV5_20151103074515","2010-07-24T00:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.31,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7307,"POWERLINKV5_20151103074515","2010-07-24T01:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7311,"POWERLINKV5_20151103074515","2010-07-24T09:05:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-15.91,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7314,"POWERLINKV5_20151103074515","2010-07-24T09:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-16.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7315,"POWERLINKV5_20151103074515","2010-07-24T09:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-17.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7319,"POWERLINKV5_20151103074515","2010-07-24T09:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7320,"POWERLINKV5_20151103074515","2010-07-24T09:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7324,"POWERLINKV5_20151103074515","2010-07-24T10:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.42,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7327,"POWERLINKV5_20151103074515","2010-07-24T18:10:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-19.07,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7330,"POWERLINKV5_20151103074515","2010-07-24T18:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-12.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7334,"POWERLINKV5_20151103074515","2010-07-25T01:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7337,"POWERLINKV5_20151103074515","2010-07-25T04:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.89,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7338,"POWERLINKV5_20151103074515","2010-07-25T19:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.17,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7340,"POWERLINKV5_20151103074515","2010-07-25T19:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7343,"POWERLINKV5_20151103074515","2010-07-25T20:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7347,"POWERLINKV5_20151103074515","2010-07-26T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7350,"POWERLINKV5_20151103074515","2010-07-26T10:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7353,"POWERLINKV5_20151103074515","2010-07-26T10:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.100000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7357,"POWERLINKV5_20151103074515","2010-07-26T11:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7360,"POWERLINKV5_20151103074515","2010-07-26T17:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.37,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7361,"POWERLINKV5_20151103074515","2010-07-26T19:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7363,"POWERLINKV5_20151103074515","2010-07-26T19:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-26.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7366,"POWERLINKV5_20151103074515","2010-07-26T19:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-26.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7370,"POWERLINKV5_20151103074515","2010-07-26T19:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.809999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7373,"POWERLINKV5_20151103074515","2010-07-26T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7377,"POWERLINKV5_20151103074515","2010-07-26T20:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7380,"POWERLINKV5_20151103074515","2010-07-26T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.53,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7383,"POWERLINKV5_20151103074515","2010-07-27T03:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.44,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7384,"POWERLINKV5_20151103074515","2010-07-27T06:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.42,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7386,"POWERLINKV5_20151103074515","2010-07-27T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.03,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7389,"POWERLINKV5_20151103074515","2010-07-28T01:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-21.98,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7393,"POWERLINKV5_20151103074515","2010-07-28T01:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-26.74,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7396,"POWERLINKV5_20151103074515","2010-07-28T02:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-50.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7400,"POWERLINKV5_20151103074515","2010-07-28T02:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.07,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7403,"POWERLINKV5_20151103074515","2010-07-28T03:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-1113.08,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7406,"POWERLINKV5_20151103074515","2010-07-28T04:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.42,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7407,"POWERLINKV5_20151103074515","2010-07-28T04:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.489999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7409,"POWERLINKV5_20151103074515","2010-07-28T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7413,"POWERLINKV5_20151103074515","2010-07-29T00:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7416,"POWERLINKV5_20151103074515","2010-07-29T01:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7419,"POWERLINKV5_20151103074515","2010-07-29T02:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.74,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7423,"POWERLINKV5_20151103074515","2010-07-29T03:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.24,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7426,"POWERLINKV5_20151103074515","2010-07-29T03:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.64,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7429,"POWERLINKV5_20151103074515","2010-07-29T05:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.69,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7430,"POWERLINKV5_20151103074515","2010-07-29T22:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.02,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7432,"POWERLINKV5_20151103074515","2010-07-30T02:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.2,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7436,"POWERLINKV5_20151103074515","2010-07-30T03:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.59,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7439,"POWERLINKV5_20151103074515","2010-07-30T04:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-1113.26,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7442,"POWERLINKV5_20151103074515","2010-07-31T01:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7446,"POWERLINKV5_20151103074515","2010-08-01T07:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.53,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7449,"POWERLINKV5_20151103074515","2010-08-03T12:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.36,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7451,"POWERLINKV5_20151103074515","2010-08-04T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7452,"POWERLINKV5_20151103074515","2010-08-05T19:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.079999999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7455,"POWERLINKV5_20151103074515","2010-08-05T20:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7459,"POWERLINKV5_20151103074515","2010-08-05T20:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-26.25,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7462,"POWERLINKV5_20151103074515","2010-08-05T20:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7465,"POWERLINKV5_20151103074515","2010-08-05T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-26.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7469,"POWERLINKV5_20151103074515","2010-08-06T01:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.65,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7472,"POWERLINKV5_20151103074515","2010-08-06T01:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.85,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7474,"POWERLINKV5_20151103074515","2010-08-06T01:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.02,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7475,"POWERLINKV5_20151103074515","2010-08-06T01:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.51,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7478,"POWERLINKV5_20151103074515","2010-08-06T06:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7482,"POWERLINKV5_20151103074515","2010-08-06T08:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7485,"POWERLINKV5_20151103074515","2010-08-06T09:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.03,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7488,"POWERLINKV5_20151103074515","2010-08-06T09:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7492,"POWERLINKV5_20151103074515","2010-08-06T10:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7495,"POWERLINKV5_20151103074515","2010-08-06T11:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.43,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7497,"POWERLINKV5_20151103074515","2010-08-06T17:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.89,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7498,"POWERLINKV5_20151103074515","2010-08-06T17:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.72,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7501,"POWERLINKV5_20151103074515","2010-08-06T17:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-90.94,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7505,"POWERLINKV5_20151103074515","2010-08-06T18:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-89.5,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7508,"POWERLINKV5_20151103074515","2010-08-06T18:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-34.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7511,"POWERLINKV5_20151103074515","2010-08-06T18:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-29.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7515,"POWERLINKV5_20151103074515","2010-08-06T18:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-35.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7518,"POWERLINKV5_20151103074515","2010-08-06T19:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.77,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7520,"POWERLINKV5_20151103074515","2010-08-06T19:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-28.67,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7521,"POWERLINKV5_20151103074515","2010-08-06T19:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7524,"POWERLINKV5_20151103074515","2010-08-06T20:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7528,"POWERLINKV5_20151103074515","2010-08-06T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-69.14,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7531,"POWERLINKV5_20151103074515","2010-08-06T22:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-30.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7535,"POWERLINKV5_20151103074515","2010-08-06T22:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-22.83,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7538,"POWERLINKV5_20151103074515","2010-08-06T23:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7539,"POWERLINKV5_20151103074515","2010-08-06T23:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-32.82,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7541,"POWERLINKV5_20151103074515","2010-08-06T23:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-22.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7544,"POWERLINKV5_20151103074515","2010-08-06T23:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7547,"POWERLINKV5_20151103074515","2010-08-07T00:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7551,"POWERLINKV5_20151103074515","2010-08-07T08:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-29.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7554,"POWERLINKV5_20151103074515","2010-08-07T08:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-28.18,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7558,"POWERLINKV5_20151103074515","2010-08-07T08:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-30.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7561,"POWERLINKV5_20151103074515","2010-08-07T08:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-29.91,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7562,"POWERLINKV5_20151103074515","2010-08-07T08:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-64.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7564,"POWERLINKV5_20151103074515","2010-08-07T09:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-44.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7567,"POWERLINKV5_20151103074515","2010-08-07T09:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-67.19,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7571,"POWERLINKV5_20151103074515","2010-08-07T09:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-42.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7574,"POWERLINKV5_20151103074515","2010-08-07T09:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-27.44,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7577,"POWERLINKV5_20151103074515","2010-08-07T10:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-34.78,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7581,"POWERLINKV5_20151103074515","2010-08-07T10:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7584,"POWERLINKV5_20151103074515","2010-08-07T10:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.76,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7585,"POWERLINKV5_20151103074515","2010-08-07T11:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7587,"POWERLINKV5_20151103074515","2010-08-07T16:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.55,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7590,"POWERLINKV5_20151103074515","2010-08-07T17:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-25.67,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7594,"POWERLINKV5_20151103074515","2010-08-07T17:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-26.37,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7597,"POWERLINKV5_20151103074515","2010-08-07T19:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7600,"POWERLINKV5_20151103074515","2010-08-07T19:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.89,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7604,"POWERLINKV5_20151103074515","2010-08-07T20:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7607,"POWERLINKV5_20151103074515","2010-08-07T20:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7608,"POWERLINKV5_20151103074515","2010-08-07T20:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7610,"POWERLINKV5_20151103074515","2010-08-07T20:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7613,"POWERLINKV5_20151103074515","2010-08-07T21:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-22.5,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7617,"POWERLINKV5_20151103074515","2010-08-07T21:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7620,"POWERLINKV5_20151103074515","2010-08-07T22:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-26.19,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7623,"POWERLINKV5_20151103074515","2010-08-07T22:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.95,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7627,"POWERLINKV5_20151103074515","2010-08-08T04:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.92,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7630,"POWERLINKV5_20151103074515","2010-08-08T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.22,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7631,"POWERLINKV5_20151103074515","2010-08-08T08:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7633,"POWERLINKV5_20151103074515","2010-08-08T09:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.3,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7636,"POWERLINKV5_20151103074515","2010-08-08T09:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-28.96,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7640,"POWERLINKV5_20151103074515","2010-08-08T12:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.72,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7643,"POWERLINKV5_20151103074515","2010-08-08T15:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.42,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7646,"POWERLINKV5_20151103074515","2010-08-08T16:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.55,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7650,"POWERLINKV5_20151103074515","2010-08-08T19:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-31.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7652,"POWERLINKV5_20151103074515","2010-08-08T19:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-29.86,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7653,"POWERLINKV5_20151103074515","2010-08-08T19:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-29.87,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7656,"POWERLINKV5_20151103074515","2010-08-08T19:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-31.91,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7659,"POWERLINKV5_20151103074515","2010-08-08T20:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-45,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7663,"POWERLINKV5_20151103074515","2010-08-08T20:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-46.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7666,"POWERLINKV5_20151103074515","2010-08-08T20:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-56.12,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7670,"POWERLINKV5_20151103074515","2010-08-08T21:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-33.71,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7673,"POWERLINKV5_20151103074515","2010-08-08T21:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-36.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7675,"POWERLINKV5_20151103074515","2010-08-08T21:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-28.97,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7676,"POWERLINKV5_20151103074515","2010-08-08T21:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7679,"POWERLINKV5_20151103074515","2010-08-09T00:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7682,"POWERLINKV5_20151103074515","2010-08-09T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.8,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7686,"POWERLINKV5_20151103074515","2010-08-09T01:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7689,"POWERLINKV5_20151103074515","2010-08-09T03:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.54,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7693,"POWERLINKV5_20151103074515","2010-08-09T04:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-51.38,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7696,"POWERLINKV5_20151103074515","2010-08-09T04:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.57,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7698,"POWERLINKV5_20151103074515","2010-08-09T04:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.49,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7699,"POWERLINKV5_20151103074515","2010-08-09T06:10:00","Q>MUTE757_758_B","Q-MUTE757_758","2007-09-18",1,-10.66,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 758","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V.","PLANNED",0]
[7702,"POWERLINKV5_20151103074515","2010-08-09T06:45:00","Q>MUTE757_758_B","Q-MUTE757_758","2007-09-18",1,-18.399999999999999,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 758","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V.","PLANNED",0]
[7705,"POWERLINKV5_20151103074515","2010-08-09T06:50:00","Q>MUTE757_758_B","Q-MUTE757_758","2007-09-18",1,-14.83,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 758","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V.","PLANNED",0]
[7709,"POWERLINKV5_20151103074515","2010-08-09T07:50:00","QNTE_ROC","Q-NIL","2006-12-27",1,-28.65,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7712,"POWERLINKV5_20151103074515","2010-08-09T08:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.54,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7716,"POWERLINKV5_20151103074515","2010-08-09T08:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-21.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7719,"POWERLINKV5_20151103074515","2010-08-09T08:15:00","QNTE_000","I-QNTE_000","2008-08-05",1,-33.01,"Qld to NSW on Terranora Interconnector upper transfer limit of 0 MW","OUTAGE","OTHER","Terranora Interconnector","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V and Market Notices 32578 & 32579.","PLANNED",0]
[7721,"POWERLINKV5_20151103074515","2010-08-09T08:20:00","QNTE_000","I-QNTE_000","2008-08-05",1,-30.22,"Qld to NSW on Terranora Interconnector upper transfer limit of 0 MW","OUTAGE","OTHER","Terranora Interconnector","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V and Market Notices 32578 & 32579.","PLANNED",0]
[7722,"POWERLINKV5_20151103074515","2010-08-09T08:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.55,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7725,"POWERLINKV5_20151103074515","2010-08-09T08:30:00","QNTE_000","I-QNTE_000","2008-08-05",1,-20.04,"Qld to NSW on Terranora Interconnector upper transfer limit of 0 MW","OUTAGE","OTHER","Terranora Interconnector","REGULATED","3","Country Energy outage of Feeder 758, refer to NOS J32644V and Market Notices 32578 & 32579.","PLANNED",0]
[7729,"POWERLINKV5_20151103074515","2010-08-09T08:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7732,"POWERLINKV5_20151103074515","2010-08-09T09:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7735,"POWERLINKV5_20151103074515","2010-08-09T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-25.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7739,"POWERLINKV5_20151103074515","2010-08-09T20:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.55,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7742,"POWERLINKV5_20151103074515","2010-08-09T20:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.44,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7743,"POWERLINKV5_20151103074515","2010-08-09T20:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7744,"POWERLINKV5_20151103074515","2010-08-09T21:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7745,"POWERLINKV5_20151103074515","2010-08-09T21:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.23,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7746,"POWERLINKV5_20151103074515","2010-08-09T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-40.06,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7747,"POWERLINKV5_20151103074515","2010-08-09T22:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-25.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7748,"POWERLINKV5_20151103074515","2010-08-09T22:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.24,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7749,"POWERLINKV5_20151103074515","2010-08-09T22:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.72,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7750,"POWERLINKV5_20151103074515","2010-08-09T23:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7751,"POWERLINKV5_20151103074515","2010-08-10","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7752,"POWERLINKV5_20151103074515","2010-08-10T00:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.78,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7753,"POWERLINKV5_20151103074515","2010-08-10T00:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.5,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7754,"POWERLINKV5_20151103074515","2010-08-10T00:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.5,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7755,"POWERLINKV5_20151103074515","2010-08-10T00:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.61,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7756,"POWERLINKV5_20151103074515","2010-08-10T00:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.71,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7757,"POWERLINKV5_20151103074515","2010-08-10T00:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.65,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7758,"POWERLINKV5_20151103074515","2010-08-10T01:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.71,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7759,"POWERLINKV5_20151103074515","2010-08-10T01:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.7,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7760,"POWERLINKV5_20151103074515","2010-08-10T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-32.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7761,"POWERLINKV5_20151103074515","2010-08-10T01:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.86,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7762,"POWERLINKV5_20151103074515","2010-08-10T02:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.64,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7763,"POWERLINKV5_20151103074515","2010-08-10T02:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.43,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7764,"POWERLINKV5_20151103074515","2010-08-10T03:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7765,"POWERLINKV5_20151103074515","2010-08-10T03:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.559999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7766,"POWERLINKV5_20151103074515","2010-08-10T06:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.9,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7767,"POWERLINKV5_20151103074515","2010-08-10T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7768,"POWERLINKV5_20151103074515","2010-08-10T06:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7769,"POWERLINKV5_20151103074515","2010-08-10T06:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7770,"POWERLINKV5_20151103074515","2010-08-10T22:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.399999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7771,"POWERLINKV5_20151103074515","2010-08-10T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.65,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7772,"POWERLINKV5_20151103074515","2010-08-10T22:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7773,"POWERLINKV5_20151103074515","2010-08-10T23:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.53,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7774,"POWERLINKV5_20151103074515","2010-08-10T23:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.6,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7775,"POWERLINKV5_20151103074515","2010-08-10T23:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.77,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7776,"POWERLINKV5_20151103074515","2010-08-11T00:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.5,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7777,"POWERLINKV5_20151103074515","2010-08-11T00:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.02,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7778,"POWERLINKV5_20151103074515","2010-08-11T00:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.29,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7779,"POWERLINKV5_20151103074515","2010-08-11T00:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.31,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7780,"POWERLINKV5_20151103074515","2010-08-11T01:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-19.27,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7781,"POWERLINKV5_20151103074515","2010-08-11T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-29.86,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7782,"POWERLINKV5_20151103074515","2010-08-11T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.62,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7783,"POWERLINKV5_20151103074515","2010-08-11T01:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.54,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7784,"POWERLINKV5_20151103074515","2010-08-11T01:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.89,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7785,"POWERLINKV5_20151103074515","2010-08-11T01:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-16.91,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7786,"POWERLINKV5_20151103074515","2010-08-11T02:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-19.78,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7787,"POWERLINKV5_20151103074515","2010-08-11T02:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.83,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7788,"POWERLINKV5_20151103074515","2010-08-11T02:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.76,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7789,"POWERLINKV5_20151103074515","2010-08-11T03:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.56,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7790,"POWERLINKV5_20151103074515","2010-08-11T03:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.34,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7791,"POWERLINKV5_20151103074515","2010-08-11T03:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.35,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7792,"POWERLINKV5_20151103074515","2010-08-11T04:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.37,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7793,"POWERLINKV5_20151103074515","2010-08-11T04:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.739999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7794,"POWERLINKV5_20151103074515","2010-08-11T04:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.49,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7795,"POWERLINKV5_20151103074515","2010-08-11T05:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.399999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7796,"POWERLINKV5_20151103074515","2010-08-11T05:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.52,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7797,"POWERLINKV5_20151103074515","2010-08-11T06:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-21.41,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7798,"POWERLINKV5_20151103074515","2010-08-11T06:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.039999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7799,"POWERLINKV5_20151103074515","2010-08-11T06:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.65,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7800,"POWERLINKV5_20151103074515","2010-08-11T06:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.72,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7801,"POWERLINKV5_20151103074515","2010-08-11T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-27.05,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7802,"POWERLINKV5_20151103074515","2010-08-11T06:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.6,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7803,"POWERLINKV5_20151103074515","2010-08-11T06:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.45,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7804,"POWERLINKV5_20151103074515","2010-08-11T07:00:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.39,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7805,"POWERLINKV5_20151103074515","2010-08-11T07:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.93,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7806,"POWERLINKV5_20151103074515","2010-08-11T08:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7807,"POWERLINKV5_20151103074515","2010-08-11T10:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.39,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7808,"POWERLINKV5_20151103074515","2010-08-11T17:30:00","Q>CLBCN_7349","Q-CLBCN_7349","2009-09-15",1,-1024.6400000000001,"Out= 7349 T13 Chinchilla to T194 Columboola 132kV line, Ergon limit on remaining T13 Chinchilla to T194 Columboola 132kV line.","OUTAGE","OTHER","Feeder 7349","REGULATED","3","Ergon outage of Feeder 7349, refer to NOS 10SW8715.","PLANNED",0]
[7809,"POWERLINKV5_20151103074515","2010-08-11T17:35:00","Q>CLBCN_7349","Q-CLBCN_7349","2009-09-15",1,-1024.3399999999999,"Out= 7349 T13 Chinchilla to T194 Columboola 132kV line, Ergon limit on remaining T13 Chinchilla to T194 Columboola 132kV line.","OUTAGE","OTHER","Feeder 7349","REGULATED","3","Ergon outage of Feeder 7349, refer to NOS 10SW8715.","PLANNED",0]
[7810,"POWERLINKV5_20151103074515","2010-08-11T17:40:00","Q>CLBCN_7349","Q-CLBCN_7349","2009-09-15",1,-1028.4000000000001,"Out= 7349 T13 Chinchilla to T194 Columboola 132kV line, Ergon limit on remaining T13 Chinchilla to T194 Columboola 132kV line.","OUTAGE","OTHER","Feeder 7349","REGULATED","3","Ergon outage of Feeder 7349, refer to NOS 10SW8715.","PLANNED",0]
[7811,"POWERLINKV5_20151103074515","2010-08-11T17:45:00","Q>CLBCN_7349","Q-CLBCN_7349","2009-09-15",1,-1039.3599999999999,"Out= 7349 T13 Chinchilla to T194 Columboola 132kV line, Ergon limit on remaining T13 Chinchilla to T194 Columboola 132kV line.","OUTAGE","OTHER","Feeder 7349","REGULATED","3","Ergon outage of Feeder 7349, refer to NOS 10SW8715.","PLANNED",0]
[7812,"POWERLINKV5_20151103074515","2010-08-12T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.21,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7813,"POWERLINKV5_20151103074515","2010-08-12T01:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.76,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7814,"POWERLINKV5_20151103074515","2010-08-12T04:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-48.1,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7815,"POWERLINKV5_20151103074515","2010-08-12T04:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-14.17,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7816,"POWERLINKV5_20151103074515","2010-08-12T04:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.44,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7817,"POWERLINKV5_20151103074515","2010-08-12T04:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.44,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7818,"POWERLINKV5_20151103074515","2010-08-12T05:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.079999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7819,"POWERLINKV5_20151103074515","2010-08-12T15:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.99,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7820,"POWERLINKV5_20151103074515","2010-08-12T17:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-36.369999999999997,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7821,"POWERLINKV5_20151103074515","2010-08-12T17:50:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-28.19,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7822,"POWERLINKV5_20151103074515","2010-08-12T17:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-48.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7823,"POWERLINKV5_20151103074515","2010-08-12T17:55:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-37.85,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7824,"POWERLINKV5_20151103074515","2010-08-12T18:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-53.55,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7825,"POWERLINKV5_20151103074515","2010-08-12T18:00:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-42.55,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7826,"POWERLINKV5_20151103074515","2010-08-12T18:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7827,"POWERLINKV5_20151103074515","2010-08-12T18:10:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-10.69,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7828,"POWERLINKV5_20151103074515","2010-08-12T18:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.99,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7829,"POWERLINKV5_20151103074515","2010-08-12T18:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-55.69,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7830,"POWERLINKV5_20151103074515","2010-08-12T18:20:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-44.35,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7831,"POWERLINKV5_20151103074515","2010-08-12T18:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.64,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7832,"POWERLINKV5_20151103074515","2010-08-12T18:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-54.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7833,"POWERLINKV5_20151103074515","2010-08-12T18:30:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-43.37,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7834,"POWERLINKV5_20151103074515","2010-08-12T18:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.65,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7835,"POWERLINKV5_20151103074515","2010-08-12T18:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-22.08,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7836,"POWERLINKV5_20151103074515","2010-08-12T18:40:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-13.54,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7837,"POWERLINKV5_20151103074515","2010-08-12T18:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.48,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7838,"POWERLINKV5_20151103074515","2010-08-12T18:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7839,"POWERLINKV5_20151103074515","2010-08-12T18:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.04,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7840,"POWERLINKV5_20151103074515","2010-08-12T18:55:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-12.17,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7841,"POWERLINKV5_20151103074515","2010-08-12T19:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.79,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7842,"POWERLINKV5_20151103074515","2010-08-12T19:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-53.74,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7843,"POWERLINKV5_20151103074515","2010-08-12T19:05:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-43.03,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7844,"POWERLINKV5_20151103074515","2010-08-12T19:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-50.76,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7845,"POWERLINKV5_20151103074515","2010-08-12T19:10:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-40.049999999999997,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7846,"POWERLINKV5_20151103074515","2010-08-12T19:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.48,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7847,"POWERLINKV5_20151103074515","2010-08-12T19:15:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-10.1,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7848,"POWERLINKV5_20151103074515","2010-08-12T19:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.59,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7849,"POWERLINKV5_20151103074515","2010-08-12T19:20:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-14.27,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7850,"POWERLINKV5_20151103074515","2010-08-12T19:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7851,"POWERLINKV5_20151103074515","2010-08-12T19:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.190000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7852,"POWERLINKV5_20151103074515","2010-08-12T19:35:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-13.87,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7853,"POWERLINKV5_20151103074515","2010-08-12T19:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.5,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7854,"POWERLINKV5_20151103074515","2010-08-12T19:40:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-10.1,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7855,"POWERLINKV5_20151103074515","2010-08-12T19:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.399999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7856,"POWERLINKV5_20151103074515","2010-08-12T20:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7857,"POWERLINKV5_20151103074515","2010-08-12T20:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-18.48,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7858,"POWERLINKV5_20151103074515","2010-08-12T20:10:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-11.6,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7859,"POWERLINKV5_20151103074515","2010-08-12T20:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7860,"POWERLINKV5_20151103074515","2010-08-12T20:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.13,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7861,"POWERLINKV5_20151103074515","2010-08-12T20:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.03,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7862,"POWERLINKV5_20151103074515","2010-08-12T21:05:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-15.2,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7863,"POWERLINKV5_20151103074515","2010-08-12T21:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.75,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7864,"POWERLINKV5_20151103074515","2010-08-13T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.149999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7865,"POWERLINKV5_20151103074515","2010-08-13T01:10:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-26.14,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7866,"POWERLINKV5_20151103074515","2010-08-13T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-25.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7867,"POWERLINKV5_20151103074515","2010-08-13T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.39,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7868,"POWERLINKV5_20151103074515","2010-08-13T02:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-21.67,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7869,"POWERLINKV5_20151103074515","2010-08-13T02:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.34,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7870,"POWERLINKV5_20151103074515","2010-08-13T02:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.16,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7871,"POWERLINKV5_20151103074515","2010-08-13T03:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-13.32,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7872,"POWERLINKV5_20151103074515","2010-08-13T03:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7873,"POWERLINKV5_20151103074515","2010-08-13T03:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.07,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7874,"POWERLINKV5_20151103074515","2010-08-13T06:05:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-10.7,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7875,"POWERLINKV5_20151103074515","2010-08-13T06:40:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-11.76,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7876,"POWERLINKV5_20151103074515","2010-08-13T06:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.58,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7877,"POWERLINKV5_20151103074515","2010-08-13T06:50:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-13.48,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7878,"POWERLINKV5_20151103074515","2010-08-13T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.6,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7879,"POWERLINKV5_20151103074515","2010-08-13T06:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.72,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7880,"POWERLINKV5_20151103074515","2010-08-13T06:55:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-13.05,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7881,"POWERLINKV5_20151103074515","2010-08-13T07:00:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-10.83,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7882,"POWERLINKV5_20151103074515","2010-08-13T08:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-16.72,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7883,"POWERLINKV5_20151103074515","2010-08-13T08:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.93,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7884,"POWERLINKV5_20151103074515","2010-08-13T08:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-11.99,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7885,"POWERLINKV5_20151103074515","2010-08-13T08:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-11.7,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7886,"POWERLINKV5_20151103074515","2010-08-13T09:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-11.97,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7887,"POWERLINKV5_20151103074515","2010-08-13T09:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-10.1,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7888,"POWERLINKV5_20151103074515","2010-08-13T10:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-10.1,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7889,"POWERLINKV5_20151103074515","2010-08-13T10:25:00","Q>NIL_CLBCN_CLBCN","Q-NIL","2010-03-24",1,-1020.24,"Out= Nil, Ergon Runback Scheme for managing 7349 and 7350 Chinchilla to Columboola 132kV lines.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7890,"POWERLINKV5_20151103074515","2010-08-13T10:50:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-10.1,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7891,"POWERLINKV5_20151103074515","2010-08-13T11:00:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-10.01,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7892,"POWERLINKV5_20151103074515","2010-08-13T11:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-11.26,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7893,"POWERLINKV5_20151103074515","2010-08-13T11:45:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2010-08-13",1,-18.5,"N-Q-MNSP1.ENERGY * -1 <= 70 (Wt = 20)","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora, refer to Market Notice 32623.","PLANNED",0]
[7894,"POWERLINKV5_20151103074515","2010-08-13T11:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.920000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7895,"POWERLINKV5_20151103074515","2010-08-13T12:00:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-18.22,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of feeder 757 and 7Bus1 at T174 Terranora.","PLANNED",0]
[7896,"POWERLINKV5_20151103074515","2010-08-13T12:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.82,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7897,"POWERLINKV5_20151103074515","2010-08-14T01:20:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-15.45,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7898,"POWERLINKV5_20151103074515","2010-08-14T01:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.3,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7899,"POWERLINKV5_20151103074515","2010-08-14T01:50:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-15.25,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7900,"POWERLINKV5_20151103074515","2010-08-14T01:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.96,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7901,"POWERLINKV5_20151103074515","2010-08-14T02:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.56,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7902,"POWERLINKV5_20151103074515","2010-08-14T05:45:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.48,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7903,"POWERLINKV5_20151103074515","2010-08-14T06:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.01,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7904,"POWERLINKV5_20151103074515","2010-08-14T10:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.899999999999999,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7905,"POWERLINKV5_20151103074515","2010-08-14T11:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.32,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7906,"POWERLINKV5_20151103074515","2010-08-14T11:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.329999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7907,"POWERLINKV5_20151103074515","2010-08-14T11:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7908,"POWERLINKV5_20151103074515","2010-08-14T11:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7909,"POWERLINKV5_20151103074515","2010-08-14T11:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.190000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7910,"POWERLINKV5_20151103074515","2010-08-14T11:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.22,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7911,"POWERLINKV5_20151103074515","2010-08-14T12:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7912,"POWERLINKV5_20151103074515","2010-08-14T12:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.18,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7913,"POWERLINKV5_20151103074515","2010-08-14T12:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.05,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7914,"POWERLINKV5_20151103074515","2010-08-17T01:10:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-12.11,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7915,"POWERLINKV5_20151103074515","2010-08-17T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.350000000000001,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7916,"POWERLINKV5_20151103074515","2010-08-17T05:05:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.31,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7917,"POWERLINKV5_20151103074515","2010-08-17T18:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7918,"POWERLINKV5_20151103074515","2010-08-17T18:20:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-13.94,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7919,"POWERLINKV5_20151103074515","2010-08-17T18:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-20.32,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7920,"POWERLINKV5_20151103074515","2010-08-17T18:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.71,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7921,"POWERLINKV5_20151103074515","2010-08-17T18:25:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-17.649999999999999,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7922,"POWERLINKV5_20151103074515","2010-08-17T18:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.77,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7923,"POWERLINKV5_20151103074515","2010-08-17T18:30:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-17.7,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7924,"POWERLINKV5_20151103074515","2010-08-17T18:35:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-17.850000000000001,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7925,"POWERLINKV5_20151103074515","2010-08-17T18:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-25.17,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7926,"POWERLINKV5_20151103074515","2010-08-17T18:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-20.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7927,"POWERLINKV5_20151103074515","2010-08-17T18:40:00","Q>NIL_757+758_B","Q-NIL","2008-02-21",1,-13.5,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter  ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7928,"POWERLINKV5_20151103074515","2010-08-17T18:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.81,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7929,"POWERLINKV5_20151103074515","2010-08-17T18:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.84,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7930,"POWERLINKV5_20151103074515","2010-08-18T06:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.43,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7931,"POWERLINKV5_20151103074515","2010-08-18T07:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-10.01,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7932,"POWERLINKV5_20151103074515","2010-08-20T05:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7933,"POWERLINKV5_20151103074515","2010-08-25T19:40:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,460.56,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0678.","PLANNED",1]
[7934,"POWERLINKV5_20151103074515","2010-08-25T21:15:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,65.33,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0678.","PLANNED",1]
[7935,"POWERLINKV5_20151103074515","2010-08-25T21:20:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,65.37,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0678.","PLANNED",1]
[7936,"POWERLINKV5_20151103074515","2010-08-25T21:25:00","Q_RS_260","Q-SMRS_A","2010-03-01",1,65.540000000000006,"Qld, Ross cutset upper limit of 260MW (discretionary)","OUTAGE","OTHER","Feeder 879","REGULATED","INCLUDED","Planned outage of Feeder 879, refer to AFW Q10S/0678.","PLANNED",1]
[7937,"POWERLINKV5_20151103074515","2010-09-03T00:30:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-15.38,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7938,"POWERLINKV5_20151103074515","2010-09-03T00:30:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.74,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7939,"POWERLINKV5_20151103074515","2010-09-03T00:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.41,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7940,"POWERLINKV5_20151103074515","2010-09-03T00:45:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.14,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7941,"POWERLINKV5_20151103074515","2010-09-03T00:50:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.19,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7942,"POWERLINKV5_20151103074515","2010-09-03T00:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.47,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7943,"POWERLINKV5_20151103074515","2010-09-03T00:55:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-18.87,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7944,"POWERLINKV5_20151103074515","2010-09-03T00:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.57,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7945,"POWERLINKV5_20151103074515","2010-09-03T01:00:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-23.6,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7946,"POWERLINKV5_20151103074515","2010-09-03T01:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.28,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7947,"POWERLINKV5_20151103074515","2010-09-03T01:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.05,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7948,"POWERLINKV5_20151103074515","2010-09-03T01:05:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-16.87,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7949,"POWERLINKV5_20151103074515","2010-09-03T01:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.100000000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7950,"POWERLINKV5_20151103074515","2010-09-03T01:10:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-16.920000000000002,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7951,"POWERLINKV5_20151103074515","2010-09-03T01:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-17.98,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7952,"POWERLINKV5_20151103074515","2010-09-03T01:15:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-18.7,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7953,"POWERLINKV5_20151103074515","2010-09-03T01:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.09,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7954,"POWERLINKV5_20151103074515","2010-09-03T01:20:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-14.75,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7955,"POWERLINKV5_20151103074515","2010-09-03T01:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-12.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7956,"POWERLINKV5_20151103074515","2010-09-03T01:25:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.99,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7957,"POWERLINKV5_20151103074515","2010-09-03T01:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.44,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7958,"POWERLINKV5_20151103074515","2010-09-03T01:30:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.2,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7959,"POWERLINKV5_20151103074515","2010-09-03T01:35:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-13.02,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7960,"POWERLINKV5_20151103074515","2010-09-03T01:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.23,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7961,"POWERLINKV5_20151103074515","2010-09-03T01:55:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-18.88,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7962,"POWERLINKV5_20151103074515","2010-09-03T01:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.54,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7963,"POWERLINKV5_20151103074515","2010-09-03T02:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7964,"POWERLINKV5_20151103074515","2010-09-03T02:05:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.2,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7965,"POWERLINKV5_20151103074515","2010-09-03T02:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7966,"POWERLINKV5_20151103074515","2010-09-03T02:10:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.2,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7967,"POWERLINKV5_20151103074515","2010-09-03T02:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.36,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7968,"POWERLINKV5_20151103074515","2010-09-03T02:15:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.14,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7969,"POWERLINKV5_20151103074515","2010-09-03T02:35:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-18.87,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7970,"POWERLINKV5_20151103074515","2010-09-03T02:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.54,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7971,"POWERLINKV5_20151103074515","2010-09-03T02:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7972,"POWERLINKV5_20151103074515","2010-09-03T02:50:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-12.19,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7973,"POWERLINKV5_20151103074515","2010-09-03T03:40:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-13.21,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7974,"POWERLINKV5_20151103074515","2010-09-03T03:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.58,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7975,"POWERLINKV5_20151103074515","2010-09-03T23:00:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-10.73,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7976,"POWERLINKV5_20151103074515","2010-09-04T00:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1020.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7977,"POWERLINKV5_20151103074515","2010-09-04T00:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7978,"POWERLINKV5_20151103074515","2010-09-04T00:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7979,"POWERLINKV5_20151103074515","2010-09-04T00:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.4,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7980,"POWERLINKV5_20151103074515","2010-09-04T01:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7981,"POWERLINKV5_20151103074515","2010-09-04T01:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.55,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7982,"POWERLINKV5_20151103074515","2010-09-04T01:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1018.55,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7983,"POWERLINKV5_20151103074515","2010-09-04T01:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7984,"POWERLINKV5_20151103074515","2010-09-04T01:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7985,"POWERLINKV5_20151103074515","2010-09-04T01:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7986,"POWERLINKV5_20151103074515","2010-09-04T01:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7987,"POWERLINKV5_20151103074515","2010-09-04T01:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017.36,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7988,"POWERLINKV5_20151103074515","2010-09-04T01:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7989,"POWERLINKV5_20151103074515","2010-09-04T01:45:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-23.62,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7990,"POWERLINKV5_20151103074515","2010-09-04T01:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-999.99,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7991,"POWERLINKV5_20151103074515","2010-09-04T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7992,"POWERLINKV5_20151103074515","2010-09-04T01:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7993,"POWERLINKV5_20151103074515","2010-09-04T01:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7994,"POWERLINKV5_20151103074515","2010-09-04T02:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7995,"POWERLINKV5_20151103074515","2010-09-04T02:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7996,"POWERLINKV5_20151103074515","2010-09-04T02:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.31,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7997,"POWERLINKV5_20151103074515","2010-09-04T02:10:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-13.97,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7998,"POWERLINKV5_20151103074515","2010-09-04T02:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1004.77,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7999,"POWERLINKV5_20151103074515","2010-09-04T02:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8000,"POWERLINKV5_20151103074515","2010-09-04T02:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8001,"POWERLINKV5_20151103074515","2010-09-04T02:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1017,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8002,"POWERLINKV5_20151103074515","2010-09-04T02:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.57,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8003,"POWERLINKV5_20151103074515","2010-09-04T02:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8004,"POWERLINKV5_20151103074515","2010-09-04T02:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8005,"POWERLINKV5_20151103074515","2010-09-04T02:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8006,"POWERLINKV5_20151103074515","2010-09-04T02:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8007,"POWERLINKV5_20151103074515","2010-09-04T02:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8008,"POWERLINKV5_20151103074515","2010-09-04T03:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.9,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8009,"POWERLINKV5_20151103074515","2010-09-04T03:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1016.04,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8010,"POWERLINKV5_20151103074515","2010-09-04T03:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8011,"POWERLINKV5_20151103074515","2010-09-04T03:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8012,"POWERLINKV5_20151103074515","2010-09-04T03:20:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8013,"POWERLINKV5_20151103074515","2010-09-04T03:25:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.65,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8014,"POWERLINKV5_20151103074515","2010-09-04T03:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8015,"POWERLINKV5_20151103074515","2010-09-04T03:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8016,"POWERLINKV5_20151103074515","2010-09-04T03:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8017,"POWERLINKV5_20151103074515","2010-09-04T03:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.93,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8018,"POWERLINKV5_20151103074515","2010-09-04T03:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1014.81,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8019,"POWERLINKV5_20151103074515","2010-09-04T03:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1012.53,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8020,"POWERLINKV5_20151103074515","2010-09-04T04:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8021,"POWERLINKV5_20151103074515","2010-09-07T18:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-29.88,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8022,"POWERLINKV5_20151103074515","2010-09-07T18:30:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-21.59,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8023,"POWERLINKV5_20151103074515","2010-09-07T18:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-15.35,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8024,"POWERLINKV5_20151103074515","2010-09-07T18:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.63,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8025,"POWERLINKV5_20151103074515","2010-09-07T18:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-27.38,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8026,"POWERLINKV5_20151103074515","2010-09-07T18:45:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-19.059999999999999,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8027,"POWERLINKV5_20151103074515","2010-09-07T18:55:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-10.1,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8028,"POWERLINKV5_20151103074515","2010-09-07T18:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.27,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8029,"POWERLINKV5_20151103074515","2010-09-07T19:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.16,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8030,"POWERLINKV5_20151103074515","2010-09-10T01:15:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-13.19,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8031,"POWERLINKV5_20151103074515","2010-09-10T01:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.96,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8032,"POWERLINKV5_20151103074515","2010-09-11T04:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.26,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8033,"POWERLINKV5_20151103074515","2010-09-12T01:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.2,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8034,"POWERLINKV5_20151103074515","2010-09-15T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.920000000000002,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8035,"POWERLINKV5_20151103074515","2010-09-15T01:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-14.47,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8036,"POWERLINKV5_20151103074515","2010-09-15T01:20:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-11.95,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8037,"POWERLINKV5_20151103074515","2010-09-15T01:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.86,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8038,"POWERLINKV5_20151103074515","2010-09-15T01:50:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.58,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8039,"POWERLINKV5_20151103074515","2010-09-15T01:55:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.37,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8040,"POWERLINKV5_20151103074515","2010-09-15T02:15:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.37,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8041,"POWERLINKV5_20151103074515","2010-09-15T02:25:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.62,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8042,"POWERLINKV5_20151103074515","2010-09-15T02:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.559999999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8043,"POWERLINKV5_20151103074515","2010-09-15T03:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.73,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8044,"POWERLINKV5_20151103074515","2010-09-23T06:05:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.42,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8045,"POWERLINKV5_20151103074515","2010-09-23T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1021.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8046,"POWERLINKV5_20151103074515","2010-09-24T06:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1022,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8047,"POWERLINKV5_20151103074515","2010-09-25T06:10:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8048,"POWERLINKV5_20151103074515","2010-09-25T06:15:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1013.66,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8049,"POWERLINKV5_20151103074515","2010-09-27T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-11.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8050,"POWERLINKV5_20151103074515","2010-09-27T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.66,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8051,"POWERLINKV5_20151103074515","2010-09-28T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-48.6,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8052,"POWERLINKV5_20151103074515","2010-09-28T22:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-19.46,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8053,"POWERLINKV5_20151103074515","2010-09-28T22:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.53,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8054,"POWERLINKV5_20151103074515","2010-09-28T22:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8055,"POWERLINKV5_20151103074515","2010-09-29T18:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-23.2,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8056,"POWERLINKV5_20151103074515","2010-09-29T18:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.66,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8057,"POWERLINKV5_20151103074515","2010-09-29T19:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-24.28,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8058,"POWERLINKV5_20151103074515","2010-09-29T19:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-36.299999999999997,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8059,"POWERLINKV5_20151103074515","2010-09-29T19:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-37.5,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8060,"POWERLINKV5_20151103074515","2010-09-29T19:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-16.32,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8061,"POWERLINKV5_20151103074515","2010-09-29T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-25.82,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8062,"POWERLINKV5_20151103074515","2010-09-29T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-31.02,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8063,"POWERLINKV5_20151103074515","2010-09-29T22:35:00","Q:N_NIL_N4","Q-NIL","2008-07-01",1,-14.84,"Outage = Nil, Qld to NSW on QNI Transient Stability Limit, Fault on Liddell to Newcastle (81) 330kV line","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8064,"POWERLINKV5_20151103074515","2010-09-29T22:40:00","Q:N_NIL_N4","Q-NIL","2008-07-01",1,-14.34,"Outage = Nil, Qld to NSW on QNI Transient Stability Limit, Fault on Liddell to Newcastle (81) 330kV line","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8065,"POWERLINKV5_20151103074515","2010-09-29T23:05:00","Q:N_NIL_N4","Q-NIL","2008-07-01",1,-10.43,"Outage = Nil, Qld to NSW on QNI Transient Stability Limit, Fault on Liddell to Newcastle (81) 330kV line","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8066,"POWERLINKV5_20151103074515","2010-09-29T23:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-24.87,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8067,"POWERLINKV5_20151103074515","2010-09-30T05:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-12.48,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8068,"POWERLINKV5_20151103074515","2010-09-30T06:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.65,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8069,"POWERLINKV5_20151103074515","2010-09-30T06:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.26,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8070,"POWERLINKV5_20151103074515","2010-09-30T06:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-14.29,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8071,"POWERLINKV5_20151103074515","2010-09-30T07:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.21,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8072,"POWERLINKV5_20151103074515","2010-09-30T22:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-31.8,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8073,"POWERLINKV5_20151103074515","2010-09-30T22:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-32.979999999999997,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8074,"POWERLINKV5_20151103074515","2010-09-30T22:20:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-14.46,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8075,"POWERLINKV5_20151103074515","2010-09-30T22:35:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-15.49,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8076,"POWERLINKV5_20151103074515","2010-09-30T23:00:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.239999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8077,"POWERLINKV5_20151103074515","2010-09-30T23:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2009-03-30",1,-13.42,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Bulli Creek, 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8078,"POWERLINKV5_20151103074515","2010-10-01T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-13.14,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8079,"POWERLINKV5_20151103074515","2010-10-01T01:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.56,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8080,"POWERLINKV5_20151103074515","2010-10-01T01:55:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-22.81,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8081,"POWERLINKV5_20151103074515","2010-10-01T02:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.38,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8082,"POWERLINKV5_20151103074515","2010-10-06T01:40:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.57,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8083,"POWERLINKV5_20151103074515","2010-10-06T04:25:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-13.34,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8084,"POWERLINKV5_20151103074515","2010-10-09T05:15:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-11.75,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8085,"POWERLINKV5_20151103074515","2010-10-17T02:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.64,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8086,"POWERLINKV5_20151103074515","2010-10-17T14:45:00","CA_BPS_3BCD0809_01","CA_BPS_3BCD0809","2010-10-17",1,-68196.13,"Constraint Automation, O/L 275KV_855     @H24_CALV for CTG LQIV on trip of 871 H24_CALV - H40_WURD 275KV.  Generated by STNET[MANFR] Host MANEEMP4(BP)","OUTAGE","OTHER","NIL","REGULATED","99","AEMO invoked constraint automation constraint to manage trip of Feeder 871 and overload on Feeder 855.  Refer to Market Notice 33059.","UNPLANNED",0]
[8087,"POWERLINKV5_20151103074515","2010-10-19T00:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-19.2,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8088,"POWERLINKV5_20151103074515","2010-10-19T01:05:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-16.739999999999998,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8089,"POWERLINKV5_20151103074515","2010-10-19T01:10:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.6,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8090,"POWERLINKV5_20151103074515","2010-10-19T01:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-23.5,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8091,"POWERLINKV5_20151103074515","2010-10-19T01:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.69,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8092,"POWERLINKV5_20151103074515","2010-10-19T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-18.63,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8093,"POWERLINKV5_20151103074515","2010-10-19T05:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,11.64,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8094,"POWERLINKV5_20151103074515","2010-10-19T05:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,25.54,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8095,"POWERLINKV5_20151103074515","2010-10-19T05:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,26.53,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8096,"POWERLINKV5_20151103074515","2010-10-19T05:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,11.89,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8097,"POWERLINKV5_20151103074515","2010-10-19T05:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,11.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8098,"POWERLINKV5_20151103074515","2010-10-19T06:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,13.77,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8099,"POWERLINKV5_20151103074515","2010-10-19T06:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,12.38,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8100,"POWERLINKV5_20151103074515","2010-10-19T06:20:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,38.619999999999997,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8101,"POWERLINKV5_20151103074515","2010-10-19T06:25:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,36.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8102,"POWERLINKV5_20151103074515","2010-10-19T06:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,45.18,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8103,"POWERLINKV5_20151103074515","2010-10-19T06:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,36.299999999999997,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8104,"POWERLINKV5_20151103074515","2010-10-19T06:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,37.26,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8105,"POWERLINKV5_20151103074515","2010-10-19T06:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,36.24,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8106,"POWERLINKV5_20151103074515","2010-10-19T06:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,36.36,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8107,"POWERLINKV5_20151103074515","2010-10-19T06:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,38.619999999999997,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8108,"POWERLINKV5_20151103074515","2010-10-19T07:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,36.36,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8109,"POWERLINKV5_20151103074515","2010-10-19T10:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,10.43,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8110,"POWERLINKV5_20151103074515","2010-10-19T14:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,10.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","TransGrid planned outage of Feeder 8L, refer to NOS TG_9054.","PLANNED",0]
[8111,"POWERLINKV5_20151103074515","2010-10-19T19:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,10.18,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8M","REGULATED","99","TransGrid planned outage of Feeder 8M, refer to NOS TG_9050.","PLANNED",0]
[8112,"POWERLINKV5_20151103074515","2010-10-21T01:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-47.52,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8113,"POWERLINKV5_20151103074515","2010-10-22T01:45:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-10.09,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8114,"POWERLINKV5_20151103074515","2010-10-22T01:50:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-17.68,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8115,"POWERLINKV5_20151103074515","2010-10-22T04:40:00","Q>N_NIL_8L_8M","Q-NIL","2008-11-18",1,-23.81,"Out= Nil, limit QNI flow to avoid overloading 8L or 8M on trip of the other","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8116,"POWERLINKV5_20151103074515","2010-10-23T02:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.14,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8117,"POWERLINKV5_20151103074515","2010-10-24T04:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-10.64,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8118,"POWERLINKV5_20151103074515","2010-10-25T04:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.09,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8119,"POWERLINKV5_20151103074515","2010-10-25T04:15:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.09,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8120,"POWERLINKV5_20151103074515","2010-10-26T02:20:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-11.02,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8121,"POWERLINKV5_20151103074515","2010-10-27T02:20:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-10.34,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8122,"POWERLINKV5_20151103074515","2010-10-27T02:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.32,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8123,"POWERLINKV5_20151103074515","2010-10-28T01:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.05,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8124,"POWERLINKV5_20151103074515","2010-10-29T01:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.52,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8125,"POWERLINKV5_20151103074515","2010-10-29T01:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-16.809999999999999,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8126,"POWERLINKV5_20151103074515","2010-10-30T01:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.41,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8127,"POWERLINKV5_20151103074515","2010-10-30T01:15:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.649999999999999,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8128,"POWERLINKV5_20151103074515","2010-10-30T01:30:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-11.57,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8129,"POWERLINKV5_20151103074515","2010-10-30T02:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-17.47,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8130,"POWERLINKV5_20151103074515","2010-10-30T04:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-13.83,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8131,"POWERLINKV5_20151103074515","2010-11-02T00:10:00","Q>NIL_757+758_B","Q-NIL","2010-08-25",2,-19.420000000000002,"Out=Nil, Thermal limit for 110kV fdrs( 757 + 758)  Mudgeeraba to Terranora (at Mudgeeraba) System Normal. Summer and Winter ECS ratings selected by status","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8132,"POWERLINKV5_20151103074515","2010-11-02T00:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-17.47,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8133,"POWERLINKV5_20151103074515","2010-11-02T00:30:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.35,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8134,"POWERLINKV5_20151103074515","2010-11-02T00:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.14,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8135,"POWERLINKV5_20151103074515","2010-11-02T00:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.29,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8136,"POWERLINKV5_20151103074515","2010-11-02T01:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-1108.98,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8137,"POWERLINKV5_20151103074515","2010-11-02T01:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.54,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8138,"POWERLINKV5_20151103074515","2010-11-02T01:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.05,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8139,"POWERLINKV5_20151103074515","2010-11-02T04:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.989999999999998,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8140,"POWERLINKV5_20151103074515","2010-11-02T07:20:00","QNTE_ROC","Q-NIL","2006-12-27",1,-352.3,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8141,"POWERLINKV5_20151103074515","2010-11-02T07:55:00","Q>>PWSP_WOSP_SPCE","Q-808_PARALLEL_CLOSE","2010-06-29",2,-42194.78,"Out= 808 Palmwoods to South Pine 275kV line, avoid O/L 745/1 or 746/1 South Pine to Caboolture 110kV line on trip of 807 Woolooga to South Pine 275kV line, Feedback.","OUTAGE","OTHER","Feeder 808","REGULATED","INCLUDED","Planned outage of Feeder 808, refer to AFW Q10S/1393.","PLANNED",1]
[8142,"POWERLINKV5_20151103074515","2010-11-02T08:00:00","Q>>PWSP_WOSP_SPCE","Q-808_PARALLEL_CLOSE","2010-06-29",2,-20117.330000000002,"Out= 808 Palmwoods to South Pine 275kV line, avoid O/L 745/1 or 746/1 South Pine to Caboolture 110kV line on trip of 807 Woolooga to South Pine 275kV line, Feedback.","OUTAGE","OTHER","Feeder 808","REGULATED","INCLUDED","Planned outage of Feeder 808, refer to AFW Q10S/1393.","PLANNED",1]
[8143,"POWERLINKV5_20151103074515","2010-11-02T08:05:00","Q>>PWSP_WOSP_SPCE","Q-808_PARALLEL_CLOSE","2010-06-29",2,-20145.259999999998,"Out= 808 Palmwoods to South Pine 275kV line, avoid O/L 745/1 or 746/1 South Pine to Caboolture 110kV line on trip of 807 Woolooga to South Pine 275kV line, Feedback.","OUTAGE","OTHER","Feeder 808","REGULATED","INCLUDED","Planned outage of Feeder 808, refer to AFW Q10S/1393.","PLANNED",1]
[8144,"POWERLINKV5_20151103074515","2010-11-03T01:40:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.18,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8145,"POWERLINKV5_20151103074515","2010-11-03T04:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-22.24,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8146,"POWERLINKV5_20151103074515","2010-11-03T21:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-13.63,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8147,"POWERLINKV5_20151103074515","2010-11-04T01:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.78,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8148,"POWERLINKV5_20151103074515","2010-11-04T01:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-20.8,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8149,"POWERLINKV5_20151103074515","2010-11-04T03:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-10.9,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8150,"POWERLINKV5_20151103074515","2010-11-04T03:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.03,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8151,"POWERLINKV5_20151103074515","2010-11-11T04:45:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-11.73,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8152,"POWERLINKV5_20151103074515","2010-11-16T01:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8153,"POWERLINKV5_20151103074515","2010-11-16T01:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.11,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8154,"POWERLINKV5_20151103074515","2010-11-16T01:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.65,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8155,"POWERLINKV5_20151103074515","2010-11-16T01:35:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.01,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8156,"POWERLINKV5_20151103074515","2010-11-16T01:40:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.72,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8157,"POWERLINKV5_20151103074515","2010-11-16T01:50:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.76,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8158,"POWERLINKV5_20151103074515","2010-11-16T01:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.82,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8159,"POWERLINKV5_20151103074515","2010-11-16T02:15:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-18.29,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8160,"POWERLINKV5_20151103074515","2010-11-16T04:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-10.09,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8161,"POWERLINKV5_20151103074515","2010-11-17T00:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-16.899999999999999,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8162,"POWERLINKV5_20151103074515","2010-11-17T01:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.57,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8163,"POWERLINKV5_20151103074515","2010-11-17T01:30:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-15.84,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8164,"POWERLINKV5_20151103074515","2010-11-17T02:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.1,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8165,"POWERLINKV5_20151103074515","2010-11-17T06:45:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-12.29,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8166,"POWERLINKV5_20151103074515","2010-11-18","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-16.23,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8167,"POWERLINKV5_20151103074515","2010-11-18T00:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-1105.71,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8168,"POWERLINKV5_20151103074515","2010-11-18T03:40:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-23.55,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8169,"POWERLINKV5_20151103074515","2010-11-18T04:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.77,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8170,"POWERLINKV5_20151103074515","2010-11-18T04:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-22.2,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8171,"POWERLINKV5_20151103074515","2010-11-18T04:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.260000000000002,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8172,"POWERLINKV5_20151103074515","2010-11-19T01:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.2,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8173,"POWERLINKV5_20151103074515","2010-11-19T01:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-1112.21,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8174,"POWERLINKV5_20151103074515","2010-11-19T02:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.11,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8175,"POWERLINKV5_20151103074515","2010-11-19T03:15:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.26,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8176,"POWERLINKV5_20151103074515","2010-11-19T03:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.91,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8177,"POWERLINKV5_20151103074515","2010-11-19T04:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-11.64,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8178,"POWERLINKV5_20151103074515","2010-11-21T07:00:00","Q>MUTE757_758_B","Q-MUTE757_758","2010-08-13",2,-24.38,"Out= Terranora to Mudgeeraba 110kV feeders 757 or 758 thermal limit for  Mudgeeraba to Terranora (at Mudgeeraba)  Transfers","OUTAGE","OTHER","Feeder 757","REGULATED","3","Country Energy outage of Feeder 757, no Country Energy number recorded in NOS, Company Booking ID 7_20101109152549.","PLANNED",0]
[8179,"POWERLINKV5_20151103074515","2010-11-21T07:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.98,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8180,"POWERLINKV5_20151103074515","2010-11-22T04:20:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.95,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8181,"POWERLINKV5_20151103074515","2010-11-22T22:20:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-10.11,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8182,"POWERLINKV5_20151103074515","2010-11-23T02:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.58,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8183,"POWERLINKV5_20151103074515","2010-11-23T21:55:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.66,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8184,"POWERLINKV5_20151103074515","2010-11-24T01:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-20.57,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8185,"POWERLINKV5_20151103074515","2010-11-24T02:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.24,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8186,"POWERLINKV5_20151103074515","2010-11-24T03:20:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-22.91,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8187,"POWERLINKV5_20151103074515","2010-11-24T03:30:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.75,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8188,"POWERLINKV5_20151103074515","2010-11-24T03:45:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-23.52,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8189,"POWERLINKV5_20151103074515","2010-11-24T04:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.78,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8190,"POWERLINKV5_20151103074515","2010-11-24T04:15:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.739999999999998,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8191,"POWERLINKV5_20151103074515","2010-11-25T01:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-12.99,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8192,"POWERLINKV5_20151103074515","2010-11-25T02:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-13.53,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8193,"POWERLINKV5_20151103074515","2010-11-25T02:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.83,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8194,"POWERLINKV5_20151103074515","2010-11-25T04:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-23.58,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8195,"POWERLINKV5_20151103074515","2010-11-25T22:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-18.95,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8196,"POWERLINKV5_20151103074515","2010-11-25T22:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-10.039999999999999,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8197,"POWERLINKV5_20151103074515","2010-11-25T23:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-23.66,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8198,"POWERLINKV5_20151103074515","2010-11-26T01:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-23.61,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8199,"POWERLINKV5_20151103074515","2010-11-26T01:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-14.11,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8200,"POWERLINKV5_20151103074515","2010-11-26T01:55:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-12.04,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8201,"POWERLINKV5_20151103074515","2010-11-26T02:25:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8202,"POWERLINKV5_20151103074515","2010-11-26T02:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-19.27,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8203,"POWERLINKV5_20151103074515","2010-11-26T03:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.23,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8204,"POWERLINKV5_20151103074515","2010-11-26T03:20:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-11.21,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8205,"POWERLINKV5_20151103074515","2010-11-26T03:40:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.23,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8206,"POWERLINKV5_20151103074515","2010-11-26T06:45:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.97,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8207,"POWERLINKV5_20151103074515","2010-11-26T12:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-13.02,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8208,"POWERLINKV5_20151103074515","2010-11-26T21:25:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-10.01,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8209,"POWERLINKV5_20151103074515","2010-11-26T22:05:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-30.37,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8210,"POWERLINKV5_20151103074515","2010-11-26T22:10:00","Q:N_NIL_OSC","Q-NIL","2004-12-07",1,-20.9,"Outage = Nil, limit Qld to NSW southerly flow to avoid Oscillatory Instability","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8211,"POWERLINKV5_20151103074515","2010-11-28T06:50:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-11.16,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8212,"POWERLINKV5_20151103074515","2010-11-29T01:45:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-17.84,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8213,"POWERLINKV5_20151103074515","2010-11-29T02:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-20.36,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8214,"POWERLINKV5_20151103074515","2010-11-29T04:35:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-21.59,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8215,"POWERLINKV5_20151103074515","2010-11-30T03:45:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-20.92,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8216,"POWERLINKV5_20151103074515","2010-11-30T04:00:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-15.59,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8217,"POWERLINKV5_20151103074515","2010-12-02T05:35:00","Q:N_NIL_BI_POT","Q-NIL","2009-03-30",1,-18.61,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 MW), 2008/2009 implementation","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8218,"POWERLINKV5_20151103074515","2010-12-11T05:10:00","QNTE_ROC","Q-NIL","2010-11-08",3,-15.96,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8219,"POWERLINKV5_20151103074515","2010-12-11T05:10:00","Q_N_NIL-1078","Q-NIL","2010-10-22",2,-17.760000000000002,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8220,"POWERLINKV5_20151103074515","2010-12-13T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.22,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8221,"POWERLINKV5_20151103074515","2010-12-13T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.5999999999999,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8222,"POWERLINKV5_20151103074515","2010-12-13T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.1099999999999,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8223,"POWERLINKV5_20151103074515","2010-12-13T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1024.72,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8224,"POWERLINKV5_20151103074515","2010-12-13T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1025.43,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8225,"POWERLINKV5_20151103074515","2010-12-17T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-1045.4000000000001,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8226,"POWERLINKV5_20151103074515","2010-12-17T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-28.54,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8227,"POWERLINKV5_20151103074515","2010-12-17T14:40:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-31.28,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8228,"POWERLINKV5_20151103074515","2010-12-17T14:45:00","Q>NIL_TR_TX1_4","Q-NIL","2009-07-02",1,-24.91,"Out= Nil, avoid thermal O/L on remaining Tarong 275/132 kV Tx #1 or #4, on trip of either Tarong 275/132 kV Tx #1 or #4, (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8229,"POWERLINKV5_20151103074515","2010-12-17T15:05:00","CA_BPS_3C1D7AE0_01","CA_BPS_3C1D7AE0","2010-12-17",1,-38.69,"Constraint Automation, O/L H14_MRDG TRANSF 4_H14 for CTG LQOP on trip of 9907 H14_MRDG - R4_MILLM 330KV LN.  Generated by STNET[MANBL] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Outage of Feeder 8814, Unplanned.  Constraint to manage overload of 4T at H014, on loss of 5T at H014.","UNPLANNED",1]
[8230,"POWERLINKV5_20151103074515","2010-12-17T15:20:00","CA_BPS_3C1D7AE0_01","CA_BPS_3C1D7AE0","2010-12-17",1,-19.579999999999998,"Constraint Automation, O/L H14_MRDG TRANSF 4_H14 for CTG LQOP on trip of 9907 H14_MRDG - R4_MILLM 330KV LN.  Generated by STNET[MANBL] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Outage of Feeder 8814, Unplanned.  Constraint to manage overload of 4T at H014, on loss of 5T at H014.","UNPLANNED",1]
[8231,"POWERLINKV5_20151103074515","2010-12-17T15:35:00","CA_BPS_3C1D7AE0_01","CA_BPS_3C1D7AE0","2010-12-17",1,-20.04,"Constraint Automation, O/L H14_MRDG TRANSF 4_H14 for CTG LQOP on trip of 9907 H14_MRDG - R4_MILLM 330KV LN.  Generated by STNET[MANBL] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Outage of Feeder 8814, Unplanned.  Constraint to manage overload of 4T at H014, on loss of 5T at H014.","UNPLANNED",1]
[8232,"POWERLINKV5_20151103074515","2010-12-17T15:40:00","CA_BPS_3C1D7AE0_01","CA_BPS_3C1D7AE0","2010-12-17",1,-20.05,"Constraint Automation, O/L H14_MRDG TRANSF 4_H14 for CTG LQOP on trip of 9907 H14_MRDG - R4_MILLM 330KV LN.  Generated by STNET[MANBL] Host MANEEMP4(BP)","OUTAGE","OTHER","Feeder 8814","REGULATED","INCLUDED","Outage of Feeder 8814, Unplanned.  Constraint to manage overload of 4T at H014, on loss of 5T at H014.","UNPLANNED",1]
[8233,"POWERLINKV5_20151103074515","2010-12-21T04:35:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-18.350000000000001,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8234,"POWERLINKV5_20151103074515","2010-12-22T00:10:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-11.73,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8235,"POWERLINKV5_20151103074515","2010-12-22T00:30:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-13.39,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8236,"POWERLINKV5_20151103074515","2010-12-22T01:35:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-18.53,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8237,"POWERLINKV5_20151103074515","2010-12-22T01:50:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-17.78,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8238,"POWERLINKV5_20151103074515","2010-12-22T04:25:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-11.31,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8239,"POWERLINKV5_20151103074515","2010-12-22T04:40:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-13.44,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8240,"POWERLINKV5_20151103074515","2010-12-23T00:50:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-18.48,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8241,"POWERLINKV5_20151103074515","2010-12-24T00:15:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-11.77,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8242,"POWERLINKV5_20151103074515","2010-12-24T01:10:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-13.97,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]