{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"POWERLINKV5_20151103070637"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"14.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"POWERLINK"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2013]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2013-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2014-01-01"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":97}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":1}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":98}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2013 Version: 5"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":1},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":40},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":97},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":97}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":138},null,{"$f":"SUM($P$46:$P$65)","v":97}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation",null,null,"2015-11-03T07:06:37"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":8655,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[1,"POWERLINKV5_20151103070403","2013-01-01T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.810090000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED",null,"System Normal Constraint","PLANNED",0]
[2,"POWERLINKV5_20151103070403","2013-01-01T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.04227,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3,"POWERLINKV5_20151103070403","2013-01-01T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.908380000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4,"POWERLINKV5_20151103070403","2013-01-01T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.650480000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5,"POWERLINKV5_20151103070403","2013-01-01T10:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-69.669129999999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6,"POWERLINKV5_20151103070403","2013-01-01T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.112099999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7,"POWERLINKV5_20151103070403","2013-01-01T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.041119999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8,"POWERLINKV5_20151103070403","2013-01-01T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.02805,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[9,"POWERLINKV5_20151103070403","2013-01-01T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.939599999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[10,"POWERLINKV5_20151103070403","2013-01-01T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.352310000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[11,"POWERLINKV5_20151103070403","2013-01-01T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.927,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[12,"POWERLINKV5_20151103070403","2013-01-01T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.39226,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[13,"POWERLINKV5_20151103070403","2013-01-01T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.383940000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[14,"POWERLINKV5_20151103070403","2013-01-01T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.399520000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[15,"POWERLINKV5_20151103070403","2013-01-01T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.429229999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[16,"POWERLINKV5_20151103070403","2013-01-01T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.394129999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[17,"POWERLINKV5_20151103070403","2013-01-01T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.697879999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[18,"POWERLINKV5_20151103070403","2013-01-01T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.56561,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[19,"POWERLINKV5_20151103070403","2013-01-01T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.582900000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[20,"POWERLINKV5_20151103070403","2013-01-01T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.93398999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[21,"POWERLINKV5_20151103070403","2013-01-01T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.715870000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[22,"POWERLINKV5_20151103070403","2013-01-01T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-142.93746999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[23,"POWERLINKV5_20151103070403","2013-01-01T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.58078,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[24,"POWERLINKV5_20151103070403","2013-01-01T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.36309,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[25,"POWERLINKV5_20151103070403","2013-01-01T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.67342,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[26,"POWERLINKV5_20151103070403","2013-01-01T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.981699999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[27,"POWERLINKV5_20151103070403","2013-01-01T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.925060000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[28,"POWERLINKV5_20151103070403","2013-01-01T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.888649999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[29,"POWERLINKV5_20151103070403","2013-01-01T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-134.27794,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[30,"POWERLINKV5_20151103070403","2013-01-01T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.946820000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[31,"POWERLINKV5_20151103070403","2013-01-01T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.343119999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[32,"POWERLINKV5_20151103070403","2013-01-01T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.087359999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[33,"POWERLINKV5_20151103070403","2013-01-01T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.6917,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[34,"POWERLINKV5_20151103070403","2013-01-01T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.574480000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[35,"POWERLINKV5_20151103070403","2013-01-01T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.010809999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[36,"POWERLINKV5_20151103070403","2013-01-01T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-256.77683999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[37,"POWERLINKV5_20151103070403","2013-01-01T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.944710000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[38,"POWERLINKV5_20151103070403","2013-01-01T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.188330000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[39,"POWERLINKV5_20151103070403","2013-01-01T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.031379999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[40,"POWERLINKV5_20151103070403","2013-01-01T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.26999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[41,"POWERLINKV5_20151103070403","2013-01-01T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.830039999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[42,"POWERLINKV5_20151103070403","2013-01-01T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.647239999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[43,"POWERLINKV5_20151103070403","2013-01-01T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.32571999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[44,"POWERLINKV5_20151103070403","2013-01-01T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.33993000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[45,"POWERLINKV5_20151103070403","2013-01-01T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-254.84816000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[46,"POWERLINKV5_20151103070403","2013-01-01T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-253.94829999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[47,"POWERLINKV5_20151103070403","2013-01-01T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-117.05846,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[48,"POWERLINKV5_20151103070403","2013-01-01T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.371470000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[49,"POWERLINKV5_20151103070403","2013-01-01T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-29.888480000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[50,"POWERLINKV5_20151103070403","2013-01-01T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.110590000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[51,"POWERLINKV5_20151103070403","2013-01-01T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.47204,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[52,"POWERLINKV5_20151103070403","2013-01-01T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.994219999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[53,"POWERLINKV5_20151103070403","2013-01-01T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.09769,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[54,"POWERLINKV5_20151103070403","2013-01-01T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.29401,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[55,"POWERLINKV5_20151103070403","2013-01-01T16:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-84.379620000000003,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[56,"POWERLINKV5_20151103070403","2013-01-01T16:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-224.06900999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[57,"POWERLINKV5_20151103070403","2013-01-01T16:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-223.6379,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[58,"POWERLINKV5_20151103070403","2013-01-01T16:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-223.30010999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[59,"POWERLINKV5_20151103070403","2013-01-01T16:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-89.352140000000006,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[60,"POWERLINKV5_20151103070403","2013-01-01T16:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-221.24301,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[61,"POWERLINKV5_20151103070403","2013-01-01T17:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-221.02356,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[62,"POWERLINKV5_20151103070403","2013-01-01T17:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-221.43810999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[63,"POWERLINKV5_20151103070403","2013-01-01T17:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-220.22908000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[64,"POWERLINKV5_20151103070403","2013-01-01T17:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-90.31474,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[65,"POWERLINKV5_20151103070403","2013-01-01T17:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-91.732010000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[66,"POWERLINKV5_20151103070403","2013-01-01T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.973410000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[67,"POWERLINKV5_20151103070403","2013-01-01T18:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.58338,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[68,"POWERLINKV5_20151103070403","2013-01-01T22:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.301409999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[69,"POWERLINKV5_20151103070403","2013-01-01T22:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-32.70346,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[70,"POWERLINKV5_20151103070403","2013-01-01T22:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.827309999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[71,"POWERLINKV5_20151103070403","2013-01-01T22:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.124699999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[72,"POWERLINKV5_20151103070403","2013-01-01T22:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.064410000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[73,"POWERLINKV5_20151103070403","2013-01-01T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.96613,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[74,"POWERLINKV5_20151103070403","2013-01-01T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.73803,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[75,"POWERLINKV5_20151103070403","2013-01-01T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.42027,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[76,"POWERLINKV5_20151103070403","2013-01-01T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.44317,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[77,"POWERLINKV5_20151103070403","2013-01-01T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.930210000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[78,"POWERLINKV5_20151103070403","2013-01-01T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1186.5276200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[79,"POWERLINKV5_20151103070403","2013-01-01T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.064019999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[80,"POWERLINKV5_20151103070403","2013-01-01T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.177499999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[81,"POWERLINKV5_20151103070403","2013-01-02","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.56542,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[82,"POWERLINKV5_20151103070403","2013-01-02T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.221119999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[83,"POWERLINKV5_20151103070403","2013-01-02T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-94223.814490000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[84,"POWERLINKV5_20151103070403","2013-01-02T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.730649999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[85,"POWERLINKV5_20151103070403","2013-01-02T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.907389999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[86,"POWERLINKV5_20151103070403","2013-01-02T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.8904,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[87,"POWERLINKV5_20151103070403","2013-01-02T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.482509999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[88,"POWERLINKV5_20151103070403","2013-01-02T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.287039999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[89,"POWERLINKV5_20151103070403","2013-01-02T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.509059999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[90,"POWERLINKV5_20151103070403","2013-01-02T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.802320000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[91,"POWERLINKV5_20151103070403","2013-01-02T07:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.364049999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[92,"POWERLINKV5_20151103070403","2013-01-02T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.037030000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[93,"POWERLINKV5_20151103070403","2013-01-02T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.02364,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[94,"POWERLINKV5_20151103070403","2013-01-02T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.791519999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[95,"POWERLINKV5_20151103070403","2013-01-02T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.121,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[96,"POWERLINKV5_20151103070403","2013-01-02T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.487639999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[97,"POWERLINKV5_20151103070403","2013-01-02T08:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.583419999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[98,"POWERLINKV5_20151103070403","2013-01-02T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.37903,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[99,"POWERLINKV5_20151103070403","2013-01-02T08:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.284140000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[100,"POWERLINKV5_20151103070403","2013-01-02T08:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.863430000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[101,"POWERLINKV5_20151103070403","2013-01-02T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.873370000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[102,"POWERLINKV5_20151103070403","2013-01-02T08:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.198140000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[103,"POWERLINKV5_20151103070403","2013-01-02T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-257.90336000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[104,"POWERLINKV5_20151103070403","2013-01-02T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-257.53595000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[105,"POWERLINKV5_20151103070403","2013-01-02T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.00000999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[106,"POWERLINKV5_20151103070403","2013-01-02T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-291.45184999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[107,"POWERLINKV5_20151103070403","2013-01-02T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-33.672289999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[108,"POWERLINKV5_20151103070403","2013-01-02T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-31.434570000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[109,"POWERLINKV5_20151103070403","2013-01-02T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.258789999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[110,"POWERLINKV5_20151103070403","2013-01-02T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.463450000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[111,"POWERLINKV5_20151103070403","2013-01-02T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.445039999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[112,"POWERLINKV5_20151103070403","2013-01-02T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.747790000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[113,"POWERLINKV5_20151103070403","2013-01-02T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.600540000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[114,"POWERLINKV5_20151103070403","2013-01-02T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.83784,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[115,"POWERLINKV5_20151103070403","2013-01-02T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-256.24925999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[116,"POWERLINKV5_20151103070403","2013-01-02T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.41165,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[117,"POWERLINKV5_20151103070403","2013-01-02T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-113.63951,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[118,"POWERLINKV5_20151103070403","2013-01-02T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12201.3632,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[119,"POWERLINKV5_20151103070403","2013-01-02T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.75811,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[120,"POWERLINKV5_20151103070403","2013-01-02T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-602.77959999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[121,"POWERLINKV5_20151103070403","2013-01-02T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.20408,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[122,"POWERLINKV5_20151103070403","2013-01-02T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-707.17731000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[123,"POWERLINKV5_20151103070403","2013-01-02T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11808.416300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[124,"POWERLINKV5_20151103070403","2013-01-02T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-50.053150000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[125,"POWERLINKV5_20151103070403","2013-01-02T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.420459999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[126,"POWERLINKV5_20151103070403","2013-01-02T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.43759,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[127,"POWERLINKV5_20151103070403","2013-01-02T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-63.856380000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[128,"POWERLINKV5_20151103070403","2013-01-02T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.07517000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[129,"POWERLINKV5_20151103070403","2013-01-02T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.49583999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[130,"POWERLINKV5_20151103070403","2013-01-02T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-309.27834999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[131,"POWERLINKV5_20151103070403","2013-01-02T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-94.672349999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[132,"POWERLINKV5_20151103070403","2013-01-02T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.23804999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[133,"POWERLINKV5_20151103070403","2013-01-02T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-706.84451999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[134,"POWERLINKV5_20151103070403","2013-01-02T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1159.5035,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[135,"POWERLINKV5_20151103070403","2013-01-02T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1170.0367200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[136,"POWERLINKV5_20151103070403","2013-01-02T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.049999999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[137,"POWERLINKV5_20151103070403","2013-01-02T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-65.535749999999993,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[138,"POWERLINKV5_20151103070403","2013-01-02T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-123.68351,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[139,"POWERLINKV5_20151103070403","2013-01-02T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-59.85501,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[140,"POWERLINKV5_20151103070403","2013-01-02T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-326.54797000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[141,"POWERLINKV5_20151103070403","2013-01-02T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12353.36515,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[142,"POWERLINKV5_20151103070403","2013-01-02T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-282.74889000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[143,"POWERLINKV5_20151103070403","2013-01-02T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-256.81759,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[144,"POWERLINKV5_20151103070403","2013-01-02T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.84917000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[145,"POWERLINKV5_20151103070403","2013-01-02T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.58330000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[146,"POWERLINKV5_20151103070403","2013-01-02T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.54489999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[147,"POWERLINKV5_20151103070403","2013-01-02T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.241390000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[148,"POWERLINKV5_20151103070403","2013-01-02T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.770949999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[149,"POWERLINKV5_20151103070403","2013-01-02T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-251.10670999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[150,"POWERLINKV5_20151103070403","2013-01-02T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-249.28063,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[151,"POWERLINKV5_20151103070403","2013-01-02T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-261.85032000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[152,"POWERLINKV5_20151103070403","2013-01-02T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-259.45184999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[153,"POWERLINKV5_20151103070403","2013-01-02T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-251.03083000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[154,"POWERLINKV5_20151103070403","2013-01-02T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.967019999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[155,"POWERLINKV5_20151103070403","2013-01-02T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.09646,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[156,"POWERLINKV5_20151103070403","2013-01-02T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.650280000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[157,"POWERLINKV5_20151103070403","2013-01-02T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.799689999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[158,"POWERLINKV5_20151103070403","2013-01-02T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-246.3279,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[159,"POWERLINKV5_20151103070403","2013-01-02T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.82705000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[160,"POWERLINKV5_20151103070403","2013-01-02T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.30563000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[161,"POWERLINKV5_20151103070403","2013-01-02T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.27439000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[162,"POWERLINKV5_20151103070403","2013-01-02T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-244.80010999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[163,"POWERLINKV5_20151103070403","2013-01-02T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-244.61894000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[164,"POWERLINKV5_20151103070403","2013-01-02T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-246.56668999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[165,"POWERLINKV5_20151103070403","2013-01-02T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.19403,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[166,"POWERLINKV5_20151103070403","2013-01-02T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.025550000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[167,"POWERLINKV5_20151103070403","2013-01-02T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.874670000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[168,"POWERLINKV5_20151103070403","2013-01-02T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.381889999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[169,"POWERLINKV5_20151103070403","2013-01-02T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.335830000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[170,"POWERLINKV5_20151103070403","2013-01-02T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.473689999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[171,"POWERLINKV5_20151103070403","2013-01-02T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-28.75384,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[172,"POWERLINKV5_20151103070403","2013-01-02T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-29.016269999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[173,"POWERLINKV5_20151103070403","2013-01-02T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-26.912579999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[174,"POWERLINKV5_20151103070403","2013-01-02T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-247.77182999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[175,"POWERLINKV5_20151103070403","2013-01-02T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-247.7226,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[176,"POWERLINKV5_20151103070403","2013-01-02T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.96669,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[177,"POWERLINKV5_20151103070403","2013-01-02T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.968449999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[178,"POWERLINKV5_20151103070403","2013-01-02T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.477719999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[179,"POWERLINKV5_20151103070403","2013-01-02T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.87201,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[180,"POWERLINKV5_20151103070403","2013-01-02T23:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-254.82554999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[181,"POWERLINKV5_20151103070403","2013-01-02T23:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-253.54536999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[182,"POWERLINKV5_20151103070403","2013-01-02T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-67.799459999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[183,"POWERLINKV5_20151103070403","2013-01-02T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-68.047430000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[184,"POWERLINKV5_20151103070403","2013-01-02T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.59854,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[185,"POWERLINKV5_20151103070403","2013-01-03","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.72724,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[186,"POWERLINKV5_20151103070403","2013-01-03T00:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.843730000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[187,"POWERLINKV5_20151103070403","2013-01-03T00:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.84577,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[188,"POWERLINKV5_20151103070403","2013-01-03T00:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-69.173550000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[189,"POWERLINKV5_20151103070403","2013-01-03T00:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.801159999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[190,"POWERLINKV5_20151103070403","2013-01-03T00:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.36261,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[191,"POWERLINKV5_20151103070403","2013-01-03T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-349.04530999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[192,"POWERLINKV5_20151103070403","2013-01-03T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.36889,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[193,"POWERLINKV5_20151103070403","2013-01-03T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.295740000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[194,"POWERLINKV5_20151103070403","2013-01-03T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.937620000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[195,"POWERLINKV5_20151103070403","2013-01-03T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.900370000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[196,"POWERLINKV5_20151103070403","2013-01-03T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-44.859200000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[197,"POWERLINKV5_20151103070403","2013-01-03T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.627699999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[198,"POWERLINKV5_20151103070403","2013-01-03T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.18214999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[199,"POWERLINKV5_20151103070403","2013-01-03T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.32902,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[200,"POWERLINKV5_20151103070403","2013-01-03T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.366379999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[201,"POWERLINKV5_20151103070403","2013-01-03T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.03925,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[202,"POWERLINKV5_20151103070403","2013-01-03T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-263.12434000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[203,"POWERLINKV5_20151103070403","2013-01-03T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-799.58362999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[204,"POWERLINKV5_20151103070403","2013-01-03T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.88171999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[205,"POWERLINKV5_20151103070403","2013-01-03T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.78994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[206,"POWERLINKV5_20151103070403","2013-01-03T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.36545000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[207,"POWERLINKV5_20151103070403","2013-01-03T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.42069,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[208,"POWERLINKV5_20151103070403","2013-01-03T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.329729999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[209,"POWERLINKV5_20151103070403","2013-01-03T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.750869999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[210,"POWERLINKV5_20151103070403","2013-01-03T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.354680000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[211,"POWERLINKV5_20151103070403","2013-01-03T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.0670399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[212,"POWERLINKV5_20151103070403","2013-01-03T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.09327000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[213,"POWERLINKV5_20151103070403","2013-01-03T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.960880000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[214,"POWERLINKV5_20151103070403","2013-01-03T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.60773,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[215,"POWERLINKV5_20151103070403","2013-01-03T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.782530000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[216,"POWERLINKV5_20151103070403","2013-01-03T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.48403999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[217,"POWERLINKV5_20151103070403","2013-01-03T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.48509000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[218,"POWERLINKV5_20151103070403","2013-01-03T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.47516000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[219,"POWERLINKV5_20151103070403","2013-01-03T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.677219999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[220,"POWERLINKV5_20151103070403","2013-01-03T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.67961,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[221,"POWERLINKV5_20151103070403","2013-01-03T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-77.894090000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[222,"POWERLINKV5_20151103070403","2013-01-03T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.03811,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[223,"POWERLINKV5_20151103070403","2013-01-03T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.585730000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[224,"POWERLINKV5_20151103070403","2013-01-03T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.612089999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[225,"POWERLINKV5_20151103070403","2013-01-03T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.188040000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[226,"POWERLINKV5_20151103070403","2013-01-03T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.964459999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[227,"POWERLINKV5_20151103070403","2013-01-03T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.82058000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[228,"POWERLINKV5_20151103070403","2013-01-03T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.568439999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[229,"POWERLINKV5_20151103070403","2013-01-03T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.28188999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[230,"POWERLINKV5_20151103070403","2013-01-03T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.4295300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[231,"POWERLINKV5_20151103070403","2013-01-03T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.59036,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[232,"POWERLINKV5_20151103070403","2013-01-03T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.18788,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[233,"POWERLINKV5_20151103070403","2013-01-03T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.593679999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[234,"POWERLINKV5_20151103070403","2013-01-03T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.75420000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[235,"POWERLINKV5_20151103070403","2013-01-03T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.69628,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[236,"POWERLINKV5_20151103070403","2013-01-03T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-804.76139000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[237,"POWERLINKV5_20151103070403","2013-01-03T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.63238999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[238,"POWERLINKV5_20151103070403","2013-01-03T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.813020000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[239,"POWERLINKV5_20151103070403","2013-01-03T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.98728999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[240,"POWERLINKV5_20151103070403","2013-01-03T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-804.14074000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[241,"POWERLINKV5_20151103070403","2013-01-03T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-803.75058000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[242,"POWERLINKV5_20151103070403","2013-01-03T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.96440000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[243,"POWERLINKV5_20151103070403","2013-01-03T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.428239999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[244,"POWERLINKV5_20151103070403","2013-01-03T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.87781,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[245,"POWERLINKV5_20151103070403","2013-01-03T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.63612000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[246,"POWERLINKV5_20151103070403","2013-01-03T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-803.43948,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[247,"POWERLINKV5_20151103070403","2013-01-03T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-803.03408000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[248,"POWERLINKV5_20151103070403","2013-01-03T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-804.81259999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[249,"POWERLINKV5_20151103070403","2013-01-03T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.87987,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[250,"POWERLINKV5_20151103070403","2013-01-03T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.111180000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[251,"POWERLINKV5_20151103070403","2013-01-03T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.180009999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[252,"POWERLINKV5_20151103070403","2013-01-03T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.948840000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[253,"POWERLINKV5_20151103070403","2013-01-03T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.34112,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[254,"POWERLINKV5_20151103070403","2013-01-03T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-262.05475999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[255,"POWERLINKV5_20151103070403","2013-01-03T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-34.967500000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[256,"POWERLINKV5_20151103070403","2013-01-03T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.54815,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[257,"POWERLINKV5_20151103070403","2013-01-03T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.496040000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[258,"POWERLINKV5_20151103070403","2013-01-03T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.06810999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[259,"POWERLINKV5_20151103070403","2013-01-03T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.69401,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[260,"POWERLINKV5_20151103070403","2013-01-03T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.182840000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[261,"POWERLINKV5_20151103070403","2013-01-03T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.2333,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[262,"POWERLINKV5_20151103070403","2013-01-03T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.573399999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[263,"POWERLINKV5_20151103070403","2013-01-03T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.13477,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[264,"POWERLINKV5_20151103070403","2013-01-03T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.180389999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[265,"POWERLINKV5_20151103070403","2013-01-03T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.79768,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[266,"POWERLINKV5_20151103070403","2013-01-03T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.576129999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[267,"POWERLINKV5_20151103070403","2013-01-03T16:35:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-25.80857,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Directlink","REGULATED","99","AEMO invoked constraint due to loss of Directlink Controls. Refer to Market Notice 40855","UNPLANNED",0]
[268,"POWERLINKV5_20151103070403","2013-01-03T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.13765999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[269,"POWERLINKV5_20151103070403","2013-01-03T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.08675,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[270,"POWERLINKV5_20151103070403","2013-01-03T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.52197,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[271,"POWERLINKV5_20151103070403","2013-01-03T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.510809999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[272,"POWERLINKV5_20151103070403","2013-01-03T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.070790000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[273,"POWERLINKV5_20151103070403","2013-01-03T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.28534,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[274,"POWERLINKV5_20151103070403","2013-01-03T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.98842,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[275,"POWERLINKV5_20151103070403","2013-01-03T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.94725,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[276,"POWERLINKV5_20151103070403","2013-01-03T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.51266,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[277,"POWERLINKV5_20151103070403","2013-01-03T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.49222,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[278,"POWERLINKV5_20151103070403","2013-01-03T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.9214,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[279,"POWERLINKV5_20151103070403","2013-01-03T17:35:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-35.403840000000002,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Directlink","REGULATED","99","AEMO invoked constraint due to loss of Directlink Controls. Refer to Market Notice 40855","UNPLANNED",0]
[280,"POWERLINKV5_20151103070403","2013-01-03T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-259.36090000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[281,"POWERLINKV5_20151103070403","2013-01-03T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.722670000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[282,"POWERLINKV5_20151103070403","2013-01-03T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.29171,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[283,"POWERLINKV5_20151103070403","2013-01-03T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.76243,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[284,"POWERLINKV5_20151103070403","2013-01-03T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.13026,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[285,"POWERLINKV5_20151103070403","2013-01-04T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.45086,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[286,"POWERLINKV5_20151103070403","2013-01-04T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.11182,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[287,"POWERLINKV5_20151103070403","2013-01-04T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2059.0356299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[288,"POWERLINKV5_20151103070403","2013-01-04T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2056.9805900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[289,"POWERLINKV5_20151103070403","2013-01-04T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2055.3381300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[290,"POWERLINKV5_20151103070403","2013-01-04T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.860989999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[291,"POWERLINKV5_20151103070403","2013-01-04T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2062.2881499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[292,"POWERLINKV5_20151103070403","2013-01-04T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.522320000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[293,"POWERLINKV5_20151103070403","2013-01-04T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.22125,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[294,"POWERLINKV5_20151103070403","2013-01-04T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.1194599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[295,"POWERLINKV5_20151103070403","2013-01-04T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2065.7927800000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[296,"POWERLINKV5_20151103070403","2013-01-04T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.08087,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[297,"POWERLINKV5_20151103070403","2013-01-04T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-63.594149999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[298,"POWERLINKV5_20151103070403","2013-01-04T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.01355,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[299,"POWERLINKV5_20151103070403","2013-01-04T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.95948,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[300,"POWERLINKV5_20151103070403","2013-01-05T01:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.13391,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[301,"POWERLINKV5_20151103070403","2013-01-05T01:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.427289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[302,"POWERLINKV5_20151103070403","2013-01-05T01:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.157889999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[303,"POWERLINKV5_20151103070403","2013-01-05T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.342840000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[304,"POWERLINKV5_20151103070403","2013-01-05T08:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.39531,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[305,"POWERLINKV5_20151103070403","2013-01-05T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.6964399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[306,"POWERLINKV5_20151103070403","2013-01-05T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-279.76382999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[307,"POWERLINKV5_20151103070403","2013-01-05T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.16660999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[308,"POWERLINKV5_20151103070403","2013-01-05T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1194.1835699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[309,"POWERLINKV5_20151103070403","2013-01-05T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.164250000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[310,"POWERLINKV5_20151103070403","2013-01-05T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.163920000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[311,"POWERLINKV5_20151103070403","2013-01-05T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.772790000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[312,"POWERLINKV5_20151103070403","2013-01-05T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.152159999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[313,"POWERLINKV5_20151103070403","2013-01-05T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.532119999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[314,"POWERLINKV5_20151103070403","2013-01-05T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.127929999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[315,"POWERLINKV5_20151103070403","2013-01-05T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-33.821719999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[316,"POWERLINKV5_20151103070403","2013-01-05T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.129550000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[317,"POWERLINKV5_20151103070403","2013-01-05T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.68637,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[318,"POWERLINKV5_20151103070403","2013-01-05T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.37332,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[319,"POWERLINKV5_20151103070403","2013-01-05T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.687719999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[320,"POWERLINKV5_20151103070403","2013-01-05T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.19583,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[321,"POWERLINKV5_20151103070403","2013-01-05T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.49290000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[322,"POWERLINKV5_20151103070403","2013-01-05T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.00990999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[323,"POWERLINKV5_20151103070403","2013-01-05T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.13610999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[324,"POWERLINKV5_20151103070403","2013-01-05T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.81790000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[325,"POWERLINKV5_20151103070403","2013-01-05T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.96337,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[326,"POWERLINKV5_20151103070403","2013-01-05T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-25.466190000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[327,"POWERLINKV5_20151103070403","2013-01-05T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.09868,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[328,"POWERLINKV5_20151103070403","2013-01-05T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.09868,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[329,"POWERLINKV5_20151103070403","2013-01-05T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.44143000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[330,"POWERLINKV5_20151103070403","2013-01-05T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-24.489439999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[331,"POWERLINKV5_20151103070403","2013-01-05T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.79424999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[332,"POWERLINKV5_20151103070403","2013-01-05T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.11932000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[333,"POWERLINKV5_20151103070403","2013-01-05T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.70837,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[334,"POWERLINKV5_20151103070403","2013-01-05T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.351460000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[335,"POWERLINKV5_20151103070403","2013-01-05T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-64.185860000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[336,"POWERLINKV5_20151103070403","2013-01-05T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.78530000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[337,"POWERLINKV5_20151103070403","2013-01-05T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.524979999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[338,"POWERLINKV5_20151103070403","2013-01-05T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-267.58449999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[339,"POWERLINKV5_20151103070403","2013-01-05T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.209969999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[340,"POWERLINKV5_20151103070403","2013-01-05T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-24.155550000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[341,"POWERLINKV5_20151103070403","2013-01-05T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.56597,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[342,"POWERLINKV5_20151103070403","2013-01-05T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.86994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[343,"POWERLINKV5_20151103070403","2013-01-05T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.563079999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[344,"POWERLINKV5_20151103070403","2013-01-05T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.849629999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[345,"POWERLINKV5_20151103070403","2013-01-05T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.274830000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[346,"POWERLINKV5_20151103070403","2013-01-05T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.786259999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[347,"POWERLINKV5_20151103070403","2013-01-05T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.66418,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[348,"POWERLINKV5_20151103070403","2013-01-05T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.463329999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[349,"POWERLINKV5_20151103070403","2013-01-05T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1183.1501800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[350,"POWERLINKV5_20151103070403","2013-01-05T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.595559999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[351,"POWERLINKV5_20151103070403","2013-01-05T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.88036,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[352,"POWERLINKV5_20151103070403","2013-01-05T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.986979999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[353,"POWERLINKV5_20151103070403","2013-01-05T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-807.55939000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[354,"POWERLINKV5_20151103070403","2013-01-05T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.223680000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[355,"POWERLINKV5_20151103070403","2013-01-05T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.902229999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[356,"POWERLINKV5_20151103070403","2013-01-05T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.816199999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[357,"POWERLINKV5_20151103070403","2013-01-05T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.800409999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[358,"POWERLINKV5_20151103070403","2013-01-05T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.630199999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[359,"POWERLINKV5_20151103070403","2013-01-05T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.613720000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[360,"POWERLINKV5_20151103070403","2013-01-05T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.356680000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[361,"POWERLINKV5_20151103070403","2013-01-05T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.225460000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[362,"POWERLINKV5_20151103070403","2013-01-05T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.73678,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[363,"POWERLINKV5_20151103070403","2013-01-05T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.787570000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[364,"POWERLINKV5_20151103070403","2013-01-05T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.91704,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[365,"POWERLINKV5_20151103070403","2013-01-05T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.46477,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[366,"POWERLINKV5_20151103070403","2013-01-05T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.03963,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[367,"POWERLINKV5_20151103070403","2013-01-05T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.50665,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[368,"POWERLINKV5_20151103070403","2013-01-05T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.079180000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[369,"POWERLINKV5_20151103070403","2013-01-05T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.264959999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[370,"POWERLINKV5_20151103070403","2013-01-05T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.22391,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[371,"POWERLINKV5_20151103070403","2013-01-05T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.786250000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[372,"POWERLINKV5_20151103070403","2013-01-05T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.0617500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[373,"POWERLINKV5_20151103070403","2013-01-05T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.032800000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[374,"POWERLINKV5_20151103070403","2013-01-06T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.18638,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[375,"POWERLINKV5_20151103070403","2013-01-06T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.951360000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[376,"POWERLINKV5_20151103070403","2013-01-06T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-70.494129999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[377,"POWERLINKV5_20151103070403","2013-01-06T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.1708,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[378,"POWERLINKV5_20151103070403","2013-01-06T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2032.9808700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[379,"POWERLINKV5_20151103070403","2013-01-06T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.115729999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[380,"POWERLINKV5_20151103070403","2013-01-06T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.235790000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[381,"POWERLINKV5_20151103070403","2013-01-06T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.705919999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[382,"POWERLINKV5_20151103070403","2013-01-06T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.948360000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[383,"POWERLINKV5_20151103070403","2013-01-06T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.04633000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[384,"POWERLINKV5_20151103070403","2013-01-06T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.06420000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[385,"POWERLINKV5_20151103070403","2013-01-06T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.09861000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[386,"POWERLINKV5_20151103070403","2013-01-06T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.09861000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[387,"POWERLINKV5_20151103070403","2013-01-06T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-812.61327000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[388,"POWERLINKV5_20151103070403","2013-01-06T10:40:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-28.16835,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[389,"POWERLINKV5_20151103070403","2013-01-06T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-841.64634999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[390,"POWERLINKV5_20151103070403","2013-01-06T10:45:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-103.52529,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[391,"POWERLINKV5_20151103070403","2013-01-06T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-917.83520999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[392,"POWERLINKV5_20151103070403","2013-01-06T10:50:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-62.84375,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[393,"POWERLINKV5_20151103070403","2013-01-06T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-520.07707000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[394,"POWERLINKV5_20151103070403","2013-01-06T10:55:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-113.09175,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[395,"POWERLINKV5_20151103070403","2013-01-06T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-926.33266000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[396,"POWERLINKV5_20151103070403","2013-01-06T11:00:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-110.95646000000001,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[397,"POWERLINKV5_20151103070403","2013-01-06T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-924.15278999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[398,"POWERLINKV5_20151103070403","2013-01-06T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.09859,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[399,"POWERLINKV5_20151103070403","2013-01-06T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.102129999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[400,"POWERLINKV5_20151103070403","2013-01-06T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.58935000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[401,"POWERLINKV5_20151103070403","2013-01-06T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.32934999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[402,"POWERLINKV5_20151103070403","2013-01-06T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.32934999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[403,"POWERLINKV5_20151103070403","2013-01-06T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.32934999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[404,"POWERLINKV5_20151103070403","2013-01-06T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.29018000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[405,"POWERLINKV5_20151103070403","2013-01-06T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.264130000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[406,"POWERLINKV5_20151103070403","2013-01-06T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.347660000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[407,"POWERLINKV5_20151103070403","2013-01-06T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1183.74954,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[408,"POWERLINKV5_20151103070403","2013-01-06T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.74610999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[409,"POWERLINKV5_20151103070403","2013-01-06T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.32934999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[410,"POWERLINKV5_20151103070403","2013-01-06T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.0661,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[411,"POWERLINKV5_20151103070403","2013-01-06T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.3782,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[412,"POWERLINKV5_20151103070403","2013-01-06T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.490220000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[413,"POWERLINKV5_20151103070403","2013-01-06T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.60617999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[414,"POWERLINKV5_20151103070403","2013-01-06T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.36941000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[415,"POWERLINKV5_20151103070403","2013-01-06T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.996490000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[416,"POWERLINKV5_20151103070403","2013-01-06T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.03095999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[417,"POWERLINKV5_20151103070403","2013-01-06T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.05552999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[418,"POWERLINKV5_20151103070403","2013-01-06T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.94405,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[419,"POWERLINKV5_20151103070403","2013-01-06T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.49709000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[420,"POWERLINKV5_20151103070403","2013-01-06T13:05:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-28.084679999999999,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[421,"POWERLINKV5_20151103070403","2013-01-06T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-841.64634999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[422,"POWERLINKV5_20151103070403","2013-01-06T13:10:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-33.393410000000003,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[423,"POWERLINKV5_20151103070403","2013-01-06T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-846.91396999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[424,"POWERLINKV5_20151103070403","2013-01-06T13:15:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-113.73415,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[425,"POWERLINKV5_20151103070403","2013-01-06T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-929.56926999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[426,"POWERLINKV5_20151103070403","2013-01-06T13:20:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-110.87747,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[427,"POWERLINKV5_20151103070403","2013-01-06T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-924.23555999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[428,"POWERLINKV5_20151103070403","2013-01-06T13:25:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-123.75252999999999,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[429,"POWERLINKV5_20151103070403","2013-01-06T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1050.26595,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[430,"POWERLINKV5_20151103070403","2013-01-06T13:30:00","Q:N_NIL_OSC","Q-NIL","2012-12-24",1,-122.88021000000001,"Out= Nil, QNI oscillatory stability limit of 1078 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[431,"POWERLINKV5_20151103070403","2013-01-06T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1051.1289899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[432,"POWERLINKV5_20151103070403","2013-01-06T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-121.89605,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[433,"POWERLINKV5_20151103070403","2013-01-06T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.88947000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[434,"POWERLINKV5_20151103070403","2013-01-06T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.957080000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[435,"POWERLINKV5_20151103070403","2013-01-06T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-269.95576,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[436,"POWERLINKV5_20151103070403","2013-01-06T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.05358999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[437,"POWERLINKV5_20151103070403","2013-01-06T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.6676399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[438,"POWERLINKV5_20151103070403","2013-01-06T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-604.34266000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[439,"POWERLINKV5_20151103070403","2013-01-06T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.58945,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[440,"POWERLINKV5_20151103070403","2013-01-06T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.41451999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[441,"POWERLINKV5_20151103070403","2013-01-06T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-269.71400999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[442,"POWERLINKV5_20151103070403","2013-01-06T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.84089999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[443,"POWERLINKV5_20151103070403","2013-01-06T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-267.44612000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[444,"POWERLINKV5_20151103070403","2013-01-06T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-810.29061000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[445,"POWERLINKV5_20151103070403","2013-01-06T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-543.0385,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[446,"POWERLINKV5_20151103070403","2013-01-06T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-841.64702999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[447,"POWERLINKV5_20151103070403","2013-01-06T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-841.96884,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[448,"POWERLINKV5_20151103070403","2013-01-06T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-807.10725000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[449,"POWERLINKV5_20151103070403","2013-01-06T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1015.8062,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[450,"POWERLINKV5_20151103070403","2013-01-06T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-444.50876,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[451,"POWERLINKV5_20151103070403","2013-01-06T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.10445,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[452,"POWERLINKV5_20151103070403","2013-01-06T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.858339999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[453,"POWERLINKV5_20151103070403","2013-01-06T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.483359999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[454,"POWERLINKV5_20151103070403","2013-01-06T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.529000000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[455,"POWERLINKV5_20151103070403","2013-01-06T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-59.084600000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[456,"POWERLINKV5_20151103070403","2013-01-06T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.465690000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[457,"POWERLINKV5_20151103070403","2013-01-06T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.535339999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[458,"POWERLINKV5_20151103070403","2013-01-06T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.03417000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[459,"POWERLINKV5_20151103070403","2013-01-06T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.50326000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[460,"POWERLINKV5_20151103070403","2013-01-06T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-73.986050000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[461,"POWERLINKV5_20151103070403","2013-01-06T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.603750000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[462,"POWERLINKV5_20151103070403","2013-01-06T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.380710000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[463,"POWERLINKV5_20151103070403","2013-01-06T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.77178,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[464,"POWERLINKV5_20151103070403","2013-01-06T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.365749999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[465,"POWERLINKV5_20151103070403","2013-01-06T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-84.101370000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[466,"POWERLINKV5_20151103070403","2013-01-06T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.361370000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[467,"POWERLINKV5_20151103070403","2013-01-06T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.949330000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[468,"POWERLINKV5_20151103070403","2013-01-06T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.63819999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[469,"POWERLINKV5_20151103070403","2013-01-06T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.17063000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[470,"POWERLINKV5_20151103070403","2013-01-06T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.98715,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[471,"POWERLINKV5_20151103070403","2013-01-06T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.575960000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[472,"POWERLINKV5_20151103070403","2013-01-06T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.576790000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[473,"POWERLINKV5_20151103070403","2013-01-06T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-267.08629000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[474,"POWERLINKV5_20151103070403","2013-01-06T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.56171,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[475,"POWERLINKV5_20151103070403","2013-01-06T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.631740000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[476,"POWERLINKV5_20151103070403","2013-01-06T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.32279999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[477,"POWERLINKV5_20151103070403","2013-01-06T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.644399999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[478,"POWERLINKV5_20151103070403","2013-01-06T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.834110000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[479,"POWERLINKV5_20151103070403","2013-01-06T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.23932000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[480,"POWERLINKV5_20151103070403","2013-01-06T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.417349999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[481,"POWERLINKV5_20151103070403","2013-01-06T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.184959999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[482,"POWERLINKV5_20151103070403","2013-01-06T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.430689999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[483,"POWERLINKV5_20151103070403","2013-01-06T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-263.86809,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[484,"POWERLINKV5_20151103070403","2013-01-06T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.184959999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[485,"POWERLINKV5_20151103070403","2013-01-06T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.184959999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[486,"POWERLINKV5_20151103070403","2013-01-06T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.59496,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[487,"POWERLINKV5_20151103070403","2013-01-06T18:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.678930000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[488,"POWERLINKV5_20151103070403","2013-01-06T18:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.776739999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[489,"POWERLINKV5_20151103070403","2013-01-06T18:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.708399999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[490,"POWERLINKV5_20151103070403","2013-01-06T18:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.475340000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[491,"POWERLINKV5_20151103070403","2013-01-06T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.00224,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[492,"POWERLINKV5_20151103070403","2013-01-06T18:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.537889999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[493,"POWERLINKV5_20151103070403","2013-01-06T18:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.952359999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[494,"POWERLINKV5_20151103070403","2013-01-06T18:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.027050000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[495,"POWERLINKV5_20151103070403","2013-01-06T19:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-28.044879999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[496,"POWERLINKV5_20151103070403","2013-01-07T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.522880000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[497,"POWERLINKV5_20151103070403","2013-01-07T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-795.09933999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[498,"POWERLINKV5_20151103070403","2013-01-07T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-714.54633999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[499,"POWERLINKV5_20151103070403","2013-01-07T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-793.49599999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[500,"POWERLINKV5_20151103070403","2013-01-07T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-792.24593000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[501,"POWERLINKV5_20151103070403","2013-01-07T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.206150000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[502,"POWERLINKV5_20151103070403","2013-01-07T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-692.83678999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[503,"POWERLINKV5_20151103070403","2013-01-07T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-719.14968999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[504,"POWERLINKV5_20151103070403","2013-01-07T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-697.29175999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[505,"POWERLINKV5_20151103070403","2013-01-07T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.88219000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[506,"POWERLINKV5_20151103070403","2013-01-07T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.28768000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[507,"POWERLINKV5_20151103070403","2013-01-07T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.31017999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[508,"POWERLINKV5_20151103070403","2013-01-07T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.31160999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[509,"POWERLINKV5_20151103070403","2013-01-07T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-690.61194999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[510,"POWERLINKV5_20151103070403","2013-01-07T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-693.04927999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[511,"POWERLINKV5_20151103070403","2013-01-07T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.89847999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[512,"POWERLINKV5_20151103070403","2013-01-07T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-691.27464999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[513,"POWERLINKV5_20151103070403","2013-01-07T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-687.40558999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[514,"POWERLINKV5_20151103070403","2013-01-07T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-668.56134999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[515,"POWERLINKV5_20151103070403","2013-01-07T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-453.08150000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[516,"POWERLINKV5_20151103070403","2013-01-07T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-701.38511000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[517,"POWERLINKV5_20151103070403","2013-01-07T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-678.70106999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[518,"POWERLINKV5_20151103070403","2013-01-07T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-530.80120999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[519,"POWERLINKV5_20151103070403","2013-01-07T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-700.29904999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[520,"POWERLINKV5_20151103070403","2013-01-07T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-700.31717000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[521,"POWERLINKV5_20151103070403","2013-01-07T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-735.23871999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[522,"POWERLINKV5_20151103070403","2013-01-07T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-32.835979999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[523,"POWERLINKV5_20151103070403","2013-01-07T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.537699999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[524,"POWERLINKV5_20151103070403","2013-01-07T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.01187,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[525,"POWERLINKV5_20151103070403","2013-01-08T05:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.17141,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[526,"POWERLINKV5_20151103070403","2013-01-08T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.49657,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[527,"POWERLINKV5_20151103070403","2013-01-08T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.49657,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[528,"POWERLINKV5_20151103070403","2013-01-08T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.46917,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[529,"POWERLINKV5_20151103070403","2013-01-08T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.71963,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[530,"POWERLINKV5_20151103070403","2013-01-08T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-33.077590000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[531,"POWERLINKV5_20151103070403","2013-01-08T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-721.31626000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[532,"POWERLINKV5_20151103070403","2013-01-08T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.68174,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[533,"POWERLINKV5_20151103070403","2013-01-08T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-32.39819,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[534,"POWERLINKV5_20151103070403","2013-01-08T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-697.56326000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[535,"POWERLINKV5_20151103070403","2013-01-08T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.154409999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[536,"POWERLINKV5_20151103070403","2013-01-08T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-62.136800000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[537,"POWERLINKV5_20151103070403","2013-01-08T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.615310000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[538,"POWERLINKV5_20151103070403","2013-01-08T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-61.367629999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[539,"POWERLINKV5_20151103070403","2013-01-08T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-267.15494999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[540,"POWERLINKV5_20151103070403","2013-01-08T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-686.57789000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[541,"POWERLINKV5_20151103070403","2013-01-08T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-274.84203000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[542,"POWERLINKV5_20151103070403","2013-01-08T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.72174000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[543,"POWERLINKV5_20151103070403","2013-01-08T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.5794,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[544,"POWERLINKV5_20151103070403","2013-01-08T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-24.039560000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[545,"POWERLINKV5_20151103070403","2013-01-08T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-688.45333000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[546,"POWERLINKV5_20151103070403","2013-01-08T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-269.34944999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[547,"POWERLINKV5_20151103070403","2013-01-08T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-697.50343999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[548,"POWERLINKV5_20151103070403","2013-01-08T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.11985000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[549,"POWERLINKV5_20151103070403","2013-01-08T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.15633000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[550,"POWERLINKV5_20151103070403","2013-01-08T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-442.35613999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[551,"POWERLINKV5_20151103070403","2013-01-08T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.66498000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[552,"POWERLINKV5_20151103070403","2013-01-08T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.07166000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[553,"POWERLINKV5_20151103070403","2013-01-08T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.440709999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[554,"POWERLINKV5_20151103070403","2013-01-08T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.45736,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[555,"POWERLINKV5_20151103070403","2013-01-08T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.474159999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[556,"POWERLINKV5_20151103070403","2013-01-08T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.50071,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[557,"POWERLINKV5_20151103070403","2013-01-08T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-427.83774,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[558,"POWERLINKV5_20151103070403","2013-01-08T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-704.60923000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[559,"POWERLINKV5_20151103070403","2013-01-08T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-686.43902000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[560,"POWERLINKV5_20151103070403","2013-01-08T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-426.04154999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[561,"POWERLINKV5_20151103070403","2013-01-08T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-367.90260999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[562,"POWERLINKV5_20151103070403","2013-01-08T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-416.85073,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[563,"POWERLINKV5_20151103070403","2013-01-08T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-427.13983999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[564,"POWERLINKV5_20151103070403","2013-01-08T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-425.74178999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[565,"POWERLINKV5_20151103070403","2013-01-08T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-33.427880000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[566,"POWERLINKV5_20151103070403","2013-01-08T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-33.405839999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[567,"POWERLINKV5_20151103070403","2013-01-09T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.980589999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[568,"POWERLINKV5_20151103070403","2013-01-09T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.3787,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[569,"POWERLINKV5_20151103070403","2013-01-09T07:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.026059999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[570,"POWERLINKV5_20151103070403","2013-01-09T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.163650000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[571,"POWERLINKV5_20151103070403","2013-01-09T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.13387,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[572,"POWERLINKV5_20151103070403","2013-01-09T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.26143,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[573,"POWERLINKV5_20151103070403","2013-01-09T09:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.1110799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[574,"POWERLINKV5_20151103070403","2013-01-09T09:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.7021999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[575,"POWERLINKV5_20151103070403","2013-01-09T09:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.38687,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[576,"POWERLINKV5_20151103070403","2013-01-09T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.89111,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[577,"POWERLINKV5_20151103070403","2013-01-09T09:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.0588700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[578,"POWERLINKV5_20151103070403","2013-01-09T09:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.7411099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[579,"POWERLINKV5_20151103070403","2013-01-09T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.67965,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[580,"POWERLINKV5_20151103070403","2013-01-09T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.77337,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[581,"POWERLINKV5_20151103070403","2013-01-09T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.366160000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[582,"POWERLINKV5_20151103070403","2013-01-09T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.35971,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[583,"POWERLINKV5_20151103070403","2013-01-09T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.632989999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[584,"POWERLINKV5_20151103070403","2013-01-09T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-139.96905000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[585,"POWERLINKV5_20151103070403","2013-01-09T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.3073899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[586,"POWERLINKV5_20151103070403","2013-01-09T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-155.49671000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[587,"POWERLINKV5_20151103070403","2013-01-09T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-31.036580000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[588,"POWERLINKV5_20151103070403","2013-01-09T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.25056000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[589,"POWERLINKV5_20151103070403","2013-01-09T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1005.4655,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[590,"POWERLINKV5_20151103070403","2013-01-09T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-191.58391,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[591,"POWERLINKV5_20151103070403","2013-01-09T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1252.5056400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[592,"POWERLINKV5_20151103070403","2013-01-09T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-192.75665000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[593,"POWERLINKV5_20151103070403","2013-01-09T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-963.32079999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[594,"POWERLINKV5_20151103070403","2013-01-10T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.923590000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[595,"POWERLINKV5_20151103070403","2013-01-10T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.104950000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[596,"POWERLINKV5_20151103070403","2013-01-10T06:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.264119999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[597,"POWERLINKV5_20151103070403","2013-01-10T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.24067,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[598,"POWERLINKV5_20151103070403","2013-01-10T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-72.125010000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[599,"POWERLINKV5_20151103070403","2013-01-10T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11799.85493,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[600,"POWERLINKV5_20151103070403","2013-01-10T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.203519999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[601,"POWERLINKV5_20151103070403","2013-01-10T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-71.779690000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[602,"POWERLINKV5_20151103070403","2013-01-10T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.8203100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[603,"POWERLINKV5_20151103070403","2013-01-10T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-724.64272000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[604,"POWERLINKV5_20151103070403","2013-01-10T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-724.64092000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[605,"POWERLINKV5_20151103070403","2013-01-10T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.4695300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[606,"POWERLINKV5_20151103070403","2013-01-10T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-700.32038999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[607,"POWERLINKV5_20151103070403","2013-01-10T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-721.70227,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[608,"POWERLINKV5_20151103070403","2013-01-10T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-700.27764000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[609,"POWERLINKV5_20151103070403","2013-01-10T07:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.66983,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[610,"POWERLINKV5_20151103070403","2013-01-10T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-720.72594000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[611,"POWERLINKV5_20151103070403","2013-01-10T07:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.6913,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[612,"POWERLINKV5_20151103070403","2013-01-10T07:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.186120000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[613,"POWERLINKV5_20151103070403","2013-01-10T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.9837,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[614,"POWERLINKV5_20151103070403","2013-01-10T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.05453999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[615,"POWERLINKV5_20151103070403","2013-01-10T07:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1024.04675,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[616,"POWERLINKV5_20151103070403","2013-01-10T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-720.44743000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[617,"POWERLINKV5_20151103070403","2013-01-10T07:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.99522,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[618,"POWERLINKV5_20151103070403","2013-01-10T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-721.59888999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[619,"POWERLINKV5_20151103070403","2013-01-10T07:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.73897,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[620,"POWERLINKV5_20151103070403","2013-01-10T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-719.66602,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[621,"POWERLINKV5_20151103070403","2013-01-10T07:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1024.8477399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[622,"POWERLINKV5_20151103070403","2013-01-10T08:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.68346,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[623,"POWERLINKV5_20151103070403","2013-01-10T08:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.0927300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[624,"POWERLINKV5_20151103070403","2013-01-10T08:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.05476,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[625,"POWERLINKV5_20151103070403","2013-01-10T08:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.2900299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[626,"POWERLINKV5_20151103070403","2013-01-10T08:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.26659,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[627,"POWERLINKV5_20151103070403","2013-01-10T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.6839199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[628,"POWERLINKV5_20151103070403","2013-01-10T08:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1079.91284,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[629,"POWERLINKV5_20151103070403","2013-01-10T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.0021400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[630,"POWERLINKV5_20151103070403","2013-01-10T08:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1288.32214,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[631,"POWERLINKV5_20151103070403","2013-01-10T08:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-690.12783999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[632,"POWERLINKV5_20151103070403","2013-01-10T08:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.5514499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[633,"POWERLINKV5_20151103070403","2013-01-10T08:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-478.76808999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[634,"POWERLINKV5_20151103070403","2013-01-10T08:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1281.39384,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[635,"POWERLINKV5_20151103070403","2013-01-10T08:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-696.90836000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[636,"POWERLINKV5_20151103070403","2013-01-10T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1040.5458599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[637,"POWERLINKV5_20151103070403","2013-01-10T09:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-377.87468000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[638,"POWERLINKV5_20151103070403","2013-01-10T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-166.2886,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[639,"POWERLINKV5_20151103070403","2013-01-10T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-542.06151,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[640,"POWERLINKV5_20151103070403","2013-01-10T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-789.53743999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[641,"POWERLINKV5_20151103070403","2013-01-10T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.93124,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[642,"POWERLINKV5_20151103070403","2013-01-10T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-265.69224000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[643,"POWERLINKV5_20151103070403","2013-01-10T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.17309,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[644,"POWERLINKV5_20151103070403","2013-01-10T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.18494999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[645,"POWERLINKV5_20151103070403","2013-01-10T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.21669999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[646,"POWERLINKV5_20151103070403","2013-01-10T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-788.69530999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[647,"POWERLINKV5_20151103070403","2013-01-10T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-789.95138999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[648,"POWERLINKV5_20151103070403","2013-01-10T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-789.47163,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[649,"POWERLINKV5_20151103070403","2013-01-10T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.87094000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[650,"POWERLINKV5_20151103070403","2013-01-10T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-789.35963000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[651,"POWERLINKV5_20151103070403","2013-01-10T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.19284000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[652,"POWERLINKV5_20151103070403","2013-01-10T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-542.06151,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[653,"POWERLINKV5_20151103070403","2013-01-10T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-789.18906000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[654,"POWERLINKV5_20151103070403","2013-01-10T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-790.66940999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[655,"POWERLINKV5_20151103070403","2013-01-10T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-157.05044000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[656,"POWERLINKV5_20151103070403","2013-01-10T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-788.19574999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[657,"POWERLINKV5_20151103070403","2013-01-10T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-786.38816999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[658,"POWERLINKV5_20151103070403","2013-01-10T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.56874000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[659,"POWERLINKV5_20151103070403","2013-01-10T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.56874000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[660,"POWERLINKV5_20151103070403","2013-01-10T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-782.62699999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[661,"POWERLINKV5_20151103070403","2013-01-10T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-895.79254000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[662,"POWERLINKV5_20151103070403","2013-01-10T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-956.21010999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[663,"POWERLINKV5_20151103070403","2013-01-10T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-601.32186999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[664,"POWERLINKV5_20151103070403","2013-01-10T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.56883000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[665,"POWERLINKV5_20151103070403","2013-01-10T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.52058999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[666,"POWERLINKV5_20151103070403","2013-01-10T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.56883000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[667,"POWERLINKV5_20151103070403","2013-01-10T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-618.56883000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[668,"POWERLINKV5_20151103070403","2013-01-10T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-558.37721999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[669,"POWERLINKV5_20151103070403","2013-01-10T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-601.32186999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[670,"POWERLINKV5_20151103070403","2013-01-10T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-849.21911,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[671,"POWERLINKV5_20151103070403","2013-01-10T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-895.79254000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[672,"POWERLINKV5_20151103070403","2013-01-11T00:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-6539.7554600000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[673,"POWERLINKV5_20151103070403","2013-01-11T03:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.30472,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[674,"POWERLINKV5_20151103070403","2013-01-11T03:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.19533,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[675,"POWERLINKV5_20151103070403","2013-01-11T05:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.701279999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[676,"POWERLINKV5_20151103070403","2013-01-11T05:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.16751,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[677,"POWERLINKV5_20151103070403","2013-01-11T05:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.153239999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[678,"POWERLINKV5_20151103070403","2013-01-11T05:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.926409999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[679,"POWERLINKV5_20151103070403","2013-01-11T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.189769999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[680,"POWERLINKV5_20151103070403","2013-01-11T05:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.04158,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[681,"POWERLINKV5_20151103070403","2013-01-11T05:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.39902,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[682,"POWERLINKV5_20151103070403","2013-01-11T05:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.595469999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[683,"POWERLINKV5_20151103070403","2013-01-11T06:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-37.243859999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[684,"POWERLINKV5_20151103070403","2013-01-11T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.98063,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[685,"POWERLINKV5_20151103070403","2013-01-11T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.38427000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[686,"POWERLINKV5_20151103070403","2013-01-11T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.03846,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[687,"POWERLINKV5_20151103070403","2013-01-11T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13515.38616,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[688,"POWERLINKV5_20151103070403","2013-01-11T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13496.661550000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[689,"POWERLINKV5_20151103070403","2013-01-11T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.7129199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[690,"POWERLINKV5_20151103070403","2013-01-11T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-32.342019999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[691,"POWERLINKV5_20151103070403","2013-01-11T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-7071.2739099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[692,"POWERLINKV5_20151103070403","2013-01-11T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11634.689319999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[693,"POWERLINKV5_20151103070403","2013-01-11T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-7196.3946299999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[694,"POWERLINKV5_20151103070403","2013-01-11T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11634.689,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[695,"POWERLINKV5_20151103070403","2013-01-11T07:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11732.20779,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[696,"POWERLINKV5_20151103070403","2013-01-11T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.6283800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[697,"POWERLINKV5_20151103070403","2013-01-11T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.56069,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[698,"POWERLINKV5_20151103070403","2013-01-11T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.46741,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[699,"POWERLINKV5_20151103070403","2013-01-11T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2020.8170600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[700,"POWERLINKV5_20151103070403","2013-01-11T07:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.6491799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[701,"POWERLINKV5_20151103070403","2013-01-11T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.72505,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[702,"POWERLINKV5_20151103070403","2013-01-11T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2021.1175800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[703,"POWERLINKV5_20151103070403","2013-01-11T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11714.86879,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[704,"POWERLINKV5_20151103070403","2013-01-11T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.85167,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[705,"POWERLINKV5_20151103070403","2013-01-11T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.98982,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[706,"POWERLINKV5_20151103070403","2013-01-11T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.7521400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[707,"POWERLINKV5_20151103070403","2013-01-11T08:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8345300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[708,"POWERLINKV5_20151103070403","2013-01-11T08:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8341800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[709,"POWERLINKV5_20151103070403","2013-01-11T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83438,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[710,"POWERLINKV5_20151103070403","2013-01-11T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.93797000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[711,"POWERLINKV5_20151103070403","2013-01-11T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.8233,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[712,"POWERLINKV5_20151103070403","2013-01-11T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8984700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[713,"POWERLINKV5_20151103070403","2013-01-11T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8964800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[714,"POWERLINKV5_20151103070403","2013-01-11T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1214.8617200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[715,"POWERLINKV5_20151103070403","2013-01-11T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-455.17563000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[716,"POWERLINKV5_20151103070403","2013-01-11T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83449,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[717,"POWERLINKV5_20151103070403","2013-01-11T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83439,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[718,"POWERLINKV5_20151103070403","2013-01-11T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1645.0099299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[719,"POWERLINKV5_20151103070403","2013-01-11T09:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-17490.523809999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[720,"POWERLINKV5_20151103070403","2013-01-11T09:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-10823.01981,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[721,"POWERLINKV5_20151103070403","2013-01-11T09:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-10823.571819999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[722,"POWERLINKV5_20151103070403","2013-01-11T09:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1859.0434399999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[723,"POWERLINKV5_20151103070403","2013-01-11T09:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-37.898090000000003,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[724,"POWERLINKV5_20151103070403","2013-01-11T11:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-848.59082000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[725,"POWERLINKV5_20151103070403","2013-01-11T11:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-10.337730000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[726,"POWERLINKV5_20151103070403","2013-01-11T11:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1542.72559,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[727,"POWERLINKV5_20151103070403","2013-01-11T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1494.3975399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[728,"POWERLINKV5_20151103070403","2013-01-11T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1042.7126599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[729,"POWERLINKV5_20151103070403","2013-01-11T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1051.0789299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[730,"POWERLINKV5_20151103070403","2013-01-11T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-970.95178999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[731,"POWERLINKV5_20151103070403","2013-01-11T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-659.53589999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[732,"POWERLINKV5_20151103070403","2013-01-11T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.32376,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[733,"POWERLINKV5_20151103070403","2013-01-11T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.58747,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[734,"POWERLINKV5_20151103070403","2013-01-11T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.7660800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[735,"POWERLINKV5_20151103070403","2013-01-11T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1265.6885600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[736,"POWERLINKV5_20151103070403","2013-01-11T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.156410000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[737,"POWERLINKV5_20151103070403","2013-01-11T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9901,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[738,"POWERLINKV5_20151103070403","2013-01-11T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.72921,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[739,"POWERLINKV5_20151103070403","2013-01-11T14:45:00","Q>>NIL_MRTX5_MRTX4","Q-NIL","2012-04-03",1,-134.28715,"Out= Nil, avoid thermal O/L on remaining Middle Ridge 330/275 kV Tx #4, on trip of Middle Ridge 330/275 kV Tx #5, (or 9907 Millmerran to Middle Ridge 330kV line), DS RHS is swamped when Middle Ridge bus splitting scheme is triggered, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[740,"POWERLINKV5_20151103070403","2013-01-11T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1627.19244,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[741,"POWERLINKV5_20151103070403","2013-01-11T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.821750000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[742,"POWERLINKV5_20151103070403","2013-01-11T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.466839999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[743,"POWERLINKV5_20151103070403","2013-01-11T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9902099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[744,"POWERLINKV5_20151103070403","2013-01-11T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.7657999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[745,"POWERLINKV5_20151103070403","2013-01-11T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.99027,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[746,"POWERLINKV5_20151103070403","2013-01-11T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1266.15274,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[747,"POWERLINKV5_20151103070403","2013-01-11T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1248.9954,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[748,"POWERLINKV5_20151103070403","2013-01-11T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1247.77801,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[749,"POWERLINKV5_20151103070403","2013-01-11T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9901,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[750,"POWERLINKV5_20151103070403","2013-01-11T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.76593,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[751,"POWERLINKV5_20151103070403","2013-01-11T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1626.9736,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[752,"POWERLINKV5_20151103070403","2013-01-11T16:20:00","Q>>NIL_MRTX5_MRTX4","Q-NIL","2012-04-03",1,-100.81016,"Out= Nil, avoid thermal O/L on remaining Middle Ridge 330/275 kV Tx #4, on trip of Middle Ridge 330/275 kV Tx #5, (or 9907 Millmerran to Middle Ridge 330kV line), DS RHS is swamped when Middle Ridge bus splitting scheme is triggered, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[753,"POWERLINKV5_20151103070403","2013-01-11T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1565.9556700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[754,"POWERLINKV5_20151103070403","2013-01-11T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1623.6432,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[755,"POWERLINKV5_20151103070403","2013-01-11T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8342600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[756,"POWERLINKV5_20151103070403","2013-01-11T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8354099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[757,"POWERLINKV5_20151103070403","2013-01-11T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.76316,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[758,"POWERLINKV5_20151103070403","2013-01-11T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-976.90553999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[759,"POWERLINKV5_20151103070403","2013-01-11T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-979.06749000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[760,"POWERLINKV5_20151103070403","2013-01-11T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-30.753399999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[761,"POWERLINKV5_20151103070403","2013-01-11T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-977.91345000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[762,"POWERLINKV5_20151103070403","2013-01-11T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-987.27719999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[763,"POWERLINKV5_20151103070403","2013-01-11T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-991.92740000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[764,"POWERLINKV5_20151103070403","2013-01-11T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-986.26777000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[765,"POWERLINKV5_20151103070403","2013-01-11T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-27.092169999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[766,"POWERLINKV5_20151103070403","2013-01-11T23:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1216.58059,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[767,"POWERLINKV5_20151103070403","2013-01-11T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-65.869789999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[768,"POWERLINKV5_20151103070403","2013-01-11T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-22.44819,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[769,"POWERLINKV5_20151103070403","2013-01-11T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1214.5645400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[770,"POWERLINKV5_20151103070403","2013-01-11T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-23.037579999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[771,"POWERLINKV5_20151103070403","2013-01-12","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.757290000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[772,"POWERLINKV5_20151103070403","2013-01-12T00:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-226.71583999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[773,"POWERLINKV5_20151103070403","2013-01-12T00:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-12611.702219999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[774,"POWERLINKV5_20151103070403","2013-01-12T00:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-933.46186999999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[775,"POWERLINKV5_20151103070403","2013-01-12T00:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-225.81397999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[776,"POWERLINKV5_20151103070403","2013-01-12T00:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-223.72363999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[777,"POWERLINKV5_20151103070403","2013-01-12T00:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-226.63039000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[778,"POWERLINKV5_20151103070403","2013-01-12T00:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-39.558999999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[779,"POWERLINKV5_20151103070403","2013-01-12T00:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-51.858449999999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[780,"POWERLINKV5_20151103070403","2013-01-12T00:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-154.52502000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[781,"POWERLINKV5_20151103070403","2013-01-12T00:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-226.63817,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[782,"POWERLINKV5_20151103070403","2013-01-12T01:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-227.31521000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[783,"POWERLINKV5_20151103070403","2013-01-12T01:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-29.140499999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[784,"POWERLINKV5_20151103070403","2013-01-12T01:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-228.28879000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[785,"POWERLINKV5_20151103070403","2013-01-12T03:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.801769999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[786,"POWERLINKV5_20151103070403","2013-01-12T04:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.163329999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[787,"POWERLINKV5_20151103070403","2013-01-12T04:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13564.481879999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[788,"POWERLINKV5_20151103070403","2013-01-12T04:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1087.4201,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[789,"POWERLINKV5_20151103070403","2013-01-12T04:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.34475,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[790,"POWERLINKV5_20151103070403","2013-01-12T04:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.1008099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[791,"POWERLINKV5_20151103070403","2013-01-12T04:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-153.68271999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[792,"POWERLINKV5_20151103070403","2013-01-12T05:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.001720000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[793,"POWERLINKV5_20151103070403","2013-01-12T05:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.539289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[794,"POWERLINKV5_20151103070403","2013-01-12T05:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.0460599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[795,"POWERLINKV5_20151103070403","2013-01-12T05:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.456,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[796,"POWERLINKV5_20151103070403","2013-01-12T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.2530999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[797,"POWERLINKV5_20151103070403","2013-01-12T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.0730799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[798,"POWERLINKV5_20151103070403","2013-01-12T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1186.43613,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[799,"POWERLINKV5_20151103070403","2013-01-12T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11833.56609,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[800,"POWERLINKV5_20151103070403","2013-01-12T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12353.72582,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[801,"POWERLINKV5_20151103070403","2013-01-12T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12353.36131,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[802,"POWERLINKV5_20151103070403","2013-01-12T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11823.356449999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[803,"POWERLINKV5_20151103070403","2013-01-12T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.8607300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[804,"POWERLINKV5_20151103070403","2013-01-12T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.977060000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[805,"POWERLINKV5_20151103070403","2013-01-12T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.617139999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[806,"POWERLINKV5_20151103070403","2013-01-12T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-700.08448999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[807,"POWERLINKV5_20151103070403","2013-01-12T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-701.33175000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[808,"POWERLINKV5_20151103070403","2013-01-12T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-288.45492000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[809,"POWERLINKV5_20151103070403","2013-01-12T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-287.92196999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[810,"POWERLINKV5_20151103070403","2013-01-12T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1023.26159,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[811,"POWERLINKV5_20151103070403","2013-01-12T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1022.92599,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[812,"POWERLINKV5_20151103070403","2013-01-12T08:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.4697100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[813,"POWERLINKV5_20151103070403","2013-01-12T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1083.72325,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[814,"POWERLINKV5_20151103070403","2013-01-12T08:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1019.9686,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[815,"POWERLINKV5_20151103070403","2013-01-12T08:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1082.3472099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[816,"POWERLINKV5_20151103070403","2013-01-12T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1625.7513100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[817,"POWERLINKV5_20151103070403","2013-01-12T08:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.8479600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[818,"POWERLINKV5_20151103070403","2013-01-12T08:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1018.91569,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[819,"POWERLINKV5_20151103070403","2013-01-12T08:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.65858,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[820,"POWERLINKV5_20151103070403","2013-01-12T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.2165399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[821,"POWERLINKV5_20151103070403","2013-01-12T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.1245200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[822,"POWERLINKV5_20151103070403","2013-01-12T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2048.6405,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[823,"POWERLINKV5_20151103070403","2013-01-12T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2045.69913,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[824,"POWERLINKV5_20151103070403","2013-01-12T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.8904600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[825,"POWERLINKV5_20151103070403","2013-01-12T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.8469600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[826,"POWERLINKV5_20151103070403","2013-01-12T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2044.3199400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[827,"POWERLINKV5_20151103070403","2013-01-12T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2039.49188,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[828,"POWERLINKV5_20151103070403","2013-01-12T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11734.974459999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[829,"POWERLINKV5_20151103070403","2013-01-12T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11733.99475,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[830,"POWERLINKV5_20151103070403","2013-01-12T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.5030899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[831,"POWERLINKV5_20151103070403","2013-01-12T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1070.2139999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[832,"POWERLINKV5_20151103070403","2013-01-12T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2038.22306,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[833,"POWERLINKV5_20151103070403","2013-01-12T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1993.2772199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[834,"POWERLINKV5_20151103070403","2013-01-12T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1993.1210699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[835,"POWERLINKV5_20151103070403","2013-01-12T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.9455599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[836,"POWERLINKV5_20151103070403","2013-01-12T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-263.87673000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[837,"POWERLINKV5_20151103070403","2013-01-12T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1215.6717000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[838,"POWERLINKV5_20151103070403","2013-01-12T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.5027500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[839,"POWERLINKV5_20151103070403","2013-01-12T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83509,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[840,"POWERLINKV5_20151103070403","2013-01-12T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.50233,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[841,"POWERLINKV5_20151103070403","2013-01-12T10:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-8302.9895699999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[842,"POWERLINKV5_20151103070403","2013-01-12T10:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-242.63656,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[843,"POWERLINKV5_20151103070403","2013-01-12T10:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-877.78282000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[844,"POWERLINKV5_20151103070403","2013-01-12T10:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1417.6292000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[845,"POWERLINKV5_20151103070403","2013-01-12T10:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-2228.8754199999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[846,"POWERLINKV5_20151103070403","2013-01-12T10:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1915.2564600000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[847,"POWERLINKV5_20151103070403","2013-01-12T11:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1855.96821,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[848,"POWERLINKV5_20151103070403","2013-01-12T11:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1768.36337,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[849,"POWERLINKV5_20151103070403","2013-01-12T11:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1793.08322,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[850,"POWERLINKV5_20151103070403","2013-01-12T11:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-4515.1225299999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[851,"POWERLINKV5_20151103070403","2013-01-12T11:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-4515.6908299999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[852,"POWERLINKV5_20151103070403","2013-01-12T11:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-3599.73495,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[853,"POWERLINKV5_20151103070403","2013-01-12T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1398.7377799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[854,"POWERLINKV5_20151103070403","2013-01-12T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.6708799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[855,"POWERLINKV5_20151103070403","2013-01-12T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1398.7382500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[856,"POWERLINKV5_20151103070403","2013-01-12T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1716.03313,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[857,"POWERLINKV5_20151103070403","2013-01-12T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83573,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[858,"POWERLINKV5_20151103070403","2013-01-12T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8354999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[859,"POWERLINKV5_20151103070403","2013-01-12T12:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1750.53,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[860,"POWERLINKV5_20151103070403","2013-01-12T12:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1793.1917699999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[861,"POWERLINKV5_20151103070403","2013-01-12T12:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1793.8130000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[862,"POWERLINKV5_20151103070403","2013-01-12T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8350499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[863,"POWERLINKV5_20151103070403","2013-01-12T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83556,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[864,"POWERLINKV5_20151103070403","2013-01-12T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8351,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[865,"POWERLINKV5_20151103070403","2013-01-12T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1398.7376899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[866,"POWERLINKV5_20151103070403","2013-01-12T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-886.61006999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[867,"POWERLINKV5_20151103070403","2013-01-12T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1300.72768,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[868,"POWERLINKV5_20151103070403","2013-01-12T12:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-134.20289,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[869,"POWERLINKV5_20151103070403","2013-01-12T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-670.09433999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[870,"POWERLINKV5_20151103070403","2013-01-12T12:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-997.71370000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[871,"POWERLINKV5_20151103070403","2013-01-12T12:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-11799.402099999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[872,"POWERLINKV5_20151103070403","2013-01-12T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.741909999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[873,"POWERLINKV5_20151103070403","2013-01-12T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-375.42160000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[874,"POWERLINKV5_20151103070403","2013-01-12T13:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1401.2002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[875,"POWERLINKV5_20151103070403","2013-01-12T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-374.51157000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[876,"POWERLINKV5_20151103070403","2013-01-12T13:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1402.4469300000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[877,"POWERLINKV5_20151103070403","2013-01-12T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-101.24243,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[878,"POWERLINKV5_20151103070403","2013-01-12T13:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1704.08609,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[879,"POWERLINKV5_20151103070403","2013-01-12T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-97.976650000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[880,"POWERLINKV5_20151103070403","2013-01-12T13:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1707.44859,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[881,"POWERLINKV5_20151103070403","2013-01-12T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-98.328460000000007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[882,"POWERLINKV5_20151103070403","2013-01-12T13:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1707.0600400000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[883,"POWERLINKV5_20151103070403","2013-01-12T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1881.41885,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[884,"POWERLINKV5_20151103070403","2013-01-12T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1746.67498,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[885,"POWERLINKV5_20151103070403","2013-01-12T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83547,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[886,"POWERLINKV5_20151103070403","2013-01-12T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-7071.2752300000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[887,"POWERLINKV5_20151103070403","2013-01-12T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.5010400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[888,"POWERLINKV5_20151103070403","2013-01-12T13:50:00","Q>NIL_MRTA_A","Q-NIL","2012-09-06",1,-1181.41984,"Out = Nil, Oakey PS constrained to the emergency rating of 731 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[889,"POWERLINKV5_20151103070403","2013-01-12T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.1700900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[890,"POWERLINKV5_20151103070403","2013-01-12T13:55:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1084.5712599999999,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[891,"POWERLINKV5_20151103070403","2013-01-12T14:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1847.37454,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[892,"POWERLINKV5_20151103070403","2013-01-12T14:00:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1206.14804,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[893,"POWERLINKV5_20151103070403","2013-01-12T14:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-17962.54336,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[894,"POWERLINKV5_20151103070403","2013-01-12T14:05:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1068.9432899999999,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[895,"POWERLINKV5_20151103070403","2013-01-12T14:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-11845.325779999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[896,"POWERLINKV5_20151103070403","2013-01-12T14:10:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-2054.7050899999999,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[897,"POWERLINKV5_20151103070403","2013-01-12T14:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1797.9869900000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[898,"POWERLINKV5_20151103070403","2013-01-12T14:15:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1203.0109600000001,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[899,"POWERLINKV5_20151103070403","2013-01-12T14:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-934.77584999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[900,"POWERLINKV5_20151103070403","2013-01-12T14:20:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1131.46118,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[901,"POWERLINKV5_20151103070403","2013-01-12T14:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1848.4983299999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[902,"POWERLINKV5_20151103070403","2013-01-12T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.33682,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[903,"POWERLINKV5_20151103070403","2013-01-12T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1398.73504,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[904,"POWERLINKV5_20151103070403","2013-01-12T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1398.73551,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[905,"POWERLINKV5_20151103070403","2013-01-12T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8359800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[906,"POWERLINKV5_20151103070403","2013-01-12T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8357599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[907,"POWERLINKV5_20151103070403","2013-01-12T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-3261.1690199999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[908,"POWERLINKV5_20151103070403","2013-01-12T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.50297,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[909,"POWERLINKV5_20151103070403","2013-01-12T15:00:00","Q>NIL_MRTA_B","Q-NIL","2012-09-06",1,-1181.41885,"Out = Nil, Oakey PS constrained to the emergency rating of 732 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[910,"POWERLINKV5_20151103070403","2013-01-12T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-591.10179000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[911,"POWERLINKV5_20151103070403","2013-01-12T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8335400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[912,"POWERLINKV5_20151103070403","2013-01-12T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8338000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[913,"POWERLINKV5_20151103070403","2013-01-12T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8350800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[914,"POWERLINKV5_20151103070403","2013-01-12T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83518,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[915,"POWERLINKV5_20151103070403","2013-01-12T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-3261.32267,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[916,"POWERLINKV5_20151103070403","2013-01-12T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1623.6432,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[917,"POWERLINKV5_20151103070403","2013-01-12T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8337200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[918,"POWERLINKV5_20151103070403","2013-01-12T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83566,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[919,"POWERLINKV5_20151103070403","2013-01-12T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.49955,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[920,"POWERLINKV5_20151103070403","2013-01-12T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83518,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[921,"POWERLINKV5_20151103070403","2013-01-12T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-7618.5279899999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[922,"POWERLINKV5_20151103070403","2013-01-12T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.85184,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[923,"POWERLINKV5_20151103070403","2013-01-12T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1830.4166499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[924,"POWERLINKV5_20151103070403","2013-01-12T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8352500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[925,"POWERLINKV5_20151103070403","2013-01-12T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8352500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[926,"POWERLINKV5_20151103070403","2013-01-12T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8352500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[927,"POWERLINKV5_20151103070403","2013-01-12T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8353999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[928,"POWERLINKV5_20151103070403","2013-01-12T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83465,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[929,"POWERLINKV5_20151103070403","2013-01-12T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8353999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[930,"POWERLINKV5_20151103070403","2013-01-12T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8353999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[931,"POWERLINKV5_20151103070403","2013-01-12T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8352500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[932,"POWERLINKV5_20151103070403","2013-01-12T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8352500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[933,"POWERLINKV5_20151103070403","2013-01-12T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8353999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[934,"POWERLINKV5_20151103070403","2013-01-12T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1216.3922500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[935,"POWERLINKV5_20151103070403","2013-01-12T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1324.34536,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[936,"POWERLINKV5_20151103070403","2013-01-12T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8336899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[937,"POWERLINKV5_20151103070403","2013-01-12T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.3071600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[938,"POWERLINKV5_20151103070403","2013-01-12T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8353999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[939,"POWERLINKV5_20151103070403","2013-01-12T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1664.53153,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[940,"POWERLINKV5_20151103070403","2013-01-12T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-3261.2179900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[941,"POWERLINKV5_20151103070403","2013-01-12T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1627.19244,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[942,"POWERLINKV5_20151103070403","2013-01-12T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83385,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[943,"POWERLINKV5_20151103070403","2013-01-12T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8336200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[944,"POWERLINKV5_20151103070403","2013-01-12T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8343400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[945,"POWERLINKV5_20151103070403","2013-01-12T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-158.50869,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[946,"POWERLINKV5_20151103070403","2013-01-12T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1627.52512,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[947,"POWERLINKV5_20151103070403","2013-01-12T18:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.33042,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[948,"POWERLINKV5_20151103070403","2013-01-12T18:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1187.3186499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[949,"POWERLINKV5_20151103070403","2013-01-12T18:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8333600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[950,"POWERLINKV5_20151103070403","2013-01-12T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1645.0525700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[951,"POWERLINKV5_20151103070403","2013-01-12T22:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11426.67936,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[952,"POWERLINKV5_20151103070403","2013-01-12T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-8508.7850500000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[953,"POWERLINKV5_20151103070403","2013-01-12T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1065.4923699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[954,"POWERLINKV5_20151103070403","2013-01-12T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11464.62328,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[955,"POWERLINKV5_20151103070403","2013-01-12T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.31285,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[956,"POWERLINKV5_20151103070403","2013-01-12T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.4671599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[957,"POWERLINKV5_20151103070403","2013-01-12T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-520.94681000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[958,"POWERLINKV5_20151103070403","2013-01-12T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.8358000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[959,"POWERLINKV5_20151103070403","2013-01-12T23:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-516.30658000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[960,"POWERLINKV5_20151103070403","2013-01-12T23:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-517.47685000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[961,"POWERLINKV5_20151103070403","2013-01-12T23:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-516.54358999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[962,"POWERLINKV5_20151103070403","2013-01-12T23:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.2579699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[963,"POWERLINKV5_20151103070403","2013-01-12T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-91.055940000000007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[964,"POWERLINKV5_20151103070403","2013-01-12T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-157.68677,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[965,"POWERLINKV5_20151103070403","2013-01-12T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-91.055940000000007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[966,"POWERLINKV5_20151103070403","2013-01-12T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-456.46606000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[967,"POWERLINKV5_20151103070403","2013-01-13","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-462.75887999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[968,"POWERLINKV5_20151103070403","2013-01-13T00:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13468.592650000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[969,"POWERLINKV5_20151103070403","2013-01-13T00:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12105.20765,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[970,"POWERLINKV5_20151103070403","2013-01-13T00:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1214.1764800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[971,"POWERLINKV5_20151103070403","2013-01-13T00:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-460.13108,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[972,"POWERLINKV5_20151103070403","2013-01-13T00:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-161.40861000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[973,"POWERLINKV5_20151103070403","2013-01-13T00:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-161.39975999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[974,"POWERLINKV5_20151103070403","2013-01-13T00:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11733.894249999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[975,"POWERLINKV5_20151103070403","2013-01-13T00:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.622910000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[976,"POWERLINKV5_20151103070403","2013-01-13T00:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.76925,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[977,"POWERLINKV5_20151103070403","2013-01-13T00:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-77.680099999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[978,"POWERLINKV5_20151103070403","2013-01-13T00:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.969239999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[979,"POWERLINKV5_20151103070403","2013-01-13T01:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-83.835769999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[980,"POWERLINKV5_20151103070403","2013-01-13T01:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1199.87601,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[981,"POWERLINKV5_20151103070403","2013-01-13T01:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.11114,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[982,"POWERLINKV5_20151103070403","2013-01-13T01:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1081.62265,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[983,"POWERLINKV5_20151103070403","2013-01-13T01:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-123.26044,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[984,"POWERLINKV5_20151103070403","2013-01-13T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.820149999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[985,"POWERLINKV5_20151103070403","2013-01-13T02:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.243099999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[986,"POWERLINKV5_20151103070403","2013-01-13T02:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.32926,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[987,"POWERLINKV5_20151103070403","2013-01-13T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1185.09835,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[988,"POWERLINKV5_20151103070403","2013-01-13T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1187.00693,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[989,"POWERLINKV5_20151103070403","2013-01-13T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1186.50521,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[990,"POWERLINKV5_20151103070403","2013-01-13T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1187.4499699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[991,"POWERLINKV5_20151103070403","2013-01-13T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1189.3229799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[992,"POWERLINKV5_20151103070403","2013-01-13T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1187.39365,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[993,"POWERLINKV5_20151103070403","2013-01-13T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.6753900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[994,"POWERLINKV5_20151103070403","2013-01-13T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11795.355960000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[995,"POWERLINKV5_20151103070403","2013-01-13T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.7354499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[996,"POWERLINKV5_20151103070403","2013-01-13T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.2717299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[997,"POWERLINKV5_20151103070403","2013-01-13T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.750480000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[998,"POWERLINKV5_20151103070403","2013-01-13T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.536290000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[999,"POWERLINKV5_20151103070403","2013-01-13T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.109690000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1000,"POWERLINKV5_20151103070403","2013-01-13T07:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-286.80540000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1001,"POWERLINKV5_20151103070403","2013-01-13T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-431.90145999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1002,"POWERLINKV5_20151103070403","2013-01-13T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1028.87202,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1003,"POWERLINKV5_20151103070403","2013-01-13T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1026.74956,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1004,"POWERLINKV5_20151103070403","2013-01-13T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1026.67118,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1005,"POWERLINKV5_20151103070403","2013-01-13T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1025.76305,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1006,"POWERLINKV5_20151103070403","2013-01-13T08:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-909.85362999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1007,"POWERLINKV5_20151103070403","2013-01-13T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-909.97044000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1008,"POWERLINKV5_20151103070403","2013-01-13T08:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11815.294550000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1009,"POWERLINKV5_20151103070403","2013-01-13T08:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1139.8605700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1010,"POWERLINKV5_20151103070403","2013-01-13T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1021.1345,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1011,"POWERLINKV5_20151103070403","2013-01-13T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.250309999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1012,"POWERLINKV5_20151103070403","2013-01-13T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.218730000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1013,"POWERLINKV5_20151103070403","2013-01-13T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1017.61222,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1014,"POWERLINKV5_20151103070403","2013-01-13T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.4782600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1015,"POWERLINKV5_20151103070403","2013-01-13T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.4383399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1016,"POWERLINKV5_20151103070403","2013-01-13T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1170.3139799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1017,"POWERLINKV5_20151103070403","2013-01-13T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1011.01937,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1018,"POWERLINKV5_20151103070403","2013-01-13T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.30807,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1019,"POWERLINKV5_20151103070403","2013-01-13T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.8971300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1020,"POWERLINKV5_20151103070403","2013-01-13T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.06305,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1021,"POWERLINKV5_20151103070403","2013-01-13T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.4782600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1022,"POWERLINKV5_20151103070403","2013-01-13T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1614.1366499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1023,"POWERLINKV5_20151103070403","2013-01-13T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11729.642809999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1024,"POWERLINKV5_20151103070403","2013-01-13T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83574,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1025,"POWERLINKV5_20151103070403","2013-01-13T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.30708,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1026,"POWERLINKV5_20151103070403","2013-01-13T10:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-886.20324000000005,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1027,"POWERLINKV5_20151103070403","2013-01-13T10:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1794.62941,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1028,"POWERLINKV5_20151103070403","2013-01-13T10:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1856.10465,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1029,"POWERLINKV5_20151103070403","2013-01-13T10:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1798.89301,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1030,"POWERLINKV5_20151103070403","2013-01-13T10:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1795.00172,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1031,"POWERLINKV5_20151103070403","2013-01-13T10:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1715.00992,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1032,"POWERLINKV5_20151103070403","2013-01-13T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1138.8820499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1033,"POWERLINKV5_20151103070403","2013-01-13T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9900600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1034,"POWERLINKV5_20151103070403","2013-01-13T11:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1801.4405200000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1035,"POWERLINKV5_20151103070403","2013-01-13T11:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1800.4023500000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1036,"POWERLINKV5_20151103070403","2013-01-13T11:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1801.1406400000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1037,"POWERLINKV5_20151103070403","2013-01-13T11:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1799.5105100000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1038,"POWERLINKV5_20151103070403","2013-01-13T11:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1799.5155,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1039,"POWERLINKV5_20151103070403","2013-01-13T11:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1799.3108400000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1040,"POWERLINKV5_20151103070403","2013-01-13T11:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1798.7524599999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1041,"POWERLINKV5_20151103070403","2013-01-13T11:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-528.53481999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1042,"POWERLINKV5_20151103070403","2013-01-13T11:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-2282.4333299999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1043,"POWERLINKV5_20151103070403","2013-01-13T11:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1793.7760800000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1044,"POWERLINKV5_20151103070403","2013-01-13T11:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-52.584690000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1045,"POWERLINKV5_20151103070403","2013-01-13T12:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1793.55988,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1046,"POWERLINKV5_20151103070403","2013-01-13T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2537.1541499999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1047,"POWERLINKV5_20151103070403","2013-01-13T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.75299,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1048,"POWERLINKV5_20151103070403","2013-01-13T12:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1850.9399100000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1049,"POWERLINKV5_20151103070403","2013-01-13T12:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1796.9195500000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1050,"POWERLINKV5_20151103070403","2013-01-13T12:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1795.5213000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1051,"POWERLINKV5_20151103070403","2013-01-13T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.0483899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1052,"POWERLINKV5_20151103070403","2013-01-13T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-359.93171999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1053,"POWERLINKV5_20151103070403","2013-01-13T12:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1418.3761300000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1054,"POWERLINKV5_20151103070403","2013-01-13T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-987.41724999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1055,"POWERLINKV5_20151103070403","2013-01-13T12:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-725.66800999999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1056,"POWERLINKV5_20151103070403","2013-01-13T13:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1857.7438400000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1057,"POWERLINKV5_20151103070403","2013-01-13T13:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1853.6252199999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1058,"POWERLINKV5_20151103070403","2013-01-13T13:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-172.55261999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1059,"POWERLINKV5_20151103070403","2013-01-13T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83413,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1060,"POWERLINKV5_20151103070403","2013-01-13T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.9495099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1061,"POWERLINKV5_20151103070403","2013-01-13T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.94894,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1062,"POWERLINKV5_20151103070403","2013-01-13T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83628,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1063,"POWERLINKV5_20151103070403","2013-01-13T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-487.28798,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1064,"POWERLINKV5_20151103070403","2013-01-13T13:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1277.7012299999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1065,"POWERLINKV5_20151103070403","2013-01-13T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-362.43763000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1066,"POWERLINKV5_20151103070403","2013-01-13T13:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1414.54026,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1067,"POWERLINKV5_20151103070403","2013-01-13T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83473,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1068,"POWERLINKV5_20151103070403","2013-01-13T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83473,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1069,"POWERLINKV5_20151103070403","2013-01-13T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.9484500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1070,"POWERLINKV5_20151103070403","2013-01-13T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83349,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1071,"POWERLINKV5_20151103070403","2013-01-13T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83349,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1072,"POWERLINKV5_20151103070403","2013-01-13T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.3799899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1073,"POWERLINKV5_20151103070403","2013-01-13T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8337200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1074,"POWERLINKV5_20151103070403","2013-01-13T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8337200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1075,"POWERLINKV5_20151103070403","2013-01-13T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8339100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1076,"POWERLINKV5_20151103070403","2013-01-13T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.9487999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1077,"POWERLINKV5_20151103070403","2013-01-13T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1627.19244,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1078,"POWERLINKV5_20151103070403","2013-01-13T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1627.19235,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1079,"POWERLINKV5_20151103070403","2013-01-13T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.9487300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1080,"POWERLINKV5_20151103070403","2013-01-13T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8334400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1081,"POWERLINKV5_20151103070403","2013-01-13T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-457.64693,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1082,"POWERLINKV5_20151103070403","2013-01-13T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83356,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1083,"POWERLINKV5_20151103070403","2013-01-13T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11734.39572,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1084,"POWERLINKV5_20151103070403","2013-01-13T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11729.275960000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1085,"POWERLINKV5_20151103070403","2013-01-13T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11714.387409999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1086,"POWERLINKV5_20151103070403","2013-01-13T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1007.12226,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1087,"POWERLINKV5_20151103070403","2013-01-13T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-227.83293,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1088,"POWERLINKV5_20151103070403","2013-01-13T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.73582,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1089,"POWERLINKV5_20151103070403","2013-01-13T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.297170000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1090,"POWERLINKV5_20151103070403","2013-01-13T23:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-248.89009999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1091,"POWERLINKV5_20151103070403","2013-01-13T23:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1321.5019299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1092,"POWERLINKV5_20151103070403","2013-01-13T23:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1443.37185,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1093,"POWERLINKV5_20151103070403","2013-01-13T23:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.5292999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1094,"POWERLINKV5_20151103070403","2013-01-13T23:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-32.927370000000003,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1095,"POWERLINKV5_20151103070403","2013-01-13T23:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-31.162199999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1096,"POWERLINKV5_20151103070403","2013-01-14T04:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-78.910129999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1097,"POWERLINKV5_20151103070403","2013-01-14T04:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.021540000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1098,"POWERLINKV5_20151103070403","2013-01-14T04:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-24.947649999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1099,"POWERLINKV5_20151103070403","2013-01-14T04:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.821630000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1100,"POWERLINKV5_20151103070403","2013-01-14T04:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11797.759179999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1101,"POWERLINKV5_20151103070403","2013-01-14T05:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-86.446460000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1102,"POWERLINKV5_20151103070403","2013-01-14T05:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.601839999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1103,"POWERLINKV5_20151103070403","2013-01-14T05:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.5555099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1104,"POWERLINKV5_20151103070403","2013-01-14T05:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1927.99695,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1105,"POWERLINKV5_20151103070403","2013-01-14T05:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.224550000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1106,"POWERLINKV5_20151103070403","2013-01-14T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1086.3989099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1107,"POWERLINKV5_20151103070403","2013-01-14T05:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.3547799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1108,"POWERLINKV5_20151103070403","2013-01-14T05:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1188.71756,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1109,"POWERLINKV5_20151103070403","2013-01-14T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1199.9572599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1110,"POWERLINKV5_20151103070403","2013-01-14T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.8491300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1111,"POWERLINKV5_20151103070403","2013-01-14T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11763.92683,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1112,"POWERLINKV5_20151103070403","2013-01-14T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.90894,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1113,"POWERLINKV5_20151103070403","2013-01-14T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-7618.4968500000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1114,"POWERLINKV5_20151103070403","2013-01-14T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.7148099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1115,"POWERLINKV5_20151103070403","2013-01-14T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.93878,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1116,"POWERLINKV5_20151103070403","2013-01-14T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.95011,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1117,"POWERLINKV5_20151103070403","2013-01-14T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.0763099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1118,"POWERLINKV5_20151103070403","2013-01-14T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.3718100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1119,"POWERLINKV5_20151103070403","2013-01-14T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14466.97003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1120,"POWERLINKV5_20151103070403","2013-01-14T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-146660.5638,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1121,"POWERLINKV5_20151103070403","2013-01-14T07:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-899.42112999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1122,"POWERLINKV5_20151103070403","2013-01-14T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14695.79536,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1123,"POWERLINKV5_20151103070403","2013-01-14T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-999.99728000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1124,"POWERLINKV5_20151103070403","2013-01-14T07:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.99028,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1125,"POWERLINKV5_20151103070403","2013-01-14T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-286.0564,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1126,"POWERLINKV5_20151103070403","2013-01-14T08:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-11.780200000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1127,"POWERLINKV5_20151103070403","2013-01-14T08:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-276.01,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1128,"POWERLINKV5_20151103070403","2013-01-14T08:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1016.25958,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1129,"POWERLINKV5_20151103070403","2013-01-14T08:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.28126,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1130,"POWERLINKV5_20151103070403","2013-01-14T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-215.33583999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1131,"POWERLINKV5_20151103070403","2013-01-14T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.056819999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1132,"POWERLINKV5_20151103070403","2013-01-14T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-840.93240000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1133,"POWERLINKV5_20151103070403","2013-01-14T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-215.6798,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1134,"POWERLINKV5_20151103070403","2013-01-14T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-215.47551999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1135,"POWERLINKV5_20151103070403","2013-01-14T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-840.93240000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1136,"POWERLINKV5_20151103070403","2013-01-14T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-622.33959000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1137,"POWERLINKV5_20151103070403","2013-01-14T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-840.93240000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1138,"POWERLINKV5_20151103070403","2013-01-14T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-892.17354999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1139,"POWERLINKV5_20151103070403","2013-01-14T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.0942500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1140,"POWERLINKV5_20151103070403","2013-01-14T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9891500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1141,"POWERLINKV5_20151103070403","2013-01-14T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8337300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1142,"POWERLINKV5_20151103070403","2013-01-14T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-6522.7934699999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1143,"POWERLINKV5_20151103070403","2013-01-14T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11656.03729,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1144,"POWERLINKV5_20151103070403","2013-01-14T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11656.03729,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1145,"POWERLINKV5_20151103070403","2013-01-14T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11655.592979999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1146,"POWERLINKV5_20151103070403","2013-01-14T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2037.02647,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1147,"POWERLINKV5_20151103070403","2013-01-14T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.83536,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1148,"POWERLINKV5_20151103070403","2013-01-14T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.8189199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1149,"POWERLINKV5_20151103070403","2013-01-14T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-63.383209999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1150,"POWERLINKV5_20151103070403","2013-01-14T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-739.57447000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1151,"POWERLINKV5_20151103070403","2013-01-14T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1253.3195000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1152,"POWERLINKV5_20151103070403","2013-01-14T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-892.42354,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1153,"POWERLINKV5_20151103070403","2013-01-14T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1253.0691200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1154,"POWERLINKV5_20151103070403","2013-01-14T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.88444,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1155,"POWERLINKV5_20151103070403","2013-01-14T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1068.7591199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1156,"POWERLINKV5_20151103070403","2013-01-14T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1587.6409900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1157,"POWERLINKV5_20151103070403","2013-01-14T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1587.6409900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1158,"POWERLINKV5_20151103070403","2013-01-14T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1021.53506,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1159,"POWERLINKV5_20151103070403","2013-01-14T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-436.07449000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1160,"POWERLINKV5_20151103070403","2013-01-14T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-586.75131999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1161,"POWERLINKV5_20151103070403","2013-01-14T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-831.37982999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1162,"POWERLINKV5_20151103070403","2013-01-14T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-497.71197000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1163,"POWERLINKV5_20151103070403","2013-01-14T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-436.03291000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1164,"POWERLINKV5_20151103070403","2013-01-14T12:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-483.68347,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1165,"POWERLINKV5_20151103070403","2013-01-14T12:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-582.11850000000004,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1166,"POWERLINKV5_20151103070403","2013-01-14T12:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-600.28062999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1167,"POWERLINKV5_20151103070403","2013-01-14T12:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-783.38264000000004,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1168,"POWERLINKV5_20151103070403","2013-01-14T12:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-780.47406000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1169,"POWERLINKV5_20151103070403","2013-01-14T12:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-890.23947999999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1170,"POWERLINKV5_20151103070403","2013-01-14T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-895.51140999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1171,"POWERLINKV5_20151103070403","2013-01-14T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.9700499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1172,"POWERLINKV5_20151103070403","2013-01-14T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.8164099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1173,"POWERLINKV5_20151103070403","2013-01-14T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2041.4164699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1174,"POWERLINKV5_20151103070403","2013-01-14T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.2715900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1175,"POWERLINKV5_20151103070403","2013-01-14T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.1980799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1176,"POWERLINKV5_20151103070403","2013-01-14T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-77.296660000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1177,"POWERLINKV5_20151103070403","2013-01-14T13:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1730.2770599999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1178,"POWERLINKV5_20151103070403","2013-01-14T13:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1841.2832100000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1179,"POWERLINKV5_20151103070403","2013-01-14T13:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1803.4390699999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1180,"POWERLINKV5_20151103070403","2013-01-14T13:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1839.9794099999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1181,"POWERLINKV5_20151103070403","2013-01-14T13:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1803.4268400000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1182,"POWERLINKV5_20151103070403","2013-01-14T13:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1803.4689699999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1183,"POWERLINKV5_20151103070403","2013-01-14T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2047.7118599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1184,"POWERLINKV5_20151103070403","2013-01-14T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2045.3343,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1185,"POWERLINKV5_20151103070403","2013-01-14T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2044.18138,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1186,"POWERLINKV5_20151103070403","2013-01-14T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2043.0176300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1187,"POWERLINKV5_20151103070403","2013-01-14T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1789.29007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1188,"POWERLINKV5_20151103070403","2013-01-14T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.98884,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1189,"POWERLINKV5_20151103070403","2013-01-14T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.9318900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1190,"POWERLINKV5_20151103070403","2013-01-14T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.8626200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1191,"POWERLINKV5_20151103070403","2013-01-14T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.0177000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1192,"POWERLINKV5_20151103070403","2013-01-14T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.9062100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1193,"POWERLINKV5_20151103070403","2013-01-14T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.82716,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1194,"POWERLINKV5_20151103070403","2013-01-14T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-897.64751000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1195,"POWERLINKV5_20151103070403","2013-01-14T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.9438299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1196,"POWERLINKV5_20151103070403","2013-01-14T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.0109399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1197,"POWERLINKV5_20151103070403","2013-01-14T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1076.33341,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1198,"POWERLINKV5_20151103070403","2013-01-14T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.9652900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1199,"POWERLINKV5_20151103070403","2013-01-14T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.9663800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1200,"POWERLINKV5_20151103070403","2013-01-14T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.94057,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1201,"POWERLINKV5_20151103070403","2013-01-14T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.4575400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1202,"POWERLINKV5_20151103070403","2013-01-14T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-897.42190000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1203,"POWERLINKV5_20151103070403","2013-01-14T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-897.45816000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1204,"POWERLINKV5_20151103070403","2013-01-14T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-898.42810999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1205,"POWERLINKV5_20151103070403","2013-01-14T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-896.67819999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1206,"POWERLINKV5_20151103070403","2013-01-14T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-269.45112999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1207,"POWERLINKV5_20151103070403","2013-01-14T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-895.56604000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1208,"POWERLINKV5_20151103070403","2013-01-14T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-897.57788000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1209,"POWERLINKV5_20151103070403","2013-01-14T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-26.04654,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1210,"POWERLINKV5_20151103070403","2013-01-14T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-896.88459,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1211,"POWERLINKV5_20151103070403","2013-01-14T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1074.5895599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1212,"POWERLINKV5_20151103070403","2013-01-14T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-518.86720000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1213,"POWERLINKV5_20151103070403","2013-01-14T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-518.86082999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1214,"POWERLINKV5_20151103070403","2013-01-14T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-518.16813000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1215,"POWERLINKV5_20151103070403","2013-01-14T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.0235700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1216,"POWERLINKV5_20151103070403","2013-01-14T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-519.01864999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1217,"POWERLINKV5_20151103070403","2013-01-14T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-519.72148000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1218,"POWERLINKV5_20151103070403","2013-01-14T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-461.15778,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1219,"POWERLINKV5_20151103070403","2013-01-14T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.947890000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1220,"POWERLINKV5_20151103070403","2013-01-14T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-461.69558000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1221,"POWERLINKV5_20151103070403","2013-01-14T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-521.55444999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1222,"POWERLINKV5_20151103070403","2013-01-14T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1076.6793299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1223,"POWERLINKV5_20151103070403","2013-01-14T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-523.07303999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1224,"POWERLINKV5_20151103070403","2013-01-14T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-522.92827999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1225,"POWERLINKV5_20151103070403","2013-01-14T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1078.58177,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1226,"POWERLINKV5_20151103070403","2013-01-14T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1078.4381599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1227,"POWERLINKV5_20151103070403","2013-01-14T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-523.68520000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1228,"POWERLINKV5_20151103070403","2013-01-14T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.65601000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1229,"POWERLINKV5_20151103070403","2013-01-14T18:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-246.04952,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1230,"POWERLINKV5_20151103070403","2013-01-14T18:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-246.49528000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1231,"POWERLINKV5_20151103070403","2013-01-14T18:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-245.55457999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1232,"POWERLINKV5_20151103070403","2013-01-14T18:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-244.58277000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1233,"POWERLINKV5_20151103070403","2013-01-14T21:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.201549999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1234,"POWERLINKV5_20151103070403","2013-01-14T21:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.693519999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1235,"POWERLINKV5_20151103070403","2013-01-14T21:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.864890000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1236,"POWERLINKV5_20151103070403","2013-01-14T21:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-50.429560000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1237,"POWERLINKV5_20151103070403","2013-01-14T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.35637999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1238,"POWERLINKV5_20151103070403","2013-01-14T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.5944099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1239,"POWERLINKV5_20151103070403","2013-01-14T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-9140.6185299999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1240,"POWERLINKV5_20151103070403","2013-01-14T23:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.0404799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1241,"POWERLINKV5_20151103070403","2013-01-14T23:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11825.87362,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1242,"POWERLINKV5_20151103070403","2013-01-14T23:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2254.69173,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1243,"POWERLINKV5_20151103070403","2013-01-14T23:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1193.79945,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1244,"POWERLINKV5_20151103070403","2013-01-14T23:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.572430000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1245,"POWERLINKV5_20151103070403","2013-01-15T01:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.29448,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1246,"POWERLINKV5_20151103070403","2013-01-15T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.3392,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1247,"POWERLINKV5_20151103070403","2013-01-15T05:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.81565,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1248,"POWERLINKV5_20151103070403","2013-01-15T05:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-448.88968999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1249,"POWERLINKV5_20151103070403","2013-01-15T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-701.34014999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1250,"POWERLINKV5_20151103070403","2013-01-15T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.68027999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1251,"POWERLINKV5_20151103070403","2013-01-15T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-702.44470000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1252,"POWERLINKV5_20151103070403","2013-01-15T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-446.99250000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1253,"POWERLINKV5_20151103070403","2013-01-15T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-445.77447000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1254,"POWERLINKV5_20151103070403","2013-01-15T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-702.44199000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1255,"POWERLINKV5_20151103070403","2013-01-15T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-702.75477999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1256,"POWERLINKV5_20151103070403","2013-01-15T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-724.98310000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1257,"POWERLINKV5_20151103070403","2013-01-15T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1187.7642499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1258,"POWERLINKV5_20151103070403","2013-01-15T07:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.29331999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1259,"POWERLINKV5_20151103070403","2013-01-15T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.80914999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1260,"POWERLINKV5_20151103070403","2013-01-15T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-450.81900999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1261,"POWERLINKV5_20151103070403","2013-01-15T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-59.06514,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1262,"POWERLINKV5_20151103070403","2013-01-15T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.813330000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1263,"POWERLINKV5_20151103070403","2013-01-15T13:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-381.15231,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1264,"POWERLINKV5_20151103070403","2013-01-15T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-289.95123000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1265,"POWERLINKV5_20151103070403","2013-01-15T13:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-128.40440000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1266,"POWERLINKV5_20151103070403","2013-01-15T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-280.90660000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1267,"POWERLINKV5_20151103070403","2013-01-15T13:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-135.74553,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1268,"POWERLINKV5_20151103070403","2013-01-15T13:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-380.29217999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1269,"POWERLINKV5_20151103070403","2013-01-15T13:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-381.11291999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1270,"POWERLINKV5_20151103070403","2013-01-15T13:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-381.12973,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1271,"POWERLINKV5_20151103070403","2013-01-15T13:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-77.859960000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1272,"POWERLINKV5_20151103070403","2013-01-15T13:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-37.531570000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1273,"POWERLINKV5_20151103070403","2013-01-16T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.850159999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1274,"POWERLINKV5_20151103070403","2013-01-16T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.099360000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1275,"POWERLINKV5_20151103070403","2013-01-16T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.53123000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1276,"POWERLINKV5_20151103070403","2013-01-16T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11737.19687,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1277,"POWERLINKV5_20151103070403","2013-01-16T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.39636000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1278,"POWERLINKV5_20151103070403","2013-01-16T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-261.37589000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1279,"POWERLINKV5_20151103070403","2013-01-16T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.1229000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1280,"POWERLINKV5_20151103070403","2013-01-16T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-272.16867000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1281,"POWERLINKV5_20151103070403","2013-01-16T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1018.12136,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1282,"POWERLINKV5_20151103070403","2013-01-16T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1020.28588,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1283,"POWERLINKV5_20151103070403","2013-01-16T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.6127300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1284,"POWERLINKV5_20151103070403","2013-01-16T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1018.12137,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1285,"POWERLINKV5_20151103070403","2013-01-16T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1199.2439899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1286,"POWERLINKV5_20151103070403","2013-01-16T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.36788,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1287,"POWERLINKV5_20151103070403","2013-01-16T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.3849499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1288,"POWERLINKV5_20151103070403","2013-01-16T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.0776900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1289,"POWERLINKV5_20151103070403","2013-01-16T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2048.9988800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1290,"POWERLINKV5_20151103070403","2013-01-16T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-261.02222999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1291,"POWERLINKV5_20151103070403","2013-01-16T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-63.436369999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1292,"POWERLINKV5_20151103070403","2013-01-16T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1010.18414,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1293,"POWERLINKV5_20151103070403","2013-01-16T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1008.39757,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1294,"POWERLINKV5_20151103070403","2013-01-16T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-334.93810999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1295,"POWERLINKV5_20151103070403","2013-01-16T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-436.38891000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1296,"POWERLINKV5_20151103070403","2013-01-16T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.22092,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1297,"POWERLINKV5_20151103070403","2013-01-16T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-65.88946,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1298,"POWERLINKV5_20151103070403","2013-01-16T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.08195000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1299,"POWERLINKV5_20151103070403","2013-01-16T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-257.33147000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1300,"POWERLINKV5_20151103070403","2013-01-16T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.78332,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1301,"POWERLINKV5_20151103070403","2013-01-16T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-256.16233999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1302,"POWERLINKV5_20151103070403","2013-01-16T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.7085199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1303,"POWERLINKV5_20151103070403","2013-01-16T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.04304,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1304,"POWERLINKV5_20151103070403","2013-01-16T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.76926,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1305,"POWERLINKV5_20151103070403","2013-01-16T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11749.48443,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1306,"POWERLINKV5_20151103070403","2013-01-16T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1616.6197400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1307,"POWERLINKV5_20151103070403","2013-01-16T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1612.6469300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1308,"POWERLINKV5_20151103070403","2013-01-16T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1613.038,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1309,"POWERLINKV5_20151103070403","2013-01-16T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1071.94579,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1310,"POWERLINKV5_20151103070403","2013-01-16T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.7658699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1311,"POWERLINKV5_20151103070403","2013-01-16T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1074.9462000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1312,"POWERLINKV5_20151103070403","2013-01-16T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.3314600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1313,"POWERLINKV5_20151103070403","2013-01-16T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1616.7303400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1314,"POWERLINKV5_20151103070403","2013-01-16T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1614.73074,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1315,"POWERLINKV5_20151103070403","2013-01-16T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.2895900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1316,"POWERLINKV5_20151103070403","2013-01-16T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-364.35658000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1317,"POWERLINKV5_20151103070403","2013-01-16T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.1680200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1318,"POWERLINKV5_20151103070403","2013-01-16T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1075.1611499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1319,"POWERLINKV5_20151103070403","2013-01-16T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.3448599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1320,"POWERLINKV5_20151103070403","2013-01-16T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.1827800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1321,"POWERLINKV5_20151103070403","2013-01-16T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1074.78639,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1322,"POWERLINKV5_20151103070403","2013-01-16T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1076.65705,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1323,"POWERLINKV5_20151103070403","2013-01-16T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.75629,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1324,"POWERLINKV5_20151103070403","2013-01-16T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-438.95697000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1325,"POWERLINKV5_20151103070403","2013-01-16T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-439.60795000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1326,"POWERLINKV5_20151103070403","2013-01-16T18:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-439.78672,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1327,"POWERLINKV5_20151103070403","2013-01-16T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-438.46827999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1328,"POWERLINKV5_20151103070403","2013-01-16T20:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.14315999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1329,"POWERLINKV5_20151103070403","2013-01-16T20:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.078670000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1330,"POWERLINKV5_20151103070403","2013-01-16T20:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.01321999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1331,"POWERLINKV5_20151103070403","2013-01-16T20:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.17615999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1332,"POWERLINKV5_20151103070403","2013-01-16T20:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-257.58985000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1333,"POWERLINKV5_20151103070403","2013-01-16T20:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-257.01337999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1334,"POWERLINKV5_20151103070403","2013-01-16T20:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.16581000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1335,"POWERLINKV5_20151103070403","2013-01-16T20:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.14103999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1336,"POWERLINKV5_20151103070403","2013-01-16T22:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.89843,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1337,"POWERLINKV5_20151103070403","2013-01-16T22:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-307.06547999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1338,"POWERLINKV5_20151103070403","2013-01-16T22:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.85877,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1339,"POWERLINKV5_20151103070403","2013-01-16T22:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-308.91392000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1340,"POWERLINKV5_20151103070403","2013-01-16T22:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.06878,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1341,"POWERLINKV5_20151103070403","2013-01-16T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13544.112999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1342,"POWERLINKV5_20151103070403","2013-01-16T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13563.6451,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1343,"POWERLINKV5_20151103070403","2013-01-16T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-311.15165999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1344,"POWERLINKV5_20151103070403","2013-01-16T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-309.03287,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1345,"POWERLINKV5_20151103070403","2013-01-16T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.765009999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1346,"POWERLINKV5_20151103070403","2013-01-16T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.750480000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1347,"POWERLINKV5_20151103070403","2013-01-16T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-754.31007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1348,"POWERLINKV5_20151103070403","2013-01-16T23:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.868569999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1349,"POWERLINKV5_20151103070403","2013-01-16T23:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-564.53890000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1350,"POWERLINKV5_20151103070403","2013-01-16T23:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.932939999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1351,"POWERLINKV5_20151103070403","2013-01-16T23:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-64.977850000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1352,"POWERLINKV5_20151103070403","2013-01-16T23:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-27.253520000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1353,"POWERLINKV5_20151103070403","2013-01-16T23:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-27.003499999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1354,"POWERLINKV5_20151103070403","2013-01-16T23:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.151330000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1355,"POWERLINKV5_20151103070403","2013-01-16T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.205979999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1356,"POWERLINKV5_20151103070403","2013-01-16T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.20861,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1357,"POWERLINKV5_20151103070403","2013-01-16T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-44.315649999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1358,"POWERLINKV5_20151103070403","2013-01-16T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-44.315890000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1359,"POWERLINKV5_20151103070403","2013-01-17","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.80007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1360,"POWERLINKV5_20151103070403","2013-01-17T00:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-66.292869999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1361,"POWERLINKV5_20151103070403","2013-01-17T00:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.160589999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1362,"POWERLINKV5_20151103070403","2013-01-17T00:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-97.954059999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1363,"POWERLINKV5_20151103070403","2013-01-17T00:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.928109999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1364,"POWERLINKV5_20151103070403","2013-01-17T00:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.304099999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1365,"POWERLINKV5_20151103070403","2013-01-17T00:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-701.70627999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1366,"POWERLINKV5_20151103070403","2013-01-17T00:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.78214000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1367,"POWERLINKV5_20151103070403","2013-01-17T01:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.79471999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1368,"POWERLINKV5_20151103070403","2013-01-17T01:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-727.19949999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1369,"POWERLINKV5_20151103070403","2013-01-17T01:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-356.70483999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1370,"POWERLINKV5_20151103070403","2013-01-17T01:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1181.5489700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1371,"POWERLINKV5_20151103070403","2013-01-17T01:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.581720000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1372,"POWERLINKV5_20151103070403","2013-01-17T01:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.62598,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1373,"POWERLINKV5_20151103070403","2013-01-17T01:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1181.90041,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1374,"POWERLINKV5_20151103070403","2013-01-17T01:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.957149999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1375,"POWERLINKV5_20151103070403","2013-01-17T01:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.444870000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1376,"POWERLINKV5_20151103070403","2013-01-17T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-94.096779999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1377,"POWERLINKV5_20151103070403","2013-01-17T02:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.524850000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1378,"POWERLINKV5_20151103070403","2013-01-17T02:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.652700000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1379,"POWERLINKV5_20151103070403","2013-01-17T02:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.48753,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1380,"POWERLINKV5_20151103070403","2013-01-17T02:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.954509999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1381,"POWERLINKV5_20151103070403","2013-01-17T02:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.783360000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1382,"POWERLINKV5_20151103070403","2013-01-17T02:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1180.0371299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1383,"POWERLINKV5_20151103070403","2013-01-17T02:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.548499999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1384,"POWERLINKV5_20151103070403","2013-01-17T02:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.757539999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1385,"POWERLINKV5_20151103070403","2013-01-17T05:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.53698,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1386,"POWERLINKV5_20151103070403","2013-01-17T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.882370000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1387,"POWERLINKV5_20151103070403","2013-01-17T05:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.66287,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1388,"POWERLINKV5_20151103070403","2013-01-17T05:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.86572,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1389,"POWERLINKV5_20151103070403","2013-01-17T05:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1180.81314,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1390,"POWERLINKV5_20151103070403","2013-01-17T06:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-453.82508999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1391,"POWERLINKV5_20151103070403","2013-01-17T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-456.07996000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1392,"POWERLINKV5_20151103070403","2013-01-17T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-121.19096,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1393,"POWERLINKV5_20151103070403","2013-01-17T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11846.152529999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1394,"POWERLINKV5_20151103070403","2013-01-17T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11841.85737,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1395,"POWERLINKV5_20151103070403","2013-01-17T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.2660100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1396,"POWERLINKV5_20151103070403","2013-01-17T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.99209,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1397,"POWERLINKV5_20151103070403","2013-01-17T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.662990000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1398,"POWERLINKV5_20151103070403","2013-01-17T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.95072,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1399,"POWERLINKV5_20151103070403","2013-01-17T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-75.357020000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1400,"POWERLINKV5_20151103070403","2013-01-17T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13618.222470000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1401,"POWERLINKV5_20151103070403","2013-01-17T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-26.40475,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1402,"POWERLINKV5_20151103070403","2013-01-17T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-724.32777999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1403,"POWERLINKV5_20151103070403","2013-01-17T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-762.22248000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1404,"POWERLINKV5_20151103070403","2013-01-17T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-792.19227999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1405,"POWERLINKV5_20151103070403","2013-01-17T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.68120999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1406,"POWERLINKV5_20151103070403","2013-01-17T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.4909399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1407,"POWERLINKV5_20151103070403","2013-01-17T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1014.49303,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1408,"POWERLINKV5_20151103070403","2013-01-17T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.4400499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1409,"POWERLINKV5_20151103070403","2013-01-17T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1622.6051299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1410,"POWERLINKV5_20151103070403","2013-01-17T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12168.59072,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1411,"POWERLINKV5_20151103070403","2013-01-17T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12353.36167,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1412,"POWERLINKV5_20151103070403","2013-01-17T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2048.78746,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1413,"POWERLINKV5_20151103070403","2013-01-17T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-427.59309000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1414,"POWERLINKV5_20151103070403","2013-01-17T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-319.57522999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1415,"POWERLINKV5_20151103070403","2013-01-17T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1178.90843,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1416,"POWERLINKV5_20151103070403","2013-01-17T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.3116500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1417,"POWERLINKV5_20151103070403","2013-01-17T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-520.07707000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1418,"POWERLINKV5_20151103070403","2013-01-17T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-579.85649999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1419,"POWERLINKV5_20151103070403","2013-01-17T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-23.119289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1420,"POWERLINKV5_20151103070403","2013-01-17T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-314.67173000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1421,"POWERLINKV5_20151103070403","2013-01-17T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.180700000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1422,"POWERLINKV5_20151103070403","2013-01-17T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-23.834289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1423,"POWERLINKV5_20151103070403","2013-01-17T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.69014,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1424,"POWERLINKV5_20151103070403","2013-01-17T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-717.20594000000006,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1425,"POWERLINKV5_20151103070403","2013-01-17T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-694.80907000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1426,"POWERLINKV5_20151103070403","2013-01-17T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1257.3710000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1427,"POWERLINKV5_20151103070403","2013-01-17T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1011.69134,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1428,"POWERLINKV5_20151103070403","2013-01-17T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1080.34375,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1429,"POWERLINKV5_20151103070403","2013-01-17T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.67957000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1430,"POWERLINKV5_20151103070403","2013-01-17T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1016.10677,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1431,"POWERLINKV5_20151103070403","2013-01-17T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1021.22752,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1432,"POWERLINKV5_20151103070403","2013-01-17T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.53333,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1433,"POWERLINKV5_20151103070403","2013-01-17T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1070.4259099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1434,"POWERLINKV5_20151103070403","2013-01-17T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1069.5694100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1435,"POWERLINKV5_20151103070403","2013-01-17T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1615.2262700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1436,"POWERLINKV5_20151103070403","2013-01-17T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.7850800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1437,"POWERLINKV5_20151103070403","2013-01-17T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-855.17584999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1438,"POWERLINKV5_20151103070403","2013-01-17T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-854.32714999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1439,"POWERLINKV5_20151103070403","2013-01-17T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1017.61223,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1440,"POWERLINKV5_20151103070403","2013-01-17T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-847.86643000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1441,"POWERLINKV5_20151103070403","2013-01-17T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1006.12131,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1442,"POWERLINKV5_20151103070403","2013-01-17T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-853.39499000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1443,"POWERLINKV5_20151103070403","2013-01-17T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1587.64102,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1444,"POWERLINKV5_20151103070403","2013-01-17T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1586.1302900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1445,"POWERLINKV5_20151103070403","2013-01-17T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2023.3238799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1446,"POWERLINKV5_20151103070403","2013-01-17T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11730.96105,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1447,"POWERLINKV5_20151103070403","2013-01-17T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2078.8478799999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1448,"POWERLINKV5_20151103070403","2013-01-17T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2304.43914,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1449,"POWERLINKV5_20151103070403","2013-01-17T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-55.4,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1450,"POWERLINKV5_20151103070403","2013-01-17T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.542999999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1451,"POWERLINKV5_20151103070403","2013-01-17T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-62.890099999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1452,"POWERLINKV5_20151103070403","2013-01-17T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1588.4846199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1453,"POWERLINKV5_20151103070403","2013-01-17T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1078.6973599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1454,"POWERLINKV5_20151103070403","2013-01-17T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.28898,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1455,"POWERLINKV5_20151103070403","2013-01-17T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1496.22813,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1456,"POWERLINKV5_20151103070403","2013-01-17T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.6858299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1457,"POWERLINKV5_20151103070403","2013-01-17T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1339.9988000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1458,"POWERLINKV5_20151103070403","2013-01-17T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.49629,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1459,"POWERLINKV5_20151103070403","2013-01-17T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1270.27289,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1460,"POWERLINKV5_20151103070403","2013-01-17T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1222.85249,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1461,"POWERLINKV5_20151103070403","2013-01-17T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11739.249400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1462,"POWERLINKV5_20151103070403","2013-01-17T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1215.6427100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1463,"POWERLINKV5_20151103070403","2013-01-17T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.39436,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1464,"POWERLINKV5_20151103070403","2013-01-17T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1072.38123,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1465,"POWERLINKV5_20151103070403","2013-01-17T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.67913,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1466,"POWERLINKV5_20151103070403","2013-01-17T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.7012299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1467,"POWERLINKV5_20151103070403","2013-01-17T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12103.54934,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1468,"POWERLINKV5_20151103070403","2013-01-17T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1587.6409900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1469,"POWERLINKV5_20151103070403","2013-01-17T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.14139,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1470,"POWERLINKV5_20151103070403","2013-01-17T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1618.4748199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1471,"POWERLINKV5_20151103070403","2013-01-17T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1616.31789,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1472,"POWERLINKV5_20151103070403","2013-01-17T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1615.75215,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1473,"POWERLINKV5_20151103070403","2013-01-17T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.84187,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1474,"POWERLINKV5_20151103070403","2013-01-17T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1071.4659099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1475,"POWERLINKV5_20151103070403","2013-01-17T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1014.74341,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1476,"POWERLINKV5_20151103070403","2013-01-17T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1382.3354400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1477,"POWERLINKV5_20151103070403","2013-01-17T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1225.19856,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1478,"POWERLINKV5_20151103070403","2013-01-17T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1225.1006600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1479,"POWERLINKV5_20151103070403","2013-01-17T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1267.08015,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1480,"POWERLINKV5_20151103070403","2013-01-17T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.98937,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1481,"POWERLINKV5_20151103070403","2013-01-17T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.2687000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1482,"POWERLINKV5_20151103070403","2013-01-17T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1285.9902300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1483,"POWERLINKV5_20151103070403","2013-01-17T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.3072199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1484,"POWERLINKV5_20151103070403","2013-01-17T22:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1222.38129,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1485,"POWERLINKV5_20151103070403","2013-01-17T22:15:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1027.9102700000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1486,"POWERLINKV5_20151103070403","2013-01-17T22:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-437.32200999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1487,"POWERLINKV5_20151103070403","2013-01-17T22:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-438.21656999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1488,"POWERLINKV5_20151103070403","2013-01-17T22:25:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1036.70443,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1489,"POWERLINKV5_20151103070403","2013-01-17T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2044.22813,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1490,"POWERLINKV5_20151103070403","2013-01-17T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11734.86904,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1491,"POWERLINKV5_20151103070403","2013-01-17T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.7889500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1492,"POWERLINKV5_20151103070403","2013-01-17T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.29322,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1493,"POWERLINKV5_20151103070403","2013-01-17T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2046.3830800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1494,"POWERLINKV5_20151103070403","2013-01-17T22:50:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-986.35757000000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1495,"POWERLINKV5_20151103070403","2013-01-17T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2045.86734,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1496,"POWERLINKV5_20151103070403","2013-01-17T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-102.96187,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1497,"POWERLINKV5_20151103070403","2013-01-17T23:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1046.5166899999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1498,"POWERLINKV5_20151103070403","2013-01-17T23:25:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1051.8483799999999,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1499,"POWERLINKV5_20151103070403","2013-01-17T23:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1838.7732800000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1500,"POWERLINKV5_20151103070403","2013-01-17T23:30:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1009.11969,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1501,"POWERLINKV5_20151103070403","2013-01-17T23:35:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1053.8716999999999,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1502,"POWERLINKV5_20151103070403","2013-01-17T23:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1842.18887,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1503,"POWERLINKV5_20151103070403","2013-01-17T23:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1802.5391199999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1504,"POWERLINKV5_20151103070403","2013-01-17T23:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1803.79484,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1505,"POWERLINKV5_20151103070403","2013-01-17T23:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1804.58887,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1506,"POWERLINKV5_20151103070403","2013-01-18","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2054.3089500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1507,"POWERLINKV5_20151103070403","2013-01-18T00:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11804.91179,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1508,"POWERLINKV5_20151103070403","2013-01-18T00:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-819.58262999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1509,"POWERLINKV5_20151103070403","2013-01-18T00:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-25.019539999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1510,"POWERLINKV5_20151103070403","2013-01-18T00:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.06381,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1511,"POWERLINKV5_20151103070403","2013-01-18T00:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.73498,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1512,"POWERLINKV5_20151103070403","2013-01-18T01:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2051.2227800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1513,"POWERLINKV5_20151103070403","2013-01-18T02:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-314.78079000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1514,"POWERLINKV5_20151103070403","2013-01-18T04:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.08028,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1515,"POWERLINKV5_20151103070403","2013-01-18T05:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14585.6284,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1516,"POWERLINKV5_20151103070403","2013-01-18T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-449.10876000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1517,"POWERLINKV5_20151103070403","2013-01-18T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-450.16282999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1518,"POWERLINKV5_20151103070403","2013-01-18T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2070.8175500000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1519,"POWERLINKV5_20151103070403","2013-01-18T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-451.14641999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1520,"POWERLINKV5_20151103070403","2013-01-18T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1181.78756,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1521,"POWERLINKV5_20151103070403","2013-01-18T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-450.06472000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1522,"POWERLINKV5_20151103070403","2013-01-18T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2074.1871900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1523,"POWERLINKV5_20151103070403","2013-01-18T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1139.8597,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1524,"POWERLINKV5_20151103070403","2013-01-18T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11859.1445,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1525,"POWERLINKV5_20151103070403","2013-01-18T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2064.31846,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1526,"POWERLINKV5_20151103070403","2013-01-18T06:50:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-968.70968000000005,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1527,"POWERLINKV5_20151103070403","2013-01-18T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1086.79421,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1528,"POWERLINKV5_20151103070403","2013-01-18T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2371.14615,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1529,"POWERLINKV5_20151103070403","2013-01-18T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-73.550759999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1530,"POWERLINKV5_20151103070403","2013-01-18T07:15:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1033.2601400000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1531,"POWERLINKV5_20151103070403","2013-01-18T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.8178499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1532,"POWERLINKV5_20151103070403","2013-01-18T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12176.45067,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1533,"POWERLINKV5_20151103070403","2013-01-18T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11789.45811,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1534,"POWERLINKV5_20151103070403","2013-01-18T07:35:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1043.58413,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1535,"POWERLINKV5_20151103070403","2013-01-18T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-64.947640000000007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1536,"POWERLINKV5_20151103070403","2013-01-18T07:55:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1051.895,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1537,"POWERLINKV5_20151103070403","2013-01-18T08:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1052.36043,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1538,"POWERLINKV5_20151103070403","2013-01-18T08:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1053.94876,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1539,"POWERLINKV5_20151103070403","2013-01-18T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-16.62988,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1540,"POWERLINKV5_20151103070403","2013-01-18T08:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-91120.433359999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1541,"POWERLINKV5_20151103070403","2013-01-18T08:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-305.38072,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1542,"POWERLINKV5_20151103070403","2013-01-18T08:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.687390000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1543,"POWERLINKV5_20151103070403","2013-01-18T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.68763,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1544,"POWERLINKV5_20151103070403","2013-01-18T08:45:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1048.6055799999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1545,"POWERLINKV5_20151103070403","2013-01-18T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11783.299429999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1546,"POWERLINKV5_20151103070403","2013-01-18T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-255.32483999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1547,"POWERLINKV5_20151103070403","2013-01-18T08:55:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1059.2673,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1548,"POWERLINKV5_20151103070403","2013-01-18T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-249.46653000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1549,"POWERLINKV5_20151103070403","2013-01-18T09:00:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1054.5159900000001,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1550,"POWERLINKV5_20151103070403","2013-01-18T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.209630000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1551,"POWERLINKV5_20151103070403","2013-01-18T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11788.043079999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1552,"POWERLINKV5_20151103070403","2013-01-18T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12595.147279999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1553,"POWERLINKV5_20151103070403","2013-01-18T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-260.02654000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1554,"POWERLINKV5_20151103070403","2013-01-18T13:25:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-144.96001000000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1555,"POWERLINKV5_20151103070403","2013-01-18T13:30:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-334.96001000000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1556,"POWERLINKV5_20151103070403","2013-01-18T13:45:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-135.40001000000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1557,"POWERLINKV5_20151103070403","2013-01-18T14:05:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1124.2258400000001,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1558,"POWERLINKV5_20151103070403","2013-01-18T14:25:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1108.0799199999999,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1559,"POWERLINKV5_20151103070403","2013-01-18T14:45:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1290.43083,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1560,"POWERLINKV5_20151103070403","2013-01-18T15:25:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1163.42218,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1561,"POWERLINKV5_20151103070403","2013-01-18T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-200.90182999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1562,"POWERLINKV5_20151103070403","2013-01-18T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-354.39600999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1563,"POWERLINKV5_20151103070403","2013-01-18T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-145.06661,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1564,"POWERLINKV5_20151103070403","2013-01-18T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-186.81584000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1565,"POWERLINKV5_20151103070403","2013-01-18T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-144.97498999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1566,"POWERLINKV5_20151103070403","2013-01-18T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-312.79899,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1567,"POWERLINKV5_20151103070403","2013-01-18T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-187.12852000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1568,"POWERLINKV5_20151103070403","2013-01-18T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-188.15299999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1569,"POWERLINKV5_20151103070403","2013-01-18T16:35:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1130.89681,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1570,"POWERLINKV5_20151103070403","2013-01-18T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-771.30998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1571,"POWERLINKV5_20151103070403","2013-01-18T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-161.14546000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1572,"POWERLINKV5_20151103070403","2013-01-18T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.179900000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1573,"POWERLINKV5_20151103070403","2013-01-18T21:45:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1052.0014799999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1574,"POWERLINKV5_20151103070403","2013-01-18T22:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-35.723269999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1575,"POWERLINKV5_20151103070403","2013-01-18T22:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-295.83344,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1576,"POWERLINKV5_20151103070403","2013-01-18T22:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1048.9016899999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1577,"POWERLINKV5_20151103070403","2013-01-18T22:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.42209,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1578,"POWERLINKV5_20151103070403","2013-01-18T22:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.4011,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1579,"POWERLINKV5_20151103070403","2013-01-18T22:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-442.55130000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1580,"POWERLINKV5_20151103070403","2013-01-18T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.61907000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1581,"POWERLINKV5_20151103070403","2013-01-18T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-444.75979999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1582,"POWERLINKV5_20151103070403","2013-01-18T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-444.73847999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1583,"POWERLINKV5_20151103070403","2013-01-18T22:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.7918299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1584,"POWERLINKV5_20151103070403","2013-01-18T22:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-309.35505999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1585,"POWERLINKV5_20151103070403","2013-01-18T23:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-310.07339000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1586,"POWERLINKV5_20151103070403","2013-01-18T23:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.879219999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1587,"POWERLINKV5_20151103070403","2013-01-18T23:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-304.98101000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1588,"POWERLINKV5_20151103070403","2013-01-18T23:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-445.51071000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1589,"POWERLINKV5_20151103070403","2013-01-18T23:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-448.31707999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1590,"POWERLINKV5_20151103070403","2013-01-18T23:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.9911400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1591,"POWERLINKV5_20151103070403","2013-01-18T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1194.25731,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1592,"POWERLINKV5_20151103070403","2013-01-18T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-311.17550999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1593,"POWERLINKV5_20151103070403","2013-01-18T23:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-391.72008,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1594,"POWERLINKV5_20151103070403","2013-01-18T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-309.29541999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1595,"POWERLINKV5_20151103070403","2013-01-19T01:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-270.49045999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1596,"POWERLINKV5_20151103070403","2013-01-19T01:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-28.02364,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1597,"POWERLINKV5_20151103070403","2013-01-19T01:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.01362,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1598,"POWERLINKV5_20151103070403","2013-01-19T01:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-20.387709999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1599,"POWERLINKV5_20151103070403","2013-01-19T06:20:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1041.8677700000001,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1600,"POWERLINKV5_20151103070403","2013-01-19T06:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.09906,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1601,"POWERLINKV5_20151103070403","2013-01-19T06:30:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1041.55853,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1602,"POWERLINKV5_20151103070403","2013-01-19T06:40:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1042.73396,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1603,"POWERLINKV5_20151103070403","2013-01-19T06:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.22687,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1604,"POWERLINKV5_20151103070403","2013-01-19T06:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.71822,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1605,"POWERLINKV5_20151103070403","2013-01-19T06:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.2845299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1606,"POWERLINKV5_20151103070403","2013-01-19T07:00:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1043.73386,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1607,"POWERLINKV5_20151103070403","2013-01-19T07:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.55673,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1608,"POWERLINKV5_20151103070403","2013-01-19T07:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.8757700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1609,"POWERLINKV5_20151103070403","2013-01-19T07:15:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1044.41815,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1610,"POWERLINKV5_20151103070403","2013-01-19T07:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.44994,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1611,"POWERLINKV5_20151103070403","2013-01-19T07:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.7320099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1612,"POWERLINKV5_20151103070403","2013-01-19T07:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.05152,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1613,"POWERLINKV5_20151103070403","2013-01-19T07:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.7415599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1614,"POWERLINKV5_20151103070403","2013-01-19T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-283.10829000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1615,"POWERLINKV5_20151103070403","2013-01-19T07:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1032.52738,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1616,"POWERLINKV5_20151103070403","2013-01-19T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.649990000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1617,"POWERLINKV5_20151103070403","2013-01-19T07:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.1982700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1618,"POWERLINKV5_20151103070403","2013-01-19T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.028790000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1619,"POWERLINKV5_20151103070403","2013-01-19T07:50:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1045.1134500000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1620,"POWERLINKV5_20151103070403","2013-01-19T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.3765,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1621,"POWERLINKV5_20151103070403","2013-01-19T07:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.7699500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1622,"POWERLINKV5_20151103070403","2013-01-19T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.687899999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1623,"POWERLINKV5_20151103070403","2013-01-19T08:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1044.74136,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1624,"POWERLINKV5_20151103070403","2013-01-19T08:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-90.016570000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1625,"POWERLINKV5_20151103070403","2013-01-19T08:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.17731,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1626,"POWERLINKV5_20151103070403","2013-01-19T08:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1194.96135,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1627,"POWERLINKV5_20151103070403","2013-01-19T08:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-311.45271000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1628,"POWERLINKV5_20151103070403","2013-01-19T08:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.2624000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1629,"POWERLINKV5_20151103070403","2013-01-19T08:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.00179,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1630,"POWERLINKV5_20151103070403","2013-01-19T08:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1194.84601,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1631,"POWERLINKV5_20151103070403","2013-01-19T08:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1193.85329,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1632,"POWERLINKV5_20151103070403","2013-01-19T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.2176400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1633,"POWERLINKV5_20151103070403","2013-01-19T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1193.4845700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1634,"POWERLINKV5_20151103070403","2013-01-19T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1633.7936299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1635,"POWERLINKV5_20151103070403","2013-01-19T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1193.33376,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1636,"POWERLINKV5_20151103070403","2013-01-19T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.572500000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1637,"POWERLINKV5_20151103070403","2013-01-19T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.69281,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1638,"POWERLINKV5_20151103070403","2013-01-19T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1126.08647,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1639,"POWERLINKV5_20151103070403","2013-01-19T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.96342,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1640,"POWERLINKV5_20151103070403","2013-01-19T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1657.383,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1641,"POWERLINKV5_20151103070403","2013-01-19T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.69659,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1642,"POWERLINKV5_20151103070403","2013-01-19T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.9915699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1643,"POWERLINKV5_20151103070403","2013-01-19T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.4261799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1644,"POWERLINKV5_20151103070403","2013-01-19T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1621.0941,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1645,"POWERLINKV5_20151103070403","2013-01-19T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1934.50586,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1646,"POWERLINKV5_20151103070403","2013-01-19T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.99332,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1647,"POWERLINKV5_20151103070403","2013-01-19T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1170.3156799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1648,"POWERLINKV5_20151103070403","2013-01-19T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.63005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1649,"POWERLINKV5_20151103070403","2013-01-19T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.98669,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1650,"POWERLINKV5_20151103070403","2013-01-19T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.8679299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1651,"POWERLINKV5_20151103070403","2013-01-19T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.9726,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1652,"POWERLINKV5_20151103070403","2013-01-19T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.9127800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1653,"POWERLINKV5_20151103070403","2013-01-19T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.9757999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1654,"POWERLINKV5_20151103070403","2013-01-19T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-358.07168000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1655,"POWERLINKV5_20151103070403","2013-01-19T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.9525900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1656,"POWERLINKV5_20151103070403","2013-01-19T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-301.50972000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1657,"POWERLINKV5_20151103070403","2013-01-19T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-96.183170000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1658,"POWERLINKV5_20151103070403","2013-01-19T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1621.0364500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1659,"POWERLINKV5_20151103070403","2013-01-19T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11745.461789999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1660,"POWERLINKV5_20151103070403","2013-01-19T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1626.0864799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1661,"POWERLINKV5_20151103070403","2013-01-19T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1621.9215300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1662,"POWERLINKV5_20151103070403","2013-01-19T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.60069,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1663,"POWERLINKV5_20151103070403","2013-01-19T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.57646,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1664,"POWERLINKV5_20151103070403","2013-01-19T12:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1052.3917300000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1665,"POWERLINKV5_20151103070403","2013-01-19T12:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-17.655190000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1666,"POWERLINKV5_20151103070403","2013-01-19T12:15:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1051.45451,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1667,"POWERLINKV5_20151103070403","2013-01-19T12:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-751.60866999999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1668,"POWERLINKV5_20151103070403","2013-01-19T12:20:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1035.4923899999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1669,"POWERLINKV5_20151103070403","2013-01-19T12:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1425.78988,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1670,"POWERLINKV5_20151103070403","2013-01-19T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.9175700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1671,"POWERLINKV5_20151103070403","2013-01-19T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.89895,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1672,"POWERLINKV5_20151103070403","2013-01-19T12:35:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1014.40075,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1673,"POWERLINKV5_20151103070403","2013-01-19T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.8510000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1674,"POWERLINKV5_20151103070403","2013-01-19T12:40:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1015.29521,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1675,"POWERLINKV5_20151103070403","2013-01-19T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-652.67944999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1676,"POWERLINKV5_20151103070403","2013-01-19T12:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-849.49684999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1677,"POWERLINKV5_20151103070403","2013-01-19T12:45:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1014.83309,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1678,"POWERLINKV5_20151103070403","2013-01-19T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-660.36554000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1679,"POWERLINKV5_20151103070403","2013-01-19T12:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-841.04341999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1680,"POWERLINKV5_20151103070403","2013-01-19T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-649.02110000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1681,"POWERLINKV5_20151103070403","2013-01-19T12:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-853.53479000000004,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1682,"POWERLINKV5_20151103070403","2013-01-19T13:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1424.9273599999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1683,"POWERLINKV5_20151103070403","2013-01-19T13:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1021.73595,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1684,"POWERLINKV5_20151103070403","2013-01-19T13:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1847.38202,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1685,"POWERLINKV5_20151103070403","2013-01-19T13:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-266.16368999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1686,"POWERLINKV5_20151103070403","2013-01-19T13:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1046.1288500000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1687,"POWERLINKV5_20151103070403","2013-01-19T13:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-265.69616000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1688,"POWERLINKV5_20151103070403","2013-01-19T13:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-264.85212000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1689,"POWERLINKV5_20151103070403","2013-01-19T13:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1797.26349,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1690,"POWERLINKV5_20151103070403","2013-01-19T13:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1798.1424500000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1691,"POWERLINKV5_20151103070403","2013-01-19T13:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1840.78971,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1692,"POWERLINKV5_20151103070403","2013-01-19T13:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1847.16679,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1693,"POWERLINKV5_20151103070403","2013-01-19T13:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1803.2189699999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1694,"POWERLINKV5_20151103070403","2013-01-19T13:45:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1009.06645,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1695,"POWERLINKV5_20151103070403","2013-01-19T13:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1802.57512,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1696,"POWERLINKV5_20151103070403","2013-01-19T13:50:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1009.77733,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1697,"POWERLINKV5_20151103070403","2013-01-19T13:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1802.29692,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1698,"POWERLINKV5_20151103070403","2013-01-19T13:55:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1010.08379,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1699,"POWERLINKV5_20151103070403","2013-01-19T14:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1802.2264399999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1700,"POWERLINKV5_20151103070403","2013-01-19T14:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1010.1623,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1701,"POWERLINKV5_20151103070403","2013-01-19T14:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1798.9592700000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1702,"POWERLINKV5_20151103070403","2013-01-19T14:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1797.9722999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1703,"POWERLINKV5_20151103070403","2013-01-19T14:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1796.30791,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1704,"POWERLINKV5_20151103070403","2013-01-19T14:30:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1796.2446399999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1705,"POWERLINKV5_20151103070403","2013-01-19T14:35:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-264.67901000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1706,"POWERLINKV5_20151103070403","2013-01-19T14:40:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-266.05090000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1707,"POWERLINKV5_20151103070403","2013-01-19T14:45:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-265.52015,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1708,"POWERLINKV5_20151103070403","2013-01-19T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-79.962940000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1709,"POWERLINKV5_20151103070403","2013-01-19T14:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1726.56035,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1710,"POWERLINKV5_20151103070403","2013-01-19T14:50:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1014.8705200000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1711,"POWERLINKV5_20151103070403","2013-01-19T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.6321499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1712,"POWERLINKV5_20151103070403","2013-01-19T14:55:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1020.18717,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1713,"POWERLINKV5_20151103070403","2013-01-19T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.5201,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1714,"POWERLINKV5_20151103070403","2013-01-19T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.2461699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1715,"POWERLINKV5_20151103070403","2013-01-19T15:05:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1018.35231,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1716,"POWERLINKV5_20151103070403","2013-01-19T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2036.13147,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1717,"POWERLINKV5_20151103070403","2013-01-19T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.84366999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1718,"POWERLINKV5_20151103070403","2013-01-19T15:15:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1044.95733,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1719,"POWERLINKV5_20151103070403","2013-01-19T15:20:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1339.5534500000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1720,"POWERLINKV5_20151103070403","2013-01-19T15:25:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-3000.0034999999998,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1721,"POWERLINKV5_20151103070403","2013-01-19T15:30:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1299.9935,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1722,"POWERLINKV5_20151103070403","2013-01-19T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1797.3284900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1723,"POWERLINKV5_20151103070403","2013-01-19T15:40:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1510.6605099999999,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1724,"POWERLINKV5_20151103070403","2013-01-19T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.24241999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1725,"POWERLINKV5_20151103070403","2013-01-19T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-297.74563000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1726,"POWERLINKV5_20151103070403","2013-01-19T15:50:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1047.02242,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1727,"POWERLINKV5_20151103070403","2013-01-19T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.25864,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1728,"POWERLINKV5_20151103070403","2013-01-19T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.28503,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1729,"POWERLINKV5_20151103070403","2013-01-19T16:00:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1382.0232100000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1730,"POWERLINKV5_20151103070403","2013-01-19T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.2057400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1731,"POWERLINKV5_20151103070403","2013-01-19T16:05:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1381.65578,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1732,"POWERLINKV5_20151103070403","2013-01-19T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.5607299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1733,"POWERLINKV5_20151103070403","2013-01-19T16:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-990.12442999999996,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1734,"POWERLINKV5_20151103070403","2013-01-19T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.3798099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1735,"POWERLINKV5_20151103070403","2013-01-19T16:15:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1015.64409,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1736,"POWERLINKV5_20151103070403","2013-01-19T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2041.52638,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1737,"POWERLINKV5_20151103070403","2013-01-19T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1209.04045,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1738,"POWERLINKV5_20151103070403","2013-01-19T16:25:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1016.19936,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1739,"POWERLINKV5_20151103070403","2013-01-19T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.36087,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1740,"POWERLINKV5_20151103070403","2013-01-19T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2034.7488699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1741,"POWERLINKV5_20151103070403","2013-01-19T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1531.1478300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1742,"POWERLINKV5_20151103070403","2013-01-19T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1531.1487199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1743,"POWERLINKV5_20151103070403","2013-01-19T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.28773,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1744,"POWERLINKV5_20151103070403","2013-01-19T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.28763,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1745,"POWERLINKV5_20151103070403","2013-01-19T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1917.0200500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1746,"POWERLINKV5_20151103070403","2013-01-19T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.3095900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1747,"POWERLINKV5_20151103070403","2013-01-19T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1013.04067,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1748,"POWERLINKV5_20151103070403","2013-01-19T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.37012,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1749,"POWERLINKV5_20151103070403","2013-01-19T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.36519,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1750,"POWERLINKV5_20151103070403","2013-01-19T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.47183,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1751,"POWERLINKV5_20151103070403","2013-01-19T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.6197199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1752,"POWERLINKV5_20151103070403","2013-01-19T17:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.6488300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1753,"POWERLINKV5_20151103070403","2013-01-19T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.6821500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1754,"POWERLINKV5_20151103070403","2013-01-19T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1214.58736,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1755,"POWERLINKV5_20151103070403","2013-01-19T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.6523299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1756,"POWERLINKV5_20151103070403","2013-01-19T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.10751,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1757,"POWERLINKV5_20151103070403","2013-01-19T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.74473999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1758,"POWERLINKV5_20151103070403","2013-01-19T18:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.3117500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1759,"POWERLINKV5_20151103070403","2013-01-19T18:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1454.6342500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1760,"POWERLINKV5_20151103070403","2013-01-19T18:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.2599299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1761,"POWERLINKV5_20151103070403","2013-01-19T18:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.4577899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1762,"POWERLINKV5_20151103070403","2013-01-19T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1422.30726,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1763,"POWERLINKV5_20151103070403","2013-01-19T18:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1374.21505,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1764,"POWERLINKV5_20151103070403","2013-01-19T18:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1006.41301,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1765,"POWERLINKV5_20151103070403","2013-01-19T18:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1213.30574,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1766,"POWERLINKV5_20151103070403","2013-01-19T18:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1008.4932,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1767,"POWERLINKV5_20151103070403","2013-01-19T18:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1009.74074,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1768,"POWERLINKV5_20151103070403","2013-01-19T19:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.74928,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1769,"POWERLINKV5_20151103070403","2013-01-19T19:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-975.60266000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1770,"POWERLINKV5_20151103070403","2013-01-19T19:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1007.2256599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1771,"POWERLINKV5_20151103070403","2013-01-19T19:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1249.50701,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1772,"POWERLINKV5_20151103070403","2013-01-19T19:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1007.76088,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1773,"POWERLINKV5_20151103070403","2013-01-19T20:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.578989999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1774,"POWERLINKV5_20151103070403","2013-01-19T20:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.47084,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1775,"POWERLINKV5_20151103070403","2013-01-19T20:40:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1018.73051,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1776,"POWERLINKV5_20151103070403","2013-01-19T20:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.01164,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1777,"POWERLINKV5_20151103070403","2013-01-19T20:45:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1051.7272800000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1778,"POWERLINKV5_20151103070403","2013-01-19T20:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1010.76788,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1779,"POWERLINKV5_20151103070403","2013-01-19T20:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.412219999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1780,"POWERLINKV5_20151103070403","2013-01-19T21:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.873179999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1781,"POWERLINKV5_20151103070403","2013-01-19T21:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.00015,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1782,"POWERLINKV5_20151103070403","2013-01-19T21:05:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1050.9842200000001,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1783,"POWERLINKV5_20151103070403","2013-01-19T21:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.844999999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1784,"POWERLINKV5_20151103070403","2013-01-19T21:10:00","Q>NIL_CLBCN_7350","Q-NIL","2012-07-01",1,-1050.96838,"Out= Nil, avoid overload on 7350 T13 Chinchilla to T194 Columboola 132kV line on trip of 7349 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1785,"POWERLINKV5_20151103070403","2013-01-19T21:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-42.825159999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1786,"POWERLINKV5_20151103070403","2013-01-19T21:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.532440000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1787,"POWERLINKV5_20151103070403","2013-01-19T21:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.784599999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1788,"POWERLINKV5_20151103070403","2013-01-19T21:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.80945,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1789,"POWERLINKV5_20151103070403","2013-01-19T21:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.782580000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1790,"POWERLINKV5_20151103070403","2013-01-19T21:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.18623,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1791,"POWERLINKV5_20151103070403","2013-01-19T21:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.95252,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1792,"POWERLINKV5_20151103070403","2013-01-19T21:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.54007,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1793,"POWERLINKV5_20151103070403","2013-01-19T22:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.6643799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1794,"POWERLINKV5_20151103070403","2013-01-19T22:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2043.7415599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1795,"POWERLINKV5_20151103070403","2013-01-19T22:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.923670000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1796,"POWERLINKV5_20151103070403","2013-01-19T22:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.20252,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1797,"POWERLINKV5_20151103070403","2013-01-19T22:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2046.7487900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1798,"POWERLINKV5_20151103070403","2013-01-19T22:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.306130000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1799,"POWERLINKV5_20151103070403","2013-01-19T23:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.496429999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1800,"POWERLINKV5_20151103070403","2013-01-19T23:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11791.363509999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1801,"POWERLINKV5_20151103070403","2013-01-19T23:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-49.954140000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1802,"POWERLINKV5_20151103070403","2013-01-19T23:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.15619,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1803,"POWERLINKV5_20151103070403","2013-01-20T00:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2052.93703,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1804,"POWERLINKV5_20151103070403","2013-01-20T00:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.58519,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1805,"POWERLINKV5_20151103070403","2013-01-20T00:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1191.89804,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1806,"POWERLINKV5_20151103070403","2013-01-20T00:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.1688899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1807,"POWERLINKV5_20151103070403","2013-01-20T00:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11796.904259999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1808,"POWERLINKV5_20151103070403","2013-01-20T00:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2059.3155499999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1809,"POWERLINKV5_20151103070403","2013-01-20T00:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2054.5908300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1810,"POWERLINKV5_20151103070403","2013-01-20T00:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2046.16715,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1811,"POWERLINKV5_20151103070403","2013-01-20T00:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-50.9589,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1812,"POWERLINKV5_20151103070403","2013-01-20T00:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-50.544150000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1813,"POWERLINKV5_20151103070403","2013-01-20T01:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.9559,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1814,"POWERLINKV5_20151103070403","2013-01-20T03:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.296810000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1815,"POWERLINKV5_20151103070403","2013-01-20T03:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.489400000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1816,"POWERLINKV5_20151103070403","2013-01-20T03:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.186210000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1817,"POWERLINKV5_20151103070403","2013-01-20T04:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.26587,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1818,"POWERLINKV5_20151103070403","2013-01-20T04:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.279210000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1819,"POWERLINKV5_20151103070403","2013-01-20T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2066.60862,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1820,"POWERLINKV5_20151103070403","2013-01-20T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.286999999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1821,"POWERLINKV5_20151103070403","2013-01-20T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2059.2880500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1822,"POWERLINKV5_20151103070403","2013-01-20T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.251069999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1823,"POWERLINKV5_20151103070403","2013-01-20T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-447.84897999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1824,"POWERLINKV5_20151103070403","2013-01-20T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.4368899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1825,"POWERLINKV5_20151103070403","2013-01-20T07:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.937109999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1826,"POWERLINKV5_20151103070403","2013-01-20T07:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.2667,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1827,"POWERLINKV5_20151103070403","2013-01-20T07:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.571300000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1828,"POWERLINKV5_20151103070403","2013-01-20T07:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-315.98872,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1829,"POWERLINKV5_20151103070403","2013-01-20T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1186.39744,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1830,"POWERLINKV5_20151103070403","2013-01-20T07:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-317.18579999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1831,"POWERLINKV5_20151103070403","2013-01-20T07:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1180.9331400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1832,"POWERLINKV5_20151103070403","2013-01-20T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1178.45398,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1833,"POWERLINKV5_20151103070403","2013-01-20T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1644.19301,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1834,"POWERLINKV5_20151103070403","2013-01-20T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1645.4447,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1835,"POWERLINKV5_20151103070403","2013-01-20T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-54.317520000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1836,"POWERLINKV5_20151103070403","2013-01-20T08:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-825.80679999999995,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1837,"POWERLINKV5_20151103070403","2013-01-20T08:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-391.17209000000003,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1838,"POWERLINKV5_20151103070403","2013-01-20T08:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-48.5,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1839,"POWERLINKV5_20151103070403","2013-01-20T08:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-44.51052,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1840,"POWERLINKV5_20151103070403","2013-01-20T08:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-422.36970000000002,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1841,"POWERLINKV5_20151103070403","2013-01-20T08:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12740.610979999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1842,"POWERLINKV5_20151103070403","2013-01-20T08:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-63900.228690000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1843,"POWERLINKV5_20151103070403","2013-01-20T08:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12997.94701,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1844,"POWERLINKV5_20151103070403","2013-01-20T08:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13309.95494,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1845,"POWERLINKV5_20151103070403","2013-01-20T08:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2637.1944600000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1846,"POWERLINKV5_20151103070403","2013-01-20T08:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1934.50576,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1847,"POWERLINKV5_20151103070403","2013-01-20T09:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1934.36022,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1848,"POWERLINKV5_20151103070403","2013-01-20T09:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.99378,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1849,"POWERLINKV5_20151103070403","2013-01-20T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1139.86229,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1850,"POWERLINKV5_20151103070403","2013-01-20T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.4177199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1851,"POWERLINKV5_20151103070403","2013-01-20T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1265.91815,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1852,"POWERLINKV5_20151103070403","2013-01-20T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1265.91815,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1853,"POWERLINKV5_20151103070403","2013-01-20T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1178.90843,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1854,"POWERLINKV5_20151103070403","2013-01-20T09:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-306.43043,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1855,"POWERLINKV5_20151103070403","2013-01-20T09:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.99263,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1856,"POWERLINKV5_20151103070403","2013-01-20T09:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.9393600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1857,"POWERLINKV5_20151103070403","2013-01-20T09:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1000.00375,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1858,"POWERLINKV5_20151103070403","2013-01-20T09:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1000.00416,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1859,"POWERLINKV5_20151103070403","2013-01-20T10:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1232.7228500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1860,"POWERLINKV5_20151103070403","2013-01-20T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1879.93932,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1861,"POWERLINKV5_20151103070403","2013-01-20T10:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.84229,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1862,"POWERLINKV5_20151103070403","2013-01-20T10:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.2926,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1863,"POWERLINKV5_20151103070403","2013-01-20T10:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.7826,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1864,"POWERLINKV5_20151103070403","2013-01-20T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.9427800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1865,"POWERLINKV5_20151103070403","2013-01-20T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-59.880319999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1866,"POWERLINKV5_20151103070403","2013-01-20T10:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-267.56608999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1867,"POWERLINKV5_20151103070403","2013-01-20T10:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-896.19174999999996,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1868,"POWERLINKV5_20151103070403","2013-01-20T11:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-39.310679999999998,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1869,"POWERLINKV5_20151103070403","2013-01-20T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.23733,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1870,"POWERLINKV5_20151103070403","2013-01-20T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-48.006619999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1871,"POWERLINKV5_20151103070403","2013-01-20T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-47.537460000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1872,"POWERLINKV5_20151103070403","2013-01-20T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-308.25598000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1873,"POWERLINKV5_20151103070403","2013-01-20T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-308.02605999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1874,"POWERLINKV5_20151103070403","2013-01-20T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1022.10153,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1875,"POWERLINKV5_20151103070403","2013-01-20T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-442.75277,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1876,"POWERLINKV5_20151103070403","2013-01-20T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-308.16019,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1877,"POWERLINKV5_20151103070403","2013-01-20T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1021.6072799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1878,"POWERLINKV5_20151103070403","2013-01-20T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1022.37201,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1879,"POWERLINKV5_20151103070403","2013-01-20T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1629.11859,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1880,"POWERLINKV5_20151103070403","2013-01-20T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1194.22253,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1881,"POWERLINKV5_20151103070403","2013-01-20T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-446.66325000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1882,"POWERLINKV5_20151103070403","2013-01-20T12:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.7188000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1883,"POWERLINKV5_20151103070403","2013-01-20T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.6105399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1884,"POWERLINKV5_20151103070403","2013-01-20T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1631.8132599999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1885,"POWERLINKV5_20151103070403","2013-01-20T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1630.4009900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1886,"POWERLINKV5_20151103070403","2013-01-20T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1023.24,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1887,"POWERLINKV5_20151103070403","2013-01-20T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1090.2895000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1888,"POWERLINKV5_20151103070403","2013-01-20T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1027.04395,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1889,"POWERLINKV5_20151103070403","2013-01-20T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.1272899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1890,"POWERLINKV5_20151103070403","2013-01-20T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.9580100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1891,"POWERLINKV5_20151103070403","2013-01-20T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1024.7432699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1892,"POWERLINKV5_20151103070403","2013-01-20T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1024.7893899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1893,"POWERLINKV5_20151103070403","2013-01-20T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1631.35257,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1894,"POWERLINKV5_20151103070403","2013-01-20T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1629.26989,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1895,"POWERLINKV5_20151103070403","2013-01-20T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.71252,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1896,"POWERLINKV5_20151103070403","2013-01-20T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1192.79997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1897,"POWERLINKV5_20151103070403","2013-01-20T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.3090099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1898,"POWERLINKV5_20151103070403","2013-01-20T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1177.6591900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1899,"POWERLINKV5_20151103070403","2013-01-20T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1178.9083800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1900,"POWERLINKV5_20151103070403","2013-01-20T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.99434,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1901,"POWERLINKV5_20151103070403","2013-01-20T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1045.2943399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1902,"POWERLINKV5_20151103070403","2013-01-20T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.5107399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1903,"POWERLINKV5_20151103070403","2013-01-20T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.9915900000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1904,"POWERLINKV5_20151103070403","2013-01-20T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.5092500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1905,"POWERLINKV5_20151103070403","2013-01-20T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.5085099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1906,"POWERLINKV5_20151103070403","2013-01-20T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.98884,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1907,"POWERLINKV5_20151103070403","2013-01-20T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.5077200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1908,"POWERLINKV5_20151103070403","2013-01-20T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.472670000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1909,"POWERLINKV5_20151103070403","2013-01-20T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.50729,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1910,"POWERLINKV5_20151103070403","2013-01-20T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.9943800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1911,"POWERLINKV5_20151103070403","2013-01-20T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.7356600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1912,"POWERLINKV5_20151103070403","2013-01-20T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.50729,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1913,"POWERLINKV5_20151103070403","2013-01-20T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1012.8354,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1914,"POWERLINKV5_20151103070403","2013-01-20T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1105.50729,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1915,"POWERLINKV5_20151103070403","2013-01-20T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.6918499999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1916,"POWERLINKV5_20151103070403","2013-01-20T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1016.01669,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1917,"POWERLINKV5_20151103070403","2013-01-20T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1016.53682,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1918,"POWERLINKV5_20151103070403","2013-01-20T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1206.8117199999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1919,"POWERLINKV5_20151103070403","2013-01-20T15:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1207.83869,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1920,"POWERLINKV5_20151103070403","2013-01-20T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1017.40049,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1921,"POWERLINKV5_20151103070403","2013-01-20T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1019.70575,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1922,"POWERLINKV5_20151103070403","2013-01-20T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1016.83852,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1923,"POWERLINKV5_20151103070403","2013-01-20T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1016.89782,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1924,"POWERLINKV5_20151103070403","2013-01-20T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.01235,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1925,"POWERLINKV5_20151103070403","2013-01-20T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1013.00093,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1926,"POWERLINKV5_20151103070403","2013-01-20T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.660589999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1927,"POWERLINKV5_20151103070403","2013-01-20T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.634340000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1928,"POWERLINKV5_20151103070403","2013-01-20T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1015.83353,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1929,"POWERLINKV5_20151103070403","2013-01-20T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-44.174120000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1930,"POWERLINKV5_20151103070403","2013-01-20T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-43.076410000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1931,"POWERLINKV5_20151103070403","2013-01-20T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.712229999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1932,"POWERLINKV5_20151103070403","2013-01-20T16:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1797.3283300000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1933,"POWERLINKV5_20151103070403","2013-01-20T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.362900000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1934,"POWERLINKV5_20151103070403","2013-01-20T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.006610000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1935,"POWERLINKV5_20151103070403","2013-01-20T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-41.391469999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1936,"POWERLINKV5_20151103070403","2013-01-20T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.314720000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1937,"POWERLINKV5_20151103070403","2013-01-20T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.456409999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1938,"POWERLINKV5_20151103070403","2013-01-20T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.431229999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1939,"POWERLINKV5_20151103070403","2013-01-21T05:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1190.93516,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1940,"POWERLINKV5_20151103070403","2013-01-21T05:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-72.767250000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1941,"POWERLINKV5_20151103070403","2013-01-21T05:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-446.86309,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1942,"POWERLINKV5_20151103070403","2013-01-21T05:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1188.0732,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1943,"POWERLINKV5_20151103070403","2013-01-21T06:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2057.3591500000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1944,"POWERLINKV5_20151103070403","2013-01-21T06:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.8638000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1945,"POWERLINKV5_20151103070403","2013-01-21T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-445.68468999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1946,"POWERLINKV5_20151103070403","2013-01-21T06:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.08473,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1947,"POWERLINKV5_20151103070403","2013-01-21T06:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2057.5049399999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1948,"POWERLINKV5_20151103070403","2013-01-21T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.94856,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1949,"POWERLINKV5_20151103070403","2013-01-21T06:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.0567100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1950,"POWERLINKV5_20151103070403","2013-01-21T06:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.94318,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1951,"POWERLINKV5_20151103070403","2013-01-21T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-442.04770000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1952,"POWERLINKV5_20151103070403","2013-01-21T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-441.97865999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1953,"POWERLINKV5_20151103070403","2013-01-21T06:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1200.27531,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1954,"POWERLINKV5_20151103070403","2013-01-21T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.87607,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1955,"POWERLINKV5_20151103070403","2013-01-21T07:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11753.55616,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1956,"POWERLINKV5_20151103070403","2013-01-21T07:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.1305299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1957,"POWERLINKV5_20151103070403","2013-01-21T07:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1169.3475699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1958,"POWERLINKV5_20151103070403","2013-01-21T07:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-3347.01287,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1959,"POWERLINKV5_20151103070403","2013-01-21T08:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-23.119289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1960,"POWERLINKV5_20151103070403","2013-01-21T09:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11736.71776,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1961,"POWERLINKV5_20151103070403","2013-01-21T09:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1211.16066,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1962,"POWERLINKV5_20151103070403","2013-01-21T09:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-433.76969000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1963,"POWERLINKV5_20151103070403","2013-01-21T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1205.1572000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1964,"POWERLINKV5_20151103070403","2013-01-21T09:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-301.65719000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1965,"POWERLINKV5_20151103070403","2013-01-21T10:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.82448,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1966,"POWERLINKV5_20151103070403","2013-01-21T10:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-432.22575000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1967,"POWERLINKV5_20151103070403","2013-01-21T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.05725000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1968,"POWERLINKV5_20151103070403","2013-01-21T10:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-300.93326999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1969,"POWERLINKV5_20151103070403","2013-01-21T10:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-301.51346999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1970,"POWERLINKV5_20151103070403","2013-01-21T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.659960000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1971,"POWERLINKV5_20151103070403","2013-01-21T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.99754000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1972,"POWERLINKV5_20151103070403","2013-01-21T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-300.71271000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1973,"POWERLINKV5_20151103070403","2013-01-21T11:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-297.91883999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1974,"POWERLINKV5_20151103070403","2013-01-21T11:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.99952999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1975,"POWERLINKV5_20151103070403","2013-01-21T11:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.37848000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1976,"POWERLINKV5_20151103070403","2013-01-21T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.56792000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1977,"POWERLINKV5_20151103070403","2013-01-21T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.89238,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1978,"POWERLINKV5_20151103070403","2013-01-21T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.45058,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1979,"POWERLINKV5_20151103070403","2013-01-21T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1011.1808600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1980,"POWERLINKV5_20151103070403","2013-01-21T11:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.6471799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1981,"POWERLINKV5_20151103070403","2013-01-21T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11725.113009999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1982,"POWERLINKV5_20151103070403","2013-01-21T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1012.01938,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1983,"POWERLINKV5_20151103070403","2013-01-21T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-304.31851999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1984,"POWERLINKV5_20151103070403","2013-01-21T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1011.89138,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1985,"POWERLINKV5_20151103070403","2013-01-21T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.019769999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1986,"POWERLINKV5_20151103070403","2013-01-21T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.35413999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1987,"POWERLINKV5_20151103070403","2013-01-21T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-300.29888999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1988,"POWERLINKV5_20151103070403","2013-01-21T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-303.09604000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1989,"POWERLINKV5_20151103070403","2013-01-21T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.129989999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1990,"POWERLINKV5_20151103070403","2013-01-21T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.548220000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1991,"POWERLINKV5_20151103070403","2013-01-21T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.608809999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1992,"POWERLINKV5_20151103070403","2013-01-21T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.590420000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1993,"POWERLINKV5_20151103070403","2013-01-21T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.565710000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1994,"POWERLINKV5_20151103070403","2013-01-21T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.248130000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1995,"POWERLINKV5_20151103070403","2013-01-21T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1010.20481,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1996,"POWERLINKV5_20151103070403","2013-01-21T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.40343000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1997,"POWERLINKV5_20151103070403","2013-01-21T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.12491,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1998,"POWERLINKV5_20151103070403","2013-01-21T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.60322,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[1999,"POWERLINKV5_20151103070403","2013-01-21T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-297.67111999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2000,"POWERLINKV5_20151103070403","2013-01-21T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.82145000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2004,"POWERLINKV5_20151103070403","2013-01-21T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.569699999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2007,"POWERLINKV5_20151103070403","2013-01-21T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-299.46373,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2011,"POWERLINKV5_20151103070403","2013-01-21T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1215.3463099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2014,"POWERLINKV5_20151103070403","2013-01-21T15:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.720350000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2017,"POWERLINKV5_20151103070403","2013-01-21T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.91460999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2018,"POWERLINKV5_20151103070403","2013-01-21T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.36259999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2021,"POWERLINKV5_20151103070403","2013-01-21T16:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.32329,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2025,"POWERLINKV5_20151103070403","2013-01-21T16:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-298.41955999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2028,"POWERLINKV5_20151103070403","2013-01-21T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-297.87817000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2031,"POWERLINKV5_20151103070403","2013-01-21T21:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.15123,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2035,"POWERLINKV5_20151103070403","2013-01-21T22:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.89508,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2037,"POWERLINKV5_20151103070403","2013-01-21T22:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-305.62281999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2042,"POWERLINKV5_20151103070403","2013-01-22T03:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-269.15282000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2043,"POWERLINKV5_20151103070403","2013-01-22T06:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2060.1800199999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2046,"POWERLINKV5_20151103070403","2013-01-22T06:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2056.4648200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2050,"POWERLINKV5_20151103070403","2013-01-22T06:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.25515,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2053,"POWERLINKV5_20151103070403","2013-01-22T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1997.00748,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2056,"POWERLINKV5_20151103070403","2013-01-22T07:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-264.41320000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2060,"POWERLINKV5_20151103070403","2013-01-22T11:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1215.3042399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2063,"POWERLINKV5_20151103070403","2013-01-22T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-404.07709,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2064,"POWERLINKV5_20151103070403","2013-01-22T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.055700000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2067,"POWERLINKV5_20151103070403","2013-01-22T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-403.14971000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2070,"POWERLINKV5_20151103070403","2013-01-22T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-406.61592000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2074,"POWERLINKV5_20151103070403","2013-01-22T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-434.44243999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2078,"POWERLINKV5_20151103070403","2013-01-22T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1012.56321,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2081,"POWERLINKV5_20151103070403","2013-01-22T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-433.80939000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2085,"POWERLINKV5_20151103070403","2013-01-22T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1210.84097,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2088,"POWERLINKV5_20151103070403","2013-01-22T13:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-58.907400000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2089,"POWERLINKV5_20151103070403","2013-01-22T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.874450000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2092,"POWERLINKV5_20151103070403","2013-01-22T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-39.435180000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2095,"POWERLINKV5_20151103070403","2013-01-22T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1208.0485699999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2099,"POWERLINKV5_20151103070403","2013-01-22T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-40.3322,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2102,"POWERLINKV5_20151103070403","2013-01-22T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.28271999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2105,"POWERLINKV5_20151103070403","2013-01-22T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.60523999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2109,"POWERLINKV5_20151103070403","2013-01-24T09:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-436.97392000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2112,"POWERLINKV5_20151103070403","2013-01-24T12:50:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-226.37387000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2113,"POWERLINKV5_20151103070403","2013-01-24T12:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-226.84461999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2119,"POWERLINKV5_20151103070403","2013-01-25T08:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9897599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2120,"POWERLINKV5_20151103070403","2013-01-25T08:15:00","Q>NIL_CLBCN_7349","Q-NIL","2012-07-01",1,-1285.9917399999999,"Out= Nil, avoid overload on 7349 T13 Chinchilla to T194 Columboola 132kV line on trip of 7350 T13 Chinchilla to T194 Columboola 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2124,"POWERLINKV5_20151103070403","2013-01-25T08:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.6621399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2127,"POWERLINKV5_20151103070403","2013-01-25T08:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9884400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2131,"POWERLINKV5_20151103070403","2013-01-25T09:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.7338099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2134,"POWERLINKV5_20151103070403","2013-01-25T09:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.3727799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2137,"POWERLINKV5_20151103070403","2013-01-25T09:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8987299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2138,"POWERLINKV5_20151103070403","2013-01-25T09:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.35878,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2141,"POWERLINKV5_20151103070403","2013-01-25T10:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.66778,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2144,"POWERLINKV5_20151103070403","2013-01-25T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.0085999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2148,"POWERLINKV5_20151103070403","2013-01-26T10:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8525199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2151,"POWERLINKV5_20151103070403","2013-01-26T10:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.30305,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2155,"POWERLINKV5_20151103070403","2013-01-26T10:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.2468200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2156,"POWERLINKV5_20151103070403","2013-01-26T10:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8978,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2162,"POWERLINKV5_20151103070403","2013-01-26T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.40778,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2163,"POWERLINKV5_20151103070403","2013-01-26T11:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.35547,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2166,"POWERLINKV5_20151103070403","2013-01-27T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.09458,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2170,"POWERLINKV5_20151103070403","2013-01-27T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.9919400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2173,"POWERLINKV5_20151103070403","2013-01-27T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.6735699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2176,"POWERLINKV5_20151103070403","2013-01-27T09:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1155.0319400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2180,"POWERLINKV5_20151103070403","2013-01-27T10:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.3076900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2183,"POWERLINKV5_20151103070403","2013-01-27T10:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1063.4160199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2186,"POWERLINKV5_20151103070403","2013-01-27T10:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1071.9927600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2187,"POWERLINKV5_20151103070403","2013-01-27T10:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.89978,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2190,"POWERLINKV5_20151103070403","2013-01-27T10:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.89978,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2194,"POWERLINKV5_20151103070403","2013-01-27T11:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.26953,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2197,"POWERLINKV5_20151103070403","2013-01-27T11:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.90194,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2201,"POWERLINKV5_20151103070403","2013-01-27T11:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1064.4058600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2205,"POWERLINKV5_20151103070403","2013-01-27T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.9919400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2208,"POWERLINKV5_20151103070403","2013-01-27T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.3873100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2211,"POWERLINKV5_20151103070403","2013-01-27T12:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.90194,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2212,"POWERLINKV5_20151103070403","2013-01-27T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.89978,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2215,"POWERLINKV5_20151103070403","2013-01-27T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.90047,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2219,"POWERLINKV5_20151103070403","2013-01-27T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1155.02964,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2222,"POWERLINKV5_20151103070403","2013-01-27T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.98874,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2225,"POWERLINKV5_20151103070403","2013-01-27T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1195.05846,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2229,"POWERLINKV5_20151103070403","2013-01-27T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.9884500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2232,"POWERLINKV5_20151103070403","2013-01-27T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1195.05846,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2233,"POWERLINKV5_20151103070403","2013-01-27T17:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1299.98846,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2238,"POWERLINKV5_20151103070403","2013-01-27T18:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.8984599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2240,"POWERLINKV5_20151103070403","2013-01-27T18:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1155.02846,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2244,"POWERLINKV5_20151103070403","2013-01-27T19:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.4047599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2247,"POWERLINKV5_20151103070403","2013-01-27T19:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.89797,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2250,"POWERLINKV5_20151103070403","2013-01-27T20:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.39769,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2254,"POWERLINKV5_20151103070403","2013-01-27T20:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.9884500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2257,"POWERLINKV5_20151103070403","2013-01-27T20:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1299.98874,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2258,"POWERLINKV5_20151103070403","2013-01-27T20:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1299.98885,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2261,"POWERLINKV5_20151103070403","2013-01-27T21:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1155.02874,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2264,"POWERLINKV5_20151103070403","2013-01-27T21:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.6356800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2268,"POWERLINKV5_20151103070403","2013-01-27T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1080.1954599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2271,"POWERLINKV5_20151103070403","2013-01-27T21:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.4350199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2274,"POWERLINKV5_20151103070403","2013-01-27T22:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1299.9918500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2279,"POWERLINKV5_20151103070403","2013-01-27T22:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.12536,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2282,"POWERLINKV5_20151103070403","2013-01-27T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.0247999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2283,"POWERLINKV5_20151103070403","2013-01-27T22:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.7912899999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2286,"POWERLINKV5_20151103070403","2013-01-27T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9916800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2289,"POWERLINKV5_20151103070403","2013-01-27T23:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.7971700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2293,"POWERLINKV5_20151103070403","2013-01-28T11:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1099.99107,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2296,"POWERLINKV5_20151103070403","2013-01-28T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.0301099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2300,"POWERLINKV5_20151103070403","2013-01-28T12:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9001699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2303,"POWERLINKV5_20151103070403","2013-01-28T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9001699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2306,"POWERLINKV5_20151103070403","2013-01-28T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9010699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2307,"POWERLINKV5_20151103070403","2013-01-28T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9010699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2310,"POWERLINKV5_20151103070403","2013-01-28T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9001699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2313,"POWERLINKV5_20151103070403","2013-01-28T13:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.8992699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2316,"POWERLINKV5_20151103070403","2013-01-28T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.98927,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2321,"POWERLINKV5_20151103070403","2013-01-28T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.26106,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2325,"POWERLINKV5_20151103070403","2013-01-28T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1143.55935,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2328,"POWERLINKV5_20151103070403","2013-01-28T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1143.55935,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2331,"POWERLINKV5_20151103070403","2013-01-28T21:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9894400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2332,"POWERLINKV5_20151103070403","2013-01-28T21:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9894400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2335,"POWERLINKV5_20151103070403","2013-01-28T21:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.8993,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2339,"POWERLINKV5_20151103070403","2013-01-28T21:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.8993700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2342,"POWERLINKV5_20151103070403","2013-01-28T22:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1286.9208799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2345,"POWERLINKV5_20151103070403","2013-01-28T22:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.9917800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2349,"POWERLINKV5_20151103070403","2013-01-28T22:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.3342700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2352,"POWERLINKV5_20151103070403","2013-01-28T22:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.49494,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2355,"POWERLINKV5_20151103070403","2013-01-28T23:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.9132300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2357,"POWERLINKV5_20151103070403","2013-01-28T23:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.41292,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2360,"POWERLINKV5_20151103070403","2013-01-28T23:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.6713,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2364,"POWERLINKV5_20151103070403","2013-01-28T23:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.9788799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2367,"POWERLINKV5_20151103070403","2013-01-29T07:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1090.02154,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2370,"POWERLINKV5_20151103070403","2013-01-29T07:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1090.0213699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2374,"POWERLINKV5_20151103070403","2013-01-29T07:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1155.03162,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2377,"POWERLINKV5_20151103070403","2013-01-29T08:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1286.9215300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2380,"POWERLINKV5_20151103070403","2013-01-29T08:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1299.99117,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2381,"POWERLINKV5_20151103070403","2013-01-29T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.8815300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2384,"POWERLINKV5_20151103070403","2013-01-29T08:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.54045,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2388,"POWERLINKV5_20151103070403","2013-01-29T09:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.6586,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2391,"POWERLINKV5_20151103070403","2013-01-29T22:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.65876,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2394,"POWERLINKV5_20151103070403","2013-01-29T22:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.7441200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2398,"POWERLINKV5_20151103070403","2013-01-29T22:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.1502,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2402,"POWERLINKV5_20151103070403","2013-01-30T07:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-196.88,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2403,"POWERLINKV5_20151103070403","2013-01-30T07:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-196.88,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2406,"POWERLINKV5_20151103070403","2013-01-31T08:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-59.889969999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2409,"POWERLINKV5_20151103070403","2013-01-31T08:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-94.89,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2413,"POWERLINKV5_20151103070403","2013-02-01T08:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-53.826099999999997,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2416,"POWERLINKV5_20151103070403","2013-02-01T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-285.98,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2419,"POWERLINKV5_20151103070403","2013-02-01T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-299.98023999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2423,"POWERLINKV5_20151103070403","2013-02-01T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-53.33014,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2426,"POWERLINKV5_20151103070403","2013-02-01T17:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-53.664540000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2427,"POWERLINKV5_20151103070403","2013-02-01T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-53.185870000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2430,"POWERLINKV5_20151103070403","2013-02-01T18:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-52.000030000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2435,"POWERLINKV5_20151103070403","2013-02-03T13:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1813.1997899999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2438,"POWERLINKV5_20151103070403","2013-02-03T13:25:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-12.128310000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2441,"POWERLINKV5_20151103070403","2013-02-03T14:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-10.823040000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2445,"POWERLINKV5_20151103070403","2013-02-03T15:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-12.34112,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2448,"POWERLINKV5_20151103070403","2013-02-03T15:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-12.18121,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2451,"POWERLINKV5_20151103070403","2013-02-03T17:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-89.483549999999994,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2452,"POWERLINKV5_20151103070403","2013-02-03T17:05:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-81.861720000000005,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2455,"POWERLINKV5_20151103070403","2013-02-04T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.61337,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2458,"POWERLINKV5_20151103070403","2013-02-04T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.1178399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2462,"POWERLINKV5_20151103070403","2013-02-04T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1071.4492399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2465,"POWERLINKV5_20151103070403","2013-02-04T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.7166400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2469,"POWERLINKV5_20151103070403","2013-02-04T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.01125,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2472,"POWERLINKV5_20151103070403","2013-02-04T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1285.99125,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2476,"POWERLINKV5_20151103070403","2013-02-04T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.31663,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2477,"POWERLINKV5_20151103070403","2013-02-04T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.33177,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2480,"POWERLINKV5_20151103070403","2013-02-04T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.2403099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2483,"POWERLINKV5_20151103070403","2013-02-04T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.4106400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2487,"POWERLINKV5_20151103070403","2013-02-04T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.85132,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2490,"POWERLINKV5_20151103070403","2013-02-05T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.80805,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2494,"POWERLINKV5_20151103070403","2013-02-05T16:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12092.78429,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2497,"POWERLINKV5_20151103070403","2013-02-05T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1039.59159,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2500,"POWERLINKV5_20151103070403","2013-02-05T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.03071,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2501,"POWERLINKV5_20151103070403","2013-02-05T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.818,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2504,"POWERLINKV5_20151103070403","2013-02-05T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.5154500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2508,"POWERLINKV5_20151103070403","2013-02-05T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.0664999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2511,"POWERLINKV5_20151103070403","2013-02-05T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.7442799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2513,"POWERLINKV5_20151103070403","2013-02-05T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.5708999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2519,"POWERLINKV5_20151103070403","2013-02-05T17:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.63004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2522,"POWERLINKV5_20151103070403","2013-02-05T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.21081,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2525,"POWERLINKV5_20151103070403","2013-02-05T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.1099099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2526,"POWERLINKV5_20151103070403","2013-02-05T18:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.0007499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2529,"POWERLINKV5_20151103070403","2013-02-07T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.87988,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2533,"POWERLINKV5_20151103070403","2013-02-07T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.72466,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2536,"POWERLINKV5_20151103070403","2013-02-07T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.28868,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2539,"POWERLINKV5_20151103070403","2013-02-07T17:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.1436200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2543,"POWERLINKV5_20151103070403","2013-02-07T17:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.6410800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2546,"POWERLINKV5_20151103070403","2013-02-07T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.02648,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2549,"POWERLINKV5_20151103070403","2013-02-07T18:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.21011,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2550,"POWERLINKV5_20151103070403","2013-02-07T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.3993599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2554,"POWERLINKV5_20151103070403","2013-02-07T18:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.7442900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2558,"POWERLINKV5_20151103070403","2013-02-08T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.4024300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2561,"POWERLINKV5_20151103070403","2013-02-08T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-268.95487000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2564,"POWERLINKV5_20151103070403","2013-02-08T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1035.83268,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2568,"POWERLINKV5_20151103070403","2013-02-08T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-961.20614,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2571,"POWERLINKV5_20151103070403","2013-02-08T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-34.412820000000004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2572,"POWERLINKV5_20151103070403","2013-02-08T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1189.4388899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2575,"POWERLINKV5_20151103070403","2013-02-08T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-946.69653000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2578,"POWERLINKV5_20151103070403","2013-02-08T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.4141,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2582,"POWERLINKV5_20151103070403","2013-02-08T14:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1045.4836600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2585,"POWERLINKV5_20151103070403","2013-02-08T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1045.9321299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2588,"POWERLINKV5_20151103070403","2013-02-08T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-36.274259999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2592,"POWERLINKV5_20151103070403","2013-02-08T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-56.826900000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2595,"POWERLINKV5_20151103070403","2013-02-08T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-990.89919999999995,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2597,"POWERLINKV5_20151103070403","2013-02-08T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-991.63376000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2600,"POWERLINKV5_20151103070403","2013-02-08T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-24.970510000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2603,"POWERLINKV5_20151103070403","2013-02-08T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-51.094889999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2607,"POWERLINKV5_20151103070403","2013-02-08T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.95388,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2610,"POWERLINKV5_20151103070403","2013-02-08T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1046.8772100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2614,"POWERLINKV5_20151103070403","2013-02-08T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2151.0227,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2617,"POWERLINKV5_20151103070403","2013-02-08T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1011.73726,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2620,"POWERLINKV5_20151103070403","2013-02-08T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-137.52886000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2621,"POWERLINKV5_20151103070403","2013-02-08T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1038.61556,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2624,"POWERLINKV5_20151103070403","2013-02-08T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1045.43866,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2627,"POWERLINKV5_20151103070403","2013-02-08T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-6457.6427000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2631,"POWERLINKV5_20151103070403","2013-02-08T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.9887000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2636,"POWERLINKV5_20151103070403","2013-02-08T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1159.9560799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2639,"POWERLINKV5_20151103070403","2013-02-08T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.9883600000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2642,"POWERLINKV5_20151103070403","2013-02-08T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.9941200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2645,"POWERLINKV5_20151103070403","2013-02-08T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1029.98903,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2646,"POWERLINKV5_20151103070403","2013-02-08T17:05:00","Q>NIL_MRTA_A","Q-NIL","2012-09-06",1,-920.80903999999998,"Out = Nil, Oakey PS constrained to the emergency rating of 731 Middle Ridge to Tangkam 110kV line.","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2649,"POWERLINKV5_20151103070403","2013-02-08T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-840.57914000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2652,"POWERLINKV5_20151103070403","2013-02-08T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.829660000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2656,"POWERLINKV5_20151103070403","2013-02-08T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-723.92120999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2659,"POWERLINKV5_20151103070403","2013-02-08T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-113.94134,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2663,"POWERLINKV5_20151103070403","2013-02-09T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-729.25012000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2666,"POWERLINKV5_20151103070403","2013-02-09T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-731.87348999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2669,"POWERLINKV5_20151103070403","2013-02-09T13:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-728.81696999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2670,"POWERLINKV5_20151103070403","2013-02-09T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-729.45219999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2673,"POWERLINKV5_20151103070403","2013-02-09T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1014.14981,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2678,"POWERLINKV5_20151103070403","2013-02-09T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.08888,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2681,"POWERLINKV5_20151103070403","2013-02-09T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1014.60059,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2684,"POWERLINKV5_20151103070403","2013-02-09T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-335.27231,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2688,"POWERLINKV5_20151103070403","2013-02-09T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-821.26661999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2691,"POWERLINKV5_20151103070403","2013-02-09T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-918.48847999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2694,"POWERLINKV5_20151103070403","2013-02-09T14:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-792.19226000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2695,"POWERLINKV5_20151103070403","2013-02-09T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-918.63940000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2698,"POWERLINKV5_20151103070403","2013-02-09T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-725.62027,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2702,"POWERLINKV5_20151103070403","2013-02-09T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-31.17286,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2705,"POWERLINKV5_20151103070403","2013-02-09T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1035.9357600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2708,"POWERLINKV5_20151103070403","2013-02-09T15:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-201.01884999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2712,"POWERLINKV5_20151103070403","2013-02-09T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-730.14873999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2714,"POWERLINKV5_20151103070403","2013-02-09T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-730.45471999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2719,"POWERLINKV5_20151103070403","2013-02-09T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1013.71613,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2720,"POWERLINKV5_20151103070403","2013-02-09T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-116.24973,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2723,"POWERLINKV5_20151103070403","2013-02-09T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.1626900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2727,"POWERLINKV5_20151103070403","2013-02-09T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1014.99059,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2730,"POWERLINKV5_20151103070403","2013-02-09T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-729.38242000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2733,"POWERLINKV5_20151103070403","2013-02-09T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1015.56736,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2737,"POWERLINKV5_20151103070403","2013-02-09T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.263489999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2740,"POWERLINKV5_20151103070403","2013-02-09T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1046.59536,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2741,"POWERLINKV5_20151103070403","2013-02-09T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.37082,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2744,"POWERLINKV5_20151103070403","2013-02-09T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1046.5972200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2747,"POWERLINKV5_20151103070403","2013-02-09T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.57141,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2751,"POWERLINKV5_20151103070403","2013-02-09T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-253.78198,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2755,"POWERLINKV5_20151103070403","2013-02-09T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-18.71312,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2758,"POWERLINKV5_20151103070403","2013-02-09T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.9372000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2762,"POWERLINKV5_20151103070403","2013-02-09T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.836,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2765,"POWERLINKV5_20151103070403","2013-02-09T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.2660000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2766,"POWERLINKV5_20151103070403","2013-02-09T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-14.56644,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2769,"POWERLINKV5_20151103070403","2013-02-09T18:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.5502100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2772,"POWERLINKV5_20151103070403","2013-02-09T18:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.03478,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2776,"POWERLINKV5_20151103070403","2013-02-09T19:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-229.50058000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2779,"POWERLINKV5_20151103070403","2013-02-09T21:15:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-82.481080000000006,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2783,"POWERLINKV5_20151103070403","2013-02-09T21:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-235.04131000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2786,"POWERLINKV5_20151103070403","2013-02-10T11:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-271.18288000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2789,"POWERLINKV5_20151103070403","2013-02-10T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-103.81631,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2790,"POWERLINKV5_20151103070403","2013-02-10T11:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-709.49104,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2796,"POWERLINKV5_20151103070403","2013-02-10T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.28407,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2797,"POWERLINKV5_20151103070403","2013-02-10T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1041.1565499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2801,"POWERLINKV5_20151103070403","2013-02-10T12:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.11884,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2804,"POWERLINKV5_20151103070403","2013-02-10T12:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-452.61333999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2808,"POWERLINKV5_20151103070403","2013-02-10T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-453.16969,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2811,"POWERLINKV5_20151103070403","2013-02-10T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-998.03722000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2814,"POWERLINKV5_20151103070403","2013-02-10T12:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-113.52919,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2815,"POWERLINKV5_20151103070403","2013-02-10T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1058.3509100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2818,"POWERLINKV5_20151103070403","2013-02-10T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1099.4932899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2821,"POWERLINKV5_20151103070403","2013-02-10T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1011.17296,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2825,"POWERLINKV5_20151103070403","2013-02-10T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-861.30727000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2828,"POWERLINKV5_20151103070403","2013-02-10T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-999.77702999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2833,"POWERLINKV5_20151103070403","2013-02-10T13:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-951.18101999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2836,"POWERLINKV5_20151103070403","2013-02-10T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-951.18113000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2839,"POWERLINKV5_20151103070403","2013-02-10T13:55:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-816.78035999999997,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2840,"POWERLINKV5_20151103070403","2013-02-10T13:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-448.25177000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2843,"POWERLINKV5_20151103070403","2013-02-10T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1044.9908600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2847,"POWERLINKV5_20151103070403","2013-02-10T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1037.9764600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2850,"POWERLINKV5_20151103070403","2013-02-10T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-80.020809999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2853,"POWERLINKV5_20151103070403","2013-02-10T14:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1045.6866,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2857,"POWERLINKV5_20151103070403","2013-02-10T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1028.5038999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2860,"POWERLINKV5_20151103070403","2013-02-10T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-102.94182000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2863,"POWERLINKV5_20151103070403","2013-02-10T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1028.12148,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2864,"POWERLINKV5_20151103070403","2013-02-10T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-448.05083999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2867,"POWERLINKV5_20151103070403","2013-02-10T15:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1028.10303,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2870,"POWERLINKV5_20151103070403","2013-02-10T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1028.83204,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2875,"POWERLINKV5_20151103070403","2013-02-10T15:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-725.43952999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2878,"POWERLINKV5_20151103070403","2013-02-10T16:00:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1820.1498999999999,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2882,"POWERLINKV5_20151103070403","2013-02-10T16:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-899.94524000000001,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2885,"POWERLINKV5_20151103070403","2013-02-10T16:20:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-901.00161000000003,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2886,"POWERLINKV5_20151103070403","2013-02-10T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.19292,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2889,"POWERLINKV5_20151103070403","2013-02-12T14:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-11.79238,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2892,"POWERLINKV5_20151103070403","2013-02-12T15:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-31.75543,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2896,"POWERLINKV5_20151103070403","2013-02-12T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-698.12656000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2899,"POWERLINKV5_20151103070403","2013-02-12T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-718.33849999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2902,"POWERLINKV5_20151103070403","2013-02-12T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1023.58726,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2906,"POWERLINKV5_20151103070403","2013-02-12T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1023.53198,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2909,"POWERLINKV5_20151103070403","2013-02-12T16:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1021.76744,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2911,"POWERLINKV5_20151103070403","2013-02-12T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-266.20285999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2914,"POWERLINKV5_20151103070403","2013-02-12T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.929139999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2917,"POWERLINKV5_20151103070403","2013-02-12T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-38.451030000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2921,"POWERLINKV5_20151103070403","2013-02-12T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-34.44632,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2924,"POWERLINKV5_20151103070403","2013-02-13T07:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.9022600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2927,"POWERLINKV5_20151103070403","2013-02-13T07:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.30512,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2931,"POWERLINKV5_20151103070403","2013-02-13T08:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.95607,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2934,"POWERLINKV5_20151103070403","2013-02-13T08:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.8662300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2935,"POWERLINKV5_20151103070403","2013-02-13T08:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.2922599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2938,"POWERLINKV5_20151103070403","2013-02-13T08:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.7539899999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2941,"POWERLINKV5_20151103070403","2013-02-13T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.92895,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2945,"POWERLINKV5_20151103070403","2013-02-13T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1057.9541999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2948,"POWERLINKV5_20151103070403","2013-02-13T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.80852,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2952,"POWERLINKV5_20151103070403","2013-02-13T09:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.7181399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2956,"POWERLINKV5_20151103070403","2013-02-13T10:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.2091800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2959,"POWERLINKV5_20151103070403","2013-02-13T10:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1092.9012499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2960,"POWERLINKV5_20151103070403","2013-02-13T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.0012200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2963,"POWERLINKV5_20151103070403","2013-02-13T10:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1065.9120600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2966,"POWERLINKV5_20151103070403","2013-02-13T10:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-21.105740000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2970,"POWERLINKV5_20151103070403","2013-02-13T11:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.0148799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2973,"POWERLINKV5_20151103070403","2013-02-13T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.7212999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2977,"POWERLINKV5_20151103070403","2013-02-13T11:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.36419,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2980,"POWERLINKV5_20151103070403","2013-02-13T11:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.0229200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2983,"POWERLINKV5_20151103070403","2013-02-13T12:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1061.06818,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2984,"POWERLINKV5_20151103070403","2013-02-13T12:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.0229200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2987,"POWERLINKV5_20151103070403","2013-02-13T12:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.6898699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2993,"POWERLINKV5_20151103070403","2013-02-13T12:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1016.06429,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2995,"POWERLINKV5_20151103070403","2013-02-13T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.9507599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[2998,"POWERLINKV5_20151103070403","2013-02-13T12:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-64.636799999999994,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3002,"POWERLINKV5_20151103070403","2013-02-13T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-64.115939999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3005,"POWERLINKV5_20151103070403","2013-02-13T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.8039100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3008,"POWERLINKV5_20151103070403","2013-02-13T13:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.11916,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3009,"POWERLINKV5_20151103070403","2013-02-13T13:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-65.054079999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3012,"POWERLINKV5_20151103070403","2013-02-13T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.22191,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3016,"POWERLINKV5_20151103070403","2013-02-13T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1008.8181499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3019,"POWERLINKV5_20151103070403","2013-02-13T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-967.16863999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3022,"POWERLINKV5_20151103070403","2013-02-13T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2059.0840800000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3026,"POWERLINKV5_20151103070403","2013-02-13T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.09932,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3029,"POWERLINKV5_20151103070403","2013-02-13T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.0517199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3030,"POWERLINKV5_20151103070403","2013-02-13T14:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.28568,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3034,"POWERLINKV5_20151103070403","2013-02-13T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.73549,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3037,"POWERLINKV5_20151103070403","2013-02-13T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1189.03532,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3041,"POWERLINKV5_20151103070403","2013-02-13T14:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.9096,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3044,"POWERLINKV5_20151103070403","2013-02-13T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.1686500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3047,"POWERLINKV5_20151103070403","2013-02-13T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.09432,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3051,"POWERLINKV5_20151103070403","2013-02-13T15:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.5562,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3054,"POWERLINKV5_20151103070403","2013-02-13T15:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.13903,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3055,"POWERLINKV5_20151103070403","2013-02-13T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.5406,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3058,"POWERLINKV5_20151103070403","2013-02-13T15:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.1608100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3061,"POWERLINKV5_20151103070403","2013-02-13T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.68822,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3065,"POWERLINKV5_20151103070403","2013-02-13T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.8214,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3068,"POWERLINKV5_20151103070403","2013-02-13T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8092899999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3071,"POWERLINKV5_20151103070403","2013-02-13T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.0228099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3076,"POWERLINKV5_20151103070403","2013-02-13T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-985.67394000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3079,"POWERLINKV5_20151103070403","2013-02-13T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.282780000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3080,"POWERLINKV5_20151103070403","2013-02-13T17:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.9134799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3083,"POWERLINKV5_20151103070403","2013-02-13T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.88733,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3086,"POWERLINKV5_20151103070403","2013-02-13T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.72387,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3090,"POWERLINKV5_20151103070403","2013-02-13T18:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-12.025690000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3093,"POWERLINKV5_20151103070403","2013-02-13T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.5553600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3096,"POWERLINKV5_20151103070403","2013-02-13T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.8141499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3100,"POWERLINKV5_20151103070403","2013-02-13T18:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.5164600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3103,"POWERLINKV5_20151103070403","2013-02-13T19:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.96263,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3104,"POWERLINKV5_20151103070403","2013-02-13T19:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.97055,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3107,"POWERLINKV5_20151103070403","2013-02-13T19:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.7006100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3112,"POWERLINKV5_20151103070403","2013-02-13T19:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.47603,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3115,"POWERLINKV5_20151103070403","2013-02-13T20:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.4218599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3118,"POWERLINKV5_20151103070403","2013-02-14T10:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.92002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3122,"POWERLINKV5_20151103070403","2013-02-14T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-25.632989999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3125,"POWERLINKV5_20151103070403","2013-02-14T10:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-995.86769000000004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3128,"POWERLINKV5_20151103070403","2013-02-14T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-2042.46667,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3129,"POWERLINKV5_20151103070403","2013-02-14T10:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-990.21423000000004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3132,"POWERLINKV5_20151103070403","2013-02-14T10:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.84476,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3135,"POWERLINKV5_20151103070403","2013-02-14T10:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1007.04099,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3139,"POWERLINKV5_20151103070403","2013-02-14T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1198.2423100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3142,"POWERLINKV5_20151103070403","2013-02-14T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-19.530180000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3146,"POWERLINKV5_20151103070403","2013-02-14T11:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2013-02-14",1,127.63108,"N-Q-MNSP1.ENERGY * -1 >= 90 (Wt = 0.01)","OUTAGE","OTHER","Feeder 96H - TransGrid","REGULATED","99","AEMO Invoked constraint to manage Terranora Interconnector oscillations, due to an outage on Feeder 96H by TransGrid. Refer to Market Notice 41471.","UNPLANNED",0]
[3149,"POWERLINKV5_20151103070403","2013-02-14T11:30:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2013-02-14",1,111.83687,"N-Q-MNSP1.ENERGY * -1 >= 90 (Wt = 0.01)","OUTAGE","OTHER","Feeder 96H - TransGrid","REGULATED","99","AEMO Invoked constraint to manage Terranora Interconnector oscillations, due to an outage on Feeder 96H by TransGrid. Refer to Market Notice 41471.","UNPLANNED",0]
[3153,"POWERLINKV5_20151103070403","2013-02-14T11:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.4685899999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3154,"POWERLINKV5_20151103070403","2013-02-14T11:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1005.63027,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3157,"POWERLINKV5_20151103070403","2013-02-14T11:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-840.50166999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3161,"POWERLINKV5_20151103070403","2013-02-14T11:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-991.63121999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3164,"POWERLINKV5_20151103070403","2013-02-14T12:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-10.501289999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3167,"POWERLINKV5_20151103070403","2013-02-14T12:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-840.50046999999995,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3171,"POWERLINKV5_20151103070403","2013-02-14T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1212.5372500000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3174,"POWERLINKV5_20151103070403","2013-02-14T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-940.15860999999995,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3177,"POWERLINKV5_20151103070403","2013-02-14T12:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1016.91323,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3178,"POWERLINKV5_20151103070403","2013-02-14T12:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1196.3456100000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3181,"POWERLINKV5_20151103070403","2013-02-14T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1005.66275,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3185,"POWERLINKV5_20151103070403","2013-02-14T12:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1006.38726,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3188,"POWERLINKV5_20151103070403","2013-02-14T13:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-722.33024999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3190,"POWERLINKV5_20151103070403","2013-02-14T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1201.0271299999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3196,"POWERLINKV5_20151103070403","2013-02-14T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.62871,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3199,"POWERLINKV5_20151103070403","2013-02-14T13:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1009.60245,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3202,"POWERLINKV5_20151103070403","2013-02-14T13:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.85501999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3203,"POWERLINKV5_20151103070403","2013-02-14T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.53542,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3206,"POWERLINKV5_20151103070403","2013-02-14T13:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.08822999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3210,"POWERLINKV5_20151103070403","2013-02-14T14:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-52.474589999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3213,"POWERLINKV5_20151103070403","2013-02-14T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-991.26931000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3216,"POWERLINKV5_20151103070403","2013-02-14T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1039.32753,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3220,"POWERLINKV5_20151103070403","2013-02-14T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1039.1942100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3223,"POWERLINKV5_20151103070403","2013-02-14T14:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1216.4824799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3224,"POWERLINKV5_20151103070403","2013-02-14T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.95095,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3227,"POWERLINKV5_20151103070403","2013-02-14T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1202.32935,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3231,"POWERLINKV5_20151103070403","2013-02-14T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-719.18452000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3235,"POWERLINKV5_20151103070403","2013-02-14T15:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-719.54516999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3238,"POWERLINKV5_20151103070403","2013-02-14T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1013.6755900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3241,"POWERLINKV5_20151103070403","2013-02-14T15:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-691.76054999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3245,"POWERLINKV5_20151103070403","2013-02-14T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-715.19653000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3248,"POWERLINKV5_20151103070403","2013-02-14T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1029.16858,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3249,"POWERLINKV5_20151103070403","2013-02-14T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-715.77724000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3252,"POWERLINKV5_20151103070403","2013-02-14T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1028.35185,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3255,"POWERLINKV5_20151103070403","2013-02-14T15:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-262.46127000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3259,"POWERLINKV5_20151103070403","2013-02-14T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-259.97658000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3262,"POWERLINKV5_20151103070403","2013-02-14T16:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1025.5038500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3265,"POWERLINKV5_20151103070403","2013-02-14T16:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-717.90578000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3268,"POWERLINKV5_20151103070403","2013-02-14T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1026.2917199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3273,"POWERLINKV5_20151103070403","2013-02-14T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-821.26676999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3274,"POWERLINKV5_20151103070403","2013-02-14T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-913.99959000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3277,"POWERLINKV5_20151103070403","2013-02-14T16:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-821.26676999999995,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3280,"POWERLINKV5_20151103070403","2013-02-14T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1038.5342700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3284,"POWERLINKV5_20151103070403","2013-02-14T17:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-327.47178000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3287,"POWERLINKV5_20151103070403","2013-02-14T17:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-693.22806000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3291,"POWERLINKV5_20151103070403","2013-02-14T17:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-994.54214999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3294,"POWERLINKV5_20151103070403","2013-02-14T17:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1029.9564399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3297,"POWERLINKV5_20151103070403","2013-02-14T17:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1203.53306,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3298,"POWERLINKV5_20151103070403","2013-02-14T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1011.5705,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3301,"POWERLINKV5_20151103070403","2013-02-14T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-696.16962999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3304,"POWERLINKV5_20151103070403","2013-02-14T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.0513,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3309,"POWERLINKV5_20151103070403","2013-02-14T18:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1020.64017,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3312,"POWERLINKV5_20151103070403","2013-02-14T18:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-723.44466999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3316,"POWERLINKV5_20151103070403","2013-02-14T18:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-46.060690000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3319,"POWERLINKV5_20151103070403","2013-02-14T18:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1024.2605100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3322,"POWERLINKV5_20151103070403","2013-02-14T18:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-697.57583999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3323,"POWERLINKV5_20151103070403","2013-02-14T18:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1025.0976800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3326,"POWERLINKV5_20151103070403","2013-02-14T19:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.3629900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3330,"POWERLINKV5_20151103070403","2013-02-14T19:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-53.278799999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3333,"POWERLINKV5_20151103070403","2013-02-14T19:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1031.4434900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3336,"POWERLINKV5_20151103070403","2013-02-14T19:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.2533800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3340,"POWERLINKV5_20151103070403","2013-02-14T19:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8019999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3343,"POWERLINKV5_20151103070403","2013-02-14T20:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.0674300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3346,"POWERLINKV5_20151103070403","2013-02-14T20:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.6055799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3350,"POWERLINKV5_20151103070403","2013-02-14T20:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.7011299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3351,"POWERLINKV5_20151103070403","2013-02-14T20:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.61709,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3355,"POWERLINKV5_20151103070403","2013-02-14T21:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1056.21198,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3358,"POWERLINKV5_20151103070403","2013-02-14T21:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.6974700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3361,"POWERLINKV5_20151103070403","2013-02-14T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.7030400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3365,"POWERLINKV5_20151103070403","2013-02-14T22:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.9362900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3368,"POWERLINKV5_20151103070403","2013-02-15T06:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-155.83614,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3371,"POWERLINKV5_20151103070403","2013-02-15T06:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1232.60474,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3372,"POWERLINKV5_20151103070403","2013-02-15T07:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1272.7097799999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3375,"POWERLINKV5_20151103070403","2013-02-15T10:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1204.42266,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3379,"POWERLINKV5_20151103070403","2013-02-15T10:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.91445999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3382,"POWERLINKV5_20151103070403","2013-02-15T10:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.9916700000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3385,"POWERLINKV5_20151103070403","2013-02-15T11:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-309.27823000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3387,"POWERLINKV5_20151103070403","2013-02-15T11:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-57.331139999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3393,"POWERLINKV5_20151103070403","2013-02-15T11:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-802.51454999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3394,"POWERLINKV5_20151103070403","2013-02-15T11:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.4667099999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3397,"POWERLINKV5_20151103070403","2013-02-15T12:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-981.80699000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3400,"POWERLINKV5_20151103070403","2013-02-15T12:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-846.39454999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3404,"POWERLINKV5_20151103070403","2013-02-15T12:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1044.8047200000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3407,"POWERLINKV5_20151103070403","2013-02-15T12:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-843.40571,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3410,"POWERLINKV5_20151103070403","2013-02-15T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-927.24098000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3414,"POWERLINKV5_20151103070403","2013-02-15T13:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-804.00784999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3417,"POWERLINKV5_20151103070403","2013-02-15T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1019.72447,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3418,"POWERLINKV5_20151103070403","2013-02-15T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-721.87207999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3421,"POWERLINKV5_20151103070403","2013-02-15T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.98562,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3424,"POWERLINKV5_20151103070403","2013-02-15T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-804.04105000000004,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3428,"POWERLINKV5_20151103070403","2013-02-15T13:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-808.80205999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3432,"POWERLINKV5_20151103070403","2013-02-15T13:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-722.22742000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3435,"POWERLINKV5_20151103070403","2013-02-15T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.2796499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3439,"POWERLINKV5_20151103070403","2013-02-15T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1014.27225,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3442,"POWERLINKV5_20151103070403","2013-02-15T14:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-722.26140999999996,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3443,"POWERLINKV5_20151103070403","2013-02-15T14:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1021.63706,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3446,"POWERLINKV5_20151103070403","2013-02-15T14:20:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-805.83636000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3449,"POWERLINKV5_20151103070403","2013-02-15T14:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-998.34190999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3453,"POWERLINKV5_20151103070403","2013-02-15T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-914.00139999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3456,"POWERLINKV5_20151103070403","2013-02-15T14:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-28.58831,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3460,"POWERLINKV5_20151103070403","2013-02-15T14:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-483.23978,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3463,"POWERLINKV5_20151103070403","2013-02-15T15:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-861.39099999999996,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3466,"POWERLINKV5_20151103070403","2013-02-15T15:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-981.80723,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3469,"POWERLINKV5_20151103070403","2013-02-15T15:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-843.40484000000004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3471,"POWERLINKV5_20151103070403","2013-02-15T15:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-976.66120999999998,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3474,"POWERLINKV5_20151103070403","2013-02-15T15:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-999.77593000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3478,"POWERLINKV5_20151103070403","2013-02-15T15:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-724.18610000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3481,"POWERLINKV5_20151103070403","2013-02-15T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1023.56897,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3485,"POWERLINKV5_20151103070403","2013-02-15T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1007.27256,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3488,"POWERLINKV5_20151103070403","2013-02-15T16:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1197.5951399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3491,"POWERLINKV5_20151103070403","2013-02-15T16:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.53739,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3492,"POWERLINKV5_20151103070403","2013-02-15T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-722.13277000000005,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3495,"POWERLINKV5_20151103070403","2013-02-15T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1022.16595,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3499,"POWERLINKV5_20151103070403","2013-02-15T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1006.67129,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3502,"POWERLINKV5_20151103070403","2013-02-15T16:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1195.6849400000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3505,"POWERLINKV5_20151103070403","2013-02-15T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1005.25815,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3510,"POWERLINKV5_20151103070403","2013-02-15T17:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-791.68479000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3513,"POWERLINKV5_20151103070403","2013-02-15T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.5777599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3516,"POWERLINKV5_20151103070403","2013-02-15T17:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-15.517580000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3517,"POWERLINKV5_20151103070403","2013-02-15T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.1451099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3520,"POWERLINKV5_20151103070403","2013-02-15T17:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-27.80527,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3524,"POWERLINKV5_20151103070403","2013-02-15T17:35:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-821.26666999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3527,"POWERLINKV5_20151103070403","2013-02-15T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1037.1062300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3530,"POWERLINKV5_20151103070403","2013-02-15T17:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-699.85501999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3534,"POWERLINKV5_20151103070403","2013-02-15T18:00:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.314730000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3537,"POWERLINKV5_20151103070403","2013-02-15T18:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.9473700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3540,"POWERLINKV5_20151103070403","2013-02-15T18:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.9393299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3541,"POWERLINKV5_20151103070403","2013-02-15T18:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.3564200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3544,"POWERLINKV5_20151103070403","2013-02-16T12:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-258.23086000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3547,"POWERLINKV5_20151103070403","2013-02-16T12:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-267.23309,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3552,"POWERLINKV5_20151103070403","2013-02-16T12:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-10.93347,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3555,"POWERLINKV5_20151103070403","2013-02-16T12:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-10.504300000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3559,"POWERLINKV5_20151103070403","2013-02-16T12:50:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-279.48484000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3562,"POWERLINKV5_20151103070403","2013-02-16T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-285.33740999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3563,"POWERLINKV5_20151103070403","2013-02-16T13:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-13.46044,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3566,"POWERLINKV5_20151103070403","2013-02-16T13:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-12.813219999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3569,"POWERLINKV5_20151103070403","2013-02-16T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-273.11928999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3573,"POWERLINKV5_20151103070403","2013-02-16T13:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1030.6245200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3576,"POWERLINKV5_20151103070403","2013-02-16T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1031.2670700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3579,"POWERLINKV5_20151103070403","2013-02-16T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1025.6524300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3583,"POWERLINKV5_20151103070403","2013-02-16T13:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-11.357749999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3586,"POWERLINKV5_20151103070403","2013-02-16T13:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-10.888730000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3588,"POWERLINKV5_20151103070403","2013-02-16T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1031.2446,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3591,"POWERLINKV5_20151103070403","2013-02-16T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1031.2333799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3594,"POWERLINKV5_20151103070403","2013-02-16T13:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-954.25897999999995,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3598,"POWERLINKV5_20151103070403","2013-02-16T14:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-33.708219999999997,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3601,"POWERLINKV5_20151103070403","2013-02-16T14:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1193.71011,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3605,"POWERLINKV5_20151103070403","2013-02-16T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.25956,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3608,"POWERLINKV5_20151103070403","2013-02-16T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1030.05297,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3611,"POWERLINKV5_20151103070403","2013-02-16T14:30:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.31474,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3612,"POWERLINKV5_20151103070403","2013-02-16T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1029.99287,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3615,"POWERLINKV5_20151103070403","2013-02-16T14:40:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-17.241160000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3618,"POWERLINKV5_20151103070403","2013-02-16T14:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1036.9432099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3622,"POWERLINKV5_20151103070403","2013-02-16T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1051.0569,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3625,"POWERLINKV5_20151103070403","2013-02-16T15:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1019.82071,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3629,"POWERLINKV5_20151103070403","2013-02-16T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1027.4596200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3633,"POWERLINKV5_20151103070403","2013-02-16T15:30:00","Q_N_NIL-1078","Q-NIL","2010-12-21",1,-104.77951,"Out= Nil, reduce QNI when it is over the 1078 MW limit by 1078 minus the MW over the 1078 MW limit (capped at 1000 MW)","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3636,"POWERLINKV5_20151103070403","2013-02-16T15:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-935.56110000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3637,"POWERLINKV5_20151103070403","2013-02-16T15:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2012-05-14",1,-44.58108,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3640,"POWERLINKV5_20151103070403","2013-02-16T15:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-448.35487999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3643,"POWERLINKV5_20151103070403","2013-02-16T15:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-984.35008000000005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3647,"POWERLINKV5_20151103070403","2013-02-16T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1010.06548,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3650,"POWERLINKV5_20151103070403","2013-02-16T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-929.26851999999997,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3654,"POWERLINKV5_20151103070403","2013-02-16T16:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-1033.9538399999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3657,"POWERLINKV5_20151103070403","2013-02-16T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-890.24748,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3660,"POWERLINKV5_20151103070403","2013-02-16T16:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-795.96281999999997,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3661,"POWERLINKV5_20151103070403","2013-02-16T16:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-941.60848999999996,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3666,"POWERLINKV5_20151103070403","2013-02-16T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1009.67971,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3669,"POWERLINKV5_20151103070403","2013-02-16T16:45:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-326.25090999999998,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3672,"POWERLINKV5_20151103070403","2013-02-16T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1037.9970699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3675,"POWERLINKV5_20151103070403","2013-02-16T17:05:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-809.78565000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3679,"POWERLINKV5_20151103070403","2013-02-16T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1042.22938,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3682,"POWERLINKV5_20151103070403","2013-02-16T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1043.73479,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3685,"POWERLINKV5_20151103070403","2013-02-16T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.88258,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3686,"POWERLINKV5_20151103070403","2013-02-16T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.00171,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3689,"POWERLINKV5_20151103070403","2013-02-16T17:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-433.08082999999999,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3693,"POWERLINKV5_20151103070403","2013-02-17T13:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-45.089010000000002,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3696,"POWERLINKV5_20151103070403","2013-02-17T14:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.7381700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3699,"POWERLINKV5_20151103070403","2013-02-17T14:15:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-122.50829,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3703,"POWERLINKV5_20151103070403","2013-02-17T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1049.46605,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3707,"POWERLINKV5_20151103070403","2013-02-17T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1048.5021099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3710,"POWERLINKV5_20151103070403","2013-02-17T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.21136,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3711,"POWERLINKV5_20151103070403","2013-02-17T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.3010200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3714,"POWERLINKV5_20151103070403","2013-02-17T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1046.56113,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3718,"POWERLINKV5_20151103070403","2013-02-17T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.23568,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3721,"POWERLINKV5_20151103070403","2013-02-17T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1050.00522,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3724,"POWERLINKV5_20151103070403","2013-02-17T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1047.91983,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3728,"POWERLINKV5_20151103070403","2013-02-17T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1065.68587,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3731,"POWERLINKV5_20151103070403","2013-02-17T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1066.63653,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3732,"POWERLINKV5_20151103070403","2013-02-17T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1052.9789499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3735,"POWERLINKV5_20151103070403","2013-02-17T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1066.63885,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3738,"POWERLINKV5_20151103070403","2013-02-17T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.1093599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3742,"POWERLINKV5_20151103070403","2013-02-17T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.4885099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3744,"POWERLINKV5_20151103070403","2013-02-17T17:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1073.1135300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3749,"POWERLINKV5_20151103070403","2013-02-20T15:10:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-18.26765,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3753,"POWERLINKV5_20151103070403","2013-02-20T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-14.06475,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3756,"POWERLINKV5_20151103070403","2013-02-20T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.4388799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3757,"POWERLINKV5_20151103070403","2013-02-20T17:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.86798,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3760,"POWERLINKV5_20151103070403","2013-02-20T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1058.16984,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3763,"POWERLINKV5_20151103070403","2013-02-23T22:30:00","#QLD1_E_20130223","#QLD1_E_20130223","2013-02-23",2,-55.539560000000002,"Multiple QLD1 LHS <= 0 (Wt = 360)","OUTAGE","OTHER","Feeder 7191","REGULATED","INCLUDED","Unplanned outage of Feeder 7191 and T049 Kareeya 1T.  AEMO invoked quick constraint to constrain Kareeya units 1 & 3.","UNPLANNED",1]
[3767,"POWERLINKV5_20151103070403","2013-02-23T22:50:00","#QLD1_E_20130223","#QLD1_E_20130223","2013-02-23",2,-56.208889999999997,"Multiple QLD1 LHS <= 0 (Wt = 360)","OUTAGE","OTHER","Feeder 7191","REGULATED","INCLUDED","Unplanned outage of Feeder 7191 and T049 Kareeya 1T.  AEMO invoked quick constraint to constrain Kareeya units 1 & 3.","UNPLANNED",1]
[3770,"POWERLINKV5_20151103070403","2013-02-23T23:05:00","#QLD1_E_20130223","#QLD1_E_20130223","2013-02-23",2,-59.150269999999999,"Multiple QLD1 LHS <= 0 (Wt = 360)","OUTAGE","OTHER","Feeder 7191","REGULATED","INCLUDED","Unplanned outage of Feeder 7191 and T049 Kareeya 1T.  AEMO invoked quick constraint to constrain Kareeya units 1 & 3.","UNPLANNED",1]
[3774,"POWERLINKV5_20151103070403","2013-02-23T23:25:00","#QLD1_E_20130223","#QLD1_E_20130223","2013-02-23",2,-54.616280000000003,"Multiple QLD1 LHS <= 0 (Wt = 360)","OUTAGE","OTHER","Feeder 7191","REGULATED","INCLUDED","Unplanned outage of Feeder 7191 and T049 Kareeya 1T.  AEMO invoked quick constraint to constrain Kareeya units 1 & 3.","UNPLANNED",1]
[3777,"POWERLINKV5_20151103070403","2013-02-25T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1068.7037800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3780,"POWERLINKV5_20151103070403","2013-02-25T12:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1075.96127,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3781,"POWERLINKV5_20151103070403","2013-02-25T12:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1075.8762200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3785,"POWERLINKV5_20151103070403","2013-02-25T12:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1062.0876900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3788,"POWERLINKV5_20151103070403","2013-02-25T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1075.45802,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3792,"POWERLINKV5_20151103070403","2013-02-25T13:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1085.5408,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3795,"POWERLINKV5_20151103070403","2013-02-25T13:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1061.7480700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3799,"POWERLINKV5_20151103070403","2013-02-25T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1074.83718,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3802,"POWERLINKV5_20151103070403","2013-02-25T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1071.395,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3805,"POWERLINKV5_20151103070403","2013-02-25T14:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9912400000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3806,"POWERLINKV5_20151103070403","2013-02-25T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1065.33861,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3809,"POWERLINKV5_20151103070403","2013-02-25T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1078.3307500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3812,"POWERLINKV5_20151103070403","2013-02-25T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1078.86922,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3816,"POWERLINKV5_20151103070403","2013-02-25T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1074.20767,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3819,"POWERLINKV5_20151103070403","2013-02-25T15:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1065.8197600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3823,"POWERLINKV5_20151103070403","2013-02-25T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.0022100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3826,"POWERLINKV5_20151103070403","2013-02-25T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.9858899999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3830,"POWERLINKV5_20151103070403","2013-02-25T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1072.0022100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3831,"POWERLINKV5_20151103070403","2013-02-25T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1071.16095,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3834,"POWERLINKV5_20151103070403","2013-02-25T16:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1061.0432000000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3838,"POWERLINKV5_20151103070403","2013-02-27T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1061.3716300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3841,"POWERLINKV5_20151103070403","2013-02-27T15:40:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1065.5989999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3844,"POWERLINKV5_20151103070403","2013-02-27T15:55:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.90013,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3848,"POWERLINKV5_20151103070403","2013-02-27T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1059.90193,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3851,"POWERLINKV5_20151103070403","2013-02-27T16:30:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1061.0741399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3854,"POWERLINKV5_20151103070403","2013-02-27T16:45:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.6800699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3855,"POWERLINKV5_20151103070403","2013-02-27T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1060.2609199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3858,"POWERLINKV5_20151103070403","2013-02-27T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.7299499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3862,"POWERLINKV5_20151103070403","2013-02-27T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1055.0632900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3867,"POWERLINKV5_20151103070403","2013-02-27T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1054.64634,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3869,"POWERLINKV5_20151103070403","2013-02-27T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2012-09-25",1,-1053.8817200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3873,"POWERLINKV5_20151103070403","2013-02-28T13:45:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1058.9572800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3876,"POWERLINKV5_20151103070403","2013-02-28T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1059.9003499999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3879,"POWERLINKV5_20151103070403","2013-02-28T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.14572,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3880,"POWERLINKV5_20151103070403","2013-02-28T14:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.76001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3883,"POWERLINKV5_20151103070403","2013-02-28T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.0042699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3887,"POWERLINKV5_20151103070403","2013-02-28T14:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.3983700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3890,"POWERLINKV5_20151103070403","2013-02-28T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.97225,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3893,"POWERLINKV5_20151103070403","2013-02-28T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.4252200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3897,"POWERLINKV5_20151103070403","2013-02-28T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.8379500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3900,"POWERLINKV5_20151103070403","2013-02-28T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.2292500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3901,"POWERLINKV5_20151103070403","2013-02-28T16:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.47443,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3904,"POWERLINKV5_20151103070403","2013-02-28T16:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.9998900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3908,"POWERLINKV5_20151103070403","2013-02-28T16:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.2754,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3912,"POWERLINKV5_20151103070403","2013-02-28T17:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.1625100000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3915,"POWERLINKV5_20151103070403","2013-02-28T17:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.1749299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3918,"POWERLINKV5_20151103070403","2013-02-28T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.0780199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3922,"POWERLINKV5_20151103070403","2013-02-28T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.9973600000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3925,"POWERLINKV5_20151103070403","2013-03-01T08:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1109.5709300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3926,"POWERLINKV5_20151103070403","2013-03-01T09:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1109.5719200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3929,"POWERLINKV5_20151103070403","2013-03-01T09:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1090.90005,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3932,"POWERLINKV5_20151103070403","2013-03-01T09:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1090.0110199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3936,"POWERLINKV5_20151103070403","2013-03-01T09:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.3272999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3939,"POWERLINKV5_20151103070403","2013-03-01T10:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1059.9920099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3943,"POWERLINKV5_20151103070403","2013-03-01T10:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1061.17562,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3945,"POWERLINKV5_20151103070403","2013-03-01T10:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1072.0120099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3950,"POWERLINKV5_20151103070403","2013-03-01T11:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1072.0120099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3951,"POWERLINKV5_20151103070403","2013-03-01T11:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1090.0120300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3954,"POWERLINKV5_20151103070403","2013-03-01T11:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1061.3520699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3957,"POWERLINKV5_20151103070403","2013-03-01T11:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1072.0120099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3961,"POWERLINKV5_20151103070403","2013-03-01T11:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1072.0020199999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3964,"POWERLINKV5_20151103070403","2013-03-01T12:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1059.9920099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3968,"POWERLINKV5_20151103070403","2013-03-01T12:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1059.9920099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3971,"POWERLINKV5_20151103070403","2013-03-01T12:45:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1072.0020099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3974,"POWERLINKV5_20151103070403","2013-03-01T13:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1090.12203,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3975,"POWERLINKV5_20151103070403","2013-03-01T13:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1059.84656,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3978,"POWERLINKV5_20151103070403","2013-03-01T13:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1058.9420399999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3981,"POWERLINKV5_20151103070403","2013-03-01T13:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.9770699999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3986,"POWERLINKV5_20151103070403","2013-03-01T14:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.97543,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3989,"POWERLINKV5_20151103070403","2013-03-01T14:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.11789,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3993,"POWERLINKV5_20151103070403","2013-03-01T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.1693700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3996,"POWERLINKV5_20151103070403","2013-03-01T14:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.6142299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[3999,"POWERLINKV5_20151103070403","2013-03-01T15:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.3905500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4000,"POWERLINKV5_20151103070403","2013-03-01T15:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.3815099999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4003,"POWERLINKV5_20151103070403","2013-03-01T15:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.9843900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4007,"POWERLINKV5_20151103070403","2013-03-01T15:45:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.4158,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4010,"POWERLINKV5_20151103070403","2013-03-01T16:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.5547799999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4013,"POWERLINKV5_20151103070403","2013-03-01T16:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.11771,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4017,"POWERLINKV5_20151103070403","2013-03-01T16:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.9854800000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4020,"POWERLINKV5_20151103070403","2013-03-01T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1055.5491300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4023,"POWERLINKV5_20151103070403","2013-03-01T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1056.11771,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4027,"POWERLINKV5_20151103070403","2013-03-01T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.51596,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4028,"POWERLINKV5_20151103070403","2013-03-01T17:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1054.53775,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4032,"POWERLINKV5_20151103070403","2013-03-01T17:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1053.9476299999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4035,"POWERLINKV5_20151103070403","2013-03-01T18:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1052.4255900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4038,"POWERLINKV5_20151103070403","2013-03-01T18:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1051.3335999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4042,"POWERLINKV5_20151103070403","2013-03-02T16:50:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1060.3042700000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4045,"POWERLINKV5_20151103070403","2013-03-02T17:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1079.9516900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4046,"POWERLINKV5_20151103070403","2013-03-02T17:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1061.1588300000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4049,"POWERLINKV5_20151103070403","2013-03-02T17:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1079.95171,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4052,"POWERLINKV5_20151103070403","2013-03-02T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1090.58169,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4056,"POWERLINKV5_20151103070403","2013-03-02T18:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1080.40167,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4059,"POWERLINKV5_20151103070403","2013-03-02T18:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1060.71595,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4064,"POWERLINKV5_20151103070403","2013-03-02T18:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1079.9516900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4067,"POWERLINKV5_20151103070403","2013-03-02T18:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1299.3716899999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4070,"POWERLINKV5_20151103070403","2013-03-02T19:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1079.9516900000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4071,"POWERLINKV5_20151103070403","2013-03-02T19:15:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1081.16164,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4074,"POWERLINKV5_20151103070403","2013-03-02T19:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1058.0123599999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4077,"POWERLINKV5_20151103070403","2013-03-12T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-19.88175,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4081,"POWERLINKV5_20151103070403","2013-03-12T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-18.15016,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4084,"POWERLINKV5_20151103070403","2013-03-12T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-33.984789999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4087,"POWERLINKV5_20151103070403","2013-03-12T11:05:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-14.39983,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4091,"POWERLINKV5_20151103070403","2013-03-12T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-10.35014,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4094,"POWERLINKV5_20151103070403","2013-03-12T14:15:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-18.15016,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4095,"POWERLINKV5_20151103070403","2013-03-12T14:20:00","Q>NIL_BI_FB","Q-NIL","2013-02-20",2,-20.150099999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4098,"POWERLINKV5_20151103070403","2013-03-13T07:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.881820000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4101,"POWERLINKV5_20151103070403","2013-03-13T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.149999999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4106,"POWERLINKV5_20151103070403","2013-03-13T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.14995,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4109,"POWERLINKV5_20151103070403","2013-03-13T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.150230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4113,"POWERLINKV5_20151103070403","2013-03-13T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-17.840060000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4116,"POWERLINKV5_20151103070403","2013-03-13T13:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.950369999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4119,"POWERLINKV5_20151103070403","2013-03-13T13:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.08182,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4120,"POWERLINKV5_20151103070403","2013-03-13T13:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-17.510059999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4123,"POWERLINKV5_20151103070403","2013-03-13T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-16.818719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4126,"POWERLINKV5_20151103070403","2013-03-13T14:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-13.58667,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4130,"POWERLINKV5_20151103070403","2013-03-13T15:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.213360000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4133,"POWERLINKV5_20151103070403","2013-03-13T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-15.74845,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4137,"POWERLINKV5_20151103070403","2013-03-13T16:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.80489,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4140,"POWERLINKV5_20151103070403","2013-03-14T06:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.857379999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4142,"POWERLINKV5_20151103070403","2013-03-14T06:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.3001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4145,"POWERLINKV5_20151103070403","2013-03-14T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-39.250100000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4148,"POWERLINKV5_20151103070403","2013-03-14T08:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.150169999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4151,"POWERLINKV5_20151103070403","2013-03-14T08:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-10.73854,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4155,"POWERLINKV5_20151103070403","2013-03-14T08:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.69538,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4158,"POWERLINKV5_20151103070403","2013-03-14T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.300180000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4162,"POWERLINKV5_20151103070403","2013-03-14T09:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.300180000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4165,"POWERLINKV5_20151103070403","2013-03-14T09:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-10.522650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4168,"POWERLINKV5_20151103070403","2013-03-14T09:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.659979999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4169,"POWERLINKV5_20151103070403","2013-03-14T10:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.300180000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4172,"POWERLINKV5_20151103070403","2013-03-14T11:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-3522.1060400000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4176,"POWERLINKV5_20151103070403","2013-03-14T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-29.343330000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4179,"POWERLINKV5_20151103070403","2013-03-14T12:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-178.59765999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4183,"POWERLINKV5_20151103070403","2013-03-14T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-61.967320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4187,"POWERLINKV5_20151103070403","2013-03-14T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-1190.81133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4190,"POWERLINKV5_20151103070403","2013-03-14T13:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-118.4414,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4193,"POWERLINKV5_20151103070403","2013-03-14T13:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.150120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4194,"POWERLINKV5_20151103070403","2013-03-14T13:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-39.250120000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4197,"POWERLINKV5_20151103070403","2013-03-14T14:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.31006,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4201,"POWERLINKV5_20151103070403","2013-03-14T14:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.690059999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4204,"POWERLINKV5_20151103070403","2013-03-14T14:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-12.439579999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4207,"POWERLINKV5_20151103070403","2013-03-14T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.65931,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4211,"POWERLINKV5_20151103070403","2013-03-14T16:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-10.92624,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4214,"POWERLINKV5_20151103070403","2013-03-14T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.100090000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4215,"POWERLINKV5_20151103070403","2013-03-14T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.200109999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4218,"POWERLINKV5_20151103070403","2013-03-14T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.150110000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4224,"POWERLINKV5_20151103070403","2013-03-14T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.200119999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4226,"POWERLINKV5_20151103070403","2013-03-14T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.200119999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4229,"POWERLINKV5_20151103070403","2013-03-14T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.10012,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4232,"POWERLINKV5_20151103070403","2013-03-14T19:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.150179999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4236,"POWERLINKV5_20151103070403","2013-03-14T20:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-10.797359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4239,"POWERLINKV5_20151103070403","2013-03-14T20:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-20.0459,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4240,"POWERLINKV5_20151103070403","2013-03-14T20:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.530069999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4243,"POWERLINKV5_20151103070403","2013-03-14T20:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-18.150169999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4246,"POWERLINKV5_20151103070403","2013-03-14T21:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.881589999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4250,"POWERLINKV5_20151103070403","2013-03-17T12:55:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-246.51946000000001,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4253,"POWERLINKV5_20151103070403","2013-03-17T13:10:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-437.90266000000003,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4256,"POWERLINKV5_20151103070403","2013-03-17T13:25:00","Q>>NIL_855_871","Q-NIL","2013-01-01",1,-13.70149,"Out = Nil, avoid overload on Calvale to Wurdong (871) line on trip of Calvale to Stanwell (855) line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4260,"POWERLINKV5_20151103070403","2013-03-17T19:10:00","Q>>NIL_871_855","Q-NIL","2013-01-01",1,-1867.51289,"Out= Nil, avoid O/L 855 Calvale to Stanwell 275kV line on trip of 871 Calvale to Wurdong 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4261,"POWERLINKV5_20151103070403","2013-03-23T08:00:00","#NSW1-QLD1_E_E","#NSW1-QLD1_E","2013-03-23",1,-30.497869999999999,"NSW1-QLD1.ENERGY * 1 <= 125 (Wt = 20)","OUTAGE","OTHER","QNI","REGULATED","99","AEMO Invoked constraint to limit the flow from NSW to QLD on the QNI interconnector, due to an outage on Bayswater - Liddell 34 330 kV by TransGrid. Refer to Market Notice 42003","UNPLANNED",0]
[4265,"POWERLINKV5_20151103070403","2013-03-23T08:45:00","#NSW1-QLD1_E_E","#NSW1-QLD1_E","2013-03-23",1,-31.885300000000001,"NSW1-QLD1.ENERGY * 1 <= 125 (Wt = 20)","OUTAGE","OTHER","QNI","REGULATED","99","AEMO Invoked constraint to limit the flow from NSW to QLD on the QNI interconnector, due to an outage on Bayswater - Liddell 34 330 kV by TransGrid. Refer to Market Notice 42003","UNPLANNED",0]
[4268,"POWERLINKV5_20151103070403","2013-03-23T09:05:00","#NSW1-QLD1_E_E","#NSW1-QLD1_E","2013-03-23",1,-31.915949999999999,"NSW1-QLD1.ENERGY * 1 <= 125 (Wt = 20)","OUTAGE","OTHER","QNI","REGULATED","99","AEMO Invoked constraint to limit the flow from NSW to QLD on the QNI interconnector, due to an outage on Bayswater - Liddell 34 330 kV by TransGrid. Refer to Market Notice 42003","UNPLANNED",0]
[4271,"POWERLINKV5_20151103070403","2013-03-23T09:20:00","#NSW1-QLD1_E_E","#NSW1-QLD1_E","2013-03-23",1,-183.74123,"NSW1-QLD1.ENERGY * 1 <= 125 (Wt = 20)","OUTAGE","OTHER","QNI","REGULATED","99","AEMO Invoked constraint to limit the flow from NSW to QLD on the QNI interconnector, due to an outage on Bayswater - Liddell 34 330 kV by TransGrid. Refer to Market Notice 42003","UNPLANNED",0]
[4275,"POWERLINKV5_20151103070403","2013-05-04T22:40:00","#NSW1-QLD1_I_E","#NSW1-QLD1_E","2013-05-04",4,10.04153,"NSW1-QLD1.ENERGY * -1 >= 100 (Wt = 20)","OUTAGE","OTHER","QNI","REGULATED","99","AEMO invoked the constraint when VSAT indicated a violation for the loss of generation.  Refer to Market Notice 42298.","UNPLANNED",0]
[4278,"POWERLINKV5_20151103070403","2013-05-29T17:05:00","N^^Q_BCDM_B1","I-BCDM_ONE","2008-01-03",1,-15.76605,"Out= one Bulli Creek - Dumaresq (8L or 8M) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Feeder 8L","REGULATED","99","TransGrid outage of Feeder 8L, under NOS Company Reference TG_131310.","PLANNED",0]
[4282,"POWERLINKV5_20151103070403","2013-05-29T20:05:00","N^^Q_BCDM_B1","I-BCDM_ONE","2008-01-03",1,-27.62782,"Out= one Bulli Creek - Dumaresq (8L or 8M) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Feeder 8L","REGULATED","INCLUDED","Powerlink outage of Feeder 8L, CB 8L2 at R003 Bulli Creek broke on restoration, Transgrid outage TG_131310 transfered to PLQ AFW Q13S/1293 at 2000hrs.","UNPLANNED",1]
[4285,"POWERLINKV5_20151103070403","2013-06-04T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-12362.408219999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4288,"POWERLINKV5_20151103070403","2013-06-11T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-15,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4289,"POWERLINKV5_20151103070403","2013-06-11T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-16.566179999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4292,"POWERLINKV5_20151103070403","2013-06-12T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-36.632959999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4295,"POWERLINKV5_20151103070403","2013-06-13T18:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-10.09937,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4299,"POWERLINKV5_20151103070403","2013-06-17T07:15:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2013-06-17",61,-11404.495569999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","OUTAGE","OTHER","Unknown","REGULATED","99","New South Wales - Constraint Automation, O/L 9U7/L@LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","PLANNED",0]
[4302,"POWERLINKV5_20151103070403","2013-06-17T17:10:00","Q>>BRTR_MRTX5_MRTX4","Q-BRTR_8814_8815","2013-04-02",1,-18.239519999999999,"Out= 8814 or 8815 R2 Braemar to H18 Tarong 275kV line, avoid O/L on Middle Ridge 330/275 kV Tx #4, on trip of Middle Ridge 330/275 kV Tx #5 (or 9907), DS RHS is swamped when Middle Ridge bus splitting scheme is triggered, Feedback","OUTAGE","OTHER","Feeder 8815","REGULATED","INCLUDED","Planned outage of Feeder 8815 for tower relocation due to a farming accident, refer to AFW Q13S/1415.","PLANNED",1]
[4307,"POWERLINKV5_20151103070403","2013-06-18T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-939.29417999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4310,"POWERLINKV5_20151103070403","2013-06-19T07:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-54.970849999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4313,"POWERLINKV5_20151103070403","2013-06-19T07:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-25,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4314,"POWERLINKV5_20151103070403","2013-06-19T07:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-25,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4317,"POWERLINKV5_20151103070403","2013-06-19T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-47.97786,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4321,"POWERLINKV5_20151103070403","2013-06-19T17:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-14.405570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4324,"POWERLINKV5_20151103070403","2013-06-19T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.213889999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4327,"POWERLINKV5_20151103070403","2013-06-19T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-50.284559999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4331,"POWERLINKV5_20151103070403","2013-06-19T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-27.702919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4334,"POWERLINKV5_20151103070403","2013-06-19T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-22.72261,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4337,"POWERLINKV5_20151103070403","2013-06-19T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.455030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4338,"POWERLINKV5_20151103070403","2013-06-19T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-11.548389999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4343,"POWERLINKV5_20151103070403","2013-06-20T06:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-19.842469999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4346,"POWERLINKV5_20151103070403","2013-06-20T06:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-39.759909999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4349,"POWERLINKV5_20151103070403","2013-06-20T06:45:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-134.15563,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4352,"POWERLINKV5_20151103070403","2013-06-20T07:00:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-27.945160000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4356,"POWERLINKV5_20151103070403","2013-06-20T07:30:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-12088.39335,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4359,"POWERLINKV5_20151103070403","2013-06-20T08:05:00","QNTE_ROC","Q-NIL","2010-11-08",3,-34.5869,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4362,"POWERLINKV5_20151103070403","2013-06-20T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-22.1401,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4363,"POWERLINKV5_20151103070403","2013-06-20T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-22.49288,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4366,"POWERLINKV5_20151103070403","2013-06-20T10:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-44.377049999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4370,"POWERLINKV5_20151103070403","2013-06-20T10:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-44.353020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4373,"POWERLINKV5_20151103070403","2013-06-20T11:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-32.453009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4376,"POWERLINKV5_20151103070403","2013-06-20T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-32.266910000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4380,"POWERLINKV5_20151103070403","2013-06-20T11:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.813970000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4384,"POWERLINKV5_20151103070403","2013-06-20T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-25.519860000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4385,"POWERLINKV5_20151103070403","2013-06-20T12:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.858059999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4388,"POWERLINKV5_20151103070403","2013-06-20T12:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-27.111799999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4391,"POWERLINKV5_20151103070403","2013-06-20T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-27.668150000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4395,"POWERLINKV5_20151103070403","2013-06-20T12:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.595929999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4398,"POWERLINKV5_20151103070403","2013-06-20T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-27.369389999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4401,"POWERLINKV5_20151103070403","2013-06-20T13:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.661580000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4405,"POWERLINKV5_20151103070403","2013-06-20T13:40:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.685500000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4408,"POWERLINKV5_20151103070403","2013-06-20T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-26.64151,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4409,"POWERLINKV5_20151103070403","2013-06-20T14:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-25.62152,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4412,"POWERLINKV5_20151103070403","2013-06-20T14:15:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.70468,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4415,"POWERLINKV5_20151103070403","2013-06-20T14:30:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.657979999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4419,"POWERLINKV5_20151103070403","2013-06-20T14:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.37642,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4421,"POWERLINKV5_20151103070403","2013-06-20T15:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.262530000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4426,"POWERLINKV5_20151103070403","2013-06-20T15:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-27.858609999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4430,"POWERLINKV5_20151103070403","2013-06-20T15:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-24.899380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4433,"POWERLINKV5_20151103070403","2013-06-20T16:00:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-29.465450000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4434,"POWERLINKV5_20151103070403","2013-06-20T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-28.405889999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4437,"POWERLINKV5_20151103070403","2013-06-20T16:20:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-29.38279,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4440,"POWERLINKV5_20151103070403","2013-06-20T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-29.43939,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4444,"POWERLINKV5_20151103070403","2013-06-20T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-31.707630000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4447,"POWERLINKV5_20151103070403","2013-06-20T17:05:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-28.108689999999999,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4451,"POWERLINKV5_20151103070403","2013-06-20T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-106.31253,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4454,"POWERLINKV5_20151103070403","2013-06-20T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-1091.3129899999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4457,"POWERLINKV5_20151103070403","2013-06-20T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-1127.1684700000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4458,"POWERLINKV5_20151103070403","2013-06-20T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-1115.4283700000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4462,"POWERLINKV5_20151103070403","2013-06-20T18:10:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-1043.44703,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4465,"POWERLINKV5_20151103070403","2013-06-20T18:25:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-110.84233999999999,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4469,"POWERLINKV5_20151103070403","2013-06-20T18:45:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-1050.7499,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4472,"POWERLINKV5_20151103070403","2013-06-20T20:35:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-15.20387,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4476,"POWERLINKV5_20151103070403","2013-06-21T07:20:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-22.128830000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4479,"POWERLINKV5_20151103070403","2013-06-21T07:35:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-15.1494,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4482,"POWERLINKV5_20151103070403","2013-06-21T07:50:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-12.564679999999999,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4483,"POWERLINKV5_20151103070403","2013-06-21T07:55:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-13.080550000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4486,"POWERLINKV5_20151103070403","2013-06-21T08:10:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-31.313780000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4490,"POWERLINKV5_20151103070403","2013-06-21T08:35:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-11.25202,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4493,"POWERLINKV5_20151103070403","2013-06-21T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-03-13",1,-31.5261,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4496,"POWERLINKV5_20151103070403","2013-06-21T17:10:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-30.799569999999999,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4499,"POWERLINKV5_20151103070403","2013-06-21T17:25:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-63.296970000000002,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4504,"POWERLINKV5_20151103070403","2013-06-21T17:50:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-101.34117999999999,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4507,"POWERLINKV5_20151103070403","2013-06-21T18:05:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-87.303889999999996,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4508,"POWERLINKV5_20151103070403","2013-06-21T18:10:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-85.848879999999994,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4511,"POWERLINKV5_20151103070403","2013-06-21T18:25:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-55.775030000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4515,"POWERLINKV5_20151103070403","2013-06-21T18:45:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-36.12547,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4518,"POWERLINKV5_20151103070403","2013-06-21T19:00:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-32.967979999999997,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4521,"POWERLINKV5_20151103070403","2013-06-25T17:25:00","Q_CS_1100","Q-CLTR_8810","2013-01-01",1,-24.569140000000001,"Qld Central to Qld South upper transfer limit of 1100MW (discretionary), 2008/2009 implementation","OUTAGE","OTHER","Feeder 8811","REGULATED","INCLUDED","Planned outage of Feeder 8811 to cut it in and out of S002 Halys, CP.01429.","PLANNED",1]
[4525,"POWERLINKV5_20151103070403","2013-06-26T15:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2006-01-03",1,10.50886,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Feeder 8L","REGULATED","99","Transgrid planned outage of Feeder 8L for protection maintenance, NOS Booking ID: TG_139655.","PLANNED",0]
[4528,"POWERLINKV5_20151103070403","2013-06-26T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-42.413760000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4531,"POWERLINKV5_20151103070403","2013-06-26T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-28.265029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4532,"POWERLINKV5_20151103070403","2013-06-26T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-23.25,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4535,"POWERLINKV5_20151103070403","2013-06-26T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.616759999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4540,"POWERLINKV5_20151103070403","2013-06-27T13:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.5,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4543,"POWERLINKV5_20151103070403","2013-06-27T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.034700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4546,"POWERLINKV5_20151103070403","2013-06-27T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.686219999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4550,"POWERLINKV5_20151103070403","2013-06-27T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.03632,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4553,"POWERLINKV5_20151103070403","2013-06-27T18:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.527710000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4554,"POWERLINKV5_20151103070403","2013-06-27T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.5238,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4557,"POWERLINKV5_20151103070403","2013-06-27T18:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-18.648440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4560,"POWERLINKV5_20151103070403","2013-06-28T07:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-33.15,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4564,"POWERLINKV5_20151103070403","2013-06-28T07:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-33.15,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4567,"POWERLINKV5_20151103070403","2013-06-28T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-37.973460000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4570,"POWERLINKV5_20151103070403","2013-06-28T09:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.41093,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4574,"POWERLINKV5_20151103070403","2013-06-28T10:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-16.100000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4577,"POWERLINKV5_20151103070403","2013-06-28T10:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-16.100000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4581,"POWERLINKV5_20151103070403","2013-06-28T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-16.459700000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4582,"POWERLINKV5_20151103070403","2013-06-28T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-20.873570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4585,"POWERLINKV5_20151103070403","2013-06-28T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-31.252410000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4589,"POWERLINKV5_20151103070403","2013-06-28T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-23.46442,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4592,"POWERLINKV5_20151103070403","2013-06-28T18:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.43507,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4595,"POWERLINKV5_20151103070403","2013-06-28T18:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.322699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4599,"POWERLINKV5_20151103070403","2013-06-28T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.810600000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4602,"POWERLINKV5_20151103070403","2013-06-28T22:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-48.058489999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4603,"POWERLINKV5_20151103070403","2013-06-28T22:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-35.821649999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4606,"POWERLINKV5_20151103070403","2013-06-28T23:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.500050000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4609,"POWERLINKV5_20151103070403","2013-06-29T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.600059999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4613,"POWERLINKV5_20151103070403","2013-06-29T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-31.991240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4616,"POWERLINKV5_20151103070403","2013-06-29T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-28.41873,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4618,"POWERLINKV5_20151103070403","2013-06-29T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.685790000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4624,"POWERLINKV5_20151103070403","2013-06-29T18:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-24.135259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4627,"POWERLINKV5_20151103070403","2013-06-30T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.31564,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4628,"POWERLINKV5_20151103070403","2013-06-30T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-16.63776,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4631,"POWERLINKV5_20151103070403","2013-06-30T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-18.07272,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4634,"POWERLINKV5_20151103070403","2013-06-30T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.84,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4638,"POWERLINKV5_20151103070403","2013-06-30T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.500170000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4641,"POWERLINKV5_20151103070403","2013-06-30T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.196,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4645,"POWERLINKV5_20151103070403","2013-07-01T22:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.8627,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4648,"POWERLINKV5_20151103070403","2013-07-02T20:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.258089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4651,"POWERLINKV5_20151103070403","2013-07-02T22:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-43.248550000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4652,"POWERLINKV5_20151103070403","2013-07-02T22:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-37.963250000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4655,"POWERLINKV5_20151103070403","2013-07-02T22:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-28.498670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4659,"POWERLINKV5_20151103070403","2013-07-21T18:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1025.2456999999999,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4663,"POWERLINKV5_20151103070403","2013-07-21T19:45:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1004.67002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4666,"POWERLINKV5_20151103070403","2013-07-21T20:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1031.1028200000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4670,"POWERLINKV5_20151103070403","2013-07-21T20:25:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1030.4755500000001,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4673,"POWERLINKV5_20151103070403","2013-07-21T20:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1022.11015,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4676,"POWERLINKV5_20151103070403","2013-07-21T21:00:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1000.74344,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4677,"POWERLINKV5_20151103070403","2013-07-21T21:05:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-1017.1,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4680,"POWERLINKV5_20151103070403","2013-07-21T21:20:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-992.08006,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4684,"POWERLINKV5_20151103070403","2013-07-21T21:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-992.42607999999996,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4687,"POWERLINKV5_20151103070403","2013-07-21T21:55:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-987.29024000000004,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4690,"POWERLINKV5_20151103070403","2013-07-21T22:10:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-991.69,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4694,"POWERLINKV5_20151103070403","2013-07-21T22:30:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-986.82871,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4697,"POWERLINKV5_20151103070403","2013-07-27T17:55:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2013-07-27",42,-45.449039999999997,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","OUTAGE","OTHER","Unknown","REGULATED","99","New South Wales - Constraint Automation, O/L 9U7/L@LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","PLANNED",0]
[4700,"POWERLINKV5_20151103070403","2013-07-29T18:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-30.935919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4702,"POWERLINKV5_20151103070403","2013-07-29T18:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-30.191880000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4705,"POWERLINKV5_20151103070403","2013-07-29T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.187659999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4709,"POWERLINKV5_20151103070403","2013-08-06T11:40:00","Q>>NIL_871_855_POST","Q-NIL_POST8868","2013-07-31",1,-33.029209999999999,"Out = Nil,  Post-8868 commissioning, avoid overload on Calvale to Stanwell (855) 275kV line on trip of  Calvale to Wurdong (871) 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4712,"POWERLINKV5_20151103070403","2013-08-06T11:55:00","Q>>NIL_871_855_POST","Q-NIL_POST8868","2013-07-31",1,-10.796749999999999,"Out = Nil,  Post-8868 commissioning, avoid overload on Calvale to Stanwell (855) 275kV line on trip of  Calvale to Wurdong (871) 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4715,"POWERLINKV5_20151103070403","2013-08-06T13:10:00","Q>>NIL_871_855_POST","Q-NIL_POST8868","2013-07-31",1,-16.424209999999999,"Out = Nil,  Post-8868 commissioning, avoid overload on Calvale to Stanwell (855) 275kV line on trip of  Calvale to Wurdong (871) 275kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4719,"POWERLINKV5_20151103070403","2013-08-19T17:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-76.384429999999995,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4722,"POWERLINKV5_20151103070403","2013-09-16T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-134.82849999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4723,"POWERLINKV5_20151103070403","2013-09-27T16:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-13.63,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4726,"POWERLINKV5_20151103070403","2013-09-27T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-14.290039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4729,"POWERLINKV5_20151103070403","2013-09-27T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.320069999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4733,"POWERLINKV5_20151103070403","2013-10-11T22:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-25.01,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4736,"POWERLINKV5_20151103070403","2013-10-12T18:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-112.57656,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4741,"POWERLINKV5_20151103070403","2013-10-12T18:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.010199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4744,"POWERLINKV5_20151103070403","2013-10-12T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.010249999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4747,"POWERLINKV5_20151103070403","2013-10-13T18:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-10.212630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4748,"POWERLINKV5_20151103070403","2013-10-13T18:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.212630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4751,"POWERLINKV5_20151103070403","2013-10-13T18:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.010160000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4754,"POWERLINKV5_20151103070403","2013-10-13T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.010199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4758,"POWERLINKV5_20151103070403","2013-10-13T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.0101,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4761,"POWERLINKV5_20151103070403","2013-10-14T16:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-22.120190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4765,"POWERLINKV5_20151103070403","2013-10-15T14:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-38.320149999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4768,"POWERLINKV5_20151103070403","2013-10-15T14:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-38.320149999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4771,"POWERLINKV5_20151103070403","2013-10-16T09:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1043.9951000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4772,"POWERLINKV5_20151103070403","2013-10-16T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1043.9951000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4775,"POWERLINKV5_20151103070403","2013-10-16T09:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1048.3802700000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4778,"POWERLINKV5_20151103070403","2013-10-16T09:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1053.0035,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4783,"POWERLINKV5_20151103070403","2013-10-16T10:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1049.07907,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4786,"POWERLINKV5_20151103070403","2013-10-16T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1048.3761999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4790,"POWERLINKV5_20151103070403","2013-10-16T10:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1047.1808100000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4793,"POWERLINKV5_20151103070403","2013-10-21T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-28.911010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4796,"POWERLINKV5_20151103070403","2013-10-21T06:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.580069999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4797,"POWERLINKV5_20151103070403","2013-10-21T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.2911,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4800,"POWERLINKV5_20151103070403","2013-10-21T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-62.825200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4803,"POWERLINKV5_20151103070403","2013-10-21T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.31358,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4807,"POWERLINKV5_20151103070403","2013-10-21T08:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-80.025459999999995,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4810,"POWERLINKV5_20151103070403","2013-10-21T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-88.351330000000004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4814,"POWERLINKV5_20151103070403","2013-10-21T09:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-294.10478999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4817,"POWERLINKV5_20151103070403","2013-10-21T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-12.01019,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4819,"POWERLINKV5_20151103070403","2013-10-21T09:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-109.93615,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4822,"POWERLINKV5_20151103070403","2013-10-21T09:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-63.418430000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4825,"POWERLINKV5_20151103070403","2013-10-21T13:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-10.140140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4829,"POWERLINKV5_20151103070403","2013-10-21T13:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.681559999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4832,"POWERLINKV5_20151103070403","2013-10-21T13:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-11.17845,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4835,"POWERLINKV5_20151103070403","2013-10-21T14:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.22518,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4839,"POWERLINKV5_20151103070403","2013-10-21T14:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.930199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4842,"POWERLINKV5_20151103070403","2013-10-21T14:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-13.374700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4845,"POWERLINKV5_20151103070403","2013-10-21T14:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.19754,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4846,"POWERLINKV5_20151103070403","2013-10-21T14:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-13.19754,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4849,"POWERLINKV5_20151103070403","2013-10-21T14:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-12.67826,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4853,"POWERLINKV5_20151103070403","2013-10-21T14:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.71424,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4856,"POWERLINKV5_20151103070403","2013-10-21T15:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.61741,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4860,"POWERLINKV5_20151103070403","2013-10-21T15:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.08944,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4864,"POWERLINKV5_20151103070403","2013-10-21T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.930199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4867,"POWERLINKV5_20151103070403","2013-10-21T15:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.810199999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4870,"POWERLINKV5_20151103070403","2013-10-21T15:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.410039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4871,"POWERLINKV5_20151103070403","2013-10-21T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4874,"POWERLINKV5_20151103070403","2013-10-21T15:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4878,"POWERLINKV5_20151103070403","2013-10-21T15:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4881,"POWERLINKV5_20151103070403","2013-10-21T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.930199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4884,"POWERLINKV5_20151103070403","2013-10-21T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-16.992010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4888,"POWERLINKV5_20151103070403","2013-10-21T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-20.07705,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4891,"POWERLINKV5_20151103070403","2013-10-21T18:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-12.22855,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4892,"POWERLINKV5_20151103070403","2013-10-21T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.22855,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4897,"POWERLINKV5_20151103070403","2013-10-21T18:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-32.000190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4899,"POWERLINKV5_20151103070403","2013-10-21T18:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1456.4612999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4903,"POWERLINKV5_20151103070403","2013-10-21T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-269.36061000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4906,"POWERLINKV5_20151103070403","2013-10-21T18:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-72.700190000000006,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4909,"POWERLINKV5_20151103070403","2013-10-21T18:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-42.270189999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4913,"POWERLINKV5_20151103070403","2013-10-21T18:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-32.010190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4916,"POWERLINKV5_20151103070403","2013-10-21T19:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.86016,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4917,"POWERLINKV5_20151103070403","2013-10-21T19:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.810040000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4920,"POWERLINKV5_20151103070403","2013-10-21T19:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4923,"POWERLINKV5_20151103070403","2013-10-21T19:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-32.000190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4927,"POWERLINKV5_20151103070403","2013-10-21T19:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-31.98028,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4930,"POWERLINKV5_20151103070403","2013-10-21T19:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-64.310040000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4934,"POWERLINKV5_20151103070403","2013-10-21T19:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.010199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4938,"POWERLINKV5_20151103070403","2013-10-21T22:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-32.000190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4941,"POWERLINKV5_20151103070403","2013-10-21T22:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-1447.0102199999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4942,"POWERLINKV5_20151103070403","2013-10-21T22:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1447.0102199999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4945,"POWERLINKV5_20151103070403","2013-10-21T23:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-32.000109999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4948,"POWERLINKV5_20151103070403","2013-10-22T00:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-32.000219999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4952,"POWERLINKV5_20151103070403","2013-10-22T06:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.9932,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4955,"POWERLINKV5_20151103070403","2013-10-22T06:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-15.6493,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4959,"POWERLINKV5_20151103070403","2013-10-22T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-48.9069,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4962,"POWERLINKV5_20151103070403","2013-10-22T10:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.920200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4965,"POWERLINKV5_20151103070403","2013-10-22T10:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4966,"POWERLINKV5_20151103070403","2013-10-22T10:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4969,"POWERLINKV5_20151103070403","2013-10-22T10:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.700240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4972,"POWERLINKV5_20151103070403","2013-10-22T10:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.800239999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4975,"POWERLINKV5_20151103070403","2013-10-22T11:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.800239999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4980,"POWERLINKV5_20151103070403","2013-10-22T11:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4984,"POWERLINKV5_20151103070403","2013-10-22T11:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.760199999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4987,"POWERLINKV5_20151103070403","2013-10-22T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4990,"POWERLINKV5_20151103070403","2013-10-22T11:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4991,"POWERLINKV5_20151103070403","2013-10-22T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4994,"POWERLINKV5_20151103070403","2013-10-22T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.800199999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[4998,"POWERLINKV5_20151103070403","2013-10-22T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5001,"POWERLINKV5_20151103070403","2013-10-22T12:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5004,"POWERLINKV5_20151103070403","2013-10-22T12:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5008,"POWERLINKV5_20151103070403","2013-10-22T12:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5011,"POWERLINKV5_20151103070403","2013-10-22T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.760199999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5014,"POWERLINKV5_20151103070403","2013-10-22T12:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5016,"POWERLINKV5_20151103070403","2013-10-22T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5019,"POWERLINKV5_20151103070403","2013-10-22T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.800199999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5023,"POWERLINKV5_20151103070403","2013-10-22T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5026,"POWERLINKV5_20151103070403","2013-10-22T13:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.460599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5029,"POWERLINKV5_20151103070403","2013-10-22T13:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-32.916379999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5033,"POWERLINKV5_20151103070403","2013-10-22T13:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-34.679940000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5036,"POWERLINKV5_20151103070403","2013-10-22T13:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-45.21022,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5037,"POWERLINKV5_20151103070403","2013-10-22T13:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-61.410220000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5040,"POWERLINKV5_20151103070403","2013-10-22T13:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-54.980310000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5043,"POWERLINKV5_20151103070403","2013-10-22T14:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-69.840329999999994,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5047,"POWERLINKV5_20151103070403","2013-10-22T14:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-30.190200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5050,"POWERLINKV5_20151103070403","2013-10-22T14:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-27.00009,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5053,"POWERLINKV5_20151103070403","2013-10-22T14:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-30.190100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5057,"POWERLINKV5_20151103070403","2013-10-22T14:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-24.8001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5061,"POWERLINKV5_20151103070403","2013-10-22T14:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-24.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5062,"POWERLINKV5_20151103070403","2013-10-22T14:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-24.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5065,"POWERLINKV5_20151103070403","2013-10-22T14:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5068,"POWERLINKV5_20151103070403","2013-10-22T15:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.800319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5072,"POWERLINKV5_20151103070403","2013-10-22T15:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-24.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5075,"POWERLINKV5_20151103070403","2013-10-22T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5078,"POWERLINKV5_20151103070403","2013-10-22T15:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.8002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5082,"POWERLINKV5_20151103070403","2013-10-22T16:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.920200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5085,"POWERLINKV5_20151103070403","2013-10-22T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.3102,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5086,"POWERLINKV5_20151103070403","2013-10-22T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-14.3102,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5089,"POWERLINKV5_20151103070403","2013-10-22T16:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.920200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5092,"POWERLINKV5_20151103070403","2013-10-22T16:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-36.0702,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5098,"POWERLINKV5_20151103070403","2013-10-22T17:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-70.240200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5100,"POWERLINKV5_20151103070403","2013-10-22T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5104,"POWERLINKV5_20151103070403","2013-10-22T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-70.240200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5107,"POWERLINKV5_20151103070403","2013-10-22T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.2102,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5110,"POWERLINKV5_20151103070403","2013-10-22T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5111,"POWERLINKV5_20151103070403","2013-10-22T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5114,"POWERLINKV5_20151103070403","2013-10-22T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5117,"POWERLINKV5_20151103070403","2013-10-22T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.860230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5121,"POWERLINKV5_20151103070403","2013-10-22T18:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-47.010150000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5124,"POWERLINKV5_20151103070403","2013-10-22T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5128,"POWERLINKV5_20151103070403","2013-10-22T18:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5131,"POWERLINKV5_20151103070403","2013-10-22T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-47.66019,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5134,"POWERLINKV5_20151103070403","2013-10-22T18:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-66.510189999999994,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5135,"POWERLINKV5_20151103070403","2013-10-22T18:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.960189999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5139,"POWERLINKV5_20151103070403","2013-10-22T18:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.960189999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5142,"POWERLINKV5_20151103070403","2013-10-22T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-66.510189999999994,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5146,"POWERLINKV5_20151103070403","2013-10-22T19:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860149999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5149,"POWERLINKV5_20151103070403","2013-10-22T19:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5153,"POWERLINKV5_20151103070403","2013-10-22T19:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5156,"POWERLINKV5_20151103070403","2013-10-22T19:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.860190000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5159,"POWERLINKV5_20151103070403","2013-10-22T19:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-22.120190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5160,"POWERLINKV5_20151103070403","2013-10-22T19:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-22.120190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5163,"POWERLINKV5_20151103070403","2013-10-22T20:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-22.120190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5167,"POWERLINKV5_20151103070403","2013-10-22T21:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-31.170069999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5170,"POWERLINKV5_20151103070403","2013-10-23T06:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-13.13762,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5173,"POWERLINKV5_20151103070403","2013-10-23T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1447.01018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5176,"POWERLINKV5_20151103070403","2013-10-23T06:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-42.010179999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5181,"POWERLINKV5_20151103070403","2013-10-23T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-1447.0103300000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5184,"POWERLINKV5_20151103070403","2013-10-23T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-22.010269999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5185,"POWERLINKV5_20151103070403","2013-10-23T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-24.689990000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5188,"POWERLINKV5_20151103070403","2013-10-23T09:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-14.581630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5192,"POWERLINKV5_20151103070403","2013-10-23T09:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-24.800059999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5195,"POWERLINKV5_20151103070403","2013-10-23T10:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-12.35923,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5198,"POWERLINKV5_20151103070403","2013-10-23T10:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.92015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5202,"POWERLINKV5_20151103070403","2013-10-23T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660089999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5205,"POWERLINKV5_20151103070403","2013-10-23T10:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-29.81015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5206,"POWERLINKV5_20151103070403","2013-10-23T10:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.81015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5209,"POWERLINKV5_20151103070403","2013-10-23T10:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-36.120080000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5212,"POWERLINKV5_20151103070403","2013-10-23T11:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-36.120049999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5217,"POWERLINKV5_20151103070403","2013-10-23T11:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.99933,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5220,"POWERLINKV5_20151103070403","2013-10-23T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-24.800149999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5223,"POWERLINKV5_20151103070403","2013-10-23T11:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-36.120049999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5227,"POWERLINKV5_20151103070403","2013-10-23T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.920089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5230,"POWERLINKV5_20151103070403","2013-10-23T13:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.920089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5231,"POWERLINKV5_20151103070403","2013-10-23T13:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.920089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5234,"POWERLINKV5_20151103070403","2013-10-23T13:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-24.800090000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5237,"POWERLINKV5_20151103070403","2013-10-23T13:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-36.120089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5241,"POWERLINKV5_20151103070403","2013-10-23T13:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660089999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5244,"POWERLINKV5_20151103070403","2013-10-23T13:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660179999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5247,"POWERLINKV5_20151103070403","2013-10-23T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.760089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5251,"POWERLINKV5_20151103070403","2013-10-23T14:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-36.070099999999996,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5254,"POWERLINKV5_20151103070403","2013-10-23T14:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.920100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5258,"POWERLINKV5_20151103070403","2013-10-23T14:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.8001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5259,"POWERLINKV5_20151103070403","2013-10-23T14:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660290000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5262,"POWERLINKV5_20151103070403","2013-10-23T14:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-39.810119999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5266,"POWERLINKV5_20151103070403","2013-10-23T14:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5269,"POWERLINKV5_20151103070403","2013-10-23T15:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.650199999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5273,"POWERLINKV5_20151103070403","2013-10-23T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-29.810199999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5276,"POWERLINKV5_20151103070403","2013-10-23T15:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.920200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5279,"POWERLINKV5_20151103070403","2013-10-23T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-39.810200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5280,"POWERLINKV5_20151103070403","2013-10-23T15:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-39.810200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5283,"POWERLINKV5_20151103070403","2013-10-23T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5286,"POWERLINKV5_20151103070403","2013-10-23T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5290,"POWERLINKV5_20151103070403","2013-10-23T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-7145.7902000000004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5295,"POWERLINKV5_20151103070403","2013-10-23T16:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5298,"POWERLINKV5_20151103070403","2013-10-23T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.6601,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5301,"POWERLINKV5_20151103070403","2013-10-23T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-235.15996000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5304,"POWERLINKV5_20151103070403","2013-10-23T17:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660110000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5305,"POWERLINKV5_20151103070403","2013-10-23T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.810299999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5308,"POWERLINKV5_20151103070403","2013-10-23T17:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.810200000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5311,"POWERLINKV5_20151103070403","2013-10-23T17:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.660200000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5315,"POWERLINKV5_20151103070403","2013-10-23T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-38.330089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5318,"POWERLINKV5_20151103070403","2013-10-23T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-38.330089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5322,"POWERLINKV5_20151103070403","2013-10-23T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.750259999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5325,"POWERLINKV5_20151103070403","2013-10-23T18:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-38.220280000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5328,"POWERLINKV5_20151103070403","2013-10-23T18:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-45.770339999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5329,"POWERLINKV5_20151103070403","2013-10-23T18:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.660110000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5332,"POWERLINKV5_20151103070403","2013-10-23T18:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.810110000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5337,"POWERLINKV5_20151103070403","2013-10-23T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-99.840109999999996,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5340,"POWERLINKV5_20151103070403","2013-10-23T18:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-45.77028,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5343,"POWERLINKV5_20151103070403","2013-10-23T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.400289999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5347,"POWERLINKV5_20151103070403","2013-10-23T19:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.400289999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5350,"POWERLINKV5_20151103070403","2013-10-23T19:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-37.710290000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5353,"POWERLINKV5_20151103070403","2013-10-23T19:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.250279999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5354,"POWERLINKV5_20151103070403","2013-10-23T19:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.250279999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5357,"POWERLINKV5_20151103070403","2013-10-23T19:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-36.070129999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5361,"POWERLINKV5_20151103070403","2013-10-23T19:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.9803,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5364,"POWERLINKV5_20151103070403","2013-10-23T20:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-21.650300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5367,"POWERLINKV5_20151103070403","2013-10-23T20:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-37.300310000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5371,"POWERLINKV5_20151103070403","2013-10-23T22:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-25.02007,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5373,"POWERLINKV5_20151103070403","2013-10-23T22:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-25.01013,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5376,"POWERLINKV5_20151103070403","2013-10-24T06:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-10.246969999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5379,"POWERLINKV5_20151103070403","2013-10-24T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.65685,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5382,"POWERLINKV5_20151103070403","2013-10-24T06:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.504200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5386,"POWERLINKV5_20151103070403","2013-10-24T06:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-15.016019999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5389,"POWERLINKV5_20151103070403","2013-10-24T07:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.59018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5392,"POWERLINKV5_20151103070403","2013-10-24T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-31.990179999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5396,"POWERLINKV5_20151103070403","2013-10-24T07:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-22.120180000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5399,"POWERLINKV5_20151103070403","2013-10-24T07:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.09018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5400,"POWERLINKV5_20151103070403","2013-10-24T07:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-11.09018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5403,"POWERLINKV5_20151103070403","2013-10-24T08:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.59018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5406,"POWERLINKV5_20151103070403","2013-10-24T08:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.25018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5410,"POWERLINKV5_20151103070403","2013-10-24T09:05:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-45.77026,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5414,"POWERLINKV5_20151103070403","2013-10-24T09:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-20.390180000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5417,"POWERLINKV5_20151103070403","2013-10-24T12:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-44.79992,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5421,"POWERLINKV5_20151103070403","2013-10-24T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-45.270069999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5424,"POWERLINKV5_20151103070403","2013-10-24T14:35:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-56.269930000000002,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5425,"POWERLINKV5_20151103070403","2013-10-24T14:40:00","Q>NIL_TR_TX1_4","Q-NIL","2013-02-28",1,-56.912239999999997,"Out= Nil, avoid overloading a Tarong 275/132 kV transformer (#1 or #4) on trip of the other Tarong 275/132 kV transformer (#1 or #4) (or either 7168 or 7183 Tarong - Chinchilla 132kV lines), Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5428,"POWERLINKV5_20151103070403","2013-10-24T19:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-11.590009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5431,"POWERLINKV5_20151103070403","2013-10-24T20:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.94004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5435,"POWERLINKV5_20151103070403","2013-10-25T06:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-10.30866,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5438,"POWERLINKV5_20151103070403","2013-10-25T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.29585,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5442,"POWERLINKV5_20151103070403","2013-10-25T06:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-21.160810000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5445,"POWERLINKV5_20151103070403","2013-10-25T07:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-32.00018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5448,"POWERLINKV5_20151103070403","2013-10-25T08:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-28.762260000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5449,"POWERLINKV5_20151103070403","2013-10-25T08:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-27.806159999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5455,"POWERLINKV5_20151103070403","2013-10-25T10:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-46.86018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5456,"POWERLINKV5_20151103070403","2013-10-25T10:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-46.86018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5460,"POWERLINKV5_20151103070403","2013-10-25T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-44.6599,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5463,"POWERLINKV5_20151103070403","2013-10-26T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12290.003049999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5467,"POWERLINKV5_20151103070403","2013-10-27T17:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-11.580220000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5470,"POWERLINKV5_20151103070403","2013-11-06T15:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.26756,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5473,"POWERLINKV5_20151103070403","2013-11-06T15:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.49034,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5474,"POWERLINKV5_20151103070403","2013-11-06T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.49034,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5477,"POWERLINKV5_20151103070403","2013-11-06T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.67024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5481,"POWERLINKV5_20151103070403","2013-11-06T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.490089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5484,"POWERLINKV5_20151103070403","2013-11-06T16:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.49024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5487,"POWERLINKV5_20151103070403","2013-11-06T16:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.547370000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5491,"POWERLINKV5_20151103070403","2013-11-06T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.490020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5492,"POWERLINKV5_20151103070403","2013-11-06T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.490020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5498,"POWERLINKV5_20151103070403","2013-11-06T16:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.490020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5499,"POWERLINKV5_20151103070403","2013-11-06T16:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.23011,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5502,"POWERLINKV5_20151103070403","2013-11-06T17:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.350989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5506,"POWERLINKV5_20151103070403","2013-11-06T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.229890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5509,"POWERLINKV5_20151103070403","2013-11-06T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.65907,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5512,"POWERLINKV5_20151103070403","2013-11-06T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.721520000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5516,"POWERLINKV5_20151103070403","2013-11-06T17:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.481369999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5519,"POWERLINKV5_20151103070403","2013-11-06T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.544699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5522,"POWERLINKV5_20151103070403","2013-11-06T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.926639999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5523,"POWERLINKV5_20151103070403","2013-11-06T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-18.570139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5526,"POWERLINKV5_20151103070403","2013-11-06T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.230039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5530,"POWERLINKV5_20151103070403","2013-11-06T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.229890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5533,"POWERLINKV5_20151103070403","2013-11-06T18:20:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.230039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5537,"POWERLINKV5_20151103070403","2013-11-06T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.61467,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5541,"POWERLINKV5_20151103070403","2013-11-06T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-19.231739999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5544,"POWERLINKV5_20151103070403","2013-11-06T18:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-18.78238,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5545,"POWERLINKV5_20151103070403","2013-11-06T18:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-19.19548,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5548,"POWERLINKV5_20151103070403","2013-11-06T18:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-18.757840000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5551,"POWERLINKV5_20151103070403","2013-11-06T19:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-18.3324,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5555,"POWERLINKV5_20151103070403","2013-11-06T19:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-18.167919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5558,"POWERLINKV5_20151103070403","2013-11-06T19:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.230160000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5561,"POWERLINKV5_20151103070403","2013-11-06T19:30:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.49006,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5565,"POWERLINKV5_20151103070403","2013-11-06T19:40:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.490259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5568,"POWERLINKV5_20151103070403","2013-11-06T19:45:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-17.490159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5569,"POWERLINKV5_20151103070403","2013-11-06T19:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-17.209710000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5574,"POWERLINKV5_20151103070403","2013-11-06T20:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-16.5703,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5576,"POWERLINKV5_20151103070403","2013-11-06T20:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-15.216480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5580,"POWERLINKV5_20151103070403","2013-11-06T20:55:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-14.85317,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5583,"POWERLINKV5_20151103070403","2013-11-06T21:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-15.10472,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5586,"POWERLINKV5_20151103070403","2013-11-06T21:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-06-24",1,-15.674289999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5590,"POWERLINKV5_20151103070403","2013-11-06T22:15:00","Q>NIL_BI_FB","Q-NIL","2013-06-24",1,-12.47504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5593,"POWERLINKV5_20151103070403","2013-11-12T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.62167,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5594,"POWERLINKV5_20151103070403","2013-11-12T06:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.62167,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5597,"POWERLINKV5_20151103070403","2013-11-12T07:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-51.107990000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5600,"POWERLINKV5_20151103070403","2013-11-12T07:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.063459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5604,"POWERLINKV5_20151103070403","2013-11-12T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.230149999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5607,"POWERLINKV5_20151103070403","2013-11-12T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.911480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5611,"POWERLINKV5_20151103070403","2013-11-12T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.650849999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5615,"POWERLINKV5_20151103070403","2013-11-12T08:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.893619999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5618,"POWERLINKV5_20151103070403","2013-11-12T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.643139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5619,"POWERLINKV5_20151103070403","2013-11-12T08:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.419560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5622,"POWERLINKV5_20151103070403","2013-11-12T08:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.426490000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5625,"POWERLINKV5_20151103070403","2013-11-12T08:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.647590000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5629,"POWERLINKV5_20151103070403","2013-11-12T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.430910000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5632,"POWERLINKV5_20151103070403","2013-11-12T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.427340000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5636,"POWERLINKV5_20151103070403","2013-11-12T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.133669999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5639,"POWERLINKV5_20151103070403","2013-11-12T09:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.94613,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5642,"POWERLINKV5_20151103070403","2013-11-12T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.030999999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5643,"POWERLINKV5_20151103070403","2013-11-12T09:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.50536,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5646,"POWERLINKV5_20151103070403","2013-11-12T09:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.882909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5650,"POWERLINKV5_20151103070403","2013-11-12T09:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.735220000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5652,"POWERLINKV5_20151103070403","2013-11-12T09:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.386890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5657,"POWERLINKV5_20151103070403","2013-11-12T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.46519,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5661,"POWERLINKV5_20151103070403","2013-11-12T10:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.549880000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5664,"POWERLINKV5_20151103070403","2013-11-12T10:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.072679999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5667,"POWERLINKV5_20151103070403","2013-11-12T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.190359999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5668,"POWERLINKV5_20151103070403","2013-11-12T10:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.190359999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5671,"POWERLINKV5_20151103070403","2013-11-12T10:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.411169999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5675,"POWERLINKV5_20151103070403","2013-11-12T11:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-63.097479999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5678,"POWERLINKV5_20151103070403","2013-11-12T11:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-78.404079999999993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5681,"POWERLINKV5_20151103070403","2013-11-12T17:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.755280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5685,"POWERLINKV5_20151103070403","2013-11-12T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.88017,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5688,"POWERLINKV5_20151103070403","2013-11-12T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.148999999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5689,"POWERLINKV5_20151103070403","2013-11-12T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.09981,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5693,"POWERLINKV5_20151103070403","2013-11-13T16:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-39.02026,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5696,"POWERLINKV5_20151103070403","2013-11-13T16:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.230039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5700,"POWERLINKV5_20151103070403","2013-11-13T16:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.230039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5703,"POWERLINKV5_20151103070403","2013-11-14T16:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-53.130040000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5706,"POWERLINKV5_20151103070403","2013-11-14T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.12959,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5710,"POWERLINKV5_20151103070403","2013-11-18T07:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.466550000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5713,"POWERLINKV5_20151103070403","2013-11-18T08:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.430580000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5714,"POWERLINKV5_20151103070403","2013-11-18T08:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.430580000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5717,"POWERLINKV5_20151103070403","2013-11-18T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.73485,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5720,"POWERLINKV5_20151103070403","2013-11-18T08:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5724,"POWERLINKV5_20151103070403","2013-11-18T08:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-112.29980999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5727,"POWERLINKV5_20151103070403","2013-11-18T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.63569,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5730,"POWERLINKV5_20151103070403","2013-11-18T08:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.41325,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5735,"POWERLINKV5_20151103070403","2013-11-18T09:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.68811,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5738,"POWERLINKV5_20151103070403","2013-11-18T09:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.06087,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5739,"POWERLINKV5_20151103070403","2013-11-18T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.203279999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5742,"POWERLINKV5_20151103070403","2013-11-18T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.68507,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5745,"POWERLINKV5_20151103070403","2013-11-18T09:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.586080000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5749,"POWERLINKV5_20151103070403","2013-11-18T10:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.66888,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5752,"POWERLINKV5_20151103070403","2013-11-18T10:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.32549,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5755,"POWERLINKV5_20151103070403","2013-11-18T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.20032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5759,"POWERLINKV5_20151103070403","2013-11-18T10:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.749000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5762,"POWERLINKV5_20151103070403","2013-11-18T11:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.20505,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5763,"POWERLINKV5_20151103070403","2013-11-18T11:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.490399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5766,"POWERLINKV5_20151103070403","2013-11-18T11:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.99488,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5771,"POWERLINKV5_20151103070403","2013-11-18T12:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.981159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5774,"POWERLINKV5_20151103070403","2013-11-18T12:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065860000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5777,"POWERLINKV5_20151103070403","2013-11-18T12:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.35177,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5781,"POWERLINKV5_20151103070403","2013-11-18T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.811540000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5784,"POWERLINKV5_20151103070403","2013-11-18T12:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.349259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5787,"POWERLINKV5_20151103070403","2013-11-18T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.38381,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5788,"POWERLINKV5_20151103070403","2013-11-18T13:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.38381,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5791,"POWERLINKV5_20151103070403","2013-11-18T13:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.06601,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5794,"POWERLINKV5_20151103070403","2013-11-18T13:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.06601,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5798,"POWERLINKV5_20151103070403","2013-11-18T13:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.77965,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5801,"POWERLINKV5_20151103070403","2013-11-18T13:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.78848,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5805,"POWERLINKV5_20151103070403","2013-11-18T13:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.67991,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5808,"POWERLINKV5_20151103070403","2013-11-18T13:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5812,"POWERLINKV5_20151103070403","2013-11-18T14:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5813,"POWERLINKV5_20151103070403","2013-11-18T14:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5816,"POWERLINKV5_20151103070403","2013-11-18T14:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5820,"POWERLINKV5_20151103070403","2013-11-18T14:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.123699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5823,"POWERLINKV5_20151103070403","2013-11-18T14:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.826499999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5826,"POWERLINKV5_20151103070403","2013-11-18T14:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.80829,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5830,"POWERLINKV5_20151103070403","2013-11-18T14:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5833,"POWERLINKV5_20151103070403","2013-11-18T15:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.123670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5836,"POWERLINKV5_20151103070403","2013-11-18T15:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.95243,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5837,"POWERLINKV5_20151103070403","2013-11-18T15:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.96903,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5840,"POWERLINKV5_20151103070403","2013-11-18T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.974930000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5844,"POWERLINKV5_20151103070403","2013-11-18T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.057539999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5847,"POWERLINKV5_20151103070403","2013-11-18T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.22856,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5849,"POWERLINKV5_20151103070403","2013-11-18T15:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.991400000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5855,"POWERLINKV5_20151103070403","2013-11-18T16:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.987819999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5858,"POWERLINKV5_20151103070403","2013-11-18T16:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.843059999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5861,"POWERLINKV5_20151103070403","2013-11-18T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.303380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5862,"POWERLINKV5_20151103070403","2013-11-18T16:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.303380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5865,"POWERLINKV5_20151103070403","2013-11-18T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.288720000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5869,"POWERLINKV5_20151103070403","2013-11-18T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.832719999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5872,"POWERLINKV5_20151103070403","2013-11-18T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5875,"POWERLINKV5_20151103070403","2013-11-18T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.23038,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5879,"POWERLINKV5_20151103070403","2013-11-18T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.23038,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5882,"POWERLINKV5_20151103070403","2013-11-18T17:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.974689999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5883,"POWERLINKV5_20151103070403","2013-11-18T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.23038,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5886,"POWERLINKV5_20151103070403","2013-11-18T17:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.833680000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5890,"POWERLINKV5_20151103070403","2013-11-18T17:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5894,"POWERLINKV5_20151103070403","2013-11-18T17:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5897,"POWERLINKV5_20151103070403","2013-11-18T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123640000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5900,"POWERLINKV5_20151103070403","2013-11-18T17:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5904,"POWERLINKV5_20151103070403","2013-11-18T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.248169999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5907,"POWERLINKV5_20151103070403","2013-11-18T18:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.124320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5908,"POWERLINKV5_20151103070403","2013-11-18T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.124320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5911,"POWERLINKV5_20151103070403","2013-11-18T18:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.36111,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5914,"POWERLINKV5_20151103070403","2013-11-18T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.012740000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5918,"POWERLINKV5_20151103070403","2013-11-18T18:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.868510000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5921,"POWERLINKV5_20151103070403","2013-11-18T19:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.123640000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5925,"POWERLINKV5_20151103070403","2013-11-18T19:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.57635,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5928,"POWERLINKV5_20151103070403","2013-11-18T19:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.49987,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5931,"POWERLINKV5_20151103070403","2013-11-18T19:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5933,"POWERLINKV5_20151103070403","2013-11-18T19:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5936,"POWERLINKV5_20151103070403","2013-11-18T22:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.941800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5939,"POWERLINKV5_20151103070403","2013-11-18T22:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.08437,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5943,"POWERLINKV5_20151103070403","2013-11-19T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.41775,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5946,"POWERLINKV5_20151103070403","2013-11-19T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5950,"POWERLINKV5_20151103070403","2013-11-19T05:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.05692,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5953,"POWERLINKV5_20151103070403","2013-11-19T06:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.30729,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5956,"POWERLINKV5_20151103070403","2013-11-19T06:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065910000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5957,"POWERLINKV5_20151103070403","2013-11-19T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5960,"POWERLINKV5_20151103070403","2013-11-19T06:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5963,"POWERLINKV5_20151103070403","2013-11-19T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5967,"POWERLINKV5_20151103070403","2013-11-19T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5972,"POWERLINKV5_20151103070403","2013-11-19T06:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.19336,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5975,"POWERLINKV5_20151103070403","2013-11-19T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5978,"POWERLINKV5_20151103070403","2013-11-19T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.300319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5981,"POWERLINKV5_20151103070403","2013-11-19T07:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5982,"POWERLINKV5_20151103070403","2013-11-19T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5985,"POWERLINKV5_20151103070403","2013-11-19T07:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.86036,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5989,"POWERLINKV5_20151103070403","2013-11-19T07:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.35162,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5992,"POWERLINKV5_20151103070403","2013-11-19T07:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5995,"POWERLINKV5_20151103070403","2013-11-19T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[5999,"POWERLINKV5_20151103070403","2013-11-19T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6002,"POWERLINKV5_20151103070403","2013-11-19T08:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.25033,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6005,"POWERLINKV5_20151103070403","2013-11-19T08:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.06597,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6006,"POWERLINKV5_20151103070403","2013-11-19T08:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.06597,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6009,"POWERLINKV5_20151103070403","2013-11-19T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.79002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6014,"POWERLINKV5_20151103070403","2013-11-19T08:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6017,"POWERLINKV5_20151103070403","2013-11-19T08:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.84159,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6020,"POWERLINKV5_20151103070403","2013-11-19T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.754300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6024,"POWERLINKV5_20151103070403","2013-11-19T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.77333,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6027,"POWERLINKV5_20151103070403","2013-11-19T09:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6030,"POWERLINKV5_20151103070403","2013-11-19T09:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.932589999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6031,"POWERLINKV5_20151103070403","2013-11-19T09:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6034,"POWERLINKV5_20151103070403","2013-11-19T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.810320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6038,"POWERLINKV5_20151103070403","2013-11-19T09:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.727460000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6041,"POWERLINKV5_20151103070403","2013-11-19T09:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6044,"POWERLINKV5_20151103070403","2013-11-19T09:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.524369999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6048,"POWERLINKV5_20151103070403","2013-11-19T10:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.95754,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6050,"POWERLINKV5_20151103070403","2013-11-19T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6053,"POWERLINKV5_20151103070403","2013-11-19T10:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6056,"POWERLINKV5_20151103070403","2013-11-19T10:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.98151,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6059,"POWERLINKV5_20151103070403","2013-11-19T10:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.02271,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6063,"POWERLINKV5_20151103070403","2013-11-19T10:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.87374,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6066,"POWERLINKV5_20151103070403","2013-11-19T10:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6069,"POWERLINKV5_20151103070403","2013-11-19T10:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.75032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6073,"POWERLINKV5_20151103070403","2013-11-19T11:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.104380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6076,"POWERLINKV5_20151103070403","2013-11-19T11:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.092829999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6077,"POWERLINKV5_20151103070403","2013-11-19T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.712199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6080,"POWERLINKV5_20151103070403","2013-11-19T11:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6083,"POWERLINKV5_20151103070403","2013-11-19T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.86619,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6087,"POWERLINKV5_20151103070403","2013-11-19T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.894159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6091,"POWERLINKV5_20151103070403","2013-11-19T12:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.434950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6095,"POWERLINKV5_20151103070403","2013-11-19T12:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.67282,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6098,"POWERLINKV5_20151103070403","2013-11-19T12:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.066079999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6101,"POWERLINKV5_20151103070403","2013-11-19T12:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.836349999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6102,"POWERLINKV5_20151103070403","2013-11-19T12:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.836349999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6105,"POWERLINKV5_20151103070403","2013-11-19T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.377829999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6108,"POWERLINKV5_20151103070403","2013-11-19T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.72537,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6112,"POWERLINKV5_20151103070403","2013-11-19T15:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.5495,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6115,"POWERLINKV5_20151103070403","2013-11-19T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6119,"POWERLINKV5_20151103070403","2013-11-19T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-40.64902,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6122,"POWERLINKV5_20151103070403","2013-11-19T18:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-36.470480000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6125,"POWERLINKV5_20151103070403","2013-11-20T05:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.24489,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6128,"POWERLINKV5_20151103070403","2013-11-20T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.2281,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6130,"POWERLINKV5_20151103070403","2013-11-20T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.321719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6133,"POWERLINKV5_20151103070403","2013-11-20T05:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066050000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6137,"POWERLINKV5_20151103070403","2013-11-20T06:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.19012,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6140,"POWERLINKV5_20151103070403","2013-11-20T06:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.98241,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6144,"POWERLINKV5_20151103070403","2013-11-20T06:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.298109999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6147,"POWERLINKV5_20151103070403","2013-11-20T07:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.94515,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6150,"POWERLINKV5_20151103070403","2013-11-20T07:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6151,"POWERLINKV5_20151103070403","2013-11-20T07:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.056940000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6154,"POWERLINKV5_20151103070403","2013-11-20T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.03284,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6158,"POWERLINKV5_20151103070403","2013-11-20T09:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.6496,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6161,"POWERLINKV5_20151103070403","2013-11-20T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.448,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6164,"POWERLINKV5_20151103070403","2013-11-20T13:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.704050000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6169,"POWERLINKV5_20151103070403","2013-11-20T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.06006,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6172,"POWERLINKV5_20151103070403","2013-11-20T15:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.113890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6175,"POWERLINKV5_20151103070403","2013-11-20T16:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-25.580159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6176,"POWERLINKV5_20151103070403","2013-11-20T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-25.580159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6179,"POWERLINKV5_20151103070403","2013-11-20T16:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.682600000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6183,"POWERLINKV5_20151103070403","2013-11-20T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.23063,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6186,"POWERLINKV5_20151103070403","2013-11-20T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.23245,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6189,"POWERLINKV5_20151103070403","2013-11-20T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.078239999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6193,"POWERLINKV5_20151103070403","2013-11-20T17:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.2844,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6196,"POWERLINKV5_20151103070403","2013-11-21T05:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.24672,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6197,"POWERLINKV5_20151103070403","2013-11-21T05:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.83658,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6200,"POWERLINKV5_20151103070403","2013-11-21T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.8444,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6203,"POWERLINKV5_20151103070403","2013-11-21T05:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.54867,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6206,"POWERLINKV5_20151103070403","2013-11-21T06:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.025840000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6211,"POWERLINKV5_20151103070403","2013-11-21T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.886320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6214,"POWERLINKV5_20151103070403","2013-11-21T06:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.820260000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6218,"POWERLINKV5_20151103070403","2013-11-21T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230440000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6221,"POWERLINKV5_20151103070403","2013-11-21T06:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.542470000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6222,"POWERLINKV5_20151103070403","2013-11-21T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.542470000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6225,"POWERLINKV5_20151103070403","2013-11-21T06:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.73546,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6228,"POWERLINKV5_20151103070403","2013-11-21T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.253810000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6232,"POWERLINKV5_20151103070403","2013-11-21T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.74732,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6235,"POWERLINKV5_20151103070403","2013-11-21T07:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.220359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6238,"POWERLINKV5_20151103070403","2013-11-21T07:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.556260000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6242,"POWERLINKV5_20151103070403","2013-11-21T07:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.59845,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6245,"POWERLINKV5_20151103070403","2013-11-21T07:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.46932,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6247,"POWERLINKV5_20151103070403","2013-11-21T07:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.638280000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6250,"POWERLINKV5_20151103070403","2013-11-21T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.775369999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6253,"POWERLINKV5_20151103070403","2013-11-21T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.813140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6257,"POWERLINKV5_20151103070403","2013-11-21T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.359120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6260,"POWERLINKV5_20151103070403","2013-11-21T08:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.388110000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6264,"POWERLINKV5_20151103070403","2013-11-21T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.590669999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6267,"POWERLINKV5_20151103070403","2013-11-21T08:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.0839,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6270,"POWERLINKV5_20151103070403","2013-11-21T08:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.004799999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6271,"POWERLINKV5_20151103070403","2013-11-21T08:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.542660000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6274,"POWERLINKV5_20151103070403","2013-11-21T08:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.028680000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6277,"POWERLINKV5_20151103070403","2013-11-21T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.120270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6281,"POWERLINKV5_20151103070403","2013-11-21T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.767900000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6284,"POWERLINKV5_20151103070403","2013-11-21T09:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.230270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6288,"POWERLINKV5_20151103070403","2013-11-21T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.27805,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6292,"POWERLINKV5_20151103070403","2013-11-21T09:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.620450000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6295,"POWERLINKV5_20151103070403","2013-11-21T09:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.256440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6296,"POWERLINKV5_20151103070403","2013-11-21T09:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.256440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6299,"POWERLINKV5_20151103070403","2013-11-21T09:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.120270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6302,"POWERLINKV5_20151103070403","2013-11-21T10:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.620450000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6306,"POWERLINKV5_20151103070403","2013-11-21T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-26.030270000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6309,"POWERLINKV5_20151103070403","2013-11-21T10:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-26.180330000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6313,"POWERLINKV5_20151103070403","2013-11-21T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.140440000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6316,"POWERLINKV5_20151103070403","2013-11-21T10:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.609010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6319,"POWERLINKV5_20151103070403","2013-11-21T10:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.581240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6320,"POWERLINKV5_20151103070403","2013-11-21T10:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.581240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6323,"POWERLINKV5_20151103070403","2013-11-21T11:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.081209999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6329,"POWERLINKV5_20151103070403","2013-11-21T11:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.12838,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6331,"POWERLINKV5_20151103070403","2013-11-21T11:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.609279999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6334,"POWERLINKV5_20151103070403","2013-11-21T11:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.59693,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6338,"POWERLINKV5_20151103070403","2013-11-21T11:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.986070000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6341,"POWERLINKV5_20151103070403","2013-11-21T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.80592,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6344,"POWERLINKV5_20151103070403","2013-11-21T11:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.3871,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6345,"POWERLINKV5_20151103070403","2013-11-21T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.464469999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6348,"POWERLINKV5_20151103070403","2013-11-21T12:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.368359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6352,"POWERLINKV5_20151103070403","2013-11-21T12:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-26.640370000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6355,"POWERLINKV5_20151103070403","2013-11-21T12:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-25.210360000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6358,"POWERLINKV5_20151103070403","2013-11-21T12:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-25.110959999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6362,"POWERLINKV5_20151103070403","2013-11-21T12:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.283899999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6365,"POWERLINKV5_20151103070403","2013-11-21T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.80592,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6366,"POWERLINKV5_20151103070403","2013-11-21T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.80592,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6370,"POWERLINKV5_20151103070403","2013-11-21T13:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.568950000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6373,"POWERLINKV5_20151103070403","2013-11-21T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.672160000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6377,"POWERLINKV5_20151103070403","2013-11-21T13:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.273409999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6380,"POWERLINKV5_20151103070403","2013-11-21T13:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.945489999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6383,"POWERLINKV5_20151103070403","2013-11-21T14:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.791880000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6387,"POWERLINKV5_20151103070403","2013-11-21T14:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.569189999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6390,"POWERLINKV5_20151103070403","2013-11-21T14:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.140440000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6391,"POWERLINKV5_20151103070403","2013-11-21T14:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.027609999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6394,"POWERLINKV5_20151103070403","2013-11-21T15:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.370270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6397,"POWERLINKV5_20151103070403","2013-11-21T15:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.781040000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6401,"POWERLINKV5_20151103070403","2013-11-21T15:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.19032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6404,"POWERLINKV5_20151103070403","2013-11-21T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.370200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6407,"POWERLINKV5_20151103070403","2013-11-21T15:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-25.026240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6412,"POWERLINKV5_20151103070403","2013-11-21T16:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13050.471380000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6415,"POWERLINKV5_20151103070403","2013-11-21T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.833299999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6416,"POWERLINKV5_20151103070403","2013-11-21T16:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.833299999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6419,"POWERLINKV5_20151103070403","2013-11-21T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.375019999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6422,"POWERLINKV5_20151103070403","2013-11-21T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.57826,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6426,"POWERLINKV5_20151103070403","2013-11-21T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-23.347490000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6429,"POWERLINKV5_20151103070403","2013-11-21T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-23.919260000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6433,"POWERLINKV5_20151103070403","2013-11-21T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.921390000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6436,"POWERLINKV5_20151103070403","2013-11-21T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-24.37021,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6439,"POWERLINKV5_20151103070403","2013-11-21T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.72993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6440,"POWERLINKV5_20151103070403","2013-11-21T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.72993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6443,"POWERLINKV5_20151103070403","2013-11-21T17:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.82019,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6448,"POWERLINKV5_20151103070403","2013-11-21T17:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.867929999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6451,"POWERLINKV5_20151103070403","2013-11-21T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.391120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6454,"POWERLINKV5_20151103070403","2013-11-21T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.658939999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6458,"POWERLINKV5_20151103070403","2013-11-21T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.19575,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6461,"POWERLINKV5_20151103070403","2013-11-21T18:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.303260000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6464,"POWERLINKV5_20151103070403","2013-11-21T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.424969999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6465,"POWERLINKV5_20151103070403","2013-11-21T19:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.878540000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6468,"POWERLINKV5_20151103070403","2013-11-21T19:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.179480000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6471,"POWERLINKV5_20151103070403","2013-11-21T20:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123799999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6475,"POWERLINKV5_20151103070403","2013-11-21T20:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.02327,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6478,"POWERLINKV5_20151103070403","2013-11-21T20:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.12378,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6482,"POWERLINKV5_20151103070403","2013-11-21T21:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.230329999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6485,"POWERLINKV5_20151103070403","2013-11-21T21:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.183680000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6489,"POWERLINKV5_20151103070403","2013-11-21T21:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.29269,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6490,"POWERLINKV5_20151103070403","2013-11-21T21:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.29269,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6493,"POWERLINKV5_20151103070403","2013-11-21T21:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.12368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6497,"POWERLINKV5_20151103070403","2013-11-21T21:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.746460000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6500,"POWERLINKV5_20151103070403","2013-11-21T21:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.065989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6503,"POWERLINKV5_20151103070403","2013-11-21T22:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.42346,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6507,"POWERLINKV5_20151103070403","2013-11-21T22:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.99708,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6510,"POWERLINKV5_20151103070403","2013-11-21T22:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.95443,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6513,"POWERLINKV5_20151103070403","2013-11-21T22:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.569800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6514,"POWERLINKV5_20151103070403","2013-11-21T22:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.569800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6517,"POWERLINKV5_20151103070403","2013-11-21T23:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-133.56996000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6521,"POWERLINKV5_20151103070403","2013-11-21T23:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.025040000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6526,"POWERLINKV5_20151103070403","2013-11-21T23:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.78234,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6528,"POWERLINKV5_20151103070403","2013-11-21T23:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.40136,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6532,"POWERLINKV5_20151103070403","2013-11-22T00:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.77304,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6535,"POWERLINKV5_20151103070403","2013-11-22T00:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.75257,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6536,"POWERLINKV5_20151103070403","2013-11-22T00:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.75257,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6539,"POWERLINKV5_20151103070403","2013-11-22T00:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.05012,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6542,"POWERLINKV5_20151103070403","2013-11-22T00:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.37318,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6546,"POWERLINKV5_20151103070403","2013-11-22T00:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.76051,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6549,"POWERLINKV5_20151103070403","2013-11-22T01:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.777760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6552,"POWERLINKV5_20151103070403","2013-11-22T01:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.58761,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6556,"POWERLINKV5_20151103070403","2013-11-22T01:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.483919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6559,"POWERLINKV5_20151103070403","2013-11-22T01:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.14124,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6560,"POWERLINKV5_20151103070403","2013-11-22T01:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.14124,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6563,"POWERLINKV5_20151103070403","2013-11-22T01:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.89554,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6567,"POWERLINKV5_20151103070403","2013-11-22T02:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.702389999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6571,"POWERLINKV5_20151103070403","2013-11-22T03:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.75028,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6574,"POWERLINKV5_20151103070403","2013-11-22T03:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.050280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6577,"POWERLINKV5_20151103070403","2013-11-22T03:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.37246,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6581,"POWERLINKV5_20151103070403","2013-11-22T04:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.74553,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6584,"POWERLINKV5_20151103070403","2013-11-22T04:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.54813,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6585,"POWERLINKV5_20151103070403","2013-11-22T05:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.968640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6588,"POWERLINKV5_20151103070403","2013-11-22T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.243590000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6591,"POWERLINKV5_20151103070403","2013-11-22T05:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.369980000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6595,"POWERLINKV5_20151103070403","2013-11-22T06:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.364450000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6598,"POWERLINKV5_20151103070403","2013-11-22T06:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.190429999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6602,"POWERLINKV5_20151103070403","2013-11-22T06:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6604,"POWERLINKV5_20151103070403","2013-11-22T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6609,"POWERLINKV5_20151103070403","2013-11-22T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.6004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6610,"POWERLINKV5_20151103070403","2013-11-22T06:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.6004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6613,"POWERLINKV5_20151103070403","2013-11-22T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.86828,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6616,"POWERLINKV5_20151103070403","2013-11-22T08:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.008100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6620,"POWERLINKV5_20151103070403","2013-11-22T09:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.212890000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6623,"POWERLINKV5_20151103070403","2013-11-22T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.655900000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6627,"POWERLINKV5_20151103070403","2013-11-22T10:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.941739999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6630,"POWERLINKV5_20151103070403","2013-11-22T11:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.765149999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6633,"POWERLINKV5_20151103070403","2013-11-22T11:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.774699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6634,"POWERLINKV5_20151103070403","2013-11-22T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.774699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6637,"POWERLINKV5_20151103070403","2013-11-22T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.02064,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6641,"POWERLINKV5_20151103070403","2013-11-22T12:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.10059,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6645,"POWERLINKV5_20151103070403","2013-11-22T12:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.10059,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6648,"POWERLINKV5_20151103070403","2013-11-22T12:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.039020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6652,"POWERLINKV5_20151103070403","2013-11-22T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.00376,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6655,"POWERLINKV5_20151103070403","2013-11-22T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.925369999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6658,"POWERLINKV5_20151103070403","2013-11-22T15:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.8133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6659,"POWERLINKV5_20151103070403","2013-11-22T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.33436,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6662,"POWERLINKV5_20151103070403","2013-11-22T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.28492,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6666,"POWERLINKV5_20151103070403","2013-11-22T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.891550000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6669,"POWERLINKV5_20151103070403","2013-11-22T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.771920000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6672,"POWERLINKV5_20151103070403","2013-11-22T17:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.02327,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6676,"POWERLINKV5_20151103070403","2013-11-22T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.906749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6679,"POWERLINKV5_20151103070403","2013-11-22T20:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.94678,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6682,"POWERLINKV5_20151103070403","2013-11-22T20:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.20398,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6686,"POWERLINKV5_20151103070403","2013-11-22T20:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.68634,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6687,"POWERLINKV5_20151103070403","2013-11-22T20:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.3172,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6691,"POWERLINKV5_20151103070403","2013-11-22T20:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.68027,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6694,"POWERLINKV5_20151103070403","2013-11-22T21:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.28308,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6697,"POWERLINKV5_20151103070403","2013-11-22T21:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.400029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6701,"POWERLINKV5_20151103070403","2013-11-22T21:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.906269999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6704,"POWERLINKV5_20151103070403","2013-11-22T21:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.82498,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6705,"POWERLINKV5_20151103070403","2013-11-22T21:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.0411,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6708,"POWERLINKV5_20151103070403","2013-11-22T21:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.838190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6711,"POWERLINKV5_20151103070403","2013-11-22T21:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.436,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6715,"POWERLINKV5_20151103070403","2013-11-22T21:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.70167,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6718,"POWERLINKV5_20151103070403","2013-11-22T22:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.982100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6721,"POWERLINKV5_20151103070403","2013-11-22T22:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.247949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6723,"POWERLINKV5_20151103070403","2013-11-22T22:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.02215,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6729,"POWERLINKV5_20151103070403","2013-11-22T22:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.92672,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6730,"POWERLINKV5_20151103070403","2013-11-22T22:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.92672,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6733,"POWERLINKV5_20151103070403","2013-11-23T04:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.013909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6736,"POWERLINKV5_20151103070403","2013-11-23T04:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.050380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6740,"POWERLINKV5_20151103070403","2013-11-23T04:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.050380000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6743,"POWERLINKV5_20151103070403","2013-11-23T04:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.06038,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6746,"POWERLINKV5_20151103070403","2013-11-23T04:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.06038,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6750,"POWERLINKV5_20151103070403","2013-11-23T04:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.06048,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6753,"POWERLINKV5_20151103070403","2013-11-23T04:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.179080000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6754,"POWERLINKV5_20151103070403","2013-11-23T04:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.179080000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6757,"POWERLINKV5_20151103070403","2013-11-23T05:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.06057,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6760,"POWERLINKV5_20151103070403","2013-11-23T05:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.050560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6764,"POWERLINKV5_20151103070403","2013-11-23T05:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6768,"POWERLINKV5_20151103070403","2013-11-23T05:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6772,"POWERLINKV5_20151103070403","2013-11-23T05:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060689999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6775,"POWERLINKV5_20151103070403","2013-11-23T05:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060639999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6778,"POWERLINKV5_20151103070403","2013-11-23T05:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.050560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6779,"POWERLINKV5_20151103070403","2013-11-23T06:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6782,"POWERLINKV5_20151103070403","2013-11-23T06:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.97461,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6785,"POWERLINKV5_20151103070403","2013-11-23T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.210570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6789,"POWERLINKV5_20151103070403","2013-11-23T06:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.796749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6792,"POWERLINKV5_20151103070403","2013-11-23T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.16112,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6796,"POWERLINKV5_20151103070403","2013-11-23T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.467359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6799,"POWERLINKV5_20151103070403","2013-11-23T06:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6802,"POWERLINKV5_20151103070403","2013-11-23T06:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.49912,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6805,"POWERLINKV5_20151103070403","2013-11-23T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.030279999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6807,"POWERLINKV5_20151103070403","2013-11-23T07:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.06068,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6811,"POWERLINKV5_20151103070403","2013-11-23T07:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.06068,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6814,"POWERLINKV5_20151103070403","2013-11-23T07:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.060639999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6817,"POWERLINKV5_20151103070403","2013-11-23T07:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.06072,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6821,"POWERLINKV5_20151103070403","2013-11-23T07:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.20064,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6824,"POWERLINKV5_20151103070403","2013-11-23T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.060639999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6827,"POWERLINKV5_20151103070403","2013-11-23T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.390700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6828,"POWERLINKV5_20151103070403","2013-11-23T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.390700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6831,"POWERLINKV5_20151103070403","2013-11-23T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.06076,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6835,"POWERLINKV5_20151103070403","2013-11-23T08:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.1106,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6838,"POWERLINKV5_20151103070403","2013-11-23T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.060639999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6841,"POWERLINKV5_20151103070403","2013-11-23T08:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-83.718149999999994,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6846,"POWERLINKV5_20151103070403","2013-11-23T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.537199999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6849,"POWERLINKV5_20151103070403","2013-11-23T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.265000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6852,"POWERLINKV5_20151103070403","2013-11-23T16:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.455909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6853,"POWERLINKV5_20151103070403","2013-11-23T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.630890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6856,"POWERLINKV5_20151103070403","2013-11-23T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.734310000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6860,"POWERLINKV5_20151103070403","2013-11-23T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.198399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6863,"POWERLINKV5_20151103070403","2013-11-23T17:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.777089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6866,"POWERLINKV5_20151103070403","2013-11-23T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.350070000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6870,"POWERLINKV5_20151103070403","2013-11-24T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.033049999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6873,"POWERLINKV5_20151103070403","2013-11-24T08:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.62364,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6874,"POWERLINKV5_20151103070403","2013-11-24T08:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.62364,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6877,"POWERLINKV5_20151103070403","2013-11-24T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.919560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6880,"POWERLINKV5_20151103070403","2013-11-24T08:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.020300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6883,"POWERLINKV5_20151103070403","2013-11-24T09:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.066280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6888,"POWERLINKV5_20151103070403","2013-11-24T09:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.373340000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6891,"POWERLINKV5_20151103070403","2013-11-24T09:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.673640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6895,"POWERLINKV5_20151103070403","2013-11-24T09:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.931649999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6898,"POWERLINKV5_20151103070403","2013-11-24T09:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.02744,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6899,"POWERLINKV5_20151103070403","2013-11-24T09:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.666,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6902,"POWERLINKV5_20151103070403","2013-11-24T09:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.03556,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6905,"POWERLINKV5_20151103070403","2013-11-24T10:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.81298,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6909,"POWERLINKV5_20151103070403","2013-11-24T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6912,"POWERLINKV5_20151103070403","2013-11-24T10:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6915,"POWERLINKV5_20151103070403","2013-11-24T10:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.06603,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6919,"POWERLINKV5_20151103070403","2013-11-24T10:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.267300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6920,"POWERLINKV5_20151103070403","2013-11-24T10:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.267300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6924,"POWERLINKV5_20151103070403","2013-11-24T10:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.06603,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6927,"POWERLINKV5_20151103070403","2013-11-24T10:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.26545,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6930,"POWERLINKV5_20151103070403","2013-11-24T11:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.670820000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6934,"POWERLINKV5_20151103070403","2013-11-24T11:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.28603,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6937,"POWERLINKV5_20151103070403","2013-11-24T11:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.674670000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6941,"POWERLINKV5_20151103070403","2013-11-24T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.065989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6944,"POWERLINKV5_20151103070403","2013-11-24T11:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.736929999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6947,"POWERLINKV5_20151103070403","2013-11-24T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.129849999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6948,"POWERLINKV5_20151103070403","2013-11-24T11:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.129849999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6951,"POWERLINKV5_20151103070403","2013-11-24T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.73578,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6954,"POWERLINKV5_20151103070403","2013-11-24T12:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.35844,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6958,"POWERLINKV5_20151103070403","2013-11-24T12:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.147930000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6961,"POWERLINKV5_20151103070403","2013-11-24T12:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.40128,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6966,"POWERLINKV5_20151103070403","2013-11-24T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.985440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6969,"POWERLINKV5_20151103070403","2013-11-24T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.988910000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6972,"POWERLINKV5_20151103070403","2013-11-24T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.005280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6973,"POWERLINKV5_20151103070403","2013-11-24T12:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.43103,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6976,"POWERLINKV5_20151103070403","2013-11-24T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066240000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6980,"POWERLINKV5_20151103070403","2013-11-24T13:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.946200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6983,"POWERLINKV5_20151103070403","2013-11-24T13:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.316230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6986,"POWERLINKV5_20151103070403","2013-11-24T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.731120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6990,"POWERLINKV5_20151103070403","2013-11-24T13:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.60876,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6993,"POWERLINKV5_20151103070403","2013-11-24T13:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.979480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6996,"POWERLINKV5_20151103070403","2013-11-24T13:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.99006,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[6997,"POWERLINKV5_20151103070403","2013-11-24T13:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.693490000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7002,"POWERLINKV5_20151103070403","2013-11-24T14:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.270050000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7005,"POWERLINKV5_20151103070403","2013-11-24T14:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.702660000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7008,"POWERLINKV5_20151103070403","2013-11-24T14:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.066190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7011,"POWERLINKV5_20151103070403","2013-11-24T14:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.95194,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7015,"POWERLINKV5_20151103070403","2013-11-24T14:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.532360000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7018,"POWERLINKV5_20151103070403","2013-11-24T14:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.164400000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7021,"POWERLINKV5_20151103070403","2013-11-24T15:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.011760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7022,"POWERLINKV5_20151103070403","2013-11-24T15:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.011760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7025,"POWERLINKV5_20151103070403","2013-11-24T15:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.15132,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7029,"POWERLINKV5_20151103070403","2013-11-24T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.669619999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7032,"POWERLINKV5_20151103070403","2013-11-24T15:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.43562,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7035,"POWERLINKV5_20151103070403","2013-11-24T15:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.93628,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7039,"POWERLINKV5_20151103070403","2013-11-24T15:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.232430000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7043,"POWERLINKV5_20151103070403","2013-11-24T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.663920000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7044,"POWERLINKV5_20151103070403","2013-11-24T15:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.663920000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7047,"POWERLINKV5_20151103070403","2013-11-24T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.408169999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7050,"POWERLINKV5_20151103070403","2013-11-24T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.088619999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7054,"POWERLINKV5_20151103070403","2013-11-24T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.812000000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7057,"POWERLINKV5_20151103070403","2013-11-24T16:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.943180000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7060,"POWERLINKV5_20151103070403","2013-11-24T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.94342,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7064,"POWERLINKV5_20151103070403","2013-11-24T16:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.926179999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7067,"POWERLINKV5_20151103070403","2013-11-24T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.110440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7068,"POWERLINKV5_20151103070403","2013-11-24T16:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.110440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7071,"POWERLINKV5_20151103070403","2013-11-24T17:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.59177,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7074,"POWERLINKV5_20151103070403","2013-11-24T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.572150000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7078,"POWERLINKV5_20151103070403","2013-11-24T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.083079999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7080,"POWERLINKV5_20151103070403","2013-11-24T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.565819999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7086,"POWERLINKV5_20151103070403","2013-11-24T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.568729999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7089,"POWERLINKV5_20151103070403","2013-11-24T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.499700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7092,"POWERLINKV5_20151103070403","2013-11-24T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-23.49579,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7093,"POWERLINKV5_20151103070403","2013-11-24T18:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.964829999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7096,"POWERLINKV5_20151103070403","2013-11-24T18:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.811350000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7099,"POWERLINKV5_20151103070403","2013-11-24T18:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.516480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7103,"POWERLINKV5_20151103070403","2013-11-24T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.48021,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7106,"POWERLINKV5_20151103070403","2013-11-24T18:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.42784,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7110,"POWERLINKV5_20151103070403","2013-11-24T18:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.528680000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7113,"POWERLINKV5_20151103070403","2013-11-24T18:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.41131,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7116,"POWERLINKV5_20151103070403","2013-11-24T19:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.4352,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7117,"POWERLINKV5_20151103070403","2013-11-24T19:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.673749999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7121,"POWERLINKV5_20151103070403","2013-11-24T19:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7124,"POWERLINKV5_20151103070403","2013-11-24T19:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.17511,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7128,"POWERLINKV5_20151103070403","2013-11-24T19:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850529999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7131,"POWERLINKV5_20151103070403","2013-11-24T19:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.81044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7135,"POWERLINKV5_20151103070403","2013-11-24T19:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.81044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7138,"POWERLINKV5_20151103070403","2013-11-24T20:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.410640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7141,"POWERLINKV5_20151103070403","2013-11-24T20:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.81062,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7142,"POWERLINKV5_20151103070403","2013-11-24T20:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.81062,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7145,"POWERLINKV5_20151103070403","2013-11-24T20:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.405419999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7149,"POWERLINKV5_20151103070403","2013-11-24T20:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.93154,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7152,"POWERLINKV5_20151103070403","2013-11-24T20:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.327269999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7155,"POWERLINKV5_20151103070403","2013-11-24T20:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.142160000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7159,"POWERLINKV5_20151103070403","2013-11-24T21:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.992559999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7162,"POWERLINKV5_20151103070403","2013-11-24T21:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.252649999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7166,"POWERLINKV5_20151103070403","2013-11-24T21:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.09862,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7167,"POWERLINKV5_20151103070403","2013-11-24T21:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.530419999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7170,"POWERLINKV5_20151103070403","2013-11-24T21:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.443840000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7174,"POWERLINKV5_20151103070403","2013-11-24T21:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.56475,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7177,"POWERLINKV5_20151103070403","2013-11-24T21:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.48363,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7180,"POWERLINKV5_20151103070403","2013-11-24T21:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.1904,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7184,"POWERLINKV5_20151103070403","2013-11-24T22:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.505269999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7187,"POWERLINKV5_20151103070403","2013-11-25T01:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.35177,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7190,"POWERLINKV5_20151103070403","2013-11-25T01:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.349880000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7191,"POWERLINKV5_20151103070403","2013-11-25T04:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.1692,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7194,"POWERLINKV5_20151103070403","2013-11-25T04:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-10.505839999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7198,"POWERLINKV5_20151103070403","2013-11-25T05:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.29406,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7203,"POWERLINKV5_20151103070403","2013-11-25T05:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-92.588210000000004,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7205,"POWERLINKV5_20151103070403","2013-11-25T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.05308,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7209,"POWERLINKV5_20151103070403","2013-11-25T05:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.67431,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7212,"POWERLINKV5_20151103070403","2013-11-25T05:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.430949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7213,"POWERLINKV5_20151103070403","2013-11-25T06:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-11.60369,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7216,"POWERLINKV5_20151103070403","2013-11-25T06:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-10.66137,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7219,"POWERLINKV5_20151103070403","2013-11-25T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.1435,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7223,"POWERLINKV5_20151103070403","2013-11-25T06:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.53335,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7226,"POWERLINKV5_20151103070403","2013-11-25T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.155909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7229,"POWERLINKV5_20151103070403","2013-11-25T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-63.940190000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7233,"POWERLINKV5_20151103070403","2013-11-25T06:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.260249999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7236,"POWERLINKV5_20151103070403","2013-11-25T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.5718,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7237,"POWERLINKV5_20151103070403","2013-11-25T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.03124,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7240,"POWERLINKV5_20151103070403","2013-11-25T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.48382,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7244,"POWERLINKV5_20151103070403","2013-11-25T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.02055,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7248,"POWERLINKV5_20151103070403","2013-11-25T07:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.688490000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7251,"POWERLINKV5_20151103070403","2013-11-25T07:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.946389999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7255,"POWERLINKV5_20151103070403","2013-11-25T07:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.7531,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7258,"POWERLINKV5_20151103070403","2013-11-25T07:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.244689999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7261,"POWERLINKV5_20151103070403","2013-11-25T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.212399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7262,"POWERLINKV5_20151103070403","2013-11-25T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.212399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7265,"POWERLINKV5_20151103070403","2013-11-25T08:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.342690000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7268,"POWERLINKV5_20151103070403","2013-11-25T08:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.3248,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7272,"POWERLINKV5_20151103070403","2013-11-25T08:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.981190000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7275,"POWERLINKV5_20151103070403","2013-11-25T08:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.8553,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7279,"POWERLINKV5_20151103070403","2013-11-25T08:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.593109999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7281,"POWERLINKV5_20151103070403","2013-11-25T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.423690000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7286,"POWERLINKV5_20151103070403","2013-11-25T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.695499999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7287,"POWERLINKV5_20151103070403","2013-11-25T09:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-19.121230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7290,"POWERLINKV5_20151103070403","2013-11-25T09:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7293,"POWERLINKV5_20151103070403","2013-11-25T09:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.370270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7297,"POWERLINKV5_20151103070403","2013-11-25T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.230440000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7300,"POWERLINKV5_20151103070403","2013-11-25T09:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.734210000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7304,"POWERLINKV5_20151103070403","2013-11-25T09:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.535990000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7307,"POWERLINKV5_20151103070403","2013-11-25T09:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.029720000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7310,"POWERLINKV5_20151103070403","2013-11-25T10:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.655850000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7311,"POWERLINKV5_20151103070403","2013-11-25T10:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.370259999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7314,"POWERLINKV5_20151103070403","2013-11-25T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.932739999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7318,"POWERLINKV5_20151103070403","2013-11-25T10:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.472010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7322,"POWERLINKV5_20151103070403","2013-11-25T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.9559,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7325,"POWERLINKV5_20151103070403","2013-11-25T10:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.24044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7329,"POWERLINKV5_20151103070403","2013-11-25T10:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.989249999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7332,"POWERLINKV5_20151103070403","2013-11-25T10:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.908909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7335,"POWERLINKV5_20151103070403","2013-11-25T11:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.370259999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7336,"POWERLINKV5_20151103070403","2013-11-25T11:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.370259999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7339,"POWERLINKV5_20151103070403","2013-11-25T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.986090000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7343,"POWERLINKV5_20151103070403","2013-11-25T11:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.99457,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7346,"POWERLINKV5_20151103070403","2013-11-25T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.370259999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7349,"POWERLINKV5_20151103070403","2013-11-25T11:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.977959999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7353,"POWERLINKV5_20151103070403","2013-11-25T11:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.479659999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7356,"POWERLINKV5_20151103070403","2013-11-25T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.370259999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7359,"POWERLINKV5_20151103070403","2013-11-25T12:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.600090000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7361,"POWERLINKV5_20151103070403","2013-11-25T12:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-23.938459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7364,"POWERLINKV5_20151103070403","2013-11-25T12:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.472719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7368,"POWERLINKV5_20151103070403","2013-11-25T12:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.24044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7371,"POWERLINKV5_20151103070403","2013-11-25T12:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.010090000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7374,"POWERLINKV5_20151103070403","2013-11-25T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.611619999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7378,"POWERLINKV5_20151103070403","2013-11-25T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.010860000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7381,"POWERLINKV5_20151103070403","2013-11-25T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.55359,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7382,"POWERLINKV5_20151103070403","2013-11-25T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-21.55359,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7385,"POWERLINKV5_20151103070403","2013-11-25T13:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.811900000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7388,"POWERLINKV5_20151103070403","2013-11-25T13:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.31568,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7392,"POWERLINKV5_20151103070403","2013-11-25T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.604089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7395,"POWERLINKV5_20151103070403","2013-11-25T13:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-17.859089999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7400,"POWERLINKV5_20151103070403","2013-11-25T13:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.918749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7403,"POWERLINKV5_20151103070403","2013-11-25T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.51867,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7406,"POWERLINKV5_20151103070403","2013-11-25T14:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.031559999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7407,"POWERLINKV5_20151103070403","2013-11-25T14:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.053809999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7410,"POWERLINKV5_20151103070403","2013-11-25T14:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.99408,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7413,"POWERLINKV5_20151103070403","2013-11-25T14:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.020440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7417,"POWERLINKV5_20151103070403","2013-11-25T14:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.283570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7420,"POWERLINKV5_20151103070403","2013-11-25T14:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.411909999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7424,"POWERLINKV5_20151103070403","2013-11-25T14:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.699470000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7427,"POWERLINKV5_20151103070403","2013-11-25T14:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7430,"POWERLINKV5_20151103070403","2013-11-25T15:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7431,"POWERLINKV5_20151103070403","2013-11-25T15:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7434,"POWERLINKV5_20151103070403","2013-11-25T15:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.8505,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7437,"POWERLINKV5_20151103070403","2013-11-25T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7442,"POWERLINKV5_20151103070403","2013-11-25T15:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.850439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7445,"POWERLINKV5_20151103070403","2013-11-25T15:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.005490000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7449,"POWERLINKV5_20151103070403","2013-11-25T15:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-27.224959999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7452,"POWERLINKV5_20151103070403","2013-11-25T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-47.030479999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7455,"POWERLINKV5_20151103070403","2013-11-25T16:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.804760000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7456,"POWERLINKV5_20151103070403","2013-11-25T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.804760000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7459,"POWERLINKV5_20151103070403","2013-11-25T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-24.02853,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7462,"POWERLINKV5_20151103070403","2013-11-25T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.358320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7466,"POWERLINKV5_20151103070403","2013-11-25T16:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-26.417090000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7469,"POWERLINKV5_20151103070403","2013-11-25T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-26.602709999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7473,"POWERLINKV5_20151103070403","2013-11-25T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-53.360439999999997,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7476,"POWERLINKV5_20151103070403","2013-11-25T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-47.030439999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7478,"POWERLINKV5_20151103070403","2013-11-25T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-28.099430000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7481,"POWERLINKV5_20151103070403","2013-11-25T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.020009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7484,"POWERLINKV5_20151103070403","2013-11-25T17:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.496700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7488,"POWERLINKV5_20151103070403","2013-11-25T17:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-24.916969999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7491,"POWERLINKV5_20151103070403","2013-11-25T17:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-24.34656,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7494,"POWERLINKV5_20151103070403","2013-11-25T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.537320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7498,"POWERLINKV5_20151103070403","2013-11-25T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-24.078099999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7501,"POWERLINKV5_20151103070403","2013-11-25T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.370270000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7504,"POWERLINKV5_20151103070403","2013-11-25T18:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.592829999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7505,"POWERLINKV5_20151103070403","2013-11-25T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.634399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7508,"POWERLINKV5_20151103070403","2013-11-25T18:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.064080000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7512,"POWERLINKV5_20151103070403","2013-11-25T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.568680000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7515,"POWERLINKV5_20151103070403","2013-11-25T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.415189999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7519,"POWERLINKV5_20151103070403","2013-11-25T18:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-12.9392,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7523,"POWERLINKV5_20151103070403","2013-11-25T19:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-20.60341,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7526,"POWERLINKV5_20151103070403","2013-11-25T19:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.199020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7527,"POWERLINKV5_20151103070403","2013-11-25T19:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.656870000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7530,"POWERLINKV5_20151103070403","2013-11-25T19:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.081849999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7533,"POWERLINKV5_20151103070403","2013-11-25T19:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-20.53538,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7537,"POWERLINKV5_20151103070403","2013-11-25T19:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-22.499400000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7540,"POWERLINKV5_20151103070403","2013-11-25T19:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-22.02009,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7543,"POWERLINKV5_20151103070403","2013-11-25T19:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-21.179169999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7547,"POWERLINKV5_20151103070403","2013-11-25T20:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-17.706589999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7550,"POWERLINKV5_20151103070403","2013-11-25T20:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.123840000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7551,"POWERLINKV5_20151103070403","2013-11-25T20:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.548850000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7554,"POWERLINKV5_20151103070403","2013-11-25T20:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-15.060230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7560,"POWERLINKV5_20151103070403","2013-11-25T20:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.495559999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7562,"POWERLINKV5_20151103070403","2013-11-25T20:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.47818,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7565,"POWERLINKV5_20151103070403","2013-11-25T20:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.204890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7568,"POWERLINKV5_20151103070403","2013-11-25T20:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.85187,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7572,"POWERLINKV5_20151103070403","2013-11-25T21:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.651350000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7575,"POWERLINKV5_20151103070403","2013-11-25T21:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.84308,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7576,"POWERLINKV5_20151103070403","2013-11-25T21:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-14.84308,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7579,"POWERLINKV5_20151103070403","2013-11-25T21:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-15.06058,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7582,"POWERLINKV5_20151103070403","2013-11-25T21:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.41311,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7586,"POWERLINKV5_20151103070403","2013-11-25T21:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-13.206569999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7589,"POWERLINKV5_20151103070403","2013-11-25T21:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-13.63561,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7593,"POWERLINKV5_20151103070403","2013-11-25T21:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-12.17323,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7596,"POWERLINKV5_20151103070403","2013-11-25T22:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-11.45058,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7597,"POWERLINKV5_20151103070403","2013-11-25T22:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.12397,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7601,"POWERLINKV5_20151103070403","2013-11-25T22:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.15488,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7604,"POWERLINKV5_20151103070403","2013-11-25T22:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.908480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7607,"POWERLINKV5_20151103070403","2013-11-25T22:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-14.43322,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7611,"POWERLINKV5_20151103070403","2013-11-25T23:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-19.249079999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7614,"POWERLINKV5_20151103070403","2013-11-25T23:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-18.850359999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7618,"POWERLINKV5_20151103070403","2013-11-25T23:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.69096,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7621,"POWERLINKV5_20151103070403","2013-11-25T23:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-18.850449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7624,"POWERLINKV5_20151103070403","2013-11-25T23:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-12",1,-16.591200000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7625,"POWERLINKV5_20151103070403","2013-11-25T23:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-12",1,-16.123719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7628,"POWERLINKV5_20151103070403","2013-11-26T00:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.12351,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7631,"POWERLINKV5_20151103070403","2013-11-26T00:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.70659,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7635,"POWERLINKV5_20151103070403","2013-11-26T00:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.671139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7638,"POWERLINKV5_20151103070403","2013-11-26T00:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.42478,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7643,"POWERLINKV5_20151103070403","2013-11-26T03:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.050179999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7646,"POWERLINKV5_20151103070403","2013-11-26T03:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.6797,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7649,"POWERLINKV5_20151103070403","2013-11-26T03:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.378769999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7650,"POWERLINKV5_20151103070403","2013-11-26T03:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.378769999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7653,"POWERLINKV5_20151103070403","2013-11-26T04:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.44069,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7657,"POWERLINKV5_20151103070403","2013-11-26T04:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-103.56497,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7660,"POWERLINKV5_20151103070403","2013-11-26T04:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.32939,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7663,"POWERLINKV5_20151103070403","2013-11-26T04:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.040430000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7667,"POWERLINKV5_20151103070403","2013-11-26T04:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.45899,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7670,"POWERLINKV5_20151103070403","2013-11-26T05:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.16597,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7673,"POWERLINKV5_20151103070403","2013-11-26T05:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.21679,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7674,"POWERLINKV5_20151103070403","2013-11-26T05:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.21679,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7679,"POWERLINKV5_20151103070403","2013-11-26T05:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.25924,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7682,"POWERLINKV5_20151103070403","2013-11-26T05:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.049010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7685,"POWERLINKV5_20151103070403","2013-11-26T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.602169999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7688,"POWERLINKV5_20151103070403","2013-11-26T05:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.043600000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7692,"POWERLINKV5_20151103070403","2013-11-26T06:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.815840000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7695,"POWERLINKV5_20151103070403","2013-11-26T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.110479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7696,"POWERLINKV5_20151103070403","2013-11-26T06:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.110479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7699,"POWERLINKV5_20151103070403","2013-11-26T06:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.110440000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7702,"POWERLINKV5_20151103070403","2013-11-26T06:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.11036,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7706,"POWERLINKV5_20151103070403","2013-11-26T22:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.88683,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7709,"POWERLINKV5_20151103070403","2013-11-26T22:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.850290000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7712,"POWERLINKV5_20151103070403","2013-11-27T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.39376,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7716,"POWERLINKV5_20151103070403","2013-11-27T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.37865,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7720,"POWERLINKV5_20151103070403","2013-11-27T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.10436,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7721,"POWERLINKV5_20151103070403","2013-11-27T07:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.431330000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7724,"POWERLINKV5_20151103070403","2013-11-27T07:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.679449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7727,"POWERLINKV5_20151103070403","2013-11-27T07:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.160410000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7731,"POWERLINKV5_20151103070403","2013-11-27T07:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.060280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7734,"POWERLINKV5_20151103070403","2013-11-27T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.073889999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7737,"POWERLINKV5_20151103070403","2013-11-27T08:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.040590000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7741,"POWERLINKV5_20151103070403","2013-11-27T08:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.51155,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7744,"POWERLINKV5_20151103070403","2013-11-27T08:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.929089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7745,"POWERLINKV5_20151103070403","2013-11-27T08:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.37415,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7748,"POWERLINKV5_20151103070403","2013-11-27T08:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.447420000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7751,"POWERLINKV5_20151103070403","2013-11-27T08:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.884630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7757,"POWERLINKV5_20151103070403","2013-11-27T08:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.454709999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7759,"POWERLINKV5_20151103070403","2013-11-27T08:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.658580000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7763,"POWERLINKV5_20151103070403","2013-11-27T09:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85022,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7766,"POWERLINKV5_20151103070403","2013-11-27T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.850259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7769,"POWERLINKV5_20151103070403","2013-11-27T09:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.515350000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7770,"POWERLINKV5_20151103070403","2013-11-27T09:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.515350000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7773,"POWERLINKV5_20151103070403","2013-11-27T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.052330000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7776,"POWERLINKV5_20151103070403","2013-11-27T09:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.229949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7780,"POWERLINKV5_20151103070403","2013-11-27T09:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.50055,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7783,"POWERLINKV5_20151103070403","2013-11-27T09:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.546150000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7787,"POWERLINKV5_20151103070403","2013-11-27T10:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.11016,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7790,"POWERLINKV5_20151103070403","2013-11-27T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.314540000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7793,"POWERLINKV5_20151103070403","2013-11-27T10:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.622969999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7794,"POWERLINKV5_20151103070403","2013-11-27T10:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.622969999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7798,"POWERLINKV5_20151103070403","2013-11-27T10:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.234010000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7802,"POWERLINKV5_20151103070403","2013-11-27T10:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.26427,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7805,"POWERLINKV5_20151103070403","2013-11-27T10:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.11159,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7808,"POWERLINKV5_20151103070403","2013-11-27T10:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.136880000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7812,"POWERLINKV5_20151103070403","2013-11-27T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7815,"POWERLINKV5_20151103070403","2013-11-27T11:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7818,"POWERLINKV5_20151103070403","2013-11-27T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7819,"POWERLINKV5_20151103070403","2013-11-27T12:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7822,"POWERLINKV5_20151103070403","2013-11-27T12:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7826,"POWERLINKV5_20151103070403","2013-11-27T12:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.616599999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7829,"POWERLINKV5_20151103070403","2013-11-27T12:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85012,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7832,"POWERLINKV5_20151103070403","2013-11-27T12:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.000309999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7835,"POWERLINKV5_20151103070403","2013-11-27T12:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.850239999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7840,"POWERLINKV5_20151103070403","2013-11-27T12:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7843,"POWERLINKV5_20151103070403","2013-11-27T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.62133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7844,"POWERLINKV5_20151103070403","2013-11-27T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.62133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7847,"POWERLINKV5_20151103070403","2013-11-27T13:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.133520000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7851,"POWERLINKV5_20151103070403","2013-11-27T13:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.81531,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7854,"POWERLINKV5_20151103070403","2013-11-27T13:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.826530000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7857,"POWERLINKV5_20151103070403","2013-11-27T13:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.858720000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7861,"POWERLINKV5_20151103070403","2013-11-27T13:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.454989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7864,"POWERLINKV5_20151103070403","2013-11-27T14:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.213650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7865,"POWERLINKV5_20151103070403","2013-11-27T14:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-25.065149999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7868,"POWERLINKV5_20151103070403","2013-11-27T14:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.46613,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7871,"POWERLINKV5_20151103070403","2013-11-27T14:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.30368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7876,"POWERLINKV5_20151103070403","2013-11-27T14:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.7179,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7879,"POWERLINKV5_20151103070403","2013-11-27T14:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.275539999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7882,"POWERLINKV5_20151103070403","2013-11-27T14:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.77364,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7886,"POWERLINKV5_20151103070403","2013-11-27T14:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.097629999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7889,"POWERLINKV5_20151103070403","2013-11-27T15:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-21.868960000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7890,"POWERLINKV5_20151103070403","2013-11-27T15:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-21.868960000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7893,"POWERLINKV5_20151103070403","2013-11-27T15:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.85033,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7896,"POWERLINKV5_20151103070403","2013-11-27T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.329640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7900,"POWERLINKV5_20151103070403","2013-11-27T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.72588,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7903,"POWERLINKV5_20151103070403","2013-11-27T15:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.499130000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7906,"POWERLINKV5_20151103070403","2013-11-27T15:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.85023,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7910,"POWERLINKV5_20151103070403","2013-11-27T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.850280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7913,"POWERLINKV5_20151103070403","2013-11-27T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.850280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7917,"POWERLINKV5_20151103070403","2013-11-27T16:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.816890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7918,"POWERLINKV5_20151103070403","2013-11-27T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-20.816890000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7921,"POWERLINKV5_20151103070403","2013-11-27T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.012119999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7925,"POWERLINKV5_20151103070403","2013-11-27T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.002320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7928,"POWERLINKV5_20151103070403","2013-11-27T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.850280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7932,"POWERLINKV5_20151103070403","2013-11-27T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-20.750599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7935,"POWERLINKV5_20151103070403","2013-11-27T17:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.477799999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7938,"POWERLINKV5_20151103070403","2013-11-27T17:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.420940000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7939,"POWERLINKV5_20151103070403","2013-11-27T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.371839999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7942,"POWERLINKV5_20151103070403","2013-11-27T17:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.441230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7945,"POWERLINKV5_20151103070403","2013-11-27T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.850280000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7949,"POWERLINKV5_20151103070403","2013-11-27T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.85033,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7952,"POWERLINKV5_20151103070403","2013-11-27T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.535830000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7954,"POWERLINKV5_20151103070403","2013-11-27T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.000330000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7960,"POWERLINKV5_20151103070403","2013-11-27T18:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.45646,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7963,"POWERLINKV5_20151103070403","2013-11-27T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.449349999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7964,"POWERLINKV5_20151103070403","2013-11-27T18:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.449349999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7967,"POWERLINKV5_20151103070403","2013-11-27T18:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.264900000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7971,"POWERLINKV5_20151103070403","2013-11-27T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.353449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7974,"POWERLINKV5_20151103070403","2013-11-27T18:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.16328,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7977,"POWERLINKV5_20151103070403","2013-11-27T18:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.706800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7981,"POWERLINKV5_20151103070403","2013-11-27T18:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.622669999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7984,"POWERLINKV5_20151103070403","2013-11-27T19:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.765049999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7987,"POWERLINKV5_20151103070403","2013-11-28T04:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.65699,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7988,"POWERLINKV5_20151103070403","2013-11-28T04:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.65699,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7991,"POWERLINKV5_20151103070403","2013-11-28T06:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.772790000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7995,"POWERLINKV5_20151103070403","2013-11-28T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.50611,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[7999,"POWERLINKV5_20151103070403","2013-11-28T06:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.968990000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8002,"POWERLINKV5_20151103070403","2013-11-28T06:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.83032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8006,"POWERLINKV5_20151103070403","2013-11-28T06:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.18168,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8009,"POWERLINKV5_20151103070403","2013-11-28T06:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.24051,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8012,"POWERLINKV5_20151103070403","2013-11-28T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.677299999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8013,"POWERLINKV5_20151103070403","2013-11-28T07:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.00056,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8016,"POWERLINKV5_20151103070403","2013-11-28T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.392139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8020,"POWERLINKV5_20151103070403","2013-11-28T07:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.12368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8023,"POWERLINKV5_20151103070403","2013-11-28T07:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.356030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8026,"POWERLINKV5_20151103070403","2013-11-28T07:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.3368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8030,"POWERLINKV5_20151103070403","2013-11-28T07:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.278309999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8033,"POWERLINKV5_20151103070403","2013-11-28T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.53622,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8036,"POWERLINKV5_20151103070403","2013-11-28T07:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.521660000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8038,"POWERLINKV5_20151103070403","2013-11-28T08:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.52018,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8041,"POWERLINKV5_20151103070403","2013-11-28T08:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.287749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8045,"POWERLINKV5_20151103070403","2013-11-28T08:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.28866,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8048,"POWERLINKV5_20151103070403","2013-11-28T08:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.284269999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8051,"POWERLINKV5_20151103070403","2013-11-28T08:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.78257,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8055,"POWERLINKV5_20151103070403","2013-11-28T08:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.62753,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8058,"POWERLINKV5_20151103070403","2013-11-28T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.56223,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8059,"POWERLINKV5_20151103070403","2013-11-28T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.65682,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8062,"POWERLINKV5_20151103070403","2013-11-28T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.107520000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8065,"POWERLINKV5_20151103070403","2013-11-28T09:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.910399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8069,"POWERLINKV5_20151103070403","2013-11-28T09:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.62574,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8072,"POWERLINKV5_20151103070403","2013-11-28T09:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.63372,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8077,"POWERLINKV5_20151103070403","2013-11-28T09:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.657599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8080,"POWERLINKV5_20151103070403","2013-11-28T09:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.66553,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8083,"POWERLINKV5_20151103070403","2013-11-28T10:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.09103,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8084,"POWERLINKV5_20151103070403","2013-11-28T10:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.09103,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8087,"POWERLINKV5_20151103070403","2013-11-28T10:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.326969999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8090,"POWERLINKV5_20151103070403","2013-11-28T10:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.471769999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8094,"POWERLINKV5_20151103070403","2013-11-28T10:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.042729999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8097,"POWERLINKV5_20151103070403","2013-11-28T10:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.02065,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8101,"POWERLINKV5_20151103070403","2013-11-28T11:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.850490000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8104,"POWERLINKV5_20151103070403","2013-11-28T11:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.433489999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8107,"POWERLINKV5_20151103070403","2013-11-28T11:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.06039,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8108,"POWERLINKV5_20151103070403","2013-11-28T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.06039,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8111,"POWERLINKV5_20151103070403","2013-11-28T11:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.06039,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8114,"POWERLINKV5_20151103070403","2013-11-28T11:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.52943,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8119,"POWERLINKV5_20151103070403","2013-11-28T11:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.105039999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8122,"POWERLINKV5_20151103070403","2013-11-28T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.92681,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8126,"POWERLINKV5_20151103070403","2013-11-28T12:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.155460000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8129,"POWERLINKV5_20151103070403","2013-11-28T12:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.14115,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8132,"POWERLINKV5_20151103070403","2013-11-28T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.147749999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8133,"POWERLINKV5_20151103070403","2013-11-28T13:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.156289999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8136,"POWERLINKV5_20151103070403","2013-11-28T13:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8140,"POWERLINKV5_20151103070403","2013-11-28T13:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.593579999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8143,"POWERLINKV5_20151103070403","2013-11-28T13:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8146,"POWERLINKV5_20151103070403","2013-11-28T13:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.44961,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8150,"POWERLINKV5_20151103070403","2013-11-28T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.8505,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8151,"POWERLINKV5_20151103070403","2013-11-28T14:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8155,"POWERLINKV5_20151103070403","2013-11-28T14:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8156,"POWERLINKV5_20151103070403","2013-11-28T14:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.8504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8157,"POWERLINKV5_20151103070403","2013-11-28T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.3299,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8158,"POWERLINKV5_20151103070403","2013-11-28T16:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.3299,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8159,"POWERLINKV5_20151103070403","2013-11-28T17:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.00985,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8160,"POWERLINKV5_20151103070403","2013-11-28T17:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.00985,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8161,"POWERLINKV5_20151103070403","2013-11-28T19:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.35017,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8162,"POWERLINKV5_20151103070403","2013-11-28T19:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.35017,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8163,"POWERLINKV5_20151103070403","2013-11-28T21:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-20.315300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8164,"POWERLINKV5_20151103070403","2013-11-28T21:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.315300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8165,"POWERLINKV5_20151103070403","2013-11-28T21:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-60.132280000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8166,"POWERLINKV5_20151103070403","2013-11-28T21:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-60.132280000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8167,"POWERLINKV5_20151103070403","2013-11-28T23:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.71175,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8168,"POWERLINKV5_20151103070403","2013-11-28T23:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.71175,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8169,"POWERLINKV5_20151103070403","2013-11-29T00:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.00154,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8170,"POWERLINKV5_20151103070403","2013-11-29T00:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.00154,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8171,"POWERLINKV5_20151103070403","2013-11-29T01:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.46148,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8172,"POWERLINKV5_20151103070403","2013-11-29T01:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.46148,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8173,"POWERLINKV5_20151103070403","2013-11-29T01:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.010910000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8174,"POWERLINKV5_20151103070403","2013-11-29T01:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.010910000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8175,"POWERLINKV5_20151103070403","2013-11-29T01:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.615919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8176,"POWERLINKV5_20151103070403","2013-11-29T01:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.615919999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8177,"POWERLINKV5_20151103070403","2013-11-29T01:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.392939999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8178,"POWERLINKV5_20151103070403","2013-11-29T01:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.392939999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8179,"POWERLINKV5_20151103070403","2013-11-29T01:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.383760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8180,"POWERLINKV5_20151103070403","2013-11-29T01:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.383760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8181,"POWERLINKV5_20151103070403","2013-11-29T03:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-77.672409999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8182,"POWERLINKV5_20151103070403","2013-11-29T03:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-77.672409999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8183,"POWERLINKV5_20151103070403","2013-11-29T03:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-72.70993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8184,"POWERLINKV5_20151103070403","2013-11-29T03:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-72.70993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8185,"POWERLINKV5_20151103070403","2013-11-29T03:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-79.297719999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8186,"POWERLINKV5_20151103070403","2013-11-29T03:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-79.297719999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8187,"POWERLINKV5_20151103070403","2013-11-29T04:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-87.421469999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8188,"POWERLINKV5_20151103070403","2013-11-29T04:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-87.421469999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8189,"POWERLINKV5_20151103070403","2013-11-29T04:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.984579999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8190,"POWERLINKV5_20151103070403","2013-11-29T04:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.984579999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8191,"POWERLINKV5_20151103070403","2013-11-29T04:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.99141,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8192,"POWERLINKV5_20151103070403","2013-11-29T04:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.99141,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8193,"POWERLINKV5_20151103070403","2013-11-29T04:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.23471,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8194,"POWERLINKV5_20151103070403","2013-11-29T04:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.23471,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8195,"POWERLINKV5_20151103070403","2013-11-29T04:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.29701,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8196,"POWERLINKV5_20151103070403","2013-11-29T04:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.29701,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8197,"POWERLINKV5_20151103070403","2013-11-29T04:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.50454,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8198,"POWERLINKV5_20151103070403","2013-11-29T04:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.50454,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8199,"POWERLINKV5_20151103070403","2013-11-29T04:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.2858,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8200,"POWERLINKV5_20151103070403","2013-11-29T04:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.2858,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8201,"POWERLINKV5_20151103070403","2013-11-29T04:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.854749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8202,"POWERLINKV5_20151103070403","2013-11-29T04:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.854749999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8203,"POWERLINKV5_20151103070403","2013-11-29T04:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.484640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8204,"POWERLINKV5_20151103070403","2013-11-29T04:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.484640000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8205,"POWERLINKV5_20151103070403","2013-11-29T04:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.66145,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8206,"POWERLINKV5_20151103070403","2013-11-29T04:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.66145,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8207,"POWERLINKV5_20151103070403","2013-11-29T04:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.65442,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8208,"POWERLINKV5_20151103070403","2013-11-29T04:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.65442,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8209,"POWERLINKV5_20151103070403","2013-11-29T04:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.117290000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8210,"POWERLINKV5_20151103070403","2013-11-29T04:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.117290000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8211,"POWERLINKV5_20151103070403","2013-11-29T05:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-86.094309999999993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8212,"POWERLINKV5_20151103070403","2013-11-29T05:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-86.094309999999993,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8213,"POWERLINKV5_20151103070403","2013-11-29T05:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.29814,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8214,"POWERLINKV5_20151103070403","2013-11-29T05:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.29814,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8215,"POWERLINKV5_20151103070403","2013-11-29T05:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.94567,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8216,"POWERLINKV5_20151103070403","2013-11-29T05:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.94567,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8217,"POWERLINKV5_20151103070403","2013-11-29T05:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.035209999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8218,"POWERLINKV5_20151103070403","2013-11-29T05:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.035209999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8219,"POWERLINKV5_20151103070403","2013-11-29T05:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.23133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8220,"POWERLINKV5_20151103070403","2013-11-29T05:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.23133,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8221,"POWERLINKV5_20151103070403","2013-11-29T05:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.423159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8222,"POWERLINKV5_20151103070403","2013-11-29T05:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.423159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8223,"POWERLINKV5_20151103070403","2013-11-29T05:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.794650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8224,"POWERLINKV5_20151103070403","2013-11-29T05:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.794650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8225,"POWERLINKV5_20151103070403","2013-11-29T05:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.499650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8226,"POWERLINKV5_20151103070403","2013-11-29T05:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.499650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8227,"POWERLINKV5_20151103070403","2013-11-29T05:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.502560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8228,"POWERLINKV5_20151103070403","2013-11-29T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.502560000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8229,"POWERLINKV5_20151103070403","2013-11-29T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.182230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8230,"POWERLINKV5_20151103070403","2013-11-29T05:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.182230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8231,"POWERLINKV5_20151103070403","2013-11-29T05:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.835229999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8232,"POWERLINKV5_20151103070403","2013-11-29T05:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.835229999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8233,"POWERLINKV5_20151103070403","2013-11-29T05:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.05926,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8234,"POWERLINKV5_20151103070403","2013-11-29T05:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.05926,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8235,"POWERLINKV5_20151103070403","2013-11-29T06:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.74549,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8236,"POWERLINKV5_20151103070403","2013-11-29T06:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.74549,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8237,"POWERLINKV5_20151103070403","2013-11-29T06:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.47504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8238,"POWERLINKV5_20151103070403","2013-11-29T06:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.47504,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8239,"POWERLINKV5_20151103070403","2013-11-29T07:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.035259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8240,"POWERLINKV5_20151103070403","2013-11-29T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.035259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8241,"POWERLINKV5_20151103070403","2013-11-29T08:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.210599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8242,"POWERLINKV5_20151103070403","2013-11-29T08:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.210599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8243,"POWERLINKV5_20151103070403","2013-11-29T09:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.891159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8244,"POWERLINKV5_20151103070403","2013-11-29T09:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.891159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8245,"POWERLINKV5_20151103070403","2013-11-29T09:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.886760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8246,"POWERLINKV5_20151103070403","2013-11-29T09:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.886760000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8247,"POWERLINKV5_20151103070403","2013-11-29T11:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-25.77,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8248,"POWERLINKV5_20151103070403","2013-11-29T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-25.77,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8249,"POWERLINKV5_20151103070403","2013-11-29T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-34.43,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8250,"POWERLINKV5_20151103070403","2013-11-29T11:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-34.43,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8251,"POWERLINKV5_20151103070403","2013-11-29T11:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.22,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8252,"POWERLINKV5_20151103070403","2013-11-29T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.22,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8253,"POWERLINKV5_20151103070403","2013-11-29T11:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8254,"POWERLINKV5_20151103070403","2013-11-29T11:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8255,"POWERLINKV5_20151103070403","2013-11-29T11:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8256,"POWERLINKV5_20151103070403","2013-11-29T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8257,"POWERLINKV5_20151103070403","2013-11-29T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.61,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8258,"POWERLINKV5_20151103070403","2013-11-29T12:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.61,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8259,"POWERLINKV5_20151103070403","2013-11-29T12:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-34.42,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8260,"POWERLINKV5_20151103070403","2013-11-29T12:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-34.42,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8261,"POWERLINKV5_20151103070403","2013-11-29T12:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8262,"POWERLINKV5_20151103070403","2013-11-29T12:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-36.36,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8263,"POWERLINKV5_20151103070403","2013-11-29T12:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8264,"POWERLINKV5_20151103070403","2013-11-29T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8265,"POWERLINKV5_20151103070403","2013-11-29T12:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8266,"POWERLINKV5_20151103070403","2013-11-29T12:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8267,"POWERLINKV5_20151103070403","2013-11-29T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8268,"POWERLINKV5_20151103070403","2013-11-29T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-53.13,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8269,"POWERLINKV5_20151103070403","2013-11-29T13:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-43.11,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8270,"POWERLINKV5_20151103070403","2013-11-29T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-43.11,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8271,"POWERLINKV5_20151103070403","2013-11-29T13:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-43.08,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8272,"POWERLINKV5_20151103070403","2013-11-29T13:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-43.08,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8273,"POWERLINKV5_20151103070403","2013-11-29T13:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-43.080030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8274,"POWERLINKV5_20151103070403","2013-11-29T13:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-43.080030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8275,"POWERLINKV5_20151103070403","2013-11-29T13:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-39.080030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8276,"POWERLINKV5_20151103070403","2013-11-29T13:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-39.080030000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8277,"POWERLINKV5_20151103070403","2013-11-29T13:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-47.730029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8278,"POWERLINKV5_20151103070403","2013-11-29T13:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-47.730029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8279,"POWERLINKV5_20151103070403","2013-11-29T13:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-47.730029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8280,"POWERLINKV5_20151103070403","2013-11-29T13:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-47.730029999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8281,"POWERLINKV5_20151103070403","2013-11-29T13:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-50.440159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8282,"POWERLINKV5_20151103070403","2013-11-29T13:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-50.440159999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8283,"POWERLINKV5_20151103070403","2013-11-29T13:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-22.87002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8284,"POWERLINKV5_20151103070403","2013-11-29T13:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-22.87002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8285,"POWERLINKV5_20151103070403","2013-11-29T13:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-39.080019999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8286,"POWERLINKV5_20151103070403","2013-11-29T13:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-39.080019999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8287,"POWERLINKV5_20151103070403","2013-11-29T13:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-47.730020000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8288,"POWERLINKV5_20151103070403","2013-11-29T13:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-47.730020000000003,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8289,"POWERLINKV5_20151103070403","2013-11-29T14:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-43.079940000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8290,"POWERLINKV5_20151103070403","2013-11-29T14:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-43.079940000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8291,"POWERLINKV5_20151103070403","2013-11-29T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.10507,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8292,"POWERLINKV5_20151103070403","2013-11-29T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.10507,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8293,"POWERLINKV5_20151103070403","2013-11-30T05:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.772130000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8294,"POWERLINKV5_20151103070403","2013-11-30T05:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.772130000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8295,"POWERLINKV5_20151103070403","2013-11-30T05:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.32912,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8296,"POWERLINKV5_20151103070403","2013-11-30T05:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.32912,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8297,"POWERLINKV5_20151103070403","2013-11-30T05:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.02614,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8298,"POWERLINKV5_20151103070403","2013-11-30T05:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.02614,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8299,"POWERLINKV5_20151103070403","2013-11-30T05:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.764329999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8300,"POWERLINKV5_20151103070403","2013-11-30T05:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.764329999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8301,"POWERLINKV5_20151103070403","2013-11-30T05:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.411300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8302,"POWERLINKV5_20151103070403","2013-11-30T05:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.411300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8303,"POWERLINKV5_20151103070403","2013-11-30T05:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.39941,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8304,"POWERLINKV5_20151103070403","2013-11-30T05:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.39941,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8305,"POWERLINKV5_20151103070403","2013-11-30T05:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.37032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8306,"POWERLINKV5_20151103070403","2013-11-30T05:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.37032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8307,"POWERLINKV5_20151103070403","2013-11-30T05:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.265610000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8308,"POWERLINKV5_20151103070403","2013-11-30T05:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.265610000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8309,"POWERLINKV5_20151103070403","2013-11-30T06:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.67868,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8310,"POWERLINKV5_20151103070403","2013-11-30T06:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.67868,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8311,"POWERLINKV5_20151103070403","2013-11-30T06:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.12368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8312,"POWERLINKV5_20151103070403","2013-11-30T06:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.12368,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8313,"POWERLINKV5_20151103070403","2013-11-30T06:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.75028,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8314,"POWERLINKV5_20151103070403","2013-11-30T06:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.75028,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8315,"POWERLINKV5_20151103070403","2013-11-30T06:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.79297,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8316,"POWERLINKV5_20151103070403","2013-11-30T06:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.79297,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8317,"POWERLINKV5_20151103070403","2013-11-30T06:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.93638,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8318,"POWERLINKV5_20151103070403","2013-11-30T06:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.93638,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8319,"POWERLINKV5_20151103070403","2013-11-30T06:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.848949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8320,"POWERLINKV5_20151103070403","2013-11-30T06:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.848949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8321,"POWERLINKV5_20151103070403","2013-11-30T06:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.889669999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8322,"POWERLINKV5_20151103070403","2013-11-30T06:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.889669999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8323,"POWERLINKV5_20151103070403","2013-11-30T06:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.438759999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8324,"POWERLINKV5_20151103070403","2013-11-30T06:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.438759999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8325,"POWERLINKV5_20151103070403","2013-11-30T06:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.223700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8326,"POWERLINKV5_20151103070403","2013-11-30T06:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.223700000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8327,"POWERLINKV5_20151103070403","2013-11-30T07:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.674939999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8328,"POWERLINKV5_20151103070403","2013-11-30T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.674939999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8329,"POWERLINKV5_20151103070403","2013-11-30T07:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.91648,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8330,"POWERLINKV5_20151103070403","2013-11-30T07:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.91648,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8331,"POWERLINKV5_20151103070403","2013-11-30T07:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-20.647860000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8332,"POWERLINKV5_20151103070403","2013-11-30T07:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-20.647860000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8333,"POWERLINKV5_20151103070403","2013-11-30T07:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.838830000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8334,"POWERLINKV5_20151103070403","2013-11-30T07:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.838830000000002,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8335,"POWERLINKV5_20151103070403","2013-11-30T07:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-19.74457,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8336,"POWERLINKV5_20151103070403","2013-11-30T07:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-19.74457,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8337,"POWERLINKV5_20151103070403","2013-11-30T07:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-22.222020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8338,"POWERLINKV5_20151103070403","2013-11-30T07:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-22.222020000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8339,"POWERLINKV5_20151103070403","2013-11-30T07:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.11321,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8340,"POWERLINKV5_20151103070403","2013-11-30T07:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.11321,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8341,"POWERLINKV5_20151103070403","2013-11-30T07:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.055899999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8342,"POWERLINKV5_20151103070403","2013-11-30T07:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.055899999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8343,"POWERLINKV5_20151103070403","2013-11-30T07:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.514709999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8344,"POWERLINKV5_20151103070403","2013-11-30T07:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.514709999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8345,"POWERLINKV5_20151103070403","2013-11-30T07:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.45936,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8346,"POWERLINKV5_20151103070403","2013-11-30T07:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.45936,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8347,"POWERLINKV5_20151103070403","2013-11-30T07:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.46665,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8348,"POWERLINKV5_20151103070403","2013-11-30T07:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.46665,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8349,"POWERLINKV5_20151103070403","2013-11-30T08:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.04612,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8350,"POWERLINKV5_20151103070403","2013-11-30T08:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.04612,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8351,"POWERLINKV5_20151103070403","2013-11-30T08:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.533989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8352,"POWERLINKV5_20151103070403","2013-11-30T08:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.533989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8353,"POWERLINKV5_20151103070403","2013-11-30T08:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.196009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8354,"POWERLINKV5_20151103070403","2013-11-30T08:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.196009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8355,"POWERLINKV5_20151103070403","2013-11-30T08:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.22757,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8356,"POWERLINKV5_20151103070403","2013-11-30T08:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.22757,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8357,"POWERLINKV5_20151103070403","2013-11-30T09:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-25.58,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8358,"POWERLINKV5_20151103070403","2013-11-30T09:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-25.58,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8359,"POWERLINKV5_20151103070403","2013-12-01T07:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.06043,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8360,"POWERLINKV5_20151103070403","2013-12-01T07:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.06043,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8361,"POWERLINKV5_20151103070403","2013-12-01T11:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060420000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8362,"POWERLINKV5_20151103070403","2013-12-01T11:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060420000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8363,"POWERLINKV5_20151103070403","2013-12-01T11:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.674609999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8364,"POWERLINKV5_20151103070403","2013-12-01T11:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.674609999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8365,"POWERLINKV5_20151103070403","2013-12-01T11:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.08459,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8366,"POWERLINKV5_20151103070403","2013-12-01T11:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.08459,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8367,"POWERLINKV5_20151103070403","2013-12-01T11:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.119479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8368,"POWERLINKV5_20151103070403","2013-12-01T11:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.119479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8369,"POWERLINKV5_20151103070403","2013-12-01T11:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.489979999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8370,"POWERLINKV5_20151103070403","2013-12-01T11:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.489979999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8371,"POWERLINKV5_20151103070403","2013-12-01T11:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.486459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8372,"POWERLINKV5_20151103070403","2013-12-01T11:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.486459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8373,"POWERLINKV5_20151103070403","2013-12-01T11:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8374,"POWERLINKV5_20151103070403","2013-12-01T11:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8375,"POWERLINKV5_20151103070403","2013-12-01T11:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8376,"POWERLINKV5_20151103070403","2013-12-01T11:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8377,"POWERLINKV5_20151103070403","2013-12-01T11:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.12463,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8378,"POWERLINKV5_20151103070403","2013-12-01T11:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.12463,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8379,"POWERLINKV5_20151103070403","2013-12-01T11:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8380,"POWERLINKV5_20151103070403","2013-12-01T11:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060449999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8381,"POWERLINKV5_20151103070403","2013-12-01T12:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.96049,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8382,"POWERLINKV5_20151103070403","2013-12-01T12:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.96049,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8383,"POWERLINKV5_20151103070403","2013-12-01T12:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.06212,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8384,"POWERLINKV5_20151103070403","2013-12-01T12:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.06212,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8385,"POWERLINKV5_20151103070403","2013-12-01T12:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.050599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8386,"POWERLINKV5_20151103070403","2013-12-01T12:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.050599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8387,"POWERLINKV5_20151103070403","2013-12-01T12:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.78984,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8388,"POWERLINKV5_20151103070403","2013-12-01T12:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.78984,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8389,"POWERLINKV5_20151103070403","2013-12-01T12:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.429399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8390,"POWERLINKV5_20151103070403","2013-12-01T12:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.429399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8391,"POWERLINKV5_20151103070403","2013-12-01T12:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.819710000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8392,"POWERLINKV5_20151103070403","2013-12-01T12:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.819710000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8393,"POWERLINKV5_20151103070403","2013-12-01T12:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.434570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8394,"POWERLINKV5_20151103070403","2013-12-01T12:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.434570000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8395,"POWERLINKV5_20151103070403","2013-12-01T12:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.05045,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8396,"POWERLINKV5_20151103070403","2013-12-01T12:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.05045,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8397,"POWERLINKV5_20151103070403","2013-12-01T12:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.4472,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8398,"POWERLINKV5_20151103070403","2013-12-01T12:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.4472,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8399,"POWERLINKV5_20151103070403","2013-12-01T12:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.049810000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8400,"POWERLINKV5_20151103070403","2013-12-01T12:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.049810000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8401,"POWERLINKV5_20151103070403","2013-12-01T13:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.133520000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8402,"POWERLINKV5_20151103070403","2013-12-01T13:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.133520000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8403,"POWERLINKV5_20151103070403","2013-12-01T13:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.387510000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8404,"POWERLINKV5_20151103070403","2013-12-01T13:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.387510000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8405,"POWERLINKV5_20151103070403","2013-12-01T14:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.73352,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8406,"POWERLINKV5_20151103070403","2013-12-01T14:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.73352,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8407,"POWERLINKV5_20151103070403","2013-12-01T15:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.359970000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8408,"POWERLINKV5_20151103070403","2013-12-01T15:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.359970000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8409,"POWERLINKV5_20151103070403","2013-12-01T15:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.55193,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8410,"POWERLINKV5_20151103070403","2013-12-01T15:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.55193,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8411,"POWERLINKV5_20151103070403","2013-12-01T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.05015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8412,"POWERLINKV5_20151103070403","2013-12-01T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.05015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8413,"POWERLINKV5_20151103070403","2013-12-01T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.06015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8414,"POWERLINKV5_20151103070403","2013-12-01T15:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.06015,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8415,"POWERLINKV5_20151103070403","2013-12-01T16:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.142480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8416,"POWERLINKV5_20151103070403","2013-12-01T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.142480000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8417,"POWERLINKV5_20151103070403","2013-12-01T16:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.511699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8418,"POWERLINKV5_20151103070403","2013-12-01T16:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.511699999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8419,"POWERLINKV5_20151103070403","2013-12-01T16:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.534319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8420,"POWERLINKV5_20151103070403","2013-12-01T16:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.534319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8421,"POWERLINKV5_20151103070403","2013-12-01T17:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.65982,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8422,"POWERLINKV5_20151103070403","2013-12-01T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.65982,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8423,"POWERLINKV5_20151103070403","2013-12-01T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.34491,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8424,"POWERLINKV5_20151103070403","2013-12-01T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.34491,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8425,"POWERLINKV5_20151103070403","2013-12-01T17:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.322089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8426,"POWERLINKV5_20151103070403","2013-12-01T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.322089999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8427,"POWERLINKV5_20151103070403","2013-12-01T18:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.341329999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8428,"POWERLINKV5_20151103070403","2013-12-01T18:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.341329999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8429,"POWERLINKV5_20151103070403","2013-12-01T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.91977,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8430,"POWERLINKV5_20151103070403","2013-12-01T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.91977,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8431,"POWERLINKV5_20151103070403","2013-12-01T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.351459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8432,"POWERLINKV5_20151103070403","2013-12-01T18:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.351459999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8433,"POWERLINKV5_20151103070403","2013-12-01T19:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.842320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8434,"POWERLINKV5_20151103070403","2013-12-01T19:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.842320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8435,"POWERLINKV5_20151103070403","2013-12-01T19:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-16.749140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8436,"POWERLINKV5_20151103070403","2013-12-01T19:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-16.749140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8437,"POWERLINKV5_20151103070403","2013-12-01T19:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-15.40044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8438,"POWERLINKV5_20151103070403","2013-12-01T19:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-15.40044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8439,"POWERLINKV5_20151103070403","2013-12-01T19:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.15587,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8440,"POWERLINKV5_20151103070403","2013-12-01T19:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.15587,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8441,"POWERLINKV5_20151103070403","2013-12-01T20:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.536989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8442,"POWERLINKV5_20151103070403","2013-12-01T20:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.536989999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8443,"POWERLINKV5_20151103070403","2013-12-01T20:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.614750000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8444,"POWERLINKV5_20151103070403","2013-12-01T20:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.614750000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8445,"POWERLINKV5_20151103070403","2013-12-01T20:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.32971,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8446,"POWERLINKV5_20151103070403","2013-12-01T20:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.32971,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8447,"POWERLINKV5_20151103070403","2013-12-01T20:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.17404,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8448,"POWERLINKV5_20151103070403","2013-12-01T20:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.17404,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8449,"POWERLINKV5_20151103070403","2013-12-01T20:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.558120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8450,"POWERLINKV5_20151103070403","2013-12-01T20:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.558120000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8451,"POWERLINKV5_20151103070403","2013-12-01T20:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.522259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8452,"POWERLINKV5_20151103070403","2013-12-01T20:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.522259999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8453,"POWERLINKV5_20151103070403","2013-12-01T20:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.63325,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8454,"POWERLINKV5_20151103070403","2013-12-01T20:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.63325,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8455,"POWERLINKV5_20151103070403","2013-12-01T20:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.260630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8456,"POWERLINKV5_20151103070403","2013-12-01T20:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.260630000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8457,"POWERLINKV5_20151103070403","2013-12-01T21:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.269869999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8458,"POWERLINKV5_20151103070403","2013-12-01T21:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.269869999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8459,"POWERLINKV5_20151103070403","2013-12-01T21:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.198370000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8460,"POWERLINKV5_20151103070403","2013-12-01T21:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.198370000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8461,"POWERLINKV5_20151103070403","2013-12-01T21:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.38349,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8462,"POWERLINKV5_20151103070403","2013-12-01T21:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.38349,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8463,"POWERLINKV5_20151103070403","2013-12-01T21:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.39777,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8464,"POWERLINKV5_20151103070403","2013-12-01T21:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.39777,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8465,"POWERLINKV5_20151103070403","2013-12-01T21:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.06044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8466,"POWERLINKV5_20151103070403","2013-12-01T21:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.06044,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8467,"POWERLINKV5_20151103070403","2013-12-01T21:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.06048,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8468,"POWERLINKV5_20151103070403","2013-12-01T21:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.06048,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8469,"POWERLINKV5_20151103070403","2013-12-01T21:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.56681,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8470,"POWERLINKV5_20151103070403","2013-12-01T21:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.56681,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8471,"POWERLINKV5_20151103070403","2013-12-01T21:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.539300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8472,"POWERLINKV5_20151103070403","2013-12-01T21:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.539300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8473,"POWERLINKV5_20151103070403","2013-12-01T21:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.77854,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8474,"POWERLINKV5_20151103070403","2013-12-01T21:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.77854,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8475,"POWERLINKV5_20151103070403","2013-12-01T21:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.05048,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8476,"POWERLINKV5_20151103070403","2013-12-01T21:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.05048,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8477,"POWERLINKV5_20151103070403","2013-12-01T22:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.01497,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8478,"POWERLINKV5_20151103070403","2013-12-01T22:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.01497,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8479,"POWERLINKV5_20151103070403","2013-12-01T22:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.023949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8480,"POWERLINKV5_20151103070403","2013-12-01T22:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.023949999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8481,"POWERLINKV5_20151103070403","2013-12-01T22:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.244210000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8482,"POWERLINKV5_20151103070403","2013-12-01T22:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.244210000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8483,"POWERLINKV5_20151103070403","2013-12-01T22:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.06073,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8484,"POWERLINKV5_20151103070403","2013-12-01T22:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.06073,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8485,"POWERLINKV5_20151103070403","2013-12-01T22:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.38552,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8486,"POWERLINKV5_20151103070403","2013-12-01T22:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.38552,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8487,"POWERLINKV5_20151103070403","2013-12-01T22:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8488,"POWERLINKV5_20151103070403","2013-12-01T22:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8489,"POWERLINKV5_20151103070403","2013-12-01T22:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8490,"POWERLINKV5_20151103070403","2013-12-01T22:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8491,"POWERLINKV5_20151103070403","2013-12-01T22:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.01343,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8492,"POWERLINKV5_20151103070403","2013-12-01T22:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.01343,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8493,"POWERLINKV5_20151103070403","2013-12-01T22:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.83954,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8494,"POWERLINKV5_20151103070403","2013-12-01T22:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.83954,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8495,"POWERLINKV5_20151103070403","2013-12-01T22:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.611800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8496,"POWERLINKV5_20151103070403","2013-12-01T22:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.611800000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8497,"POWERLINKV5_20151103070403","2013-12-01T22:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.422140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8498,"POWERLINKV5_20151103070403","2013-12-01T22:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.422140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8499,"POWERLINKV5_20151103070403","2013-12-01T22:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.64939,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8500,"POWERLINKV5_20151103070403","2013-12-01T22:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.64939,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8501,"POWERLINKV5_20151103070403","2013-12-01T23:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.03032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8502,"POWERLINKV5_20151103070403","2013-12-01T23:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.03032,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8503,"POWERLINKV5_20151103070403","2013-12-01T23:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.229990000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8504,"POWERLINKV5_20151103070403","2013-12-01T23:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.229990000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8505,"POWERLINKV5_20151103070403","2013-12-01T23:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.880319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8506,"POWERLINKV5_20151103070403","2013-12-01T23:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.880319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8507,"POWERLINKV5_20151103070403","2013-12-01T23:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.633599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8508,"POWERLINKV5_20151103070403","2013-12-01T23:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.633599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8509,"POWERLINKV5_20151103070403","2013-12-01T23:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.22667,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8510,"POWERLINKV5_20151103070403","2013-12-01T23:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.22667,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8511,"POWERLINKV5_20151103070403","2013-12-01T23:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.796709999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8512,"POWERLINKV5_20151103070403","2013-12-01T23:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.796709999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8513,"POWERLINKV5_20151103070403","2013-12-01T23:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8514,"POWERLINKV5_20151103070403","2013-12-01T23:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8515,"POWERLINKV5_20151103070403","2013-12-01T23:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8516,"POWERLINKV5_20151103070403","2013-12-01T23:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8517,"POWERLINKV5_20151103070403","2013-12-01T23:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8518,"POWERLINKV5_20151103070403","2013-12-01T23:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8519,"POWERLINKV5_20151103070403","2013-12-01T23:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8520,"POWERLINKV5_20151103070403","2013-12-01T23:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.050319999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8521,"POWERLINKV5_20151103070403","2013-12-01T23:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8522,"POWERLINKV5_20151103070403","2013-12-01T23:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.060320000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8523,"POWERLINKV5_20151103070403","2013-12-02","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.76019,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8524,"POWERLINKV5_20151103070403","2013-12-02","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.76019,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8525,"POWERLINKV5_20151103070403","2013-12-02T00:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.093019999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8526,"POWERLINKV5_20151103070403","2013-12-02T00:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.093019999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8527,"POWERLINKV5_20151103070403","2013-12-02T15:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.75691,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8528,"POWERLINKV5_20151103070403","2013-12-02T15:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.75691,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8529,"POWERLINKV5_20151103070403","2013-12-02T15:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.75691,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8530,"POWERLINKV5_20151103070403","2013-12-02T15:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.75691,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8531,"POWERLINKV5_20151103070403","2013-12-02T15:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.370100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8532,"POWERLINKV5_20151103070403","2013-12-02T15:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.370100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8533,"POWERLINKV5_20151103070403","2013-12-02T15:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.420100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8534,"POWERLINKV5_20151103070403","2013-12-02T15:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.420100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8535,"POWERLINKV5_20151103070403","2013-12-02T15:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8536,"POWERLINKV5_20151103070403","2013-12-02T15:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.660139999999998,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8537,"POWERLINKV5_20151103070403","2013-12-02T15:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.88114,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8538,"POWERLINKV5_20151103070403","2013-12-02T15:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.88114,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8539,"POWERLINKV5_20151103070403","2013-12-02T16:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.88114,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8540,"POWERLINKV5_20151103070403","2013-12-02T16:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.88114,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8541,"POWERLINKV5_20151103070403","2013-12-02T16:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-18.170300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8542,"POWERLINKV5_20151103070403","2013-12-02T16:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-18.170300000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8543,"POWERLINKV5_20151103070403","2013-12-02T16:15:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8544,"POWERLINKV5_20151103070403","2013-12-02T16:15:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8545,"POWERLINKV5_20151103070403","2013-12-02T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-24.735230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8546,"POWERLINKV5_20151103070403","2013-12-02T16:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-24.735230000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8547,"POWERLINKV5_20151103070403","2013-12-02T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.80025,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8548,"POWERLINKV5_20151103070403","2013-12-02T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.80025,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8549,"POWERLINKV5_20151103070403","2013-12-02T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.56814,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8550,"POWERLINKV5_20151103070403","2013-12-02T16:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.56814,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8551,"POWERLINKV5_20151103070403","2013-12-02T16:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-14.77309,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8552,"POWERLINKV5_20151103070403","2013-12-02T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-14.77309,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8553,"POWERLINKV5_20151103070403","2013-12-02T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.897489999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8554,"POWERLINKV5_20151103070403","2013-12-02T16:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.897489999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8555,"POWERLINKV5_20151103070403","2013-12-02T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.54026,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8556,"POWERLINKV5_20151103070403","2013-12-02T17:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.54026,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8557,"POWERLINKV5_20151103070403","2013-12-02T17:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8558,"POWERLINKV5_20151103070403","2013-12-02T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8559,"POWERLINKV5_20151103070403","2013-12-02T17:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8560,"POWERLINKV5_20151103070403","2013-12-02T17:25:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8561,"POWERLINKV5_20151103070403","2013-12-02T17:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8562,"POWERLINKV5_20151103070403","2013-12-02T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8563,"POWERLINKV5_20151103070403","2013-12-02T17:35:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8564,"POWERLINKV5_20151103070403","2013-12-02T17:35:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8565,"POWERLINKV5_20151103070403","2013-12-02T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8566,"POWERLINKV5_20151103070403","2013-12-02T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-17.47024,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8567,"POWERLINKV5_20151103070403","2013-12-02T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-13.332599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8568,"POWERLINKV5_20151103070403","2013-12-02T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-13.332599999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8569,"POWERLINKV5_20151103070403","2013-12-02T17:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.01707,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8570,"POWERLINKV5_20151103070403","2013-12-02T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.01707,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8571,"POWERLINKV5_20151103070403","2013-12-02T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.45571,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8572,"POWERLINKV5_20151103070403","2013-12-02T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.45571,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8573,"POWERLINKV5_20151103070403","2013-12-02T18:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.388479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8574,"POWERLINKV5_20151103070403","2013-12-02T18:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.388479999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8575,"POWERLINKV5_20151103070403","2013-12-02T18:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.500719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8576,"POWERLINKV5_20151103070403","2013-12-02T18:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.500719999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8577,"POWERLINKV5_20151103070403","2013-12-02T18:10:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.817399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8578,"POWERLINKV5_20151103070403","2013-12-02T18:10:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.817399999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8579,"POWERLINKV5_20151103070403","2013-12-02T18:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.2682,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8580,"POWERLINKV5_20151103070403","2013-12-02T18:30:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.2682,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8581,"POWERLINKV5_20151103070403","2013-12-02T18:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.75231,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8582,"POWERLINKV5_20151103070403","2013-12-02T18:40:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.75231,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8583,"POWERLINKV5_20151103070403","2013-12-02T18:45:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-12.06537,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8584,"POWERLINKV5_20151103070403","2013-12-02T18:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-12.06537,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8585,"POWERLINKV5_20151103070403","2013-12-02T18:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.70983,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8586,"POWERLINKV5_20151103070403","2013-12-02T18:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.70983,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8587,"POWERLINKV5_20151103070403","2013-12-02T18:55:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.166650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8588,"POWERLINKV5_20151103070403","2013-12-02T18:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.166650000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8589,"POWERLINKV5_20151103070403","2013-12-02T19:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-11.7539,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8590,"POWERLINKV5_20151103070403","2013-12-02T19:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-11.7539,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8591,"POWERLINKV5_20151103070403","2013-12-02T19:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.489929999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8592,"POWERLINKV5_20151103070403","2013-12-02T19:50:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.489929999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8593,"POWERLINKV5_20151103070403","2013-12-02T20:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.15034,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8594,"POWERLINKV5_20151103070403","2013-12-02T20:00:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.15034,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8595,"POWERLINKV5_20151103070403","2013-12-02T20:05:00","Q>NIL_BI_FB","Q-NIL","2013-11-26",1,-10.136139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8596,"POWERLINKV5_20151103070403","2013-12-02T20:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-11-26",1,-10.136139999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8597,"POWERLINKV5_20151103070403","2013-12-05T16:25:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-14.77013,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8598,"POWERLINKV5_20151103070403","2013-12-05T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-14.77013,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8599,"POWERLINKV5_20151103070403","2013-12-05T16:30:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-30.950140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8600,"POWERLINKV5_20151103070403","2013-12-05T16:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-30.950140000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8601,"POWERLINKV5_20151103070403","2013-12-05T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-15.17005,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8602,"POWERLINKV5_20151103070403","2013-12-05T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-15.17005,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8603,"POWERLINKV5_20151103070403","2013-12-06T16:05:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.44645,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8604,"POWERLINKV5_20151103070403","2013-12-06T16:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.44645,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8605,"POWERLINKV5_20151103070403","2013-12-06T16:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.46007,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8606,"POWERLINKV5_20151103070403","2013-12-06T16:20:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.46007,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8607,"POWERLINKV5_20151103070403","2013-12-06T16:25:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.46007,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8608,"POWERLINKV5_20151103070403","2013-12-06T16:25:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.46007,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8609,"POWERLINKV5_20151103070403","2013-12-06T16:40:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.537100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8610,"POWERLINKV5_20151103070403","2013-12-06T16:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.537100000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8611,"POWERLINKV5_20151103070403","2013-12-06T16:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.975759999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8612,"POWERLINKV5_20151103070403","2013-12-06T16:45:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.975759999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8613,"POWERLINKV5_20151103070403","2013-12-06T16:50:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-11.48115,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8614,"POWERLINKV5_20151103070403","2013-12-06T16:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-11.48115,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8615,"POWERLINKV5_20151103070403","2013-12-06T16:55:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-11.496359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8616,"POWERLINKV5_20151103070403","2013-12-06T16:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-11.496359999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8617,"POWERLINKV5_20151103070403","2013-12-06T17:00:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-11.49924,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8618,"POWERLINKV5_20151103070403","2013-12-06T17:00:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-11.49924,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8619,"POWERLINKV5_20151103070403","2013-12-06T17:05:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.51224,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8620,"POWERLINKV5_20151103070403","2013-12-06T17:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.51224,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8621,"POWERLINKV5_20151103070403","2013-12-06T17:20:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-11.58592,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8622,"POWERLINKV5_20151103070403","2013-12-06T17:20:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-11.58592,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8623,"POWERLINKV5_20151103070403","2013-12-06T17:30:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-12.3323,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8624,"POWERLINKV5_20151103070403","2013-12-06T17:30:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-12.3323,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8625,"POWERLINKV5_20151103070403","2013-12-06T17:40:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-12.21949,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8626,"POWERLINKV5_20151103070403","2013-12-06T17:40:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-12.21949,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8627,"POWERLINKV5_20151103070403","2013-12-06T17:45:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-12.971170000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8628,"POWERLINKV5_20151103070403","2013-12-06T17:45:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-12.971170000000001,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8629,"POWERLINKV5_20151103070403","2013-12-06T17:50:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-12.949009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8630,"POWERLINKV5_20151103070403","2013-12-06T17:50:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-12.949009999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8631,"POWERLINKV5_20151103070403","2013-12-06T17:55:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-12.693339999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8632,"POWERLINKV5_20151103070403","2013-12-06T17:55:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-12.693339999999999,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8633,"POWERLINKV5_20151103070403","2013-12-06T19:05:00","Q>NIL_BI_FB","Q-NIL","2013-12-03",1,-10.00642,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8634,"POWERLINKV5_20151103070403","2013-12-06T19:05:00","Q>NIL_BI_FB","Q-NIL_BI_INTACT","2013-12-03",1,-10.00642,"Out= Nil, H8 Boyne Island feeder bushing (FB) limit on Calliope River to Boyne Island 132kV lines, for the contingent loss of a single Calliope River to Boyne Island 132kV line, Feedback","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8635,"POWERLINKV5_20151103070403","2013-12-20T11:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-66.039370000000005,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8636,"POWERLINKV5_20151103070403","2013-12-20T12:00:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-80.658789999999996,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8637,"POWERLINKV5_20151103070403","2013-12-20T12:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-261.05993999999998,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8638,"POWERLINKV5_20151103070403","2013-12-20T12:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.40057000000002,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8639,"POWERLINKV5_20151103070403","2013-12-20T12:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-73.244230000000002,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8640,"POWERLINKV5_20151103070403","2013-12-20T12:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.44752999999997,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8641,"POWERLINKV5_20151103070403","2013-12-20T12:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.45015000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8642,"POWERLINKV5_20151103070403","2013-12-20T12:30:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.41696000000002,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8643,"POWERLINKV5_20151103070403","2013-12-20T12:35:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-185.29147,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8644,"POWERLINKV5_20151103070403","2013-12-20T12:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.2636,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8645,"POWERLINKV5_20151103070403","2013-12-20T12:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.34546,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8646,"POWERLINKV5_20151103070403","2013-12-20T12:50:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-260.37768,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8647,"POWERLINKV5_20151103070403","2013-12-20T12:55:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-225.18213,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8648,"POWERLINKV5_20151103070403","2013-12-20T13:05:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-215.56544,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8649,"POWERLINKV5_20151103070403","2013-12-20T13:10:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-11177.540150000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8650,"POWERLINKV5_20151103070403","2013-12-20T13:15:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-11177.079659999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8651,"POWERLINKV5_20151103070403","2013-12-20T13:20:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-157.50529,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8652,"POWERLINKV5_20151103070403","2013-12-20T13:40:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-212.63668999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8653,"POWERLINKV5_20151103070403","2013-12-20T13:45:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-177.56121999999999,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]
[8654,"POWERLINKV5_20151103070403","2013-12-20T14:25:00","Q:N_NIL_BCK2L-G","Q-NIL","2013-04-02",1,-308.99072000000001,"Outage=Nil, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault between Armidale and Bulli Creek","SYSTEM NORMAL","OTHER","NIL","REGULATED","","System Normal Constraint","PLANNED",0]