{"text_format":"1","workbook":"xlsx","n_sheets":39,"sheets":["CF","AER only","Contents","Instructions","Business & other details","CPI series","2.1 Expenditure summary","2.2 Repex","2.3 Augex (a)","2.3 Augex (b)","2.4 Augex model","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.4 MD & utilisation-Spatial","6.1 Telephone answering","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.4 Shared Assets","7.3 Obligations","7.7 TSS-LRMC","7.8 WACC Inputs","Amendments"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":2,"defined_names":1113,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CF","index":0,"n_rows":125,"n_cols":21,"rows_kept":125,"cut":false,"hidden":true,"merged":[[1,1,1,20]]}
[]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,{"$f":"INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":false},"=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"",{"$f":"INDEX(dms_CF_3.6.6, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","v":false},"=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_4.1","dms_CF_6.6.1","dms_CF_6.8","dms_CF_7.12","dms_CF_8.1_A","dms_CF_8.1_B","dms_CF_8.1_Neg","dms_CF_4.4.1","Spare2"]
[null,"ActewAGL Distribution","ACT","Electricity","Distribution",null,"Y",null,"Y","Y","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Energex","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","Y","N"]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","Y","N"]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"Power and Water","NT","Electricity","Distribution",null,"N",null,"N","Y","N","N","Y","Y","Y","Y","N","Y","Y","N","N"]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","Y","Y","N","N","N"]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y",null,"N","N","N","N","Y","N","Y","Y","N","Y","Y","N","N"]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,"N","N","N","N","Y","N","Y","N","N","Y","Y","N","N"]
[null,"United Energy","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","Y","N","Y","N","N","N","Y","N","N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"0"]
[null,null,{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"}]

{"sheet":"AER only","index":1,"n_rows":223,"n_cols":40,"rows_kept":223,"cut":false,"hidden":true,"merged":[[93,1,95,1],[96,1,100,1],[104,1,105,1],[131,11,131,12],[148,1,148,8],[54,1,54,5],[54,14,54,21],[54,25,54,29],[54,30,54,33],[72,14,72,15],[72,25,72,28],[0,1,0,11],[4,27,4,38],[6,27,6,30],[6,33,6,37],[53,25,53,29],[53,30,53,33]]}
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,"2018-03-28","major changes to accommodate STPIS"]
[null,null,"Template Version",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_ContactName1_List","dms_ContactPh1_List","dms_ContactEmail_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_Public_Lighting_List","Column1"]
[null,"ActewAGL Distribution","ActewAGL Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution"]
[null,"ActewAGL Distribution (Tx Assets)","ActewAGL Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution (Tx Assets)"]
[null,"ActewAGL Gas","ActewAGL Gas",76670568688,"ACT","Gas","Distribution","Weighted average price cap","Financial","June",5,5,"x",null,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,"Philip Deamer","02 6248 3438","GasAAReview@actewagl.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Gas"]
[null,"AEMO","Australian Energy Market Operator Ltd",94072010327,"Vic","Electricity","Transmission","-","Financial","March",5,5,"x","-","Level 22","530 Collins Street","MELBOURNE","VIC",3000,"GPO Box 2008",null,"MELBOURNE","VIC",3001,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AEMO"]
[null,"AGN (Albury and Victoria)","Australian Gas Networks Limited (reporting data for Albury and Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Albury)"]
[null,"AGN (Albury)","Australian Gas Networks Limited (reporting data for Albury)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"AGN (SA)","Australian Gas Networks Limited (reporting data for SA)",19078551685,"SA","Gas","Distribution","Weighted average price cap","Financial","June",5,5,5,"distribution determination","Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (SA)"]
[null,"AGN (Victoria)","Australian Gas Networks Limited (reporting data for Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,"Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Victoria)"]
[null,"Amadeus","APT Pipelines (NT) Pty Ltd",39009737393,"NT","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Amadeus"]
[null,"APA GasNet","APA GasNet Australia (Operations) Pty Ltd","065083009","Vic","Gas","Transmission","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","APA GasNet"]
[null,"Ausgrid","Ausgrid",78508211731,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"John Thomson","02 9269 2312","john.thomson@ausgrid.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ausgrid"]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,"John Thomson","02 9269 2312","john.thomson@ausgrid.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Ausgrid (Tx Assets)"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","VIC",8001,"please provide contact details",null,null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","AusNet (D)"]
[null,"AusNet (Gas)","AusNet Gas Services","086015036","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"X",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (Gas)"]
[null,"AusNet (T)","Ausnet Services (Transmission) Ltd",48116124362,"Vic","Electricity","Transmission","Revenue cap","Financial","March",5,5,2,"transmission determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,"Clare Thompson","03 9695 6670","clare.e.thompson@ausnetservices.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (T)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"-","Electricity","Distribution","Revenue cap","Financial","June",5,5,2,"distribution determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co."]
[null,"Australian Distribution Co. (Gas)","Australian Gas Distribution Co. ",11222333444,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,"123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Australian Distribution Co. (Vic)"]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","VIC",3000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co. (Vic)"]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"-","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Australian Transmission Co."]
[null,"Central Ranges Pipeline (D)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",15,5,5,"distribution determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"Central Ranges Pipeline (T)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",14,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au","YES","YES","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","CitiPower"]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",9,5,5,"transmission determination","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Directlink"]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","52-55 East Terrace","Rymill Park","ADELAIDE","SA",5000,"PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,"Bill Jackson","08 8404 7969","jackson.bill@electranet.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ElectraNet"]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","51 Huntingwood Drive",null,"HUNTINGWOOD","NSW",2148,"PO Box 811",null,"SEVEN HILLS","NSW",1730,"Jon Hocking","02 9853 4386 / 0407 348 156","Jon.Hocking@Endeavourenergy.com.au","NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Endeavour Energy"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","26 Reddacliff Street",null,"NEWSTEAD","Qld",4006,"26 Reddacliff Street",null,"NEWSTEAD","QLD",4006,"Jenny Doyle, General Manager Regulation and Pricing","(07) 3851 6416","jenny.doyle@energyq.com.au","YES","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","22 Walker Street",null,"TOWNSVILLE","Qld",4810,"Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,"Jenny Doyle, General Manager Regulation and Pricing","(07) 3851 6416","jenny.doyle@energyq.com.au","NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ergon Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","8 Buller Street",null,"PORT MACQUARIE","NSW",2444,"PO Box 5730",null,"PORT MACQUARIE","NSW",2444,"Catherine Waddell","02 6338 3553","catherine.waddell@essentialenergy.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Essential Energy"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","VIC",3000,"PO Box 16182",null,"MELBOURNE","VIC",8001,"Matthew Serpell","03 9173 8231","matthew.serpell@jemena.com.au","NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Jemena Electricity"]
[null,"JGN","Jemena Gas Networks (NSW) Ltd","003 004 322","NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,null,null,null,null,null,null,null,null,null,null,"please provide contact details",null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","JGN"]
[null,"Multinet Gas","Multinet Gas (DB No.1) Pty Ltd (ACN 086 026 986), Multinet Gas (DB No.2) Pty Ltd (ACN 086 230 122)","086026986","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"43-45 Centreway",null,"MT WAVERLEY","Vic",3149,null,null,null,null,null,"Andrew Schille","03 8846 9860","andrew.schille@ue.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Multinet Gas"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Scott Young","02 9275 0031","scott.young@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Murraylink"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,"x","distribution determination","GPO Box 1921",null,"DARWIN","NT",801,"GPO Box 1921",null,"DARWIN","NT",801,"Lucy Moon","08 8924 5822","Lucy.Moon@powerwater.com.au","YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Power and Water"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Powercor Australia"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","33 Harold St",null,"VIRGINIA","Qld",4014,"PO Box 1193",null,"VIRGINIA","QLD",4014,"Jennifer Harris","07 3860 2667","jharris@powerlink.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Powerlink"]
[null,"Roma to Brisbane Pipeline","APT Petroleum Pipelines Limited t/a Roma to Brisbane Pipeline","009 737 393","Qld","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","580 George Street",null,"SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,"Mark Allen","02 9275 0010","mark.allen@apa.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Roma to Brisbane Pipeline"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","1 Anzac Highway",null,"KESWICK","SA",5035,"GPO Box 77",null,"ADELAIDE","SA",5000,"Richard Sibly","08 8404 5613","richard.sibly@sapowernetworks.com.au","NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","SA Power Networks"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au","YES","YES","YES","YES","YES",null,"Critical Infrastructure","High density commercial","Urban","High density rural","Low density rural","YES","TasNetworks (D)"]
[null,"TasNetworks (T)","TasNetworks (T)",24167357299,"Tas","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,"John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TasNetworks (T)"]
[null,"TransGrid","NSW Electricity Networks Operations Pty Ltd trading as TransGrid","70 250 995 390","NSW","Electricity","Transmission","Revenue cap","Financial","June",4,5,5,"transmission determination","180 Thomas Street",null,"SYDNEY","NSW",2000,"PO Box A1000",null,"SYDNEY SOUTH","NSW",1235,"Garrie Chubb","0408 210 221","garrie.chubb@transgrid.com.au","NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TransGrid"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 3","6 Nexus Court","MULGRAVE","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","VIC",3170,"Mathew Abraham","03 8846 9758","mathew.abraham@ue.com.au","NO","NO","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","United Energy"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For EB & Reset RINs only",null,null,null,null,"For AARs only"]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68",null,null,null,null,null,null,null,null,null,null,null,"Drop down selector box for CA & Reset RINs.","For CA & Reset RINs only",null,null,null,null,null,null,null,null,null,null,"for DNSP only",null,null,null,null,"For DNSPs only"]
[null,"dms_Model_List ","dms_Worksheet_List",null,"dms_RYE_Formula_Result",null,null,null,null,null,null,null,null,"dms_0203_ProjectType","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020603_01_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM","dms_030605_UOM","dms_03060703_UOM"]
[null,"ARR","ANNUAL REPORTING STATEMENT",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","minutes/customer","minutes/customer","Customer / km","%","km","number","number"]
[null,"CA","CATEGORY ANALYSIS",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - dual circuit","Circuit line length in km","0's","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","minutes/customer","minutes/customer","MWh/customer","Number of spans",null,"number","number"]
[null,"CPI","CPI",null,null,null,null,null,null,null,null,null,null,"New line on new route - other","Circuit line length in km","MVA added","MVA added","MVA added","MVA added","0's","km","km","Total length of maintenance spans","0's","$0s","interruptions/customer","interruptions/customer","kVA / customer","Number of spans",null,"number","number"]
[null,"EB","ECONOMIC BENCHMARKING",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"noIN"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Line rebuild over existing route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","interruptions/customer","interruptions/customer",null,"Number of spans",null,"number","number"]
[null,"PTRM","POST TAX REVENUE MODEL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Line rebuild over existing route - dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","(per cent)","0's","0's","Average number of trees per maintenance span",null,null,null,null,null,"Number of spans",null,"number","(per cent)"]
[null,"Reset","REGULATORY REPORTING STATEMENT",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Reconductor - Single circuit","Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,"years","years","Average frequency of cutting cycle",null,null,null,null,null,"Years",null,"number"]
[null,"RFM","ROLL FORWARD MODEL",null,{"$f":"LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)","v":"2020"},"=LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)",null,null,null,null,null,null,null,"Reconductor - Dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,null,"Years",null,"number"]
[null,"WACC","WEIGHTED AVERAGE COST OF CAPITAL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Other",null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,null,null,null,null,null,null,null,null,"Trees",null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,null,"Trees",null,"number"]
[null,"dms_DataQuality_List",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,"$0s",null,null,null,null,null,null,null,null,null,null,"Defects",null,"number"]
[null,"Actual",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,null,"Defects",null,"number"]
[null,"Estimate",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"number"]
[null,"Consolidated",null,null,null,null,null,null,null,null,null,null,null,null,null,"$0s",null,null,null,null,null,null,null,null,null,null,null,null,"km",null,"(per cent)"]
[null,"Recast",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"(per cent)",""]
[null,"Public"]
[]
[null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above.",null,null,null,null,null,null,null,null,null,null,null,"For PTRM files - this field set the text for the named range \"DMS_Xfactor\" which in all cases is simply the text \"x factors\" - this saves putting in each old gas PTRM file ",null,null,null,null,null,null,null,null,null,null,"for TNSP only"]
[null,"dms_SourceList","dms_FormControl_Choices",null,null,null,null,null,null,null,null,null,null,null,"DMS_Xfactor",null,null,null,null,null,null,null,null,null,null,"dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,"After appeal","Revenue cap",null,null,null,null,null,null,null,null,null,null,null,"x factors",null,null,null,null,null,null,null,null,null,null,"%",null,"Number of spans","km"]
[null,"Draft decision","Revenue yield",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Years","%"]
[null,"Final decision","Weighted average price cap",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Trees","km"]
[null,"PTRM update 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"Defects","number"]
[null,"PTRM update 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans"]
[null,"PTRM update 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"km"]
[null,"PTRM update 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"km"]
[null,"PTRM update 5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans"]
[null,"PTRM update 6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,"PTRM update 7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,"Reporting",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Revised regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[]
[]
[]
[null,"Reason for interruption","dms_Reason_Interruption_Detailed","dms_Reason_Interruption","dms_STPIS_Exclusion_List","dms_020301_ProjectType_List","dms_020302_ProjectType_List"]
[null,"Animal","Animal impact","Animal","Weather","New substation establishment","New line on new route - single circuit"]
[null,null,"Animal nesting/burrowing, etc and other","Asset failure","Equipment failure","Capacity upgrade","New line on new route - dual circuit"]
[null,null,"Other","Other","Operational error","Voltage upgrade","New line on new route - other"]
[null,"Asset failure","LV","Overloads","Vegetation","Other","Line rebuild over existing route - single circuit"]
[null,null,"Distribution substation","Planned","Animals",null,"Line rebuild over existing route - dual circuit"]
[null,null,"HV","Network business","Third party impacts",null,"Reconductor - Single circuit"]
[null,null,"Zone substation","Third party","Transmission failure",null,"Reconductor - Dual circuit"]
[null,null,"Subtransmission","Unknown","Load shedding",null,"Reconductor - Other"]
[null,"Other","insert description of 'other'","Vegetation","Inter-distributor connection failure",null,"Line upgrade - raising/retensoring"]
[null,"Overloads","-","Weather","Other",null,"Line upgrade - voltage upgrade"]
[null,"Planned","-","2 - STPIS Exclusion (3.3)(a)",null,null,"Line upgrade - capacity"]
[null,"Network business","Network error","3 - STPIS Exclusion (3.3)(a)",null,null,"String spare circuit"]
[null,null,"Switching and protection error","4 - STPIS Exclusion (3.3)(a)",null,null,"Other"]
[null,"Third party","Fire","5 - STPIS Exclusion (3.3)(a)"]
[null,null,"Other","6 - STPIS Exclusion (3.3)(a)"]
[null,null,"Dig-in","7 - STPIS Exclusion (3.3)(a)"]
[null,null,"Unauthorised access"]
[null,null,"Vehicle impact"]
[null,"Unknown","Unknown"]
[null,"Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,"Grow-in - NSP responsibility"]
[null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,"Grow-in - Other responsible party"]
[null,"Weather"]
[null,"2 - STPIS Exclusion (3.3)(a)"]
[null,"3 - STPIS Exclusion (3.3)(a)"]
[null,"4 - STPIS Exclusion (3.3)(a)"]
[null,"5 - STPIS Exclusion (3.3)(a)"]
[null,"6 - STPIS Exclusion (3.3)(a)"]
[null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[]
[]
[]
[]
[]
[null,"These are indeces and lookup values for various dates. All step from the value placed in FRCP_y1 on the business and other details worksheet",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"},null,null,null,null,null,null,null,null,null,null,null,"These date tables are currently used in the Recast templates to provide column headings and conditional formatting"]
[null,"dms_FRCPlength_Num_List","dms_FinalYear_List","dms_CRCPlength_Num_List","dms_CFinalYear_List","dms_FRCP_years",null,"dms_CRCP_years",null,"dms_CRCP_index",null,"These are static values for cut / paste purposes only",null,null,"CRY from input cell on business sheet","CRY - financial","dms_FinYears","CRY calendar","dms_CalYears"]
[null,1,"dms_FRCP_y1",1,"CRCP_y1",{"$f":"FRCP_y1","v":"2020-21"},"dms_FRCP_y1",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)-1)&\"-\"&TEXT(VALUE(MID(dms_FRCP_y1,3,2)),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)-1))","v":"2019-20"},"dms_CRCP_yZ",1,null,"2005-06","2006",null,{"$f":"'Business & other details'!C48","v":"2018-19"},{"$f":"VALUE(LEFT(CRY,4))&\"-\"&TEXT(MID(CRY,3,2)+1,\"00\")","v":"2018-19"},"dms_CRYf_y1",{"$f":"VALUE(LEFT(CRY,4)+1)","v":2019},"dms_CRYc_y1"]
[null,2,"dms_FRCP_y2",2,"CRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y1,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)+1))","v":"2021-22"},"dms_FRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yZ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yZ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yZ,4)-1))","v":"2018-19"},"dms_CRCP_yY",2,null,"2006-07","2007",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y1,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y1,3,2)+2,\"00\")","v":"2019-20"},"dms_CRYf_y2",{"$f":"VALUE(LEFT(dms_CRYc_y1,4)+1)","v":2020},"dms_CRYc_y2"]
[null,3,"dms_FRCP_y3",3,"CRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y2,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y2,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y2,4)+1))","v":"2022-23"},"dms_FRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yY,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yY,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yY,4)-1))","v":"2017-18"},"dms_CRCP_yX",3,null,"2007-08","2008",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y2,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y2,3,2)+2,\"00\")","v":"2020-21"},"dms_CRYf_y3",{"$f":"VALUE(LEFT(dms_CRYc_y2,4)+1)","v":2021},"dms_CRYc_y3"]
[null,4,"dms_FRCP_y4",4,"CRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y3,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y3,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y3,4)+1))","v":"2023-24"},"dms_FRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yX,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yX,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yX,4)-1))","v":"2016-17"},"dms_CRCP_yW",4,null,"2008-09","2009",null,null,{"$f":"VALUE(LEFT(dms_CRYf_y3,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y3,3,2)+2,\"00\")","v":"2021-22"},"dms_CRYf_y4",{"$f":"VALUE(LEFT(dms_CRYc_y3,4)+1)","v":2022},"dms_CRYc_y4"]
[null,5,"dms_FRCP_y5",5,"CRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y4,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y4,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y4,4)+1))","v":"2024-25"},"dms_FRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yW,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yW,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yW,4)-1))","v":"2015-16"},"dms_CRCP_yV",5,null,"2009-10",2010,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y4,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y4,3,2)+2,\"00\")","v":"2022-23"},"dms_CRYf_y5",{"$f":"VALUE(LEFT(dms_CRYc_y4,4)+1)","v":2023},"dms_CRYc_y5"]
[null,6,"dms_FRCP_y6",6,"CRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y5,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y5,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y5,4)+1))","v":"2025-26"},"dms_FRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yV,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yV,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yV,4)-1))","v":"2014-15"},"dms_CRCP_yU",6,null,"2010-11",2011,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y5,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y5,3,2)+2,\"00\")","v":"2023-24"},"dms_CRYf_y6",{"$f":"VALUE(LEFT(dms_CRYc_y5,4)+1)","v":2024},"dms_CRYc_y6"]
[null,7,"dms_FRCP_y7",7,"CRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y6,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y6,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y6,4)+1))","v":"2026-27"},"dms_FRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yU,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yU,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yU,4)-1))","v":"2013-14"},"dms_CRCP_yT",7,null,"2011-12",2012,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y6,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y6,3,2)+2,\"00\")","v":"2024-25"},"dms_CRYf_y7",{"$f":"VALUE(LEFT(dms_CRYc_y6,4)+1)","v":2025},"dms_CRYc_y7"]
[null,8,"dms_FRCP_y8",8,"CRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y7,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y7,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y7,4)+1))","v":"2027-28"},"dms_FRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yT,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yT,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yT,4)-1))","v":"2012-13"},"dms_CRCP_yS",8,null,"2012-13",2013,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y7,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y7,3,2)+2,\"00\")","v":"2025-26"},"dms_CRYf_y8",{"$f":"VALUE(LEFT(dms_CRYc_y7,4)+1)","v":2026},"dms_CRYc_y8"]
[null,9,"dms_FRCP_y9",9,"CRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y8,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y8,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y8,4)+1))","v":"2028-29"},"dms_FRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yS,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yS,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yS,4)-1))","v":"2011-12"},"dms_CRCP_yR",9,null,"2013-14",2014,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y8,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y8,3,2)+2,\"00\")","v":"2026-27"},"dms_CRYf_y9",{"$f":"VALUE(LEFT(dms_CRYc_y8,4)+1)","v":2027},"dms_CRYc_y9"]
[null,10,"dms_FRCP_y10",10,"CRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y9,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y9,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y9,4)+1))","v":"2029-30"},"dms_FRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yR,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yR,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yR,4)-1))","v":"2010-11"},"dms_CRCP_yQ",10,null,"2014-15",2015,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y9,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y9,3,2)+2,\"00\")","v":"2027-28"},"dms_CRYf_y10",{"$f":"VALUE(LEFT(dms_CRYc_y9,4)+1)","v":2028},"dms_CRYc_y10"]
[null,11,"dms_FRCP_y11",11,"CRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y10,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y10,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y10,4)+1))","v":"2030-31"},"dms_FRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yQ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yQ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yQ,4)-1))","v":"2009-10"},"dms_CRCP_yP",11,null,"2015-16",2016,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y10,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y10,3,2)+2,\"00\")","v":"2028-29"},"dms_CRYf_y11",{"$f":"VALUE(LEFT(dms_CRYc_y10,4)+1)","v":2029},"dms_CRYc_y11"]
[null,12,"dms_FRCP_y12",12,"CRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y11,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y11,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y11,4)+1))","v":"2031-32"},"dms_FRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yP,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yP,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yP,4)-1))","v":"2008-09"},"dms_CRCP_yO",12,null,"2016-17",2017,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y11,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y11,3,2)+2,\"00\")","v":"2029-30"},"dms_CRYf_y12",{"$f":"VALUE(LEFT(dms_CRYc_y11,4)+1)","v":2030},"dms_CRYc_y12"]
[null,13,"dms_FRCP_y13",13,"CRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y12,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y12,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y12,4)+1))","v":"2032-33"},"dms_FRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yO,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yO,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yO,4)-1))","v":"2007-08"},"dms_CRCP_yN",13,null,"2017-18",2018,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y12,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y12,3,2)+2,\"00\")","v":"2030-31"},"dms_CRYf_y13",{"$f":"VALUE(LEFT(dms_CRYc_y12,4)+1)","v":2031},"dms_CRYc_y13"]
[null,14,"dms_FRCP_y14",14,"CRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y13,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y13,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y13,4)+1))","v":"2033-34"},"dms_FRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yN,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yN,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yN,4)-1))","v":"2006-07"},"dms_CRCP_yM",14,null,"2018-19",2019,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y13,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y13,3,2)+2,\"00\")","v":"2031-32"},"dms_CRYf_y14",{"$f":"VALUE(LEFT(dms_CRYc_y13,4)+1)","v":2032},"dms_CRYc_y14"]
[null,15,"dms_FRCP_y15",15,"CRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y14,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y14,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y14,4)+1))","v":"2034-35"},"dms_FRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yM,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yM,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yM,4)-1))","v":"2005-06"},"dms_CRCP_yL",15,null,"2019-20",2020,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y14,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y14,3,2)+2,\"00\")","v":"2032-33"},"dms_CRYf_y15",{"$f":"VALUE(LEFT(dms_CRYc_y14,4)+1)","v":2033},"dms_CRYc_y15"]
[null,null,null,null,null,null,null,null,null,null,null,"2020-21",2021,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y15,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y15,3,2)+2,\"00\")","v":"2033-34"},"dms_CRYf_y16",{"$f":"VALUE(LEFT(dms_CRYc_y15,4)+1)","v":2034},"dms_CRYc_y16"]
[null,"These are drop down lists for businesses to select the correct FRCP_y1 on the business and other details worksheet.\nThis also populates the column headings in the worksheets",null,null,null,null,null,null,null,null,null,"2021-22",2022,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y16,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y16,3,2)+2,\"00\")","v":"2034-35"},"dms_CRYf_y17",{"$f":"VALUE(LEFT(dms_CRYc_y16,4)+1)","v":2035},"dms_CRYc_y17"]
[null,"dms_RCP_fyear_list","dms_CRY_ListF","dms_CRY_ListC","dms_RCP_cyear_list","dms_FRCP_fyear_list","dms_FRCP_ListF","dms_FRCP_ListC","dms_FRCP_cyear_list",null,null,"2022-23",2023,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y17,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y17,3,2)+2,\"00\")","v":"2035-36"},"dms_CRYf_y18",{"$f":"VALUE(LEFT(dms_CRYc_y17,4)+1)","v":2036},"dms_CRYc_y18"]
[null,"dms_fy1","2005-06","2006","dms_cy1","dms_frcp_fy1","2010-11",2011,"dms_crcp_cy1",null,null,"2023-24",2024,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y18,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y18,3,2)+2,\"00\")","v":"2036-37"},"dms_CRYf_y19",{"$f":"VALUE(LEFT(dms_CRYc_y18,4)+1)","v":2037},"dms_CRYc_y19"]
[null,"dms_fy2","2006-07","2007","dms_cy2","dms_frcp_fy2","2011-12",2012,"dms_crcp_cy2",null,null,"2024-25",2025,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y19,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y19,3,2)+2,\"00\")","v":"2037-38"},"dms_CRYf_y20",{"$f":"VALUE(LEFT(dms_CRYc_y19,4)+1)","v":2038},"dms_CRYc_y20"]
[null,"dms_fy3","2007-08","2008","dms_cy3","dms_frcp_fy3","2012-13",2013,"dms_crcp_cy3",null,null,"2025-26",2026]
[null,"dms_fy4","2008-09","2009","dms_cy4","dms_frcp_fy4","2013-14",2014,"dms_crcp_cy4",null,null,"2026-27",2027]
[null,"dms_fy5","2009-10",2010,"dms_cy5","dms_frcp_fy5","2014-15",2015,"dms_crcp_cy5",null,null,"2027-28",2028]
[null,"dms_fy6","2010-11",2011,"dms_cy6","dms_frcp_fy6","2015-16",2016,"dms_crcp_cy6",null,null,"2028-29",2029]
[null,"dms_fy7","2011-12",2012,"dms_cy7","dms_frcp_fy7","2016-17",2017,"dms_crcp_cy7",null,null,"2029-30",2030]
[null,"dms_fy8","2012-13",2013,"dms_cy8","dms_frcp_fy8","2017-18",2018,"dms_crcp_cy8",null,null,"2030-31",2031]
[null,"dms_fy9","2013-14",2014,"dms_cy9","dms_frcp_fy9","2018-19",2019,"dms_crcp_cy9",null,null,"2031-32",2032]
[null,"dms_fy10","2014-15",2015,"dms_cy10","dms_frcp_fy10","2019-20",2020,"dms_crcp_cy10",null,null,"2032-33",2033]
[null,"dms_fy11","2015-16",2016,"dms_cy11","dms_frcp_fy11","2020-21",2021,"dms_crcp_cy11",null,null,"2033-34",2034]
[null,"dms_fy12","2016-17",2017,"dms_cy12","dms_frcp_fy12","2021-22",2022,"dms_crcp_cy12",null,null,"2034-35",2035]
[null,"dms_fy13","2017-18",2018,"dms_cy13","dms_frcp_fy13","2022-23",2023,"dms_crcp_cy13",null,null,"2035-36",2036]
[null,"dms_fy14","2018-19",2019,"dms_cy14","dms_frcp_fy14","2023-24",2024,"dms_crcp_cy14"]
[null,"dms_fy15","2019-20",2020,"dms_cy15","dms_frcp_fy15","2024-25",2025,"dms_crcp_cy15"]
[null,"dms_fy16","2020-21",2021,"dms_cy16"]
[null,"dms_fy17","2021-22",2022,"dms_cy17"]
[null,"dms_fy18","2022-23",2023,"dms_cy18"]
[null,"dms_fy19","2023-24",2024,"dms_cy19"]
[null,"dms_fy20","2024-25",2025,"dms_cy20"]
[]
[]
[]
[]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[null,null,"Table 6.3 sustained interruptions - row descriptions"]
[null,null,"dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[]
[null,null,"Table 6.1 telephone answering - row descriptions and start date"]
[null,null,"dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":"1-Jul-2018"}]
[]
[]
[]
[null,null,null,null,null,null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values"]
[null,null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[null,"dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[]
[]
[]
[null,null,"Table 6.8.1 - row descriptions"]
[null,null,"dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[]
[]
[null,null,"Table 7.9.4 - market impact component - row descriptions"]
[null,"dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[]
[]
[]
[null,null,"Use this to add to existing files"]
[null,null,"ARRs 6.7 STPIS daily performance"]
[null,null,"dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[]
[null,null,"ARR's  6.8 STPIS exclusions"]
[null,null,"dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[null,null,"CA 6.3 sustained interruptions"]
[null,null,"dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]

{"sheet":"Contents","index":2,"n_rows":34,"n_cols":19,"rows_kept":34,"cut":false,"hidden":false,"merged":[[29,18,29,23]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"CONCATENATE(FRCP_y1,\" to \",FRCP_y5)","v":"2020-21 to 2024-25"}]
[null,"CONTENTS"]
[]
[]
[null,null,null,null,"1. Business and other details",null,null,null,null,null,null,"2. Expenditure",null,null,null,null,null,null,"3. Economic benchmarking"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"4. Alternative control services",null,null,null,null,null,null,"5. Network information",null,null,null,null,null,null,"6. Service & quality"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"7. Other templates"]

{"sheet":"Instructions","index":3,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[7,2,7,3],[1,1,1,5],[2,1,2,5],[3,2,3,4],[4,2,4,4],[5,2,5,4],[24,2,24,4],[25,2,25,3],[26,2,26,4],[8,2,8,4],[10,2,10,4],[12,2,12,4],[20,2,20,4],[22,2,22,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Segment,\" Network Service Provider\")","v":"Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingName,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by SA Power Networks to fulfil its reporting obligations to the AER."}]
[null,null,"INSTRUCTIONS"]
[null,null,"Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,null,"Identifying CONFIDENTIAL INFORMATION:\n\nPlease use the macro at the top of each \nworksheet to identify confidential information. \n\nSee Returning completed responses below, for how to deal with confidential and public information."]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selected cells as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return cells to NON-CONFIDENTIAL macro."]
[]
[null,null,"UNITS OF MEASURE\n\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,null,"COLOUR CODING OF INPUT / NON-INPUT CELLS:"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," \nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,null,"WORKSHEET NAVIGATION\n\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]
[]
[null,null,"RETURNING COMPLETED RESPONSES\n\nPlease return two (2) files to the AER: \n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,null,"SUBMITTING AMENDED DATA TO THE AER\n\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]

{"sheet":"Business & other details","index":4,"n_rows":156,"n_cols":9,"rows_kept":156,"cut":false,"hidden":false,"merged":[[59,2,59,8],[18,4,18,7],[19,2,19,3],[19,4,19,7],[22,2,22,3],[22,4,22,7],[23,4,23,7],[24,2,24,3],[24,4,24,7],[32,1,32,8],[57,2,57,3],[58,4,58,8],[7,1,7,8],[11,1,11,8],[13,2,13,4],[14,2,14,4],[17,2,17,3],[17,4,17,7]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"}]
[null,{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result))","v":"2020-21 to 2024-25"}]
[null,"BUSINESS & OTHER DETAILS"]
[]
[]
[null,"Instructions"]
[null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,"SUBMISSION PARTICULARS INPUT SHEETS"]
[]
[null,"ENTITY DETAILS"]
[]
[null,"Short name","SA Power Networks",null,null,"Select business name from drop down list first"]
[null,"ACN / ABN",{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":13332330749}]
[]
[]
[null,"Business address","Address 1",null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"1 Anzac Highway"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"KESWICK"}]
[null,null,null,"State",{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},"p/code",{"$f":"INDEX(dms_PostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5035}]
[]
[null,"Postal address","Address 1",null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 77"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"ADELAIDE"}]
[null,null,null,"State",{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},"p/code",{"$f":"INDEX(dms_PPostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5000}]
[]
[]
[null,"Contact name/s",{"$f":"INDEX(dms_ContactName1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Richard Sibly"}]
[null,"Contact phone/s",{"$f":"INDEX(dms_ContactPh1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"08 8404 5613"}]
[null,"Contact email address/s",{"$f":"INDEX(dms_ContactEmail_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"richard.sibly@sapowernetworks.com.au"}]
[]
[null,"REGULATORY CONTROL PERIODS"]
[]
[null,"Forthcoming regulatory control period","2020-21",{"$f":"dms_FRCP_y2","v":"2021-22"},{"$f":"dms_FRCP_y3","v":"2022-23"},{"$f":"dms_FRCP_y4","v":"2023-24"},{"$f":"dms_FRCP_y5","v":"2024-25"}]
[null,null,{"$f":"dms_FRCP_y6","v":"2025-26"},{"$f":"dms_FRCP_y7","v":"2026-27"},0,{"$f":"dms_FRCP_y9","v":"2028-29"},{"$f":"dms_FRCP_y10","v":"2029-30"}]
[]
[]
[null,"Current regulatory control period",{"$f":"dms_CRCP_FirstYear_Result","v":"2015-16"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+1)&\"-\"&TEXT(MID(CRCP_y1,3,2)+2,\"00\"),VALUE(LEFT(CRCP_y1,4)+1))","v":"2016-17"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+2)&\"-\"&TEXT(VALUE(MID(CRCP_y1,3,2)+3),\"00\"),VALUE(LEFT(CRCP_y1,4)+2))","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+3)&\"-\"&TEXT(MID(CRCP_y1,3,2)+4,\"00\"),VALUE(LEFT(CRCP_y1,4)+3))","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+4)&\"-\"&TEXT(MID(CRCP_y1,3,2)+5,\"00\"),VALUE(LEFT(CRCP_y1,4)+4))","v":"2019-20"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+5)&\"-\"&TEXT(MID(CRCP_y1,3,2)+6,\"00\"),VALUE(LEFT(CRCP_y1,4)+5))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+6)&\"-\"&TEXT(MID(CRCP_y1,3,2)+7,\"00\"),VALUE(LEFT(CRCP_y1,4)+6))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+7)&\"-\"&TEXT(MID(CRCP_y1,3,2)+8,\"00\"),VALUE(LEFT(CRCP_y1,4)+7))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+8)&\"-\"&TEXT(MID(CRCP_y1,3,2)+9,\"00\"),VALUE(LEFT(CRCP_y1,4)+8))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+9)&\"-\"&TEXT(MID(CRCP_y1,3,2)+10,\"00\"),VALUE(LEFT(CRCP_y1,4)+9))","v":"2024-25"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+10)&\"-\"&TEXT(MID(CRCP_y1,3,2)+11,\"00\"),VALUE(LEFT(CRCP_y1,4)+10))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+11)&\"-\"&TEXT(MID(CRCP_y1,3,2)+12,\"00\"),VALUE(LEFT(CRCP_y1,4)+11))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+12)&\"-\"&TEXT(MID(CRCP_y1,3,2)+13,\"00\"),VALUE(LEFT(CRCP_y1,4)+12))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+13)&\"-\"&TEXT(MID(CRCP_y1,3,2)+14,\"00\"),VALUE(LEFT(CRCP_y1,4)+13))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+14)&\"-\"&TEXT(MID(CRCP_y1,3,2)+15,\"00\"),VALUE(LEFT(CRCP_y1,4)+14))","v":"2029-30"}]
[]
[]
[null,"Previous regulatory control period",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y2,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y2,3,2)),\"00\"),VALUE(LEFT(PRCP_y2,4)-1))","v":"2010-11"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y3,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y3,3,2)),\"00\"),VALUE(LEFT(PRCP_y3,4)-1))","v":"2011-12"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y4,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y4,3,2)),\"00\"),VALUE(LEFT(PRCP_y4,4)-1))","v":"2012-13"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y5,4)-1)&\"-\"&TEXT(VALUE(RIGHT(PRCP_y5,2)-1),\"00\"),VALUE(LEFT(PRCP_y5,4)-1))","v":"2013-14"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2014-15"}]
[]
[]
[]
[null,"Commencing regulatory year","2018-19","CRY"]
[]
[null,"Last completed regulatory year","2024-25","dms_FinalYear"]
[]
[]
[]
[null,null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Source","Regulatory proposal",null,"Please select the correct submission type from the dropdown list."]
[null,"Data quality (actual, estimate, public, consolidated)","Public",null,"Use Consolidated for Consolidated Confidential version\nUse Public for Consolidated Public version"]
[null,"Amended RIN submission - amendment reason","."]
[null,"Submission Date","31/01/2019","dms_SubmissionDate","Please enter date this file submitted to AER (dd/mm/yyyy)"]
[null,"EBSS - First application of scheme in forthcoming period?","No"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))","v":"2025"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Model or RIN Type","Reset","dms_Model","Drop down selection"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an ABC RIN apply the NAMED RANGE to the cell"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FORECAST and MultiYear RINS"]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))","v":{"$error":"#VALUE!"}},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))","v":"June 2020"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)","v":"June 2015"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"Single Year Model T/F",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},null,"=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Reference","CRY","dms_SingleYear_FinalYear_Ref","This is the reference for EB, CA & ARR RINs"]
[null,"Single Year Final Year Result",{"$f":"IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")","v":"not a single year RIN"},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Multi Year Final Year Reference",{"$f":"INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))","v":"dms_FRCP_y5"},"dms_MultiYear_FinalYear_Ref","=INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))"]
[null,"Multi Year Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)","v":"2024-25"},"dms_MultiYear_FinalYear_Result","=IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)",null,null,null,"Formula errors OK"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP Final Year Reference",{"$f":"INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))","v":"CRCP_y5"},"dms_CRCP_FinalYear_Ref","=INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))"]
[null,"CRCP First Year Result",{"$f":"INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))","v":"2015-16"},"dms_CRCP_FirstYear_Result","=INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))"]
[null,"CRCP Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)","v":"2019-20"},"dms_CRCP_FinalYear_Result","=IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"Is this a multi year ABC RIN?","No"]
[null,"Multiyear EB, CA or ARR?",{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year RINS",{"$f":"IF(dms_MultiYear_Flag=1,FRY,CRY)","v":"2018-19"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))","v":{"$error":"#VALUE!"}},"dms_0306_Year","=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(SUM(dms_SingleYear_Model)>0,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))","v":"1-Jul-2018"},"dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060701_StartDateTxt)","v":43282},"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes",null,"=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","6.8 not present","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"6.8 not present\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2012"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2015-20 Distribution Determination"},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]

{"sheet":"CPI series","index":5,"n_rows":13,"n_cols":12,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,2,9,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"CPI SERIES"]
[]
[]
[]
[null,"NOMINATED CPI SERIES"]
[]
[null,"Name of CPI series","2015/16 to 2017/18: All groups weighted average of 8 capital cities CPI movement from December to December\n2018/19 and 2019/20: Reserve Bank of Australian forecast per Statement on Monetary Policy, November 2018.\n2020/21 to 2024/25: Mid-point of RBA target range\n"]
[]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Series data",1.6885553470919357E-2,1.4760147601476037E-2,1.9090909090909047E-2,2.0000000000000018E-2,2.2499999999999964E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]

{"sheet":"2.1 Expenditure summary","index":6,"n_rows":120,"n_cols":9,"rows_kept":120,"cut":false,"hidden":false,"merged":[[100,1,101,1],[100,2,100,8],[112,1,113,1],[112,2,112,8],[8,1,9,1],[23,1,24,1],[36,1,37,1],[8,2,8,8],[36,2,36,8],[23,2,23,3],[73,1,74,1],[48,1,49,1],[60,1,61,1],[48,2,48,8],[60,2,60,8],[73,2,73,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",147112951.00663885,148926610.53503478,122753636.34494518,129282607.6562753,131249141.15242518,128579545.73280086,125310498.24797373]
[null,"Connections",{"$f":"75860628.5534858+26893483.78","v":102754112.3334858},{"$f":"67543811.9280951+26301695.63","v":93845507.558095098},{"$f":"81915063.5706786+27452246.32","v":109367309.89067861},{"$f":"83693552.2761814+27452246.32","v":111145798.59618139},{"$f":"84874477.065914+27452246.32","v":112326723.385914},{"$f":"84465056.5725603+27452246.32","v":111917302.8925603},{"$f":"80744048.870547+27452246.32","v":108196295.19054699}]
[null,"Augmentation Expenditure",96204386.300860882,93274257.166313961,80826309.203480124,79022747.64021346,69903224.435436592,70582202.345374361,71714786.548437655]
[null,"Non-network",106253451.67851318,114477633.81693402,113683411.41644204,120205812.31101638,91472492.807988495,92212312.668995857,87270612.698632568]
[null,"Public lighting"]
[null,"Metering"]
[null,"Capitalised network overheads",14391040.05051885,14153119.163660742,12505684.283527927,12744409.747919237,12424946.776067952,12415356.601362135,12332388.022562472]
[null,"Capitalised corporate overheads",-10552454.993224638,-10648557.627008881,-7498424.1512738997,-7578441.3625455964,-7670285.8997864816,-7753980.2099380232,-7828688.8329113321]
[null,"capcons (included in the above)",{"$f":"35488265.8274336+26893483.78","v":62381749.607433602},{"$f":"30745099.61415+26301695.63","v":57046795.244149998},{"$f":"43181108.4629098+27452246.32","v":70633354.782909811},{"$f":"42801189.3120298+27452246.32","v":70253435.632029802},{"$f":"43332570.1165832+27452246.32","v":70784816.436583191},{"$f":"43186020.0485091+27452246.32","v":70638266.368509099},{"$f":"40300755.5816824+27452246.32","v":67753001.901682407}]
[null,"Total",{"$f":"SUM(C11:C18)","v":456163486.37679297},{"$f":"SUM(D11:D18)","v":454028570.61302978},{"$f":"SUM(E11:E18)","v":431637926.98779994},444822934.58906019,409706242.65804577,407952740.03115541,396995891.87524211]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"}]
[null,"Vegetation management",38711177.69851312,39162260.490005068]
[null,"Maintenance",27621020.368912727,28102124.577151921]
[null,"Emergency response",35967788.130561113,36673588.430959091,null," "]
[null,"Non-network",28202266.140273821,27757942.985530782]
[null,"Metering",0,0]
[null,"Network overheads",96385185.087744132,97987310.311315283]
[null,"Corporate overheads",49304845.989438072,50109044.763587043]
[null,"Total",{"$f":"SUM(C26:C32)","v":276192283.415443},{"$f":"SUM(D26:D32)","v":279792271.55854917}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Public lighting",21504134.256002266,27072774.318086781,16299635.197779935,9500874.1874257252,10107399.267028848,2432784.5107311136,2314423.8583642873]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Network overheads",1225735.6525921263,1543148.1361309439,929079.20627345517,541549.82868326642,576121.75822064281,138668.71711167321,131922.1599267642]
[null,"Corporate overheads",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C39:C44)","v":22729869.908594392},28615922.454217725,17228714.40405339,10042424.016108992,10683521.025249491,2571453.2278427868,2446346.0182910515]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Metering",5597191.8900834145,5317316.7850912418,5061697.2036617631,4806077.6222322844,4550458.0408028066,4294838.4593733288,4039218.8779438511]
[null,"Public lighting",8967725.8718429655,7766707.012932539,6786781.3624396529,6852600.5296113892,7091131.3273993796,7334984.3071630262,6817008.9344895622]
[null,"Fee and quoted",39990952,39540516,39134496,38767587,38436798,38138548,37869477]
[null,"Network overheads",6203562.219158045,6127794.2144831363,6056505.556468172,6047590.4495086716,6050248.1503610089,6054487.4121109219,6016311.5449013608]
[null,"Corporate overheads",9651583.8997327592,9696397.4612076301,10339077.669873884,10502691.985571951,10690886.970359815,10821969.95288053,10947153.455783095]
[null,"Total",{"$f":"SUM(C51:C56)","v":70411015.88081719},68448731.473714545,67378557.792443469,66976547.5869243,66819522.488923013,66644828.131527811,65689169.813117877]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",0,0,0,0,0,0,0]
[null,"Connections",0,0,0,0,0,0,0]
[null,"Augmentation expenditure",0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0]
[null,"capcons (included in the above)",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C63:C68)","v":0},{"$f":"SUM(D63:D68)","v":0},0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"}]
[null,"Vegetation management",0,0]
[null,"Maintenance",0,0]
[null,"Emergency response",0,0]
[null,"Non-network",0,0]
[null,"Metering",0,0]
[null,"Network overheads",0,0]
[null,"Corporate overheads",0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C76:C96)","v":0},{"$f":"SUM(D76:D96)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",3249262.4731392357,3249262.4731392357,3249262.4731392357,3249262.4731392357,3249262.4731392357,3249262.4731392357,3249262.4731392357]
[null,"Connections",{"$f":"28434756.4638823+26893483.78","v":55328240.243882298},{"$f":"23876829.4613128+26301695.63","v":50178525.091312796},{"$f":"35827163.4760079+27452246.32","v":63279409.796007901},{"$f":"35462081.6554004+27452246.32","v":62914327.975400403},{"$f":"35972709.9591141+27452246.32","v":63424956.279114097},{"$f":"35831883.24496+27452246.32","v":63284129.564960003},{"$f":"33059299.651732+27452246.32","v":60511545.971732005}]
[null,"Augmentation Expenditure",2418291.1688781912,2418291.1688781912,2418291.1688781912,2418291.1688781912,2418291.1688781912,2418291.1688781912,2418291.1688781912]
[null,"Non-network",0,0,0,0,0,0,0]
[null,"Capitalised network overheads",1385955.7215338957,1200716.5108197767,1686391.3448845337,1671554.0146119604,1692306.5154516818,1686583.1615316535,1573902.2879329866]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C103:C108)","v":62381749.607433617},{"$f":"SUM(D103:D108)","v":57046795.244149998},70633354.782909855,70253435.632029787,70784816.436583206,70638266.368509084,67753001.901682422]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Replacement expenditure",1097761.5252897888,983192.09475509217,1549643.2510488345,1601720.1576627991,1461139.9033045541,1428076.0058506993,1373442.0913367495]
[null,"Connections",559043.63978891959,484097.74601594219,891727.9638386115,924079.28999848408,832479.85793064209,810075.22300464148,773935.91436604736]
[null,"Augmentation Expenditure",2563338.7554271533,2455244.5558596044,2633517.4763714042,2699121.2791467225,2563014.368762305,2539269.9976442498,2491569.2486321926]
[null,"Non-network",-381558.86321164691,-417972.8599787741,-67628.559004820418,-58952.341434361646,-101973.25371602853,-116044.83507547551,-135248.06468384736]
[null,"capcons (included in the above)",1385955.7215338957,1200716.5108197767,1686391.3448845337,1671554.0146119604,1692306.5154516818,1686583.1615316535,1573902.2879329866]
[null,"Total",{"$f":"SUM(C115:C118)","v":3838585.0572942151},{"$f":"SUM(D115:D118)","v":3504561.5366518646},5007260.1322540287,5165968.3853736445,4754660.8762814729,4661376.3914241157,4503699.1896511428]

{"sheet":"2.2 Repex","index":7,"n_rows":524,"n_cols":11,"rows_kept":524,"cut":false,"hidden":false,"merged":[[399,1,406,1],[390,1,398,1],[475,1,482,1],[466,1,474,1],[452,1,465,1],[423,1,451,1],[407,1,422,1],[357,1,376,1],[377,1,383,1],[384,1,389,1],[129,1,136,1],[120,1,128,1],[302,1,309,1],[293,1,301,1],[279,1,292,1],[250,1,278,1],[234,1,249,1],[226,1,233,1],[217,1,225,1],[9,4,9,10],[182,4,182,10],[355,4,355,10],[11,1,30,1],[31,1,37,1],[38,1,43,1],[184,1,203,1],[204,1,210,1],[211,1,216,1],[106,1,119,1],[77,1,105,1],[61,1,76,1],[44,1,52,1],[53,1,60,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.2 REPEX"]
[]
[null,"There is ONE table on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($0's, real June 2020)"}]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,7663438.1399999997,6927816.7800000003,5633399.2400000002,5882167.9500000002,5928502.5599999996,5964837.5300000003,5994381.3899999997]
[null,null,"> 1 kV & < = 11 kV",null,14267974.970000001,12898377.279999999,10488399.32,10951562.939999999,11037829.84,11105479.17,11160484.640000001]
[null,null,"˃ 11 kV & < = 22 kV",null,4863022.5599999996,4396215.99,3574811.6,3732673.89,3762076.65,3785133.9,3803881.68]
[null,null,"> 22 kV & < = 66 kV",null,3501782.91,3165643.14,2574163.2999999998,2687837.34,2709009.79,2725612.93,2739112.9]
[null,null,"> 66 kV & < = 132 kV",null,5538.02,5006.42,4071.01,4250.78,4284.26,4310.5200000000004,4331.87]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",98363.06,100110.89,49691.24,51885.58,52294.29,52614.8,52875.4]
[null,null,"> 1 kV & < = 11 kV","per km",2445648.0299999998,2489105.08,1235497.06,1290056.1299999999,1300218.07,1308186.93,1314666.3799999999]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",2237852.91,2277617.92,1130522.74,1180446.18,1189744.71,1197036.49,1202965.42]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",756510.23,1020061.1,629363.54,657155.99,662332.5,666391.84,669692.48]
[null,null,"> 1 kV & < = 11 kV","per km",1247960.05,1682720.78,3722237.62,3886610.18,3917225.52,3941233.65,3960754.59]
[null,null,"> 11 kV & < = 22 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",8106293.6600000001,6521988.5199999996,6693430.5800000001,6989009.8600000003,7044063.21,7087235.2999999998,7122338.3899999997]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",972989.85,782827.38,803405.39,838883.46,845491.45,850673.35,854886.74]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,4227847.04,4150036.61,3433239.34,3584849.85,3613088.18,3635232.3,3653237.62]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,696056.37,713439.83,566263.18000000005,532102.62,417028.9,359586.76,361367.79]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,944016.95,926643.01,766592.57,800445,806750.21,811694.67,815715]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,1892833.15,1857996.94,1537082.39,1604959.35,1617601.83,1627515.88,1635576.97]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,11443.75,11233.14,9292.94,9703.31,9779.75,9839.69,9888.42]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,2986.86,2931.89,2425.4899999999998,2532.6,2552.5500000000002,2568.19,2580.91]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,187918.49,184459.99,152599.93,159338.68,160593.81,161578.07,162378.37]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,73079.41,71734.44,59344.42,61965.04,62453.15,62835.92,63147.14]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,49009.63,48107.64,39798.46,41555.94,41883.279999999999,42139.98,42348.7]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,868946.22,852953.9,705631.1,736791.49,742595.3,747146.56,750847.18]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,289573.40999999997,284244.02,235149.19,245533.29,247467.39,248984.08,250217.3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,40621.32,88576.06,66273.97,69200.600000000006,69745.710000000006,70173.17,70520.740000000005]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,739308.11,1612084.21,1206186.28,1259451,1269371.8600000001,1277151.6599999999,1283477.3999999999]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,1943053.37,1718080.22,727246.38,759361.3,765342.89,770033.57,773847.55]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,3344759.88,3276723.55,1700369.2,1775456.84,2580126.17,1800409.59,1009856.94]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,205814.71,89757.07,67157.62,140246.56,70675.649999999994,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,11975587.33,8897247.1400000006,6104322.8099999996,6373887.3200000003,5545950.3300000001,5579940.6799999997,6495481.2300000004]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,143535.18,56771.35,42477.2,44352.97,44702.35,44976.32,45199.08]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,3566457.98,2691001.87,2619401.7400000002,2735073.5,4502306.57,4529900.58,2787250.18]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,62485.35,85157.02,63715.8,66529.460000000006,67053.52,67464.479999999996,67798.64]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,828715.2,1066385.46,820645.82,935773.91,943145.12,868928.12,873231.92]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,3992095.36,4071952.88,3240355.38,3427275.26,3339424.43,3182119.27,3180015.07]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,4412719.5199999996,5363378.8899999997,4890754.09,5037481.51,4248931.5599999996,4810955.0199999996,4761536.25]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,236123.31,371792.13,277025.65999999997,289259,291537.53999999998,293324.33,817334.83]
[null,null,"Communications Linear Assets",null,335844,2635953.9500000002,1093936.76,482097.67,485895.22,488873.21,491294.6]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"OTHER BY: \nenter DNSP defined asset group here","˂ = 1 kV; stobie pole",null,11773254.35,12640943.449999999,6794248.4299999997,7094279.79,7150162.3600000003,7193984.71,7229616.54]
[null,null,"> 1 kV & < = 11 kV; stobie pole",null,10507613.84,11282025.199999999,14097205.16,14719732.25,14835681.52,14926607.34,15000538.869999999]
[null,null,"˃ 11 kV & < = 22 kV; stobie pole",null,3138769.3,3370096.66,3623105.01,3783099.92,3812899.89,3836268.62,3855269.67]
[null,null,"> 22 kV & < = 66 kV; stobie pole",null,773689.54,830710.48,1350834.39,1410486.71,1421597.3,1430310.07,1437394.4]
[null,null,"> 66 kV & < = 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,null,"Pole REFURBISHED; STOBIE Pole",null,6818552.9900000002,7321080.5,6631931.4100000001,6924794.9100000001,6979342.4299999997,7022117.8499999996,7056898.4199999999]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA",null,88222.64,86598.97,71641.53,74805.19,75394.44,75856.53,76232.240000000005]
[null,null,"Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA ",null,244581.51,240080.16,198613.35,207384.03,209017.63,210298.67,211340.28]
[null,null,"Kiosk Mounted; > = 22 kV & < = 33 kV ; ",null,3554.85,3489.42,2886.73,3014.2,3037.95,3056.57,3071.71]
[null,null,"Recloser ;SWITCHGEAR",null,5914867.1699999999,5105526.59,3321803.34,3468492.88,3495814.65,3517240.01,3534660.92]
[null,null,"Sectionalizer ;SWITCHGEAR",null,101649.87,87740.96,57086.81,59607.74,60077.279999999999,60445.48,60744.87]
[null,null,">= 11 kV & < ≈ 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,6347272.21,6631403.1799999997,3781409.75,3948395.34,3979497.36,4003887.15,4023718.41]
[null,null,"> 22 kV & < ≈ 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,0,0,0,0,0,0,0]
[null,null,"Non Category Substation asset replacement/refurbishment",null,5106319.91,6806273.2400000002,5353965.72,5305535.0999999996,5320824.13,5346653.0599999996,4865204.71]
[null,null,"Pipe Buswork Substations",null,2243380.36,3598697.51,2593963.25,2708511.65,2729846.96,2577694.38,2215291.39]
[null,null,"˂ = 11 kV ;  Circuit Breaker REFURBISHED",null,1435557.62,1352843.13,529214.86,214109.72,215796.29,217118.87,218194.26]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",null,46308.31,116276.2,148815.19,155386.81,156610.81,157570.66,158351.10999999999]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED",null,77180.52,112196.34,83947.03,87654.1,88344.56,88886.01,89326.27]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",null,336490.71,428242.2,264433.15000000002,219135.25,167854.67,168883.43,169719.91]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",null,499023.8,428242.2,264433.15000000002,219135.25,167854.67,168883.43,169719.91]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA REFURBISHED",null,1226182.92,1284726.6000000001,793299.44,657405.74,503564,506650.28,509159.72]
[null,null,"Northfield GIS Replacement",null,391047.95,190733.77,1049337.8799999999,3681472.15,4417228.08,1777720.26,0]
[null,null,"˂ = 11 kV  ; Switch REFURBISHED",null,11115.48,18729.09,14837.71,15492.94,15614.98,15710.68,15788.5]
[null,null,"> 22 kV & < = 33 kV ; Switch REFURBISHED",null,65650.81,110618.7,87635.24,91505.18,92225.98,92791.22,93250.82]
[null,null,"> 33 kV & < = 66 kV ; Switch REFURBISHED",null,141140.04,225753.61,177490.39,185328.3,174640.77,163489.29999999999,164299.06]
[null,null,"OTHER - Non Category Line asset replacement/refurbishment",null,2583318.02,3257448.18,4495217.1100000003,4720078.0999999996,4777136.3,4835302.66,4868184.5599999996]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"ASSET REPLACEMENTS (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,6181.7181448669726,5125.6586351260612,5570.5381921294411,5570.5381921294411,5570.5381921294411,5570.5381921294411,5570.5381921294411]
[null,null,"> 1 kV & < = 11 kV",null,6680.0071168589193,5538.8219518973683,6019.5618590371441,6019.5618590371441,6019.5618590371441,6019.5618590371441,6019.5618590371441]
[null,null,"˃ 11 kV & < = 22 kV",null,1791.0176247866716,1485.047480169176,1613.941601322525,1613.941601322525,1613.941601322525,1613.941601322525,1613.941601322525]
[null,null,"> 22 kV & < = 66 kV",null,606.52330359782843,502.90733670425152,546.55698430924349,546.55698430924349,546.55698430924349,546.55698430924349,546.55698430924349]
[null,null,"> 66 kV & < = 132 kV",null,1.2671238619578276,1.0506535905735941,1.1418446622409906,1.1418446622409906,1.1418446622409906,1.1418446622409906,1.1418446622409906]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",1.5418243197485677,1.4393019385389736,0.9548249010253097,0.9548249010253097,0.9548249010253097,0.9548249010253097,0.9548249010253097]
[null,null,"> 1 kV & < = 11 kV","per km",98.953852229819915,92.373994569955101,61.280394238961541,61.280394238961541,61.280394238961541,61.280394238961541,61.280394238961541]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",7.005425640070432,6.5396054368167382,4.3383378752977606,4.3383378752977606,4.3383378752977606,4.3383378752977606,4.3383378752977606]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",2.0764041295250308,2.5679762511430928,2.1175795829445283,2.1175795829445283,2.1175795829445283,2.1175795829445283,2.1175795829445283]
[null,null,"> 1 kV & < = 11 kV","per km",1.6636673581289323,2.0575273400435452,6.0829043703693797,6.0829043703693797,6.0829043703693797,6.0829043703693797,6.0829043703693797]
[null,null,"> 11 kV & < = 22 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",12879.986919694595,9504.7535757828009,13037.158172560305,13037.158172560305,13037.158172560305,13037.158172560305,13037.158172560305]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",1462.9562687499251,1079.5848562045301,1480.8083575044238,1480.8083575044238,1480.8083575044238,1480.8083575044238,1480.8083575044238]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,246.71433478921946,222.12364339870376,245.59542907033261,245.59542907033261,245.59542907033261,245.59542907033261,245.59542907033261]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,23.166899058336949,20.806318260088457,22.582240418099847,21.582240418099847,19.582240418099847,18.582240418099847,18.582240418099847]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,52.702694077152486,47.449672656215391,52.463675351896612,52.463675351896612,52.463675351896612,52.463675351896612,52.463675351896612]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,103.13346352171757,92.853869611358448,102.66572976704278,102.66572976704278,102.66572976704278,102.66572976704278,102.66572976704278]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.6846509162168638,0.61640988998988522,0.68154586832311004,0.68154586832311004,0.68154586832311004,0.68154586832311004,0.68154586832311004]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0.23842611900562427,0.21466153671284915,0.23734480223367704,0.23734480223367704,0.23734480223367704,0.23734480223367704,0.23734480223367704]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,4.1615035187011999,3.746715100199471,4.1426301521000228,4.1426301521000228,4.1426301521000228,4.1426301521000228,4.1426301521000228]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,1.6183624794949112,1.4570558722997944,1.6110228369277866,1.6110228369277866,1.6110228369277866,1.6110228369277866,1.6110228369277866]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0.95282539703253666,0.85785468806464993,0.94850411676825375,0.94850411676825375,0.94850411676825375,0.94850411676825375,0.94850411676825375]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,32.592937856532288,29.344310746863165,32.445121457480511,32.445121457480511,32.445121457480511,32.445121457480511,32.445121457480511]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,4.9990971922698195,4.5008235253127413,4.9764251475243011,4.9764251475243011,4.9764251475243011,4.9764251475243011,4.9764251475243011]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0.15789473684210525,0.31578947368421051,0.31578947368421051,0.31578947368421051,0.31578947368421051,0.31578947368421051,0.31578947368421051]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,1.736842105263158,3.4736842105263159,3.4736842105263159,3.4736842105263159,3.4736842105263159,3.4736842105263159,3.4736842105263159]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0.86842105263157898,0.73684210526315785,0.73684210526315785,0.73684210526315785,0.73684210526315785,0.73684210526315785,0.73684210526315785]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,1.3157894736842106,1.631578947368421,1.131578947368421,1.131578947368421,1.631578947368421,1.131578947368421,0.63157894736842102]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,2.5,1,1,2,1,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,26.5,17.590909090909093,19.181818181818183,19.181818181818183,19.181818181818183,19.181818181818183,19.181818181818183]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,1.6,2,2,2,2,2,2]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,10,5.0075757575757578,7.0151515151515147,7.0151515151515147,12.515151515151516,12.515151515151516,7.0151515151515147]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,2.4,3,3,3,3,3,3]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,3,2.7171717171717171,2.4343434343434343,2.9343434343434343,2.9343434343434343,2.4343434343434343,2.4343434343434343]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,94.45859999999999,98.458600000000004,75.599999999999994,77.599999999999994,81.8,80.8,78.599999999999994]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,669,170,466,125,79,218,220]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,1]
[null,null,"Communications Linear Assets",null,6.34,13.34,9.34,8.34,8.34,8.34,8.34]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C138),\"\",C138)","v":"˂ = 1 kV; stobie pole"},null,1263.7442448148549,1257.9597262923928,1013.0873578555751,1013.0873578555751,1013.0873578555751,1013.0873578555751,1013.0873578555751]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":""},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"> 1 kV & < = 11 kV; stobie pole"},null,728.71130771569278,725.37578783158335,1358.0857810541693,1358.0857810541693,1358.0857810541693,1358.0857810541693,1358.0857810541693]
[null,"","˃ 11 kV & < = 22 kV; stobie pole",null,281.81002556118318,280.52010054719199,451.87627299661563,451.87627299661563,451.87627299661563,451.87627299661563,451.87627299661563]
[null,"","> 22 kV & < = 66 kV; stobie pole",null,35.624772560871975,35.461707797109554,86.403165928668699,86.403165928668699,86.403165928668699,86.403165928668699,86.403165928668699]
[null,"","> 66 kV & < = 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,"","> 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,"","Pole REFURBISHED; STOBIE Pole",null,4167.0473275809682,4147.9735612320665,5630.1285703946251,5630.1285703946251,5630.1285703946251,5630.1285703946251,5630.1285703946251]
[null,"","Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA",null,7.056396363749224,6.3530660710106091,7.0243939985324761,7.0243939985324761,7.0243939985324761,7.0243939985324761,7.0243939985324761]
[null,"","Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA ",null,7.708417804434208,6.9400987543881492,7.6734583734294404,7.6734583734294404,7.6734583734294404,7.6734583734294404,7.6734583734294404]
[null,"","Kiosk Mounted; > = 22 kV & < = 33 kV ; ",null,6.1420921949570398E-2,5.5298930951871647E-2,6.11423640745795E-2,6.11423640745795E-2,6.11423640745795E-2,6.11423640745795E-2,6.11423640745795E-2]
[null,"","Recloser ;SWITCHGEAR",null,308.1042540835669,243.92762280863778,212.11320073017575,212.11320073017575,212.11320073017575,212.11320073017575,212.11320073017575]
[null,"","Sectionalizer ;SWITCHGEAR",null,29.893812477957109,23.667075406422295,20.580281390750674,20.580281390750674,20.580281390750674,20.580281390750674,20.580281390750674]
[null,"",">= 11 kV & < ≈ 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,134.70671615743586,129.08485792183771,98.377763989286422,98.377763989286422,98.377763989286422,98.377763989286422,98.377763989286422]
[null,"","> 22 kV & < ≈ 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,0,0,0,0,0,0,0]
[null,"","Non Category Substation asset replacement/refurbishment",null,115.75,147.26666666666665,152.73333333333335,159.73333333333335,157.53333333333333,156.03333333333333,106.11666666666667]
[null,"","Pipe Buswork Substations",null,3,3.5,3,3,3,3,2]
[null,"","˂ = 11 kV ;  Circuit Breaker REFURBISHED",null,90,75,67.2,74.400000000000006,74.400000000000006,74.400000000000006,74.400000000000006]
[null,"","> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",null,1.5,3.4545454545454546,5.9090909090909092,5.9090909090909092,5.9090909090909092,5.9090909090909092,5.9090909090909092]
[null,"","> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED",null,1.5,2,2,2,2,2,2]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",null,2,2,2,1.5,1,1,1]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",null,3.5,2,2,1.5,1,1,1]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA REFURBISHED",null,8,6,6,4.5,3,3,3]
[null,"","Northfield GIS Replacement",null,0,0,0,0,0,0,0]
[null,"","˂ = 11 kV  ; Switch REFURBISHED",null,1.5884476534296028,2.4548736462093865,2.5992779783393503,2.5992779783393503,2.5992779783393503,2.5992779783393503,2.5992779783393503]
[null,"","> 22 kV & < = 33 kV ; Switch REFURBISHED",null,9.3817689530685922,14.499097472924188,15.351985559566788,15.351985559566788,15.351985559566788,15.351985559566788,15.351985559566788]
[null,"","> 33 kV & < = 66 kV ; Switch REFURBISHED",null,21.029783393501805,30.546028880866427,32.048736462093864,32.048736462093864,29.548736462093864,27.048736462093864,27.048736462093864]
[null,"","OTHER - Non Category Line asset replacement/refurbishment",null,1926.308888888889,2095.3088888888888,2327.508888888889,2327.508888888889,2327.508888888889,2327.508888888889,2327.508888888889]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"ASSET FAILURES (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,3028.5,3028.5,3028.5,3028.5,3028.5,3028.5,3028.5]
[null,null,"> 1 kV & < = 11 kV",null,943.25,943.25,943.25,943.25,943.25,943.25,943.25]
[null,null,"˃ 11 kV & < = 22 kV",null,368.625,368.625,368.625,368.625,368.625,368.625,368.625]
[null,null,"> 22 kV & < = 66 kV",null,56.625,56.625,56.625,56.625,56.625,56.625,56.625]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",1011.75,1011.75,1011.75,1011.75,1011.75,1011.75,1011.75]
[null,null,"> 1 kV & < = 11 kV","per km",201.375,201.375,201.375,201.375,201.375,201.375,201.375]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",64.875,64.875,64.875,64.875,64.875,64.875,64.875]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","per km",3.625,3.625,3.625,3.625,3.625,3.625,3.625]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",684.125,684.125,684.125,684.125,684.125,684.125,684.125]
[null,null,"> 1 kV & < = 11 kV","per km",165.25,165.25,165.25,165.25,165.25,165.25,165.25]
[null,null,"> 11 kV & < = 22 kV","per km",4,4,4,4,4,4,4]
[null,null,"> 22 kV & < = 33 kV","per km",2.25,2.25,2.25,2.25,2.25,2.25,2.25]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",6160.9949999999999,6160.9949999999999,6160.9949999999999,6160.9949999999999,6160.9949999999999,6160.9949999999999,6160.9949999999999]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",694.255,694.255,694.255,694.255,694.255,694.255,694.255]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,101.25,101.25,101.25,101.25,101.25,101.25,101.25]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,18.875,18.875,18.875,18.875,18.875,18.875,18.875]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,25.375,25.375,25.375,25.375,25.375,25.375,25.375]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.14285714285714285,0.14285714285714285,0.14285714285714285,0.14285714285714285,0.14285714285714285,0.14285714285714285,0.14285714285714285]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,1,1,1,1,1,1,1]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0.2857142857142857,0.2857142857142857,0.2857142857142857,0.2857142857142857,0.2857142857142857,0.2857142857142857,0.2857142857142857]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0.125,0.125,0.125,0.125,0.125,0.125,0.125]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,8.75,8.75,8.75,8.75,8.75,8.75,8.75]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0.16666666666666666,0.16666666666666666,0.16666666666666666,0.16666666666666666,0.16666666666666666,0.16666666666666666,0.16666666666666666]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,1.1666666666666667,1.1666666666666667,1.1666666666666667,1.1666666666666667,1.1666666666666667,1.1666666666666667,1.1666666666666667]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,5.2631578947368425E-2,0.10526315789473685,0.10526315789473685,0.10526315789473685,0.10526315789473685,0.10526315789473685,0.10526315789473685]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0.63157894736842113,1.2631578947368423,1.2631578947368423,1.2631578947368423,1.2631578947368423,1.2631578947368423,1.2631578947368423]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0.76315789473684204,0.52631578947368418,0.52631578947368418,0.52631578947368418,0.52631578947368418,0.52631578947368418,0.52631578947368418]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0.2105263157894737,0.4210526315789474,0.4210526315789474,0.4210526315789474,0.4210526315789474,0.4210526315789474,0.4210526315789474]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0.3,0.6,0.6,0.6,0.6,0.6,0.6]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0.1,0.2,0.2,0.2,0.2,0.2,0.2]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0.33333333333333331,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0.3,0.6,0.6,0.6,0.6,0.6,0.6]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0.44444444444444442,0.88888888888888884,0.88888888888888884,0.88888888888888884,0.88888888888888884,0.88888888888888884,0.88888888888888884]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,40,50,50,50,50,50,50]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,9,10,11,12,13,14,15]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,1]
[null,null,"Communications Linear Assets",null,3.9624999999999999,8.3374999999999986,5.8374999999999995,5.2124999999999995,5.2124999999999995,5.2124999999999995,5.2124999999999995]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C138),\"\",C138)","v":"˂ = 1 kV; stobie pole"},null,78,78,78,78,78,78,78]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":""},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"> 1 kV & < = 11 kV; stobie pole"},null,74.5,74.5,74.5,74.5,74.5,74.5,74.5]
[null,"","˃ 11 kV & < = 22 kV; stobie pole",null,21.625,21.625,21.625,21.625,21.625,21.625,21.625]
[null,"","> 22 kV & < = 66 kV; stobie pole",null,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,"","> 66 kV & < = 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,"","> 132 kV; stobie pole",null,0,0,0,0,0,0,0]
[null,"","Pole REFURBISHED; STOBIE Pole",null,0,0,0,0,0,0,0]
[null,"","Pole Mounted ;> = 22 kV & < = 33 kV ;  < = 60kVA",null,3.4285714285714284,3.4285714285714284,3.4285714285714284,3.4285714285714284,3.4285714285714284,3.4285714285714284,3.4285714285714284]
[null,"","Pole Mounted ;> = 22 kV & < = 33 kV ; > 60 KVA AND < = 600 KVA ",null,3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,"","Kiosk Mounted; > = 22 kV & < = 33 kV ; ",null,0,0,0,0,0,0,0]
[null,"","Recloser ;SWITCHGEAR",null,84,84,84,84,84,84,84]
[null,"","Sectionalizer ;SWITCHGEAR",null,28.125,28.125,28.125,28.125,28.125,28.125,28.125]
[null,"",">= 11 kV & < ≈ 22 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993]
[null,"","> 22 kV & < ≈ 33 kV  ; LOAD BREAK SWITCH; GROUND LEVEL (Switching Cubicle);SWITCHGEAR",null,0,0,0,0,0,0,0]
[null,"","Non Category Substation asset replacement/refurbishment",null,7.5,7.6,12.899999999999999,12.899999999999999,10.199999999999999,10.199999999999999,10.199999999999999]
[null,"","Pipe Buswork Substations",null,0,0,0,0,0,0,0]
[null,"","˂ = 11 kV ;  Circuit Breaker REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","> 22 kV & < = 33 kV ; Circuit Breaker REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","> 33 kV & < = 66 kV ; Circuit Breaker REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","Northfield GIS Replacement",null,0,0,0,0,0,0,0]
[null,"","˂ = 11 kV  ; Switch REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","> 22 kV & < = 33 kV ; Switch REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","> 33 kV & < = 66 kV ; Switch REFURBISHED",null,0,0,0,0,0,0,0]
[null,"","OTHER - Non Category Line asset replacement/refurbishment",null,55,55,55,55,55,55,55]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]

{"sheet":"2.3 Augex (a)","index":8,"n_rows":126,"n_cols":32,"rows_kept":126,"cut":false,"hidden":false,"merged":[[68,30,68,31],[68,29,69,29],[69,14,69,16],[11,14,11,15],[10,14,10,16],[10,17,10,19],[11,17,11,18],[68,25,70,25],[68,26,70,26],[70,27,70,29],[70,30,70,31],[68,23,68,24],[68,27,68,28],[70,23,70,24],[9,30,9,31],[9,23,9,24],[9,26,11,26],[11,27,11,29],[11,30,11,31],[9,27,9,28],[9,29,10,29],[9,25,11,25],[11,23,11,24],[10,6,11,6],[10,7,10,8],[10,9,10,10],[10,11,10,13],[5,1,5,3],[9,11,9,22],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,21,10,22],[68,1,68,10],[69,7,69,10],[70,7,70,10],[68,11,68,22],[69,21,69,22],[69,17,69,19],[69,11,69,13],[69,3,70,3],[69,4,70,4],[69,5,70,5],[69,6,70,6],[69,1,70,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both ROWS and COLUMNS have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON-RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE","PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,null,"CAPACITORS",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"UNITS ADDED ",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"MVAR ADDED",null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"Murray Bridge North","Zone substation","Murray Bridge North Sub Upgrade","Capacity upgrade","Demand growth","33/11",26.013829787234044,55.9,14.8,31.4,2,29.886170212765954,1161488.8485073131,28,null,795484.34286260942,0,0,0,1824820.4553518754,16849.021898168685,4991522.7373324726,1732671.9829825286,205612.78226998952,{"$f":"SUM(N13,Q13,T13,U13,W13,X13,Y13)","v":10711601.149306789},"2025,2026",0,0,10711601.149306789,0,0]
[null,"Myponga","Zone substation","Myponga to Square Water Hole new 66kV line","Other","Other","66/11",14.10200296735905,14.10200296735905,7.5,7.5,0,0,0,3,null,130667.75900006601,0,0,0,490536.80052596895,2767.6521260670365,819916.94234735961,284611.96895943244,33774.34354560051,1759507.8143784276,"2019, 2020,2021",0,0,1759507.8143784276,0,0]
[null,"Square Water Hole","Zone substation","Myponga to Square Water Hole new 66kV line","Other","Other","66/11",7.125,7.125,0,0,0,0,0,3,null,130667.75900006601,0,0,0,490536.80052596895,2767.6521260670365,819916.94234735961,284611.96895943244,33774.34354560051,1759507.8143784276,"2019, 2020,2021",0,0,1759507.8143784276,0,0]
[null,"Athol Park","Zone substation","Athol Park to Woodville New 66kV Line","Other","Demand growth","66/11",26.506616257088844,26.506616257088844,14.3,14.3,0,0,0,8,null,667841.3231455849,0,0,0,330936.52999929048,4449.8540880546016,1318269.2735861756,457601.48887755262,54302.670224426431,2828951.28583303,"2024,2025,2026",0,0,2828951.28583303,0,0]
[null,"Port Adelaide North","Zone substation","Athol Park to Woodville New 66kV Line","Other","Demand growth","66/11",47.192079207920784,47.192079207920784,25.3,25.3,0,0,0,3,null,74765.746837966741,0,0,0,280676.35446944687,1583.6008804052719,469141.76082006184,162849.86121377826,19325.073288718511,1006758.7966299722,"2024,2025,2026",0,0,1006758.7966299722,0,0]
[null,"Woodville","Zone substation","Athol Park to Woodville New 66kV Line","Other","Demand growth","66/11",28.2,28.2,0,0,0,0,0,9,null,442953.55239729781,0,0,0,219497.51610273612,2951.4176611137041,874357.48210493487,303509.5284698609,36016.87982899067,1876334.9589038205,"2024,2025,2026",0,0,1876334.9589038205,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N45,Q45,T45,U45,W45,X45,Y45)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31135865.000000004]
[]
[]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID",null,"PROJECT ID","PROJECT TYPE","PROJECT TRIGGER","VOLTAGE (KV)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"Myponga to Square Water Hole new 66kV line",null,"Myponga to Square Water Hole new 66kV line","New line on new route - single circuit","Other",66,19,null,null,null,162,0,6201052.4540035147,19,0,1097301.9390405028,0,0,0,0,31194.648097728092,9241414.4989519473,0,0,{"$f":"SUM(N72,Q72,T72,U72,W72,X72,Y72)","v":16539768.891995965},"2019,2020,2021",0,0,16539768.891995965,0,0]
[null,"Athol Park Tee - Port Adelaide North",null,"Athol Park to Woodville New 66kV Line","Line rebuild over existing route - dual circuit","Demand growth",66,0.55200000000000005,null,null,null,5,1,470602.13984233973,0.55200000000000005,0,83274.999590144827,0,0,0,0,2367.383320059123,701337.30856751523,0,0,1255214.4479999999,"2024,2025,2026",0,0,1255214.4479999999,0,0]
[null,"Athol Park Tee - Athol Park",null,"Athol Park to Woodville New 66kV Line","Reconductor - Single circuit","Demand growth",66,2.4,null,null,null,1,8,705903.20976350969,0,2.4,124912.49938521725,0,0,0,0,3551.0749800886847,1052005.9628512729,0,0,1882821.6719999998,"2024,2025,2026",0,0,1882821.6719999998,0,0]
[null,"Athol Park - Woodville",null,"Athol Park to Woodville New 66kV Line","New line on new route - single circuit","Demand growth",66,3.3460000000000001,null,null,null,21,25,2133457.0073772236,3.3460000000000001,0,377524.06199098547,0,0,0,0,10732.442770065118,3179486.170631791,0,0,5690467.2400000002,"2024,2025,2026",0,0,5690467.2400000002,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N104,Q104,T104,U104,W104,X104,Y104)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3428700.0000000005]

{"sheet":"2.3 Augex (b)","index":9,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[77,1,77,2],[78,1,78,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[68,1,69,2],[68,3,68,9],[70,1,70,2],[71,1,71,2],[60,1,61,2],[60,3,60,9],[62,1,62,2],[63,1,63,2],[45,3,45,9],[47,1,47,2],[9,3,9,9],[29,3,29,9],[31,1,31,2],[32,1,32,2],[33,1,33,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[45,1,46,2],[5,1,5,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[9,1,10,1],[9,2,10,2],[34,1,34,2],[29,1,30,1],[29,2,30,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[51,1,51,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUMES (0's)"]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0.6,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0.13544112642969666,0.11971158142809779,0.12527956195963721,0.13084754249117667,0.13641552302271612,0.14198350355425551,0.14755148408579494]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.15500484469176398,0.13700325430104526,0.14337549868714036,0.14974774307323552,0.15611998745933064,0.1624922318454258,0.1688644762315209]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",96,85,89,93,97,101,105]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",1,1,1,1,1,1,1]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",4.2648905811306692,3.7695846863025446,3.9449142065956861,4.1202437268888277,4.2955732471819701,4.4709027674751107,4.6462322877682523]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",98,87,91,95,99,103,107]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",6,5,5,6,6,6,6]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,"PROJECT TYPE",null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,0,0,0,0,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables",null,0,409375,409375,0,4094.9999999999995,4094.9999999999995,0]
[null,"HV Feeder Non-Material Projects",null,6316500.0579419415,6678381.7110278215,4722995.8603779525,2636575.0097280834,2456079.1590782143,3062553.3084283457,3411882.4577784771]
[null,"LV Feeder Augmentations - Overhead Lines",null,607877.47827796498,537281.22437723528,562271.04876687413,587260.87315651297,612250.69754615193,637240.52193579066,662230.34632542951]
[null,"LV Feeder Augmentations - Underground Cables",null,75179.052179454186,66448.083118530936,69538.691635671901,72629.300152812881,75719.90866995386,78810.51718709484,81901.125704235805]
[null,"LV Feeder Non-Material Projects",null,1312186.5983429861,1159794.93789822,1213738.8884981372,1267682.8390980545,1321626.7896979717,1375570.7402978889,1429514.6908978061]
[null,"Distribution Substation Augmentations - Pole Mounted",null,2239151.7988411388,1979106.4203529076,2071157.8817646708,2163209.3431764338,2255260.8045881973,2347312.2659999602,2439363.7274117232]
[null,"Distribution Substation Augmentations - Ground Mounted",null,169039.0092337149,149407.55184069354,156356.74029840023,163305.92875610688,170255.11721381356,177204.30567152024,184153.49412922692]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,4854775,5650075,8111305,7200984.9999999991,3840740.0000000005,2831235.0000000005,1852070]
[null,"Subtransmission Lines",null,10194204.999999998,9736549.9999999981,7317475,3483165,0,513619.99999999994,4549205.0000000009]
[null,"HV Feeders",null,6316500.0579419415,7087756.7110278215,5132370.8603779525,2636575.0097280834,2460174.1590782143,3066648.3084283457,3411882.4577784771]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,2408190.8080748538,2128513.9721936011,2227514.622063071,2326515.2719325405,2425515.9218020109,2524516.5716714803,2623517.2215409502]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,1995243.1288004052,1763524.2453939863,1845548.6289006833,1927573.0124073802,2009597.3959140773,2091621.7794207744,2173646.1629274711]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,70435472.310000002,66907837.240000002,56192094.869999997,61447934.520000003,59167196.759999998,59554560.420000002,57104465.420000002]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,7668019.9999999991,12151519.999999998,12489019.999999998,7718219.9999999991,4004095,6232695,10435200]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,88536366.299999997,81122737.170000002,68337288.979999989,71304527.810000002,65899129.240000002,64349507.079999998,61279586.259999998]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,1765000,1485000,735000,0,0,1551525,1551525]
[null,"Subtransmission Lines",null,4653020,6761440,6863885,3483165,0,513620,4549205]
[null,"HV Feeders",null,0,655080,890135,235055,4094.9999999999995,167550,334470]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,1250000,3250000,4000000,4000000,4000000,4000000,4000000]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.4 Augex model","index":10,"n_rows":7857,"n_cols":50,"rows_kept":7857,"cut":false,"hidden":false,"merged":[[7727,4,7727,7],[7727,8,7727,11],[7728,1,7730,1],[7728,2,7730,2],[7728,3,7729,3],[7728,5,7730,5],[7728,6,7729,6],[7728,7,7729,7],[7728,9,7730,9],[7728,10,7729,10],[7728,11,7729,11],[7836,38,7836,43],[7836,44,7836,49],[7837,38,7837,43],[7837,44,7837,49],[7838,26,7838,28],[7838,29,7838,31],[7838,32,7838,34],[7838,35,7838,37],[7838,38,7838,40],[7838,41,7838,43],[7838,44,7838,46],[7838,47,7838,49],[7836,32,7836,37],[7837,32,7837,37],[7839,38,7839,40],[7839,41,7839,43],[7839,44,7839,46],[7839,47,7839,49],[7839,32,7839,34],[7839,35,7839,37],[7836,1,7840,1],[7836,2,7836,9],[7836,10,7836,17],[7836,18,7836,25],[7836,26,7836,31],[7839,3,7839,9],[7839,11,7839,17],[7839,19,7839,25],[7837,2,7838,9],[7837,10,7838,17],[7837,18,7838,25],[7837,26,7837,31],[7839,26,7839,28],[7839,29,7839,31],[7664,28,7666,28],[7665,3,7665,13],[7665,14,7666,14],[7665,15,7665,25],[7665,26,7666,26],[7664,1,7667,1],[7664,2,7667,2],[7664,3,7664,14],[7664,15,7664,26],[7664,27,7666,27],[1275,17,1278,17],[6717,22,6719,22],[6717,23,6720,23],[6718,6,6720,6],[6718,7,6719,8],[6718,9,6718,13],[6718,14,6720,14],[6718,15,6719,16],[6718,17,6718,21],[1275,6,1275,10],[8,17,11,17],[9,6,10,6],[6717,1,6720,1],[6717,2,6719,2],[6717,3,6719,3],[6717,4,6718,5],[6717,6,6717,13],[6717,14,6717,21],[9,7,10,8],[9,9,9,10],[9,11,10,11],[9,12,10,13],[9,14,9,15],[8,6,8,10],[1275,1,1278,1],[1275,2,1277,2],[1278,4,1278,5],[5,1,5,4],[1276,14,1276,15],[8,11,8,15],[8,16,10,16],[8,1,11,1],[8,2,10,2],[8,3,10,3],[8,4,10,4],[8,5,10,5],[1276,11,1277,11],[1276,12,1277,13],[1275,4,1277,5],[1275,3,1277,3],[1275,11,1275,15],[1275,16,1277,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.4 AUGEX MODEL"]
[]
[null,"There are SIX tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.4.1 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION LINES"]
[null,"Line ID","Primary type of area supplied by line","Line voltage","Originating substation","Terminating substation",{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual line maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual line maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network Segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","N-1 emergency",null,null,null,"Thermal","N-1 emergency"]
[null,null," CBD, urban, long rural, or short rural "," kV "," name "," name "," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.2 - AUGEX MODEL INPUTS - ASSET STATUS - HIGH VOLTAGE FEEDERS"]
[null,"High voltage feeder ID","High voltage feeder type","Voltage level","Originating substation",null,{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from \", CRCP_y4, \" to \",dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","Operational",null,null,null,"Thermal","Operational"]
[null,null," CBD, urban, short rural, or long rural "," kV "," name ",null," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.3 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION SUBSTATIONS, SUBTRANSMISSION SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"Substation ID","Subtransmission substation, subtransmission switching station, or zone substation","Primary type of area supplied by substation","Substation voltage",null,{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "},null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "}]
[null,null,null,null,"Primary","Secondary",null,null,null,"tx name plate total\n(ONAN)","tx name plate total\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency",null,null,null,"tx name plate\n(ONAN)","tx name plate\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency"]
[null,null," STS, SSW or ZSS ","CBD, Urban, Short rural, Long rural"," kV "," kV ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.4 - AUGEX MODEL INPUTS - ASSET STATUS - DISTRIBUTION SUBSTATIONS"]
[null,"Distribution substation \ncategory ID","Description of distribution substation category",{"$f":"CRCP_y4","v":"2018-19"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2014-15"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2018-19 to 2019-20"},"Network segment ID"]
[null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category","Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category"]
[null,null,null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%",null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%"]
[null,null,null," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"ED_AUG245_00001","ED_AUG245_00002","ED_AUG245_00003","ED_AUG245_00004","ED_AUG245_00005","ED_AUG245_00006","ED_AUG245_00007","ED_AUG245_00008"]
[null,"2.4.5 - AUGEX MODEL INPUTS - NETWORK SEGMENT DATA"]
[null,null,null,null,"HISTORICAL",null,null,null,"FORECAST"]
[null,"Network segment ID","Network segment title","AER segment group","Average unit cost of augmentation for the network segment for the period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period","Average unit cost of augmentation for the network segment for the period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period"]
[null,null,null,null,{"$f":"CONCATENATE(PRCP_y5,\" to \",CRCP_y3)","v":"2014-15 to 2017-18"},null,null,null,{"$f":"CONCATENATE(CRCP_y4,\" to \",FRCP_y5)","v":"2018-19 to 2024-25"}]
[null,null,null," ID ",{"$f":"CONCATENATE(\"$0's, real \", dms_DollarReal, \" \nper MVA\")","v":"$0's, real June 2020 \nper MVA"},null," % "," % ",{"$f":"CONCATENATE(\"$0's, real \", dms_DollarReal, \" \nper MVA\")","v":"$0's, real June 2020 \nper MVA"},null," % "," % "]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
[null,6]
[null,7]
[null,8]
[null,9]
[null,10]
[null,11]
[null,12]
[null,13]
[null,14]
[null,15]
[null,16]
[null,17]
[null,18]
[null,19]
[null,20]
[null,21]
[null,22]
[null,23]
[null,24]
[null,25]
[null,26]
[null,27]
[null,28]
[null,29]
[null,30]
[null,31]
[null,32]
[null,33]
[null,34]
[null,35]
[null,36]
[null,37]
[null,38]
[null,39]
[null,40]
[null,41]
[null,42]
[null,43]
[null,44]
[null,45]
[null,46]
[null,47]
[null,48]
[null,49]
[null,50]
[null,51]
[null,52]
[null,53]
[null,54]
[null,55]
[null,56]
[null,57]
[null,58]
[null,59]
[null,60]
[null,61]
[null,62]
[null,63]
[null,64]
[null,65]
[null,66]
[null,67]
[null,68]
[null,69]
[null,70]
[null,71]
[null,72]
[null,73]
[null,74]
[null,75]
[null,76]
[null,77]
[null,78]
[null,79]
[null,80]
[null,81]
[null,82]
[null,83]
[null,84]
[null,85]
[null,86]
[null,87]
[null,88]
[null,89]
[null,90]
[null,91]
[null,92]
[null,93]
[null,94]
[null,95]
[null,96]
[null,97]
[null,98]
[null,99]
[null,100]
[]
[]
[]
[]
[null,"2.4.6 - CAPEX AND NET CAPACITY ADDED BY SEGMENT GROUP"]
[null,"AER DNSP segment group",{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"CAPEX\n ($0's, real \", dms_DollarReal, \")\")","v":"CAPEX\n ($0's, real June 2020)"},null,null,null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)"]
[null,null,"In total for all purposes",null,null,null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"In total for all purposes",null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,"Residual"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2018-19 to 2019-20"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2020-21 to 2024-25"}]
[null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast"]
[null,null,{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2014-15 to 2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},"type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3"]
[null,"Subtransmission lines",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AA7842-AG7842-AM7842","v":0},{"$f":"AB7842-AH7842-AN7842","v":0},null,{"$f":"AD7842-AJ7842-AP7842","v":0},{"$f":"AE7842-AK7842-AQ7842","v":0}]
[null,"Subtransmission substations and subtransmission switching stations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AA7843-AG7843-AM7843","v":0},{"$f":"AB7843-AH7843-AN7843","v":0},{"$f":"AC7843-AI7843-AO7843","v":0},{"$f":"AD7843-AJ7843-AP7843","v":0},{"$f":"AE7843-AK7843-AQ7843","v":0},{"$f":"AF7843-AL7843-AR7843","v":0}]
[null,"Zone substations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AB7844-AH7844-AN7844","v":0},{"$f":"AC7844-AI7844-AO7844","v":0},0,{"$f":"AE7844-AK7844-AQ7844","v":0},{"$f":"AF7844-AL7844-AR7844","v":0}]
[null,"High voltage feeders - CBD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - urban",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - short rural",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"High voltage feeders - long rural",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - CBD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - urban ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - short rural ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[null,"Distribution substations - long rural ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0]
[]
[null,"Unmodelled augmentation"]
[]
[]
[null,"Unmodelled augmentation - see comments in guidance paper - this should cover capex allocated to the augmentation category that is not considered to be primarily related to peak demand and capacity needs."]

{"sheet":"2.5 Connections","index":11,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[195,4,195,10],[138,2,139,3],[138,4,138,10],[102,1,103,1],[102,2,103,3],[102,4,102,10],[120,4,120,10],[120,2,121,3],[120,1,121,1],[159,4,159,10],[177,4,177,10],[5,1,5,2],[9,4,9,10],[9,2,10,2],[9,1,10,1],[9,3,10,3],[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,54,10],[138,1,139,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Underground connections","0's",10695.706341995427,10588.666403584552,10588.053984967461,10766.386261840809,10990.169824479488,10668.306674987549,10617.644856648891]
[null,null,"Overhead connections","0's",479.26219857734213,474.46586305932578,474.43842129124641,482.42928382606078,492.45676577127597,478.03445127103078,475.76435393808606]
[null,null,"Distribution substations installed","MVA added",5.3572008444626178,5.3035873260926847,5.3032805815516753,5.3926025761645722,5.5046899364951027,5.3434770646074927,5.3181018787798644]
[null,null,"Distribution substations installed","0's",96.91507160445488,95.945169948227161,95.939620750050864,97.555510793208285,99.583240360901456,96.666799951784256,96.20774716976976]
[null,null,"Distribution substations installed ","total spend $0's",2008843.2911455748,1988739.2928414093,1988624.2697666374,2022118.2332821789,2064148.7541380362,2003697.1478719616,1994181.9601290766]
[null,null,"Augmentation HV ","net circuit KM added",7.4954997424990903,7.4204866666776601,7.4200574866459794,7.5450318915747223,7.7018583397306291,7.476298187180042,7.4407946276983301]
[null,null,"Augmentation HV","total spend $0's",1003747.0382117907,993701.7903604696,993644.31744999555,1010380.0513048383,1031381.1970933221,1001175.694746688,996421.29625425837]
[null,null,"Augmentation LV","net circuit KM added",3.5722014347296573,3.5364517414098819,3.5362472030098293,3.5958074410096632,3.6705477094843175,3.5630503673137204,3.5461300990893769]
[null,null,"Augmentation LV","total spend $0's",579642.65618923388,573841.73830359592,573808.54891501705,583473.08076975541,595600.79767892906,578157.75979667052,575412.19536079071]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998]
[null,null,"Volume of GSL breaches for residential customers","0's",182,182,182,182,182,182,182]
[null,null,"Volume of customer complaints relating to connection services","0's",94.4,94.4,94.4,94.4,94.4,94.4,94.4]
[null,null,"GSL payments","$0's",50806,50806,50806,50806,50806,50806,50806]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1230.2604967936186,1217.1606216352809,1217.8859252652994,1237.5894088788655,1264.1088910794047,1226.3152213321098,1221.2873775726746]
[null,null,"Overhead connections","0's",315.87411071831571,312.51066742565922,312.69689192017063,317.75583706285306,324.5648160381495,314.86114608099638,313.5702278726319]
[null,null,"Distribution substations installed","MVA added",110.90718506734805,109.79725385950246,109.79090349583946,111.64008766397772,113.9605706880066,110.6230691948231,110.09774066740526]
[null,null,"Distribution substations installed","0's",285.67919970676815,282.82019414284235,282.80383662003629,287.56703976997983,293.54423351838449,284.94736258514581,283.59420017998036]
[null,null,"Distribution substations installed ","total spend $0's",12985815.670405691,12855856.893946247,12855113.347422028,13071629.209162582,13343328.150922272,12952549.328397235,12891040.063516775]
[null,null,"Augmentation HV ","net circuit KM added",46.108446623451279,45.64700488889121,45.644364794799763,46.413142845218758,47.377858229430238,45.990328563424448,45.771928985872165]
[null,null,"Augmentation HV","total spend $0's",8029646.394382406,7949287.713241253,7948827.9488476412,8082708.318989791,8250710.5826466,8009076.4918100759,7971042.8665450821]
[null,null,"Augmentation LV","net circuit KM added",5.2369380510625447,5.1845280924751123,5.1842282339845678,5.271545055953001,5.3811161882290763,5.2235223537582343,5.1987168107010149]
[null,null,"Augmentation LV","total spend $0's",1614065.4124349696,1597912.2518288479,1597819.8330884515,1624731.5629750397,1658502.2459741,1609930.5892250233,1602285.3261543247]
[null,"SUBDIVISION","Underground connections","0's",241.37795268174813,257.58112122521317,267.88436607422176,283.33923334773453,269.83090976953622,258.09790194101362,249.45277198824368]
[null,null,"Overhead connections","0's",43.151073814499341,46.047710040301183,47.889618441913228,50.652481044331296,48.237601551996249,46.140094794441609,44.594607161526881]
[null,null,"Distribution substations installed","MVA added",26.422895152417254,28.19660571216092,29.324469940647358,31.016266283377014,29.537552036172077,28.253176092838519,27.306820554633084]
[null,null,"Distribution substations installed","0's",96.577695935348984,103.06074323686963,107.18317296634442,113.3668175605566,107.96200426821902,103.26751229046928,99.808510659939159]
[null,null,"Distribution substations installed ","total spend $0's",3708290.225155862,3957219.5530365519,4115508.3351580142,4352941.5083402079,4145413.0919014388,3965158.8567536506,3832343.698853428]
[null,null,"Augmentation HV ","net circuit KM added",9.7712302325566895,10.427151324670126,10.844237377656931,11.469866457137138,10.923035488227232,10.448071144801705,10.098107305021095]
[null,null,"Augmentation HV","total spend $0's",1587137.4855333285,1693678.517529133,1761425.6582302984,1863046.3692820463,1774224.8075798478,1697076.5165457583,1640232.0132971995]
[null,null,"Augmentation LV","net circuit KM added",14.693243521833223,15.679568488920586,16.30675122847741,17.247525337812647,16.425241920039678,15.711026146176692,15.184776759011566]
[null,null,"Augmentation LV","total spend $0's",3745962.1382257445,3997420.2983798231,4157317.110315016,4397162.3282178054,4187525.6645845268,4005440.256183119,3871275.8508456708]
[null,null,"Cost per lot","$0's",1674.3688358872546,1786.7655156601463,1858.2361362865522,1965.442067226161,1871.7387452237679,1790.3502735715892,1730.3815149741602]
[null,"EMBEDDED GENERATION","Underground connections","0's",6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641]
[null,null,"Overhead connections","0's",512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Underground connections","0's",10695.706341995427,10588.666403584552,10588.053984967461,10766.386261840809,10990.169824479488,10668.306674987549,10617.644856648891]
[null,null,"Overhead connections","0's",479.26219857734213,474.46586305932578,474.43842129124641,482.42928382606078,492.45676577127597,478.03445127103078,475.76435393808606]
[null,null,"Distribution substations installed","MVA added",5.3572008444626178,5.3035873260926847,5.3032805815516753,5.3926025761645722,5.5046899364951027,5.3434770646074927,5.3181018787798644]
[null,null,"Distribution substations installed","0's",96.91507160445488,95.945169948227161,95.939620750050864,97.555510793208285,99.583240360901456,96.666799951784256,96.20774716976976]
[null,null,"Distribution substations installed ","total spend $0's",2008843.2911455748,1988739.2928414093,1988624.2697666374,2022118.2332821789,2064148.7541380362,2003697.1478719616,1994181.9601290766]
[null,null,"Augmentation HV ","net circuit KM added",7.4954997424990903,7.4204866666776601,7.4200574866459794,7.5450318915747223,7.7018583397306291,7.476298187180042,7.4407946276983301]
[null,null,"Augmentation HV","total spend $0's",1003747.0382117907,993701.7903604696,993644.31744999555,1010380.0513048383,1031381.1970933221,1001175.694746688,996421.29625425837]
[null,null,"Augmentation LV","net circuit KM added",3.5722014347296573,3.5364517414098819,3.5362472030098293,3.5958074410096632,3.6705477094843175,3.5630503673137204,3.5461300990893769]
[null,null,"Augmentation LV","total spend $0's",579642.65618923388,573841.73830359592,573808.54891501705,583473.08076975541,595600.79767892906,578157.75979667052,575412.19536079071]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998,16.419999999999998]
[null,null,"Volume of GSL breaches for residential customers","0's",182,182,182,182,182,182,182]
[null,null,"Volume of customer complaints relating to connection services","0's",94.4,94.4,94.4,94.4,94.4,94.4,94.4]
[null,null,"GSL payments","$0's",50806,50806,50806,50806,50806,50806,50806]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1230.2604967936186,1217.1606216352809,1217.8859252652994,1237.5894088788655,1264.1088910794047,1226.3152213321098,1221.2873775726746]
[null,null,"Overhead connections","0's",315.87411071831571,312.51066742565922,312.69689192017063,317.75583706285306,324.5648160381495,314.86114608099638,313.5702278726319]
[null,null,"Distribution substations installed","MVA added",110.90718506734805,109.79725385950246,109.79090349583946,111.64008766397772,113.9605706880066,110.6230691948231,110.09774066740526]
[null,null,"Distribution substations installed","0's",285.67919970676815,282.82019414284235,282.80383662003629,287.56703976997983,293.54423351838449,284.94736258514581,283.59420017998036]
[null,null,"Distribution substations installed ","total spend $0's",12985815.670405691,12855856.893946247,12855113.347422028,13071629.209162582,13343328.150922272,12952549.328397235,12891040.063516775]
[null,null,"Augmentation HV ","net circuit KM added",46.108446623451279,45.64700488889121,45.644364794799763,46.413142845218758,47.377858229430238,45.990328563424448,45.771928985872165]
[null,null,"Augmentation HV","total spend $0's",8029646.394382406,7949287.713241253,7948827.9488476412,8082708.318989791,8250710.5826466,8009076.4918100759,7971042.8665450821]
[null,null,"Augmentation LV","net circuit KM added",5.2369380510625447,5.1845280924751123,5.1842282339845678,5.271545055953001,5.3811161882290763,5.2235223537582343,5.1987168107010149]
[null,null,"Augmentation LV","total spend $0's",1614065.4124349696,1597912.2518288479,1597819.8330884515,1624731.5629750397,1658502.2459741,1609930.5892250233,1602285.3261543247]
[null,"SUBDIVISION","Underground connections","0's",241.37795268174813,257.58112122521317,267.88436607422176,283.33923334773453,269.83090976953622,258.09790194101362,249.45277198824368]
[null,null,"Overhead connections","0's",43.151073814499341,46.047710040301183,47.889618441913228,50.652481044331296,48.237601551996249,46.140094794441609,44.594607161526881]
[null,null,"Distribution substations installed","MVA added",26.422895152417254,28.19660571216092,29.324469940647358,31.016266283377014,29.537552036172077,28.253176092838519,27.306820554633084]
[null,null,"Distribution substations installed","0's",96.577695935348984,103.06074323686963,107.18317296634442,113.3668175605566,107.96200426821902,103.26751229046928,99.808510659939159]
[null,null,"Distribution substations installed ","total spend $0's",3708290.225155862,3957219.5530365519,4115508.3351580142,4352941.5083402079,4145413.0919014388,3965158.8567536506,3832343.698853428]
[null,null,"Augmentation HV ","net circuit KM added",9.7712302325566895,10.427151324670126,10.844237377656931,11.469866457137138,10.923035488227232,10.448071144801705,10.098107305021095]
[null,null,"Augmentation HV","total spend $0's",1587137.4855333285,1693678.517529133,1761425.6582302984,1863046.3692820463,1774224.8075798478,1697076.5165457583,1640232.0132971995]
[null,null,"Augmentation LV","net circuit KM added",14.693243521833223,15.679568488920586,16.30675122847741,17.247525337812647,16.425241920039678,15.711026146176692,15.184776759011566]
[null,null,"Augmentation LV","total spend $0's",3745962.1382257445,3997420.2983798231,4157317.110315016,4397162.3282178054,4187525.6645845268,4005440.256183119,3871275.8508456708]
[null,null,"Cost per lot","$0's",1674.3688358872546,1786.7655156601463,1858.2361362865522,1965.442067226161,1871.7387452237679,1790.3502735715892,1730.3815149741602]
[null,"EMBEDDED GENERATION","Underground connections","0's",6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641,6867.095389028641]
[null,null,"Overhead connections","0's",512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903,512.90461097135903]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,10773519.539999999,9537901.6400000006,11536284.189999999,11770278.310000001,12014626.529999999,11939231.949999999,11430706.130000001]
[null,null,"Complex connection LV",null,8494161.2400000002,7519963.5700000003,9095547.4399999995,9280035.3100000005,9472686.6699999999,9413243.3599999994,9012306.5800000001]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1726187.18,1528210.3,1848401.14,1885892.85,1925043.54,1912963.45,1831484.9]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,25286425.690000001,22386318.629999999,27076703.390000001,27625908.760000002,28199416.149999999,28022458.260000002,26828902.129999999]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,15258676.52,13508654.75,16338990.07,16670398.99,17016472.57,16909690.25,16189458.49]
[null,null,"Complex connection HV (customer connected at HV)",null,3230843.88,2860297.51,3459587.46,3529759.38,3603036.35,3580426.46,3427925.92]
[null,null,"Complex connection sub-transmission",null,5188031.05,4639444.75,5611826.4699999997,5630814.3499999996,5630672.9900000002,5764150.7699999996,5544971.25]
[null,"SUBDIVISION","Complex connection LV",null,965347.54,921220.44,1158871.1000000001,1229876.3600000001,1171212.05,1146841.33,1066279.75]
[null,null,"Complex connection HV (no upstream asset works)",null,{"$f":"2550224.64+26893483.78","v":29443708.420000002},{"$f":"2433651.06+26301695.63","v":28735346.689999998},{"$f":"3061469.05+27452246.32","v":30513715.370000001},{"$f":"3249048.5+27452246.32","v":30701294.82},{"$f":"3094071+27452246.32","v":30546317.32},{"$f":"3029689.19+27452246.32","v":30481935.510000002},{"$f":"2816864.16+27452246.32","v":30269110.48}]
[null,null,"Complex connection HV (with upstream asset works)",null,1222121.71,1166257.17,1467120.86,1557012.91,1482744.41,1451891.28,1349901.02]
[null,"EMBEDDED GENERATION","Simple connection LV",null,1165089.56,1041892.12,1260262.3899999999,1264526.55,1264494.81,1294470.26,1245248.55]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,9598767.5199999996,8847192.3300000001,8742801.8599999994,9066542.9499999993,9276432.4499999993,9239426.6300000008,9074720.7300000004]
[null,null,"Complex connection LV",null,5083928.4400000004,4643975.74,4883932.83,5114191.79,5217029.6399999997,5177228.62,5084680.46]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1111831.49,1016126.77,1065003.08,1114642.55,1137234.3,1128776.3999999999,1108601.3400000001]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,14203115.74,12953003.77,13771430.76,14444192.869999999,14727317.380000001,14605994.26,14344775.76]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,9859488.6899999995,9024447.6600000001,9361666.3200000003,9782701.5399999991,9985754.3800000008,9917334.0199999996,9740157.0299999993]
[null,null,"Complex connection HV (customer connected at HV)",null,975196.02,867145.35,1079945.28,1157322.03,1172343.74,1153298.45,1132545.02]
[null,null,"Complex connection sub-transmission",null,2016989.72,1833690.8,2592147.79,2687786.06,2680386.9500000002,2733104.4,2696958.65]
[null,"SUBDIVISION","Complex connection LV",null,748072.65,745765.48,771603.46,828971.59,792262.35,778744.8,742785.89]
[null,null,"Complex connection HV (no upstream asset works)",null,1309135.23,1305097.67,1419204.59,1524721.38,1457202.35,1432339.6,1366200.65]
[null,null,"Complex connection HV (with upstream asset works)",null,1227077.04,1223292.55,1236074.49,1327975.69,1269169.1299999999,1247514.6000000001,1189910.02]
[null,"EMBEDDED GENERATION","Simple connection LV",null,1292269.54,1207244.3400000001,1164089.6399999999,1182422.1599999999,1186634.44,1219411.56,1203413.6599999999]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,1820582.09,1521386.68,2317479.84,2290493.9300000002,2338075.71,2325357.9700000002,2148234.98]
[null,null,"Complex connection LV",null,3359175.88,2808543.9,4260965.79,4208148.34,4296587.8099999996,4274442.41,3948872.72]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,621723.91,520802.82,778106.45,766214.32,783034.69,779859.6,720471.2]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,10721266,8962438.2100000009,13614432.07,13448871.310000001,13730494.68,13658499.699999999,12618162.93]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,5471407.1399999997,4574409.16,6941635.3099999996,6855887.6900000004,6999877.4000000004,6963684.4100000001,6433282.8899999997]
[null,null,"Complex connection HV (customer connected at HV)",null,2020040.32,1688874.91,2562786.9700000002,2531116.7799999998,2584280.31,2570923.21,2375104.29]
[null,null,"Complex connection sub-transmission",null,2894434.3,2444567.37,3139144.59,3043860.14,3046119,3123787.79,2899653.92]
[null,"SUBDIVISION","Complex connection LV",null,249880.25,221992.85,361992.15,379150.39,358986.4,349348.13,313386.11]
[null,null,"Complex connection HV (no upstream asset works)",null,{"$f":"1176767.11+26893483.78","v":28070250.890000001},{"$f":"1045436.31+26301695.63","v":27347131.939999998},{"$f":"1706362.49+27452246.32","v":29158608.809999999},{"$f":"1787243.19+27452246.32","v":29239489.510000002},{"$f":"1692193.96+27452246.32","v":29144440.280000001},{"$f":"1646760.98+27452246.32","v":29099007.300000001},{"$f":"1477242.83+27452246.32","v":28929489.149999999}]
[null,null,"Complex connection HV (with upstream asset works)",null,99479.46,88377.25,144257.81,151095.56,143059.99,139219.03,124887.78]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,10940.75711752867,10831.264772602328,10830.638322779418,11013.056394583284,11241.967092711919,10912.729693041767,10860.907154926699]
[null,null,"Complex connection LV",null,234.21142304409929,231.86749404154898,231.85408347928959,235.75915108358666,240.65949753884516,233.61143321681192,232.50205566027688]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1129.9416302973946,1118.6334587145577,1118.5687601085476,1137.4085690208149,1161.0500523896012,1127.0470085287575,1121.6948704111794]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,351.31713456614898,347.80124106232353,347.78112521893445,353.63872662538006,360.98924630826781,350.41714982521796,348.75308349041541]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,51.394356153877588,50.880014366484104,50.877071609875458,51.733982996398332,52.809294130781076,51.262696944128017,51.019259862756691]
[null,null,"Complex connection HV (customer connected at HV)",null,12.481486494513129,12.356574917574711,12.355860248112613,12.563967299125311,12.825114288903977,12.44951211500252,12.390391680955197]
[null,null,"Complex connection sub-transmission",null,1,0,1,0,1,0,1]
[null,"SUBDIVISION","Complex connection LV",null,166.10637552790286,177.25672943935282,184.34699861692695,194.98240238328813,185.68652989740679,177.61235666499886,171.66313393579759]
[null,null,"Complex connection HV (no upstream asset works)",null,90.58697419499839,96.667877584958532,100.53459268835688,106.33466534345439,101.26511302601745,96.861820738616842,93.617381239303811]
[null,null,"Complex connection HV (with upstream asset works)",null,27.835676773346201,29.704224241203026,30.892393210851147,32.67464666532333,31.116868398108238,29.763819331839517,28.766863974669178]
[null,"EMBEDDED GENERATION","Simple connection LV",null,7380,7380,7380,7380,7380,7380,7380]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV",null,10940.75711752867,10831.264772602328,10830.638322779418,11013.056394583284,11241.967092711919,10912.729693041767,10860.907154926699]
[null,null,"Complex connection LV",null,234.21142304409929,231.86749404154898,231.85408347928959,235.75915108358666,240.65949753884516,233.61143321681192,232.50205566027688]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1129.9416302973946,1118.6334587145577,1118.5687601085476,1137.4085690208149,1161.0500523896012,1127.0470085287575,1121.6948704111794]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,351.31713456614898,347.80124106232353,347.78112521893445,353.63872662538006,360.98924630826781,350.41714982521796,348.75308349041541]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,51.394356153877588,50.880014366484104,50.877071609875458,51.733982996398332,52.809294130781076,51.262696944128017,51.019259862756691]
[null,null,"Complex connection HV (customer connected at HV)",null,12.481486494513129,12.356574917574711,12.355860248112613,12.563967299125311,12.825114288903977,12.44951211500252,12.390391680955197]
[null,null,"Complex connection sub-transmission",null,1,0,1,0,1,0,1]
[null,"SUBDIVISION","Complex connection LV",null,166.10637552790286,177.25672943935282,184.34699861692695,194.98240238328813,185.68652989740679,177.61235666499886,171.66313393579759]
[null,null,"Complex connection HV (no upstream asset works)",null,90.58697419499839,96.667877584958532,100.53459268835688,106.33466534345439,101.26511302601745,96.861820738616842,93.617381239303811]
[null,null,"Complex connection HV (with upstream asset works)",null,27.835676773346201,29.704224241203026,30.892393210851147,32.67464666532333,31.116868398108238,29.763819331839517,28.766863974669178]
[null,"EMBEDDED GENERATION","Simple connection LV",null,7380,7380,7380,7380,7380,7380,7380]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"RESIDENTIAL","Simple connection LV"]
[null,null,"Complex connection LV"]
[null,null,"Complex connection HV"]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV"]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)"]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)"]
[null,null,"Complex connection HV (customer connected at HV)"]
[null,null,"Complex connection sub-transmission"]
[null,"SUBDIVISION","Complex connection LV"]
[null,null,"Complex connection HV (no upstream asset works)"]
[null,null,"Complex connection HV (with upstream asset works)"]
[null,"EMBEDDED GENERATION","Simple connection LV"]
[null,null,"Complex connection HV (small capacity)"]
[null,null,"Complex connection HV (large capacity)"]

{"sheet":"2.6 Non-network","index":12,"n_rows":118,"n_cols":11,"rows_kept":118,"cut":false,"hidden":false,"merged":[[8,4,8,10],[62,4,62,10],[55,1,56,3],[12,1,16,1],[59,1,59,3],[58,1,58,3],[57,1,57,3],[69,1,73,1],[74,1,78,1],[79,1,83,1],[84,1,88,1],[55,4,55,10],[5,1,5,2],[19,1,29,1],[32,1,36,1],[39,1,49,1],[64,1,68,1],[106,1,106,3],[100,1,100,3],[101,1,101,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[93,4,93,10],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[107,1,107,3],[108,1,108,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[119,1,119,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[117,1,117,3],[118,1,118,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2020)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,23581220,23076665,27528350.95485368,28084180.016631853,28857692.525003057,29206680.318228927,29547009.155615382]
[null,"MOTOR VEHICLES","Car",null,679364.52745174605,687849.33024901606,696939.46645349613,706285.33412741031,715222.49074897775,723611.56042825233,731418.09206849441]
[null,null,"Light commercial vehicle",null,2223958.5491671213,2251734.2851034165,2281491.6323126918,2312086.1386092585,2341342.6939203423,2368805.0392134683,2394360.3958432614]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,6214801.9524743287,6292420.6194197843,6375576.8543261942,6461072.5114004212,6542829.2946543591,6619572.1985233016,6690986.0656290948]
[null,null,"Heavy commercial vehicle",null,1885805.3225828579,1909357.753758762,1934590.4919202775,1960533.0990059474,1985341.1907515172,2008627.882377933,2030297.5432495417]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,4621046,4681278,4744086.9026612118,4809519.345773601,4873075.9890537392,4933641.0744157312,4990812.078097851]
[null,"OTHER","Other expenditure",null,3191644.8246596879,3231506.3067387459,3274211.6364993444,3318118.3890424725,3360105.0229124972,3399516.7521736603,3436191.7260666564]
[null,"OTHER - DNSP nominated","TEC Vehicles",null,269735.02550481167,273103.83327508124,276712.98274032434,280423.66787845426,283972.07830003055,287302.87617431534,290402.38303108804]
[null,null,"Cranes",null,1587169.9141178683,1606992.5913152834,1628229.4827277644,1650063.8284935094,1670943.3203337993,1690542.3403949828,1708780.4020722336]
[null,null,"Trailers",null,535978.33546910807,542672.34184757248,549843.9203966317,557217.25591382186,564268.14264148474,570886.62126546807,577045.51191290631]
[null,null,"Other Commercial Vehicles",null,798761.54956790025,808737.54030080896,819425.25063462439,830413.63675668684,840921.48163718265,850784.9143388943,859963.42905042891]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,68587359,73536953,72472364,72902553,48456474,45487637,45237620]
[null,"MOTOR VEHICLES","Car",null,1025821," -   ",981915,787623,811613,1275946," -   "]
[null,null,"Light commercial vehicle",null,6807329,7567966,5656683,7152473,11384818,8403642,4695337]
[null,null,"Elevated work platform (LCV)  ",null," -   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,null,"Elevated work platform (HCV)",null,10136483,6477666,5277792,4198885,6025949,13364431,10264096]
[null,null,"Heavy commercial vehicle",null,128764,2045916,997924,1825371,3074123,2804881,1535442]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,11224153,15424027,13791882,17896651,11117224,9451895,9239217]
[null,"OTHER","Other expenditure",null,8343543,9425106,14504851.202580016,15442256.921724116,10602292.000206847,11423879.867858218,16298900.850528751]
[null,"OTHER - DNSP nominated","TEC Vehicles",null,1734023,2616720,1857100,2426732,2268069,1913919,2536817]
[null,null,"Cranes",null,1047281,1924059,2401422,6109404,1823350,956959,2881735]
[null,null,"Trailers",null,351955," -   "," -   ",74505,244596,181492,445056]
[null,null,"Other Commercial Vehicles",null,60090," -   "," -   "," -   "," -   "," -   "," -   "]
[null,null,"Non-Network Telecommunications",null," -   "," -   ",4863466,2347528,2585383,4970317,6514479]
[null,null,"Non-Network Other Plant and Tools",null,5150193,4884326,5382864,4484089,3680894,3401193,3920814]
[null,null,"Other Strategic Non-Network",null," -   "," -   ",0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Employee numbers",null,null,1734,1734,1734,1734,1734,1734,1734]
[null,"User numbers",null,null,2462.6595115683558,2462.6595115683558,2436.0744862545557,2427.2128111499555,2444.9361613591559,2462.6595115683558,2480.3828617775562]
[null,"Number of devices",null,null,5702.8357234513915,5513.9081469027833,5324.9805703541751,5324.9805703541742,5324.9805703541742,5324.9805703541742,5324.9805703541742]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"CAR","Average kilometres travelled ","0's",33320,33320,33320,33320,33320,33320,33320]
[null,null,"Number purchased","0's",29,0,24,32,20,44,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",86,86,86,86,86,86,86]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.88629999999999998,0.88629999999999998,0.88629999999999998,0.88629999999999998,0.88629999999999998,0.88629999999999998,0.88629999999999998]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",21424.042338709678,21424.042338709678,21424.042338709678,21424.042338709678,21424.042338709678,21424.042338709678,21424.042338709678]
[null,null,"Number purchased","0's",119,82,80,87,126,98,58]
[null,null,"Number leased","0's",25,25,25,25,25,25,25]
[null,null,"Number in fleet","0's",496,496,496,496,496,496,496]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.93920000000000003,0.93920000000000003,0.93920000000000003,0.93920000000000003,0.93920000000000003,0.93920000000000003,0.93920000000000003]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",16610.668965517241,16610.668965517241,16610.668965517241,16610.668965517241,16610.668965517241,16610.668965517241,16610.668965517241]
[null,null,"Number purchased","0's",25,13,11,9,12,28,16]
[null,null,"Number leased","0's",3,3,3,3,3,3,3]
[null,null,"Number in fleet","0's",158,158,158,158,158,158,158]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.86860000000000004,0.86860000000000004,0.86860000000000004,0.86860000000000004,0.86860000000000004,0.86860000000000004,0.86860000000000004]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",3867.7590361445782,3867.7590361445782,3867.7590361445782,3867.7590361445782,3867.7590361445782,3867.7590361445782,3867.7590361445782]
[null,null,"Number purchased","0's",0,6,4,7,11,9,5]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",83,83,83,83,83,83,83]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.92510000000000003,0.92510000000000003,0.92510000000000003,0.92510000000000003,0.92510000000000003,0.92510000000000003,0.92510000000000003]
[]
[]
[]
[null,"2.6.4 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX BY PURPOSE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2020)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"ICT CAPABILITY GROWTH"]
[null,"Capability Growth",null,null,431842.50119315041," -   ",0,2618903.6973897889,1355945.8030407787,2109756.1476106858,1866794.6231082017]
[]
[]
[]
[]
[]
[null,"ICT ASSET EXTENSIONS"]
[null,"Asset Extension",null,null,11762824.689090379,14354732.376095468,17836520.067658566,18043480.330337021,3295703.7592701828,15285678.387383588,17081769.21820315]
[]
[]
[]
[]
[]
[null,"ICT ASSET REMEDIATION"]
[null,"Asset Remediation",null,null,2623610.7611291176,2977067.4382245457,842035.311129348,814343.72144026612,526641.88979744166,532681.68504304695,537207.66394207429]
[]
[]
[]
[]
[]
[null,"ICT ASSET REPLACEMENT"]
[null,"Asset Replacement",null,null,53769080.862451158,56205152.956966378,53793809.057137698,51425825.273747556,43278182.806526922,27559521.240151916,25751848.266997378]

{"sheet":"2.10 Overheads","index":13,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[23,3,23,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE ($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE ($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",96385185.087744132,97987310.311315283,96086622.673584446,97822334.362599984,99687398.519970909,101117418.72309323,102548354.1634288]
[null,"Alternative Control Services","Total  ",6203562.219158045,6127794.2144831363,6056505.556468172,6047590.4495086716,6050248.1503610089,6054487.4121109219,6016311.5449013608]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",14391040.05051885,14153119.163660742,12505684.283527927,12744409.747919237,12424946.776067952,12415356.601362135,12332388.022562472]
[null,"Alternative Control Services","Total  ",1225735.6525921263,1543148.1361309439,929079.20627345517,541549.82868326642,576121.75822064281,138668.71711167321,131922.1599267642]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total  ",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",49304845.989438072,50109044.763587043,50756557.612134673,51449272.623487882,52122581.996750355,52764696.519657232,53371406.172117941]
[null,"Alternative Control Services","Total  ",9651583.8997327592,9696397.4612076301,10339077.669873884,10502691.985571951,10690886.970359815,10821969.95288053,10947153.455783095]
[null,"CAPEX"]
[null,"Standard Control Services","Total",-10552454.993224638,-10648557.627008881,-7498424.1512738997,-7578441.3625455964,-7670285.8997864816,-7753980.2099380232,-7828688.8329113321]
[null,"Alternative Control Services","Total",0,0,0,0,0,0,0]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,0,0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",418981.69900704036,420927.08562133671,448826.26243444427,455928.86908276327,464098.53898256144,469788.93874471448,475223.23815905437]

{"sheet":"2.11 Labour","index":14,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[8,2,8,8],[9,2,9,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"($0's, real \", dms_DollarReal,\")\")","v":"($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"In-house labour expenditure",100231893.75191158,100833285.11442304,109115653.1048021,108890593.05743827,118032733.06787099,121001199.0381555,125384321.82894331]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",12027660.359907806,13004993.656395614,12657663.437336206,14562628.889572442,7517422.0558189154,6224647.3720980287,3463566.1266315579]
[null,"Controllable non-labour expenditure",155072004.37000918,157093267.85411608,167252608.81376421,169403415.43622783,172088148.60643166,174233559.83369026,176310282.53930807]
[null,"Uncontrollable non-labour expenditure",8860724.9336144384,8860724.9336144384,8860724.9336144384,8860724.9336144384,8860724.9336144384,8860724.9336144384,8860724.9336144384]
[null,"Total",{"$f":"SUM(C13:C17)","v":276192283.415443},{"$f":"SUM(D13:D17)","v":279792271.55854917},297886650.28951699,301717362.31685299,306499028.66373599,310320131.17755824,314018895.42849737]
[null,"CAPEX"]
[null,"In-house labour expenditure",134334530.95640656,135140538.14214501,128698765.97316718,131539784.63038863,125378981.30328493,125039361.8482089,123141248.72237337]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",15497675.564772069,14153055.818371952,6101143.7006141543,6235826.1348454952,5943764.6987807751,5927664.5669475198,5837681.8786662221]
[null,"Controllable non-labour expenditure",279437796.07561421,278433281.02251267,269385770.99401861,279595077.50382602,250931250.33598,249533467.29599905,240564714.95420235]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":429270002.59679282},{"$f":"SUM(D20:D24)","v":427726874.9830296},{"$f":"SUM(E20:E24)","v":404185680.66779995},{"$f":"SUM(F20:F24)","v":417370688.26906013},{"$f":"SUM(G20:G24)","v":382253996.33804572},{"$f":"SUM(H20:H24)","v":380500493.71115547},{"$f":"SUM(I20:I24)","v":369543645.55524194}]

{"sheet":"2.14 Forecast price changes","index":15,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,4,11,8],[12,2,12,8],[11,1,13,1],[11,2,11,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet. It has been grouped for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"SA Power Networks must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"OPEX"]
[null,"CPI",2.0000000000000018E-2,2.2499999999999964E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]
[null,"Labour EGWWS (real)",null,null,8.7167712128783E-3,7.3747300076547825E-3,5.9366534882403857E-3,5.876070337363995E-3,5.8025976193435752E-3]
[]
[null,"CAPEX"]
[null,"Labour EGWWS (real)",7.4000000000000003E-3,7.7000000000000002E-3,7.7999999999999996E-3,1.0699999999999999E-2,1.21E-2,1.09E-2,9.5999999999999992E-3]
[null,"Contracted construction and labour services (real)",1.5E-3,2.0999999999999999E-3,6.8999999999999999E-3,1.38E-2,1.6500000000000001E-2,1.29E-2,8.8999999999999999E-3]

{"sheet":"2.16 Opex Summary","index":16,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[[57,2,57,11],[43,2,43,11],[56,2,56,11],[5,1,5,6],[15,2,15,11],[14,2,14,11],[28,2,28,11],[42,2,42,11],[7,9,7,11],[9,1,9,7],[9,9,9,10],[8,11,9,11],[8,9,8,10],[8,1,8,7],[10,1,10,7],[10,9,10,10],[29,2,29,11]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nSA Power Networks's total forecast opex must reconcile to Table 2.16.1 (and if SA Power Networks owns any dual function assets Table 2.16.3). If SA Power Networks did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if SA Power Networks owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has SA Power Networks used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If SA Power Networks does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2018-19"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Base year total opex, excluding category specific",null,null,null,276192283,276192283,279792271.55854923,279792271.55854923,279792271.55854923,279792271.55854923,279792271.55854923]
[null,"Increment from base year to final year",null,null,null,null,3599989]
[null,"Price growth",null,null,null,null,null,1309774,3131805,5234275,7166079,8907189]
[null,"Output growth",null,null,null,null,null,2429262,4509998,6207063,7897410,9577186]
[null,"Productivity growth",null,null,null,null,null,0,0,0,0,0]
[null,"Step changes",null,null,null,null,null,14345675,14272908,15264333,15473311,15762041]
[null,"Category specific",null,null,null,0,0," -   "," -   "," -   "," -   "," -   "]
[null,"Total opex",{"$f":"SUM(C18:C24)","v":0},{"$f":"SUM(D18:D24)","v":0},{"$f":"SUM(E18:E24)","v":0},276192283,279792272,297876982.55854923,301706982.55854923,306497942.55854923,310329071.55854923,314038687.55854923]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C32:C38)","v":0},{"$f":"SUM(D32:D38)","v":0},0,0,0,{"$f":"SUM(H32:H38)","v":0},0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth"]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C46:C52)","v":0},{"$f":"SUM(D46:D52)","v":0},0,0,0,{"$f":"SUM(H46:H52)","v":0},0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C60:C66)","v":0},{"$f":"SUM(D60:D66)","v":0},0,0,0,{"$f":"SUM(H60:H66)","v":0},0,0,0,0]

{"sheet":"2.17 Step Changes","index":17,"n_rows":93,"n_cols":11,"rows_kept":93,"cut":false,"hidden":false,"merged":[[8,1,8,2],[5,1,5,2],[13,4,13,10],[30,4,30,10],[9,1,9,2],[12,4,12,10],[29,4,29,10],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[46,4,46,10],[63,4,63,10],[45,4,45,10],[62,4,62,10],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,2,38,3],[39,2,39,3],[40,2,40,3],[92,1,92,2],[58,1,58,3],[59,1,59,3],[79,3,79,10],[80,3,80,10],[64,2,64,3],[65,2,65,3],[66,2,66,3],[67,2,67,3],[73,2,73,3],[74,2,74,3],[75,1,75,3],[68,2,68,3],[69,2,69,3],[71,2,71,3],[72,2,72,3],[23,2,23,3],[24,2,24,3],[25,1,25,3],[26,1,26,3],[31,2,31,3],[32,2,32,3],[41,2,41,3],[47,2,47,3],[48,2,48,3],[70,2,70,3],[57,2,57,3],[42,1,42,3],[50,2,50,3],[51,2,51,3],[52,2,52,3],[53,2,53,3],[49,2,49,3],[54,2,54,3],[55,2,55,3],[56,2,56,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Complete the Tables below in accordance with the regulatory information notice. If \",dms_TradingName,\" does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\"&\"\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively.\")","v":"Complete the Tables below in accordance with the regulatory information notice. If SA Power Networks does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively."}]
[null," The total category specific forecast in Table 2.17.5 must reconcile (in each year) to the total category specific forecasts for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary'."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"LV Management - Future Networks","capex/opex trade-off and positive npv",null,null,null,0,404658,936116,1094892,1325337]
[null,"Cloud Transition - Cloud Hosting","capex/opex trade-off",null,null,null,954852,1187882,1647849,1698050,1756336]
[null,"Cloud Transition - Work Scheduling","capex/opex trade-off",null,null,null,754988,754988,754988,754988,754988]
[null,"Critical Infrastructure Compliance","change in regualtory obligations",null,null,null,2414416,2414416,2414416,2414416,2414416]
[null,"Cable/Conductor Repair","capex/opex trade-off",null,null,null,14199116,13488661,13488661,13488661,13488661]
[null,"GSL reliability duration payments","change in regualtory obligations",null,null,null,-3977697,-3977697,-3977697,-3977696,-3977697]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E16:E25)","v":0},0,14345675,14272908,15264333,15473311,15762041]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$23=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E33:E42)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E49:E58)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$51=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E66:E75)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,"Category","Description",{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D90:D92)","v":0},0,0,0,0,0,0,0]

{"sheet":"3.1 Revenue","index":18,"n_rows":53,"n_cols":17,"rows_kept":53,"cut":false,"hidden":false,"merged":[[45,2,45,8],[45,10,45,16],[8,2,8,8],[8,10,8,16],[43,2,43,8],[43,10,43,16],[44,2,44,8],[44,10,44,16],[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[30,2,30,8],[30,10,30,16],[10,2,10,8],[10,10,10,16],[31,2,31,8],[31,10,31,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0101","Revenue from Fixed Customer Charges ",140426604,154854079,152545550,160308246,167382741,174161404,180622959,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",463017039,411921667,246359023,221047908,198238214,176247412,155734716,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",37457394,86093315,153189726,165544895,176638273,187118315,197126308,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges"," -   ",8590716,36180576,41300822,45813350,50001380,53588190,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",18293802,31012942,68366031,70372130,71814978,72982342,73749645,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",21852870,22414653,21332232,19902539,18613656,17414702,16148643,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",5388984,5801750,6475557,6403511,6336529,6238642,6131577,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",114970433,113173019,8738786,8741344,8743896,8746464,8749025,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",20923511,24503019,89745515,89311603,89351360,90022337,91081934,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,25980000,25630000,17155953.210000001,17141056.699999999,17113422.620000001,17046696.870000001,16936668.600000001]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,22170000,24300000,16109627.32,15835662.76,15697420.23,15607052.25,15690355.08]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,47860000,48890000,41482565.810000002,41093642.630000003,40743006.109999999,40426860.289999999,40141645.530000001]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":822330637},{"$f":"SUM(D13:D25)","v":858365160},782932996,782932998,782932997,782932998,782932997,null,{"$f":"SUM(K13:K25)","v":96010000},{"$f":"SUM(L13:L25)","v":98820000},74748146.340000004,74070362.090000004,73553848.960000008,73080609.409999996,72768669.210000008]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0201","Revenue from residential Customers ",430232942,455858532,422799444.58999997,422799410,422799059.10000002,422799424.12,422799454.48000002,null,22643548.02,22338496.370000001,14952719.42,14939735.970000001,14915650.77,14857494.199999999,14761596.18]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",118156520,115065029,117742655.23,118649474.76000001,119713184.66,120540425.44,120827680.98999999,null,3336451.98,3291503.63,2203233.7999999998,2201320.73,2197771.85,2189202.67,2175072.42]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",218083498,233108101,194472818.93000001,193638086.16999999,192641098.34999999,191912003.37,191731790.30000001,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",50468693,48531748,41442522.200000003,41442515.740000002,41443125.859999999,41442502.75,41442494.32,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",5388984,5801750,6475556.5199999996,6403510.7999999998,6336529.5,6238641.79,6131577.3899999997,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,70030000,73190000,57592193.130000003,56929305.390000001,56440426.329999998,56033912.539999999,55832000.609999999]
["DREV02","Total revenue by customer class",{"$f":"SUM(C34:C39)","v":822330637},{"$f":"SUM(D34:D39)","v":858365160},782932997.47000003,782932997.46999991,782932997.47000003,782932997.46999991,782932997.48000002,null,{"$f":"SUM(K34:K39)","v":96010000},{"$f":"SUM(L34:L39)","v":98820000},74748146.349999994,74070362.090000004,73553848.950000003,73080609.409999996,72768669.210000008]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DREV0301","EBSS",5454908," -   ",8969273,-24003441,-5125480,-9941230," -   ",null,0,0,0,0,0,0,0]
["DREV0302","STPIS",23436625,35467000," -   "," -   "," -   "," -   "," -   ",null,0,0,0,0,0,0,0]
["DREV0303","F-Factor"," -   "," -   "," -   "," -   "," -   "," -   "," -   ",null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up"," -   "," -   "," -   "," -   "," -   "," -   "," -   ",null,0,0,0,0,0,0,0]
["DREV0305","Other",-152389,-132657,13413304,13433134,13492586,13526424,13562892,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C48:C52)","v":28739144},{"$f":"SUM(D48:D52)","v":35334343},22382577,-10570307,8367106,3585194,13562892,null,{"$f":"SUM(K48:K52)","v":0},{"$f":"SUM(L48:L52)","v":0},0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":19,"n_rows":88,"n_cols":17,"rows_kept":88,"cut":false,"hidden":false,"merged":[[12,2,12,8],[12,10,12,16],[14,10,14,16],[14,2,14,8],[13,2,13,8],[13,10,13,16],[85,2,85,8],[72,2,72,8],[72,10,72,16],[70,2,70,8],[70,10,70,16],[83,2,83,8],[71,2,71,8],[71,10,71,16],[84,2,84,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Forecasts for opex in table 3.2.1 are to be for the opex categories that \",dms_TradingName,\" has reported in its response to its annual reporting RIN.\")","v":"Forecasts for opex in table 3.2.1 are to be for the opex categories that SA Power Networks has reported in its response to its annual reporting RIN."}]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0101","Distribution licence fee",2465997.8363291626,2507913.3444040967,2541475.2240841738,2576523.1399188479,2610655.8093252853,2643192.3759947768,2673918.0351405307,null,0,0,0,0,0,0,0]
["DOPEX0102","Network operating costs",38231746.59806899,38882977.728308149,39403324.981546551,40351369.829046384,41412024.755514137,42075251.296553321,42782070.977054194,null,0,0,0,0,0,0,0]
["DOPEX0103","Inspections",12790556.105678828,13007112.660774956,13181178.942243649,13362952.443630433,13539979.08507047,13708727.654158471,13868084.081276311,null,0,0,0,0,0,0,0]
["DOPEX0104","Maintenance & repair",16404862.424261922,16696833.017274622,31119392.542486522,30642274.951067001,30869518.640640553,31086136.021718763,31290696.997179519,null,2277797.2225633929,2170332.4107850273,2088505.6874124296,2006678.9640398324,1924852.2406672351,1843025.5172946379,1761198.7939220406]
["DOPEX0105","Substation property maintenance",8336479.155766774,8431658.7514561601,8544494.5147616398,8662326.3636678681,8777081.1343434565,8886469.7731946688,8989770.1018956639,null,0,0,0,0,0,0,0]
["DOPEX0106","Vegetation management",40917714.827328369,41394509.337935358,41948466.891897686,42526952.301902287,43090331.058838226,43627365.249365501,44134509.400602259,null,0,0,0,0,0,0,0]
["DOPEX0107","Emergency response",38017952.054003097,38763982.971523754,39282737.790271282,39824461.775924191,40352039.101750076,40854945.998091713,41329862.298757538,null,0,0,0,0,0,0,0]
["DOPEX0108","Guaranteed service level payments",9578781.9820204396,9705719.7337416578,5857908.7816613363,5993545.5448302571,6125640.2696191045,6251558.0162975965,6370467.482196236,null,0,0,0,0,0,0,0]
["DOPEX0109","Network insurance",2015642.1956162648,2058864.6828990041,2086417.2173273559,2115189.7091210764,2143210.8318328252,2169921.6383158625,2195145.7851609429,null,0,0,0,0,0,0,0]
["DOPEX0110","Call centre",3812749.1451689107,3851245.8209833102,3902784.7025601589,3956605.5970075848,4009021.004702535,4058985.3771536876,4106168.8520716215,null,0,0,0,0,0,0,0]
["DOPEX0111","Customer billing (previously full retail contestability)",16206106.797525257,16446432.559024379,16666525.167863553,16896362.927368078,17120198.669821061,17333567.465288412,17535060.663647819,null,2408364.150179618,2408364.150179618,2408364.150179618,2408364.150179618,2408364.150179618,2408364.150179618,2408364.150179618]
["DOPEX0112","Meter reading",0,0,0,0,0,0,0,null,3442227.6303261835,3264022.167508434,3085816.7046906846,2907611.2418729351,2729405.7790551856,2551200.3162374366,2372994.8534196876]
["DOPEX0113","Other customer services",9906582.1639630999,10178033.201105919,10314239.632016918,10456476.943282407,10594999.848484155,10727045.182726264,10851741.189312428,null,881720.46747721802,905880.55936414527,918003.40818814433,930663.02646072302,942992.049600014,954744.54626426846,965842.92705796391]
["DOPEX0114","Corporate costs and other operating",77507112.129711896,77866987.749117821,83028035.667690158,84341941.576251686,85853242.720160946,86905905.529714048,87911192.526859447,null,9651583.8997327592,9696397.4612076301,10339077.669873884,10502691.985571951,10690886.970359815,10821969.95288053,10947153.455783095]
["DOPEX0115","Public lighting",0,0,0,0,0,0,0,null,9478886.2465380132,8209409.3126696935,7173627.9000987131,7243198.7597992383,7495325.8130611442,7753078.4126713183,7205578.4437554665]
["DOPEX0116","Fee-based and quoted services",0,0,0,0,0,0,0,null,42270436.263999999,41794325.412,41365162.272,40977339.458999999,40627695.486000001,40312445.236000001,40028037.188999996]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C17:C65)","v":276192283.415443},{"$f":"SUM(D17:D65)","v":279792271.55854923},297876982.05641103,301706983.10301805,306497942.93010283,310329071.57857311,314038688.39115453,null,{"$f":"SUM(K17:K65)","v":70411015.880817175},{"$f":"SUM(L17:L65)","v":68448731.47371456},67378557.792443469,66976547.5869243,66819522.488923013,66644828.131527811,65689169.813117862]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0201","Opex for network services",273835024.63878214,277370421.34872323,295422721.69751561,299218877.55465162,303976876.0305205,307776584.65764463,311456530.21215999,null,50820147.929920413,50583058.485456869,50869618.118457265,50605393.768653616,50365722.625033394,50109966.485167079,50034724.215488479]
["DOPEX0202","Opex for metering",0,0,0,0,0,0,0,null,8128389.003069194,7842718.7284730803,7582686.5422827322,7322654.3560923859,7062622.1699020388,6802589.9837116925,6542557.7975213462]
["DOPEX0203","Opex for connection services",2357258.7766608666,2421850.2098260084,2454260.3588954392,2488105.5483664251,2521066.8995823073,2552486.9209284796,2582158.1789945615,null,215719.0085304942,221629.94205205073,224595.88083348854,227693.143971713,230709.52472486376,233584.85428982752,236300.14988454132]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,11246759.939297076,9801324.3177325577,8701657.2508699838,8820806.3182065878,9160468.1692627128,9498686.8083592132,8875587.6502234954]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.2.4 - OPEX FOR HIGH VOLTAGE CUSTOMERS"]
[null,null,"End user costs (not standard control services)"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPEX0401","Opex for high voltage customers",1374699.3548723015,1398635.5038637249,1761902.2817430953,1774027.7826060629,1805959.3294914311,1827957.3997140783,1850684.6522152254]

{"sheet":"3.3 Assets (RAB)","index":20,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[98,2,98,8],[98,10,98,16],[98,18,98,24],[22,10,22,16],[22,18,22,24],[97,2,97,8],[97,10,97,16],[97,18,97,24],[115,2,115,8],[114,2,114,8],[8,2,8,8],[8,10,8,16],[8,18,8,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[114,10,114,16],[114,18,114,24],[115,18,115,24],[115,10,115,16],[21,2,21,8],[21,10,21,16],[21,18,21,24],[22,2,22,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",4066683442.4058886,4144150319.972826,4193853478.3753862,4234792015.2897139,4276418071.1328573,4269312662.6983786,4254943092.0351706,null,4274919521.5299997,4361575784.504302,4417679391.3288279,4461692154.4090157,4506727613.2758207,4502806363.0279922,4491345265.1752157,null,96571481.579999998,87002399.949247509,77690387.565816075,69942282.877112612,61686390.25724192,53586917.661898308,45439772.588851765]
["DRAB0102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-293588697.61524493,-302210584.3895036,-302091061.84841037,-313340805.57062894,-325592143.41261381,-330794546.9574433,-326506388.13563591,null,-309797678.26844245,-318972360.5679611,-318512183.47323716,-330193399.57781142,-342893287.39375061,-348549063.64627308,-343344111.92257392,null,-12395893.12679584,-12604736.13743131,-9216054.0392509457,-9321279.3706559595,-9376928.4204315413,-9440151.3657179307,-9503929.6848465856]
["DRAB0105","Actual additions (recognised in RAB)",373498162.75415945,354308436.49008054,346631098.76273841,359608861.4137724,323225234.97813487,321413976.29423541,313196874.73763931,null,398896528.81472182,377470661.09050441,366126446.55342484,379870858.44461602,343710537.14592248,342076965.79349631,333912087.35333699,null,2826811.4960433529,3292723.753999874,1467949.3505474709,1065386.750785266,1277455.8250879254,1293006.292671388,1306919.8689302756]
["DRAB0106","Disposals ",-2442587.5719769998,-2394693.6980166668,-3601500,-4642000,-4738500,-4989000,-3427500,null,-2442587.5719769998,-2394693.6980166668,-3601500,-4642000,-4738500,-4989000,-3427500,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":4144150319.972826},4193853478.3753862,4234792015.2897139,4276418071.1328573,4269312662.6983786,4254943092.0351706,4238206078.6371741,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":4361575784.504302},4417679391.3288279,4461692154.4090157,4506727613.2758207,4502806363.0279922,4491345265.1752157,4478485740.605979,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":87002399.949247509},77690387.565816075,69942282.877112612,61686390.25724192,53586917.661898308,45439772.588851765,37242762.77293545]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",463863048.61019689,484333162.85669929,498590689.84229016,505438782.29298872,513033508.85117412,520126483.9490996,526605347.12363315,null,546408395.74952948,570521207.32129192,587315889.43898511,595382613.48855495,604328836.66207123,612684020.71038222,620315810.40366411,null,0,0,0,0,0,0,0]
["DRAB0202","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-36106841.870445691,-37338239.516250916,-36579403.389318839,-37540543.723464787,-38539725.802034736,-39549650.917949863,-37507419.08087106,null,-42532125.809812725,-43982653.102706894,-43088780.585816294,-44220957.743803665,-45397946.249891549,-46587589.538072646,-44181938.505531415,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",56576956.116948046,51595766.501841791,43427495.840017378,45135270.281650156,45632700.899960205,46028514.092483401,46144845.393476769,null,66644937.381575137,60777335.220400095,51155504.635386109,53167180.917319864,53753130.29820253,54219379.231354445,54356411.917492494,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":484333162.85669929},498590689.84229016,505438782.29298872,513033508.85117412,520126483.9490996,526605347.12363315,535242773.43623888,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":570521207.32129192},587315889.43898511,595382613.48855495,604328836.66207123,612684020.71038222,620315810.40366411,630490283.81562519,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",942455603.7656914,984045840.23557675,1013013627.6971351,1026927266.9158734,1042357882.9679074,1056769063.48431,1069932519.6448405,null,1068146335.7504705,1115283260.3024607,1148114341.0538831,1163883574.8396099,1181372097.2999742,1197705227.0526419,1212624229.5048552,null,0,0,0,0,0,0,0]
["DRAB0302","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-73360220.343136847,-75862117.43373321,-74320349.098640025,-76273149.815651417,-78303241.999005824,-80355161.391442209,-76205848.690613061,null,-83143917.056967363,-85979480.025734723,-84232093.526969403,-86445329.802495003,-88746165.53228581,-91071739.460149229,-86369053.052890703,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",114950456.8130223,104829904.89529157,88233988.317378387,91703765.867685422,92714422.515408382,93518617.551972613,93754974.137915462,null,130280841.60895753,118810560.77715713,100001327.31269613,103933852.26285931,105079295.28495367,105990741.91236252,106258620.2295974,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":984045840.23557675},1013013627.6971351,1026927266.9158734,1042357882.9679074,1056769063.48431,1069932519.6448405,1087481645.0921428,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":1115283260.3024607},1148114341.0538831,1163883574.8396099,1181372097.2999742,1197705227.0526419,1212624229.5048552,1232513796.6815617,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",1208922909.7333033,1201655808.7239954,1192421811.4129875,1172279787.8701935,1152614763.2611518,1130358307.9920573,1104101522.6038556,null,1208922909.7333033,1201655808.7239954,1192421811.4129875,1172279787.8701935,1152614763.2611518,1130358307.9920573,1104101522.6038556,null,0,0,0,0,0,0,0]
["DRAB0402","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-56660474.235991269,-57512153.446858123,-63200143.630542628,-64346966.698495097,-65524628.670500785,-66668417.056091703,-67741421.435774654,null,-56660474.235991269,-57512153.446858123,-63200143.630542628,-64346966.698495097,-65524628.670500785,-66668417.056091703,-67741421.435774654,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",49393373.226683266,48278156.135850258,43058120.087748595,44681942.089453571,43268173.401406206,40411631.66789005,36379794.025578551,null,49393373.226683266,48278156.135850258,43058120.087748595,44681942.089453571,43268173.401406206,40411631.66789005,36379794.025578551,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":1201655808.7239954},1192421811.4129875,1172279787.8701935,1152614763.2611518,1130358307.9920573,1104101522.6038556,1072739895.1936594,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":1201655808.7239954},1192421811.4129875,1172279787.8701935,1152614763.2611518,1130358307.9920573,1104101522.6038556,1072739895.1936594,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",160868194.84303653,159995702.98165578,159039787.47382861,170079724.88208482,177633330.16827729,182080561.89928162,186836300.3123095,null,160868194.84303653,159995702.98165578,159039787.47382861,170079724.88208482,177633330.16827729,182080561.89928162,186836300.3123095,null,0,0,0,0,0,0,0]
["DRAB0502","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-3596017.4467329751,-3610188.7305624383,-3353203.1124883355,-3614896.5765018729,-3817960.2467326792,-3968236.4645097158,-4126854.1895558541,null,-3596017.4467329751,-3610188.7305624383,-3353203.1124883355,-3614896.5765018729,-3817960.2467326792,-3968236.4645097158,-4126854.1895558541,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",2723525.5853522248,2654273.2227352797,14393140.520744527,11168501.862694342,8265191.9777369993,8723974.877537623,12155576.926366914,null,2723525.5853522248,2654273.2227352797,14393140.520744527,11168501.862694342,8265191.9777369993,8723974.877537623,12155576.926366914,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":159995702.98165578},159039787.47382861,170079724.88208482,177633330.16827729,182080561.89928162,186836300.3123095,194865023.04912058,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":159995702.98165578},159039787.47382861,170079724.88208482,177633330.16827729,182080561.89928162,186836300.3123095,194865023.04912058,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",23176644.72696346,23050942.850852281,22913221.941287018,24503770.696861267,25592035.697264947,26232758.432722606,26917928.423724666,null,23176644.72696346,23050942.850852281,22913221.941287018,24503770.696861267,25592035.697264947,26232758.432722606,26917928.423724666,null,0,0,0,0,0,0,0]
["DRAB0602","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-518086.36801210511,-520128.05692992359,-483103.55761323683,-520806.3269439186,-550062.16925932933,-571712.80389054725,-594565.21834314009,null,-518086.36801210511,-520128.05692992359,-483103.55761323683,-520806.3269439186,-550062.16925932933,-571712.80389054725,-594565.21834314009,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",392384.49190092413,382407.14736466017,2073652.3131874874,1609071.3273475971,1190784.9047169881,1256882.7948926073,1751281.4646087624,null,392384.49190092413,382407.14736466017,2073652.3131874874,1609071.3273475971,1190784.9047169881,1256882.7948926073,1751281.4646087624,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":23050942.850852281},22913221.941287018,24503770.696861267,25592035.697264947,26232758.432722606,26917928.423724666,28074644.66999029,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":23050942.850852281},22913221.941287018,24503770.696861267,25592035.697264947,26232758.432722606,26917928.423724666,28074644.66999029,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",516706887.06669664,513600848.53414279,509654136.98840356,501045215.60869604,492640168.79552132,483127516.14691693,471905078.609267,null,516706887.06669664,513600848.53414279,509654136.98840356,501045215.60869604,492640168.79552132,483127516.14691693,471905078.609267,null,0,0,0,0,0,0,0]
["DRAB0702","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-24217307.014771104,-24581324.033791378,-27012433.311161198,-27502598.045973547,-28005943.66600661,-28494811.344353534,-28953425.163622797,null,-24217307.014771104,-24581324.033791378,-27012433.311161198,-27502598.045973547,-28005943.66600661,-28494811.344353534,-28953425.163622797,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",21111268.48221723,20634612.488052122,18403511.931453705,19097551.232798807,18493291.017402209,17272373.806703597,15549122.257291988,null,21111268.48221723,20634612.488052122,18403511.931453705,19097551.232798807,18493291.017402209,17272373.806703597,15549122.257291988,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":513600848.53414279},509654136.98840356,501045215.60869604,492640168.79552132,483127516.14691693,471905078.609267,458500775.70293617,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":513600848.53414279},509654136.98840356,501045215.60869604,492640168.79552132,483127516.14691693,471905078.609267,458500775.70293617,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",8454227.5099999998,9618086.426844269,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,8454227.5099999998,9618086.426844269,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,0,0,0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",1163858.91684427,1134881.4369064874,0,0,0,0,0,null,1163858.91684427,1134881.4369064874,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":9618086.426844269},{"$f":"SUM(D68+D69+D70+D71)","v":10752967.863750756},{"$f":"SUM(E68+E69+E70+E71)","v":10752967.863750756},10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,{"$f":"SUM(K68+K69+K70+K71)","v":9618086.426844269},{"$f":"SUM(L68+L69+L70+L71)","v":10752967.863750756},{"$f":"SUM(M68+M69+M70+M71)","v":10752967.863750756},10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},{"$f":"SUM(T68+T69+T70+T71)","v":0},{"$f":"SUM(U68+U69+U70+U71)","v":0},0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,54999352.899999999,45372114.953044377,35521031.146813899,28416824.967297539,21312618.787781179,14208412.608264817,7104206.4287484549]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0903","Straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-9627237.9469556231,-9851083.8062304743,-7104206.179516362,-7104206.179516362,-7104206.179516362,-7104206.179516362,-7104206.179516362]
["DRAB0905","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":45372114.953044377},35521031.146813899,28416824.967297539,21312618.787781179,14208412.608264817,7104206.4287484549,0.249232092872262]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",524508157.66000003,548115661.56107402,567804686.97842526,586089759.76249933,605962515.6010257,616255605.87081587,631771042.6623807,null,524508157.66000003,548115661.56107402,567804686.97842526,586089759.76249933,605962515.6010257,616255605.87081587,631771042.6623807,null,42239687.129999995,42234328.534739859,42549593.051672012,41461375.929800369,40143902.457548589,39004274.516038276,37838399.603039429]
["DRAB1002","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-25432945.768253185,-28345896.738449764,-31019822.22952028,-32846440.009822886,-33797128.45045577,-34748017.305529103,-37103917.913193308,null,-25432945.768253185,-28345896.738449764,-31019822.22952028,-32846440.009822886,-33797128.45045577,-34748017.305529103,-37103917.913193308,null,-2312242.7441241695,-2442211.8605798143,-2234783.8792032497,-2275732.6919650934,-2309956.2355262833,-2351753.6745982822,-2394106.4875125475]
["DRAB1005","Actual additions (recognised in RAB)",49813097.264447734,48792419.798075967,50078895.013594359,53833195.848349184,44926218.720245957,51665454.097093917,51693212.594930038,null,49813097.264447734,48792419.798075967,50078895.013594359,53833195.848349184,44926218.720245957,51665454.097093917,51693212.594930038,null,2306884.1488640276,2757476.377511967,1146566.7573316104,958259.21971331257,1170328.2940159719,1185878.7615994345,1199792.3378583221]
["DRAB1006","Disposals ",-772647.59512050007,-757497.64227500011,-774000,-1113999.9999999998,-836000,-1402000.0000000002,-910000,null,-772647.59512050007,-757497.64227500011,-774000,-1113999.9999999998,-836000,-1402000.0000000002,-910000,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":548115661.56107402},567804686.97842526,586089759.76249933,605962515.6010257,616255605.87081587,631771042.6623807,645450337.3441174,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":548115661.56107402},567804686.97842526,586089759.76249933,605962515.6010257,616255605.87081587,631771042.6623807,645450337.3441174,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":42234328.534739859},42549593.051672012,41461375.929800369,40143902.457548589,39004274.516038276,37838399.603039429,36644085.453385204]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",217727768.49000001,219734265.80198523,219662548.17727816,237674739.3967663,255830897.92678416,243609397.05942404,226120384.79140899,null,217727768.49000001,219734265.80198523,219662548.17727816,237674739.3967663,255830897.92678416,243609397.05942404,226120384.79140899,null,-667558.44999999995,-604043.53853672254,-380236.63266983733,64081.980014690635,229869.0119121396,374230.53759519791,497166.55706386548]
["DRAB1102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Straight line depreciation",-73696804.56790176,-74440536.432927817,-66122603.519125819,-70695404.373775437,-77053452.408618018,-76438539.673676625,-74272936.443662047,null,-73696804.56790176,-74440536.432927817,-66122603.519125819,-70695404.373775437,-77053452.408618018,-76438539.673676625,-74272936.443662047,null,-456412.43571604782,-311440.47062102193,122936.0194686676,58659.500825495517,37233.994611104834,15808.488396714121,-5617.0178176765912]
["DRAB1105","Actual additions (recognised in RAB)",77373241.856743485,76006014.863962427,86962294.738613963,92379562.90379329,68734451.541257918,62536527.405661561,55768067.937470801,null,77373241.856743485,76006014.863962427,86962294.738613963,92379562.90379329,68734451.541257918,62536527.405661561,55768067.937470801,null,519927.34717932536,535247.37648790714,321382.59321586037,107127.53107195345,107127.53107195345,107127.53107195345,107127.53107195345]
["DRAB1106","Disposals ",-1669939.9768564999,-1637196.0557416668,-2827500,-3528000,-3902500,-3587000,-2517500,null,-1669939.9768564999,-1637196.0557416668,-2827500,-3528000,-3902500,-3587000,-2517500,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":219734265.80198523},219662548.17727816,237674739.3967663,255830897.92678416,243609397.05942404,226120384.79140899,205098016.28521773,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":219734265.80198523},219662548.17727816,237674739.3967663,255830897.92678416,243609397.05942404,226120384.79140899,205098016.28521773,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":-604043.53853672254},-380236.63266983733,64081.980014690635,229869.0119121396,374230.53759519791,497166.55706386548,598677.0703181423]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2020)"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",474098105.73344809,491461926.3494947,502014736.06763947,509236145.57208145,516579996.40013683,523365915.53636634,530924060.27993602,null,558464801.53541064,578918548.38013852,591349251.46377003,599855725.07531309,608506428.68622673,616499915.55702317,625403047.10964465,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",963250722.00063407,998529733.96635592,1019970447.3065042,1034642574.9418905,1049563473.2261088,1063350791.5645752,1078707082.3684916,null,1091714798.0264657,1131698800.6781719,1155998957.9467463,1172627836.069792,1189538662.1763082,1205164728.2787485,1222569013.0932083,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",1205289359.2286494,1197038810.0684915,1182350799.6415906,1162447275.5656726,1141486535.6266046,1117229915.2979565,1088420708.8987575,null,1205289359.2286494,1197038810.0684915,1182350799.6415906,1162447275.5656726,1141486535.6266046,1117229915.2979565,1088420708.8987575,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",160431948.91234615,159517745.2277422,164559756.1779567,173856527.52518106,179856946.03377944,184458431.10579556,190850661.68071502,null,160431948.91234615,159517745.2277422,164559756.1779567,173856527.52518106,179856946.03377944,184458431.10579556,190850661.68071502,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",23113793.788907871,22982082.39606965,23708496.319074143,25047903.197063107,25912397.064993776,26575343.428223636,27496286.546857476,null,23113793.788907871,22982082.39606965,23708496.319074143,25047903.197063107,25912397.064993776,26575343.428223636,27496286.546857476,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",515153867.80041969,511627492.76127315,505349676.29854977,496842692.20210868,487883842.47121912,477516297.37809193,465202927.15610158,null,515153867.80041969,511627492.76127315,505349676.29854977,496842692.20210868,487883842.47121912,477516297.37809193,465202927.15610158,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",9036156.9684221335,10185527.145297512,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,9036156.9684221335,10185527.145297512,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,10752967.863750756,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,50185733.926522188,40446573.049929142,31968928.057055719,24864721.877539359,17760515.698022999,10656309.518506635,3552103.3389902739]
["DRAB1209","“Other” assets with long lives",536311909.61053705,557960174.26974964,576947223.3704623,596026137.68176246,611109060.73592079,624013324.26659822,638610690.00324905,null,536311909.61053705,557960174.26974964,576947223.3704623,596026137.68176246,611109060.73592079,624013324.26659822,638610690.00324905,null,42237007.832369924,42391960.793205932,42005484.490736187,40802639.193674475,39574088.486793429,38421337.059538856,37241242.528212316]
["DRAB1210","“Other” assets with short lives",218731017.14599264,219698406.98963171,228668643.78702223,246752818.66177523,249720147.4931041,234864890.92541653,215609200.53831336,null,218731017.14599264,219698406.98963171,228668643.78702223,246752818.66177523,249720147.4931041,234864890.92541653,215609200.53831336,null,-635800.99426836125,-492140.08560327993,-158077.32632757333,146975.49596341513,302049.77475366875,435698.54732953169,547921.81369100395]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,-62882584.349999942,-57645741.191363841,-70633354.77849251,-70253435.627612457,-70784816.432165861,-70638266.364091784,-67753001.897265047,null,-1207435.6156755001,-1207435.6156755001,-1157711.8900000001,-1157711.8900000001,-1157711.8900000001,-1157711.8900000001,-1157711.8900000001]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",55,55,54.727186737691042,54.471002949387248,54.237597440634438,54.024117621770344,53.827864922254953,null,55,55,54.727186737691042,54.471002949387248,54.237597440634438,54.024117621770344,53.827864922254953,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",55,55,54.727186737691042,54.471002949387248,54.237597440634438,54.024117621770344,53.827864922254953,null,55,55,54.727186737691042,54.471002949387248,54.237597440634438,54.024117621770344,53.827864922254953,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",45,45,44.859939974274688,44.733873858966938,44.617302717550743,44.496387975453771,44.383027580812026,null,45,45,44.859939974274688,44.733873858966938,44.617302717550743,44.496387975453771,44.383027580812026,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",55,55,55,55,55,55,55,null,55,55,55,55,55,55,55,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",55,55,55,55,55,55,55,null,55,55,55,55,55,55,55,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",45,45,44.859939974274688,44.733873858966938,44.617302717550743,44.496387975453771,44.383027580812026,null,45,45,44.859939974274688,44.733873858966938,44.617302717550743,44.496387975453771,44.383027580812026,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,15,15,15,15,15,15,15]
["DRAB1408","“Other” assets with long lives",17.472841207453495,18.357150170134606,18.70619413352906,19.209852829406479,19.319295824708853,19.219482018199361,19.141358780997084,null,17.472841207453495,18.357150170134606,18.70619413352906,19.209852829406479,19.319295824708853,19.219482018199361,19.141358780997084,null,27.910130379529615,27.915566007925989,27.930679923513868,27.946303688308575,27.963156518999572,27.981010639910725,27.999999979711305]
["DRAB1409","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5,null,7,7,7,7,7,7,7]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",12.971505061075534,13.630366918118689,13.463810913773827,13.311810039501841,13.151228187276789,14.040031546510862,14.270317354606116,null,12.971505061075533,13.630366918118686,13.463810913773825,13.311810039501839,13.151228187276789,14.040031546510864,14.270317354606117,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",12.971505061075533,13.630366918118689,13.463810913773823,13.311810039501834,13.151228187276786,14.040031546510857,14.27031735460611,null,12.971505061075533,13.630366918118689,13.463810913773825,13.311810039501838,13.151228187276784,14.040031546510855,14.270317354606107,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",20.893945656796504,18.867390846193075,18.21810487762448,17.590557728411202,16.954929453942583,16.298765204545486,15.835804334438413,null,20.893945656796504,18.867390846193075,18.21810487762448,17.590557728411202,16.954929453942583,16.298765204545486,15.835804334438413,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",44.317822397260031,47.429213840794993,47.049679370542485,46.525714960047509,45.884503992575972,45.273298190459563,47.21878072219765,null,44.317822397260031,47.429213840794993,47.049679370542485,46.525714960047509,45.884503992575972,45.273298190459563,47.21878072219765,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",44.317822397259981,47.429213840794965,47.049679370542435,46.52571496004748,45.884503992575951,45.273298190459542,47.218780722197636,null,44.317822397259981,47.429213840794965,47.049679370542435,46.52571496004748,45.884503992575951,45.273298190459542,47.218780722197636,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",20.8939456567965,18.867390846193071,18.218104877624477,17.590557728411202,16.954929453942579,16.298765204545489,15.835804334438416,null,20.8939456567965,18.867390846193071,18.218104877624477,17.590557728411202,16.954929453942579,16.298765204545489,15.835804334438416,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,4.6057993054884037,5.0000000350823273,4.0000000350823282,3.0000000350823282,2.0000000350823282,1.0000000350823282,0]
["DRAB1508","“Other” assets with long lives",11.367786599659018,10.705634896657493,10.666969206640287,10.954916495755475,10.951353192180655,10.674162441794106,11.042837650534601,null,11.367786599659018,10.705634896657493,10.666969206640287,10.954916495755475,10.951353192180655,10.674162441794106,11.042837650534601,null,18.262558660187736,17.420766739942859,18.740291436148588,17.946802726153631,17.195011165935725,16.224121036298722,15.472517351291982]
["DRAB1509","“Other” assets with short lives",2.9518092739695598,3.3220492915670095,3.3619545924109899,3.3201743715531538,3.1869970056913131,3.0444519311947116,2.7614098230893283,null,2.9518092739695598,3.3220492915670095,3.3619545924109899,3.3201743715531538,3.1869970056913131,3.0444519311947116,2.7614098230893283,null,7,6.5439893294027502,5.3822001782932904,4.4379230554423801,3.8889014726516349,2.7530565688551105,2.0830389776431986]

{"sheet":"3.4 Operational data","index":21,"n_rows":88,"n_cols":10,"rows_kept":88,"cut":false,"hidden":false,"merged":[[44,3,44,9],[45,3,45,9],[9,3,9,9],[10,3,10,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOPED01","Total energy delivered","GWh",10168,9693,9639,9664,9687,9737,9819]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",8891.0499999999993,8398.8230000000003,3661.9209999999998,3433.0729999999999,3227.2159999999999,3022.3150000000001,2840.6759999999999]
["DOPED0202","Energy Delivery at On-peak times","GWh",322.505,361.69400000000002,2694.6570000000002,2825.6489999999999,2947.703,3083.0630000000001,3229.89]
["DOPED0203","Energy Delivery at Shoulder times ","GWh"," -   "," -   ",433.16899999999998,505.41199999999998,571.72199999999998,638.19799999999998,702.53300000000002]
["DOPED0204","Energy Delivery at Off-peak times","GWh",312.505,340.69600000000003,2273.5279999999998,2339.9119999999998,2396.7240000000002,2465.5030000000002,2534.277]
["DOPED0205","Controlled load energy deliveries","GWh",520,477.02600000000001,461.02600000000001,445.02600000000001,429.02600000000001,413.02600000000001,397.02600000000001]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",122,115,115,115,115,115,115]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",4449.1869999999999,4217.451,4217.38,4224.5649999999996,4231.0069999999996,4249.3990000000003,4282.4930000000004]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh"]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",5329.2460000000001,5051.6719999999996,5051.5870000000004,5060.1940000000004,5067.91,5089.9399999999996,5129.5789999999997]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh"]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",133.285,133.285,133.285,133.285,133.285,133.285,133.285]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh"]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",171.715,171.715,171.715,171.715,171.715,171.715,171.715]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",107.145,129.952,132.36799999999999,134.92400000000001,137.494,140.03800000000001,142.67099999999999]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh"]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh"]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh"]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",657.6,656.97,605.85599999999999,611.42999999999995,617.15300000000002,623.02099999999996,629.05100000000004]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",3755.05,3478.453,3438.989,3459.509,3472.8449999999998,3482.114,3517.7550000000001]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",1214.01,1163.432,1313.528,1323.7260000000001,1335.4259999999999,1351.4590000000001,1364.2570000000001]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",3240,3216.4540000000002,3054.134,3047.5250000000001,3044.2550000000001,3062.373,3088.9740000000002]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",1959,1834.9,1832.65,1833.3119999999999,1834.865,1841.1579999999999,1848.4179999999999]
["DOPED0505","Other Customer Class Energy Deliveries","GWh"]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3062.7261406493712,3068.5052532680702,3072.5357543924183,3080.2395610844437,3087.9343294872979,3095.7300905718471,3103.6090694253185]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2783.8318708523511,2790.6597811399388,2796.8822545627008,2803.2828169201439,2809.9627800529315,2816.9197471040966,2823.9515212039169]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2780.7684857193194,2786.236399184193,2791.637154770287,2799.1009577874083,2806.5665376168658,2814.1412209401979,2821.7596166473577]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2522.6870340498776,2529.0736283841516,2536.41823753157,2542.1397176433093,2548.1202433022972,2554.3574856623845,2560.7012873706399]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",3035.5511606115456,3049.0343644580498,3063.312065299695,3071.5482897941897,3079.6938546225692,3087.8582515045746,3096.1722093357243]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2760.3916504896661,2773.3158445696049,2787.3763738752532,2795.5797111620464,2803.8822333770772,2812.2839123623048,2820.7847324413819]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2885.5996014783495,2898.609252164747,2912.5872824893436,2920.6756682846144,2928.6951157925532,2936.7612689571001,2944.9206331485575]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2619.866005907686,2632.2917985246513,2646.0730425884826,2653.9960808068108,2662.0146662701727,2670.1287712438789,2678.3383800411652]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3161.2050509288983,3167.1826862641756,3171.1755160228436,3179.0757645864674,3186.9551054470621,3194.9420305510484,3203.011680484321]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2874.1568902576983,2881.1635995730676,2887.3475838757063,2894.0045235406119,2900.9492900841469,2908.1794374213141,2915.4790283256157]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2864.8282956710632,2870.466140668233,2875.9859814618976,2883.6477368910887,2891.3006393527608,2899.0693162012076,2906.8801696921078]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2599.4727397684128,2606.022104370375,2613.525961715613,2619.4677538312449,2625.6761598984176,2632.1488007907001,2638.7254966085102]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",3082.4220198592352,3096.1341450089803,3110.5984114906532,3118.9505413318243,3127.1951041946222,3135.456076029564,3143.879501868365]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2803.0263027449723,2816.181372347764,2830.4100251904088,2838.7694171741214,2847.2295156894438,2855.790296235406,2864.451746909413]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2929.2885306361259,2942.5110570456632,2956.6654525014465,2964.86490556738,2972.9794250720079,2981.1390985530261,2989.4030946938647]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2659.6175022265861,2672.259118300341,2686.1995551614295,2694.2689598872248,2702.4353433267997,2710.6986810310932,2719.0589607103916]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.98479414598464676,0.98478755171934129,0.98479831211374602,0.98480185853880409,0.98481026990981857,0.98481948929571272,0.98482534317734227]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.95886995891263882,0.95888769095221127,0.95886986943753616,0.95891480327942369,0.95896286320162516,0.95901029913717117,0.9590587352677965]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0.88874336365975148,0.88874336365975148,0.88874336365975148,0.8887433636597516,0.88874336365975148,0.88874336365975148,0.88874336365975148]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0.87253029241842317,0.87253029241842317,0.87253029241842317,0.87253029241842317,0.87253029241842317,0.87253029241842317,0.87253029241842317]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0.95916925599996217,0.96027937726183232,0.95997491707221194,0.95995453261180963,0.95993407959618737,0.95991711863961859,0.95989954104453878]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.9696778563373607,0.96963711578468714,0.96959756043067025,0.96961400317872259,0.96963349364124596,0.96965231896532833,0.96967219045126751]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.96326599753908471,0.96319067825086191,0.96307288812860659,0.96300688179309857,0.96294635685454877,0.96288750866392969,0.96283139519402428]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.96683725376455509,0.96679649157292458,0.96709089924112024,0.96703084080932067,0.9669758128499959,0.96692260268935726,0.96687045394372095]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.98814058251701598,0.98814578129302411,0.9881514030831533,0.98815721767038189,0.98816513451762467,0.98817290651707701,0.98817762880682847]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW ",0,0,0,0,0,0,0]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",0,0,10,14,19,24,29]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",1819,1795,401,401,401,401,401]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",197,204,1437,1447,1451,1462,1473]

{"sheet":"3.5 Physical assets","index":22,"n_rows":97,"n_cols":10,"rows_kept":97,"cut":false,"hidden":false,"merged":[[10,3,10,9],[77,3,77,9],[93,3,93,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Circuit length"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",18815.266899335336,18819.534766531498,18823.80360180802,18828.073405384497,18832.344177480565,18836.615918315914,18840.888628110282]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",267.06056361291451,267.12114096347403,267.18173205479462,267.24233688999311,267.30295547218702,267.36358780449461,267.42423389003483]
["DPA0104","Overhead 11 kV","km",17614.994703322238,17618.990312763075,17622.986828528046,17626.98425082273,17630.982579852756,17634.981815823801,17638.981958941586]
["DPA0105","Overhead SWER","km",29137.607785047989,29144.217068939932,29150.827852015813,29157.440134615692,29164.053917079706,29170.669199748067,29177.285982961068]
["DPA0106","Overhead 22 kV","km",0,0,0,0,0,0,0]
["DPA0107","Overhead 33 kV","km",3986.9041444235104,3987.8084939341102,3988.7130485783196,3989.6178084026687,3990.5227734536988,3991.4279437779614,3992.3333194220186]
["DPA0108","Overhead 44 kV","km",0,0,0,0,0,0,0]
["DPA0109","Overhead 66 kV","km",1441.3268620457297,1441.6537982335808,1441.9808085803709,1442.3078931029215,1442.6350518180579,1442.9622847426094,1443.2895918934087]
["DPA0110","Overhead 132 kV","km",0,0,0,0,0,0,0]
["DPA0111","Overhead 6.6kv","km",0,0,0,0,0,0,0]
["DPA0112","Overhead 110kV","km",0,0,0,0,0,0,0]
["DPA0113","Overhead 220kV","km",0,0,0,0,0,0,0]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D15:D28)","v":71263.16095778771},{"$f":"SUM(E15:E28)","v":71279.325581365672},71295.493871565355,71311.665829218502,71327.841455156973,71344.020750212847,71360.203715218391]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",13963.11452543879,14200.186981101218,14441.284566624998,14686.475622595523,14935.829649917425,15189.41732951503,15447.310542367299]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",0,0,0,0,0,0,0]
["DPA0204","Underground 7.6 kV","km",109.83367580097519,111.69848462920113,113.5949550761471,115.52362470796187,117.48504021785011,119.47975758103594,121.50834221235749]
["DPA0205","Underground 11 kV","km",4044.5234135229475,4113.1932719475271,4183.0290401651582,4254.0505135515223,4326.2778235776841,4399.7314435164808,4474.4321942457937]
["DPA0206","Underground SWER","km",62.035687257958209,63.088958910937677,64.160113515231231,65.249454696163639,66.357291234156065,67.483937152251755,68.629711805127812]
["DPA0207","Underground 22 kV","km",0,0,0,0,0,0,0]
["DPA0208","Underground 33 kV","km",136.27511627158032,138.58886055845326,140.94188870558995,143.33486769321198,145.76847582585108,148.24340292461869,150.76035052273988]
["DPA0209","Underground 66 kV","km",54.916837900487593,55.849242314600566,56.797477538073551,57.761812353980936,58.742520108925056,59.73987879051797,60.754171106178745]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",0,0,0,0,0,0,0]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D31:D42)","v":18370.699256192736},{"$f":"SUM(E31:E42)","v":18682.605799461944},18999.808041625198,19322.395895598362,19650.46080088189,19984.095749479933,20323.395312259498]
[]
[null,"Circuit Capacity MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.16669373411401062,0.16669373411401062,0.16669373411401062,0.16669373411401062,0.16669373411401062,0.16669373411401062,0.16669373411401062]
["DPA0302","Overhead 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0303","Overhead 7.6 kV","MVA",2.5862831033661511,1.8043014541590683,1.8043014541590683,1.8043014541590683,1.8043014541590683,1.8043014541590683,1.8043014541590683]
["DPA0304","Overhead 11 kV","MVA",3.9632597650278751,3.977094046746525,3.977094046746525,3.9774244565846155,3.9774244565846155,3.977682175182232,3.9784362469211354]
["DPA0305","Overhead SWER","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0306","Overhead 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0307","Overhead 33 kV","MVA",10.103306123041603,10.103306123041603,10.226456574352431,10.226456574352431,10.226456574352431,10.226456574352431,10.226456574352431]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",59.320184403706222,59.320184403706222,59.320184403706222,59.08550933472565,59.695680475359438,59.695680475359438,59.695680475359438]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0,0,0,0,0,0,0]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0404","Underground 7.6 kV","MVA",3.119295814586037,2.1710783427136193,2.1710783427136193,2.1710783427136193,2.1710783427136193,2.1710783427136193,2.1710783427136193]
["DPA0405","Underground 11 kV","MVA",4.7776182227635484,4.7818168176067957,4.7826186024929322,4.7827570205667875,4.7827570205667875,4.7842261303097677,4.7848936066842507]
["DPA0406","Underground SWER","MVA",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",0,0,0,0,0,0,0]
["DPA0409","Underground 33 kV","MVA",14.00404830464208,14.00404830464208,14.00404830464208,14.00404830464208,14.00404830464208,14.00404830464208,14.00404830464208]
["DPA0410","Underground 66 kV","MVA",126.31775420935942,126.31775420935942,126.31775420935942,126.31775420935942,126.31775420935942,126.31775420935942,126.31775420935942]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",9347,9482,9607,9727,9842,9952,10057]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",755,751,625,625,625,627,629]
["DPA0503","Cold spare capacity included in DPA0501","MVA",140,140,140,140,140,140,140]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",322.5,325.5,320.5,320.5,320.5,320.5,320.5]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",115.51499999999997,117.01499999999997,119.01499999999997,120.01499999999997,118.01499999999997,118.01499999999997,118.01499999999997]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",4819.6600000000017,4878.9100000000017,4886.4100000000017,4898.010000000002,4909.010000000002,4927.4450000000015,4933.9450000000015]
["DPA0604","Total zone substation transformer  capacity ","MVA",5741.8750000000018,5835.6250000000018,5840.1250000000018,5852.7250000000022,5861.7250000000022,5880.1600000000017,5886.6600000000017]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",484.2,514.20000000000005,514.20000000000005,514.20000000000005,514.20000000000005,514.20000000000005,514.20000000000005]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DPA0701","Public lighting luminaires","0's",231727,232927,234127,235327,236527,237727,238927]
["DPA0702","Public lighting poles","0's",112523,113623,114723,115823,116923,118023,119123]

{"sheet":"3.6 Quality of service","index":23,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[[7,3,7,9],[14,3,14,9],[19,3,19,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS0201","Energy Not Supplied (planned)","GWh",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
["DQS0202","Energy Not Supplied (unplanned)","GWh",4.7,4.7,4.7,4.7,4.7,4.7,4.7]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":6},{"$f":"SUM(E10:E11)","v":6},6,6,6,6,6]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS03","System losses","%",6.3E-2,6.4000000000000001E-2,6.5000000000000002E-2,6.5000000000000002E-2,6.5000000000000002E-2,6.4000000000000001E-2,6.4000000000000001E-2]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DQS04","Overall utilisation","%",0.55055274643368191,0.54273238706465454,0.54299788378208391,0.54317873547560602,0.54368894914842658,0.54334270335348822,0.544113585714874]

{"sheet":"3.7 Operating Environment","index":24,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[8,3,8,9],[15,3,15,9],[33,3,33,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0101","Customer density","Customer / km",0.11,0.111,0.112,0.113,0.113,0.114,0.115]
["DOEF0102","Energy density","MWh/customer",11.2,10.6,10.4,10.3,10.199999999999999,10.199999999999999,10.199999999999999]
["DOEF0103","Demand density","kVA / customer",3.2,3.1,3.1,3.1,3.1,3.1,3]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0201","Rural proportion","%",0.79800000000000004,0.79800000000000004,0.79800000000000004,0.79800000000000004,0.79800000000000004,0.79800000000000004,0.79800000000000004]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",14673,14677,14680,14683,14687,14690,14693]
["DOEF0203","Rural vegetation maintenance spans","0's",63347,63362,63376,63390,63405,63419,63434]
["DOEF0204","Total vegetation maintenance spans","0's",78021,78038,78056,78074,78092,78109,78127]
["DOEF0205","Total number of spans","0's",648141,648288,648435,648582,648729,648876,649024]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",3,3,3,3,3,3,3]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1,1,1,1,1,1,1]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",3,3,3,3,3,3,3]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",9,9,9,9,9,9,9]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",2,2,2,2,2,2,2]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",1,1,1,1,1,1,1]
["DOEF0212","Tropical proportion","Spans"," -   "," -   ",0,0,0,0,0]
["DOEF0213","Standard vehicle access","km",5766,5768,5769,5770,5772,5773,5774]
["DOEF0214","Bushfire risk","Spans",391029,391117,391206,391295,391384,391472,391561]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
["DOEF0301","Route Line length","km",82547,82738,82930,83121,83314,83507,83700]

{"sheet":"4.1 Public lighting","index":25,"n_rows":152,"n_cols":10,"rows_kept":152,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[31,3,31,9],[184,1,184,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[57,1,57,2],[58,1,58,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[210,1,210,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[90,1,90,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[156,1,156,2],[151,1,151,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[182,1,182,2],[183,1,183,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",1200,1200,1200,1200,1200,1200,1200]
[null,"Number of poles installed ","0's",1100,1100,1100,1100,1100,1100,1100]
[null,"Total expenditure","$0's",850000,850000,850000,850000,850000,850000,850000]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",37953,47800,26915,10487,10897,182,0]
[null,"Number of poles replaced","0's",627,627,223,223,223,223,223]
[null,"Total expenditure","$0's",20654134,26222774,15449635,8650874,9257399,1582785,1464424]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",57059,42361,41265,56538,70901,77557,64136]
[null,"Number of poles maintained","0's",10040,10060,10080,10110,10130,10150,10170]
[null,"Total expenditure","$0's",8967726,7766707,6786781,6852601,7091131,7334984,6817009]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",7,7,7,7,7,7,7]
[null,"GSO breaches","0's",1890,1370,830,490,320,270,270]
[null,"GSL payments ","$0's",186900,135800,82400,48400,31300,26800,26000]
[null,"Customer complaints ","0's",64,47,28,17,11,9,9]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2020)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"LIGHT INSTALLATION"]
[null,"All Lights",null,708.3,708.3,708.3,708.3,708.3,708.3,708.3]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"All Lights",null,553.79999999999995,514.5,302.10000000000002,244.9,508.7,31.9,200]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"All Lights",null,258,258.39999999999998,257.60000000000002,258,258.7,260.39999999999998,1100]

{"sheet":"4.2 Metering","index":26,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":false,"merged":[[75,1,77,1],[78,1,80,1],[5,1,5,2],[8,4,8,10],[26,4,26,10],[64,4,64,10],[10,1,13,1],[14,1,17,1],[65,2,65,3],[27,2,27,3],[81,1,83,1],[84,1,86,1],[87,1,89,1],[18,1,21,1],[28,1,30,1],[31,1,33,1],[34,1,36,1],[37,1,39,1],[40,1,42,1],[43,1,45,1],[46,1,48,1],[49,1,51,1],[54,1,56,1],[66,1,68,1],[69,1,71,1],[72,1,74,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,null,"VOLUMES (0's)"]
[null,"ASSET CATEGORY","ASSET SUBCATEGORY",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter Type 4","Single phase meter population ",null," -   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,null,"Multi phase meter population ",null," -   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,null,"Current transformer connected meter population ",null," -   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,null,"Direct connect meter population ",null," -   "," -   "," -   "," -   "," -   "," -   "," -   "]
[null,"Meter Type 5","Single phase meter population ",null,352,334,315,297,279,261,243]
[null,null,"Multi phase meter population ",null,8669,8220,7772,7323,6874,6425,5976]
[null,null,"Current transformer connected meter population ",null,4566,4329,4093,3857,3620,3384,3147]
[null,null,"Direct connect meter population ",null,4455,4225,3994,3763,3533,3302,3071]
[null,"Meter Type 6","Single phase meter population ",null,768460,728676,688893,649109,609326,569542,529759]
[null,null,"Multi phase meter population ",null,169006,160257,151507,142758,134008,125259,116509]
[null,null,"Current transformer connected meter population ",null,72,69,65,61,57,54,50]
[null,null,"Direct connect meter population ",null,937394,888865,840335,791806,743277,694748,646218]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2020)"}]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter purchase ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",22958,22958,22958,22958,22958,22958,22958]
[null,null,null,"Meter Type 6",535001,535001,535001,535001,535001,535001,535001]
[null,"Meter investigation ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",216864,203058,192545,182033,171520,161008,150496]
[null,null,null,"Meter Type 6",771890,722749,685332,647915,610498,573081,535664]
[null,"Scheduled meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",88638,84049,79460,74871,70282,65694,61105]
[null,null,null,"Meter Type 6",3353590,3179973,3006357,2832740,2659123,2485507,2311890]
[null,"Special meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",608252,569529,540044,510560,481075,451590,422105]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"Remote meter re-configuration ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"Other metering ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 7"," -   "," -   ",0,0,0,0,0]
[null,"IT infrastructure capex ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"IT infrastructure opex ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"Communications infrastructure capex ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"Communications infrastructure opex ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[]
[null,"VOLUMES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Meter purchase ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",61,61,61,61,61,61,61]
[null,null,null,"Meter Type 6",3243,3243,3243,3243,3243,3243,3243]
[null,"Meter investigation ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",354,331,314,297,280,263,245]
[null,null,null,"Meter Type 6",5243,4909,4655,4401,4147,3893,3639]
[null,"Scheduled meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",90424,85743,81062,76381,71699,67018,62337]
[null,null,null,"Meter Type 6",4275669,4054316,3832963,3611610,3390257,3168904,2947551]
[null,"Special meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,null,null,"Meter Type 5",1297,1214,1152,1089,1026,963,900]
[null,null,null,"Meter Type 6"," -   "," -   ",0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]
[null,"Remote meter re-configuration ",null,"Meter Type 4"," -   "," -   ",0,0,0,0,0]

{"sheet":"4.3 Fee-based services","index":27,"n_rows":57,"n_cols":16,"rows_kept":57,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"COMMON FEE-BASED SERVICES"]
[null,"Energisation"]
[null,"De-energisation"]
[null,"Re-energisation"]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Alt/upgrade/relocate to O/under or U/ground service or O/head service",1347607.9649999999,1353217.6249499999,1358850.6361160597,1364507.095701806,1370187.101315493,1375890.7509716868,1381618.1430929566,1051,1051,1051,1051,1051,1051,1051]
[null,"Multiphase upgrade - O/under or O/head (diagram 1 or 3)",354324.88,355832.2904,357346.11380185868,358866.37748851965,360393.10885899671,361926.33542886784,363466.08483077085,272,272,272,272,272,272,272]
[null,"Multiphase upgrade - existing pit/pillar (diagram 2)",29974.587499999998,30148.361374999993,30323.142682033285,30498.937261559509,30675.75098789762,30853.589769422197,31032.459548760868,55,55,55,55,55,55,55]
[null,"Additional service from existing asset - O/under or pit/pillar (diagram 1 or 2) ",12822.15,12875.5245,12929.121180933014,12982.94096766704,13036.98478892001,13091.253577275802,13145.748269200349,10,10,10,10,10,10,10]
[null,"Temp supply - O/head or O/Under on existing pole (diagram 3 or 3A)",134108.03249999997,134630.82652499995,135155.65856060587,135682.53655160483,136211.46847375511,136742.46233390702,137275.52617012395,117,117,117,117,117,117,117]
[null,"Temp supply - Existing pit/pillar (diagram 2)",19368.195,19471.324349999999,19575.002830305199,19679.233364856173,19784.018893162553,19889.362370385887,19995.266767423007,41,41,41,41,41,41,41]
[null,"Permanent abolishment of LV service",1869005.2549999999,1880694.1477999999,1892456.1437732119,1904291.7001121193,1916201.2768685208,1928185.3369714122,1940244.3462449792,2977,2977,2977,2977,2977,2977,2977]
[null,"Temp disconnect & reconnect - truck attendance",376437.46499999997,379198.74670000002,381980.28322938248,384782.22316339542,387604.71616713086,390447.91300351906,393311.96554138162,362,362,362,362,362,362,362]
[null,"Temp disconnect & reconnect -  single person crew",305983.125,307581.03687499999,309187.29340090277,310801.93815532973,312425.01494347421,314056.56779929012,315696.6409866864,665,665,665,665,665,665,665]
[null,"Connections specification fee - $0-$100k proj",380500.88,380500.88,380500.88,380500.88,380500.88,380500.88,380500.88,116,116,116,116,116,116,116]
[null,"Connections specification fee - $101k-$200k proj",40182.204999999994,40182.204999999994,40182.204999999994,40182.204999999994,40182.204999999994,40182.204999999994,40182.204999999994,7,7,7,7,7,7,7]
[null,"Works re-inspection for compliance - Up to 3hrs normal time",785.28,785.28,785.28,785.28,785.28,785.28,785.28,2,2,2,2,2,2,2]
[null,"Works re-inspection for compliance - After 3hrs normal time",261.76,261.76,261.76,261.76,261.76,261.76,261.76,2,2,2,2,2,2,2]
[null,"Works re-inspection for compliance - Out of hours",130.88,130.88,130.88,130.88,130.88,130.88,130.88,1,1,1,1,1,1,1]
[null,"Meter test - 1ph",24822.21,22612.546599999998,20604.4541465,18679.303039197497,16966.824653187847,15473.997319896171,14078.779875598095,204,184,166,149,134,121,109]
[null,"Meter test - Additional 1ph meter",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Meter test - 3ph",10099.2325,9217.0706250000003,8440.3788069999991,7647.2314455774995,6963.9951934726241,6394.2137685521366,5812.3403156138929,83,75,68,61,55,50,45]
[null,"Meter test - Additional 3ph meter",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"PV installation enquiry - 1ph",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"PV installation enquiry - 3ph",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Meter inspection fee - 1st meter",34754.775000000001,31580.730500000001,28683.936874999999,26073.698619375002,23700.992045011877,21573.754857762047,19640.391785440414,618,556,500,450,405,365,329]
[null,"Meter inspection fee - Addition meter",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Temporary line insulation (eg tiger tails)",132012.93,132845.32679999998,133682.9722103645,134525.89932577961,135374.14144960718,136227.73209520074,137086.70498722958,159,159,159,159,159,159,159]
[null,"Location of U/ground mains - Provision of plans from office",261.76,264.37759999999997,267.02137599999998,269.69158976,272.38850565759998,275.112390714176,277.86351462131779,2,2,2,2,2,2,2]
[null,"Asset info request - <1hr",327.2,327.2,327.2,327.2,327.2,327.2,327.2,2,2,2,2,2,2,2]
[null,"Asset info request - Ground level T/fs (site visit to open and visually see equipment)",656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,2,2,2,2,2,2,2]
[null,"Network Access Management fee - <0.5 day planning req",842566.58499999996,842566.58499999996,842566.58499999996,842566.58499999996,842566.58499999996,842566.58499999996,842566.58499999996,1658,1658,1658,1658,1658,1658,1658]
[null,"Special meter reader visit - Normal hours",1000765.74,909698.53619999997,826910.96275499999,751668.38604092994,683265.28609008505,621092.01382388175,564575.2455363581,81562,73406,66065,59459,53513,48162,43346]
[null,"Special meter reader visit - Out of hours",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Special meter reader visit - Request cancellation",61805.01249999999,56186.436349999996,51068.881212249995,46422.771852984995,42193.617936922368,38359.909322431682,34875.12729803734,5495,4946,4451,4006,3605,3245,2921]
[null,"Meter read - Subsequent attempt",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Site inspection to determine nature of connection service - <2hrs",656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,656.44499999999994,2,2,2,2,2,2,2]
[null,"Priority or out of hour appointment - <3hrs",5061.375,5061.375,5061.375,5061.375,5061.375,5061.375,5061.375,25,25,25,25,25,25,25]
[null,"Retailer fee - disconnection & reconnection - D/N at meter",1379751.2749999985,1254215.5962,1140064.4536680002,1036336.2868947901,942038.62253520614,856313.10788450239,778352.1454807187,16064.16666666665,14458,13012,11711,10540,9486,8537]
[null,"Retailer fee - disconnection & reconnection - R/C at meter",1379751.2749999985,1254215.5962,1140064.4536680002,1036336.2868947901,942038.62253520614,856313.10788450239,778352.1454807187,16064.16666666665,14458,13012,11711,10540,9486,8537]
[null,"Retailer fee - disconnection & reconnection - R/C at meter after hours",1292730.3899999999,1175100.5994000002,1068131.3982990002,970940.29030908016,882602.59938663756,802330.89846905519,729300.55191522418,15051,13546,12191,10972,9875,8888,7999]
[null,"Swing & sag calculations - up to and incld 11kV",23865.149999999998,23865.149999999998,23865.149999999998,23865.149999999998,23865.149999999998,23865.149999999998,23865.149999999998,12,12,12,12,12,12,12]
[null,"Embedded generation firm offer - >30kW-200kW",471664.935,471664.935,471664.935,471664.935,471664.935,471664.935,471664.935,126,126,126,126,126,126,126]
[null,"Swing & sag calculations - >11kV",13231.15,13231.15,13231.15,13231.15,13231.15,13231.15,13231.15,5,5,5,5,5,5,5]
[null,"Network Access Management request cancellation - <2 business days",122471.9825,122471.9825,122471.9825,122471.9825,122471.9825,122471.9825,122471.9825,241,241,241,241,241,241,241]
[null,"Temp disconnect & reconnect retailer O/head - truck attendance",6257.7000000000007,5252.8892499999993,5291.3074400049018,5330.0066101053289,5368.9888153125694,5408.2561256676991,5447.8106263515037,6,5,5,5,5,5,5]
[null,"Temp disconnect & reconnect retailer - single person crew",27607.5,24976.505249999998,22782.221619013886,20564.338765164674,18792.482101863112,17001.558557555556,15191.417310637542,60,54,49,44,40,36,32]

{"sheet":"4.4 Quoted services","index":28,"n_rows":24,"n_cols":16,"rows_kept":24,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2020)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Customer initiated asset relocations",23235015.251386479,23235015.251386479,23235015.251386479,23235015.251386479,23235015.251386479,23235015.251386479,23235015.251386479,376,376,376,376,376,376,376]
[null,"Access permits, oversight & facilitations services",594674.86679768749,594674.86679768749,594674.86679768749,594674.86679768749,594674.86679768749,594674.86679768749,594674.86679768749,1658,1658,1658,1658,1658,1658,1658]
[null,"High load escorts",458915.69429179421,458915.69429179421,458915.69429179421,458915.69429179421,458915.69429179421,458915.69429179421,458915.69429179421,170,170,170,170,170,170,170]
[null,"Large embedded generators (>200kW)",3482546.4427368026,3482546.4427368026,3482546.4427368026,3482546.4427368026,3482546.4427368026,3482546.4427368026,3482546.4427368026,20,20,20,20,20,20,20]
[null,"Enhanced connection service (non-embedded generation)",100000,100000,100000,100000,100000,100000,100000,2,2,2,2,2,2,2]
[null,"Connection point alterations (non Fee-based services)",3000,3000,3000,3000,3000,3000,3000,2,2,2,2,2,2,2]
[null,"Temporary supply (non Fee-based services)",996.32,996.32,996.32,996.32,996.32,996.32,996.32,2,2,2,2,2,2,2]
[null,"Technical/Engineering studies",18920,18920,18920,18920,18920,18920,18920,2,2,2,2,2,2,2]
[null,"Specification fee (>$200k project)",2420,2420,2420,2420,2420,2420,2420,1,1,1,1,1,1,1]
[null,"Specification/design compliance",10000,10000,10000,10000,10000,10000,10000,2,2,2,2,2,2,2]
[null,"Retailer fee - disconnection & reconnection - R/C at Pole Top (non Fee-based)",380049.36363636359,380049.36363636359,380049.36363636359,380049.36363636359,380049.36363636359,380049.36363636359,380049.36363636359,1717,1717,1717,1717,1717,1717,1717]
[null,"Inspection and auditing services",800,800,800,800,800,800,800,2,2,2,2,2,2,2]
[null,"Third party funded network upgrades or other improvements",1000,1000,1000,1000,1000,1000,1000,2,2,2,2,2,2,2]
[null,"Customer requested provision of electricity network or consumption data",0,0,0,0,0,0,0,2,2,2,2,2,2,2]

{"sheet":"5.4 MD & utilisation-Spatial","index":29,"n_rows":11577,"n_cols":12,"rows_kept":11577,"cut":false,"hidden":false,"merged":[[11564,1,11564,2],[11565,1,11565,2],[11566,1,11566,2],[11567,1,11567,2],[11568,1,11568,2],[11569,1,11569,2],[11570,1,11570,2],[11571,1,11571,2],[11572,1,11572,2],[11573,1,11573,2],[11574,1,11574,2],[11575,1,11575,2],[11576,1,11576,2],[11531,1,11531,2],[11532,1,11532,2],[11533,1,11533,2],[11534,1,11534,2],[11535,1,11535,2],[11536,1,11536,2],[11537,1,11537,2],[11538,1,11538,2],[11539,1,11539,2],[11540,1,11540,2],[11541,1,11541,2],[11542,1,11542,2],[11543,1,11543,2],[11544,1,11544,2],[11545,1,11545,2],[11546,1,11546,2],[11547,1,11547,2],[11548,1,11548,2],[11549,1,11549,2],[11550,1,11550,2],[11551,1,11551,2],[11552,1,11552,2],[11553,1,11553,2],[11554,1,11554,2],[11555,1,11555,2],[11556,1,11556,2],[11557,1,11557,2],[11558,1,11558,2],[11559,1,11559,2],[11560,1,11560,2],[11561,1,11561,2],[11562,1,11562,2],[11563,1,11563,2],[11498,1,11498,2],[11499,1,11499,2],[11500,1,11500,2],[11501,1,11501,2],[11502,1,11502,2],[11503,1,11503,2],[11504,1,11504,2],[11505,1,11505,2],[11506,1,11506,2],[11507,1,11507,2],[11508,1,11508,2],[11509,1,11509,2],[11510,1,11510,2],[11511,1,11511,2],[11512,1,11512,2],[11513,1,11513,2],[11514,1,11514,2],[11515,1,11515,2],[11516,1,11516,2],[11517,1,11517,2],[11518,1,11518,2],[11519,1,11519,2],[11520,1,11520,2],[11521,1,11521,2],[11522,1,11522,2],[11523,1,11523,2],[11524,1,11524,2],[11525,1,11525,2],[11526,1,11526,2],[11527,1,11527,2],[11528,1,11528,2],[11529,1,11529,2],[11530,1,11530,2],[11456,1,11456,2],[11457,1,11457,2],[11458,1,11458,2],[11459,1,11459,2],[11460,1,11460,2],[11461,1,11461,2],[11462,1,11462,2],[11463,1,11463,2],[11464,1,11464,2],[11465,1,11465,2],[11466,1,11466,2],[11467,1,11467,2],[11468,1,11468,2],[11469,1,11469,2],[11470,1,11470,2],[11471,1,11471,2],[11472,1,11472,2],[11473,1,11473,2],[11474,1,11474,2],[11475,1,11475,2],[11476,1,11476,2],[11477,1,11477,2],[11478,1,11478,2],[11479,1,11479,2],[11480,1,11480,2],[11481,1,11481,2],[11482,1,11482,2],[11483,1,11483,2],[11484,1,11484,2],[11485,1,11485,2],[11486,1,11486,2],[11487,1,11487,2],[11488,1,11488,2],[11422,1,11422,2],[11423,1,11423,2],[11424,1,11424,2],[11425,1,11425,2],[11426,1,11426,2],[11427,1,11427,2],[11428,1,11428,2],[11429,1,11429,2],[11430,1,11430,2],[11431,1,11431,2],[11432,1,11432,2],[11433,1,11433,2],[11434,1,11434,2],[11435,1,11435,2],[11436,1,11436,2],[11437,1,11437,2],[11438,1,11438,2],[11439,1,11439,2],[11440,1,11440,2],[11441,1,11441,2],[11442,1,11442,2],[11443,1,11443,2],[11444,1,11444,2],[11445,1,11445,2],[11446,1,11446,2],[11447,1,11447,2],[11448,1,11448,2],[11449,1,11449,2],[11450,1,11450,2],[11451,1,11451,2],[11452,1,11452,2],[11453,1,11453,2],[11454,1,11454,2],[11389,1,11389,2],[11390,1,11390,2],[11391,1,11391,2],[11392,1,11392,2],[11393,1,11393,2],[11394,1,11394,2],[11395,1,11395,2],[11396,1,11396,2],[11397,1,11397,2],[11398,1,11398,2],[11399,1,11399,2],[11400,1,11400,2],[11401,1,11401,2],[11402,1,11402,2],[11403,1,11403,2],[11404,1,11404,2],[11405,1,11405,2],[11406,1,11406,2],[11407,1,11407,2],[11408,1,11408,2],[11409,1,11409,2],[11410,1,11410,2],[11411,1,11411,2],[11412,1,11412,2],[11413,1,11413,2],[11414,1,11414,2],[11415,1,11415,2],[11416,1,11416,2],[11417,1,11417,2],[11418,1,11418,2],[11419,1,11419,2],[11420,1,11420,2],[11421,1,11421,2],[11356,1,11356,2],[11357,1,11357,2],[11358,1,11358,2],[11359,1,11359,2],[11360,1,11360,2],[11361,1,11361,2],[11362,1,11362,2],[11363,1,11363,2],[11364,1,11364,2],[11365,1,11365,2],[11366,1,11366,2],[11367,1,11367,2],[11368,1,11368,2],[11369,1,11369,2],[11370,1,11370,2],[11371,1,11371,2],[11372,1,11372,2],[11373,1,11373,2],[11374,1,11374,2],[11375,1,11375,2],[11376,1,11376,2],[11377,1,11377,2],[11378,1,11378,2],[11379,1,11379,2],[11380,1,11380,2],[11381,1,11381,2],[11382,1,11382,2],[11383,1,11383,2],[11384,1,11384,2],[11385,1,11385,2],[11386,1,11386,2],[11387,1,11387,2],[11388,1,11388,2],[11290,1,11290,2],[11291,1,11291,2],[11292,1,11292,2],[11293,1,11293,2],[11294,1,11294,2],[11295,1,11295,2],[11296,1,11296,2],[11297,1,11297,2],[11298,1,11298,2],[11299,1,11299,2],[11300,1,11300,2],[11301,1,11301,2],[11302,1,11302,2],[11303,1,11303,2],[11304,1,11304,2],[11305,1,11305,2],[11306,1,11306,2],[11307,1,11307,2],[11308,1,11308,2],[11309,1,11309,2],[11310,1,11310,2],[11311,1,11311,2],[11312,1,11312,2],[11313,1,11313,2],[11314,1,11314,2],[11315,1,11315,2],[11316,1,11316,2],[11317,1,11317,2],[11318,1,11318,2],[11319,1,11319,2],[11320,1,11320,2],[11321,1,11321,2],[11322,1,11322,2],[11224,1,11224,2],[11225,1,11225,2],[11226,1,11226,2],[11227,1,11227,2],[11228,1,11228,2],[11229,1,11229,2],[11230,1,11230,2],[11231,1,11231,2],[11232,1,11232,2],[11233,1,11233,2],[11234,1,11234,2],[11235,1,11235,2],[11236,1,11236,2],[11237,1,11237,2],[11238,1,11238,2],[11239,1,11239,2],[11207,1,11207,2],[11208,1,11208,2],[11209,1,11209,2],[11210,1,11210,2],[11211,1,11211,2],[11212,1,11212,2],[11213,1,11213,2],[11214,1,11214,2],[11215,1,11215,2],[11216,1,11216,2],[11217,1,11217,2],[11218,1,11218,2],[11219,1,11219,2],[11220,1,11220,2],[11221,1,11221,2],[11222,1,11222,2],[11223,1,11223,2],[11135,1,11135,2],[11136,1,11136,2],[11137,1,11137,2],[11138,1,11138,2],[11139,1,11139,2],[11140,1,11140,2],[11141,1,11141,2],[11142,1,11142,2],[11143,1,11143,2],[11144,1,11144,2],[11145,1,11145,2],[11146,1,11146,2],[11147,1,11147,2],[11148,1,11148,2],[11149,1,11149,2],[11150,1,11150,2],[11151,1,11151,2],[11152,1,11152,2],[11153,1,11153,2],[11154,1,11154,2],[11155,1,11155,2],[11156,1,11156,2],[11157,1,11157,2],[11158,1,11158,2],[11159,1,11159,2],[11160,1,11160,2],[11161,1,11161,2],[11162,1,11162,2],[11163,1,11163,2],[11164,1,11164,2],[11165,1,11165,2],[11166,1,11166,2],[11167,1,11167,2],[11058,1,11058,2],[11059,1,11059,2],[11060,1,11060,2],[11061,1,11061,2],[11062,1,11062,2],[11063,1,11063,2],[11064,1,11064,2],[11065,1,11065,2],[11066,1,11066,2],[11067,1,11067,2],[11068,1,11068,2],[11069,1,11069,2],[11070,1,11070,2],[11071,1,11071,2],[11045,1,11045,2],[11046,1,11046,2],[11047,1,11047,2],[11076,1,11076,2],[11022,1,11022,2],[11023,1,11023,2],[11024,1,11024,2],[11025,1,11025,2],[11026,1,11026,2],[11027,1,11027,2],[11028,1,11028,2],[11029,1,11029,2],[11030,1,11030,2],[11031,1,11031,2],[11032,1,11032,2],[11033,1,11033,2],[11034,1,11034,2],[11035,1,11035,2],[11036,1,11036,2],[11037,1,11037,2],[11038,1,11038,2],[11039,1,11039,2],[11040,1,11040,2],[11041,1,11041,2],[11042,1,11042,2],[11043,1,11043,2],[11044,1,11044,2],[11048,1,11048,2],[11049,1,11049,2],[11050,1,11050,2],[11051,1,11051,2],[11052,1,11052,2],[11053,1,11053,2],[11054,1,11054,2],[11055,1,11055,2],[11056,1,11056,2],[11057,1,11057,2],[5,1,5,2],[9,5,9,6],[5533,2,5534,2],[5533,3,5534,3],[5535,2,5536,2],[5535,3,5536,3],[5527,2,5528,2],[5527,3,5528,3],[5529,2,5530,2],[5529,3,5530,3],[5531,2,5532,2],[5531,3,5532,3],[5521,2,5522,2],[5521,3,5522,3],[5523,2,5524,2],[5523,3,5524,3],[5525,2,5526,2],[5525,3,5526,3],[5515,2,5516,2],[5515,3,5516,3],[5517,2,5518,2],[5517,3,5518,3],[5519,2,5520,2],[5519,3,5520,3],[5491,2,5492,2],[5491,3,5492,3],[5493,2,5494,2],[5493,3,5494,3],[5495,2,5496,2],[5495,3,5496,3],[5485,2,5486,2],[5485,3,5486,3],[5487,2,5488,2],[5487,3,5488,3],[5489,2,5490,2],[5489,3,5490,3],[5479,2,5480,2],[5479,3,5480,3],[5481,2,5482,2],[5481,3,5482,3],[5483,2,5484,2],[5483,3,5484,3],[5509,2,5510,2],[5509,3,5510,3],[5511,2,5512,2],[5511,3,5512,3],[5513,2,5514,2],[5513,3,5514,3],[5503,2,5504,2],[5503,3,5504,3],[5505,2,5506,2],[5505,3,5506,3],[5507,2,5508,2],[5507,3,5508,3],[5497,2,5498,2],[5497,3,5498,3],[5499,2,5500,2],[5499,3,5500,3],[5501,2,5502,2],[5501,3,5502,3],[5455,2,5456,2],[5455,3,5456,3],[5457,2,5458,2],[5457,3,5458,3],[5459,2,5460,2],[5459,3,5460,3],[5449,2,5450,2],[5449,3,5450,3],[5451,2,5452,2],[5451,3,5452,3],[5453,2,5454,2],[5453,3,5454,3],[5443,2,5444,2],[5443,3,5444,3],[5445,2,5446,2],[5445,3,5446,3],[5447,2,5448,2],[5447,3,5448,3],[5473,2,5474,2],[5473,3,5474,3],[5475,2,5476,2],[5475,3,5476,3],[5477,2,5478,2],[5477,3,5478,3],[5467,2,5468,2],[5467,3,5468,3],[5469,2,5470,2],[5469,3,5470,3],[5471,2,5472,2],[5471,3,5472,3],[5461,2,5462,2],[5461,3,5462,3],[5463,2,5464,2],[5463,3,5464,3],[5465,2,5466,2],[5465,3,5466,3],[5419,2,5420,2],[5419,3,5420,3],[5421,2,5422,2],[5421,3,5422,3],[5423,2,5424,2],[5423,3,5424,3],[5413,2,5414,2],[5413,3,5414,3],[5415,2,5416,2],[5415,3,5416,3],[5417,2,5418,2],[5417,3,5418,3],[5407,2,5408,2],[5407,3,5408,3],[5409,2,5410,2],[5409,3,5410,3],[5411,2,5412,2],[5411,3,5412,3],[5437,2,5438,2],[5437,3,5438,3],[5439,2,5440,2],[5439,3,5440,3],[5441,2,5442,2],[5441,3,5442,3],[5431,2,5432,2],[5431,3,5432,3],[5433,2,5434,2],[5433,3,5434,3],[5435,2,5436,2],[5435,3,5436,3],[5425,2,5426,2],[5425,3,5426,3],[5427,2,5428,2],[5427,3,5428,3],[5429,2,5430,2],[5429,3,5430,3],[5383,2,5384,2],[5383,3,5384,3],[5385,2,5386,2],[5385,3,5386,3],[5387,2,5388,2],[5387,3,5388,3],[5377,2,5378,2],[5377,3,5378,3],[5379,2,5380,2],[5379,3,5380,3],[5381,2,5382,2],[5381,3,5382,3],[5371,2,5372,2],[5371,3,5372,3],[5373,2,5374,2],[5373,3,5374,3],[5375,2,5376,2],[5375,3,5376,3],[5401,2,5402,2],[5401,3,5402,3],[5403,2,5404,2],[5403,3,5404,3],[5405,2,5406,2],[5405,3,5406,3],[5395,2,5396,2],[5395,3,5396,3],[5397,2,5398,2],[5397,3,5398,3],[5399,2,5400,2],[5399,3,5400,3],[5389,2,5390,2],[5389,3,5390,3],[5391,2,5392,2],[5391,3,5392,3],[5393,2,5394,2],[5393,3,5394,3],[5347,2,5348,2],[5347,3,5348,3],[5349,2,5350,2],[5349,3,5350,3],[5351,2,5352,2],[5351,3,5352,3],[5341,2,5342,2],[5341,3,5342,3],[5343,2,5344,2],[5343,3,5344,3],[5345,2,5346,2],[5345,3,5346,3],[5335,2,5336,2],[5335,3,5336,3],[5337,2,5338,2],[5337,3,5338,3],[5339,2,5340,2],[5339,3,5340,3],[5365,2,5366,2],[5365,3,5366,3],[5367,2,5368,2],[5367,3,5368,3],[5369,2,5370,2],[5369,3,5370,3],[5359,2,5360,2],[5359,3,5360,3],[5361,2,5362,2],[5361,3,5362,3],[5363,2,5364,2],[5363,3,5364,3],[5353,2,5354,2],[5353,3,5354,3],[5355,2,5356,2],[5355,3,5356,3],[5357,2,5358,2],[5357,3,5358,3],[5311,2,5312,2],[5311,3,5312,3],[5313,2,5314,2],[5313,3,5314,3],[5315,2,5316,2],[5315,3,5316,3],[5305,2,5306,2],[5305,3,5306,3],[5307,2,5308,2],[5307,3,5308,3],[5309,2,5310,2],[5309,3,5310,3],[5299,2,5300,2],[5299,3,5300,3],[5301,2,5302,2],[5301,3,5302,3],[5303,2,5304,2],[5303,3,5304,3],[5329,2,5330,2],[5329,3,5330,3],[5331,2,5332,2],[5331,3,5332,3],[5333,2,5334,2],[5333,3,5334,3],[5323,2,5324,2],[5323,3,5324,3],[5325,2,5326,2],[5325,3,5326,3],[5327,2,5328,2],[5327,3,5328,3],[5317,2,5318,2],[5317,3,5318,3],[5319,2,5320,2],[5319,3,5320,3],[5321,2,5322,2],[5321,3,5322,3],[5275,2,5276,2],[5275,3,5276,3],[5277,2,5278,2],[5277,3,5278,3],[5279,2,5280,2],[5279,3,5280,3],[5269,2,5270,2],[5269,3,5270,3],[5271,2,5272,2],[5271,3,5272,3],[5273,2,5274,2],[5273,3,5274,3],[5263,2,5264,2],[5263,3,5264,3],[5265,2,5266,2],[5265,3,5266,3],[5267,2,5268,2],[5267,3,5268,3],[5293,2,5294,2],[5293,3,5294,3],[5295,2,5296,2],[5295,3,5296,3],[5297,2,5298,2],[5297,3,5298,3],[5287,2,5288,2],[5287,3,5288,3],[5289,2,5290,2],[5289,3,5290,3],[5291,2,5292,2],[5291,3,5292,3],[5281,2,5282,2],[5281,3,5282,3],[5283,2,5284,2],[5283,3,5284,3],[5285,2,5286,2],[5285,3,5286,3],[5239,2,5240,2],[5239,3,5240,3],[5241,2,5242,2],[5241,3,5242,3],[5243,2,5244,2],[5243,3,5244,3],[5233,2,5234,2],[5233,3,5234,3],[5235,2,5236,2],[5235,3,5236,3],[5237,2,5238,2],[5237,3,5238,3],[5227,2,5228,2],[5227,3,5228,3],[5229,2,5230,2],[5229,3,5230,3],[5231,2,5232,2],[5231,3,5232,3],[5257,2,5258,2],[5257,3,5258,3],[5259,2,5260,2],[5259,3,5260,3],[5261,2,5262,2],[5261,3,5262,3],[5251,2,5252,2],[5251,3,5252,3],[5253,2,5254,2],[5253,3,5254,3],[5255,2,5256,2],[5255,3,5256,3],[5245,2,5246,2],[5245,3,5246,3],[5247,2,5248,2],[5247,3,5248,3],[5249,2,5250,2],[5249,3,5250,3],[5203,2,5204,2],[5203,3,5204,3],[5205,2,5206,2],[5205,3,5206,3],[5207,2,5208,2],[5207,3,5208,3],[5197,2,5198,2],[5197,3,5198,3],[5199,2,5200,2],[5199,3,5200,3],[5201,2,5202,2],[5201,3,5202,3],[5191,2,5192,2],[5191,3,5192,3],[5193,2,5194,2],[5193,3,5194,3],[5195,2,5196,2],[5195,3,5196,3],[5221,2,5222,2],[5221,3,5222,3],[5223,2,5224,2],[5223,3,5224,3],[5225,2,5226,2],[5225,3,5226,3],[5215,2,5216,2],[5215,3,5216,3],[5217,2,5218,2],[5217,3,5218,3],[5219,2,5220,2],[5219,3,5220,3],[5209,2,5210,2],[5209,3,5210,3],[5211,2,5212,2],[5211,3,5212,3],[5213,2,5214,2],[5213,3,5214,3],[5167,2,5168,2],[5167,3,5168,3],[5169,2,5170,2],[5169,3,5170,3],[5171,2,5172,2],[5171,3,5172,3],[5161,2,5162,2],[5161,3,5162,3],[5163,2,5164,2],[5163,3,5164,3],[5165,2,5166,2],[5165,3,5166,3],[5155,2,5156,2],[5155,3,5156,3],[5157,2,5158,2],[5157,3,5158,3],[5159,2,5160,2],[5159,3,5160,3],[5185,2,5186,2],[5185,3,5186,3],[5187,2,5188,2],[5187,3,5188,3],[5189,2,5190,2],[5189,3,5190,3],[5179,2,5180,2],[5179,3,5180,3],[5181,2,5182,2],[5181,3,5182,3],[5183,2,5184,2],[5183,3,5184,3],[5173,2,5174,2],[5173,3,5174,3],[5175,2,5176,2],[5175,3,5176,3],[5177,2,5178,2],[5177,3,5178,3],[5131,2,5132,2],[5131,3,5132,3],[5133,2,5134,2],[5133,3,5134,3],[5135,2,5136,2],[5135,3,5136,3],[5125,2,5126,2],[5125,3,5126,3],[5127,2,5128,2],[5127,3,5128,3],[5129,2,5130,2],[5129,3,5130,3],[5119,2,5120,2],[5119,3,5120,3],[5121,2,5122,2],[5121,3,5122,3],[5123,2,5124,2],[5123,3,5124,3],[5149,2,5150,2],[5149,3,5150,3],[5151,2,5152,2],[5151,3,5152,3],[5153,2,5154,2],[5153,3,5154,3],[5143,2,5144,2],[5143,3,5144,3],[5145,2,5146,2],[5145,3,5146,3],[5147,2,5148,2],[5147,3,5148,3],[5137,2,5138,2],[5137,3,5138,3],[5139,2,5140,2],[5139,3,5140,3],[5141,2,5142,2],[5141,3,5142,3],[5095,2,5096,2],[5095,3,5096,3],[5097,2,5098,2],[5097,3,5098,3],[5099,2,5100,2],[5099,3,5100,3],[5089,2,5090,2],[5089,3,5090,3],[5091,2,5092,2],[5091,3,5092,3],[5093,2,5094,2],[5093,3,5094,3],[5083,2,5084,2],[5083,3,5084,3],[5085,2,5086,2],[5085,3,5086,3],[5087,2,5088,2],[5087,3,5088,3],[5113,2,5114,2],[5113,3,5114,3],[5115,2,5116,2],[5115,3,5116,3],[5117,2,5118,2],[5117,3,5118,3],[5107,2,5108,2],[5107,3,5108,3],[5109,2,5110,2],[5109,3,5110,3],[5111,2,5112,2],[5111,3,5112,3],[5101,2,5102,2],[5101,3,5102,3],[5103,2,5104,2],[5103,3,5104,3],[5105,2,5106,2],[5105,3,5106,3],[5059,2,5060,2],[5059,3,5060,3],[5061,2,5062,2],[5061,3,5062,3],[5063,2,5064,2],[5063,3,5064,3],[5053,2,5054,2],[5053,3,5054,3],[5055,2,5056,2],[5055,3,5056,3],[5057,2,5058,2],[5057,3,5058,3],[5047,2,5048,2],[5047,3,5048,3],[5049,2,5050,2],[5049,3,5050,3],[5051,2,5052,2],[5051,3,5052,3],[5077,2,5078,2],[5077,3,5078,3],[5079,2,5080,2],[5079,3,5080,3],[5081,2,5082,2],[5081,3,5082,3],[5071,2,5072,2],[5071,3,5072,3],[5073,2,5074,2],[5073,3,5074,3],[5075,2,5076,2],[5075,3,5076,3],[5065,2,5066,2],[5065,3,5066,3],[5067,2,5068,2],[5067,3,5068,3],[5069,2,5070,2],[5069,3,5070,3],[5023,2,5024,2],[5023,3,5024,3],[5025,2,5026,2],[5025,3,5026,3],[5027,2,5028,2],[5027,3,5028,3],[5017,2,5018,2],[5017,3,5018,3],[5019,2,5020,2],[5019,3,5020,3],[5021,2,5022,2],[5021,3,5022,3],[5011,2,5012,2],[5011,3,5012,3],[5013,2,5014,2],[5013,3,5014,3],[5015,2,5016,2],[5015,3,5016,3],[5041,2,5042,2],[5041,3,5042,3],[5043,2,5044,2],[5043,3,5044,3],[5045,2,5046,2],[5045,3,5046,3],[5035,2,5036,2],[5035,3,5036,3],[5037,2,5038,2],[5037,3,5038,3],[5039,2,5040,2],[5039,3,5040,3],[5029,2,5030,2],[5029,3,5030,3],[5031,2,5032,2],[5031,3,5032,3],[5033,2,5034,2],[5033,3,5034,3],[4987,2,4988,2],[4987,3,4988,3],[4989,2,4990,2],[4989,3,4990,3],[4991,2,4992,2],[4991,3,4992,3],[4981,2,4982,2],[4981,3,4982,3],[4983,2,4984,2],[4983,3,4984,3],[4985,2,4986,2],[4985,3,4986,3],[4975,2,4976,2],[4975,3,4976,3],[4977,2,4978,2],[4977,3,4978,3],[4979,2,4980,2],[4979,3,4980,3],[5005,2,5006,2],[5005,3,5006,3],[5007,2,5008,2],[5007,3,5008,3],[5009,2,5010,2],[5009,3,5010,3],[4999,2,5000,2],[4999,3,5000,3],[5001,2,5002,2],[5001,3,5002,3],[5003,2,5004,2],[5003,3,5004,3],[4993,2,4994,2],[4993,3,4994,3],[4995,2,4996,2],[4995,3,4996,3],[4997,2,4998,2],[4997,3,4998,3],[4951,2,4952,2],[4951,3,4952,3],[4953,2,4954,2],[4953,3,4954,3],[4955,2,4956,2],[4955,3,4956,3],[4945,2,4946,2],[4945,3,4946,3],[4947,2,4948,2],[4947,3,4948,3],[4949,2,4950,2],[4949,3,4950,3],[4939,2,4940,2],[4939,3,4940,3],[4941,2,4942,2],[4941,3,4942,3],[4943,2,4944,2],[4943,3,4944,3],[4969,2,4970,2],[4969,3,4970,3],[4971,2,4972,2],[4971,3,4972,3],[4973,2,4974,2],[4973,3,4974,3],[4963,2,4964,2],[4963,3,4964,3],[4965,2,4966,2],[4965,3,4966,3],[4967,2,4968,2],[4967,3,4968,3],[4957,2,4958,2],[4957,3,4958,3],[4959,2,4960,2],[4959,3,4960,3],[4961,2,4962,2],[4961,3,4962,3],[4915,2,4916,2],[4915,3,4916,3],[4917,2,4918,2],[4917,3,4918,3],[4919,2,4920,2],[4919,3,4920,3],[4909,2,4910,2],[4909,3,4910,3],[4911,2,4912,2],[4911,3,4912,3],[4913,2,4914,2],[4913,3,4914,3],[4903,2,4904,2],[4903,3,4904,3],[4905,2,4906,2],[4905,3,4906,3],[4907,2,4908,2],[4907,3,4908,3],[4933,2,4934,2],[4933,3,4934,3],[4935,2,4936,2],[4935,3,4936,3],[4937,2,4938,2],[4937,3,4938,3],[4927,2,4928,2],[4927,3,4928,3],[4929,2,4930,2],[4929,3,4930,3],[4931,2,4932,2],[4931,3,4932,3],[4921,2,4922,2],[4921,3,4922,3],[4923,2,4924,2],[4923,3,4924,3],[4925,2,4926,2],[4925,3,4926,3],[4879,2,4880,2],[4879,3,4880,3],[4881,2,4882,2]],"merged_total":11560,"flags":["merged_cut"]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Angas Creek 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",10.681639999999998,11.457578319837124,11.659256509594174,11.98636735733912,12.296795089883682,12.598233171766498,12.899171133192317]
[null,null,null,null,"Coincident",10.681639999999998,11.457578319837124,11.659256509594174,11.98636735733912,12.296795089883682,12.598233171766498,12.899171133192317]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.323983301370422,18.471559551100992,18.465983869031824,18.576177055713078,18.68825565920881,18.79951231317273,18.917515910357771]
[null,null,null,null,"Coincident",16.595570373333175,16.729226467510749,16.724176712627418,16.823975907712573,16.925482677341599,17.026245027972081,17.13311791522495]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.952828209942325,19.105469001139827,19.099701972068029,19.213676783260947,19.329601715254636,19.444676489942598,19.566729750351108]
[null,null,null,null,"Coincident",17.1650993759784,17.303342297863733,17.29811924481724,17.401343362020949,17.506333654540001,17.610553980989799,17.721094546274678]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.38843402269125,16.401006381343862,16.413588384859544,16.426180040637337,16.438781356081957,16.451392338603799,16.464012995618948]
[null,null,null,null,"Coincident",14.842592118710332,14.853978587435316,14.865373791269977,14.876777736915438,14.888190431077962,14.899611880468962,14.911042091804994]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.950854492364194,16.963858310901777,16.976872105296131,16.989895883200216,17.002929652272869,17.015973420178788,17.029027194588576]
[null,null,null,null,"Coincident",15.35196217926711,15.363739410347995,15.375525676311218,15.387320984087872,15.399125340614368,15.41093875283244,15.422761227689147]
[null,"Ardrossan West 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.8695400000000015,7.3685588141197371,7.4982614058250974,7.7086318220737082,7.908273049996029,8.1021328843489258,8.2956710829338913]
[null,null,null,null,"Coincident",6.8695400000000015,7.3685588141197371,7.4982614058250974,7.7086318220737082,7.908273049996029,8.1021328843489258,8.2956710829338913]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.923340173918174,10.668934799242898,10.504675802024375,10.414920914209127,10.334366728749805,10.257967419747716,10.185988078567897]
[null,null,null,null,"Coincident",10.923340173918174,10.668934799242898,10.504675802024375,10.414920914209127,10.334366728749805,10.257967419747716,10.185988078567897]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.048799042041574,10.791471721345841,10.62532614478968,10.534540386704482,10.453061004668891,10.37578421948459,10.302978167195448]
[null,null,null,null,"Coincident",11.048799042041574,10.791471721345841,10.62532614478968,10.534540386704482,10.453061004668891,10.37578421948459,10.302978167195448]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.7961477763041138,9.5868642612575456,9.3820518496151344,9.1816150213563645,8.9854602971369228,8.7934961946919863,8.6056331861708877]
[null,null,null,null,"Coincident",9.7961477763041138,9.5868642612575456,9.3820518496151344,9.1816150213563645,8.9854602971369228,8.7934961946919863,8.6056331861708877]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9086603953763657,9.6969731766552254,9.489808413723452,9.2870694894754315,9.088661850919733,8.8944929650816569,8.7044722758478787]
[null,null,null,null,"Coincident",9.9086603953763657,9.6969731766552272,9.489808413723452,9.2870694894754315,9.088661850919733,8.8944929650816569,8.7044722758478787]
[null,"Baroota 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.5617399999999995,4.8931150389578573,4.9792444596593901,5.1189416071565939,5.2515140028428213,5.3802472456452488,5.5087669051876604]
[null,null,null,null,"Coincident",4.5617399999999995,4.8931150389578573,4.9792444596593901,5.1189416071565939,5.2515140028428213,5.3802472456452488,5.5087669051876604]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.2686164778670168,8.2808823163583032,8.2068433926653217,8.2208078321020785,8.2356268264615302,8.2500982605359088,8.2675516915967897]
[null,null,null,null,"Coincident",7.5850225634922808,7.5962743444843728,7.5283564638702245,7.5411664168409356,7.5547602758481318,7.5680353085303311,7.5840458066301641]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.2744244155397464,8.2866988696471573,8.2126079404638599,8.2265821886266721,8.2414115919579078,8.2558931908751418,8.2733588813557279]
[null,null,null,null,"Coincident",7.5903503397185617,7.6016100240452538,7.5336444374069451,7.5464633881838354,7.5600667956186385,7.5733511527824637,7.5893728967751644]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3678529118004441,7.3557258170631821,7.3436186828800363,7.3315314763969948,7.3194641648141205,7.3074167153854646,7.2953890954189751]
[null,null,null,null,"Coincident",6.7587281052506771,6.7476035976068705,6.7364974003120501,6.725409483228356,6.714339816267529,6.7032883693908367,6.6922551126089882]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3730281464492053,7.3608925335504614,7.3487768952262762,7.3366811985995604,7.3246054108473357,7.3125494992006548,7.3005134309445028]
[null,null,null,null,"Coincident",6.7634754861078372,6.7523431645271756,6.7412291661568258,6.7301334608377577,6.719056018460579,6.7079968089654578,6.6969558023420381]
[null,"Berri + Monash 66kV","Substation Rating","MVA","Non-Coincident",160,160,160,160,160,160,160]
[null,null,null,null,"Coincident",160,160,160,160,160,160,160]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",32.430579999999999,34.786410168077509,35.398726316830995,36.391869178475865,37.33436035160144,38.249558001919858,39.163237234046846]
[null,null,null,null,"Coincident",32.430579999999999,34.786410168077509,35.398726316830995,36.391869178475865,37.33436035160144,38.249558001919858,39.163237234046846]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",90.12903852218119,89.835962363380872,90.386034158996694,90.352856999850403,90.36951191039546,90.407120002705625,90.484127749210572]
[null,null,null,null,"Coincident",82.910694142716352,82.641090159790963,83.147107256507397,83.116587222791239,83.131908258240159,83.166504356123212,83.237344629377887]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",92.108708789259182,91.809195258363474,92.371349295134806,92.337443404864956,92.354464137921241,92.392898286110494,92.471597495750856]
[null,null,null,null,"Coincident",84.73181460187601,84.45628880953565,84.973420492820722,84.942230091326451,84.957887650928257,84.993243646702808,85.065639915505344]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",84.469811478743139,84.492407776139771,84.515010118212572,84.537618506578525,84.560232942855066,84.582853428660059,84.605479965611792]
[null,null,null,null,"Coincident",77.704708922234872,77.725495504816124,77.746287647961481,77.767085353158436,77.787888621894879,77.8086974556591,77.829511855939785]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",86.325177706898302,86.348270328441245,86.371369127430725,86.394474105519251,86.417585264359758,86.440702605605665,86.463826130910832]
[null,null,null,null,"Coincident",79.41148072838746,79.432723885011484,79.453972724336552,79.475227247882813,79.496487457170829,79.517753353721602,79.539024939056489]
[null,"Blanche 33kV","Substation Rating","MVA","Non-Coincident",110,110,110,110,110,110,110]
[null,null,null,null,"Coincident",110,110,110,110,110,110,110]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.7032000000000025,9.3354199947954157,9.4997436025086088,9.7662673881907516,10.019198084402367,10.264804181803378,10.510002790432875]
[null,null,null,null,"Coincident",8.7032000000000025,9.3354199947954157,9.4997436025086088,9.7662673881907516,10.019198084402367,10.264804181803378,10.510002790432875]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.325641132066998,36.265693396837051,36.149444691209894,36.154382520187959,36.169714262365225,36.18719063702595,36.218015593640963]
[null,null,null,null,"Coincident",34.057920350456769,34.001715005471148,33.892723421738346,33.897352994150502,33.911727613224912,33.928112980630978,33.95701361072264]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.231999714027573,38.168905939912612,38.046556537623047,38.051753502361841,38.067889849698581,38.086283379178262,38.118726020127269]
[null,null,null,null,"Coincident",35.845269636537459,35.786114652166923,35.671403223318237,35.676275754280432,35.691404748985413,35.708650015482036,35.739067341837888]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.725224071327062,33.871076195986255,34.01755909013189,34.164675481664887,34.31242811028357,34.460819727534691,34.609853096864668]
[null,null,null,null,"Coincident",31.619840956051593,31.75658788989174,31.893926215824614,32.031858491454962,32.170387285448456,32.309515177579527,32.4492447587794]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.495113558017017,35.648619957752338,35.802790229564607,35.957627244514178,36.113133886077883,36.269313050202825,36.426167645360252]
[null,null,null,null,"Coincident",33.279240578143487,33.423163949418971,33.567709748864083,33.712880668305871,33.858679411212805,34.005108692745097,34.152171239805249]
[null,"Brinkworth 33kV","Substation Rating","MVA","Non-Coincident",20,20,20,20,20,20,20]
[null,null,null,null,"Coincident",20,20,20,20,20,20,20]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.6712399999999996,2.8652848730234046,2.9157200915485206,2.9975232211175951,3.075154275551403,3.1505372187931386,3.2257950930595527]
[null,null,null,null,"Coincident",2.6712399999999996,2.8652848730234046,2.9157200915485206,2.9975232211175951,3.075154275551403,3.1505372187931386,3.2257950930595527]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.7508612602694305,4.6848583664920556,4.5731719090722827,4.5478863326654597,4.5237547344208213,4.4929104127781994,4.4404979710673524]
[null,null,null,null,"Coincident",3.837417198160189,3.7841046247479162,3.6938920276997935,3.6734680876069956,3.6539762512746048,3.6290623411743823,3.5867271951450146]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7549485930762776,4.6888889146911641,4.5771063694893064,4.5517990390129945,4.5276466795068115,4.4967758214109343,4.4443182874355998]
[null,null,null,null,"Coincident",3.8407186629574817,3.7873602228658032,3.6970700127519001,3.67662850122609,3.6571198953822899,3.6321845509701562,3.5898129825277207]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2239528729966205,4.1300411743741678,4.0382174268731719,3.9484352088023043,3.8606491305697928,3.7748148117366158,3.6908888585798785]
[null,null,null,null,"Coincident",3.4118170392827101,3.335961663244682,3.2617927897381853,3.1892729225310807,3.1183653990498814,3.0490343718449071,2.9812447904675325]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2275868880112784,4.1335943938560371,4.0416916471599382,3.9518321862934407,3.8639705826145128,3.7780624175020825,3.6940642599001103]
[null,null,null,null,"Coincident",3.4147523453149535,3.3388317082326493,3.2645990246392396,3.1920167660432592,3.1210482383291223,3.0516575632063279,2.983809660071119]
[null,"Clare North 33kV","Substation Rating","MVA","Non-Coincident",80,80,80,80,80,80,80]
[null,null,null,null,"Coincident",80,80,80,80,80,80,80]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.1335000000000006,5.5064089694919405,5.603333691455779,5.7605402193764617,5.9097289923567828,6.0545974201773642,6.1992254946097018]
[null,null,null,null,"Coincident",5.1335000000000006,5.5064089694919405,5.603333691455779,5.7605402193764617,5.9097289923567828,6.0545974201773642,6.1992254946097018]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.868697483690653,11.660627649328907,11.504282021130498,11.395386409851584,11.29270864722667,11.192336622471149,11.096263875196581]
[null,null,null,null,"Coincident",11.012833936201353,10.819768223969021,10.674696834091051,10.573653793349322,10.478380226027994,10.385246127531357,10.296101281352291]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.511693712132731,12.292351527209265,12.127535748903556,12.012740630333091,11.90450021736652,11.798690457472196,11.697412891872911]
[null,null,null,null,"Coincident",11.609463068856138,11.405937866441548,11.253007117381614,11.146489988670542,11.046054899240994,10.947875186079816,10.853900846187818]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.926768789487587,10.754303384878403,10.584560131379035,10.417496063232488,10.253068892842601,10.091237000070128,9.9319594216977674]
[null,null,null,null,"Coincident",10.138828654387085,9.9787999011636845,9.8212970020336137,9.6662800895432248,9.5137099254968653,9.3635478910248064,9.2157559768079782]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.518735273624007,11.3369264170604,11.157987186331555,10.981872287976044,10.80853714343319,10.63793787775924,10.47003130852166]
[null,null,null,null,"Coincident",10.688107848211828,10.519409408621719,10.353373663301198,10.189958584945259,10.029122809597458,9.8708256261797462,9.7150269661876347]
[null,"Dalrymple 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4615100000000005,4.7856041066480932,4.8698411021265944,5.0064688407811975,5.1361283718105986,5.2620331033594061,5.3877289444737757]
[null,null,null,null,"Coincident",4.4615100000000005,4.7856041066480932,4.8698411021265944,5.0064688407811975,5.1361283718105986,5.2620331033594061,5.3877289444737757]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0182573338227581,7.8069632355938161,7.6139048021610813,7.5280441637616295,7.4485953836489518,7.3719399447017269,7.2983111090871979]
[null,null,null,null,"Coincident",8.0182573338227581,7.8069632355938161,7.6139048021610813,7.5280441637616295,7.4485953836489518,7.3719399447017269,7.2983111090871979]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.0193243302692654,7.8080021149517105,7.6149179910660676,7.5290459271171164,7.4495865746864736,7.3729209351336111,7.299282301666171]
[null,null,null,null,"Coincident",8.0193243302692654,7.8080021149517105,7.6149179910660676,7.5290459271171164,7.4495865746864736,7.3729209351336111,7.299282301666171]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1837741647502389,7.0117678328985038,6.8438799738047607,6.6800119758791006,6.5200675886606625,6.3639528662834035,6.2115761122955089]
[null,null,null,null,"Coincident",7.1837741647502389,7.0117678328985038,6.8438799738047607,6.6800119758791006,6.5200675886606625,6.3639528662834035,6.2115761122955089]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.1847301157988497,7.0127008949155938,6.8447906948390651,6.6809008908570258,6.5209352197004824,6.3647997230019353,6.2124026921074433]
[null,null,null,null,"Coincident",7.1847301157988497,7.0127008949155938,6.8447906948390651,6.6809008908570258,6.5209352197004824,6.3647997230019353,6.2124026921074433]
[null,"Davenport West 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.404979999999998,12.23346336200958,12.448798808684,12.798060970329042,13.129510268481393,13.451361154217281,13.772678052306173]
[null,null,null,null,"Coincident",11.404979999999998,12.23346336200958,12.448798808684,12.798060970329042,13.129510268481393,13.451361154217281,13.772678052306173]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.58145363059559,39.425233451896496,39.394111729203367,39.219406524245024,39.059818007058418,38.904926605601347,38.764912121872811]
[null,null,null,null,"Coincident",36.864001506374954,36.718506574414242,36.689521503705429,36.526810629090718,36.378178610851251,36.233921229353157,36.10351939552325]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.769753846053796,39.612790483600449,39.581520706034368,39.405984378802387,39.24563665371879,39.090008389878157,38.949327817488516]
[null,null,null,null,"Coincident",37.039374030362715,36.893186937692292,36.864063976770794,36.700579040318104,36.551239937358609,36.406296282529809,36.275274090144208]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.038143444814281,36.888037551113314,36.738539997281151,36.589648317875643,36.441360057446438,36.293672770494489,36.146584021431714]
[null,null,null,null,"Coincident",34.495301473404233,34.355501052147574,34.216267205379289,34.077597636921382,33.939490059901665,33.801942196716048,33.664951778990975]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.214344411456892,37.063524421391769,36.913315665240972,36.76371566583353,36.614721956037833,36.466332078720882,36.318543586707825]
[null,null,null,null,"Coincident",34.659405418659972,34.518939927098181,34.379043705380496,34.239714446405365,34.100949852421294,33.962747634988979,33.825105514943566]
[null,"Dorrien 33kV","Substation Rating","MVA","Non-Coincident",180,180,180,180,180,180,180]
[null,null,null,null,"Coincident",180,180,180,180,180,180,180]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",21.867959999999997,23.456497728351213,23.869382883297416,24.539059724499005,25.174582101041857,25.791700438402987,26.407794905445623]
[null,null,null,null,"Coincident",21.867959999999997,23.456497728351213,23.869382883297416,24.539059724499005,25.174582101041857,25.791700438402987,26.407794905445623]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.433365485864748,58.647255413537266,59.085644679732454,59.287250187291662,59.509305887493447,59.736756821348635,59.959845107878898]
[null,null,null,null,"Coincident",53.007314840166778,53.201343211509183,53.599024188165906,53.78190885557887,53.983344735829462,54.189674854954099,54.392047436833259]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",62.20032265381122,62.428001179650181,62.894651586974476,63.109253766990989,63.345624478909166,63.587738232858968,63.825208097671478]
[null,null,null,null,"Coincident",56.424476985979929,56.631013563175884,57.054331386061079,57.249005870868444,57.463427488405983,57.683058856136398,57.898477560578705]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.521064518960614,53.685921916810706,53.851287114008031,54.017161674693355,54.183547167825367,54.350445167195517,54.517857251442898]
[null,null,null,null,"Coincident",48.551164115708985,48.700713057805849,48.850722645625417,49.00119429806427,49.152129438389508,49.303529494252246,49.455395897701074]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.971345979722869,57.1468310515287,57.322856658403474,57.499424465321631,57.676536142386141,57.854193364844257,58.032397813103415]
[null,null,null,null,"Coincident",51.681056672078299,51.840246415363083,51.99992650029332,52.160098437235973,52.320763741210271,52.481923931902102,52.643580533678296]
[null,"Hummocks 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.5117000000000012,4.8394400209714217,4.924624645123413,5.0627893849733683,5.1939075279665143,5.3212286316575863,5.4483384949898896]
[null,null,null,null,"Coincident",4.5117000000000012,4.8394400209714217,4.924624645123413,5.0627893849733683,5.1939075279665143,5.3212286316575863,5.4483384949898896]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.107323338589797,14.031984855645739,14.005684835644979,13.941922467504174,13.883883955293058,13.827658998206312,13.776650443352979]
[null,null,null,null,"Coincident",13.189938149779691,13.119498853360353,13.094909097471009,13.035293132636619,12.981028807080559,12.928460102965046,12.880768583640137]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.751815016746548,14.673034702624665,14.645533168798851,14.578857823145587,14.518167827216764,14.459374238499665,14.406035362838569]
[null,null,null,null,"Coincident",13.792519175882763,13.718861867139763,13.693148730672954,13.630809216353033,13.574065830425114,13.519095530236358,13.46922522854531]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.25117668144172,13.201533212321801,13.152075724725297,13.102803521901404,13.053715909709586,13.004812196609796,12.956091693652734]
[null,null,null,null,"Coincident",12.389465857205682,12.343050653448278,12.296809337021019,12.250741256482113,12.204845762830292,12.159122209495667,12.113569952330627]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.856555383836138,13.804643957715822,13.752927009666513,13.701403811106415,13.650073636183246,13.598935761764025,13.54798946742487]
[null,null,null,null,"Coincident",12.955477385412028,12.906941707639559,12.858587861222798,12.810415164958897,12.76242294019703,12.714610510828827,12.666977203278856]
[null,"Kadina East 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",13.34915,14.318862237283204,14.57090522008316,14.97970497116768,15.36765535761557,15.744371121371509,16.120461870335848]
[null,null,null,null,"Coincident",13.34915,14.318862237283204,14.57090522008316,14.97970497116768,15.36765535761557,15.744371121371509,16.120461870335848]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.662291923649811,25.480272976956925,25.563157186450503,25.726067271171399,25.907187205031381,26.095539674338607,26.293755575477991]
[null,null,null,null,"Coincident",25.048885318437048,24.87121717659462,24.952120202111239,25.111136241735895,25.287926859878638,25.471777133936705,25.665255073892464]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.90871140474685,26.717851783894318,26.804761685781056,26.975584325774388,27.165501268671978,27.363002031816549,27.570845294431614]
[null,null,null,null,"Coincident",26.26551159381242,26.079214096734631,26.164046588387151,26.330786049216147,26.516163401201055,26.708943297128936,26.911818475423377]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.302127772480219,23.367344654487813,23.432744062389194,23.498326507029113,23.564092500682047,23.63004255705621,23.696177191297551]
[null,null,null,null,"Coincident",22.745136248353006,22.808794249091779,22.872630412801914,22.936645238117425,23.000839225067875,23.065212875082292,23.129766690993076]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.433913900275964,24.502298371229728,24.570874233373896,24.639642022364988,24.708602275358693,24.777755531014073,24.847102329497758]
[null,null,null,null,"Coincident",23.849869255229407,23.916619129931917,23.98355582099493,24.050679851271152,24.117991745076623,24.185492028194819,24.253181227880745]
[null,"Kanmantoo Mine 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.03424,1.1093695164327153,1.1288968222560094,1.16056903019147,1.1906259107928465,1.2198123767106723,1.248950418923763]
[null,null,null,null,"Coincident",1.03424,1.1093695164327153,1.1288968222560094,1.16056903019147,1.1906259107928465,1.2198123767106723,1.248950418923763]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6263933203679442,1.6193080810919136,1.6274620874637833,1.6415387278483693,1.6566252136121893,1.6720885681976754,1.688174301759821]
[null,null,null,null,"Coincident",1.5333097558563997,1.5266300269319986,1.5343173540765018,1.547588344408954,1.5618113835185961,1.5763897220713077,1.5915548189098538]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6455280176819302,1.6383594197820992,1.6466093589408712,1.6608516125566379,1.676115592494227,1.6917608751568558,1.7080358591536475]
[null,null,null,null,"Coincident",1.5513493147376773,1.5445909980636172,1.5523687674622921,1.5657958924639466,1.5801862672019631,1.5949361215202977,1.6102796374006025]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4291623627308816,1.4333368835414149,1.4375235979448189,1.4417225415580459,1.4459337501020832,1.4501572594022578,1.4543931053885411]
[null,null,null,null,"Coincident",1.3473669413388194,1.3513025412977322,1.3552496369721485,1.3592082619405512,1.3631784498795041,1.3671602345639389,1.3711536498674424]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4459766160120067,1.4502002505216312,1.4544362220830953,1.4586845667323887,1.4629453206107599,1.4672185199650252,1.4715042011478756]
[null,null,null,null,"Coincident",1.3632188624396493,1.3672007651674063,1.3711942988590313,1.3751994974880617,1.3792163951272698,1.3832450259489533,1.3872854242252251]
[null,"Keith 33kV","Substation Rating","MVA","Non-Coincident",51,51,51,51,51,51,51]
[null,null,null,null,"Coincident",51,51,51,51,51,51,51]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.5700099999999999,5.9746280362637183,6.0797944277287614,6.2503684868664804,6.4122430280933465,6.5694298580621631,6.7263558969963917]
[null,null,null,null,"Coincident",5.5700099999999999,5.9746280362637183,6.0797944277287614,6.2503684868664804,6.4122430280933465,6.5694298580621631,6.7263558969963917]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.522312811125033,22.786403290638873,22.878005938216457,22.991217835437432,23.105630875515232,23.148183936734206,23.160681573409811]
[null,null,null,null,"Coincident",21.104306685577914,21.35177001312962,21.437605352683793,21.543689422265999,21.650899010680849,21.690772928688585,21.702483713431644]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.374450194261787,24.660258330116697,24.759393982381479,24.881915935315526,25.005737807888615,25.051790248416967,25.065315636562055]
[null,null,null,null,"Coincident",22.839833391264818,23.107647030250238,23.200541096078027,23.315349059723701,23.431375099992277,23.474528076184381,23.48720190510458]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.208201846900522,20.257441805171485,20.306801743117479,20.35628195308486,20.405882728132326,20.455604362032648,20.505447149274421]
[null,null,null,null,"Coincident",18.935892282358683,18.982032089990792,19.028284323370606,19.074649256438342,19.121127163801702,19.167718320737507,19.214423003193332]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.870036774800543,21.923326013810236,21.976745099103383,22.030294347067642,22.083974074861587,22.137784600416587,22.191726242438698]
[null,null,null,null,"Coincident",20.493097986467511,20.543032131887344,20.593087948461065,20.643265732656548,20.693565781664045,20.743988393397945,20.794533866498558]
[null,"Kincraig 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.2241800000000005,7.7489606602170618,7.8853591481720091,8.1065899370828962,8.3165376433240521,8.5204054915548681,8.7239350995713494]
[null,null,null,null,"Coincident",7.2241800000000005,7.7489606602170618,7.8853591481720091,8.1065899370828962,8.3165376433240521,8.5204054915548681,8.7239350995713494]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.876951232148709,19.895966520609953,19.740416410083839,19.726964145407557,19.614869284106426,19.505200929494851,19.397815829848003]
[null,null,null,null,"Coincident",19.876951232148709,19.895966520609953,19.740416410083839,19.726964145407557,19.614869284106426,19.505200929494851,19.397815829848003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.624427789365097,20.644158151390062,20.482758549172154,20.468800409506816,20.352490199482009,20.238697745395456,20.127274408513788]
[null,null,null,null,"Coincident",20.6244277893651,20.644158151390066,20.482758549172154,20.468800409506819,20.352490199482013,20.238697745395459,20.127274408513792]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.915239432732022,17.746819598193731,17.579983066003837,17.414714951654624,17.251000510566527,17.08882513677268,16.928174361615827]
[null,null,null,null,"Coincident",17.915239432732022,17.746819598193731,17.579983066003837,17.414714951654624,17.251000510566527,17.08882513677268,16.928174361615827]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.58894544209361,18.414192147427691,18.24108169549816,18.06959864206253,17.899727688068513,17.731453678289046,17.564761599970261]
[null,null,null,null,"Coincident",18.588945442093614,18.414192147427695,18.24108169549816,18.069598642062534,17.899727688068513,17.73145367828905,17.564761599970264]
[null,"Leigh Creek South 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.35375000000000001,0.37944719449844627,0.38612628681259992,0.39695940442279598,0.40724001773569918,0.41722291563022157,0.4271892507486475]
[null,null,null,null,"Coincident",0.35375000000000001,0.37944719449844627,0.38612628681259992,0.39695940442279598,0.40724001773569918,0.41722291563022157,0.4271892507486475]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1277777994169662,1.1112180757681416,1.0866661827028088,1.0805191916555834,1.0747080043345376,1.0689722058802518,1.0636341067443804]
[null,null,null,null,"Coincident",1.016228582970248,1.0013067920760454,0.97918334230436255,0.97364435403496941,0.96840795493250964,0.96323948793624914,0.95842938356692597]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1338178461061925,1.1171694334407449,1.0924860476465252,1.0863061351204919,1.0804638247867773,1.0746973070804526,1.0693306186532963]
[null,null,null,null,"Coincident",1.0216712048158276,0.50199049177092858,0.32697506529074799,0.24373569421545865,0.19388816624559366,0.16068257870636557,0.13702276112393114]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0459400880958896,1.0421631125104414,1.038399775894123,1.0346500289954963,1.0309138227409742,1.0271911082341785,1.0234818367552998]
[null,null,null,null,"Coincident",0.94248549150990835,0.93908209897185912,0.93569099636386455,0.93231213930597734,0.92894548357851003,0.92559098512145621,0.92224860003391362]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0515418360372826,1.0477446320798165,1.0439611401377935,1.0401913106959988,1.0364350944180223,1.0326924421456103,1.0289633048980253]
[null,null,null,null,"Coincident",0.94753316701441037,0.47079505343089451,0.31245182736466631,0.23338886068360062,0.18598725406558222,0.15440225217025583,0.13185014126865263]
[null,"Mannum 33kV","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident",40,40,40,40,40,40,40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.8667699999999998,6.2929453491664997,6.4037148146531635,6.5833767493583784,6.7538756716643604,6.9194371299842112,7.0847239027975757]
[null,null,null,null,"Coincident",5.8667699999999998,6.2929453491664997,6.4037148146531635,6.5833767493583784,6.7538756716643604,6.9194371299842112,7.0847239027975757]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.791013918881159,13.735573338441585,13.736322950787681,13.802090389894353,13.874399465773532,13.948856136438391,14.028477441283691]
[null,null,null,null,"Coincident",12.956019468317674,12.903935608223344,12.904639834338033,12.966425300327655,13.034356331384341,13.104304928373233,13.179105460207682]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.188692427214999,14.131653158857333,14.132424387070207,14.200088300013736,14.274482484761906,14.351086192468395,14.433003462057748]
[null,null,null,null,"Coincident",13.329620026362996,13.276034272940704,13.27675880616207,13.340325921571813,13.410215815933192,13.482181454879566,13.559138939357052]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.365265496263698,12.410697304633889,12.456296036165771,12.502062304159649,12.547996724169183,12.594099914009668,12.640372493766343]
[null,null,null,null,"Coincident",11.616594794467904,11.659275876307666,11.702113774734324,11.745109065915136,11.788262328134284,11.831574141800653,11.875045089455631]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.721831037175354,12.768572919909175,12.815486539211033,12.862572526066401,12.909831513779078,12.957264137979724,13.004871036634388]
[null,null,null,null,"Coincident",11.95157162191189,11.995483457999306,12.039556632646166,12.083791738634122,12.128189370922795,12.172750126657773,12.217474605178646]
[null,"Mobilong 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",13.495029999999998,14.475339288119763,14.730136605864704,15.143403735597916,15.535593658074319,15.916426185490621,16.296626867930794]
[null,null,null,null,"Coincident",13.495029999999998,14.475339288119763,14.730136605864704,15.143403735597916,15.535593658074319,15.916426185490621,16.296626867930794]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.374355157254115,41.817503144148205,42.194588595855471,42.501112840981335,42.711963844237218,42.92702050506746,43.157939342505308]
[null,null,null,null,"Coincident",39.978909246692098,40.407111041827193,40.771478413711399,41.0676644190575,41.271403984102129,41.479207361183192,41.702337926244354]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.348811062606416,44.823817531440639,45.228012143988963,45.556572813551732,45.782582168143847,46.0130995304729,46.26061942180182]
[null,null,null,null,"Coincident",42.853044740681,43.312030516699451,43.702592730216828,44.020071930570701,44.23845859646071,44.461201227090541,44.700372937068359]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.596465226552766,37.885129925794459,38.176010985220181,38.469125421986782,38.764490383908417,39.062123150459712,39.362041133786661]
[null,null,null,null,"Coincident",36.328437399833106,36.607366213825365,36.888436636123501,37.171665109941365,37.457068204743372,37.744662617213869,38.034465172233915]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.299323738509187,40.608740916334838,40.920533791344766,41.23472060408124,41.551319735136936,41.870349706230279,42.191829181288938]
[null,null,null,null,"Coincident",38.940135751274589,39.239117118467952,39.540394056958228,39.843984192083191,40.149905284507469,40.458175231261649,40.768812066789259]
[null,"Mount Barker + Mount Barker South 66kV","Substation Rating","MVA","Non-Coincident",345,345,345,345,345,345,345]
[null,null,null,null,"Coincident",345,345,345,345,345,345,345]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",52.208250000000014,56.000774536179534,56.986509437410383,58.585316822491706,60.102582773003022,61.575910346152703,63.046793499358529]
[null,null,null,null,"Coincident",52.208250000000014,56.000774536179534,56.986509437410383,58.585316822491706,60.102582773003022,61.575910346152703,63.046793499358529]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",91.707078572385598,92.756150736850245,92.971961420802842,94.173031367067495,95.385958292226192,96.5954536036094,97.839191474267878]
[null,null,null,null,"Coincident",91.707078572385598,92.756150736850245,92.971961420802842,94.173031367067495,95.385958292226192,96.5954536036094,97.839191474267878]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",92.000200742357592,93.052626042851557,93.269126519751097,94.474035430623687,95.690839218701313,96.904200424579926,98.151913638790944]
[null,null,null,null,"Coincident",92.000200742357592,93.052626042851557,93.269126519751097,94.474035430623687,95.690839218701313,96.904200424579926,98.151913638790944]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",79.480693939445615,79.585525966234457,79.690496262498513,79.795605010609989,79.900852393181623,80.006238593067039,80.111763793360993]
[null,null,null,null,"Coincident",79.480693939445615,79.585525966234457,79.690496262498513,79.795605010609989,79.900852393181623,80.006238593067039,80.111763793360993]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",79.734737071568958,79.83990417163298,79.945209983121188,80.050654688988701,80.156238472431923,80.261961516888945,80.367824006039768]
[null,null,null,null,"Coincident",79.734737071568958,79.83990417163298,79.945209983121188,80.050654688988701,80.156238472431923,80.26196151688896,80.367824006039768]
[null,"Mount Gambier 33kV","Substation Rating","MVA","Non-Coincident",66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994]
[null,null,null,null,"Coincident",66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994,66.099999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.9063399999999993,6.3353898028380291,6.4469063826225614,6.6277800953174175,6.7994289932242236,6.9661071250979578,7.1325087187753109]
[null,null,null,null,"Coincident",5.9063399999999993,6.3353898028380291,6.4469063826225614,6.6277800953174175,6.7994289932242236,6.9661071250979578,7.1325087187753109]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.26798033759804,24.604260767695965,24.740402343679321,24.915113297780806,25.092415506367448,25.203577056666074,25.316518849061406]
[null,null,null,null,"Coincident",19.66403552380347,22.748707215869988,22.87458154638508,23.036116508958642,23.200047304114264,23.302825501162385,23.407249681668972]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.820579271828176,25.243545178435863,25.38322407618643,25.562474487514333,25.74438348103995,25.858433305318865,25.974309627139043]
[null,null,null,null,"Coincident",20.174959687764048,23.33977938929964,23.468924271121693,23.634656343469764,23.802846498529458,23.908295147649159,24.015432547273868]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.28602873861492,23.441692437350291,23.621570943707177,23.80282973764934,23.98547941073581,24.169530635799347,24.354994167570094]
[null,null,null,null,"Coincident",18.756138731604331,21.673815073603315,21.840127872600853,22.007716863492451,22.176591839064724,22.346762667248672,22.518239291696307]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.81311394758999,24.050770217741608,24.235322448134621,24.421290829671015,24.608686229106809,24.79751959658347,24.98780196626775]
[null,null,null,null,"Coincident",19.243473311984502,22.236958678226699,22.407592727950259,22.579536128441895,22.752798926930968,22.927391247743685,23.103323292894697]
[null,"Mount Gunson 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.15958083255336933,0.16174620889354657,0.16353069103837467,0.16343557676919246,0.16334912637102544,0.16325286689423199,0.16321606374670838]
[null,null,null,null,"Coincident",8.4108969734958836E-2,8.5250257007036798E-2,8.619078947770005E-2,8.6140658374484175E-2,8.6095093667202846E-2,8.6044358968738258E-2,8.6024961433509961E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.21036210482163167,0.21321653988981762,0.21556887390134194,0.21544349269143348,0.2153295323402428,0.21520264149863419,0.21515412697810407]
[null,null,null,null,"Coincident",0.11087384132995794,0.11237830517388585,0.11361813070315574,0.11355204704999523,0.11349198289582385,0.11342510357337808,0.11339953342016051]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.1425867746550363,0.14383363070568958,0.14509138994154228,0.14636014770595615,0.14764000017602699,0.14893104436987523,0.15023337815400037]
[null,null,null,null,"Coincident",7.5152050043698265E-2,7.580922030750907E-2,7.6472137224343803E-2,7.7140851046051631E-2,7.7815412463911132E-2,7.84958726124729E-2,7.9182283073435764E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.18796025535290906,0.18960388171472348,0.19126188083641832,0.19293437840119718,0.19462150119130561,0.19632337709764186,0.19804013512945162]
[null,null,null,null,"Coincident",9.9066680978530691E-2,9.9932973738816891E-2,0.10080684183259678,0.10168835150269284,0.10257756957119071,0.10347456344450455,0.10437940111848676]
[null,"Neuroodla 33kV","Substation Rating","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",10,10,10,10,10,10,10]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.32973000000000002,0.35368232775115954,0.35990790261687228,0.37000544005746577,0.37958798882824618,0.38889303737315323,0.39818264777201845]
[null,null,null,null,"Coincident",0.32973000000000002,0.35368232775115954,0.35990790261687228,0.37000544005746577,0.37958798882824618,0.38889303737315323,0.39818264777201845]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.93444754324040469,0.93675944293518942,0.92947551844966192,0.92853581712000877,0.92765231388967939,0.92454928032272954,0.92136719324764149]
[null,null,null,null,"Coincident",0.81516762691557332,0.81718441833580568,0.81083026878460707,0.81001051800411228,0.80923979177464156,0.80653285276312858,0.80375695122814983]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.93852805650999449,0.94085005172854708,0.93353432005305692,0.93259051526808112,0.93170315398634884,0.9285865701995526,0.92539058769648808]
[null,null,null,null,"Coincident",0.81872727276474999,0.82075287104012551,0.81437097440804673,0.81354764396814594,0.81277355215798608,0.81005479257865587,0.80726676933269348]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.80731906706405243,0.80047749239907839,0.79369389622836517,0.78696778721680916,0.78029867819309517,0.77368608611441081,0.7671295320314595]
[null,null,null,null,"Coincident",0.70426678610571203,0.69829852151520011,0.69238083460764166,0.68651329676564321,0.68069548300410221,0.67492697193942597,0.6692073457590102]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.81084444009304457,0.80397298987603216,0.79715977133176741,0.79040429097960174,0.78370605952085703,0.77706459180338638,0.77047940678643356]
[null,null,null,null,"Coincident",0.70734215399214284,0.70134782738987422,0.69540429933143866,0.68951113932777119,0.683667920537959,0.67787421973832607,0.67212961729177845]
[null,"North West Bend 66kV","Substation Rating","MVA","Non-Coincident",65,65,65,65,65,65,65]
[null,null,null,null,"Coincident",65,65,65,65,65,65,65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.7264400000000002,9.360348200590872,9.5251105987079683,9.7923460781095777,10.04595217065587,10.292214105645767,10.538067463754139]
[null,null,null,null,"Coincident",8.7264400000000002,9.360348200590872,9.5251105987079683,9.7923460781095777,10.04595217065587,10.292214105645767,10.538067463754139]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.716450512963686,27.897504655275302,27.987063585920367,27.967144482952719,27.950977162572975,27.934302978046283,27.927922928232984]
[null,null,null,null,"Coincident",20.198235411563044,20.330177782283933,20.395443439714736,20.380927485345342,20.369145625223986,20.356994390194505,20.35234495833431]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.53986423227034,29.732829589795962,29.828280435884828,29.807050892187746,29.789819953875718,29.772048805767415,29.765249024345483]
[null,null,null,null,"Coincident",21.527039745220534,21.667662359063382,21.737221722685145,21.721750790681309,21.709193823899952,21.696243181722394,21.691287872389296]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.601239078726575,25.627505077854025,25.653798025001766,25.68011794781755,25.706464873977492,25.7328388311861,25.759239847176314]
[null,null,null,null,"Coincident",18.65678483967368,18.675926065331275,18.6950869292343,18.71426745153093,18.733467652390008,18.752687552001063,18.771927170574351]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.285496972628447,27.313490962976772,27.341513674205515,27.369565135781322,27.397645377201062,27.425754427991876,27.453892317711205]
[null,null,null,null,"Coincident",19.884180007713027,19.904580498998886,19.925001920493809,19.945444293671478,19.965907640027616,19.986391981079976,20.006897338368415]
[null,"Penola West 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.5407,1.6526199083074378,1.6817095974337035,1.7288914611850223,1.7736669832519905,1.8171458547321055,1.8605525897623778]
[null,null,null,null,"Coincident",1.5407,1.6526199083074378,1.6817095974337035,1.7288914611850223,1.7736669832519905,1.8171458547321055,1.8605525897623778]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7336596391327994,8.8193786755684993,8.8445382333319582,8.8572140449571215,8.8703729080326994,8.8829908904737156,8.8988758184145578]
[null,null,null,null,"Coincident",7.4051378526868987,7.4778177266038623,7.4991501349239966,7.50989776379408,7.5210549646795677,7.5317535610594684,7.5452221510941513]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.280161491527096,9.3712443289503753,9.3979782261650229,9.4114472166888365,9.4254294852259672,9.4388370279501217,9.4557159427078901]
[null,null,null,null,"Coincident",7.8685085038164111,7.9457362634271833,7.9684035303455101,7.9798236836015946,7.9916790375183879,8.0030470901149524,8.0173584665309718]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3450155221265181,8.4349908023900824,8.5259361888250549,8.6178621410374632,8.7107792314079582,8.8046981463077412,8.899629687327602]
[null,null,null,null,"Coincident",7.0756123867330807,7.1519010653873805,7.229012282385038,7.3069549062677321,7.3857379011970377,7.4653703279853936,7.5458613451381842]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8671982759250323,8.962803688271304,9.0594399104162822,9.1571180564675831,9.255849360364218,9.3556451771686326,9.4565169843726178]
[null,null,null,null,"Coincident",7.5183632421531357,7.599425624606754,7.6813620150907678,7.7641818370888434,7.8478946156878857,7.9325099786735143,8.0180376576373504]
[null,"Port Lincoln Terminal 33kV","Substation Rating","MVA","Non-Coincident",75,75,75,75,75,75,75]
[null,null,null,null,"Coincident",75,75,75,75,75,75,75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",15.195440000000001,16.299270889525005,16.58617335316934,17.051513250437687,17.493120155764672,17.921938603771292,18.350045592638949]
[null,null,null,null,"Coincident",15.195440000000001,16.299270889525005,16.58617335316934,17.051513250437687,17.493120155764672,17.921938603771292,18.350045592638949]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.378033538578325,29.643913462574218,29.194993176542244,28.996080404608811,28.818696193007138,28.650134538436919,28.492668273626023]
[null,null,null,null,"Coincident",29.94156205870199,29.217989817388155,28.775519616459352,28.579464822538942,28.404629266670568,28.23848950536501,28.083285715297428]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.620996726363458,29.881005165832331,29.428494420147423,29.227990745988578,29.04918781735709,28.879278008473964,28.720552330158949]
[null,null,null,null,"Coincident",30.181034352252858,29.451674987881201,29.005665915011228,28.808043076943029,28.631809188166173,28.464340642824173,28.307895534501302]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.480115001548004,27.07043018706279,26.666853121661244,26.269292748517362,25.877659368317612,25.491864619022586,25.111821455930361]
[null,null,null,null,"Coincident",27.085280805099263,26.681482340598951,26.283703869064787,25.891855641974928,25.50584924881526,25.125597597131851,24.75101489288075]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.699900667825553,27.286939198569776,26.880134328109602,26.479394271347509,26.084628611555811,25.695748279976453,25.312665535724918]
[null,null,null,null,"Coincident",27.30190859169069,26.894880551384123,26.493920651883155,26.098938426858215,25.709844758688845,25.326551858356599,24.948973245637674]
[null,"Snuggery Industrial 33kV","Substation Rating","MVA","Non-Coincident",75,75,75,75,75,75,75]
[null,null,null,null,"Coincident",75,75,75,75,75,75,75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698]
[null,null,null,null,"Coincident",-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7,7,7,7,7,7,7]
[null,null,null,null,"Coincident",-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398,-10.225663327006398]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698,7.0040327589591698]
[null,null,null,null,"Coincident",-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176,-10.231554417777176]
[null,"Snuggery Rural 33kV","Substation Rating","MVA","Non-Coincident",25,25,25,25,25,25,25]
[null,null,null,null,"Coincident",25,25,25,25,25,25,25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.5057399999999985,6.9783315650496709,7.1011653121362635,7.3003948430517598,7.4894633865267757,7.6730567099142251,7.8563454308565523]
[null,null,null,null,"Coincident",6.5057399999999985,6.9783315650496709,7.1011653121362635,7.3003948430517598,7.4894633865267757,7.6730567099142251,7.8563454308565523]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.51773590287195,14.532228503070678,14.380635588209342,14.438388603167917,14.497879638275501,14.556848385422949,14.621055233498421]
[null,null,null,null,"Coincident",14.51773590287195,14.532228503070678,14.380635588209342,14.438388603167917,14.497879638275501,14.556848385422949,14.621055233498421]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.973095397745322,14.988042569039024,14.831694830588152,14.891259311459518,14.952616326763829,15.013434672160894,15.079655415385215]
[null,null,null,null,"Coincident",14.973095397745322,14.988042569039024,14.831694830588152,14.891259311459518,14.952616326763829,15.013434672160894,15.079655415385215]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.201947869128841,13.156055822704975,13.110323304249698,13.06474975921871,13.019334634995392,12.974077380884111,12.928977448103538]
[null,null,null,null,"Coincident",13.201947869128841,13.156055822704975,13.110323304249698,13.06474975921871,13.019334634995392,12.974077380884111,12.928977448103538]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.616036701798807,13.56870521748889,13.521538264859966,13.474535271974041,13.427695668881269,13.381018887613044,13.334504362175105]
[null,null,null,null,"Coincident",13.616036701798807,13.56870521748889,13.521538264859966,13.474535271974041,13.427695668881269,13.381018887613044,13.334504362175105]
[null,"Stony Point 11kV","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",30,30,30,30,30,30,30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.8459999999999998E-2,6.2706665697184916E-2,6.3810438804422859E-2,6.5600697618534695E-2,6.7299650704816874E-2,6.8949403951216251E-2,7.0596420067182836E-2]
[null,null,null,null,"Coincident",5.8459999999999998E-2,6.2706665697184916E-2,6.3810438804422859E-2,6.5600697618534695E-2,6.7299650704816874E-2,6.8949403951216251E-2,7.0596420067182836E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.2,0.2,0.2,0.2,0.2,0.2,0.2]
[null,null,null,null,"Coincident",0.14715622750179988,0.14715622750179988,0.14715622750179988,0.14715622750179988,0.14715622750179988,0.14715622750179988,0.14715622750179988]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.222,0.222,0.222,0.222,0.222,0.222,0.222]
[null,null,null,null,"Coincident",0.1635069194464443,0.1635069194464443,0.1635069194464443,0.1635069194464443,0.1635069194464443,0.1635069194464443,0.1635069194464443]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.13495671234259277,0.13495671234259277,0.13495671234259277,0.13495671234259277,0.13495671234259277,0.13495671234259277,0.13495671234259277]
[null,null,null,null,"Coincident",9.9298603321907708E-2,9.9298603321907708E-2,9.9298603321907708E-2,9.9298603321907708E-2,9.9298603321907708E-2,9.9298603321907708E-2,9.9298603321907708E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.14799999999999999,0.14799999999999999,0.14799999999999999,0.14799999999999999,0.14799999999999999,0.14799999999999999,0.14799999999999999]
[null,null,null,null,"Coincident",0.11033178146878633,0.11033178146878633,0.11033178146878633,0.11033178146878633,0.11033178146878633,0.11033178146878633,0.11033178146878633]
[null,"Tailem Bend 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.2998899999999987,7.8301704046565712,7.9679983599729445,8.1915476657298179,8.403695641183468,8.6097000412152571,8.8153626562474727]
[null,null,null,null,"Coincident",7.2998899999999987,7.8301704046565712,7.9679983599729445,8.1915476657298179,8.403695641183468,8.6097000412152571,8.8153626562474727]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.748266432499157,24.590974045472564,24.469382419321359,24.363243813152192,24.265870906163045,24.163041041062506,24.068384326543551]
[null,null,null,null,"Coincident",24.748266432499157,24.590974045472564,24.469382419321359,24.363243813152192,24.265870906163045,24.163041041062506,24.068384326543551]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.085367522673277,24.92593262456263,24.802684774536377,24.695100433170087,24.596401190326709,24.492170659053354,24.396224606481422]
[null,null,null,null,"Coincident",25.085367522673277,24.92593262456263,24.802684774536377,24.695100433170087,24.596401190326709,24.492170659053354,24.396224606481422]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.736954247535927,22.613869831473952,22.491451721607277,22.369696310948431,22.248600012036047,22.12815925682915,22.008370496602026]
[null,null,null,null,"Coincident",22.736954247535927,22.613869831473952,22.491451721607277,22.369696310948431,22.248600012036047,22.12815925682915,22.008370496602026]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.046658851896346,22.921897878369183,22.797812286927361,22.674398421451905,22.551652645615924,22.429571342777443,22.30815091587284]
[null,null,null,null,"Coincident",23.04665885189635,22.921897878369183,22.797812286927357,22.674398421451905,22.551652645615924,22.429571342777443,22.308150915872844]
[null,"Templers 33kV","Substation Rating","MVA","Non-Coincident",120,120,120,120,120,120,120]
[null,null,null,null,"Coincident",120,120,120,120,120,120,120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",13.45063,14.427713972400385,14.681672981456284,15.09358042095093,15.484479999311171,15.864059549578309,16.24300933370256]
[null,null,null,null,"Coincident",13.45063,14.427713972400385,14.681672981456284,15.09358042095093,15.484479999311171,15.864059549578309,16.24300933370256]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.297713481710147,30.599900064875474,30.726247107563335,30.816506499357288,30.717585596452974,30.624621237387547,30.543329066262039]
[null,null,null,null,"Coincident",28.58850628101677,28.873645390147104,28.992864724162207,29.078032246482987,28.984691841250392,28.896971948966872,28.820265772897773]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.375578523917014,31.688515633006165,31.819357571342891,31.912828012155586,31.810387920146507,31.714116280719207,31.629932076519513]
[null,null,null,null,"Coincident",29.605564929611528,29.900848087337582,30.02430874314641,30.112506167215269,30.015845103481944,29.925004506876771,29.845569448122973]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.14162705029058,26.999037006240307,26.857196066900102,26.716100296806793,26.575745781172387,26.436128625775446,26.297244956853039]
[null,null,null,null,"Coincident",25.610466475387941,25.475920468396275,25.34208130631955,25.208945275708775,25.076508682623768,24.944767852530678,24.813719130200006]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.107211829610144,27.959549032332426,27.812661989755391,27.666546626408664,27.521198888232579,27.376614742465701,27.23279017753293]
[null,null,null,null,"Coincident",26.521579010170331,26.38224642291107,26.243645827131836,26.105773377274765,25.968625247984839,25.832197634003769,25.696486750064391]
[null,"Waterloo 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4399299999999995,4.7624564869808799,4.8462860342271847,4.9822529144279981,5.1112852917180565,5.2365810312200409,5.361668890675455]
[null,null,null,null,"Coincident",4.4399299999999995,4.7624564869808799,4.8462860342271847,4.9822529144279981,5.1112852917180565,5.2365810312200409,5.361668890675455]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.5812435584325932,8.3862787153216427,8.2412315558397662,8.174832749457801,8.1136819055899227,8.0545855245577371,7.998597974406227]
[null,null,null,null,"Coincident",7.7179220832667328,7.5425718024058686,7.4121172048108361,7.3523984926465209,7.2973997683841718,7.2442488164150651,7.1938939294152995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7985806605450865,8.5986779440679957,8.4499571760820853,8.3818766875447874,8.3191770766354569,8.2585839619292507,8.2011784154440566]
[null,null,null,null,"Coincident",7.9133938477592904,7.7336024714281244,7.5998438510530022,7.538612643437963,7.4822209668290611,7.4277238610307537,7.376093636121837]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.7940588952338237,7.6831567585357865,7.5738326550665862,7.4660641308957079,7.3598290515909763,7.2551055976723946,7.151872260130669]
[null,null,null,null,"Coincident",7.009932634611534,6.9101878780299382,6.8118623956388529,6.7149359924997469,6.6193887610290973,6.5252010769095925,6.4323535950595208]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9914589762884658,7.877748021865596,7.7656550675093126,7.6551570905985429,7.5462313961024865,7.438855611919311,7.3330076842811804]
[null,null,null,null,"Coincident",7.1874731547513147,7.0852021633415445,6.9843863920708609,6.8850051345236496,6.7870379789171453,6.6904648039090731,6.5952657744649574]
[null,"Whyalla LMF 33kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.6,11.6,11.6,11.6,11.6,11.6,11.6]
[null,null,null,null,"Coincident",0.71962558402320864,0.71962558402320864,0.71962558402320864,0.71962558402320864,0.71962558402320864,0.71962558402320864,0.71962558402320864]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.60479987718038,11.60479987718038,11.60479987718038,11.60479987718038,11.60479987718038,11.60479987718038,11.60479987718038]
[null,null,null,null,"Coincident",0.71992335250761996,0.35988721873446944,0.2399082709373071,0.17992500076233581,0.14393702360255842,0.11994586583285825,0.10280972961376637]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.25,12.25,12.25,12.25,12.25,12.25,12.25]
[null,null,null,null,"Coincident",0.75994943140381954,0.75994943140381954,0.75994943140381954,0.75994943140381954,0.75994943140381954,0.75994943140381954,0.75994943140381954]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.255068835815488,12.255068835815488,12.255068835815488,12.255068835815488,12.255068835815488,12.255068835815488,12.255068835815488]
[null,null,null,null,"Coincident",0.76026388519123667,0.38005331288769406,0.2533514068087942,0.19000700511539773,0.15200246026994318,0.1266669703838374,0.10857061963522743]
[null,"Whyalla Central 33kV","Substation Rating","MVA","Non-Coincident",240,240,240,240,240,240,240]
[null,null,null,null,"Coincident",240,240,240,240,240,240,240]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",19.45477,20.868008186890563,21.235330320546048,21.831106466098877,22.396497186838012,22.945514805131772,23.493621540034667]
[null,null,null,null,"Coincident",19.45477,20.868008186890563,21.235330320546048,21.831106466098877,22.396497186838012,22.945514805131772,23.493621540034667]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.7,73.5,73.2,73,72.8,72.5,72.3]
[null,null,null,null,"Coincident",51.208982341677903,51.070016310899938,50.861567264733004,50.722601233955039,50.583635203177082,50.375186157010141,50.236220126232183]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",76.000634477748946,75.794391236289641,75.485026374100713,75.278783132641422,75.072539891182117,74.763175028993189,74.556931787533898]
[null,null,null,null,"Coincident",52.807532549896372,52.664228526694473,52.449272491891648,52.305968468689748,52.162664445487863,51.947708410685024,51.804404387483139]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",70.23166466481878,70.068708311549898,69.906130060853371,69.743929035429531,69.582104360014284,69.42065516137437,69.259580568302667]
[null,null,null,null,"Coincident",48.799078366992518,48.685851378973382,48.572887108022776,48.46018494456645,48.347744280444509,48.235564508908148,48.123645024616401]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",72.42403086777108,72.255987635198267,72.088334308126107,71.921069981868953,71.754193753840241,71.587704723547745,71.421601992588535]
[null,null,null,null,"Coincident",50.322400513172653,50.205639008023958,50.089148420974261,49.972928123420722,49.856977488219002,49.74129588967989,49.625882703565978]
[null,"Wudinna 66kV","Substation Rating","MVA","Non-Coincident",50,50,50,50,50,50,50]
[null,null,null,null,"Coincident",50,50,50,50,50,50,50]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.1083299999999987,6.5520528100938336,6.6673831279887148,6.8544425125594248,7.0319616043406432,7.2043399356368925,7.3764322714501347]
[null,null,null,null,"Coincident",6.1083299999999987,6.5520528100938336,6.6673831279887148,6.8544425125594248,7.0319616043406432,7.2043399356368925,7.3764322714501347]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.056343350267973,13.787289942618896,13.606532224700347,13.506425621297574,13.409426172002481,13.31146789871327,13.218780303924021]
[null,null,null,null,"Coincident",13.846249130837855,13.581217150686419,13.403161141932603,13.304550789594394,13.209001150045477,13.11250701763918,13.021204785130353]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.07205125131931,13.80269717768623,13.621737463823461,13.521518991737514,13.424411145990115,13.326343404767057,13.233552232003698]
[null,null,null,null,"Coincident",13.861722252535269,13.596394100327139,13.418139114777054,13.319418565809567,13.223762149964275,13.127160185795042,13.035755923448278]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.598943324697004,12.420451713531079,12.244488826753823,12.071018839448916,11.900006434238398,11.731416794092274,11.56521559524]
[null,null,null,null,"Coincident",12.41063224709402,12.234808474553565,12.061475630627777,11.890598425860206,11.722142070746806,11.556072268653002,11.392355208831138]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.61302258771472,12.434331512968772,12.258171988449726,12.08450814920708,11.913304638395863,11.744526600078201,11.578139672126891]
[null,null,null,null,"Coincident",12.424501073321727,12.248480818499024,12.074954275892612,11.903886116610234,11.735241512270726,11.568986127913179,11.405086115006574]
[null,"Yadnarie 66kV","Substation Rating","MVA","Non-Coincident",40,40,40,40,40,40,40]
[null,null,null,null,"Coincident",40,40,40,40,40,40,40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.2112500000000006,4.5171646581811506,4.5966765380623649,4.725640401061483,4.8480269249172103,4.966869267696878,5.085514437357574]
[null,null,null,null,"Coincident",4.2112500000000006,4.5171646581811506,4.5966765380623649,4.725640401061483,4.8480269249172103,4.966869267696878,5.085514437357574]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0235688466385415,7.7981389648369737,7.647155180560361,7.5716974007693549,7.5021473994253256,7.4351036957750436,7.3710494455935214]
[null,null,null,null,"Coincident",7.8819226995737379,7.6604725024736782,7.512154149468464,7.4380284831020145,7.3697063006883177,7.3038461703940492,7.2409227184788296]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.2143182479889614,7.983529078341542,7.8289558606077154,7.7517041750626134,7.6805007173360353,7.6118631411110869,7.5462860885320762]
[null,null,null,null,"Coincident",8.0693046570506599,7.8425897836783367,7.6907453642074657,7.6148574612659505,7.5449110121894423,7.4774851471620876,7.4130657760352117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.0719942138252128,6.9308622727795584,6.7925468250992944,6.6569916635586246,6.5241417026287802,6.3939429560929204,6.2663425151077625]
[null,null,null,null,"Coincident",6.9471469355629223,6.808506503727072,6.6726328435628037,6.5394707401131136,6.4089660803158575,6.281065831013831,6.1557180174036956]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.2401212266825832,7.0956340663099136,6.9540303575893541,6.8152525570450102,6.6792442695648289,6.5459502254833275,6.4153162581216661]
[null,null,null,null,"Coincident",7.1123058747308976,6.9703694557998865,6.8312655847617521,6.6949377339992271,6.5613305039859515,6.4303896007737693,6.3020618139293125]
[null,"Bungama + Port Pirie 33kV","Substation Rating","MVA","Non-Coincident",180,180,180,180,180,180,180]
[null,null,null,null,"Coincident",180,180,180,180,180,180,180]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",23.427779999999998,25.129626556400872,25.571962401872767,26.289406631090571,26.970260191400868,27.631396970582024,28.291436847785576]
[null,null,null,null,"Coincident",23.427779999999998,25.129626556400872,25.571962401872767,26.289406631090571,26.970260191400868,27.631396970582024,28.291436847785576]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",71.099999999999994,71.2,71.3,71.400000000000006,71.400000000000006,71.5,71.599999999999994]
[null,null,null,null,"Coincident",65.78831291409972,65.880842186834045,65.973371459568355,66.06590073230268,66.06590073230268,66.158430005037005,66.250959277771315]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",73.57587869828366,73.679360946804451,73.782843195325242,73.886325443846047,73.886325443846047,73.989807692366824,74.093289940887615]
[null,null,null,null,"Coincident",68.079225467405479,68.174976839370899,68.270728211336291,68.366479583301711,68.366479583301711,68.462230955267131,68.557982327232523]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.500277956295363,67.645869262521458,67.791774594542574,67.93799462968073,68.084530046718882,68.231381525904055,68.378549748950476]
[null,null,null,null,"Coincident",62.457516286602917,62.592230863418315,62.727236006018046,62.862532341123249,62.998120496806848,63.134001102496477,63.27017478897735]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",69.850805386959479,70.00146654429301,70.152452662580203,70.303764442729062,70.455402587159455,70.607367799806312,70.759660786122851]
[null,null,null,null,"Coincident",64.632442223617048,64.771847896790902,64.911554253971801,65.051561943704883,65.191871615934147,65.332483922005451,65.473399514669509]
[null,"Metro North Region 66kV","Substation Rating","MVA","Non-Coincident",875,875,875,875,875,875,875]
[null,null,null,null,"Coincident",875,875,875,875,875,875,875]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",105.29411999999998,112.94292136023387,114.93096135349909,118.1554520549043,121.21548917672034,124.18691094026406,127.15340277325275]
[null,null,null,null,"Coincident",105.29411999999998,112.94292136023387,114.93096135349909,118.1554520549043,121.21548917672034,124.18691094026406,127.15340277325275]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",320.68275207264935,321.05092186252574,322.88658679977226,324.35211717156659,325.94959259121379,327.58683804841627,329.34540583749401]
[null,null,null,null,"Coincident",317.11605931489498,317.48013425241436,319.29538258541561,320.74461305791834,322.32432106109826,323.9433567721353,325.68236544567975]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",322.94554270646103,323.31631036337831,325.16492805658055,326.64079945350778,328.24954692440798,329.89834505683814,331.66932159161962]
[null,null,null,null,"Coincident",319.35368277362858,319.72032668423208,321.54838371024664,323.00784019309202,324.59869487769043,326.22915477296891,327.98043417985713]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",291.71826759403206,293.5779116875475,295.44941063054858,297.33283999526816,299.22827583569642,301.13579469065223,303.05547358687369]
[null,null,null,null,"Coincident",288.4737231786948,290.31268396736311,292.16336775369297,294.02584926938897,295.90020372255475,297.78650680073031,299.68483467394816]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",293.77668002612319,295.64944607649426,297.53415062613317,299.43086978052304,301.33968013030358,303.26065875436427,305.19388322295657]
[null,null,null,null,"Coincident",290.50924156778996,292.36117836848774,294.22492088626103,296.10054438013367,297.98812458889017,299.8877377341343,301.79946052336703]
[null,"Metro South Region 66kV","Substation Rating","MVA","Non-Coincident",1515,1515,1515,1515,1515,1515,1515]
[null,null,null,null,"Coincident",1515,1515,1515,1515,1515,1515,1515]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",245.08127999999999,262.88453461509022,267.51187169944626,275.0171560253753,282.13966025127314,289.05590447487413,295.96067385362403]
[null,null,null,null,"Coincident",245.08127999999999,262.88453461509022,267.51187169944626,275.0171560253753,282.13966025127314,289.05590447487413,295.96067385362403]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",675.50769774590128,677.79668899853539,677.08492206091262,678.67318192221012,680.39149758190922,682.1145581924377,683.15401768808283]
[null,null,null,null,"Coincident",675.50769774590128,677.79668899853539,677.08492206091262,678.67318192221012,680.39149758190922,682.1145581924377,683.15401768808283]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",679.09216090182042,681.39329828518942,680.67775448111195,682.27444216488118,684.00187576534245,685.73407949488262,686.77905470008466]
[null,null,null,null,"Coincident",679.09216090182031,681.39329828518942,680.67775448111195,682.27444216488107,684.00187576534233,685.73407949488262,686.77905470008466]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",609.57600337078156,609.45203195915212,609.3280857599832,609.20416476814717,609.08026897851755,608.95639838596901,608.83255298537699]
[null,null,null,null,"Coincident",609.57600337078156,609.45203195915212,609.3280857599832,609.20416476814717,609.08026897851755,608.95639838596901,608.83255298537699]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",612.81061155083057,612.68598230664225,612.56137840869985,612.43679985184883,612.31224663093519,612.18771874080642,612.06321617631102]
[null,null,null,null,"Coincident",612.81061155083057,612.68598230664225,612.56137840869985,612.43679985184872,612.31224663093508,612.18771874080642,612.0632161763109]
[null,"Metro East Region 66kV","Substation Rating","MVA","Non-Coincident",1650,1650,1650,1650,1650,1650,1650]
[null,null,null,null,"Coincident",1650,1650,1650,1650,1650,1650,1650]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",182.46520000000004,195.41478449951782,198.78057878135829,204.23971059027735,209.420418967231,214.45109964495995,219.47343384468635]
[null,null,null,null,"Coincident",182.46520000000004,195.41478449951782,198.78057878135829,204.23971059027735,209.420418967231,214.45109964495995,219.47343384468635]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",735.6580028091231,739.27439648191421,743.58739693309508,745.95120629818246,748.10460240922419,750.28867031642528,752.74956250400203]
[null,null,null,null,"Coincident",686.62613116334671,690.00149089141382,694.0270283044398,696.23328892141126,698.24316040373151,700.2816593959169,702.57853223018742]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",757.82607644796531,761.55144532518477,765.99441229782133,768.42945190831256,770.64773774172647,772.89761962500643,775.4326675194784]
[null,null,null,null,"Coincident",707.31669468588029,710.79376638163308,714.94060800050886,717.21335134129595,719.28378762255068,721.38371406553381,723.74980010204604]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",658.81015119743449,663.11237818858194,667.44270000651636,671.80130011884501,676.18836319127342,680.60407509542938,685.04862291673794]
[null,null,null,null,"Coincident",614.90021662308243,618.91569863107816,622.95740293550614,627.02550077579133,631.12016450960334,635.24156762015889,639.38988472357164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",678.66251722892434,683.09438609766516,687.55519639336148,692.04513711217214,696.56439848445791,701.1131719828403,705.69165033031447]
[null,null,null,null,"Coincident",633.42941528684969,637.56589849446368,641.7293941724713,645.92007872036947,650.13812968959633,654.3837257910543,658.6570469026808]
[null,"Metro West Region 66kV","Substation Rating","MVA","Non-Coincident",845,845,845,845,845,845,845]
[null,null,null,null,"Coincident",845,845,845,845,845,845,845]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",106.87642999999998,114.47309674675093,116.44758615976754,119.65009857091788,122.68927832632109,125.64044673017598,128.58671880612965]
[null,null,null,null,"Coincident",106.87642999999998,114.47309674675093,116.44758615976754,119.65009857091788,122.68927832632109,125.64044673017598,128.58671880612965]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",432.26893113191926,436.67163210201539,445.83360921752234,447.39158291399417,449.07122302491325,450.77397595548018,452.64210853246118]
[null,null,null,null,"Coincident",432.07845010963047,436.47921101204832,445.63715086593072,447.194438035102,448.87333800593149,450.57534061165302,452.44264998859023]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",434.45348004872187,438.87843086131778,448.08670967870978,449.652556875926,451.34068535073305,453.05204344998589,454.92961697148905]
[null,null,null,null,"Coincident",434.26203639627175,438.68503733670786,447.88925848944638,449.45441568987263,451.14180028415888,452.85240426666451,454.7291504279342]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",398.72705231199643,403.64448066012613,412.5978891224205,415.61680838341493,418.65781664133516,421.72107551818658,424.80674781853952]
[null,null,null,null,"Coincident",398.55135165190109,403.46661311568795,412.41607622296357,415.43366518518883,418.47333341073562,421.53524245038994,424.61955503698164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",400.74209130160693,405.68437075976954,414.68302688468629,417.71720279802497,420.77357933901482,423.85231894644704,426.95358524765425]
[null,null,null,null,"Coincident",400.56550270657328,405.50560432965261,414.50029516098829,417.53313405265339,420.58816378917476,423.66554673776443,426.76544645365198]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Aldgate 11kV","Substation Rating","MVA","Non-Coincident",12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392]
[null,null,null,null,"Coincident",12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392,12.580828651685392]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3494299999999999,3.5927401177920304,3.6559801239257284,3.7585519094158171,3.8558923889879368,3.9504139937790326,4.0447787763534757]
[null,null,null,null,"Coincident",3.3494299999999999,3.5927401177920304,3.6559801239257284,3.7585519094158171,3.8558923889879368,3.9504139937790326,4.0447787763534757]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.5756824919977577,6.7166241244790461,6.7967906687613135,6.9113215734914695,7.0327138037516193,7.1600312534893256,7.2947915398394443]
[null,null,null,null,"Coincident",6.1183692090956487,6.2495088961931629,6.3241001674008475,6.4306658907069254,6.5436157608916554,6.6620787744577354,6.7874670041383602]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5880153906365617,6.7292213635676053,6.8095382627166199,6.9242839737487474,7.0459038789419797,7.1734601165476342,7.3084731500390747]
[null,null,null,null,"Coincident",6.1298444023371701,6.2612300460286141,6.3359612155036293,6.4427268061642371,6.5558885173710886,6.6745737120325206,6.8001971112684014]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.6944615416809583,5.7576158113784581,5.821470491773586,5.8860333507519922,5.95131224234885,6.0173151077042952,6.0840499760294602]
[null,null,null,null,"Coincident",5.2984337673541058,5.3571959018717523,5.4166097362321608,5.476682498094581,5.5374214952764174,5.5988341166422275,5.6609278330025639]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.705141682804193,5.76841440031418,5.832388842164014,5.8970727908082576,5.9624741150125748,6.0286007708109572,6.0954608024735748]
[null,null,null,null,"Coincident",5.3083711459724805,5.3672434907154063,5.4267687575845773,5.4869541877949448,5.5478071028699549,5.6093349055322115,5.6715450806040062]
[null,"Aldinga 11kV","Substation Rating","MVA","Non-Coincident",33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003]
[null,null,null,null,"Coincident",33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003,33.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.9413499999999999,9.5908697456641185,9.7596898221677453,10.03350663105517,10.293358395988957,10.545685135463692,10.797593235848533]
[null,null,null,null,"Coincident",8.9413499999999999,9.5908697456641185,9.7596898221677453,10.03350663105517,10.293358395988957,10.545685135463692,10.797593235848533]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.740105177680473,19.118106265649615,19.327090249318616,19.669759527516337,20.018385203472025,20.369685774920391,20.705399945179767]
[null,null,null,null,"Coincident",18.740105177680473,19.118106265649615,19.327090249318616,19.669759527516337,20.018385203472025,20.369685774920391,20.705399945179767]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.154956978906419,19.541325919175353,19.754936204630308,20.105191190909029,20.461534432388099,20.820611783820105,21.163757696159298]
[null,null,null,null,"Coincident",19.154956978906419,19.541325919175353,19.754936204630308,20.105191190909029,20.461534432388099,20.820611783820105,21.163757696159298]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.570922230016979,16.764069813997004,16.959468690251501,17.157145099424028,17.357125588014195,17.559437011942673,17.764106540157741]
[null,null,null,null,"Coincident",16.570922230016979,16.764069813997004,16.959468690251501,17.157145099424028,17.357125588014195,17.559437011942673,17.764106540157741]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.937754586074679,17.135177899692124,17.334902342692544,17.536954736611559,17.741362215611602,17.948152230125864,18.157352550544658]
[null,null,null,null,"Coincident",16.937754586074679,17.135177899692124,17.334902342692544,17.536954736611559,17.741362215611602,17.948152230125864,18.157352550544658]
[null,"Allendale East 11kV","Substation Rating","MVA","Non-Coincident",6.8,6.8,6.8,6.8,6.8,6.8,6.8]
[null,null,null,null,"Coincident",6.8,6.8,6.8,6.8,6.8,6.8,6.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.1143599999999998,1.1953096131767873,1.216349650805622,1.2504754259013056,1.2828607382726605,1.3143082071001939,1.3457035009590466]
[null,null,null,null,"Coincident",1.1143599999999998,1.1953096131767873,1.216349650805622,1.2504754259013056,1.2828607382726605,1.3143082071001939,1.3457035009590466]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.9064013095500743,3.8762974408327144,3.850684474295214,3.834716282470735,3.8203021126387631,3.8064256790875581,3.7941067302294331]
[null,null,null,null,"Coincident",3.5838544124312608,3.5562361842501971,3.532738049812123,3.518088332541959,3.5048643235218013,3.4921336505390443,3.4808318625958106]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.2927486918132685,4.2596675173985874,4.2315214003244108,4.2139739367810272,4.1981341897129267,4.1828853616346793,4.1693480551971795]
[null,null,null,null,"Coincident",3.9383015521222644,3.9079518508243924,3.8821297250682671,3.8660311346614931,3.8514992566173638,3.8375095060868616,3.8250899588964948]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6397281771858063,3.634793344910797,3.6298652034018,3.6249437435873118,3.6200289564081274,3.6151208328173254,3.6102193637802502]
[null,null,null,null,"Coincident",3.3392001625557857,3.3346727934961442,3.3301515627539451,3.3256364620067083,3.3211274829432362,3.3166246172636016,3.3121278566791288]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.9997012936107761,3.9942784010008756,3.9888628608810985,3.9834546632827599,3.9780537982506896,3.9726602558432145,3.9672740261321433]
[null,null,null,null,"Coincident",3.6694507280832807,3.6644755972485101,3.6595072118175218,3.6545455626447341,3.6495906405969629,3.6446424365534082,3.639700941405636]
[null,"Alma 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.6000000000000001E-3,1.7162275934912057E-3,1.7464369156188265E-3,1.7954347620536355E-3,1.8419336491225968E-3,1.8870859788222036E-3,1.9321633956122571E-3]
[null,null,null,null,"Coincident",1.6000000000000001E-3,1.7162275934912057E-3,1.7464369156188265E-3,1.7954347620536355E-3,1.8419336491225968E-3,1.8870859788222036E-3,1.9321633956122571E-3]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3733863503885342E-2,8.3561703226009476E-2,8.3389896916767542E-2,8.3218443848385421E-2,8.3047343294585338E-2,8.287659453058277E-2,8.2706196833083376E-2]
[null,null,null,null,"Coincident",8.3733863503885342E-2,8.3561703226009476E-2,8.3389896916767542E-2,8.3218443848385421E-2,8.3047343294585338E-2,8.287659453058277E-2,8.2706196833083376E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6712761709330538E-2,8.6534476693847298E-2,8.6356558239711181E-2,8.617900559325696E-2,8.6001818002368918E-2,8.5824994716477782E-2,8.5648534986557417E-2]
[null,null,null,null,"Coincident",8.6712761709330538E-2,8.6534476693847298E-2,8.6356558239711181E-2,8.617900559325696E-2,8.6001818002368918E-2,8.5824994716477782E-2,8.5648534986557417E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5360477153496808E-2,7.5205532903408534E-2,7.5050907225090793E-2,7.4896599463546876E-2,7.47426089651268E-2,7.4588935077524496E-2,7.4435577149775042E-2]
[null,null,null,null,"Coincident",7.5360477153496808E-2,7.5205532903408534E-2,7.5050907225090793E-2,7.4896599463546876E-2,7.47426089651268E-2,7.4588935077524496E-2,7.4435577149775042E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.8041485538397487E-2,7.7881029024462575E-2,7.7720902415740076E-2,7.7561105033931252E-2,7.7401636202132029E-2,7.7242495244829998E-2,7.7083681487901679E-2]
[null,null,null,null,"Coincident",7.8041485538397487E-2,7.7881029024462575E-2,7.7720902415740076E-2,7.7561105033931252E-2,7.7401636202132029E-2,7.7242495244829998E-2,7.7083681487901679E-2]
[null,"American River 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.43087000000000003,0.4621693645047224,0.47030454614542738,0.48349935995378124,0.49602121962340834,0.50818045980945181,0.52031952641715828]
[null,null,null,null,"Coincident",0.43087000000000003,0.4621693645047224,0.47030454614542738,0.48349935995378124,0.49602121962340834,0.50818045980945181,0.52031952641715828]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.39110705440923732,0.3807401251618015,0.36437628530258481,0.35795513198666307,0.3520490022272228,0.34639601352221305,0.34047912956203924]
[null,null,null,null,"Coincident",0.33870993707211461,0.32973187872864146,0.31556032363525288,0.30999942052433499,0.30488454259869535,0.29998889209339979,0.29486470072119186]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.40108078820890308,0.39044948890864356,0.37366835004943127,0.36708344905077706,0.36102670537286397,0.35522955817242269,0.34916178604780135]
[null,null,null,null,"Coincident",0.3473474768699113,0.33814046647112189,0.32360751846386154,0.31790480515880692,0.31265949125592524,0.30763899535506462,0.30238413050072749]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.3689910644980085,0.34688667087234848,0.32610643998277755,0.30657104791834205,0.28820592266351441,0.27094095943610474,0.25471025307784284]
[null,null,null,null,"Coincident",0.31955685490018915,0.30041381544447404,0.28241753893245325,0.26549932857999958,0.24959460288084262,0.2346426490810285,0.22058639142148112]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.37840081206013665,0.35573272791716193,0.33442257436613138,0.31438900463415909,0.29555554502324105,0.27785030298891672,0.26120569270646615]
[null,null,null,null,"Coincident",0.32770596642528577,0.30807475479907326,0.2896195500491377,0.27226990353484593,0.25595958683830922,0.24062633895212404,0.22621162861181998]
[null,"Angaston 11kV","Substation Rating","MVA","Non-Coincident",28.956,28.956,28.956,28.956,28.956,28.956,28.956]
[null,null,null,null,"Coincident",28.956,28.956,28.956,28.956,28.956,28.956,28.956]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.8075799999999997,5.156813408697781,5.2475844917442229,5.394810158346135,5.5345271080305087,5.6701980062912805,5.8056438109234838]
[null,null,null,null,"Coincident",4.8075799999999997,5.156813408697781,5.2475844917442229,5.394810158346135,5.5345271080305087,5.6701980062912805,5.8056438109234838]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.406798306981294,14.462038540582284,14.585402391461342,14.648226685758157,14.715120291775317,14.78412608085762,14.851737120498711]
[null,null,null,null,"Coincident",14.122078161476988,14.176226687745551,14.297152510908537,14.35873521482335,14.424306809049085,14.491948843472684,14.558223692751827]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.814269564635948,14.871072172261959,14.997925155312906,15.062526325613877,15.131311901046592,15.202269398972433,15.271792699392559]
[null,null,null,null,"Coincident",14.521496604530078,14.577176627778654,14.701522627735763,14.764847091428095,14.83227326426292,14.901828436099121,14.969977754334602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.333276287774961,13.380720801305289,13.428334139197727,13.476116902189075,13.524069693153768,13.572193117111482,13.620487781234763]
[null,null,null,null,"Coincident",13.06977205291212,13.116278925163108,13.162951285316856,13.209789722237858,13.256794826886003,13.30396719232402,13.351307413724964]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.710384840409029,13.759171239567591,13.808131237992006,13.857265453409871,13.906574505746875,13.956059017134624,14.005719611918488]
[null,null,null,null,"Coincident",13.439427846113519,13.487250084438351,13.535242491203729,13.583405671929155,13.631740234288795,13.680246788119126,13.728925945426637]
[null,"Angle Vale 11kV","Substation Rating","MVA","Non-Coincident",27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191]
[null,null,null,null,"Coincident",27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191,27.349292452830191]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.6326700000000027,9.2597665371898312,9.4227584802219866,9.6871223795859756,9.9380033467319819,10.181619072999421,10.424830612750041]
[null,null,null,null,"Coincident",8.6326700000000027,9.2597665371898312,9.4227584802219866,9.6871223795859756,9.9380033467319819,10.181619072999421,10.424830612750041]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.142873857289967,18.443338394158438,18.810596661172749,19.086078946658279,19.368582126042927,19.656411616283354,19.840827278896082]
[null,null,null,null,"Coincident",17.678232583490662,17.971002185904965,18.328854922663094,18.597282072284042,18.872550309831244,19.153008450745521,19.332701205121168]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.15307813858492,19.470272690990587,19.85798008180949,20.148801358593058,20.447034456155976,20.750890436224363,20.945574455072968]
[null,null,null,null,"Coincident",18.662565406506705,18.97163656666309,19.349414722601761,19.632788030030774,19.923383340579864,20.219457530908592,20.409155667629719]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.36544352681474,16.499489424094648,16.634633263055644,16.770884036706537,16.908250811715977,17.046742729015779,17.186369004409212]
[null,null,null,null,"Coincident",15.946322466590074,16.076935431637214,16.208618219941357,16.341379594199228,16.475228388880957,16.610173510817951,16.746223939795595]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.276679599232018,17.41818923904728,17.560857954485005,17.704695239289233,17.849710664965254,17.995913881416531,18.14331461758686]
[null,null,null,null,"Coincident",16.834221668964037,16.972107229164575,17.111122180915594,17.25127577482515,17.392577337271085,17.535036271021628,17.6786620558611]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Ardrossan 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2033699999999998,1.2907854994871948,1.3135061194676416,1.3503577060078016,1.3853298095904116,1.4192891589595464,1.4531921658612006]
[null,null,null,null,"Coincident",1.2033699999999998,1.2907854994871948,1.3135061194676416,1.3503577060078016,1.3853298095904116,1.4192891589595464,1.4531921658612006]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2378192482754415,2.2144192553727695,2.1862846047220086,2.1792817205113924,2.1734171962532436,2.1679573521907622,2.1633113956663119]
[null,null,null,null,"Coincident",2.2378192482754415,2.2144192553727695,2.1862846047220086,2.1792817205113924,2.1734171962532436,2.1679573521907622,2.1633113956663119]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2950924695160415,2.2710935931371563,2.2422388834054443,2.2350567721473236,2.2290421552507427,2.2234425756590537,2.2186777136885514]
[null,null,null,null,"Coincident",2.2950924695160415,2.2710935931371563,2.2422388834054443,2.2350567721473236,2.2290421552507427,2.2234425756590537,2.2186777136885514]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9618494509295796,1.9225041299264198,1.8839478879650329,1.846164899892178,1.8091396579315342,1.7728569653186352,1.7373019300634591]
[null,null,null,null,"Coincident",1.9618494509295796,1.9225041299264198,1.8839478879650329,1.846164899892178,1.8091396579315342,1.7728569653186352,1.7373019300634591]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0120596891918656,1.9717073908484519,1.9321643666982167,1.8934143865697273,1.8554415457912019,1.8182302586625376,1.7817652520582647]
[null,null,null,null,"Coincident",2.0120596891918652,1.9717073908484521,1.9321643666982167,1.8934143865697275,1.8554415457912021,1.8182302586625376,1.781765252058265]
[null,"Arno Bay 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.29419999999999996,0.31557134875319537,0.32112608785941166,0.33013556687261214,0.33868554973241743,0.34698793435593261,0.35527654436820372]
[null,null,null,null,"Coincident",0.29419999999999996,0.31557134875319537,0.32112608785941166,0.33013556687261214,0.33868554973241743,0.34698793435593261,0.35527654436820372]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.64159305656241716,0.62056310980832863,0.60501028908930032,0.59654118077098739,0.58990531770307031,0.58341983243588802,0.57716733871902548]
[null,null,null,null,"Coincident",0.59368744167242349,0.57422773094264024,0.55983618750396602,0.55199943927342043,0.54585905398124124,0.53985781828067514,0.53407217742800506]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.6949988534587479,0.67221838734725381,0.65537095974931725,0.6461968882551804,0.63900866017705593,0.63198332725190642,0.62521037994515083]
[null,null,null,null,"Coincident",0.64310560573382813,0.62202608109199231,0.60643659475470169,0.59794752059879364,0.59129601355050265,0.5847952388170975,0.57852800490924638]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.56662643687575043,0.55439638206114639,0.54243030052952745,0.53072249468630495,0.51926738991366939,0.50805953191626163,0.49709358412413551]
[null,null,null,null,"Coincident",0.52431832958902791,0.51300145220058091,0.50192883808998956,0.49109521508306098,0.48049542480011553,0.47012442019984757,0.45997726317620019]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.61379206015417809,0.60054398337568426,0.58758185284792031,0.57489949671215745,0.56249087632295425,0.55035008337288427,0.53847133707932193]
[null,null,null,null,"Coincident",0.56796225299599967,0.5557033659502999,0.54370907450194239,0.53197366762431642,0.5204915575575072,0.50925727714770908,0.49826547724406606]
[null,"Ascot Park 11kV","Substation Rating","MVA","Non-Coincident",27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999]
[null,null,null,null,"Coincident",27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999,27.024999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.9440200000000001,6.3758069626647478,6.4880349719853854,6.670062583963781,6.8428065306610613,7.0105479998992211,7.1780111667419799]
[null,null,null,null,"Coincident",5.9440200000000001,6.3758069626647478,6.4880349719853854,6.670062583963781,6.8428065306610613,7.0105479998992211,7.1780111667419799]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.617193992631528,17.536774979236323,17.268803312517054,17.26614618885937,17.267052383947888,17.268962154196458,17.257060030367629]
[null,null,null,null,"Coincident",17.195465284150004,17.116971379070613,16.85541454464316,16.852821028466266,16.853705530628858,16.855569583895441,16.843952378726904]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.937567743705042,17.855686287369728,17.582841478645882,17.580136034428545,17.581058708935966,17.583003208907016,17.570884641525463]
[null,null,null,null,"Coincident",17.508169777092618,17.428248437722772,17.161935116865102,17.159294436848928,17.160195023938311,17.16209297555088,17.150264508157587]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.282384394083437,15.179697625107478,15.077700838286843,14.9763893974315,14.875758697503324,14.775804164406772,14.676521254780976]
[null,null,null,null,"Coincident",14.91654746024876,14.816318855636347,14.716763716060621,14.617877516314856,14.519655761598502,14.422093987312877,14.325187758858231]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.560298959577104,15.455744802106917,15.351893174316441,15.248739355705194,15.146278657491104,15.044506422397381,14.943418024440831]
[null,null,null,null,"Coincident",15.187809175644798,15.085757884965695,14.984392306479103,14.88370783268611,14.783699887046918,14.684363923772834,14.585695427619632]
[null,"Athol Park 11kV","Substation Rating","MVA","Non-Coincident",26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844]
[null,null,null,null,"Coincident",26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844,26.506616257088844]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.0360100000000001,6.4744793228680324,6.5884441794027451,6.7732888613146018,6.9487062034003024,7.1190436493941291,7.2890984859684611]
[null,null,null,null,"Coincident",6.0360100000000001,6.4744793228680324,6.5884441794027451,6.7732888613146018,6.9487062034003024,7.1190436493941291,7.2890984859684611]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.795286012777105,16.556582681309649,18.512142422534836,18.398511684844109,18.292606937746058,18.189484086274067,18.092219773779703]
[null,null,null,null,"Coincident",15.285212760691614,15.067971374900967,16.847705681785065,16.744291545197228,16.647908751207922,16.554057731103864,16.465538505568333]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.12694257502573,17.86931304858086,19.979924270339968,19.857284033352602,19.742982361585383,19.631683155047096,19.526706996508121]
[null,null,null,null,"Coincident",16.497139360968411,16.262673444630323,18.183518469546744,18.071904882618398,17.967880135999877,17.866587901337148,17.771050206007185]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.875390594668273,15.743879718470883,17.713458271251952,17.566720941934172,17.421199176708143,17.276882905906742,17.133762143279423]
[null,null,null,null,"Coincident",14.448025637311753,14.328338975143998,16.120831654652452,15.98728755800226,15.854849733418678,15.723509016603803,15.593256319176277]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.134110931289353,16.992172883970131,19.117914434075551,18.959542665941779,18.802482840961016,18.64672409106722,18.492255638224819]
[null,null,null,null,"Coincident",15.593573747467531,15.464397426774873,17.399012404030096,17.254879927252379,17.111941436108996,16.970187039687598,16.829606929011618]
[null,"Auburn 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.5807800000000001,1.6956114095243926,1.7254578421699553,1.7738671019744663,1.8198074211625117,1.8644173585016017,1.9089532828224649]
[null,null,null,null,"Coincident",1.5807800000000001,1.6956114095243926,1.7254578421699553,1.7738671019744663,1.8198074211625117,1.8644173585016017,1.9089532828224649]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1346505434374956,3.0914277628672258,3.0488009685909101,3.0067619427276564,2.9653025807105302,2.9244148897241034,2.8840909871635447]
[null,null,null,null,"Coincident",3.1346505434374956,3.0914277628672258,3.0488009685909101,3.0067619427276564,2.9653025807105302,2.9244148897241034,2.8840909871635447]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2140418182110202,3.1697243345466797,3.1260179317174459,3.0829141837082075,3.0404047806877141,2.9984815274065508,2.9571363416172036]
[null,null,null,null,"Coincident",3.2140418182110202,3.1697243345466797,3.1260179317174459,3.0829141837082075,3.0404047806877141,2.9984815274065508,2.9571363416172036]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8211854890937462,2.7822849865805033,2.7439208717318193,2.7060857484548908,2.6687723226394771,2.6319734007516931,2.5956818884471904]
[null,null,null,null,"Coincident",2.8211854890937462,2.7822849865805033,2.7439208717318193,2.7060857484548908,2.6687723226394771,2.6319734007516931,2.5956818884471904]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8926376363899182,2.8527519010920122,2.8134161385457013,2.7746227653373867,2.7363643026189424,2.6986333746658957,2.6614227074554835]
[null,null,null,null,"Coincident",2.8926376363899182,2.8527519010920122,2.8134161385457013,2.7746227653373867,2.7363643026189424,2.6986333746658957,2.6614227074554835]
[null,"Balaklava 7.6kV","Substation Rating","MVA","Non-Coincident",5,5,5,5,5,5,5]
[null,null,null,null,"Coincident",5,5,5,5,5,5,5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2311399999999999,1.3205727746567266,1.3438177151843511,1.3815197205966954,1.4172988704879961,1.4520418949794798,1.4867272767962965]
[null,null,null,null,"Coincident",1.2311399999999999,1.3205727746567266,1.3438177151843511,1.3815197205966954,1.4172988704879961,1.4520418949794798,1.4867272767962965]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9579238329795303,2.865049697951946,2.7940334841363206,2.7533931081353504,2.7151194873232929,2.6780122304714893,2.6425048739922063]
[null,null,null,null,"Coincident",2.931513798756499,2.8394688970773752,2.7690867565993891,2.7288092410984279,2.6908773490436206,2.654101406985137,2.6189110804744189]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0899301291517189,2.9929112049857216,2.9187256778668087,2.8762716021852999,2.8362899053003674,2.7975266248946435,2.7604346452538593]
[null,null,null,null,"Coincident",3.062341467284293,2.966188783512635,2.8926656271715694,2.8505906057372168,2.8109658882887567,2.7725487086009415,2.735787907349807]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6961353676061326,2.6357970062460132,2.5768089917176469,2.5191411038339933,2.4627637987229276,2.4076481936916032,2.3537660524295383]
[null,null,null,null,"Coincident",2.6720627303953637,2.6122631044045312,2.5538017685773107,2.4966487725497615,2.44077483623433,2.386151334819357,2.3327502841042747]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8164585618305158,2.7534274186240753,2.6918068855603692,2.631565393785122,2.5726720809415702,2.5150967753593547,2.4588099805972474]
[null,null,null,null,"Coincident",2.7913116103856006,2.7288432452435032,2.6677728955107232,2.6080692741977551,2.5497017945045921,2.492640554150789,2.4368563200562008]
[null,"Balhannah 33kV","Substation Rating","MVA","Non-Coincident",35.4,35.4,35.4,35.4,35.4,35.4,35.4]
[null,null,null,null,"Coincident",35.4,35.4,35.4,35.4,35.4,35.4,35.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.998810000000002,13.943072752843388,14.188501026946975,14.586572087081512,14.964340960969565,15.331170057733654,15.697390542824103]
[null,null,null,null,"Coincident",12.998810000000002,13.943072752843388,14.188501026946975,14.586572087081512,14.964340960969565,15.331170057733654,15.697390542824103]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.343181120946724,19.018258820162426,18.361947978293792,18.672358624469407,19.0068637045039,19.358755804414308,19.72802942574716]
[null,null,null,null,"Coincident",18.843938287165091,18.527402152502496,17.88803053497795,18.190429557333072,18.516301142027448,18.859110991813317,19.218853750150974]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.237603545847897,19.897656943199554,19.210998500747404,19.53576243458194,19.88573492108673,20.253898397630454,20.640247111512945]
[null,null,null,null,"Coincident",19.715275885262777,19.384103222339213,18.715167268473941,19.031549123599508,19.372488904738216,19.731150170855674,20.10752731772752]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.386701732385969,17.526518850356751,17.667460323411007,17.809535193176629,17.952752573990779,18.097121653484585,18.242651693172544]
[null,null,null,null,"Coincident",16.937955159176632,17.074163631095328,17.211467438764299,17.349875390449206,17.489396365248368,17.630039313662376,17.771813258168272]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.190657184556855,18.336939400740601,18.48439796182242,18.63304232751215,18.782882033590944,18.933926692523009,19.086185994072284]
[null,null,null,null,"Coincident",17.721160715264428,17.863667422772394,18.00732011400067,18.15212800450627,18.298100383954136,18.445246616713113,18.593576142456648]
[null,"Baroota 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.9549999999999999E-2,6.3875845745250806E-2,6.500019895318819E-2,6.6823837550183743E-2,6.8554468003281646E-2,7.0234981274288885E-2,7.1912706380443697E-2]
[null,null,null,null,"Coincident",5.9549999999999999E-2,6.3875845745250806E-2,6.500019895318819E-2,6.6823837550183743E-2,6.8554468003281646E-2,7.0234981274288885E-2,7.1912706380443697E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.29201089034700101,0.29102317086799667,0.29003879232524321,0.28905774341810792,0.28808001288418222,0.28710558949915232,0.28613446207667043]
[null,null,null,null,"Coincident",0.29201089034700101,0.29102317086799667,0.29003879232524321,0.28905774341810792,0.28808001288418222,0.28710558949915232,0.28613446207667043]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.29221600096682876,0.2912275877063209,0.29024251772876236,0.28926077972558278,0.28828236242646282,0.28730725459920464,0.28633544504960301]
[null,null,null,null,"Coincident",0.29221600096682876,0.2912275877063209,0.29024251772876236,0.28926077972558278,0.28828236242646282,0.28730725459920464,0.28633544504960301]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.26280980131230092,0.26192085378119701,0.26103491309271892,0.26015196907629712,0.25927201159576402,0.25839503054923713,0.25752101586900339]
[null,null,null,null,"Coincident",0.26280980131230092,0.26192085378119701,0.26103491309271892,0.26015196907629712,0.25927201159576402,0.25839503054923713,0.25752101586900339]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.26299440087014592,0.26210482893568882,0.26121826595588615,0.26033470175302448,0.25945412618381658,0.25857652913928419,0.2577019005446427]
[null,null,null,null,"Coincident",0.26299440087014592,0.26210482893568882,0.26121826595588615,0.26033470175302448,0.25945412618381658,0.25857652913928419,0.2577019005446427]
[null,"Barossa South TF1 11kV","Substation Rating","MVA","Non-Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,null,null,"Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.70184000000000002,0.75282323388491734,0.7660745530361982,0.78756745837482711,0.80796419518762708,0.82777026461035952,0.84754347348531656]
[null,null,null,null,"Coincident",0.70184000000000002,0.75282323388491734,0.7660745530361982,0.78756745837482711,0.80796419518762708,0.82777026461035952,0.84754347348531656]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9530896226808063,2.9690911717465518,3.0124870588079937,3.0216768607119637,3.0318830144622213,3.0426567556104587,3.0532120749720995]
[null,null,null,null,"Coincident",2.6567222053508326,2.671117864187758,2.7101586084616716,2.7184261363394366,2.7276080165950449,2.7373005220724913,2.7467965262293794]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9946984121880318,3.0109254217619017,3.054932753297074,3.0642520387528127,3.0746019963686253,3.0855275386420975,3.0962315815839938]
[null,null,null,null,"Coincident",2.6941552023627096,2.7087536948467288,2.7483445199912748,2.7567285366557561,2.7660397888477601,2.7758688609289126,2.7854986630020875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8055621221476463,2.8212110470357006,2.8369472588343596,2.8527712444144351,2.8686834933624175,2.884684497995623,2.900774753377426]
[null,null,null,null,"Coincident",2.5240003321113234,2.5380787555769206,2.5522357059764307,2.5664716213190792,2.5807869420572285,2.5951821111000046,2.6096575738270031]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8450922613257159,2.8609616782762806,2.8769196120028293,2.8929665562361437,2.909103007460947,2.9253294649312673,2.9416464306858807]
[null,null,null,null,"Coincident",2.5595632888629205,2.5738400761553639,2.5881964968197493,2.6026329950368172,2.617150017464867,2.6317480132535778,2.646427434057907]
[null,"Barossa South TF2 11kV","Substation Rating","MVA","Non-Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,null,null,"Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.7039999999999998E-2,5.0457091248641443E-2,5.1345245319193496E-2,5.2785782004376877E-2,5.4152849284204344E-2,5.548032777737278E-2,5.6805603831000355E-2]
[null,null,null,null,"Coincident",4.7039999999999998E-2,5.0457091248641443E-2,5.1345245319193496E-2,5.2785782004376877E-2,5.4152849284204344E-2,5.548032777737278E-2,5.6805603831000355E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.9409575618269583,6.0416709911701849,6.1502506376942341,6.1867787115224937,6.223827916897168,6.2612117695232099,6.2981181480982]
[null,null,null,null,"Coincident",4.3710672216550677,4.4451672577521562,4.5250548733294362,4.5519304509647363,4.5791894518103513,4.6066946698046412,4.6338485856473799]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6840014508706087,6.7973112499807158,6.9194711050796602,6.9605677962989994,7.0022507977176751,7.0443103011884851,7.0858326122594555]
[null,null,null,null,"Coincident",4.9177627255110181,5.0011305569806295,5.0910098286078327,5.1212467724065176,5.151915094693833,5.1828604288537035,5.2134105230095473]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5633242205750628,5.6407101117618232,5.7191724414082765,5.7987261827833185,5.8793865174341544,5.9611688380834504,6.044088751566786]
[null,null,null,null,"Coincident",4.093223001666626,4.1501597713480773,4.207888532020597,4.266420300286172,4.3257662459878228,4.385937694341191,4.4469461280957701]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.2591369783412727,6.3462016314020424,6.4344773545893839,6.5239809938999205,6.6147296296582452,6.7067405797764206,6.8000314030588278]
[null,null,null,null,"Coincident",4.6051681395049773,4.6692260707724875,4.7341750484543654,4.8000274670144494,4.8667958933236823,4.9344930690582984,5.0031319131313658]
[null,"Beachport 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.67598999999999998,0.72509543182757508,0.73785868161823154,0.75855996550039817,0.77820545466899016,0.79728203176501333,0.81632695862495608]
[null,null,null,null,"Coincident",0.67598999999999998,0.72509543182757508,0.73785868161823154,0.75855996550039817,0.77820545466899016,0.79728203176501333,0.81632695862495608]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1925507098356189,1.1781377282310792,1.1483336831933189,1.1489476101951046,1.1506261290467907,1.1552355053361485,1.1602174651478796]
[null,null,null,null,"Coincident",1.1925507098356189,1.1781377282310792,1.1483336831933189,1.1489476101951046,1.1506261290467907,1.1552355053361485,1.1602174651478796]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2233545316724865,1.2085692598887345,1.1779953704445358,1.1786251553027867,1.1803470306299926,1.1850754680249498,1.1901861128487088]
[null,null,null,null,"Coincident",1.2233545316724865,1.2085692598887348,1.1779953704445358,1.1786251553027867,1.1803470306299926,1.18507546802495,1.1901861128487088]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0490013174768289,1.0357560165397759,1.0226779584783898,1.0097650315868214,0.99701515082284831,0.98442625747120427,0.97199631881115978]
[null,null,null,null,"Coincident",1.0490013174768289,1.0357560165397759,1.0226779584783898,1.0097650315868214,0.99701515082284831,0.98442625747120427,0.97199631881115978]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0760972299807505,1.0625098002881859,1.0490939333880036,1.0358474630285728,1.0227682503106159,1.0098541833418426,0.99710317689594286]
[null,null,null,null,"Coincident",1.0760972299807507,1.0625098002881859,1.0490939333880036,1.0358474630285728,1.0227682503106161,1.0098541833418426,0.99710317689594286]
[null,"Belvedere Road 7.6kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8260000000000002E-2,1.9586447410718386E-2,1.993121129949986E-2,2.0490399221937117E-2,2.1021067770611638E-2,2.15363687333084E-2,2.2050814752424888E-2]
[null,null,null,null,"Coincident",1.8260000000000002E-2,1.9586447410718386E-2,1.993121129949986E-2,2.0490399221937117E-2,2.1021067770611638E-2,2.15363687333084E-2,2.2050814752424888E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10558669694241735,0.1058053886571016,0.10602453332720027,0.10624413189087699,0.10646418528823846,0.1066846944613386,0.10690566035418247]
[null,null,null,null,"Coincident",0.10558669694241735,0.1058053886571016,0.10602453332720027,0.10624413189087699,0.10646418528823846,0.1066846944613386,0.10690566035418247]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10863140129750978,0.1088563992196558,0.10908186315866586,0.10930779407975653,0.10953419295014351,0.1097610607390458,0.10998839841768988]
[null,null,null,null,"Coincident",0.10863140129750978,0.1088563992196558,0.10908186315866586,0.10930779407975653,0.10953419295014351,0.1097610607390458,0.10998839841768988]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.502802724817562E-2,9.5224849791391439E-2,9.5422079994480241E-2,9.5619718701789286E-2,9.5817766759414613E-2,9.6016225015204751E-2,9.6215094318764224E-2]
[null,null,null,null,"Coincident",9.502802724817562E-2,9.5224849791391439E-2,9.5422079994480241E-2,9.5619718701789286E-2,9.5817766759414613E-2,9.6016225015204751E-2,9.6215094318764224E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7768261167758802E-2,9.7970759297690224E-2,9.8173676842799276E-2,9.837701467178088E-2,9.8580773655129156E-2,9.8784954665141228E-2,9.89895585759209E-2]
[null,null,null,null,"Coincident",9.7768261167758802E-2,9.7970759297690224E-2,9.8173676842799276E-2,9.837701467178088E-2,9.8580773655129156E-2,9.8784954665141228E-2,9.89895585759209E-2]
[null,"Berri 11kV","Substation Rating","MVA","Non-Coincident",28,28,28,28,28,28,28]
[null,null,null,null,"Coincident",28,28,28,28,28,28,28]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.32925,5.7163786891331299,5.8169993328510197,5.9802004410464606,6.1350780622416243,6.2854705953988921,6.4356136100416377]
[null,null,null,null,"Coincident",5.32925,5.7163786891331299,5.8169993328510197,5.9802004410464606,6.1350780622416243,6.2854705953988921,6.4356136100416377]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.144281398999643,10.960253940040429,10.94216336347203,10.905969762849338,10.876295790385429,10.833545577139793,10.809263624990228]
[null,null,null,null,"Coincident",10.079887483201077,9.9134365462842471,9.8970738065267909,9.8643370683893821,9.8374972666196001,9.7988301400485192,9.7768673649913449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.798493878471291,11.603663294940279,11.584510731463244,11.546192426307652,11.514776476734017,11.469516660401018,11.443809263617258]
[null,null,null,null,"Coincident",10.671615917460835,10.495393665889253,10.478070369935805,10.443411858481671,10.414996456398537,10.374059419741519,10.350807344727551]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.429706449874045,10.373427934552888,10.317453097125444,10.261780298951061,10.206407910231162,10.151334309961534,10.096557885884875]
[null,null,null,null,"Coincident",9.4335618182598875,9.3826584821138894,9.3320298194878948,9.2816743482483481,9.2315905942592611,9.1817770913390575,9.1322323812176496]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.041970612312191,10.982388330177274,10.92312755300456,10.86418654595885,10.805563583566075,10.747256949662795,10.689264937345968]
[null,null,null,null,"Coincident",9.9873484327944819,9.9334568736701563,9.8798561124652551,9.826544580039247,9.7735207157186519,9.7207829672513526,9.6683297907611632]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Binnies 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.0000000000000001E-3,6.4358534755920207E-3,6.549138433570599E-3,6.7328803577011327E-3,6.9072511842097383E-3,7.0765724205832633E-3,7.2456127335459638E-3]
[null,null,null,null,"Coincident",6.0000000000000001E-3,6.4358534755920207E-3,6.549138433570599E-3,6.7328803577011327E-3,6.9072511842097383E-3,7.0765724205832633E-3,7.2456127335459638E-3]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.73977194055041651,0.73700425465664787,0.73450349516354152,0.72890825676957771,0.72349077384717198,0.71786790734694106,0.71248624088390033]
[null,null,null,null,"Coincident",0.43535746577021484,0.43372867634105294,0.43225697370441396,0.42896416321235359,0.42577596221868363,0.42246689252338887,0.41929976959733317]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.74994553096824779,0.74713978293512917,0.74460463216354666,0.7389324461853477,0.73344046023122766,0.7277402661958311,0.72228458926096895]
[null,null,null,null,"Coincident",0.4413446468179249,0.43969345773338159,0.43820151575131561,0.43486342143131657,0.43163137523441386,0.42827679810919556,0.4250661198525218]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.63257229264475556,0.62817536172973676,0.62380899333175555,0.61947297501457721,0.61516709581858475,0.61089114625051522,0.60664491827326705]
[null,null,null,null,"Coincident",0.3722702297107563,0.36968262588936096,0.36711300817859743,0.3645612515592595,0.36202723188113384,0.35951082585695976,0.35701191105643099]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.64127163775677476,0.63681423878157017,0.63238782262932935,0.62799217394232332,0.62362707885974811,0.61929232500731979,0.61498770148694093]
[null,null,null,null,"Coincident",0.37738981405050742,0.37476662463847327,0.37216166868806216,0.36957481946076209,0.36700595109900458,0.36445493862004141,0.36192165790986386]
[null,"Birdwood 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.6574699999999998,1.7778723433649175,1.8091667465817098,1.8599245344131492,1.9080936033820188,1.9548677483240233,2.0015642895784045]
[null,null,null,null,"Coincident",1.6574699999999998,1.7778723433649175,1.8091667465817098,1.8599245344131492,1.9080936033820188,1.9548677483240233,2.0015642895784045]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.517832198349232,2.5477191807230488,2.5310948532739546,2.5540591148676355,2.5767933421026745,2.5991520828395842,2.6066106496377168]
[null,null,null,null,"Coincident",2.3170417901113542,2.3445453652844166,2.3292467836484754,2.350379706575783,2.3713009397715492,2.3918766305168067,2.3987403964885581]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5994103567394244,2.6302656820327952,2.6131027237652287,2.6368110310386936,2.6602818508041941,2.6833650182500945,2.6910652437830787]
[null,null,null,null,"Coincident",2.3921143077613896,2.420509003086635,2.4047147450046382,2.426532377951518,2.4481314623863311,2.4693738087410071,2.4764599618074836]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1772541521980138,2.1430721365330685,2.1094267647843785,2.0763096118580089,2.043712384930616,2.0116269213728515,1.9800451867053688]
[null,null,null,null,"Coincident",2.0036239355600354,1.972167844555303,1.9412056015445662,1.9107294533126802,1.8807317683668638,1.8512050350257074,1.822141859538182]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2477975284405467,2.2125080101033268,2.1777725230294731,2.1435823691506846,2.1099289869548401,2.0768039493421191,2.0441989615147831]
[null,null,null,null,"Coincident",2.0685416655329312,2.0360663922427378,2.0041009676990531,1.9726373874813448,1.9416677728352674,1.9111843686997549,1.8811795417650847]
[null,"Black Point 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.17563000000000001,0.18838815765303779,0.19170419718133408,0.19708262953717501,0.20218675424712607,0.20714306903783977,0.21209116073211298]
[null,null,null,null,"Coincident",0.17563000000000001,0.18838815765303779,0.19170419718133408,0.19708262953717501,0.20218675424712607,0.20714306903783977,0.21209116073211298]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.51680490907389354,0.50466984951386251,0.49281973243007343,0.48124786710837153,0.46994771993878848,0.45891291072659002,0.44813720908994376]
[null,null,null,null,"Coincident",0.51680490907389354,0.50466984951386251,0.49281973243007343,0.48124786710837153,0.46994771993878848,0.45891291072659002,0.44813720908994376]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52274061719070575,0.51046618168771485,0.49847996133763628,0.48677518858082547,0.47534525476622808,0.46418370642005796,0.4532842416020913]
[null,null,null,null,"Coincident",0.52274061719070575,0.51046618168771485,0.49847996133763628,0.48677518858082547,0.47534525476622808,0.46418370642005796,0.4532842416020913]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.46512441816650418,0.45420286456247627,0.44353775918706612,0.43312308039753439,0.42295294794490962,0.41302161965393103,0.40332348818094937]
[null,null,null,null,"Coincident",0.46512441816650418,0.45420286456247627,0.44353775918706612,0.43312308039753439,0.42295294794490962,0.41302161965393103,0.40332348818094937]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.47046655547163524,0.45941956351894342,0.44863196520387266,0.43809766972274294,0.42781072928960523,0.41776533577805214,0.40795581744188214]
[null,null,null,null,"Coincident",0.47046655547163524,0.45941956351894342,0.44863196520387266,0.43809766972274294,0.42781072928960523,0.41776533577805214,0.40795581744188214]
[null,"Blackpool 11kV","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",24,24,24,24,24,24,24]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.76417,6.1828922547338765,6.2917245474391068,6.4682444952416898,6.6357616764143739,6.7984277415922376,6.9608239250539397]
[null,null,null,null,"Coincident",5.76417,6.1828922547338765,6.2917245474391068,6.4682444952416898,6.6357616764143739,6.7984277415922376,6.9608239250539397]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.286781608668466,15.333944982420411,15.277538929967521,15.374414193622657,15.47527241052383,15.577293585113281,15.684709761728584]
[null,null,null,null,"Coincident",15.066722501469098,15.113206940296342,15.057612874686805,15.153093581621279,15.252499905656238,15.353052446155774,15.458922325549736]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.74783609621567,15.796421933222003,15.738314655208759,15.838111709479076,15.942011844208258,16.047110011821712,16.157765896541143]
[null,null,null,null,"Coincident",15.521139932146047,15.569026357321436,15.511755555948517,15.610115993197274,15.712520445481864,15.816105684506072,15.925168635158602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.182666291371886,14.213998498641912,14.245399924716939,14.276870722514472,14.308411045289839,14.34002104663694,14.371700880488993]
[null,null,null,null,"Coincident",13.978501349287798,14.009382517370183,14.040331907826218,14.071349671372104,14.102435959056999,14.133590922263759,14.164814712709672]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.610420288675904,14.642697485881444,14.675045989554482,14.707465957224569,14.739957546769261,14.772520916414905,14.805156224737399]
[null,null,null,null,"Coincident",14.400097663100459,14.431910217624381,14.463793052131747,14.495746321884408,14.527770182487213,14.559864789888779,14.592030300382238]
[null,"Blackwood 11kV","Substation Rating","MVA","Non-Coincident",57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056]
[null,null,null,null,"Coincident",57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056,57.87557735849056]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.784189999999999,12.640220028089455,12.862715272916386,13.223590230403019,13.566060055408759,13.898612325485514,14.230612853087502]
[null,null,null,null,"Coincident",11.784189999999999,12.640220028089455,12.862715272916386,13.223590230403019,13.566060055408759,13.898612325485514,14.230612853087502]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.056640924036245,28.247425463419336,28.255178017654035,28.387024909914807,28.506752926416283,28.630071004902746,28.731781667562966]
[null,null,null,null,"Coincident",27.004133185609078,27.187760695588093,27.195222423014741,27.32212325367221,27.4373598321496,27.556051796189703,27.653946918000958]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.702303329566814,28.897478359064873,28.905409321428674,29.04029038238588,29.162773678086783,29.288929653220123,29.392980964972981]
[null,null,null,null,"Coincident",27.625574420826624,27.813427717496772,27.821061160307764,27.950882336840134,28.06877083386566,28.190194234617191,28.290342199169299]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.982026037430298,25.03416064720599,25.086404055905053,25.138756490578302,25.191218178750383,25.243789348420759,25.296470228064702]
[null,null,null,null,"Coincident",24.044858405810565,24.095037254724598,24.145320821114439,24.195709323513391,24.246202980910812,24.296802012753069,24.347506638944488]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.556932886401512,25.610267260527127,25.663712937346066,25.717270149134226,25.770939128652234,25.824720109146465,25.878613324350052]
[null,null,null,null,"Coincident",24.598198385495639,24.649531991188443,24.700972724201396,24.752520808096865,24.804176466903776,24.855939925118573,24.907811407706198]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Booleroo Centre 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.28929000000000005,0.31030467532566935,0.31576670957460651,0.32462582644656018,0.33303311584667261,0.34119693925842209,0.34934721794791873]
[null,null,null,null,"Coincident",0.28929000000000005,0.31030467532566935,0.31576670957460651,0.32462582644656018,0.33303311584667261,0.34119693925842209,0.34934721794791873]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.5333591153049938,0.52453778986193078,0.52113718610770965,0.51687224113727126,0.51285716274068338,0.50892633826943934,0.50580825947514263]
[null,null,null,null,"Coincident",0.44354950482408417,0.43621355720476712,0.43338556370469322,0.42983877098013618,0.42649977107644454,0.42323083801101136,0.42063779653946565]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.57350442505913313,0.56401912888379646,0.56036256570721465,0.55577660337340995,0.55145931477492838,0.54723262179509602,0.54387984889800278]
[null,null,null,null,"Coincident",0.47693495142374642,0.46904683570405065,0.46600598247816472,0.46219222686036143,0.4586019043832737,0.45508692259248529,0.45229870595641464]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.48729167995391864,0.47735740490048201,0.4676256570497398,0.45809230753797414,0.44875331167542198,0.43960470723024492,0.43064261274748311]
[null,null,null,null,"Coincident",0.40523912903384296,0.39697763569043515,0.38888456703105506,0.38095648943020527,0.37319003926272204,0.36558192147669849,0.35812890819550142]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.52396954833754694,0.51328753215105583,0.50282328715025781,0.49257237369674639,0.48253044266174411,0.47269323358090848,0.463056572846756]
[null,null,null,null,"Coincident",0.43574099896112145,0.42685767278541409,0.4181554484204893,0.40963063379591963,0.40127961211045376,0.39309884029752523,0.38508484752204453]
[null,"Booyoolie 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.0400000000000002E-3,3.2608324276332907E-3,3.3182301396757702E-3,3.4113260479019074E-3,3.499673933332934E-3,3.5854633597621867E-3,3.6711104516632884E-3]
[null,null,null,null,"Coincident",3.0400000000000002E-3,3.2608324276332907E-3,3.3182301396757702E-3,3.4113260479019074E-3,3.499673933332934E-3,3.5854633597621867E-3,3.6711104516632884E-3]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.979426843431863E-2,1.9833352575767339E-2,1.9872513889561055E-2,1.9911752528077968E-2,1.995106864399715E-2,1.999046239029913E-2,2.0029933920266509E-2]
[null,null,null,null,"Coincident",1.979426843431863E-2,1.9833352575767339E-2,1.9872513889561055E-2,1.9911752528077968E-2,1.995106864399715E-2,1.999046239029913E-2,2.0029933920266509E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.048355405407444E-2,2.0523999202460612E-2,2.0564524210524633E-2,2.060512923595088E-2,2.0645814436735091E-2,2.0686579971184955E-2,2.0727425997920757E-2]
[null,null,null,null,"Coincident",2.048355405407444E-2,2.0523999202460612E-2,2.0564524210524633E-2,2.060512923595088E-2,2.0645814436735091E-2,2.0686579971184955E-2,2.0727425997920757E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7814841590886768E-2,1.7850017318190605E-2,1.7885262500604949E-2,1.7920577275270171E-2,1.7955961779597435E-2,1.7991416151269219E-2,1.802694052823986E-2]
[null,null,null,null,"Coincident",1.7814841590886768E-2,1.7850017318190605E-2,1.7885262500604949E-2,1.7920577275270171E-2,1.7955961779597435E-2,1.7991416151269219E-2,1.802694052823986E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8435198648666998E-2,1.8471599282214552E-2,1.8508071789472169E-2,1.854461631235579E-2,1.858123299306158E-2,1.8617921974066462E-2,1.8654683398128685E-2]
[null,null,null,null,"Coincident",1.8435198648666998E-2,1.8471599282214552E-2,1.8508071789472169E-2,1.854461631235579E-2,1.858123299306158E-2,1.8617921974066462E-2,1.8654683398128685E-2]
[null,"Bordertown 11kV","Substation Rating","MVA","Non-Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,null,null,"Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.2764199999999999,3.5144265074165348,3.5762880244198967,3.6766239769298572,3.7718426541614112,3.8643039017079017,3.9566117454074439]
[null,null,null,null,"Coincident",3.2764199999999999,3.5144265074165348,3.5762880244198967,3.6766239769298572,3.7718426541614112,3.8643039017079017,3.9566117454074439]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.372380074186575,10.503119025320897,10.529960095020892,10.602138128948713,10.674249947070551,10.712601060338979,10.736552575148959]
[null,null,null,null,"Coincident",9.9303770894419365,10.055544801746748,10.081242080644989,10.15034435894094,10.219383243115386,10.256100082821558,10.279030940756313]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.790109903228153,10.926114141530492,10.954036189306576,11.029121069836391,11.104137067832131,11.144032706452947,11.16894882746857]
[null,null,null,null,"Coincident",10.330306005874002,10.460514633252176,10.487246826012445,10.559132080124215,10.630951387024895,10.669146934516908,10.693001293451083]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3877710725765766,9.3964018039056256,9.4050404699747432,9.4136870780788016,9.4223416355193823,9.4310041496047798,9.4396746276500068]
[null,null,null,null,"Coincident",8.9877256823671718,8.9959886283874795,9.0042591710211415,9.0125373172521694,9.0208230740710018,9.0291164484744986,9.0374174474659554]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.765847461715877,9.7748257809559735,9.7838123544941951,9.792807189919202,9.8018102948266357,9.8108216768191188,9.8198413435062601]
[null,null,null,null,"Coincident",9.3496909291007917,9.3582866511092302,9.3668902756716026,9.3755018100531942,9.3841212615259693,9.3927486373685731,9.4013839448663497]
[null,"Brinkworth Town 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.40361999999999998,0.43293986330307521,0.44056054242629417,0.45292086166255519,0.46465078716178904,0.47604102673263604,0.48741236858563691]
[null,null,null,null,"Coincident",0.40361999999999998,0.43293986330307521,0.44056054242629417,0.45292086166255519,0.46465078716178904,0.47604102673263604,0.48741236858563691]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.75589333568641992,0.72756055994536917,0.6945138799339734,0.68660419612316992,0.67909518517467338,0.67070868906628067,0.65915429818155247]
[null,null,null,null,"Coincident",0.7055004466406587,0.67905652261567795,0.64821295460504191,0.64083058304829199,0.63382217282969522,0.62599477646186208,0.61521067830278242]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.82162319096349978,0.79082669559279239,0.75490639123257963,0.74630890882953238,0.73814694040725359,0.72903118376769627,0.7164720632408178]
[null,null,null,null,"Coincident",0.76684831156593325,0.73810491588660632,0.70457929848374112,0.69655498157423035,0.68893714438010334,0.68042910484984997,0.66870725902476336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.68334940950272516,0.65800446320029671,0.63359954303111743,0.61009978409073473,0.58747161458934405,0.56568270789108122,0.54470193633214337]
[null,null,null,null,"Coincident",0.63779278220254354,0.6141374989869437,0.59135957349570967,0.56942646515135253,0.54830684028338783,0.52797052736500916,0.50838847391000053]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74277109728557067,0.71522224260901801,0.68869515546860582,0.66315193922905935,0.63855610281450426,0.61487250857726206,0.59206732210015578]
[null,null,null,null,"Coincident",0.69325302413319934,0.66754075976841698,0.64278214510403209,0.61894180994712222,0.59598569596020412,0.57388100800544461,0.55259616729347871]
[null,"Brukunga 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.29626999999999998,0.31779171820227464,0.32338554061899355,0.3324584105960191,0.34106855139096987,0.34942935184103391,0.35777628076127715]
[null,null,null,null,"Coincident",0.29626999999999998,0.31779171820227464,0.32338554061899355,0.3324584105960191,0.34106855139096987,0.34942935184103391,0.35777628076127715]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.48389414132198921,0.48569285524177341,0.48749825527632723,0.48931036627903635,0.49112921319567049,0.49295482106472693,0.49478721501777512]
[null,null,null,null,"Coincident",0.48389414132198921,0.48569285524177341,0.48749825527632723,0.48931036627903635,0.49112921319567049,0.49295482106472693,0.49478721501777512]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.48544080601733308,0.48724526914356386,0.48905643975530794,0.49087434278538961,0.49269900325931232,0.49453044629560372,0.49636869710616083]
[null,null,null,null,"Coincident",0.48544080601733308,0.48724526914356386,0.48905643975530794,0.49087434278538961,0.49269900325931232,0.49453044629560372,0.49636869710616083]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.43550472718979027,0.43712356971759608,0.43874842974869449,0.44037932965113274,0.44201629187610347,0.44365933895825427,0.44530849351599761]
[null,null,null,null,"Coincident",0.43550472718979027,0.43712356971759608,0.43874842974869449,0.44037932965113274,0.44201629187610347,0.44365933895825427,0.44530849351599761]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.43689672541559976,0.43852074222920751,0.44015079577977717,0.44178690850685065,0.44342910293338111,0.44507740166604337,0.44673182739554473]
[null,null,null,null,"Coincident",0.43689672541559976,0.43852074222920751,0.44015079577977717,0.44178690850685065,0.44342910293338111,0.44507740166604337,0.44673182739554473]
[null,"Bungama Napperby 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.79977999999999994,0.85787781545149766,0.8729783227335155,0.89747050874703516,0.92071355868454385,0.94328351508901354,0.96581602533923172]
[null,null,null,null,"Coincident",0.79977999999999994,0.85787781545149766,0.8729783227335155,0.89747050874703516,0.92071355868454385,0.94328351508901354,0.96581602533923172]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.134097265857706,1.0868122384969077,1.0498882433477059,1.0352778625914001,1.0214919248426877,1.0080454205814888,0.99621575005015028]
[null,null,null,null,"Coincident",0.90846534909020416,0.87058781408391017,0.84100995409528267,0.82930635066222091,0.81826316492634132,0.80749188140820827,0.79801575789357582]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2194594256534472,1.1686153102117287,1.1289120896211891,1.1132020027864518,1.0983784138093415,1.0839198070768696,1.0711997312367207]
[null,null,null,null,"Coincident",0.97684446138731618,0.93611592912248387,0.90431177859707801,0.89172725877658143,0.87985286551219477,0.86827084022387968,0.85808146010061903]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.94596721932423466,0.90917616743665186,0.87381601238285345,0.83983110297474095,0.80716795243933215,0.77577515423919619,0.74560330116684459]
[null,null,null,null,"Coincident",0.75776431705030312,0.72829295087857449,0.69996780049516527,0.67274428667610131,0.64657956399590477,0.62143245339579578,0.59726337737448798]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0171690530368114,0.97760878218994829,0.93958711008908968,0.90304419674703329,0.8679225295046582,0.83416683251526469,0.80172397974929521]
[null,null,null,null,"Coincident",0.81480034091430431,0.78311069986943482,0.7526535489195324,0.72338095341516262,0.69524684300634909,0.66820693913526419,0.64221868534891169]
[null,"Burnside 11kV","Substation Rating","MVA","Non-Coincident",31.2,31.2,31.2,31.2,31.2,31.2,31.2]
[null,null,null,null,"Coincident",31.2,31.2,31.2,31.2,31.2,31.2,31.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4191599999999998,4.7401777075328724,4.8236151000163074,4.9589459269230893,5.087374690535384,5.212084296357455,5.3365869945961633]
[null,null,null,null,"Coincident",4.4191599999999998,4.7401777075328724,4.8236151000163074,4.9589459269230893,5.087374690535384,5.212084296357455,5.3365869945961633]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.92212583785034,12.787031365869378,12.782142182689451,12.749189948932313,12.718056823630189,12.69105067822635,12.669363927268112]
[null,null,null,null,"Coincident",12.676903977891135,12.54437317988341,12.539576778232474,12.507249875643996,12.476707560475493,12.450213907929978,12.428938704225898]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.289371637371287,13.150437791126674,13.145409657745484,13.111520924097849,13.079502997824379,13.051729339893171,13.029426253179142]
[null,null,null,null,"Coincident",13.037180591447576,12.900883278588793,12.895950563580348,12.862704932963981,12.831294607601643,12.804048007535464,12.782168164216175]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.506069199337631,11.450668665924455,11.395534880350988,11.340666558253965,11.286062421454197,11.231721197926795,11.17764162177154]
[null,null,null,null,"Coincident",11.287719701330401,11.233370498171766,11.179282980806375,11.125455889244195,11.071887969561915,11.018577973873731,10.965524660302281]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.83307078061592,11.77609576840239,11.719395084981183,11.662967409487532,11.606811427416499,11.550925830592343,11.495309317138062]
[null,null,null,null,"Coincident",11.60851580705638,11.552622003820499,11.496997323467516,11.441640470198578,11.386550154453975,11.331725092883085,11.277164008314488]
[null,"Burra 11kV","Substation Rating","MVA","Non-Coincident",11.4,11.4,11.4,11.4,11.4,11.4,11.4]
[null,null,null,null,"Coincident",11.4,11.4,11.4,11.4,11.4,11.4,11.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.96111000000000002,1.0309271889877079,1.0490737399815064,1.0785064400983559,1.1064380309426369,1.13356075319113,1.1606384757230603]
[null,null,null,null,"Coincident",0.96111000000000002,1.0309271889877079,1.0490737399815064,1.0785064400983559,1.1064380309426369,1.13356075319113,1.1606384757230603]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8921882191370578,2.8304599758399429,2.7666939554193237,2.7092923366952064,2.6534948276155377,2.5986091502225288,2.5453166753997603]
[null,null,null,null,"Coincident",2.7093446857119146,2.6515188890266383,2.5917841430607793,2.5380114426492373,2.4857414404064135,2.4343256240420081,2.38440228831506]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9901091285361745,2.9262909501237484,2.8603660015023178,2.801020934329979,2.743334287193826,2.6865903436590259,2.6314935438050422]
[null,null,null,null,"Coincident",2.8010750557290263,2.7412914491886777,2.6795342620106601,2.6239409775547244,2.5699012681676545,2.5167446648577152,2.4651310731500971]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6617302823148998,2.5903327348271081,2.5208503362261667,2.4532317150660266,2.3874268778746894,2.3233871721917967,2.2610652505976891]
[null,null,null,null,"Coincident",2.4934562513846545,2.4265724418943337,2.3614827059793781,2.2981389198857971,2.2364942507184207,2.176503121815244,2.118121179050561]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7518485699473727,2.6780337134018195,2.6061988470004711,2.5362908600125804,2.468258066335562,2.4020501662811458,2.3376182093865636]
[null,null,null,null,"Coincident",2.5778772797488969,2.5087289829731243,2.4414355017793627,2.3759470830861384,2.3122153083754449,2.2501930578947689,2.189834475819346]
[null,"Cadell 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.70947000000000005,0.76100749422137859,0.77440287407755559,0.79612943789637058,0.81674791627688059,0.83676930587186804,0.85675747767814259]
[null,null,null,null,"Coincident",0.70947000000000005,0.76100749422137859,0.77440287407755559,0.79612943789637058,0.81674791627688059,0.83676930587186804,0.85675747767814259]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3888297747549729,2.391605378537105,2.394384207319376,2.3971662648489436,2.3999515548773203,2.4027400811603763,2.4055318474583465]
[null,null,null,null,"Coincident",2.3888297747549729,2.391605378537105,2.394384207319376,2.3971662648489436,2.3999515548773203,2.4027400811603763,2.4055318474583465]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5459864417798181,2.5489446473714183,2.5519062901299172,2.5548713740489912,2.5578399031269572,2.560811881366778,2.5637873127760664]
[null,null,null,null,"Coincident",2.5459864417798181,2.5489446473714183,2.5519062901299172,2.5548713740489912,2.5578399031269572,2.560811881366778,2.5637873127760664]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1499467972794757,2.1524448406833945,2.1549457865874384,2.1574496383640493,2.1599563993895883,2.1624660730443388,2.164978662712512]
[null,null,null,null,"Coincident",2.1499467972794757,2.1524448406833945,2.1549457865874384,2.1574496383640493,2.1599563993895883,2.1624660730443388,2.164978662712512]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2913877976018364,2.2940501826342765,2.2967156611169255,2.2993842366440922,2.3020559128142617,2.3047306932301002,2.3074085814984602]
[null,null,null,null,"Coincident",2.2913877976018364,2.2940501826342765,2.2967156611169255,2.2993842366440922,2.3020559128142617,2.3047306932301002,2.3074085814984602]
[null,"Caloote 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.86705999999999994,0.93004518575780293,0.94641599503528728,0.9729685404913907,0.99816686863014925,1.0226354804984874,1.0470634961247274]
[null,null,null,null,"Coincident",0.86705999999999994,0.93004518575780293,0.94641599503528728,0.9729685404913907,0.99816686863014925,1.0226354804984874,1.0470634961247274]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6877839388257194,1.6277206698216657,1.5922739316103134,1.5828290714423279,1.5749686976590338,1.567796691217745,1.5612416819720352]
[null,null,null,null,"Coincident",1.5696390631079191,1.5137802229341493,1.4808147563975915,1.4720310364413649,1.4647208888229015,1.4580509228325029,1.4519547642339927]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8474607607019509,1.7817150629903831,1.7429148016335234,1.73257638796026,1.7239723647822758,1.7161218335792112,1.7089466720618471]
[null,null,null,null,"Coincident",1.7181385074528144,1.6569950085810565,1.620910765519177,1.6112960408030419,1.6032942992475165,1.5959933052286666,1.5893204050175178]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5600544143431543,1.5364708179997235,1.5132437387183748,1.490367786972689,1.4678376547105942,1.4456481141227053,1.4237940164292817]
[null,null,null,null,"Coincident",1.4508506053391335,1.428917860739743,1.4073166770080887,1.3860420418846009,1.3650890188808527,1.344452746134116,1.324128435279232]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7076470801494279,1.6818323014692633,1.6564077689974941,1.6313675833187098,1.6067059341999221,1.5824170992423803,1.5584954425537654]
[null,null,null,null,"Coincident",1.5881117845389678,1.564104040366415,1.5404592251676696,1.5171718524864002,1.4942365188059277,1.4716479022954136,1.4494007615750018]
[null,"Caltowie 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.10094,0.10827250830437643,0.11017833891410271,0.11326949055105873,0.11620298908902182,0.11905153668894576,0.12189535822068827]
[null,null,null,null,"Coincident",0.10094,0.10827250830437643,0.11017833891410271,0.11326949055105873,0.11620298908902182,0.11905153668894576,0.12189535822068827]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1866648701549999E-2,7.785517072805366E-2,7.4990011237588111E-2,7.3821941603241376E-2,7.261146077714116E-2,7.1175368597740679E-2,6.9419606046274326E-2]
[null,null,null,null,"Coincident",8.1866648701549999E-2,7.785517072805366E-2,7.4990011237588111E-2,7.3821941603241376E-2,7.261146077714116E-2,7.1175368597740679E-2,6.9419606046274326E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.8028654517795679E-2,8.3715237341993168E-2,8.0634420685578606E-2,7.9378431831442331E-2,7.8076839545313068E-2,7.6532654406172754E-2,7.4644737684165935E-2]
[null,null,null,null,"Coincident",8.8028654517795693E-2,8.3715237341993182E-2,8.0634420685578606E-2,7.9378431831442331E-2,7.8076839545313068E-2,7.6532654406172768E-2,7.4644737684165935E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.8730506867954996E-2,6.3080244463616555E-2,5.7894484166024038E-2,5.3135039747400532E-2,4.8766864229437865E-2,4.4757791808912172E-2,4.1078300999322158E-2]
[null,null,null,null,"Coincident",6.8730506867954996E-2,6.3080244463616555E-2,5.7894484166024038E-2,5.3135039747400532E-2,4.8766864229437865E-2,4.4757791808912172E-2,4.1078300999322158E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3903770825758053E-2,6.7828219853351121E-2,6.2252133511853804E-2,5.7134451341290894E-2,5.2437488418750386E-2,4.8126657859045331E-2,4.4170216128303394E-2]
[null,null,null,null,"Coincident",7.3903770825758053E-2,6.7828219853351135E-2,6.2252133511853804E-2,5.7134451341290894E-2,5.2437488418750386E-2,4.8126657859045345E-2,4.4170216128303394E-2]
[null,"Cambrai 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.47149999999999997,0.50575081895693963,0.51465312857142287,0.52909218144268066,0.54279482222581521,0.55610064938416803,0.56938440064448692]
[null,null,null,null,"Coincident",0.47149999999999997,0.50575081895693963,0.51465312857142287,0.52909218144268066,0.54279482222581521,0.55610064938416803,0.56938440064448692]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.95987906311288496,0.96186716961001451,0.96385939388363884,0.9658557444625181,0.96785622989307696,0.96986085873944183,0.97186963958347694]
[null,null,null,null,"Coincident",0.95987906311288496,0.96186716961001451,0.96385939388363884,0.9658557444625181,0.96785622989307696,0.96986085873944183,0.97186963958347694]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.98755819361372521,0.98960362926959811,0.99165330144241692,0.99370721890687763,0.99576539045585011,0.99782782490041644,0.999894531069908]
[null,null,null,null,"Coincident",0.98755819361372521,0.98960362926959811,0.99165330144241692,0.99370721890687763,0.99576539045585011,0.99782782490041644,0.999894531069908]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.86389115680159645,0.86568045264901305,0.86747345449527502,0.86927017001626627,0.87107060690376925,0.87287477286549764,0.87468267562512925]
[null,null,null,null,"Coincident",0.86389115680159645,0.86568045264901305,0.86747345449527502,0.86927017001626627,0.87107060690376925,0.87287477286549764,0.87468267562512925]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.88880237425235276,0.89064326634263835,0.89248797129817536,0.89433649701618989,0.89618885141026505,0.89804504241037475,0.89990507796291719]
[null,null,null,null,"Coincident",0.88880237425235276,0.89064326634263835,0.89248797129817536,0.89433649701618989,0.89618885141026505,0.89804504241037475,0.89990507796291719]
[null,"Campbell Park 11kV","Substation Rating","MVA","Non-Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,null,null,"Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.11686999999999999,0.12535969928207324,0.12756630145523265,0.13114528790075522,0.13454174098309868,0.13783983646559433,0.1411324600282528]
[null,null,null,null,"Coincident",0.11686999999999999,0.12535969928207324,0.12756630145523265,0.13114528790075522,0.13454174098309868,0.13783983646559433,0.1411324600282528]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4453111695124832,1.4433811593433536,1.4414537264318634,1.439528867336447,1.4376065786201342,1.4356868568505445,1.4337696985998809]
[null,null,null,null,"Coincident",1.4453111695124832,1.4433811593433536,1.4414537264318634,1.439528867336447,1.4376065786201342,1.4356868568505445,1.4337696985998809]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4649980422157642,1.4630417429918503,1.4610880561309179,1.4591369781445231,1.4571885055488802,1.4552426348648555,1.4532993626179611]
[null,null,null,null,"Coincident",1.4649980422157642,1.4630417429918503,1.4610880561309179,1.4591369781445231,1.4571885055488802,1.4552426348648555,1.4532993626179611]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.300780052561235,1.2990430434090183,1.2973083537886771,1.2955759806028024,1.2938459207581208,1.2921181711654901,1.2903927287398929]
[null,null,null,null,"Coincident",1.300780052561235,1.2990430434090183,1.2973083537886771,1.2955759806028024,1.2938459207581208,1.2921181711654901,1.2903927287398929]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3184982379941879,1.3167375686926652,1.3149792505178262,1.313223280330071,1.3114696549939922,1.30971837137837,1.307969426356165]
[null,null,null,null,"Coincident",1.3184982379941879,1.3167375686926652,1.3149792505178262,1.313223280330071,1.3114696549939922,1.30971837137837,1.307969426356165]
[null,"Campbelltown 11kV","Substation Rating","MVA","Non-Coincident",73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994]
[null,null,null,null,"Coincident",73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994,73.599999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",15.024269999999998,16.115666716288821,16.399337348890288,16.85943539529973,17.296067791564472,17.720055786899415,18.143340337372102]
[null,null,null,null,"Coincident",15.024269999999998,16.115666716288821,16.399337348890288,16.85943539529973,17.296067791564472,17.720055786899415,18.143340337372102]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.746043056778355,51.128343448834755,51.56249043252145,51.940208807473155,52.27126256462784,52.611741217733183,52.972594015787557]
[null,null,null,null,"Coincident",47.317383999218293,47.673854245257864,48.078668065248145,48.430865878408738,48.739551971118381,49.057026166190035,49.393497926039899]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.46796821761469,52.863240905133473,53.312119453483739,53.702654645951874,54.044941787222761,54.396973631950431,54.770070961300235]
[null,null,null,null,"Coincident",48.92296719635636,49.29153326403582,49.71008330975144,50.074231971481531,50.393392464121078,50.721639258817859,51.069528247564726]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.450049418611073,44.776460561700361,45.105268647779063,45.436491278377687,45.770146184280499,46.106251226474662,46.44482439710638]
[null,null,null,null,"Coincident",41.44677950104149,41.751136658148276,42.057728808665829,42.366572364876326,42.677683859582658,42.991079946993466,43.306777403614646]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.958337629549739,46.295824622620749,46.635789892243238,46.978251637206462,47.323228189939307,47.670738017491622,48.020799722522817]
[null,null,null,null,"Coincident",42.853160139993513,43.167844806697772,43.484840305068481,43.804163604292754,44.125831798167944,44.449862106016717,44.77627187360882]
[null,"Cape Jervis 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.40582000000000001,0.43529967624412569,0.44296189318527013,0.45538958446037897,0.46718344592933264,0.47863576995351664,0.49006909325460385]
[null,null,null,null,"Coincident",0.40582000000000001,0.43529967624412569,0.44296189318527013,0.45538958446037897,0.46718344592933264,0.47863576995351664,0.49006909325460385]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.58027029895504645,0.59402277093982059,0.6067616235104456,0.61948283044129304,0.63218902412027922,0.64488273174813893,0.6575663815982199]
[null,null,null,null,"Coincident",0.35079711064576719,0.32597349350873545,0.30817148532133098,0.29989837761901444,0.29207840057623635,0.28447405328751729,0.27663963830316091]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.63072647706091223,0.64567476619695063,0.65952129878381172,0.6733486513915623,0.68715968530184945,0.70095714746280935,0.71474367729316945]
[null,null,null,null,"Coincident",0.38129993239218429,0.35431783006341788,0.33496788585832776,0.32597540755153809,0.31747546092361195,0.3092098936795214,0.30069425368930514]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.38245917443018834,0.34781705383685846,0.31631272310303649,0.28766196968532731,0.26160632424604424,0.23791072890306092,0.21636141668330336]
[null,null,null,null,"Coincident",0.33465177762641474,0.30433992210725114,0.27677363271515687,0.25170422347466137,0.22890553371528868,0.20817188779017828,0.18931623959789043]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.41571510405130263,0.37806075103840969,0.34381702777411638,0.31267500861367586,0.28435374956412324,0.25859775378171862,0.23517466663779726]
[null,null,null,null,"Coincident",0.36375071604488973,0.33080315715860847,0.30083989930235178,0.27359063253696636,0.2488095308686078,0.22627303455900377,0.20577783330807262]
[null,"Caralue 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.63727999999999996,0.68357345048754714,0.69560582349097855,0.71512166572596292,0.73364217244553021,0.75162634536488349,0.76958068047236183]
[null,null,null,null,"Coincident",0.63727999999999996,0.68357345048754714,0.69560582349097855,0.71512166572596292,0.73364217244553021,0.75162634536488349,0.76958068047236183]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2327469850376511,2.1716189436140141,2.1142692315137701,2.0883673328675885,2.0684293394496187,2.0487553269799301,2.0298314269952029]
[null,null,null,null,"Coincident",1.9688941579855517,1.9149898667897141,1.8644174043150108,1.8415764387837816,1.8239945994505922,1.8066455453592476,1.7899579598979671]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.370367657853043,2.3054718441538267,2.2445872460956595,2.217088822297828,2.1959219032169157,2.175035236178124,2.1549449165920529]
[null,null,null,null,"Coincident",2.0902516340184647,2.0330248235798645,1.9793352070530721,1.9550863842656352,1.936420846432535,1.9180024421135284,1.9002862776174376]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9916436836841651,1.9633593786560819,1.9354767528628314,1.9079901018613477,1.8808938022201476,1.854182310368846,1.8278501614640095]
[null,null,null,null,"Coincident",1.7562830181264137,1.7313411849022899,1.7067535628378478,1.6825151216073488,1.6586209023231673,1.6350660165212636,1.611845645161065]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1144033808616394,2.084375705396079,2.0547744676207089,2.025593611485542,1.9968271669455162,1.9684692487390951,1.9405140551842186]
[null,null,null,null,"Coincident",1.8645357006867387,1.8380565182275446,1.8119533795756366,1.7862209443491806,1.760853948007713,1.7358472007750827,1.7111955865776847]
[null,"Cavan 11kV","Substation Rating","MVA","Non-Coincident",58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971]
[null,null,null,null,"Coincident",58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971,58.2263989747971]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.9324000000000003,5.2907006138350141,5.3838284016239371,5.5348765127208441,5.6782209568326847,5.8174143012141473,5.9563767078236847]
[null,null,null,null,"Coincident",4.9324000000000003,5.2907006138350141,5.3838284016239371,5.5348765127208441,5.6782209568326847,5.8174143012141473,5.9563767078236847]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.387276793890301,38.605188980727647,39.128000735254929,39.210062359436037,39.306106972514449,39.411424109867376,39.547669843039614]
[null,null,null,null,"Coincident",34.432286945736649,34.627747931063709,35.096695088923902,35.170302013588248,35.256451278483077,35.350917731863191,35.473126249151541]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.452404030983615,41.687715956352974,42.252272910918229,42.34088694882611,42.444600482028846,42.558326927183586,42.705451538530127]
[null,null,null,null,"Coincident",37.181618218164587,37.392686270206276,37.899077675910156,37.978561927868093,38.071589994291422,38.173599355724157,38.305565914901145]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.37199132859471,35.687321038960953,36.005461810353303,36.326438702459555,36.650276998366394,36.977002206550949,37.306640062890061]
[null,null,null,null,"Coincident",31.727662313939604,32.010504025482284,32.295867178188722,32.58377424988057,32.874247918761853,33.167311065205382,33.462986773554981]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.196355626005882,38.536863618465375,38.880407128084258,39.227013215503185,39.576709182599558,39.929522574638057,40.2854811824404]
[null,null,null,null,"Coincident",34.261036130735938,34.566462039602392,34.874610720350312,35.185506445598719,35.499173704349033,35.815637203914129,36.134921871864464]
[null,"Ceduna 11kV","Substation Rating","MVA","Non-Coincident",14.2,14.2,14.2,14.2,14.2,14.2,14.2]
[null,null,null,null,"Coincident",14.2,14.2,14.2,14.2,14.2,14.2,14.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.6341899999999998,2.8255434778116242,2.8752791617212226,2.9559476849087911,3.0325019994889084,3.1068393840960375,3.1810534344299071]
[null,null,null,null,"Coincident",2.6341899999999998,2.8255434778116242,2.8752791617212226,2.9559476849087911,3.0325019994889084,3.1068393840960375,3.1810534344299071]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6071300256862067,6.5557306799762864,6.5191266413032904,6.5098760573931118,6.5002199595796846,6.4888435112659284,6.4795016382593662]
[null,null,null,null,"Coincident",6.4271332547551152,6.3771341715222141,6.3415273296258157,6.3325287575916844,6.3231357189914794,6.3120691970683307,6.3029818229090884]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.8163236020323783,6.7632968609315531,6.7255338728010852,6.7159903988276053,6.7060285716540351,6.6942919246004902,6.6846542711542485]
[null,null,null,null,"Coincident",6.6306278107860441,6.5790456669814787,6.5423114486644955,6.5330279657146546,6.5233375266803888,6.5119206188423551,6.5025455221329924]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7886536619270448,5.7693717661400461,5.7501540979829686,5.7310004435147928,5.7119105895071325,5.6928843234418611,5.6739214335087462]
[null,null,null,null,"Coincident",5.6309544849569209,5.612197882143664,5.5935037572193744,5.5748719020713873,5.5563021092802565,5.5377941721174455,5.5193478845430262]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9719328099171918,5.9520404147571311,5.9322142807888492,5.9124541872975689,5.8927599143037135,5.8731312425604498,5.8535679535512539]
[null,null,null,null,"Coincident",5.8092405944130938,5.7898901239436293,5.7706041095250553,5.751382336455487,5.7322245907482063,5.7131306591292805,5.6941003290351899]
[null,"Chain of Ponds 11kV","Substation Rating","MVA","Non-Coincident",0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994]
[null,null,null,null,"Coincident",0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994,0.61749999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.20627999999999999,0.22126464249085367,0.22515937934615718,0.23147642669776491,0.23747129571313075,0.24329255981965253,0.24910416577931019]
[null,null,null,null,"Coincident",0.20627999999999999,0.22126464249085367,0.22515937934615718,0.23147642669776491,0.23747129571313075,0.24329255981965253,0.24910416577931019]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.47514104507159993,0.48230515976740707,0.4845703310240273,0.4884502565604929,0.49232482784216752,0.49615014841030475,0.50060557730698774]
[null,null,null,null,"Coincident",0.30079493579129513,0.30533028259468914,0.30676428214021084,0.30922052532257011,0.31167337891621089,0.3140950536307171,0.31691562756934305]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.48983612893979378,0.49722181419320316,0.49955704229281167,0.50355696552628137,0.50755136890945107,0.51149499836113888,0.5160882240278224]
[null,null,null,null,"Coincident",0.31009787194978877,0.31477348721101972,0.31625183725794931,0.31878404672429911,0.32131276176928958,0.32380933363991454,0.32671714182406503]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.44857292076392163,0.45292048953186881,0.45731019493650782,0.46174244536612336,0.4662176531670994,0.47073623468228104,0.47529861028970832]
[null,null,null,null,"Coincident",0.28397559903199876,0.28672789055041692,0.28950685727835374,0.29231275775194099,0.29514585301304275,0.29800640663354083,0.30089468473985564]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.46244631006589859,0.46692833972357611,0.47145380921289465,0.47602313955270448,0.48063675584237053,0.48529508730132059,0.48999856730897767]
[null,null,null,null,"Coincident",0.2927583495175245,0.2955957634540381,0.29846067760655026,0.30135335850715567,0.30427407527117811,0.30722309962220706,0.31020070591737697]
[null,"Cheltenham 11kV","Substation Rating","MVA","Non-Coincident",29.9,29.9,29.9,29.9,29.9,29.9,29.9]
[null,null,null,null,"Coincident",29.9,29.9,29.9,29.9,29.9,29.9,29.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3448800000000003,3.5878595955730401,3.651013693946938,3.7534461418112279,3.8506543901732453,3.9450475930267581,4.0392841866972047]
[null,null,null,null,"Coincident",3.3448800000000003,3.5878595955730401,3.651013693946938,3.7534461418112279,3.8506543901732453,3.9450475930267581,4.0392841866972047]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.339219647438693,10.454481676383132,12.548474781121275,12.646727584926532,12.749373441706144,12.854826994849152,12.967328122274427]
[null,null,null,null,"Coincident",10.161441210061918,10.274721357965683,12.332709151400636,12.429272540479829,12.5301534458759,12.633793770503328,12.744360489402737]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.478522534554955,10.595337517586294,12.717543514113018,12.817120102469147,12.921148932498918,13.028023287686025,13.142040170882876]
[null,null,null,null,"Coincident",10.298348843915548,10.413155243528248,12.498870820205191,12.596735231928951,12.698975330944634,12.804012027535768,12.916068439437828]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.1505940694452743,9.2883387275387559,11.42815686749465,11.600185868934897,11.774804437326287,11.952051553636785,12.131966785618131]
[null,null,null,null,"Coincident",8.9932535379344483,9.1286297358435178,11.231654622714197,11.400725659423797,11.572341736593978,11.746541164931717,11.92336283183827]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.2738823074525261,9.4134828337073948,11.582131277589896,11.756478068707267,11.933449316657704,12.113084527609484,12.295423802420542]
[null,null,null,null,"Coincident",9.1144218876863725,9.2516220429015643,11.38298150901595,11.554330482005511,11.728258785421055,11.904805246139274,12.084009275501092]
[null,"Cheltenham 33kV","Substation Rating","MVA","Non-Coincident",19,19,19,19,19,19,19]
[null,null,null,null,"Coincident",19,19,19,19,19,19,19]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.1,0.10726422459320036,0.10915230722617665,0.11221467262835222,0.1151208530701623,0.11794287367638771,0.12076021222576606]
[null,null,null,null,"Coincident",0.1,0.10726422459320036,0.10915230722617665,0.11221467262835222,0.1151208530701623,0.11794287367638771,0.12076021222576606]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.9910260384869392,4.0061824038494702,0,0,0,0,0]
[null,null,null,null,"Coincident",2.1103723352447177,2.1183867089560136,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.5146384388173315,4.5317832805193374,0,0,0,0,0]
[null,null,null,null,"Coincident",2.3872477836613037,2.3963136226889494,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7766192000000003,3.7766192000000003,0,0,0,0,0]
[null,null,null,null,"Coincident",1.9969984168421056,1.9969984168421056,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2721019719429121,4.2721019719429121,0,0,0,0,0]
[null,null,null,null,"Coincident",2.2589994973700374,2.2589994973700374,0,0,0,0,0]
[null,"Clare 11kV","Substation Rating","MVA","Non-Coincident",12.6,12.6,12.6,12.6,12.6,12.6,12.6]
[null,null,null,null,"Coincident",12.6,12.6,12.6,12.6,12.6,12.6,12.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.1708699999999999,4.4738513642904154,4.5526008364044337,4.6803281162541532,4.8015411244474775,4.9192439353063513,5.0367514636608082]
[null,null,null,null,"Coincident",4.1708699999999999,4.4738513642904154,4.5526008364044337,4.6803281162541532,4.8015411244474775,4.9192439353063513,5.0367514636608082]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.6180711547657474,8.4775536055213045,8.388625420627168,8.3391330911658041,8.2940704280883555,8.250346629816864,8.2092218148022429]
[null,null,null,null,"Coincident",8.4245178693449816,8.2871562041524474,8.2002252576244903,8.1518444765361142,8.1077938759413044,8.0650520705838353,8.0248508779106249]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0510146017256385,8.9034379146491052,8.8100422712937263,8.7580636105721208,8.7107371480514342,8.6648168104850249,8.6216260205151887]
[null,null,null,null,"Coincident",8.8477378381558047,8.7034755763285201,8.6121775060020465,8.5613662341745176,8.5151026768148252,8.4702136642449268,8.4279928963540982]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8763892721650297,7.7768500182273206,7.6785687091082462,7.5815294473090402,7.4857165362383711,7.3911144776733391,7.2977079692525608]
[null,null,null,null,"Coincident",7.6994934223277518,7.6021897207870923,7.5061157118786834,7.4112558551457326,7.3175948065266985,7.2251174158733145,7.1338087244999766]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2720730696007596,8.1675332921197068,8.064314654452561,7.9624004604626917,7.8617742250138347,7.7624196713035278,7.6643207282302681]
[null,null,null,null,"Coincident",8.0862905561927008,7.9840986378816714,7.883198187901578,7.7835728850943768,7.6852066145635254,7.5880834650673181,7.4921877264451648]
[null,"Clarence Gardens 11kV","Substation Rating","MVA","Non-Coincident",35.9,35.9,35.9,35.9,35.9,35.9,35.9]
[null,null,null,null,"Coincident",35.9,35.9,35.9,35.9,35.9,35.9,35.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.3008499999999996,6.7585578952806635,6.8775231498605507,7.0704782003035298,7.2535922706713203,7.4314035560386742,7.6089198320271798]
[null,null,null,null,"Coincident",6.3008499999999996,6.7585578952806635,6.8775231498605507,7.0704782003035298,7.2535922706713203,7.4314035560386742,7.6089198320271798]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.679702338309724,17.536572049357058,17.383911352473923,17.324200173672459,17.271251321675738,17.221030525258882,17.157088618098388]
[null,null,null,null,"Coincident",16.861895048162712,16.725385515120212,16.57978642077093,16.522837292845249,16.47233768780638,16.424439947097181,16.363455790967848]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.129582442883077,17.982810041177071,17.826264719487259,17.765034121928096,17.710737926259092,17.6592392046424,17.593670223036334]
[null,null,null,null,"Coincident",17.290965117466698,17.150981944324084,17.001677915664356,16.94327965250233,16.891495027661598,16.842378474543299,16.779842507302458]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.423854311366938,15.301724122862277,15.180560993734803,15.060357266550671,14.941105344509639,14.822797690964949,14.705426828947026]
[null,null,null,null,"Coincident",14.710395438777841,14.593914607745093,14.478356102971659,14.363712621232441,14.249976917131226,14.137141802642773,14.025200146658545]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.81633180096167,15.69109387110907,15.566847608557781,15.443585161021867,15.321298738391864,15.199980612242488,15.079623115344175]
[null,null,null,null,"Coincident",15.084718157094912,14.965273339030988,14.846774316865519,14.72921360153455,14.612583763274531,14.496877431152758,14.382087292601536]
[null,"Clarendon 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8520000000000001,1.9865334394660705,2.0215007298287917,2.0782157370770831,2.1320381988594059,2.1843020204867005,2.2364791304211877]
[null,null,null,null,"Coincident",1.8520000000000001,1.9865334394660705,2.0215007298287917,2.0782157370770831,2.1320381988594059,2.1843020204867005,2.2364791304211877]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3187718716934711,2.3214228446456007,2.3040229927556797,2.3124031169346027,2.3212876259620159,2.3303344583579912,2.3375318336984798]
[null,null,null,null,"Coincident",2.280803876437751,2.2834114418732989,2.2662964983445981,2.2745394048355925,2.2832784372852015,2.2921771351908102,2.2992566593894432]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3974387113876223,2.4001796214598303,2.3821894608051548,2.3908538897462015,2.4000398153363878,2.4093935712907011,2.416835125361767]
[null,null,null,null,"Coincident",2.3581826108927659,2.3608786408015181,2.3431830543318783,2.3517056103267575,2.3607411238891434,2.3699417197305399,2.3772614244325005]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0737714903983009,2.0323857251364794,1.9918258857658357,1.9520754894794581,1.9131183824138982,1.8749387330845257,1.8375210259518899]
[null,null,null,null,"Coincident",2.0398151762519738,1.9991070690893804,1.9592113639561737,1.9201118479379409,1.8817926316775515,1.8442381429180044,1.8074331201741327]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1441264275911176,2.1013366055519929,2.0594007298317876,2.018301758426567,1.9780229894356205,1.9385480542741067,1.899860911021144]
[null,null,null,null,"Coincident",2.1090181088193409,2.066928935162236,2.0256797251506442,1.9852537158295238,1.9456344787781457,1.9068059134338737,1.8687522405491768]
[null,"Clearview 11kV","Substation Rating","MVA","Non-Coincident",26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614]
[null,null,null,null,"Coincident",26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614,26.597262247838614]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.4281200000000016,9.0403575657844399,9.1994874357908429,9.4575872667246816,9.7025236417769669,9.9403669248943718,10.177815598642239]
[null,null,null,null,"Coincident",8.4281200000000016,9.0403575657844399,9.1994874357908429,9.4575872667246816,9.7025236417769669,9.9403669248943718,10.177815598642239]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.128470711038368,22.172290877796634,22.087005843122377,22.202860467607703,22.313390179094032,22.426232573139512,22.547725232899111]
[null,null,null,null,"Coincident",19.817351908103198,19.856595454422337,19.780217670945802,19.883972326818231,19.98295820873609,20.084015234418242,20.19281908372837]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.483596270724686,22.528119679087347,22.441465959876908,22.559179860536346,22.671483392101166,22.786136720976486,22.909579138103339]
[null,null,null,null,"Coincident",20.135387812154864,20.175261152847625,20.097657631566662,20.203077379018076,20.303651821536263,20.406330646269705,20.516880618408962]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.563217646808564,19.740679375611258,19.919750894058897,20.100446804864518,20.282781843205193,20.466770877923633,20.652428912740696]
[null,null,null,null,"Coincident",17.520016345649566,17.678943800502967,17.839312917019683,18.001136772791334,18.164428564038893,18.329201606688819,18.495469337458903]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.877175113947157,20.057484811621578,20.239430133417088,20.423025916396245,20.608287132211483,20.79522888832598,20.983866429245641]
[null,null,null,null,"Coincident",17.801183792406682,17.962661771518686,18.12560454859257,18.290025411093783,18.455937767020945,18.623355145999234,18.792291200383655]
[null,"Cleve 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3527399999999998,1.4510060717620583,1.4765469207713819,1.5179727625127717,1.5572858278213135,1.5954604293699672,1.6335716948628278]
[null,null,null,null,"Coincident",1.3527399999999998,1.4510060717620583,1.4765469207713819,1.5179727625127717,1.5572858278213135,1.5954604293699672,1.6335716948628278]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4475698445802143,2.3336094577300583,2.2804069499422104,2.2494366245330619,2.2265994338233148,2.2049967640209607,2.1843567059807611]
[null,null,null,null,"Coincident",2.4378804185821741,2.3243711774827873,2.2713792874892635,2.2405315672334885,2.2177847842683356,2.1962676349960182,2.1757092867037215]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4485385285214423,2.3345330391395152,2.2813094751946625,2.250326892543113,2.2274806634723352,2.205869443899942,2.1852212170661884]
[null,null,null,null,"Coincident",2.4388452677027597,2.3252911026232552,2.272278239829725,2.2414183108554528,2.218662525310283,2.1971368601147092,2.176570375367433]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2249495774394363,2.1636366355541634,2.1040132945842305,2.0460329941923687,1.9896504571046569,1.9348216537531413,1.8815037678927984]
[null,null,null,null,"Coincident",2.2161414593268081,2.1550712427776211,2.0956839383609913,2.0379331700624568,1.9817738398515183,1.9271620924642325,1.8740552811562909]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2258301541185781,2.1644929461792333,2.1048460078549498,2.0468427603810988,1.9904379085642023,1.9355874054105582,1.8822484177295962]
[null,null,null,null,"Coincident",2.2170185499838504,2.155924163444912,2.0965133550910084,2.0387397305532664,1.9825581739525699,1.9279248126682125,1.8747969830774229]
[null,"Cleve 33kV","Substation Rating","MVA","Non-Coincident",17.8,17.8,17.8,17.8,17.8,17.8,17.8]
[null,null,null,null,"Coincident",17.8,17.8,17.8,17.8,17.8,17.8,17.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2789800000000002,1.3718879797021142,1.3960361789613545,1.4352032199820994,1.4723726865967621,1.5084657657462639,1.5444989623251031]
[null,null,null,null,"Coincident",1.2789800000000002,1.3718879797021142,1.3960361789613545,1.4352032199820994,1.4723726865967621,1.5084657657462639,1.5444989623251031]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1880481409768282,2.1317127419442152,2.0701059426689015,2.0498263176154157,2.017567761695862,1.9863360584504346,1.9560695916363824]
[null,null,null,null,"Coincident",2.0786457339279867,2.0251271048470043,1.9666006455354563,1.9473350017346447,1.9166893736110688,1.8870192555279128,1.8582661120545632]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1880481409768282,2.1317127419442152,2.0701059426689015,2.0498263176154157,2.017567761695862,1.9863360584504346,1.9560695916363824]
[null,null,null,null,"Coincident",2.0786457339279867,2.0251271048470043,1.9666006455354563,1.9473350017346447,1.9166893736110688,1.8870192555279128,1.8582661120545632]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8637348387520607,1.7941671225093849,1.7271961636179116,1.6627250327962841,1.6006604188468994,1.5409124936035288,1.4833947819200455]
[null,null,null,null,"Coincident",1.7705480968144576,1.7044587663839157,1.640836355437016,1.5795887811564699,1.5206273979045544,1.4638668689233523,1.4092250428240432]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8637348387520607,1.7941671225093849,1.7271961636179116,1.6627250327962841,1.6006604188468994,1.5409124936035288,1.4833947819200455]
[null,null,null,null,"Coincident",1.7705480968144576,1.7044587663839157,1.640836355437016,1.5795887811564699,1.5206273979045544,1.4638668689233523,1.4092250428240432]
[null,"Coffin Bay 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.83928000000000003,0.90024718416581195,0.9160934840878554,0.9417953044352344,0.96618629564725811,0.98987095019118676,1.0135163091684094]
[null,null,null,null,"Coincident",0.83928000000000003,0.90024718416581195,0.9160934840878554,0.9417953044352344,0.96618629564725811,0.98987095019118676,1.0135163091684094]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3632518989171925,1.3393513391457441,1.3058779974845705,1.3000929586564998,1.2946678122694135,1.2892685276471303,1.2785946351605277]
[null,null,null,null,"Coincident",1.3632518989171925,1.3393513391457441,1.3058779974845705,1.3000929586564998,1.2946678122694135,1.2892685276471303,1.2785946351605277]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4053341814349225,1.3806958342381033,1.3461892025285411,1.3402255850837581,1.3346329696154677,1.3290670142399299,1.3180636288991145]
[null,null,null,null,"Coincident",1.4053341814349225,1.3806958342381033,1.3461892025285411,1.3402255850837581,1.3346329696154677,1.3290670142399299,1.3180636288991145]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2950599892195045,1.2559693696283383,1.218058677262738,1.1812922967174686,1.1456356876172311,1.1110553521675204,1.0775188036849401]
[null,null,null,null,"Coincident",1.2950599892195045,1.2559693696283383,1.218058677262738,1.1812922967174686,1.1456356876172311,1.1110553521675204,1.0775188036849401]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3350372526929912,1.2947399430552273,1.2556589838681842,1.2177576603131237,1.1810003657863906,1.1453525684485959,1.1107807787834911]
[null,null,null,null,"Coincident",1.3350372526929912,1.2947399430552273,1.2556589838681842,1.2177576603131237,1.1810003657863908,1.1453525684485957,1.1107807787834911]
[null,"Collinsfield 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.2702,0.28982793485082736,0.29492953412512934,0.30320404544180773,0.31105654499557861,0.31868164467359966,0.32629409343401994]
[null,null,null,null,"Coincident",0.2702,0.28982793485082736,0.29492953412512934,0.30320404544180773,0.31105654499557861,0.31868164467359966,0.32629409343401994]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.50813702276758899,0.49824161224897007,0.47789357552233103,0.4762335127721255,0.47462900381521617,0.47227860118397474,0.4676469546572391]
[null,null,null,null,"Coincident",0.50813702276758899,0.49824161224897007,0.47789357552233103,0.4762335127721255,0.47462900381521617,0.47227860118397474,0.4676469546572391]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.50813702276758899,0.49824161224897007,0.47789357552233103,0.4762335127721255,0.47462900381521617,0.47227860118397474,0.4676469546572391]
[null,null,null,null,"Coincident",0.50813702276758899,0.49824161224897007,0.47789357552233103,0.4762335127721255,0.47462900381521617,0.47227860118397474,0.4676469546572391]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.44537811085288748,0.43784855778041754,0.43044629917547894,0.42316918300045303,0.4160150936000242,0.40898195108610169,0.40206771073313952]
[null,null,null,null,"Coincident",0.44537811085288748,0.43784855778041754,0.43044629917547894,0.42316918300045303,0.4160150936000242,0.40898195108610169,0.40206771073313952]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.44537811085288748,0.43784855778041754,0.43044629917547894,0.42316918300045303,0.4160150936000242,0.40898195108610169,0.40206771073313952]
[null,null,null,null,"Coincident",0.44537811085288748,0.43784855778041754,0.43044629917547894,0.42316918300045303,0.4160150936000242,0.40898195108610169,0.40206771073313952]
[null,"Coomandook 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15717,0.16858718179313301,0.17155468126738185,0.17636780096998117,0.18093544477037407,0.18537081455717855,0.1897988255552365]
[null,null,null,null,"Coincident",0.15717,0.16858718179313301,0.17155468126738185,0.17636780096998117,0.18093544477037407,0.18537081455717855,0.1897988255552365]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.52098238426008225,0.50851831949494597,0.49148292110497616,0.48674781601374439,0.48218541736595516,0.47751674720027448,0.47302341714684987]
[null,null,null,null,"Coincident",0.47947554595364716,0.46800449733738164,0.45232631475320612,0.44796845704561644,0.44376954620218406,0.43947283052772518,0.43533748556097451]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52530739354515654,0.51273985657545518,0.49556303640533017,0.49078862216641106,0.4861883481180132,0.48148092032361883,0.4769502882523351]
[null,null,null,null,"Coincident",0.4834559803231524,0.47188970316697115,0.45608136592248799,0.45168733083996626,0.44745356214157811,0.44312117667146245,0.43895150155091284]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.44529690963286211,0.43580074226060961,0.4265070851524328,0.41741161968109514,0.40851011931613018,0.39979844765983419,0.39127255652514231]
[null,null,null,null,"Coincident",0.409819958041233,0.40108035345413251,0.39252712507160714,0.38415629833287607,0.37596398343654841,0.36794637353308918,0.36009974295583153]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.44899360519678655,0.43941860404186034,0.43004779431874002,0.42087682154849149,0.41190142411350517,0.40311743127718408,0.39452076124586316]
[null,null,null,null,"Coincident",0.41322213665088875,0.40440997899456926,0.39578574477136791,0.38734542642512271,0.379085101862704,0.37100093263147438,0.36308916213561582]
[null,"Coonalpyn 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.19662000000000002,0.21090291839515055,0.21461526646810855,0.22063648932186614,0.22635062130655312,0.23189927822251352,0.23743872927830123]
[null,null,null,null,"Coincident",0.19662000000000002,0.21090291839515055,0.21461526646810855,0.22063648932186614,0.22635062130655312,0.23189927822251352,0.23743872927830123]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.5045742127465529,0.48316788969942037,0.46238505984613038,0.45487819812738861,0.44775329522406854,0.44066756572350402,0.43379535407549324]
[null,null,null,null,"Coincident",0.40218125665790488,0.38511890649011055,0.36855352439932576,0.36257002583096515,0.35689097539431081,0.35124314892422037,0.34576551125111882]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.53413337348546819,0.51147301698241443,0.48947267939146383,0.48152604781016556,0.47398375110262786,0.46648292266920355,0.45920812047335313]
[null,null,null,null,"Coincident",0.42574199383275807,0.40768009050023074,0.39014426881988051,0.383810242635373,0.37779849988020381,0.37181981026602567,0.3660212795144463]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.43720007052925774,0.42476422593508428,0.41268211008249867,0.40094366140940291,0.38953910454766616,0.37845894218254117,0.3676939471436339]
[null,null,null,null,"Coincident",0.3484793105443591,0.33856706477329085,0.3289367657728145,0.31958039376786762,0.31049015710017702,0.30165848573963933,0.29307802498026531]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.46281229333686835,0.44964792730819197,0.4368580122943912,0.4244318973030648,0.41235923430170357,0.40062996960021219,0.38923433547854919]
[null,null,null,null,"Coincident",0.3688940596424094,0.35840113087441239,0.34820666599124178,0.33830217540028579,0.32867941098934722,0.31933035925790554,0.31024723464375442]
[null,"Coonawarra 11kV","Substation Rating","MVA","Non-Coincident",13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204]
[null,null,null,null,"Coincident",13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204,13.452227171492204]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.41274,0.44272236058597514,0.45051523284532152,0.46315483980626093,0.47514980896178788,0.48679741681192268,0.49842569994062685]
[null,null,null,null,"Coincident",0.41274,0.44272236058597514,0.45051523284532152,0.46315483980626093,0.47514980896178788,0.48679741681192268,0.49842569994062685]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.9528725984371027,4.0118864415208284,4.0325389185670932,4.0422521721548224,4.0517248055335644,4.0606850886610228,4.071084122136738]
[null,null,null,null,"Coincident",2.9808845392520502,3.0253872263661448,3.0409613811083971,3.0482862029245479,3.055429571622001,3.0621865739732841,3.0700285464474741]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.3887986333428479,4.4543205714838772,4.4772506206515708,4.4880350598181638,4.4985523429816077,4.5085007734874889,4.5200466209110441]
[null,null,null,null,"Coincident",3.3096189331259542,3.3590294131054117,3.3763210984168213,3.384453707595501,3.3923848528566061,3.3998870229737332,3.4085938146095289]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7853522492711162,3.8377825291625913,3.8909390120778475,3.9448317565333157,3.9994709603642526,4.0548669626544225,4.1110302456925076]
[null,null,null,null,"Coincident",2.8545564559648651,2.8940944392479464,2.9341800565141725,2.9748208929501065,3.0160246388034584,3.0577990908382717,3.1001521538102628]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2028040025602902,4.2610163367560521,4.3200349602411672,4.3798710407935157,4.4405359008739973,4.5020410197690213,4.5643980357626699]
[null,null,null,null,"Coincident",3.1693592851163448,3.2132575496509843,3.2577638416939596,3.3028865829324352,3.3486343117009505,3.3950156845970878,3.4420394781195127]
[null,"Cordola 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.34852,0.37383727555222185,0.38041762114467087,0.39109057704433314,0.40121919712012966,0.41105450333694649,0.42087349164923993]
[null,null,null,null,"Coincident",0.34852,0.37383727555222185,0.38041762114467087,0.39109057704433314,0.40121919712012966,0.41105450333694649,0.42087349164923993]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0066170107941765,2.0089485179711675,2.0112827341482751,2.0136196624731122,2.0159593060969483,2.0183016681747152,2.0206467518650104]
[null,null,null,null,"Coincident",2.0066170107941765,2.0089485179711675,2.0112827341482751,2.0136196624731122,2.0159593060969483,2.0183016681747152,2.0206467518650104]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1386286110950468,2.1411135037919906,2.1436012837091298,2.1460919542011521,2.1485855186266432,2.1510819803480925,2.1535813427318953]
[null,null,null,null,"Coincident",2.1386286110950468,2.1411135037919906,2.1436012837091298,2.1460919542011521,2.1485855186266432,2.1510819803480925,2.1535813427318953]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8059553097147589,1.8080536661740507,1.8101544607334477,1.812257696225801,1.8143633754872535,1.8164715013572437,1.8185820766785095]
[null,null,null,null,"Coincident",1.8059553097147589,1.8080536661740507,1.8101544607334477,1.812257696225801,1.8143633754872535,1.8164715013572437,1.8185820766785095]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.924765749985542,1.9270021534127917,1.9292411553382167,1.9314827587810368,1.9337269667639789,1.9359737823132832,1.9382232084587057]
[null,null,null,null,"Coincident",1.924765749985542,1.9270021534127917,1.9292411553382167,1.9314827587810368,1.9337269667639789,1.9359737823132832,1.9382232084587057]
[null,"Coromandel Place 11kV","Substation Rating","MVA","Non-Coincident",93,93,93,93,93,93,93]
[null,null,null,null,"Coincident",93,93,93,93,93,93,93]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.25004999999999999,0.26821419359529747,0.27293534421905469,0.28059278890719469,0.28785969310194082,0.29491615562780749,0.30196091067052805]
[null,null,null,null,"Coincident",0.25004999999999999,0.26821419359529747,0.27293534421905469,0.28059278890719469,0.28785969310194082,0.29491615562780749,0.30196091067052805]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.415056883964084,53.292287890712899,54.346278794904201,54.631709404916876,54.905508501455301,55.187667101741361,55.494253656410478]
[null,null,null,null,"Coincident",46.874848993114561,49.550037266135369,50.530015620375778,50.795402938556357,51.049975522580802,51.312320595620371,51.597378261755928]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",52.255859689032846,55.238146907862195,56.330622136635697,56.62647466224341,56.910270973425334,57.202732018555928,57.520512954917997]
[null,null,null,null,"Coincident",48.586388339629629,51.359255647078548,52.375015908845995,52.650093302768447,52.913961084611358,53.185885152026728,53.481351116473576]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.551751571275439,50.189590141919389,50.862811535022935,51.54506322789284,52.236466349053401,52.937143651794393,53.647219535964993]
[null,null,null,null,"Coincident",44.212608534626568,46.665214805640773,47.291161756633912,47.925504888531592,48.568356824062747,49.219831696628717,49.880045170566824]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",49.28800663253233,52.022160489526861,52.719963186420458,53.427125906027641,54.143774199633313,54.870035302612841,55.606038157021743]
[null,null,null,null,"Coincident",45.826941609709046,48.36909978807909,49.017901913189448,49.675406788596824,50.341731149219029,51.016993295805364,51.701313115940138]
[null,"Cowell 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.1119700000000001,1.1927459982090101,1.2137409106629167,1.2477934952254883,1.2801093498842839,1.3114893724193286,1.342817331886851]
[null,null,null,null,"Coincident",1.1119700000000001,1.1927459982090101,1.2137409106629167,1.2477934952254883,1.2801093498842839,1.3114893724193286,1.342817331886851]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0081416470494995,1.9157685380053471,1.8592811181504043,1.8282978580806013,1.8036718566493066,1.7799315424260038,1.7570141586279124]
[null,null,null,null,"Coincident",2.0081416470494995,1.9157685380053471,1.8592811181504043,1.8282978580806013,1.8036718566493066,1.7799315424260038,1.7570141586279124]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0336135515440161,1.9400687527363993,1.8828648285622513,1.8514885670114092,1.8265502015805624,1.802508757694691,1.7793006825441111]
[null,null,null,null,"Coincident",2.0336135515440157,1.9400687527363991,1.8828648285622511,1.851488567011409,1.8265502015805621,1.8025087576946908,1.7793006825441109]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7574496281947114,1.7005488141227849,1.6454902734168233,1.5922143589309941,1.5406633547106066,1.4907814134660828,1.4425144960713276]
[null,null,null,null,"Coincident",1.7574496281947114,1.7005488141227849,1.6454902734168233,1.5922143589309941,1.5406633547106066,1.4907814134660828,1.4425144960713276]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7797416757447795,1.7221191137305054,1.6663621930608941,1.6124105100068291,1.560205616526176,1.5096909569446522,1.4608118066867768]
[null,null,null,null,"Coincident",1.779741675744779,1.7221191137305052,1.6663621930608938,1.6124105100068291,1.5602056165261757,1.5096909569446519,1.4608118066867766]
[null,"Croydon 11kV","Substation Rating","MVA","Non-Coincident",48.4,48.4,48.4,48.4,48.4,48.4,48.4]
[null,null,null,null,"Coincident",48.4,48.4,48.4,48.4,48.4,48.4,48.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.5757700000000003,5.9808064556002876,6.0860816006249898,6.2568320520098739,6.418873989230188,6.5762233675859232,6.7333116852205963]
[null,null,null,null,"Coincident",5.5757700000000003,5.9808064556002876,6.0860816006249898,6.2568320520098739,6.418873989230188,6.5762233675859232,6.7333116852205963]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.556554467534735,24.676993639323683,24.720604867042038,24.917905606148789,25.124823630228143,25.336184385146851,25.558164183024804]
[null,null,null,null,"Coincident",19.682938501437388,19.779474716019934,19.814430642523686,19.972574095395323,20.13842613901884,20.30783918701718,20.485763769880368]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.764892751586629,24.886353731643361,24.930334957862939,25.12930960026431,25.337983120870387,25.551137064530369,25.775000143315879]
[null,null,null,null,"Coincident",19.84992893317364,19.947284162871746,19.982536656133465,20.142021801124365,20.309280936700489,20.480131288281569,20.659565386754263]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.260556356305251,22.522187431906829,22.786893489940329,23.05471067105508,23.325675540665934,23.599825093945597,23.87719676087562]
[null,null,null,null,"Coincident",17.842615597729829,18.052322068478361,18.264493245347634,18.479158096333922,18.69634592989793,18.916086398966343,19.138409504980366]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.449415347880983,22.713266106598837,22.980217935959164,23.250307283229265,23.523571024045669,23.800046467448862,24.07977136097707]
[null,null,null,null,"Coincident",17.993992694282323,18.205478318793169,18.419449560039251,18.635935631781891,18.854966091135339,19.076570842602287,19.300780142156746]
[null,"Croydon Park 11kV","Substation Rating","MVA","Non-Coincident",26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487]
[null,null,null,null,"Coincident",26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487,26.422061491935487]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.7265699999999997,5.0699186603548299,5.1591602076602978,5.3039050520499069,5.4412677049583698,5.5746524843260383,5.7078159629993905]
[null,null,null,null,"Coincident",4.7265699999999997,5.0699186603548299,5.1591602076602978,5.3039050520499069,5.4412677049583698,5.5746524843260383,5.7078159629993905]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.436269727257066,16.307115430201709,16.176093464269705,16.154213887734123,16.13908687376847,16.126454217466719,16.119208769229235]
[null,null,null,null,"Coincident",16.25764308716678,16.129892417486676,16.000294376444007,15.978652583499713,15.963689967400738,15.951194600702287,15.944027894788706]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.093541799815505,16.959222735211664,16.822961315283845,16.800206793590093,16.784474863546411,16.771337038351284,16.763801850966249]
[null,null,null,null,"Coincident",16.90777203638309,16.774912728987449,16.640132175461773,16.617624946117466,16.602063988067581,16.589068942567096,16.58161564634273]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.219195904463334,15.190271838055541,15.161402741806672,15.132588511245995,15.103829042101326,15.07512423029865,15.046473971961742]
[null,null,null,null,"Coincident",15.053796219838919,15.025186495364295,14.996631143642071,14.968130061336884,14.939683145309761,14.91129029261775,14.88295140051353]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.827798257721797,15.797717543157813,15.767693996961407,15.737727510484147,15.707817975284096,15.677965283125413,15.648169325977952]
[null,null,null,null,"Coincident",15.655784384153202,15.62603058178178,15.596333326481643,15.566692510785137,15.53710802742885,15.507579769353233,15.47810762970219]
[null,"Crystal Brook 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.02173,1.095950761936106,1.1152418686220147,1.1465309746456631,1.1762242920737693,1.2050577232137563,1.2338433163743197]
[null,null,null,null,"Coincident",1.02173,1.095950761936106,1.1152418686220147,1.1465309746456631,1.1762242920737693,1.2050577232137563,1.2338433163743197]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9269025585836475,1.8751716321743539,1.8333952890296505,1.8161765113924893,1.7970525534990873,1.7807837134957918,1.7645513406299462]
[null,null,null,null,"Coincident",1.7519103757607775,1.7048774075806046,1.6668949944634903,1.6512399448264015,1.633852734399067,1.6190613535498375,1.6043031280649975]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.987539082772567,1.9341802673158699,1.891089289847633,1.8733286649738026,1.853602906885458,1.8368221126549023,1.8200789331239562]
[null,null,null,null,"Coincident",1.8070401774227363,1.7585271573841912,1.7193494988191587,1.7032018099503818,1.6852674519773874,1.6700106101640544,1.6547879670610997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.756594383193965,1.714235459482548,1.6728979886660942,1.632557339192968,1.5931894734824734,1.5547709336017017,1.5172788272877702]
[null,null,null,null,"Coincident",1.5970687838946163,1.5585566974242775,1.5209733003249009,1.4842961979659492,1.4485035357461911,1.4135739860713099,1.3794867356455371]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8118715830358465,1.7681796921275144,1.7255413975937921,1.683931292767733,1.6433245836446402,1.6036970741081864,1.565025151512798]
[null,null,null,null,"Coincident",1.6473259697157696,1.6076019698290405,1.5688358836740257,1.5310046118971856,1.4940856121681403,1.4580568857474845,1.4228969643785088]
[null,"Cudmore Park 11kV","Substation Rating","MVA","Non-Coincident",22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709]
[null,null,null,null,"Coincident",22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709,22.130865921787709]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.2692200000000002,3.5067034832458246,3.5684290582996123,3.6685445205006162,3.7635539527403599,3.8558120148032025,3.9479170101271892]
[null,null,null,null,"Coincident",3.2692200000000002,3.5067034832458246,3.5684290582996123,3.6685445205006162,3.7635539527403599,3.8558120148032025,3.9479170101271892]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.787474060636688,15.825862346686428,15.883664227988371,15.86566567413727,15.852519824283213,15.84127841845226,15.817498839753165]
[null,null,null,null,"Coincident",12.108239903805879,12.137681888964551,12.18201317609808,12.168209143412822,12.158126903330528,12.149505281015619,12.131267477894347]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.076152514351833,17.117674307187862,17.180194361817083,17.160726646499313,17.146507745098337,17.134348741086182,17.108628115289228]
[null,null,null,null,"Coincident",13.096594837376507,13.1284400728438,13.176389973970613,13.161459164485752,13.150553945026939,13.141228568655452,13.121502074953584]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.479034783959062,14.477298612697394,14.475562649618848,14.473826894698458,14.472091347911267,14.470356009232315,14.468620878636651]
[null,null,null,null,"Coincident",11.104729361161414,11.103397800579295,11.102066399663705,11.100735158395496,11.099404076755528,11.098073154724657,11.096742392283748]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.660909736533183,15.659031847445835,15.657154183534896,15.655276744773365,15.653399531134244,15.651522542590541,15.649645779115266]
[null,null,null,null,"Coincident",12.011171101436206,12.009730850038482,12.008290771340331,12.006850865321038,12.005411131959903,12.003971571236219,12.00253218312929]
[null,"Cummins 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.5258099999999999,1.6366482652655101,1.6654568188877257,1.7121826964306606,1.7565254882298431,1.7995841608416911,1.842571394161961]
[null,null,null,null,"Coincident",1.5258099999999999,1.6366482652655101,1.6654568188877257,1.7121826964306606,1.7565254882298431,1.7995841608416911,1.842571394161961]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4294015022411801,2.3279824177801633,2.2588819259134496,2.227342910051568,2.1980745770990828,2.1698474403181054,2.1430205599779559]
[null,null,null,null,"Coincident",2.2774521809089503,2.182376453459844,2.1175979202455739,2.0880315433448842,2.0605938272437316,2.0341321846690699,2.0089832181103131]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5187019994575883,2.4135549290456093,2.3419144254616464,2.3092160912262543,2.278871906183062,2.249607189838883,2.2217942008827101]
[null,null,null,null,"Coincident",2.3611672901464074,2.262596747317223,2.1954370699324044,2.1647838853732506,2.1363376074151739,2.1089032817179816,2.0828298836825403]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2354175944978714,2.1697698384599473,2.1060499673431328,2.0442013647374635,1.9841690768933571,1.9258997638940798,1.8693416522621396]
[null,null,null,null,"Coincident",2.095601188660992,2.0340594364959328,1.9743249877815681,1.9163447672373277,1.8600672582502846,1.8054424571015877,1.7524218285371345]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3175875867740801,2.2495267354738373,2.1834646347304885,2.1193425870150948,2.0571036185755527,1.9966924288142442,1.9380553411523256]
[null,null,null,null,"Coincident",2.1726317774467829,2.1088278594508227,2.0468976781800161,1.9867862074004641,1.9284400368397752,1.8718073247309401,1.8168377517498624]
[null,"Curramulka 7.6kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.14708000000000002,0.1577642215316791,0.16054121346826064,0.16504534050178046,0.16931975069559474,0.17347037860323108,0.17761412014165676]
[null,null,null,null,"Coincident",0.14708000000000002,0.1577642215316791,0.16054121346826064,0.16504534050178046,0.16931975069559474,0.17347037860323108,0.17761412014165676]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.23175827811313837,0.23897254357969522,0.24641137762108653,0.25408177069878574,0.26199093087617986,0.27014629059216988,0.27014629059216988]
[null,null,null,null,"Coincident",0.21755533113935382,0.21244692977817239,0.20745847842846737,0.20258716055249321,0.19783022574742817,0.19318498819246491,0.18864882513236469]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.23442011330158449,0.24171723745105017,0.24924150943396225,0.25700000000000001,0.26500000000000001,0.27324902723735411,0.27324902723735411]
[null,null,null,null,"Coincident",0.22005403988268546,0.21488696651802433,0.20984122083800844,0.20491395395584583,0.20010238387925411,0.19540379393971516,0.19081553125861236]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.19579979802541844,0.19120223680035517,0.18671263058562065,0.18232844449724389,0.17804720317268535,0.17386648937321841,0.16978394261912824]
[null,null,null,null,"Coincident",0.19579979802541844,0.19120223680035517,0.18671263058562065,0.18232844449724389,0.17804720317268535,0.17386648937321841,0.16978394261912824]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.1980486358944169,0.19339826986622191,0.18885709875420761,0.18442255856026124,0.18009214549132871,0.17586341454574364,0.17173397813275115]
[null,null,null,null,"Coincident",0.1980486358944169,0.19339826986622191,0.18885709875420761,0.18442255856026124,0.18009214549132871,0.17586341454574364,0.17173397813275115]
[null,"Curramulka South 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.512E-2,1.6218350758491894E-2,1.6503828852597911E-2,1.6966858501406855E-2,1.7406272984208541E-2,1.7832962499869823E-2,1.8258944088535831E-2]
[null,null,null,null,"Coincident",1.512E-2,1.6218350758491894E-2,1.6503828852597911E-2,1.6966858501406855E-2,1.7406272984208541E-2,1.7832962499869823E-2,1.8258944088535831E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6106639736722458E-2,2.5493631573380686E-2,2.4895017411416084E-2,2.4310459266299184E-2,2.3739627089691379E-2,2.3182198583095788E-2,2.2637859015883759E-2]
[null,null,null,null,"Coincident",2.6106639736722458E-2,2.5493631573380686E-2,2.4895017411416084E-2,2.4310459266299184E-2,2.3739627089691379E-2,2.3182198583095788E-2,2.2637859015883759E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6406484785922252E-2,2.578643598216292E-2,2.5180946500561012E-2,2.4589674474701496E-2,2.401228606551049E-2,2.3448455272765817E-2,2.2897863751033479E-2]
[null,null,null,null,"Coincident",2.6406484785922252E-2,2.578643598216292E-2,2.5180946500561012E-2,2.4589674474701496E-2,2.401228606551049E-2,2.3448455272765817E-2,2.2897863751033479E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3495975763050212E-2,2.2944268416042617E-2,2.2405515670274476E-2,2.1879413339669265E-2,2.1365664380722241E-2,2.0863978724786209E-2,2.0374073114295385E-2]
[null,null,null,null,"Coincident",2.3495975763050212E-2,2.2944268416042617E-2,2.2405515670274476E-2,2.1879413339669265E-2,2.1365664380722241E-2,2.0863978724786209E-2,2.0374073114295385E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3765836307330028E-2,2.3207792383946626E-2,2.2662851850504911E-2,2.2130707027231349E-2,2.1611057458959443E-2,2.1103609745489235E-2,2.0608077375930133E-2]
[null,null,null,null,"Coincident",2.3765836307330028E-2,2.3207792383946626E-2,2.2662851850504911E-2,2.2130707027231349E-2,2.1611057458959443E-2,2.1103609745489235E-2,2.0608077375930133E-2]
[null,"Darke Peak 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.12594,0.13508856445267653,0.13746641572064688,0.1413231587081468,0.14498320235656242,0.14853725510804272,0.15208541127712982]
[null,null,null,null,"Coincident",0.12594,0.13508856445267653,0.13746641572064688,0.1413231587081468,0.14498320235656242,0.14853725510804272,0.15208541127712982]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.63024632923685364,0.61839467745024734,0.60676589352269072,0.59535578647021881,0.58416024411945255,0.57317523162558226,0.56239679001821996]
[null,null,null,null,"Coincident",0.63024632923685364,0.61839467745024734,0.60676589352269072,0.59535578647021881,0.58416024411945255,0.57317523162558226,0.56239679001821996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.645229575757583,0.63309616712106132,0.62119092472283988,0.60950955794402872,0.59804785684993766,0.58680169067282695,0.57576700632318967]
[null,null,null,null,"Coincident",0.645229575757583,0.63309616712106132,0.62119092472283988,0.60950955794402872,0.59804785684993766,0.58680169067282695,0.57576700632318967]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.56722169631316832,0.55655520970522265,0.54608930417042167,0.53582020782319695,0.52574421970750729,0.51585770846302403,0.50615711101639793]
[null,null,null,null,"Coincident",0.56722169631316832,0.55655520970522265,0.54608930417042167,0.53582020782319695,0.52574421970750729,0.51585770846302403,0.50615711101639793]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.58070661818182479,0.56978655040895521,0.55907183225055601,0.54855860214962593,0.53824307116494385,0.52812152160554426,0.51819030569087066]
[null,null,null,null,"Coincident",0.58070661818182479,0.56978655040895521,0.55907183225055601,0.54855860214962593,0.53824307116494385,0.52812152160554426,0.51819030569087066]
[null,"Deloraine 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.23761000000000002,0.25487052405590338,0.25935679720011834,0.26663328363222771,0.27353865898001267,0.28024406214246489,0.28693834026964277]
[null,null,null,null,"Coincident",0.23761000000000002,0.25487052405590338,0.25935679720011834,0.26663328363222771,0.27353865898001267,0.28024406214246489,0.28693834026964277]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.34698924415282267,0.35370516500739346,0.36055107142689136,0.36752947926096013,0.37464295305310774,0.38189410698316789,0.38928560582800342]
[null,null,null,null,"Coincident",0.38510488336707022,0.38532624123792025,0.38554772634503526,0.38576933876155056,0.38599107856064341,0.38621294581553317,0.3864349405994813]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.3588972674207983,0.3658436661450718,0.37292451129626669,0.38014240506329117,0.38750000000000001,0.39500000000000002,0.40264516129032257]
[null,null,null,null,"Coincident",0.39832096423707664,0.39854991869693063,0.3987790047595608,0.39900822250061224,0.39923757199577359,0.39946705332077687,0.39969666655139785]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.34659439503036321,0.34679361711412826,0.34699295371053174,0.34719240488539549,0.34739197070457906,0.34759165123397984,0.3477914465395332]
[null,null,null,null,"Coincident",0.34659439503036321,0.34679361711412826,0.34699295371053174,0.34719240488539549,0.34739197070457906,0.34759165123397984,0.3477914465395332]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.35848886781336897,0.35869492682723764,0.35890110428360472,0.35910740025055099,0.35931381479619617,0.3595203479886992,0.35972699989625812]
[null,null,null,null,"Coincident",0.35848886781336897,0.35869492682723764,0.35890110428360472,0.35910740025055099,0.35931381479619617,0.3595203479886992,0.35972699989625812]
[null,"Desert Camp 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.3120000000000002E-2,2.4799488725947921E-2,2.5236013430692043E-2,2.5944032311675032E-2,2.6615941229821524E-2,2.726839239398084E-2,2.7919761066597115E-2]
[null,null,null,null,"Coincident",2.3120000000000002E-2,2.4799488725947921E-2,2.5236013430692043E-2,2.5944032311675032E-2,2.6615941229821524E-2,2.726839239398084E-2,2.7919761066597115E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.9359432743070609E-2,5.9594076417903138E-2,5.9829647622727015E-2,6.0066150024003256E-2,6.0303587302686132E-2,6.0541963154280475E-2,6.0781281288899175E-2]
[null,null,null,null,"Coincident",5.9359432743070609E-2,5.9594076417903138E-2,5.9829647622727015E-2,6.0066150024003256E-2,6.0303587302686132E-2,6.0541963154280475E-2,6.0781281288899175E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.4240895199756079E-2,6.4494834953349178E-2,6.4749778512979778E-2,6.5005729846622715E-2,6.5262692937938016E-2,6.5520671786332793E-2,6.5779670407023552E-2]
[null,null,null,null,"Coincident",6.4240895199756079E-2,6.4494834953349178E-2,6.4749778512979778E-2,6.5005729846622715E-2,6.5262692937938016E-2,6.5520671786332793E-2,6.5779670407023552E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.3423489468763546E-2,5.3634668776112823E-2,5.3846682860454312E-2,5.4059535021602934E-2,5.4273228572417523E-2,5.4487766838852425E-2,5.470315316000926E-2]
[null,null,null,null,"Coincident",5.3423489468763546E-2,5.3634668776112823E-2,5.3846682860454312E-2,5.4059535021602934E-2,5.4273228572417523E-2,5.4487766838852425E-2,5.470315316000926E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7816805679780467E-2,5.8045351458014267E-2,5.8274800661681794E-2,5.850515686196045E-2,5.873642364414422E-2,5.8968604607699517E-2,5.9201703366321204E-2]
[null,null,null,null,"Coincident",5.7816805679780467E-2,5.8045351458014267E-2,5.8274800661681794E-2,5.850515686196045E-2,5.873642364414422E-2,5.8968604607699517E-2,5.9201703366321204E-2]
[null,"Direk 11kV","Substation Rating","MVA","Non-Coincident",56.4,56.4,56.4,56.4,56.4,56.4,56.4]
[null,null,null,null,"Coincident",56.4,56.4,56.4,56.4,56.4,56.4,56.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.2563799999999992,6.7108574946040669,6.8289831188370691,7.0205763353857007,7.2023980273110189,7.3789543601147844,7.5552177656503812]
[null,null,null,null,"Coincident",6.2563799999999992,6.7108574946040669,6.8289831188370691,7.0205763353857007,7.2023980273110189,7.3789543601147844,7.5552177656503812]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.785417198871993,21.559834453273336,21.551152795639364,21.430159914068685,21.319877288882292,21.215958835914062,21.128128837867724]
[null,null,null,null,"Coincident",20.030244426501937,19.822836072028171,19.814853864350063,19.703608944429366,19.602211394026057,19.506665277356536,19.425911426613734]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.557341177164695,22.323765344776508,22.314776069453242,22.189496039941602,22.075305763963247,21.967705162294305,21.87676307872367]
[null,null,null,null,"Coincident",20.739977263965393,20.525219796979574,20.516954755263896,20.401768087504905,20.296777711690819,20.197846103808683,20.11423089708822]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.155157642978597,20.070670929511785,19.986538368807199,19.902758476321608,19.819329773734708,19.736250788923041,19.65352005593402]
[null,null,null,null,"Coincident",18.531329024281593,18.453649101694676,18.376294799054669,18.299264751422651,18.222557599581279,18.146171990010785,18.070106574865118]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.869316537842,20.781836201651473,20.694722566938974,20.607974096559371,20.521589259810948,20.435566532408401,20.349904396455969]
[null,null,null,null,"Coincident",19.18795070349438,19.107518343608266,19.027423141379931,18.947663683506494,18.868238562609381,18.789146377209484,18.710385731702438]
[null,"Dorrien TF4 11kV","Substation Rating","MVA","Non-Coincident",13.6,13.6,13.6,13.6,13.6,13.6,13.6]
[null,null,null,null,"Coincident",13.6,13.6,13.6,13.6,13.6,13.6,13.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.9950399999999999,3.2126064322561878,3.2691552623468811,3.3608743310881999,3.4479155977925888,3.5324362437572825,3.6168166602465837]
[null,null,null,null,"Coincident",2.9950399999999999,3.2126064322561878,3.2691552623468811,3.3608743310881999,3.4479155977925888,3.5324362437572825,3.6168166602465837]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1704464222319029,8.1452240746568858,8.2088883586900021,8.216835521339771,8.2286882521363438,8.2427536769759424,8.2564057563156847]
[null,null,null,null,"Coincident",8.1704464222319029,8.1452240746568858,8.2088883586900021,8.216835521339771,8.2286882521363438,8.2427536769759424,8.2564057563156847]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.5912573497981466,8.5647359496463249,8.6316792009515257,8.6400356745144737,8.6524988687279691,8.6672887196475497,8.6816439361077489]
[null,null,null,null,"Coincident",8.5912573497981466,8.5647359496463249,8.6316792009515257,8.6400356745144737,8.6524988687279691,8.6672887196475497,8.6816439361077489]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6483752297436203,7.6527529637566412,7.6571332034724442,7.6615159503252288,7.665901205750016,7.6702889711826483,7.6746792480597898]
[null,null,null,null,"Coincident",7.6483752297436203,7.6527529637566412,7.6571332034724442,7.6615159503252288,7.665901205750016,7.6702889711826483,7.6746792480597898]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.0422973863158056,8.0469005912780815,8.051506430996934,8.0561149069804294,8.0607260207374978,8.065339773777934,8.0699561676123963]
[null,null,null,null,"Coincident",8.0422973863158056,8.0469005912780815,8.051506430996934,8.0561149069804294,8.0607260207374978,8.065339773777934,8.0699561676123963]
[null,"Dorrien TF5 11kV","Substation Rating","MVA","Non-Coincident",13.6,13.6,13.6,13.6,13.6,13.6,13.6]
[null,null,null,null,"Coincident",13.6,13.6,13.6,13.6,13.6,13.6,13.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.72373,1.8489456185803723,1.8814910653497747,1.9342779764966955,1.9843726806263084,2.0330166964219978,2.0815800061991974]
[null,null,null,null,"Coincident",1.72373,1.8489456185803723,1.8814910653497747,1.9342779764966955,1.9843726806263084,2.0330166964219978,2.0815800061991974]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.6188577313036987,3.6057597399707304,3.609729146825325,3.6361909099550074,3.6628547500873885,3.683335329430943,3.7039469139506811]
[null,null,null,null,"Coincident",3.2264661408751301,3.2147883605678964,3.2183273659023488,3.2419198884895852,3.2656925769345224,3.2839524535872804,3.3023291305667213]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8393357679518396,3.8254397846480495,3.8296510266602928,3.8577249663424311,3.886013294520041,3.9077416482328458,3.9296089885806755]
[null,null,null,null,"Coincident",3.4230378142787106,3.4106485680157208,3.4144031863987543,3.439433077748685,3.4646541115178522,3.4840264667626846,3.5035227383660024]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3533099337991104,3.3603420658972287,3.3673889448821015,3.3744506016790106,3.3815270672780904,3.3886183727344643,3.3957245491683805]
[null,null,null,null,"Coincident",2.9897116064204519,2.9959812466764029,3.0022640348188769,3.0085599984199383,3.014869165109471,3.021191562575301,3.0275272185633177]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.5576095347702683,3.5650700978246612,3.5725463062163358,3.58003819275469,3.5875457903179244,3.5950691318531884,3.6026082503767238]
[null,null,null,null,"Coincident",3.1718590667712281,3.1785106833514112,3.1851762488499409,3.1918557925187021,3.1985493436709236,3.2052569316813049,3.2119785859861478]
[null,"Dowlingville 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.4480000000000002E-2,2.6258282180415447E-2,2.6720484808968045E-2,2.7470151859420623E-2,2.8181584831575731E-2,2.8872415475979712E-2,2.9562099952867533E-2]
[null,null,null,null,"Coincident",2.4480000000000002E-2,2.6258282180415447E-2,2.6720484808968045E-2,2.7470151859420623E-2,2.8181584831575731E-2,2.8872415475979712E-2,2.9562099952867533E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.6462310145566015E-2,3.6316536981134677E-2,3.6171346605215184E-2,3.6026736687869446E-2,3.5882704908474249E-2,3.573924895568404E-2,3.559636652739382E-2]
[null,null,null,null,"Coincident",3.6462310145566015E-2,3.6316536981134677E-2,3.6171346605215184E-2,3.6026736687869446E-2,3.5882704908474249E-2,3.573924895568404E-2,3.559636652739382E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8128087195625243E-2,3.7975654398525134E-2,3.7823831014572672E-2,3.7672614607386773E-2,3.7522002750326779E-2,3.7371993026453547E-2,3.722258302849063E-2]
[null,null,null,null,"Coincident",3.8128087195625243E-2,3.7975654398525134E-2,3.7823831014572672E-2,3.7672614607386773E-2,3.7522002750326779E-2,3.7371993026453547E-2,3.722258302849063E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2816079131009417E-2,3.2684883283021209E-2,3.2554211944693663E-2,3.2424063019082502E-2,3.2294434417626826E-2,3.2165324060115637E-2,3.2036729874654439E-2]
[null,null,null,null,"Coincident",3.2816079131009417E-2,3.2684883283021209E-2,3.2554211944693663E-2,3.2424063019082502E-2,3.2294434417626826E-2,3.2165324060115637E-2,3.2036729874654439E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4315278476062722E-2,3.4178088958672616E-2,3.4041447913115398E-2,3.3905353146648096E-2,3.3769802475294104E-2,3.363479372380819E-2,3.3500324725641566E-2]
[null,null,null,null,"Coincident",3.4315278476062722E-2,3.4178088958672616E-2,3.4041447913115398E-2,3.3905353146648096E-2,3.3769802475294104E-2,3.363479372380819E-2,3.3500324725641566E-2]
[null,"East Terrace 11kV","Substation Rating","MVA","Non-Coincident",62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471]
[null,null,null,null,"Coincident",62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471,62.239362782732471]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4794899999999997,1.5869634764339395,1.6148974701805605,1.6602048600692076,1.7032015090877437,1.7449530217547882,1.786635263858986]
[null,null,null,null,"Coincident",1.4794899999999997,1.5869634764339395,1.6148974701805605,1.6602048600692076,1.7032015090877437,1.7449530217547882,1.786635263858986]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.661137277703759,42.277624867806715,43.070768618591032,43.29829348207614,43.518159347328812,43.745564242222706,43.992579139932872]
[null,null,null,null,"Coincident",39.142854000923329,39.722076876475882,40.467277609517566,40.681049318475303,40.887624991290117,41.101283983376511,41.333367615963674]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.091284378312153,44.743732473277554,45.583141307357273,45.823937985378528,46.056628906063672,46.297298617573276,46.558722208293332]
[null,null,null,null,"Coincident",41.426106436540096,42.039116118781273,42.827785357944165,43.054026642450282,43.272652136877042,43.498774129593421,43.744395495513949]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.825972675874972,39.326051321908871,39.832570982423121,40.345614617703802,40.865266256565725,41.391611010115099,41.924735085689434]
[null,null,null,null,"Coincident",36.479066084183899,36.948916566185986,37.424818723823847,37.90685050269807,38.395090852348794,38.889619739186486,39.39051815958922]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.090741020955029,41.619989890154827,42.156055486397975,42.699025609149508,43.248989188731841,43.806036300890206,44.370258181545701]
[null,null,null,null,"Coincident",38.606936384182283,39.104193842113659,39.607855977614051,40.118005282950023,40.634725312888754,41.158100698383095,41.688217160432821]
[null,"East Terrace 33kV","Substation Rating","MVA","Non-Coincident",23.8,23.8,23.8,23.8,23.8,23.8,23.8]
[null,null,null,null,"Coincident",23.8,23.8,23.8,23.8,23.8,23.8,23.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.147579094741987,8.2918099655318187,8.466968577815015,8.5383342459543776,8.6079659451534845,8.6789988474654969,8.7539991665630712]
[null,null,null,null,"Coincident",7.0926306479525296,6.4291048898755632,6.5649151768231473,6.620248978238191,6.6742383363725715,6.7293141257954563,6.7874660757625724]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.4234955472400106,8.5419140386184722,8.7223559222923939,8.7958741776659561,8.8676061627686273,8.9407816151710602,9.0180441526946566]
[null,null,null,null,"Coincident",7.306564134287366,6.6230245920809026,6.7629312953807492,6.8199341182966231,6.8755519457795389,6.932288974343261,6.9921949490173061]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.5797480945664919,7.7236227786674796,7.8531410087073246,7.9848311433563621,8.1187296035078518,8.2548734208007826,8.3933002478615322]
[null,null,null,null,"Coincident",6.6523594556523502,5.9885575260769439,6.0889802672563231,6.191087007779795,6.2949059868067145,6.4004659170418217,6.5077959926761766]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8385371832490023,7.9565887443564556,8.0900136047950415,8.2256758805324512,8.3636130910174771,8.50386338486644,8.6464655504137529]
[null,null,null,null,"Coincident",6.8530131371056555,6.1691890932994946,6.2726408639312972,6.3778274280156895,6.4847778764836921,6.5935217880951562,6.7040892376192209]
[null,"Edinburgh 11kV","Substation Rating","MVA","Non-Coincident",57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023]
[null,null,null,null,"Coincident",57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023,57.057998289136023]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.1492199999999997,2.3053441678019801,2.3459232173664333,2.4117401870630708,2.4742003983545415,2.5348518296276592,2.5954026331986086]
[null,null,null,null,"Coincident",2.1492199999999997,2.3053441678019801,2.3459232173664333,2.4117401870630708,2.4742003983545415,2.5348518296276592,2.5954026331986086]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.818875283185102,14.76073997099869,14.727596461744723,14.741859957320264,14.761211597788273,14.783723070050875,14.817475428084151]
[null,null,null,null,"Coincident",13.190197512705511,13.138451598420662,13.108950747312207,13.121646604471925,13.138871390772511,13.158908725575001,13.188951509556293]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.543211534556017,15.482234609001742,15.447471068214238,15.462431753469778,15.482729288578684,15.506341105848579,15.541743255517559]
[null,null,null,null,"Coincident",13.834925134648325,13.780649916292782,13.749707084231265,13.763023506002487,13.781090227800956,13.802106973503459,13.833618227737313]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.988483003654569,14.083976707924368,14.180122309011912,14.276924257152578,14.374387032961696,14.472515147641941,14.571313143192139]
[null,null,null,null,"Coincident",12.451070016811013,12.536068425696184,12.621647084271002,12.707809953664935,12.794561022048478,12.881904304817754,12.969843844780359]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.672230261635073,14.772391631328766,14.87323676210036,14.97477032170962,15.076997009781223,15.179921558022269,15.283548730441307]
[null,null,null,null,"Coincident",13.059669604106764,13.14882267572361,13.238584359228787,13.328958809368997,13.419950209253722,13.511562770548831,13.603800733671532]
[null,"Edithburgh 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.94721,1.016017461769253,1.0339015692770679,1.0629086006030151,1.0904362323658845,1.1171666937501123,1.143852806223679]
[null,null,null,null,"Coincident",0.94721,1.016017461769253,1.0339015692770679,1.0629086006030151,1.0904362323658845,1.1171666937501123,1.143852806223679]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1353274738472163,1.0573407166385134,1.0015225584406944,0.9796035361576596,0.95930325062851451,0.93982012608965204,0.92084120726017449]
[null,null,null,null,"Coincident",1.1353274738472163,1.0573407166385134,1.0015225584406944,0.9796035361576596,0.95930325062851451,0.93982012608965204,0.92084120726017449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2207822299432434,1.1369255017618423,1.076905976817951,1.0533371356533974,1.0315088716435639,1.0105592753652173,0.99015183576362842]
[null,null,null,null,"Coincident",1.2207822299432434,1.1369255017618423,1.076905976817951,1.0533371356533974,1.0315088716435639,1.0105592753652173,0.99015183576362842]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0297176790192424,0.96774917536605243,0.90950994190337997,0.85477555081170387,0.80333508035811008,0.75499030209877038,0.70955491699564988]
[null,null,null,null,"Coincident",1.0297176790192424,0.96774917536605243,0.90950994190337997,0.85477555081170387,0.80333508035811008,0.75499030209877038,0.70955491699564988]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1072233107733789,1.040590511146293,0.97796767946600005,0.91911349549645571,0.86380116167538701,0.81181752913846283,0.76296227633940839]
[null,null,null,null,"Coincident",1.1072233107733789,1.040590511146293,0.97796767946599994,0.91911349549645571,0.86380116167538712,0.81181752913846272,0.76296227633940839]
[null,"Elizabeth Downs 11kV","Substation Rating","MVA","Non-Coincident",59.6,59.6,59.6,59.6,59.6,59.6,59.6]
[null,null,null,null,"Coincident",59.6,59.6,59.6,59.6,59.6,59.6,59.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",14.126149999999997,15.152305262372369,15.419018647230551,15.851612977489975,16.262144385970728,16.660787249837039,17.05876871933005]
[null,null,null,null,"Coincident",14.126149999999997,15.152305262372369,15.419018647230551,15.851612977489975,16.262144385970728,16.660787249837039,17.05876871933005]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.591888044489664,44.961592409184085,45.408359901416347,45.830027836148361,46.267972009855875,46.717800664670762,47.206920270218745]
[null,null,null,null,"Coincident",44.591888044489664,44.961592409184085,45.408359901416347,45.830027836148361,46.267972009855875,46.717800664670762,47.206920270218745]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.731958776063884,46.111115288761162,46.569305184575093,47.001753808170328,47.450894801667339,47.912224124116349,48.413848940162893]
[null,null,null,null,"Coincident",45.731958776063891,46.111115288761169,46.5693051845751,47.001753808170335,47.450894801667346,47.912224124116356,48.413848940162893]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.799345332845277,40.2733620773637,40.753024439220923,41.238399658647381,41.729555776715728,42.226561644878956,42.729486934622187]
[null,null,null,null,"Coincident",39.799345332845277,40.2733620773637,40.753024439220923,41.238399658647381,41.729555776715728,42.226561644878956,42.729486934622187]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.816886207197172,41.303022030776845,41.794947811918888,42.292732509969518,42.796445905592122,43.306158610549261,43.821942077601172]
[null,null,null,null,"Coincident",40.816886207197179,41.303022030776852,41.794947811918888,42.292732509969518,42.79644590559213,43.306158610549268,43.821942077601179]
[null,"Elizabeth Heights 11kV","Substation Rating","MVA","Non-Coincident",27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162]
[null,null,null,null,"Coincident",27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162,27.56536388140162]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.1970899999999993,7.7199027817747625,7.8557897881444365,8.0761909822678728,8.2853514042273417,8.4884547670759307,8.6912211580793848]
[null,null,null,null,"Coincident",7.1970899999999993,7.7199027817747625,7.8557897881444365,8.0761909822678728,8.2853514042273417,8.4884547670759307,8.6912211580793848]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.612077820794728,19.425495434188388,19.298013210177853,19.259051168167186,19.227678679429577,19.152791355318449,19.083256209101975]
[null,null,null,null,"Coincident",19.220902899634684,19.038042013169097,18.913102500307392,18.87491758012191,18.844170834914419,18.770777184414658,18.7026289593387]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.142973207131732,19.951340069191129,19.820406924519073,19.780390187104139,19.748168450791596,19.671253940411425,19.59983649040991]
[null,null,null,null,"Coincident",19.741209251867694,19.553398354401072,19.425076751607055,19.385858172564035,19.354279118545378,19.278898715250083,19.208905730092582]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.585018684575861,17.467646811621094,17.351058341675902,17.235248045887239,17.120210730302233,17.005941235635255,16.892434437036517]
[null,null,null,null,"Coincident",17.234274701179913,17.119243882221006,17.004980840818149,16.891480452410978,16.778737626643196,16.66674730713429,16.555504471252746]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.061041948076916,17.940492839828327,17.820748341166567,17.701803081694486,17.583651726859856,17.466288977716115,17.349709570684727]
[null,null,null,null,"Coincident",17.70080338872263,17.582658706376588,17.465302585185658,17.348729761868558,17.232935008273973,17.117913131146086,17.003658971891657]
[null,"Elizabeth South 11kV","Substation Rating","MVA","Non-Coincident",28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529]
[null,null,null,null,"Coincident",28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529,28.430147058823529]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.0979700000000001,2.2503712526979656,2.2899826599130186,2.3542301673410413,2.4152009611560845,2.4744061068685119,2.5335130244329047]
[null,null,null,null,"Coincident",2.0979700000000001,2.2503712526979656,2.2899826599130186,2.3542301673410413,2.4152009611560845,2.4744061068685119,2.5335130244329047]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.55543828267624,10.492715042436354,10.433649611955143,10.423115132856624,10.41568384247182,10.410072387474482,10.404903015860352]
[null,null,null,null,"Coincident",10.005392983337265,9.9459382595274235,9.8899507365209729,9.8799652105359073,9.8729211656860301,9.8676021243584131,9.8627021293898327]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.844686642065733,10.780244610635076,10.719560623121389,10.708737470003404,10.701102541598615,10.695337317131143,10.690026290360835]
[null,null,null,null,"Coincident",10.279568572069303,10.21848462350731,10.160962886691616,10.150703729528813,10.143466658263383,10.138001860413267,10.132967591957625]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.6731081219782453,9.6862340310022255,9.6993777512080435,9.7125393067645565,9.7257187218734149,9.7389160207691106,9.7521312277190209]
[null,null,null,null,"Coincident",9.1690411652111212,9.1814830813619643,9.1939418805515807,9.2064175856893815,9.2189102197158714,9.2314198056026751,9.2439463663525956]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9381781815579977,9.951663776987127,9.9651676716740063,9.9786898904497789,9.9922304581792911,10.005789399761129,10.019366740127662]
[null,null,null,null,"Coincident",9.4202983885672342,9.4330812478165935,9.4458814527469332,9.4586990268954469,9.4715339938312724,9.4843863771555199,9.497256200501333]
[null,"Eudunda 11kV","Substation Rating","MVA","Non-Coincident",2.4,2.4,2.4,2.4,2.4,2.4,2.4]
[null,null,null,null,"Coincident",2.4,2.4,2.4,2.4,2.4,2.4,2.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.66723999999999994,0.71570981217566998,0.72830785473594106,0.74874118164541725,0.76813238002535089,0.78696203031832934,0.80576044005520142]
[null,null,null,null,"Coincident",0.66723999999999994,0.71570981217566998,0.72830785473594106,0.74874118164541725,0.76813238002535089,0.78696203031832934,0.80576044005520142]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.680885391121411,1.6059243671965995,1.5517199473095311,1.5230686486483156,1.4960987876362468,1.4707135103736506,1.4461581610727254]
[null,null,null,null,"Coincident",1.5436280284487967,1.474788155020923,1.4250099475087117,1.3986982501743661,1.3739306880303326,1.3506183160509766,1.3280681019617395]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7693530432856956,1.6904467023122098,1.6333894182205591,1.6032301564719111,1.574840829090786,1.5481194846038426,1.5222717484976056]
[null,null,null,null,"Coincident",1.62487160889347,1.5524085842325503,1.5000104710618016,1.4723139475519642,1.4462428295056131,1.4217034905799752,1.3979664231176205]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5562412640886583,1.5038441765224606,1.4532112465125322,1.4042830766376058,1.3570022693282078,1.3113133595336477,1.2671627496560427]
[null,null,null,null,"Coincident",1.4291620636152718,1.381043605686199,1.3345452481309179,1.2896124437894796,1.2461924820502785,1.2042344270153071,1.1636890577473218]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6381486990406928,1.5829938700236426,1.5296960489605602,1.4781927122501115,1.4284234413981134,1.3803298521406817,1.333855525953729]
[null,null,null,null,"Coincident",1.5043811195950227,1.4537301112486305,1.4047844717167557,1.3574867829362942,1.3117815600529248,1.2676151863319021,1.2249358502603387]
[null,"Evanston 11kV","Substation Rating","MVA","Non-Coincident",57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173]
[null,null,null,null,"Coincident",57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173,57.660208695652173]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",16.017109999999999,17.180628843739953,17.483045115954663,17.973547551023067,18.439033669186276,18.891039813908069,19.342296028434404]
[null,null,null,null,"Coincident",16.017109999999999,17.180628843739953,17.483045115954663,17.973547551023067,18.439033669186276,18.891039813908069,19.342296028434404]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.451999457199534,39.834704159617907,40.364856295797019,40.737558612602257,41.119823816781654,41.507347579444506,41.923950833746972]
[null,null,null,null,"Coincident",39.451999457199534,39.834704159617907,40.364856295797019,40.737558612602257,41.119823816781654,41.507347579444506,41.923950833746972]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.124756979487735,40.513987776170261,41.053180362579496,41.4322382073847,41.821022011258897,42.21515404549185,42.638861451092041]
[null,null,null,null,"Coincident",40.124756979487735,40.513987776170261,41.053180362579496,41.4322382073847,41.821022011258897,42.21515404549185,42.638861451092041]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.169738363394309,35.4147677644076,35.661504298034181,35.909959857955975,36.160146420718824,36.412076046309778,36.665760878738446]
[null,null,null,null,"Coincident",35.169738363394309,35.4147677644076,35.661504298034181,35.909959857955975,36.160146420718824,36.412076046309778,36.665760878738446]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.769472378562547,36.018680157731104,36.269624180491427,36.522316543343145,36.77676942706286,37.032995097291227,37.291005905124301]
[null,null,null,null,"Coincident",35.769472378562547,36.018680157731104,36.269624180491427,36.522316543343145,36.776769427062852,37.032995097291227,37.291005905124308]
[null,"Findon 11kV","Substation Rating","MVA","Non-Coincident",24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126]
[null,null,null,null,"Coincident",24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126,24.821457654723126]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.9347200000000004,4.2205468979135734,4.2948376628898188,4.4153331668423013,4.5296832299222913,4.6407218391195642,4.751576222489664]
[null,null,null,null,"Coincident",3.9347200000000004,4.2205468979135734,4.2948376628898188,4.4153331668423013,4.5296832299222913,4.6407218391195642,4.751576222489664]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.280621081925034,18.497029030513843,18.573305892226781,18.743494876703789,18.916821306957857,19.090728803304124,19.271321880081224]
[null,null,null,null,"Coincident",18.025693471347441,18.239083559602268,18.314296722329722,18.48211238092437,18.653021732868208,18.824504047799337,19.002578711151461]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.905341550466439,19.12914500681358,19.208028547838705,19.384033556927054,19.56328323061107,19.743133827692997,19.929898477691484]
[null,null,null,null,"Coincident",18.641702064312494,18.862384528210313,18.940168019486727,19.113718596845679,19.290468591180492,19.467811128893452,19.651971301409962]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.381207071083125,16.610443117160592,16.84288705656321,17.07858378004774,17.317578806565162,17.559918292051531,17.805649038341837]
[null,null,null,null,"Coincident",16.152767240822815,16.378806535694572,16.608008989055794,16.840418865650953,17.076081049658431,17.315041053358772,17.557345025924239]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.941017118611509,17.17808705881491,17.418474518630891,17.662225922909311,17.909388346162096,18.160009521654548,18.414137850623778]
[null,null,null,null,"Coincident",16.704770604040299,16.938534547520451,17.175569747012833,17.415921979961723,17.65963766441379,17.906763867982576,18.157348316938432]
[null,"Flinders Park 11kV","Substation Rating","MVA","Non-Coincident",27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743]
[null,null,null,null,"Coincident",27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743,27.260915492957743]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.15625,5.5308115805868932,5.628165841349734,5.7860690573994118,5.9359189864302442,6.0814294239387419,6.2266984428910632]
[null,null,null,null,"Coincident",5.15625,5.5308115805868932,5.628165841349734,5.7860690573994118,5.9359189864302442,6.0814294239387419,6.2266984428910632]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.028046513990702,21.414868785027437,21.628692311084958,21.959411562338683,22.293725456146383,22.628810965423245,22.972128554604463]
[null,null,null,null,"Coincident",20.95022394773919,21.335614630644553,21.548646818547496,21.878142112986012,22.211218746588283,22.545064139992839,22.887111147248554]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.816822142798458,22.218154367475957,22.439998552328753,22.783123296655408,23.129977520903783,23.477632304416762,23.833827958477045]
[null,null,null,null,"Coincident",21.736080401739642,22.135927338488798,22.356950501580883,22.698805377680348,23.044375931292546,23.390744081384561,23.745621493169313]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.256789210946568,19.64943844544085,20.050093865164666,20.458918717607883,20.876079578904687,21.3017464217052,21.736092684431036]
[null,null,null,null,"Coincident",19.185521879805595,19.576717961195776,19.975890597774484,20.383202432869972,20.798819426135847,21.222910921171515,21.65564971452141]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.979123832404479,20.386501593708562,20.80218585742973,21.226345994576818,21.659154829662551,22.100788711121133,22.551427583161576]
[null,null,null,null,"Coincident",19.905183217566098,20.31105331705303,20.725199177474035,21.147789543013829,21.578996598579995,22.018996039959902,22.467967145408164]
[null,"Forreston 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.48548000000000002,0.52074635755506904,0.52991262112164239,0.54477979267612431,0.55888871748502389,0.57258906312412705,0.58626667831364909]
[null,null,null,null,"Coincident",0.48548000000000002,0.52074635755506904,0.52991262112164239,0.54477979267612431,0.55888871748502389,0.57258906312412705,0.58626667831364909]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0017595330735569,1.0047614349509961,1.0067450490846872,1.0072503781134863,1.0081201553663011,1.0090743551156278,1.0112698297116534]
[null,null,null,null,"Coincident",0.91395590866073506,0.91669469563258199,0.91850444717288182,0.91896548441429615,0.91975902621068883,0.92062959092222607,0.92263263348194657]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.03274178667377,1.0358365308773156,1.0378814939017393,1.0384024516633878,1.0392991292436093,1.0402828403253894,1.0425462161975807]
[null,null,null,null,"Coincident",0.94222258624818045,0.94504607797173401,0.94691180120915652,0.94738709733432591,0.94820518166050394,0.94910267105384138,0.95116766338345016]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.88902032743012549,0.88234289213939376,0.87571561109225593,0.86913810757998466,0.86261000772331342,0.85613094045118432,0.84970053747965557]
[null,null,null,null,"Coincident",0.81109822701792311,0.80500606493992488,0.79895966111604211,0.79295867185584246,0.78700275605035352,0.78109157515267402,0.7752247931587295]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.91651580147435618,0.90963184756638538,0.90279959906418128,0.89601866760823157,0.88928866775599325,0.88260921695998373,0.87597993554603659]
[null,null,null,null,"Coincident",0.83618373919373523,0.82990315973188133,0.82366975372787854,0.81748316686169331,0.81134304747459129,0.80524904654914853,0.79920081768941187]
[null,"Freeling 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.30773,0.33008419834065544,0.33589439502711343,0.3453182120792283,0.35426140115281046,0.36294560516434793,0.37161540108234992]
[null,null,null,null,"Coincident",0.30773,0.33008419834065544,0.33589439502711343,0.3453182120792283,0.35426140115281046,0.36294560516434793,0.37161540108234992]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.37215050446171261,0.37138534767115317,0.37062176407452235,0.36985975043726849,0.36909930353149034,0.36834042013592333,0.36758309703592601]
[null,null,null,null,"Coincident",0.37215050446171261,0.37138534767115317,0.37062176407452235,0.36985975043726849,0.36909930353149034,0.36834042013592333,0.36758309703592601]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.38539005204146903,0.38459767419487684,0.38380692550982742,0.38301780263669755,0.38223030223275067,0.38144442096212333,0.38066015549581067]
[null,null,null,null,"Coincident",0.38539005204146903,0.38459767419487684,0.38380692550982742,0.38301780263669755,0.38223030223275067,0.38144442096212333,0.38066015549581067]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.33493545401554137,0.33424681290403785,0.33355958766707011,0.33287377539354163,0.3321893731783413,0.33150637812233102,0.33082478733233339]
[null,null,null,null,"Coincident",0.33493545401554137,0.33424681290403785,0.33355958766707011,0.33287377539354163,0.3321893731783413,0.33150637812233102,0.33082478733233339]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.34685104683732215,0.34613790677538914,0.34542623295884467,0.34471602237302779,0.34400727200947562,0.34329997886591107,0.34259413994622956]
[null,null,null,null,"Coincident",0.34685104683732215,0.34613790677538914,0.34542623295884467,0.34471602237302779,0.34400727200947562,0.34329997886591107,0.34259413994622956]
[null,"Freeling North 11kV","Substation Rating","MVA","Non-Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,null,null,"Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3770200000000001,1.4770498254932876,1.5030491009658977,1.5452184850269357,1.585237170946749,1.6240969590985943,1.662892274391244]
[null,null,null,null,"Coincident",1.3770200000000001,1.4770498254932876,1.5030491009658977,1.5452184850269357,1.585237170946749,1.6240969590985943,1.662892274391244]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5369202575572936,3.5249442540859159,3.5024268765414499,3.4893674134711374,3.4553585010588086,3.4223787380023052,3.390774894596821]
[null,null,null,null,"Coincident",3.5134969445933377,3.5016002524032275,3.4792319965643541,3.4662590200044412,3.4324753321776242,3.399713978147985,3.3683194317186964]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8031400618895632,3.7902626388020604,3.7660504048832797,3.7520079714743417,3.7154392484503322,3.6799771376368877,3.6459945103191624]
[null,null,null,null,"Coincident",3.7779537038638042,3.7651615617239007,3.7411096737251124,3.7271602365639156,3.6908336905135748,3.6556064281161134,3.6218488513104266]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2667774358042063,3.2160452749855155,3.1661009707600303,3.1169322879301671,3.0685271813076174,3.0208737927625546,2.9739604483186683]
[null,null,null,null,"Coincident",3.2451431481498738,3.1947469619061413,3.1451334146622818,3.0962903522485101,3.0482058092459776,3.000868006055518,2.9542653460119221]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.5126639094668888,3.4581131989091567,3.4044096459785274,3.3515400945485672,3.2994915928038897,3.2482513900672632,3.1978069336759876]
[null,null,null,null,"Coincident",3.4894012345697569,3.4352117869958509,3.3818638867336364,3.3293444647833446,3.2776406551032018,3.2267397914575464,3.176629404313895]
[null,"Fulham Gardens 11kV","Substation Rating","MVA","Non-Coincident",48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233]
[null,null,null,null,"Coincident",48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233,48.998612471433233]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.726810000000002,13.651314061949885,13.891606751291775,14.281348177532395,14.651212240618726,15.010365441333883,15.368922765570023]
[null,null,null,null,"Coincident",12.726810000000002,13.651314061949885,13.891606751291775,14.281348177532395,14.651212240618726,15.010365441333883,15.368922765570023]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.93297197337337,42.231396438631656,42.203822860664992,42.470436664490784,42.744942981890105,43.0210294595053,43.31190961002283]
[null,null,null,null,"Coincident",41.891106413954013,42.189232934502094,42.161686885785386,42.428034504422747,42.702266756808285,42.978077591789777,43.268667329783412]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.627750345417688,43.938236043295731,43.909548041490766,44.186937406578934,44.472538271963387,44.759783161898447,45.06241963124468]
[null,null,null,null,"Coincident",43.584192732196783,43.894368443521955,43.865709083599214,44.142821505260763,44.42813722891934,44.715095335746931,45.01742965515021]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.664138973340677,39.113439103867123,39.567960367274104,40.027763436209369,40.492909688372677,40.963461214708907,41.439480827696393]
[null,null,null,null,"Coincident",38.625536991859022,39.074388544561707,39.528456017405681,39.987800022463574,40.452481876156128,40.922563607437091,41.398107966073304]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.226802992178698,40.694262201538294,41.167153562999509,41.645540201378076,42.129485975037362,42.619055484412662,43.114314080634443]
[null,null,null,null,"Coincident",40.186640858858169,40.653633360508188,41.126052590840601,41.60396161164779,42.087424217537439,42.576504944448232,43.071269078264613]
[null,"Fullerville 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9201089034700093E-2,2.910231708679966E-2,2.9003879232524316E-2,2.8905774341810787E-2,2.8808001288418216E-2,2.8710558949915227E-2,2.8613446207667037E-2]
[null,null,null,null,"Coincident",2.9201089034700093E-2,2.910231708679966E-2,2.9003879232524316E-2,2.8905774341810787E-2,2.8808001288418216E-2,2.8710558949915227E-2,2.8613446207667037E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.922160009668287E-2,2.9122758770632085E-2,2.9024251772876229E-2,2.8926077972558275E-2,2.8828236242646275E-2,2.8730725459920458E-2,2.8633544504960296E-2]
[null,null,null,null,"Coincident",2.922160009668287E-2,2.9122758770632085E-2,2.9024251772876229E-2,2.8926077972558275E-2,2.8828236242646275E-2,2.8730725459920458E-2,2.8633544504960296E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6280980131230085E-2,2.6192085378119696E-2,2.6103491309271885E-2,2.6015196907629708E-2,2.5927201159576394E-2,2.5839503054923704E-2,2.5752101586900333E-2]
[null,null,null,null,"Coincident",2.6280980131230085E-2,2.6192085378119696E-2,2.6103491309271885E-2,2.6015196907629708E-2,2.5927201159576394E-2,2.5839503054923704E-2,2.5752101586900333E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6299440087014583E-2,2.6210482893568875E-2,2.6121826595588607E-2,2.6033470175302446E-2,2.5945412618381649E-2,2.585765291392841E-2,2.5770190054464265E-2]
[null,null,null,null,"Coincident",2.6299440087014583E-2,2.6210482893568875E-2,2.6121826595588607E-2,2.6033470175302446E-2,2.5945412618381649E-2,2.585765291392841E-2,2.5770190054464265E-2]
[null,"Gawler Belt TF1 11kV","Substation Rating","MVA","Non-Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,null,null,"Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.3856299999999999,2.5589275211627656,2.6039701868798382,2.6770268946237592,2.7463576070977131,2.8136805772860085,2.8808918509215431]
[null,null,null,null,"Coincident",2.3856299999999999,2.5589275211627656,2.6039701868798382,2.6770268946237592,2.7463576070977131,2.8136805772860085,2.8808918509215431]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.817096298988246,4.8139191985366434,4.8363059400874935,4.8313940413844563,4.798436234502967,4.7674845406933199,4.7386955643893973]
[null,null,null,null,"Coincident",3.9079502387604359,3.9053727626840256,3.9235343825808684,3.9195495223003434,3.8928119481940113,3.8677018669945022,3.844346326677774]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.2233258008370225,5.2198807730172145,5.2441554060080033,5.2388292830421701,5.2030921185060892,5.1695302441276398,5.1383134709152074]
[null,null,null,null,"Coincident",4.2375107416457309,4.2347159049940775,4.2544091085142357,4.250088201846796,4.2210958271851702,4.1938681931812463,4.1685430618662513]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4100448775412104,4.3486097739855154,4.2880305056999148,4.2282951502822774,4.1693919514181275,4.1113093165669223,4.0540358146805637]
[null,null,null,null,"Coincident",3.577722939803214,3.5278826807120316,3.4787367323509062,3.4302754224709631,3.3824892135647273,3.3353687009890751,3.2889046111143405]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.781947414368342,4.715331440436711,4.6496434750334732,4.5848705903309916,4.521000038595588,4.458019249678701,4.3959158285429982]
[null,null,null,null,"Coincident",3.87943511605646,3.8253917888997964,3.7721013242405808,3.7195532341616198,3.667737176849966,3.6166429545615797,3.5662605116143449]
[null,"Gawler Belt TF2 11kV","Substation Rating","MVA","Non-Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,null,null,"Coincident",14.6,14.6,14.6,14.6,14.6,14.6,14.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.4612699999999998,2.6400621806450619,2.6865329920657177,2.7619060729998441,2.8334350203599832,2.9028925669348276,2.9722348754491121]
[null,null,null,null,"Coincident",2.4612699999999998,2.6400621806450619,2.6865329920657177,2.7619060729998441,2.8334350203599832,2.9028925669348276,2.9722348754491121]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9941577691364198,5.0409369071101109,5.0915568364836687,5.1173130423445494,5.1126655263940091,5.1096003105167549,5.1086970450761875]
[null,null,null,null,"Coincident",4.7740119979954718,4.8187290806880565,4.8671176501602691,4.8917385054649563,4.8872958550853722,4.884365755947357,4.8835023070436616]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1699886729628615,5.2184147789520541,5.2708169003076888,5.2974799131148069,5.2926687705893958,5.2894956366801056,5.2885605696853721]
[null,null,null,null,"Coincident",4.9420921595140728,4.9883836107848607,5.0384758120401436,5.0639635016422879,5.0593644374552644,5.0563311773833028,5.0554373287589414]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4483395884418924,4.4240764193162345,4.3999455920148272,4.3759463846880902,4.3520780794237233,4.3283399622252308,4.3047313229905626]
[null,null,null,null,"Coincident",4.252253843004242,4.2290602103899255,4.2059930858848871,4.1830517794591522,4.160235604846469,4.1375438795237782,4.1149759246907971]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.6049536976709504,4.5798362874191065,4.5548558783922859,4.5300117233265214,4.5053030790337463,4.4807292063795598,4.4562893702611248]
[null,null,null,null,"Coincident",4.4019642989164476,4.3779540806886779,4.354074824581498,4.3303258162708271,4.3067063453288208,4.2832157052026112,4.2598531931931785]
[null,"Georgetown 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.4840000000000004E-2,8.0276545685551148E-2,8.1689586728070612E-2,8.3981460995058807E-2,8.6156446437709477E-2,8.8268446659408584E-2,9.0376942829763343E-2]
[null,null,null,null,"Coincident",7.4840000000000004E-2,8.0276545685551148E-2,8.1689586728070612E-2,8.3981460995058807E-2,8.6156446437709477E-2,8.8268446659408584E-2,9.0376942829763343E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.20065455607104715,0.20000892359360162,0.19654215539780803,0.19446182313615926,0.19249742918160487,0.19028721706982674,0.18717725802086557]
[null,null,null,null,"Coincident",0.20065455607104715,0.20000892359360162,0.19654215539780803,0.19446182313615926,0.19249742918160487,0.19028721706982674,0.18717725802086557]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.20070631321779675,0.20006051420491075,0.19659285178556316,0.19451198291979105,0.19254708226641967,0.19033630004910865,0.18722553881249707]
[null,null,null,null,"Coincident",0.20070631321779675,0.20006051420491075,0.19659285178556316,0.19451198291979105,0.19254708226641967,0.19033630004910865,0.18722553881249707]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.1737992679780096,0.16781214194273328,0.16203126348593824,0.15644952768560033,0.15106007437368157,0.14585627970471968,0.1408317480148672]
[null,null,null,null,"Coincident",0.1737992679780096,0.16781214194273328,0.16203126348593824,0.15644952768560033,0.15106007437368157,0.14585627970471968,0.1408317480148672]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.17384409803018408,0.16785542766635186,0.16207305808082048,0.1564898825189113,0.1510990390430639,0.14589390209925107,0.14086807437391796]
[null,null,null,null,"Coincident",0.17384409803018408,0.16785542766635184,0.16207305808082048,0.15648988251891127,0.1510990390430639,0.14589390209925107,0.14086807437391796]
[null,"Geranium 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.8920000000000003E-2,4.1747236211673582E-2,4.2482077972427958E-2,4.3673950586954689E-2,4.4805036014907172E-2,4.5903366434850101E-2,4.6999874598268154E-2]
[null,null,null,null,"Coincident",3.8920000000000003E-2,4.1747236211673582E-2,4.2482077972427958E-2,4.3673950586954689E-2,4.4805036014907172E-2,4.5903366434850101E-2,4.6999874598268154E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.14453111695124832,0.14433811593433538,0.14414537264318636,0.1439528867336447,0.14376065786201342,0.14356868568505443,0.14337696985998807]
[null,null,null,null,"Coincident",0.14453111695124832,0.14433811593433538,0.14414537264318636,0.1439528867336447,0.14376065786201342,0.14356868568505443,0.14337696985998807]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.14649980422157641,0.14630417429918505,0.14610880561309181,0.14591369781445232,0.14571885055488801,0.14552426348648553,0.14532993626179611]
[null,null,null,null,"Coincident",0.14649980422157641,0.14630417429918505,0.14610880561309181,0.14591369781445232,0.14571885055488801,0.14552426348648553,0.14532993626179611]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.13007800525612348,0.12990430434090183,0.12973083537886773,0.12955759806028025,0.12938459207581207,0.129211817116549,0.12903927287398928]
[null,null,null,null,"Coincident",0.13007800525612348,0.12990430434090183,0.12973083537886773,0.12955759806028025,0.12938459207581207,0.129211817116549,0.12903927287398928]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.13184982379941876,0.13167375686926652,0.13149792505178262,0.13132232803300711,0.13114696549939922,0.13097183713783697,0.1307969426356165]
[null,null,null,null,"Coincident",0.13184982379941876,0.13167375686926652,0.13149792505178262,0.13132232803300711,0.13114696549939922,0.13097183713783697,0.1307969426356165]
[null,"Gladstone 11kV","Substation Rating","MVA","Non-Coincident",4.8,4.8,4.8,4.8,4.8,4.8,4.8]
[null,null,null,null,"Coincident",4.8,4.8,4.8,4.8,4.8,4.8,4.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2912399999999999,1.3850385736372401,1.4094182518272833,1.448960738846335,1.4864865031831636,1.5229255620589885,1.5593041643439816]
[null,null,null,null,"Coincident",1.2912399999999999,1.3850385736372401,1.4094182518272833,1.448960738846335,1.4864865031831636,1.5229255620589885,1.5593041643439816]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4742835542898289,2.4791690719709174,2.4840642361951319,2.4889690660097461,2.4938835804996438,2.4988077987873916,2.5037417400333135]
[null,null,null,null,"Coincident",2.4742835542898289,2.4791690719709174,2.4840642361951319,2.4889690660097461,2.4938835804996438,2.4988077987873916,2.5037417400333135]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5604442567593053,2.5654999003075765,2.5705655263155793,2.57564115449386,2.5807268045918863,2.5858224963981198,2.5909282497400947]
[null,null,null,null,"Coincident",2.5604442567593053,2.5654999003075765,2.5705655263155793,2.57564115449386,2.5807268045918863,2.5858224963981198,2.5909282497400947]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.226855198860846,2.2312521647738257,2.235657812575619,2.2400721594087716,2.2444952224496793,2.2489270189086525,2.2533675660299823]
[null,null,null,null,"Coincident",2.226855198860846,2.2312521647738257,2.235657812575619,2.2400721594087716,2.2444952224496793,2.2489270189086525,2.2533675660299823]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3043998310833747,2.308949910276819,2.3135089736840215,2.318077039044474,2.3226541241326975,2.3272402467583082,2.3318354247660853]
[null,null,null,null,"Coincident",2.3043998310833747,2.308949910276819,2.3135089736840215,2.318077039044474,2.3226541241326975,2.3272402467583082,2.3318354247660853]
[null,"Glanville 7.6kV","Substation Rating","MVA","Non-Coincident",20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926]
[null,null,null,null,"Coincident",20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926,20.35970501474926]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4816700000000003,4.8072285743260821,4.8918462072633906,5.0290913187830721,5.1593367357895419,5.2858103866925648,5.4120742032584896]
[null,null,null,null,"Coincident",4.4816700000000003,4.8072285743260821,4.8918462072633906,5.0290913187830721,5.1593367357895419,5.2858103866925648,5.4120742032584896]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.4387047610950248,8.2615075443362986,7.9850491013081726,7.9200311829069285,7.8575694907344227,7.7958940279598679,7.7368242645320242]
[null,null,null,null,"Coincident",8.2814782599350067,8.1075825093603697,7.8362749271508205,7.7724683960551335,7.7111704646249271,7.6506441138875863,7.5926749141707672]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.595654257449155,8.4151613910957366,8.1335611621390225,8.0673339906786925,8.0037105881009243,7.9408880378178104,7.8807196496741811]
[null,null,null,null,"Coincident",8.435503537363461,8.2583735403916005,7.9820199719092333,7.9170267180636591,7.8545887207420764,7.7929366545622214,7.7338892992566972]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5299816769286991,7.4058927959708036,7.283848813797265,7.1638160318929067,7.0457613070707339,6.9296520423205106,6.8154561778081444]
[null,null,null,null,"Coincident",7.3896861331954078,7.2679092255957718,7.1481391170613788,7.0303427369340241,6.914487559537041,6.8005415951943755,6.6884733813976736]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.6700300451567669,7.5436332641216852,7.4193194144652246,7.2970541709214052,7.1768037738808506,7.0585350200691535,6.9422152533788646]
[null,null,null,null,"Coincident",7.5271251774154626,7.4030833695904459,7.281085684817171,7.1610984373639957,7.0430884966168001,6.927023277931025,6.8128707336344823]
[null,"Glencoe 11kV","Substation Rating","MVA","Non-Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,null,null,"Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.48422999999999999,0.51940555474765404,0.52854821728131518,0.54337710926826988,0.55744970682164685,0.57111477720317216,0.58475717566082697]
[null,null,null,null,"Coincident",0.48422999999999999,0.51940555474765404,0.52854821728131518,0.54337710926826988,0.55744970682164685,0.57111477720317216,0.58475717566082697]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0611208132240533,1.0610528829849235,1.0518853957729093,1.0514431094932053,1.0511454032980374,1.0508270842461067,1.0508960264553222]
[null,null,null,null,"Coincident",0.88981440887515173,0.8897574452336674,0.8820699490383529,0.88169906506395168,0.88144942029328044,0.88118249038718732,0.88124030262720288]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1794479389226638,1.1793724336837377,1.1691826666350094,1.168691060368777,1.1683601565226556,1.1680063412501243,1.1680829713053928]
[null,null,null,null,"Coincident",0.98903890819252904,0.98897559245250688,0.98043085237197747,0.98001861058599471,0.97974112756373977,0.97944443191546404,0.97950869088247439]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.95918799307020552,0.96125941145882199,0.96333530318756755,0.96541567791686222,0.96750054532798846,0.96958991512313575,0.97168379702544616]
[null,null,null,null,"Coincident",0.80433753293433286,0.80607454337275752,0.80781530497924259,0.80955982585463815,0.8113081141172892,0.81306017790307239,0.81481602536543407]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0661484416922338,1.0684508469590548,1.0707582243946703,1.073070584736749,1.0753879387461465,1.0777102972069577,1.0800376709265664]
[null,null,null,null,"Coincident",0.89403038145594138,0.89596108845551714,0.89789596492136114,0.89983501985766123,0.9017782622880508,0.90372570125564999,0.90567734582310777]
[null,"Glenelg North 11kV","Substation Rating","MVA","Non-Coincident",27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638]
[null,null,null,null,"Coincident",27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638,27.912511984659638]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4088500000000002,4.7291187659773142,4.81236149714129,4.9473765941751076,5.0755057305838518,5.1999243860814213,5.3241366167156885]
[null,null,null,null,"Coincident",4.4088500000000002,4.7291187659773142,4.81236149714129,4.9473765941751076,5.0755057305838518,5.1999243860814213,5.3241366167156885]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.937636644965252,21.055466281372613,20.986899342102376,21.020663622245312,21.057844011279702,21.095907408704946,21.11721852531263]
[null,null,null,null,"Coincident",20.937636644965252,21.055466281372613,20.986899342102376,21.020663622245312,21.057844011279702,21.095907408704946,21.11721852531263]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.900938186448123,22.024188944269916,21.952467368236523,21.987785079822572,22.026676069087401,22.066490692309308,22.08878229357374]
[null,null,null,null,"Coincident",21.900938186448123,22.024188944269916,21.952467368236523,21.987785079822572,22.026676069087401,22.066490692309308,22.08878229357374]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.648908279282733,18.758456311170445,18.868647853718979,18.979486687059882,19.090976613530064,19.203121457802254,19.315925067016199]
[null,null,null,null,"Coincident",18.648908279282733,18.758456311170445,18.868647853718979,18.979486687059882,19.090976613530064,19.203121457802254,19.315925067016199]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.506909704994051,19.62149783714586,19.736759086681641,19.852697407649725,19.969316777325442,20.086621196347576,20.204614688855571]
[null,null,null,null,"Coincident",19.506909704994051,19.62149783714586,19.736759086681641,19.852697407649725,19.969316777325446,20.086621196347576,20.204614688855571]
[null,"Glossop 11kV","Substation Rating","MVA","Non-Coincident",15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672]
[null,null,null,null,"Coincident",15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672,15.352603309692672]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.6105800000000001,2.80021839438517,2.8495083019851228,2.9294538007012378,3.0053219660790438,3.0789930716210434,3.152541948323405]
[null,null,null,null,"Coincident",2.6105800000000001,2.80021839438517,2.8495083019851228,2.9294538007012378,3.0053219660790438,3.0789930716210434,3.152541948323405]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.3547970108845373,10.035694202959929,10.082909206314257,10.040200484101202,10.002677923379013,9.9691191108646482,9.957007819184474]
[null,null,null,null,"Coincident",7.5993781900244164,8.1525056673054372,8.1908608198881527,8.1561663490479983,8.125684861394733,8.0984233283429692,8.0885847091040635]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.7999765160104815,10.513276492951979,10.562738381172258,10.51799722065004,10.478689022570467,10.443533200999639,10.430845552736811]
[null,null,null,null,"Coincident",7.9610201816105155,8.540470091791045,8.580650503417429,8.5443049793966157,8.5123729275490465,8.4838140626814411,8.4735072396280859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.9166954270532894,9.72132170442719,9.7263654486050086,9.7314118096446194,9.7364607889037362,9.7415123877407783,9.74656660751487]
[null,null,null,null,"Coincident",7.2434859544891488,7.8971248711092734,7.9012221614573575,7.9053215776155898,7.9094231206869123,7.9135267917748369,7.91763259198345]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3410263936104148,10.183943520861217,10.189227288583581,10.194513797699916,10.199803049632544,10.20509504580453,10.210389787639679]
[null,null,null,null,"Coincident",7.5881916160715699,8.272936140765653,8.2772284144669186,8.2815229151421637,8.2858196439468195,8.2901186020369089,8.2944197905690622]
[null,"Golden Grove 11kV","Substation Rating","MVA","Non-Coincident",84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394]
[null,null,null,null,"Coincident",84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394,84.63205352980394]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",19.400919999999999,20.810246401947126,21.176551803104751,21.770678864888509,22.334504607459731,22.88200256765704,23.428592165751095]
[null,null,null,null,"Coincident",19.400919999999999,20.810246401947126,21.176551803104751,21.770678864888509,22.334504607459731,22.88200256765704,23.428592165751095]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.066804911135158,47.094479468336885,47.046323234140502,47.10718196195068,47.159384315649085,47.218309993133794,47.296089080302075]
[null,null,null,null,"Coincident",40.004373172454692,40.027895128444072,39.986964796185283,40.038691597329233,40.08306092390184,40.133144731289846,40.199252971141]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.57311366783297,48.601673911410252,48.55197650276201,48.614782930969419,48.668655949643799,48.729467462892316,48.809735763431057]
[null,null,null,null,"Coincident",41.284658454824033,41.308933198863258,41.266692947267209,41.320075193977651,41.365864500199848,41.417551171384957,41.485775115090789]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.210718050631399,42.41818313016136,42.62666789760975,42.836177364728201,43.046716567901029,43.258290568266318,43.470904451837562]
[null,null,null,null,"Coincident",35.876948094584435,36.053282784764477,36.230484157441566,36.408556472347854,36.587504010152031,36.7673310725622,36.948041982429309]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.56161438502707,43.775719100848356,43.99087613830612,44.207090669546247,44.424367892135649,44.64271302918722,44.862131329485365]
[null,null,null,null,"Coincident",37.025140779014556,37.207118819926166,37.389991280323493,37.573762556265592,37.758437065418114,37.944019247159432,38.130513562687447]
[null,"Gomersal North 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.39110584246133251,0.39710753145626448,0.40386226322659746,0.4049907698671481,0.40613615887529353,0.40728791274249482,0.40839469368252235]
[null,null,null,null,"Coincident",0.17441206488140507,0.17708849375752336,0.18010073900645565,0.18060399196778229,0.18111477355249578,0.18162839352030177,0.18212195799355729]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.42511504615362228,0.43163862114811358,0.43898072089847551,0.44020735855124793,0.4414523466035799,0.4427042529809726,0.44390727574187211]
[null,null,null,null,"Coincident",0.18957833139283159,0.1924874932146993,0.19576167283310397,0.19630868692150247,0.19686388429619106,0.19742216686989322,0.19795864999299706]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.35391325703955923,0.35764901897590562,0.36142421406986186,0.36523925856152717,0.36909457308465909,0.37299058271305108,0.37692771700739974]
[null,null,null,null,"Coincident",0.15782618219331698,0.15949213008384983,0.16117566303115463,0.16287696665581619,0.16459622853775341,0.16633363823690117,0.16808938731411072]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.38468832286908611,0.38874893366946262,0.3928524065976759,0.39699919408861645,0.40118975335289031,0.40542454642722942,0.4097040402254345]
[null,null,null,null,"Coincident",0.1715501980362141,0.17336101096070633,0.17519093807734198,0.17704018114762629,0.17890894406277544,0.18079743286619693,0.18270585577620729]
[null,"Goolwa 11kV","Substation Rating","MVA","Non-Coincident",33.4,33.4,33.4,33.4,33.4,33.4,33.4]
[null,null,null,null,"Coincident",33.4,33.4,33.4,33.4,33.4,33.4,33.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",9.0574099999999991,9.7153606047269871,9.886371989934446,10.163742980107635,10.426967658062186,10.682569634652507,10.937747538157756]
[null,null,null,null,"Coincident",9.0574099999999991,9.7153606047269871,9.886371989934446,10.163742980107635,10.426967658062186,10.682569634652507,10.937747538157756]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.638021214924089,15.577967079235066,15.537517969640188,15.696646182680173,15.869703669893349,16.052208731490929,16.22785003585847]
[null,null,null,null,"Coincident",15.541614973859835,15.481931063623417,15.441731317202871,15.599878526786242,15.77186913849126,15.953249081589382,16.127807581572853]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.653099741840647,15.592987700621954,15.552499589098419,15.71178123709098,15.885005590171851,16.067686627197901,16.243497288806946]
[null,null,null,null,"Coincident",15.556600543740407,15.496859084953913,15.456620577046213,15.614920275676869,15.787076724544553,15.968631558206932,16.143358371367903]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.004881580343474,14.106495115034804,14.208845914827108,14.311939329006098,14.41578074566965,14.520375592009421,14.625729334594483]
[null,null,null,null,"Coincident",13.918543419577814,14.019530520861348,14.121250342108331,14.223708199626866,14.32690944829795,14.430859481855354,14.535563733167507]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.018385397800307,14.120096910515638,14.222546399219308,14.325739218354926,14.429680761215693,14.534376460226285,14.639831787226758]
[null,null,null,null,"Coincident",13.931963987865002,14.033048463151552,14.13486636490639,14.237423014563724,14.340723772167845,14.444774036653282,14.549579246126957]
[null,"Gulnare 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.7979999999999999E-2,1.9286107581857424E-2,1.962558483926656E-2,2.0176198138577725E-2,2.0698729382015179E-2,2.1206128687014509E-2,2.1712686158192735E-2]
[null,null,null,null,"Coincident",1.7979999999999999E-2,1.9286107581857424E-2,1.962558483926656E-2,2.0176198138577725E-2,2.0698729382015179E-2,2.1206128687014509E-2,2.1712686158192735E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.0691123997608494E-2,8.8936030446506775E-2,8.7214902218992849E-2,8.5527082003548638E-2,8.3871925209230661E-2,8.2248799719495988E-2,8.0657085650792298E-2]
[null,null,null,null,"Coincident",9.0691123997608494E-2,8.8936030446506775E-2,8.7214902218992849E-2,8.5527082003548638E-2,8.3871925209230661E-2,8.2248799719495988E-2,8.0657085650792298E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0769148756930595E-2,8.9012545237202673E-2,8.728993626262338E-2,8.5600663956166459E-2,8.3944083172324213E-2,8.2319561250721637E-2,8.0726477774498817E-2]
[null,null,null,null,"Coincident",9.0769148756930595E-2,8.9012545237202673E-2,8.728993626262338E-2,8.5600663956166459E-2,8.3944083172324213E-2,8.2319561250721637E-2,8.0726477774498817E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.1622011597847641E-2,8.0042427401856103E-2,7.849341199709356E-2,7.6974373803193774E-2,7.548473268830759E-2,7.4023919747546393E-2,7.2591377085713074E-2]
[null,null,null,null,"Coincident",8.1622011597847641E-2,8.0042427401856103E-2,7.849341199709356E-2,7.6974373803193774E-2,7.548473268830759E-2,7.4023919747546393E-2,7.2591377085713074E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.169223388123753E-2,8.01112907134824E-2,7.8560942636361028E-2,7.7040597560549817E-2,7.5549674855091786E-2,7.4087605125649478E-2,7.2653829997048947E-2]
[null,null,null,null,"Coincident",8.169223388123753E-2,8.01112907134824E-2,7.8560942636361028E-2,7.7040597560549817E-2,7.5549674855091786E-2,7.4087605125649478E-2,7.2653829997048947E-2]
[null,"Gumeracha 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.19083,0.20469231979120422,0.20829534787971291,0.21413925977668452,0.21968512391379072,0.22507038583665068,0.23044671299042938]
[null,null,null,null,"Coincident",0.19083,0.20469231979120422,0.20829534787971291,0.21413925977668452,0.21968512391379072,0.22507038583665068,0.23044671299042938]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.29845628460947937,0.29862783695938816,0.2987994879174023,0.29897123754020166,0.29914308588449862,0.29931503300703821,0.29948707896459803]
[null,null,null,null,"Coincident",0.29845628460947937,0.29862783695938816,0.2987994879174023,0.29897123754020166,0.29914308588449862,0.29931503300703821,0.29948707896459803]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.30869874728373436,0.3088761869901212,0.3090537286886596,0.30923137243797444,0.30940911829672452,0.30958696632360211,0.30976491657733335]
[null,null,null,null,"Coincident",0.30869874728373436,0.3088761869901212,0.3090537286886596,0.30923137243797444,0.30940911829672452,0.30958696632360211,0.30976491657733335]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.26861065614853147,0.26876505326344935,0.26891953912566208,0.26907411378618151,0.26922877729604877,0.26938352970633439,0.26953837106813822]
[null,null,null,null,"Coincident",0.26861065614853147,0.26876505326344935,0.26891953912566208,0.26907411378618151,0.26922877729604877,0.26938352970633439,0.26953837106813822]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.27782887255536093,0.27798856829110907,0.27814835581979364,0.27830823519417702,0.27846820646705206,0.27862826969124188,0.27878842491959999]
[null,null,null,null,"Coincident",0.27782887255536093,0.27798856829110907,0.27814835581979364,0.27830823519417702,0.27846820646705206,0.27862826969124188,0.27878842491959999]
[null,"Gumeracha Weir 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.2749999999999995E-2,7.8034723391553248E-2,7.9408303507043504E-2,8.1636174337126222E-2,8.3750420608543055E-2,8.580344059957204E-2,8.7853054394244789E-2]
[null,null,null,null,"Coincident",7.2749999999999995E-2,7.8034723391553248E-2,7.9408303507043504E-2,8.1636174337126222E-2,8.3750420608543055E-2,8.580344059957204E-2,8.7853054394244789E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.28882866252530259,0.28899468092844011,0.28916079475877637,0.28932700407116285,0.28949330892048247,0.28965970936164981,0.28982620544961091]
[null,null,null,null,"Coincident",0.28882866252530259,0.28899468092844011,0.28916079475877637,0.28932700407116285,0.28949330892048247,0.28965970936164981,0.28982620544961091]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.29874072317780742,0.29891243902269787,0.2990842535696705,0.29925616687545908,0.29942817899683011,0.29960028999058258,0.29977249991354832]
[null,null,null,null,"Coincident",0.29874072317780742,0.29891243902269787,0.2990842535696705,0.29925616687545908,0.29942817899683011,0.29960028999058258,0.29977249991354832]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.25994579627277237,0.26009521283559611,0.26024471528289872,0.26039430366404659,0.26054397802843421,0.26069373842548482,0.26084358490464982]
[null,null,null,null,"Coincident",0.25994579627277237,0.26009521283559611,0.26024471528289872,0.26039430366404659,0.26054397802843421,0.26069373842548482,0.26084358490464982]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.2688666508600267,0.2690211951204281,0.26917582821270347,0.26933055018791324,0.26948536109714705,0.26964026099152433,0.2697952499221935]
[null,null,null,null,"Coincident",0.2688666508600267,0.2690211951204281,0.26917582821270347,0.26933055018791324,0.26948536109714705,0.26964026099152433,0.2697952499221935]
[null,"Gumhaven 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.864E-2,1.9994051464172546E-2,2.0345990066959328E-2,2.0916814977924855E-2,2.1458527012278256E-2,2.1984551653278676E-2,2.25097035588828E-2]
[null,null,null,null,"Coincident",1.864E-2,1.9994051464172546E-2,2.0345990066959328E-2,2.0916814977924855E-2,2.1458527012278256E-2,2.1984551653278676E-2,2.25097035588828E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7020976673414038E-2,7.7065248247584053E-2,7.7109545269007054E-2,7.7153867752310118E-2,7.719821571212869E-2,7.724258916310664E-2,7.7286988119896274E-2]
[null,null,null,null,"Coincident",7.7020976673414038E-2,7.7065248247584053E-2,7.7109545269007054E-2,7.7153867752310118E-2,7.719821571212869E-2,7.724258916310664E-2,7.7286988119896274E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.9664192847415313E-2,7.9709983739386134E-2,7.9755800951912162E-2,7.9801644500122448E-2,7.9847514399154718E-2,7.9893410664155382E-2,7.9939333310279581E-2]
[null,null,null,null,"Coincident",7.9664192847415313E-2,7.9709983739386134E-2,7.9755800951912162E-2,7.9801644500122448E-2,7.9847514399154718E-2,7.9893410664155382E-2,7.9939333310279581E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.9318879006072642E-2,6.9358723422825647E-2,6.9398590742106345E-2,6.9438480977079109E-2,6.947839414091582E-2,6.9518330246795976E-2,6.9558289307906654E-2]
[null,null,null,null,"Coincident",6.9318879006072642E-2,6.9358723422825647E-2,6.9398590742106345E-2,6.9438480977079109E-2,6.947839414091582E-2,6.9518330246795976E-2,6.9558289307906654E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.1697773562673803E-2,7.1738985365447525E-2,7.1780220856720936E-2,7.1821480050110215E-2,7.1862762959239254E-2,7.1904069597739845E-2,7.1945399979251631E-2]
[null,null,null,null,"Coincident",7.1697773562673803E-2,7.1738985365447525E-2,7.1780220856720936E-2,7.1821480050110215E-2,7.1862762959239254E-2,7.1904069597739845E-2,7.1945399979251631E-2]
[null,"Hackham 11kV","Substation Rating","MVA","Non-Coincident",31.6,31.6,31.6,31.6,31.6,31.6,31.6]
[null,null,null,null,"Coincident",31.6,31.6,31.6,31.6,31.6,31.6,31.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.1371400000000005,7.6555978791311396,7.7903529799623445,8.0089182860271766,8.216336452811781,8.4177480143069374,8.6188254108500395]
[null,null,null,null,"Coincident",7.1371400000000005,7.6555978791311396,7.7903529799623445,8.0089182860271766,8.216336452811781,8.4177480143069374,8.6188254108500395]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.535538679915007,13.418174686977999,13.211966466534442,13.162929841000977,13.117626999568433,13.073585259528073,13.019025133642295]
[null,null,null,null,"Coincident",13.535538679915007,13.418174686977999,13.211966466534442,13.162929841000977,13.117626999568433,13.073585259528073,13.019025133642295]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.794019554192554,13.674414324447728,13.464268256951023,13.41429520545482,13.368127240118628,13.323244458747034,13.267642427594451]
[null,null,null,null,"Coincident",13.794019554192554,13.674414324447728,13.464268256951023,13.41429520545482,13.368127240118628,13.323244458747034,13.267642427594451]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.924829980427491,11.786763771358945,11.650296098967052,11.515408455323451,11.382082546785391,11.250300291514732,11.12004381702565]
[null,null,null,null,"Coincident",11.924829980427491,11.786763771358945,11.650296098967052,11.515408455323451,11.382082546785391,11.250300291514732,11.12004381702565]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.152552020299151,12.011849235378534,11.872775513526429,11.735311993378556,11.599440031948349,11.465141202098566,11.332397290042172]
[null,null,null,null,"Coincident",12.152552020299151,12.011849235378534,11.872775513526429,11.735311993378557,11.599440031948349,11.465141202098566,11.332397290042172]
[null,"Hahndorf 11kV","Substation Rating","MVA","Non-Coincident",6.8,6.8,6.8,6.8,6.8,6.8,6.8]
[null,null,null,null,"Coincident",6.8,6.8,6.8,6.8,6.8,6.8,6.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.5683000000000002,2.7548670802271649,2.8033587064898953,2.8820094371139704,2.9566488694009787,3.0291268246306662,3.1014845305943504]
[null,null,null,null,"Coincident",2.5683000000000002,2.7548670802271649,2.8033587064898953,2.8820094371139704,2.9566488694009787,3.0291268246306662,3.1014845305943504]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0687375686554041,5.1023937731014213,5.1703084568272732,5.2214357841685874,5.279225452078661,5.3420074772434596,5.409791629345257]
[null,null,null,null,"Coincident",4.879452922166295,4.9118522845141683,4.9772307929643542,5.026448844484884,5.0820804411369931,5.1425179627092836,5.2077708140494297]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.2943671950960587,5.3295215707797281,5.4004594066240994,5.4538626142240929,5.5142247296136553,5.5798014318934657,5.6506029256331303]
[null,null,null,null,"Coincident",5.0966567377418555,5.1304983242973243,5.1987870896387101,5.2501960319734318,5.3083040117881914,5.3714318473155149,5.4395893620501736]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.5059048139963496,4.5238810590007752,4.5419290199862967,4.5600489830628295,4.5782412354817206,4.5965060656403036,4.6148437630864674]
[null,null,null,null,"Coincident",4.337638339696098,4.3549432879259768,4.3723172740077434,4.3897605733669538,4.4072734625279706,4.4248562191183485,4.4425091218732291]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7064805207060649,4.7252569597213698,4.7441083070807215,4.7630348616299232,4.7820369234070208,4.8011147936470566,4.8202687747868458]
[null,null,null,null,"Coincident",4.5307238378036505,4.5487990979606705,4.5669464691183688,4.5851662389625867,4.603458696326884,4.6218241311971191,4.640262834716042]
[null,"Halbury 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.5500000000000001E-2,5.9531644649226195E-2,6.0579530510528043E-2,6.2279143308735477E-2,6.3892073453940074E-2,6.5458294890395174E-2,6.7021917785300159E-2]
[null,null,null,null,"Coincident",5.5500000000000001E-2,5.9531644649226195E-2,6.0579530510528043E-2,6.2279143308735477E-2,6.3892073453940074E-2,6.5458294890395174E-2,6.7021917785300159E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1622011597847641E-2,8.0042427401856089E-2,7.8493411997093546E-2,7.697437380319376E-2,7.5484732688307576E-2,7.4023919747546366E-2,7.2591377085713046E-2]
[null,null,null,null,"Coincident",8.1622011597847641E-2,8.0042427401856089E-2,7.8493411997093546E-2,7.697437380319376E-2,7.5484732688307576E-2,7.4023919747546366E-2,7.2591377085713046E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.169223388123753E-2,8.0111290713482386E-2,7.8560942636361014E-2,7.7040597560549803E-2,7.5549674855091772E-2,7.408760512564945E-2,7.2653829997048919E-2]
[null,null,null,null,"Coincident",8.169223388123753E-2,8.0111290713482386E-2,7.8560942636361014E-2,7.7040597560549803E-2,7.5549674855091772E-2,7.408760512564945E-2,7.2653829997048919E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3459810438062878E-2,7.2038184661670487E-2,7.064407079738419E-2,6.9276936422874386E-2,6.7936259419476827E-2,6.6621527772791733E-2,6.5332239377141749E-2]
[null,null,null,null,"Coincident",7.3459810438062878E-2,7.2038184661670487E-2,7.064407079738419E-2,6.9276936422874386E-2,6.7936259419476827E-2,6.6621527772791733E-2,6.5332239377141749E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3523010493113786E-2,7.2100161642134161E-2,7.0704848372724921E-2,6.9336537804494822E-2,6.7994707369582602E-2,6.6678844613084501E-2,6.538844699734403E-2]
[null,null,null,null,"Coincident",7.3523010493113786E-2,7.2100161642134161E-2,7.0704848372724921E-2,6.9336537804494822E-2,6.7994707369582602E-2,6.6678844613084501E-2,6.538844699734403E-2]
[null,"Hamley Bridge 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.75097999999999998,0.80553287385001593,0.81971199680714135,0.84270974850439939,0.86453458238630476,0.88572739273493639,0.90688504177305795]
[null,null,null,null,"Coincident",0.75097999999999998,0.80553287385001593,0.81971199680714135,0.84270974850439939,0.86453458238630476,0.88572739273493639,0.90688504177305795]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5803508167169813,2.6249209929157988,2.6203343787824527,2.6334057733457596,2.6293801848082996,2.6252677434755207,2.621967781067315]
[null,null,null,null,"Coincident",2.5208208017466753,2.5643627211522091,2.5598819225561349,2.5726517533518352,2.5687190372037985,2.5647014719989163,2.5614776414136737]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8047291486054147,2.8531749922997816,2.8481895421548402,2.8623975797236518,2.8580219400090217,2.853551895082088,2.8499649794209949]
[null,null,null,null,"Coincident",2.7400226105942127,2.7873507838610969,2.7824803506044948,2.7963606014693863,2.7920859100041291,2.7877189913031701,2.7842148276235585]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2541402349728115,2.2398061287888207,2.2255631733668393,2.2114107890780219,2.1973483999793908,2.1833754337903963,2.1694913218696286]
[null,null,null,null,"Coincident",2.2021360652049848,2.1881326541924375,2.1742182910471337,2.1603924095125624,2.1466544469330446,2.1330038442308372,2.1194400458833784]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4501524293182735,2.4345718791182835,2.4190904058335212,2.4037073794326322,2.3884221738906422,2.3732341671634742,2.3581427411626401]
[null,null,null,null,"Coincident",2.3936261578315055,2.3784050589048236,2.363280751138189,2.3482526190353941,2.3333200510141792,2.318482439381345,2.3037391803080203]
[null,"Happy Valley 11kV","Substation Rating","MVA","Non-Coincident",59.8,59.8,59.8,59.8,59.8,59.8,59.8]
[null,null,null,null,"Coincident",59.8,59.8,59.8,59.8,59.8,59.8,59.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",15.364619999999999,16.480740504691777,16.770837226534582,17.241358033590327,17.687881614988768,18.121474357457,18.554347719682497]
[null,null,null,null,"Coincident",15.364619999999999,16.480740504691777,16.770837226534582,17.241358033590327,17.687881614988768,18.121474357457,18.554347719682497]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.575949706837612,31.61728884557597,31.458113826739325,31.469230320143495,31.45395274646085,31.440086310708541,31.401106235225576]
[null,null,null,null,"Coincident",30.919236640047639,30.959716012006808,30.803851497390845,30.814736791209786,30.79977695879413,30.786198915620126,30.748029543382884]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.524379503470378,32.56696032365651,32.403004250500167,32.414454644030116,32.39871818609425,32.384435251678795,32.34428435266063]
[null,null,null,null,"Coincident",31.847941099955321,31.889636329010521,31.729090195907325,31.740302445434608,31.724893272589057,31.710907393044469,31.671591547928831]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.294592974413728,27.05902082899118,26.825481842141503,26.593958466230724,26.364433305073682,26.136889112626925,25.911308791692864]
[null,null,null,null,"Coincident",26.726923085608142,26.496250343291663,26.267568474143687,26.040860295483967,25.816108772931251,25.593297019123373,25.372408292448345]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.114425964529353,27.871778065438285,27.631224393809202,27.39274687493932,27.156327590123627,26.921948775308557,26.689592819757191]
[null,null,null,null,"Coincident",27.529705280983055,27.292103945730648,27.056553282431956,26.823035592299817,26.591533329300447,26.362029098835066,26.134505656432914]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Harrow 11kV","Substation Rating","MVA","Non-Coincident",28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434]
[null,null,null,null,"Coincident",28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434,28.314734561213434]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.0305900000000001,6.468665601895081,6.5825281243510867,6.7672068260581462,6.9424666531639012,7.1126511456408705,7.2825532824658268]
[null,null,null,null,"Coincident",6.0305900000000001,6.468665601895081,6.5825281243510867,6.7672068260581462,6.9424666531639012,7.1126511456408705,7.2825532824658268]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.758519315676818,19.858102674601625,19.984340613068319,20.141579467864226,20.296199858314896,20.454066006639536,20.619748036993954]
[null,null,null,null,"Coincident",18.359930588983946,18.452465030885506,18.569767332283465,18.715876178489044,18.859551905954287,19.006243643289633,19.160198022590492]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.570576031439561,20.674252173538104,20.805678373537866,20.969379598614452,21.130354742903368,21.294709042687661,21.467200449963546]
[null,null,null,null,"Coincident",19.114506612496644,19.210844133656572,19.332967450238044,19.485081233751828,19.634661899614336,19.787382530539677,19.94766429124169]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.414076260111464,17.554128771459101,17.69530765354509,17.83762196519335,17.981080838083294,18.125693477335762,18.271469162103674]
[null,null,null,null,"Coincident",16.181436791837243,16.31157581420393,16.442761478185972,16.575002201386724,16.70830646910801,16.842682834894617,16.978139921083102]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.129778552874271,18.275587091815993,18.422568294282883,18.570731591408077,18.720086490174495,18.870642574024856,19.022409503476613]
[null,null,null,null,"Coincident",16.846478752095674,16.981966366905308,17.118543639324521,17.256219332912316,17.395002281708503,17.534901390800588,17.675925636895116]
[null,"Hatherleigh 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3180000000000001E-2,3.5590269720023875E-2,3.6216735537645407E-2,3.7232828378087258E-2,3.8197099048679843E-2,3.9133445485825438E-2,4.0068238416509173E-2]
[null,null,null,null,"Coincident",3.3180000000000001E-2,3.5590269720023875E-2,3.6216735537645407E-2,3.7232828378087258E-2,3.8197099048679843E-2,3.9133445485825438E-2,4.0068238416509173E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3409224820590956E-2,6.3212906475689973E-2,6.3017195942864493E-2,6.2822091340295899E-2,6.2627590791991761E-2,6.2433692427767827E-2,6.2240394383230049E-2]
[null,null,null,null,"Coincident",6.3409224820590956E-2,6.3212906475689973E-2,6.3017195942864493E-2,6.2822091340295899E-2,6.2627590791991761E-2,6.2433692427767827E-2,6.2240394383230049E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.539810192772337E-2,6.519562591313019E-2,6.4993776775086581E-2,6.4792552572749296E-2,6.4591951371284026E-2,6.4391971241846799E-2,6.4192610261565489E-2]
[null,null,null,null,"Coincident",6.539810192772337E-2,6.519562591313019E-2,6.4993776775086581E-2,6.4792552572749296E-2,6.4591951371284026E-2,6.4391971241846799E-2,6.4192610261565489E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7068302338531864E-2,5.6891615828120974E-2,5.6715476348578042E-2,5.6539882206266309E-2,5.6364831712792586E-2,5.6190323184991044E-2,5.6016354944907046E-2]
[null,null,null,null,"Coincident",5.7068302338531864E-2,5.6891615828120974E-2,5.6715476348578042E-2,5.6539882206266309E-2,5.6364831712792586E-2,5.6190323184991044E-2,5.6016354944907046E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8858291734951038E-2,5.8676063321817171E-2,5.849439909757792E-2,5.8313297315474369E-2,5.8132756234155626E-2,5.7952774117662122E-2,5.7773349235408944E-2]
[null,null,null,null,"Coincident",5.8858291734951038E-2,5.8676063321817171E-2,5.849439909757792E-2,5.8313297315474369E-2,5.8132756234155626E-2,5.7952774117662122E-2,5.7773349235408944E-2]
[null,"Hawker 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.32973000000000002,0.35368232775115954,0.35990790261687228,0.37000544005746577,0.37958798882824618,0.38889303737315323,0.39818264777201845]
[null,null,null,null,"Coincident",0.32973000000000002,0.35368232775115954,0.35990790261687228,0.37000544005746577,0.37958798882824618,0.38889303737315323,0.39818264777201845]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.90944762939084367,0.91155163141227757,0.90421133264679343,0.90329177802357707,0.90242697239646874,0.89940295557801275,0.896302038106777]
[null,null,null,null,"Coincident",0.90944762939084367,0.91155163141227757,0.90421133264679343,0.90329177802357707,0.90242697239646874,0.89940295557801275,0.896302038106777]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.9094532937529024,0.91155730887880637,0.90421696439534083,0.9032974040448124,0.90243259303138823,0.89940855737828407,0.89630762059343561]
[null,null,null,null,"Coincident",0.90945329375290251,0.91155730887880648,0.90421696439534094,0.90329740404481251,0.90243259303138834,0.89940855737828418,0.89630762059343572]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.78512261475403222,0.7783049497452128,0.77154648638884737,0.76484671060340681,0.75820511277142344,0.75162118770072706,0.74509443458601776]
[null,null,null,null,"Coincident",0.78512261475403222,0.7783049497452128,0.77154648638884737,0.76484671060340681,0.75820511277142344,0.75162118770072706,0.74509443458601776]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.78512750477585069,0.77830979730419803,0.77155129185372828,0.76485147433971035,0.75820983514150253,0.75162586906378803,0.74509907529814778]
[null,null,null,null,"Coincident",0.7851275047758508,0.77830979730419814,0.77155129185372839,0.76485147433971046,0.75820983514150264,0.75162586906378814,0.74509907529814801]
[null,"Hay Flat 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0189999999999999E-2,1.0930224486047115E-2,1.1122620106347399E-2,1.143467514082909E-2,1.1730814927849538E-2,1.2018378827623908E-2,1.2305465625805562E-2]
[null,null,null,null,"Coincident",1.0189999999999999E-2,1.0930224486047115E-2,1.1122620106347399E-2,1.143467514082909E-2,1.1730814927849538E-2,1.2018378827623908E-2,1.2305465625805562E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9600458133125788E-2,4.9620574211581024E-2,4.9640698448360346E-2,4.9660830846772468E-2,4.9680971410127436E-2,4.9701120141736652E-2,4.9721277044912845E-2]
[null,null,null,null,"Coincident",4.9600458133125788E-2,4.9620574211581024E-2,4.9640698448360346E-2,4.9660830846772468E-2,4.9680971410127436E-2,4.9701120141736652E-2,4.9721277044912845E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9863654267364034E-2,4.9883877088262481E-2,4.9904108110775725E-2,4.9924347338230049E-2,4.9944594773953056E-2,4.9964850421273715E-2,4.9985114283522342E-2]
[null,null,null,null,"Coincident",4.9863654267364034E-2,4.9883877088262481E-2,4.9904108110775725E-2,4.9924347338230049E-2,4.9944594773953056E-2,4.9964850421273715E-2,4.9985114283522342E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4640412319813208E-2,4.4658516790422924E-2,4.467662860352431E-2,4.469474776209522E-2,4.4712874269114695E-2,4.4731008127562991E-2,4.4749149340421561E-2]
[null,null,null,null,"Coincident",4.4640412319813208E-2,4.4658516790422924E-2,4.467662860352431E-2,4.469474776209522E-2,4.4712874269114695E-2,4.4731008127562991E-2,4.4749149340421561E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4877288840627631E-2,4.4895489379436236E-2,4.4913697299698151E-2,4.4931912604407043E-2,4.4950135296557753E-2,4.4968365379146349E-2,4.4986602855170109E-2]
[null,null,null,null,"Coincident",4.4877288840627631E-2,4.4895489379436236E-2,4.4913697299698151E-2,4.4931912604407043E-2,4.4950135296557753E-2,4.4968365379146349E-2,4.4986602855170109E-2]
[null,"Henley South 11kV","Substation Rating","MVA","Non-Coincident",55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076]
[null,null,null,null,"Coincident",55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076,55.725068364931076]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",9.9071299999999987,10.626806173940329,10.813860974896714,11.11725349636527,11.40517257076997,11.68475382085551,11.963871213482538]
[null,null,null,null,"Coincident",9.9071299999999987,10.626806173940329,10.813860974896714,11.11725349636527,11.40517257076997,11.68475382085551,11.963871213482538]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",34.51194063914528,34.827762991548852,34.914290662762063,35.146173766451831,35.386416043514444,35.611273529768638,35.848919873250622]
[null,null,null,null,"Coincident",34.440431302194312,34.755599265230131,34.84194764961444,35.073350287509243,35.313094778425317,35.537486356085189,35.774640292239845]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.684190821505545,36.010740557050781,36.100207271287381,36.339966634774555,36.588369103581869,36.820864213927464,37.066582574349816]
[null,null,null,null,"Coincident",35.610252561934502,35.936125680788884,36.025407018448675,36.264669596394583,36.512557370997158,36.744570747459427,36.989779975195958]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.106678243684577,32.477592559656223,32.852791885392769,33.232325723725182,33.616244149368825,34.004597815530211,34.39743796059004]
[null,null,null,null,"Coincident",32.040152651950685,32.410298427054748,32.784720333309487,33.163467770975146,33.546590711011412,33.934139701670482,34.326165875166247]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.197230056452,33.580743037305581,33.968686574751779,34.361111853059967,34.758070647808836,35.159615332717557,35.565798886555811]
[null,null,null,null,"Coincident",33.128444822530582,33.511163157865397,33.898302869603057,34.289915035958252,34.686051325229784,35.086764002617564,35.492105937118353]
[null,"Hermitage 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.14382,0.15426740780994075,0.15698284825268727,0.16138714217409617,0.16556681088550743,0.16962544092138082,0.17367733722309675]
[null,null,null,null,"Coincident",0.14382,0.15426740780994075,0.15698284825268727,0.16138714217409617,0.16556681088550743,0.16962544092138082,0.17367733722309675]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.20476817690526986,0.20607551891960357,0.20511565619372893,0.20363684468495286,0.20227979356414408,0.20096036540399942,0.19987506112253206]
[null,null,null,null,"Coincident",0.18376631260729345,0.18493956826118269,0.18407815299437211,0.18275101446085512,0.1815331480703857,0.18034904587538408,0.1793750548535544]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.21330018427632277,0.21466199887458706,0.21366214186846763,0.21212171321349257,0.21070811829598343,0.20933371396249939,0.20820318866930423]
[null,null,null,null,"Coincident",0.19142324229926402,0.19264538360539865,0.19174807603580429,0.19036564006339077,0.18909702923998511,0.1878635894535251,0.1868490154724525]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.17708145755045249,0.17229583850655331,0.1676395506187793,0.16310909871800161,0.1587010820918921,0.15441219193223221,0.15023920885120823]
[null,null,null,null,"Coincident",0.1589192567760471,0.15462447045459909,0.15044575055531476,0.14637996038795015,0.14242404803118519,0.13857504404174684,0.13483005922544328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.18445985161505468,0.17947483177765969,0.17462453189456179,0.16990531116458502,0.16531362717905426,0.16084603326274188,0.15649917588667525]
[null,null,null,null,"Coincident",0.16554089247504908,0.16106715672354072,0.15671432349511955,0.15247912540411473,0.14835838336581791,0.14434900421015295,0.14044797835983674]
[null,"Hillcrest 11kV","Substation Rating","MVA","Non-Coincident",61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295]
[null,null,null,null,"Coincident",61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295,61.681609195402295]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",10.50055,11.2633335355213,11.461592596438292,11.783157806676439,12.088322737058927,12.384650421825931,12.680486464872679]
[null,null,null,null,"Coincident",10.50055,11.2633335355213,11.461592596438292,11.783157806676439,12.088322737058927,12.384650421825931,12.680486464872679]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.262072889237217,37.260696116953952,37.31431619683962,37.409850110649934,37.501333571299675,37.580615740867749,37.674728847395045]
[null,null,null,null,"Coincident",35.10261860342446,35.101321619423949,35.15183424708443,35.241831670205364,35.328013376662085,35.402700895219432,35.491359851306804]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.281512385927485,38.280097947032175,38.335184999177109,38.433332590581287,38.527318913950381,38.60877013555379,38.705458048325369]
[null,null,null,null,"Coincident",36.062978375892236,36.061645908178285,36.11354049244305,36.206000122323189,36.29453964273501,36.371270509942164,36.462355054156085]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.89103877409466,34.079374523530518,34.2687568727697,34.45919163786759,34.65068466719994,34.843241841642488,35.036869074751571]
[null,null,null,null,"Coincident",31.926946514683504,32.1043676152618,32.282774661894024,32.462173133576869,32.642568539754322,32.823966420486883,33.006372346621703]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.818251374769723,35.011739733460153,35.206303325497196,35.401948126055551,35.598680143514592,35.79650541964277,35.995430029783265]
[null,null,null,null,"Coincident",32.800424229746085,32.982699329671476,33.165987349790207,33.350293918996854,33.535624697466275,33.721985376827469,33.909381680338363]
[null,"Hindley Street 11kV","Substation Rating","MVA","Non-Coincident",77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096]
[null,null,null,null,"Coincident",77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096,77.12395688259096]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.46457000000000009,0.49831740819263098,0.50708887368064903,0.52131570462953603,0.53481694710805316,0.54792720823839458,0.56101571793724159]
[null,null,null,null,"Coincident",0.46457000000000009,0.49831740819263098,0.50708887368064903,0.52131570462953603,0.53481694710805316,0.54792720823839458,0.56101571793724159]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.897344692703257,45.638783733956942,46.537582249814349,46.820764974196585,47.094503572159077,47.375776066343946,47.678262284050668]
[null,null,null,null,"Coincident",42.07960382140184,42.774510420605367,43.616900671552443,43.882310952107552,44.13886981615012,44.402489751853814,44.685992045578587]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.00285390624056,45.746035336730493,46.646946038178953,46.930794244823929,47.205176131256671,47.48710961864402,47.790306682017771]
[null,null,null,null,"Coincident",42.178491315429497,42.875030952160429,43.719400828706242,43.985434826101567,44.242596606066144,44.506836051281574,44.791004578260271]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.263646803506212,42.862485841159348,43.469809906020018,44.085739223528087,44.710395722613121,45.343903059831341,45.986386643844583]
[null,null,null,null,"Coincident",39.611195844912189,40.172451964393325,40.741660593889264,41.318934413535395,41.904387700046435,42.498136349338523,43.100297899471919]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.362966800400841,42.963213115841356,43.571964398389042,44.189341156014777,44.815465604182336,45.450461690042104,46.094455116967517]
[null,null,null,null,"Coincident",39.704282555261635,40.266857632292812,40.837403907817666,41.416034326771026,42.002863434419048,42.598007399034444,43.201584034893102]
[null,"Hindley Street 33kV","Substation Rating","MVA","Non-Coincident",27.4,27.4,27.4,27.4,27.4,27.4,27.4]
[null,null,null,null,"Coincident",27.4,27.4,27.4,27.4,27.4,27.4,27.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.9880000000000001E-2,5.3503395227088336E-2,5.4445170844416912E-2,5.5972678707022085E-2,5.7422281511396958E-2,5.8829905389782194E-2,6.0235193858212112E-2]
[null,null,null,null,"Coincident",4.9880000000000001E-2,5.3503395227088336E-2,5.4445170844416912E-2,5.5972678707022085E-2,5.7422281511396958E-2,5.8829905389782194E-2,6.0235193858212112E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.1305490710420099,8.260594215075054,8.4234858436391651,8.4824994702137602,8.5398156980427249,8.5985169054653117,8.661102805359981]
[null,null,null,null,"Coincident",8.6028680327111733,7.7831904030233598,7.9366680496870048,7.9922711068090662,8.046274862805431,8.1015835563887073,8.1605524347456431]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.7541318079739643,8.8247622524232074,8.9987787768476846,9.061822815885904,9.1230535301211209,9.1857638129345709,9.2526240983504184]
[null,null,null,null,"Coincident",9.1904121060809292,8.3147535254398228,8.4787131278127834,8.5381136681170915,8.5958056809430072,8.654891753767382,8.7178879884501548]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.43,7.43,7.43,7.43,7.43,7.43,7.43]
[null,null,null,null,"Coincident",7.9428057339687133,7.0005986480886762,7.0005986480886762,7.0005986480886762,7.0005986480886762,7.0005986480886762,7.0005986480886762]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.0057378259987217,7.9374415239822662,7.9374415239822653,7.9374415239822653,7.9374415239822662,7.9374415239822653,7.9374415239822653]
[null,null,null,null,"Coincident",8.485269993233878,7.4787136476545326,7.4787136476545326,7.4787136476545326,7.4787136476545326,7.4787136476545326,7.4787136476545326]
[null,"Holden Hill 11kV","Substation Rating","MVA","Non-Coincident",46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872]
[null,null,null,null,"Coincident",46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872,46.713043478260872]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.205549999999999,12.019546318903361,12.231116362382837,12.574271248706321,12.899924751203571,13.216147681244463,13.531845961064329]
[null,null,null,null,"Coincident",11.205549999999999,12.019546318903361,12.231116362382837,12.574271248706321,12.899924751203571,13.216147681244463,13.531845961064329]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",37.422040609839719,37.625409446326941,37.774395941319376,37.957439915169097,38.134110498579261,38.316325360064312,38.513475449743204]
[null,null,null,null,"Coincident",34.368352819176167,34.555126490812349,34.691955491629749,34.860062836183189,35.022316867349353,35.189662756198842,35.370725138955031]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",38.179246950125048,38.386730799313213,38.538731921963219,38.725479650479741,38.905725027880827,39.091626867578775,39.292766138378205]
[null,null,null,null,"Coincident",35.06377012501386,35.254323018895981,35.393920649784469,35.565429517746843,35.730966635007022,35.901698639792272,36.08642468123665]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.672179189421129,33.945214468451717,34.220463689834411,34.497944805611006,34.777675913389764,35.059675257525797,35.343961230310939]
[null,null,null,null,"Coincident",30.924485028436916,31.175240269168981,31.428028791641925,31.6828670829873,31.939771764024695,32.198759590345823,32.459847453407292]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.353509954872472,34.632069893730119,34.912888572368296,35.195984306074635,35.481375558648629,35.769080943605964,36.059119225392408]
[null,null,null,null,"Coincident",31.550218306259136,31.806047387301557,32.063950891984149,32.323945641042933,32.586048591607067,32.850276838304829,33.116647614378522]
[null,"Hope Valley 11kV","Substation Rating","MVA","Non-Coincident",31.2,31.2,31.2,31.2,31.2,31.2,31.2]
[null,null,null,null,"Coincident",31.2,31.2,31.2,31.2,31.2,31.2,31.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.8915299999999995,8.4647884630397829,8.6137870704458983,8.8554545548682029,9.0847966562877787,9.3074972590342391,9.5298283758599958]
[null,null,null,null,"Coincident",7.8915299999999995,8.4647884630397829,8.6137870704458983,8.8554545548682029,9.0847966562877787,9.3074972590342391,9.5298283758599958]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.433555006269227,18.409663049579031,18.398107686955605,18.446195642660825,18.487328977088293,18.532412673235893,18.584912079417183]
[null,null,null,null,"Coincident",16.169397560921599,16.148440206461174,16.13830416638886,16.180485572711472,16.21656658026199,16.256112734342331,16.302163741322204]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.008262921887773,18.983626079220631,18.971710451940428,19.0212976588091,19.06371341829691,19.11020270099754,19.164338895323461]
[null,null,null,null,"Coincident",16.673515229265249,16.651904481713004,16.64145242758585,16.684948934988928,16.722154849842227,16.762933945033193,16.810420696676783]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.282805704545055,16.247358044002489,16.21198755300065,16.176694063541483,16.14147740799266,16.106337419086799,16.07127392992065]
[null,null,null,null,"Coincident",14.282820582057496,14.251726888208296,14.220700885316329,14.189742426018412,14.158851363272172,14.128027550355347,14.097270840865088]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.790459129166528,16.753906307351649,16.717433061013082,16.681039216915046,16.644724602198899,16.608489044382313,16.57233237135846]
[null,null,null,null,"Coincident",14.728119931156261,14.696056820828531,14.664063511877263,14.632139852344892,14.600285690604666,14.568500875359922,14.53678525564337]
[null,"Houghton 7.6kV","Substation Rating","MVA","Non-Coincident",3.6,3.6,3.6,3.6,3.6,3.6,3.6]
[null,null,null,null,"Coincident",3.6,3.6,3.6,3.6,3.6,3.6,3.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.6672199999999999,1.7883306052627548,1.8198090965362623,1.8708654649944136,1.9193178865563598,1.9663671785074712,2.0133384102704168]
[null,null,null,null,"Coincident",1.6672199999999999,1.7883306052627548,1.8198090965362623,1.8708654649944136,1.9193178865563598,1.9663671785074712,2.0133384102704168]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1727312818583533,2.2170831246648572,2.2180241053417165,2.2416081615481231,2.2647315356758893,2.2873923245585193,2.3129623082739674]
[null,null,null,null,"Coincident",2.1198431383853977,2.1631153784608941,2.1640334539946009,2.1870434323301113,2.2096039424080707,2.2317131273884412,2.2566606922255699]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3137741914004311,2.3610051352744317,2.3620071997372132,2.3871222155859511,2.4117466441665347,2.4358784587683653,2.463108318663755]
[null,null,null,null,"Coincident",2.2574528126728493,2.3035340713755508,2.3045117438071965,2.3290154155046237,2.3530404417004838,2.3765848450179181,2.4031518816967781]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9227708318920584,1.9346141663918774,1.9465304500803091,1.9585201322889265,1.9705836651169666,1.9827215034483783,1.9949341049689746]
[null,null,null,null,"Coincident",1.8759671703109801,1.8875222169864121,1.8991484371374701,1.9108462691581976,1.9226161541429321,1.9344585359029385,1.9463738609831427]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0475875521082574,2.0601996969853564,2.0728895265496079,2.0856575193009546,2.0985041566866678,2.1114299231195015,2.124435305995954]
[null,null,null,null,"Coincident",1.9977456295780514,2.0100507724188974,2.022431708963452,2.0348889060641202,2.04742283344889,2.0600339637390466,2.072722772466991]
[null,"Hoyleton 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.1340000000000004E-2,5.5069452906149063E-2,5.6038794529919098E-2,5.7611012927396031E-2,5.9103045966221332E-2,6.0551871345457461E-2,6.1998292956708306E-2]
[null,null,null,null,"Coincident",5.1340000000000004E-2,5.5069452906149063E-2,5.6038794529919098E-2,5.7611012927396031E-2,5.9103045966221332E-2,6.0551871345457461E-2,6.1998292956708306E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7485668497902833E-2,8.5967698307690507E-2,8.2545581682133412E-2,8.2324439616906928E-2,8.2109218065163123E-2,8.1762791501601109E-2,8.1020582010178518E-2]
[null,null,null,null,"Coincident",6.5614251373427121E-2,6.4475773730767877E-2,6.1909186261600059E-2,6.1743329712680192E-2,6.1581913548872338E-2,6.1322093626200835E-2,6.0765436507633885E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.8662268353161974E-2,8.7123882893377413E-2,8.3655742021844462E-2,8.3431625804092149E-2,8.3213509725153442E-2,8.2862424050544517E-2,8.2110232540407627E-2]
[null,null,null,null,"Coincident",6.6496701264871477E-2,6.534291217003306E-2,6.274180651638335E-2,6.2573719353069102E-2,6.2410132293865078E-2,6.2146818037908398E-2,6.1582674405305717E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5866422322010546E-2,7.4253033674950536E-2,7.2673955633910853E-2,7.1128458543524425E-2,6.961582826540326E-2,6.8135365848151566E-2,6.6686387204396597E-2]
[null,null,null,null,"Coincident",5.689981674150791E-2,5.5689775256212902E-2,5.450546672543314E-2,5.3346343907643319E-2,5.2211871199052448E-2,5.1101524386113678E-2,5.0014790403297447E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.688675425815214E-2,7.5251667053131702E-2,7.3651351899471973E-2,7.2085069328628321E-2,7.0552095597723893E-2,6.905172235512487E-2,6.7583256313127574E-2]
[null,null,null,null,"Coincident",5.7665065693614105E-2,5.643875028984878E-2,5.5238513924603987E-2,5.4063801996471234E-2,5.2914071698292924E-2,5.178879176634367E-2,5.0687442234845684E-2]
[null,"Ingle Farm 11kV","Substation Rating","MVA","Non-Coincident",51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414]
[null,null,null,null,"Coincident",51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414,51.712945994724414]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.985110000000001,13.928377554074119,14.173547160856987,14.571198676931427,14.948569404098953,15.31501188403999,15.680846393749173]
[null,null,null,null,"Coincident",12.985110000000001,13.928377554074119,14.173547160856987,14.571198676931427,14.948569404098953,15.31501188403999,15.680846393749173]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.160509441148932,36.212355560161171,36.211705325194984,36.381012372501445,36.546562920272706,36.719656100352537,36.909245228113534]
[null,null,null,null,"Coincident",34.108420633201035,34.157324513782328,34.156711179288983,34.316410145784253,34.472565792004588,34.635836030343178,34.814666080502683]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.231941705271538,37.285324019584614,37.284654518221664,37.458978116340901,37.629433910220875,37.807655823847419,38.002862458428687]
[null,null,null,null,"Coincident",35.119049711979734,35.169402609632563,35.168771102099761,35.333201932938053,35.49398445527742,35.662092374385182,35.846221140975864]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.61495116475907,32.65400701874632,32.693109641460062,32.73225908890506,32.771455417153142,32.810698682343279,32.849988940681662]
[null,null,null,null,"Coincident",30.764070817901803,30.800910273887734,30.837793844500926,30.874721582567908,30.911693540978462,30.948709772685703,30.985770330706153]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.581328893136444,33.621541968156016,33.661803197654748,33.702112639296828,33.742470350815474,33.782876390013058,33.823330814761157]
[null,null,null,null,"Coincident",31.675607147435478,31.713538152803487,31.751514579910733,31.789536483148989,31.827603916975157,31.865716935911347,31.903875594544957]
[null,"Inverness 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.30922632825003055,0.31630653854287694,0.32011272218009762,0.32085771452684386,0.3198987049642818,0.3189216998274772,0.31797186132437982]
[null,null,null,null,"Coincident",0.11159037062935885,0.11414540303938603,0.11551893887368742,0.11578778393794802,0.11544170657406692,0.11508913515513308,0.11474636734749359]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.36061676892911404,0.36887364205370921,0.37331237679202545,0.3741811796992065,0.37306279197400727,0.37192341798326239,0.37081572545937586]
[null,null,null,null,"Coincident",0.13013561661354986,0.13311527082807767,0.13471707510320918,0.13503059963058323,0.13462700753844611,0.134215842141786,0.13381610962229651]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.27362157504906653,0.27424456531989722,0.27486897403471383,0.27549480442307456,0.2761220597218908,0.27675074317544379,0.27738085803540152]
[null,null,null,null,"Coincident",9.8741698822054455E-2,9.8966517050223787E-2,9.9191847151657603E-2,9.941769029180518E-2,9.9644047638769301E-2,9.9870920363312327E-2,0.10009830963886229]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.31909484830058199,0.31982137356061602,0.32054955299637961,0.32127939037415237,0.32201088946878925,0.32274405406373979,0.32347888795106788]
[null,null,null,null,"Coincident",0.11515161916934046,0.11541380002404841,0.11567657782043264,0.11593995391762892,0.11620392967786743,0.11646850646648001,0.11673368565190712]
[null,"Jabuk 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.9999999999999993E-3,9.6537802133880302E-3,9.8237076503558968E-3,1.0099320536551697E-2,1.0360876776314604E-2,1.0614858630874892E-2,1.0868419100318943E-2]
[null,null,null,null,"Coincident",8.9999999999999993E-3,9.6537802133880302E-3,9.8237076503558968E-3,1.0099320536551697E-2,1.0360876776314604E-2,1.0614858630874892E-2,1.0868419100318943E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7083262373999123E-2,7.6980328498312212E-2,7.6877532076366079E-2,7.6774872924610535E-2,7.6672350859740515E-2,7.656996569869573E-2,7.6467717258660334E-2]
[null,null,null,null,"Coincident",7.7083262373999123E-2,7.6980328498312212E-2,7.6877532076366079E-2,7.6774872924610535E-2,7.6672350859740515E-2,7.656996569869573E-2,7.6467717258660334E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8133228918174105E-2,7.802889295956536E-2,7.7924696326982318E-2,7.7820638834374595E-2,7.7716720295940303E-2,7.7612940526125648E-2,7.750929933962461E-2]
[null,null,null,null,"Coincident",7.8133228918174105E-2,7.802889295956536E-2,7.7924696326982318E-2,7.7820638834374595E-2,7.7716720295940303E-2,7.7612940526125648E-2,7.750929933962461E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.9374936136599216E-2,6.9282295648480999E-2,6.9189778868729471E-2,6.9097385632149483E-2,6.9005115773766459E-2,6.8912969128826163E-2,6.8820945532794303E-2]
[null,null,null,null,"Coincident",6.9374936136599216E-2,6.9282295648480999E-2,6.9189778868729471E-2,6.9097385632149483E-2,6.9005115773766459E-2,6.8912969128826163E-2,6.8820945532794303E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.0319906026356696E-2,7.0226003663608844E-2,7.0132226694284081E-2,7.0038574950937141E-2,6.994504826634626E-2,6.9851646473513093E-2,6.9758369405662157E-2]
[null,null,null,null,"Coincident",7.0319906026356696E-2,7.0226003663608844E-2,7.0132226694284081E-2,7.0038574950937141E-2,6.994504826634626E-2,6.9851646473513093E-2,6.9758369405662157E-2]
[null,"James Well 7.6kV","Substation Rating","MVA","Non-Coincident",0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992]
[null,null,null,null,"Coincident",0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992,0.90999999999999992]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15253,0.16361012177200848,0.16649001421208723,0.17116104016002562,0.17559383718791854,0.17989826521859417,0.18419555170796098]
[null,null,null,null,"Coincident",0.15253,0.16361012177200848,0.16649001421208723,0.17116104016002562,0.17559383718791854,0.17989826521859417,0.18419555170796098]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.37037685150295707,0.36168005881826815,0.35318747490821928,0.34489430476099958,0.33679586595613176,0.32888758602072288,0.32116499984779306]
[null,null,null,null,"Coincident",0.37037685150295707,0.36168005881826815,0.35318747490821928,0.34489430476099958,0.33679586595613176,0.32888758602072288,0.32116499984779306]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.37463077565333919,0.36583409687619567,0.35724397229197263,0.34885555181625827,0.3406640992491301,0.33266498960104157,0.32485370648149881]
[null,null,null,null,"Coincident",0.37463077565333919,0.36583409687619567,0.35724397229197263,0.34885555181625827,0.3406640992491301,0.33266498960104157,0.32485370648149881]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.33333916635266136,0.32551205293644137,0.31786872741739736,0.31040487428489966,0.3031162793605186,0.29599882741865058,0.28904849986301379]
[null,null,null,null,"Coincident",0.33333916635266136,0.32551205293644137,0.31786872741739736,0.31040487428489966,0.3031162793605186,0.29599882741865058,0.28904849986301379]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.33716769808800529,0.32925068718857614,0.3215195750627754,0.31396999663463249,0.3065976893242171,0.29939849064093738,0.29236833583334892]
[null,null,null,null,"Coincident",0.33716769808800529,0.32925068718857614,0.3215195750627754,0.31396999663463249,0.3065976893242171,0.29939849064093738,0.29236833583334892]
[null,"Jamestown 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4570500000000002,1.562893384435226,1.590403692439007,1.635023887531406,1.6773683896587999,1.7184866409018074,1.7595366722355246]
[null,null,null,null,"Coincident",1.4570500000000002,1.562893384435226,1.590403692439007,1.635023887531406,1.6773683896587999,1.7184866409018074,1.7595366722355246]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.31,2.31,2.31,2.31,2.31,2.31,2.31]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0868643517842465,2.0868643517842465,2.0868643517842465,2.0868643517842465,2.0868643517842465,2.0868643517842465,2.0868643517842465]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.19,2.19,2.19,2.19,2.19,2.19,2.19]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Jervois 11kV","Substation Rating","MVA","Non-Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,null,null,"Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.60163,0.64533375442007124,0.65669302596484658,0.67511713493395542,0.69260158832601748,0.70957971089925143,0.72652966481387637]
[null,null,null,null,"Coincident",0.60163,0.64533375442007124,0.65669302596484658,0.67511713493395542,0.69260158832601748,0.70957971089925143,0.72652966481387637]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.517896032019725,1.4890459466830619,1.4619167206435322,1.4514160565191956,1.4415808527032064,1.4314824149860466,1.4218516290027758]
[null,null,null,null,"Coincident",1.0266962136164546,1.007182180538543,0.98883212686848498,0.98172953758075276,0.97507706184788845,0.96824653620651513,0.96173232752911486]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6621280791151927,1.6305366289029333,1.6008295558137671,1.5893311077499734,1.578561352719634,1.5675033510312357,1.5569574378269937]
[null,null,null,null,"Coincident",1.124253947157682,1.1028856705225416,1.0827919758195583,1.0750144911694046,1.0677298903285202,1.0602503210931118,1.0531171255859626]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.333335588020903,1.3181266610438394,1.3030912173682578,1.2882272781263568,1.2735328870226386,1.2590061100764338,1.2446450353673641]
[null,null,null,null,"Coincident",0.90186058255888568,0.89157335114703262,0.88140346285025473,0.87134957917366407,0.86141037689015032,0.85158454786622595,0.84187079888985772]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4600305113020484,1.4433764163913756,1.4269122893444883,1.4106359632595245,1.3945452959517695,1.3786381696717158,1.3629124908263379]
[null,null,null,null,"Coincident",0.98755630563426477,0.97629157087951013,0.96515532930369718,0.95414611522677284,0.94326247968722132,0.93250299025136152,0.92186623082481856]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kadina 11kV","Substation Rating","MVA","Non-Coincident",16,16,16,16,16,16,16]
[null,null,null,null,"Coincident",16,16,16,16,16,16,16]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.3309100000000003,4.6455170293293735,4.7272881888892071,4.8599164783285689,4.9857805377009665,5.1079997103380439,5.230016107306926]
[null,null,null,null,"Coincident",4.3309100000000003,4.6455170293293735,4.7272881888892071,4.8599164783285689,4.9857805377009665,5.1079997103380439,5.230016107306926]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.2836465621781326,8.2791078575604899,8.3136093406235769,8.3691141355614516,8.428911342621408,8.4901567751876783,8.5545155064443374]
[null,null,null,null,"Coincident",8.2702449386984931,8.2657135769835097,8.3001592421308956,8.3555742391328636,8.4152747038163618,8.4764210510074971,8.5406756600665883]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.681700703322706,8.6769439002921338,8.7131032834244486,8.7712752507618887,8.8339458935388855,8.8981343534151929,8.9655857153512564]
[null,null,null,null,"Coincident",8.6676550915120725,8.6629059842327241,8.6990068672305441,8.7570847215710739,8.8196539732093431,8.8837385863601135,8.9510808227137328]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5453128065667476,7.5678984924441144,7.5905517849561734,7.6132728864725614,7.6360619999686765,7.6589193290274915,7.6818450778413725]
[null,null,null,null,"Coincident",7.5331056897480018,7.5556548355755382,7.5782714786609775,7.6009558210465551,7.6237080653792875,7.6465284149127815,7.6694170735090523]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9078877892559341,7.9315587852955103,7.9553006366719901,7.9791135554794801,8.002997754446957,8.0269534469401691,8.0509808469635402]
[null,null,null,null,"Coincident",7.8950940837452812,7.9187267838756901,7.9424302247103302,7.9662046180001731,7.9900501761300351,8.0139671121204703,8.0379556396296774]
[null,"Kalangadoo 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.19487000000000002,0.20902579446476954,0.21270510109165044,0.21867273255086997,0.22433600637782528,0.22983527793317673,0.23532542556435032]
[null,null,null,null,"Coincident",0.19487000000000002,0.20902579446476954,0.21270510109165044,0.21867273255086997,0.22433600637782528,0.22983527793317673,0.23532542556435032]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.54350764131935092,0.54182491264877108,0.54014739379598131,0.53847506863110761,0.53680792107421493,0.53514593509515263,0.53348909471340022]
[null,null,null,null,"Coincident",0.54350764131935092,0.54182491264877108,0.54014739379598131,0.53847506863110761,0.53680792107421493,0.53514593509515263,0.53348909471340022]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.56055515938048595,0.55881965068397299,0.55708951521502781,0.55536473633785099,0.55364529746814861,0.55193118207297243,0.55022237367056115]
[null,null,null,null,"Coincident",0.56055515938048595,0.55881965068397299,0.55708951521502781,0.55536473633785099,0.55364529746814861,0.55193118207297243,0.55022237367056115]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.48915687718741585,0.48764242138389396,0.4861326544163832,0.48462756176799687,0.48312712896679344,0.48163134158563736,0.4801401852420602]
[null,null,null,null,"Coincident",0.48915687718741585,0.48764242138389396,0.4861326544163832,0.48462756176799687,0.48312712896679344,0.48163134158563736,0.4801401852420602]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.50449964344243736,0.50293768561557561,0.50138056369352502,0.49982826270406594,0.49828076772133378,0.49673806386567521,0.49520013630350501]
[null,null,null,null,"Coincident",0.50449964344243736,0.50293768561557561,0.50138056369352502,0.49982826270406594,0.49828076772133378,0.49673806386567521,0.49520013630350501]
[null,"Kalangadoo West 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.10327,0.110771764737398,0.11272158767247262,0.11588409242329932,0.1188853049655566,0.12179960564560559,0.12470907116554861]
[null,null,null,null,"Coincident",0.10327,0.110771764737398,0.11272158767247262,0.11588409242329932,0.1188853049655566,0.12179960564560559,0.12470907116554861]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.79471558829945177,0.79331094426302218,0.77763562261365826,0.78055233229643184,0.78403823906196102,0.78944555583549103,0.79511466655886098]
[null,null,null,null,"Coincident",0.7490422786270694,0.74771836125940017,0.73294392016459742,0.7356930028541081,0.73897857015035406,0.74407512159207201,0.74941842135432868]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.85436087163181318,0.85285080574036087,0.83599901415021871,0.83913462978876896,0.84288216209651889,0.84869531077491345,0.85478990165787283]
[null,null,null,null,"Coincident",0.80525967211274341,0.80383639161735165,0.78795309379675782,0.79090850163998905,0.79444065852775347,0.79991971820164254,0.80566404524075363]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.72154847766326191,0.72699393068273521,0.73248047998264598,0.73800843571244545,0.7435781103622513,0.74918981878051238,0.75484387819180665]
[null,null,null,null,"Coincident",0.68008017434928136,0.68521267029866995,0.69038390067329847,0.6955941577979371,0.70084373620350116,0.70613293264370125,0.71146204611181774]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.77570239640084526,0.78155654354058191,0.78745487133374004,0.79339771320722041,0.79938540510426259,0.80541828550343575,0.81149669543777214]
[null,null,null,null,"Coincident",0.73112179890654383,0.73663950080836449,0.74219884424559401,0.74780014348266743,0.7534437151557416,0.75912987829059453,0.76485895432065876]
[null,"Kapunda TF1 11kV","Substation Rating","MVA","Non-Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,null,null,"Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.95599000000000001,1.025435260688536,1.0434851418515261,1.0727610488597843,1.1005438432654446,1.127522078058899,1.1544555528571012]
[null,null,null,null,"Coincident",0.95599000000000001,1.025435260688536,1.0434851418515261,1.0727610488597843,1.1005438432654446,1.127522078058899,1.1544555528571012]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.2299798738322769,4.339616733815892,4.3735347247517948,4.4191309499840967,4.4361634727795893,4.4530814497465725,4.4714695003831197]
[null,null,null,null,"Coincident",3.2563810512539413,3.3407832006774498,3.3668944130885414,3.4019959238010866,3.4151081338211413,3.4281321626023762,3.4422879036338578]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.3969628470884849,4.5109277392151821,4.5461846790686415,4.5935808639900308,4.6112857638140863,4.628871595990713,4.6479855345650893]
[null,null,null,null,"Coincident",3.384930171158127,3.4726641855739824,3.4998061659825059,3.5362933463198232,3.549923174834626,3.5634613410620268,3.5781758950894531]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7094911834359934,3.7290853224903433,3.7487829609914627,3.7685846456403547,3.7884909260257866,3.8085023546395442,3.8286194868917645]
[null,null,null,null,"Coincident",2.8556913176493977,2.8707755461883888,2.8859394520892891,2.901183456220954,2.9165079816753368,2.9319134537792317,2.9474003001060796]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8559273097423459,3.8762949483629536,3.8967701721815331,3.9173535494806919,3.9380456515448028,3.9588470526758535,3.9797583302093891]
[null,null,null,null,"Coincident",2.9684227823717144,2.9841024769426601,2.9998649942244735,3.0157107717002578,3.0316402491639738,3.0476538687326449,3.0637520748586295]
[null,"Kapunda TF2 11kV","Substation Rating","MVA","Non-Coincident",17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999]
[null,null,null,null,"Coincident",17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999,17.399999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3353100000000002,1.4323099174154639,1.4575216736218597,1.4984137450736501,1.5372202631311844,1.574902986488173,1.612523189871877]
[null,null,null,null,"Coincident",1.3353100000000002,1.4323099174154639,1.4575216736218597,1.4984137450736501,1.5372202631311844,1.574902986488173,1.612523189871877]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7350259070451375,2.725084249402987,2.7173895861081205,2.7239415828051787,2.7147732936945967,2.7067446507062081,2.6999486915628657]
[null,null,null,null,"Coincident",2.5970475522783518,2.587607437806811,2.5803009598593576,2.5865224171921017,2.5778166558565747,2.5701930470390488,2.5637399348351981]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7919415504593488,2.7817930078148119,2.7739382192680582,2.7806265624277589,2.7712674820444536,2.7630717637167601,2.7561343812741854]
[null,null,null,null,"Coincident",2.6510918785256736,2.6414553161200685,2.6339967910229336,2.640347716323844,2.6314607888770398,2.6236785334449171,2.6170911325558439]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4953884284276402,2.4710172256867331,2.4468840442158903,2.4229865593811741,2.3993224692521755,2.375889494380282,2.3526853775791081]
[null,null,null,null,"Coincident",2.369499460073953,2.3463577515214613,2.3234420563881546,2.3007501673147308,2.2782798985000539,2.2560290854906082,2.2339955849720057]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5473172374405606,2.522438872160095,2.4978034813509393,2.4734086920037335,2.4492521542851033,2.4253315413113157,2.4016445489241391]
[null,null,null,null,"Coincident",2.418808530965145,2.3951852455366991,2.3717926768463862,2.3486285715999564,2.3256906985099475,2.3029768480807613,2.2804848323958296]
[null,"Karoonda 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.39596999999999999,0.42473415012169541,0.43221039092349167,0.44433643920648624,0.45584404190192163,0.46701839689639241,0.47817421235036583]
[null,null,null,null,"Coincident",0.39596999999999999,0.42473415012169541,0.43221039092349167,0.44433643920648624,0.45584404190192163,0.46701839689639241,0.47817421235036583]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.77083262373999106,0.769803284983122,0.76877532076366062,0.76774872924610515,0.7667235085974049,0.76569965698695708,0.76467717258660317]
[null,null,null,null,"Coincident",0.77083262373999106,0.769803284983122,0.76877532076366062,0.76774872924610515,0.7667235085974049,0.76569965698695708,0.76467717258660317]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.78133228918174091,0.78028892959565355,0.77924696326982301,0.77820638834374578,0.77716720295940278,0.77612940526125629,0.77509299339624593]
[null,null,null,null,"Coincident",0.78133228918174091,0.78028892959565355,0.77924696326982301,0.77820638834374578,0.77716720295940278,0.77612940526125629,0.77509299339624593]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.69374936136599197,0.69282295648480985,0.69189778868729457,0.69097385632149466,0.69005115773766446,0.6891296912882614,0.68820945532794287]
[null,null,null,null,"Coincident",0.69374936136599197,0.69282295648480985,0.69189778868729457,0.69097385632149466,0.69005115773766446,0.6891296912882614,0.68820945532794287]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.70319906026356682,0.70226003663608827,0.70132226694284072,0.70038574950937116,0.69945048266346255,0.69851646473513063,0.69758369405662135]
[null,null,null,null,"Coincident",0.70319906026356682,0.70226003663608827,0.70132226694284072,0.70038574950937116,0.69945048266346255,0.69851646473513063,0.69758369405662135]
[null,"Keith 11kV","Substation Rating","MVA","Non-Coincident",16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993]
[null,null,null,null,"Coincident",16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993,16.590415704387993]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2527999999999997,1.3438062057036135,1.3674601049295405,1.4058254186879959,1.4422340472629926,1.4775883214177847,1.5128839387643966]
[null,null,null,null,"Coincident",1.2527999999999997,1.3438062057036135,1.3674601049295405,1.4058254186879959,1.4422340472629926,1.4775883214177847,1.5128839387643966]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2439443791729738,5.2400376388918906,5.2249032276009304,5.223642575655064,5.2237980514730165,5.2084369734801843,5.186620878449208]
[null,null,null,null,"Coincident",5.0880579233890764,5.0842673185686404,5.0695828071175599,5.0683596305050695,5.0685104845016475,5.0536060444576902,5.0324384753239242]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9060008197218954,5.9016008471756267,5.884555692035268,5.8831358807467957,5.8833109856376709,5.8660105467585337,5.8414401345230784]
[null,null,null,null,"Coincident",5.7304334473256917,5.7261642725293971,5.7096258178097505,5.7082482131759704,5.7084181127330647,5.6916319630807699,5.667791954183639]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8355305259950976,4.8151700518138378,4.7948953074003171,4.7747059317809635,4.7546015655021208,4.7345818506236466,4.7146464307125413]
[null,null,null,null,"Coincident",4.6917849671127394,4.6720297476650732,4.6523577095008974,4.6327685023772842,4.6132617775260352,4.593837187647476,4.5744943869042718]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4460240584819664,5.4230930415775846,5.4002585779624717,5.3775202610895576,5.3548776861235812,5.3323304499338802,5.3098781510872133]
[null,null,null,null,"Coincident",5.2841303908141031,5.2618810430301926,5.2397253783010509,5.2176630021650157,5.1956935218213403,5.1738165461232066,5.1520316855707575]
[null,"Kent Town 11kV","Substation Rating","MVA","Non-Coincident",59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955]
[null,null,null,null,"Coincident",59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955,59.182192121630955]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.3499799999999995,4.6659723169592962,4.7481035338772388,4.8813158163987955,5.007734084381446,5.1304914163481303,5.2530450797783788]
[null,null,null,null,"Coincident",4.3499799999999995,4.6659723169592962,4.7481035338772388,4.8813158163987955,5.007734084381446,5.1304914163481303,5.2530450797783788]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.73012254487432,31.81499431730904,31.950553021768762,31.96650017423439,31.977220524645144,31.992958777771328,32.021583988862261]
[null,null,null,null,"Coincident",30.034619813468822,30.11495645302535,30.24327156259028,30.258366577137895,30.26851408439693,30.283411362165229,30.310506981823821]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.596782991918182,33.686647710108168,33.830181236332592,33.847066548388007,33.858417569356739,33.875081692673774,33.905390904488499]
[null,null,null,null,"Coincident",31.801535045785155,31.886597832468798,32.022461628284283,32.038444671756587,32.049189149620119,32.0649628235996,32.093652459210489]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.716657837570235,28.886851109339965,29.058053055236034,29.23026965330612,29.403506917027631,29.577770895517691,29.753067673744358]
[null,null,null,null,"Coincident",27.182179937852741,27.343278912657677,27.505332662971515,27.668346847404266,27.83232715810249,27.997279320948046,28.16320909575802]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.406038308158543,30.586243928551141,30.767517562648514,30.949865540182618,31.133294228399436,31.317810032281351,31.503419394770713]
[null,null,null,null,"Coincident",28.781288169554653,28.951864481987343,29.1234517386902,29.296055931165228,29.469683086423899,29.644339267197612,29.820030572149381]
[null,"Kersbrook 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.34558,0.37068370734918177,0.37720854331222126,0.38779146566905959,0.3978346440398669,0.4075869828508607,0.41732314140980242]
[null,null,null,null,"Coincident",0.34558,0.37068370734918177,0.37720854331222126,0.38779146566905959,0.3978346440398669,0.4075869828508607,0.41732314140980242]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.49185087150657719,0.49568926209835279,0.49195360789333004,0.49560776698807263,0.49925554094114349,0.50284922736269033,0.50707719618332459]
[null,null,null,null,"Coincident",0.41403268088281847,0.41726378046818741,0.41411916283109929,0.41719517910760673,0.42026582046769684,0.4232909317556115,0.4268499724464091]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.50790863115313223,0.5118723360568731,0.50801472163825312,0.51178818032531714,0.51555504541103947,0.51926605713613927,0.52363205907015797]
[null,null,null,null,"Coincident",0.42754986192403621,0.43088644921623187,0.42763916730197776,0.43081560818459752,0.43398649867257888,0.43711037263995495,0.44078560753370288]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.43568074886412106,0.43982798908365095,0.44401470683686423,0.44824127790996648,0.45250808166626799,0.45681550108023422,0.46116392277186036]
[null,null,null,null,"Coincident",0.36674951476391526,0.37024059933005099,0.37376491549147794,0.37732277957938354,0.3809145109361079,0.38454043194380766,0.38820086805339155]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.44990468777158238,0.45418732550792013,0.45851072962540296,0.46287528817876133,0.46728139291661402,0.47172943931663092,0.47621982662102941]
[null,null,null,null,"Coincident",0.37872301303287359,0.38232807319632217,0.38596744988750953,0.38964146976508302,0.39335046259714973,0.39709476129087595,0.40087470192236752]
[null,"Keswick 11kV","Substation Rating","MVA","Non-Coincident",49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865]
[null,null,null,null,"Coincident",49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865,49.069085348901865]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.8595699999999997,4.139937833131782,4.2128097040093451,4.3310038403620927,4.443169908840062,4.5520877695517559,4.6608249230019982]
[null,null,null,null,"Coincident",3.8595699999999997,4.139937833131782,4.2128097040093451,4.3310038403620927,4.443169908840062,4.5520877695517559,4.6608249230019982]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.191151278011155,35.236005863055723,35.194533641863863,34.976005067374189,34.763498510570365,34.552338191289991,34.313135848578149]
[null,null,null,null,"Coincident",26.556683742873041,26.590532849429287,26.559236213135524,26.394325602634147,26.233959453264877,26.07460922985582,25.894097347315565]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.567650128453025,37.615533795125337,37.571260907220157,37.337974847192129,37.111117478618432,36.885697260533831,36.630341308979048]
[null,null,null,null,"Coincident",28.35008708702339,28.386222062609153,28.35281192853331,28.176764715163046,28.005568855602849,27.835457528649396,27.642755471426902]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.20226544433347,32.071652176842129,31.941568680328366,31.812012806026644,31.682982413886865,31.554475372539045,31.426489559258084]
[null,null,null,null,"Coincident",24.301148105477502,24.20258198554615,24.104415652487255,24.00664748475436,23.909275867378032,23.812299191939207,23.715715856542598]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.376921402744827,34.237487671336481,34.098619486948081,33.960314555705494,33.822570593038563,33.685385323643473,33.548756481445032]
[null,null,null,null,"Coincident",25.94223253834658,25.837010135167805,25.732214516927996,25.627843952575809,25.523896718081062,25.42037109640631,25.317265377478439]
[null,"Ki Ki 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4500000000000001E-2,1.5553312566014051E-2,1.5827084547795616E-2,1.6271127531111072E-2,1.6692523695173534E-2,1.710171668307622E-2,1.7510230772736082E-2]
[null,null,null,null,"Coincident",1.4500000000000001E-2,1.5553312566014051E-2,1.5827084547795616E-2,1.6271127531111072E-2,1.6692523695173534E-2,1.710171668307622E-2,1.7510230772736082E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.10598948576424877,0.10584795168517927,0.10570660660500333,0.10556545027133946,0.10542448243214318,0.10528370283570659,0.10514311123065793]
[null,null,null,null,"Coincident",0.10598948576424877,0.10584795168517927,0.10570660660500333,0.10556545027133946,0.10542448243214318,0.10528370283570659,0.10514311123065793]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10743318976248938,0.10728972781940235,0.10714645744960066,0.10700337839726504,0.10686049040691789,0.10671779322342273,0.10657528659198381]
[null,null,null,null,"Coincident",0.10743318976248938,0.10728972781940235,0.10714645744960066,0.10700337839726504,0.10686049040691789,0.10671779322342273,0.10657528659198381]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.5390537187823893E-2,9.526315651666134E-2,9.5135945944503003E-2,9.5008905244205508E-2,9.4882034188928863E-2,9.4755332552135932E-2,9.4628800107592143E-2]
[null,null,null,null,"Coincident",9.5390537187823893E-2,9.526315651666134E-2,9.5135945944503003E-2,9.5008905244205508E-2,9.4882034188928863E-2,9.4755332552135932E-2,9.4628800107592143E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.6689870786240431E-2,9.6560755037462115E-2,9.6431811704640602E-2,9.6303040557538536E-2,9.6174441366226104E-2,9.6046013901080446E-2,9.5917757932785438E-2]
[null,null,null,null,"Coincident",9.6689870786240431E-2,9.6560755037462115E-2,9.6431811704640602E-2,9.6303040557538536E-2,9.6174441366226104E-2,9.6046013901080446E-2,9.5917757932785438E-2]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kilburn - Bus A 11kV","Substation Rating","MVA","Non-Coincident",21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999]
[null,null,null,null,"Coincident",21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999,21.716999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.86921999999999999,0.93236209300901607,0.9487736848713727,0.97539237742016316,1.0006534790564647,1.0251830465698972,1.0496719167088038]
[null,null,null,null,"Coincident",0.86921999999999999,0.93236209300901607,0.9487736848713727,0.97539237742016316,1.0006534790564647,1.0251830465698972,1.0496719167088038]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5850000000000009,9.5850000000000009,9.5850000000000009,9.5850000000000009,9.5850000000000009,9.5850000000000009,9.5850000000000009]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.65,10.65,10.65,10.65,10.65,10.65,10.65]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10,10,10,10,10,10,10]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kilburn 11kV","Substation Rating","MVA","Non-Coincident",76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702]
[null,null,null,null,"Coincident",76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702,76.170675340973702]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.0874100000000002,5.3262148456993277,5.3882838629840544,5.4889563694517136,5.5844944359138227,5.6772658235249382,5.7698832927310573]
[null,null,null,null,"Coincident",5.0874100000000002,5.3262148456993277,5.3882838629840544,5.4889563694517136,5.5844944359138227,5.6772658235249382,5.7698832927310573]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.605881515930022,42.190706772429394,42.673119194121966,42.799891815032971,42.932455813282679,43.065542143461599,43.21310247498824]
[null,null,null,null,"Coincident",17.646925362088268,17.894976052886804,18.099588854951666,18.153358824428608,18.209585177472395,18.266033074976558,18.328620047346284]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.314601009543821,45.951557184800592,46.476971516009435,46.615044560641763,46.759425221982042,46.904374775558331,47.065088532948756]
[null,null,null,null,"Coincident",19.219960079972232,19.490121837736545,19.712973683417641,19.771536670773408,19.832775002027738,19.89425462606237,19.962420557848805]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.804117689833056,40.186881041625391,40.573325112699507,40.963485297495254,41.357397330811601,41.755097291079586,42.15662160366675]
[null,null,null,null,"Coincident",16.882716298351212,17.045063448665424,17.208971757548518,17.374456237374115,17.541532044877449,17.710214482543563,17.880519000008878]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.352229202525322,43.769111814684479,44.19000324289572,44.614942036634773,45.043967116075855,45.477117775656403,45.914433687676009]
[null,null,null,null,"Coincident",18.387629949005948,18.564448611980513,18.742967594118713,18.923203245986773,19.105172075380814,19.28889074883881,19.474376093167084]
[null,"Kilburn South 11kV","Substation Rating","MVA","Non-Coincident",36.195,36.195,36.195,36.195,36.195,36.195,36.195]
[null,null,null,null,"Coincident",36.195,36.195,36.195,36.195,36.195,36.195,36.195]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.0881899999999995,3.3125230574647535,3.3708306365280643,3.4654022986415098,3.5551506724274446,3.6423000305868372,3.7293047979348843]
[null,null,null,null,"Coincident",3.0881899999999995,3.3125230574647535,3.3708306365280643,3.4654022986415098,3.5551506724274446,3.6423000305868372,3.7293047979348843]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.443387340727993,14.347515575160207,14.31695074335634,14.302650648249418,14.288937933870788,14.279290074857752,14.276058997850962]
[null,null,null,null,"Coincident",13.988727270705077,13.895873430407727,13.86627074191833,13.852420796218141,13.839139741223319,13.829795584946417,13.826666218270002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.931175616169238,14.832066028192719,14.800468947772718,14.785685903717166,14.771510077663928,14.761536387016065,14.758196188690032]
[null,null,null,null,"Coincident",14.461160571150733,14.365170831111982,14.334568387923357,14.320250695913478,14.306521107429997,14.296861376297404,14.293626323306672]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.391670937885246,13.406973647086643,13.422293842747347,13.437631544849197,13.452986773396862,13.468359548417874,13.483749889962651]
[null,null,null,null,"Coincident",12.970117606751231,12.984938605487283,12.99977654023041,13.014631430333447,13.029503295171338,13.044392154141176,13.059298026662216]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.843940195640846,13.859759714504328,13.875597310387326,13.891453003946511,13.907326815862161,13.923218766838186,13.939128877602155]
[null,null,null,null,"Coincident",13.408149984504275,13.423471524369857,13.438810572212615,13.454167148038971,13.469541271878214,13.484932963782519,13.500342243826978]
[null,"Kilkenny 11kV","Substation Rating","MVA","Non-Coincident",55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844]
[null,null,null,null,"Coincident",55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844,55.90518027351844]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.6591100000000001,3.9249159685122534,3.9940029889437527,4.1060583076112991,4.2123986467756165,4.3156594849800713,4.4187490015742297]
[null,null,null,null,"Coincident",3.6591100000000001,3.9249159685122534,3.9940029889437527,4.1060583076112991,4.2123986467756165,4.3156594849800713,4.4187490015742297]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.337622348123141,20.313045503817118,20.301701328537384,20.201235027281992,20.106654254302143,20.013918688702471,19.927831792624438]
[null,null,null,null,"Coincident",19.473081457723591,19.44954936124973,19.438687420482434,19.342491885202325,19.251931687700129,19.163138258849923,19.080710868318459]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.840489499603546,20.815304969331237,20.803680298474823,20.700729871894097,20.60381049890098,20.508781957804182,20.420566480937818]
[null,null,null,null,"Coincident",19.954572009351175,19.93045805929976,19.919327546665031,19.820753484830369,19.7279540998865,19.636965168638238,19.552499682090875]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.319720124730054,19.259029431502206,19.198529391152388,19.138219404766364,19.078098875311326,19.018167207629975,18.958423808434627]
[null,null,null,null,"Coincident",18.498449685491828,18.440338919507393,18.382410701854347,18.324664459077958,18.267099619524945,18.209715613337821,18.152511872449214]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.797418670814928,19.735227342188189,19.673231380514117,19.611430172069749,19.549823105060074,19.488409569611953,19.427188957768102]
[null,null,null,null,"Coincident",18.955841534987218,18.896293924770909,18.836933376567963,18.777759302744435,18.718771117512368,18.659968236924001,18.601350078865959]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kingscote 11kV","Substation Rating","MVA","Non-Coincident",8,8,8,8,8,8,8]
[null,null,null,null,"Coincident",8,8,8,8,8,8,8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.5164699999999998,1.6266297866885051,1.6552619933928008,1.7017018460071724,1.7457732005530899,1.7885682964403165,1.8312923903400744]
[null,null,null,null,"Coincident",1.5164699999999998,1.6266297866885051,1.6552619933928008,1.7017018460071724,1.7457732005530899,1.7885682964403165,1.8312923903400744]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2390793697893776,3.2439012478704279,3.209386559445301,3.2076242460543964,3.2064237417323356,3.2059182109891622,3.2029518351663673]
[null,null,null,null,"Coincident",3.2390793697893776,3.2439012478704279,3.209386559445301,3.2076242460543964,3.2064237417323356,3.2059182109891622,3.2029518351663673]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.357012462583794,3.3620099025854566,3.3262385533971588,3.324412075147992,3.323167861125905,3.3226439242872834,3.3195695443573845]
[null,null,null,null,"Coincident",3.357012462583794,3.3620099025854566,3.3262385533971588,3.324412075147992,3.323167861125905,3.3226439242872834,3.3195695443573845]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.8560322058026024,2.8322638752019715,2.8086933482319836,2.7853189787410026,2.7621391342769157,2.7391521959731215,2.716356558435471]
[null,null,null,null,"Coincident",2.8560322058026024,2.8322638752019715,2.8086933482319836,2.7853189787410026,2.7621391342769157,2.7391521959731215,2.716356558435471]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.96001876269042,2.9353850402860453,2.9109563234333726,2.8867309060452944,2.8627070962330161,2.8388832161878974,2.815257602064273]
[null,null,null,null,"Coincident",2.96001876269042,2.9353850402860453,2.9109563234333726,2.8867309060452944,2.8627070962330161,2.8388832161878974,2.815257602064273]
[null,"Kingston SE 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.78833,1.9182383076675797,1.9520034558178847,2.0067686550146111,2.0587407517096334,2.1092077928169446,2.1595911032970423]
[null,null,null,null,"Coincident",1.78833,1.9182383076675797,1.9520034558178847,2.0067686550146111,2.0587407517096334,2.1092077928169446,2.1595911032970423]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2849950654772515,3.255023337119046,3.1764196613446876,3.1668320042512463,3.141427902560824,3.1164352741680839,3.0918194029405051]
[null,null,null,null,"Coincident",3.1616200058659243,3.1327739302710089,3.0571223847102531,3.0478948127133978,3.0234448167363648,2.9993908402917517,2.9756994710861102]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2857125406485266,3.2557342661706135,3.1771134225818094,3.1675236714499362,3.1421140212543115,3.1171159342261765,3.092494686650666]
[null,null,null,null,"Coincident",3.1623105347130007,3.1334581588519916,3.05779009025101,3.048560502861843,3.0241051667656618,3.0000459366964543,2.9763493930631988]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9429226360855658,2.8840471668281102,2.8263495473849116,2.769806213949134,2.714394074126329,2.6600904975034614,2.6068733064066101]
[null,null,null,null,"Coincident",2.8323948427642596,2.7757305684658529,2.720199907296974,2.6657801804402674,2.6124491627858561,2.5601850738545724,2.5089665689027694]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9435653992801183,2.884677071042193,2.8269668498724871,2.7704111668175981,2.7149869244394722,2.6606714873823689,2.6074426731285461]
[null,null,null,null,"Coincident",2.8330134656036932,2.7763368152715033,2.7207940256610779,2.6663624130017842,2.6130197473295635,2.5607442434081782,2.5095145518320785]
[null,"Kingswood 11kV","Substation Rating","MVA","Non-Coincident",71.2,71.2,71.2,71.2,71.2,71.2,71.2]
[null,null,null,null,"Coincident",71.2,71.2,71.2,71.2,71.2,71.2,71.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.891919999999999,13.828418023175713,14.07182812575291,14.466625823509062,14.841288281122866,15.205100920060962,15.56830995197598]
[null,null,null,null,"Coincident",12.891919999999999,13.828418023175713,14.07182812575291,14.466625823509062,14.841288281122866,15.205100920060962,15.56830995197598]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.451766677302281,47.735316617995622,48.027564950048934,48.133534517433965,48.253153172791187,48.378034192787581,48.464601466539925]
[null,null,null,null,"Coincident",44.967751502548509,45.236458110636924,45.513407764844288,45.613830014776703,45.727186847321057,45.845530569121173,45.927566200814745]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",49.814076559013202,50.111742577436878,50.418540022643718,50.529785114497564,50.655358792214834,50.786456812930759,50.877333699170421]
[null,null,null,null,"Coincident",47.206398684121282,47.488482418500588,47.779219565791607,47.88464117591586,48.003641296043163,48.127876569686819,48.213996213356594]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.895631771867357,41.959630207877169,42.023726405864508,42.087920515167461,42.152212685352247,42.216603066213551,42.281091807774885]
[null,null,null,null,"Coincident",39.702470328902699,39.763118561172149,39.823859437754336,39.88469310016977,39.945619690155127,40.006639349663622,40.067752220865302]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.981338413903622,44.048522909113885,44.115810033224484,44.18319994300807,44.250692795476759,44.318288747882541,44.385987957717596]
[null,null,null,null,"Coincident",41.678993956023291,41.742661462988515,41.806426226414573,41.870288394867345,41.934248117139639,41.998305542251593,42.062460819450955]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Kongorong 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.21123,0.22657422160821711,0.23056241855385295,0.23703105299286839,0.24316977794010383,0.24913073206663378,0.25508179628448568]
[null,null,null,null,"Coincident",0.21123,0.22657422160821711,0.23056241855385295,0.23703105299286839,0.24316977794010383,0.24913073206663378,0.25508179628448568]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.90276743604106824,0.89671907253096483,0.87816478384936314,0.87612172171105462,0.87417430542830243,0.8721937100692555,0.87053333645634701]
[null,null,null,null,"Coincident",0.72424771777512476,0.71939540111683153,0.70451017077276812,0.70287111841900618,0.70130879822220504,0.69971986001801345,0.69838782061141225]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.951481399931141,0.94510666248478081,0.9255511713752258,0.92339786417129199,0.92134536394034938,0.9192578942668892,0.91750792572953599]
[null,null,null,null,"Coincident",0.76332863248543348,0.75821448141770265,0.74252603360640757,0.74079853683829544,0.73915191274814007,0.73747723432425027,0.73607331713721214]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.82329543887130763,0.82761340618595725,0.83195402009968911,0.83631739938793914,0.84070366344908909,0.84511293230773354,0.84954532661796467]
[null,null,null,null,"Coincident",0.66049108425094882,0.6639551856886089,0.667437455424156,0.67093798874551802,0.67445688144038307,0.67799422979881996,0.68155013061591407]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.86772103806650724,0.8722720059253134,0.87684684240956856,0.8814456727039145,0.88606862264955344,0.89071581874769112,0.89538738816299912]
[null,null,null,null,"Coincident",0.69613164630867463,0.69978267308901854,0.70345284854134338,0.70714227309538058,0.71085104770758911,0.71457927386391729,0.71832705358258131]
[null,"Kumorna 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.59359432743070617,0.59594076417903141,0.59829647622727022,0.60066150024003262,0.60303587302686135,0.60541963154280476,0.6078128128889918]
[null,null,null,null,"Coincident",0.59359432743070617,0.59594076417903141,0.59829647622727022,0.60066150024003262,0.60303587302686135,0.60541963154280476,0.6078128128889918]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.64240895199756087,0.64494834953349189,0.64749778512979783,0.65005729846622728,0.65262692937938016,0.65520671786332796,0.6577967040702356]
[null,null,null,null,"Coincident",0.64240895199756087,0.64494834953349189,0.64749778512979783,0.65005729846622728,0.65262692937938016,0.65520671786332796,0.6577967040702356]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.53423489468763552,0.53634668776112826,0.5384668286045432,0.54059535021602934,0.5427322857241752,0.54487766838852425,0.54703153160009266]
[null,null,null,null,"Coincident",0.53423489468763552,0.53634668776112826,0.5384668286045432,0.54059535021602934,0.5427322857241752,0.54487766838852425,0.54703153160009266]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.5781680567978047,0.58045351458014272,0.58274800661681803,0.5850515686196045,0.5873642364414422,0.58968604607699515,0.59201703366321212]
[null,null,null,null,"Coincident",0.5781680567978047,0.58045351458014272,0.58274800661681803,0.5850515686196045,0.5873642364414422,0.58968604607699515,0.59201703366321212]
[null,"Kybunga 11kV","Substation Rating","MVA","Non-Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.5160000000000002E-2,2.698767890764921E-2,2.7462720498106045E-2,2.8233211633293415E-2,2.8964406632452835E-2,2.967442701697915E-2,3.0383269396002742E-2]
[null,null,null,null,"Coincident",2.5160000000000002E-2,2.698767890764921E-2,2.7462720498106045E-2,2.8233211633293415E-2,2.8964406632452835E-2,2.967442701697915E-2,3.0383269396002742E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9389344906693985E-2,4.8285778464866543E-2,4.6123810747279087E-2,4.5944757355389741E-2,4.5771981100465535E-2,4.5527759254978373E-2,4.5063846370149756E-2]
[null,null,null,null,"Coincident",1.6463114968897991E-2,1.6095259488288844E-2,1.5374603582426359E-2,1.5314919118463244E-2,1.5257327033488508E-2,1.5175919751659455E-2,1.5021282123383248E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.0909371457590231E-2,4.977184120645483E-2,4.7543335891757681E-2,4.7358771879911457E-2,4.7180678192748675E-2,4.6928940076491961E-2,4.6450749620183612E-2]
[null,null,null,null,"Coincident",1.6969790485863407E-2,1.6590613735484941E-2,1.5847778630585889E-2,1.5786257293303817E-2,1.5726892730916219E-2,1.5642980025497317E-2,1.5483583206727868E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2657866075219035E-2,4.1896108659675399E-2,4.1147954230251901E-2,4.0413159873354774E-2,3.9691487013188843E-2,3.8982701334295849E-2,3.8286572705476009E-2]
[null,null,null,null,"Coincident",1.4219288691739676E-2,1.3965369553225131E-2,1.3715984743417297E-2,1.3471053291118255E-2,1.3230495671062945E-2,1.2994233778098614E-2,1.2762190901825333E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3970721897895089E-2,4.3185520326549098E-2,4.2414340392352409E-2,4.1656931705703747E-2,4.0913048348302311E-2,4.0182448793302072E-2,3.946489582689193E-2]
[null,null,null,null,"Coincident",1.4656907299298361E-2,1.4395173442183032E-2,1.4138113464117466E-2,1.3885643901901244E-2,1.3637682782767434E-2,1.3394149597767356E-2,1.3154965275630639E-2]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Lameroo 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.58079000000000003,0.62297989001484833,0.63394568513891136,0.65173159715820683,0.66861040254619564,0.68500041602509221,0.70136323658602673]
[null,null,null,null,"Coincident",0.58079000000000003,0.62297989001484833,0.63394568513891136,0.65173159715820683,0.66861040254619564,0.68500041602509221,0.70136323658602673]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3104154603579852,1.3086655844713078,1.3069180452982234,1.3051728397183791,1.3034299646155887,1.3016894168778272,1.2999511933972256]
[null,null,null,null,"Coincident",1.3104154603579852,1.3086655844713078,1.3069180452982234,1.3051728397183791,1.3034299646155887,1.3016894168778272,1.2999511933972256]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3282648916089599,1.3264911803126114,1.3247198375586995,1.322950860184368,1.321184245030985,1.3194199889441358,1.3176580887736185]
[null,null,null,null,"Coincident",1.3282648916089599,1.3264911803126114,1.3247198375586995,1.322950860184368,1.321184245030985,1.3194199889441358,1.3176580887736185]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1793739143221866,1.1777990260241771,1.1762262407684012,1.1746555557465412,1.1730869681540299,1.1715204751900445,1.169956074057503]
[null,null,null,null,"Coincident",1.1793739143221866,1.1777990260241771,1.1762262407684012,1.1746555557465412,1.1730869681540299,1.1715204751900445,1.169956074057503]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.195438402448064,1.1938420622813504,1.1922478538028296,1.1906557741659314,1.1890658205278866,1.1874779900497223,1.1858922798962566]
[null,null,null,null,"Coincident",1.195438402448064,1.1938420622813504,1.1922478538028296,1.1906557741659314,1.1890658205278866,1.1874779900497223,1.1858922798962566]
[null,"Langhorne Creek 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0883399999999999,1.1673994619376364,1.1879482204653706,1.221277168083408,1.2529062923038039,1.2836194713695976,1.314281693737902]
[null,null,null,null,"Coincident",1.0883399999999999,1.1673994619376364,1.1879482204653706,1.221277168083408,1.2529062923038039,1.2836194713695976,1.314281693737902]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7078106058209639,3.820802737518465,3.8967375845539154,3.9497650419602519,4.0052800852772261,4.0630294259129371,4.1241616977920135]
[null,null,null,null,"Coincident",3.3610631378765694,3.4634884581241439,3.5323220212113391,3.5803904506246305,3.6307138315970491,3.6830625626089959,3.7384778595027588]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.0626544572201624,4.1864601302367381,4.2696620727206902,4.3277643489935649,4.388592277426695,4.4518683292743457,4.5188510647030702]
[null,null,null,null,"Coincident",3.6827226602824954,3.7949502598213547,3.8703713132709336,3.9230399740436548,3.9781793891176123,4.0355379837129304,4.0962566198186101]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.4314141221921983,3.4610767038941774,3.4909957013833202,3.5211733312251492,3.5516118291461081,3.5823134501991967,3.6132804689310385]
[null,null,null,null,"Coincident",3.1105147330834781,3.1374033259841663,3.1645243551503022,3.1918798298583742,3.2194717767538967,3.2473022400015585,3.2753732814366647]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.759806354781619,3.7923076965640217,3.8250899935653839,3.8581556744803613,3.8915071889982649,3.9251470079845419,3.9590776236638399]
[null,null,null,null,"Coincident",3.4081963422758403,3.4376582197581644,3.4673747780562665,3.4973482187378506,3.5275807624018913,3.5580746488431547,3.5888321372181293]
[null,"Largs North 7.6kV","Substation Rating","MVA","Non-Coincident",27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754]
[null,null,null,null,"Coincident",27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754,27.498694942903754]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.7307999999999995,6.1470981829871247,6.2553004225177302,6.4307984589856071,6.5973458477448599,6.7590702046464264,6.9205262422342004]
[null,null,null,null,"Coincident",5.7307999999999995,6.1470981829871247,6.2553004225177302,6.4307984589856071,6.5973458477448599,6.7590702046464264,6.9205262422342004]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.589345470645002,15.7152000300648,15.730195049745854,15.807448383992501,15.887286024366272,15.967516235287414,16.053178250432818]
[null,null,null,null,"Coincident",15.425065803919415,15.549594114901373,15.564431117888244,15.640870360739754,15.719866676442296,15.799251425805334,15.884010739337919]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.122725012899217,16.252885606040593,16.268393670784935,16.34829017873863,16.430859413210268,16.513834649780925,16.602427536303377]
[null,null,null,null,"Coincident",15.952824621839516,16.081613589796092,16.096958231405541,16.176012794344679,16.257711918756449,16.339812766839408,16.42747206638737]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.350422049446426,14.506523879771636,14.664323763390815,14.82384017148385,14.985091776157475,15.148097452630919,15.312876281445336]
[null,null,null,null,"Coincident",14.199198089717408,14.353654927524531,14.509791924633234,14.667627357575123,14.827179701691296,14.98846763329496,15.151510031857571]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.841412614656592,15.002855369843637,15.16605427613834,15.33102843670026,15.497797162490389,15.666379974531582,15.83679660619357]
[null,null,null,null,"Coincident",14.685014623306426,14.844756103602402,15.006235228782076,15.169470900696959,15.334482226810197,15.501288522433176,15.669909312986464]
[null,"LeFevre 11kV","Substation Rating","MVA","Non-Coincident",72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932]
[null,null,null,null,"Coincident",72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932,72.176879293424932]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.154,0.16518690587352852,0.16809455312831204,0.1728105958476624,0.17728611372804992,0.18163202546163706,0.18597072682767973]
[null,null,null,null,"Coincident",0.154,0.16518690587352852,0.16809455312831204,0.1728105958476624,0.17728611372804992,0.18163202546163706,0.18597072682767973]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.8944340554333721,6.9836262779180558,7.0595496355348661,7.0632344895389352,7.0677850725702998,7.0723603667021493,7.0792696475067398]
[null,null,null,null,"Coincident",5.0784025074358707,5.1441010118625003,5.200025742825777,5.2027399861796679,5.2060919208114251,5.2094620575049699,5.2145513960468275]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2306499420663028,7.324191737253015,7.4038175944212092,7.4076821450394057,7.4124546430671696,7.4172530572638102,7.4244992779757286]
[null,null,null,null,"Coincident",5.3260572950497789,5.3949596709963412,5.453611642927382,5.4564582498267695,5.4599736458340491,5.4635081315499194,5.4688456581890836]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4194477319744614,6.4650234063896157,6.5109226510221978,6.5571477630995529,6.6037010561584824,6.6505848601610307,6.6978015216111002]
[null,null,null,null,"Coincident",4.728530173222957,4.7621009663246188,4.7959100994829553,4.8299592648230956,4.8642501664836235,4.8987845207018701,4.9335640558998044]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.7325003035917961,6.7802985340078035,6.828436113956359,6.8769154526920344,6.9257389765742117,6.9749091291885099,7.0244283714690932]
[null,null,null,null,"Coincident",4.9591229893813518,4.9943309051064073,5.0297887838455591,5.0654984002425811,5.1014615415405533,5.1376800076713112,5.1741556113455323]
[null,"Leigh Creek South 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.10871,0.1166069385552681,0.11865947318557664,0.12198857061428169,0.12514787937257343,0.12821569797360108,0.13127842671063028]
[null,null,null,null,"Coincident",0.10871,0.1166069385552681,0.11865947318557664,0.12198857061428169,0.12514787937257343,0.12821569797360108,0.13127842671063028]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Linden Park 11kV","Substation Rating","MVA","Non-Coincident",55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408]
[null,null,null,null,"Coincident",55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408,55.658683823529408]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.111120000000001,11.918256711620003,12.128043838669159,12.468306933343369,12.791216129649419,13.104774225631852,13.41781209265954]
[null,null,null,null,"Coincident",11.111120000000001,11.918256711620003,12.128043838669159,12.468306933343369,12.791216129649419,13.104774225631852,13.41781209265954]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",39.731531814372168,39.601944498654362,39.591358696769831,39.535242924820302,39.440469181190309,39.330802644846841,39.23760071183019]
[null,null,null,null,"Coincident",38.018519388033916,37.894519188442352,37.884389790057583,37.830693431865171,37.74000582821305,37.635067529894421,37.545883968738238]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.370917534243134,41.235983241322018,41.224960652541782,41.166529455261475,41.067845197366594,40.953653646622243,40.856606054727763]
[null,null,null,null,"Coincident",39.587223511161497,39.458106867597387,39.447559514245754,39.391647559553292,39.29721804222185,39.187949824066884,39.095086408398927]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.210778283483066,35.08421632799481,34.958109287999982,34.832455528346024,34.707253419757777,34.582501338816364,34.458197667938151]
[null,null,null,null,"Coincident",33.692676715628863,33.571571438817529,33.450901463962026,33.330665226408875,33.210861167128606,33.091487732695526,32.97254337526762]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.663630576547796,36.531846474994907,36.400536059466802,36.269697627341941,36.13932948211869,36.009429933393378,35.879997296838305]
[null,null,null,null,"Coincident",35.082889741642887,34.956787469942633,34.831138461444041,34.705941086933557,34.581193723053701,34.456894752281976,34.333042562909974]
[null,"Little Swamp 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.17446999999999999,0.18714389264775663,0.19043803041751037,0.19578093933468607,0.20085135235151214,0.20577493170319361,0.21069034227029401]
[null,null,null,null,"Coincident",0.17446999999999999,0.18714389264775663,0.19043803041751037,0.19578093933468607,0.20085135235151214,0.20577493170319361,0.21069034227029401]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.26575635311580176,0.2639807791552935,0.26052344381379783,0.25996155876339533,0.25943709339896837,0.25889751708930753,0.25848402819647204]
[null,null,null,null,"Coincident",0.26160391009836731,0.25985607948099199,0.25645276500420722,0.25589965940771725,0.25538338881460948,0.25485224338478707,0.25444521525590214]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.27397562176886781,0.27214513314978717,0.26858086991113184,0.26800160697257253,0.26746092102986435,0.2669046567931006,0.26647837958399184]
[null,null,null,null,"Coincident",0.26969475267872922,0.26789286544432167,0.26438429381877038,0.26381408186362609,0.2632818441387727,0.26273427153070833,0.26231465490299194]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.23303685277659922,0.23288592506540079,0.23273509510343701,0.23258436282740003,0.23243372817402294,0.23228319108007989,0.23213275148238588]
[null,null,null,null,"Coincident",0.22939565195196482,0.22924708248625389,0.22909860924244579,0.22895023215822188,0.22880195117130381,0.2286537662194536,0.22850567724047358]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.24024417812020538,0.24008858254165033,0.23993308773550215,0.23977769363649487,0.23962240017940514,0.23946720729905149,0.23931211493029475]
[null,null,null,null,"Coincident",0.23649036283707717,0.23633719843943704,0.23618413323963489,0.23603116717342465,0.23587830017660188,0.23572553218500375,0.23557286313450887]
[null,"Lobethal 11kV","Substation Rating","MVA","Non-Coincident",12.8,12.8,12.8,12.8,12.8,12.8,12.8]
[null,null,null,null,"Coincident",12.8,12.8,12.8,12.8,12.8,12.8,12.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.4434,3.6935363096422611,3.7585505470261671,3.8640000372846806,3.9640714546179692,4.061244912172735,4.1582571477820292]
[null,null,null,null,"Coincident",3.4434,3.6935363096422611,3.7585505470261671,3.8640000372846806,3.9640714546179692,4.061244912172735,4.1582571477820292]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.9316256406398047,6.8978828218075314,6.8697661034000674,6.8851389540948666,6.9030241011435178,6.9215455877935277,6.9487426389810958]
[null,null,null,null,"Coincident",6.9316256406398047,6.8978828218075314,6.8697661034000674,6.8851389540948666,6.9030241011435178,6.9215455877935277,6.9487426389810958]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.1747318491625869,7.1398056010488631,7.1107027721440197,7.1266147799774693,7.1451271955073228,7.1642982683625211,7.1924491754476794]
[null,null,null,null,"Coincident",7.1747318491625869,7.1398056010488631,7.1107027721440197,7.1266147799774693,7.1451271955073228,7.1642982683625211,7.1924491754476794]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3389015143485272,6.3079548522150786,6.2771592723937681,6.2465140372972936,6.2160184129392695,6.1856716689166511,6.1554730783922356]
[null,null,null,null,"Coincident",6.3389015143485272,6.3079548522150786,6.2771592723937681,6.2465140372972936,6.2160184129392695,6.1856716689166511,6.1554730783922356]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5612196823000142,6.5291876577872712,6.4973120143506202,6.4655919885340714,6.4340268206088425,6.4026157545551703,6.3713580380441925]
[null,null,null,null,"Coincident",6.5612196823000142,6.5291876577872721,6.4973120143506202,6.4655919885340714,6.4340268206088425,6.4026157545551703,6.3713580380441925]
[null,"Lock 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.2311,0.24788762303488601,0.25225098199969426,0.25932810844412196,0.26604429144514508,0.272565981066132,0.27907685045374536]
[null,null,null,null,"Coincident",0.2311,0.24788762303488601,0.25225098199969426,0.25932810844412196,0.26604429144514508,0.272565981066132,0.27907685045374536]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.81031670901881181,0.79507887100746077,0.78012757738631655,0.76545743974742408,0.75106317101072462,0.73693958351860578,0.7230815871662829]
[null,null,null,null,"Coincident",0.81031670901881181,0.79507887100746077,0.78012757738631655,0.76545743974742408,0.75106317101072462,0.73693958351860578,0.7230815871662829]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.82958088311689249,0.81398078629850723,0.7986740460722227,0.78365514592803687,0.76891867309277684,0.75445931657934895,0.74027186527267252]
[null,null,null,null,"Coincident",0.82958088311689249,0.81398078629850723,0.7986740460722227,0.78365514592803687,0.76891867309277684,0.75445931657934895,0.74027186527267252]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.72928503811693068,0.7155709839067147,0.70211481964768496,0.68891169577268174,0.67595685390965221,0.66324562516674523,0.65077342844965458]
[null,null,null,null,"Coincident",0.72928503811693068,0.7155709839067147,0.70211481964768496,0.68891169577268174,0.67595685390965221,0.66324562516674523,0.65077342844965458]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74662279480520333,0.73258270766865652,0.71880664146500051,0.70528963133523326,0.69202680578349929,0.67901338492141405,0.66624467874540527]
[null,null,null,null,"Coincident",0.74662279480520333,0.73258270766865652,0.71880664146500051,0.70528963133523326,0.69202680578349929,0.67901338492141405,0.66624467874540527]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Loveday 11kV","Substation Rating","MVA","Non-Coincident",20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973]
[null,null,null,null,"Coincident",20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973,20.362170439600973]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.0068799999999998,5.3705910083120294,5.4651250400459928,5.6184540008944408,5.7639629681993414,5.9052581535283206,6.0463189138894355]
[null,null,null,null,"Coincident",5.0068799999999998,5.3705910083120294,5.4651250400459928,5.6184540008944408,5.7639629681993414,5.9052581535283206,6.0463189138894355]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.942499025875401,11.699005443696667,11.687275472288318,11.6330687005751,11.587337607243484,11.547670479860821,11.533289214250548]
[null,null,null,null,"Coincident",11.942499025875401,11.699005443696667,11.687275472288318,11.6330687005751,11.587337607243484,11.547670479860821,11.533289214250548]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.944578815738508,11.70104282907786,11.689310814891398,11.635094603052284,11.589355545636757,11.549681510211713,11.535297740099628]
[null,null,null,null,"Coincident",11.944578815738508,11.70104282907786,11.689310814891398,11.635094603052284,11.589355545636757,11.549681510211713,11.535297740099628]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.301303461127796,11.259460455285847,11.217772372913027,11.176238640406156,11.134858686285813,11.093631941188479,11.052557837858696]
[null,null,null,null,"Coincident",11.301303461127796,11.259460455285847,11.217772372913027,11.176238640406156,11.134858686285813,11.093631941188479,11.052557837858696]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.303271586586916,11.261421293772685,11.21972595140755,11.178184985788445,11.136797825336416,11.095563900588797,11.054482644191339]
[null,null,null,null,"Coincident",11.303271586586916,11.261421293772685,11.21972595140755,11.178184985788445,11.136797825336417,11.095563900588797,11.054482644191339]
[null,"Lower Mitcham 11kV","Substation Rating","MVA","Non-Coincident",28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622]
[null,null,null,null,"Coincident",28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622,28.217087509637622]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.21713,6.6687562864512371,6.7861408382507964,6.9765320763790735,7.1572130924809807,7.3326617821968032,7.5078193823517694]
[null,null,null,null,"Coincident",6.21713,6.6687562864512371,6.7861408382507964,6.9765320763790735,7.1572130924809807,7.3326617821968032,7.5078193823517694]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.776881320138703,18.810666665481673,18.735509423372601,18.732961750171789,18.734173582465548,18.736483740634597,18.723802396670813]
[null,null,null,null,"Coincident",18.294640076083397,18.327557722116175,18.254330721846337,18.251848479803812,18.253029188957207,18.255280015998238,18.242924363345228]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.298571861348943,19.333295887338419,19.256050501748902,19.253432044854659,19.254677546288377,19.257051889113278,19.244018210963482]
[null,null,null,null,"Coincident",18.802932189124668,18.836764407938805,18.761502893377131,18.758951685558419,18.760165199136935,18.762478562397757,18.749779624456327]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.404678754952727,16.361181752543157,16.317800082426704,16.274533438799814,16.231381516669771,16.188344011852553,16.145420620970675]
[null,null,null,null,"Coincident",15.983362107303083,15.940982225899768,15.898714714743447,15.856559275884431,15.814515612163042,15.772583427207534,15.730762425431973]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.860460819723652,16.815755311261281,16.771168339445584,16.726699589976665,16.682348749387987,16.638115505044187,16.593999545138843]
[null,null,null,null,"Coincident",16.42743845235486,16.383881102612222,16.340439245173638,16.297112573811294,16.253900783109319,16.210803568461682,16.167820626069982]
[null,"Loxton 11kV","Substation Rating","MVA","Non-Coincident",19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857]
[null,null,null,null,"Coincident",19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857,19.905216368996857]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3412299999999995,3.5839444513753875,3.6470296347331814,3.749350306260292,3.8464524790361829,3.9407426781375685,4.0348764389509624]
[null,null,null,null,"Coincident",3.3412299999999995,3.5839444513753875,3.6470296347331814,3.749350306260292,3.8464524790361829,3.9407426781375685,4.0348764389509624]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.154802350230295,12.01872122864903,12.106028449954932,12.082083372707574,12.064956940718588,12.052861849332082,12.066654908411257]
[null,null,null,null,"Coincident",11.949959245419429,11.81617147906087,11.902007324545973,11.87846579018043,11.861627987442818,11.849736732860991,11.863297339534508]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.189207289191897,12.052740981365153,12.140295331298356,12.11628247599115,12.09910756655019,12.086978239240391,12.100810340448104]
[null,null,null,null,"Coincident",11.983784362980842,11.849617901864216,11.935696711154041,11.912088540982371,11.895203077776184,11.88327816424407,11.896877155074849]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.522877566000323,11.545800643568134,11.56876932324203,11.591783695740725,11.614843851963402,11.637949882990075,11.661101880081951]
[null,null,null,null,"Coincident",11.3286841970781,11.351220955375098,11.373802547252563,11.396429061900339,11.419100588685698,11.441817217153698,11.46457903702753]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.555493801780804,11.578481764573549,11.601515458552033,11.624594974691755,11.647720404149196,11.670891838262172,11.694109368550214]
[null,null,null,null,"Coincident",11.360750756211278,11.383351306232012,11.405996816737506,11.428687377170062,11.451423077149911,11.474204006475576,11.497030255124212]
[null,"Lucindale 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.44172,0.47380753287308458,0.48214757147946746,0.49567465193395738,0.50851183218152085,0.52097726160333979,0.53342200944365381]
[null,null,null,null,"Coincident",0.44172,0.47380753287308458,0.48214757147946746,0.49567465193395738,0.50851183218152085,0.52097726160333979,0.53342200944365381]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2952894779962829,1.2946915912717443,1.2703634899195462,1.2691565830865641,1.2613983804358462,1.2536790499699493,1.2460904901518304]
[null,null,null,null,"Coincident",1.2497850273804005,1.2492081448463481,1.2257347071854445,1.2245701998572158,1.2170845484434105,1.2096364036066258,1.2023144353507449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3266573845535696,1.3260450188610273,1.3011277661083931,1.2998916317232665,1.2919455493901035,1.2840392806058984,1.2762669493302614]
[null,null,null,null,"Coincident",1.2800509568282401,1.2794601039827398,1.2554182122336701,1.2542255041382171,1.246558573390288,1.2389300575127171,1.2314307738227441]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1663490378144086,1.1554932330350021,1.1447384687619859,1.1340838045598844,1.1235283087463339,1.1130710583106134,1.1027111388329329]
[null,null,null,null,"Coincident",1.1253743575643926,1.1148999250117135,1.104522983339792,1.0942426251513264,1.0840579514946245,1.0739680717849955,1.0639721037268741]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1945944055510009,1.1834757067423372,1.1724604953287459,1.1615478081003106,1.1507366908122016,1.1400261981012323,1.1294153934031919]
[null,null,null,null,"Coincident",1.1526274452252712,1.1418993542995917,1.1312711151823929,1.1207417985020154,1.1103104835369364,1.0999762581352577,1.0897382186349427]
[null,"Lyndoch 11kV","Substation Rating","MVA","Non-Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,null,null,"Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4995799999999999,1.6085128591547138,1.6368261687022998,1.6827487878002441,1.7263292884695398,1.7686477450763749,1.8108959904951427]
[null,null,null,null,"Coincident",1.4995799999999999,1.6085128591547138,1.6368261687022998,1.6827487878002441,1.7263292884695398,1.7686477450763749,1.8108959904951427]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9304975154807749,2.9315775712216023,2.936006512269536,2.9503159582695329,2.9654367279830893,2.9809748428854657,2.9962381577365207]
[null,null,null,null,"Coincident",2.5970876185099083,2.598044793657468,2.6019698432089302,2.6146512684065319,2.6280517110269295,2.6418220164493946,2.6553487864970364]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0989526671754333,3.1000948082627588,3.1047783401889086,3.1199103427288315,3.1359003066806976,3.1523316062689855,3.1684723093467886]
[null,null,null,null,"Coincident",2.7463772140237372,2.7473894109154986,2.7515400859159191,2.7649504833764493,2.7791212298727141,2.7936831001665259,2.8079874358282919]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6926357150547657,2.713966389173093,2.7354660418338197,2.7571360116607337,2.7789776478820092,2.800992310414212,2.8231813699469721]
[null,null,null,null,"Coincident",2.386287939090451,2.4051917700456151,2.4242453544395528,2.4434498785975363,2.4628065382427389,2.4823165385706787,2.5019810943242629]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8474177462429378,2.8699745814227811,2.8927101086171705,2.9156257433986283,2.9387229125536387,2.9620030541714844,2.9854676177337844]
[null,null,null,null,"Coincident",2.5234600385865553,2.5434505272489316,2.5635993776966544,2.5839078444490835,2.604377191963704,2.6250086947148481,2.6458036372730547]
[null,"Lyndoch South 7.6kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.10668000000000001,0.11442947479602615,0.11644368134888526,0.11971061275992614,0.12281092605524914,0.12582145763797042,0.12882699440244724]
[null,null,null,null,"Coincident",0.10668000000000001,0.11442947479602615,0.11644368134888526,0.11971061275992614,0.12281092605524914,0.12582145763797042,0.12882699440244724]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.50022197833477811,0.50301909424404556,0.5024501047220532,0.50611892411238835,0.50985816127894878,0.51364186759332642,0.51739825584684729]
[null,null,null,null,"Coincident",0.42443076949617536,0.42680407996464476,0.42632130097628756,0.42943423864081437,0.43260692472153234,0.43581734220039819,0.4390045807185371]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.51781290766497201,0.52070838764143246,0.52011938889372733,0.5239172268906328,0.5277879589926312,0.53170472405545488,0.5355932103837634]
[null,null,null,null,"Coincident",0.43935640650361268,0.44181317739273063,0.44131342087952624,0.44453582887690063,0.4478200864179902,0.45114340222887089,0.4544427239619811]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.45644548220747982,0.46298328495026392,0.46961473056250275,0.47634116031852725,0.48316393470413471,0.49008443369176014,0.49710405701958915]
[null,null,null,null,"Coincident",0.38728707581240712,0.39283430238204214,0.39846098350757808,0.40416825723996253,0.40995727793078096,0.4158292164657359,0.42178526050146958]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.47249695648961215,0.47926466921437261,0.48612931787680574,0.49309229091882623,0.5001549966694101,0.50731886362944301,0.51458534076064855]
[null,null,null,null,"Coincident",0.40090650853664073,0.40664881024249799,0.41247336062274426,0.41838133774930719,0.42437393656798439,0.43045236914013357,0.436617864887823]
[null,"Lyrup 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.15147,1.2351153669233241,1.2568560720172564,1.2921182909136872,1.3255820868469979,1.3580768075215017,1.3905176157160286]
[null,null,null,null,"Coincident",1.15147,1.2351153669233241,1.2568560720172564,1.2921182909136872,1.3255820868469979,1.3580768075215017,1.3905176157160286]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.8686229567031343,4.0421065597996533,4.268976936613468,4.4563076151688445,4.644300517783396,4.8328685895251242,4.8300314353151821]
[null,null,null,null,"Coincident",2.8631423144073773,2.9915363839356202,3.1594416522987951,3.2980838509729273,3.4372161573020734,3.5767741425056903,3.5746743834022841]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.1691582628475015,4.3561189993713816,4.6006138795068985,4.8024974063134396,5.0050946022831599,5.2083116495917006,5.2052540900802837]
[null,null,null,null,"Coincident",3.0855665107236336,3.2239349177421537,3.4048839646786178,3.5542966302835901,3.7042374777254725,3.8546370730517268,3.8523741934395415]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6008641216772093,3.8263258737428822,4.0533818684784819,4.2820433787924621,4.5123217573041421,4.7442284369073437,4.7777749313380147]
[null,null,null,null,"Coincident",2.6649757680162867,2.8318385225013545,2.9998811654632234,3.1691120399070298,3.3395395478313965,3.5111721506455749,3.5359996897413821]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8805984905480324,4.1235753164369369,4.3682702342863902,4.614695392744621,4.8628630263630885,5.1127854562039063,5.1489380216026266]
[null,null,null,null,"Coincident",2.8720053279583713,3.0518308729672277,3.2329279664953754,3.4153055996771777,3.5989728272234123,3.7839387678708212,3.8106950428880348]
[null,"MacGillivray 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.92935999999999985,0.99687079767936659,1.0144178824371952,1.042878281538854,1.0698871600928601,1.0961138907988766,1.1222971083413791]
[null,null,null,null,"Coincident",0.92935999999999985,0.99687079767936659,1.0144178824371952,1.042878281538854,1.0698871600928601,1.0961138907988766,1.1222971083413791]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8069575330771164,1.7968651083072473,1.7596242444722601,1.7668436209359097,1.7744755241958263,1.7822613788109494,1.7837663144848022]
[null,null,null,null,"Coincident",1.760072940704148,1.7502423810931045,1.7139677949312551,1.7209998523702517,1.7284337328948129,1.7360175702443261,1.737483457797609]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8206384836595055,1.810469646488124,1.7729468222813818,1.7802208585424131,1.7879105449485504,1.7957553483160824,1.7972716782536116]
[null,null,null,null,"Coincident",1.7733989157104162,1.7634939263478295,1.7269446957565497,1.7340299947513407,1.7415201591399276,1.749161415716016,1.7506384018893877]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7537756527786601,1.7415279422908485,1.7293657652131715,1.717288524212417,1.705295626126923,1.6933864819374467,1.6815605067382338]
[null,null,null,null,"Coincident",1.7082709549155395,1.6963410321472574,1.6844944234790291,1.6727305470764708,1.6610488251685107,1.6494486840190139,1.6379295538986025]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7670539493623123,1.7547135082381329,1.7424592481200258,1.7302905671522115,1.7182068676820452,1.7062075562306649,1.6942920434638404]
[null,null,null,null,"Coincident",1.7212047234672172,1.7091844761169475,1.6972481736596887,1.6853952298558359,1.6736250625598605,1.6619370936917208,1.6503307492084676]
[null,"Maitland 11kV","Substation Rating","MVA","Non-Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,null,null,"Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.3370200000000003,2.5067863815880109,2.5509112503371938,2.6224793422591173,2.6903973604203073,2.7563485463919166,2.8221903117585985]
[null,null,null,null,"Coincident",2.3370200000000003,2.5067863815880109,2.5509112503371938,2.6224793422591173,2.6903973604203073,2.7563485463919166,2.8221903117585985]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2415375809870772,3.0818902989172456,2.9794117899940917,2.9256021386453948,2.8759703427801107,2.8284090741245889,2.7822583900493156]
[null,null,null,null,"Coincident",3.0986598914669861,2.9460494041991305,2.8480878543469696,2.7966499782643308,2.7492058097650096,2.7037409055681336,2.6596244114245526]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3370727440773518,3.1727203093605421,3.0672215358812571,3.0118259970674321,2.9607314442252544,2.9117684415332565,2.8642575964172106]
[null,null,null,null,"Coincident",3.1899841382777994,3.0328758880113176,2.9320271982115602,2.8790733360396672,2.8302308847001743,2.783426030887163,2.7380093277046065]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9261731141384351,2.798199050296283,2.6758218395374787,2.5587967075421632,2.4468895850182437,2.3398766395247503,2.2375438277705602]
[null,null,null,null,"Coincident",2.7971957867934907,2.6748624530380449,2.5578792791170941,2.4460122796615171,2.3390377024830045,2.2367415810333013,2.1389193064363208]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0124138004501657,2.8806680625937444,2.7546841292545974,2.6342100120812573,2.519004743250477,2.4088378934923971,2.3034891111945472]
[null,null,null,null,"Coincident",2.8796352307333541,2.7536964675482904,2.6332655450450289,2.5181015817966848,2.407974231151282,2.3026632205009965,2.2019579107011236]
[null,"Mallala 11kV","Substation Rating","MVA","Non-Coincident",7.8,7.8,7.8,7.8,7.8,7.8,7.8]
[null,null,null,null,"Coincident",7.8,7.8,7.8,7.8,7.8,7.8,7.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8508500000000001,1.9852999008832488,2.0202454782956907,2.0769252683418569,2.130714309049099,2.182945677439422,2.2350903879805912]
[null,null,null,null,"Coincident",1.8508500000000001,1.9852999008832488,2.0202454782956907,2.0769252683418569,2.130714309049099,2.182945677439422,2.2350903879805912]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.403752095893422,4.3758658925960443,4.3362443945751572,4.3199197663782893,4.2778881600212815,4.2372550848328157,4.1983451990021381]
[null,null,null,null,"Coincident",3.4525416431804428,3.4306788597952989,3.3996156053469235,3.3868170968405789,3.3538643174566847,3.3220079865089276,3.2915026360176762]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7866870607537191,4.7563759702130914,4.7133091245382142,4.6955649634546619,4.6498784348057409,4.6057120487313208,4.5634186945675408]
[null,null,null,null,"Coincident",3.7527626556309164,3.7289987606470643,3.6952343536379608,3.6813229313484555,3.6455046928877008,3.6108782462053561,3.5777202565409527]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9820814022898081,3.9153018011018186,3.8496420954368746,3.7850835046200357,3.7216075629287344,3.659196114311015,3.5978313071923518]
[null,null,null,null,"Coincident",3.1219518193952096,3.0695966120638261,3.01811940282251,2.9675054676221082,2.9177403293361279,2.868809753619836,2.8206997448388038]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3283493503150083,4.2557628272845855,4.1843935819966029,4.1142212006739518,4.0452256118790597,3.9773870807728415,3.9106862034699468]
[null,null,null,null,"Coincident",3.3934258906469674,3.3365180565911157,3.280564568285337,3.2255494213283789,3.1714568797131828,3.118271471325909,3.065977983520439]
[null,"Mannum Town 7.6kV","Substation Rating","MVA","Non-Coincident",7.8,7.8,7.8,7.8,7.8,7.8,7.8]
[null,null,null,null,"Coincident",7.8,7.8,7.8,7.8,7.8,7.8,7.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.0398199999999997,2.1879971060970189,2.2265105932609961,2.2889773352076537,2.348258185095784,2.4058223258256914,2.4632909610236209]
[null,null,null,null,"Coincident",2.0398199999999997,2.1879971060970189,2.2265105932609961,2.2889773352076537,2.348258185095784,2.4058223258256914,2.4632909610236209]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.4681517114555405,4.450243808362397,4.4263405484108702,4.4623277879705805,4.5003554851913128,4.5391134203699242,4.5797280810857819]
[null,null,null,null,"Coincident",4.0963512174463466,4.0799334533741387,4.0580192135885174,4.0910119099208737,4.1258752748794647,4.1614081137818602,4.1986431777666002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.703317591005832,4.6844671666972602,4.659305840432495,4.6971871452321903,4.7372163002013821,4.7780141267051839,4.8207664011429285]
[null,null,null,null,"Coincident",4.3119486499435222,4.2946667930254092,4.2715991721984388,4.3063283262324985,4.343026605136278,4.3804295934545889,4.4196243976490521]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.9490262475521232,3.9380829050140411,3.9271698881153441,3.9162871128191488,3.9054344953214497,3.8946119520504761,3.8838193996660459]
[null,null,null,null,"Coincident",3.6204228328715469,3.6103900995572609,3.600385168447966,3.5904079624995937,3.5804584048815742,3.5705364189762485,3.5606419283782755]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.1568697342653929,4.1453504263305696,4.1338630401214154,4.1224074871780516,4.110983679285737,4.0995915284741864,4.0882309470168909]
[null,null,null,null,"Coincident",3.8109714030226804,3.8004106311129058,3.7898791246820691,3.7793768026311509,3.7689035840858671,3.7584593883960506,3.7480441351350264]
[null,"Marion Bay 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.27310000000000001,0.29293859736403016,0.29809495103468842,0.30645827094802985,0.31439504973461319,0.32210198801021478,0.32979613958856707]
[null,null,null,null,"Coincident",0.27310000000000001,0.29293859736403016,0.29809495103468842,0.30645827094802985,0.31439504973461319,0.32210198801021478,0.32979613958856707]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.65169365441927563,0.63791179396521414,0.62442138897690291,0.61121627582434435,0.59829042122450382,0.58563791948476329,0.57325298980466977]
[null,null,null,null,"Coincident",0.65169365441927563,0.63791179396521414,0.62442138897690291,0.61121627582434435,0.59829042122450382,0.58563791948476329,0.57325298980466977]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.65178037585817783,0.63799668144001187,0.62450448127182734,0.61129761090342705,0.59837003624892238,0.58571585082981936,0.57332927307640902]
[null,null,null,null,"Coincident",0.65178037585817783,0.63799668144001187,0.62450448127182734,0.61129761090342705,0.59837003624892238,0.58571585082981936,0.57332927307640902]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.5865242889773481,0.57412061456869279,0.56197925007921268,0.5500946482419099,0.53846137910205349,0.52707412753628702,0.51592769082420276]
[null,null,null,null,"Coincident",0.5865242889773481,0.57412061456869279,0.56197925007921268,0.5500946482419099,0.53846137910205349,0.52707412753628702,0.51592769082420276]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.58660233827236008,0.57419701329601069,0.56205403314464464,0.55016784981308442,0.53853303262403018,0.52714426574683748,0.51599634576876807]
[null,null,null,null,"Coincident",0.58660233827236008,0.57419701329601069,0.56205403314464464,0.55016784981308442,0.53853303262403018,0.52714426574683748,0.51599634576876807]
[null,"Marrabel 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.61004999999999998,0.65436540213081873,0.66588365023329066,0.68456561036926267,0.70229476415452508,0.71951050086280322,0.73669767468328584]
[null,null,null,null,"Coincident",0.61004999999999998,0.65436540213081873,0.66588365023329066,0.68456561036926267,0.70229476415452508,0.71951050086280322,0.73669767468328584]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.92932201444465934,0.8508193842609213,0.76533566597235314,0.74725799846545593,0.73023998689617631,0.714130610959405,0.69848755319420786]
[null,null,null,null,"Coincident",0.83211706810619501,0.76182563257385949,0.68528331470398063,0.66909652966044852,0.65385856297944989,0.63943419073261665,0.62542736084860684]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.94249442798467431,0.86287908434673388,0.77618370113391655,0.75784979681293496,0.74059056822465119,0.72425285446911258,0.70838806858092829]
[null,null,null,null,"Coincident",0.843911677471335,0.77262391575414469,0.69499667032565648,0.67858045024974312,0.66312649729540618,0.64849767084073418,0.6342923050856818]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.85478652781551334,0.81184445348322376,0.77105966835467543,0.73232379627941591,0.69553390562039696,0.66059223573691339,0.62740593720827031]
[null,null,null,null,"Coincident",0.76537782203251137,0.72692738995796702,0.69040859959573819,0.65572441069156895,0.62278265802102217,0.5914958064816731,0.56178071848878464]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.86690245906195862,0.82335171437366861,0.78198883677824282,0.74270391397796265,0.70539255536023826,0.66995561460365594,0.63629892621951922]
[null,null,null,null,"Coincident",0.77622645472329399,0.7372310178127448,0.70019460212672557,0.6650187919411874,0.63161011566163872,0.59987979744396325,0.56974352129310979]
[null,"McLaren Flat TF1 11kV","Substation Rating","MVA","Non-Coincident",15.5,15.5,15.5,15.5,15.5,15.5,15.5]
[null,null,null,null,"Coincident",15.5,15.5,15.5,15.5,15.5,15.5,15.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.6314899999999999,3.8952895896796114,3.9638551216878826,4.0750646150313479,4.1806022671576368,4.2830836632706522,4.3853950309574721]
[null,null,null,null,"Coincident",3.6314899999999999,3.8952895896796114,3.9638551216878826,4.0750646150313479,4.1806022671576368,4.2830836632706522,4.3853950309574721]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0632245306945682,5.9589598032831548,5.9496847900013394,5.9277233453390412,5.9109715818598927,5.896923576059848,5.8786846571746896]
[null,null,null,null,"Coincident",5.702125825310981,5.6040706416654027,5.5953480069523716,5.5746944883277392,5.5589403854291266,5.5457290164189512,5.5285763264807306]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6628840996643612,6.5483074761353359,6.5381151538476265,6.5139816981747716,6.4955731668790033,6.4801357978679652,6.4600930298622972]
[null,null,null,null,"Coincident",6.2660723355065731,6.1583193864454984,6.148734073574035,6.1260378992612523,6.1087256982737657,6.0942077103504966,6.0753586005282756]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.6500396816113074,5.5682798541396137,5.4877031456838727,5.4082924357259863,5.3300308514931265,5.2529017643726972,5.1768887863791715]
[null,null,null,null,"Coincident",5.3135484294620126,5.2366578539375217,5.1608799361187003,5.0861985751094165,5.0125979030042034,4.9400622815167239,4.8685762986570342]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.2088348149574815,6.1189888507028733,6.0304430172350258,5.9431785007977886,5.8571767598825568,5.7724195212886791,5.688888776240848]
[null,null,null,null,"Coincident",5.8390642082000141,5.7545690702610131,5.671296633097473,5.5892292034169415,5.5083493439606634,5.428639869798598,5.3500838446780596]
[null,"McLaren Flat TF2 11kV","Substation Rating","MVA","Non-Coincident",15.2,15.2,15.2,15.2,15.2,15.2,15.2]
[null,null,null,null,"Coincident",15.2,15.2,15.2,15.2,15.2,15.2,15.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.9571900000000001,1.0267224313836545,1.0447949695382404,1.0741076249313246,1.1019252935022865,1.1289373925430155,1.15590467540381]
[null,null,null,null,"Coincident",0.9571900000000001,1.0267224313836545,1.0447949695382404,1.0741076249313246,1.1019252935022865,1.1289373925430155,1.15590467540381]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6642550434716115,2.6925370074224224,2.7155054119377535,2.7323523316815717,2.7500276215493198,2.7636590232788372,2.769427866711816]
[null,null,null,null,"Coincident",2.3060358779628234,2.3305152249118448,2.3503954405847782,2.3649772282622008,2.3802760085678987,2.3920746167875651,2.3970678174060258]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7794408486468165,2.808945548685748,2.8329069640519626,2.8504822397466003,2.8689216991333706,2.8831424378288548,2.8891606901453355]
[null,null,null,null,"Coincident",2.4057345160556478,2.4312721976019502,2.452011910061783,2.4672241234781502,2.4831843278213208,2.4954930344232946,2.5007021099577278]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3710192932939247,2.372785238631657,2.37455249925305,2.3763210761377329,2.3780909702660638,2.3798621826191315,2.3816347141787557]
[null,null,null,null,"Coincident",2.052226783271212,2.0537552905803418,2.0552849363282704,2.0568157213629119,2.0583476465328117,2.0598807126871477,2.06141492067573]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4735274097947153,2.4753697036172215,2.4772133695880685,2.4790584087292369,2.4809048220634695,2.4827526106142721,2.4846017754059111]
[null,null,null,null,"Coincident",2.1409522958727365,2.1425468863241504,2.1441426644333705,2.1457396310849699,2.1473377871641799,2.148937133556891,2.1505376711496544]
[null,"McLaren Vale 11kV","Substation Rating","MVA","Non-Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,null,null,"Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3449899999999999,1.4426930943560854,1.4680876169613533,1.5092761253840743,1.5483639617083758,1.5863198566600469,1.6242127784153308]
[null,null,null,null,"Coincident",1.3449899999999999,1.4426930943560854,1.4680876169613533,1.5092761253840743,1.5483639617083758,1.5863198566600469,1.6242127784153308]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5502033420724768,2.5939435941795654,2.6281331263508321,2.6717752165744462,2.7165567492122751,2.7620649727943634,2.8058546527006705]
[null,null,null,null,"Coincident",2.207318859104749,2.2451780689117249,2.2747706891944177,2.3125449353543526,2.3513054215870954,2.3906948924186509,2.4285968842703283]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6604582615618493,2.7060895699211787,2.7417572446604255,2.78728614722742,2.8340037546064822,2.8814794705231503,2.9271623436320868]
[null,null,null,null,"Coincident",2.3027495877384077,2.3422455941334577,2.3731176151262505,2.4125249845749939,2.45296123297872,2.4940536593603739,2.5335942974294534]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.308555077800321,2.3426050757088555,2.377157293542191,2.4122191387854475,2.4477981281803349,2.48390188933663,2.5205381623674237]
[null,null,null,null,"Coincident",1.9981611177599419,2.0276329646891775,2.0575395061751736,2.0878871537386647,2.1186824134670128,2.1499318874090161,2.1816422749902911]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4083626304140697,2.4438847382975548,2.479930778969464,2.5165084801684667,2.553625683613399,2.5912903466844082,2.6295105441288982]
[null,null,null,null,"Coincident",2.0845491675012537,2.1152951936525062,2.1464947078475194,2.1781543988012779,2.2102810538838664,2.2428815605755799,2.2759629079435006]
[null,"McLaren Vale Vineyard 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9600458133125788E-2,4.9620574211581024E-2,4.9640698448360346E-2,4.9660830846772468E-2,4.9680971410127436E-2,4.9701120141736652E-2,4.9721277044912845E-2]
[null,null,null,null,"Coincident",4.9600458133125788E-2,4.9620574211581024E-2,4.9640698448360346E-2,4.9660830846772468E-2,4.9680971410127436E-2,4.9701120141736652E-2,4.9721277044912845E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9863654267364034E-2,4.9883877088262481E-2,4.9904108110775725E-2,4.9924347338230049E-2,4.9944594773953056E-2,4.9964850421273715E-2,4.9985114283522342E-2]
[null,null,null,null,"Coincident",4.9863654267364034E-2,4.9883877088262481E-2,4.9904108110775725E-2,4.9924347338230049E-2,4.9944594773953056E-2,4.9964850421273715E-2,4.9985114283522342E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4640412319813208E-2,4.4658516790422924E-2,4.467662860352431E-2,4.469474776209522E-2,4.4712874269114695E-2,4.4731008127562991E-2,4.4749149340421561E-2]
[null,null,null,null,"Coincident",4.4640412319813208E-2,4.4658516790422924E-2,4.467662860352431E-2,4.469474776209522E-2,4.4712874269114695E-2,4.4731008127562991E-2,4.4749149340421561E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4877288840627631E-2,4.4895489379436236E-2,4.4913697299698151E-2,4.4931912604407043E-2,4.4950135296557753E-2,4.4968365379146349E-2,4.4986602855170109E-2]
[null,null,null,null,"Coincident",4.4877288840627631E-2,4.4895489379436236E-2,4.4913697299698151E-2,4.4931912604407043E-2,4.4950135296557753E-2,4.4968365379146349E-2,4.4986602855170109E-2]
[null,"Meadows 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.6325200000000004,4.9690366571249251,5.0565024627140787,5.198367152442942,5.3329965426458825,5.4637272116333966,5.5942409834010585]
[null,null,null,null,"Coincident",4.6325200000000004,4.9690366571249251,5.0565024627140787,5.198367152442942,5.3329965426458825,5.4637272116333966,5.5942409834010585]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6531800594307962,5.7536509110522154,5.7797526449069867,5.8102221002024628,5.7963424603525402,5.7871494608722109,5.7809797214202234]
[null,null,null,null,"Coincident",5.6531800594307962,5.7536509110522154,5.7797526449069867,5.8102221002024628,5.7963424603525402,5.7871494608722109,5.7809797214202234]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9664457179803305,6.0724840673936713,6.1000322042922761,6.1321900958092126,6.1175413287649842,6.1078389078606117,6.1013272780969432]
[null,null,null,null,"Coincident",5.9664457179803305,6.0724840673936713,6.1000322042922761,6.1321900958092126,6.1175413287649842,6.1078389078606117,6.1013272780969432]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.6903975279384849,4.5454192086965808,4.4049221115525921,4.2687677237164978,4.1368218137734409,4.0089542993481295,3.8850391188596749]
[null,null,null,null,"Coincident",4.6903975279384849,4.5454192086965808,4.4049221115525921,4.2687677237164978,4.1368218137734409,4.0089542993481295,3.8850391188596749]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.9503114975983689,4.7972993410869522,4.6490167293832982,4.5053174741413384,4.3660599056385525,4.2311067331071079,4.1003249093821195]
[null,null,null,null,"Coincident",4.9503114975983689,4.7972993410869522,4.6490167293832982,4.5053174741413393,4.3660599056385525,4.2311067331071079,4.1003249093821195]
[null,"Melrose 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.19885,0.21329491060357889,0.21704936291925225,0.22313887652147835,0.2289178163300177,0.23452940430549693,0.24013168201093577]
[null,null,null,null,"Coincident",0.19885,0.21329491060357889,0.21704936291925225,0.22313887652147835,0.2289178163300177,0.23452940430549693,0.24013168201093577]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.31147828303680103,0.31042471559252977,0.30937471181359272,0.30832825964598171,0.30728534707646094,0.30624596213242905,0.30521009288178169]
[null,null,null,null,"Coincident",0.31147828303680103,0.31042471559252977,0.30937471181359272,0.30832825964598171,0.30728534707646094,0.30624596213242905,0.30521009288178169]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.31169706769795064,0.31064276022007559,0.30959201891067983,0.30854483170728825,0.30750118658822689,0.30646107157248481,0.30542447471957646]
[null,null,null,null,"Coincident",0.31169706769795064,0.31064276022007559,0.30959201891067983,0.30854483170728825,0.30750118658822689,0.30646107157248481,0.30542447471957646]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.28033045473312096,0.27938224403327677,0.27843724063223346,0.27749543368138352,0.27655681236881485,0.27562136591918618,0.27468908359360356]
[null,null,null,null,"Coincident",0.28033045473312096,0.27938224403327677,0.27843724063223346,0.27749543368138352,0.27655681236881485,0.27562136591918618,0.27468908359360356]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.28052736092815561,0.27957848419806802,0.27863281701961184,0.27769034853655938,0.27675106792940424,0.2758149644152364,0.27488202724761884]
[null,null,null,null,"Coincident",0.28052736092815561,0.27957848419806802,0.27863281701961184,0.27769034853655938,0.27675106792940424,0.2758149644152364,0.27488202724761884]
[null,"Meningie 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.02607,1.100606029283451,1.119979078755631,1.1514010914377337,1.1812205370970146,1.2101764439313116,1.239084309584918]
[null,null,null,null,"Coincident",1.02607,1.100606029283451,1.119979078755631,1.1514010914377337,1.1812205370970146,1.2101764439313116,1.239084309584918]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.086068141174235,1.9884175922623395,1.9129355212489836,1.8754738282496113,1.8400729085531029,1.8051431746061408,1.7712000717601413]
[null,null,null,null,"Coincident",2.0391997368434764,1.9437431361153381,1.8699569465327708,1.8333369181654182,1.7987313630043573,1.7645864073019211,1.7314059157230355]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1535953657959763,2.0527838124946949,1.9748583434620566,1.9361839939305465,1.8996371261180689,1.8635766966086471,1.8285348360159566]
[null,null,null,null,"Coincident",2.1052098042811176,2.0066632185271933,1.9304885275819048,1.8926830878502692,1.8569573309803582,1.8217070834382603,1.7874525202776832]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8381852213766361,1.7681449021912465,1.7007733272948125,1.6359688095996296,1.5736335365982033,1.5136734227302284,1.4559979673748273]
[null,null,null,null,"Coincident",1.7968860871394341,1.7284193876907366,1.6625614729429439,1.5992129404468294,1.5382781752818606,1.4796652057401016,1.423285564508987]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8976883334228201,1.8253807688522687,1.7558283373570704,1.6889260601800506,1.6245729585666329,1.5626719013528532,1.5031294583607238]
[null,null,null,null,"Coincident",1.855052322475182,1.7843693166165802,1.7163795433189559,1.6509803824186731,1.5880731238852701,1.527562818833768,1.4693581362138501]
[null,"Milang 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.6597200000000001,1.780285788418265,1.8116226734942993,1.8624493645472875,1.9106838225760978,1.9575214629817423,2.0042813943534847]
[null,null,null,null,"Coincident",1.6597200000000001,1.780285788418265,1.8116226734942993,1.8624493645472875,1.9106838225760978,1.9575214629817423,2.0042813943534847]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.595412818602524,3.6250583641039649,3.6549349409551533,3.6879698096624778,3.7247587252816117,3.7643319922565754,3.8069420797599696]
[null,null,null,null,"Coincident",3.0494924921543691,3.0746367170302218,3.0999768939154966,3.1279958139074009,3.1591987737996825,3.1927633146796022,3.2289035713030811]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8546304947796188,3.8864133885638843,3.9184439703135983,3.9538605465830758,3.9933018244473812,4.0357281964262857,4.0814103339060228]
[null,null,null,null,"Coincident",3.2693510723001116,3.2963081147494759,3.3234752367165874,3.3535142305347057,3.3869668232678327,3.4229512593664118,3.4616971120121089]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2423427264512421,3.2578997402339347,3.2735313977844993,3.2892380572495674,3.3050200784941861,3.3208778231100631,3.3368116544238511]
[null,null,null,null,"Coincident",2.7500318600820628,2.763226727855022,2.7764849056347027,2.7898066971874642,2.8031924077371619,2.8166423439721373,2.8301568140522484]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4761051869319481,3.4927838112679934,3.5095424609469972,3.526381519936808,3.5433013740475836,3.5603024109406287,3.577385020137275]
[null,null,null,null,"Coincident",2.9483002938193938,2.9624464690316197,2.9766605186980026,2.9909427684854779,3.0052935456235574,3.0197131789118226,3.0342019987274651]
[null,"Millicent 11kV","Substation Rating","MVA","Non-Coincident",13.2,13.2,13.2,13.2,13.2,13.2,13.2]
[null,null,null,null,"Coincident",13.2,13.2,13.2,13.2,13.2,13.2,13.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.2110900000000004,3.4443507894897976,3.5049788221090363,3.6033141313017554,3.6966342008506747,3.7872518223351186,3.8777190987603518]
[null,null,null,null,"Coincident",3.2110900000000004,3.4443507894897976,3.5049788221090363,3.6033141313017554,3.6966342008506747,3.7872518223351186,3.8777190987603518]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.7366235430509969,5.6883792159189053,5.5745900527665517,5.5873280564298469,5.6002438547794942,5.5892991176630371,5.5802331698343224]
[null,null,null,null,"Coincident",5.3791867994539997,5.3339484731615512,5.2272492693953367,5.2391935952941484,5.2513046378726687,5.2410418439175626,5.2325407759079958]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9971288128742657,5.9466936671600115,5.8277372350684447,5.8410536830128423,5.8545559994612999,5.843114251921504,5.8336366111923228]
[null,null,null,null,"Coincident",5.6234605430778064,5.5761679034233724,5.4646233921939,5.4771101207478239,5.4897711367368496,5.4790423000148873,5.4701551908089616]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5047162581294051,5.3994834430709542,5.2962623475718491,5.195014513898319,5.0957022195071815,4.9982884629913178,4.9027369502938241]
[null,null,null,null,"Coincident",5.1617291614574201,5.0630531780355161,4.9662635682298388,4.871324270525756,4.778199912791071,4.6868557990972048,4.5972578967923141]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.754690408143416,5.644678875660798,5.5367704167444058,5.4309248272599513,5.3271026716494099,5.2252652682382568,5.1253746748235987]
[null,null,null,null,"Coincident",5.3961279568235447,5.2929710076395526,5.1917860940058835,5.0925355168218722,4.9951822976747664,4.8996901650624523,4.8060235408795489]
[null,"Minlaton 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2390600000000003,1.3290681012445085,1.3524625779166646,1.390407122668861,1.4264164420511531,1.4613829705746497,1.496291485604577]
[null,null,null,null,"Coincident",1.2390600000000003,1.3290681012445085,1.3524625779166646,1.390407122668861,1.4264164420511531,1.4613829705746497,1.496291485604577]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4631572878627659,1.3711957206622931,1.3089532586430004,1.2772982434021738,1.2478048275767868,1.219410766360872,1.191677481808374]
[null,null,null,null,"Coincident",1.4631572878627659,1.3711957206622931,1.3089532586430004,1.2772982434021738,1.2478048275767868,1.219410766360872,1.191677481808374]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5241221748570479,1.4283288756898886,1.3634929777531255,1.3305190035439312,1.2997966953924862,1.2702195482925751,1.2413307102170563]
[null,null,null,null,"Coincident",1.5241221748570479,1.4283288756898886,1.3634929777531255,1.3305190035439312,1.2997966953924862,1.2702195482925751,1.2413307102170563]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3818304011185014,1.2937161240134294,1.2112205724939753,1.1339854609537237,1.0616753503506278,0.99397619136505466,0.93059396045531961]
[null,null,null,null,"Coincident",1.3818304011185014,1.2937161240134294,1.2112205724939753,1.1339854609537237,1.0616753503506278,0.99397619136505466,0.93059396045531961]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4394066678317723,1.347620962513989,1.2616880963478909,1.1812348551601288,1.1059118232819038,1.0353918660052654,0.9693687088076246]
[null,null,null,null,"Coincident",1.4394066678317723,1.347620962513989,1.2616880963478909,1.1812348551601288,1.1059118232819041,1.0353918660052652,0.9693687088076246]
[null,"Monarto South 11kV","Substation Rating","MVA","Non-Coincident",14.5,14.5,14.5,14.5,14.5,14.5,14.5]
[null,null,null,null,"Coincident",14.5,14.5,14.5,14.5,14.5,14.5,14.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.75812000000000002,0.81319153948597056,0.82750547154309051,0.85072187613006389,0.87275421129551456,0.89414851391543071,0.91550732092597786]
[null,null,null,null,"Coincident",0.75812000000000002,0.81319153948597056,0.82750547154309051,0.85072187613006389,0.87275421129551456,0.89414851391543071,0.91550732092597786]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0545186465825713,4.1775479644925104,4.2826888217405772,4.3441938641261704,4.3949413175342595,4.445585344324499,4.4978939555108175]
[null,null,null,null,"Coincident",2.4327111879495429,2.5065287786955062,2.569613293044346,2.6065163184757023,2.6369647905205555,2.6673512065946992,2.6987363733064904]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7145565657936874,4.8576139122005939,4.9798707229541597,5.0513882141001982,5.1103968808537905,5.1692852840982546,5.2301092505939737]
[null,null,null,null,"Coincident",2.8287339394762125,2.9145683473203561,2.9879224337724954,3.0308329284601192,3.066238128512274,3.1015711704589526,3.1380655503563841]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.796747496827078,3.858558973248285,3.9213767474600512,3.9852172021036258,4.0500969865315009,4.1160330211494998,4.1830425018295569]
[null,null,null,null,"Coincident",2.2780484980962465,2.315135383948971,2.3528260484760306,2.3911303212621755,2.4300581919189006,2.4696198126896998,2.5098255010977342]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4148226707291602,4.4866964805212621,4.5597404040233149,4.6339734908181693,4.709415100618024,4.7860849083133719,4.8640029091041361]
[null,null,null,null,"Coincident",2.6488936024374961,2.692017888312757,2.735844242413989,2.780384094490902,2.8256490603708149,2.8716509449880232,2.9184017454624818]
[null,"Monarto Central 11kV","Substation Rating","MVA","Non-Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,null,null,"Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.03,3.2179267377960105E-2,3.2745692167852995E-2,3.3664401788505667E-2,3.4536255921048691E-2,3.5382862102916315E-2,3.6228063667729821E-2]
[null,null,null,null,"Coincident",0.03,3.2179267377960105E-2,3.2745692167852995E-2,3.3664401788505667E-2,3.4536255921048691E-2,3.5382862102916315E-2,3.6228063667729821E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8542775916497241,2.9204848827942373,2.970688822063523,2.9933608832011851,3.0082576931946114,3.0227892418588986,3.0381724772388958]
[null,null,null,null,"Coincident",2.0615362132960424,2.1093552231491661,2.1456156202305614,2.161990788224764,2.1727501878549482,2.183245773110686,2.1943564993085509]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0333110804848857,3.1036711990749866,3.1570241615601442,3.1811183192088235,3.1969495260084471,3.2123925605993859,3.2287407036350753]
[null,null,null,null,"Coincident",2.1908452972149246,2.2416637364829355,2.2801985533387152,2.2976008475889067,2.3090351265157643,2.3201890434107231,2.3319966857321335]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6956172020673539,2.7317113158200867,2.7682887270701779,2.8053559071351541,2.8429194139830032,2.8809858933924155,2.9195620801285638]
[null,null,null,null,"Coincident",1.9469418445855116,1.9730112510110718,1.9994297248488255,2.0262019400854476,2.053332633291947,2.0808266044616657,2.1086887178594993]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8646987776163026,2.9030568810841464,2.9419285967031681,2.981320801701854,3.0212404653942677,3.0616946504130707,3.1026905139590477]
[null,null,null,null,"Coincident",2.0690630398101999,2.0967676399526867,2.1248432026295605,2.1532946950015535,2.1821271507393099,2.2113456709139498,2.2409554248995551]
[null,"Moonta 11kV","Substation Rating","MVA","Non-Coincident",12.8,12.8,12.8,12.8,12.8,12.8,12.8]
[null,null,null,null,"Coincident",12.8,12.8,12.8,12.8,12.8,12.8,12.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.0407800000000007,5.4069535804491249,5.5021276721956678,5.656494774915453,5.8029889373901273,5.9452407877046172,6.0872566258339713]
[null,null,null,null,"Coincident",5.0407800000000007,5.4069535804491249,5.5021276721956678,5.656494774915453,5.8029889373901273,5.9452407877046172,6.0872566258339713]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3468496794795932,8.1838776894271046,8.1545442817315568,8.1702392753941453,8.1932064076191971,8.2190582467380864,8.2476052326498213]
[null,null,null,null,"Coincident",8.3468496794795932,8.1838776894271046,8.1545442817315568,8.1702392753941453,8.1932064076191971,8.2190582467380864,8.2476052326498213]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.60499966956659,8.4369873086877352,8.4067466821974808,8.4229270880352001,8.4466045439373154,8.4732559244722534,8.5026858068554851]
[null,null,null,null,"Coincident",8.60499966956659,8.4369873086877352,8.4067466821974808,8.4229270880352001,8.4466045439373154,8.4732559244722534,8.5026858068554851]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6029537329974026,7.5522479051605877,7.5018802460233216,7.4518485002616259,7.4021504275927912,7.3527838026750629,7.3037464150079963]
[null,null,null,null,"Coincident",7.6029537329974026,7.5522479051605877,7.5018802460233216,7.4518485002616259,7.4021504275927912,7.3527838026750629,7.3037464150079963]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.8380966319560841,7.7858225826397796,7.7338971608487848,7.6823180415068295,7.6310829150441144,7.5801894872938789,7.529635479389686]
[null,null,null,null,"Coincident",7.8380966319560841,7.7858225826397804,7.7338971608487848,7.6823180415068304,7.6310829150441144,7.5801894872938789,7.529635479389686]
[null,"Moorkitabie 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.28919,0.31019741110107607,0.31565755726738021,0.32451361177393173,0.33291799499360231,0.34107899638474559,0.34922645773569283]
[null,null,null,null,"Coincident",0.28919,0.31019741110107607,0.31565755726738021,0.32451361177393173,0.33291799499360231,0.34107899638474559,0.34922645773569283]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.70755915486673071,0.68893284308537017,0.66883560397422592,0.66017906561861472,0.65175243715719755,0.64333777094580835,0.63521645266273064]
[null,null,null,null,"Coincident",0.70025217564263365,0.68181821819980692,0.66192852372664346,0.65336138163632262,0.64502177515557413,0.63669400739042992,0.62865655814297783]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.70811335435148359,0.68947245341199948,0.66935947303104948,0.66069615439556562,0.65226292573242761,0.64384166868881387,0.63571398933984213]
[null,null,null,null,"Coincident",0.70080065189690699,0.68235225595851923,0.66244698277599534,0.65387313042590389,0.64552699190386542,0.63719270137016848,0.62914895674769222]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.61562828396582603,0.60158441907731386,0.58786092631292863,0.57445049726442721,0.56134599024478538,0.54854042648491197,0.53602698641712487]
[null,null,null,null,"Coincident",0.60927067690249559,0.59537184332092163,0.58179007337338029,0.56851813412572394,0.55554895764329015,0.54287563722689214,0.53049142373467606]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.61611047810525099,0.60205561328460344,0.58832137152125941,0.57490043868262553,0.56178566748791325,0.54897007370187345,0.53644683241536084]
[null,null,null,null,"Coincident",0.60974789141225327,0.59583817149508944,0.58224576355374202,0.5689634289888289,0.55598409432969031,0.54330084746743046,0.53090693397389399]
[null,"Morgan 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.49948000000000004,0.53576334899811717,0.54519394413330724,0.56048984684409375,0.57500563691484674,0.58910106543882146,0.60317310802525648]
[null,null,null,null,"Coincident",0.49948000000000004,0.53576334899811717,0.54519394413330724,0.56048984684409375,0.57500563691484674,0.58910106543882146,0.60317310802525648]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0510851008921875,1.0523063665563257,1.0535290512205249,1.0547531565335346,1.0559786841460204,1.057205635710565,1.058434012881672]
[null,null,null,null,"Coincident",1.0510851008921875,1.0523063665563257,1.0535290512205249,1.0547531565335346,1.0559786841460204,1.057205635710565,1.058434012881672]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1202340343831194,1.1215356448434235,1.122838767657163,1.1241434045815555,1.1254495573758605,1.1267572278013818,1.1280664176214688]
[null,null,null,null,"Coincident",1.1202340343831194,1.1215356448434235,1.122838767657163,1.1241434045815555,1.1254495573758605,1.1267572278013818,1.1280664176214688]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.94597659080296881,0.94707572990069311,0.94817614609847245,0.94927784088018119,0.9503808157314183,0.9514850721395085,0.95259061159350489]
[null,null,null,null,"Coincident",0.94597659080296881,0.94707572990069311,0.94817614609847245,0.94927784088018119,0.9503808157314183,0.9514850721395085,0.95259061159350489]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0082106309448076,1.0093820803590812,1.0105548908914468,1.0117290641234,1.0129046016382746,1.0140815050212435,1.015259775859322]
[null,null,null,null,"Coincident",1.0082106309448076,1.0093820803590812,1.0105548908914468,1.0117290641234,1.0129046016382746,1.0140815050212435,1.015259775859322]
[null,"Morphett Vale East 11kV","Substation Rating","MVA","Non-Coincident",57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246]
[null,null,null,null,"Coincident",57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246,57.342498251748246]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",16.569380000000002,17.773016976900823,18.085860563072671,18.593275523547668,19.07481160443686,19.542402922360655,20.009218452493641]
[null,null,null,null,"Coincident",16.569380000000002,17.773016976900823,18.085860563072671,18.593275523547668,19.07481160443686,19.542402922360655,20.009218452493641]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.029226356667543,35.04991785749705,34.736593568462879,34.72823886967646,34.725079453212551,34.710222741607389,34.618112069131662]
[null,null,null,null,"Coincident",35.029226356667543,35.04991785749705,34.736593568462879,34.72823886967646,34.725079453212551,34.710222741607389,34.618112069131662]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.638023798161079,35.659074911065296,35.340305139919145,35.331805238975136,35.328590912801253,35.313475996007028,35.219764467686907]
[null,null,null,null,"Coincident",35.638023798161079,35.659074911065296,35.340305139919145,35.331805238975136,35.328590912801253,35.313475996007028,35.219764467686915]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.620832936019958,30.360891419086375,30.103156556438353,29.84760961569642,29.594232023501046,29.343005364162721,29.09391137832348]
[null,null,null,null,"Coincident",30.620832936019958,30.360891419086375,30.103156556438353,29.84760961569642,29.594232023501046,29.343005364162721,29.09391137832348]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.153013822861087,30.888554600373979,30.626340383161683,30.366352113281582,30.108570894574743,29.852977991292498,29.599554826734707]
[null,null,null,null,"Coincident",31.153013822861087,30.888554600373983,30.626340383161683,30.366352113281586,30.108570894574747,29.852977991292498,29.599554826734714]
[null,"Morphettville 11kV","Substation Rating","MVA","Non-Coincident",27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343]
[null,null,null,null,"Coincident",27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343,27.987443946188343]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.0068900000000003,6.4432439806664927,6.5566590275384824,6.7406119486452258,6.9151830109862722,7.0846986845795659,7.253933112168319]
[null,null,null,null,"Coincident",6.0068900000000003,6.4432439806664927,6.5566590275384824,6.7406119486452258,6.9151830109862722,7.0846986845795659,7.253933112168319]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.608854776788601,22.877476932194224,22.9210611022948,23.103284012484004,23.289928725095088,23.478042588580028,23.647710441389311]
[null,null,null,null,"Coincident",22.608854776788601,22.877476932194224,22.9210611022948,23.103284012484004,23.289928725095088,23.478042588580028,23.647710441389311]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.139329637251649,24.426135794450843,24.472670334099618,24.667228569797274,24.866507935658589,25.067355904511125,25.248509185747324]
[null,null,null,null,"Coincident",24.139329637251645,24.42613579445084,24.472670334099615,24.66722856979727,24.866507935658589,25.067355904511121,25.248509185747324]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.796752384481742,20.010532436899631,20.226621045282872,20.44504313913534,20.665823917168229,20.888988850207156,21.114563684130648]
[null,null,null,null,"Coincident",19.796752384481742,20.010532436899631,20.226621045282872,20.44504313913534,20.665823917168229,20.888988850207156,21.114563684130648]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.136865899402768,21.36511749401615,21.595833919068042,21.829041791630278,22.06476801620563,22.303039787831697,22.543884595218302]
[null,null,null,null,"Coincident",21.136865899402768,21.365117494016147,21.595833919068038,21.829041791630274,22.064768016205626,22.303039787831693,22.543884595218302]
[null,"Mount Barker 11kV","Substation Rating","MVA","Non-Coincident",72.39,72.39,72.39,72.39,72.39,72.39,72.39]
[null,null,null,null,"Coincident",72.39,72.39,72.39,72.39,72.39,72.39,72.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.573919999999999,13.487317788969337,13.724723788773671,14.109783164550905,14.475203968359752,14.830042581770051,15.184292477098046]
[null,null,null,null,"Coincident",12.573919999999999,13.487317788969337,13.724723788773671,14.109783164550905,14.475203968359752,14.830042581770051,15.184292477098046]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.295235127085817,24.93858376264583,25.408669556409631,25.886176995415113,26.360781808622239,26.78007615764357,27.222101556172341]
[null,null,null,null,"Coincident",23.436746253337201,24.057361721562938,24.51083670989339,24.971471094517053,25.429305419624985,25.833783713910581,26.260189840406532]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.325478131253554,24.969627615019593,25.440298577296712,25.918400423369768,26.393596030420575,26.813412322147077,27.255987959267902]
[null,null,null,null,"Coincident",23.465920600113847,24.08730861802243,24.541348097533575,25.002555885441506,25.460960128285567,25.865941922071205,26.29287884409942]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.832735709952217,20.986599475856785,21.141599629165675,21.297744562864231,21.455042731925648,21.613502653768773,21.773132908719329]
[null,null,null,null,"Coincident",20.096596638929171,20.245023522646296,20.394546638735793,20.545174083611077,20.696914013483045,20.849774644801677,21.003764254700979]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.858668552734176,21.012723850125852,21.167916949510708,21.324256254321789,21.481750230057131,21.640407404738173,21.800236369371536]
[null,null,null,null,"Coincident",20.121613126842504,20.270224774149668,20.419934018432592,20.570748966183203,20.722677783765356,20.875728697856964,21.029909995895508]
[null,"Mount Burr 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.17868000000000001,0.19165971650313038,0.19503334255173244,0.20050517705233972,0.20569794026576599,0.21074032668496956,0.2157743472049988]
[null,null,null,null,"Coincident",0.17868000000000001,0.19165971650313038,0.19503334255173244,0.20050517705233972,0.20569794026576599,0.21074032668496956,0.2157743472049988]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.35655203182242601,0.3629846715717997,0.36953336410015686,0.37620020314320091,0.38298732021021742,0.38989688526555638,0.39693110742240917]
[null,null,null,null,"Coincident",0.36233842754623413,0.36121660843251419,0.3600982625306543,0.35898337908740519,0.35787194738281008,0.35676395673010192,0.35565939647560035]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.36773554929326085,0.37436995353308772,0.38112405063291144,0.38800000000000001,0.39500000000000002,0.40212628865979383,0.40938114438303752]
[null,null,null,null,"Coincident",0.37370343958699082,0.37254643378931546,0.37139301014335196,0.37024315755856746,0.36909686497876587,0.3679541213819818,0.36681491578037428]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.32610458479161075,0.32509494758926277,0.32408843627758888,0.32308504117866466,0.32208475264452907,0.32108756105709174,0.3200934568280403]
[null,null,null,null,"Coincident",0.32610458479161075,0.32509494758926277,0.32408843627758888,0.32308504117866466,0.32208475264452907,0.32108756105709174,0.3200934568280403]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.33633309562829178,0.33529179041038387,0.33425370912901675,0.33321884180271072,0.3321871784808893,0.3311587092437836,0.33013342420233688]
[null,null,null,null,"Coincident",0.33633309562829178,0.33529179041038387,0.33425370912901675,0.33321884180271072,0.3321871784808893,0.3311587092437836,0.33013342420233688]
[null,"Mount Gambier 11kV","Substation Rating","MVA","Non-Coincident",25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742]
[null,null,null,null,"Coincident",25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742,25.444066953927742]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.4486499999999998,5.8444521732974106,5.9473271876790736,6.1141847601647124,6.2725323608073973,6.4262943865684985,6.5798013034392016]
[null,null,null,null,"Coincident",5.4486499999999998,5.8444521732974106,5.9473271876790736,6.1141847601647124,6.2725323608073973,6.4262943865684985,6.5798013034392016]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.135516798969993,14.099630132959719,14.006112890991609,14.09571944877562,14.189214402575843,14.246517496786929,14.304801794367242]
[null,null,null,null,"Coincident",13.629642853001027,13.595040478863519,13.504869979493034,13.591269748051326,13.681418756890375,13.736671120109659,13.792869571942392]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.151069960310773,14.115143808577098,14.021523670565415,14.11122882150808,14.204826646828437,14.262192791034954,14.320541218218507]
[null,null,null,null,"Coincident",13.644639406528194,13.609998959760206,13.519729246732036,13.606224080052325,13.696472278903252,13.751785435720098,13.808045722121802]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.337916023135405,13.375940138361818,13.414072653831287,13.452313878574346,13.490664122502524,13.529123696410855,13.567692911980394]
[null,null,null,null,"Coincident",12.86058616632268,12.897249495842766,12.934017346238818,12.970890015481956,13.00786780239277,13.044951006643734,13.08213992876164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.352591592681804,13.390657545444643,13.428832017722188,13.467115318885005,13.505507759185608,13.544009649760996,13.582621302635172]
[null,null,null,null,"Coincident",12.874736534818325,12.911440204616552,12.94824851029397,12.985161750149556,13.022180223332688,13.059304229845567,13.096534070545653]
[null,"Mount Gambier North 11kV","Substation Rating","MVA","Non-Coincident",17,17,17,17,17,17,17]
[null,null,null,null,"Coincident",17,17,17,17,17,17,17]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.57917,2.7665267014404455,2.8152235622853805,2.8942071720286719,2.9691625061297051,3.041947214999289,3.1146111656632907]
[null,null,null,null,"Coincident",2.57917,2.7665267014404455,2.8152235622853805,2.8942071720286719,2.9691625061297051,3.041947214999289,3.1146111656632907]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.16334037187826,10.113403381386645,10.01964174059086,10.024674520088217,10.032978576756687,10.042247495758227,10.055613581348508]
[null,null,null,null,"Coincident",9.266954387302702,9.2214217379775434,9.1359296835209811,9.1405185820855124,9.1480902378168523,9.156541656982597,9.1687288809630747]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.586812887373187,10.534795188944422,10.43712681311548,10.44236929175856,10.451019350788215,10.460674474748153,10.474597480571363]
[null,null,null,null,"Coincident",9.6530774867736486,9.6056476437266092,9.5165934203343561,9.5213735230057441,9.5292606643925559,9.5380642260235398,9.5507592510032051]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3968563050641531,9.430241068796132,9.4637444405405411,9.4973668416830375,9.5311086951063615,9.5649704251956518,9.5989524578437866]
[null,null,null,null,"Coincident",8.5680726588687737,8.5985129542259155,8.6290613966096181,8.6597183702401814,8.6904842607029451,8.7213594549531415,8.7523443413207627]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7883919844418248,9.8231677799959716,9.8580671255630659,9.8930904600864977,9.9282382240691263,9.963510859578804,9.9989088102539441]
[null,null,null,null,"Coincident",8.9250756863216409,8.9567843273186636,8.9886056214683538,9.0205399690001897,9.0525877715655696,9.084749432242857,9.117025355542463]
[null,"Mount Gambier West 11kV","Substation Rating","MVA","Non-Coincident",25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532]
[null,null,null,null,"Coincident",25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532,25.635966875559532]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.7579400000000001,4.0309252016777135,4.1018782141753833,4.2169600685698994,4.3261725858648576,4.4322224270344455,4.5380963193169546]
[null,null,null,null,"Coincident",3.7579400000000001,4.0309252016777135,4.1018782141753833,4.2169600685698994,4.3261725858648576,4.4322224270344455,4.5380963193169546]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.03656498549449,15.978908154386675,15.932889027500915,15.967671479616408,16.007787465873051,16.048874917951473,16.095168180809548]
[null,null,null,null,"Coincident",13.979937833726671,13.929675267191628,13.889557914528686,13.919879652302267,13.954850919186027,13.990669065174407,14.031025396936329]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.359582116558439,16.300763930497894,16.253817861567242,16.289300920571048,16.330224944633926,16.372140002306509,16.419365729003911]
[null,null,null,null,"Coincident",14.261529272765355,14.210254290538002,14.169328872545933,14.200261367096502,14.235937044077353,14.272476658457977,14.313645869194779]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.979236963606203,15.054853731338323,15.13085222048764,15.207234358024117,15.284002080645269,15.361157334825263,15.438702076864272]
[null,null,null,null,"Coincident",13.058208022559155,13.124127233627021,13.190379211823451,13.256965636991994,13.323888197456235,13.39114859006259,13.458748520223338]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.280956824055602,15.358096705459214,15.435625997118446,15.513546664817328,15.591860684263384,15.670570041137706,15.749676731145323]
[null,null,null,null,"Coincident",13.321233483192316,13.388480474521129,13.456066935753276,13.523994580568621,13.592265131297868,13.660880318966234,13.729841883337325]
[null,"Mount Pleasant 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2796400000000001,1.3725959235844292,1.396756584189047,1.4359438368214463,1.473132484227025,1.5092441887125279,1.545295979725793]
[null,null,null,null,"Coincident",1.2796400000000001,1.3725959235844292,1.396756584189047,1.4359438368214463,1.473132484227025,1.5092441887125279,1.545295979725793]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4372346109850116,2.440751568587801,2.4117209673411657,2.417737125118042,2.423697810863652,2.4293067964429826,2.4377981810939557]
[null,null,null,null,"Coincident",2.28183385693512,2.2851265694607341,2.2579469912152965,2.2635795521686273,2.2691601780482942,2.2744115285503312,2.2823614931953098]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5387860531093871,2.5424495506122926,2.5122093409803812,2.5184761719979605,2.5246852196496374,2.5305279129614404,2.5393731053062041]
[null,null,null,null,"Coincident",2.3769102676407501,2.3803401765215981,2.3520281158492673,2.3578953668423202,2.3637085188003066,2.369178675573262,2.3774598887451144]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.188555151062868,2.1931198027673138,2.1976939749287481,2.2022776874039107,2.2068709600909564,2.2114738129295417,2.2160862659009108]
[null,null,null,null,"Coincident",2.0490104723429599,2.0532840768442973,2.0575665947678354,2.0618580447042265,2.0661584452828974,2.0704678151721296,2.0747861730791421]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2797449490238209,2.2844997945492849,2.2892645572174461,2.2940392577124071,2.2988239167614126,2.3036185551349395,2.3084231936467821]
[null,null,null,null,"Coincident",2.1343859086905832,2.1388375800461432,2.1432985362164954,2.1477687965669028,2.1522483805030181,2.1567373074709684,2.1612355969574399]
[null,"Mount Schank 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.12556,0.13468096039922237,0.13705163695318739,0.14089674295215904,0.14454574311489579,0.14808907218807243,0.1516265224706719]
[null,null,null,null,"Coincident",0.12556,0.13468096039922237,0.13705163695318739,0.14089674295215904,0.14454574311489579,0.14808907218807243,0.1516265224706719]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.56477892304116,2.5954278257041183,2.6192036750191066,2.6248580630091638,2.6308142737297584,2.6367020816040898,2.6435659852705573]
[null,null,null,null,"Coincident",2.03763068589436,2.0619802093538646,2.0808693228412665,2.0853615441298099,2.0900935534374758,2.0947712189819052,2.1002243598394545]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9234518876220279,2.9583869034780248,2.9854876999386031,2.9919328290272649,2.998721989417569,3.0054331811267394,3.0132569712982513]
[null,null,null,null,"Coincident",2.3225843059763935,2.3503390023679169,2.3718696746547794,2.3769901131797639,2.3823838730155384,2.3877156893536546,2.3939314277903105]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.3528933888402705,2.3784616339784557,2.404307722202327,2.4304346727562578,2.4568455376939191,2.4835434022348095,2.5105313851246591]
[null,null,null,null,"Coincident",1.8692947476557089,1.8896078594058086,1.9101417081528369,1.9308986925850111,1.9518812374564336,1.9730917938703427,1.9945328395654405]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6819351005981775,2.7110789514934348,2.7405395005984348,2.7703201893854934,2.8004244967244607,2.8308559392891066,2.8616180719679303]
[null,null,null,null,"Coincident",2.1307073328862991,2.1538611432813455,2.1772665597639738,2.2009263164683168,2.2248431772395909,2.2490199359569587,2.2734594168598972]
[null,"Murray Bridge North 11kV","Substation Rating","MVA","Non-Coincident",26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044]
[null,null,null,null,"Coincident",26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044,26.013829787234044]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.3685499999999999,5.7585335293982576,5.8598961895909065,6.0243008073894027,6.1803205574981979,6.3318221447537129,6.4830723734463644]
[null,null,null,null,"Coincident",5.3685499999999999,5.7585335293982576,5.8598961895909065,6.0243008073894027,6.1803205574981979,6.3318221447537129,6.4830723734463644]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.027174884627939,18.214053854046892,18.41183993616843,18.545033395457246,18.636390116133359,18.729472622429917,18.829320697150052]
[null,null,null,null,"Coincident",18.027174884627939,18.214053854046892,18.41183993616843,18.545033395457246,18.636390116133359,18.729472622429917,18.829320697150052]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.595560212795501,18.788331356947356,18.992353508109836,19.129746472232444,19.223983612053217,19.32000095041451,19.422997171257371]
[null,null,null,null,"Coincident",18.595560212795505,18.78833135694736,18.992353508109836,19.129746472232448,19.223983612053221,19.320000950414514,19.422997171257371]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.150599418276315,16.282263518703321,16.415000980860892,16.548820555087207,16.683731063055589,16.819741398356058,16.956860527081609]
[null,null,null,null,"Coincident",16.150599418276315,16.282263518703321,16.415000980860892,16.548820555087207,16.683731063055589,16.819741398356058,16.956860527081609]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.659817518683582,16.795632904234743,16.932555493927353,17.070594313992164,17.209758464244242,17.350057118682827,17.491499526096113]
[null,null,null,null,"Coincident",16.659817518683585,16.795632904234743,16.932555493927353,17.070594313992167,17.209758464244246,17.35005711868283,17.491499526096113]
[null,"Murray Bridge South 11kV","Substation Rating","MVA","Non-Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,null,null,"Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.3629800000000003,6.8252011580204197,6.9453394783401752,7.1401971764075256,7.3251168566838132,7.5046814634538155,7.6839481518830501]
[null,null,null,null,"Coincident",6.3629800000000003,6.8252011580204197,6.9453394783401752,7.1401971764075256,7.3251168566838132,7.5046814634538155,7.6839481518830501]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.829360828236892,15.875275533328129,15.869698529260152,15.951406448558764,15.999593870917062,16.050845720285015,16.108506851313255]
[null,null,null,null,"Coincident",14.026262606507984,14.066947237940559,14.062005501855078,14.134406197344267,14.177104664304634,14.22251849409249,14.273611534093678]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.466576780309726,16.514339796450052,16.508538288310465,16.593535385874247,16.643662608237687,16.696977617094191,16.756959915281637]
[null,null,null,null,"Coincident",14.590894266485444,14.633216670689412,14.628076003446902,14.703391211948176,14.747808519269277,14.795050497211664,14.848200303779862]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.284049696247893,14.317863700822517,14.351757751807627,14.385732038693579,14.419786751419306,14.453922080373369,14.488138216395033]
[null,null,null,null,"Coincident",12.656975496230391,12.686937799388918,12.716971030994042,12.747075358951564,12.777250951564765,12.807497977535336,12.837816605964335]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.85905865746974,14.894233855547514,14.92949232232947,14.964834254933967,15.000259850945987,15.035769308418239,15.071362825872281]
[null,null,null,null,"Coincident",13.166486068306428,13.197654513503197,13.228896742393729,13.260212929642927,13.291603250329171,13.323067879945292,13.354606994399568]
[null,"Mylor 11kV","Substation Rating","MVA","Non-Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,null,null,"Coincident",4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5999999999999996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.16709,2.3245122847367856,2.3654287346677516,2.4317929490617578,2.49477249479818,2.5559282211536303,2.6169824831233535]
[null,null,null,null,"Coincident",2.16709,2.3245122847367856,2.3654287346677516,2.4317929490617578,2.49477249479818,2.5559282211536303,2.6169824831233535]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3691539534044446,2.4167832115694394,2.4333235489970479,2.4439397437463524,2.4449448490991474,2.4483579655846146,2.4534591002016648]
[null,null,null,null,"Coincident",2.2963925942026329,2.3425590645412484,2.3585914158030952,2.3688815664139842,2.3698558030123427,2.3731640960040727,2.378108564783652]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4294705203460931,2.4783123773522742,2.4952738171604416,2.5061602908506067,2.507190985297858,2.5106909967141844,2.5159220017126698]
[null,null,null,null,"Coincident",2.3548567212102891,2.4021985491041353,2.4186390698674733,2.4291911986234593,2.4301902384250531,2.4335827576340838,2.4386531082212617]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9710731545892262,1.9195303264537171,1.8693353240577151,1.8204529022606293,1.7728487375691555,1.7264894040365428,1.6813423497920859]
[null,null,null,null,"Coincident",1.9105376365795059,1.8605777896710531,1.8119243741331879,1.7645432272726342,1.7184010797378089,1.6734655321582685,1.629705032395028]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0212549360242513,1.9683998730130265,1.91692695019408,1.8668000251166745,1.8179839004416847,1.7704442992272815,1.7241478408608844]
[null,null,null,null,"Coincident",1.9591782371980062,1.9079464567176054,1.8580543681964954,1.809466939189406,1.7621500533364496,1.7160704864078307,1.6711958829749756]
[null,"Mypolonga 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.97538000000000002,1.0462337938371575,1.0646497742226817,1.0945194738824218,1.122865776675749,1.1503912012647506,1.1778709580076772]
[null,null,null,null,"Coincident",0.97538000000000002,1.0462337938371575,1.0646497742226817,1.0945194738824218,1.122865776675749,1.1503912012647506,1.1778709580076772]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6661279349824527,2.6720880874102919,2.6820895218524652,2.69329044798857,2.6985711926492288,2.7041601272995641,2.7106577514130774]
[null,null,null,null,"Coincident",1.4466155073125329,1.4498494289915822,1.4552761116235666,1.4613536269716281,1.4642189084969564,1.4672514109618409,1.4707769596348672]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7766728011544193,2.7828800776020231,2.7932961985329547,2.8049615453236241,2.8104612439227421,2.8162819109010195,2.8230489440622533]
[null,null,null,null,"Coincident",1.5065960939752687,1.5099641027828952,1.5156157903358511,1.5219452958873811,1.5249293797247088,1.5280876179334593,1.5317593453780025]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4235404994607364,2.4294387282610344,2.4353513117226178,2.4412782847807706,2.4472196824558003,2.4531755398532438,2.4591458921640754]
[null,null,null,null,"Coincident",1.3149898859384395,1.3181902084496864,1.3213983196627974,1.3246142385333239,1.3278379840629491,1.3310695752996016,1.3343090313375674]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5240270352566982,2.5301698205558889,2.5363275556993989,2.5425002770710221,2.5486880211431031,2.554890824476749,2.5611087237220471]
[null,null,null,null,"Coincident",1.3695129187798891,1.3728459353074549,1.3761870634775037,1.3795363230315354,1.3828937337590936,1.3862593154978864,1.3896330881339001]
[null,"Myponga 11kV","Substation Rating","MVA","Non-Coincident",14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905]
[null,null,null,null,"Coincident",14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905,14.10200296735905]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.4770299999999996,2.6569670224409503,2.7037353956845629,2.7795911054060722,2.8515780668038406,2.9214803638262259,2.9912666848958924]
[null,null,null,null,"Coincident",2.4770299999999996,2.6569670224409503,2.7037353956845629,2.7795911054060722,2.8515780668038406,2.9214803638262259,2.9912666848958924]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6606165974852951,5.6885009299118936,5.6795805841298872,5.6989916966158711,5.719641095535243,5.7407489083624874,5.7569938722338678]
[null,null,null,null,"Coincident",5.5884785752530943,5.6160075540608991,5.607200887785579,5.6263646280569022,5.6467508742308663,5.6675896923567768,5.6836276329216444]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9628003781570555,5.9921732750976187,5.9827767296354395,6.0032240761176743,6.0249758131527962,6.0472104358552548,6.064322613485948]
[null,null,null,null,"Coincident",5.8868113725712048,5.9158099458570863,5.9065331485166501,5.9267199171784801,5.9481944534417766,5.9701457215521669,5.9870398242383542]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.9806246265044187,4.977251538953106,4.9738807357979251,4.9705122154917873,4.9671459764886512,4.9637820172435223,4.9604203362124535]
[null,null,null,null,"Coincident",4.9171523167569902,4.9138222153116216,4.9104943691503937,4.9071687767459338,4.9038454365719026,4.900524347102996,4.8972055068149416]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2465080252162473,5.2429548702939623,5.2394041217169729,5.2358557778556003,5.2323098370812717,5.228766297766513,5.2252251582849585]
[null,null,null,null,"Coincident",5.1796473385672694,5.1761394645016479,5.1726339661152299,5.1691308417991051,5.165630089945453,5.1621317089475447,5.1586356971997356]
[null,"Nairne 11kV","Substation Rating","MVA","Non-Coincident",9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993]
[null,null,null,null,"Coincident",9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993,9.1999999999999993]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.6479600000000003,4.9855982534021157,5.0733555789498013,5.2156930978967608,5.3507712023599172,5.4819375913290322,5.6128863601687184]
[null,null,null,null,"Coincident",4.6479600000000003,4.9855982534021157,5.0733555789498013,5.2156930978967608,5.3507712023599172,5.4819375913290322,5.6128863601687184]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.2338077582017846,7.2663969920707716,7.2850167640478816,7.306039858159191,7.3368895993389796,7.3743035982011707,7.4172392966266676]
[null,null,null,null,"Coincident",6.6158554114356187,6.6456606905435995,6.662689857382432,6.6819170411272211,6.7101314247475603,6.7443493104185235,6.7836172011708076]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.5295704400786185,8.5679972514019571,8.5899523077105648,8.6147411835121783,8.6511169138670336,8.6952327307932222,8.7458593269588487]
[null,null,null,null,"Coincident",7.8009267925642476,7.8360709705871541,7.8561505031020991,7.8788217743878981,7.9120900862586732,7.9524372831841257,7.9987390721451552]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.2591441672278885,6.1832205975604317,6.1082179826236924,6.0341251512145808,5.9609310676369702,5.8886248300579949,5.817195668884283]
[null,null,null,null,"Coincident",5.7244530396539206,5.6550152862562797,5.5864198144816193,5.5186564074335438,5.4517149721468554,5.3855855380842721,5.320258255651364]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.3803193081051548,7.2907958569453513,7.2023583274066851,7.1149935472337047,7.0286885039507441,6.9434303429237705,6.8592063654457807]
[null,null,null,null,"Coincident",6.749851124712217,6.6679752678186661,6.5870925670434062,6.5071909753787747,6.4282585919476025,6.3502836602306507,6.2732545663155372]
[null,"Nangwarry 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.22753999999999999,0.24406901663936806,0.24836515986244234,0.25533326609855261,0.26194598907584726,0.26836721476325259,0.27477778689850807]
[null,null,null,null,"Coincident",0.22753999999999999,0.24406901663936806,0.24836515986244234,0.25533326609855261,0.26194598907584726,0.26836721476325259,0.27477778689850807]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0048143529122222,1.0196748451288316,1.0293736343978643,1.0432328995542408,1.0572433344719618,1.071220032772519,1.0855626890068408]
[null,null,null,null,"Coincident",0.43807455020258468,0.4445533623579967,0.44878179792345912,0.45482409950078184,0.46093230740698338,0.46702580697094576,0.47327885526822633]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0519762283487533,1.0675342112817463,1.0776882220452428,1.0921979844154104,1.1068660118371461,1.1214987191829107,1.1365145610308651]
[null,null,null,null,"Coincident",0.45863597760326752,0.46541887869905407,0.4698457797331394,0.47617168222988943,0.48256658442899969,0.48894608793645195,0.49549262874211503]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.90962077030116584,0.92844312682430752,0.947654965554377,0.96726434586424437,0.98727949389560732,1.0077088060098607,1.0285608523103724]
[null,null,null,null,"Coincident",0.39657246997886192,0.40477855834108528,0.41315445144596313,0.42170366298349676,0.43042977935082882,0.43933646115673802,0.44842744475726604]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.95231464836838386,0.9720204493120731,0.9921340131642693,1.0126637775718368,1.0336183547779156,1.0550065352347577,1.0768372912913269]
[null,null,null,null,"Coincident",0.41518595950206982,0.42377720808422703,0.4325462313490564,0.44149670790479478,0.45063239247939624,0.45995711749564139,0.46947479467884073]
[null,"Naracoorte 11kV","Substation Rating","MVA","Non-Coincident",27.8,27.8,27.8,27.8,27.8,27.8,27.8]
[null,null,null,null,"Coincident",27.8,27.8,27.8,27.8,27.8,27.8,27.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.4529700000000005,4.7764437418678343,4.8605194950894788,4.9968857077387359,5.1262970509584065,5.2519607819474423,5.3774160223496956]
[null,null,null,null,"Coincident",4.4529700000000005,4.7764437418678343,4.8605194950894788,4.9968857077387359,5.1262970509584065,5.2519607819474423,5.3774160223496956]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.686631447865993,10.613404343452038,10.481419976196818,10.451947235499976,10.371742905733484,10.293738518292656,10.217078199473455]
[null,null,null,null,"Coincident",9.8251802963343433,9.7578560410762201,9.6365109557791051,9.6094140176479215,9.5356749723419476,9.4639585316421702,9.3934778139672357]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.387497501092183,11.309467911263608,11.16882755516691,11.137421890746561,11.051957485124611,10.968837301614021,10.887149335368971]
[null,null,null,null,"Coincident",10.469549419581563,10.397809808062737,10.268506494634945,10.239632446085464,10.161057340520054,10.084637488928838,10.00953440332942]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.705328907108461,9.5686112550949947,9.433819526102889,9.3009265899157487,9.1699056984968568,9.0407304806054611,8.9133749364889034]
[null,null,null,null,"Coincident",8.922980717802135,8.797283898624185,8.6733577534901602,8.5511773391549557,8.430718063745573,8.311955681811396,8.194866289444187]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.341837763951791,10.196153697999518,10.052521863725678,9.9109133516209535,9.7712996594203627,9.6336526863664691,9.4979447275533921]
[null,null,null,null,"Coincident",9.5081804890498081,9.3742400400629613,9.2421863920150997,9.1119929657973007,8.9836335567169368,8.8570823292233314,8.7323138117077175]
[null,"Naracoorte East 11kV","Substation Rating","MVA","Non-Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,null,null,"Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.43524999999999997,0.46686753754190446,0.47508541720193381,0.48841436261490295,0.50106351298788132,0.51334635767647741,0.52560882371264672]
[null,null,null,null,"Coincident",0.43524999999999997,0.46686753754190446,0.47508541720193381,0.48841436261490295,0.50106351298788132,0.51334635767647741,0.52560882371264672]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9517812331213404,5.0464649005960531,5.0958088751415902,5.1102005840503493,5.0978900901204431,5.0855137287921108,5.0735833757704247]
[null,null,null,null,"Coincident",4.2531905525726579,4.3345163747420132,4.3768989672846113,4.3892603131285446,4.3786865672348521,4.3680562464273009,4.3578090116703843]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.4942215893544857,5.5992773310175545,5.6540266661536212,5.6699949074937921,5.6563358667686279,5.6426037432343836,5.6293664857598547]
[null,null,null,null,"Coincident",4.7191041480750746,4.8093387660638873,4.856364138146728,4.8700796013329732,4.8583475598241739,4.8465527459313567,4.8351829830557165]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.5506684361059992,4.5558976743073307,4.5611329215010885,4.5663741845922914,4.5716214704938931,4.5768747861267922,4.5821341384198382]
[null,null,null,null,"Coincident",3.908666213054075,3.9131577173164787,3.9176543828306856,3.9221562155275635,3.9266632213447958,3.93117540622689,3.9356927761251832]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0491690950343981,5.0549711674744042,5.0607799071588548,5.0665953217491762,5.0724174189155979,5.0782462063371652,5.0840816917017433]
[null,null,null,null,"Coincident",4.3368390650419313,4.3418225888539519,4.3468118393044781,4.3518068229740736,4.3568075464508604,4.3618140163305359,4.3668262392163717]
[null,"Narrung 11kV","Substation Rating","MVA","Non-Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,null,null,"Coincident",3.9,3.9,3.9,3.9,3.9,3.9,3.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.9650000000000004E-2,7.4709532429164047E-2,7.6024581983032039E-2,7.8157519485647323E-2,8.018167416336805E-2,8.2147211515604057E-2,8.4109487815246076E-2]
[null,null,null,null,"Coincident",6.9650000000000004E-2,7.4709532429164047E-2,7.6024581983032039E-2,7.8157519485647323E-2,8.018167416336805E-2,8.2147211515604057E-2,8.4109487815246076E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.264478136597919,1.2531183830125554,1.2381587639030855,1.2278175010280559,1.2177915829049115,1.2074316469808788,1.1974906555861555]
[null,null,null,null,"Coincident",0.66314853386024197,0.65719097420214023,0.64934548506917378,0.6439220672058249,0.63866403014568696,0.6332308193055276,0.62801732159629498]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3035857078329061,1.2918746216624282,1.2764523339207066,1.2657912381732535,1.255455240108156,1.2447748937947203,1.2345264490578922]
[null,null,null,null,"Coincident",0.68365828233014636,0.67751646824962908,0.6694283351228596,0.66383718268641745,0.65841652592338862,0.65281527763456459,0.64744053772813914]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0832322025877987,1.0745348028600858,1.0659072355855099,1.057348940071029,1.0488593601254717,1.0404379440233917,1.0320841444692119]
[null,null,null,null,"Coincident",0.56809511069049001,0.56353380772217843,0.55900912799595637,0.55452077745947304,0.55006846442135848,0.54565189953226767,0.54127079576607562]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1167342294719573,1.1077678380000884,1.0988734387479482,1.0900504536814732,1.0812983094077024,1.0726164371375171,1.064004272648672]
[null,null,null,null,"Coincident",0.58566506256751549,0.58096268837337983,0.57629807009892409,0.57167090459739489,0.56708089115603966,0.56252773147656465,0.55801112965574806]
[null,"New Osborne 11kV","Substation Rating","MVA","Non-Coincident",9.5,9.5,9.5,9.5,9.5,9.5,9.5]
[null,null,null,null,"Coincident",9.5,9.5,9.5,9.5,9.5,9.5,9.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"New Richmond 11kV","Substation Rating","MVA","Non-Coincident",51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008]
[null,null,null,null,"Coincident",51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008,51.129295401244008]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.1362800000000011,7.6546754067996394,7.7894142701202007,8.0079532398425748,8.2153464134753804,8.4167337055933231,8.617786873024901]
[null,null,null,null,"Coincident",7.1362800000000011,7.6546754067996394,7.7894142701202007,8.0079532398425748,8.2153464134753804,8.4167337055933231,8.617786873024901]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.554411298691864,29.579053425589748,29.559068249526135,29.64735359910954,29.746426084551686,29.849826655736869,29.964395052266564]
[null,null,null,null,"Coincident",28.000615158117466,28.023961747733878,28.005027274021344,28.088671102105113,28.182534942246857,28.2804993229826,28.389044390860594]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.153479153633459,31.179454564845539,31.158388072957507,31.251450180337041,31.3558830712083,31.464878222772491,31.585645444859267]
[null,null,null,null,"Coincident",29.515613483254729,29.540223260982074,29.520264320635508,29.608433772843586,29.707376200002173,29.810641031170867,29.925059027022353]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.755627313368123,27.912132157919803,28.069519481764477,28.227794260912344,28.386961499431688,28.547026229607081,28.707993512098497]
[null,null,null,null,"Coincident",26.296400595472321,26.44467734097686,26.593790170232769,26.743743797641059,26.894542964185707,27.046192437583525,27.198697012434913]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.257370352063344,29.422343031197684,29.588245936956401,29.755084314581175,29.92286343888988,30.091588614443342,30.261265175713074]
[null,null,null,null,"Coincident",27.719190867554243,27.875490258983795,28.03267097122383,28.190737973752235,28.349696264068172,28.509550867850027,28.67030683911435]
[null,"Nildottie 11kV","Substation Rating","MVA","Non-Coincident",4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995]
[null,null,null,null,"Coincident",4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995,4.9399999999999995]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.39612000000000003,0.42489504645858528,0.43237411938433101,0.44450476121542887,0.45601672318152697,0.4671953112069071,0.4783553526687046]
[null,null,null,null,"Coincident",0.39612000000000003,0.42489504645858528,0.43237411938433101,0.44450476121542887,0.45601672318152697,0.4671953112069071,0.4783553526687046]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9618606879726672,1.9599034777739226,1.9642317850403028,1.9742593406886721,1.9850636740932395,1.9960636018825555,2.0077394086582698]
[null,null,null,null,"Coincident",1.74629333415309,1.7445511803169089,1.7484038973695437,1.7573296349073564,1.7669467986132363,1.7767380649821538,1.7871309454085205]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9828512312736604,1.9808730802886112,1.9852476974289044,1.9953825409404389,2.0063024731892858,2.0174200925466041,2.0292208223248549]
[null,null,null,null,"Coincident",1.7649774568695988,1.7632166632004473,1.7671106016428655,1.7761318383572657,1.7858518990182854,1.7957479251196082,1.8062520021298858]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7627385233567885,1.7797190602811535,1.7968631714568433,1.8141724326017412,1.8316484346126891,1.8492927837117079,1.8671071015936245]
[null,null,null,null,"Coincident",1.569050520286335,1.5841652522462284,1.5994255850770087,1.6148329213582031,1.6303886771804481,1.6460942822756433,1.6619511801483573]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7815985981468516,1.7987608149926146,1.8160883562202936,1.833582814406856,1.851245797470632,1.8690789288190999,1.8870838474980915]
[null,null,null,null,"Coincident",1.5858382683101513,1.6011147173774989,1.6165383251436687,1.6321105091948125,1.64783270077275,1.6637063449065173,1.6797329005451762]
[null,"Ninnes 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.5524,0.59252757665283873,0.60295734511739985,0.61987385159901764,0.63592759235957652,0.65151643418836569,0.66707941233513168]
[null,null,null,null,"Coincident",0.5524,0.59252757665283873,0.60295734511739985,0.61987385159901764,0.63592759235957652,0.65151643418836569,0.66707941233513168]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.82040197827523531,0.81712208207553017,0.81385529861734163,0.81060157547706246,0.80736086044067057,0.80413310150289086,0.80091824686636093]
[null,null,null,null,"Coincident",0.82040197827523531,0.81712208207553017,0.81385529861734163,0.81060157547706246,0.80736086044067057,0.80413310150289086,0.80091824686636093]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.85788196190156785,0.85445222396681542,0.85103619782788509,0.84763382866620229,0.84424506188235249,0.84086984309520463,0.83750811814103909]
[null,null,null,null,"Coincident",0.85788196190156785,0.85445222396681542,0.85103619782788509,0.84763382866620229,0.84424506188235249,0.84086984309520463,0.83750811814103909]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.73836178044771184,0.73540987386797718,0.73246976875560743,0.72954141792935623,0.72662477439660356,0.72371979135260178,0.72082642217972481]
[null,null,null,null,"Coincident",0.73836178044771184,0.73540987386797718,0.73246976875560743,0.72954141792935623,0.72662477439660356,0.72371979135260178,0.72082642217972481]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.7720937657114112,0.76900700157013391,0.76593257804509651,0.76287044579958208,0.75982055569411722,0.75678285878568419,0.75375730632693516]
[null,null,null,null,"Coincident",0.7720937657114112,0.76900700157013391,0.76593257804509651,0.76287044579958208,0.75982055569411722,0.75678285878568419,0.75375730632693516]
[null,"Noarlunga Centre 11kV","Substation Rating","MVA","Non-Coincident",28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427]
[null,null,null,null,"Coincident",28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427,28.272321428571427]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.2543299999999999,3.4907318402038969,3.5521762797536347,3.6518357557462546,3.746412457718213,3.8382503209127887,3.9299358145267731]
[null,null,null,null,"Coincident",3.2543299999999999,3.4907318402038969,3.5521762797536347,3.6518357557462546,3.746412457718213,3.8382503209127887,3.9299358145267731]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.162835833916031,18.210066118311516,18.240305336166184,18.232344373324015,18.229313934897323,18.228069842484448,18.212284412783763]
[null,null,null,null,"Coincident",15.525461531140289,15.565833638788682,15.591681904875948,15.584876931055389,15.582286534068579,15.581223092815577,15.567729820960261]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.271141194855851,19.321253494916341,19.353337925025603,19.344891180234136,19.341675822933265,19.340355815376778,19.323607150830941]
[null,null,null,null,"Coincident",16.472832988074163,16.515668621999414,16.543094162260026,16.53587394552061,16.533125481209197,16.531997148237053,16.51768051015905]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.631972485169026,16.652238495849215,16.67252920060518,16.692844629526583,16.713184812739751,16.733549780407717,16.753939562730267]
[null,null,null,null,"Coincident",14.216890543231965,14.234213783505789,14.251558132098106,14.268923614729342,14.286310257151264,14.303718085147018,14.321147124531162]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.646863796023432,17.668366448849547,17.689895302596334,17.711450389189551,17.733031740593841,17.754639388812805,17.776273365889033]
[null,null,null,null,"Coincident",15.084412341537039,15.102792654629219,15.121195364080087,15.139620497179537,15.158068081250724,15.176538143650093,15.195030711767421]
[null,"North Adelaide 11kV","Substation Rating","MVA","Non-Coincident",72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544]
[null,null,null,null,"Coincident",72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544,72.104033832140544]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.4392900000000002,3.6891277500114805,3.754064387199171,3.8593880142396548,3.9593399875567852,4.0563974600646349,4.1532939030595495]
[null,null,null,null,"Coincident",3.4392900000000002,3.6891277500114805,3.754064387199171,3.8593880142396548,3.9593399875567852,4.0563974600646349,4.1532939030595495]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.886643548608916,21.906256931659549,21.987914132458059,22.018689604914542,22.047955046129239,22.082178585554342,22.12619384522019]
[null,null,null,null,"Coincident",21.011960270938516,21.030789819860594,21.109183651934647,21.138729205739587,21.16682507556764,21.199680896933494,21.24193711979196]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.56430826552516,22.584528927514807,22.668714437587436,22.700442794929344,22.730614366720534,22.765897551728337,22.811275632898322]
[null,null,null,null,"Coincident",21.662542626210893,21.68195518462511,21.762776283991311,21.793236641352628,21.822202428928975,21.856075547937362,21.89964012816171]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.062220806246689,20.179798898699733,20.298066077767785,20.41702638196136,20.536683873459364,20.657042638247791,20.778106786259269]
[null,null,null,null,"Coincident",19.260449213760069,19.373328386021871,19.486869106069459,19.601075251017299,19.71595072070237,19.831499437817307,19.947725348044365]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.683396874344187,20.804615475884919,20.926544499869742,21.04918810985146,21.172550493784104,21.296635864165918,21.421448458183232]
[null,null,null,null,"Coincident",19.856800446653978,19.973174637790951,20.090230859872399,20.207973110057861,20.326405408932928,20.445531800646524,20.565356353048998]
[null,"North Unley 11kV","Substation Rating","MVA","Non-Coincident",25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003]
[null,null,null,null,"Coincident",25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003,25.393359375000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3442500000000002,3.5871838309581028,3.6503260344114126,3.7527391893736688,3.8499291287989026,3.944304552922596,4.0385233973601817]
[null,null,null,null,"Coincident",3.3442500000000002,3.5871838309581028,3.6503260344114126,3.7527391893736688,3.8499291287989026,3.944304552922596,4.0385233973601817]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.141685525568729,18.209296523883118,18.208320759751512,18.218161877701355,18.232082278081247,18.247374690999955,18.248189200605708]
[null,null,null,null,"Coincident",14.680758671498863,14.735471379884956,14.734681764294045,14.74264547182694,14.753910248647143,14.766285296337616,14.76694442026195]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.152193256168868,19.223570246147812,19.222540131101741,19.232929407917645,19.247625186758214,19.26376940043447,19.264629278936741]
[null,null,null,null,"Coincident",15.498489753195562,15.556250007230503,15.555416409361447,15.563823702360249,15.575715937089161,15.58878028574564,15.589476123448307]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.178300897149661,16.234378274711691,16.290650028203199,16.347116831371842,16.403779360300636,16.460638293416036,16.517694311496065]
[null,null,null,null,"Coincident",13.091932987770273,13.137312368079693,13.182849042820669,13.228543557208626,13.274396458348821,13.320408295242897,13.366579618795445]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.079446388923497,17.138647325399514,17.198053464714075,17.257665518143167,17.317484199428208,17.377510224784615,17.437744312910333]
[null,null,null,null,"Coincident",13.821165091038479,13.869072142470182,13.917145249770675,13.965384988524361,14.013791936310735,14.062366672711311,14.11110977931655]
[null,"Northfield 11kV","Substation Rating","MVA","Non-Coincident",26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499]
[null,null,null,null,"Coincident",26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499,26.532076395690499]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.8655799999999996,8.4369533967578469,8.5854620467207035,8.826334847321144,9.0549227949160702,9.2768910833152152,9.4984911007874082]
[null,null,null,null,"Coincident",7.8655799999999996,8.4369533967578469,8.5854620467207035,8.826334847321144,9.0549227949160702,9.2768910833152152,9.4984911007874082]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.923349946421357,20.087842027240157,20.275609554808053,20.458839959209527,20.638689411490876,20.79332924900298,20.937391329878846]
[null,null,null,null,"Coincident",19.127128223588127,19.285046501892079,19.465310041190214,19.641217780042957,19.813879683988752,19.96233945649303,20.100644204463617]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.540226228592225,20.709811391826129,20.903392667314428,21.092296339060592,21.277714376031369,21.437142246093046,21.58566484596253]
[null,null,null,null,"Coincident",19.719351508271828,19.882159327775877,20.068004272923545,20.249358551250843,20.427366495579658,20.580422950507355,20.723009956178785]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.696786125497475,17.777586223412406,17.85875523892496,17.940294856441433,18.022206768058801,18.104492673599818,18.187154280648304]
[null,null,null,null,"Coincident",16.989547354138857,17.06711833680259,17.145043493549132,17.223324441468737,17.301962805035004,17.38096021613854,17.460318314120865]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.244722474596777,18.328024343756748,18.411706553117298,18.495770839238119,18.580218946607705,18.665052627679529,18.750273642908439]
[null,null,null,null,"Coincident",17.515585838418435,17.595558610917642,17.67589652360687,17.756601243645484,17.837674445804822,17.919117812502858,18.000933033839196]
[null,"Norwood 11kV","Substation Rating","MVA","Non-Coincident",73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775]
[null,null,null,null,"Coincident",73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775,73.795831807077775]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",15.60521,16.738807502640562,17.033446762490044,17.511335314466884,17.964850875390276,18.405233117235024,18.844884714276468]
[null,null,null,null,"Coincident",15.60521,16.738807502640562,17.033446762490044,17.511335314466884,17.964850875390276,18.405233117235024,18.844884714276468]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.868603622339748,57.831234973899988,57.664216241393774,57.558329563953926,57.440484055104712,57.302339784203127,57.169140348884177]
[null,null,null,null,"Coincident",53.952270408253625,53.917430731827864,53.761715209845917,53.662994551384045,53.553124391023438,53.424329213803091,53.300144223968978]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.97039968162607,57.932965298385156,57.765652764962176,57.659579823368375,57.541527013709143,57.40313973465615,57.269705989594684]
[null,null,null,null,"Coincident",54.047177286479901,54.012276323941379,53.856286884402842,53.757392567456534,53.647329135638557,53.518307396160353,53.393903953801093]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.176238311360471,51.201207803161701,51.226189477873227,51.251183341439237,51.276189399806817,51.301207658925961,51.326238124749551]
[null,null,null,null,"Coincident",47.712819646919158,47.736099295801104,47.759390303099003,47.78269267435477,47.806006415113004,47.829331530921024,47.85266802732886]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.266261900372442,51.291275315747228,51.31630093546314,51.341338765474823,51.366388811739824,51.391451080218602,51.41652557687452]
[null,null,null,null,"Coincident",47.796750772148869,47.820071372019257,47.84340335028606,47.866746712500955,47.89010146421829,47.913467610995141,47.936845158391307]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Nuriootpa 11kV","Substation Rating","MVA","Non-Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,null,null,"Coincident",13.4,13.4,13.4,13.4,13.4,13.4,13.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.2895600000000007,4.6011632724600853,4.6821537098511836,4.8135157111967457,4.9381780649564542,5.0592303320728575,5.1800817595515714]
[null,null,null,null,"Coincident",4.2895600000000007,4.6011632724600853,4.6821537098511836,4.8135157111967457,4.9381780649564542,5.0592303320728575,5.1800817595515714]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.233529448844898,11.19952246404055,11.247876718449934,11.292394354708204,11.341606687741697,11.393266843350936,11.443889035036015]
[null,null,null,null,"Coincident",11.230348105259264,11.196350751257368,11.244691311707271,11.289196340539068,11.338394736604599,11.390040262020769,11.440648117464907]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.758840082874126,11.72324283822933,11.773858270139291,11.820457673115209,11.871971309758186,11.926047235871319,11.979036660021594]
[null,null,null,null,"Coincident",11.755509970940693,11.719922807461074,11.770523905044469,11.817110111036087,11.868609158980272,11.922669770752398,11.975644188259801]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.449727029922077,10.470093073171741,10.490498808914468,10.510944314509125,10.531429667465344,10.551954945443825,10.572520226256621]
[null,null,null,null,"Coincident",10.446767659742859,10.467127935314489,10.487527892138237,10.507967607551066,10.528447159040656,10.548966624245713,10.569526080956253]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.938384914028587,10.959703329294623,10.981063293183514,11.002464886671641,11.023908190893197,11.045393287140513,11.066920256864346]
[null,null,null,null,"Coincident",10.935287155586602,10.956599533462164,10.977953448193981,10.999348980735505,11.020786212197949,11.04226522385062,11.063786097121207]
[null,"Oaklands 11kV","Substation Rating","MVA","Non-Coincident",57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872]
[null,null,null,null,"Coincident",57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872,57.499621026894872]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.50881,12.344835806404701,12.562131649276941,12.914573464919062,13.249040250224146,13.573821239955478,13.898063380660188]
[null,null,null,null,"Coincident",11.50881,12.344835806404701,12.562131649276941,12.914573464919062,13.249040250224146,13.573821239955478,13.898063380660188]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",43.482120639839351,43.932964960918291,44.086599372706438,44.359851564548755,44.641643046648348,44.926233767017301,45.175403114206233]
[null,null,null,null,"Coincident",43.482120639839351,43.932964960918291,44.086599372706438,44.359851564548755,44.641643046648348,44.926233767017301,45.175403114206233]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",43.834036461458744,44.288529621355572,44.443407449505614,44.718871165721318,45.002943283619928,45.289837294990107,45.541023255772117]
[null,null,null,null,"Coincident",43.834036461458744,44.288529621355572,44.443407449505614,44.718871165721318,45.002943283619928,45.289837294990107,45.541023255772117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.51914733295078,38.855931206724009,39.195659677807591,39.538358491654307,39.884053618816772,40.23277125691552,40.584537832624356]
[null,null,null,null,"Coincident",38.51914733295078,38.855931206724009,39.195659677807591,39.538358491654307,39.884053618816772,40.23277125691552,40.584537832624356]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",38.830896097323006,39.17040567931614,39.512883690262761,39.8583560839825,40.206849041216614,40.558388971612025,40.913002515722752]
[null,null,null,null,"Coincident",38.830896097322999,39.17040567931614,39.512883690262761,39.8583560839825,40.206849041216614,40.558388971612025,40.913002515722759]
[null,"Orroroo 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.79786000000000001,0.85581834233930831,0.870882598434773,0.89531598703257098,0.91850323830559699,0.94101901191442705,0.96349742926449711]
[null,null,null,null,"Coincident",0.79786000000000001,0.85581834233930831,0.870882598434773,0.89531598703257098,0.91850323830559699,0.94101901191442705,0.96349742926449711]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4600544517350047,1.4551158543399831,1.4501939616262158,1.4452887170905393,1.4404000644209107,1.4355279474957612,1.4306723103833516]
[null,null,null,null,"Coincident",1.4600544517350047,1.4551158543399831,1.4501939616262158,1.4452887170905393,1.4404000644209107,1.4355279474957612,1.4306723103833516]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4610800048341435,1.4561379385316042,1.4512125886438116,1.4463038986279138,1.4414118121323136,1.4365362729960227,1.4316772252480146]
[null,null,null,null,"Coincident",1.4610800048341435,1.4561379385316042,1.4512125886438116,1.4463038986279138,1.4414118121323136,1.4365362729960227,1.4316772252480146]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3140490065615043,1.3096042689059848,1.3051745654635942,1.3007598453814855,1.2963600579788197,1.2919751527461851,1.2876050793450164]
[null,null,null,null,"Coincident",1.3140490065615043,1.3096042689059848,1.3051745654635942,1.3007598453814855,1.2963600579788197,1.2919751527461851,1.2876050793450164]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3149720043507291,1.3105241446784439,1.3060913297794303,1.3016735087651223,1.2972706309190825,1.2928826456964204,1.288509502723213]
[null,null,null,null,"Coincident",1.3149720043507291,1.3105241446784439,1.3060913297794303,1.3016735087651223,1.2972706309190825,1.2928826456964204,1.288509502723213]
[null,"Padthaway 11kV","Substation Rating","MVA","Non-Coincident",13.8,13.8,13.8,13.8,13.8,13.8,13.8]
[null,null,null,null,"Coincident",13.8,13.8,13.8,13.8,13.8,13.8,13.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.5301300000000001,0.56863983383593308,0.57864912629813037,0.59488364400468363,0.61029017838085142,0.62525055622063419,0.64018611307245366]
[null,null,null,null,"Coincident",0.5301300000000001,0.56863983383593308,0.57864912629813037,0.59488364400468363,0.61029017838085142,0.62525055622063419,0.64018611307245366]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.3931330790508012,3.4257837179942356,3.41611599834803,3.4215728269894998,3.4268321380822648,3.4212498439590378,3.4112672760238749]
[null,null,null,null,"Coincident",2.8666604559124802,2.8942450785426077,2.8860773854510127,2.8906875420575342,2.8951308275944481,2.8904146725119588,2.8819809824439595]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5047766448309643,3.5385015810895117,3.528515766435206,3.5341521399967224,3.5395844971299062,3.5338185299214708,3.5235075075891595]
[null,null,null,null,"Coincident",2.960981600330602,2.9894738341741363,2.9810374011422858,2.9857992447915391,2.9903887268464096,2.9855173970749487,2.9768062150224202]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0894044600867541,3.1005699970714846,3.1117758878583048,3.1230222782914625,3.1343093147423069,3.1456371441111934,3.1570059138293964]
[null,null,null,null,"Coincident",2.6100578408577499,2.6194909525564252,2.6289581568314895,2.6384595768982511,2.6479953364173352,2.6575655594962941,2.6671703706912222]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1910545050527803,3.2025874194240691,3.2141620153503685,3.2257784434746104,3.2374368549841708,3.2491374016128369,3.2608802356427846]
[null,null,null,null,"Coincident",2.6959360417585376,2.7056795292078561,2.7154582309746522,2.7252722743283631,2.7351217869983935,2.7450068971757817,2.7549277335148656]
[null,"Palmer 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.0819999999999999E-2,6.5238101397584458E-2,6.6386433254960645E-2,6.8248963892563824E-2,7.0016502837272718E-2,7.1732855769979009E-2,7.3446361075710925E-2]
[null,null,null,null,"Coincident",6.0819999999999999E-2,6.5238101397584458E-2,6.6386433254960645E-2,6.8248963892563824E-2,7.0016502837272718E-2,7.1732855769979009E-2,7.3446361075710925E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.879637189338655E-2,2.8856015088300439E-2,2.8915781816509171E-2,2.8975672333875546E-2,2.9035686896792312E-2,2.909582576218326E-2,2.9156089187504314E-2]
[null,null,null,null,"Coincident",2.879637189338655E-2,2.8856015088300439E-2,2.8915781816509171E-2,2.8975672333875546E-2,2.9035686896792312E-2,2.909582576218326E-2,2.9156089187504314E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9626745808411757E-2,2.9688108878087947E-2,2.9749599043272516E-2,2.9811216567206332E-2,2.9872961713675508E-2,2.9934834747012497E-2,2.9996835932097246E-2]
[null,null,null,null,"Coincident",2.9626745808411757E-2,2.9688108878087947E-2,2.9749599043272516E-2,2.9811216567206332E-2,2.9872961713675508E-2,2.9934834747012497E-2,2.9996835932097246E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.5916734704047897E-2,2.5970413579470396E-2,2.6024203634858255E-2,2.6078105100487994E-2,2.6132118207113083E-2,2.6186243185964936E-2,2.6240480268753884E-2]
[null,null,null,null,"Coincident",2.5916734704047897E-2,2.5970413579470396E-2,2.6024203634858255E-2,2.6078105100487994E-2,2.6132118207113083E-2,2.6186243185964936E-2,2.6240480268753884E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6664071227570585E-2,2.6719297990279153E-2,2.6774639138945264E-2,2.6830094910485703E-2,2.6885665542307959E-2,2.6941351272311249E-2,2.6997152338887522E-2]
[null,null,null,null,"Coincident",2.6664071227570585E-2,2.6719297990279153E-2,2.6774639138945264E-2,2.6830094910485703E-2,2.6885665542307959E-2,2.6941351272311249E-2,2.6997152338887522E-2]
[null,"Panorama 11kV","Substation Rating","MVA","Non-Coincident",58.2,58.2,58.2,58.2,58.2,58.2,58.2]
[null,null,null,null,"Coincident",58.2,58.2,58.2,58.2,58.2,58.2,58.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.0347799999999996,8.6184444647695422,8.7701477505473946,9.0162020734083157,9.249707278310785,9.4764504255756634,9.7028173798734052]
[null,null,null,null,"Coincident",8.0347799999999996,8.6184444647695422,8.7701477505473946,9.0162020734083157,9.249707278310785,9.4764504255756634,9.7028173798734052]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.161324978826993,24.179274140458929,24.074714936500641,24.03278485893691,23.995747916775251,23.955769577008663,23.825062335153344]
[null,null,null,null,"Coincident",23.110361515622412,23.127529928968116,23.027518815944337,22.987412602740999,22.9519866845209,22.913747312896628,22.788725542996449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.768334556716045,24.786734658560707,24.679548593769464,24.636565098866036,24.598597670539085,24.557614947313905,24.423623922479997]
[null,null,null,null,"Coincident",23.69096753788131,23.708567276551562,23.606043565251241,23.564929756000559,23.52861382567707,23.489413759022671,23.361251043340729]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.130018386099568,20.924765683106404,20.721506763143438,20.520222259007639,20.320892991625051,20.123499968223342,19.928024380522107]
[null,null,null,null,"Coincident",20.210909963027074,20.014585292406259,19.820167679724193,19.627638600207757,19.4369797090297,19.248172839560713,19.061200001638412]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.660871870027869,21.450462564211243,21.24209713161633,21.035755718474171,20.831418663871265,20.629066497876249,20.428679939684688]
[null,null,null,null,"Coincident",20.718672510658941,20.517415537875593,20.318113534411491,20.120747510092109,19.925298659209599,19.731748358730954,19.540078166523514]
[null,"Parafield Gardens 11kV","Substation Rating","MVA","Non-Coincident",70.2,70.2,70.2,70.2,70.2,70.2,70.2]
[null,null,null,null,"Coincident",70.2,70.2,70.2,70.2,70.2,70.2,70.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.65305,13.572195969889938,13.811096009481746,14.198578635001722,14.566299099394174,14.923370777710179,15.279850033032297]
[null,null,null,null,"Coincident",12.65305,13.572195969889938,13.811096009481746,14.198578635001722,14.566299099394174,14.923370777710179,15.279850033032297]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.641972710028956,28.749804386063825,28.894612758210691,29.137704696084832,29.392423962814505,29.655355554207976,29.94328556576448]
[null,null,null,null,"Coincident",26.542445389463559,26.642372737394023,26.776566298310986,27.001838996911946,27.237886712453871,27.481544768984396,27.748368799755507]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.279678418090093,29.389910936972395,29.537943428017353,29.786447741566015,30.046838263274914,30.315623954815702,30.609964649524187]
[null,null,null,null,"Coincident",27.133405694541818,27.235557897610992,27.372739241550033,27.603027575324678,27.844330828852755,28.093413865535229,28.366178660554436]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.353657020238479,25.632338835873039,25.914083860665293,26.198925764735847,26.486898588299862,26.778036745735047,27.072375029694378]
[null,null,null,null,"Coincident",23.495171359032724,23.753425109478023,24.014517528286277,24.278479817475116,24.545343522027881,24.815140533663417,25.087903094647334]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.91814927661051,26.203035866838015,26.491053867739382,26.782237699091265,27.076622159004927,27.374242428084809,27.675134073632815]
[null,null,null,null,"Coincident",24.018284939204644,24.282288638944795,24.549194209224531,24.819033546765898,25.091838898892682,25.367642867384145,25.646478412371149]
[null,"Paralowie 11kV","Substation Rating","MVA","Non-Coincident",27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493]
[null,null,null,null,"Coincident",27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493,27.4830985915493]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.50556,5.9054962435134009,6.009445765721491,6.178046130357508,6.3380476382896278,6.4934156759777322,6.6485259402168868]
[null,null,null,null,"Coincident",5.50556,5.9054962435134009,6.009445765721491,6.178046130357508,6.3380476382896278,6.4934156759777322,6.6485259402168868]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.827050278370955,18.899086767996167,18.987075404980455,19.029065208653876,19.074774239307086,19.122685973155207,19.184244529343658]
[null,null,null,null,"Coincident",17.190752119053723,17.256527767302586,17.336869128552788,17.37520951091777,17.416945874498012,17.460693499749926,17.516901873584157]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.897469237635473,18.969775165890397,19.058092907442418,19.10023976589769,19.146119762385698,19.194210700856118,19.255999504980199]
[null,null,null,null,"Coincident",17.255050819875109,17.321072489281089,17.401714351935468,17.440198139124043,17.482090609542229,17.526001864369409,17.582420474811546]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.385734571294286,17.536802051748662,17.689182182155058,17.842886368342782,17.997926115248259,18.154313027776173,18.312058811668123]
[null,null,null,null,"Coincident",15.874704162560054,16.012642053591485,16.151778509433154,16.292123944609983,16.433688864140411,16.576483864322675,16.720519633527992]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.450762566463883,17.6023950857637,17.75534516473013,17.909624251853788,18.065243895103109,18.222215742788681,18.380551544435178]
[null,null,null,null,"Coincident",15.934080439206211,16.07253426037996,16.212191129365021,16.353061499639836,16.495155915514847,16.638485012921709,16.783059520209431]
[null,"Parilla 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.9240000000000004E-2,4.2090481730371825E-2,4.2831365355551723E-2,4.4033037539365411E-2,4.5173422744731691E-2,4.6280783630614546E-2,4.7386307277390613E-2]
[null,null,null,null,"Coincident",3.9240000000000004E-2,4.2090481730371825E-2,4.2831365355551723E-2,4.4033037539365411E-2,4.5173422744731691E-2,4.6280783630614546E-2,4.7386307277390613E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.93326223039866574,0.92826160027019544,0.92209956629016399,0.91485610439408849,0.90782916692057569,0.90054174474208182,0.8935598361854219]
[null,null,null,null,"Coincident",0.48585561807271366,0.48325229377362239,0.4800443434993738,0.47627340266209106,0.47261518427700389,0.46882135774962319,0.46518658138492008]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.98238129515649031,0.9771174739686268,0.97063112241069893,0.96300642567798789,0.95560964939007975,0.94793867867587567,0.94058930124781259]
[null,null,null,null,"Coincident",0.51142696639233021,0.50868662502486572,0.50530983526249873,0.50134042385483268,0.49748966766000413,0.49349616605223495,0.48967008566833697]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.83665492896612281,0.83072096185407529,0.82482908134723121,0.81897898894674404,0.81317038827086774,0.80740298503994068,0.80167648706147721]
[null,null,null,null,"Coincident",0.43556192931195165,0.43247271047833885,0.42940540189986948,0.42635984817826755,0.42333589501741808,0.42033338921554969,0.41735217865747321]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.88068939891170828,0.87444311774113193,0.86824113826024341,0.86208314625973059,0.85596882975880817,0.84989787898941127,0.84386998638050237]
[null,null,null,null,"Coincident",0.45848624138100175,0.45523443208246195,0.45200568621038895,0.44879984018765007,0.44561673159728221,0.44245619917426288,0.43931808279734025]
[null,"Paringa 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3515699999999999,1.4497510803343179,1.4752698387768357,1.51665985084302,1.5559389138403925,1.5940804977479535,1.6321588003797864]
[null,null,null,null,"Coincident",1.3515699999999999,1.4497510803343179,1.4752698387768357,1.51665985084302,1.5559389138403925,1.5940804977479535,1.6321588003797864]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4864279184677129,2.4317112872094668,2.4341400366955659,2.4264935607479607,2.4207808594077962,2.4163792263065131,2.4171902708425748]
[null,null,null,null,"Coincident",2.3042991923357623,2.2535905076885072,2.2558413533444925,2.2487549752438398,2.2434607244085658,2.2393815071809473,2.240133143395902]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5763367555705505,2.5196415796498695,2.5221581523301526,2.5142351810314145,2.5083159093216065,2.5037551138691647,2.5045954856463397]
[null,null,null,null,"Coincident",2.3876222837397516,2.3350799811404994,2.3374122170165368,2.3300695966135963,2.3245839065122191,2.3203571854400287,2.3211360007006774]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2890800443175112,2.2788491979581704,2.2686640774866107,2.2585244785349099,2.2484301976485503,2.2383810322823372,2.2283767807963342]
[null,null,null,null,"Coincident",2.1214068817902256,2.1119254362081357,2.1024863671315139,2.0930894851622144,2.0837346017485889,2.0744215291817061,2.0651500805915828]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.371852813755658,2.3612520216231405,2.350698608819215,2.3401923635860498,2.3297330751122427,2.3193205335285976,2.30895452990391]
[null,null,null,null,"Coincident",2.198116616404715,2.1882923232620715,2.1785119389525773,2.1687752672294796,2.1590821127231332,2.1494322809370816,2.1398255782441526]
[null,"Paringa 33kV","Substation Rating","MVA","Non-Coincident",36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996]
[null,null,null,null,"Coincident",36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996,36.574999999999996]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.35765,2.5289149911215882,2.5734293713179541,2.6456292292223464,2.7141467924086822,2.7806801612313556,2.8471031435407745]
[null,null,null,null,"Coincident",2.35765,2.5289149911215882,2.5734293713179541,2.6456292292223464,2.7141467924086822,2.7806801612313556,2.8471031435407745]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.157444166779699,13.17729837472787,13.408136996521005,13.433578972506831,13.464776425865299,13.500889829368901,13.566572362614597]
[null,null,null,null,"Coincident",10.169813987556036,10.185159946782143,10.363582580769618,10.383247506569189,10.407361026909419,10.435274244053556,10.486042397569777]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.66776105492827,13.688385316504512,13.928177109266475,13.954605862763865,13.987013322192983,14.02452739891722,14.092757456252457]
[null,null,null,null,"Coincident",10.564254409373127,10.580195567944841,10.765538397237545,10.785966035279136,10.811014808431869,10.840010651193159,10.892747868441747]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.655712664903444,12.788831432151447,12.923350405508963,13.059284313005627,13.196648037587451,13.335456618746308,13.475725254166555]
[null,null,null,null,"Coincident",9.7820094883614583,9.884901287407283,9.988875351024971,10.093943062984799,10.200115926796917,10.307405566970829,10.415823730288134]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.14656969021862,13.284851523651444,13.424587870764119,13.565794030818976,13.708485464003211,13.852677793121581,13.998386805306888]
[null,null,null,null,"Coincident",10.161408753041158,10.268291252867431,10.376297993342492,10.485440799760832,10.595731621800978,10.707182534833821,10.819805741244721]
[null,"Paskeville 11kV","Substation Rating","MVA","Non-Coincident",1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999]
[null,null,null,null,"Coincident",1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999,1.2349999999999999]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.24784999999999999,0.26585438065424705,0.27053399346007878,0.2781240661093709,0.28532703433439721,0.29232141240692688,0.29930418600156111]
[null,null,null,null,"Coincident",0.24784999999999999,0.26585438065424705,0.27053399346007878,0.2781240661093709,0.28532703433439721,0.29232141240692688,0.29930418600156111]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.28522936162257279,0.2840890392879083,0.28295327586337682,0.28182205312284964,0.28069535291306463,0.27957315715333475,0.27845544783525805]
[null,null,null,null,"Coincident",0.28522936162257279,0.2840890392879083,0.28295327586337682,0.28182205312284964,0.28069535291306463,0.27957315715333475,0.27845544783525805]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.29826003693351993,0.29706761908523688,0.2958799684204475,0.29469706588036421,0.29351889248239488,0.29234542931983815,0.29117665756157984]
[null,null,null,null,"Coincident",0.29826003693351993,0.29706761908523688,0.2958799684204475,0.29469706588036421,0.29351889248239488,0.29234542931983815,0.29117665756157984]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.25670642546031552,0.25568013535911749,0.25465794827703914,0.2536398478105647,0.25262581762175818,0.25161584143800131,0.25060990305173225]
[null,null,null,null,"Coincident",0.25670642546031552,0.25568013535911749,0.25465794827703914,0.2536398478105647,0.25262581762175818,0.25161584143800131,0.25060990305173225]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.26843403324016796,0.26736085717671321,0.26629197157840273,0.26522735929232782,0.26416700323415543,0.26311088638785435,0.26205899180542186]
[null,null,null,null,"Coincident",0.26843403324016796,0.26736085717671321,0.26629197157840273,0.26522735929232782,0.26416700323415543,0.26311088638785435,0.26205899180542186]
[null,"Peake 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.8200000000000001E-2,9.4607046091202712E-2,9.6272334973487805E-2,9.8973341258206657E-2,0.10153659240788315,0.10402561458257396,0.10651050718312567]
[null,null,null,null,"Coincident",8.8200000000000001E-2,9.4607046091202712E-2,9.6272334973487805E-2,9.8973341258206657E-2,0.10153659240788315,0.10402561458257396,0.10651050718312567]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.15416652474799825,0.15396065699662442,0.15375506415273216,0.15354974584922107,0.15334470171948103,0.15313993139739146,0.15293543451732067]
[null,null,null,null,"Coincident",0.15416652474799825,0.15396065699662442,0.15375506415273216,0.15354974584922107,0.15334470171948103,0.15313993139739146,0.15293543451732067]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.15626645783634821,0.15605778591913072,0.15584939265396464,0.15564127766874919,0.15543344059188061,0.1552258810522513,0.15501859867924922]
[null,null,null,null,"Coincident",0.15626645783634821,0.15605778591913072,0.15584939265396464,0.15564127766874919,0.15543344059188061,0.1552258810522513,0.15501859867924922]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.13874987227319843,0.138564591296962,0.13837955773745894,0.13819477126429897,0.13801023154753292,0.13782593825765233,0.13764189106558861]
[null,null,null,null,"Coincident",0.13874987227319843,0.138564591296962,0.13837955773745894,0.13819477126429897,0.13801023154753292,0.13782593825765233,0.13764189106558861]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.14063981205271339,0.14045200732721769,0.14026445338856816,0.14007714990187428,0.13989009653269252,0.13970329294702619,0.13951673881132431]
[null,null,null,null,"Coincident",0.14063981205271339,0.14045200732721769,0.14026445338856816,0.14007714990187428,0.13989009653269252,0.13970329294702619,0.13951673881132431]
[null,"Pellaring Flat 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.504E-2,1.6132539378817333E-2,1.6416507006816967E-2,1.6877086763304173E-2,1.7314176301752408E-2,1.7738608200928711E-2,1.8162335918755216E-2]
[null,null,null,null,"Coincident",1.504E-2,1.6132539378817333E-2,1.6416507006816967E-2,1.6877086763304173E-2,1.7314176301752408E-2,1.7738608200928711E-2,1.8162335918755216E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5987906311288507E-2,9.6186716961001464E-2,9.63859393883639E-2,9.6585574446251821E-2,9.6785622989307707E-2,9.6986085873944194E-2,9.7186963958347708E-2]
[null,null,null,null,"Coincident",9.5987906311288507E-2,9.6186716961001464E-2,9.63859393883639E-2,9.6585574446251821E-2,9.6785622989307707E-2,9.6986085873944194E-2,9.7186963958347708E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.8755819361372538E-2,9.8960362926959825E-2,9.9165330144241712E-2,9.9370721890687769E-2,9.9576539045585027E-2,9.9782782490041647E-2,9.9989453106990811E-2]
[null,null,null,null,"Coincident",9.8755819361372538E-2,9.8960362926959825E-2,9.9165330144241712E-2,9.9370721890687769E-2,9.9576539045585027E-2,9.9782782490041647E-2,9.9989453106990811E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6389115680159653E-2,8.6568045264901319E-2,8.6747345449527516E-2,8.6927017001626639E-2,8.7107060690376936E-2,8.7287477286549772E-2,8.7468267562512941E-2]
[null,null,null,null,"Coincident",8.6389115680159653E-2,8.6568045264901319E-2,8.6747345449527516E-2,8.6927017001626639E-2,8.7107060690376936E-2,8.7287477286549772E-2,8.7468267562512941E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8880237425235278E-2,8.9064326634263849E-2,8.924879712981755E-2,8.9433649701619003E-2,8.9618885141026519E-2,8.9804504241037489E-2,8.9990507796291738E-2]
[null,null,null,null,"Coincident",8.8880237425235278E-2,8.9064326634263849E-2,8.924879712981755E-2,8.9433649701619003E-2,8.9618885141026519E-2,8.9804504241037489E-2,8.9990507796291738E-2]
[null,"Penfield 11kV","Substation Rating","MVA","Non-Coincident",51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454]
[null,null,null,null,"Coincident",51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454,51.362367864693454]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.9135400000000002,3.1251860892127299,3.1801961319575476,3.2694193728960936,3.3540921025404073,3.4363128017110274,3.5183970872825854]
[null,null,null,null,"Coincident",2.9135400000000002,3.1251860892127299,3.1801961319575476,3.2694193728960936,3.3540921025404073,3.4363128017110274,3.5183970872825854]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.457652766222829,23.724970540966211,24.126526908222633,24.36130605224459,24.606403257772275,24.859197544546202,25.133871382837832]
[null,null,null,null,"Coincident",20.589371053575675,20.824002579085032,21.176458689112945,21.382530241117053,21.597658214878791,21.819542110189367,22.06063023744818]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.884314713966326,25.167890385481503,25.593868854759307,25.842926941105034,26.102930619164706,26.371099504290033,26.662478624948857]
[null,null,null,null,"Coincident",21.84158808069461,22.090489570574285,22.464381572992526,22.682986111339584,22.91119787047063,23.146576436940826,23.402327210144684]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.767880851988586,22.156561303718362,22.552181911661968,22.954866597071575,23.364741493898357,23.781934988301749,24.206577758864178]
[null,null,null,null,"Coincident",19.106215799944483,19.447370395491188,19.794616540472969,20.148063003685571,20.507820496066234,20.87400170537196,21.246721331476994]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.091773212577355,23.504092670981876,23.923774376287664,24.350949786465783,24.785752706759606,25.228319331596936,25.678788287250576]
[null,null,null,null,"Coincident",20.268229379001543,20.630132524482672,20.998497698997511,21.373440286509304,21.75507773124113,22.143529574463283,22.538917491937472]
[null,"Penneshaw 11kV","Substation Rating","MVA","Non-Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,null,null,"Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.33906000000000003,0.36369007990570512,0.37009181288107457,0.38047506901369105,0.39032876441969233,0.39989710748716023,0.40944957557268247]
[null,null,null,null,"Coincident",0.33906000000000003,0.36369007990570512,0.37009181288107457,0.38047506901369105,0.39032876441969233,0.39989710748716023,0.40944957557268247]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.58818697651056528,0.58796010523616926,0.57704549782000969,0.58386128598149867,0.59086250273597241,0.59797339439509267,0.60469279026001366]
[null,null,null,null,"Coincident",0.58818697651056528,0.58796010523616926,0.57704549782000969,0.58386128598149867,0.59086250273597241,0.59797339439509267,0.60469279026001366]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.64371240525760565,0.64346411711190121,0.63151916002703046,0.63897836529061314,0.64664050378862725,0.65442267061009263,0.66177638404956152]
[null,null,null,null,"Coincident",0.64371240525760576,0.64346411711190132,0.63151916002703057,0.63897836529061325,0.64664050378862736,0.65442267061009274,0.66177638404956163]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.55668249362226929,0.55668388916851441,0.55668528471825807,0.55668668027150026,0.55668807582824087,0.55668947138848002,0.5566908669522177]
[null,null,null,null,"Coincident",0.55668249362226929,0.55668388916851441,0.55668528471825807,0.55668668027150026,0.55668807582824087,0.55668947138848002,0.5566908669522177]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.60923386821699876,0.60923539550418127,0.60923692279519248,0.60923845009003241,0.60923997738870117,0.60924150469119864,0.60924303199752494]
[null,null,null,null,"Coincident",0.60923386821699888,0.60923539550418127,0.60923692279519248,0.60923845009003252,0.60923997738870128,0.60924150469119875,0.60924303199752505]
[null,"Penola 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.1212599999999999,1.2027108446737182,1.2238811600042283,1.2582182383126621,1.290804077134502,1.3224462653838651,1.3540359556026249]
[null,null,null,null,"Coincident",1.1212599999999999,1.2027108446737182,1.2238811600042283,1.2582182383126621,1.290804077134502,1.3224462653838651,1.3540359556026249]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7816574739781896,2.7492674282736074,2.7046454264968345,2.6969647198147517,2.69025549460298,2.6838247354040972,2.6784305679270193]
[null,null,null,null,"Coincident",2.0637444053264655,2.0397138493588747,2.0066082612759599,2.0009098546272677,1.9959322015105929,1.9911611456049512,1.9871591492929133]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9047240468418991,2.8709009951122937,2.8243048189864655,2.8162843011459713,2.8092782452276488,2.8025629752638994,2.7969301580928652]
[null,null,null,null,"Coincident",2.1550489435760851,2.1299552235796351,2.0953849723215758,2.0894344557766797,2.0842365804666891,2.0792544426774073,2.0750753893497795]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6017016200777747,2.5994052687846838,2.5971109443301899,2.5948186449253354,2.5925283687827423,2.5902401141166091,2.5879538791427117]
[null,null,null,null,"Coincident",1.9302330401900547,1.9285293501498131,1.9268271638449714,1.9251264799482817,1.9234272971336668,1.9217296140762195,1.9200334294522028]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7168065548126124,2.7144086079469627,2.7120127775916547,2.7096190618785836,2.7072274589412944,2.7048379669149778,2.7024505839364719]
[null,null,null,null,"Coincident",2.0156307454455336,2.0138516804547684,2.0120741857279256,2.0102982598790371,2.0085239015233576,2.0067511092773622,2.0049798817587496]
[null,"Peterborough 11kV","Substation Rating","MVA","Non-Coincident",6.2,6.2,6.2,6.2,6.2,6.2,6.2]
[null,null,null,null,"Coincident",6.2,6.2,6.2,6.2,6.2,6.2,6.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.1154200000000001,1.1964466139574754,1.2175066652622197,1.2516649014311665,1.2840810193152046,1.3155584015611641,1.3469835592086401]
[null,null,null,null,"Coincident",1.1154200000000001,1.1964466139574754,1.2175066652622197,1.2516649014311665,1.2840810193152046,1.3155584015611641,1.3469835592086401]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8097523923882253,1.7552195503660475,1.6935741662789521,1.6818219633077784,1.6681540729443713,1.6570397558126309,1.6437715856816453]
[null,null,null,null,"Coincident",1.6951580324068858,1.6440782352077339,1.5863362654026014,1.5753282173685985,1.5625257841556157,1.5521152307341475,1.5396872072832708]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.82555344709408,1.7705444756170208,1.7083608620514505,1.6965060499041029,1.6827188243850943,1.6715074674960062,1.6581234521903059]
[null,null,null,null,"Coincident",1.7099585570078137,1.6584327790914641,1.6001866607478066,1.5890825007982059,1.5761682887869648,1.5656668402105445,1.5531303069550897]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6491213112380902,1.6004814427922163,1.5532761788149825,1.5074632064867368,1.4630014609796931,1.4198510886491398,1.3779734113103048]
[null,null,null,null,"Coincident",1.5446981857388442,1.4991382162988094,1.4549220115077788,1.4120099378134452,1.3703635306319442,1.3299454598698119,1.2907194964628568]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6635198865156047,1.614455340514154,1.5668379245974362,1.5206249565100793,1.4757750128848679,1.4322478921125719,1.3900045783069093]
[null,null,null,null,"Coincident",1.5581850365586318,1.5122272803426011,1.4676250212638531,1.4243382797272015,1.3823282553122354,1.3415572919942464,1.3019888443909504]
[null,"Piccadilly 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.91689999999999994,0.98350567529505395,1.0008175049568135,1.0288963333293613,1.0555431018003179,1.0814182087387987,1.1072503858980487]
[null,null,null,null,"Coincident",0.91689999999999994,0.98350567529505395,1.0008175049568135,1.0288963333293613,1.0555431018003179,1.0814182087387987,1.1072503858980487]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7860092321707859,1.7916872685178389,1.8045549215535353,1.8228558816328377,1.8434632538954099,1.865778322384716,1.8897949417555695]
[null,null,null,null,"Coincident",1.5391138645128399,1.5440069772177138,1.5550958242596238,1.570866885732646,1.5886255242599239,1.6078557895243983,1.6285523857046322]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8412466311039031,1.8471002768225144,1.8603658985087992,1.8792328676627195,1.9004775813354742,1.9234828065821814,1.9482422079954325]
[null,null,null,null,"Coincident",1.5867153242400411,1.5917597703275401,1.603191571401674,1.6194503976625216,1.6377582724329112,1.657583288169483,1.6789199852625074]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6077249217199041,1.6134703020719547,1.6192362141673053,1.62502273137838,1.6308299273398068,1.6366578759493555,1.6425066513688775]
[null,null,null,null,"Coincident",1.3854753227307532,1.3904264699014726,1.3953953105365964,1.4003819078656496,1.4053863253441143,1.4104086266542382,1.4154488757058441]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6574483729071177,1.663371445435005,1.6693156847085622,1.675281166369464,1.6812679663296979,1.6872761607725315,1.6933058261534821]
[null,null,null,null,"Coincident",1.4283250749801579,1.4334293504138893,1.4385518665325736,1.4436926885212884,1.448851881798056,1.4540295120146784,1.4592256450575714]
[null,"Pinnaroo 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.52664999999999995,0.56490703882008964,0.57485062600665926,0.59097857339721682,0.60628397269400969,0.62114614421669589,0.63598365768699694]
[null,null,null,null,"Coincident",0.52664999999999995,0.56490703882008964,0.57485062600665926,0.59097857339721682,0.60628397269400969,0.62114614421669589,0.63598365768699694]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4098744505473062,1.3570995145206686,1.3123300425550737,1.2915091998498329,1.2717804671450537,1.2521680926824594,1.2331566037112696]
[null,null,null,null,"Coincident",1.088900757822747,1.048140626442861,1.0135634256632198,0.99748268074905821,0.98224541477493055,0.96709801678730678,0.95241470598609945]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4980217046899418,1.4419472084106195,1.3943786886137437,1.3722560987120132,1.3512938990024483,1.330455332409467,1.3102552194800781]
[null,null,null,null,"Coincident",1.1569803033444421,1.1136717935197695,1.0769327794641441,1.059846644667074,1.0436567242521635,1.0275622904916051,1.0119609592749297]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.232093589252683,1.196574114945776,1.162078615656712,1.1285775716682758,1.0960423142739597,1.0644450012445577,1.0337585930020199]
[null,null,null,null,"Coincident",0.95159369866230403,0.92416063008286964,0.89751841715195624,0.87164426064624734,0.84651601861102499,0.82211218741206815,0.79841188333379631]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3091257439223474,1.2713855441263529,1.2347333396488023,1.1991377651599047,1.1645683595469163,1.1309955398468698,1.0983905759307899]
[null,null,null,null,"Coincident",1.0110886214647952,0.98194040039994268,0.95363248034650372,0.92614063664293855,0.89944134298962597,0.87351175131610115,0.84832967222868982]
[null,"Pinnaroo South 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.1999999999999998E-3,5.5777396788464183E-3,5.675919975761186E-3,5.8351629766743148E-3,5.9862843596484392E-3,6.1330294311721613E-3,6.2795310357398352E-3]
[null,null,null,null,"Coincident",5.1999999999999998E-3,5.5777396788464183E-3,5.675919975761186E-3,5.8351629766743148E-3,5.9862843596484392E-3,6.1330294311721613E-3,6.2795310357398352E-3]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.11562489356099866,0.11547049274746829,0.11531629811454908,0.11516230938691575,0.11500852628961072,0.11485494854804354,0.11470157588799045]
[null,null,null,null,"Coincident",0.11562489356099866,0.11547049274746829,0.11531629811454908,0.11516230938691575,0.11500852628961072,0.11485494854804354,0.11470157588799045]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11719984337726114,0.11704333943934803,0.11688704449047344,0.11673095825156184,0.11657508044391041,0.11641941078918841,0.11626394900943686]
[null,null,null,null,"Coincident",0.11719984337726114,0.11704333943934803,0.11688704449047344,0.11673095825156184,0.11657508044391041,0.11641941078918841,0.11626394900943686]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10406240420489879,0.10392344347272146,0.10378466830309417,0.10364607844822418,0.10350767366064965,0.10336945369323919,0.1032314182991914]
[null,null,null,null,"Coincident",0.10406240420489879,0.10392344347272146,0.10378466830309417,0.10364607844822418,0.10350767366064965,0.10336945369323919,0.1032314182991914]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10547985903953502,0.10533900549541322,0.10519834004142609,0.10505786242640566,0.10491757239951936,0.10477746971026958,0.10463755410849318]
[null,null,null,null,"Coincident",0.10547985903953502,0.10533900549541322,0.10519834004142609,0.10505786242640566,0.10491757239951936,0.10477746971026958,0.10463755410849318]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Plympton 11kV","Substation Rating","MVA","Non-Coincident",28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194]
[null,null,null,null,"Coincident",28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194,28.42910447761194]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.0184600000000001,5.3830122055199228,5.4777648772227856,5.6314484599848056,5.7772939629848681,5.9189159383000485,6.060302946465181]
[null,null,null,null,"Coincident",5.0184600000000001,5.3830122055199228,5.4777648772227856,5.6314484599848056,5.7772939629848681,5.9189159383000485,6.060302946465181]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.025938190061886,21.975345268016746,21.779941283511697,21.683268060325133,21.590460425591051,21.498534463513991,21.389217866130217]
[null,null,null,null,"Coincident",21.943466043402296,21.893062557414353,21.698390227830377,21.602078980064427,21.509618846753295,21.418037084835195,21.309129803702742]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.869711830726466,22.817180785834637,22.614291230000752,22.513914631422004,22.41755170496026,22.322104226431822,22.208599908980752]
[null,null,null,null,"Coincident",22.784080326093562,22.731745974209819,22.529616101666612,22.429615345128632,22.333613232237468,22.238523139550193,22.125443818511741]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.712682244335408,19.585823027911392,19.459780202711677,19.334548514923021,19.21012274454263,19.086497705160578,18.963668243743616]
[null,null,null,null,"Coincident",19.638871666684633,19.512487451679934,19.386916571070071,19.262153790713764,19.138193910153571,19.01503176239914,18.892662213711827]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.467839256084027,20.336120293756323,20.205248997116222,20.07521991108645,19.946027615695389,19.817666725851186,19.690131891117261]
[null,null,null,null,"Coincident",20.391201129418693,20.259975364950954,20.12959409223977,20.000051876633428,19.871343318454418,19.743463052774381,19.616405749190481]
[null,"Point Boston 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.35E-2,2.5207092779402081E-2,2.5650792198151511E-2,2.6370448067662769E-2,2.7053400471488138E-2,2.7716575313951112E-2,2.8378649873055023E-2]
[null,null,null,null,"Coincident",2.35E-2,2.5207092779402081E-2,2.5650792198151511E-2,2.6370448067662769E-2,2.7053400471488138E-2,2.7716575313951112E-2,2.8378649873055023E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.035376716408801,1.0360058219762835,1.0396662188196188,1.033142824992767,1.0268182043292327,1.020483475053986,1.0146800753948544]
[null,null,null,null,"Coincident",0.96403975604379277,0.96462551653868311,0.96803371379089875,0.96195977867747584,0.95607092135152483,0.95017265189237166,0.94476910369300793]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0897234006794425,1.0903855278525947,1.0942380580792652,1.0873722528198764,1.0807156542811538,1.0740484165320292,1.0679403977676263]
[null,null,null,null,"Coincident",1.0146419797713853,1.0152584866991146,1.0188455794364832,1.012452824874392,1.0062548627900123,1.0000469945317363,0.99435981533770379]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.93757113857335894,0.9346513980709672,0.93174075008886592,0.92883916631155072,0.92594661851169602,0.92306307854988034,0.9201885183743127]
[null,null,null,null,"Coincident",0.87297293572428547,0.87025436394550348,0.86754425821671444,0.86484259217333859,0.86214933953289974,0.859464474094769,0.85678796973991034]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.98678403069444653,0.98371103368867674,0.98064760646748383,0.97759371922908878,0.97454934226452028,0.97151444595732528,0.96848900078328037]
[null,null,null,null,"Coincident",0.91879508312506841,0.91593381414266284,0.91308145559125542,0.91023797972239562,0.90740335887404622,0.90457756547031343,0.90176057202117899]
[null,"Polda 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.52710999999999997,0.56540045425321828,0.57535272661989967,0.59149476089130726,0.60681352861813243,0.62168868143560718,0.63653915466323541]
[null,null,null,null,"Coincident",0.52710999999999997,0.56540045425321828,0.57535272661989967,0.59149476089130726,0.60681352861813243,0.62168868143560718,0.63653915466323541]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.86506705091362968,0.8333110305562148,0.80985667031863073,0.79819674084851866,0.78692900700587054,0.7757446531017087,0.7649323294845467]
[null,null,null,null,"Coincident",0.79825761156211095,0.76895412007384401,0.74731114850973512,0.7365517195845851,0.72615419687758753,0.71583361464645023,0.70585633066949516]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.86595313588148504,0.83416458795034298,0.81068620349866449,0.79901433080609485,0.78773505546551403,0.77653924546918085,0.765715846829089]
[null,null,null,null,"Coincident",0.79907526386933303,0.76974175692355218,0.74807661654404056,0.73730616677579719,0.72689799392490173,0.71656684035971019,0.7065793366878278]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.7874619369843644,0.76555099036934204,0.74424971078585245,0.72354113438948187,0.70340876935087115,0.68383658272200609,0.66480898766794982]
[null,null,null,null,"Coincident",0.72664596848224305,0.70642721215173643,0.6867710380487293,0.66766179245261104,0.64908425720393303,0.63102363758502023,0.61346555053780194]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.78826853132220587,0.76633514140593129,0.74501204300086588,0.72428225488659304,0.70412926834123402,0.68453703399428567,0.66548994904527381]
[null,null,null,null,"Coincident",0.72739026924938566,0.7071508029218514,0.68747449507270297,0.66834567594728211,0.64974911179823591,0.63166999275371494,0.61409392102313554]
[null,"Poonindie 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.26756999999999997,0.28700688574402616,0.29205882844508085,0.30025279955168199,0.30802886655983325,0.31557974709591058,0.32311809985248224]
[null,null,null,null,"Coincident",0.26756999999999997,0.28700688574402616,0.29205882844508085,0.30025279955168199,0.30802886655983325,0.31557974709591058,0.32311809985248224]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.50089872455734974,0.50103650671434874,0.5045467476671297,0.50216141915377333,0.49991378844411399,0.4976808134204343,0.4957034548122809]
[null,null,null,null,"Coincident",0.4646017155314548,0.46472951347417851,0.46798538914052606,0.46577291051944186,0.46368815160033755,0.46161698636098247,0.45978291460849235]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52726181532352612,0.52740684917299874,0.53110183964961022,0.52859096753028778,0.52622504046748841,0.52387454044256243,0.52179311032871678]
[null,null,null,null,"Coincident",0.48905443740153137,0.48918896155176689,0.49261619909529064,0.49028727423099144,0.48809279115825005,0.48591261722208684,0.48398201537736041]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.47445894710427361,0.47083540453890388,0.46723953572866761,0.4636711293232883,0.46012997558661584,0.45661586638429913,0.45312859517155279]
[null,null,null,null,"Coincident",0.44007786398077547,0.43671689696362093,0.433381598357025,0.43007177212594855,0.42678722373251321,0.42352776012456728,0.42029318972433877]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.49943047063607754,0.49561621530410943,0.49183109024070276,0.48807487297188251,0.48434734272275354,0.4806482804045254,0.47697746860163454]
[null,null,null,null,"Coincident",0.46323985682186897,0.45970199680381152,0.45619115616528949,0.45270712855363004,0.44924970919211921,0.44581869486796555,0.44241388392035663]
[null,"Port Adelaide 11kV","Substation Rating","MVA","Non-Coincident",24.5,24.5,24.5,24.5,24.5,24.5,24.5]
[null,null,null,null,"Coincident",24.5,24.5,24.5,24.5,24.5,24.5,24.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.6962100000000002,2.8920687499043272,2.9429754226628972,3.0255432248728948,3.1038999525630224,3.1799875543501326,3.2559489180523267]
[null,null,null,null,"Coincident",2.6962100000000002,2.8920687499043272,2.9429754226628972,3.0255432248728948,3.1038999525630224,3.1799875543501326,3.2559489180523267]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.7604899650457604,9.6852966758296937,9.6128779009477565,9.6047413371864181,9.6007287612605445,9.5982586802686782,9.5990009035449173]
[null,null,null,null,"Coincident",8.6724673032393529,8.6056559705619264,8.5413098711802942,8.5340803075586287,8.5305150220408397,8.5283202862524696,8.5289797723149459]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.674049510583783,10.591818301409832,10.512621294768373,10.503723167241418,10.499335023382745,10.496633748457331,10.497445442135298]
[null,null,null,null,"Coincident",9.4841904151542131,9.4111256944874384,9.3407569473167342,9.332850713068872,9.3289517249778502,9.3265515669374643,9.32727277938762]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.4813327810823438,9.466871571305532,9.4524324181944905,9.4380152881077386,9.4236201474551073,9.4092469626976598,9.3948957003476146]
[null,null,null,null,"Coincident",8.4244283667661719,8.4115791789278749,8.3987495890517092,8.3859395672462806,8.3731490836657887,8.360378108509952,8.3476266120239462]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.368763852432227,10.352949106482647,10.337158481652326,10.321391941151017,10.305649448244587,10.289930966254934,10.274236458559896]
[null,null,null,null,"Coincident",9.2129356013130241,9.198883758869874,9.1848533487133039,9.1708443381541542,9.1568566945531256,9.1428903853206975,9.1289453779170628]
[null,"Port Adelaide North 11kV","Substation Rating","MVA","Non-Coincident",47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784]
[null,null,null,null,"Coincident",47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784,47.192079207920784]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.0953400000000002,3.276607101963966,3.3237211831376769,3.4001376119643245,3.4726566950009885,3.5430757039963736,3.6133778797544314]
[null,null,null,null,"Coincident",3.0953400000000002,3.276607101963966,3.3237211831376769,3.4001376119643245,3.4726566950009885,3.5430757039963736,3.6133778797544314]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.533958231346904,18.64591526077216,18.700170490059129,18.70151364237304,18.706381763962906,18.711917101747474,18.723630282137957]
[null,null,null,null,"Coincident",11.366080250601868,11.434738686386741,11.468011087370549,11.468834784974597,11.471820194781257,11.475214779612424,11.482397969875732]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.188271605364367,20.310221751682494,20.369319721537856,20.370782761617161,20.37608540445456,20.382114818205658,20.39487349954798]
[null,null,null,null,"Coincident",12.38059956342326,12.45538634843285,12.491628594133374,12.492525813752822,12.495777696770894,12.499475277163794,12.507299628239723]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.112793468534292,18.203257212089063,18.294172773797239,18.385542410249535,18.477368389307131,18.569652990157966,18.662398503373311]
[null,null,null,null,"Coincident",11.107797997393943,11.163275524438024,11.219030132142704,11.275063204378112,11.331376131926071,11.387970312514613,11.444847150852683]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.729514306133527,19.828052708050983,19.927083256734026,20.026608410193287,20.126630638715838,20.22715242492653,20.328176263849592]
[null,null,null,null,"Coincident",12.099263422836298,12.159692790917294,12.220423971463976,12.281458471868655,12.342797807052252,12.404443499501916,12.466397079308809]
[null,"Port Augusta 11kV","Substation Rating","MVA","Non-Coincident",28.4,28.4,28.4,28.4,28.4,28.4,28.4]
[null,null,null,null,"Coincident",28.4,28.4,28.4,28.4,28.4,28.4,28.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.0415600000000005,4.3351479954689482,4.4114559879302648,4.5352233230784318,4.6526783493424517,4.7667320053554159,4.8805964332316716]
[null,null,null,null,"Coincident",4.0415600000000005,4.3351479954689482,4.4114559879302648,4.5352233230784318,4.6526783493424517,4.7667320053554159,4.8805964332316716]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.840165290971754,13.721833871017706,13.613080724936058,13.518171611078646,13.432268642041523,13.348024437030034,13.268794942517241]
[null,null,null,null,"Coincident",13.619407303295878,13.502963332342523,13.395944856705748,13.302549593625894,13.218016822572778,13.135116357378026,13.057150615385922]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.892357393863659,13.77357973894668,13.664416478153914,13.569149456270718,13.482922541926262,13.398360646907209,13.318832373164344]
[null,null,null,null,"Coincident",13.670766914424515,13.553883826192909,13.446461777392495,13.352714315109971,13.267862765849241,13.184649677971287,13.106389922436529]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.520679404079784,12.39716741079512,12.274873818844187,12.153786609136606,12.033893881146,11.915183851740395,11.797644854024171]
[null,null,null,null,"Coincident",12.320967917152494,12.199426005764838,12.07908306156248,11.959927257165916,11.841946881868484,11.725130340485427,11.609466152214305]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.567895645648848,12.443917881144955,12.321163112640134,12.199619275719288,12.079274424978431,11.960116732850686,11.842134488443858]
[null,null,null,null,"Coincident",12.367431034589348,12.245430781280808,12.124634016535552,12.005028868372314,11.886603581922646,11.769346518275645,11.653246153334068]
[null,"Port Augusta West TF1 11kV","Substation Rating","MVA","Non-Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,null,null,"Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.7904599999999999,1.9205230356514149,1.9543283999618024,2.009158827541595,2.0611928258800281,2.1117199760262517,2.1621632958174515]
[null,null,null,null,"Coincident",1.7904599999999999,1.9205230356514149,1.9543283999618024,2.009158827541595,2.0611928258800281,2.1117199760262517,2.1621632958174515]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5325166723610275,5.4970809210777576,5.4757947117908232,5.4453750526731994,5.4186287438228815,5.3925493136213865,5.3684338396956957]
[null,null,null,null,"Coincident",5.2437427201237714,5.2101565650648896,5.189981405802377,5.1611495241302308,5.1357992593900104,5.1110810650559104,5.0882243167930605]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.7733695471948154,5.7363911340319875,5.7141782497787252,5.6824342996044566,5.6545236155232477,5.6273088420213995,5.6021435237722379]
[null,null,null,null,"Coincident",5.4720240943743033,5.4369757978561903,5.415922332138158,5.3858352817970596,5.3593814172844283,5.3335871397645676,5.3097353446081472]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.0259460929621573,5.0119313748733276,4.9979557364561611,4.9840190687380241,4.9701212630501512,4.9562622110267949,4.9424418046043854]
[null,null,null,null,"Coincident",4.763612980755429,4.7503297716292785,4.7370836023813467,4.7238743697269099,4.7107019706692537,4.6975663024988625,4.6844672627926274]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2447458972712857,5.2301210617003804,5.2155370070976428,5.2009936197464155,5.1864907862471448,5.1720283935164799,5.1576063287864073]
[null,null,null,null,"Coincident",4.970992361416358,4.9571308803581884,4.9433080516742649,4.9295237675834604,4.9157779206051959,4.9020704035585956,4.8884011095616557]
[null,"Port Augusta West TF2 11kV","Substation Rating","MVA","Non-Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,null,null,"Coincident",14.8,14.8,14.8,14.8,14.8,14.8,14.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8813199999999999,2.0179833101167968,2.0535041863075065,2.111117079091716,2.1657916329795777,2.2188828710486175,2.2718860246457822]
[null,null,null,null,"Coincident",1.8813199999999999,2.0179833101167968,2.0535041863075065,2.111117079091716,2.1657916329795777,2.2188828710486175,2.2718860246457822]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8872718772592592,1.7578902929582854,1.6771853980196949,1.6315423174959947,1.5893622215631744,1.5488000619559452,1.5092536636989253]
[null,null,null,null,"Coincident",1.8872718772592592,1.7578902929582854,1.6771853980196949,1.6315423174959947,1.5893622215631744,1.5488000619559452,1.5092536636989253]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9323955170188662,1.799920489705324,1.7172859848096698,1.6705516031608445,1.6273630041729887,1.5858310254845542,1.5453390944454048]
[null,null,null,null,"Coincident",1.9323955170188665,1.7999204897053243,1.71728598480967,1.6705516031608445,1.627363004172989,1.5858310254845545,1.5453390944454051]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7570632263639059,1.6334768155768986,1.5185830919408383,1.4117706386387541,1.3124710440277465,1.2201558767876171,1.1343338738282174]
[null,null,null,null,"Coincident",1.7570632263639059,1.6334768155768986,1.5185830919408383,1.4117706386387541,1.3124710440277465,1.2201558767876171,1.1343338738282174]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7990736484004157,1.6725323540342423,1.5548915842208593,1.4455253035011577,1.3438515098203216,1.2493291373539157,1.1614551771796331]
[null,null,null,null,"Coincident",1.7990736484004159,1.6725323540342425,1.5548915842208595,1.4455253035011577,1.3438515098203219,1.2493291373539157,1.1614551771796331]
[null,"Port Broughton 11kV","Substation Rating","MVA","Non-Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,null,null,"Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8706400000000001,2.0065274909302433,2.0418467198957511,2.0991325520550079,2.1534967258716842,2.2062865721399794,2.2589888339800703]
[null,null,null,null,"Coincident",1.8706400000000001,2.0065274909302433,2.0418467198957511,2.0991325520550079,2.1534967258716842,2.2062865721399794,2.2589888339800703]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9550303108420946,2.8461789368424526,2.7692790929781594,2.7383443770020097,2.7055547735966781,2.6776452697400428,2.6498989225413521]
[null,null,null,null,"Coincident",2.8726737925571793,2.7668560998501617,2.6920994500418076,2.6620268827524516,2.6301511236357888,2.6030194559848461,2.576046397825535]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2119894683066246,3.0936727574374485,3.0100859706284342,2.9764612793500103,2.9408204060833456,2.9104839888478726,2.8803249158058173]
[null,null,null,null,"Coincident",3.1224715136491077,3.0074522824458279,2.9261950543932689,2.8935074812526644,2.8588599169954225,2.8293689738965715,2.8000504324190598]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.620446180742146,2.5432363652467034,2.4683014889019486,2.3955745220419491,2.3249904099881542,2.2564860148576202,2.1900000590858206]
[null,null,null,null,"Coincident",2.5474145021813168,2.4723565196326613,2.3995100738164266,2.3288100031794663,2.2601930661132359,2.1935978843838182,2.1289648882287509]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8483110660240718,2.7643873535290253,2.6829364009803789,2.6038853500455965,2.5271634891175587,2.4527021900626305,2.3804348468324137]
[null,null,null,null,"Coincident",2.7689288067188227,2.6873440430789794,2.6081631237135072,2.531315220847246,2.4567315936013432,2.3843455265041502,2.3140922698138597]
[null,"Port Clinton 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.36825999999999998,0.39501123348691958,0.4019642865911181,0.41324175342116981,0.42394405351617964,0.43433642660066535,0.44471155754260605]
[null,null,null,null,"Coincident",0.36825999999999998,0.39501123348691958,0.4019642865911181,0.41324175342116981,0.42394405351617964,0.43433642660066535,0.44471155754260605]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.48614974824340634,0.46767934202269101,0.44567706400259283,0.43857296797026479,0.43186345993259984,0.42535080691957866,0.41725396276077709]
[null,null,null,null,"Coincident",0.26779435284594422,0.25761997653792307,0.24550007762854695,0.24158680439040014,0.23789088894592367,0.23430341059129337,0.22984328457161454]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.52274166477785622,0.50288101292762477,0.47922264946515353,0.4715838365271664,0.46436931175548368,0.45736645905331036,0.44866017501158822]
[null,null,null,null,"Coincident",0.28795091703864967,0.27701072746013233,0.26397857809521175,0.25977075740903238,0.25579665478056307,0.25193915117343374,0.24714331674367154]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.43178853660557537,0.40976118756919622,0.38885754623794705,0.36902028755630328,0.35019501086088967,0.33233009069493868,0.3153765352333312]
[null,null,null,null,"Coincident",0.23784961762171528,0.22571590840676067,0.21420119072429289,0.20327388721321793,0.19290403140642232,0.18306318555229675,0.17372436262852992]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.46428874903825301,0.44060342749375941,0.4181263938042441,0.39679600812505728,0.37655377511923616,0.35734418354294478,0.3391145540143346]
[null,null,null,null,"Coincident",0.25575227701259706,0.2427052778567319,0.23032386099386332,0.21857407227227732,0.20742368968432506,0.19684213500246961,0.18680038992315043]
[null,"Port Germein 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.66127999999999998,0.70931686438991526,0.72180237722526097,0.74205318715676749,0.76127117718236925,0.77993263504721666,0.79856313140654578]
[null,null,null,null,"Coincident",0.66127999999999998,0.70931686438991526,0.72180237722526097,0.74205318715676749,0.76127117718236925,0.77993263504721666,0.79856313140654578]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.90098594154029443,0.89119027422971087,0.85929406778042894,0.86016681088609181,0.86093812910053424,0.86149226024664305,0.85299276285298253]
[null,null,null,null,"Coincident",0.88914502713534449,0.87947809619323924,0.84800107525284873,0.84886234861638221,0.84962353003230751,0.85017037869023571,0.84178258317391119]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.90714066335301602,0.89727808089482919,0.86516398838481601,0.8660426932827574,0.8668192804462701,0.86737719691565074,0.85881963863602728]
[null,null,null,null,"Coincident",0.89521886252041982,0.88548589584125337,0.85379385233674809,0.854661009141646,0.85542739026119374,0.855977974495015,0.8475328811390187]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.78374923098200544,0.75834920625294433,0.73377235458834489,0.7099919983018157,0.68698232428694483,0.66471835599768359,0.64317592633679932]
[null,null,null,null,"Coincident",0.7734490618771046,0.74838284870362259,0.72412899031060096,0.70066115961445619,0.67795388274912372,0.65598251141467945,0.63472319612209838]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.78910309752445362,0.76352956277815909,0.73878482427087544,0.71484202207836378,0.69167516676239427,0.66925911115972447,0.64756952308535132]
[null,null,null,null,"Coincident",0.77873256697156357,0.7534951240797606,0.72907558524222615,0.70544744353253108,0.68258505107017653,0.6604635911803256,0.63905905145579489]
[null,"Port Giles 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.19594,0.21017352166791678,0.21387303077897055,0.21987342954799335,0.22556779950567604,0.23109726668151412,0.23661755983516605]
[null,null,null,null,"Coincident",0.19594,0.21017352166791678,0.21387303077897055,0.21987342954799335,0.22556779950567604,0.23109726668151412,0.23661755983516605]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7352756172987387,1.7304464387266512,1.7249256386789646,1.7140162587437211,1.7034988855058133,1.6929881056373794,1.6829855358310681]
[null,null,null,null,"Coincident",0.27016267095668983,0.269410822795766,0.26855129703983877,0.26685283070261523,0.26521539534821043,0.26357898650641831,0.26202170018926807]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0450422562599835,2.0393510138172886,2.0328446875176911,2.0199878578966435,2.0075930126732313,1.9952059378115128,1.9834177943482054]
[null,null,null,null,"Coincident",0.31838981235185371,0.31750375065418862,0.31649078967341299,0.31448912757672298,0.31255939119463477,0.3106308645694571,0.3087955847488224]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6049020677502153,1.5948672737268834,1.5848952231525844,1.5749855237182797,1.5651377855678781,1.5553516212828982,1.5456266458672279]
[null,null,null,null,"Coincident",0.24986499258386582,0.24830268932274829,0.24675015450279753,0.24520732704595968,0.24367414625607681,0.24215055181649908,0.2406364837877121]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8913955299028327,1.8795694098294555,1.8678172336317924,1.8561385389691338,1.8445328663915956,1.8329997593220453,1.8215387640381406]
[null,null,null,null,"Coincident",0.29446876513457276,0.29262757278781942,0.29079789266123712,0.28897965277363757,0.28717278159390108,0.28537720803816274,0.28359286146701596]
[null,"Port Julia 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.25358999999999998,0.27201134714589675,0.27679933589486133,0.28456518831823835,0.29193497130062457,0.29909133335595162,0.30623582218332018]
[null,null,null,null,"Coincident",0.25358999999999998,0.27201134714589675,0.27679933589486133,0.28456518831823835,0.29193497130062457,0.29909133335595162,0.30623582218332018]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.25021317242618052,0.23475639254102876,0.22909741299845029,0.22291746477196847,0.21718743652696729,0.21169328337843257,0.20632379954337149]
[null,null,null,null,"Coincident",0.21031585563840693,0.19732371035908802,0.19256707379596397,0.18737253872632437,0.18255618241105001,0.17793809012902426,0.17342478822666083]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.25795172415070156,0.24201689952683375,0.23618289999840233,0.2298118193525448,0.22390457373914152,0.21824049832828099,0.21270494798285719]
[null,null,null,null,"Coincident",0.21682046973031641,0.20342650552483299,0.19852275649068449,0.19316756569724161,0.18820224990829895,0.18344133002992191,0.17878844147078435]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.22080235916148974,0.20320592145782854,0.18701179947685564,0.1721082382475243,0.15839238890555929,0.14576959893766633,0.13415275898842322]
[null,null,null,null,"Coincident",0.18559469369154838,0.17080406610008828,0.15719215035753931,0.14466501119211045,0.133136199330641,0.12252615491571502,0.11276165846635121]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.22763129810462859,0.20949064067817372,0.1927956695637687,0.17743117345105597,0.16329112258305081,0.15027793704914053,0.13830181339012701]
[null,null,null,null,"Coincident",0.19133473576448284,0.17608666608256521,0.16205376325519516,0.14913918679599014,0.13725381374292886,0.12631562362444845,0.11624913243953731]
[null,"Port Lincoln City 11kV","Substation Rating","MVA","Non-Coincident",29,29,29,29,29,29,29]
[null,null,null,null,"Coincident",29,29,29,29,29,29,29]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.3896899999999999,6.8538514324092636,6.9744940596002873,7.1701697154665593,7.3558656365388542,7.5361840050127791,7.7162032045685525]
[null,null,null,null,"Coincident",6.3896899999999999,6.8538514324092636,6.9744940596002873,7.1701697154665593,7.3558656365388542,7.5361840050127791,7.7162032045685525]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.773854839856977,11.390670234741565,11.201987749434245,11.116361344294328,11.041817930503825,10.97231757464834,10.909800813313801]
[null,null,null,null,"Coincident",11.479530025853766,11.105924334285657,10.921958565648374,10.838472663861806,10.765792698932994,10.698029724724265,10.637075767959864]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.801682341917733,11.417592080113536,11.228463643813944,11.142634860693502,11.067915263568901,10.998250643645097,10.935586123965603]
[null,null,null,null,"Coincident",11.50666189131295,11.132173182815091,10.94777261114384,10.864089390455721,10.791237646453586,10.723314514477492,10.662216493056228]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.818828945888372,10.610230554532038,10.405654159372713,10.205022212097086,10.008258659604824,9.8152889151792877,9.6260398302141201]
[null,null,null,null,"Coincident",10.548378030657807,10.344994217158291,10.145531857314815,9.9499153413799171,9.7580705174415225,9.569924663314346,9.3854064589732626]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.844399244561286,10.63530783097525,10.430247919572917,10.229141778755567,10.031913175671384,9.8384873473180523,9.6487909722025051]
[null,null,null,null,"Coincident",10.573309118681085,10.369444607604924,10.169510818539237,9.9734319630329455,9.781133713915958,9.5925431771241279,9.4075888640674723]
[null,"Port Lincoln Docks 11kV","Substation Rating","MVA","Non-Coincident",12.3,12.3,12.3,12.3,12.3,12.3,12.3]
[null,null,null,null,"Coincident",12.3,12.3,12.3,12.3,12.3,12.3,12.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.2754300000000001,1.3680800997290552,1.3921612720548249,1.4312195991037926,1.468285896312771,1.5042787937307518,1.5402119747910881]
[null,null,null,null,"Coincident",1.2754300000000001,1.3680800997290552,1.3921612720548249,1.4312195991037926,1.468285896312771,1.5042787937307518,1.5402119747910881]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2626062154519389,5.1614969439822476,5.0866817237270983,5.029739447414455,4.9753059611526336,4.9217403272997542,4.8710282091617039]
[null,null,null,null,"Coincident",2.4102103394504542,2.3639035094248633,2.3296390385477204,2.3035601609912715,2.2786302790982731,2.254097863168623,2.2308723231096157]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3278883035705391,5.2255247820012842,5.1497814866439233,5.0921328472579797,5.0370241192050633,4.9827940091808447,4.9314528124400194]
[null,null,null,null,"Coincident",2.4401087504891477,2.3932274890061267,2.3585379708965744,2.3321355875498431,2.3068964530394349,2.2820597150167163,2.2585460645252238]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.1048853516711059,5.0303355352349826,4.9568744161442053,4.8844860954741831,4.8131549064822119,4.7428654112167772,4.6736023971763734]
[null,null,null,null,"Coincident",2.3379760811630947,2.3038331620423547,2.2701888532091528,2.2370358731472848,2.2043670466770564,2.1721753034023878,2.1404536761805897]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.1682109287178246,5.09273632948653,5.0183639327790299,4.9450776424462068,4.8728615974010312,4.8017001681857874,4.7315779535894551]
[null,null,null,null,"Coincident",2.3669784336669788,2.332411975150849,2.2983503121315239,2.2647860727663396,2.2317119928682376,2.1991209143336028,2.1670057835930581]
[null,"Port Lincoln Marina 11kV","Substation Rating","MVA","Non-Coincident",16.8,16.8,16.8,16.8,16.8,16.8,16.8]
[null,null,null,null,"Coincident",16.8,16.8,16.8,16.8,16.8,16.8,16.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.0230299999999999,2.169987442787821,2.2081839208777212,2.2701364916733535,2.328929393865304,2.3860197173354258,2.4430153213909147]
[null,null,null,null,"Coincident",2.0230299999999999,2.169987442787821,2.2081839208777212,2.2701364916733535,2.328929393865304,2.3860197173354258,2.4430153213909147]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.2634963814455302,5.1426134183670529,5.0553297755604181,5.0396160802662804,5.027290581707315,5.0162596753433579,5.0081304290645772]
[null,null,null,null,"Coincident",5.0519979149901415,4.9359722861736968,4.8521958855616836,4.8371135999268686,4.8252833660844727,4.814695704972439,4.806893109079029]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6728895694419066,5.5426043653352792,5.4485318266695133,5.4315959248142871,5.4183117526317419,5.4064228656413045,5.3976613289971667]
[null,null,null,null,"Coincident",5.4449408149719307,5.3198907471461059,5.2295982429330117,5.2133428615932056,5.2005924756700459,5.1891813094158099,5.1807718299271706]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8011180156629703,4.7625483884965982,4.7242886091895997,4.6863361885891619,4.648688657539001,4.6113435667187197,4.5742984864844587]
[null,null,null,null,"Coincident",4.6081988942281065,4.5711790766191607,4.5344566565243536,4.4980292448103203,4.4618944715367217,4.4260499858020586,4.3904934555907218]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.1745475514574446,5.1329779901254229,5.091742376527411,5.0508380279050282,5.0102622830517483,4.9700125021397579,4.9300860665482205]
[null,null,null,null,"Coincident",4.9666232379551758,4.9267240299084607,4.8871453508663594,4.8478846258694217,4.8089393006440542,4.7703068414363328,4.7319847348471686]
[null,"Port Noarlunga 11kV","Substation Rating","MVA","Non-Coincident",63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049]
[null,null,null,null,"Coincident",63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049,63.090271877655049]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.81442,12.672646003183981,12.89571201539086,13.25751272593857,13.60086108929187,13.934266456197888,14.267118665243354]
[null,null,null,null,"Coincident",11.81442,12.672646003183981,12.89571201539086,13.25751272593857,13.60086108929187,13.934266456197888,14.267118665243354]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.154773560759963,30.443076645660376,30.558976961049197,30.740645919563569,30.929107044063425,31.120457044612877,31.275025341394905]
[null,null,null,null,"Coincident",30.154773560759963,30.443076645660376,30.558976961049197,30.740645919563569,30.929107044063425,31.120457044612877,31.275025341394905]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.568187851567824,30.86044349857724,30.97793277786905,31.162092371688466,31.353137250364853,31.54711061084814,31.703797999742292]
[null,null,null,null,"Coincident",30.568187851567824,30.86044349857724,30.97793277786905,31.162092371688466,31.353137250364853,31.54711061084814,31.703797999742292]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.103055857085682,27.17932574064108,27.255810252951562,27.332509997997366,27.409425581458375,27.486557610718894,27.56390669487245]
[null,null,null,null,"Coincident",27.103055857085682,27.17932574064108,27.255810252951562,27.332509997997366,27.409425581458375,27.486557610718894,27.56390669487245]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.4746318728467,27.551947397144733,27.6294804927036,27.707231771783952,27.785201848369393,27.863391338171308,27.941800858633748]
[null,null,null,null,"Coincident",27.4746318728467,27.551947397144733,27.6294804927036,27.707231771783952,27.785201848369393,27.863391338171308,27.941800858633748]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Port Pirie South 11kV","Substation Rating","MVA","Non-Coincident",40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844]
[null,null,null,null,"Coincident",40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844,40.509658862242844]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",9.968770000000001,10.69292384197958,10.881142457070931,11.186422620573389,11.47613306460242,11.757453808189638,12.038307808298502]
[null,null,null,null,"Coincident",9.968770000000001,10.69292384197958,10.881142457070931,11.186422620573389,11.47613306460242,11.757453808189638,12.038307808298502]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.666685187996499,22.377975486915268,22.133208254132725,22.117592638849256,22.074609532808061,22.064087641311392,22.053451486542492]
[null,null,null,null,"Coincident",20.564756343840305,20.302819293601363,20.080749835214274,20.066582288402721,20.027585095151601,20.018038920529651,20.008389078506276]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.353805850306305,23.056344168096079,22.804157031533766,22.788068042581983,22.74378194141617,22.732941088015988,22.721982507552788]
[null,null,null,null,"Coincident",21.188158878530391,20.918281436568932,20.689480137506411,20.674883113951008,20.634703755022255,20.624868196497264,20.614925827984582]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.558454960648085,20.364602790625828,20.172578513988277,19.98236489495094,19.793944860250985,19.60730149761477,19.422418054239831]
[null,null,null,null,"Coincident",18.652026688729613,18.476150833474712,18.301933367250555,18.129358652582773,17.958411199447699,17.789075663881988,17.621336846605377]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.18166647443871,20.98193784606574,20.784092522060728,20.588112744151495,20.393980921514231,20.201679629194579,20.011191606543569]
[null,null,null,null,"Coincident",19.217446503117252,19.036239125712342,18.85674040994574,18.678934244306763,18.502804669205283,18.328335875539171,18.155512203275332]
[null,"Port Stanvac 11kV","Substation Rating","MVA","Non-Coincident",59,59,59,59,59,59,59]
[null,null,null,null,"Coincident",59,59,59,59,59,59,59]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.378450000000001,12.205006163225006,12.419840701576899,12.768290417680744,13.098968706161884,13.42007090983094,13.740640368002682]
[null,null,null,null,"Coincident",11.378450000000001,12.205006163225006,12.419840701576899,12.768290417680744,13.098968706161884,13.42007090983094,13.740640368002682]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.370785738199814,31.977795896214932,31.709832996962149,31.532935377811437,31.371603499653247,31.216882772149713,31.037180901699177]
[null,null,null,null,"Coincident",31.843331588856078,31.456745178795316,31.193148504824308,31.019133280434868,30.860430166658372,30.70823048051513,30.531456697692139]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.37777819085229,31.984703458655435,31.716682676412084,31.539746845392305,31.378380117739621,31.223625968824255,31.043885280754928]
[null,null,null,null,"Coincident",31.850210105498611,31.463540188438969,31.199886574631005,31.025833761002083,30.867096365573673,30.7148638025918,30.538051834649774]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.622282514632175,29.303369919683483,28.987890728057668,28.675807975838708,28.367085097062983,28.061685919434925,27.759574660088802]
[null,null,null,null,"Coincident",29.139612864542798,28.825896676404987,28.515557947231965,28.208560315402973,27.904867810765353,27.604444850420027,27.307256234552327]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.62868125977284,29.309699776128074,28.994152437459793,28.682002271867361,28.373212705488498,28.067747558214016,27.76557103944868]
[null,null,null,null,"Coincident",29.145907347627475,28.832123393275719,28.521717627457758,28.214653680698312,27.910895575074765,27.610407720001739,27.313154908061009]
[null,"Port Vincent 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.72328999999999999,0.77583141006015877,0.78948772293621305,0.8116375056536087,0.83265761817117689,0.85306901101394472,0.87344653900774338]
[null,null,null,null,"Coincident",0.72328999999999999,0.77583141006015877,0.78948772293621305,0.8116375056536087,0.83265761817117689,0.85306901101394472,0.87344653900774338]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5278703386881158,1.5115217342628324,1.4898387752681062,1.4839547247053919,1.4787984899945568,1.4738910761009236,1.4695332545614808]
[null,null,null,null,"Coincident",1.4475451133558686,1.4320560094399388,1.411512995716103,1.4059382892615557,1.4010531349588717,1.3964037201354629,1.3922750037682652]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5751240605032122,1.5582698291369408,1.5359162631629961,1.5298502316550433,1.5245345257675844,1.5194753361865192,1.5149827366613204]
[null,null,null,null,"Coincident",1.492314549851411,1.4763464014844732,1.4551680368207247,1.4494209167644905,1.4443846752153318,1.4395914640571783,1.4353350554312012]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3324732009320264,1.3151739490385483,1.2980992901168951,1.2812463083182595,1.2646121256497578,1.2481939014829531,1.2319888320687591]
[null,null,null,null,"Coincident",1.2624206530136299,1.2460308803287188,1.2298538930161176,1.213886928522889,1.1981272601618072,1.1825721966457199,1.1672190816279555]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3736837123010581,1.3558494319985037,1.33824669084216,1.3208724828023295,1.303723840876039,1.2867978365803641,1.2700915794523291]
[null,null,null,null,"Coincident",1.301464590735701,1.2845679178646585,1.2678906113568222,1.2514298232194734,1.2351827424348527,1.2191465944801236,1.2033186408535623]
[null,"Portee 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.7239999999999998E-2,1.849235231986774E-2,1.8817857765792853E-2,1.934580956112792E-2,1.9846835069295979E-2,2.033335142180924E-2,2.0819060587722066E-2]
[null,null,null,null,"Coincident",1.7239999999999998E-2,1.849235231986774E-2,1.8817857765792853E-2,1.934580956112792E-2,1.9846835069295979E-2,2.033335142180924E-2,2.0819060587722066E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.59492048176798196,0.60042051703856425,0.60597140009284989,0.61157360101820746,0.6172275942479597,0.62293385860156181,0.628692877325151]
[null,null,null,null,"Coincident",0.2570788198548557,0.26020767084207824,0.2613296101777462,0.26095248875383814,0.26056061431622923,0.26013439092585644,0.25979571142629798]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.62554460666628986,0.63132776173562377,0.63716438202901937,0.64305496183206112,0.64900000000000002,0.65500000000000003,0.66105546995377507]
[null,null,null,null,"Coincident",0.27031220839873016,0.2736021201097929,0.2747818123912692,0.27438527826609849,0.27397323170113885,0.27352506803682797,0.273168954672387]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.54101660605813007,0.54279309583338597,0.5445754189155797,0.54636359445904026,0.54815764168099235,0.54995757986176241,0.55176342834498604]
[null,null,null,null,"Coincident",0.23500408825650024,0.23577575100262702,0.2365499475914549,0.23732668634314558,0.23810597560518101,0.23888782375245302,0.23967223918735328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.56886597521540905,0.57073391157289777,0.57260798151261449,0.5744882051748762,0.57637460276613361,0.57826719455918696,0.58016600089340498]
[null,null,null,null,"Coincident",0.2471011579841933,0.24791254283947747,0.24872659196954186,0.24954331412283681,0.2503627180765392,0.25118481263664677,0.2520096066380727]
[null,"Prospect 11kV","Substation Rating","MVA","Non-Coincident",49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271]
[null,null,null,null,"Coincident",49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271,49.420722891566271]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.2907600000000015,7.8203771809512155,7.9580327543231988,8.1813024661188543,8.3931851072981676,8.5989318568486084,8.8043372488712652]
[null,null,null,null,"Coincident",7.2907600000000015,7.8203771809512155,7.9580327543231988,8.1813024661188543,8.3931851072981676,8.5989318568486084,8.8043372488712652]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.409720107906058,28.282251346521043,28.300993739745643,28.277142728264341,28.25289728169345,28.235370465836379,28.229422953897505]
[null,null,null,null,"Coincident",26.501754817135232,26.382846716378214,26.400330391262656,26.378081187257223,26.35546403798531,26.339114303640695,26.333566220006734]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.270843648156749,30.135024395758123,30.154994604994229,30.129581111420247,30.103747343275419,30.085072343998963,30.078735209971828]
[null,null,null,null,"Coincident",28.237887364755668,28.111189582699264,28.129818614833756,28.106111863299905,28.082013062369214,28.064592255330112,28.058680716195173]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.62322571457829,25.658928097618624,25.694680226938715,25.730482171853055,25.766334001772709,25.802235786205458,25.838187594755929]
[null,null,null,null,"Coincident",23.902398296521575,23.93570294711752,23.96905400308825,24.002451529093175,24.03589558988179,24.069386250293807,24.102923575259286]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.30180573484704,27.339846984488911,27.377941239294188,27.416088573118159,27.454289059919017,27.492542773758007,27.530849788799557]
[null,null,null,null,"Coincident",25.468246744487264,25.503733185998026,25.539269072904208,25.57485447410107,25.610489458579845,25.646174095427906,25.681908453828886]
[null,"Punyelroo 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15765000000000001,0.16910205007118037,0.17207861234206751,0.17690643139859727,0.18148802486511087,0.18593694035082522,0.19037847457392018]
[null,null,null,null,"Coincident",0.15765000000000001,0.16910205007118037,0.17207861234206751,0.17690643139859727,0.18148802486511087,0.18593694035082522,0.19037847457392018]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.49029786623848226,0.48276818791226411,0.47524717933822347,0.47480671956884418,0.47457311724274759,0.47438982922654016,0.47435652856461086]
[null,null,null,null,"Coincident",0.24898795444325608,0.24516415806730191,0.24134476445140207,0.24112108577657188,0.24100245551253624,0.24090937636336604,0.24089246528896346]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.50599170116352155,0.49822100704501188,0.49045926018684133,0.49000470183905137,0.48976362218825825,0.48957446734686522,0.48954010077148369]
[null,null,null,null,"Coincident",0.25695775428214629,0.25301156286178456,0.24906991512844068,0.24883907677285158,0.24871664929918261,0.24862059080030963,0.24860313842310247]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.4372802056999619,0.434577223402275,0.43189094918605708,0.42922127977279739,0.4265681125223858,0.42393134542916672,0.42131087711801735]
[null,null,null,null,"Coincident",0.22206399707805671,0.22069134163829179,0.21932717106316546,0.21797143290475393,0.2166240750393324,0.21528504566537102,0.21395429330154347]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.45127701016678867,0.44848750871226628,0.44571525014446195,0.44296012787904615,0.4402220359905244,0.43750086920816489,0.43479652291195109]
[null,null,null,null,"Coincident",0.22917199397731775,0.2277554015160726,0.22634756550960372,0.22494843183119345,0.22355794668870033,0.2221760566224909,0.22080270850338454]
[null,"Pyap 11kV","Substation Rating","MVA","Non-Coincident",15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319]
[null,null,null,null,"Coincident",15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319,15.169945987654319]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.5816599999999998,3.8418398265648195,3.9094645269970782,4.019148043660639,4.1232375460727742,4.224312729317707,4.3252202172053718]
[null,null,null,null,"Coincident",3.5816599999999998,3.8418398265648195,3.9094645269970782,4.019148043660639,4.1232375460727742,4.224312729317707,4.3252202172053718]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.5318112248315643,8.4788327008009006,8.471532658269755,8.4721973761271148,8.4753760054569955,8.4808887938314754,8.5046516213314227]
[null,null,null,null,"Coincident",8.417613573886646,8.3653441634117556,8.3581418314003209,8.3587976520592022,8.361933735674798,8.3673727357919052,8.3908174996347]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6533421283573499,8.5996089547308117,8.5922049271557857,8.592879113549154,8.5961030206851472,8.6016943356625308,8.6257956514178193]
[null,null,null,null,"Coincident",8.5375177954179389,8.4845038362752003,8.47719891105187,8.4778640735111175,8.4810448288928004,8.4865613045401425,8.5103400259984632]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8658012581492498,7.8198722741029218,7.7742114727256313,7.7288172880793224,7.6836881633695659,7.6388225508921677,7.5942189119800902]
[null,null,null,null,"Coincident",7.7605181004692154,7.7152038724166809,7.6701542374283473,7.6253676505261243,7.5808425757531568,7.5365774861211552,7.4925708635580248]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9778452202888372,7.9312620034211232,7.8849507893353392,7.838909989787517,7.7931380258075533,7.7476333276450733,7.7023943347155805]
[null,null,null,null,"Coincident",7.8710623626105596,7.8251026585936989,7.7794113166220109,7.7339867697100511,7.6888274600221145,7.6439318388188129,7.5992983664039597]
[null,"Qualco 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.14080999999999999,0.15103875464968541,0.15369736380517934,0.15800948052798275,0.16210167320809554,0.16607536042372156,0.17004245483510122]
[null,null,null,null,"Coincident",0.14080999999999999,0.15103875464968541,0.15369736380517934,0.15800948052798275,0.16210167320809554,0.16607536042372156,0.17004245483510122]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7710425387157671,2.7742622391030403,2.7774856804904746,2.7807128672247732,2.78394380365769,2.7871784941460351,2.7904169430516808]
[null,null,null,null,"Coincident",2.7710425387157671,2.7742622391030403,2.7774856804904746,2.7807128672247732,2.78394380365769,2.7871784941460351,2.7904169430516808]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9533442724645877,2.9567757909508439,2.9602112965507024,2.9636507938968282,2.9670942876272686,2.9705417823854607,2.9739932828202358]
[null,null,null,null,"Coincident",2.9533442724645877,2.9567757909508439,2.9602112965507024,2.9636507938968282,2.9670942876272686,2.9705417823854607,2.9739932828202358]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4939382848441904,2.4968360151927365,2.4997371124414274,2.5026415805022961,2.5055494232919209,2.5084606447314317,2.5113752487465129]
[null,null,null,null,"Coincident",2.4939382848441904,2.4968360151927365,2.4997371124414274,2.5026415805022961,2.5055494232919209,2.5084606447314317,2.5113752487465129]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6580098452181291,2.6610982118557596,2.6641901668956325,2.6672857145071456,2.6703848588645416,2.6734876041469149,2.6765939545382125]
[null,null,null,null,"Coincident",2.6580098452181291,2.6610982118557596,2.6641901668956325,2.6672857145071456,2.6703848588645416,2.6734876041469149,2.6765939545382125]
[null,"Queenstown 7.6kV","Substation Rating","MVA","Non-Coincident",22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401]
[null,null,null,null,"Coincident",22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401,22.700644699140401]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.88375,5.2385165685704225,5.3307258041584022,5.4802840744871508,5.6222146618140512,5.7600350931705853,5.8976268645758507]
[null,null,null,null,"Coincident",4.88375,5.2385165685704225,5.3307258041584022,5.4802840744871508,5.6222146618140512,5.7600350931705853,5.8976268645758507]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.377010295417271,14.849285180230547,14.797548571988886,14.853002244277413,14.914519461067007,14.978330044435138,15.047323434232549]
[null,null,null,null,"Coincident",10.922026771063178,14.255440230634102,14.205772646129319,14.259008643773885,14.318065695777072,14.379324399226133,14.445558640984467]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.844509807164581,15.459466009050807,15.40560346100032,15.463335813192119,15.527380870606484,15.593813532692511,15.665641970996214]
[null,null,null,null,"Coincident",11.370830283601075,14.841219022646698,14.789510517820782,14.844934067577896,14.906417868108141,14.9701937894562,15.039149701924057]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.693837610339189,14.240881265737295,14.303528851687448,14.366452032943267,14.429652021886223,14.493130036231223,14.556887299050064]
[null,null,null,null,"Coincident",10.266175175439017,13.671367291507767,13.731509507531397,13.791916297395456,13.852588824996484,13.913528259351157,13.974735774618818]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.133264466052974,14.826061806644892,14.891283681892793,14.956792477097341,15.022589454458704,15.08867588172963,15.155053032239895]
[null,null,null,null,"Coincident",10.688028699115911,14.233145594219904,14.295759149892209,14.35864815116633,14.421813809765171,14.485257342742171,14.548979972504757]
[null,"Quorn 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0751599999999999,1.1532620371362527,1.1735619463729607,1.2064872742309916,1.237733363869157,1.2680746006190502,1.2983654977665464]
[null,null,null,null,"Coincident",1.0751599999999999,1.1532620371362527,1.1735619463729607,1.2064872742309916,1.237733363869157,1.2680746006190502,1.2983654977665464]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8914103773143083,1.8737159804949948,1.8421201080974325,1.8281880627474723,1.8019308511717163,1.7752299084605758,1.7493880774729988]
[null,null,null,null,"Coincident",1.6068619134705628,1.5918295055532699,1.5649869944898542,1.5531509205642242,1.5308439089600421,1.5081599222319937,1.4862058003310432]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9287446843727534,1.9107010201221148,1.8784814808482266,1.8642744326404592,1.8374989333302032,1.8102709441325446,1.7839190245546679]
[null,null,null,null,"Coincident",1.6385795548653481,1.62325042417454,1.5958780722250421,1.5838083675529564,1.5610610407053054,1.5379292976701264,1.5155418261703373]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6516204246302819,1.5952339339508261,1.5407724838459056,1.4881703532328823,1.4373640647536197,1.3882923081734979,1.3408958663955945]
[null,null,null,null,"Coincident",1.4031465554381155,1.355242988135215,1.3089748535328047,1.2642863177907673,1.2211234532420132,1.179434173315538,1.139168169681213]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6842215485411611,1.6267220521479668,1.5711855944585196,1.5175451571301533,1.4657360098332934,1.4156956321384555,1.36736363807003]
[null,null,null,null,"Coincident",1.4308430854862959,1.3819939558071221,1.3348125404249371,1.2892419034026081,1.2452270526017359,1.2027148733211659,1.1616540642010873]
[null,"Ramco 11kV","Substation Rating","MVA","Non-Coincident",8.4,8.4,8.4,8.4,8.4,8.4,8.4]
[null,null,null,null,"Coincident",8.4,8.4,8.4,8.4,8.4,8.4,8.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.5705899999999997,2.7573234309703487,2.805858294325374,2.884579153117159,2.9592851369362849,3.0318277164378546,3.1042499394543195]
[null,null,null,null,"Coincident",2.5705899999999997,2.7573234309703487,2.805858294325374,2.884579153117159,2.9592851369362849,3.0318277164378546,3.1042499394543195]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0790280247846438,6.1282305777446382,6.1416192224889876,6.1344133973200767,6.1274438171622618,6.1199804241008868,6.1146102943485978]
[null,null,null,null,"Coincident",6.0790280247846438,6.1282305777446382,6.1416192224889876,6.1344133973200767,6.1274438171622618,6.1199804241008868,6.1146102943485978]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5506619315623293,6.6036818040315195,6.6181091902986076,6.6103443100534385,6.6028340035977635,6.5947915723722277,6.5890048077130672]
[null,null,null,null,"Coincident",6.5506619315623293,6.6036818040315195,6.6181091902986076,6.6103443100534385,6.6028340035977635,6.5947915723722277,6.5890048077130672]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5294154163224958,5.5388468924392891,5.5482944557434335,5.5577581336747048,5.5672379537196832,5.576733943411833,5.586246130331582]
[null,null,null,null,"Coincident",5.5294154163224958,5.5388468924392891,5.5482944557434335,5.5577581336747048,5.5672379537196832,5.576733943411833,5.586246130331582]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9584083053772101,5.9685715109595545,5.9787520518338786,5.988949957568841,5.9991652577835328,6.0093979821475694,6.0196481603811716]
[null,null,null,null,"Coincident",5.9584083053772101,5.9685715109595545,5.9787520518338786,5.988949957568841,5.9991652577835328,6.0093979821475694,6.0196481603811716]
[null,"Rapid Bay 11kV","Substation Rating","MVA","Non-Coincident",0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003]
[null,null,null,null,"Coincident",0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003,0.40950000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.9000000000000001E-2,3.1106625132028103E-2,3.1654169095591232E-2,3.2542255062222143E-2,3.3385047390347068E-2,3.420343336615244E-2,3.5020461545472163E-2]
[null,null,null,null,"Coincident",2.9000000000000001E-2,3.1106625132028103E-2,3.1654169095591232E-2,3.2542255062222143E-2,3.3385047390347068E-2,3.420343336615244E-2,3.5020461545472163E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.9440641386376081E-2,6.9468803896213405E-2,6.9496977827704462E-2,6.9525163185481437E-2,6.95533599741784E-2,6.9581568198431296E-2,6.960978786287797E-2]
[null,null,null,null,"Coincident",6.9440641386376081E-2,6.9468803896213405E-2,6.9496977827704462E-2,6.9525163185481437E-2,6.95533599741784E-2,6.9581568198431296E-2,6.960978786287797E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.9809115974309624E-2,6.9837427923567438E-2,6.9865751355085992E-2,6.9894086273522046E-2,6.9922432683534264E-2,6.9950790589783179E-2,6.9979159996931273E-2]
[null,null,null,null,"Coincident",6.9809115974309624E-2,6.9837427923567438E-2,6.9865751355085992E-2,6.9894086273522046E-2,6.9922432683534264E-2,6.9950790589783179E-2,6.9979159996931273E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.2496577247738473E-2,6.2521923506592067E-2,6.2547280044934012E-2,6.2572646866933299E-2,6.2598023976760564E-2,6.2623411378588165E-2,6.2648809076590178E-2]
[null,null,null,null,"Coincident",6.2496577247738473E-2,6.2521923506592067E-2,6.2547280044934012E-2,6.2572646866933299E-2,6.2598023976760564E-2,6.2623411378588165E-2,6.2648809076590178E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.2828204376878666E-2,6.2853685131210701E-2,6.2879176219577393E-2,6.2904677646169846E-2,6.2930189415180846E-2,6.295571153080487E-2,6.2981243997238145E-2]
[null,null,null,null,"Coincident",6.2828204376878666E-2,6.2853685131210701E-2,6.2879176219577393E-2,6.2904677646169846E-2,6.2930189415180846E-2,6.295571153080487E-2,6.2981243997238145E-2]
[null,"Renmark 11kV","Substation Rating","MVA","Non-Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,null,null,"Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.7714399999999983,9.4086171016578106,9.5742291369597474,9.8428426807923355,10.097756554537442,10.345288398800141,10.592409559255733]
[null,null,null,null,"Coincident",8.7714399999999983,9.4086171016578106,9.5742291369597474,9.8428426807923355,10.097756554537442,10.345288398800141,10.592409559255733]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.98105402243165,18.602170818818635,18.628758109012349,18.577703946630756,18.540409839768355,18.512587543038261,18.524657435332834]
[null,null,null,null,"Coincident",18.39184509464657,18.024723164453501,18.050485133317366,18.001015791685994,17.964879366619932,17.937920728230701,17.949615947533513]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.080695232927066,18.699823078595102,18.726549939003174,18.675227767345884,18.637737884740591,18.609769534618433,18.621902787919055]
[null,null,null,null,"Coincident",18.488393247679014,18.119344107675541,18.145241314222165,18.095512282845601,18.05918615929745,18.032086001298229,18.043842614757917]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.115431252889945,18.065299488020909,18.015306455363863,17.965451770998023,17.915735052065042,17.866155916766079,17.81671398435887]
[null,null,null,null,"Coincident",17.553092943738861,17.504517366602684,17.456076215160124,17.407769117408048,17.359595702372779,17.311555600107255,17.263648441688197]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.210528369022235,18.160133437011382,18.109877965488483,18.059761568517366,18.00978386122987,17.959944459822889,17.910242981555449]
[null,null,null,null,"Coincident",17.645238059957684,17.596407484900915,17.54771204120663,17.499151354918855,17.450725053116489,17.402432763910429,17.354274116440731]
[null,"Riverton 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.92735999999999996,0.99472551318750269,1.0122348362926716,1.0406339880862869,1.0675847430314569,1.093755033325349,1.1198819040968639]
[null,null,null,null,"Coincident",0.92735999999999996,0.99472551318750269,1.0122348362926716,1.0406339880862869,1.0675847430314569,1.093755033325349,1.1198819040968639]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8587561864536715,1.8028570258884176,1.762809722823623,1.7420199704351136,1.7225998705027914,1.7004675294134175,1.6787873855301481]
[null,null,null,null,"Coincident",1.7844059389955247,1.7307427448528809,1.6922973339106782,1.6723391716177092,1.6536958756826798,1.632448828236881,1.6116358901089423]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0203871591887732,1.9596272020526277,1.9160975248082859,1.8934999678642539,1.8723911635899906,1.8483342711015407,1.8247688973153782]
[null,null,null,null,"Coincident",1.9395716728212224,1.8812421139705227,1.8394536238159545,1.8177599691496837,1.7974955170463911,1.7744009002574792,1.7517781414227633]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6634694843698026,1.6182051025903725,1.5741724021114565,1.5313378678652152,1.4896688967565512,1.4491337728475748,1.4097016432173228]
[null,null,null,null,"Coincident",1.5969307049950106,1.5534768984867577,1.5112055060269984,1.4700843531506067,1.4300821408862894,1.391168421933672,1.35331357748863]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8081190047497853,1.758918589772144,1.7110569588168005,1.6644976824621904,1.6192053225614687,1.575145405269103,1.5322843948014377]
[null,null,null,null,"Coincident",1.735794244559794,1.6885618461812584,1.6426146804641286,1.5979177751637028,1.5544371096590102,1.5121395890583391,1.4709930190093803]
[null,"Robe 7.6kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0811500000000001,1.1596871641893856,1.1801001695758089,1.21320893312143,1.2446291029680596,1.2751393787522658,1.3055990344788697]
[null,null,null,null,"Coincident",1.0811500000000001,1.1596871641893856,1.1801001695758089,1.21320893312143,1.2446291029680596,1.2751393787522658,1.3055990344788697]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.9944514568838847,4.0043054080803788,3.9626758853884652,3.9754028199339837,3.9912251359323214,4.0169896470284341,4.0441842451880232]
[null,null,null,null,"Coincident",3.8425938167041771,3.8520731488093398,3.8120262617173424,3.8242693545470043,3.8394901512640036,3.8642751692062576,3.8904359063847513]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.0426381036793044,4.0526109269840145,4.0104792109051317,4.023359675492598,4.039372862342848,4.065448180920149,4.0929708382664387]
[null,null,null,null,"Coincident",3.8889485447619405,3.8985422297971462,3.8580122412769833,3.8704030273747283,3.8858074385787886,3.9108914479891563,3.9373677724806853]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.5088982087579303,3.5218440044120745,3.5348375625304307,3.5478790593287406,3.5609686716728803,3.5741065770812579,3.5872929537272209]
[null,null,null,null,"Coincident",3.3754999168111137,3.387953550274903,3.4004531304103773,3.412998826734059,3.4255908093878884,3.4382292491415307,3.4509143173946915]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.5512274347984945,3.5643294007026487,3.577479705248499,3.5906785267775474,3.603926044289274,3.6172224374435609,3.630567886563131]
[null,null,null,null,"Coincident",3.4162199065281085,3.4288237730948699,3.4414741406061782,3.4541711806235003,3.4669150653412659,3.4797059675892026,3.4925440608346778]
[null,"Robertstown 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.38461000000000001,0.41254893420790789,0.41981068882259803,0.43158885239590544,0.44276631299315122,0.45362008644675478,0.46445585224151886]
[null,null,null,null,"Coincident",0.38461000000000001,0.41254893420790789,0.41981068882259803,0.43158885239590544,0.44276631299315122,0.45362008644675478,0.46445585224151886]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.8956144409821416,0.88326507510492158,0.87108599102597428,0.85907484077933027,0.84722930877443714,0.8355471113497438,0.82402599633244134]
[null,null,null,null,"Coincident",0.8956144409821416,0.88326507510492158,0.87108599102597428,0.85907484077933027,0.84722930877443714,0.8355471113497438,0.82402599633244134]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.91829766234600574,0.90563552415619419,0.89314798049069877,0.88083262391663053,0.86868708019648966,0.85670900783044313,0.84489609760491524]
[null,null,null,null,"Coincident",0.91829766234600574,0.90563552415619419,0.89314798049069877,0.88083262391663053,0.86868708019648966,0.85670900783044313,0.84489609760491524]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.80605299688392751,0.79493856759442949,0.7839773919233769,0.77316735670139725,0.76250637789699349,0.75199240021476943,0.74162339669919719]
[null,null,null,null,"Coincident",0.80605299688392751,0.79493856759442949,0.7839773919233769,0.77316735670139725,0.76250637789699349,0.75199240021476943,0.74162339669919719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.82646789611140525,0.81507197174057489,0.80383318244162894,0.79274936152496756,0.7818183721768408,0.77103810704739884,0.76040648784442377]
[null,null,null,null,"Coincident",0.82646789611140525,0.81507197174057489,0.80383318244162894,0.79274936152496756,0.7818183721768408,0.77103810704739884,0.76040648784442377]
[null,"Roonka 11kV","Substation Rating","MVA","Non-Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,null,null,"Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.97359999999999991,1.0443244906393985,1.0627068631540557,1.0925220527096369,1.1208166254910998,1.1482918181133104,1.1757214262300579]
[null,null,null,null,"Coincident",0.97359999999999991,1.0443244906393985,1.0627068631540557,1.0925220527096369,1.1208166254910998,1.1482918181133104,1.1757214262300579]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9061061325302089,2.9060396248377569,2.8915160737566143,2.8845602726551025,2.8780619239817122,2.8715210719003461,2.8659918763708436]
[null,null,null,null,"Coincident",2.3892465942717651,2.3891919151683747,2.3772514204393884,2.3715327290584409,2.3661901308434303,2.3608125885767843,2.3562667767634959]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2024673745555492,3.2023940844878358,3.1863894389659757,3.178724293552964,3.1715632510218366,3.1643553706358127,3.1582623143318593]
[null,null,null,null,"Coincident",2.6328991162003783,2.6328388609871509,2.619680688827644,2.613378812111018,2.6074913820934382,2.6015654444714587,2.5965560561838221]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6621857812206544,2.6563842330335179,2.6505953278262986,2.6448190380468781,2.6390553362031812,2.6333041948630442,2.627565586654085]
[null,null,null,null,"Coincident",2.1887081961326298,2.1839384703843305,2.1791791390247193,2.1744301794019019,2.1696915689133509,2.1649632850057929,2.1602453051751049]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9336723163451772,2.9272791331839549,2.9208998823186834,2.9145345333875117,2.9081830560947557,2.9018454202107518,2.8955215955717155]
[null,null,null,null,"Coincident",2.4119100510738876,2.4066539143748447,2.4014092320718676,2.3961759792030493,2.3909541308608833,2.3857436621921404,2.3805445483977539]
[null,"Rudall 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.8099999999999992E-2,6.2320514488649392E-2,6.3417490498408627E-2,6.5196724797072628E-2,6.6885215633764289E-2,6.8524809605981257E-2,7.0161683303170075E-2]
[null,null,null,null,"Coincident",5.8099999999999992E-2,6.2320514488649392E-2,6.3417490498408627E-2,6.5196724797072628E-2,6.6885215633764289E-2,6.8524809605981257E-2,7.0161683303170075E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.0035189890979084E-2,8.8342096778606757E-2,8.6680841931812955E-2,8.5050826638602681E-2,8.3451463445636073E-2,8.1882175946511745E-2,8.0342398574031429E-2]
[null,null,null,null,"Coincident",9.0035189890979084E-2,8.8342096778606757E-2,8.6680841931812955E-2,8.5050826638602681E-2,8.3451463445636073E-2,8.1882175946511745E-2,8.0342398574031429E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.2175653679654718E-2,9.0442309588723027E-2,8.8741560674691411E-2,8.7072793992004099E-2,8.5435408121419656E-2,8.3828812953260987E-2,8.2252429474741387E-2]
[null,null,null,null,"Coincident",9.2175653679654718E-2,9.0442309588723027E-2,8.8741560674691411E-2,8.7072793992004099E-2,8.5435408121419656E-2,8.3828812953260987E-2,8.2252429474741387E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.1031670901881181E-2,7.9507887100746077E-2,7.8012757738631658E-2,7.6545743974742411E-2,7.5106317101072462E-2,7.3693958351860572E-2,7.2308158716628282E-2]
[null,null,null,null,"Coincident",8.1031670901881181E-2,7.9507887100746077E-2,7.8012757738631658E-2,7.6545743974742411E-2,7.5106317101072462E-2,7.3693958351860572E-2,7.2308158716628282E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2958088311689243E-2,8.1398078629850726E-2,7.9867404607222275E-2,7.8365514592803692E-2,7.6891867309277689E-2,7.5445931657934895E-2,7.4027186527267239E-2]
[null,null,null,null,"Coincident",8.2958088311689243E-2,8.1398078629850726E-2,7.9867404607222275E-2,7.8365514592803692E-2,7.6891867309277689E-2,7.5445931657934895E-2,7.4027186527267239E-2]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Salisbury 11kV","Substation Rating","MVA","Non-Coincident",72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627]
[null,null,null,null,"Coincident",72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627,72.581223017832627]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",17.41761,18.682864309167723,19.011723178657267,19.545114041183137,20.051301216433895,20.542829759745874,21.033542800656253]
[null,null,null,null,"Coincident",17.41761,18.682864309167723,19.011723178657267,19.545114041183137,20.051301216433895,20.542829759745874,21.033542800656253]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",56.610372743090117,56.023046505689152,55.976336014235812,55.946178529994235,55.947881757928272,55.968607901425713,56.032848947551365]
[null,null,null,null,"Coincident",54.00774661758507,53.447422332928546,53.402859326812276,53.374088313857911,53.375713236963627,53.395486509106689,53.456774113718453]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",56.809782846907424,56.220387752152241,56.17351272293844,56.143249008923547,56.144958236479965,56.165757387841978,56.230224723127307]
[null,null,null,null,"Coincident",54.197988967848808,53.635690940248004,53.590970960890864,53.562098602009911,53.563729248909155,53.583572172426337,53.645075662696613]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",52.134796320506858,52.183325590817155,52.231900034221873,52.280519692770042,52.329184608549824,52.377894823688557,52.426650380352797]
[null,null,null,null,"Coincident",49.737931993762118,49.784230161526338,49.830571425580501,49.876955826040465,49.923383403059397,49.969854196827875,50.016368247573865]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",52.318441201171161,52.367141415892561,52.415886962830662,52.464677884182599,52.513514222184803,52.562396019113002,52.611323317282292]
[null,null,null,null,"Coincident",49.913133917048249,49.95959517016226,50.006099671372944,50.052647460937465,50.09923857915043,50.145873066344002,50.192550962887836]
[null,"Salt Cliffs 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.1225,0.13139867512667042,0.13371157635206637,0.13746297396973145,0.14102304501094881,0.14448002025357495,0.14793125997656342]
[null,null,null,null,"Coincident",0.1225,0.13139867512667042,0.13371157635206637,0.13746297396973145,0.14102304501094881,0.14448002025357495,0.14793125997656342]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.19840183253250315,0.1984822968463241,0.19856279379344138,0.19864332338708987,0.19872388564050975,0.19880448056694661,0.19888510817965138]
[null,null,null,null,"Coincident",0.19840183253250315,0.1984822968463241,0.19856279379344138,0.19864332338708987,0.19872388564050975,0.19880448056694661,0.19888510817965138]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.19945461706945614,0.19953550835304992,0.1996164324431029,0.1996973893529202,0.19977837909581223,0.19985940168509486,0.19994045713408937]
[null,null,null,null,"Coincident",0.19945461706945614,0.19953550835304992,0.1996164324431029,0.1996973893529202,0.19977837909581223,0.19985940168509486,0.19994045713408937]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.17856164927925283,0.1786340671616917,0.17870651441409724,0.17877899104838088,0.17885149707645878,0.17892403251025196,0.17899659736168624]
[null,null,null,null,"Coincident",0.17856164927925283,0.1786340671616917,0.17870651441409724,0.17877899104838088,0.17885149707645878,0.17892403251025196,0.17899659736168624]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.17950915536251053,0.17958195751774494,0.1796547891987926,0.17972765041762817,0.17980054118623101,0.1798734615165854,0.17994641142068044]
[null,null,null,null,"Coincident",0.17950915536251053,0.17958195751774494,0.1796547891987926,0.17972765041762817,0.17980054118623101,0.1798734615165854,0.17994641142068044]
[null,"Sandy Creek 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4040999999999999,1.5060969775131261,1.5326075457627464,1.5756062183746935,1.616411897958149,1.6560358892901601,1.6955941398619816]
[null,null,null,null,"Coincident",1.4040999999999999,1.5060969775131261,1.5326075457627464,1.5756062183746935,1.616411897958149,1.6560358892901601,1.6955941398619816]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4816403605070696,2.6585089993338764,2.6675669499898644,2.6581714315556795,2.6503589364212745,2.6433568095481781,2.6360731021600028]
[null,null,null,null,"Coincident",2.1930775278899683,2.3493800459229601,2.3573847465026705,2.3490817302119957,2.3421776647443817,2.3359897386704827,2.3295529740018628]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6400429367096483,2.8282010631211452,2.8378371808402814,2.8278419484634885,2.8195307834268877,2.8120817122852957,2.8043330874042582]
[null,null,null,null,"Coincident",2.3330611998829451,2.4993404743861278,2.5078561133007136,2.499023117246804,2.4916783667493423,2.4850954666707263,2.4782478446828331]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2910269811853858,2.4684794257641043,2.4441854400905214,2.4201305480604778,2.3963123965907394,2.3727286557563656,2.3493770185627918]
[null,null,null,null,"Coincident",2.0246284950010383,2.1814469343961851,2.1599778307776698,2.1387200192162359,2.1176714202429787,2.0968299748544625,2.0761936443113043]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.4372627459418998,2.6260419423022388,2.600197276692044,2.5746069660217845,2.5492685070114245,2.52417942101741,2.4993372537902041]
[null,null,null,null,"Coincident",2.1538601010649345,2.3206882280810479,2.2978487561464576,2.2752340629959957,2.2528419364287009,2.2306701860153857,2.2087166428843665]
[null,"Seacombe 11kV","Substation Rating","MVA","Non-Coincident",59.2,59.2,59.2,59.2,59.2,59.2,59.2]
[null,null,null,null,"Coincident",59.2,59.2,59.2,59.2,59.2,59.2,59.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",14.501130000000002,15.554524651751956,15.828317968867273,16.272395556911775,16.69382456081323,17.103049437548766,17.511595363134234]
[null,null,null,null,"Coincident",14.501130000000002,15.554524651751956,15.828317968867273,16.272395556911775,16.69382456081323,17.103049437548766,17.511595363134234]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",44.680100079083964,44.853522455792259,44.886678268918573,44.963426554670853,45.05129336838452,45.143088060250868,45.199012691056829]
[null,null,null,null,"Coincident",43.505402791676531,43.67426567108884,43.706549775251382,43.781280249876858,43.866836932065752,43.956218223439642,44.010672523785495]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",44.782252898012963,44.95607177304187,44.989303390827722,45.066227147398635,45.154294852397129,45.246299415918202,45.302351908091403]
[null,null,null,null,"Coincident",43.604869881632574,43.774118834914766,43.806476750734873,43.881378082825513,43.96713037460902,44.05671601984195,44.111294819915273]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.817241549999594,40.786506261041254,40.755794115684772,40.725105096503071,40.694439186082192,40.663796367021291,40.633176621932627]
[null,null,null,null,"Coincident",39.744103780760703,39.714176562073092,39.684271878512284,39.654389713109381,39.624530048908262,39.594692868965573,39.564878156350723]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.910562654425462,40.879757094890238,40.848974731870456,40.818215547899193,40.787479525522677,40.756766647300282,40.726076895804511]
[null,null,null,null,"Coincident",39.834971353345033,39.804975711584369,39.775002656472928,39.74505217100301,39.715124238179733,39.685218841020998,39.655335962557508]
[null,"Seaford 11kV","Substation Rating","MVA","Non-Coincident",15.8,15.8,15.8,15.8,15.8,15.8,15.8]
[null,null,null,null,"Coincident",15.8,15.8,15.8,15.8,15.8,15.8,15.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.8769400000000003,5.2312118748756253,5.3232925320362998,5.4726422552811602,5.6143749317199729,5.7520031834732226,5.8894030941232751]
[null,null,null,null,"Coincident",4.8769400000000003,5.2312118748756253,5.3232925320362998,5.4726422552811602,5.6143749317199729,5.7520031834732226,5.8894030941232751]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.6390610614184595,9.8214804246070262,9.9496304659256882,10.126741142432479,10.306369095515809,10.487085502819602,10.659760515901691]
[null,null,null,null,"Coincident",9.6390610614184595,9.8214804246070262,9.9496304659256882,10.126741142432479,10.306369095515809,10.487085502819602,10.659760515901691]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.8177932995009201,10.003595172753956,10.134121435527105,10.314516185804012,10.49747488924489,10.681542229562782,10.857419068149705]
[null,null,null,null,"Coincident",9.8177932995009201,10.003595172753956,10.134121435527105,10.314516185804012,10.49747488924489,10.681542229562782,10.857419068149705]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6752086206844492,8.7981347454287793,8.9228027109524355,9.0492371988217375,9.1774632403363032,9.3075062214847009,9.4393918879703325]
[null,null,null,null,"Coincident",8.6752086206844492,8.7981347454287793,8.9228027109524355,9.0492371988217375,9.1774632403363032,9.3075062214847009,9.4393918879703325]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8360686300492013,8.9612741118029291,9.0882537324093011,9.2170326310924473,9.3476363032947241,9.4800906057242571,9.6144217614740182]
[null,null,null,null,"Coincident",8.8360686300492013,8.9612741118029291,9.0882537324093011,9.2170326310924473,9.3476363032947241,9.4800906057242571,9.6144217614740182]
[null,"Second Valley 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.38083999999999996,0.40850507294074417,0.41569564684017113,0.42735835923781651,0.43842625683240605,0.44917364010915495,0.45990319224060744]
[null,null,null,null,"Coincident",0.38083999999999996,0.40850507294074417,0.41569564684017113,0.42735835923781651,0.43842625683240605,0.44917364010915495,0.45990319224060744]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.2976027487987547,0.29772344526948608,0.29784419069016199,0.29796498508063474,0.29808582846076453,0.29820672085041983,0.29832766226947699]
[null,null,null,null,"Coincident",0.2976027487987547,0.29772344526948608,0.29784419069016199,0.29796498508063474,0.29808582846076453,0.29820672085041983,0.29832766226947699]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.29918192560418416,0.29930326252957479,0.29942464866465429,0.29954608402938021,0.29966756864371824,0.29978910252764224,0.29991068570113399]
[null,null,null,null,"Coincident",0.29918192560418416,0.29930326252957479,0.29942464866465429,0.29954608402938021,0.29966756864371824,0.29978910252764224,0.29991068570113399]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.26784247391887922,0.26795110074253747,0.2680597716211458,0.26816848657257125,0.26827724561468808,0.26838604876537786,0.2684948960425293]
[null,null,null,null,"Coincident",0.26784247391887922,0.26795110074253747,0.2680597716211458,0.26816848657257125,0.26827724561468808,0.26838604876537786,0.2684948960425293]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.26926373304376577,0.26937293627661735,0.26948218379818889,0.2695914756264422,0.26970081177934641,0.26981019227487801,0.26991961713102058]
[null,null,null,null,"Coincident",0.26926373304376577,0.26937293627661735,0.26948218379818889,0.2695914756264422,0.26970081177934641,0.26981019227487801,0.26991961713102058]
[null,"Sheidow Park 11kV","Substation Rating","MVA","Non-Coincident",35,35,35,35,35,35,35]
[null,null,null,null,"Coincident",35,35,35,35,35,35,35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",11.706010000000001,12.556360857302494,12.777379999126962,13.135860799342174,13.476058572478507,13.806404586845316,14.1362025191694]
[null,null,null,null,"Coincident",11.706010000000001,12.556360857302494,12.777379999126962,13.135860799342174,13.476058572478507,13.806404586845316,14.1362025191694]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.651368411540247,24.94788055087492,25.052102855734443,25.289770473262468,25.53184146521901,25.775339306783568,25.998636955621404]
[null,null,null,null,"Coincident",24.651368411540247,24.94788055087492,25.052102855734443,25.289770473262468,25.53184146521901,25.775339306783568,25.998636955621404]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.768250508088904,25.066168531264143,25.170884996175786,25.409679491893886,25.652898240217585,25.897550603419724,26.121906996620748]
[null,null,null,null,"Coincident",24.768250508088904,25.066168531264143,25.170884996175786,25.409679491893886,25.652898240217585,25.897550603419724,26.121906996620748]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.609259077869932,21.848272791148005,22.089930165410895,22.334260441421847,22.581293183367666,22.831058282436,23.083585960432213]
[null,null,null,null,"Coincident",21.609259077869932,21.848272791148005,22.089930165410895,22.334260441421847,22.581293183367666,22.831058282436,23.083585960432213]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.711717305085511,21.951864278937418,22.194667448438882,22.440156192995424,22.688360216969595,22.939309553275248,23.19303456701153]
[null,null,null,null,"Coincident",21.711717305085514,21.951864278937418,22.194667448438882,22.440156192995424,22.688360216969595,22.939309553275248,23.19303456701153]
[null,"Sherlock 11kV","Substation Rating","MVA","Non-Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,null,null,"Coincident",0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001,0.19500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.8460000000000001E-2,4.1253820778544857E-2,4.1979977359187542E-2,4.3157763092864267E-2,4.4275480090784428E-2,4.5360829215938724E-2,4.6444377622029638E-2]
[null,null,null,null,"Coincident",3.8460000000000001E-2,4.1253820778544857E-2,4.1979977359187542E-2,4.3157763092864267E-2,4.4275480090784428E-2,4.5360829215938724E-2,4.6444377622029638E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8906223390249664E-2,2.8867623186867072E-2,2.8829074528637269E-2,2.8790577346728938E-2,2.8752131572402681E-2,2.8713737137010885E-2,2.8675393971997611E-2]
[null,null,null,null,"Coincident",2.8906223390249664E-2,2.8867623186867072E-2,2.8829074528637269E-2,2.8790577346728938E-2,2.8752131572402681E-2,2.8713737137010885E-2,2.8675393971997611E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9299960844315284E-2,2.9260834859837007E-2,2.9221761122618359E-2,2.9182739562890459E-2,2.9143770110977602E-2,2.9104852697297103E-2,2.9065987252359215E-2]
[null,null,null,null,"Coincident",2.9299960844315284E-2,2.9260834859837007E-2,2.9221761122618359E-2,2.9182739562890459E-2,2.9143770110977602E-2,2.9104852697297103E-2,2.9065987252359215E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6015601051224697E-2,2.5980860868180366E-2,2.5946167075773543E-2,2.5911519612056046E-2,2.5876918415162414E-2,2.5842363423309797E-2,2.580785457479785E-2]
[null,null,null,null,"Coincident",2.6015601051224697E-2,2.5980860868180366E-2,2.5946167075773543E-2,2.5911519612056046E-2,2.5876918415162414E-2,2.5842363423309797E-2,2.580785457479785E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6369964759883756E-2,2.6334751373853306E-2,2.6299585010356522E-2,2.6264465606601416E-2,2.6229393099879841E-2,2.6194367427567394E-2,2.6159388527123295E-2]
[null,null,null,null,"Coincident",2.6369964759883756E-2,2.6334751373853306E-2,2.6299585010356522E-2,2.6264465606601416E-2,2.6229393099879841E-2,2.6194367427567394E-2,2.6159388527123295E-2]
[null,"Smithfield West 11kV","Substation Rating","MVA","Non-Coincident",36.195,36.195,36.195,36.195,36.195,36.195,36.195]
[null,null,null,null,"Coincident",36.195,36.195,36.195,36.195,36.195,36.195,36.195]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.7128100000000002,6.1278013489828087,6.2356639224477419,6.4106110393797673,6.576635606277538,6.7378522816720441,6.898801480054785]
[null,null,null,null,"Coincident",5.7128100000000002,6.1278013489828087,6.2356639224477419,6.4106110393797673,6.576635606277538,6.7378522816720441,6.898801480054785]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.746968083668001,18.820193334942093,18.980533248709307,19.195069366145727,19.421066890679008,19.655544085164031,19.899893244398157]
[null,null,null,null,"Coincident",17.649370420689781,17.718308479266327,17.869260810260286,18.071236265083332,18.284002084433165,18.504751105938972,18.734794108309273]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.894910252266421,18.968713362446621,19.130318602662875,19.346547737248233,19.57432872691188,19.810656304055271,20.056933750805062]
[null,null,null,null,"Coincident",17.788650869815225,17.858132954809232,18.01027652990744,18.213845879095526,18.42829074524257,18.650781813185528,18.882640205675962]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.681640582206757,16.911479214748077,17.144484550033539,17.380700218701556,17.620170452530832,17.862940092722837,18.109054598298393]
[null,null,null,null,"Coincident",15.704963733131422,15.921345771261656,16.140709107994105,16.363094819480153,16.588544547815914,16.817100508839768,17.048805500037364]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.813284167051876,17.0449365769237,17.279780679653758,17.517860450192739,17.759220469375538,18.003905932269092,18.251962656635218]
[null,null,null,null,"Coincident",15.828899848137834,16.046989470546436,16.268083918549909,16.49222459245312,16.719453462971821,16.949813079091744,17.183346576035969]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"South End 11kV","Substation Rating","MVA","Non-Coincident",0.78,0.78,0.78,0.78,0.78,0.78,0.78]
[null,null,null,null,"Coincident",0.78,0.78,0.78,0.78,0.78,0.78,0.78]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.40770999999999996,0.43732697008893712,0.4450248717918448,0.45751044177305478,0.46935923005235869,0.48086489026600032,0.49235146126567081]
[null,null,null,null,"Coincident",0.40770999999999996,0.43732697008893712,0.4450248717918448,0.45751044177305478,0.46935923005235869,0.48086489026600032,0.49235146126567081]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.5273830680693512,0.5265127827250301,0.51459375649489469,0.51637901738037972,0.51181759012714712,0.50757052760870225,0.50345770468497353]
[null,null,null,null,"Coincident",0.43094033108444663,0.43022919514336944,0.42048980565439309,0.42194859522054173,0.41822131785852523,0.41475091723581453,0.41139020776341584]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.54361402370306089,0.54271695410329512,0.53043110307795627,0.53227130787799082,0.52756949628582861,0.52319172444529105,0.51895232361179233]
[null,null,null,null,"Coincident",0.44420312584995481,0.44347010370014628,0.43343097080212628,0.43493465666882125,0.43109266710392935,0.42751546002126795,0.42405131998833956]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.4431154769719427,0.42685070854798318,0.411182946334894,0.39609027693025056,0.38155159127368876,0.36754655512313983,0.35405558061474895]
[null,null,null,null,"Coincident",0.36208278558124019,0.34879236138295844,0.33598976864865177,0.32365710128791303,0.31177711046206508,0.30033318045941748,0.28930930545603328]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.45675297897531747,0.43998763942826841,0.42383767979786158,0.40828051226589329,0.39329437811097917,0.37885831727615232,0.36495213905349966]
[null,null,null,null,"Coincident",0.3732263925423312,0.35952693684763604,0.34633032631630811,0.33361810377282486,0.32137248952123987,0.30957635647796711,0.29821320621732728]
[null,"Spalding 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.49565000000000003,0.53165512919619762,0.54101341076654463,0.5561920248824278,0.57059650824225949,0.58458385337701579,0.59854799189700958]
[null,null,null,null,"Coincident",0.49565000000000003,0.53165512919619762,0.54101341076654463,0.5561920248824278,0.57059650824225949,0.58458385337701579,0.59854799189700958]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.92021870424088958,0.88719448094046871,0.84446326991240606,0.83601051796675951,0.82796598658120613,0.81880349297056276,0.80575713740428256]
[null,null,null,null,"Coincident",0.92021870424088958,0.88719448094046871,0.84446326991240606,0.83601051796675951,0.82796598658120613,0.81880349297056276,0.80575713740428256]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.92021870424088958,0.88719448094046871,0.84446326991240606,0.83601051796675951,0.82796598658120613,0.81880349297056276,0.80575713740428256]
[null,null,null,null,"Coincident",0.92021870424088958,0.88719448094046871,0.84446326991240606,0.83601051796675951,0.82796598658120613,0.81880349297056276,0.80575713740428256]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.8231550925087644,0.7927460659475104,0.7634604107956281,0.73525662742402376,0.70809474928447125,0.68193628627448055,0.6567441701943838]
[null,null,null,null,"Coincident",0.8231550925087644,0.7927460659475104,0.7634604107956281,0.73525662742402376,0.70809474928447125,0.68193628627448055,0.6567441701943838]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.8231550925087644,0.7927460659475104,0.7634604107956281,0.73525662742402376,0.70809474928447125,0.68193628627448055,0.6567441701943838]
[null,null,null,null,"Coincident",0.8231550925087644,0.7927460659475104,0.7634604107956281,0.73525662742402376,0.70809474928447125,0.68193628627448055,0.6567441701943838]
[null,"Square Water Hole 11kV","Substation Rating","MVA","Non-Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,null,null,"Coincident",7.125,7.125,7.125,7.125,7.125,7.125,7.125]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.5033799999999995,2.6852311456212585,2.7324970286386607,2.8091596716436431,2.8819124115878285,2.9525583110399545,3.023087000817382]
[null,null,null,null,"Coincident",2.5033799999999995,2.6852311456212585,2.7324970286386607,2.8091596716436431,2.8819124115878285,2.9525583110399545,3.023087000817382]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0420924096530584,4.0273078816513035,3.998777564647384,3.9995931511713971,4.0017399093701682,4.0044033596336979,4.0038830682168625]
[null,null,null,null,"Coincident",4.0420924096530584,4.0273078816513035,3.998777564647384,3.9995931511713971,4.0017399093701682,4.0044033596336979,4.0038830682168625]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.3009324278534482,4.2852011556634801,4.2548438671249862,4.2557116806664261,4.2579959089858495,4.2608299163383361,4.2602763074645615]
[null,null,null,null,"Coincident",4.3009324278534482,4.2852011556634801,4.2548438671249862,4.2557116806664261,4.2579959089858495,4.2608299163383361,4.2602763074645615]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.5995480475506647,3.5595456446774181,3.5199877954577121,3.4808695594895536,3.4421860512744957,3.4039324396074844,3.3661039469734861]
[null,null,null,null,"Coincident",3.5995480475506647,3.5595456446774181,3.5199877954577121,3.4808695594895536,3.4421860512744957,3.4039324396074844,3.3661039469734861]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8300492305310812,3.7874852279618345,3.7453942465486278,3.7037710295251665,3.6626103785445134,3.6219071530298632,3.5816562695325356]
[null,null,null,null,"Coincident",3.8300492305310812,3.7874852279618345,3.7453942465486278,3.7037710295251665,3.662610378544513,3.6219071530298632,3.5816562695325356]
[null,"Stansbury 11kV","Substation Rating","MVA","Non-Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,null,null,"Coincident",2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.68764000000000003,0.73759171399268286,0.75057492541008108,0.7716329748616011,0.79161703405166395,0.81102237654831244,0.8303955233492577]
[null,null,null,null,"Coincident",0.68764000000000003,0.73759171399268286,0.75057492541008108,0.7716329748616011,0.79161703405166395,0.81102237654831244,0.8303955233492577]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2202031217027152,1.200977010860516,1.1596795931994506,1.138922718869352,1.1194043125501048,1.1004774752213171,1.0820702044844677]
[null,null,null,null,"Coincident",1.2202031217027152,1.200977010860516,1.1596795931994506,1.138922718869352,1.1194043125501048,1.1004774752213171,1.0820702044844677]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2616130959570833,1.2417345095222334,1.1990355833977819,1.1775742840286694,1.1573934824993208,1.1378243260086154,1.1187923686161192]
[null,null,null,null,"Coincident",1.2616130959570835,1.2417345095222336,1.1990355833977819,1.1775742840286694,1.1573934824993211,1.1378243260086154,1.1187923686161192]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0621078351630242,1.0218053020966356,0.98303208094923678,0.94573014075434469,0.90984365257701005,0.87531890595596629,0.84210422851644751]
[null,null,null,null,"Coincident",1.0621078351630242,1.0218053020966356,0.98303208094923678,0.94573014075434469,0.90984365257701005,0.87531890595596629,0.84210422851644751]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0981525373336674,1.056482259154206,1.0163931930782741,0.97782533874528943,0.94072097255644016,0.90502456128113717,0.87068267894173379]
[null,null,null,null,"Coincident",1.0981525373336676,1.0564822591542062,1.0163931930782744,0.97782533874528943,0.94072097255644027,0.90502456128113717,0.8706826789417339]
[null,"Stirling East 11kV","Substation Rating","MVA","Non-Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,null,null,"Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.1994799999999994,3.4318974130145259,3.4923062392400759,3.5902860078096026,3.6832686698092281,3.7735586547012892,3.8636988381209396]
[null,null,null,null,"Coincident",3.1994799999999994,3.4318974130145259,3.4923062392400759,3.5902860078096026,3.6832686698092281,3.7735586547012892,3.8636988381209396]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.943295836754495,8.1931926065365044,8.4671171930772129,8.571682274145406,8.674147978281102,8.7773139091184458,8.8876685438090881]
[null,null,null,null,"Coincident",7.2314906404965829,7.4589939576218454,7.7083719393162031,7.8035668584791731,7.8968505275829459,7.9907716755044849,8.0912373416840371]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.1494520593926101,8.4058345216587576,8.6868684063056296,8.7941473158117773,8.8992723622341892,9.0051158086826177,9.1183345309139963]
[null,null,null,null,"Coincident",7.4191730364599167,7.6525808578942307,7.9084310677130079,8.006096626941801,8.1018013325084581,8.1981600616908832,8.3012331621987094]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.8215975200381518,6.8675018780092483,6.9137151387079747,6.9602393808235758,7.0070766970333516,7.0542291940967878,7.1016989929503218]
[null,null,null,null,"Coincident",6.2103086216597703,6.2520994528019251,6.2941715056472098,6.3365266726118374,6.3791668588465935,6.4220939823225338,6.4653099739172575]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.9986417603623545,7.0457374964762813,7.0931501524206624,7.1408818608339786,7.1889347687057992,7.2373110374733667,7.2860128431188107]
[null,null,null,null,"Coincident",6.3714877837066171,6.4143632326278697,6.4575272019359753,6.5009816331619481,6.5447284809018784,6.588769712904857,6.633107310161491]
[null,"Stirling North TF1 11kV","Substation Rating","MVA","Non-Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,null,null,"Coincident",3.25,3.25,3.25,3.25,3.25,3.25,3.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0933299999999999,1.1727519467448373,1.1933949205959571,1.2268766802475632,1.2586508228720055,1.2895048207660498,1.320307628327968]
[null,null,null,null,"Coincident",1.0933299999999999,1.1727519467448373,1.1933949205959571,1.2268766802475632,1.2586508228720055,1.2895048207660498,1.320307628327968]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5541546233083388,1.492027546660126,1.4704523413261554,1.4423888650786061,1.4166423779333783,1.3918822536053523,1.3678756963256671]
[null,null,null,null,"Coincident",1.5046077290063815,1.4444612813469537,1.4235738997354064,1.3964050951444151,1.3714794133798744,1.3475086489035553,1.3242674275423505]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7660847992140214,1.695485848477416,1.670968569688813,1.6390782557711432,1.6098208840152026,1.5816843790969912,1.5544042003700762]
[null,null,null,null,"Coincident",1.7097815102345244,1.6414332742579019,1.6176976133356891,1.5868239717550172,1.5584993333862209,1.5312598282994947,1.5048493494799438]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3828425602858412,1.3279538517624307,1.2752438224393083,1.2246259947296358,1.1760173235725864,1.1293380601872345,1.084511621234417]
[null,null,null,null,"Coincident",1.3387571435948808,1.2856183028122947,1.2345886843133969,1.1855845674415735,1.1385255546363102,1.0933344395306475,1.0499370802841983]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5714120003248195,1.5090384679118531,1.4491407073173959,1.3916204485564043,1.3363833222415755,1.283338704758221,1.2323995695845649]
[null,null,null,null,"Coincident",1.5213149359032736,1.4609298895594258,1.402941686719769,1.3472551902745153,1.2937790393594435,1.2424254994666448,1.1931103185047709]
[null,"Stirling North TF2 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.97936999999999996,1.0505136363984262,1.0690049512810063,1.0989968393202931,1.1274590987132487,1.1550971219244386,1.1826892904754853]
[null,null,null,null,"Coincident",0.97936999999999996,1.0505136363984262,1.0690049512810063,1.0989968393202931,1.1274590987132487,1.1550971219244386,1.1826892904754853]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6678251678942779,1.6563915056991698,1.6426556857706551,1.631432710040382,1.6211901432440938,1.611087020426061,1.6015772656603513]
[null,null,null,null,"Coincident",1.6678251678942779,1.6563915056991698,1.6426556857706551,1.631432710040382,1.6211901432440938,1.611087020426061,1.6015772656603513]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7003936015244656,1.6887366686439647,1.6747326226757488,1.6632904904372032,1.6528479120549713,1.6425475006414123,1.6328520442668719]
[null,null,null,null,"Coincident",1.7003936015244656,1.6887366686439647,1.6747326226757488,1.6632904904372032,1.6528479120549713,1.6425475006414123,1.6328520442668719]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4907331567954603,1.4854078730539413,1.4801016126009288,1.4748143074803242,1.4695458899787859,1.4642962926248619,1.4590654481881258]
[null,null,null,null,"Coincident",1.4907331567954603,1.4854078730539413,1.4801016126009288,1.4748143074803242,1.4695458899787859,1.4642962926248619,1.4590654481881258]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5198434285505695,1.5144141554021053,1.5090042770191592,1.5036137241186207,1.4982424276648769,1.4928903188689278,1.4875573291875059]
[null,null,null,null,"Coincident",1.5198434285505695,1.5144141554021053,1.5090042770191592,1.5036137241186207,1.4982424276648769,1.492890318868928,1.4875573291875059]
[null,"Stockwell TF1 11kV","Substation Rating","MVA","Non-Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,null,null,"Coincident",8.90625,8.90625,8.90625,8.90625,8.90625,8.90625,8.90625]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.3228599999999999,1.41895552145361,1.4439322113722004,1.4844430183314201,1.522887716923949,1.5602190987154625,1.597488543449769]
[null,null,null,null,"Coincident",1.3228599999999999,1.41895552145361,1.4439322113722004,1.4844430183314201,1.522887716923949,1.5602190987154625,1.597488543449769]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0074585599685739,1.9593300689579158,1.9611197190660099,1.948061260498134,1.9367248626746585,1.9262844968078849,1.9156557070766362]
[null,null,null,null,"Coincident",1.8591241836162165,1.8145519850447696,1.816209394997093,1.8041158471608336,1.7936171142011617,1.7839482039403074,1.7741047927606288]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.027839372435372,1.9792222547754974,1.9810300743860467,1.9678390392357772,1.9563875481283373,1.94584118598196,1.9351044869894287]
[null,null,null,null,"Coincident",1.8779990247184726,1.8329743049152392,1.8346485417959448,1.8224322136764834,1.8118268918626967,1.8020598175596478,1.7921164707094219]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7717192475933996,1.7334645459095912,1.6960358341239594,1.6594152775839814,1.6235854267203318,1.5885292087322216,1.5542299194522682]
[null,null,null,null,"Coincident",1.6408040322539861,1.6053760326650404,1.5707129892379528,1.5367983851516678,1.5036160602139035,1.4711502031608754,1.4393853441232829]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7897067061886012,1.7510636219416162,1.7132549134920489,1.6762625651202721,1.6400689500994301,1.6046568222963637,1.5700093079538864]
[null,null,null,null,"Coincident",1.6574623682928917,1.6216746843597236,1.5866597228399273,1.5524007992246858,1.5188815892546448,1.4860861211414602,1.4539987679572939]
[null,"Stockwell TF2 11kV","Substation Rating","MVA","Non-Coincident",7.9,7.9,7.9,7.9,7.9,7.9,7.9]
[null,null,null,null,"Coincident",7.9,7.9,7.9,7.9,7.9,7.9,7.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.62278,0.66802013792153314,0.67977873894318297,0.69885053819485199,0.71694964875035683,0.73452462868180746,0.752070449699626]
[null,null,null,null,"Coincident",0.62278,0.66802013792153314,0.67977873894318297,0.69885053819485199,0.71694964875035683,0.73452462868180746,0.752070449699626]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.9442381259683499,5.0068818944477327,5.0872591107355163,5.1182681149739446,5.150268706730377,5.1828730957562739,5.215158713426578]
[null,null,null,null,"Coincident",3.705681504513652,3.7526326926062801,3.8128750102684372,3.8361161023340067,3.8601003842363024,3.8845372091425805,3.9087351165277986]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.2116845907674954,5.2777169206378653,5.3624419457889925,5.3951283062447422,5.4288598917192532,5.4632279353992645,5.4972599645671112]
[null,null,null,null,"Coincident",3.9061312791408898,3.9556221768821165,4.0191231553287192,4.0436214174076746,4.0689030703592781,4.094661745521468,4.1201685795038339]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.509303719255696,4.5642693675630186,4.6199050134313717,4.6762188237203404,4.7332190648385239,4.7909141039569736,4.8493124102374292]
[null,null,null,null,"Coincident",3.3797003633209357,3.4208968391229893,3.4625954747132095,3.5048023911116082,3.5475237839496812,3.5907659243798729,3.6345351599961333]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7532234714388242,4.8111623520117961,4.8698074720246405,4.929167440103229,4.9892509698073102,5.0500668809095819,5.1116241006903671]
[null,null,null,null,"Coincident",3.5625169856642493,3.6059418840330828,3.6498961052952348,3.6943861015723183,3.7394184036333571,3.7849996218534434,3.8311364471840923]
[null,"Strathalbyn 11kV","Substation Rating","MVA","Non-Coincident",16.7,16.7,16.7,16.7,16.7,16.7,16.7]
[null,null,null,null,"Coincident",16.7,16.7,16.7,16.7,16.7,16.7,16.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.7749499999999996,6.1944553381450227,6.3034911661580875,6.4803412369510252,6.6481717043753363,6.8111419833745508,6.9738418759318757]
[null,null,null,null,"Coincident",5.7749499999999996,6.1944553381450227,6.3034911661580875,6.4803412369510252,6.6481717043753363,6.8111419833745508,6.9738418759318757]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.303571359586094,11.527373592641041,11.640650445313534,11.761370845647834,11.88983067085678,12.024597433148752,12.125505524860408]
[null,null,null,null,"Coincident",11.303571359586094,11.527373592641041,11.640650445313534,11.761370845647834,11.88983067085678,12.024597433148752,12.125505524860408]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.404639775319087,11.630443087184686,11.744732780106922,11.866532575547451,11.996140996240619,12.132112746117931,12.23392308550331]
[null,null,null,null,"Coincident",11.404639775319087,11.630443087184686,11.744732780106922,11.866532575547451,11.996140996240619,12.132112746117931,12.23392308550331]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8352940189821645,9.7710109535178109,9.7071480394487821,9.6437025306833384,9.5806716990780814,9.5180528343206401,9.455843243813133]
[null,null,null,null,"Coincident",9.8352940189821645,9.7710109535178109,9.7071480394487821,9.6437025306833384,9.5806716990780814,9.5180528343206401,9.455843243813133]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9232341534002746,9.8583763149391164,9.7939423845652662,9.7299295916334021,9.6663351836070284,9.6031564259401065,9.5403906019594817]
[null,null,null,null,"Coincident",9.9232341534002746,9.8583763149391164,9.7939423845652662,9.7299295916334021,9.6663351836070266,9.6031564259401065,9.54039060195948]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Streaky Bay 11kV","Substation Rating","MVA","Non-Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,null,null,"Coincident",6.5,6.5,6.5,6.5,6.5,6.5,6.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8667499999999999,2.0023549125935673,2.0376006951446524,2.0947674012897646,2.1490185246872544,2.2016985943539673,2.2542912617244877]
[null,null,null,null,"Coincident",1.8667499999999999,2.0023549125935673,2.0376006951446524,2.0947674012897646,2.1490185246872544,2.2016985943539673,2.2542912617244877]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0505524308479339,2.9334698935540655,2.8756051705119288,2.8315134902424228,2.7894241072737511,2.7479917112908687,2.7079530167839851]
[null,null,null,null,"Coincident",3.0505524308479339,2.9334698935540655,2.8756051705119288,2.8315134902424228,2.7894241072737511,2.7479917112908687,2.7079530167839851]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1470175393568596,3.0262325973607016,2.9665380658121929,2.9210521106308618,2.8776317697497511,2.8348891912130934,2.7935843860270078]
[null,null,null,null,"Coincident",3.1470175393568596,3.0262325973607016,2.9665380658121929,2.9210521106308618,2.8776317697497511,2.8348891912130934,2.7935843860270078]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6660798924948055,2.5761867696233138,2.4893246037619017,2.405391199101774,2.3242878056049934,2.2459190028222515,2.1701925876279957]
[null,null,null,null,"Coincident",2.6660798924948055,2.5761867696233138,2.4893246037619017,2.405391199101774,2.3242878056049934,2.2459190028222515,2.1701925876279957]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7503871423956014,2.6576514032935821,2.5680424666602892,2.4814549050329884,2.3977868456825759,2.3169398507574188,2.2388188014684212]
[null,null,null,null,"Coincident",2.7503871423956014,2.6576514032935816,2.5680424666602892,2.4814549050329884,2.3977868456825759,2.3169398507574193,2.2388188014684216]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Swan Reach 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.34312999999999999,0.36805573384664836,0.37453431178517993,0.38504220618966495,0.39501418313964792,0.40469738244578918,0.41436451621027109]
[null,null,null,null,"Coincident",0.34312999999999999,0.36805573384664836,0.37453431178517993,0.38504220618966495,0.39501418313964792,0.40469738244578918,0.41436451621027109]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2900340632847656,1.2850968916513916,1.2695350872390359,1.2682704310962141,1.2672325496243737,1.2661889817779157,1.2655991358650742]
[null,null,null,null,"Coincident",0.90465938669335788,0.90119710706139589,0.89028411426826215,0.88939725160075245,0.88866941871439842,0.88793759815646234,0.88752395819381202]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3709715222717438,1.3657245897274288,1.3491864289984179,1.3478424276215395,1.3467394288853949,1.3456303870083073,1.3450035338328377]
[null,null,null,null,"Coincident",0.96141822282923406,0.95773871783579601,0.94614103776830427,0.9451985328407787,0.94442503531186583,0.94364729992262442,0.9432077079572595]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2391522914569681,1.2379410263305346,1.2367309452096642,1.2355220469369972,1.2343143303563056,1.2331077943124913,1.2319024376515857]
[null,null,null,null,"Coincident",0.86897763703598807,0.8681282157706206,0.86727962481026377,0.86643186334329836,0.86558493055889896,0.86473882564703242,0.86389354779845751]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3168973996078677,1.3156101390296213,1.3143241367421099,1.3130393915153598,1.3117559021206009,1.3104736673302639,1.309192685917979]
[null,null,null,null,"Coincident",0.9234977802321418,0.9225950658012797,0.92169323376922918,0.92079228327344964,0.91989221345224403,0.9189930234447572,0.91809471239097573]
[null,"Swan Reach 33kV","Substation Rating","MVA","Non-Coincident",10.69,10.69,10.69,10.69,10.69,10.69,10.69]
[null,null,null,null,"Coincident",10.69,10.69,10.69,10.69,10.69,10.69,10.69]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.34504000000000001,0.37010448053637851,0.37661912085319993,0.3871855064368665,0.39721299143328803,0.40695009133300819,0.41667103626378327]
[null,null,null,null,"Coincident",0.34504000000000001,0.37010448053637851,0.37661912085319993,0.3871855064368665,0.39721299143328803,0.40695009133300819,0.41667103626378327]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4139753513313402,2.4167801719953892,2.4195882516069469,2.4223995939526155,2.4252142028233958,2.4280320820146946,2.4308532353263277]
[null,null,null,null,"Coincident",2.4139753513313402,2.4167801719953892,2.4195882516069469,2.4223995939526155,2.4252142028233958,2.4280320820146946,2.4308532353263277]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5727862990617103,2.5757756436595374,2.5787684616049673,2.5817647569337159,2.5847645336861866,2.587767795907479,2.590774547647392]
[null,null,null,null,"Coincident",2.5727862990617103,2.5757756436595374,2.5787684616049673,2.5817647569337159,2.5847645336861866,2.587767795907479,2.590774547647392]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1725778161982063,2.1751021547958502,2.1776294264462521,2.180159634557354,2.1826927825410563,2.1852288738132253,2.1877679117936948]
[null,null,null,null,"Coincident",2.1725778161982063,2.1751021547958502,2.1776294264462521,2.180159634557354,2.1826927825410563,2.1852288738132253,2.1877679117936948]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3155076691555392,2.3181980792935835,2.3208916154444705,2.3235882812403443,2.3262880803175681,2.3289910163167313,2.3316970928826528]
[null,null,null,null,"Coincident",2.3155076691555392,2.3181980792935835,2.3208916154444705,2.3235882812403443,2.3262880803175681,2.3289910163167313,2.3316970928826528]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Tailem Bend Town 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.7449700000000004,1.8717285398839685,1.904675015404615,1.9581123729629579,2.0088243498184113,2.0580677627908628,2.1072294752759504]
[null,null,null,null,"Coincident",1.7449700000000004,1.8717285398839685,1.904675015404615,1.9581123729629579,2.0088243498184113,2.0580677627908628,2.1072294752759504]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0833304949599643,3.079213139932488,3.0751012830546425,3.0709949169844206,3.0668940343896196,3.0627986279478283,3.0587086903464127]
[null,null,null,null,"Coincident",3.0833304949599643,3.079213139932488,3.0751012830546425,3.0709949169844206,3.0668940343896196,3.0627986279478283,3.0587086903464127]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1253291567269637,3.1211557183826142,3.116987853079292,3.1128255533749831,3.1086688118376111,3.1045176210450252,3.1003719735849837]
[null,null,null,null,"Coincident",3.1253291567269637,3.1211557183826142,3.116987853079292,3.1128255533749831,3.1086688118376111,3.1045176210450252,3.1003719735849837]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.7749974454639679,2.7712918259392394,2.7675911547491783,2.7638954252859786,2.7602046309506578,2.7565187651530456,2.7528378213117715]
[null,null,null,null,"Coincident",2.7749974454639679,2.7712918259392394,2.7675911547491783,2.7638954252859786,2.7602046309506578,2.7565187651530456,2.7528378213117715]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8127962410542673,2.8090401465443531,2.8052890677713629,2.8015429980374846,2.7978019306538502,2.7940658589405225,2.7903347762264854]
[null,null,null,null,"Coincident",2.8127962410542673,2.8090401465443531,2.8052890677713629,2.8015429980374846,2.7978019306538502,2.7940658589405225,2.7903347762264854]
[null,"Tantanoola 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.20812,0.22323830422336857,0.22716778179911884,0.2335411766741266,0.23958951940962175,0.2454627086952981,0.25132615368426431]
[null,null,null,null,"Coincident",0.20812,0.22323830422336857,0.22716778179911884,0.2335411766741266,0.23958951940962175,0.2454627086952981,0.25132615368426431]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.48999501741668833,0.48772479794758106,0.47937385774130303,0.4783655591195265,0.477409182584422,0.47643479612884948,0.47563483353904018]
[null,null,null,null,"Coincident",0.42194015388659267,0.41998524267708365,0.41279415527723312,0.41192589813070335,0.41110235166991893,0.41026329666650924,0.40957443999195126]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.51409352831258881,0.51171165687424147,0.5029500079537953,0.50189212006180273,0.5008887078436145,0.49986639995663601,0.49902709429903702]
[null,null,null,null,"Coincident",0.44269164938028477,0.44064059341948575,0.43309584018243485,0.43218488116433018,0.43132083175422364,0.4304405110737699,0.42971777564639302]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.47011378916618268,0.47273483403474303,0.47537049212325427,0.47802084490540642,0.48068597430913323,0.48336596271914462,0.48606089297947336]
[null,null,null,null,"Coincident",0.40482020733754615,0.40707721819658427,0.40934681266169115,0.41162906089076662,0.41392403343286471,0.41623180123037451,0.41855243562121314]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.4932345186998468,0.49598446952883235,0.49874975227250579,0.50153045241152583,0.50432665590313475,0.50713844918381612,0.50996591917196621]
[null,null,null,null,"Coincident",0.42472972443597923,0.42709773764982789,0.42947895334576891,0.43187344513214726,0.43428128702769941,0.43670255346384174,0.43913731928697097]
[null,"Tarlton 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.24874000000000002,0.26680903225312658,0.27150544899439183,0.2791227766957633,0.28635160992672171,0.29337110398264682,0.3003789518903705]
[null,null,null,null,"Coincident",0.24874000000000002,0.26680903225312658,0.27150544899439183,0.2791227766957633,0.28635160992672171,0.29337110398264682,0.3003789518903705]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.6883068027087329,0.67343753042770915,0.6618130168580868,0.65538850836709717,0.64907843376131391,0.64271107609591416,0.63661341681232353]
[null,null,null,null,"Coincident",0.6335383044286832,0.61985217854421404,0.60915262626937883,0.60323931522820984,0.59743133258030612,0.59157062487968015,0.58595815568962251]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.76082365793002871,0.74438782715938134,0.73153860803080051,0.72443724272207255,0.71746236752907677,0.71042417419541559,0.70368409343100158]
[null,null,null,null,"Coincident",0.70028500127753179,0.68515696779401125,0.6733301596498551,0.66679384921515494,0.66037396409127924,0.65389579904438255,0.64769202578165308]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.62069143431538099,0.61152040735315061,0.60248488690976676,0.59358287080851302,0.58481238645583722,0.5761714904042452,0.56765826792165353]
[null,null,null,null,"Coincident",0.57130308362792059,0.56286179429494287,0.55454522924167782,0.54635154560439481,0.53827892774859853,0.53032558686670306,0.52248976058165097]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.68608464371301325,0.67594739931426551,0.66595993778114748,0.65612004599676566,0.64642554354413684,0.63687428222303188,0.62746414557395613]
[null,null,null,null,"Coincident",0.63149296238531116,0.62216233743334537,0.61296957714049716,0.60391264448734561,0.59498953255245279,0.58619826406765074,0.57753689097989935]
[null,"Tarpeena 11kV","Substation Rating","MVA","Non-Coincident",9.5,9.5,9.5,9.5,9.5,9.5,9.5]
[null,null,null,null,"Coincident",9.5,9.5,9.5,9.5,9.5,9.5,9.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.23014999999999997,0.24686861290125056,0.25121403508104551,0.25826206905415255,0.26495064334097845,0.27144552376620623,0.2779296284376005]
[null,null,null,null,"Coincident",0.23014999999999997,0.24686861290125056,0.25121403508104551,0.25826206905415255,0.26495064334097845,0.27144552376620623,0.2779296284376005]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6888769974624127,4.7553919770854209,4.8228505179314354,4.8912660050723087,4.9606520134564427,5.0310223106023182,5.1023908593302369]
[null,null,null,null,"Coincident",4.6888769974624127,4.7553919770854209,4.8228505179314354,4.8912660050723087,4.9606520134564427,5.0310223106023182,5.1023908593302369]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.8107065454685944,4.8789497619183519,4.9481610558318643,5.0183541600609036,5.0895430022672867,5.1617417076863976,5.2349646019299021]
[null,null,null,null,"Coincident",4.8107065454685944,4.8789497619183519,4.9481610558318643,5.0183541600609036,5.0895430022672867,5.1617417076863976,5.2349646019299021]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2199892977161717,4.2798527793768786,4.3405654661382922,4.4021394045650784,4.4645868121107988,4.5279200795420866,4.5921517733972133]
[null,null,null,null,"Coincident",4.2199892977161717,4.2798527793768786,4.3405654661382922,4.4021394045650784,4.4645868121107988,4.5279200795420866,4.5921517733972133]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3296358909217352,4.3910547857265163,4.4533449502486784,4.5165187440548138,4.5805887020405587,4.645567536917758,4.711468141736912]
[null,null,null,null,"Coincident",4.3296358909217352,4.3910547857265163,4.4533449502486784,4.5165187440548138,4.5805887020405587,4.645567536917758,4.711468141736912]
[null,"Tea Tree Gully 11kV","Substation Rating","MVA","Non-Coincident",49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874]
[null,null,null,null,"Coincident",49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874,49.068208955223874]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.472589999999999,13.378626950189046,13.614119755861385,13.996076036776593,14.358552007943754,14.710531067873765,15.061926154049674]
[null,null,null,null,"Coincident",12.472589999999999,13.378626950189046,13.614119755861385,13.996076036776593,14.358552007943754,14.710531067873765,15.061926154049674]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.455297539236156,32.443085724353551,32.374635683270292,32.445241207404848,32.487018818321445,32.531460463375311,32.588959322565159]
[null,null,null,null,"Coincident",29.303878650749535,29.292852606665587,29.23104908460212,29.294798791681842,29.332519784353014,29.372646132667146,29.424561835803711]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.332792447238113,33.320250461129568,33.249949734116512,33.322464222044424,33.365371375551206,33.411014590770648,33.470068048438421]
[null,null,null,null,"Coincident",30.096168546402275,30.084844390815039,30.021369884967132,30.086843194897249,30.125584051242562,30.166795296907576,30.220114646554933]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.025057588997676,29.123118447182897,29.221510602967737,29.320235175637723,29.41929328825988,29.518686067695501,29.618414644612969]
[null,null,null,null,"Coincident",26.206716003473826,26.295255123633613,26.384093372299148,26.473231760073006,26.562671300972074,26.652413012439087,26.742457915354194]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.80980899076863,29.910521123483935,30.011573511102547,30.112967303172166,30.214703653124207,30.316783718286963,30.419208659898715]
[null,null,null,null,"Coincident",26.915267814490221,27.006200769647368,27.097440940857155,27.188989366045845,27.280847086646332,27.373015147609987,27.465494597418527]
[null,"Teal Flat 11kV","Substation Rating","MVA","Non-Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,null,null,"Coincident",3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004,3.9000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.75714000000000004,0.81214035008495711,0.82643577893227382,0.84962217233830584,0.87162602693542668,0.89299267375340174,0.91432387084616495]
[null,null,null,null,"Coincident",0.75714000000000004,0.81214035008495711,0.82643577893227382,0.84962217233830584,0.87162602693542668,0.89299267375340174,0.91432387084616495]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2251936520592936,3.2318736898896492,3.2385675634490272,3.2452753013940612,3.251996932440739,3.2587324853645248,3.2654819890004827]
[null,null,null,null,"Coincident",3.2251936520592936,3.2318736898896492,3.2385675634490272,3.2452753013940612,3.251996932440739,3.2587324853645248,3.2654819890004827]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3181955305421171,3.3250681943458504,3.3319550928465218,3.3388562555271091,3.3457717119316568,3.3527014916653992,3.3596456243948909]
[null,null,null,null,"Coincident",3.3181955305421171,3.3250681943458504,3.3319550928465218,3.3388562555271091,3.3457717119316568,3.3527014916653992,3.3596456243948909]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9026742868533644,2.9086863209006841,2.9147108071041243,2.9207477712546552,2.9267972391966652,2.9328592368280724,2.9389337901004344]
[null,null,null,null,"Coincident",2.9026742868533644,2.9086863209006841,2.9147108071041243,2.9207477712546552,2.9267972391966652,2.9328592368280724,2.9389337901004344]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9863759774879055,2.9925613749112649,2.9987595835618692,3.0049706299743986,3.011194540738491,3.0174313424988597,3.023681061955402]
[null,null,null,null,"Coincident",2.9863759774879055,2.9925613749112649,2.9987595835618692,3.0049706299743986,3.011194540738491,3.0174313424988597,3.023681061955402]
[null,"Telowie 11kV","Substation Rating","MVA","Non-Coincident",1,1,1,1,1,1,1]
[null,null,null,null,"Coincident",1,1,1,1,1,1,1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.47925000000000001,0.51406379636291266,0.52311243238145155,0.53778881857137795,0.55171668833875276,0.56524122209408811,0.5787433170919839]
[null,null,null,null,"Coincident",0.47925000000000001,0.51406379636291266,0.52311243238145155,0.53778881857137795,0.55171668833875276,0.56524122209408811,0.5787433170919839]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.60416121505147047,0.60844842137123922,0.60291155171219157,0.59529728860962439,0.58811974774964904,0.58112181173437305,0.57505609573199079]
[null,null,null,null,"Coincident",0.60416121505147047,0.60844842137123922,0.60291155171219157,0.59529728860962439,0.58811974774964904,0.58112181173437305,0.57505609573199079]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.61228883600643336,0.61663371697835578,0.61102236127693288,0.60330566550770781,0.59603156708984006,0.58893948969312104,0.58279217321844834]
[null,null,null,null,"Coincident",0.61228883600643347,0.61663371697835578,0.61102236127693299,0.60330566550770781,0.59603156708984018,0.58893948969312115,0.58279217321844834]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.51318114609767385,0.49580870371183533,0.47902436117484015,0.46280820986218241,0.44714101510519977,0.43200419337601265,0.41737979024480915]
[null,null,null,null,"Coincident",0.51318114609767385,0.49580870371183533,0.47902436117484015,0.46280820986218241,0.44714101510519977,0.43200419337601265,0.41737979024480915]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.52008483625984347,0.50247868700362608,0.48546854914789739,0.46903424624269435,0.45315628486044679,0.43781583147399211,0.42299469011732538]
[null,null,null,null,"Coincident",0.52008483625984359,0.50247868700362619,0.4854685491478975,0.46903424624269441,0.45315628486044685,0.43781583147399222,0.42299469011732538]
[null,"Thebarton 11kV","Substation Rating","MVA","Non-Coincident",49,49,49,49,49,49,49]
[null,null,null,null,"Coincident",49,49,49,49,49,49,49]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.0415400000000004,5.4077687885560337,5.5029572297305869,5.6573476064274288,5.8038638558734608,5.9461371535445577,6.088174403446887]
[null,null,null,null,"Coincident",5.0415400000000004,5.4077687885560337,5.5029572297305869,5.6573476064274288,5.8038638558734608,5.9461371535445577,6.088174403446887]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.074651878353411,26.050847274838592,25.983570631718891,25.934654661835413,25.893064662889564,25.853632944967817,25.822705105867673]
[null,null,null,null,"Coincident",17.496185718019511,17.480212742963808,17.435069872102151,17.402247079389475,17.374340039672756,17.347881214329352,17.327128522432346]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.991117606609819,27.965563384077122,27.893341962348195,27.84083070842091,27.796183878343058,27.753853961191044,27.720652951044897]
[null,null,null,null,"Coincident",18.782141153214802,18.764994177470026,18.716533342277142,18.681298100967531,18.651339916505194,18.622936388995978,18.600658391105426]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.925741892576511,24.939072146194608,24.952409528814613,24.96575404424911,24.979105696312715,24.992464488822087,25.005830425595931]
[null,null,null,null,"Coincident",16.72526296214841,16.734207610539446,16.743157042516547,16.752111260637967,16.761070267463335,16.770034065553638,16.779002657471239]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.757763670330139,26.772073686758766,26.786391356165151,26.800716682642104,26.815049670284601,26.829390323189831,26.843738645457165]
[null,null,null,null,"Coincident",17.954556201136722,17.964158273917263,17.97376548187356,17.983377827751895,17.992995314300028,18.002617944267175,18.012245720404032]
[null,"Tintinara 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.37734000000000001,0.40475082507998222,0.41187531608725497,0.42343084569582423,0.43439702697495042,0.44504563953048143,0.45567658481270568]
[null,null,null,null,"Coincident",0.37734000000000001,0.40475082507998222,0.41187531608725497,0.42343084569582423,0.43439702697495042,0.44504563953048143,0.45567658481270568]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1871886548614123,1.1918815283580628,1.1965929524545404,1.2013230004800652,1.2060717460537227,1.2108392630856095,1.2156256257779836]
[null,null,null,null,"Coincident",1.1871886548614123,1.1918815283580628,1.1965929524545404,1.2013230004800652,1.2060717460537227,1.2108392630856095,1.2156256257779836]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2848179039951217,1.2898966990669838,1.2949955702595957,1.3001145969324546,1.3052538587587603,1.3104134357266559,1.3155934081404712]
[null,null,null,null,"Coincident",1.2848179039951217,1.2898966990669838,1.2949955702595957,1.3001145969324546,1.3052538587587603,1.3104134357266559,1.3155934081404712]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.068469789375271,1.0726933755222565,1.0769336572090864,1.0811907004320587,1.0854645714483504,1.0897553367770485,1.0940630632001853]
[null,null,null,null,"Coincident",1.068469789375271,1.0726933755222565,1.0769336572090864,1.0811907004320587,1.0854645714483504,1.0897553367770485,1.0940630632001853]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1563361135956094,1.1609070291602854,1.1654960132336361,1.170103137239209,1.1747284728828844,1.1793720921539903,1.1840340673264242]
[null,null,null,null,"Coincident",1.1563361135956094,1.1609070291602854,1.1654960132336361,1.170103137239209,1.1747284728828844,1.1793720921539903,1.1840340673264242]
[null,"Tonsley Park 11kV","Substation Rating","MVA","Non-Coincident",40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982]
[null,null,null,null,"Coincident",40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982,40.055389803311982]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.3649,3.6093338933365984,3.6728659858536177,3.775911519271423,3.8737015849578906,3.9686597563367698,4.063460381184802]
[null,null,null,null,"Coincident",3.3649,3.6093338933365984,3.6728659858536177,3.775911519271423,3.8737015849578906,3.9686597563367698,4.063460381184802]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.826941910161583,22.10946094400057,22.348884812462565,22.51771166670656,22.693325971214112,22.8725343575979,23.035454481112797]
[null,null,null,null,"Coincident",17.567277943347982,17.794661624129443,17.987360430075562,18.123239669824883,18.264581746548679,18.408816497634778,18.539941742029107]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.489594038489695,22.780690171211209,23.027382796637045,23.201335127218687,23.382280970753822,23.566930010213991,23.734796285463702]
[null,null,null,null,"Coincident",18.100609372276722,18.334896277551888,18.533445297165684,18.673449744549963,18.819082877178374,18.967696503930128,19.102802627672244]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.236455811881338,20.480827398160841,20.728149969174819,20.9784591604529,21.231791037852581,21.488182102755786,21.747669297328176]
[null,null,null,null,"Coincident",16.287185135637142,16.483866081382928,16.682922108770953,16.884381898834789,17.088274478954705,17.294629227040083,17.503475875762348]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.850821789889373,21.102612342711122,21.357443470294339,21.61535189004076,21.876374762744465,22.140549697946213,22.407914759352401]
[null,null,null,null,"Coincident",16.781653757903431,16.984305812558404,17.189405054829582,17.396981036488548,17.607063666168447,17.819683213673379,18.034870314339834]
[null,"Tumby Bay 11kV","Substation Rating","MVA","Non-Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,null,null,"Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.9820199999999997,2.1259983842821493,2.1634205596842659,2.224117254428466,2.2817183320212302,2.3376513448407392,2.3934915583571281]
[null,null,null,null,"Coincident",1.9820199999999997,2.1259983842821493,2.1634205596842659,2.224117254428466,2.2817183320212302,2.3376513448407392,2.3934915583571281]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2782614103140655,2.158954911426493,2.0511931330776285,2.007525503465025,1.9667208607972715,1.9273437442651837,1.8893706213865942]
[null,null,null,null,"Coincident",2.0502395423573745,1.9428739430577764,1.8458976004285363,1.8066004852917645,1.7698798124442803,1.7344437904791927,1.7002712421842421]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.279443410345809,2.1600750132560225,2.0522573262985793,2.008567041191152,1.9677412283939701,1.9283436823568307,1.8903508583885222]
[null,null,null,null,"Coincident",2.0513032408395495,1.9438819384756734,1.8468552829018576,1.807537779766093,1.7707980556208625,1.7353436488563407,1.7011533712731763]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0222780489042367,1.9183825895051958,1.819824806836408,1.7263304753153359,1.637639457824128,1.5535049819083036,1.4736929531610614]
[null,null,null,null,"Coincident",1.8198765087862443,1.7263795210538599,1.6376859838154103,1.553549117605511,1.4737348213666446,1.3980210210901618,1.3261970519211443]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0233272404970792,1.9193778784002393,1.8207689623093974,1.7272261243692086,1.6384890924983448,1.554310966212658,1.4744575296532634]
[null,null,null,null,"Coincident",1.820820691083068,1.7272751955534802,1.6385356426280877,1.5543551248082015,1.4744994195807701,1.3987463377214429,1.3268851050788604]
[null,"Two Wells 11kV","Substation Rating","MVA","Non-Coincident",16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001]
[null,null,null,null,"Coincident",16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.8897699999999997,2.0270471370949221,2.0627275562681184,2.1205992189288114,2.1755193450640058,2.2288490438742716,2.2820902625788588]
[null,null,null,null,"Coincident",1.8897699999999997,2.0270471370949221,2.0627275562681184,2.1205992189288114,2.1755193450640058,2.2288490438742716,2.2820902625788588]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2946179624575658,3.3071184488809005,3.3284185538647706,3.3606623497510264,3.3945353302786474,3.4295885296038544,3.4677064965709059]
[null,null,null,null,"Coincident",3.168657814919555,3.1806803815560976,3.2011661388987793,3.2321771869115947,3.2647551324234931,3.2984681744955693,3.3351288117212881]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3451238858666046,3.357816002584276,3.379442634492718,3.4121807221918652,3.4465729696510876,3.4821635284578898,3.5208658372642936]
[null,null,null,null,"Coincident",3.2172327910574268,3.2294396615606527,3.2502394620194455,3.2817259040335127,3.3148032638142571,3.34903312098908,3.3862557594413287]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9529103944015764,2.9677441043009107,2.982652330159075,2.9976354463010466,3.0126938289321941,3.0278278561477241,3.0430379079421748]
[null,null,null,null,"Coincident",2.8400144431308263,2.8542810292213465,2.8686192823694658,2.8830295625889337,2.8975122317019988,2.9120676533484966,2.9266961929949771]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9981779999063289,3.0132391080122489,3.028375874393757,3.0435886791141669,3.0588779041460117,3.0742439333806306,3.0896871526378136]
[null,null,null,null,"Coincident",2.8835513732331362,2.8980366636203629,2.912594719708784,2.9272259070310969,2.9419305929562225,2.9567091466985325,2.971561939327116]
[null,"Uley 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.15024999999999999,0.16116449745128353,0.16400134160733043,0.16860254562409921,0.17296908173791886,0.17720916769877254,0.18144221886921352]
[null,null,null,null,"Coincident",0.15024999999999999,0.16116449745128353,0.16400134160733043,0.16860254562409921,0.17296908173791886,0.17720916769877254,0.18144221886921352]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,null,null,null,"Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218]
[null,null,null,null,"Coincident",0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218,0.30239939679581218]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.27,0.27,0.27,0.27,0.27,0.27,0.27]
[null,null,null,null,"Coincident",0.27,0.27,0.27,0.27,0.27,0.27,0.27]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096]
[null,null,null,null,"Coincident",0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096,0.27215945711623096]
[null,"Uley South 11kV","Substation Rating","MVA","Non-Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,null,null,"Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.50163982783618555,0.50398741259542079,0.5075168061693377,0.50643586377228311,0.50543003022725419,0.50439938024449471,0.5036150820780686]
[null,null,null,null,"Coincident",0.34985213085254269,0.35148937631193555,0.3539508352989108,0.35319696772310522,0.35249548233561268,0.35177668954320851,0.35122970668913273]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.51715446168678914,0.51957465216022758,0.52321320223643053,0.5220988286312197,0.52106188683222077,0.51999936107679867,0.51919080626605008]
[null,null,null,null,"Coincident",0.3606722998479821,0.36236018176488199,0.36489776834939253,0.36412058528155172,0.36339740446970376,0.3626563809723799,0.36209248112281722]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.45428873952567012,0.45505546978215311,0.45582349409511397,0.45659281464860918,0.45736343363038134,0.45813535323186544,0.45890857564819509]
[null,null,null,null,"Coincident",0.31682867811937876,0.31736340881485953,0.31789904200729352,0.31843557921987869,0.31897302197838401,0.31951137181115336,0.32005063024911024]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.4683389067274949,0.46912935029087943,0.46992112793310709,0.47071424190578265,0.4715086944643106,0.47230448786790252,0.47310162437958253]
[null,null,null,null,"Coincident",0.32662750321585438,0.32717877197408196,0.32773097114153971,0.32828410228853472,0.3288381669880247,0.32939316681562197,0.32994910334959815]
[null,"Uraidla 11kV","Substation Rating","MVA","Non-Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,null,null,"Coincident",17.2,17.2,17.2,17.2,17.2,17.2,17.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.4458800000000003,3.6961964624121726,3.7612575242453765,3.866782961165864,3.9669264517741096,4.0641698954399104,4.161252001045229]
[null,null,null,null,"Coincident",3.4458800000000003,3.6961964624121726,3.7612575242453765,3.866782961165864,3.9669264517741096,4.0641698954399104,4.161252001045229]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.3131782346120771,4.3101895241475949,4.3133927297620351,4.3220223788200771,4.3356553327261063,4.3536160768177714,4.3748638664561526]
[null,null,null,null,"Coincident",4.028374662552876,4.0255832996984013,4.0285749943686122,4.0366348188695271,4.0493675748799536,4.0661423526618803,4.0859871290097809]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.480824569042027,4.4777196921854348,4.4810474012751493,4.4900124709797078,4.5041753159835496,4.5228341654506057,4.5449078226636273]
[null,null,null,null,"Coincident",4.1849511379853164,4.1820512793244635,4.1851592563780846,4.1935323533570266,4.2067600112138939,4.2241867977589758,4.2448029088005397]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7124071856988206,3.6421688986332552,3.5732595113147081,3.5056538811235143,3.4393273411352783,3.3742556911207786,3.3104151887161519]
[null,null,null,null,"Coincident",3.467273140706042,3.4016727596029677,3.3373135296368903,3.2741719683810477,3.2122250376933015,3.151450135310327,3.0918250866008403]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8567025110344284,3.7837341741720136,3.7121463892627844,3.6419130364336914,3.5730084899964711,3.5054076090977255,3.4390857285459084]
[null,null,null,null,"Coincident",3.6020404980673049,3.5338903351488433,3.4670295649255229,3.4014337922462383,3.3370790835131405,3.273941957949106,3.2119993790304253]
[null,"Uraidla 33kV","Substation Rating","MVA","Non-Coincident",31.4,31.4,31.4,31.4,31.4,31.4,31.4]
[null,null,null,null,"Coincident",31.4,31.4,31.4,31.4,31.4,31.4,31.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.4658099999999994,8.0081432061016109,8.1491038681226193,8.3777342505547825,8.5947041605974839,8.8053908572191215,9.0157280003724658]
[null,null,null,null,"Coincident",7.4658099999999994,8.0081432061016109,8.1491038681226193,8.3777342505547825,8.5947041605974839,8.8053908572191215,9.0157280003724658]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.331964486567411,16.559218226307038,16.62455191411695,16.752659044042726,16.89207992292997,17.040347564874512,17.200814655463361]
[null,null,null,null,"Coincident",14.879998792433902,15.087048922605502,15.146574229344708,15.263292211444508,15.390318112779802,15.525404270657893,15.671605305821258]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.720208669663897,16.952864695369389,17.019751498499463,17.150903996791538,17.293639194986461,17.445431461881892,17.609713183255103]
[null,null,null,null,"Coincident",15.233726782743743,15.445698917779767,15.506639262747077,15.626131869886644,15.756177436574294,15.894474868580255,16.044151401226582]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.061333166209236,14.042691080336354,14.02407370957132,14.005481021147599,13.986912982342098,13.968369560475105,13.949850722910236]
[null,null,null,null,"Coincident",12.81123411119907,12.794249368457002,12.777287143567898,12.760347406678278,12.743430127974239,12.726535277681405,12.709662826064873]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.395599800994813,14.376514554630923,14.357454610903526,14.338419936267149,14.31941049722081,14.30042626030793,14.281467192116292]
[null,null,null,null,"Coincident",13.115783335883656,13.098394831084891,13.081029379434488,13.063686950369288,13.046367513366652,13.029071037944407,13.011797493660787]
[null,"Verdun 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.99521999999999999,1.0675150159964486,1.0863055919763553,1.1167828649318869,1.1457057539248694,1.1737910674021459,1.201829784113269]
[null,null,null,null,"Coincident",0.99521999999999999,1.0675150159964486,1.0863055919763553,1.1167828649318869,1.1457057539248694,1.1737910674021459,1.201829784113269]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0645671109083763,1.0685242815319016,1.0724961616079201,1.07648280581388,1.080484269030475,1.0845006063423992,1.0885318730391051]
[null,null,null,null,"Coincident",1.0645671109083763,1.0685242815319016,1.0724961616079201,1.07648280581388,1.080484269030475,1.0845006063423992,1.0885318730391051]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0679697732381328,1.0719395921158406,1.0759241674616777,1.0799235541278571,1.083937807170487,1.0879669818503281,1.0920111336335536]
[null,null,null,null,"Coincident",1.0679697732381328,1.0719395921158406,1.0759241674616777,1.0799235541278571,1.083937807170487,1.0879669818503281,1.0920111336335536]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.95811039981753865,0.96167185337871142,0.96524654544712807,0.96883452523249203,0.97243584212742751,0.9760505457081593,0.97967868573519468]
[null,null,null,null,"Coincident",0.95811039981753865,0.96167185337871142,0.96524654544712807,0.96883452523249203,0.97243584212742751,0.9760505457081593,0.97967868573519468]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.96117279591431948,0.96474563290425652,0.96833175071550992,0.9719311987150715,0.9755440264534383,0.97917028366529524,0.98281002027019837]
[null,null,null,null,"Coincident",0.96117279591431948,0.96474563290425652,0.96833175071550992,0.9719311987150715,0.9755440264534383,0.97917028366529524,0.98281002027019837]
[null,"Victor Harbor 11kV","Substation Rating","MVA","Non-Coincident",62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341]
[null,null,null,null,"Coincident",62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341,62.733333333333341]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",14.686439999999999,15.753295986345613,16.030588109388098,16.48034056675937,16.907155013637542,17.321609376758474,17.735376112409796]
[null,null,null,null,"Coincident",14.686439999999999,15.753295986345613,16.030588109388098,16.48034056675937,16.907155013637542,17.321609376758474,17.735376112409796]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.756110733008981,24.67600650446407,24.598922992060494,24.664991852060957,24.746433165373521,24.835019736883222,24.904232275397359]
[null,null,null,null,"Coincident",23.384209596554737,23.308544477341687,23.235732676250478,23.298140220259249,23.375068327459076,23.458745726464279,23.524122736802425]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.807685963702752,24.727414851348371,24.650170748293956,24.716377251752753,24.79798823446805,24.886759361335063,24.956116092637771]
[null,null,null,null,"Coincident",23.432926699880895,23.357103945002816,23.284140452659337,23.346678012384789,23.423766386474618,23.507618113394415,23.573131325837434]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.667715954742096,21.512551076584732,21.358497351050183,21.205546821053282,21.053691586490409,20.902923803831452,20.753235685714674]
[null,null,null,null,"Coincident",20.466963362250141,20.320397204423998,20.174880622846153,20.030406101386582,19.886966177739069,19.744553443035795,19.603160541464653]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.712857029647811,21.557368891327616,21.402994220531539,21.249725043597145,21.097553443962266,20.946471561756102,20.79647159339325]
[null,null,null,null,"Coincident",20.509602869254831,20.362731365266548,20.216911624143751,20.072136114097805,19.928397357276026,19.785687929375452,19.644000459259374]
[null,"Virginia 11kV","Substation Rating","MVA","Non-Coincident",14.9,14.9,14.9,14.9,14.9,14.9,14.9]
[null,null,null,null,"Coincident",14.9,14.9,14.9,14.9,14.9,14.9,14.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.65903,2.8521879112005752,2.902392594836205,2.9838218095896738,3.0610980193915367,3.1361363939172522,3.2110502711467874]
[null,null,null,null,"Coincident",2.65903,2.8521879112005752,2.902392594836205,2.9838218095896738,3.0610980193915367,3.1361363939172522,3.2110502711467874]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0159100823138134,5.9597205067437633,5.976500754370357,6.0122784462819654,6.0529863435573628,6.0969679360961271,6.1466405684708452]
[null,null,null,null,"Coincident",5.4457942206137879,5.3949296196288561,5.4101196364833344,5.4425067475227671,5.4793568381462014,5.5191703824285776,5.5641356379938456]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6282487587011101,6.5663398406108842,6.5848280915953286,6.6242474710005306,6.6690988843183989,6.7175572110157686,6.7722858488069289]
[null,null,null,null,"Coincident",6.0001027756455265,5.9440608428827062,5.9607969990058409,5.9964806820409553,6.0370816159131016,6.0809476431406315,6.1304897565211789]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5932399460964284,5.6358013141071472,5.6786865498697239,5.7218981178331552,5.7654385011994904,5.8093102020665297,5.8535157415716128]
[null,null,null,null,"Coincident",5.0631796945413869,5.1017076061562241,5.1405286932186947,5.1796451866268551,5.2190593342546228,5.2587734010809557,5.2987896693200094]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.1625564914647306,6.2094500338923408,6.2567004094499108,6.3043103334341772,6.352282541803735,6.4006197913362639,6.4493248597869526]
[null,null,null,null,"Coincident",5.5785432405460593,5.6209927750042228,5.6637653262246488,5.7068633521807914,5.7502893295498767,5.7940457538552366,5.8381351396097099]
[null,"Waikerie 11kV","Substation Rating","MVA","Non-Coincident",12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061]
[null,null,null,null,"Coincident",12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061,12.04672860249061]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.1216899999999996,3.3484565727034754,3.4073966594488332,3.5029942139720074,3.5937161582059485,3.6818108932684268,3.7697594690305158]
[null,null,null,null,"Coincident",3.1216899999999996,3.3484565727034754,3.4073966594488332,3.5029942139720074,3.5937161582059485,3.6818108932684268,3.7697594690305158]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.4774304869168056,7.3746941621901252,7.3054329764940107,7.2527961358134094,7.2036363280595248,7.1556693816186936,7.1103907550959145]
[null,null,null,null,"Coincident",6.7528273324981534,6.6600467091451714,6.5974973041499263,6.5499612558956182,6.5055652974120681,6.4622466055768362,6.4213557210281955]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.6133919629152915,7.508787592424369,7.4382670365404442,7.3846731047088978,7.3346194283949897,7.2857803030888855,7.2396783791908925]
[null,null,null,null,"Coincident",6.875613411605916,6.7811457661512646,6.7174590306999402,6.6690586385650574,6.6238554321834027,6.5797490802969607,6.5381146803083778]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.9002366099853996,6.7964899043943765,6.6943030553023917,6.5936526098944022,6.4945154679740407,6.3968688766619097,6.3006904251735882]
[null,null,null,null,"Coincident",6.2315666407253945,6.1378735478377369,6.045589152980761,5.9546922760431009,5.8651620553614237,5.7769779429324863,5.6901196996971839]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.0257030193186463,6.9200698962949483,6.8160249925069696,6.7135444286991479,6.6126046846462296,6.5131825937551655,6.4152553377481691]
[null,null,null,null,"Coincident",6.3448746814672488,6.2494779751227814,6.155515581044237,6.0629659340041036,5.971807793013217,5.882020236445757,5.7935826572375468]
[null,"Walker Flat 11kV","Substation Rating","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.43561,0.46725368875044004,0.47547836550794809,0.48881833543636505,0.50147794805893398,0.51377095202171252,0.52604356047665957]
[null,null,null,null,"Coincident",0.43561,0.46725368875044004,0.47547836550794809,0.48881833543636505,0.50147794805893398,0.51377095202171252,0.52604356047665957]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2453028158106725,1.2142411027120363,1.1913838141530977,1.1862931458509278,1.1819984016300986,1.1779878084499369,1.1743790655539295]
[null,null,null,null,"Coincident",0.95315582610994098,0.92938116469182874,0.91188617673996597,0.90798977492556254,0.90470257407468313,0.90163286267012055,0.89887072781216382]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2996822304905613,1.2672641261946893,1.2434087141615053,1.2380957484718353,1.2336134629767366,1.2294277367230064,1.225661408600399]
[null,null,null,null,"Coincident",0.9947778759957292,0.96996503161061876,0.9517060791092703,0.94763953068688145,0.94420878558641352,0.94100502717955004,0.93812227645617041]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1359713673747547,1.1279990799783826,1.1200827423780668,1.1122219619161517,1.1044163486906671,1.0966655155359883,1.0889690780036336]
[null,null,null,null,"Coincident",0.86947344321426379,0.8633714477134119,0.85731227623367656,0.85129562823455673,0.84532120528475541,0.83938871104737678,0.83349785126522846]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1855765375122191,1.1772561192702644,1.1689940940190029,1.1607900519543528,1.1526435861482505,1.1445542925284691,1.136521769858575]
[null,null,null,null,"Coincident",0.90744128229838206,0.90107282715453996,0.89474906605505133,0.88846968533552562,0.88223437353288026,0.87604282136989142,0.86989472173985438]
[null,"Wallaroo 11kV","Substation Rating","MVA","Non-Coincident",16.2,16.2,16.2,16.2,16.2,16.2,16.2]
[null,null,null,null,"Coincident",16.2,16.2,16.2,16.2,16.2,16.2,16.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.8652999999999995,4.1460840732009725,4.219064131213405,4.3374337411036965,4.4497663337209818,4.5588458962134126,4.6677444831625339]
[null,null,null,null,"Coincident",3.8652999999999995,4.1460840732009725,4.219064131213405,4.3374337411036965,4.4497663337209818,4.5588458962134126,4.6677444831625339]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7253062724558932,7.683494779264934,7.7279892126988399,7.8007806673179152,7.8795819742320248,7.960969834740105,8.045661308600188]
[null,null,null,null,"Coincident",7.7253062724558932,7.683494779264934,7.7279892126988399,7.8007806673179152,7.8795819742320248,7.960969834740105,8.045661308600188]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.1332819376406515,8.0892623673657109,8.1361065647360888,8.2127421571887496,8.2957049839794674,8.381390961009755,8.4705550161714669]
[null,null,null,null,"Coincident",8.1332819376406533,8.0892623673657127,8.1361065647360906,8.2127421571887513,8.2957049839794692,8.381390961009755,8.4705550161714669]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1113426304191547,7.1684704263225454,7.2260571489342089,7.2841064849660206,7.3426221507464469,7.4016078924584638,7.46106748637939]
[null,null,null,null,"Coincident",7.1113426304191547,7.1684704263225454,7.2260571489342089,7.2841064849660206,7.3426221507464469,7.4016078924584638,7.46106748637939]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.4868946975710067,7.547039428947536,7.6076673230849252,7.6687822613913745,7.7303881564557342,7.7924889522979912,7.8550886246217617]
[null,null,null,null,"Coincident",7.4868946975710085,7.5470394289475369,7.6076673230849261,7.6687822613913754,7.7303881564557351,7.7924889522979912,7.8550886246217635]
[null,"Warooka 11kV","Substation Rating","MVA","Non-Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,null,null,"Coincident",5.4,5.4,5.4,5.4,5.4,5.4,5.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.16934,1.2542834838581289,1.276361589318574,1.3121710529123738,1.3461541832906359,1.3791531990474721,1.412097465640773]
[null,null,null,null,"Coincident",1.16934,1.2542834838581289,1.276361589318574,1.3121710529123738,1.3461541832906359,1.3791531990474721,1.412097465640773]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.237847647551753,2.1579877915169416,2.0790816114635464,2.0467580647646866,2.0164390940611749,1.9870488825651871,1.9585581531156959]
[null,null,null,null,"Coincident",1.7311241277465459,1.6693472128741358,1.6083080298590702,1.583303614725647,1.5598498725682173,1.5371145874848291,1.5150751116424628]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2940208206216393,2.2121563681080247,2.1312695302054361,2.0981346163051788,2.0670545961216042,2.0369266483285409,2.0077207608663921]
[null,null,null,null,"Coincident",1.7745778165353017,1.7112502128415823,1.6486788591287926,1.6230467974527918,1.5990043328598615,1.5756983596399599,1.5531056614671024]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9592256962086161,1.8965243718795135,1.8358296852135609,1.7770774175558213,1.7202054054483265,1.6651534748573722,1.6118633775057463]
[null,null,null,null,"Coincident",1.5155915006628364,1.4670878522994102,1.4201364717492659,1.3746876816078075,1.3306933943021071,1.2881070612113397,1.2468836234155241]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0084050602446344,1.9441298430961955,1.8819116330830488,1.8216845995702711,1.7633850187082891,1.7069512060091854,1.6523234510807718]
[null,null,null,null,"Coincident",1.5536350125896301,1.5039138533572132,1.4557839260778496,1.4091943063731158,1.3640956996033031,1.3204403887107015,1.2781821837320648]
[null,"Wasleys 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.86924000000000001,0.93238354585393468,0.94879551533281781,0.97541482035468863,1.0006765032270786,1.0252066351446323,1.0496960687512487]
[null,null,null,null,"Coincident",0.86924000000000001,0.93238354585393468,0.94879551533281781,0.97541482035468863,1.0006765032270786,1.0252066351446323,1.0496960687512487]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2329030267702756,2.2283120860269192,2.223730584447134,2.2191585026236109,2.2145958211889418,2.2100425208155401,2.2054985822155562]
[null,null,null,null,"Coincident",2.2329030267702756,2.2283120860269192,2.223730584447134,2.2191585026236109,2.2145958211889418,2.2100425208155401,2.2054985822155562]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3123403122488142,2.3075860451692614,2.3028415530589648,2.2981068158201849,2.293381813396504,2.2886665257727401,2.283960932974864]
[null,null,null,null,"Coincident",2.3123403122488142,2.3075860451692614,2.3028415530589648,2.2981068158201849,2.293381813396504,2.2886665257727401,2.283960932974864]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0096127240932482,2.0054808774242274,2.0013575260024208,1.9972426523612499,1.9931362390700478,1.989038268733986,1.9849487239940007]
[null,null,null,null,"Coincident",2.0096127240932482,2.0054808774242274,2.0013575260024208,1.9972426523612499,1.9931362390700478,1.989038268733986,1.9849487239940007]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0811062810239331,2.0768274406523353,2.0725573977530685,2.0682961342381665,2.0640436320568538,2.0597998731954661,2.0555648396773778]
[null,null,null,null,"Coincident",2.0811062810239331,2.0768274406523353,2.0725573977530685,2.0682961342381665,2.0640436320568538,2.0597998731954661,2.0555648396773778]
[null,"Waterloo Town 11kV","Substation Rating","MVA","Non-Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,null,null,"Coincident",0.65,0.65,0.65,0.65,0.65,0.65,0.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",5.3990000000000003E-2,5.7911954857868875E-2,5.8931330671412777E-2,6.058470175204736E-2,6.2153748572580624E-2,6.3677357497881726E-2,6.519843858069109E-2]
[null,null,null,null,"Coincident",5.3990000000000003E-2,5.7911954857868875E-2,5.8931330671412777E-2,6.058470175204736E-2,6.2153748572580624E-2,6.3677357497881726E-2,6.519843858069109E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.47131253166599663,0.46299219556583632,0.45380736599275434,0.44966396129172209,0.44569692119477144,0.44200132004253084,0.43847969774312823]
[null,null,null,null,"Coincident",0.42767248243766359,0.42012254782825886,0.41178816543786967,0.40802840932026629,0.40442868775081109,0.40107527189044462,0.39787972572987557]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.51229623007173541,0.50325238648460469,0.49326887607908076,0.48876517531708918,0.48445317521170805,0.48043621743753351,0.47660836711209587]
[null,null,null,null,"Coincident",0.46486139395398218,0.45665494329158574,0.44759583199768443,0.44350914056550689,0.4395963997291425,0.43595138248961374,0.43247796274986477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.41500614052524981,0.41080137851977766,0.40663921835026939,0.4025192283831569,0.39844098135809997,0.39440405434367753,0.39040802869352798]
[null,null,null,null,"Coincident",0.37657964603217109,0.37276421384202046,0.36898743887339258,0.36524892945879051,0.3615482978990166,0.35788516042296664,0.35425913714783092]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.45109363100570632,0.44652323752149742,0.44199915038072757,0.4375209004164749,0.43308802321532602,0.42870005906921471,0.42435655292774777]
[null,null,null,null,"Coincident",0.40932570220888165,0.40517849330654404,0.40107330312325284,0.39700970593346796,0.39298728032501806,0.38900560915539856,0.38506427950851191]
[null,"Whitmore Square 11kV","Substation Rating","MVA","Non-Coincident",72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314]
[null,null,null,null,"Coincident",72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314,72.410188271083314]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.5278500000000002,1.6388364554472117,1.6676835259551401,1.7144718757522794,1.7588739536324749,1.80199019546469,1.845034902491367]
[null,null,null,null,"Coincident",1.5278500000000002,1.6388364554472117,1.6676835259551401,1.7144718757522794,1.7588739536324749,1.80199019546469,1.845034902491367]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.656308862305174,41.1400020387672,41.704436414160945,41.94093214818173,42.170310916370426,42.40713147352065,42.663073676390482]
[null,null,null,null,"Coincident",38.091604330705991,38.544784897531535,39.073613300792751,39.295190275641346,39.510099241167467,39.73198054846705,39.971777258893113]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.537111730619358,43.043181053345791,43.633726746316619,43.881163017423468,44.121153084503085,44.368929205393059,44.636711559096817]
[null,null,null,null,"Coincident",39.853761316637026,40.327906484868869,40.881199036635756,41.113026391351816,41.337877267742421,41.570023033643196,41.820912987735547]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",38.108140693874581,38.606741990656992,39.11186691332685,39.623600816043876,40.142030169729026,40.667242576676045,41.199326785354188]
[null,null,null,null,"Coincident",35.704181164262287,36.171329408834524,36.644589752194371,37.124042164141635,37.60976766078916,38.101848318252692,38.600367286519784]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",39.871062669056961,40.392729777158088,40.92122230082272,41.45662954278221,41.999041974191698,42.548551249917573,43.105250224025013]
[null,null,null,null,"Coincident",37.355893486991491,37.844652492178888,38.339806348160977,38.841438724223146,39.349634384367363,39.864479201635312,40.386060172618919]
[null,"Whyalla City 11kV","Substation Rating","MVA","Non-Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,null,null,"Coincident",28.5,28.5,28.5,28.5,28.5,28.5,28.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.7571599999999989,8.3206575244538996,8.4671191152260832,8.7046716992574851,8.9301087660174012,9.1490174196752765,9.3675628786922349]
[null,null,null,null,"Coincident",7.7571599999999989,8.3206575244538996,8.4671191152260832,8.7046716992574851,8.9301087660174012,9.1490174196752765,9.3675628786922349]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.42678933116618,18.152587724437492,17.921636962878843,17.956185903896138,17.997039656553763,18.016809075829773,18.062515970421337]
[null,null,null,null,"Coincident",8.6633412527124598,8.5344255719370317,8.4258442437415475,8.4420874025780357,8.4612947639021439,8.4705893416214622,8.4920784040040633]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.46786994745057,18.193057036669497,17.961591394333428,17.996217358632613,18.03716219049598,18.056975683642531,18.102784477016598]
[null,null,null,null,"Coincident",8.6826552738013891,8.5534521888819288,8.44462878987318,8.4609081611481685,8.4801583432928886,8.4894736423095498,8.5110106123287004]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.708323368257783,16.669412925150066,16.630593096914318,16.591863672526085,16.553224441452347,16.514675193650376,16.476215719566593]
[null,null,null,null,"Coincident",7.8554057626883624,7.8371120468989135,7.8188609336238972,7.8006523236503247,7.7824861179962541,7.7643622179102527,7.7462805248708619]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.745572842852141,16.706575652945837,16.66766927992796,16.628853512303607,16.590128139070384,16.551492949717311,16.512947734223619]
[null,null,null,null,"Coincident",7.8729185753707851,7.8545840756387157,7.8362922733989677,7.8180430692173672,7.7998363638913029,7.7816720584491845,7.7635500541499116]
[null,"Whyalla North 11kV","Substation Rating","MVA","Non-Coincident",2.9,2.9,2.9,2.9,2.9,2.9,2.9]
[null,null,null,null,"Coincident",2.9,2.9,2.9,2.9,2.9,2.9,2.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",8.4970000000000004E-2,9.1142411636842335E-2,9.2746715450082298E-2,9.5348807332310867E-2,9.7818188853716903E-2,0.10021605976282665,0.10260995232823343]
[null,null,null,null,"Coincident",8.4970000000000004E-2,9.1142411636842335E-2,9.2746715450082298E-2,9.5348807332310867E-2,9.7818188853716903E-2,0.10021605976282665,0.10260995232823343]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.19832403222203995,0.19343764126084992,0.18464025471715062,0.18378848561266214,0.18292304518169147,0.18179611431245798,0.18091768382490267]
[null,null,null,null,"Coincident",6.8387597317944804E-2,6.6702634917534448E-2,6.3669053350741592E-2,6.3375339866435218E-2,6.3076912131617743E-2,6.2688315280157919E-2,6.2385408215483676E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.19844190684298002,0.1935526116372773,0.18474999633439798,0.18389772097779675,0.18303176616910996,0.18190416550435271,0.18102521291839316]
[null,null,null,null,"Coincident",6.8428243738958616E-2,6.6742279874923205E-2,6.3706895287723442E-2,6.3413007233723021E-2,6.3114402127279284E-2,6.272557431184575E-2,6.2422487213239022E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.17639665108163841,0.1728654361823182,0.16940491127959784,0.16601366125835068,0.16269029933208107,0.15943346647582449,0.15624183087040056]
[null,null,null,null,"Coincident",6.0826431407461516E-2,5.9608771097351097E-2,5.8415486648137178E-2,5.7246090089086439E-2,5.6100103217958983E-2,5.4977057405456713E-2,5.3876493403586391E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.17650149308262228,0.17296817939268627,0.16950559771421062,0.16611233209098983,0.16278699491228651,0.15952822634539471,0.1563346937795623]
[null,null,null,null,"Coincident",6.0862583821593881E-2,5.9644199790581463E-2,5.8450206108348488E-2,5.7280114514134423E-2,5.6133446521478107E-2,5.5009733222549893E-2,5.3908515096400794E-2]
[null,"Whyalla Stuart 11kV","Substation Rating","MVA","Non-Coincident",31,31,31,31,31,31,31]
[null,null,null,null,"Coincident",31,31,31,31,31,31,31]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.2126399999999995,6.6639401227670021,6.7812398996563408,6.9714936375780603,7.1520441661781309,7.3273661471687337,7.5023972488228328]
[null,null,null,null,"Coincident",6.2126399999999995,6.6639401227670021,6.7812398996563408,6.9714936375780603,7.1520441661781309,7.3273661471687337,7.5023972488228328]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.908611643937839,16.662561673352045,16.426167203341286,16.445646983219827,16.469971086497701,16.474440361362756,16.502445833394532]
[null,null,null,null,"Coincident",6.6435441216738829,6.5468688966379256,6.4539874037804541,6.4616411828031675,6.4711983396383737,6.4729543575411519,6.4839579569501025]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.734858318037762,19.447681498857051,19.171774081319164,19.194509874420628,19.222899711623747,19.22811601844441,19.260802559144221]
[null,null,null,null,"Coincident",7.7540016136021865,7.6411672834321482,7.5327608015453151,7.541693897164965,7.5528485170733166,7.5548980504853454,7.5677408834687352]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.306551005878235,15.269416467483811,15.232372019531136,15.19541744345582,15.158552521223724,15.121777035329671,15.085090768796166]
[null,null,null,null,"Coincident",6.014080227258761,5.9994897363623778,5.9849346428030028,5.9704148607047411,5.9559303044000362,5.941480888429167,5.9270665275397434]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.865015874743683,17.821674359227686,17.778437992622855,17.735306519832129,17.692279686377312,17.649357238397595,17.606538922648053]
[null,null,null,null,"Coincident",7.0193238627499186,7.0022945952562763,6.9853066417064031,6.9683599018703912,6.9514542757614928,6.9345896636355331,6.9177659659903252]
[null,"Williamstown 11kV","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",3,3,3,3,3,3,3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.42208999999999997,0.45275156558543933,0.46072097357096897,0.47364691169701179,0.48591360872384798,0.49782507550066485,0.50971677978373597]
[null,null,null,null,"Coincident",0.42208999999999997,0.45275156558543933,0.46072097357096897,0.47364691169701179,0.48591360872384798,0.49782507550066485,0.50971677978373597]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.97914846377697318,0.98703607983730057,0.99368598382266604,1.001479792612002,1.0095021665031831,1.0176734797355029,1.0258154523105303]
[null,null,null,null,"Coincident",0.93817990880722524,0.94573749909096994,0.9521091644158598,0.95957687241903111,0.96726358213066488,0.97509299941184158,0.98289430367829045]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0306825934494455,1.0389853471971586,1.0459852461291221,1.0541892553810548,1.062633859477035,1.0712352418268452,1.0798057392742424]
[null,null,null,null,"Coincident",0.98755779874444782,0.99551315693786324,1.0022201730693263,1.0100809183358224,1.0181721917164894,1.0264136835914124,1.0346255828192532]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.87009172744369934,0.87777718478987232,0.88553052722534897,0.89335235437421689,0.90124327115700009,0.90920388783744166,0.91723482006970047]
[null,null,null,null,"Coincident",0.83368621583517621,0.84105010592837126,0.84847904073056435,0.85597359477696922,0.8635343476776276,0.87116188416223483,0.87885679412536144]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.91588602888810455,0.92397598398933944,0.93213739707931476,0.94037089934128104,0.94867712753368449,0.95705672403941222,0.96551033691547428]
[null,null,null,null,"Coincident",0.87756443772123827,0.88531590097723301,0.89313583234796257,0.90102483660733612,0.90898352387118708,0.91701250964445791,0.92511241486880169]
[null,"Williamstown South 11kV","Substation Rating","MVA","Non-Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,null,null,"Coincident",4.3,4.3,4.3,4.3,4.3,4.3,4.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4521999999999999,1.5576910695424555,1.5851098055385373,1.6295814759089309,1.6717850282848969,1.7127664115285024,1.7536798019425748]
[null,null,null,null,"Coincident",1.4521999999999999,1.5576910695424555,1.5851098055385373,1.6295814759089309,1.6717850282848969,1.7127664115285024,1.7536798019425748]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6200593605418554,2.5849597541890716,2.5818633441010994,2.5827785704835704,2.5853604830252959,2.5888666068196411,2.5922549779071122]
[null,null,null,null,"Coincident",2.3580534244876703,2.3264637787701647,2.3236770096909898,2.3245007134352136,2.3268244347227665,2.3299799461376773,2.3330294801164015]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8478906092846255,2.8097388632489908,2.8063732001098907,2.8073680113951851,2.8101744380709737,2.8139854421952619,2.8176684542468609]
[null,null,null,null,"Coincident",2.5631015483561632,2.5287649769240921,2.5257358800989018,2.5266312102556667,2.5291569942638765,2.5325868979757362,2.5359016088221753]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4126777509353907,2.395478983480928,2.3784028173982557,2.3614483787237943,2.3446147997240119,2.3279012188510126,2.3113067806984429]
[null,null,null,null,"Coincident",2.1714099758418519,2.1559310851328357,2.1405625356584306,2.1253035408514154,2.1101533197516109,2.0951110969659115,2.0801761026285988]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6224758162341204,2.6037815037836172,2.585220453693756,2.5667917160041243,2.5484943475260997,2.5303274117945787,2.5122899790200464]
[null,null,null,null,"Coincident",2.3602282346107084,2.3434033534052561,2.3266984083243809,2.3101125444037121,2.2936449127734901,2.2772946706151211,2.261060981118042]
[null,"Willunga 11kV","Substation Rating","MVA","Non-Coincident",6.7,6.7,6.7,6.7,6.7,6.7,6.7]
[null,null,null,null,"Coincident",6.7,6.7,6.7,6.7,6.7,6.7,6.7]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.8460800000000002,3.0528256433021568,3.1065619855027689,3.193719354741007,3.2764315750592754,3.3567485391289358,3.4369322481150832]
[null,null,null,null,"Coincident",2.8460800000000002,3.0528256433021568,3.1065619855027689,3.193719354741007,3.2764315750592754,3.3567485391289358,3.4369322481150832]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.2228485569425196,4.2255549882342534,4.2005301356748683,4.2135716688354163,4.2277916524344308,4.2425009411007784,4.2432230600802248]
[null,null,null,null,"Coincident",4.2228485569425196,4.2255549882342534,4.2005301356748683,4.2135716688354163,4.2277916524344308,4.2425009411007784,4.2432230600802248]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4458604831001143,4.4487098431394081,4.4223634085967189,4.4360936752960063,4.4510646273206182,4.4665507249948329,4.4673109796408443]
[null,null,null,null,"Coincident",4.4458604831001143,4.4487098431394081,4.4223634085967189,4.4360936752960063,4.4510646273206182,4.4665507249948329,4.4673109796408443]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7405283532836386,3.6607933965773962,3.5827581097360715,3.5063862617542303,3.4316423939445113,3.3584918034745121,3.2869005272546081]
[null,null,null,null,"Coincident",3.7405283532836386,3.6607933965773962,3.5827581097360715,3.5063862617542303,3.4316423939445113,3.3584918034745121,3.2869005272546081]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.9380685732712708,3.8541227513072815,3.7719663600995377,3.6915612552549462,3.6128701054852073,3.535856375274272,3.4604843079152605]
[null,null,null,null,"Coincident",3.9380685732712704,3.854122751307282,3.7719663600995377,3.6915612552549462,3.6128701054852073,3.535856375274272,3.4604843079152605]
[null,"Willunga 33kV","Substation Rating","MVA","Non-Coincident",10.6,10.6,10.6,10.6,10.6,10.6,10.6]
[null,null,null,null,"Coincident",10.6,10.6,10.6,10.6,10.6,10.6,10.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.4213899999999999,1.5246429619452904,1.5514799796821521,1.5950081352721353,1.6363162934539797,1.676428212148807,1.716473580555816]
[null,null,null,null,"Coincident",1.4213899999999999,1.5246429619452904,1.5514799796821521,1.5950081352721353,1.6363162934539797,1.676428212148807,1.716473580555816]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.944132561994377,2.9750240405476247,3.007240438244732,3.044466892858642,3.0831871889160247,3.1227773343372438,3.1603103345813364]
[null,null,null,null,"Coincident",2.830383014677587,2.8600809696284197,2.8910526541283259,2.9268408269151185,2.9640651250662402,3.0021256650688706,3.0382085397845411]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0600545537844899,3.0921623504374933,3.1256472334730532,3.1643394389236734,3.2045843041868101,3.2457332681788134,3.2847440891577193]
[null,null,null,null,"Coincident",2.9418262427529123,2.9726935221201907,3.0048846827410673,3.0420819755945065,3.0807719396739803,3.1203310717110413,3.1578346700587074]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6692637244335655,2.6998745095024446,2.730836335254923,2.762153227381988,2.7938292577407502,2.8258685448838725,2.8582752545950689]
[null,null,null,null,"Coincident",2.5661340134134316,2.5955621197573286,2.6253277039720078,2.6554346362118015,2.6858868310134918,2.7166882478052825,2.7478428914216089]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7743630571007829,2.8061791082712126,2.8383600219672904,2.8709099823871722,2.9038332217128788,2.9371340206605678,2.9708167090371207]
[null,null,null,null,"Coincident",2.6671727267768448,2.6977595325441417,2.7286971040033845,2.7599894636919897,2.7916406802773324,2.8236548690857619,2.8560361926376783]
[null,"Wilmington 11kV","Substation Rating","MVA","Non-Coincident",2,2,2,2,2,2,2]
[null,null,null,null,"Coincident",2,2,2,2,2,2,2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.5408400000000001,0.58012783228986486,0.59033933840205388,0.60690183544318022,0.6226196217446659,0.63788223799137544,0.65311953180183335]
[null,null,null,null,"Coincident",0.5408400000000001,0.58012783228986486,0.59033933840205388,0.60690183544318022,0.6226196217446659,0.63788223799137544,0.65311953180183335]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.75843177388133165,0.73172583630581811,0.70394606773352031,0.69719996531573714,0.69083638131792158,0.68460407465020412,0.67946460890735783]
[null,null,null,null,"Coincident",0.68451252222133541,0.66040943303435662,0.63533717194640826,0.62924856682702046,0.6235051986260548,0.61788031303543123,0.61324175650383705]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.76686417643269311,0.73986131667656496,0.7117726868467984,0.70495157985616042,0.69851724420501637,0.6922156454526901,0.68701903805843223]
[null,null,null,null,"Coincident",0.69212307512483384,0.66775200276816815,0.64240098305532145,0.63624468355509267,0.63043745938930718,0.62475003514822236,0.62005990617823803]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.70179692657254178,0.68405406409259106,0.66675977748560677,0.64990272583554254,0.63347185494791802,0.61745639010091091,0.60184582897971617]
[null,null,null,null,"Coincident",0.63339749314157312,0.61738390831320644,0.60177517967993355,0.58656107164863391,0.57173160740292739,0.55727706236076879,0.54318795779744744]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.70959965108641987,0.69165951976305207,0.67417295167270852,0.65712847980867428,0.64051492707363089,0.62432139895015248,0.60853727635650934]
[null,null,null,null,"Coincident",0.6404397384972228,0.62424811129482405,0.60846584156308536,0.59308257990742841,0.57808823858714875,0.5634729849002712,0.54922723473564794]
[null,"Wirrabara Forest 11kV","Substation Rating","MVA","Non-Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,null,null,"Coincident",1.3,1.3,1.3,1.3,1.3,1.3,1.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.10965999999999999,0.1176259486889035,0.11969642010422531,0.12305461000425102,0.12624152747673997,0.12933615527352676,0.13242564872677506]
[null,null,null,null,"Coincident",0.10965999999999999,0.1176259486889035,0.11969642010422531,0.12305461000425102,0.12624152747673997,0.12933615527352676,0.13242564872677506]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.51379024956331798,0.51357274641120187,0.50743827011828235,0.50725676595953195,0.50705445238972979,0.50678467445395126,0.50731241878954603]
[null,null,null,null,"Coincident",0.41634727119786108,0.4161710186435601,0.4111999775096426,0.41105289655341382,0.41088895279857413,0.41067033964371907,0.41109799453635626]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.55246263393905148,0.5522287595819374,0.545632548514282,0.54543738275218479,0.54521984127927925,0.54492975747736683,0.54549722450488813]
[null,null,null,null,"Coincident",0.44768523784716235,0.44749571897156992,0.44215051345122852,0.44199236188539115,0.44181607827803659,0.4415810103695903,0.44204085434016793]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.47258286818874645,0.47299975500416436,0.47341700957437949,0.47383463222380506,0.47425262327714046,0.47467098305937155,0.47508971189577082]
[null,null,null,null,"Coincident",0.38295508284260488,0.38329290491716766,0.38363102499992818,0.38396944335377303,0.38430816024182068,0.38464717592742176,0.38498649067415908]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.50815362170832945,0.50860188710125187,0.50905054792944027,0.50949960454172583,0.50994905728724771,0.51039890651545317,0.51084915257609753]
[null,null,null,null,"Coincident",0.41177965897054281,0.41214290851308344,0.41250647849454636,0.41287036919760534,0.41323458090518345,0.41359911390045345,0.41396396846683764]
[null,"Wirrabara South 11kV","Substation Rating","MVA","Non-Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,null,null,"Coincident",0.13,0.13,0.13,0.13,0.13,0.13,0.13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.0400000000000002E-3,3.2608324276332907E-3,3.3182301396757702E-3,3.4113260479019074E-3,3.499673933332934E-3,3.5854633597621867E-3,3.6711104516632884E-3]
[null,null,null,null,"Coincident",3.0400000000000002E-3,3.2608324276332907E-3,3.3182301396757702E-3,3.4113260479019074E-3,3.499673933332934E-3,3.5854633597621867E-3,3.6711104516632884E-3]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8176880899000164E-2,4.8013923813238511E-2,4.785151792571353E-2,4.7689661372011076E-2,4.7528352294023329E-2,4.7367588839927484E-2,4.7207369164164473E-2]
[null,null,null,null,"Coincident",4.8176880899000164E-2,4.8013923813238511E-2,4.785151792571353E-2,4.7689661372011076E-2,4.7528352294023329E-2,4.7367588839927484E-2,4.7207369164164473E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.8210720698231006E-2,4.8047649150201092E-2,4.7885129187573594E-2,4.7723158944624776E-2,4.7561736561941674E-2,4.7400860186400759E-2,4.7240527971146619E-2]
[null,null,null,null,"Coincident",4.8210720698231006E-2,4.8047649150201092E-2,4.7885129187573594E-2,4.7723158944624776E-2,4.7561736561941674E-2,4.7400860186400759E-2,4.7240527971146619E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.3359192809100146E-2,4.3212531431914662E-2,4.306636613314218E-2,4.2920695234809972E-2,4.2775517064620995E-2,4.2630829955934736E-2,4.2486632247748027E-2]
[null,null,null,null,"Coincident",4.3359192809100146E-2,4.3212531431914662E-2,4.306636613314218E-2,4.2920695234809972E-2,4.2775517064620995E-2,4.2630829955934736E-2,4.2486632247748027E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.3389648628407905E-2,4.3242884235180988E-2,4.3096616268816237E-2,4.29508430501623E-2,4.280556290574751E-2,4.2660774167760686E-2,4.2516475174031954E-2]
[null,null,null,null,"Coincident",4.3389648628407905E-2,4.3242884235180988E-2,4.3096616268816237E-2,4.29508430501623E-2,4.280556290574751E-2,4.2660774167760686E-2,4.2516475174031954E-2]
[null,"Wirrina Cove 11kV","Substation Rating","MVA","Non-Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,null,null,"Coincident",1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002,1.9500000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.6700000000000004E-2,8.2271660262984672E-2,8.3719819642477489E-2,8.6068653905946146E-2,8.8297694304814489E-2,9.0462184109789387E-2,9.262308277716258E-2]
[null,null,null,null,"Coincident",7.6700000000000004E-2,8.2271660262984672E-2,8.3719819642477489E-2,8.6068653905946146E-2,8.8297694304814489E-2,9.0462184109789387E-2,9.262308277716258E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.69440641386376101,0.69468803896213427,0.69496977827704476,0.69525163185481442,0.69553359974178397,0.69581568198431298,0.6960978786287797]
[null,null,null,null,"Coincident",0.69440641386376101,0.69468803896213427,0.69496977827704476,0.69525163185481442,0.69553359974178397,0.69581568198431298,0.6960978786287797]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.69809115974309643,0.69837427923567463,0.69865751355086014,0.6989408627352206,0.69922432683534264,0.69950790589783185,0.69979159996931262]
[null,null,null,null,"Coincident",0.69809115974309643,0.69837427923567463,0.69865751355086014,0.6989408627352206,0.69922432683534264,0.69950790589783185,0.69979159996931262]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.62496577247738494,0.62521923506592081,0.62547280044934028,0.62572646866933301,0.62598023976760564,0.62623411378588167,0.62648809076590173]
[null,null,null,null,"Coincident",0.62496577247738494,0.62521923506592081,0.62547280044934028,0.62572646866933301,0.62598023976760564,0.62623411378588167,0.62648809076590173]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.62828204376878682,0.62853685131210713,0.62879176219577404,0.62904677646169849,0.62930189415180837,0.6295571153080487,0.62981243997238134]
[null,null,null,null,"Coincident",0.62828204376878682,0.62853685131210713,0.62879176219577404,0.62904677646169849,0.62930189415180837,0.6295571153080487,0.62981243997238134]
[null,"Wongyarra 11kV","Substation Rating","MVA","Non-Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,null,null,"Coincident",0.26,0.26,0.26,0.26,0.26,0.26,0.26]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.286E-2,1.3794179282685564E-2,1.4036986709286317E-2,1.4430806900006095E-2,1.4804541704822873E-2,1.5167453554783461E-2,1.5529763292233517E-2]
[null,null,null,null,"Coincident",1.286E-2,1.3794179282685564E-2,1.4036986709286317E-2,1.4430806900006095E-2,1.4804541704822873E-2,1.5167453554783461E-2,1.5529763292233517E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.6353761798000329E-2,9.6027847626477023E-2,9.570303585142706E-2,9.5379322744022152E-2,9.5056704588046659E-2,9.4735177679854968E-2,9.4414738328328945E-2]
[null,null,null,null,"Coincident",9.6353761798000329E-2,9.6027847626477023E-2,9.570303585142706E-2,9.5379322744022152E-2,9.5056704588046659E-2,9.4735177679854968E-2,9.4414738328328945E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6421441396462013E-2,9.6095298300402185E-2,9.5770258375147188E-2,9.5446317889249552E-2,9.5123473123883348E-2,9.4801720372801518E-2,9.4481055942293238E-2]
[null,null,null,null,"Coincident",9.6421441396462013E-2,9.6095298300402185E-2,9.5770258375147188E-2,9.5446317889249552E-2,9.5123473123883348E-2,9.4801720372801518E-2,9.4481055942293238E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6718385618200292E-2,8.6425062863829324E-2,8.6132732266284359E-2,8.5841390469619944E-2,8.555103412924199E-2,8.5261659911869472E-2,8.4973264495496054E-2]
[null,null,null,null,"Coincident",8.6718385618200292E-2,8.6425062863829324E-2,8.6132732266284359E-2,8.5841390469619944E-2,8.555103412924199E-2,8.5261659911869472E-2,8.4973264495496054E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.677929725681581E-2,8.6485768470361976E-2,8.6193232537632475E-2,8.5901686100324601E-2,8.561112581149502E-2,8.5321548335521372E-2,8.5032950348063907E-2]
[null,null,null,null,"Coincident",8.677929725681581E-2,8.6485768470361976E-2,8.6193232537632475E-2,8.5901686100324601E-2,8.561112581149502E-2,8.5321548335521372E-2,8.5032950348063907E-2]
[null,"Woodforde 11kV","Substation Rating","MVA","Non-Coincident",50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687]
[null,null,null,null,"Coincident",50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687,50.47598039215687]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",13.384840000000001,14.357144839040519,14.609861678532184,15.019754387828739,15.408741990076312,15.786464932986613,16.163561190079225]
[null,null,null,null,"Coincident",13.384840000000001,14.357144839040519,14.609861678532184,15.019754387828739,15.408741990076312,15.786464932986613,16.163561190079225]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",40.19839843561715,40.311833016791653,40.344044679625092,40.458599469565854,40.564787252880386,40.676158601939427,40.803566726236802]
[null,null,null,null,"Coincident",35.325078870034972,35.42476158582766,35.453068174508019,35.553735294270986,35.64704975371712,35.74491936649968,35.856881589240878]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.884749980590811,42.002943223519551,42.036506188631172,42.15586663388455,42.266509070603661,42.38255252735506,42.515305513527842]
[null,null,null,null,"Coincident",36.806991176173476,36.910855653138896,36.940349723445685,37.045239900831511,37.142468968545117,37.244444281533276,37.361103399540113]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.087183249382562,35.402701258000775,35.721056530957213,36.042274582069496,36.366381154585703,36.69340222324751,37.023363996371884]
[null,null,null,null,"Coincident",30.833504911817766,31.11077214069023,31.390532667565186,31.67280891317716,31.957623499876902,32.244999253444384,32.53495920491816]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.55911566420594,36.887869878792721,37.219580382984567,37.554273760921973,37.891976835800691,38.232716672021354,38.576520577358579]
[null,null,null,null,"Coincident",32.126992480191298,32.415891267483396,32.707387948411203,33.001505884275076,33.298268646449557,33.597700018272391,33.899823996950673]
[null,"Woods Point 11kV","Substation Rating","MVA","Non-Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,null,null,"Coincident",8.1,8.1,8.1,8.1,8.1,8.1,8.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.72983000000000009,0.78284649034855425,0.79662628382880518,0.81897634524350305,0.84018652196196564,0.86078247495238058,0.88134425688730855]
[null,null,null,null,"Coincident",0.72983000000000009,0.78284649034855425,0.79662628382880518,0.81897634524350305,0.84018652196196564,0.86078247495238058,0.88134425688730855]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8741100696272253,1.8337750617777318,1.7958780512655796,1.7741455566256823,1.7538539274145262,1.7336603087652411,1.7142266087996305]
[null,null,null,null,"Coincident",1.7594856005368751,1.7216175656445372,1.6860384151025471,1.6656351250277812,1.6465845740558396,1.6276260391159909,1.609380944652864]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0167799928859367,1.9733744116652263,1.9325924246145412,1.9092055056199893,1.8873691404676161,1.8656382471034141,1.8447251225684249]
[null,null,null,null,"Coincident",1.8934295346054513,1.8526787289945703,1.8143910530784835,1.7924345266829869,1.7719337190322879,1.7515319322958658,1.7318978979465027]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5641642062731647,1.529234395699625,1.4950846129913251,1.4616974391167681,1.4290558440339689,1.397143178003815,1.365943163097411]
[null,null,null,null,"Coincident",1.468496670721289,1.4357032399993421,1.4036421290163204,1.3722969841249169,1.3416518168759279,1.3116909958629088,1.2823992387489456]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6832389558781353,1.6456500520769712,1.6089005571333788,1.5729717259614702,1.5378452320773794,1.5035031582513385,1.4699279873685021]
[null,null,null,null,"Coincident",1.5802885610232031,1.5449986727450464,1.510496853333172,1.4767655041901264,1.4437874197179068,1.4115457785417764,1.3800241349300617]
[null,"Woodside 11kV","Substation Rating","MVA","Non-Coincident",13,13,13,13,13,13,13]
[null,null,null,null,"Coincident",13,13,13,13,13,13,13]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.8373800000000005,5.1887781476265555,5.2801118792976247,5.4282501307893849,5.5688331222454179,5.705344982646845,5.8416303541667638]
[null,null,null,null,"Coincident",4.8373800000000005,5.1887781476265555,5.2801118792976247,5.4282501307893849,5.5688331222454179,5.705344982646845,5.8416303541667638]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7086887537715674,7.8696985665794275,7.9430857029092135,8.0423439907854437,8.147406066475714,8.2573822276816706,8.3742341400784284]
[null,null,null,null,"Coincident",7.4980163849170554,7.6546259268414323,7.7260074507580203,7.8225530881040166,7.9247439003317925,8.0317145000033765,8.1453729420219521]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.1564800351383866,8.3268427732870958,8.4044929069777332,8.5095170257668578,8.6206820695492539,8.7370466539642972,8.8606863962052298]
[null,null,null,null,"Coincident",7.9335698846051432,8.0992767438155866,8.1748047607456442,8.2769586534043729,8.3850856444315589,8.4982700767568584,8.6185308425966873]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.7869708480405171,6.7756494039733441,6.764346845370488,6.7530631407288322,6.7417982585978118,6.730552167579325,6.7193248363276465]
[null,null,null,null,"Coincident",6.601488300803978,6.5904762628519915,6.5794825942395132,6.5685072643243831,6.5575502425155534,6.5466114982730099,6.5356910011076792]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.1812203072830334,7.1692412100004193,7.1572820952229446,7.1453429296175059,7.1334236799066,7.1215243128682353,7.109644795335841]
[null,null,null,null,"Coincident",6.9849632340341952,6.9733115160091783,6.9616792343832357,6.9500663567342302,6.9384728506941054,6.9268986839488029,6.915343824238164]
[null,"Woodville 11kV","Substation Rating","MVA","Non-Coincident",28.2,28.2,28.2,28.2,28.2,28.2,28.2]
[null,null,null,null,"Coincident",28.2,28.2,28.2,28.2,28.2,28.2,28.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.9363899999999998,2.077053718600272,2.1136143618969618,2.172913699308149,2.2291886867653155,2.2838340115822038,2.3383886735185113]
[null,null,null,null,"Coincident",1.9363899999999998,2.077053718600272,2.1136143618969618,2.172913699308149,2.2291886867653155,2.2838340115822038,2.3383886735185113]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.115126166558296,6.6231093534753454,7.3598700609179497,7.4123699216997245,7.4682995157947811,7.5260091457851948,7.5871989765632435]
[null,null,null,null,"Coincident",9.0348841999582721,5.9157963100988846,6.5738748713758106,6.620768024745014,6.6707246340525819,6.7222711808380913,6.7769262613770245]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.876479748987414,7.1216229607261772,7.913838775180591,7.9702902383868004,8.0304295868761084,8.092482952457198,8.1582784694228412]
[null,null,null,null,"Coincident",9.7149292472669586,6.361071301181596,7.0686826573933441,7.1191054029516279,7.1728221871533133,7.2282485815463344,7.2870174853516385]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3804220095628725,5.979887640324451,6.7432955867283413,6.8147983558214511,6.8870593070114641,6.9600864797085924,7.033887998569214]
[null,null,null,null,"Coincident",8.3786425604197117,5.3412672733350792,6.0231472894134077,6.0870139410097481,6.1515578048657487,6.2167860618251378,6.2827059688739721]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.086475279099862,6.4299867100262906,7.2508554696003662,7.3277401675499467,7.4054401150660896,7.4839639566759057,7.5633204285690461]
[null,null,null,null,"Coincident",9.0092930757201195,5.743298143371053,6.4765024617348468,6.5451762806556424,6.6145782848018797,6.6847161955109007,6.7555978159935179]
[null,"Woodville 33kV","Substation Rating","MVA","Non-Coincident",37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034]
[null,null,null,null,"Coincident",37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034,37.890014471780034]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.94927133029110011,0.907121016958084,0,0,0,0,0]
[null,null,null,null,"Coincident",0.63347600194202525,0.60534788817858254,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0480146541361086,1.0014798598788301,0,0,0,0,0]
[null,null,null,null,"Coincident",0.69937025578894263,0.66831625207405565,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.9,0.9,0,0,0,0,0]
[null,null,null,null,"Coincident",0.6005958291956307,0.6005958291956307,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0819397239548292,1.0819397239548294,0,0,0,0,0]
[null,null,null,null,"Coincident",0.66306988331463523,0.66306988331463523,0,0,0,0,0]
[null,"Woolpunda 11kV","Substation Rating","MVA","Non-Coincident",18.8,18.8,18.8,18.8,18.8,18.8,18.8]
[null,null,null,null,"Coincident",18.8,18.8,18.8,18.8,18.8,18.8,18.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.28042,0.30079033860425242,0.30608489992364457,0.31467238498442529,0.32282189617934914,0.33073540636332643,0.33863578712349318]
[null,null,null,null,"Coincident",0.28042,0.30079033860425242,0.30608489992364457,0.31467238498442529,0.32282189617934914,0.33073540636332643,0.33863578712349318]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.8514232886134616,5.8784677752299395,5.96318024279232,5.9702749435498488,5.9787908199477773,5.9887851017901657,6.0116521419468043]
[null,null,null,null,"Coincident",4.4733853713216831,4.494060753162624,4.5588230331192854,4.5642468982230788,4.570757245368295,4.5783978264688976,4.5958795702903013]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3163017814012488,6.3454948735033279,6.4369374992337844,6.4445958532483525,6.4537882911577924,6.4645765895069722,6.4892603492270755]
[null,null,null,null,"Coincident",4.828782775766121,4.8511007563174875,4.9210082102960548,4.9268629856434201,4.9338905608576225,4.9421381638144259,4.9610087811317554]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5123136437935925,5.5807348153645231,5.6500052594953365,5.720135517716737,5.7911362624053728,5.863018298407952,5.9357925646855145]
[null,null,null,null,"Coincident",4.2141376550672076,4.2664453164510103,4.3194022426817158,4.3730164927095858,4.4272962255159873,4.4822497013550171,4.5378852830105458]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9502508655780613,6.0241078994248536,6.0988816780563404,6.1745835804970586,6.2512251270128143,6.3288179808638345,6.4073739500796698]
[null,null,null,null,"Coincident",4.5489385855177744,4.6054019378482014,4.6625661372216163,4.7204398828483436,4.7790319819169955,4.8383513509347349,4.8984070170841889]
[null,"Wudinna 11kV","Substation Rating","MVA","Non-Coincident",5.2,5.2,5.2,5.2,5.2,5.2,5.2]
[null,null,null,null,"Coincident",5.2,5.2,5.2,5.2,5.2,5.2,5.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.0694600000000003,1.1471479763344408,1.1673402648610691,1.200091037891176,1.2311714752441583,1.2613518568194966,1.2914821656696782]
[null,null,null,null,"Coincident",1.0694600000000003,1.1471479763344408,1.1673402648610691,1.200091037891176,1.2311714752441583,1.2613518568194966,1.2914821656696782]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1003691419560884,2.0503712624959491,2.003634834200605,1.9779901646290161,1.9533474276709537,1.928919591737871,1.9054003599501959]
[null,null,null,null,"Coincident",1.8266912599638785,1.7832080990269839,1.7425614225053867,1.7202582507269935,1.6988264598461966,1.6775815684090483,1.6571268900911218]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.1015188664761491,2.0514936185945176,2.0047316071687997,1.9790728999193445,1.9544166737329576,1.9299754662065756,1.9064433601879194]
[null,null,null,null,"Coincident",1.8276911754978713,1.7841842122419747,1.743515286069246,1.7211999057209606,1.6997563832568949,1.6784998625436713,1.6580339875057293]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8257441747546914,1.7787196977999342,1.7329063989847242,1.6882730828002388,1.6447893572196035,1.6024256130031416,1.5611530035366465]
[null,null,null,null,"Coincident",1.5878498975891371,1.5469527051186605,1.5071088744013994,1.4682912747001045,1.43047347406586,1.3936297213398574,1.3577349286187381]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8267435718621534,1.7796933541015931,1.7338549774693743,1.6891972293805138,1.6456897011717952,1.6033027673956914,1.5620075656476005]
[null,null,null,null,"Coincident",1.588719073356847,1.5477994941049016,1.5079338532075948,1.4690950050765381,1.4312565032941882,1.3943925826057668,1.3584781413750073]
[null,"Yankalilla 11kV","Substation Rating","MVA","Non-Coincident",16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001]
[null,null,null,null,"Coincident",16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001,16.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",3.56887,3.8281207322393493,3.8955039469028505,4.0047957870314734,4.108513588965101,4.2092278357744979,4.3097749860616972]
[null,null,null,null,"Coincident",3.56887,3.8281207322393493,3.8955039469028505,4.0047957870314734,4.108513588965101,4.2092278357744979,4.3097749860616972]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.4211906910337699,7.4762733105010515,7.4577288224186544,7.5163161270490839,7.5705569550008827,7.5701792017735636,7.5645068818342995]
[null,null,null,null,"Coincident",6.5393483828494974,6.5878856666268408,6.571544775629536,6.623170291229532,6.6709658115601922,6.6706329458437557,6.6656346540916456]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.6779198538787607,7.7349080051362753,7.7157219878035201,7.7763360655351024,7.8324533042856306,7.8320624830381176,7.8261939344867582]
[null,null,null,null,"Coincident",6.7655710344125488,6.8157874202032636,6.7988812313392772,6.8522926834490896,6.9017416451792624,6.9013972642841601,6.8962260612957538]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3728269496077328,6.3220615394842161,6.2717005224009288,6.2217406769965038,6.1721788075706696,6.1230117438798395,6.0742363409343216]
[null,null,null,null,"Coincident",5.6155591928728388,5.5708261147972413,5.5264493767058536,5.4824261400239616,5.4387535887886989,5.3954289294689284,5.352449390786548]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5932889476676264,6.5407673555801784,6.4886641461326064,6.4369759865235565,6.3856995705004902,6.3348316181482023,6.2843688756790206]
[null,null,null,null,"Coincident",5.8098242199438399,5.7635436427991644,5.7176317328877397,5.6720855534370109,5.6269021910685053,5.5820787556114837,5.5376123799180661]
[null,"Yankalilla 33kV","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.62492999999999999,0.67032631875028692,0.68212551354854567,0.70126315365636138,0.71942474709136517,0.73706040046584964,0.75466679426247973]
[null,null,null,null,"Coincident",0.62492999999999999,0.67032631875028692,0.68212551354854567,0.70126315365636138,0.71942474709136517,0.73706040046584964,0.75466679426247973]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.99357197356542937,0.99471282769053149,0.99803218208226774,0.99650347387094407,0.99538948844150921,0.99445605990048658,0.99274309662684723]
[null,null,null,null,"Coincident",0.78831450554217697,0.78921967585641029,0.7918533000785698,0.79064040067139008,0.78975654837246223,0.78901595254412515,0.78765686248120281]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.99953289271015278,1.0006805913713093,1.0040198601765637,1.0024819805048064,1.0013613117376265,1.0004222831070197,0.99869904293765088]
[null,null,null,null,"Coincident",0.7930439857944096,0.79395458666344809,0.79660401127195468,0.79538383509420441,0.79449468013756286,0.79374964111641333,0.79238239721442238]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.88891631033434959,0.87951859995914272,0.87022024309930002,0.86102018937971725,0.85191739952995871,0.84291084526685767,0.83399950917835775]
[null,null,null,null,"Coincident",0.70527917482915303,0.69782289425284516,0.690445442205745,0.68314598530491411,0.67592369897802007,0.66877776737019001,0.66170738325184875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.89424934950343393,0.88479525771532241,0.87544111551239934,0.8661858662178521,0.85702846432615853,0.84796787538498364,0.83900307587832346]
[null,null,null,null,"Coincident",0.70951048594446897,0.70200947153224558,0.69458775857972854,0.6872445087041118,0.67997889238605458,0.67279008887597558,0.66567728610133869]
[null,"Yankalilla Hill 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9840183253250317E-2,1.9848229684632412E-2,1.985627937934414E-2,1.986433233870899E-2,1.9872388564050977E-2,1.9880448056694661E-2,1.9888510817965138E-2]
[null,null,null,null,"Coincident",1.9840183253250317E-2,1.9848229684632412E-2,1.985627937934414E-2,1.986433233870899E-2,1.9872388564050977E-2,1.9880448056694661E-2,1.9888510817965138E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9945461706945614E-2,1.9953550835304992E-2,1.9961643244310292E-2,1.9969738935292022E-2,1.9977837909581225E-2,1.9985940168509488E-2,1.9994045713408938E-2]
[null,null,null,null,"Coincident",1.9945461706945614E-2,1.9953550835304992E-2,1.9961643244310292E-2,1.9969738935292022E-2,1.9977837909581225E-2,1.9985940168509488E-2,1.9994045713408938E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.7856164927925286E-2,1.7863406716169171E-2,1.7870651441409726E-2,1.7877899104838092E-2,1.7885149707645879E-2,1.7892403251025195E-2,1.7899659736168624E-2]
[null,null,null,null,"Coincident",1.7856164927925286E-2,1.7863406716169171E-2,1.7870651441409726E-2,1.7877899104838092E-2,1.7885149707645879E-2,1.7892403251025195E-2,1.7899659736168624E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7950915536251055E-2,1.7958195751774497E-2,1.7965478919879263E-2,1.7972765041762821E-2,1.79800541186231E-2,1.7987346151658538E-2,1.7994641142068044E-2]
[null,null,null,null,"Coincident",1.7950915536251055E-2,1.7958195751774497E-2,1.7965478919879263E-2,1.7972765041762821E-2,1.79800541186231E-2,1.7987346151658538E-2,1.7994641142068044E-2]
[null,"Yongala 11kV","Substation Rating","MVA","Non-Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,null,null,"Coincident",0.39,0.39,0.39,0.39,0.39,0.39,0.39]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.1939999999999995E-2,6.6439460713028295E-2,6.7608939095893814E-2,6.9505768226001352E-2,7.1305856391658526E-2,7.3053815955154547E-2,7.4798875452639496E-2]
[null,null,null,null,"Coincident",6.1939999999999995E-2,6.6439460713028295E-2,6.7608939095893814E-2,6.9505768226001352E-2,7.1305856391658526E-2,7.3053815955154547E-2,7.4798875452639496E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,null,null,"Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277]
[null,null,null,null,"Coincident",0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277,0.10348224852079277]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2]
[null,null,null,null,"Coincident",9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2,9.0000000000000011E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2]
[null,null,null,null,"Coincident",9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2,9.3134023668713498E-2]
[null,"Yorketown 11kV","Substation Rating","MVA","Non-Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,null,null,"Coincident",2.6,2.6,2.6,2.6,2.6,2.6,2.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.97292999999999996,1.0436058203346241,1.0619755426956405,1.0917702144030272,1.1200453157755301,1.147501600859679,1.1749123328081459]
[null,null,null,null,"Coincident",0.97292999999999996,1.0436058203346241,1.0619755426956405,1.0917702144030272,1.1200453157755301,1.147501600859679,1.1749123328081459]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1934547673359923,1.1187420378200539,1.0606263204460362,1.0393325820573993,1.0195611732840051,1.0005586395048294,0.98209697516365924]
[null,null,null,null,"Coincident",1.1934547673359923,1.1187420378200539,1.0606263204460362,1.0393325820573993,1.0195611732840051,1.0005586395048294,0.98209697516365924]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1934547673359923,1.1187420378200539,1.0606263204460362,1.0393325820573993,1.0195611732840051,1.0005586395048294,0.98209697516365924]
[null,null,null,null,"Coincident",1.1934547673359923,1.1187420378200539,1.0606263204460362,1.0393325820573993,1.0195611732840051,1.0005586395048294,0.98209697516365924]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1564264156342254,1.0925967708909914,1.0322902414043498,0.97531236672945298,0.92147941978152148,0.87061781440164243,0.8225635456223267]
[null,null,null,null,"Coincident",1.1564264156342254,1.0925967708909914,1.0322902414043498,0.97531236672945298,0.92147941978152148,0.87061781440164243,0.8225635456223267]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1564264156342254,1.0925967708909914,1.0322902414043498,0.97531236672945298,0.92147941978152148,0.87061781440164243,0.8225635456223267]
[null,null,null,null,"Coincident",1.1564264156342254,1.0925967708909914,1.0322902414043498,0.97531236672945298,0.92147941978152148,0.87061781440164243,0.8225635456223267]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Cape Jervis 11kV",null,"MWh","Non-Coincident",0,0,1.3121566618370642E-2,3.6716830998751629E-2,6.1967768377361544E-2,9.5370525441904136E-2,0.13248307769471881]
[null,"Gumeracha 11kV",null,"MWh","Non-Coincident",5.0361094243675204,5.0590523047241049,5.0820083726235321,5.1049776356459819,5.1279601013760088,5.1527060777456661,5.1806466083375211]
[null,"Curramulka 7.6kV",null,"MWh","Non-Coincident",0,0,0,0,1.4939414930075312E-2,3.9586543063740431E-2,3.9586543063740431E-2]
[null,"Mount Burr 11kV",null,"MWh","Non-Coincident",0,0,0,0,5.2660271734828717E-3,1.495667956894556E-2,2.956776738784413E-2]
[null,"Portee 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,9.4975063901353331E-3,2.311065985792194E-2]
[null,"Deloraine 11kV",null,"MWh","Non-Coincident",0,0,0,0,0,2.4137641202384252E-3,8.5945575352231029E-3]
[null,"Tintinara 11kV",null,"MWh","Non-Coincident",0,0,0,1.0574506484324516E-4,4.8480323445204091E-3,9.6090655532438864E-3,1.4388918792356405E-2]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]

{"sheet":"6.1 Telephone answering","index":30,"n_rows":1834,"n_cols":4,"rows_kept":1834,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"6.1 TELEPHONE ANSWERING"]
[]
[]
[null,"6.1.1 - TELEPHONE ANSWERING DATA"]
["C10 starts at first day of PRCP_y5 and goes for 5 full years","Date","Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) "]
[null,{"$f":"IF(dms_RPT=\"calendar\",DATE(VALUE(PRCP_y3),1,1),(DATE(VALUE(LEFT(PRCP_y3,2)&RIGHT(PRCP_y3,2)),7,1)))","v":"2013-07-01"},460,337]
[null,{"$f":"B9+1","v":"2013-07-02"},411,373]
[null,"2013-07-03",534,378]
[null,"2013-07-04",854,594]
[null,"2013-07-05",523,433]
[null,"2013-07-06",381,341]
[null,"2013-07-07",177,167]
[null,{"$f":"B15+1","v":"2013-07-08"},480,369]
[null,"2013-07-09",397,304]
[null,"2013-07-10",434,346]
[null,"2013-07-11",519,444]
[null,"2013-07-12",440,372]
[null,"2013-07-13",386,301]
[null,"2013-07-14",279,182]
[null,"2013-07-15",502,346]
[null,"2013-07-16",400,388]
[null,"2013-07-17",712,516]
[null,"2013-07-18",2578,1257]
[null,"2013-07-19",1447,1189]
[null,"2013-07-20",629,507]
[null,"2013-07-21",324,247]
[null,"2013-07-22",746,556]
[null,"2013-07-23",612,510]
[null,"2013-07-24",437,345]
[null,"2013-07-25",412,343]
[null,"2013-07-26",499,461]
[null,"2013-07-27",248,213]
[null,"2013-07-28",213,204]
[null,"2013-07-29",432,406]
[null,"2013-07-30",387,312]
[null,"2013-07-31",525,386]
[null,"2013-08-01",397,345]
[null,"2013-08-02",624,536]
[null,"2013-08-03",388,261]
[null,"2013-08-04",205,190]
[null,"2013-08-05",489,366]
[null,"2013-08-06",421,385]
[null,"2013-08-07",505,398]
[null,"2013-08-08",325,295]
[null,"2013-08-09",317,277]
[null,"2013-08-10",187,176]
[null,"2013-08-11",112,112]
[null,"2013-08-12",438,341]
[null,"2013-08-13",422,317]
[null,"2013-08-14",556,490]
[null,"2013-08-15",766,485]
[null,"2013-08-16",990,642]
[null,"2013-08-17",474,375]
[null,"2013-08-18",638,395]
[null,"2013-08-19",817,603]
[null,"2013-08-20",441,410]
[null,"2013-08-21",484,434]
[null,"2013-08-22",509,482]
[null,"2013-08-23",520,463]
[null,"2013-08-24",410,309]
[null,"2013-08-25",162,159]
[null,"2013-08-26",467,416]
[null,"2013-08-27",750,488]
[null,"2013-08-28",533,391]
[null,"2013-08-29",631,512]
[null,"2013-08-30",498,434]
[null,"2013-08-31",559,313]
[null,"2013-09-01",458,205]
[null,"2013-09-02",457,444]
[null,"2013-09-03",353,326]
[null,"2013-09-04",548,438]
[null,"2013-09-05",367,319]
[null,"2013-09-06",334,322]
[null,"2013-09-07",298,191]
[null,"2013-09-08",184,172]
[null,"2013-09-09",735,530]
[null,{"$f":"B79+1","v":"2013-09-10"},401,377]
[null,"2013-09-11",359,293]
[null,"2013-09-12",595,492]
[null,"2013-09-13",495,459]
[null,"2013-09-14",343,297]
[null,"2013-09-15",1367,669]
[null,"2013-09-16",751,553]
[null,"2013-09-17",420,383]
[null,"2013-09-18",825,678]
[null,"2013-09-19",795,642]
[null,"2013-09-20",429,338]
[null,"2013-09-21",189,180]
[null,"2013-09-22",120,109]
[null,"2013-09-23",512,501]
[null,"2013-09-24",419,388]
[null,"2013-09-25",401,387]
[null,"2013-09-26",1447,579]
[null,"2013-09-27",530,435]
[null,"2013-09-28",212,199]
[null,"2013-09-29",135,134]
[null,"2013-09-30",2551,691]
[null,"2013-10-01",1103,235]
[null,"2013-10-02",1141,523]
[null,"2013-10-03",422,386]
[null,"2013-10-04",485,434]
[null,"2013-10-05",175,174]
[null,"2013-10-06",116,112]
[null,"2013-10-07",253,232]
[null,"2013-10-08",492,360]
[null,"2013-10-09",498,442]
[null,"2013-10-10",501,383]
[null,"2013-10-11",395,356]
[null,"2013-10-12",196,189]
[null,"2013-10-13",573,332]
[null,"2013-10-14",528,444]
[null,"2013-10-15",438,260]
[null,"2013-10-16",1069,574]
[null,"2013-10-17",514,361]
[null,"2013-10-18",537,396]
[null,"2013-10-19",220,205]
[null,"2013-10-20",179,173]
[null,"2013-10-21",499,456]
[null,"2013-10-22",1932,791]
[null,"2013-10-23",477,438]
[null,"2013-10-24",344,326]
[null,"2013-10-25",376,343]
[null,"2013-10-26",310,204]
[null,"2013-10-27",170,152]
[null,"2013-10-28",446,371]
[null,"2013-10-29",323,296]
[null,"2013-10-30",326,309]
[null,"2013-10-31",343,335]
[null,"2013-11-01",405,332]
[null,"2013-11-02",218,199]
[null,"2013-11-03",196,192]
[null,"2013-11-04",371,363]
[null,"2013-11-05",308,305]
[null,"2013-11-06",633,547]
[null,"2013-11-07",479,439]
[null,"2013-11-08",475,427]
[null,"2013-11-09",139,124]
[null,"2013-11-10",114,110]
[null,"2013-11-11",362,348]
[null,"2013-11-12",390,365]
[null,{"$f":"B143+1","v":"2013-11-13"},386,353]
[null,"2013-11-14",356,339]
[null,"2013-11-15",460,401]
[null,"2013-11-16",154,147]
[null,"2013-11-17",326,286]
[null,"2013-11-18",482,433]
[null,"2013-11-19",906,458]
[null,"2013-11-20",662,392]
[null,"2013-11-21",416,353]
[null,"2013-11-22",301,296]
[null,"2013-11-23",149,139]
[null,"2013-11-24",103,94]
[null,"2013-11-25",408,380]
[null,"2013-11-26",503,465]
[null,"2013-11-27",702,514]
[null,"2013-11-28",527,436]
[null,"2013-11-29",273,262]
[null,"2013-11-30",171,165]
[null,"2013-12-01",454,339]
[null,"2013-12-02",463,386]
[null,"2013-12-03",1110,636]
[null,"2013-12-04",734,496]
[null,"2013-12-05",797,607]
[null,"2013-12-06",408,352]
[null,"2013-12-07",217,176]
[null,"2013-12-08",187,176]
[null,"2013-12-09",435,309]
[null,"2013-12-10",439,407]
[null,"2013-12-11",505,429]
[null,"2013-12-12",441,409]
[null,"2013-12-13",341,305]
[null,"2013-12-14",222,149]
[null,"2013-12-15",136,133]
[null,"2013-12-16",425,372]
[null,"2013-12-17",342,326]
[null,"2013-12-18",517,489]
[null,"2013-12-19",772,539]
[null,"2013-12-20",1569,746]
[null,"2013-12-21",4276,1062]
[null,"2013-12-22",332,260]
[null,"2013-12-23",532,511]
[null,"2013-12-24",193,189]
[null,"2013-12-25",89,77]
[null,"2013-12-26",123,119]
[null,"2013-12-27",171,169]
[null,"2013-12-28",199,187]
[null,"2013-12-29",64,63]
[null,"2013-12-30",223,221]
[null,"2013-12-31",358,331]
[null,"2014-01-01",412,365]
[null,"2014-01-02",282,278]
[null,"2014-01-03",238,234]
[null,"2014-01-04",89,87]
[null,"2014-01-05",276,231]
[null,"2014-01-06",277,264]
[null,"2014-01-07",235,226]
[null,"2014-01-08",256,249]
[null,"2014-01-09",307,266]
[null,"2014-01-10",364,347]
[null,"2014-01-11",358,238]
[null,"2014-01-12",201,182]
[null,"2014-01-13",1037,603]
[null,"2014-01-14",2420,719]
[null,"2014-01-15",1275,720]
[null,{"$f":"B207+1","v":"2014-01-16"},1573,885]
[null,"2014-01-17",1699,765]
[null,"2014-01-18",1102,485]
[null,"2014-01-19",247,225]
[null,"2014-01-20",413,325]
[null,"2014-01-21",371,335]
[null,"2014-01-22",287,284]
[null,"2014-01-23",347,301]
[null,"2014-01-24",358,331]
[null,"2014-01-25",157,152]
[null,"2014-01-26",137,134]
[null,"2014-01-27",219,171]
[null,"2014-01-28",604,478]
[null,"2014-01-29",565,492]
[null,"2014-01-30",447,399]
[null,"2014-01-31",365,337]
[null,"2014-02-01",534,373]
[null,"2014-02-02",1339,320]
[null,"2014-02-03",1372,727]
[null,"2014-02-04",7237,3504]
[null,"2014-02-05",3306,1851]
[null,"2014-02-06",1212,875]
[null,"2014-02-07",727,579]
[null,"2014-02-08",766,333]
[null,"2014-02-09",193,172]
[null,"2014-02-10",613,586]
[null,"2014-02-11",990,542]
[null,"2014-02-12",860,692]
[null,"2014-02-13",1091,670]
[null,"2014-02-14",1676,978]
[null,"2014-02-15",740,371]
[null,"2014-02-16",358,146]
[null,"2014-02-17",473,428]
[null,"2014-02-18",351,342]
[null,"2014-02-19",562,474]
[null,"2014-02-20",410,337]
[null,"2014-02-21",344,334]
[null,"2014-02-22",220,177]
[null,"2014-02-23",150,143]
[null,"2014-02-24",386,364]
[null,"2014-02-25",518,454]
[null,"2014-02-26",444,333]
[null,"2014-02-27",286,281]
[null,"2014-02-28",349,346]
[null,"2014-03-01",158,155]
[null,"2014-03-02",171,158]
[null,"2014-03-03",417,404]
[null,"2014-03-04",362,341]
[null,"2014-03-05",258,250]
[null,"2014-03-06",408,390]
[null,"2014-03-07",249,218]
[null,"2014-03-08",267,202]
[null,"2014-03-09",206,197]
[null,"2014-03-10",138,112]
[null,"2014-03-11",874,666]
[null,"2014-03-12",329,292]
[null,"2014-03-13",368,330]
[null,"2014-03-14",335,314]
[null,"2014-03-15",514,310]
[null,"2014-03-16",264,219]
[null,"2014-03-17",848,637]
[null,"2014-03-18",341,338]
[null,"2014-03-19",418,367]
[null,"2014-03-20",332,285]
[null,{"$f":"B271+1","v":"2014-03-21"},376,336]
[null,"2014-03-22",105,75]
[null,"2014-03-23",212,180]
[null,"2014-03-24",856,808]
[null,"2014-03-25",479,393]
[null,"2014-03-26",513,393]
[null,"2014-03-27",538,403]
[null,"2014-03-28",452,365]
[null,"2014-03-29",152,152]
[null,"2014-03-30",179,165]
[null,"2014-03-31",338,296]
[null,"2014-04-01",393,372]
[null,"2014-04-02",294,283]
[null,"2014-04-03",250,244]
[null,"2014-04-04",270,245]
[null,"2014-04-05",129,127]
[null,"2014-04-06",80,76]
[null,"2014-04-07",439,417]
[null,"2014-04-08",360,310]
[null,"2014-04-09",562,386]
[null,"2014-04-10",424,329]
[null,"2014-04-11",320,237]
[null,"2014-04-12",213,176]
[null,"2014-04-13",151,142]
[null,"2014-04-14",255,215]
[null,"2014-04-15",510,372]
[null,"2014-04-16",248,220]
[null,"2014-04-17",257,224]
[null,"2014-04-18",153,151]
[null,"2014-04-19",104,96]
[null,"2014-04-20",44,43]
[null,"2014-04-21",156,150]
[null,"2014-04-22",298,277]
[null,"2014-04-23",412,265]
[null,"2014-04-24",281,209]
[null,"2014-04-25",125,122]
[null,"2014-04-26",148,138]
[null,"2014-04-27",99,98]
[null,"2014-04-28",330,309]
[null,"2014-04-29",701,406]
[null,"2014-04-30",397,338]
[null,"2014-05-01",386,307]
[null,"2014-05-02",497,353]
[null,"2014-05-03",300,283]
[null,"2014-05-04",179,159]
[null,"2014-05-05",451,408]
[null,"2014-05-06",351,317]
[null,"2014-05-07",371,323]
[null,"2014-05-08",467,312]
[null,"2014-05-09",620,400]
[null,"2014-05-10",306,209]
[null,"2014-05-11",131,125]
[null,"2014-05-12",377,322]
[null,"2014-05-13",296,284]
[null,"2014-05-14",267,236]
[null,"2014-05-15",519,198]
[null,"2014-05-16",242,206]
[null,"2014-05-17",244,223]
[null,"2014-05-18",155,130]
[null,"2014-05-19",481,312]
[null,"2014-05-20",270,224]
[null,"2014-05-21",308,256]
[null,"2014-05-22",289,259]
[null,"2014-05-23",293,230]
[null,{"$f":"B335+1","v":"2014-05-24"},418,159]
[null,"2014-05-25",95,66]
[null,"2014-05-26",345,281]
[null,"2014-05-27",420,332]
[null,"2014-05-28",374,274]
[null,"2014-05-29",335,286]
[null,"2014-05-30",276,137]
[null,"2014-05-31",255,218]
[null,"2014-06-01",193,128]
[null,"2014-06-02",304,189]
[null,"2014-06-03",374,179]
[null,"2014-06-04",267,227]
[null,"2014-06-05",294,235]
[null,"2014-06-06",284,227]
[null,"2014-06-07",179,146]
[null,"2014-06-08",147,131]
[null,"2014-06-09",102,100]
[null,"2014-06-10",377,326]
[null,"2014-06-11",364,268]
[null,"2014-06-12",285,217]
[null,"2014-06-13",436,313]
[null,"2014-06-14",214,168]
[null,"2014-06-15",122,117]
[null,"2014-06-16",500,422]
[null,"2014-06-17",347,231]
[null,"2014-06-18",272,206]
[null,"2014-06-19",237,151]
[null,"2014-06-20",334,162]
[null,"2014-06-21",170,142]
[null,"2014-06-22",238,146]
[null,"2014-06-23",2190,450]
[null,"2014-06-24",680,111]
[null,"2014-06-25",427,198]
[null,"2014-06-26",364,261]
[null,"2014-06-27",689,257]
[null,"2014-06-28",918,566]
[null,"2014-06-29",233,180]
[null,"2014-06-30",463,209]
[null,"2014-07-01",345,165]
[null,"2014-07-02",335,229]
[null,"2014-07-03",339,214]
[null,"2014-07-04",519,327]
[null,"2014-07-05",178,145]
[null,"2014-07-06",215,159]
[null,"2014-07-07",305,248]
[null,"2014-07-08",937,429]
[null,"2014-07-09",566,403]
[null,"2014-07-10",503,391]
[null,"2014-07-11",502,268]
[null,"2014-07-12",234,144]
[null,"2014-07-13",163,142]
[null,"2014-07-14",314,245]
[null,"2014-07-15",632,437]
[null,"2014-07-16",968,431]
[null,"2014-07-17",579,403]
[null,"2014-07-18",486,387]
[null,"2014-07-19",203,192]
[null,"2014-07-20",166,151]
[null,"2014-07-21",353,257]
[null,"2014-07-22",359,319]
[null,"2014-07-23",548,427]
[null,"2014-07-24",407,327]
[null,"2014-07-25",282,265]
[null,"2014-07-26",190,151]
[null,{"$f":"B399+1","v":"2014-07-27"},136,123]
[null,"2014-07-28",395,309]
[null,"2014-07-29",561,294]
[null,"2014-07-30",314,299]
[null,"2014-07-31",564,357]
[null,"2014-08-01",938,344]
[null,"2014-08-02",274,168]
[null,"2014-08-03",195,173]
[null,"2014-08-04",672,280]
[null,"2014-08-05",499,406]
[null,"2014-08-06",331,298]
[null,"2014-08-07",287,245]
[null,"2014-08-08",339,288]
[null,"2014-08-09",146,128]
[null,"2014-08-10",142,118]
[null,"2014-08-11",322,268]
[null,"2014-08-12",307,254]
[null,"2014-08-13",362,334]
[null,"2014-08-14",339,297]
[null,"2014-08-15",255,221]
[null,"2014-08-16",219,174]
[null,"2014-08-17",166,138]
[null,"2014-08-18",710,345]
[null,"2014-08-19",290,244]
[null,"2014-08-20",371,319]
[null,"2014-08-21",257,221]
[null,"2014-08-22",388,280]
[null,"2014-08-23",129,102]
[null,"2014-08-24",135,104]
[null,"2014-08-25",261,240]
[null,"2014-08-26",270,252]
[null,"2014-08-27",247,229]
[null,"2014-08-28",220,205]
[null,"2014-08-29",233,213]
[null,"2014-08-30",126,125]
[null,"2014-08-31",174,154]
[null,"2014-09-01",390,305]
[null,"2014-09-02",443,398]
[null,"2014-09-03",375,333]
[null,"2014-09-04",431,377]
[null,"2014-09-05",273,237]
[null,"2014-09-06",132,130]
[null,"2014-09-07",156,145]
[null,"2014-09-08",531,438]
[null,"2014-09-09",433,321]
[null,"2014-09-10",488,416]
[null,"2014-09-11",336,314]
[null,"2014-09-12",295,203]
[null,"2014-09-13",199,146]
[null,"2014-09-14",141,129]
[null,"2014-09-15",341,306]
[null,"2014-09-16",364,318]
[null,"2014-09-17",231,223]
[null,"2014-09-18",281,266]
[null,"2014-09-19",285,246]
[null,"2014-09-20",308,209]
[null,"2014-09-21",118,116]
[null,"2014-09-22",282,261]
[null,"2014-09-23",377,330]
[null,"2014-09-24",249,235]
[null,"2014-09-25",284,220]
[null,"2014-09-26",265,232]
[null,"2014-09-27",153,115]
[null,"2014-09-28",1565,496]
[null,{"$f":"B463+1","v":"2014-09-29"},340,328]
[null,"2014-09-30",517,339]
[null,"2014-10-01",311,259]
[null,"2014-10-02",347,308]
[null,"2014-10-03",293,223]
[null,"2014-10-04",242,156]
[null,"2014-10-05",171,125]
[null,"2014-10-06",1421,425]
[null,"2014-10-07",368,309]
[null,"2014-10-08",455,357]
[null,"2014-10-09",287,209]
[null,"2014-10-10",327,254]
[null,"2014-10-11",134,130]
[null,"2014-10-12",96,93]
[null,"2014-10-13",346,264]
[null,"2014-10-14",252,196]
[null,"2014-10-15",293,239]
[null,"2014-10-16",331,276]
[null,"2014-10-17",259,225]
[null,"2014-10-18",140,131]
[null,"2014-10-19",124,116]
[null,"2014-10-20",333,273]
[null,"2014-10-21",286,235]
[null,"2014-10-22",292,246]
[null,"2014-10-23",262,214]
[null,"2014-10-24",277,226]
[null,"2014-10-25",130,114]
[null,"2014-10-26",1235,293]
[null,"2014-10-27",899,388]
[null,"2014-10-28",304,280]
[null,"2014-10-29",269,262]
[null,"2014-10-30",241,210]
[null,"2014-10-31",302,253]
[null,"2014-11-01",215,204]
[null,"2014-11-02",96,94]
[null,"2014-11-03",321,294]
[null,"2014-11-04",327,279]
[null,"2014-11-05",253,227]
[null,"2014-11-06",270,253]
[null,"2014-11-07",369,350]
[null,"2014-11-08",181,148]
[null,"2014-11-09",160,127]
[null,"2014-11-10",267,213]
[null,"2014-11-11",357,315]
[null,"2014-11-12",476,354]
[null,"2014-11-13",383,326]
[null,"2014-11-14",322,255]
[null,"2014-11-15",366,200]
[null,"2014-11-16",105,85]
[null,"2014-11-17",284,238]
[null,"2014-11-18",458,380]
[null,"2014-11-19",334,305]
[null,"2014-11-20",433,373]
[null,"2014-11-21",241,223]
[null,"2014-11-22",1863,646]
[null,"2014-11-23",706,383]
[null,"2014-11-24",607,417]
[null,"2014-11-25",357,309]
[null,"2014-11-26",298,264]
[null,"2014-11-27",269,246]
[null,"2014-11-28",306,260]
[null,"2014-11-29",228,213]
[null,"2014-11-30",249,221]
[null,"2014-12-01",348,320]
[null,{"$f":"B527+1","v":"2014-12-02"},343,315]
[null,"2014-12-03",570,499]
[null,"2014-12-04",251,209]
[null,"2014-12-05",262,234]
[null,"2014-12-06",151,134]
[null,"2014-12-07",98,95]
[null,"2014-12-08",250,240]
[null,"2014-12-09",259,228]
[null,"2014-12-10",662,513]
[null,"2014-12-11",623,495]
[null,"2014-12-12",192,167]
[null,"2014-12-13",132,110]
[null,"2014-12-14",221,198]
[null,"2014-12-15",565,484]
[null,"2014-12-16",398,337]
[null,"2014-12-17",202,194]
[null,"2014-12-18",290,267]
[null,"2014-12-19",246,229]
[null,"2014-12-20",170,167]
[null,"2014-12-21",156,146]
[null,"2014-12-22",366,331]
[null,"2014-12-23",258,250]
[null,"2014-12-24",159,152]
[null,"2014-12-25",44,43]
[null,"2014-12-26",105,102]
[null,"2014-12-27",65,65]
[null,"2014-12-28",80,80]
[null,"2014-12-29",441,373]
[null,"2014-12-30",157,157]
[null,"2014-12-31",120,120]
[null,"2015-01-01",170,166]
[null,"2015-01-02",644,513]
[null,"2015-01-03",630,507]
[null,"2015-01-04",216,208]
[null,"2015-01-05",403,386]
[null,"2015-01-06",471,450]
[null,"2015-01-07",1986,774]
[null,"2015-01-08",1964,1258]
[null,"2015-01-09",727,681]
[null,"2015-01-10",604,547]
[null,"2015-01-11",170,170]
[null,"2015-01-12",574,543]
[null,"2015-01-13",588,544]
[null,"2015-01-14",358,351]
[null,"2015-01-15",305,304]
[null,"2015-01-16",279,278]
[null,"2015-01-17",124,122]
[null,"2015-01-18",86,86]
[null,"2015-01-19",416,394]
[null,"2015-01-20",318,313]
[null,"2015-01-21",619,479]
[null,"2015-01-22",323,307]
[null,"2015-01-23",313,302]
[null,"2015-01-24",189,165]
[null,"2015-01-25",171,132]
[null,"2015-01-26",113,113]
[null,"2015-01-27",288,282]
[null,"2015-01-28",275,272]
[null,"2015-01-29",348,343]
[null,"2015-01-30",303,295]
[null,"2015-01-31",214,213]
[null,"2015-02-01",142,140]
[null,"2015-02-02",325,320]
[null,"2015-02-03",267,264]
[null,{"$f":"B591+1","v":"2015-02-04"},257,252]
[null,"2015-02-05",329,321]
[null,"2015-02-06",429,410]
[null,"2015-02-07",445,406]
[null,"2015-02-08",167,165]
[null,"2015-02-09",304,286]
[null,"2015-02-10",354,345]
[null,"2015-02-11",264,260]
[null,"2015-02-12",368,352]
[null,"2015-02-13",251,224]
[null,"2015-02-14",277,231]
[null,"2015-02-15",286,270]
[null,"2015-02-16",381,353]
[null,"2015-02-17",284,278]
[null,"2015-02-18",280,278]
[null,"2015-02-19",361,348]
[null,"2015-02-20",380,355]
[null,"2015-02-21",542,428]
[null,"2015-02-22",285,267]
[null,"2015-02-23",576,500]
[null,"2015-02-24",260,256]
[null,"2015-02-25",280,244]
[null,"2015-02-26",183,178]
[null,"2015-02-27",255,233]
[null,"2015-02-28",239,227]
[null,"2015-03-01",260,212]
[null,"2015-03-02",302,298]
[null,"2015-03-03",303,285]
[null,"2015-03-04",242,241]
[null,"2015-03-05",335,298]
[null,"2015-03-06",240,231]
[null,"2015-03-07",143,141]
[null,"2015-03-08",161,155]
[null,"2015-03-09",367,342]
[null,"2015-03-10",254,254]
[null,"2015-03-11",266,265]
[null,"2015-03-12",394,372]
[null,"2015-03-13",302,294]
[null,"2015-03-14",165,164]
[null,"2015-03-15",172,166]
[null,"2015-03-16",263,259]
[null,"2015-03-17",381,376]
[null,"2015-03-18",290,288]
[null,"2015-03-19",280,254]
[null,"2015-03-20",227,217]
[null,"2015-03-21",157,154]
[null,"2015-03-22",168,158]
[null,"2015-03-23",323,301]
[null,"2015-03-24",199,198]
[null,"2015-03-25",337,317]
[null,"2015-03-26",188,185]
[null,"2015-03-27",259,255]
[null,"2015-03-28",225,221]
[null,"2015-03-29",75,74]
[null,"2015-03-30",293,276]
[null,"2015-03-31",239,236]
[null,"2015-04-01",213,212]
[null,"2015-04-02",237,234]
[null,"2015-04-03",180,169]
[null,"2015-04-04",88,88]
[null,"2015-04-05",56,56]
[null,"2015-04-06",666,544]
[null,"2015-04-07",499,465]
[null,"2015-04-08",301,295]
[null,{"$f":"B655+1","v":"2015-04-09"},346,323]
[null,"2015-04-10",320,315]
[null,"2015-04-11",264,251]
[null,"2015-04-12",137,129]
[null,"2015-04-13",366,339]
[null,"2015-04-14",255,253]
[null,"2015-04-15",255,245]
[null,"2015-04-16",478,458]
[null,"2015-04-17",392,357]
[null,"2015-04-18",206,196]
[null,"2015-04-19",151,131]
[null,"2015-04-20",284,268]
[null,"2015-04-21",341,337]
[null,"2015-04-22",246,234]
[null,"2015-04-23",224,218]
[null,"2015-04-24",301,275]
[null,"2015-04-25",180,164]
[null,"2015-04-26",126,125]
[null,"2015-04-27",387,309]
[null,"2015-04-28",267,216]
[null,"2015-04-29",267,225]
[null,"2015-04-30",255,232]
[null,"2015-05-01",218,215]
[null,"2015-05-02",303,245]
[null,"2015-05-03",112,111]
[null,"2015-05-04",358,302]
[null,"2015-05-05",1467,911]
[null,"2015-05-06",334,323]
[null,"2015-05-07",210,200]
[null,"2015-05-08",287,273]
[null,"2015-05-09",248,241]
[null,"2015-05-10",264,258]
[null,"2015-05-11",331,305]
[null,"2015-05-12",393,370]
[null,"2015-05-13",402,348]
[null,"2015-05-14",405,354]
[null,"2015-05-15",294,263]
[null,"2015-05-16",177,177]
[null,"2015-05-17",444,252]
[null,"2015-05-18",342,287]
[null,"2015-05-19",788,505]
[null,"2015-05-20",379,335]
[null,"2015-05-21",258,239]
[null,"2015-05-22",336,311]
[null,"2015-05-23",230,180]
[null,"2015-05-24",424,360]
[null,"2015-05-25",330,288]
[null,"2015-05-26",468,428]
[null,"2015-05-27",261,244]
[null,"2015-05-28",273,257]
[null,"2015-05-29",253,245]
[null,"2015-05-30",138,133]
[null,"2015-05-31",141,128]
[null,"2015-06-01",304,263]
[null,"2015-06-02",237,227]
[null,"2015-06-03",278,253]
[null,"2015-06-04",351,299]
[null,"2015-06-05",333,276]
[null,"2015-06-06",184,172]
[null,"2015-06-07",92,90]
[null,"2015-06-08",122,112]
[null,"2015-06-09",286,233]
[null,"2015-06-10",328,297]
[null,"2015-06-11",251,235]
[null,{"$f":"B719+1","v":"2015-06-12"},278,261]
[null,"2015-06-13",311,184]
[null,"2015-06-14",137,127]
[null,"2015-06-15",299,285]
[null,"2015-06-16",351,319]
[null,"2015-06-17",359,293]
[null,"2015-06-18",365,302]
[null,"2015-06-19",285,257]
[null,"2015-06-20",142,130]
[null,"2015-06-21",103,95]
[null,"2015-06-22",427,365]
[null,"2015-06-23",394,352]
[null,"2015-06-24",251,234]
[null,"2015-06-25",285,254]
[null,"2015-06-26",502,387]
[null,"2015-06-27",191,171]
[null,"2015-06-28",178,176]
[null,"2015-06-29",318,233]
[null,"2015-06-30",300,281]
[null,"2015-07-01",275,233]
[null,"2015-07-02",290,233]
[null,"2015-07-03",229,210]
[null,"2015-07-04",176,144]
[null,"2015-07-05",210,193]
[null,"2015-07-06",412,331]
[null,"2015-07-07",350,321]
[null,"2015-07-08",267,240]
[null,"2015-07-09",293,247]
[null,"2015-07-10",240,219]
[null,"2015-07-11",557,441]
[null,"2015-07-12",439,314]
[null,"2015-07-13",335,247]
[null,"2015-07-14",431,250]
[null,"2015-07-15",455,337]
[null,"2015-07-16",394,309]
[null,"2015-07-17",356,271]
[null,"2015-07-18",203,179]
[null,"2015-07-19",109,106]
[null,"2015-07-20",616,408]
[null,"2015-07-21",332,287]
[null,"2015-07-22",365,226]
[null,"2015-07-23",272,242]
[null,"2015-07-24",472,327]
[null,"2015-07-25",446,338]
[null,"2015-07-26",245,214]
[null,"2015-07-27",404,332]
[null,"2015-07-28",354,323]
[null,"2015-07-29",304,268]
[null,"2015-07-30",335,283]
[null,"2015-07-31",426,295]
[null,"2015-08-01",284,265]
[null,"2015-08-02",223,197]
[null,"2015-08-03",344,261]
[null,"2015-08-04",424,361]
[null,"2015-08-05",301,273]
[null,"2015-08-06",291,247]
[null,"2015-08-07",306,249]
[null,"2015-08-08",173,165]
[null,"2015-08-09",145,140]
[null,"2015-08-10",305,260]
[null,"2015-08-11",525,416]
[null,"2015-08-12",543,378]
[null,"2015-08-13",330,279]
[null,"2015-08-14",263,191]
[null,{"$f":"B783+1","v":"2015-08-15"},217,176]
[null,"2015-08-16",126,113]
[null,"2015-08-17",383,280]
[null,"2015-08-18",269,244]
[null,"2015-08-19",265,146]
[null,"2015-08-20",352,298]
[null,"2015-08-21",270,229]
[null,"2015-08-22",204,172]
[null,"2015-08-23",215,203]
[null,"2015-08-24",323,228]
[null,"2015-08-25",308,225]
[null,"2015-08-26",322,283]
[null,"2015-08-27",253,191]
[null,"2015-08-28",269,164]
[null,"2015-08-29",197,176]
[null,"2015-08-30",136,125]
[null,"2015-08-31",289,256]
[null,"2015-09-01",185,173]
[null,"2015-09-02",311,273]
[null,"2015-09-03",293,278]
[null,"2015-09-04",254,175]
[null,"2015-09-05",183,156]
[null,"2015-09-06",281,243]
[null,"2015-09-07",354,300]
[null,"2015-09-08",366,251]
[null,"2015-09-09",204,109]
[null,"2015-09-10",415,229]
[null,"2015-09-11",229,159]
[null,"2015-09-12",173,167]
[null,"2015-09-13",146,139]
[null,"2015-09-14",326,167]
[null,"2015-09-15",204,119]
[null,"2015-09-16",326,231]
[null,"2015-09-17",228,143]
[null,"2015-09-18",233,110]
[null,"2015-09-19",142,132]
[null,"2015-09-20",106,98]
[null,"2015-09-21",225,113]
[null,"2015-09-22",207,113]
[null,"2015-09-23",267,209]
[null,"2015-09-24",175,155]
[null,"2015-09-25",213,157]
[null,"2015-09-26",125,114]
[null,"2015-09-27",128,96]
[null,"2015-09-28",228,163]
[null,"2015-09-29",255,196]
[null,"2015-09-30",255,201]
[null,"2015-10-01",213,176]
[null,"2015-10-02",284,267]
[null,"2015-10-03",240,175]
[null,"2015-10-04",79,77]
[null,"2015-10-05",262,159]
[null,"2015-10-06",309,174]
[null,"2015-10-07",202,146]
[null,"2015-10-08",246,189]
[null,"2015-10-09",272,122]
[null,"2015-10-10",311,236]
[null,"2015-10-11",90,83]
[null,"2015-10-12",262,206]
[null,"2015-10-13",299,282]
[null,"2015-10-14",223,206]
[null,"2015-10-15",278,187]
[null,"2015-10-16",291,234]
[null,"2015-10-17",146,114]
[null,{"$f":"B847+1","v":"2015-10-18"},67,66]
[null,"2015-10-19",235,190]
[null,"2015-10-20",432,306]
[null,"2015-10-21",315,250]
[null,"2015-10-22",222,142]
[null,"2015-10-23",193,151]
[null,"2015-10-24",107,94]
[null,"2015-10-25",116,99]
[null,"2015-10-26",328,256]
[null,"2015-10-27",288,239]
[null,"2015-10-28",228,194]
[null,"2015-10-29",319,270]
[null,"2015-10-30",259,143]
[null,"2015-10-31",195,66]
[null,"2015-11-01",2006,192]
[null,"2015-11-02",547,239]
[null,"2015-11-03",448,345]
[null,"2015-11-04",715,373]
[null,"2015-11-05",389,184]
[null,"2015-11-06",272,173]
[null,"2015-11-07",183,142]
[null,"2015-11-08",145,122]
[null,"2015-11-09",345,178]
[null,"2015-11-10",292,177]
[null,"2015-11-11",278,187]
[null,"2015-11-12",381,268]
[null,"2015-11-13",249,137]
[null,"2015-11-14",131,103]
[null,"2015-11-15",108,92]
[null,"2015-11-16",254,149]
[null,"2015-11-17",331,261]
[null,"2015-11-18",297,211]
[null,"2015-11-19",263,214]
[null,"2015-11-20",220,168]
[null,"2015-11-21",175,131]
[null,"2015-11-22",54,49]
[null,"2015-11-23",203,163]
[null,"2015-11-24",270,214]
[null,"2015-11-25",791,529]
[null,"2015-11-26",540,319]
[null,"2015-11-27",336,262]
[null,"2015-11-28",143,118]
[null,"2015-11-29",113,108]
[null,"2015-11-30",430,258]
[null,"2015-12-01",328,212]
[null,"2015-12-02",333,223]
[null,"2015-12-03",367,296]
[null,"2015-12-04",363,261]
[null,"2015-12-05",294,204]
[null,"2015-12-06",468,290]
[null,"2015-12-07",893,631]
[null,"2015-12-08",1241,508]
[null,"2015-12-09",452,381]
[null,"2015-12-10",309,279]
[null,"2015-12-11",252,167]
[null,"2015-12-12",154,139]
[null,"2015-12-13",128,113]
[null,"2015-12-14",255,220]
[null,"2015-12-15",675,364]
[null,"2015-12-16",555,428]
[null,"2015-12-17",916,438]
[null,"2015-12-18",725,428]
[null,"2015-12-19",876,309]
[null,"2015-12-20",275,212]
[null,{"$f":"B911+1","v":"2015-12-21"},222,157]
[null,"2015-12-22",293,208]
[null,"2015-12-23",209,185]
[null,"2015-12-24",276,222]
[null,"2015-12-25",222,170]
[null,"2015-12-26",236,121]
[null,"2015-12-27",103,74]
[null,"2015-12-28",188,174]
[null,"2015-12-29",215,174]
[null,"2015-12-30",391,287]
[null,"2015-12-31",194,173]
[null,"2016-01-01",140,137]
[null,"2016-01-02",130,130]
[null,"2016-01-03",272,117]
[null,"2016-01-04",293,232]
[null,"2016-01-05",261,207]
[null,"2016-01-06",314,215]
[null,"2016-01-07",350,321]
[null,"2016-01-08",333,257]
[null,"2016-01-09",120,118]
[null,"2016-01-10",189,147]
[null,"2016-01-11",313,269]
[null,"2016-01-12",594,425]
[null,"2016-01-13",333,180]
[null,"2016-01-14",477,247]
[null,"2016-01-15",217,188]
[null,"2016-01-16",208,168]
[null,"2016-01-17",182,158]
[null,"2016-01-18",334,242]
[null,"2016-01-19",312,240]
[null,"2016-01-20",318,235]
[null,"2016-01-21",312,223]
[null,"2016-01-22",1678,530]
[null,"2016-01-23",315,234]
[null,"2016-01-24",162,143]
[null,"2016-01-25",252,244]
[null,"2016-01-26",111,106]
[null,"2016-01-27",316,164]
[null,"2016-01-28",374,261]
[null,"2016-01-29",849,354]
[null,"2016-01-30",524,350]
[null,"2016-01-31",164,131]
[null,"2016-02-01",335,284]
[null,"2016-02-02",617,497]
[null,"2016-02-03",347,311]
[null,"2016-02-04",271,253]
[null,"2016-02-05",246,228]
[null,"2016-02-06",190,175]
[null,"2016-02-07",138,111]
[null,"2016-02-08",392,353]
[null,"2016-02-09",299,285]
[null,"2016-02-10",313,281]
[null,"2016-02-11",296,271]
[null,"2016-02-12",289,265]
[null,"2016-02-13",189,169]
[null,"2016-02-14",137,109]
[null,"2016-02-15",262,241]
[null,"2016-02-16",244,227]
[null,"2016-02-17",254,244]
[null,"2016-02-18",411,350]
[null,"2016-02-19",414,306]
[null,"2016-02-20",100,93]
[null,"2016-02-21",105,101]
[null,"2016-02-22",428,390]
[null,{"$f":"B975+1","v":"2016-02-23"},296,268]
[null,"2016-02-24",224,214]
[null,"2016-02-25",238,219]
[null,"2016-02-26",220,196]
[null,"2016-02-27",193,175]
[null,"2016-02-28",164,150]
[null,"2016-02-29",258,208]
[null,"2016-03-01",229,207]
[null,"2016-03-02",417,296]
[null,"2016-03-03",270,248]
[null,"2016-03-04",238,183]
[null,"2016-03-05",242,196]
[null,"2016-03-06",974,636]
[null,"2016-03-07",396,298]
[null,"2016-03-08",484,301]
[null,"2016-03-09",284,215]
[null,"2016-03-10",563,326]
[null,"2016-03-11",370,255]
[null,"2016-03-12",270,206]
[null,"2016-03-13",270,219]
[null,"2016-03-14",116,113]
[null,"2016-03-15",291,231]
[null,"2016-03-16",228,218]
[null,"2016-03-17",439,372]
[null,"2016-03-18",463,281]
[null,"2016-03-19",140,118]
[null,"2016-03-20",122,98]
[null,"2016-03-21",256,210]
[null,"2016-03-22",264,206]
[null,"2016-03-23",259,184]
[null,"2016-03-24",301,222]
[null,"2016-03-25",135,111]
[null,"2016-03-26",79,76]
[null,"2016-03-27",112,108]
[null,"2016-03-28",80,73]
[null,"2016-03-29",229,216]
[null,"2016-03-30",189,166]
[null,"2016-03-31",250,176]
[null,"2016-04-01",206,153]
[null,"2016-04-02",172,156]
[null,"2016-04-03",94,89]
[null,"2016-04-04",215,153]
[null,"2016-04-05",249,204]
[null,"2016-04-06",248,206]
[null,"2016-04-07",227,201]
[null,"2016-04-08",243,216]
[null,"2016-04-09",134,119]
[null,"2016-04-10",86,81]
[null,"2016-04-11",247,212]
[null,"2016-04-12",291,246]
[null,"2016-04-13",179,168]
[null,"2016-04-14",214,183]
[null,"2016-04-15",179,159]
[null,"2016-04-16",111,105]
[null,"2016-04-17",77,77]
[null,"2016-04-18",193,140]
[null,"2016-04-19",195,136]
[null,"2016-04-20",246,175]
[null,"2016-04-21",367,299]
[null,"2016-04-22",231,212]
[null,"2016-04-23",133,107]
[null,"2016-04-24",65,55]
[null,"2016-04-25",63,62]
[null,"2016-04-26",212,191]
[null,{"$f":"B1039+1","v":"2016-04-27"},252,239]
[null,"2016-04-28",264,223]
[null,"2016-04-29",260,216]
[null,"2016-04-30",455,366]
[null,"2016-05-01",271,156]
[null,"2016-05-02",318,260]
[null,"2016-05-03",512,391]
[null,"2016-05-04",247,218]
[null,"2016-05-05",245,213]
[null,"2016-05-06",201,180]
[null,"2016-05-07",147,140]
[null,"2016-05-08",197,179]
[null,"2016-05-09",2515,823]
[null,"2016-05-10",739,457]
[null,"2016-05-11",313,262]
[null,"2016-05-12",317,272]
[null,"2016-05-13",251,228]
[null,"2016-05-14",202,182]
[null,"2016-05-15",79,76]
[null,"2016-05-16",257,206]
[null,"2016-05-17",227,181]
[null,"2016-05-18",288,262]
[null,"2016-05-19",259,236]
[null,"2016-05-20",220,206]
[null,"2016-05-21",137,129]
[null,"2016-05-22",147,123]
[null,"2016-05-23",359,280]
[null,"2016-05-24",224,206]
[null,"2016-05-25",330,270]
[null,"2016-05-26",369,262]
[null,"2016-05-27",346,302]
[null,"2016-05-28",258,231]
[null,"2016-05-29",175,150]
[null,"2016-05-30",273,230]
[null,"2016-05-31",329,287]
[null,"2016-06-01",227,203]
[null,"2016-06-02",258,208]
[null,"2016-06-03",293,264]
[null,"2016-06-04",192,169]
[null,"2016-06-05",205,193]
[null,"2016-06-06",301,259]
[null,"2016-06-07",225,191]
[null,"2016-06-08",312,255]
[null,"2016-06-09",427,385]
[null,"2016-06-10",290,273]
[null,"2016-06-11",183,173]
[null,"2016-06-12",107,98]
[null,"2016-06-13",155,148]
[null,"2016-06-14",462,345]
[null,"2016-06-15",347,305]
[null,"2016-06-16",387,356]
[null,"2016-06-17",262,234]
[null,"2016-06-18",183,160]
[null,"2016-06-19",83,71]
[null,"2016-06-20",279,208]
[null,"2016-06-21",489,418]
[null,"2016-06-22",240,232]
[null,"2016-06-23",405,333]
[null,"2016-06-24",775,501]
[null,"2016-06-25",312,239]
[null,"2016-06-26",153,132]
[null,"2016-06-27",506,372]
[null,"2016-06-28",324,306]
[null,"2016-06-29",351,329]
[null,{"$f":"B1103+1","v":"2016-06-30"},405,367]
[null,"2016-07-01",283,245]
[null,"2016-07-02",192,175]
[null,"2016-07-03",102,96]
[null,"2016-07-04",389,220]
[null,"2016-07-05",918,545]
[null,"2016-07-06",445,327]
[null,"2016-07-07",439,296]
[null,"2016-07-08",377,252]
[null,"2016-07-09",273,225]
[null,"2016-07-10",367,304]
[null,"2016-07-11",1599,965]
[null,"2016-07-12",5979,1117]
[null,"2016-07-13",1631,796]
[null,"2016-07-14",573,451]
[null,"2016-07-15",290,188]
[null,"2016-07-16",274,207]
[null,"2016-07-17",189,165]
[null,"2016-07-18",442,271]
[null,"2016-07-19",276,210]
[null,"2016-07-20",352,272]
[null,"2016-07-21",379,336]
[null,"2016-07-22",872,452]
[null,"2016-07-23",382,336]
[null,"2016-07-24",620,461]
[null,"2016-07-25",581,390]
[null,"2016-07-26",527,387]
[null,"2016-07-27",353,320]
[null,"2016-07-28",377,326]
[null,"2016-07-29",303,236]
[null,"2016-07-30",367,274]
[null,"2016-07-31",123,120]
[null,"2016-08-01",433,338]
[null,"2016-08-02",677,494]
[null,"2016-08-03",295,278]
[null,"2016-08-04",422,347]
[null,"2016-08-05",585,417]
[null,"2016-08-06",194,185]
[null,"2016-08-07",210,188]
[null,"2016-08-08",347,243]
[null,"2016-08-09",478,349]
[null,"2016-08-10",497,337]
[null,"2016-08-11",173,161]
[null,"2016-08-12",265,196]
[null,"2016-08-13",335,280]
[null,"2016-08-14",181,156]
[null,"2016-08-15",315,245]
[null,"2016-08-16",215,199]
[null,"2016-08-17",250,205]
[null,"2016-08-18",367,348]
[null,"2016-08-19",376,304]
[null,"2016-08-20",242,206]
[null,"2016-08-21",144,130]
[null,"2016-08-22",323,290]
[null,"2016-08-23",324,298]
[null,"2016-08-24",223,185]
[null,"2016-08-25",316,290]
[null,"2016-08-26",282,237]
[null,"2016-08-27",167,155]
[null,"2016-08-28",132,124]
[null,"2016-08-29",339,290]
[null,"2016-08-30",392,348]
[null,"2016-08-31",239,232]
[null,"2016-09-01",212,207]
[null,{"$f":"B1167+1","v":"2016-09-02"},241,220]
[null,"2016-09-03",264,202]
[null,"2016-09-04",94,82]
[null,"2016-09-05",256,246]
[null,"2016-09-06",239,231]
[null,"2016-09-07",232,218]
[null,"2016-09-08",1300,642]
[null,"2016-09-09",520,480]
[null,"2016-09-10",193,184]
[null,"2016-09-11",147,138]
[null,"2016-09-12",383,368]
[null,"2016-09-13",301,290]
[null,"2016-09-14",1425,1077]
[null,"2016-09-15",498,434]
[null,"2016-09-16",344,320]
[null,"2016-09-17",409,314]
[null,"2016-09-18",151,141]
[null,"2016-09-19",257,236]
[null,"2016-09-20",428,389]
[null,"2016-09-21",307,276]
[null,"2016-09-22",250,218]
[null,"2016-09-23",213,211]
[null,"2016-09-24",205,187]
[null,"2016-09-25",165,152]
[null,"2016-09-26",325,294]
[null,"2016-09-27",305,287]
[null,"2016-09-28",7878,3568]
[null,"2016-09-29",4487,3197]
[null,"2016-09-30",1884,1554]
[null,"2016-10-01",896,632]
[null,"2016-10-02",524,342]
[null,"2016-10-03",656,513]
[null,"2016-10-04",819,568]
[null,"2016-10-05",599,376]
[null,"2016-10-06",445,378]
[null,"2016-10-07",462,405]
[null,"2016-10-08",232,201]
[null,"2016-10-09",392,155]
[null,"2016-10-10",601,404]
[null,"2016-10-11",359,329]
[null,"2016-10-12",300,275]
[null,"2016-10-13",290,282]
[null,"2016-10-14",263,245]
[null,"2016-10-15",231,198]
[null,"2016-10-16",233,162]
[null,"2016-10-17",276,268]
[null,"2016-10-18",294,285]
[null,"2016-10-19",248,241]
[null,"2016-10-20",496,414]
[null,"2016-10-21",543,458]
[null,"2016-10-22",212,189]
[null,"2016-10-23",110,102]
[null,"2016-10-24",307,289]
[null,"2016-10-25",322,280]
[null,"2016-10-26",224,212]
[null,"2016-10-27",425,406]
[null,"2016-10-28",326,305]
[null,"2016-10-29",222,203]
[null,"2016-10-30",284,246]
[null,"2016-10-31",253,217]
[null,"2016-11-01",259,231]
[null,"2016-11-02",278,259]
[null,"2016-11-03",230,215]
[null,"2016-11-04",224,215]
[null,{"$f":"B1231+1","v":"2016-11-05"},146,133]
[null,"2016-11-06",102,99]
[null,"2016-11-07",410,380]
[null,"2016-11-08",299,290]
[null,"2016-11-09",243,241]
[null,"2016-11-10",244,228]
[null,"2016-11-11",1480,677]
[null,"2016-11-12",1359,731]
[null,"2016-11-13",577,442]
[null,"2016-11-14",353,334]
[null,"2016-11-15",248,236]
[null,"2016-11-16",424,382]
[null,"2016-11-17",348,327]
[null,"2016-11-18",253,235]
[null,"2016-11-19",220,195]
[null,"2016-11-20",229,178]
[null,"2016-11-21",805,423]
[null,"2016-11-22",290,276]
[null,"2016-11-23",232,213]
[null,"2016-11-24",245,230]
[null,"2016-11-25",249,244]
[null,"2016-11-26",214,196]
[null,"2016-11-27",133,129]
[null,"2016-11-28",333,306]
[null,"2016-11-29",249,228]
[null,"2016-11-30",251,241]
[null,"2016-12-01",1816,323]
[null,"2016-12-02",229,219]
[null,"2016-12-03",132,127]
[null,"2016-12-04",295,260]
[null,"2016-12-05",252,244]
[null,"2016-12-06",235,214]
[null,"2016-12-07",288,243]
[null,"2016-12-08",568,439]
[null,"2016-12-09",242,220]
[null,"2016-12-10",126,119]
[null,"2016-12-11",106,102]
[null,"2016-12-12",362,317]
[null,"2016-12-13",325,305]
[null,"2016-12-14",252,225]
[null,"2016-12-15",288,273]
[null,"2016-12-16",255,246]
[null,"2016-12-17",212,195]
[null,"2016-12-18",121,111]
[null,"2016-12-19",328,277]
[null,"2016-12-20",300,249]
[null,"2016-12-21",222,211]
[null,"2016-12-22",214,187]
[null,"2016-12-23",400,339]
[null,"2016-12-24",303,263]
[null,"2016-12-25",182,177]
[null,"2016-12-26",257,242]
[null,"2016-12-27",302,261]
[null,"2016-12-28",8904,3030]
[null,"2016-12-29",2881,939]
[null,"2016-12-30",1824,1137]
[null,"2016-12-31",726,544]
[null,"2017-01-01",291,261]
[null,"2017-01-02",247,226]
[null,"2017-01-03",404,398]
[null,"2017-01-04",304,299]
[null,"2017-01-05",412,375]
[null,"2017-01-06",572,536]
[null,"2017-01-07",305,280]
[null,{"$f":"B1295+1","v":"2017-01-08"},141,136]
[null,"2017-01-09",338,334]
[null,"2017-01-10",257,255]
[null,"2017-01-11",236,232]
[null,"2017-01-12",321,311]
[null,"2017-01-13",455,421]
[null,"2017-01-14",167,166]
[null,"2017-01-15",96,95]
[null,"2017-01-16",361,339]
[null,"2017-01-17",690,504]
[null,"2017-01-18",386,372]
[null,"2017-01-19",2329,595]
[null,"2017-01-20",2298,1628]
[null,"2017-01-21",377,308]
[null,"2017-01-22",190,171]
[null,"2017-01-23",427,404]
[null,"2017-01-24",384,373]
[null,"2017-01-25",282,266]
[null,"2017-01-26",123,118]
[null,"2017-01-27",257,245]
[null,"2017-01-28",150,136]
[null,"2017-01-29",151,142]
[null,"2017-01-30",396,385]
[null,"2017-01-31",265,257]
[null,"2017-02-01",257,257]
[null,"2017-02-02",266,256]
[null,"2017-02-03",235,226]
[null,"2017-02-04",184,179]
[null,"2017-02-05",319,235]
[null,"2017-02-06",470,441]
[null,"2017-02-07",396,379]
[null,"2017-02-08",2569,531]
[null,"2017-02-09",787,578]
[null,"2017-02-10",488,380]
[null,"2017-02-11",344,304]
[null,"2017-02-12",178,170]
[null,"2017-02-13",387,323]
[null,"2017-02-14",302,296]
[null,"2017-02-15",377,358]
[null,"2017-02-16",401,370]
[null,"2017-02-17",310,282]
[null,"2017-02-18",259,232]
[null,"2017-02-19",138,117]
[null,"2017-02-20",270,265]
[null,"2017-02-21",276,238]
[null,"2017-02-22",340,318]
[null,"2017-02-23",254,246]
[null,"2017-02-24",261,252]
[null,"2017-02-25",119,114]
[null,"2017-02-26",87,74]
[null,"2017-02-27",271,251]
[null,"2017-02-28",638,510]
[null,"2017-03-01",382,374]
[null,"2017-03-02",430,400]
[null,"2017-03-03",312,281]
[null,"2017-03-04",219,172]
[null,"2017-03-05",104,103]
[null,"2017-03-06",267,253]
[null,"2017-03-07",277,265]
[null,"2017-03-08",287,278]
[null,"2017-03-09",258,237]
[null,"2017-03-10",299,272]
[null,"2017-03-11",142,121]
[null,"2017-03-12",333,276]
[null,{"$f":"B1359+1","v":"2017-03-13"},126,118]
[null,"2017-03-14",333,329]
[null,"2017-03-15",216,201]
[null,"2017-03-16",278,270]
[null,"2017-03-17",227,207]
[null,"2017-03-18",193,165]
[null,"2017-03-19",162,149]
[null,"2017-03-20",350,301]
[null,"2017-03-21",392,338]
[null,"2017-03-22",199,180]
[null,"2017-03-23",204,198]
[null,"2017-03-24",276,262]
[null,"2017-03-25",172,151]
[null,"2017-03-26",110,106]
[null,"2017-03-27",296,271]
[null,"2017-03-28",211,191]
[null,"2017-03-29",455,409]
[null,"2017-03-30",302,272]
[null,"2017-03-31",236,225]
[null,"2017-04-01",197,166]
[null,"2017-04-02",90,89]
[null,"2017-04-03",285,251]
[null,"2017-04-04",229,223]
[null,"2017-04-05",261,241]
[null,"2017-04-06",195,169]
[null,"2017-04-07",224,188]
[null,"2017-04-08",150,127]
[null,"2017-04-09",400,275]
[null,"2017-04-10",246,197]
[null,"2017-04-11",263,222]
[null,"2017-04-12",227,216]
[null,"2017-04-13",191,172]
[null,"2017-04-14",147,119]
[null,"2017-04-15",79,78]
[null,"2017-04-16",210,141]
[null,"2017-04-17",100,96]
[null,"2017-04-18",240,206]
[null,"2017-04-19",300,268]
[null,"2017-04-20",516,376]
[null,"2017-04-21",324,259]
[null,"2017-04-22",137,104]
[null,"2017-04-23",81,81]
[null,"2017-04-24",249,223]
[null,"2017-04-25",119,113]
[null,"2017-04-26",413,346]
[null,"2017-04-27",282,246]
[null,"2017-04-28",296,239]
[null,"2017-04-29",155,146]
[null,"2017-04-30",140,120]
[null,"2017-05-01",279,253]
[null,"2017-05-02",229,207]
[null,"2017-05-03",229,198]
[null,"2017-05-04",218,191]
[null,"2017-05-05",220,188]
[null,"2017-05-06",191,180]
[null,"2017-05-07",151,148]
[null,"2017-05-08",266,237]
[null,"2017-05-09",350,270]
[null,"2017-05-10",321,280]
[null,"2017-05-11",270,230]
[null,"2017-05-12",206,168]
[null,"2017-05-13",122,111]
[null,"2017-05-14",77,73]
[null,"2017-05-15",225,186]
[null,{"$f":"B1423+1","v":"2017-05-16"},257,222]
[null,"2017-05-17",248,224]
[null,"2017-05-18",214,189]
[null,"2017-05-19",198,175]
[null,"2017-05-20",91,83]
[null,"2017-05-21",89,86]
[null,"2017-05-22",227,202]
[null,"2017-05-23",296,265]
[null,"2017-05-24",357,294]
[null,"2017-05-25",248,185]
[null,"2017-05-26",309,246]
[null,"2017-05-27",194,163]
[null,"2017-05-28",163,146]
[null,"2017-05-29",335,224]
[null,"2017-05-30",269,208]
[null,"2017-05-31",225,204]
[null,"2017-06-01",277,235]
[null,"2017-06-02",275,197]
[null,"2017-06-03",176,150]
[null,"2017-06-04",103,95]
[null,"2017-06-05",216,181]
[null,"2017-06-06",251,190]
[null,"2017-06-07",323,210]
[null,"2017-06-08",305,219]
[null,"2017-06-09",208,145]
[null,"2017-06-10",140,73]
[null,"2017-06-11",125,116]
[null,"2017-06-12",94,80]
[null,"2017-06-13",223,171]
[null,"2017-06-14",264,206]
[null,"2017-06-15",271,222]
[null,"2017-06-16",221,139]
[null,"2017-06-17",134,123]
[null,"2017-06-18",276,117]
[null,"2017-06-19",252,221]
[null,"2017-06-20",208,156]
[null,"2017-06-21",212,173]
[null,"2017-06-22",210,176]
[null,"2017-06-23",208,167]
[null,"2017-06-24",157,129]
[null,"2017-06-25",93,89]
[null,"2017-06-26",302,239]
[null,"2017-06-27",235,168]
[null,"2017-06-28",253,206]
[null,"2017-06-29",268,206]
[null,"2017-06-30",280,178]
[null,"2017-07-01",194,146]
[null,"2017-07-02",81,66]
[null,"2017-07-03",385,312]
[null,"2017-07-04",324,251]
[null,"2017-07-05",370,308]
[null,"2017-07-06",289,208]
[null,"2017-07-07",286,226]
[null,"2017-07-08",215,141]
[null,"2017-07-09",101,85]
[null,"2017-07-10",292,241]
[null,"2017-07-11",309,237]
[null,"2017-07-12",243,213]
[null,"2017-07-13",233,199]
[null,"2017-07-14",304,225]
[null,"2017-07-15",245,175]
[null,"2017-07-16",127,110]
[null,"2017-07-17",359,276]
[null,"2017-07-18",411,272]
[null,{"$f":"B1487+1","v":"2017-07-19"},316,261]
[null,"2017-07-20",252,216]
[null,"2017-07-21",277,230]
[null,"2017-07-22",183,147]
[null,"2017-07-23",121,112]
[null,"2017-07-24",261,230]
[null,"2017-07-25",213,120]
[null,"2017-07-26",213,149]
[null,"2017-07-27",304,214]
[null,"2017-07-28",228,191]
[null,"2017-07-29",354,212]
[null,"2017-07-30",136,120]
[null,"2017-07-31",351,269]
[null,"2017-08-01",242,176]
[null,"2017-08-02",247,161]
[null,"2017-08-03",306,206]
[null,"2017-08-04",770,241]
[null,"2017-08-05",249,197]
[null,"2017-08-06",406,290]
[null,"2017-08-07",834,395]
[null,"2017-08-08",272,223]
[null,"2017-08-09",272,189]
[null,"2017-08-10",317,226]
[null,"2017-08-11",225,158]
[null,"2017-08-12",112,83]
[null,"2017-08-13",130,103]
[null,"2017-08-14",232,160]
[null,"2017-08-15",330,203]
[null,"2017-08-16",226,168]
[null,"2017-08-17",453,312]
[null,"2017-08-18",333,207]
[null,"2017-08-19",213,190]
[null,"2017-08-20",237,198]
[null,"2017-08-21",363,263]
[null,"2017-08-22",283,180]
[null,"2017-08-23",294,225]
[null,"2017-08-24",276,250]
[null,"2017-08-25",240,183]
[null,"2017-08-26",155,130]
[null,"2017-08-27",159,134]
[null,"2017-08-28",346,213]
[null,"2017-08-29",247,185]
[null,"2017-08-30",259,171]
[null,"2017-08-31",195,160]
[null,"2017-09-01",223,181]
[null,"2017-09-02",234,196]
[null,"2017-09-03",338,276]
[null,"2017-09-04",688,426]
[null,"2017-09-05",508,282]
[null,"2017-09-06",279,172]
[null,"2017-09-07",271,190]
[null,"2017-09-08",210,122]
[null,"2017-09-09",181,153]
[null,"2017-09-10",110,94]
[null,"2017-09-11",287,196]
[null,"2017-09-12",260,174]
[null,"2017-09-13",367,225]
[null,"2017-09-14",220,177]
[null,"2017-09-15",329,185]
[null,"2017-09-16",154,142]
[null,"2017-09-17",77,68]
[null,"2017-09-18",361,266]
[null,"2017-09-19",287,266]
[null,"2017-09-20",305,218]
[null,{"$f":"B1551+1","v":"2017-09-21"},207,175]
[null,"2017-09-22",219,170]
[null,"2017-09-23",228,177]
[null,"2017-09-24",158,139]
[null,"2017-09-25",226,167]
[null,"2017-09-26",225,151]
[null,"2017-09-27",197,186]
[null,"2017-09-28",202,158]
[null,"2017-09-29",256,227]
[null,"2017-09-30",201,195]
[null,"2017-10-01",83,82]
[null,"2017-10-02",55,45]
[null,"2017-10-03",255,179]
[null,"2017-10-04",253,199]
[null,"2017-10-05",180,142]
[null,"2017-10-06",241,165]
[null,"2017-10-07",196,152]
[null,"2017-10-08",65,58]
[null,"2017-10-09",212,145]
[null,"2017-10-10",269,213]
[null,"2017-10-11",337,288]
[null,"2017-10-12",204,175]
[null,"2017-10-13",228,213]
[null,"2017-10-14",117,89]
[null,"2017-10-15",91,87]
[null,"2017-10-16",314,289]
[null,"2017-10-17",304,243]
[null,"2017-10-18",342,302]
[null,"2017-10-19",186,154]
[null,"2017-10-20",196,179]
[null,"2017-10-21",248,211]
[null,"2017-10-22",117,112]
[null,"2017-10-23",294,256]
[null,"2017-10-24",259,220]
[null,"2017-10-25",556,475]
[null,"2017-10-26",282,261]
[null,"2017-10-27",316,275]
[null,"2017-10-28",198,158]
[null,"2017-10-29",460,280]
[null,"2017-10-30",522,373]
[null,"2017-10-31",252,225]
[null,"2017-11-01",308,263]
[null,"2017-11-02",202,176]
[null,"2017-11-03",210,191]
[null,"2017-11-04",195,178]
[null,"2017-11-05",206,181]
[null,"2017-11-06",308,283]
[null,"2017-11-07",290,279]
[null,"2017-11-08",216,190]
[null,"2017-11-09",216,213]
[null,"2017-11-10",385,319]
[null,"2017-11-11",130,110]
[null,"2017-11-12",95,92]
[null,"2017-11-13",332,294]
[null,"2017-11-14",674,347]
[null,"2017-11-15",701,583]
[null,"2017-11-16",297,203]
[null,"2017-11-17",320,291]
[null,"2017-11-18",152,114]
[null,"2017-11-19",148,111]
[null,"2017-11-20",949,675]
[null,"2017-11-21",392,348]
[null,"2017-11-22",462,405]
[null,"2017-11-23",686,556]
[null,{"$f":"B1615+1","v":"2017-11-24"},325,294]
[null,"2017-11-25",177,161]
[null,"2017-11-26",106,88]
[null,"2017-11-27",253,220]
[null,"2017-11-28",332,314]
[null,"2017-11-29",541,424]
[null,"2017-11-30",887,500]
[null,"2017-12-01",700,548]
[null,"2017-12-02",153,134]
[null,"2017-12-03",94,85]
[null,"2017-12-04",238,214]
[null,"2017-12-05",295,231]
[null,"2017-12-06",226,202]
[null,"2017-12-07",293,243]
[null,"2017-12-08",243,201]
[null,"2017-12-09",182,138]
[null,"2017-12-10",130,125]
[null,"2017-12-11",279,226]
[null,"2017-12-12",316,275]
[null,"2017-12-13",311,258]
[null,"2017-12-14",302,245]
[null,"2017-12-15",286,260]
[null,"2017-12-16",183,158]
[null,"2017-12-17",100,97]
[null,"2017-12-18",429,314]
[null,"2017-12-19",398,294]
[null,"2017-12-20",267,216]
[null,"2017-12-21",202,179]
[null,"2017-12-22",156,141]
[null,"2017-12-23",215,141]
[null,"2017-12-24",213,181]
[null,"2017-12-25",85,83]
[null,"2017-12-26",88,87]
[null,"2017-12-27",297,242]
[null,"2017-12-28",213,205]
[null,"2017-12-29",166,157]
[null,"2017-12-30",92,89]
[null,"2017-12-31",101,98]
[null,"2018-01-01",92,91]
[null,"2018-01-02",212,197]
[null,"2018-01-03",238,224]
[null,"2018-01-04",268,250]
[null,"2018-01-05",401,313]
[null,"2018-01-06",274,205]
[null,"2018-01-07",104,101]
[null,"2018-01-08",252,221]
[null,"2018-01-09",226,212]
[null,"2018-01-10",226,215]
[null,"2018-01-11",256,222]
[null,"2018-01-12",326,299]
[null,"2018-01-13",172,137]
[null,"2018-01-14",182,161]
[null,"2018-01-15",385,327]
[null,"2018-01-16",255,219]
[null,"2018-01-17",361,294]
[null,"2018-01-18",615,443]
[null,"2018-01-19",655,417]
[null,"2018-01-20",302,264]
[null,"2018-01-21",281,246]
[null,"2018-01-22",551,399]
[null,"2018-01-23",319,261]
[null,"2018-01-24",318,281]
[null,"2018-01-25",218,195]
[null,"2018-01-26",233,196]
[null,{"$f":"B1679+1","v":"2018-01-27"},218,154]
[null,"2018-01-28",247,153]
[null,"2018-01-29",369,317]
[null,"2018-01-30",339,250]
[null,"2018-01-31",268,254]
[null,"2018-02-01",333,246]
[null,"2018-02-02",312,258]
[null,"2018-02-03",215,164]
[null,"2018-02-04",108,100]
[null,"2018-02-05",368,321]
[null,"2018-02-06",326,301]
[null,"2018-02-07",342,277]
[null,"2018-02-08",302,220]
[null,"2018-02-09",428,334]
[null,"2018-02-10",195,149]
[null,"2018-02-11",107,94]
[null,"2018-02-12",311,281]
[null,"2018-02-13",296,270]
[null,"2018-02-14",379,343]
[null,"2018-02-15",284,245]
[null,"2018-02-16",235,211]
[null,"2018-02-17",161,134]
[null,"2018-02-18",292,259]
[null,"2018-02-19",311,281]
[null,"2018-02-20",293,259]
[null,"2018-02-21",334,293]
[null,"2018-02-22",468,330]
[null,"2018-02-23",594,494]
[null,"2018-02-24",259,192]
[null,"2018-02-25",95,85]
[null,"2018-02-26",304,272]
[null,"2018-02-27",302,263]
[null,"2018-02-28",258,235]
[null,"2018-03-01",243,204]
[null,"2018-03-02",273,237]
[null,"2018-03-03",209,191]
[null,"2018-03-04",111,103]
[null,"2018-03-05",257,208]
[null,"2018-03-06",222,181]
[null,"2018-03-07",325,267]
[null,"2018-03-08",290,273]
[null,"2018-03-09",340,254]
[null,"2018-03-10",250,159]
[null,"2018-03-11",130,121]
[null,"2018-03-12",62,62]
[null,"2018-03-13",257,189]
[null,"2018-03-14",318,261]
[null,"2018-03-15",254,203]
[null,"2018-03-16",293,248]
[null,"2018-03-17",231,203]
[null,"2018-03-18",238,164]
[null,"2018-03-19",280,230]
[null,"2018-03-20",364,287]
[null,"2018-03-21",220,198]
[null,"2018-03-22",219,167]
[null,"2018-03-23",256,210]
[null,"2018-03-24",233,172]
[null,"2018-03-25",263,192]
[null,"2018-03-26",312,257]
[null,"2018-03-27",351,263]
[null,"2018-03-28",256,187]
[null,"2018-03-29",257,199]
[null,"2018-03-30",151,149]
[null,"2018-03-31",68,65]
[null,{"$f":"B1743+1","v":"2018-04-01"},68,62]
[null,"2018-04-02",78,77]
[null,"2018-04-03",264,203]
[null,"2018-04-04",282,201]
[null,"2018-04-05",292,235]
[null,"2018-04-06",249,221]
[null,"2018-04-07",140,126]
[null,"2018-04-08",85,80]
[null,"2018-04-09",309,252]
[null,"2018-04-10",286,218]
[null,"2018-04-11",558,443]
[null,"2018-04-12",272,257]
[null,"2018-04-13",518,440]
[null,"2018-04-14",750,579]
[null,"2018-04-15",280,242]
[null,"2018-04-16",385,311]
[null,"2018-04-17",304,281]
[null,"2018-04-18",288,261]
[null,"2018-04-19",407,369]
[null,"2018-04-20",297,271]
[null,"2018-04-21",298,237]
[null,"2018-04-22",119,104]
[null,"2018-04-23",396,299]
[null,"2018-04-24",436,357]
[null,"2018-04-25",125,121]
[null,"2018-04-26",239,212]
[null,"2018-04-27",235,202]
[null,"2018-04-28",128,118]
[null,"2018-04-29",94,82]
[null,"2018-04-30",245,221]
[null,"2018-05-01",321,284]
[null,"2018-05-02",271,230]
[null,"2018-05-03",521,396]
[null,"2018-05-04",389,323]
[null,"2018-05-05",171,143]
[null,"2018-05-06",95,92]
[null,"2018-05-07",303,258]
[null,"2018-05-08",235,210]
[null,"2018-05-09",308,270]
[null,"2018-05-10",406,300]
[null,"2018-05-11",315,245]
[null,"2018-05-12",152,122]
[null,"2018-05-13",93,85]
[null,"2018-05-14",340,295]
[null,"2018-05-15",251,224]
[null,"2018-05-16",249,195]
[null,"2018-05-17",315,265]
[null,"2018-05-18",375,301]
[null,"2018-05-19",182,168]
[null,"2018-05-20",119,113]
[null,"2018-05-21",290,230]
[null,"2018-05-22",263,201]
[null,"2018-05-23",218,186]
[null,"2018-05-24",244,216]
[null,"2018-05-25",205,164]
[null,"2018-05-26",115,111]
[null,"2018-05-27",73,70]
[null,"2018-05-28",398,249]
[null,"2018-05-29",405,303]
[null,"2018-05-30",277,211]
[null,"2018-05-31",246,223]
[null,"2018-06-01",308,230]
[null,"2018-06-02",202,156]
[null,"2018-06-03",98,87]
[null,{"$f":"B1807+1","v":"2018-06-04"},312,220]
[null,"2018-06-05",277,222]
[null,"2018-06-06",288,207]
[null,"2018-06-07",241,220]
[null,"2018-06-08",291,274]
[null,"2018-06-09",177,118]
[null,"2018-06-10",81,75]
[null,"2018-06-11",172,169]
[null,"2018-06-12",352,303]
[null,"2018-06-13",307,258]
[null,"2018-06-14",548,389]
[null,"2018-06-15",497,338]
[null,"2018-06-16",254,228]
[null,"2018-06-17",157,125]
[null,"2018-06-18",338,287]
[null,"2018-06-19",353,311]
[null,"2018-06-20",292,274]
[null,"2018-06-21",213,195]
[null,"2018-06-22",273,254]
[null,"2018-06-23",236,141]
[null,"2018-06-24",154,145]
[null,"2018-06-25",427,350]
[null,"2018-06-26",357,280]
[null,"2018-06-27",420,340]
[null,"2018-06-28",368,311]
[null,"2018-06-29",285,266]
[null,"2018-06-30",185,144]

{"sheet":"6.2 Reliability & Cust serv","index":31,"n_rows":71,"n_cols":9,"rows_kept":71,"cut":false,"hidden":false,"merged":[[28,4,28,8],[40,4,40,8],[66,4,66,8],[24,1,24,3],[36,1,36,3],[48,1,48,3],[5,1,5,7],[63,1,63,8],[51,1,51,8],[54,2,54,8],[12,1,12,7],[13,1,13,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[7,1,7,7],[16,4,16,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,"This regulatory template requires the input of performance Historicals and proposed targets for the forthcoming regulatory control period under the STPIS."]
[null,{"$f":"CONCATENATE(\"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"\"whole network (system)\"\" cell. \",dms_TradingName,\" must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition.\")","v":"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"whole network (system)\" cell. SA Power Networks must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" should insert \"\"n/a\"\" against parameters which do not apply to it. Do not delete inapplicable fields.\")","v":"SA Power Networks should insert \"n/a\" against parameters which do not apply to it. Do not delete inapplicable fields."}]
[null,{"$f":"CONCATENATE(\"If parts of this template are unsuitable to record any of the requested information \",dms_TradingName,\" must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column.\")","v":"If parts of this template are unsuitable to record any of the requested information SA Power Networks must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers \"&\"and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. \"&\"Table 6.2.3 is not compulsory - those businesses who want to \"&\" include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information \"&\"necessary to establish the MAIFI targets, including the estimated performance for \",CRCP_y4)","v":"SA Power Networks must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. Table 6.2.3 is not compulsory - those businesses who want to  include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information necessary to establish the MAIFI targets, including the estimated performance for 2018-19"}]
[null,"Definitions of parameters under the AER's STPIS apply. Where exclusions apply, data provided below must exclude all events outlined under clause 3.3 of the AER's STPIS."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,21,21,21,21,21]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,109,109,109,109,109]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,184,184,184,184,184]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,268,268,268,268,268]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},null,null,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,1,1,1,1,1]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1,1,1,1,1]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},null,null,2,2,2,2,2]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""},{"$f":"IFERROR(#REF!-#REF!,\"\")","v":""}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E44:E48)","v":0},{"$f":"SUM(F44:F48)","v":0},{"$f":"SUM(G44:G48)","v":0},{"$f":"SUM(H44:H48)","v":0},{"$f":"SUM(I44:I48)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},5194,5211,5228,5242,5253,5264,5276]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},629044,637621,646219,653521,659380,665218,671019]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},127072,128258,129441,130443,131243,132038,132827]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},143412,144403,145391,146225,146890,147549,148202]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C57:C61)","v":904722},915493,926279,935431,942766,950069,957324]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"}]
[null,"Number of calls received",null,null,119910,119910,119910,119910,119910]
[null,"Number of calls answered within 30 seconds",null,null,90898,90898,90898,90898,90898]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E70/E69),\"\")","v":0.75805187223751147},0.75805187223751147,0.75805187223751147,0.75805187223751147,0.75805187223751147]

{"sheet":"7.1  Policies and Procedures","index":32,"n_rows":219,"n_cols":5,"rows_kept":219,"cut":false,"hidden":false,"merged":[[6,1,6,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"Instructions"]
[null,"List and provide a brief description of key internal plans, policies, procedures or strategies that are used to plan and conduct day to day operations and that have been relied upon in the development of the regulatory proposal. Identify any internal plans, policies, procedures and strategies that have changed in the current regulatory control period or that are expected to change before the next regulatory control period where the change has been identified as a step change."]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"SA Power Networks Corporate Strategic Plan 2019 - 2023","Represents our view of internal and external business environments, corporate objectives and strategic directions for the next 5 years","Balanced corporate directions that set the tone and priorities of almost all aspects of our Regulatory Proposal. ","No"]
[null,"Human Relations Policy\n","SA Power Networks will endeavour to be recognised as an employer of choice with a reputation for very high ethical standards and professionalism. SA Power Networks recognises that committed employees are key stakeholders in the achievement of its Strategic Intent.  SA Power Networks’ employees should perform their roles in a professional, courteous and ethical manner which reflects the values that underpin SA Power Networks’ Ethics Policy.","How we achieve our business plans.  ","No"]
[null,"Customer Service Policy","SA Power Networks is committed to providing our customers with value for money services which are targeted to their needs and expectations and delivered in a way which reinforces their vital importance to our business.\n","How we achieve our business plans.  ","No"]
[null,"Governance framework"]
[null,"Corporate Governance Manual","The Corporate Governance Manual explains the Board approved Corporate Governance Model and details the Policies and Directives that emanate from the Model. The Policies and Directives provide approved direction to SA Power Networks’ managers, employees and directors in the manner in which we must conduct ourselves in our business operations. Compliance with the Policies and Directives is mandatory","Corporate governance applies to all aspects of the day to day operations and set the tone of our Regulatory Proposal. ","No"]
[null,"Risk Management Policy","SA Power Networks will apply a risk management approach to all business activities in order to ensure that the organisation maximises opportunities while not exposing the business to unacceptable levels of risk. ","How we achieve our business plans.  ","No"]
[null,"Compliance Policy","SA Power Networks will conduct its business activities in compliance with all relevant legal, regulatory and contractual obligations and requirements of relevant standards and internal policies (including directives, procedures and instructions).","How we achieve our business plans. ","No"]
[null,"Environmental Policy","\nEnsures that environmental considerations are incorporated into all SA Power Networks’ business activities as a fundamental part of sound management practice. \n","How we achieve our business plans. ","No"]
[null,"Risk Management Framework","This document outlines SA Power Networks Framework for the management of risk across the business. It is closely aligned to the requirements of AS/NZS ISO 31000:2009 Risk Management – Principles and Guidelines. This document is designed to outline the risk management activities of SA Power Networks as they relate to the principles and guidelines described in AS/NZS ISO 31000:2009.","Supports Risk Management Policy. ","No"]
[null,"Expenditure Governance Procedures","This document describes SA Power Networks’ robust planning and governance processes employed in its business planning and annual budget cycles. ","Attachment 5, Attachment 6","Yes"]
[null,"Negotiating Framework ","This document specifies the Negotiated Distribution Service Criteria, information disclosure process, and identifies the timetable that will apply to each classification of negotiated distribution service. ","Attachment 15","No"]
[null,"Ring Fencing Corporate Compliance Directive","This Directive contains information relating to the responsibilities of all SA Power Networks (SAPN) staff and contractors and all Enerven staff, and other third parties to appropriately follow the AER Ring-fencing guideline.","How we achieve our business plans","No"]
[null,"Ring Fencing Staff Movement Directive","This directive focuses on movement of staff from the regulated parts of the SAPN business to the areas of the business providing contestable electricity services, ie Enerven.","How we achieve our business plans","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Accounting practices and guidelines ","Sets out the required accounting treatments for items in the Income Statement, the Balance Sheet, the Statement of Changes in Equity (or Statement of Recognised Income and Expense) and the Cash Flow Statement","Supporting Document 18.21","Yes"]
[null,"Financial Management Policy","Obligations in regard to the following financial management areas: \n• business plans and budgets; \n• accounts and financial statements; \n• taxation returns; and \n• management reporting. ","How we achieve our business plans. ","No"]
[null,"Cost Allocation Method","This AER approved document describes the principles and policies for allocating costs within the categories of distribution services that SA Power Networks provides.","See AER website","No"]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy","SA Power Networks will manage its assets to satisfy customer service needs; meet Licence and Regulatory obligations; to provide a safe environment for employees, contractors and the community; and to deliver optimal returns to shareholders. \nAsset management includes risk management for the whole of life consideration of procurement, operation, maintenance, condition and performance monitoring, disposal or replacement and legal compliance. It includes assets owned or leased and those owned by clients if part of an asset management contract. It also includes long term planning and financial links, provision of assets for current and future services. ","Supporting Document 5.6","No"]
[null,"Connections Policy",null,"Attachment 16","No"]
[null,"Asset Management Strategies"]
[null,"Strategic Asset Management Plan (SAMP)","The Plan outlines SA Power Networks strategic direction and priorities for electricity distribution assets. ","Supporting Document 5.7","Yes"]
[null,"Future Network Strategy",null,"Supporting Document 5.17","Yes"]
[]
[]
[null,"Asset Management Plans"]
[null,"Powerline Asset Management Plan (PAMP)","The Plan outlines SA Power Networks approach to managing the electricity distribution assets over the planning period 2018 - 2030","Supporting Document 5.8","Yes"]
[null,"Reliability and Resiliance Performance Management","The document outlines SA Power Networks approach to reliability and resiliance of the network ","Supporting Document 5.25","No"]
[null,"Metering Asset Management Plan","The Plan outlines SA Power Networks approach to managing metering assets","Supporting Document 14.1","No"]
[null,"Public Lighting Asset Management Plan","The Plan outlines SA Power Networks approach to managing pubic lighting assets","Supporting Document 14.5","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Expenditure Forecasting Methodology","This document describes the methodology which SA Power Networks is proposing to use when developing its operating and capital expenditure forecasts for the 2015-2020 regulatory control period.","How we achieve our business plans. ","No"]
[null,"Capital Monitoring and Post Implementation Review Procedures","These procedures detail the principles and practices which govern SA Power Networks’ monitoring and Post Implementation Review (‘PIR’) of capital expenditure projects.\n","How we achieve our business plans. ","No"]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Future Operating Model","The SA Power Networks Future Operating Model (FOM) represents a ‘living document’ vision that offers long-term directional insights into our most likely future development paths. These insights will help to guide our staff and decision makers in the coming years.\n","Supporting Document 18.5","No"]
[null,"Customer Strategy ","The SA Power Networks Customer Service Strategy provides our customer service vision. This strategy outlines SA Power Networks customer service vision and initiatives. It provides an overview of key customer segments, their current and future needs, and outlines our roadmap in response to this which we expect to deliver improved customer satisfaction. ","How we achieve our business plans. ","No"]
[null,"SA Power Network’s Connection Policy","The SA Power Networks Connection Policy sets out the circumstances in which it may require a retail customer or real estate developer to pay a connection charge, for the provision of a connection service.\n\n","Attachment 16","No"]
[null,"Environment policy","SA Power Networks is committed to conducting its electricity distribution operations and business activities in a manner that prevents or minimises pollution and other adverse impacts on the environment.","How we achieve our business plans. ","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Information technology policies or strategies"]
[null,"IT Investment Plan 2020-25","The IT Investment Plan provides the overview, rationalse and portfolio summary of the proposed IT expenditure for the 2020-25 RCP and supports our regulatory proposal","Attachment 5 Capex, Attachment 6 Opex, relating to the IT sections\nSupporting Document 5.32","Yes"]
[null,"Digital Strategy","The Digital Strategy outlines the important role that digital capabilities will play in equiping our business for the future world","Is discussed and outlined in Supporting Document 5.32","No"]
[null,"IT Asset Management Plan 2019-2023","The IT Asset Management Plan provides alignment with SA Power Networks' Asset Management Policy to enable the delivery of essential energy services; Describe how we manage our IT Assets to deliver the most value to our customers and stakeholders; and provide a framework for ensuring IT Assets are prudently managed throughout the entire asset lifecycle. ","Supporting document 5.34","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Distribution Annual Planning Report","SA Power Networks produces each year a Distribution Annual Planning Report (DAPR) in accordance with the requirements of Section 5.13.2 of the National Electricity Rules (NER).  The information contained within the DAPR complies with the requirements of Schedule 5.8 of the NER ","Available from our website www.sapowernetworks.com.au","No"]
[null,"Future Network Strategy","This strategy sets out SA Power Networks' six core strategies to adapt our network business into the future in response to increased distributed energy resources on the network","Supporting Document 5.17","No"]
[]
[null,"Self insurance guidelines or policy"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Land and easement acquisition polices"]
[null,"Property Services Capital Expenditure 2020-2025","The document describes SA Power Networks' property strategyt, asset management plan and expenditure program for 2020-25 to meet our strategic objectives and operational requirements. Property associated with substations and line easements is excluded from this document","Supporting Document 5.31","No"]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"Refer to Asset Management Plans",null,null,"No"]
[null,"Bushfire Risk Management Policy & Manuals","This manual details the policies and procedures which govern SA Power Networks bushfire risk management practices. It is a self contained document except where it specifically refers to other related documents. It supersedes all previous bushfire related letters and documents including all previous Bushfire Risk Management Manuals","Attachment 5 Capital Expenditure","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"<insert relevant policy, plan, strategy etc>"]

{"sheet":"7.2 Contingent projects","index":33,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2020-21 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2020-21"}]
[null,"Electricity System Security ",79200000,"Notification from AEMO",802271443,{"$f":"+E8*0.05","v":40113572.149999999}]
[null,null,null,null,{"$f":"+$E$8","v":802271443},{"$f":"+E9*0.05","v":40113572.149999999}]
[null,null,null,null,{"$f":"+$E$8","v":802271443},40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]
[null,null,null,null,802271443,40113572.149999999]

{"sheet":"7.4 Shared Assets","index":34,"n_rows":37,"n_cols":19,"rows_kept":37,"cut":false,"hidden":false,"merged":[[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8],[6,11,6,18],[32,2,32,8],[6,1,7,1],[6,2,7,2],[6,3,6,10],[25,1,26,1],[25,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service","Shared asset unregulated revenue  ($0's, nominal)",null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Shared asset unregulated revenue  ($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  ($0's, real June 2020)"}]
[null,null,null,{"$f":"PRCP_y1","v":"2010-11"},{"$f":"PRCP_y2","v":"2011-12"},{"$f":"PRCP_y3","v":"2012-13"},{"$f":"PRCP_y4","v":"2013-14"},{"$f":"PRCP_y5","v":"2014-15"},{"$f":"CRCP_y1","v":"2015-16"},{"$f":"CRCP_y2","v":"2016-17"},{"$f":"CRCP_y3","v":"2017-18"},{"$f":"CRCP_y4","v":"2018-19"},{"$f":"CRCP_y5","v":"2019-20"},{"$f":"FRCP_y1","v":"2020-21"},{"$f":"FRCP_y2","v":"2021-22"},{"$f":"FRCP_y3","v":"2022-23"},{"$f":"FRCP_y4","v":"2023-24"},{"$f":"FRCP_y5","v":"2024-25"},{"$f":"CONCATENATE(\"Total \n\",CRCP_y5, \" to \", dms_MultiYear_FinalYear_Result)","v":"Total \n2019-20 to 2024-25"}]
[null,"Pole Rental - Non NBN","Rental of overhead distribution assets for telecommunication services (non NBN)",1409633,1455815,1389814,1422823,1527638,1921728,1449248,1098196,null,null,null,null,null,null,null,{"$f":"SUM(M9:R9)","v":0}]
[null,"Pole Rental - NBN","Rental of overhead and underground distribution assets for telecommunication services - NBN.",0,0,0,83388,369083,565303,1052245,2045810,null,null,null,null,null,null,null,{"$f":"SUM(M10:R10)","v":0}]
[null,"Duct Rental","Rental of underground distribution assets for telecommunication services (non NBN).",327485,323246,332493,330174,334858,342356,347035,352618,372130,372131,372131,372131,372131,372130,372130,2232784]
[null,"Facilities Access","Facilities Access Agreements for access to other assets - e.g. towers, base stations etc",630989,928467,549424,699186,960109,1001077,988671,944338,996594,996594,996594,996594,996594,996594,996594,5979564]
[null,"Property Rentals","Rental fees received for lease of properties. ",193318,200806,199056,180823,168174,199704,213775,325627,343646,343646,343647,343646,343646,343647,343646,2061878]
[null,"HV Test Equipment Hire","Hire of high voltage test equipment by electrical contractors for compliance testing for new subdivisions. Ceased in December 2015, as not cost effective to continue to provide this service.",13360,18460,12837,11936,10800,3660,0,0,0,0,0,0,0,0,0,0]
[null,"Managed Communications","Lease of SA Power Networks' communications fibre network to Nextgen for delivery of data services to external organisations. Ceased in August 2012.",237180,214158,37808,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Training - Overheads revenue only","Electrical related training programs provided to external groups, principally electrical contractors requiring accreditation to work on SA Power Networks' assets. Relates to corporate infrastructure assets e.g. property, IT. Ceases from 2020 as service will be reclassified as an Alternative Control Service.",27151,41388,39655,33409,46151,28695,35413,57718,60912,60912,0,0,0,0,0,60912]
[null,"Unregulated Services - Vehicle revenue","Unregulated construction and maintenance services provided to external groups, e.g. ElectraNet. Relates specifically to use of regulated heavy vehicles in undertaking work.",1219643,1523546,1964363,2161840,2238994,1777373,1425950,1630256,1720468,1720468,1720468,1720468,1720468,1720467,1720468,10322807]
[null,"Unregulated Services - Property/IT revenue","Unregulated construction and maintenance services provided to external groups, e.g. ElectraNet. Relates specifically to use of infrastructure assets of property and IT in undertaking work.",1932069,2259886,2253867,3020877,2705963,2662215,4229450,5992930,6324556,6324557,5144963,5144963,5144963,5144963,5144963,32049372]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[]
[null,"Pole Rental - Non NBN","100% Shared Asset"]
[null,"Pole Rental - NBN","100% Shared Asset"]
[null,"Duct Rental","100% Shared Asset"]
[null,"Facilities Access","100% Shared Asset"]
[null,"Property Rentals","100% Shared Asset"]
[null,"HV Test Equipment Hire","100% Shared Asset"]
[null,"Managed Communications","100% Shared Asset"]
[null,"Training - Overheads revenue only","100% of revenue received for overheads"]
[null,"Unregulated Services - Vehicle revenue","100% of revenue received for regulated vehicles"]
[null,"Unregulated Services - Property/IT revenue","CAM apportionment for property and IT of revenue received for overheads"]

{"sheet":"7.3 Obligations","index":35,"n_rows":301,"n_cols":6,"rows_kept":301,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"Instructions"]
[null,"Outline those obligations and requirements that have been relied upon in the development of the regulatory proposal."]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact","EE Additional Data \n(not required by the AER)"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?","Location (cut and paste location into browser)"]
[null,"LEGISLATION"]
[null,"State Government SA","Aboriginal Heritage Act 1988 (SA)","Business as usual","No"]
[null,"State Government SA","Adelaide Parklands Act 2005 SA","Capex and Opex","No"]
[null,"State Government SA","Building and Construction Industry Security of Payment Act 2009 (SA)","Business as usual","No"]
[null,"State Government SA","Building and Construction Industry Security of Payment Regulations 2011 (SA)","Business as usual","No"]
[null,"State Government SA","Building Work Contractors Act 1995 (SA)","Business as usual","No"]
[null,"State Government SA","Building Work Contractors Regulations 2011 (SA)","Business as usual","No"]
[null,"State Government SA","Business Names (Commonwealth Powers) Act 2012 SA","Business as usual","No"]
[null,"State Government SA","Children’s Protection Act 1993 (SA) ","Business as usual","No"]
[null,"State Government SA","Civil Liability Act 1936 (SA)","Business as usual","No"]
[null,"State Government SA","Civil Liability Regulations 2013 (SA)","Business as usual","No"]
[null,"State Government SA","Civil Liability Regulations 2013 SA","Business as usual","No"]
[null,"State Government SA","Construction Industry Long Service Leave Act 1987 (SA)","Opex","No"]
[null,"State Government SA","Construction Industry Training Fund Act 1993 SA","Opex","No"]
[null,"State Government SA","Dangerous Substances (Goods Transport) Regulations 2008 SA","Business as usual","No"]
[null,"State Government SA","Dangerous Substances Act 1979 SA","Business as usual","No"]
[null,"State Government SA","Dangerous Substances Regulations 2002 SA","Business as usual","No"]
[null,"State Government SA","Development Act 1993  (SA)","Capex","No"]
[null,"State Government SA","Development Regulations 2008 (SA)","Capex / Opex","No"]
[null,"State Government SA","Electricity (General) Regulations 2012 (SA)","Capex / Opex","No"]
[null,"State Government SA","Electricity (Principles of Vegetation Clearance) Regulations 2010 (SA) ","Opex","No"]
[null,"State Government SA","Electricity Act 1996 (SA)","Capex / Opex\n\nComply with and adapt to:\n- distribution licence conditions\n- changes in vegetation cleareance practices\n- report 'prescribed fires'\n- change in penalties\n- enhanced powers of Essential Services Commission of SA and the Office of the Technical Regulator","No"]
[null,"State Government SA","Electricity Corporations (Restructuring and Disposal) Act 1999 SA","Opex","No"]
[null,"State Government SA","Electricity Corporations (Restructuring and Disposal) Regulations 2012 SA","Opex","No"]
[null,"State Government SA","Emergency Management Act 2004 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Management Regulations 2009 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Services Funding (Remissions - Land) Regulations 2014 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Services Funding (Remissions - Motor Vehicles and Vessels) Regulations 2014 (SA)","Business as usual","No"]
[null,"State Government SA","Emergency Services Funding Act 1998 (SA)","Opex","No"]
[null,"State Government SA","Energy Products (Safety and Efficiency) Act 2000 SA","Business as usual","No"]
[null,"State Government SA","Energy Products (Safety and Efficiency) Regulations 2012 SA","Business as usual","No"]
[null,"State Government SA","Environment Protection Act 1993 (SA)","Capex / Opex - Environmental","No"]
[null,"State Government SA","Environment Protection Regulations 2009 (SA)","Capex / Opex - Environmental","No"]
[null,"State Government SA","Equal Opportunity Act 1984 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Act 1981 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Commission Act 2002 (SA)","Business as usual","No"]
[null,"State Government SA","Essential Services Commission Regulations 2004 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Trading Act 1987 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Trading Regulations 2010 (SA)","Business as usual","No"]
[null,"State Government SA","Fair Work (Clothing Outworker Code of Practice) Regulations 2007","Business as usual","No"]
[null,"State Government SA","Fair Work (General) Regulations 2009","Business as usual","No"]
[null,"State Government SA","Fair Work (Representation) Regulations 2009","Business as usual","No"]
[null,"State Government SA","Fair Work Act 1994 (SA)","Business as usual","No"]
[null,"State Government SA","Fences Act 1975 SA","Business as usual","No"]
[null,"State Government SA","Fences Regulations 2003 SA","Business as usual","No"]
[null,"State Government SA","Fire & Emergency Services Act 2005 (SA)","Business as usual","No"]
[null,"State Government SA","Fire & Emergency Services Regulations 2005  (SA)","Business as usual","No"]
[null,"State Government SA","Foreign Acquisitions and Takeovers (Notices) Regulations 1975 (Cth)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (Exempt Agency) Regulations 2008 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (Fees and Charges) Regulations 2003 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information (General) Regulations 2002 (SA)","Business as usual","No"]
[null,"State Government SA","Freedom of Information Act 1991 (SA)","Business as usual","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Expiation Fees) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Fees) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) (Savings, Transitional and Declaratory) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Heavy Vehicle National Law (South Australia) Act 2013  (SA)","Opex\nComply with and adapt to:\n- overarching primary duty of care \n- reasonably practicable’ defence \n- Eexcutive Officers  proactive duty to exercise due diligence\n- increase in penalties","No"]
[null,"State Government SA","Highways Act 1926 SA","Business as usual","No"]
[null,"State Government SA","Land Tax Act 1936 SA","Opex","No"]
[null,"State Government SA","Land Tax Regulations 2010 SA","Business as usual","No"]
[null,"State Government SA","Landlord and Tenant Act 1936 SA","Business as usual","No"]
[null,"State Government SA","Law of Property Act 1936 (SA)","Business as usual","No"]
[null,"State Government SA","Listening and Surveillance Devices Act 1972 (SA)","Business as usual","No"]
[null,"State Government SA","Listening and Surveillance Devices Regulations 2003 (SA)","Business as usual","No"]
[null,"State Government SA","Mines and Works Inspection Act 1920 (SA)","Business as usual","No"]
[null,"State Government SA","Mines and Works Inspection Regulations 1998 (SA)","Opex","No"]
[null,"State Government SA","Misrepresentation Act 1972 SA","Business as usual","No"]
[null,"State Government SA","Motor Vehicles Act 1959 SA","Opex","No"]
[null,"State Government SA","Motor Vehicles Regulations 2010 SA","Opex","No"]
[null,"State Government SA","National Electricity (South Australia) Act 1996 (SA) ","Capex / Opex","No"]
[null,"State Government SA","National Electricity (South Australia) Regulations 1998 (SA)","Opex","No"]
[null,"State Government SA","National Energy Retail Law  (Local Provisions) Regulations 2013 (SA)","Capex / Opex","No"]
[null,"State Government SA","National Energy Retail Law (South Australia) Act 2011 (SA)","Capex / Opex","No"]
[null,"State Government SA","National Energy Retail Regulations 2012 (SA)","Business as usual","No"]
[null,"State Government SA","Native Title (South Australia) Act 1994 (SA)","Opex","No"]
[null,"State Government SA","Native Title (South Australia) Regulations 2001 (SA)","Opex","No"]
[null,"State Government SA","Native Vegetation Act 1991 SA","Capex / Opex","No"]
[null,"State Government SA","Native Vegetation Regulations 2017 (SA)","Capex / Opex","No"]
[null,"State Government SA","Partnership Act 1981 SA","Business as usual","No"]
[null,"State Government SA","Payroll Tax Act 2009 (SA)","Opex","No"]
[null,"State Government SA","Payroll Tax Act 2009 SA","Opex","No"]
[null,"State Government SA","Plumbers, Gas Fitters and Electricians Act 1995 (SA)","Opex","No"]
[null,"State Government SA","Plumbers, Gas Fitters and Electricians Regulations 2010 (SA)","Opex","No"]
[null,"State Government SA","Race Discrimination Commissioner (Cth) (Allowances) Regulations 1987 ","Business as usual","No"]
[null,"State Government SA","Racial Vilification Act 1996 (SA)","Business as usual","No"]
[null,"State Government SA","Real Property Act 1886 (SA)","Business as usual","No"]
[null,"State Government SA","Real Property Regulations 2009 (SA)","Opex","No"]
[null,"State Government SA","Retail and Commercial Leases Act 1995 SA","Business as usual","No"]
[null,"State Government SA","Road Traffic (Light Vehicle Mass and Loading Requirements) Regulations 2013 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic (Miscellaneous) Regulations 1999 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic (Oversize or Overmass Vehicle Exemptions) Regulations 1999 (SA)","Opex","No"]
[null,"State Government SA","Road Traffic Act 1961 (SA)","Capex / Opex\nComply with and adapt to:\n - requirement to obtain a permit from Comissioner of Highways on main roads\n- increased penalties","No"]
[null,"State Government SA","Sale of Goods Act 1895 SA","Business as usual","No"]
[null,"State Government SA","Stamp Duties Act 1923 SA","Opex","No"]
[null,"State Government SA","State Records Act 1997 (SA)","Business as usual","No"]
[null,"State Government SA","State Records Regulations 2013 (SA)","Business as usual","No"]
[null,"State Government SA","Surveillance Devices Act 2016 (SA) ","Business as usual","No"]
[null,"State Government SA","Telecommunications (Interception) Act 2012 (SA)","Opex","No"]
[null,"State Government SA","Training and Skills Development Act 2008 SA","Business as usual","No"]
[null,"State Government SA","Work Health & Safety Act 2012  (SA)","Capex / Opex","No"]
[null,"State Government SA","Work Health & Safety Regulations 2012 (SA)","Capex / Opex","No"]
[null,"State Government SA","Workers Rehabilitation & Compensation Act 1986 (SA)","Opex","No"]
[null,"State Government SA","Workers Rehabilitation and Compensation Regulations 2010 (SA)","Opex","No"]
[null,"Commonwealth Government","A New Tax System (Goods and Services Tax) Act 1999  (Cth)","Capex / Opex","No"]
[null,"Commonwealth Government","A New Tax System (Goods and Services Tax) Regulations 1999 (Cth)","Capex / Opex","No"]
[null,"Commonwealth Government","Aboriginal and Torres Strait Islander Heritage Protection Act 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Aboriginal and Torres Strait Islander Heritage Protection Regulations 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Affirmative Action (Equal Employment Opportunity for Women) Regulations 1986 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Age Discrimination Act 2004 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Human Rights Commission Act 1986 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Human Rights Commission Regulations 1989 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Modern Slavery Act 2018 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Securities and Investments Commission Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Australian Securities and Investments Commission Regulations 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Building and Construction Industry (Improving Productivity) Act 2016","Business as usual","No"]
[null,"Commonwealth Government","Competition and Consumer Act 2010 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Competition and Consumer Regulations 2010 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Corporations Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Corporations Regulations 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Designs Act 2003 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Disability Discrimination Act 1992 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Disability Discrimination Regulations 1996 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Environment Protection and Biodiversity Conservation Act 1999 (Cth)","Capex / Opex","No"]
[null,"Commonwealth Government","Equal Employment Opportunity (Commonwealth Authorities) Act 1987 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work (Transitional Provisions and Consequential Amendments) Regulations 2009 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work Act 2009 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fair Work Regulations 2009  (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Foreign Acquisitions and Takeovers Act 1975 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Foreign Acquisitions and Takeovers Regulations 1989 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Assessment Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Fringe Benefits Tax Regulations 1992 (Cth)","Opex","No"]
[null,"Commonwealth Government","National Harmonisation of Work Health and Safety Regulations 2011 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Income Tax (Excluded STBs) Regulations 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Act 1986 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Act 1936 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Act 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Assessment Regulations 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Income Tax Regulations 1936 (Cth)","Opex","No"]
[null,"Commonwealth Government","Law Reform (Contributory Negligence and Apportionment of Liability) Act 2001 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","National Greenhouse and Energy Reporting Act 2007 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Native Title (Indigenous Land Use Agreements) Regulations 1999 (Cth)","Opex","No"]
[null,"Commonwealth Government","Native Title Act 1993 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Patents Act 1990 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Personal Property Securities Act 2000 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Privacy Act 1988 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Privacy Amendment (Notifiable Data Breaches) Act 2017 ","Business as usual","No"]
[null,"Commonwealth Government","Privacy Regulation 2013 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Racial Discrimination Act 1975 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Racial Discrimination Regulations 1987 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Security of Critical Infrastructure Act 2018 (Cth)","Opex","Yes"]
[null,"Commonwealth Government","Sex Discrimination Amendment (Sexual Orientation, Gender Identity and Intersex Status) Act 2013","Business as usual","No"]
[null,"Commonwealth Government","Sex Discrimination Act 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Sex Discrimination Regulations 1984 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Superannuation Guarantee (Administration) Act 1992  (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Guarantee (Administration) Regulations 1993  (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Industry (Supervision) Act 1993 (Cth)","Opex","No"]
[null,"Commonwealth Government","Superannuation Industry (Supervision) Regulations 1994  (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications (Interception and Access) Act 1979 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications (Interception and Access) Regulations 1987 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications Act 1997 (Cth)","Opex","No"]
[null,"Commonwealth Government","Telecommunications Regulations 2001 (Cth)","Opex","No"]
[null,"Commonwealth Government","Trade Marks Act 1995 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Workplace Gender Equality Act 2012 (Cth)","Business as usual","No"]
[null,"Commonwealth Government","Workplace Relations Acts and Regulations (Cth)","Business as usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"ACMA","Carrier licences for telecommunications and radio communications permits us to operate our radio and operational telecommunications","Opex","No"]
[null,"ESCoSA","Electricity Distribution Licence - Licenses and imposes obligations on DNSPs","Opex","No"]
[null,"ESCoSA","Electricity Generation Licence- Kangaroo Island Power Station - Permits us to operate the Kingscote Generator in SA","Opex","No"]
[]
[null,"RULES"]
[null,"Equal Opportunity Tribunal Rules (SA)","Equal Opportunity Tribunal Rules (SA)","Business as usual","No"]
[null,"Industrial Proceedings Rules 2010","Industrial Proceedings Rules 2010","Business as usual","No"]
[null,"Fair Work Commission Rules 2013 (Cth)","Fair Work Commission Rules 2013 (Cth)","Business as usual","No"]
[null,"National Electricity Rules\n\n\nNational Energy Retail Rules","National Electricity Rules - Details the technical operational requirements for the operation of the National Electricity Market\nNational Energy Retail Rules","Capex / Opex","No"]
[null,"ORDERS"]
[]
[]
[]
[null,"CODES"]
[null,"AEMO","National Metrology procedures","Opex","No"]
[null,"AEMO","MSATS","Opex","No"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Distribution Code (SA)","Capex / Opex","Yes"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Metering Code (SA)","Opex","No"]
[null,"ESCoSA (ESC Act)","ESCOSA Electricity Transmission Code (SA)","Capex / Opex","No"]
[null,"Building Code of Australia","Building Code of Australia published by the Australian Building Codes Board as in force from time to time\nBuilding and Construction Industry (Fair and Lawful Building Sites) Code 2014\nCode for the Tendering and Performance of Building Work ","Capex / Opex","No"]
[null,"State Government SA","Approved Code of Working Hours","Capex / Opex","No"]
[null,"Commonwealth Government","National Harmonisation of Work Health and Safety Code of Practice","Capex / Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"AER","Compliance Procedures and Guidelines","Opex","No"]
[null,"AER","Confidentiality","Confidentiality template Supporting Document 18.3","No"]
[null,"AER","Consumer Engagement","Customer and stakeholder engagement","Yes"]
[null,"AER","Cost Allocation Guideline (Distribution) ","Cost must be in acordance with this","No"]
[null,"AER","Distribution Annual Planning Report Template v1.0 (June 2017)","Business as usual/Capex","No"]
[null,"AER","Distribution Reliability Measures Guideline (Nov 2018)","Business as usual","No"]
[null,"AER","Electricity Distribution Service Classification Guideline (Sept 2018)","Discussed in Attachment - 12","No"]
[null,"AER","Expenditure Forecasts Assessment Guideline for Electricity Distribution","Business as usual","No"]
[null,"AER","National Electricity Connection Charge Guideline","Customer capex","No"]
[null,"AER","Rate of Return Binding Instrument","Relevant to SA Power Network's calculation of weighted average cost of capital in Attachment - 3","No"]
[null,"AER","Restricted Asset Exemptin Guideline (Sept 2018)","Business as usual","No"]
[null,"AER","Ring Fencing Guidelines (Oct 2017)","Capex/Opex","Yes"]
[null,"AER","RIT-D Application","All proposed network capex projects > $6 million are subject to a RIT-D process.\nAttachment - 5\n","No"]
[null,"AER","Shared Assets","Discussed in Attachment - 1","No"]
[null,"AER Scheme","Demand Management Incentive Scheme and Innovation allowance mechanism","Discussed in Attachment - 11","No"]
[null,"AER Scheme","Capital Expenditure Incentive Guideline for Electricity Network Service Providers","Discussed in Attachment - 5, Attachment - 9","No"]
[null,"AER Scheme","Efficiency Benefit Sharing Scheme for Electricity Network Service Providers","Discussed in Attachment - 6, Attachment - 8","No"]
[null,"AER Scheme","Service Target Performance Incentive Scheme ","Discussed in Attachment - 10","No"]
[null,"ESCoSA (ESC Act)","Electricity Industry Guideline No.1 - Information requirements - Details SA Power Networks reporting requirements for both Operational and Financial Perfromance","Opex","No"]
[null,"ESCoSA (ESC Act)","Energy Industry Guideline No.4 - Compliance Systems and Reporting - Details SA Power Networks compliance reporting obligations and system for compliance","Opex","No"]
[null,"SAPN Real Estate Guidelines","To hold only such real property as is necessary for the efficient and effective operation of the business, ensure prudent provision for planned expansion of SA Power Networks’ operations, and appropriate legal tenure is obtained in all cases, to deliver optimal returns to shareholders and to meet the obligations to the Treasurer of South Australia under the Distribution Network Land Lease","Capex/Opex","No"]
[null,"SAPN Easement Guideilines","To provide adequate legal protection for electricity distribution network assets constructed on, under or over private and public property, to secure the right of access to those assets for maintenance purposes by the acquisition and registration of easements.\nThese Guidelines do not extend to land owned or leased by SA Power Networks (although it is possible to have an easement in favour of oneself), which are the subject of another document, “SA POWER NETWORKS Real Estate Guidelines” dated 28 April 2008","Business as usual","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[]
[]
[]
[null,"OTHER"]
[null,"AS / NZS 3000:2007  Electrical Installations","AS / NZS 3000:2007  Electrical Installations (known as the Australian/New Zealand Wiring Rules)",null,"No"]
[null,"AER Regulatory Information Notice 31 October 2018","Reset 2020-25 information requirements","Capex/Opex, RIM templates 1-7                                                      ","Yes"]
[null,"AER Framework and Approach for SA Power Networks - RCP commencing 1 July 2020","Sets parameters for our 2020-25 Regulatory Control Period.","Capex/Opex                                                      ","Yes"]
[null,"Easement Standard for Distribution Networks","This Technical Standard specifies the standard easement requiremetns and space allocation for a new or upgraded installation that will be a component of SA Power Networks distribution network. ","Business as usual","No"]

{"sheet":"7.7 TSS-LRMC","index":36,"n_rows":150,"n_cols":22,"rows_kept":150,"cut":false,"hidden":false,"merged":[[107,2,107,21],[122,2,122,21],[137,2,137,21],[44,1,45,1],[44,2,44,21],[64,1,65,1],[64,2,64,21],[84,1,85,1],[84,2,84,21],[8,1,9,1],[8,2,8,21],[19,1,20,1],[19,2,19,21],[30,1,31,1],[30,2,30,21]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C10,4)+1)&\"-\"&MID(C10,3,2)+2),VALUE(LEFT(C10,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure",11634748,9365043,7371460,7924408,8199755,7085862,6167348,6012284,7126853,7126853,7126853,7126853,7126853,7126853,7126853,7126853,7126853,7126853,7126853,7126853]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",28663956,28281675,30333024,24215243,18879444,19256773,20700091,21100353,22414155,22414155,22414155,22414155,22414155,22414155,22414155,22414155,22414155,22414155,22414155,22414155]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C11:C16)","v":40298704},{"$f":"SUM(D11:D16)","v":37646718},37704484,32139651,27079199,26342635,26867439,27112637,29541008,29541008,29541008,29541008,29541008,29541008,29541008,29541008,29541008,29541008,29541008,29541008]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C21,4)+1)&\"-\"&MID(C21,3,2)+2),VALUE(LEFT(C21,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C32,4)+1)&\"-\"&MID(C32,3,2)+2),VALUE(LEFT(C32,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C46,4)+1)&\"-\"&MID(C46,3,2)+2),VALUE(LEFT(C46,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Opex on incremental capex",333886,740923,741016,764638,638412,588167,587336,533407,487445,498466,503516,504437,527582,527582,527582,527582,527582,527582,527582,527582]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C47:C61)","v":333886},{"$f":"SUM(D47:D61)","v":740923},741016,764638,638412,588167,587336,533407,487445,498466,503516,504437,527582,527582,527582,527582,527582,527582,527582,527582]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C66,4)+1)&\"-\"&MID(C66,3,2)+2),VALUE(LEFT(C66,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C86,4)+1)&\"-\"&MID(C86,3,2)+2),VALUE(LEFT(C86,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C109,4)+1)&\"-\"&MID(C109,3,2)+2),VALUE(LEFT(C109,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[null,"Sub-Transmission",64,64,64,64,65,65,65,66,66,66,66,67,67,67,68,68,68,69,69,69]
[null,"Zone Sub Station",62,62,62,63,63,63,63,64,64,64,65,65,65,66,66,66,66,67,67,67]
[null,"HV Feeder",153,154,155,155,156,156,157,158,159,159,160,161,162,163,163,164,165,166,166,167]
[null,"Distribution Transformer",705,708,712,714,716,718,720,726,729,733,736,740,743,747,750,754,757,761,764,768]
[null,"LV Feeder",1902,1910,1919,1925,1930,1935,1941,1958,1967,1977,1986,1996,2005,2015,2024,2034,2043,2052,2062,2071]
[]
[null,"NOTE: These are in MW"]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C110:C119)","v":2886},{"$f":"SUM(D110:D119)","v":2898},2912,2921,2930,2937,2946,2972,2985,2999,3013,3029,3042,3058,3071,3086,3099,3115,3128,{"$f":"SUM(V110:V119)","v":3142}]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C124,4)+1)&\"-\"&MID(C124,3,2)+2),VALUE(LEFT(C124,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2020"}]
[null,null,{"$f":"CRCP_y4","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C139,4)+1)&\"-\"&MID(C139,3,2)+2),VALUE(LEFT(C139,4)+1))","v":"2019-20"},"2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]

{"sheet":"7.8 WACC Inputs","index":37,"n_rows":66,"n_cols":3,"rows_kept":66,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"SA Power Networks"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2020-21 to 2024-25"}]
[null,"7.8 WACC AND CAPM PARAMETERS"]
[]
[]
[null,"Business Days means Business Days as defined in the Rate of Return Guideline"]
[]
[null,"7.8 - WACC AND CAPM PARAMETERS"]
[null,"7.8.1 - RATE OF RETURN ON EQUITY"]
[null,"Equity averaging period - nominated (placeholder)"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[]
[null,"Nominated equity averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[]
[null,"Nominal risk free rate"]
[null,"Equity term - risk free rate"]
[null,"Forecast Inflation rate"]
[null,"Market risk premium"]
[null,"Equity beta"]
[null,"Equity risk premium",{"$f":"C26*C27","v":0}]
[]
[]
[null,"7.8.2 - RATE OF RETURN ON DEBT - Transition - 'trailing average' approach"]
[null,"Debt averaging period - Year 1 nominated (placeholder)"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[]
[null,"Year 1 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[null,"Year 2 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[null,"Year 3 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[null,"Year 4 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[null,"Year 5 nominated debt averaging period"]
[null,"Start date (inclusive)"]
[null,"End date (inclusive)"]
[null,"Number of Business Days"]
[]
[]
[null,"Credit rating"]
[]
[null,"Debt term"]

{"sheet":"Amendments","index":38,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,1,0,3]]}
[null,{"$f":"CONCATENATE(dms_TradingName,\" data amendments\")","v":"SA Power Networks data amendments"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"SA Power Networks"},"Table","Comments"]