{"text_format":"1","workbook":"xlsx","n_sheets":17,"sheets":["2016 DUOS Ex GST","2016 TUOS Ex GST","2016 NUOS Ex GST","2017 DUOS Ex GST","2017 TUOS Ex GST","2017 NUOS Ex GST","2018 DUOS Ex GST","2018 TUOS Ex GST","2018 NUOS Ex GST","2019 DUOS Ex GST","2019 TUOS Ex GST","2019 NUOS Ex GST","2020 DUOS Ex GST","2020 TUOS Ex GST","2020 NUOS Ex GST","PFIT TFIT Ex GST","Prescribed Ex GST"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":15,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"2016 DUOS Ex GST","index":0,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Distribution Use of System (DUOS) Tariffs: 1 January 2016 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R","F,T",6.2279999999999998,7.68,4.944,0,0,0,0,0,0,0,0,null,null,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.721,9.1300000000000008,6.9249999999999998,0,0,0,1.583,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.752,0,0,0,0,null,null,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,7.6749999999999998,5.6139999999999999,0,0,0,1.3839999999999999,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,8.0210000000000008,5.9820000000000002,4.4320000000000004,1.661,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,5.1989999999999998,1.3069999999999999,0,0,0,1.284,0,65.322999999999993,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F,T",10.715999999999999,9.4190000000000005,5.8769999999999998,0,0,0,0,0,0,0,0,null,null,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,19.145,9.2970000000000006,6.9669999999999996,0,0,0,1.736,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.960999999999999,9.1,7.0469999999999997,0,0,0,1.66,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,7.6509999999999998,4.4829999999999997,0,0,0,1.782,0,36.637,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,6.851,5.2670000000000003,0,0,0,1.548,0,60.292000000000002,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.851000000000001,5.4269999999999996,4.282,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,17.094999999999999,8.4960000000000004,6.7549999999999999,0,0,0,1.617,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.222,1.036,0,0,0,1.0249999999999999,12.333,18.398,0,0,null,null,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.0660000000000001,0.88200000000000001,0,0,0,0.876,12.272,28.948,0,0,null,null,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.73599999999999999,0.65,0,0,0,0.63900000000000001,7.5019999999999998,10.302,0,0,null,null,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.76200000000000001,0.63,0,0,0,0.623,8.6519999999999992,20.952000000000002,0,0,null,null,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.41899999999999998,0.32700000000000001,0,0,0,0.28299999999999997,0.73399999999999999,1.0760000000000001,0,0,null,null,null,null,11100]
[null,"Time of Day","TOD","F,T",5.9249999999999998,14.243,8.3940000000000001,0,4.0140000000000002,2.9569999999999999,2.746,0,0,0,0,null,null,"NA","<20"]
[null,"Time of Use","TOU","F,T",0,8.9649999999999999,5.4459999999999997,0,0,0,2.63,0,38.930999999999997,0,0,null,null,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F, T",6.1459999999999999,16.059000000000001,9.98,0,4.9779999999999998,3.9990000000000001,3.8039999999999998,0,0,0,0,null,null,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F,T",6.6189999999999998,15.798999999999999,9.0690000000000008,0,4.29,4.29,3.6379999999999999,0,0,0,0,null,null,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F,T",0,2.444,2.444,0,2.444,2.444,2.444,0,0,22.82,9.0050000000000008,null,null,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F,T",0,2.444,2.444,0,2.444,2.444,2.444,0,0,22.82,9.0050000000000008,null,null,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F,T",0,3.5950000000000002,3.5950000000000002,0,3.5950000000000002,3.5950000000000002,3.5950000000000002,0,0,37.469000000000001,24.978999999999999,null,null,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2016 TUOS Ex GST","index":1,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Transmission Use of System (TUOS) Tariffs: 1 January 2016 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R","F,T",0,2.2690000000000001,1.897,0,0,0,0,0,0,0,0,null,null,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,0,3.8109999999999999,3.05,0,0,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,0,0,0,0,0,null,null,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,3.5710000000000002,2.8540000000000001,0,0,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,0,2.5390000000000001,2.0310000000000001,2.0310000000000001,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,17.204999999999998,3.831,0,0,0,0,0,10.91,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F,T",0,2.6930000000000001,2.1509999999999998,0,0,0,0,0,0,0,0,null,null,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,0,2.008,1.605,0,0,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,0,2.6680000000000001,2.1360000000000001,0,0,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,1.86,1.4870000000000001,0,0,0,0,0,8.6750000000000007,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,1.17,0.93500000000000005,0,0,0,0,0,10.484,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,0,2.6589999999999998,2.125,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,0,2.044,1.637,0,0,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.165,0.93500000000000005,0,0,0,0,4.7569999999999997,6.5019999999999998,0,0,null,null,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.73599999999999999,0.59,0,0,0,0,3.0019999999999998,7.8929999999999998,0,0,null,null,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.81899999999999995,0.65600000000000003,0,0,0,0,5.4470000000000001,5.718,0,0,null,null,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.47099999999999997,0.375,0,0,0,0,3.1230000000000002,6.3049999999999997,0,0,null,null,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.55200000000000005,0.44500000000000001,0,0,0,0,3.9159999999999999,4.7510000000000003,0,0,null,null,null,null,11100]
[null,"Time of Day","TOD","F,T",0,3.1960000000000002,2.7130000000000001,0,2.7130000000000001,2.3959999999999999,0,0,0,0,0,null,null,"NA","<20"]
[null,"Time of Use","TOU","F,T",0,2.375,1.091,0,0,0,0,0,6.2220000000000004,0,0,null,null,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F, T",0,4.9329999999999998,4.5860000000000003,0,4.5860000000000003,4.3579999999999997,0,0,0,0,0,null,null,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F,T",0,4.1710000000000003,3.891,0,2.0840000000000001,1.839,0,0,0,0,0,null,null,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F,T",0,0.96899999999999997,0.96899999999999997,0,0.96899999999999997,0.96899999999999997,0.96899999999999997,0,0,5.42,5.3869999999999996,null,null,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F,T",0,0.96899999999999997,0.96899999999999997,0,0.96899999999999997,0.96899999999999997,0.96899999999999997,0,0,5.42,5.3869999999999996,null,null,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F,T",0,0.90100000000000002,0.90100000000000002,0,0.90100000000000002,0.90100000000000002,0.90100000000000002,0,0,9.3919999999999995,6.2619999999999996,null,null,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2016 NUOS Ex GST","index":2,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Network Use of System (NUOS) Tariffs: 1 January 2016 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R","F,T",6.2279999999999998,9.9489999999999998,6.8410000000000002,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.721,12.941000000000001,9.9749999999999996,0,0,0,1.583,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.752,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,11.246,8.468,0,0,0,1.3839999999999999,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,8.0210000000000008,8.5210000000000008,6.463000000000001,3.6920000000000002,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,22.403999999999996,5.1379999999999999,0,0,0,1.284,0,76.23299999999999,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F,T",10.715999999999999,12.112,8.0279999999999987,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,19.145,11.305,8.5719999999999992,0,0,0,1.736,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.960999999999999,11.768000000000001,9.1829999999999998,0,0,0,1.66,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,9.5109999999999992,5.97,0,0,0,1.782,0,45.311999999999998,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,8.0210000000000008,6.202,0,0,0,1.548,0,70.775999999999996,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.851000000000001,8.0859999999999985,6.407,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,17.094999999999999,10.540000000000001,8.3919999999999995,0,0,0,1.617,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,2.387,1.9710000000000001,0,0,0,1.0249999999999999,17.09,24.9,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.802,1.472,0,0,0,0.876,15.274000000000001,36.841000000000001,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,1.5549999999999999,1.306,0,0,0,0.63900000000000001,12.949,16.02,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,1.2330000000000001,1.0049999999999999,0,0,0,0.623,11.774999999999999,27.257000000000001,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.97100000000000009,0.77200000000000002,0,0,0,0.28299999999999997,4.6500000000000004,5.827,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F,T",5.9249999999999998,17.439,11.106999999999999,0,6.7270000000000003,5.3529999999999998,2.746,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F,T",0,11.34,6.5369999999999999,0,0,0,2.63,0,45.152999999999999,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F, T",6.1459999999999999,20.992000000000001,14.566000000000001,0,9.5640000000000001,8.3569999999999993,3.8039999999999998,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F,T",6.6189999999999998,19.97,12.96,0,6.3740000000000006,6.1289999999999996,3.6379999999999999,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F,T",0,3.4129999999999998,3.4129999999999998,0,3.4129999999999998,3.4129999999999998,3.4129999999999998,0,0,28.240000000000002,14.391999999999999,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F,T",0,3.4129999999999998,3.4129999999999998,0,3.4129999999999998,3.4129999999999998,3.4129999999999998,0,0,28.240000000000002,14.391999999999999,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F,T",0,4.4960000000000004,4.4960000000000004,0,4.4960000000000004,4.4960000000000004,4.4960000000000004,0,0,46.861000000000004,31.241,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2017 DUOS Ex GST","index":3,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Distribution Use of System (DUOS) Tariffs: 1 January 2017 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,5.8270413599999999,7.1855615999999998,4.62570528,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,11.90202202,8.5422106000000007,6.4791685000000001,0,0,0,1.48108646,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.63920624,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,7.1808835000000002,5.2525706799999998,0,0,0,1.2948980799999998,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.5046080200000009,5.5968788400000005,4.1466678400000001,1.55406482,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,4.8642883799999996,1.22285534,0,0,0,1.2013360800000001,0,61.117505259999994,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.026103919999999,8.8126047800000009,5.4986387399999996,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,17.912444900000001,8.6984591400000006,6.5184645400000001,0,0,0,1.6242363200000001,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,19.611530819999999,8.5141419999999997,6.5933141399999995,0,0,0,1.5531291999999999,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,7.1584286199999996,4.1943844599999993,0,0,0,1.6672748400000001,0,34.27830994,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,6.4099326200000002,4.9279105400000001,0,0,0,1.4483397600000001,0,56.410401040000004,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.088032620000002,5.0776097399999998,4.0063248400000004,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,15.994423899999999,7.9490275200000005,6.3201131000000004,0,0,0,1.51289754,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.1433276400000001,0.96930232000000005,0,0,0,0.95901049999999988,11.53900146,17.21353676,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.99737092000000005,0.82521684000000006,0,0,0,0.81960312000000002,11.48192864,27.084327760000001,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.68861631999999995,0.60815300000000005,0,0,0,0.59786117999999999,7.0190212399999998,9.6387572400000003,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.71294244000000007,0.58944059999999998,0,0,0,0.58289126000000002,8.0949842399999987,19.603110240000003,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.39202477999999996,0.30594774000000002,0,0,0,0.26478046,0.68674508000000001,1.0067271200000001,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.5435485,13.326035660000001,7.8535942800000003,0,3.7555786800000002,2.76662834,2.5692125200000002,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,8.3878333000000005,5.0953865199999999,0,0,0,2.4606805999999999,0,36.424622219999996,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",5.7503205199999998,15.02512158,9.3374876000000011,0,4.6575163599999998,3.7415443800000001,3.5590984799999998,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.1928687799999995,14.781860379999999,8.4851377800000005,0,4.0138097999999998,4.0138097999999998,3.4037855599999998,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,2.2866552800000002,2.2866552800000002,0,2.2866552800000002,2.2866552800000002,2.2866552800000002,0,0,21.3508484,8.4252581000000006,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,2.2866552800000002,2.2866552800000002,0,2.2866552800000002,2.2866552800000002,2.2866552800000002,0,0,21.3508484,8.4252581000000006,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,3.3635539000000003,3.3635539000000003,0,3.3635539000000003,3.3635539000000003,3.3635539000000003,0,0,35.05674578,23.370851980000001,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2017 TUOS Ex GST","index":4,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Transmission Use of System (TUOS) Tariffs: 1 January 2017 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,0,2.3257249999999998,1.9444249999999998,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,0,3.9062749999999995,3.1262499999999998,0,0,0,0,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,3.6602749999999999,2.9253499999999999,0,0,0,0,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,0,2.6024750000000001,2.0817749999999999,2.0817749999999999,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,17.635124999999995,3.9267749999999997,0,0,0,0,0,11.182749999999999,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",0,2.7603249999999999,2.2047749999999997,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,0,2.0581999999999998,1.6451249999999999,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,0,2.7347000000000001,2.1894,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,1.9064999999999999,1.5241750000000001,0,0,0,0,0,8.8918750000000006,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,1.1992499999999999,0.95837499999999998,0,0,0,0,0,10.746099999999998,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,0,2.7254749999999994,2.1781249999999996,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,0,2.0951,1.6779249999999999,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.1941249999999999,0.95837499999999998,0,0,0,0,4.8759249999999996,6.6645499999999993,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.75439999999999996,0.6047499999999999,0,0,0,0,3.0770499999999994,8.0903249999999982,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.83947499999999986,0.6724,0,0,0,0,5.5831749999999998,5.8609499999999999,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.48277499999999995,0.38437499999999997,0,0,0,0,3.2010749999999999,6.4626249999999992,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.56579999999999997,0.45612499999999995,0,0,0,0,4.0138999999999996,4.8697749999999997,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",0,3.2759,2.7808249999999997,0,2.7808249999999997,2.4558999999999997,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,2.4343749999999997,1.1182749999999999,0,0,0,0,0,6.3775500000000003,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",0,5.0563249999999993,4.7006499999999996,0,4.7006499999999996,4.4669499999999989,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",0,4.2752749999999997,3.9882749999999998,0,2.1360999999999999,1.8849749999999998,0,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,0.99322499999999991,0.99322499999999991,0,0.99322499999999991,0.99322499999999991,0.99322499999999991,0,0,5.5554999999999994,5.5216749999999992,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,0.99322499999999991,0.99322499999999991,0,0.99322499999999991,0.99322499999999991,0.99322499999999991,0,0,5.5554999999999994,5.5216749999999992,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,0.92352499999999993,0.92352499999999993,0,0.92352499999999993,0.92352499999999993,0.92352499999999993,0,0,9.6267999999999994,6.4185499999999989,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2017 NUOS Ex GST","index":5,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Network Use of System (NUOS) Tariffs: 1 January 2017 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,5.8270413599999999,9.5112866,6.5701302799999999,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,11.90202202,12.4484856,9.605418499999999,0,0,0,1.48108646,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.63920624,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,10.841158500000001,8.1779206799999997,0,0,0,1.2948980799999998,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.5046080200000009,8.1993538400000006,6.2284428399999996,3.6358398200000002,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,22.499413379999993,5.1496303399999999,0,0,0,1.2013360800000001,0,72.30025526,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.026103919999999,11.572929780000001,7.7034137399999993,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,17.912444900000001,10.75665914,8.1635895400000003,0,0,0,1.6242363200000001,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,19.611530819999999,11.248842,8.7827141399999995,0,0,0,1.5531291999999999,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,9.0649286199999999,5.7185594599999998,0,0,0,1.6672748400000001,0,43.170184939999999,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,7.6091826200000003,5.8862855400000003,0,0,0,1.4483397600000001,0,67.156501039999995,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.088032620000002,7.8030847399999992,6.1844498400000001,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,15.994423899999999,10.04412752,7.9980381000000005,0,0,0,1.51289754,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,2.33745264,1.9276773199999999,0,0,0,0.95901049999999988,16.41492646,23.878086759999999,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.75177092,1.4299668400000001,0,0,0,0.81960312000000002,14.558978639999999,35.174652760000001,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,1.5280913199999997,1.2805530000000001,0,0,0,0.59786117999999999,12.60219624,15.499707239999999,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,1.1957174400000001,0.9738156,0,0,0,0.58289126000000002,11.296059239999998,26.065735240000002,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.95782477999999993,0.76207274000000003,0,0,0,0.26478046,4.7006450799999993,5.8765021199999996,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.5435485,16.601935660000002,10.634419279999999,0,6.5364036799999994,5.2225283400000002,2.5692125200000002,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,10.8222083,6.2136615199999996,0,0,0,2.4606805999999999,0,42.802172219999996,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",5.7503205199999998,20.081446579999998,14.038137600000001,0,9.3581663599999985,8.2084943799999994,3.5590984799999998,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.1928687799999995,19.057135379999998,12.47341278,0,6.1499097999999996,5.8987847999999996,3.4037855599999998,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,3.27988028,3.27988028,0,3.27988028,3.27988028,3.27988028,0,0,26.906348399999999,13.946933099999999,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,3.27988028,3.27988028,0,3.27988028,3.27988028,3.27988028,0,0,26.906348399999999,13.946933099999999,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,4.2870789,4.2870789,0,4.2870789,4.2870789,4.2870789,0,0,44.683545780000003,29.789401980000001,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2018 DUOS Ex GST","index":6,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Distribution Use of System (DUOS) Tariffs: 1 January 2018 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,5.9727173939999991,7.3652006399999994,4.7413479119999993,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.199572570499999,8.7557658650000008,6.6411477124999996,0,0,0,1.5181136215,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.6801863959999999,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,7.3604055874999998,5.3838849469999994,0,0,0,1.3272705319999998,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.6922232204999998,5.7368008110000002,4.2503345359999996,1.5929164404999998,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,4.9858955894999992,1.2534267234999998,0,0,0,1.2313694820000001,0,62.645442891499989,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.276756517999997,9.0329198994999995,5.6361047084999996,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,18.3602560225,8.9159206184999995,6.6814261534999995,0,0,0,1.6648422279999999,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.101819090499998,8.726995549999998,6.7581469934999987,0,0,0,1.5919574299999997,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,7.3373893354999993,4.2992440714999987,0,0,0,1.7089567109999999,0,35.135267688499994,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,6.5701809354999998,5.0511083034999995,0,0,0,1.4845482539999999,0,57.820661066,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.3652334355,5.2045499834999989,4.1064829610000002,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,16.394284497499999,8.1477532079999992,6.4781159275000002,0,0,0,1.5507199784999999,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.1719108309999999,0.99353487799999995,0,0,0,0.9829857624999998,11.827476496499999,17.643875178999998,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.022305193,0.84584726099999996,0,0,0,0.84009319799999993,11.768976855999998,27.761435954,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.70583172799999994,0.623356825,0,0,0,0.61280770949999996,7.194496770999999,9.8797261709999997,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.730766001,0.60417661499999997,0,0,0,0.59746354149999992,8.2973588459999981,20.093187996000001,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.4018253994999999,0.31359643349999999,0,0,0,0.27139997149999995,0.703913707,1.031895298,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.6821372124999998,13.659186551499999,8.0499341369999993,0,3.8494681469999996,2.8357940484999999,2.6334428330000001,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,8.5975291325000001,5.2227711829999999,0,0,0,2.5221976149999996,0,37.335237775499991,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",5.8940785329999992,15.400749619499999,9.5709247900000012,0,4.773954268999999,3.8350829894999996,3.6480759419999997,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.3476904994999988,15.151406889499999,8.6972662244999999,0,4.1141550449999995,4.1141550449999995,3.4888801989999996,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,2.3438216619999999,2.3438216619999999,0,2.3438216619999999,2.3438216619999999,2.3438216619999999,0,0,21.884619609999998,8.6358895525000001,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,2.3438216619999999,2.3438216619999999,0,2.3438216619999999,2.3438216619999999,2.3438216619999999,0,0,21.884619609999998,8.6358895525000001,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,3.4476427475000002,3.4476427475000002,0,3.4476427475000002,3.4476427475000002,3.4476427475000002,0,0,35.933164424499999,23.9551232795,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2018 TUOS Ex GST","index":7,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Transmission Use of System (TUOS) Tariffs: 1 January 2018 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,0,2.3838681249999998,1.9930356249999996,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,0,4.0039318749999993,3.2044062499999995,0,0,0,0,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,3.7517818749999998,2.9984837499999997,0,0,0,0,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,0,2.6675368749999997,2.1338193749999999,2.1338193749999999,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,18.076003124999993,4.0249443749999996,0,0,0,0,0,11.462318749999998,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",0,2.8293331249999998,2.2598943749999996,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,0,2.1096549999999996,1.6862531249999999,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,0,2.8030675,2.244135,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,1.9541624999999996,1.5622793749999999,0,0,0,0,0,9.1141718750000003,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,1.2292312499999998,0.98233437499999987,0,0,0,0,0,11.014752499999997,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,0,2.793611874999999,2.2325781249999994,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,0,2.1474774999999999,1.7198731249999997,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.2239781249999997,0.98233437499999987,0,0,0,0,4.9978231249999991,6.8311637499999991,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.77325999999999984,0.61986874999999986,0,0,0,0,3.153976249999999,8.2925831249999966,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.86046187499999982,0.68920999999999999,0,0,0,0,5.7227543749999992,6.0074737499999991,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.49484437499999989,0.39398437499999994,0,0,0,0,3.2811018749999996,6.6241906249999989,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.57994499999999993,0.46752812499999991,0,0,0,0,4.1142474999999994,4.9915193749999993,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",0,3.3577974999999998,2.8503456249999992,0,2.8503456249999992,2.5172974999999997,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,2.4952343749999994,1.1462318749999998,0,0,0,0,0,6.5369887499999999,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",0,5.1827331249999986,4.8181662499999991,0,4.8181662499999991,4.5786237499999984,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",0,4.3821568749999997,4.0879818749999997,0,2.1895024999999997,1.9320993749999997,0,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,1.0180556249999999,1.0180556249999999,0,1.0180556249999999,1.0180556249999999,1.0180556249999999,0,0,5.6943874999999986,5.6597168749999991,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,1.0180556249999999,1.0180556249999999,0,1.0180556249999999,1.0180556249999999,1.0180556249999999,0,0,5.6943874999999986,5.6597168749999991,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,0.94661312499999983,0.94661312499999983,0,0.94661312499999983,0.94661312499999983,0.94661312499999983,0,0,9.8674699999999991,6.5790137499999979,0,0,"NA",">20 & <400",null,1.5]
[null,null,null,null,0]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2018 NUOS Ex GST","index":8,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Network Use of System (NUOS) Tariffs: 1 January 2018 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,5.9727173939999991,9.7490687649999987,6.7343835369999994,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.199572570499999,12.75969774,9.8455539624999986,0,0,0,1.5181136215,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.6801863959999999,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,11.1121874625,8.3823686969999986,0,0,0,1.3272705319999998,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.6922232204999998,8.4043376859999999,6.3841539109999994,3.7267358154999997,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,23.061898714499993,5.2783710984999992,0,0,0,1.2313694820000001,0,74.107761641499991,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.276756517999997,11.862253024499999,7.8959990834999996,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,18.3602560225,11.0255756185,8.3676792784999989,0,0,0,1.6648422279999999,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.101819090499998,11.530063049999999,9.0022819934999987,0,0,0,1.5919574299999997,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,9.2915518354999982,5.8615234464999988,0,0,0,1.7089567109999999,0,44.24943956349999,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,7.7994121854999996,6.0334426784999993,0,0,0,1.4845482539999999,0,68.835413566,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.3652334355,7.9981618584999978,6.3390610859999992,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,16.394284497499999,10.295230707999998,8.1979890525000005,0,0,0,1.5507199784999999,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,2.3958889559999994,1.9758692529999999,0,0,0,0.9829857624999998,16.825299621499997,24.475038928999997,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.7955651929999998,1.4657160109999998,0,0,0,0.84009319799999993,14.922953105999998,36.054019079,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,1.5662936029999996,1.312566825,0,0,0,0.61280770949999996,12.917251145999998,15.887199920999999,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,1.2256103759999999,0.99816098999999991,0,0,0,0.59746354149999992,11.578460720999997,26.717378621000002,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.98177039949999978,0.78112455849999995,0,0,0,0.27139997149999995,4.8181612069999993,6.0234146729999996,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.6821372124999998,17.0169840515,10.900279761999998,0,6.6998137719999988,5.3530915485000001,2.6334428330000001,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,11.092763507499999,6.3690030579999997,0,0,0,2.5221976149999996,0,43.87222652549999,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",5.8940785329999992,20.583482744499996,14.38909104,0,9.5921205189999981,8.4137067394999985,3.6480759419999997,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.3476904994999988,19.533563764499998,12.785248099499999,0,6.3036575449999992,6.0462544199999995,3.4888801989999996,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,3.3618772869999995,3.3618772869999995,0,3.3618772869999995,3.3618772869999995,3.3618772869999995,0,0,27.579007109999996,14.295606427499999,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,3.3618772869999995,3.3618772869999995,0,3.3618772869999995,3.3618772869999995,3.3618772869999995,0,0,27.579007109999996,14.295606427499999,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,4.3942558725000005,4.3942558725000005,0,4.3942558725000005,4.3942558725000005,4.3942558725000005,0,0,45.800634424499997,30.534137029499998,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2019 DUOS Ex GST","index":9,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Distribution Use of System (DUOS) Tariffs: 1 January 2019 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,6.1220353288499982,7.5493306559999986,4.8598816097999986,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.504561884762499,8.9746600116249997,6.8071764053124992,0,0,0,1.5560664620374998,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.7221910558999998,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,7.5444157271874994,5.5184820706749989,0,0,0,1.3604522952999996,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.8845288010124994,5.8802208312749995,4.3565928993999989,1.6327393515124997,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,5.1105429792374988,1.2847623915874997,0,0,0,1.2621537190500001,0,64.211578963787488,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.533675430949996,9.2587428969874992,5.777007326212499,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,18.819262423062497,9.138818633962499,6.8484618073374985,0,0,0,1.7064632836999998,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.604364567762495,8.9451704387499973,6.9271006683374985,0,0,0,1.6317563657499996,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,7.5208240688874985,4.4067251732874979,0,0,0,1.7516806287749997,0,36.013649380712494,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,6.7344354588874991,5.1773860110874992,0,0,0,1.5216619603499997,0,59.266177592649996,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.649364271387499,5.3346637330874982,4.2091450350250001,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,16.804141609937499,8.3514470381999981,6.6400688256875,0,0,0,1.5894879779624997,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.2012086017749999,1.0183732499499998,0,0,0,1.0075604065624997,12.123163408912498,18.084972058474996,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.047862822825,0.86699344252499988,0,0,0,0.86109552794999988,12.063201277399997,28.455471852849996,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.72347752119999986,0.63894074562499992,0,0,0,0.62812790223749992,7.3743591902749985,10.126719325274999,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.74903515102499996,0.61928103037499993,0,0,0,0.61240013003749982,8.5047928171499976,20.5955176959,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.41187103448749984,0.32143634433749996,0,0,0,0.27818497078749993,0.72151154967499997,1.05769268045,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.824190642812499,14.000666215287499,8.2511824904249984,0,3.9457048506749994,2.9066888997124996,2.6992789038249998,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,8.8124673608124997,5.3533404625749998,0,0,0,2.5852525553749994,0,38.268618719887485,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",6.041430496324999,15.785768359987498,9.8101979097500003,0,4.8933031257249988,3.9309600642374991,3.7392778405499993,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.5063827619874983,15.530192061737496,8.9146978801124988,0,4.2170089211249993,4.2170089211249993,3.5761022039749992,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,2.4024172035499998,2.4024172035499998,0,2.4024172035499998,2.4024172035499998,2.4024172035499998,0,0,22.431735100249995,8.8517867913124988,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,2.4024172035499998,2.4024172035499998,0,2.4024172035499998,2.4024172035499998,2.4024172035499998,0,0,22.431735100249995,8.8517867913124988,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,3.5338338161874998,3.5338338161874998,0,3.5338338161874998,3.5338338161874998,3.5338338161874998,0,0,36.831493535112493,24.554001361487497,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2019 TUOS Ex GST","index":10,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Transmission Use of System (TUOS) Tariffs: 1 January 2019 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,0,2.4434648281249998,2.0428615156249994,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,0,4.1040301718749985,3.284516406249999,0,0,0,0,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,3.8455764218749993,3.0734458437499992,0,0,0,0,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,0,2.7342252968749996,2.1871648593749997,2.1871648593749997,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,18.527903203124989,4.1255679843749995,0,0,0,0,0,11.748876718749997,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",0,2.9000664531249996,2.3163917343749993,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,0,2.1623963749999993,1.7284094531249998,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,0,2.8731441874999999,2.3002383749999997,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,2.0030165624999996,1.6013363593749999,0,0,0,0,0,9.3420261718750002,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,1.2599620312499997,1.0068927343749998,0,0,0,0,0,11.290121312499995,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,0,2.8634521718749988,2.2883925781249994,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,0,2.2011644374999997,1.7628699531249996,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.2545775781249995,1.0068927343749998,0,0,0,0,5.1227687031249989,7.0019428437499984,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.79259149999999978,0.63536546874999977,0,0,0,0,3.2328256562499988,8.4998977031249954,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.88197342187499972,0.70644024999999988,0,0,0,0,5.8658232343749983,6.1576605937499984,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.50721548437499986,0.4038339843749999,0,0,0,0,3.3631294218749992,6.7897953906249979,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.59444362499999992,0.47921632812499987,0,0,0,0,4.217103687499999,5.116307359374999,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",0,3.4417424374999994,2.9216042656249988,0,2.9216042656249988,2.5802299374999995,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,2.5576152343749992,1.1748876718749997,0,0,0,0,0,6.700413468749999,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",0,5.3123014531249977,4.9386204062499983,0,4.9386204062499983,4.6930893437499979,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",0,4.4917107968749992,4.1901814218749989,0,2.2442400624999994,1.9804018593749995,0,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,1.0435070156249999,1.0435070156249999,0,1.0435070156249999,1.0435070156249999,1.0435070156249999,0,0,5.8367471874999977,5.8012097968749989,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,1.0435070156249999,1.0435070156249999,0,1.0435070156249999,1.0435070156249999,1.0435070156249999,0,0,5.8367471874999977,5.8012097968749989,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,0.97027845312499972,0.97027845312499972,0,0.97027845312499972,0.97027845312499972,0.97027845312499972,0,0,10.114156749999998,6.7434890937499974,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2019 NUOS Ex GST","index":11,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Network Use of System (NUOS) Tariffs: 1 January 2019 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,6.1220353288499982,9.9927954841249989,6.9027431254249976,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.504561884762499,13.078690183499997,10.091692811562499,0,0,0,1.5560664620374998,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.7221910558999998,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,11.389992149062499,8.591927914424998,0,0,0,1.3604522952999996,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,7.8845288010124994,8.61444612815,6.5437577587749987,3.8199042108874997,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,23.638446182362486,5.4103303759624994,0,0,0,1.2621537190500001,0,75.960455682537486,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.533675430949996,12.158809350112499,8.0933990605874975,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,18.819262423062497,11.301215008962497,8.5768712604624984,0,0,0,1.7064632836999998,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,20.604364567762495,11.818314626249997,9.2273390433374978,0,0,0,1.6317563657499996,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,9.5238406313874986,6.0080615326624978,0,0,0,1.7516806287749997,0,45.355675552587492,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,7.9943974901374988,6.1842787454624988,0,0,0,1.5216619603499997,0,70.556298905149987,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.649364271387499,8.1981159049624974,6.4975376131499996,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,16.804141609937499,10.552611475699997,8.4029387788124996,0,0,0,1.5894879779624997,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,2.4557861798999996,2.0252659843249994,0,0,0,1.0075604065624997,17.245932112037497,25.086914902224994,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.8404543228249999,1.5023589112749995,0,0,0,0.86109552794999988,15.296026933649996,36.95536955597499,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,1.6054509430749997,1.3453809956249998,0,0,0,0.62812790223749992,13.240182424649998,16.284379919025,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,1.2562506353999998,1.0231150147499999,0,0,0,0.61240013003749982,11.867922239024997,27.385313086524999,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,1.0063146594874999,0.80065267246249983,0,0,0,0.27818497078749993,4.9386152371749992,6.1740000398249988,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.824190642812499,17.442408652787499,11.172786756049998,0,6.8673091162999977,5.4869188372124995,2.6992789038249998,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,11.370082595187499,6.5282281344499999,0,0,0,2.5852525553749994,0,44.969032188637485,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",6.041430496324999,21.098069813112495,14.748818315999998,0,9.8319235319749971,8.6240494079874974,3.7392778405499993,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.5063827619874983,20.021902858612496,13.104879301987499,0,6.4612489836249987,6.1974107804999985,3.5761022039749992,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,3.4459242191749997,3.4459242191749997,0,3.4459242191749997,3.4459242191749997,3.4459242191749997,0,0,28.268482287749993,14.652996588187499,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,3.4459242191749997,3.4459242191749997,0,3.4459242191749997,3.4459242191749997,3.4459242191749997,0,0,28.268482287749993,14.652996588187499,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,4.5041122693124995,4.5041122693124995,0,4.5041122693124995,4.5041122693124995,4.5041122693124995,0,0,46.945650285112492,31.297490455237494,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2020 DUOS Ex GST","index":12,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Distribution Use of System (DUOS) Tariffs: 1 January 2020 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,6.2750862120712476,7.7380639223999976,4.9813786500449986,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.817175931881559,9.1990265119156245,6.9773558154453115,0,0,0,1.5949681235884372,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.7652458322974995,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,7.7330261203671862,5.6564441224418731,0,0,0,1.3944636026824995,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,8.0816420210378119,6.0272263520568741,4.4655077218849986,1.673557835300312,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,5.2383065537184361,1.3168814513771872,0,0,0,1.2937075620262499,0,65.816868437882164,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.797017316723744,9.490211469412186,5.9214325093678113,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,19.28974398363906,9.3672890998115612,7.0196733525209352,0,0,0,1.7491248657924996,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,21.119473681956556,9.1687996997187469,7.1002781850459353,0,0,0,1.6725502748937495,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,7.7088446706096851,4.5168933026196854,0,0,0,1.7954726444943745,0,36.913990615230304,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,6.9027963453596861,5.3068206613646858,0,0,0,1.5597035093587495,0,60.747832032466242,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.940598378172187,5.4680303264146852,4.3143736609006247,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,17.224245150185936,8.5602332141549979,6.8060705463296873,0,0,0,1.629225177411562,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.2312388168193749,1.0438325811987497,0,0,0,1.0327494167265621,12.426242494135311,18.537096359936868,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.0740593933956248,0.8886682785881248,0,0,0,0.88262291614874977,12.364781309334996,29.166858649171242,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.74156445922999981,0.65491426426562482,0,0,0,0.64383109979343733,7.5587181700318729,10.379887308406873,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.76776102980062488,0.63476305613437489,0,0,0,0.62771013328843728,8.7174126375787466,21.110405638297497,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.42216781034968731,0.3294722529459374,0,0,0,0.28513959505718739,0.73954933841687487,1.08413499746125,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.9697954088828107,14.350682870669685,8.4574620526856226,0,4.0443474719418742,2.9793561222053118,2.7667608764206246,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,9.0327790448328109,5.4871739741393748,0,0,0,2.6498838692593742,0,39.22533418788467,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",6.1924662587331234,16.180412568987183,10.05545285749375,0,5.0156357038681234,4.0292340658434362,3.832759786563749,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.6690423310371854,15.918446863280932,9.1375653271153112,0,4.3224341441531235,4.3224341441531235,3.6655047590743739,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,2.4624776336387497,2.4624776336387497,0,2.4624776336387497,2.4624776336387497,2.4624776336387497,0,0,22.992528477756242,9.0730814610953097,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,2.4624776336387497,2.4624776336387497,0,2.4624776336387497,2.4624776336387497,2.4624776336387497,0,0,22.992528477756242,9.0730814610953097,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,3.6221796615921869,3.6221796615921869,0,3.6221796615921869,3.6221796615921869,3.6221796615921869,0,0,37.752280873490299,25.167851395524682,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2020 TUOS Ex GST","index":13,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Transmission Use of System (TUOS) Tariffs: 1 January 2020 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,0,2.5045514488281246,2.0939330535156242,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,0,4.2066309261718731,3.3666293164062489,0,0,0,0,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,3.941715832421874,3.1502819898437489,0,0,0,0,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,0,2.8025809292968744,2.2418439808593744,2.2418439808593744,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,18.991100783203112,4.2287071839843744,0,0,0,0,0,12.042598636718747,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",0,2.9725681144531242,2.374301527734374,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,0,2.2164562843749991,1.7716196894531246,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,0,2.9449727921874995,2.3577443343749995,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,2.0530919765624995,1.6413697683593746,0,0,0,0,0,9.5755768261718739,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,1.2914610820312495,1.0320650527343747,0,0,0,0,0,11.572374345312493,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,0,2.9350384761718735,2.3456023925781242,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,0,2.2561935484374995,1.8069417019531244,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,1.2859420175781244,1.0320650527343747,0,0,0,0,5.2508379207031233,7.1769914148437479,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,0.81240628749999966,0.65124960546874966,0,0,0,0,3.3136462976562484,8.7123951457031197,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,0.90402275742187466,0.72410125624999977,0,0,0,0,6.0124688152343726,6.3116021085937479,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,0.51989587148437477,0.41392983398437488,0,0,0,0,3.447207657421874,6.9595402753906219,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,0.60930471562499988,0.49119673632812483,0,0,0,0,4.3225312796874986,5.2442150433593735,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",0,3.5277859984374991,2.9946443722656233,0,2.9946443722656233,2.6447356859374991,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,2.621555615234374,1.2042598636718744,0,0,0,0,0,6.8679238054687488,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",0,5.4451089894531224,5.0620859164062475,0,5.0620859164062475,4.8104165773437471,0,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",0,4.6040035667968739,4.2949359574218731,0,2.3003460640624991,2.0299119058593744,0,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,1.0695946910156249,1.0695946910156249,0,1.0695946910156249,1.0695946910156249,1.0695946910156249,0,0,5.9826658671874968,5.946240041796873,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,1.0695946910156249,1.0695946910156249,0,1.0695946910156249,1.0695946910156249,1.0695946910156249,0,0,5.9826658671874968,5.946240041796873,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,0.99453541445312466,0.99453541445312466,0,0.99453541445312466,0.99453541445312466,0.99453541445312466,0,0,10.367010668749996,6.912076321093747,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"2020 NUOS Ex GST","index":14,"n_rows":40,"n_cols":21,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,1,1,19],[3,4,3,16],[3,17,3,18],[26,17,26,18]]}
[]
[null,"Schedule of Indicative Network Use of System (NUOS) Tariffs: 1 January 2020 (GST Exclusive)"]
[]
[null,null,null,null,"Network Tariff Component",null,null,null,null,null,null,null,null,null,null,null,null,"Eligibility (consumption/   category)",null,"Minimum Chargeable Rolling Demand","Minimum Chargeable Demand"]
[null,"Description","Tariff Code","PFIT (F)\nTFIT (T)","Standing Charge (c/day)","Summer Peak Energy (c/kWh)","Non Summer Peak Energy Block 1 (c/kWh)","Non Summer Peak Energy Block 2 (c/kWh)","Summer Shoulder Energy (c/kWh)","Non Summer Shoulder Energy (c/kWh)","Off Peak Energy (c/kWh)","Rolling Peak Demand c/kVA/day","Summer Demand Incentive Charge c/kW/day or c/kVA/day","Summer Demand Max kW  c/KW/day","Non-summer Demand Max kW  c/KW/day","Summer Demand Overrun Max kW  c/KW/day","Non-summer Demand Overrun Max kW  c/KW/day","kVA","MWh pa","kVA","kW"]
[null,"Low voltage small 1 rate","LVS1R",null,6.2750862120712476,10.242615371228123,7.0753117035606223,0,0,0,0,0,0,0,0,0,0,"NA","<20"]
[null,"Low voltage small 2 rate*","LVS2R*",null,12.817175931881559,13.405657438087498,10.343985131851561,0,0,0,1.5949681235884372,0,0,0,0,0,0]
[null,"Dedicated circuit**","LVDed**",null,0,0,0,0,0,0,1.7652458322974995,0,0,0,0,0,0,"NA","<20 (on LVS1R)"]
[null,"Unmetered supplies","UnMet",null,0,11.674741952789059,8.806726112285622,0,0,0,1.3944636026824995,0,0,0,0,0,0]
[null,"Winter Energy Tariff*","WET2Step*",null,8.0816420210378119,8.829807281353748,6.707351702744373,3.9154018161596866,0,0,0,0,0,0,0,0,0]
[null,"Reverse cycle airconditioning time of use*","RCACkWTOU*",null,0,24.229407336921547,5.5455886353615611,0,0,0,1.2937075620262499,0,77.859467074600914,0,0,0,0]
[null,"Low voltage medium 1 rate","LVM1R","F",10.797017316723744,12.462779583865309,8.2957340371021857,0,0,0,0,0,0,0,0,0,0,"NA",">20 & <400"]
[null,"Low voltage medium 2 rate 5 day*","LVM2R5D*",null,19.28974398363906,11.58374538418656,8.7912930419740594,0,0,0,1.7491248657924996,0,0,0,0,0,0]
[null,"Low voltage medium 2 rate 7 day*","LVM2R7D*",null,21.119473681956556,12.113772491906246,9.4580225194209344,0,0,0,1.6725502748937495,0,0,0,0,0,0]
[null,"Low voltage KW time of use*","LVkWTOU*",null,0,9.7619366471721847,6.1582630709790598,0,0,0,1.7954726444943745,0,46.48956744140218,0,0,0,0]
[null,"Low voltage KW time of use - HOT*","LVkWTOUH*",null,0,8.1942574273909354,6.3388857140990602,0,0,0,1.5597035093587495,0,72.320206377778732,0,0,0,0]
[null,"Low voltage large 1 rate*","LVL1R*",null,11.940598378172187,8.4030688025865583,6.6599760534787489,0,0,0,0,0,0,0,0,0,0]
[null,"Low voltage large 2 rate*","LVL2R*",null,17.224245150185936,10.816426762592497,8.6130122482828124,0,0,0,1.629225177411562,0,0,0,0,0,0]
[null,"Low voltage large KVA time of use","LVkVATOU",null,0,2.5171808343974993,2.0758976339331241,0,0,0,1.0327494167265621,17.677080414838436,25.714087774780616,0,0,0,0,">150",">400",150]
[null,"Low voltage large KVA time of use - HOT*","LVkVATOUH*",null,0,1.8864656808956246,1.5399178840568744,0,0,0,0.88262291614874977,15.678427606991244,37.879253794874359,0,0,0,0,null,null,150]
[null,"High voltage KVA time of use","HVkVATOU",null,0,1.6455872166518746,1.3790155205156247,0,0,0,0.64383109979343733,13.571186985266245,16.691489417000621,0,0,0,0,">150",">400",1150]
[null,"High voltage KVA time of use - HOT*","HVkVATOUH*",null,0,1.2876569012849997,1.0486928901187498,0,0,0,0.62771013328843728,12.164620295000621,28.06994591368812,0,0,0,0,null,null,1150]
[null,"Subtransmission KVA time of use*","SubTkVATOU*",null,0,1.0314725259746873,0.82066898927406218,0,0,0,0.28513959505718739,5.0620806181043738,6.3283500408206237,0,0,0,0,null,null,11100]
[null,"Time of Day","TOD","F",5.9697954088828107,17.878468869107184,11.452106424951246,0,7.0389918442074979,5.6240918081428113,2.7667608764206246,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Use","TOU","F",0,11.654334660067185,6.6914338378112497,0,0,0,2.6498838692593742,0,46.093257993353419,0,0,0,0,"NA",">20 & <400"]
[null,"Time of Day 9pm off-peak","TOD9","F",6.1924662587331234,21.625521558440305,15.117538773899998,0,10.077721620274371,8.8396506431871842,3.832759786563749,0,0,0,0,0,0,"NA","<20"]
[null,"Time of Day Flexible","TODFLEX","F",6.6690423310371854,20.522450430077807,13.432501284537185,0,6.6227802082156231,6.352346050012498,3.6655047590743739,0,0,0,0,0,0,"Residential Customer"]
[null,"Residential KW time of use","RESKWTOU","F",0,3.5320723246543748,3.5320723246543748,0,3.5320723246543748,3.5320723246543748,3.5320723246543748,0,0,28.975194344943738,15.019321502892183,0,0,"NA","<20",null,1.5]
[null,"Residential KW 1 rate1","RESKW1R1","F",0,3.5320723246543748,3.5320723246543748,0,3.5320723246543748,3.5320723246543748,3.5320723246543748,0,0,28.975194344943738,15.019321502892183,0,0,"NA","<20",null,1.5]
[null,"Low Voltage Medium kW Time of Use2","LVMKWTOU2","F",0,4.6167150760453115,4.6167150760453115,0,4.6167150760453115,4.6167150760453115,4.6167150760453115,0,0,48.119291542240298,32.079927716618428,0,0,"NA",">20 & <400",null,1.5]
[]
[]
[null,"* Tariff closed to premises not already taking supply under this tariff and new connections."]
[null,"** Tariff only available in conjunction with the LVS1R tariff for new connections."]
[null,"Summer peak energy rates apply for period 1st November to 31st March (except TODFLEX which follows daylight savings periods) & RESKWTOU which applies from 1st December to 31st March."]
[null,"Non-summer peak energy rates apply for period 1st April to 31st October (except TODFLEX which follows non-daylight savings periods) & RESKWTOU which applies from 1st April to 30th November."]
[null,"PFIT (Premium Feed-In Tariff) is defined by an “F” added to the front of an existing distribution tariff ie. FTOD. The PFIT tariffs are closed to new connections. "]
[null,"TFIT (Transitional Feed-In Tariff) is defined by a “T” added to the front of an existing distribution tariff ie. TTOD. The TFIT tariffs are closed to new connections."]
[null,"1 RESKWTOU csutomers will be transitioned to RESKW1R by 1 April 2016."]
[null,"2 LVMKWTOU available from 1st July 2016 for low voltage business customers with energy consumption between 20-400MWh per annum. "]

{"sheet":"PFIT TFIT Ex GST","index":15,"n_rows":29,"n_cols":3,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,0,0,2],[31,0,31,2],[32,0,32,2]]}
["UED PFIT/TFIT pass through charge: 1 January 2016 (GST Exclusive)"]
["UED Network Tariff Description","UED Tariff Code","PFIT/TFIT Pass Through Charge (c/cust/day)"]
["Low voltage small 1 rate","LVS1R",8.843]
["Low voltage small 2 rate*","LVS2R*",8.843]
["Dedicated circuit**","LVDed**"]
["Unmetered supplies","UnMet"]
["Winter Energy Tariff*","WET2Step*",8.843]
["Reverse cycle airconditioning time of use*","RCACkWTOU*",8.843]
["Low voltage medium 1 rate","LVM1R",8.843]
["Low voltage medium 2 rate 5 day*","LVM2R5D*",8.843]
["Low voltage medium 2 rate 7 day*","LVM2R7D*",8.843]
["Low voltage KW time of use*","LVkWTOU*",8.843]
["Low voltage KW time of use - HOT","LVkWTOUH*",8.843]
["Low voltage large 1 rate*","LVL1R*",8.843]
["Low voltage large 2 rate*","LVL2R*",8.843]
["Low voltage large KVA time of use","LVkVATOU",8.843]
["Low voltage large KVA time of use - HOT*","LVkVATOUH*",8.843]
["High voltage KVA time of use","HVkVATOU",8.843]
["High voltage KVA time of use - HOT*","HVkVATOUH*",8.843]
["Subtransmission KVA time of use*","SubTkVATOU*",8.843]
["Time of Day","TOD",8.843]
["Time of Use","TOU",8.843]
["Time of Day 9pm off-peak","TOD9",8.843]
["Time of Day Flexible","TODFLEX",8.843]
["Residential KW time of use","RESKWTOU",8.843]
["Residential KW 1 rate","RESKW1R",8.843]
["Low Voltage Medium kW Time of Use","LVMKWTOU",8.843]
[]
["* Tariff closed to premises not already taking supply under this tariff and new connections."]

{"sheet":"Prescribed Ex GST","index":16,"n_rows":4,"n_cols":2,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["2016 Prescribed Metering Service Charges (GST Exclusive)"]
[]
["Metering Data Services (Unmetered Supplies)","$/light/annum"]
["Per light",1.3220000000000001]