{"text_format":"1","workbook":"xlsx","n_sheets":42,"sheets":["AER Sheet Heading","AER CF","AER NRs","AER lookups","AER ETL","Instructions","CONTENTS","Business & other details","CPI series","2.1 Expenditure summary","2.2 Repex","2.3 Augex (a)","2.3 Augex (b)","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.4 MD & utilisation-Spatial","6.1 Telephone answering","6.2 Reliability & Cust serv","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.3(b) Obligations cont.","7.4 Shared Assets","7.7 TSS-LRMC","8.2 Capex","Sheet1"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":2,"defined_names":861,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AER Sheet Heading","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":true,"merged":[[10,2,10,8],[11,2,11,8],[41,2,41,8],[42,2,42,8]]}
[null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"XX"]
[]
[]
[]
[]
[]
[]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"VOLUMES"]
[null,null,"0's"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]

{"sheet":"AER CF","index":1,"n_rows":67,"n_cols":24,"rows_kept":67,"cut":false,"hidden":true,"merged":[[33,37,33,58],[33,68,33,89],[3,1,3,21],[31,37,31,58],[31,68,31,89],[32,37,32,58],[32,68,32,89]]}
[null,"AER CONDITIONAL FORMATTING"]
[]
[]
[null,"CONDITIONAL FORMATTING MAP"]
[null,null,null,null,null,"=INDEX(dms_CF_3.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.5, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.6, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.2, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.3, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.7.4, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_3.6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.6.1, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_6.8, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_7.12, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_A, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_B, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_8.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\"","=INDEX(dms_CF_4.4.1_Neg, MATCH(dms_TradingName,dms_CF_TradingName))=\"Y\""]
[null,"dms_CF_TradingName","JurisdictionList","Sector","Segment","dms_CF_3.6.1","dms_CF_3.6.5","dms_CF_3.6.6","dms_CF_3.6.7.1","dms_CF_3.6.7.2","dms_CF_3.6.7.3","dms_CF_3.6.7.4","dms_CF_3.6.8","dms_CF_4.1","dms_CF_6.6.1","dms_CF_6.8","dms_CF_7.12","dms_CF_8.1_A","dms_CF_8.1_B","dms_CF_8.1_Neg","dms_CF_4.4.1","dms_CF_MAIFI_flag","Spare1","Spare2"]
[null,"ActewAGL Distribution","ACT","Electricity","Distribution",null,"Y",null,"Y","Y","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Ausgrid","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"AusNet (D)","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"AusNet (T)","Vic","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"CitiPower","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Directlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"ElectraNet","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"Endeavour Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","Y","N","N","N"]
[null,"Energex","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","Y","N","N","N"]
[null,"Ergon Energy","Qld","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Essential Energy","NSW","Electricity","Distribution",null,"Y",null,"N","N","N","Y","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Jemena Electricity","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Murraylink","SA","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"Power and Water","NT","Electricity","Distribution",null,"N",null,"N","Y","N","N","Y","Y","Y","Y","Y","N","Y","Y","N","N","N","N"]
[null,"Powercor Australia","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[null,"Powerlink","Qld","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"SA Power Networks","SA","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","Y","N","Y","Y","Y","Y","N","N","N","N","N"]
[null,"TasNetworks (D)","Tas","Electricity","Distribution",null,"Y",null,"N","N","N","N","N","N","N","Y","Y","N","Y","Y","N","N","N","N"]
[null,"TasNetworks (T)","Tas","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"TransGrid","NSW","Electricity","Transmission",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","Y","Y","N","N","N","N"]
[null,"United Energy","Vic","Electricity","Distribution",null,"N",null,"N","N","N","N","N","Y","N","Y","N","N","N","Y","N","N","N","N"]
[]
[]
[null,"Confidential"]
[null,"Amended"]
[]
[null,"Worksheet 6.2 STPIS reliability"]
[null,"Formula",null,null,null,"Applied to:"]
[]
[null,"=INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$11,$D$17,$D$23,$D$33,$D$39,$D$45,$D$55,$D$61,$D$67,$D$77,$D$83,$D$89"]
[null,"=INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$12,$D$18,$D$24,$D$56,$D$62,$D$78,$D$68,$D$84"]
[null,"=INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$13,$D$19,$D$25,$D$57,$D$63,$D$69,$D$79,$D$85"]
[null,"=INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$14,$D$20,$D$26,$D$58,$D$64,$D$65,$D$70,$D$71,$D$80,$D$86"]
[null,"=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))=\"NO\"",null,null,null,"$D$87,$D$81,$D$71,$D$65,$D$59,$D$49,$D$43,$D$37,$D$21,$D$15"]
[null,"=dms_MAIFI_Flag=\"No\"",null,null,null,"$D$55:$D$72"]
[]
[]
[null,"Business & other details"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))>1)"]
[null,"=(INDEX(dms_Model_Span,MATCH(dms_Model,dms_Model_List))=1)"]
[]
[]
[null,"STYLES IN USE"]
[null,"HEADING ONE","dms_1"]
[null,"HEADING TWO","dms_2"]
[null,"HEADING THREE","dms_3"]
[null,"HEADING FOUR","dms_4"]
[null,"HEADING FIVE","dms_5"]
[null,null,"dms_NUM"]
[null,null,"dms_NUM%"]
[null,null,"dms_Row_Locked"]
[null,null,"dms_Row1"]
[null,null,"dms_Row2"]
[null,null,"dms_T1"]
[null,null,"dms_T2"]
[null,null,"dms_BH"]
[null,null,"dms_BY1"]
[null,null,"dms_BY2"]
[null,null,"dms_GH"]
[null,null,"dms_GY1"]
[null,null,"dms_GY2"]

{"sheet":"AER NRs","index":2,"n_rows":226,"n_cols":15,"rows_kept":226,"cut":false,"hidden":true,"merged":[[193,1,194,1],[197,1,198,1],[206,1,211,1],[133,1,148,1],[150,1,156,1],[158,1,172,1],[174,1,175,1],[177,1,182,1],[189,1,190,1],[116,1,130,1],[4,1,26,1],[30,1,53,1],[31,10,33,10],[31,36,31,57],[34,10,38,10],[42,10,43,10],[63,1,76,1],[82,1,95,1],[98,1,105,1],[108,1,113,1],[31,67,31,88],[32,36,32,57],[32,67,32,88],[33,36,33,57],[33,67,33,88]]}
[null,"AER NAMED RANGES"]
[]
[null,"DROP DOWN SELECTORS USED IN WORKBOOKS"]
[]
[null,"COVER SHEET","dms_DataQuality_List","dms_Confid_status_List"]
[null,null,"-- select --","-- select --"]
[null,null,"Actual","Public"]
[null,null,"Estimate","Confidential"]
[null,null,"Consolidated"]
[]
[]
[null,null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above."]
[null,null,"dms_SourceList","dms_FormControl_Choices"]
[null,null,"-- select --","Revenue cap"]
[null,null,"After appeal","Revenue yield"]
[null,null,"Draft decision","Weighted average price cap"]
[null,null,"Final decision"]
[null,null,"PTRM update 1"]
[null,null,"PTRM update 2"]
[null,null,"PTRM update 3"]
[null,null,"PTRM update 4"]
[null,null,"PTRM update 5"]
[null,null,"PTRM update 6"]
[null,null,"PTRM update 7"]
[null,null,"Regulatory proposal"]
[null,null,"Reporting"]
[null,null,"Revised regulatory proposal"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"This is used to create an image to insert on 6.3 STPIS sheet - not for dropdown lists.",null,null,"GAS"]
[null,"CA & RESET RINS \nDNSP","dms_DNSP_020301_SubstationType","dms_DNSP_020301_ProjectType","dms_DNSP_020301_ProjectTrigger","dms_DNSP_020302_ProjectType","dms_DNSP_020302_ProjectTrigger","dms_STPIS_Exclusion_List","dms_Reason_Interruption","dms_Reason_Interruption_Detailed","Reason for interruption",null,null,"dms_N0205_AssetType"]
[null,null,"Subtransmission substation","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth","Weather","Animal","Animal impact","Animal","Animal impact",null,"Cast Iron"]
[null,null,"Zone substation","Substation upgrade - capacity"," Voltage issues","New line on new route - dual circuit"," Voltage issues","Equipment failure","Asset failure","Animal nesting/burrowing, etc and other",null,"Animal nesting/burrowing, etc and other",null,"PVC"]
[null,null,"Switching station","Substation upgrade - voltage"," Reactive power issue","New line on new route - other"," Reactive power issue","Operational error","Other","Other",null,"Other",null,"Polyamide"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues","Vegetation","Overloads","LV","Asset failure","LV",null,"High density polyethylene (80)"]
[null,null,null,null," Safety","Line rebuild over existing route - dual circuit"," Net market benefit","Animals","Planned","Distribution substation",null,"Distribution substation",null,"High density polyethylene (100)"]
[null,null,null,null," Environment","Reconductor - Single circuit"," Safety","Third party impacts","Network business","HV",null,"HV",null,"High density polyethylene (250)"]
[null,null,null,null," Other","Reconductor - Dual circuit"," Environment","Transmission failure","Third party","Zone substation",null,"Zone substation",null,"High density polyethylene (575)"]
[null,null,null,null,null,"Reconductor - Other"," Other","Load shedding","Unknown","Subtransmission",null,"Subtransmission",null,"Medium density polyethylene"]
[null,null,null,null,null,"Line upgrade - raising/retensoring",null,"Inter-distributor connection failure","Vegetation","insert description of 'other'","Other","insert description of 'other'",null,"Unprotected steel"]
[null,null,null,null,null,"Line upgrade - voltage upgrade",null,"Other","Weather","Network error","Overloads",null,null,"Protected steel"]
[null,null,null,null,null,"Line upgrade - capacity",null,null,"2 - STPIS Exclusion (3.3)(a)","Switching and protection error","Planned",null,null,"Other"]
[null,null,null,null,null,"String spare circuit",null,null,"3 - STPIS Exclusion (3.3)(a)","Fire","Network business","Network error"]
[null,null,null,null,null,"Other",null,null,"4 - STPIS Exclusion (3.3)(a)","Other",null,"Switching and protection error"]
[null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)","Dig-in","Third party","Fire"]
[null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)","Unauthorised access",null,"Other"]
[null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)","Vehicle impact",null,"Dig-in"]
[null,null,null,null,null,null,null,null,null,"Unknown",null,"Unauthorised access"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - NSP responsibility",null,"Vehicle impact"]
[null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility","Unknown","Unknown"]
[null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party","Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party",null,"Grow-in - NSP responsibility"]
[null,null,null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,null,null,null,null,null,null,null,null,null,"Weather"]
[null,null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[]
[]
[null,"CA & RESET RINS \nTNSP ","dms_TNSP_0203_SubstationType","dms_TNSP_020301_ProjectType","dms_TNSP_020301_ProjectTrigger","dms_TNSP_020302_ProjectType","dms_TNSP_0203_ProjectTrigger"]
[null,null,"Terminal station","New substation establishment","Demand growth","New line on new route - single circuit","Demand growth"]
[null,null,"Switching station","Capacity upgrade"," Voltage issues","New line on new route - dual circuit"," Voltage issues"]
[null,null,"Transmission substation","Voltage upgrade"," Reactive power issue","New line on new route - other"," Reactive power issue"]
[null,null,"Other","Other"," Fault level issues","Line rebuild over existing route - single circuit"," Fault level issues"]
[null,null,null,null,"Net market benefit","Line rebuild over existing route - dual circuit"," Net market benefit"]
[null,null,null,null," Safety","Reconductor - Single circuit"," Safety"]
[null,null,null,null," Environment","Reconductor - Dual circuit"," Environment"]
[null,null,null,null," Other","Reconductor - Other"," Other"]
[null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,"Other"]
[]
[]
[]
[null,"NAMED RANGES USED IN ETL PROCESS"]
[]
[null,"CA & RESET RINS \nDNSP ONLY","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_020701_01_Rows","dms_040102_01_UOM","dms_040102_04_UOM","dms_S140101_UOM","dms_S140102_UOM","dms_S140201_UOM"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Route line length within zone","0's","days","number","number","number per km"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","0's","0's","Number of maintenance spans","0's","0's","number","number","number"]
[null,null,"Circuit line length in km","MVA added","MVA added","MVA added","MVA added","km","km","Total length of maintenance spans","0's","$0s","number","number","number"]
[null,null,"Circuit line length in km","0's","0's","0's","0's","km","km","Length of vegetation corridors","$0s","0's","km","number"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","0's","0's","Average number of trees per maintenance span"]
[null,null,"Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added","years","years","Average frequency of cutting cycle"]
[null,null,"Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added"]
[null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s"]
[null,null,null,"0's",null,"$0s"]
[null,null,null,"0's"]
[null,null,null,"0's"]
[null,null,null,"$0s"]
[]
[]
[null,"CA & RESET RINS \nTNSP ONLY","dms_020701_01_UOM"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"0's"]
[null,null,"km"]
[null,null,"metres"]
[null,null,"years"]
[]
[]
[null,"CA & RESET RINS \nDNSP & TNSP","dms_020603_01_UOM"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"0's"]
[null,null,"(per cent)"]
[]
[]
[null,"EB & RESET RINS \nDNSP ONLY","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM"]
[null,null,"minutes/customer","minutes/customer","Customer / km","%","km"]
[null,null,"minutes/customer","minutes/customer","MWh/customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer","kVA / customer","Number of spans"]
[null,null,"interruptions/customer","interruptions/customer",null,"Number of spans"]
[null,null,null,null,null,"Number of spans"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Years"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Trees"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Defects"]
[null,null,null,null,null,"Spans"]
[null,null,null,null,null,"km"]
[null,null,null,null,null,"Spans"]
[]
[null,null,"WHEN INSERTING COVER SHEET INTO A TNSP FILE - APPLY THESE NAMED RANGES"]
[null,"EB & RESET RINS \nTNSP ONLY","dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM"]
[null,null,"%",null,"Number of spans","km"]
[null,null,"number",null,"Years","%"]
[null,null,"number",null,"Trees","km"]
[null,null,"%",null,"Defects","number"]
[null,null,"number",null,"Number of spans"]
[null,null,"number",null,"km"]
[null,null,"%",null,"km"]
[null,null,"number",null,"Number of spans"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[null,null,"%"]
[null,null,"number"]
[]
[null,"EB & RESET RINS \nDNSP & TNSP","dms_EB_RAB_PIT"]
[null,null,"Beginning of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[null,null,"End of year"]
[]
[null,"ARR \nDNSP ONLY","dms_030605_UOM","dms_03060703_UOM","Spare","Spare"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","number"]
[null,null,"number","(per cent)"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"number"]
[null,null,"(per cent)"]
[null,null,"(per cent)",""]
[]
[null,"RFM","dms_Beg","dms_Mid","dms_End"]
[null,null,"Beginning of year","Mid year","End of Year"]
[]
[null,"PTRM","dms_PTRM_RAB_PIT","dms_PTRM_TAB_PIT","DMS_Xfactor"]
[null,null,"Beginning of year","Beginning of year","x factors"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year","End of year"]
[null,null,"End of year"]
[]
[]
[null,"STPIS & MIC NAMED RANGES "]
[]
[null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[]
[null,"Table 6.3 sustained interruptions - row descriptions","dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[]
[]
[null,"Table 6.1 telephone answering - row descriptions and start date","dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":"2015-01-01"}]
[]
[]
[null,"Table 6.8.1 - row descriptions","dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[]
[]
[null,"Table 7.9.4 - market impact component - row descriptions","dms_070904_01_Rows","without exclusions","with exclusions"]
[]
[]
[null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[]
[null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values","dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[]
[null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[]
[null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[]
[]
[null,"Use these to add to specific worksheets in existing files","Use these to add to specific worksheets in existing files"]
[]
[]
[null,"ARRs 6.7 STPIS daily performance","dms_060101_Values","dms_060102_Values","dms_060701_Values"]
[null,null,"dms_LeapYear"]
[]
[]
[null,"ARR's  6.8 STPIS exclusions","dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,"dms_060801_StartCell"]
[]
[]
[null,"CA 6.3 sustained interruptions","dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]

{"sheet":"AER lookups","index":3,"n_rows":88,"n_cols":38,"rows_kept":88,"cut":false,"hidden":true,"merged":[[22,1,22,4],[6,25,6,36],[8,25,8,28],[8,31,8,35],[8,36,10,36]]}
[null,"AER LOOKUP TABLES"]
[]
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,"2018-03-28","major changes to accommodate STPIS"]
[null,null,"Template Version",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_PRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_Public_Lighting_List","Name"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,"NO","YES","YES","YES","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES",{"$f":"B13","v":"AusNet (D)"}]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","Vic",3000,"NO","NO","NO","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co. (Vic)"]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","Vic",8001,"YES","YES","NO","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","CitiPower"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","Vic",3000,"PO Box 16182",null,"MELBOURNE","Vic",8001,"NO","YES","YES","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Jemena Electricity"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","Vic",8001,"NO","NO","YES","YES","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","Powercor Australia"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,2,"2016-20 Distribution Determination","43-45 Centreway",null,"MOUNT WAVERLEY","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","Vic",3170,"NO","NO","YES","NO","NO","YES","CBD","Urban","Short rural","Long rural",null,"YES","United Energy"]
[]
[]
[]
[]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68"]
[null,"dms_Model_List ","dms_Model_Name_Format1","dms_Worksheet_List","dms_Model_Span_List"]
[null,"ARR","Annual Reporting",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ANNUAL REPORTING\",\"ANNUAL REPORTING\")","v":"ANNUAL REPORTING"},1]
[null,"CA","Category Analysis",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL CATEGORY ANALYSIS\",\"CATEGORY ANALYSIS\")","v":"CATEGORY ANALYSIS"},1]
[null,"CESS","Capitlal Expenditure","CAPITLAL EXPENDITURE SHARING SCHEMING",5]
[null,"CPI","CPI","CPI",5]
[null,"EB","Economic Benchmarking",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",\"NEW HISTORICAL ECONOMIC BENCHMARKING\",\"ECONOMIC BENCHMARKING\")","v":"ECONOMIC BENCHMARKING"},1]
[null,"Pricing","Pricing Proposal","PRICING PROPOSAL",5]
[null,"PTRM","Post Tax Revenue Model","POST TAX REVENUE MODEL",5]
[null,"Reset","Regulatory Reporting (Reset)","REGULATORY REPORTING STATEMENT",5]
[null,"RFM","Roll Forward Model","ROLL FORWARD MODEL",5]
[null,"WACC","Weighted Average Cost of Capital","WEIGHTED AVERAGE COST OF CAPITAL",1]
[]
[]
[]
[null,"Financial","Calendar",null,"PREVIOUS",null,"CURRENT",null,"FORTHCOMING"]
[null,"1987-88","1988","PRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2011-12"},"CRCP_y1",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2016-17"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2021-22"}]
[null,"1988-89","1989","PRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+1)","v":"2012-13"},"CRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+1)","v":"2017-18"},"FRCP_y2",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+1)","v":"2022-23"}]
[null,"1989-90","1990","PRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+2)","v":"2013-14"},"CRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+2)","v":"2018-19"},"FRCP_y3",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+2)","v":"2023-24"}]
[null,"1990-91","1991","PRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+3)","v":"2014-15"},"CRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+3)","v":"2019-20"},"FRCP_y4",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+3)","v":"2024-25"}]
[null,"1991-92","1992","PRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+4)","v":"2015-16"},"CRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+4)","v":"2020-21"},"FRCP_y5",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+4)","v":"2025-26"}]
[null,"1992-93","1993","PRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+5)","v":"2016-17"},"CRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+5)","v":"2021-22"},"FRCP_y6",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+5)","v":"2026-27"}]
[null,"1993-94","1994","PRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+6)","v":"2017-18"},"CRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+6)","v":"2022-23"},"FRCP_y7",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+6)","v":"2027-28"}]
[null,"1994-95","1995","PRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+7)","v":"2018-19"},"CRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+7)","v":"2023-24"},"FRCP_y8",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+7)","v":"2028-29"}]
[null,"1995-96","1996","PRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+8)","v":"2019-20"},"CRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+8)","v":"2024-25"},"FRCP_y9",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+8)","v":"2029-30"}]
[null,"1996-97","1997","PRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+9)","v":"2020-21"},"CRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+9)","v":"2025-26"},"FRCP_y10",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+9)","v":"2030-31"}]
[null,"1997-98","1998","PRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+10)","v":"2021-22"},"CRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+10)","v":"2026-27"},"FRCP_y11",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+10)","v":"2031-32"}]
[null,"1998-99","1999","PRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+11)","v":"2022-23"},"CRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+11)","v":"2027-28"},"FRCP_y12",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+11)","v":"2032-33"}]
[null,"1999-00","2000","PRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+12)","v":"2023-24"},"CRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+12)","v":"2028-29"},"FRCP_y13",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+12)","v":"2033-34"}]
[null,"2000-01","2001","PRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+13)","v":"2024-25"},"CRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+13)","v":"2029-30"},"FRCP_y14",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+13)","v":"2034-35"}]
[null,"2001-02","2002","PRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+14)","v":"2025-26"},"CRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+14)","v":"2030-31"},"FRCP_y15",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+14)","v":"2035-36"}]
[null,"2002-03","2003","PRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+15)","v":"2026-27"},"CRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+15)","v":"2031-32"},"FRCP_y16",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+15)","v":"2036-37"}]
[null,"2003-04","2004"]
[null,"2004-05","2005"]
[null,"2005-06","2006",null,"CRY - FRY"]
[null,"2006-07","2007","dms_y1",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row),0)","v":"2019-20"}]
[null,"2007-08","2008","dms_y2",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+1),0)","v":"2020-21"}]
[null,"2008-09","2009","dms_y3",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+2),0)","v":"2021-22"}]
[null,"2009-10",2010,"dms_y4",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+3),0)","v":"2022-23"}]
[null,"2010-11",2011,"dms_y5",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+4),0)","v":"2023-24"}]
[null,"2011-12",2012,"dms_y6",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+5),0)","v":"2024-25"}]
[null,"2012-13",2013,"dms_y7",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+6),0)","v":"2025-26"}]
[null,"2013-14",2014,"dms_y8",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+7),0)","v":"2026-27"}]
[null,"2014-15",2015,"dms_y9",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+8),0)","v":"2027-28"}]
[null,"2015-16",2016,"dms_y10",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+9),0)","v":"2028-29"}]
[null,"2016-17",2017,"dms_y11",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+10),0)","v":"2029-30"}]
[null,"2017-18",2018,"dms_y12",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+11),0)","v":"2030-31"}]
[null,"2018-19",2019,"dms_y13",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+12),0)","v":"2031-32"}]
[null,"2019-20",2020,"dms_y14",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+13),0)","v":"2032-33"}]
[null,"2020-21",2021,"dms_y15",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+14),0)","v":"2033-34"}]
[null,"2021-22",2022,"dms_y16",{"$f":"IFERROR(INDEX(INDIRECT(dms_RPT),dms_CRY_start_row+15),0)","v":"2034-35"}]
[null,"2022-23",2023]
[null,"2023-24",2024]
[null,"2024-25",2025]
[null,"2025-26",2026]
[null,"2026-27",2027]
[null,"2027-28",2028]
[null,"2028-29",2029]
[null,"2029-30",2030]
[null,"2030-31",2031]
[null,"2031-32",2032]
[null,"2032-33",2033]
[null,"2033-34",2034]
[null,"2034-35",2035]
[null,"2035-36",2036]
[null,"2036-37","2037"]

{"sheet":"AER ETL","index":4,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":true,"merged":[[71,1,73,1],[32,68,32,89],[33,37,33,58],[33,68,33,89],[34,0,59,0],[34,37,34,58],[34,68,34,89],[32,37,32,58],[11,0,15,0],[12,4,12,8],[14,2,14,4],[18,0,25,0],[26,0,31,0]]}
[null,"AER ETL INFORMATION"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Full trading name",{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"},null,"dms_TradingNameFull"]
[null,"Trading name",{"$f":"dms_TradingName","v":"United Energy"}]
["Selected here","Model / RIN","Reset","dms_Model"]
["Read from Business & other details","Source","Regulatory proposal","dms_Source"]
[null,"Data quality",{"$f":"dms_Selected_Quality","v":"Consolidated"},"dms_DQ_1"]
[null,"Data status",{"$f":"dms_Selected_Status","v":"Public"},"dms_DQ_2"]
[null,"Amendment reason",{"$f":"dms_Amendment_Text","v":"."},null,null,"dms_AmendmentReason"]
[null,"Submission date",{"$f":"dms_Typed_Submission_Date","v":"2020-01-31"},"dms_SubmissionDate"]
[]
["Redundant","EBSS - First application of scheme in forthcoming period?","No"]
["Pre-populated from lookup table","Data ingestion data quality",{"$f":"dms_Selected_Quality","v":"Consolidated"},"dms_DataQuality","=IF(dms_DQ_2=\"Confidential\",\"Consolidated\",\"Public\")"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"dms_RYE_result","v":"2026"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an ABC RIN apply the NAMED RANGE to the cell"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
["Relevant for PTRM, RFMs and Reset RINS","$ REAL REFERENCES"]
[null,"Does the named range CRY exist in this file? ",{"$f":"IFERROR(CRY,\"NO\")","v":"NO"}]
[null,"CRY-1  (last full calendar year before CRY)",{"$f":"IFERROR(IF(dms_RPT=\"calendar\",CRY-1,LEFT(CRY,4)),\"CRY not present\")","v":"CRY not present"},"dms_Cal_Year_B4_CRY","'=IF(dms_RPT=\"financial\",VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)),VALUE(LEFT(dms_SingleYear_FinalYear_Result,4)-1))"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&dms_DollarReal_year)","v":"June 2021"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_RYE,2)&RIGHT(dms_RYE,2))))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"IF(dms_SingleYearModel=\"yes\",CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&dms_Previous_DollarReal_year)","v":"June 2016"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
["All potential values for Regulatory Years or RYEs as calculated","This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"dms_start_year",{"$f":"FRCP_y1","v":"2021-22"},"=FRCP_y1","FRCP_y1 from cover sheet"]
[null,"dms_CRY_start_year",{"$f":"IFERROR(CRY,CRCP_y4)","v":"2019-20"},"=IFERROR(CRY,CRCP_y4)"]
[null,"dms_CRY_start_row",{"$f":"IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)","v":33},"=IFERROR(MATCH(dms_CRY_start_year,INDIRECT(dms_RPT),0),0)"]
[null,"dms_FRCP_start_row",{"$f":"MATCH(dms_start_year,INDIRECT(dms_RPT),0)","v":35},"=MATCH(dms_start_year,INDIRECT(dms_RPT),0)","Uses FRCP_y1 as a start reference"]
[null,"dms_CRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num","v":30},"=dms_FRCP_start_row-dms_CRCPlength_Num","Uses the value in dms_CRCPlength_Num"]
[null,"dms_PRCP_start_row",{"$f":"dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","v":25},"=dms_FRCP_start_row-dms_CRCPlength_Num-dms_PRCPlength_Num","Uses the value in dms_CRCPlength_Num and dms_PRCPlength_Num"]
[null,"dms_RYE_start_row",{"$f":"dms_FRCP_start_row+(dms_FRCPlength_Num-1)","v":39},"=dms_FRCP_start_row+(dms_FRCPlength_Num-1)","Uses the value in dms_FRCPlength_Num-1"]
[null,"FRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","v":"2021-22"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row)","Converts the FRCP start row to display the year"]
[null,"CRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","v":"2016-17"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row)","Converts the CRCP start row to display the year"]
[null,"PRCP_start_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","v":"2011-12"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row)","Converts the PRCP start row to display the year"]
[null,"FRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_FRCP_start_row+dms_FRCPlength_Num-1)","Finds the FRCP final year"]
[null,"CRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","v":"2020-21"},"=INDEX(INDIRECT(dms_RPT),dms_CRCP_start_row+dms_CRCPlength_Num-1)","Finds the CRCP final year"]
[null,"PRCP_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","v":"2015-16"},"=INDEX(INDIRECT(dms_RPT),dms_PRCP_start_row+dms_FRCPlength_Num-1)","Finds the PRCP final year"]
[null,"dms_Reset_final_year",{"$f":"INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","v":"2025-26"},"=INDEX(INDIRECT(dms_RPT),dms_RYE_start_row)","For Resets and PTRM/RFMs (same as FRCP_final_year)"]
[null,"dms_SpecifiedYear_final_year",{"$f":"FRY","v":"2017-18"},"=FRY","FRY from cover sheet"]
[null,"dms_DollarReal_year",{"$f":"LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","v":"2021"},"=LEFT(CRCP_final_year,2)&RIGHT(CRCP_final_year,2)","Uses the value in CRCP_final_year"]
[null,"dms_Previous_DollarReal_year",{"$f":"LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","v":"2016"},"=LEFT(PRCP_final_year,2)&RIGHT(PRCP_final_year,2)","Uses the value in PRCP_final_year"]
[null,"dms_CRY_RYE",{"$f":"IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","v":0},"=IFERROR(LEFT(CRY,2)&RIGHT(CRY,2),0)","For ABC single year RINS"]
[null,"dms_Reset_RYE",{"$f":"IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","v":"2026"},"=IF(dms_Model_Span>1,IF(dms_Model=\"RFM\",(LEFT(dms_DollarReal_year,2)&RIGHT(dms_DollarReal_year,2)),(LEFT(dms_Reset_final_year,2)&RIGHT(dms_Reset_final_year,2))),0)","If model span > 1 then uses dms_Reset_RYE otherwise it's a multi year ABC and uses dms_Specified_RYE"]
[null,"dms_Specified_RYE",{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","v":0},"=IF(dms_MultiYear_ResponseFlag=\"Yes\",(LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2)),0)","If multi year ABC - uses dms_Specified_FinalYear"]
[null,"dms_Model_Span",{"$f":"INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","v":5},"=INDEX(dms_Model_Span_List,MATCH(dms_Model,dms_Model_List))","A result of 5 is used to signify that it is more than 1 year span"]
[null,"dms_RYE_result",{"$f":"IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","v":"2026"},"=IF(dms_MultiYear_ResponseFlag=\"yes\",dms_Specified_RYE,(IF(dms_Model_Span>1,dms_Reset_RYE,dms_CRY_RYE)))","Nested IF - feeds into dms_RYE"]
[null,"dms_Reset_Span",{"$f":"IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","v":"2021-22 to 2025-26"},"=IF(dms_Reset_RYE>0,CONCATENATE(FRCP_y1,\" to \",FRCP_final_year),0)","Reset span of years as text"]
[null,"dms_SpecifiedYear_Span",{"$f":"IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","v":0},"=IF(dms_Specified_RYE>0,CONCATENATE(CRY,\" to \",dms_Specified_FinalYear),0)","Multi year ABC span of years as text"]
[null,"dms_Header_Span",{"$f":"IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","v":"2021-22 to 2025-26"},"=IF(dms_MultiYear_Flag=1,dms_SpecifiedYear_Span,IF(dms_Model_Span>1,dms_Reset_Span,CRY))","NESTED IF - for Sheet Headers"]
[null,"ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"This is a multi year ABC RIN?","No"]
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,FRY,\"not a Multiple year submission\")","v":"not a Multiple year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null," Start year for 5.2 in Multi year ABC RINS",{"$f":"IFERROR(IF(dms_MultiYear_Flag=1,FRY,CRY),\"not an ABC\")","v":"not an ABC"},"dms_0502_Inst_Year","=IF(dms_MultiYear_Flag=1,FRY,CRY)",null,"For single year RINS this is CRY - multi year RINS need to start a the end of the span of years (ie. FRY)"]
[null,"WHAT IS THE RYE?"]
[null,"Reg Period Lengths"]
[null,"PRCP length in years",{"$f":"INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_PRCPlength_Num","=INDEX(dms_PRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Single year RIN?"]
[null,"Single Year ABC RIN ?",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Is this a single Year ABC RIN?",{"$f":"IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")","v":"no"},"dms_SingleYearModel","=IF(SUM(dms_SingleYear_Model)=1,\"yes\",\"no\")"]
[null,"Single Year Final Year Result",{"$f":"IF(AND(dms_SingleYearModel=\"yes\",dms_MultiYear_Flag=0),CRY,0)","v":0},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"Multi year RIN?"]
[]
[null,"Multi Year Reset/Model?",{"$f":"IF(dms_Model_Span>1,\"yes\",\"no\")","v":"yes"}]
[null,"Final year result for Reset/Model",{"$f":"IF(dms_Model_Span>1,dms_Reset_final_year,0)","v":"2025-26"},"dms_MultiYear_FinalYear_Result","dms_CRCP_FinalYear_Result"]
[]
[null,"Multi Year ABC RIN?",{"$f":"IF(dms_MultiYear_Flag=1,\"yes\",\"no\")","v":"no"},"dms_MultiYear_ABC_RIN"]
[null,"Final year result for ABC multi year",{"$f":"IF(dms_MultiYear_Flag=1,C50,0)","v":0}]
[]
[null,"EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"IFERROR(IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY),\"CRY not present\")","v":"CRY not present"},"dms_0306_Year","=IF(dms_Segment=\"Transmission\",dms_Cal_Year_B4_CRY,CRY)"]
[null,"CA RINS"]
[null,"Find how many rows in tables 6.3 sustained interruptions?",null,null,"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,null,{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"not a CA"},null,"=IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")"]
[null,"dms_060301_Avg_Duration_Sustained_Int_Values present?",{"$f":"IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")","v":"no"},"dms_060301_checkvalue","=IFERROR(IF(INDEX(dms_060301_Avg_Duration_Sustained_Int_Values,1,1)<>\"\",\"yes\",\"no\"),\"no\")"]
[null,null,{"$f":"IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")","v":"no errors"},null,"=IF(AND(dms_Model=\"CA\",(dms_060301_checkvalue=\"no\")),\"error - NR not present\",\"no errors\")"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")","v":"not a CA"},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")","v":"not a CA"},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-15),\"not a CA\"),\"error\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":2},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required",null,"'dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"MaxRows if Reset and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)","v":1826},"dms_060701_Reset_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)",null,null,"number of days present in Reset RIN table"]
[null,"MaxRows if ARR and leap year",{"$f":"IF(dms_LeapYear_Result=\"is a leap year\",366,365)","v":365},"dms_060701_ARR_MaxRows","=IF(dms_LeapYear_Result=\"is a leap year\",366,365)",null,null,"number of days present in ARR RIN table"]
[null,"Table 6.7.1 - Max Rows (leap year/ non leap year)",{"$f":"IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))","v":1826},"dms_060701_MaxRows","=IF(dms_Model=\"ARR\",dms_060701_ARR_MaxRows,IF(dms_Model=\"Reset\",dms_060701_Reset_MaxRows,\"not a relevant RIN type\"))"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060101 as naming standard not 060701 for start dates"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text","2015-01-01","dms_060101_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",42005,"dms_060101_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required",null,"dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Is dms_060801_StartCell named range present?","yes",null,"=IFERROR(IF((ROW(dms_060801_StartCell)-1)=1,\"yes\",\"yes\"),\"no\")"]
[null,"Table 6.8 - Number of offset rows",12,"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 error\")"]
[null,"Table 6.8 - Last row","0","dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"0\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"0\")"]
[null,"TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2013"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2016-20 Distribution Determination"},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]
[null,null,2018,"dms_RYE_06"]
[null,null,2019,"dms_RYE_07"]
[null,null,2020,"dms_RYE_08"]
[null,null,2021,"dms_RYE_09"]

{"sheet":"Instructions","index":5,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,1,1,4],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,2,5,4],[7,1,8,1],[7,2,7,3],[8,2,8,4],[18,1,24,1],[18,2,18,4],[26,2,26,4],[10,2,10,4],[12,1,14,1],[12,2,12,4],[13,2,13,3],[14,2,14,4],[16,2,16,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Sector,\" \",dms_Segment,\" \", \"Network Service Provider\")","v":"Electricity Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingNameFull,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by United Energy to fulfil its reporting obligations to the AER."}]
[null,"INSTRUCTIONS"]
[null,"GENERAL","Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,"CONFIDENTIAL INFORMATION","\nPlease use the macro at the top of each \nworksheet to identify confidential information\nin the confidential workbook. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selection as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return selection to NON-CONFIDENTIAL macro."]
[]
[null,"RESPONSES","\nPlease return two (2) files to the AER: \n\n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,"AMENDMENTS","\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]
[]
[null,"UNITS OF MEASURE","\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,"INPUT / NON-INPUT CELLS"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," \nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,"NAVIGATION","\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]

{"sheet":"CONTENTS","index":6,"n_rows":48,"n_cols":5,"rows_kept":48,"cut":false,"hidden":false,"merged":[[6,3,6,4]]}
[null,null,{"$f":"IF(dms_MultiYear_ResponseFlag=\"Yes\",\"REGULATORY REPORTING STATEMENT - HISTORICAL INFORMATION\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[]
[]
[]
[null,null,null,"CONTENTS"]
[]
[null,null,null,"SUBMISSION","Business & other details"]
[null,null,null,null,"CPI series"]
[]
[null,null,null,"EXPENDITURE","2.1 Expenditure summary"]
[null,null,null,null,"2.2 Repex"]
[null,null,null,null,"2.3 Augex (a)"]
[null,null,null,null,"2.3 Augex (b)"]
[null,null,null,null,"2.5 Connections"]
[null,null,null,null,"2.6 Non-network"]
[null,null,null,null,"2.10 Overheads"]
[null,null,null,null,"2.11 Labour"]
[null,null,null,null,"2.14 Forecast price changes"]
[null,null,null,null,"2.16 Opex Summary"]
[null,null,null,null,"2.17 Step Changes"]
[]
[null,null,null,"ECONOMIC BENCHMARKING","3.1 Revenue"]
[null,null,null,null,"3.2 Operating expenditure"]
[null,null,null,null,"3.3 Assets (RAB)"]
[null,null,null,null,"3.4 Operational data"]
[null,null,null,null,"3.5 Physical assets"]
[null,null,null,null,"3.6 Quality of service"]
[null,null,null,null,"3.7 Operating Environment"]
[]
[null,null,null,"ALTERNATIVE CONTROL","4.1 Public lighting"]
[null,null,null,null,"4.2 Metering"]
[null,null,null,null,"4.3 Fee-based services"]
[null,null,null,null,"4.4 Quoted services"]
[]
[null,null,null,"NETWORK","5.4 MD & utilisation-Spatial"]
[]
[null,null,null,"SERVICE","6.1 Telephone answering"]
[null,null,null,null,"6.2 Reliability & Cust serv"]
[]
[null,null,null,"OTHER","7.1  Policies and Procedures"]
[null,null,null,null,"7.2 Contingent projects"]
[null,null,null,null,"7.3 Obligations"]
[null,null,null,null,"7.4 Shared Assets"]
[null,null,null,null,"7.7 TSS-LRMC"]
[]
[null,null,null,"FINANCIAL","8.2 Capex"]

{"sheet":"Business & other details","index":7,"n_rows":74,"n_cols":79,"rows_kept":74,"cut":false,"hidden":false,"merged":[[69,25,71,34],[69,37,71,81],[73,25,73,34],[73,37,73,52],[63,25,63,34],[63,37,63,52],[65,25,65,34],[65,37,65,52],[67,25,67,34],[67,37,67,52],[53,25,53,34],[53,37,53,44],[55,25,55,34],[55,37,55,44],[61,25,61,34],[61,37,61,52],[50,37,50,44],[50,46,50,53],[50,55,50,62],[50,64,50,71],[50,73,50,80],[51,37,51,44],[51,46,51,53],[51,55,51,62],[51,64,51,71],[51,73,51,80],[49,25,49,34],[49,37,49,44],[49,46,49,53],[49,55,49,62],[49,64,49,71],[49,73,49,80],[46,37,46,44],[46,46,46,53],[46,55,46,62],[46,64,46,71],[46,73,46,80],[47,37,47,44],[47,46,47,53],[47,55,47,62],[47,64,47,71],[47,73,47,80],[45,25,45,34],[45,37,45,44],[45,46,45,53],[45,55,45,62],[45,64,45,71],[45,73,45,80],[42,37,42,44],[42,46,42,53],[42,55,42,62],[42,64,42,71],[42,73,42,80],[43,37,43,44],[43,46,43,53],[43,55,43,62],[43,64,43,71],[43,73,43,80],[33,21,33,35],[33,37,33,58],[33,60,33,66],[33,68,33,89],[41,25,41,34],[41,37,41,44],[41,46,41,53],[41,55,41,62],[41,64,41,71],[41,73,41,80],[31,21,31,35],[31,37,31,58],[31,60,31,66],[31,68,31,89],[32,21,32,35],[32,37,32,58],[32,60,32,66],[32,68,32,89],[25,21,25,35],[25,37,25,40],[25,49,25,51],[25,60,25,66],[25,68,25,71],[25,80,25,82],[24,21,24,35],[24,37,24,51],[24,60,24,66],[24,68,24,82],[16,21,16,35],[16,37,16,48],[22,21,22,35],[22,37,22,58],[22,60,22,66],[22,68,22,89],[0,7,2,15],[3,21,3,57],[6,21,6,75],[8,16,8,93],[15,21,15,35],[15,37,15,58],[23,21,23,35],[23,37,23,58],[23,60,23,66],[23,68,23,89]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSINESS & OTHER DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUCTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION PARTICULARS INPUT SHEET"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENTITY DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Name"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Short name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"United Energy"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACN/ABN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":70064651029}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Business Address",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Postal Address"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"43-45 Centreway"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 1",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"PO Box 449"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Address 2",null,null,null,null,null,null,null,{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"MOUNT WAVERLEY"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suburb",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"MOUNT WAVERLEY"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code",null,null,null,null,null,null,null,null,null,null,null,null,"State",null,null,null,null,null,null,null,{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Vic"},null,null,null,null,null,null,null,null,null,"Post code"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contact Names"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brent Cleeve",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(03) 9683 4465",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Phone"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bcleeve@powercor.com.au",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATORY CONTROL PERIODS"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Forthcoming period",null,null,null,null,null,null,null,null,null,null,null,"2021-22",null,null,null,null,null,null,null,null,{"$f":"FRCP_y2","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y3","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y4","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y5","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y6","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y7","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y8","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y9","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y10","v":"2030-31"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"FRCP_y11","v":"2031-32"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y12","v":"2032-33"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y13","v":"2033-34"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y14","v":"2034-35"},null,null,null,null,null,null,null,null,{"$f":"FRCP_y15","v":"2035-36"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESETS",null,"Current period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y1","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y2","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y3","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y5","v":"2020-21"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y6","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y7","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y8","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y9","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y10","v":"2025-26"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CRCP_y11","v":"2026-27"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y12","v":"2027-28"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y13","v":"2028-29"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y14","v":"2029-30"},null,null,null,null,null,null,null,null,{"$f":"CRCP_y15","v":"2030-31"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Previous period",null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y1","v":"2011-12"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y2","v":"2012-13"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y3","v":"2013-14"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y4","v":"2014-15"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2015-16"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y6","v":"2016-17"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y7","v":"2017-18"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y8","v":"2018-19"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y9","v":"2019-20"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y10","v":"2020-21"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y11","v":"2021-22"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y12","v":"2022-23"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y13","v":"2023-24"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y14","v":"2024-25"},null,null,null,null,null,null,null,null,{"$f":"PRCP_y15","v":"2025-26"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Commencing year",null,null,null,null,null,null,null,null,null,null,null,"2017-18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUAL RINS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Final year",null,null,null,null,null,null,null,null,null,null,null,"2017-18"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMISSION DETAILS"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIN type",null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDIRECT(dms_Model)","v":"Regulatory Reporting (Reset)"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source",null,null,null,null,null,null,null,null,null,null,null,"Regulatory proposal"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THIS FILE",null,"Data Quality",null,null,null,null,null,null,null,null,null,null,null,"Consolidated"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidentiality Status",null,null,null,null,null,null,null,null,null,null,null,"Public"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Amended RIN \nAmendment Reason",null,null,null,null,null,null,null,null,null,null,null,"."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Submission Date",null,null,null,null,null,null,null,null,null,null,null,"2020-01-31",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Please enter date this file submitted to AER"]

{"sheet":"CPI series","index":8,"n_rows":13,"n_cols":12,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,2,9,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"CPI SERIES"]
[]
[]
[]
[null,"NOMINATED CPI SERIES"]
[]
[null,"Name of CPI series","ABS CPI All Groups, Weighted Average of Eight Capital Cities , December quarter (to December 2018)"]
[]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Series data",110,112.1,114.1,{"$f":"E13*1.02","v":116.38199999999999},{"$f":"F13*1.02","v":118.70963999999999},{"$f":"G13*1.024","v":121.55867135999999},{"$f":"H13*1.024","v":124.47607947264},127.46350537998336,130.52262950910296,133.65517261732143]

{"sheet":"2.1 Expenditure summary","index":9,"n_rows":119,"n_cols":9,"rows_kept":119,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,7,8],[22,1,23,1],[22,2,22,3],[35,1,36,1],[35,2,35,8],[99,1,100,1],[99,2,99,8],[111,1,112,1],[111,2,111,8],[47,1,48,1],[47,2,47,8],[59,1,60,1],[59,2,59,8],[72,1,73,1],[72,2,72,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",{"$f":"SUM('2.2 Repex'!E$12:E$146)","v":65051964.139196813},{"$f":"SUM('2.2 Repex'!F$12:F$146)","v":71947067.801485643},{"$f":"SUM('2.2 Repex'!G$12:G$146)","v":89283675.337094545},{"$f":"SUM('2.2 Repex'!H$12:H$146)","v":108165612.56488752},{"$f":"SUM('2.2 Repex'!I$12:I$146)","v":107979641.54389223},{"$f":"SUM('2.2 Repex'!J$12:J$146)","v":106432555.8099547},{"$f":"SUM('2.2 Repex'!K$12:K$146)","v":93069949.638837829}]
[null,"Connections",{"$f":"SUM('2.5 Connections'!E$105:E$118)","v":67756815.771160796},{"$f":"SUM('2.5 Connections'!F$105:F$118)","v":68523366.421526536},{"$f":"SUM('2.5 Connections'!G$105:G$118)","v":73612243.359166548},{"$f":"SUM('2.5 Connections'!H$105:H$118)","v":72203856.414727911},{"$f":"SUM('2.5 Connections'!I$105:I$118)","v":77535839.11888957},{"$f":"SUM('2.5 Connections'!J$105:J$118)","v":75646640.362144679},{"$f":"SUM('2.5 Connections'!K$105:K$118)","v":70241227.549076468}]
[null,"Augmentation Expenditure",{"$f":"SUM('2.3 Augex (b)'!D$48:D$56)","v":21840560.987360265},{"$f":"SUM('2.3 Augex (b)'!E$48:E$56)","v":20698208.833804198},{"$f":"SUM('2.3 Augex (b)'!F$48:F$56)","v":38273781.059898667},{"$f":"SUM('2.3 Augex (b)'!G$48:G$56)","v":39235673.204357952},{"$f":"SUM('2.3 Augex (b)'!H$48:H$56)","v":35343183.681890413},{"$f":"SUM('2.3 Augex (b)'!I$48:I$56)","v":37994285.526980013},{"$f":"SUM('2.3 Augex (b)'!J$48:J$56)","v":31196841.680168368}]
[null,"Non-network",{"$f":"SUM('2.6 Non-network'!E$32:E$39)","v":32750468.157883752},{"$f":"SUM('2.6 Non-network'!F$32:F$39)","v":31170888.886154607},{"$f":"SUM('2.6 Non-network'!G$32:G$39)","v":77927121.876750827},{"$f":"SUM('2.6 Non-network'!H$32:H$39)","v":55687568.904364571},{"$f":"SUM('2.6 Non-network'!I$32:I$39)","v":60276351.617589846},{"$f":"SUM('2.6 Non-network'!J$32:J$39)","v":50000018.27810663},{"$f":"SUM('2.6 Non-network'!K$32:K$39)","v":35954221.490166754}]
[null,"Public lighting"]
[null,"Metering"]
[null,"Capitalised network overheads",{"$f":"'2.10 Overheads'!D$15","v":22311277.895483259},{"$f":"'2.10 Overheads'!E$15","v":22738034.008921564},{"$f":"'2.10 Overheads'!F$15","v":23172952.845320437},{"$f":"'2.10 Overheads'!G$15","v":23626970.268600453},{"$f":"'2.10 Overheads'!H$15","v":24077325.291750468},{"$f":"'2.10 Overheads'!I$15","v":24527510.83839523},{"$f":"'2.10 Overheads'!J$15","v":24997404.792333938}]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)",{"$f":"SUM('2.5 Connections'!E$141:E$154)","v":43541975.325680181},{"$f":"SUM('2.5 Connections'!F$141:F$154)","v":44318354.860939324},{"$f":"SUM('2.5 Connections'!G$141:G$154)","v":47984081.811788641},{"$f":"SUM('2.5 Connections'!H$141:H$154)","v":47037092.563624389},{"$f":"SUM('2.5 Connections'!I$141:I$154)","v":51194416.554125659},{"$f":"SUM('2.5 Connections'!J$141:J$154)","v":48681103.601338372},{"$f":"SUM('2.5 Connections'!K$141:K$154)","v":45072911.416872643}]
[null,"Total",{"$f":"SUM(C10:C17)","v":209711086.95108488},215077565.95189255,302269774.47823107,298919681.35693842,305212341.25401253,294601010.81558126,255459645.15058336]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"}]
[null,"Vegetation management",16480082.346490407,17528211.871887408]
[null,"Maintenance",24835105.907987371,26414613.05007799]
[null,"Emergency response",15580195.765976164,16571092.707535598,null," "]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads",{"$f":"'2.10 Overheads'!D12","v":16183565.146717999},{"$f":"'2.10 Overheads'!E12","v":16493114.218534598}]
[null,"Corporate overheads",{"$f":"'2.10 Overheads'!D27","v":54578305.008656576},{"$f":"'2.10 Overheads'!E27","v":55622244.554954819}]
[null,"Total",{"$f":"SUM(C25:C31)","v":127657254.17582852},{"$f":"SUM(D25:D31)","v":132629276.40299043}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Connections"]
[null,"Metering",{"$f":"SUM('4.2 Metering'!E29,'4.2 Metering'!E47,'4.2 Metering'!E59,'4.2 Metering'!E61)","v":13848870.241184734},{"$f":"SUM('4.2 Metering'!F29,'4.2 Metering'!F47,'4.2 Metering'!F59,'4.2 Metering'!F61)","v":12873071.697200116},{"$f":"SUM('4.2 Metering'!G29,'4.2 Metering'!G47,'4.2 Metering'!G59,'4.2 Metering'!G61)","v":11913275.270568911},{"$f":"SUM('4.2 Metering'!H29,'4.2 Metering'!H47,'4.2 Metering'!H59,'4.2 Metering'!H61)","v":10190473.456872864},{"$f":"SUM('4.2 Metering'!I29,'4.2 Metering'!I47,'4.2 Metering'!I59,'4.2 Metering'!I61)","v":9778606.8382956516},{"$f":"SUM('4.2 Metering'!J29,'4.2 Metering'!J47,'4.2 Metering'!J59,'4.2 Metering'!J61)","v":10412782.659612518},{"$f":"SUM('4.2 Metering'!K29,'4.2 Metering'!K47,'4.2 Metering'!K59,'4.2 Metering'!K61)","v":12533187.84036351}]
[null,"Public lighting",{"$f":"'4.1 Public lighting'!D18","v":1873644.5249999976},{"$f":"'4.1 Public lighting'!E18","v":1835364.2637208826},{"$f":"'4.1 Public lighting'!F18","v":1797084.0024417676},{"$f":"'4.1 Public lighting'!G18","v":2916647.7874355479},{"$f":"'4.1 Public lighting'!H18","v":2956701.5611371407},{"$f":"'4.1 Public lighting'!I18","v":2986997.0220311349},{"$f":"'4.1 Public lighting'!J18","v":3004074.5164914541}]
[null,"Fee and quoted"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total",{"$f":"SUM(C38:C43)","v":15722514.766184732},14708435.960920999,13710359.273010679,13107121.244308412,12735308.399432793,13399779.681643654,15537262.356854964]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Connections",{"$f":"SUM('4.2 Metering'!E44:E46)","v":10368184.337279599},{"$f":"SUM('4.2 Metering'!F44:F46)","v":13182785.147727612},{"$f":"SUM('4.2 Metering'!G44:G46)","v":11098143.31484223},{"$f":"SUM('4.2 Metering'!H44:H46)","v":10934742.260251457},{"$f":"SUM('4.2 Metering'!I44:I46)","v":10794779.016709179},{"$f":"SUM('4.2 Metering'!J44:J46)","v":10729215.194288487},{"$f":"SUM('4.2 Metering'!K44:K46)","v":10640581.863130575}]
[null,"Metering",{"$f":"SUM('4.2 Metering'!E32:E43,'4.2 Metering'!E50:E58,'4.2 Metering'!E60,'4.2 Metering'!E62)","v":7638696.0770764677},{"$f":"SUM('4.2 Metering'!F32:F43,'4.2 Metering'!F50:F58,'4.2 Metering'!F60,'4.2 Metering'!F62)","v":7857970.6789677124},{"$f":"SUM('4.2 Metering'!G32:G43,'4.2 Metering'!G50:G58,'4.2 Metering'!G60,'4.2 Metering'!G62)","v":7017502.5630530277},{"$f":"SUM('4.2 Metering'!H32:H43,'4.2 Metering'!H50:H58,'4.2 Metering'!H60,'4.2 Metering'!H62)","v":7205805.2039582543},{"$f":"SUM('4.2 Metering'!I32:I43,'4.2 Metering'!I50:I58,'4.2 Metering'!I60,'4.2 Metering'!I62)","v":7396434.421316511},{"$f":"SUM('4.2 Metering'!J32:J43,'4.2 Metering'!J50:J58,'4.2 Metering'!J60,'4.2 Metering'!J62)","v":7580823.2839377625},{"$f":"SUM('4.2 Metering'!K32:K43,'4.2 Metering'!K50:K58,'4.2 Metering'!K60,'4.2 Metering'!K62)","v":7754817.9482922675}]
[null,"Public lighting",{"$f":"'4.1 Public lighting'!D22","v":2749666.4436546406},{"$f":"'4.1 Public lighting'!E22","v":3394785.0840796423},{"$f":"'4.1 Public lighting'!F22","v":4039903.7245046441},{"$f":"'4.1 Public lighting'!G22","v":3973100.457610867},{"$f":"'4.1 Public lighting'!H22","v":3918291.7182181505},{"$f":"'4.1 Public lighting'!I22","v":3855224.4964738726},{"$f":"'4.1 Public lighting'!J22","v":3837635.9636825565}]
[null,"Fee and quoted",{"$f":"SUM('4.3 Fee-based services'!C13:C14,'4.3 Fee-based services'!C16:C28,'4.4 Quoted services'!C12:C20)","v":5022068.7158067375},{"$f":"SUM('4.3 Fee-based services'!D13:D14,'4.3 Fee-based services'!D16:D28,'4.4 Quoted services'!D12:D20)","v":5167244.4171425831},{"$f":"SUM('4.3 Fee-based services'!E13:E14,'4.3 Fee-based services'!E16:E28,'4.4 Quoted services'!E12:E20)","v":4083384.3601804958},{"$f":"SUM('4.3 Fee-based services'!F13:F14,'4.3 Fee-based services'!F16:F28,'4.4 Quoted services'!F12:F20)","v":4142297.0421547252},{"$f":"SUM('4.3 Fee-based services'!G13:G14,'4.3 Fee-based services'!G16:G28,'4.4 Quoted services'!G12:G20)","v":4208039.9766005948},{"$f":"SUM('4.3 Fee-based services'!H13:H14,'4.3 Fee-based services'!H16:H28,'4.4 Quoted services'!H12:H20)","v":4281430.4011210501},{"$f":"SUM('4.3 Fee-based services'!I13:I14,'4.3 Fee-based services'!I16:I28,'4.4 Quoted services'!I12:I20)","v":4363383.5979044521}]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total",{"$f":"SUM(C50:C55)","v":25778615.573817447},29602785.327917546,26238933.962580398,26255944.963975307,26317545.132844437,26446693.375821169,26596419.373009853]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C62:C67)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C75:C95)","v":0},{"$f":"SUM(D75:D95)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure"]
[null,"Connections",{"$f":"C18","v":43541975.325680181},{"$f":"D18","v":44318354.860939324},47984081.811788641,47037092.563624389,51194416.554125659,48681103.601338372,45072911.416872643]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total",{"$f":"SUM(C102:C107)","v":43541975.325680181},44318354.860939324,47984081.811788641,47037092.563624389,51194416.554125659,48681103.601338372,45072911.416872643]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Replacement expenditure",{"$f":"C10/SUM(C$10:C$12)*'2.10 Overheads'!D$15","v":9385054.2209329884},{"$f":"D10/SUM(D$10:D$12)*'2.10 Overheads'!E$15","v":10150453.856806712},10516509.790043572,11828307.890183453,11631801.239374923,11721439.973925002,11858157.271342535]
[null,"Connections",{"$f":"C11/SUM(C$10:C$12)*'2.10 Overheads'!D$15","v":9775283.4716784749},{"$f":"D11/SUM(D$10:D$12)*'2.10 Overheads'!E$15","v":9667430.3794268221},8470733.8069360815,7779038.8163193567,8458755.0996467508,8438697.8407836035,9056672.2712099198]
[null,"Augmentation Expenditure",{"$f":"C12/SUM(C$10:C$12)*'2.10 Overheads'!D$15","v":3150940.2028717985},{"$f":"D12/SUM(D$10:D$12)*'2.10 Overheads'!E$15","v":2920149.7726880303},4185709.2483407641,4019623.5620976281,3986768.9527288377,4367373.0236866036,4082575.249781474]
[null,"Non-network"]
[null,"capcons (included in the above)"]
[null,"Total",{"$f":"SUM(C114:C117)","v":22311277.895483263},22738034.008921564,23172952.845320418,23626970.268600438,24077325.291750513,24527510.838395208,24997404.792333931]

{"sheet":"2.2 Repex","index":10,"n_rows":524,"n_cols":11,"rows_kept":524,"cut":false,"hidden":false,"merged":[[9,4,9,10],[11,1,30,1],[31,1,37,1],[38,1,43,1],[44,1,52,1],[53,1,60,1],[61,1,76,1],[77,1,105,1],[106,1,119,1],[120,1,128,1],[129,1,136,1],[182,4,182,10],[184,1,203,1],[204,1,210,1],[211,1,216,1],[217,1,225,1],[226,1,233,1],[234,1,249,1],[250,1,278,1],[279,1,292,1],[293,1,301,1],[302,1,309,1],[355,4,355,10],[357,1,376,1],[452,1,465,1],[466,1,474,1],[475,1,482,1],[377,1,383,1],[384,1,389,1],[390,1,398,1],[399,1,406,1],[407,1,422,1],[423,1,451,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.2 REPEX"]
[]
[null,"There are THREE sub-tables on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($0's, real June 2021)"}]
[null,"ASSET GROUP","ASSET CATEGORY","UNITS",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,3753576.6478375811,4020448.94701534,5230670.1588941682,5607007.8271150552,5973940.5202222159,6049773.9355889643,6405223.4180799304]
[null,null,"> 1 kV & < = 11 kV; Wood",null,2224527.0538995075,2359969.7340285457,3049672.8999901139,3248483.3348360043,3441182.8787989793,3462226.3326711548,3647186.1895747618]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,3336790.5808492606,3539954.6010428178,4573511.7856608406,4871685.1815559017,5160706.88046744,5192575.2052382138,5470006.091421294]
[null,null,"> 22 kV & < = 66 kV; Wood",null,819638.59268336243,872697.99485246616,1262480.3894666422,1344681.5978496482,1422771.1156337326,1393781.0049795301,1466674.84250399]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,386894.82943589002,784187.39670353848,795802.21250155405,806707.87416653184,816862.43318391382,826373.69686609157]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,9155455.4509257004,9155455.4509257004,9188519.3428656422,9324587.1033176649,9450458.4927019849,9597601.3962689415,9709960.0195449609]
[null,null,"> 1 kV & < = 11 kV",null,1294768.5590283659,1294768.5590283659,1249111.8472073057,1267594.6101830259,1283625.1396620376,1319537.2567507287,1335327.2746958097]
[null,null,"˃ 11 kV & < = 22 kV",null,1942152.8385425485,2624114.0033449712,3248081.8202274689,3281849.2927732002,3310303.1994949002,3366911.2899188576,3391889.7505036648]
[null,null,"> 22 kV & < = 66 kV",null,434883.10420707962,434883.10420707962,436399.95710655773,442862.34990717715,448839.33881845907,455844.7171998478,461181.63274730014]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,989450.79057369847,989450.79057369847,1002746.4579425438,1017598.4122714122,1031543.5657539165,1044528.2785017263,1056690.4045546995]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",1771146.2003273808,1889843.4705478104,2035530.3493879316,2187753.0880038524,2341480.8603949314,2496259.1285633459,2652088.2280164016]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",295768.54778232489,282866.34300720197,286667.33729847427,290913.2462891388,294899.91708252201,298612.01499073871,302088.95002638857]
[null,null,"> 1 kV & < = 11 kV","per km",35929.37224890331,35929.37224890331,36412.170369581814,36951.481066778004,37457.863612847301,37929.370212574853,38371.006682481544]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",197651.43674155005,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",1873070.5161585798,2411871.7624899433,2465410.0137258749,2501925.881356982,2536212.2363636633,2568137.1966367606,2323089.3965289928]
[null,null,"> 22 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",649230.58559150354,824579.47151818068,226164.99278703879,229514.78486763511,232660.05206035697,235588.69612754794,238331.80943326789]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",229614.25839779555,229614.25839779555,232699.68198013571,236146.26114452624,239382.40598935686,242395.66871702424,245218.04005756837]
[null,null,"> 1 kV & < = 11 kV","per km",1272097.1106972988,1612243.74763827,1572598.7215167559,1638846.5378704732,1531413.6484664651,1576625.2336087807,1749743.1945158693]
[null,null,"> 11 kV & < = 22 kV","per km",970716.24858380877,656411.40456677414,594749.86890471808,643001.97641244205,711999.50178714399,800631.47783010686,911714.63948416826]
[null,null,"> 22 kV & < = 33 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,500464.4637372733,506764.13688521815,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",2540175.0803370015,2858244.4997597635,3218995.3882670053,3273976.9066198613,3326247.6224282822,3375614.660586352,3422503.8336702441]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",3036027.8750800374,3744195.6237815963,4495061.1929469025,4416212.0491675492,4330434.1567663662,4218139.2175026629,4115853.7414228027]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",365786.4909734985,365786.4909734985,377292.96103937685,382884.12190593965,388269.36012847378,391091.362363661,395601.60248968273]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",219471.89458409909,219471.89458409909,226375.77662362612,229730.47314356381,232961.61607708427,234654.81741819662,237360.96149380962]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",36578.649097349851,36578.649097349851,37729.29610393769,38288.412190593968,38826.936012847385,39109.13623636611,39560.16024896827]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,292238.49337857892,292238.49337857892,296165.42520515434,300552.01299521455,304670.77330394817,308505.86336251837,312097.9989470889]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,13955.080210351265,13955.080210351265,14142.600505802044,14352.070462180229,14548.751021989747,14731.885655495869,14903.418637443598]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,97412.831126192963,97412.831126192963,98721.80840171811,100184.00433173816,101556.92443464939,102835.28778750611,104032.66631569629]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,707738.41021280119,692311.72590375866,701614.61040378571,712006.41789175686,721763.74323571613,730849.05498486198,739358.80863669433]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,1316532.7836431225,1328798.9875127086,1329323.0939298451,1348788.9446375638,1343591.2301767308,1379289.0716461113,1448229.2870258181]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,99525.777111283678,99525.777111283678,100863.14693270776,102357.05881825477,103759.75842747701,105065.85029086645,106289.20071746595]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,360152.00136027706,345504.27020211436,350146.95672567503,355333.07986626658,360202.55909932218,364736.66402344371,368983.53160500602]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,175403.28927616967,180505.0772181577,138857.82016510778,140914.48163417933,142845.57159127729,144643.66211889725,146327.84289950482]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,336143.17350330233,274033.33883943531,277715.64033021557,281828.96326835867,285691.14318255457,289287.3242377945,292655.68579900963]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,2107500.3980698744,3414142.9467463563,3702637.4821597128,4650677.708280935,5486498.0603350932,5479753.996131097,4895448.1167133562]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1965320.7507568579,1564702.8556762342,1590227.20919569,1476738.7825885718,1294996.9241600856,1106776.3892966025,1135416.1146873489]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  FUSE",null,2205049.0112387952,2828008.4670100706,2937181.8263356206,3051936.7510009892,3167348.7415196346,2541576.767632761,1859127.5363854177]
[null,null,"˂ = 11 kV  ; Switch",null,4899888.7169983741,5056495.4356230134,5283152.805440221,5522464.8617707714,5761413.6499187555,5999260.5130049717,6236362.9910457237]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,1596695.3735779298,2031993.1695830319,1891188.3326300073,1916521.8016899703,1658607.8111284524,1904907.9621644856,2561651.0567470444]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,1365934.8443150283,1418137.0838565752,1490096.8926976516,1565854.4030939755,1641735.8524909483,1717509.5160658772,1793257.3240198521]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,1127713.4085589452,652263.34240244317,41487.871738910137,615985.74522776459,1295821.5821621164,723062.21986907325,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,500351.94069823425,746843.76960076566,809951.94922243722,1017335.7486864544,1200171.4506983019,1198696.1866536776,1070879.275531047]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,83395.040312958678,169031.30924845382,171534.87858566977,173885.5900064359,176074.40152363715,89062.275482200479]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,722846.2292856389,748406.2943783747,791682.11122866743,837119.11752655206,882764.14722490648,928479.3979316114,974296.5217571673]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,3999613.4978561634,4232645.1767706461,5613294.5995907541,5656465.5273335436,5810955.0897195777,5513841.7160706054,5506949.4630454518]
[null,null,"Local Network Wiring Assets",null,519482.38765254198,864222.10432972817,948688.18089911959,1083886.0140632007,956370.70156399987,871568.28754200379,682439.64135122334]
[null,null,"Communications Network Assets",null,576003.37696130038,889808.42719215655,1254156.6821938709,4720238.5957129002,804220.85377976601,3649118.9902046989,217465.02796255419]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,117875.59667759322,24407.964755109882,68778.943000761356,52348.235103193372,19144.24104850342,96765.236081854266,136625.55759614537]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,43122.269313875702,0,0,0,0,0,0]
[null,"OTHER BY: \nenter DNSP defined asset group here","Zone Substaion Miscellaneous",null,0,0,0,0,0,0,0]
[null,null,"Buildings ",null,919740.77663820283,1212576.6371883962,957484.94731897546,1002650.0083761861,1016390.309154398,1001232.4667202093,814281.59698817879]
[null,null,"Civil",null,764302.44200930826,987566.64272914547,741845.79567860393,965568.69020853657,1207118.1269296145,990385.6975459212,618764.98903810687]
[null,null,"Capacitor Banks - Large",null,91139.127793864449,120257.38552136472,121873.33470425637,271988.63743980794,426058.60965488938,279186.58265482646,128429.65670236258]
[null,null,"Fences",null,207032.76380997617,234548.53003143615,0,0,0,0,0]
[null,null,"CTs and VTs",null,183139.00125554189,142993.27627273486,20699.418944126461,143981.014856414,289824.35228013934,167243.12179257747,12444.448657851601]
[null,null,"NER's",null,0,0,0,0,0,0,0]
[null,null,"Other ",null,295602.50075846346,523092.66693645745,11711594.735250536,22777701.867086593,22434895.349015143,18925977.728979517,10362130.719979912]
[null,null,0,null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,441,473,579.30655391120513,612.75475687103597,645.2029598308668,653.75581395348831,685.75581395348831]
[null,null,"> 1 kV & < = 11 kV; Wood",null,163,173,211.69344608879493,222.24524312896406,232.7970401691332,234.24418604651163,244.24418604651163]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,245,260,370,386,402,388,403]
[null,null,"> 22 kV & < = 66 kV; Wood",null,40,43,54,58,60,60,63]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,278,278,278,278,278,278]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,3119,3119,3039.3467627688528,3039.3241360162124,3037.6779612661098,3061.6340439745541,3062.1444486006526]
[null,null,"> 1 kV & < = 11 kV",null,366,366,352.80032068740985,352.79657111125806,352.52377643838389,356.49364157292609,356.57822291096528]
[null,null,"˃ 11 kV & < = 22 kV",null,549,990,975.76704349473846,971.7644207284801,966.57360538442003,965.35046012846078,960.4096233699895]
[null,null,"> 22 kV & < = 66 kV",null,77,77,76.745860842343546,76.745788650125675,76.740536415830007,76.816969953146327,76.818598434376341]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,584,584,584,584,584,584,584]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,1444,1542,1639,1737,1835,1932,2028]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",null,3956,3796,3796,3796,3796,3796,3796]
[null,null,"> 1 kV & < = 11 kV",null,460,460,460,460,460,460,460]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,2961.11,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,12388.791698113208,10054.254833333329,10054.254833333329,10054.254833333329,10054.254833333329,10054.254833333329,10054.254833333329]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,22,22,22,22,22,22,22]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",null,1323,1323,1323,1323,1323,1323,1323]
[null,null,"> 1 kV & < = 11 kV",null,1272,1192,1192,1192,1212,1192,1692]
[null,null,"> 11 kV & < = 22 kV",null,2772.6666666666665,1563.3333333333333,1386,1386,1386,1406,1406]
[null,null,"> 22 kV & < = 33 kV",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",null,0,0,0,0,0,188,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,">  132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,734,925,935,944,954,963,973]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",null,3797,3797,5938.4436731112955,5731.4762921214551,5526.9732115757724,5297.8798533489135,5090.4199735690872]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,457,457,465.84863531461389,465.85256531583792,466.03291705732192,463.37106666854385,463.31565946615518]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,274,274,279.30918118876832,279.31153918950275,279.41975023439318,277.82264000112633,277.78939567969309]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,46,46,46.884863531461392,46.885256531583792,46.903291705732194,46.637106666854386,46.631565946615517]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,25,25,25,25,25,25,25]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,1,1,1,1,1,1,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,8,8,8,8,8,8,8]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,33,32,32,32,32,32,32]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,29,27,27,27,27,27,29]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,2,2,2,2,2,2,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,6,5,5,5,5,5,5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,9,5,5,5,5,5,5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,10,9,9,9,9,9,9]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,1,2,2,2,3,3,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,396,415,433,453,473,493,512]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,930,930,930,930,930,930,930]
[null,null,"˂ = 11 kV  ; Switch",null,1188,1200,1213,1225,1237,1249,1261]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,16,16,16,16,16,16,32]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,95,99,103,107,111,115,119]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,16,4,0,0,4,15,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,2,2,2,2,3,3,3]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,0,1,1,1,1,1]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,678,721,765,809,852,896,940]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,94,93,109,108,95,100,95]
[null,null,"Local Network Wiring Assets",null,8,4,7,4,7,7,5]
[null,null,"Communications Network Assets",null,2,3,4,5,10,2,1]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},"Zone Substaion Miscellaneous",null,16,14,14,15,14,15,13]
[null,null,"Buildings ",null,2,2,0,0,2,5,0]
[null,null,"Civil",null,10,10,10,10,10,10,10]
[null,null,"Capacitor Banks - Large",null,3,0,0,0,0,0,0]
[null,null,"Fences",null,5,7,6,6,8,11,6]
[null,null,"CTs and VTs",null,0,0,0,0,0,0,0]
[null,null,"NER's",null,1,1,3,5,4,3,4]
[null,null,"Other "]
[null,null,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C158),\"\",C158)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C178),\"\",C178)","v":""}]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","Staking of a wooden pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood",null,2.77,2.67,2.48,2.21,2.02,1.97,1.94]
[null,null,"> 1 kV & < = 11 kV; Wood",null,0.23,0.21,0.2,0.19,0.18,0.18,0.18]
[null,null,"˃ 11 kV & < = 22 kV; Wood",null,0.9,0.84,0.8,0.76,0.73,0.72,0.7]
[null,null,"> 22 kV & < = 66 kV; Wood",null,0.13,0.13,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,null,"> 66 kV & < = 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,10.67,10.67,10.67,10.67,10.67,10.67,10.67]
[null,null,"> 1 kV & < = 11 kV",null,2,2,2,2,2,2,2]
[null,null,"˃ 11 kV & < = 22 kV",null,4.33,4.33,4.33,4.33,4.33,4.33,4.33]
[null,null,"> 22 kV & < = 66 kV",null,1,1,1,1,1,1,1]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV",null,1170,1170,1170,1170,1170,1170,1170]
[null,null,"> 1 kV & < = 11 kV",null,186.33333333333334,186.33333333333334,186.33333333333334,186.33333333333334,186.33333333333334,186.33333333333334,186.33333333333334]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,601.25,601.25,601.25,601.25,601.25,601.25,601.25]
[null,null,"> 22 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV",null,914,914,914,914,914,914,914]
[null,null,"> 1 kV & < = 11 kV",null,40,40,40,40,40,40,40]
[null,null,"> 11 kV & < = 22 kV",null,215,215,215,215,215,215,215]
[null,null,"> 22 kV & < = 33 kV",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",null,0,0,0,0,0,0,0]
[null,null,">  132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,40,40,40,40,40,40,40]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type",null,206.25,206.25,206.25,206.25,206.25,206.25,206.25]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,21,21,21,21,21,21,21]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,13.75,13.75,13.75,13.75,13.75,13.75,13.75]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,3.5,3.5,3.5,3.5,3.5,3.5,3.5]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,4.75,4.75,4.75,4.75,4.75,4.75,4.75]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,5,5,5,5,5,5,5]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,7,7,7,7,7,7,7]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,2,2,2,2,2,2,2]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0.55000000000000004,0.56999999999999995,0.57999999999999996,0.59,0.59,0.6,0.6]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[null,null,"˂ = 11 kV  ; Switch",null,148.25,148.25,148.25,148.25,148.25,148.25,148.25]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0.6,0.53,0.47,0.42,0.4,0.38,0.34]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,5.75,5.75,5.75,5.75,5.75,5.75,5.75]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,0.85,0.96,1.08,1.25,1.41,1.54,1.7]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires ;  Major Road",null,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,17.7,19.41,20.87,21.58,22.69,23.48,23.84]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,0,0,0,0,0,0,0]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B138),\"\",B138)","v":"OTHER BY: \nenter DNSP defined asset group here"},"Zone Substaion Miscellaneous",null,0,0,0,0,0,0,0]
[null,null,"Buildings ",null,0,0,0,0,0,0,0]
[null,null,"Civil",null,0,0,0,0,0,0,0]
[null,null,"Capacitor Banks - Large",null,0,0,0,0,0,0,0]
[null,null,"Fences",null,0,0,0,0,0,0,0]
[null,null,"CTs and VTs",null,0,0,0,0,0,0,0]
[null,null,"NER's",null,0,0,0,0,0,0,0]
[null,null,"Other "]
[null,null,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C158),\"\",C158)","v":""}]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,{"$f":"IF(ISBLANK(C178),\"\",C178)","v":""}]

{"sheet":"2.3 Augex (a)","index":11,"n_rows":126,"n_cols":32,"rows_kept":126,"cut":false,"hidden":false,"merged":[[5,1,5,3],[9,11,9,22],[9,23,9,24],[9,25,11,25],[9,26,11,26],[9,27,9,28],[10,11,10,13],[10,14,10,16],[10,17,10,19],[10,21,10,22],[9,29,10,29],[9,30,9,31],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,6,11,6],[10,7,10,8],[10,9,10,10],[11,14,11,15],[11,17,11,18],[11,23,11,24],[11,27,11,29],[11,30,11,31],[9,1,9,10],[12,14,12,15],[12,17,12,18],[13,14,13,15],[13,17,13,18],[14,14,14,15],[14,17,14,18],[15,14,15,15],[15,17,15,18],[16,14,16,15],[16,17,16,18],[17,14,17,15],[17,17,17,18],[18,14,18,15],[18,17,18,18],[19,14,19,15],[19,17,19,18],[20,14,20,15],[20,17,20,18],[21,14,21,15],[21,17,21,18],[22,14,22,15],[22,17,22,18],[23,14,23,15],[23,17,23,18],[24,14,24,15],[24,17,24,18],[25,14,25,15],[25,17,25,18],[26,14,26,15],[26,17,26,18],[27,14,27,15],[27,17,27,18],[28,14,28,15],[28,17,28,18],[29,14,29,15],[29,17,29,18],[30,14,30,15],[30,17,30,18],[31,14,31,15],[31,17,31,18],[32,14,32,15],[32,17,32,18],[33,14,33,15],[33,17,33,18],[34,14,34,15],[34,17,34,18],[35,14,35,15],[35,17,35,18],[36,14,36,15],[36,17,36,18],[37,14,37,15],[37,17,37,18],[38,14,38,15],[38,17,38,18],[39,14,39,15],[39,17,39,18],[40,14,40,15],[40,17,40,18],[41,14,41,15],[41,17,41,18],[42,14,42,15],[42,17,42,18],[43,14,43,15],[43,17,43,18],[44,14,44,15],[44,17,44,18],[45,14,45,15],[45,17,45,18],[46,14,46,15],[46,17,46,18],[47,14,47,15],[47,17,47,18],[48,14,48,15],[48,17,48,18],[49,14,49,15],[49,17,49,18],[50,14,50,15],[50,17,50,18],[51,14,51,15],[51,17,51,18],[52,14,52,15],[52,17,52,18],[53,14,53,15],[53,17,53,18],[54,14,54,15],[54,17,54,18],[55,14,55,15],[55,17,55,18],[56,14,56,15],[56,17,56,18],[57,14,57,15],[57,17,57,18],[58,14,58,15],[58,17,58,18],[59,14,59,15],[59,17,59,18],[60,14,60,15],[60,17,60,18],[61,14,61,15],[61,17,61,18],[62,14,62,15],[62,17,62,18],[63,14,63,15],[63,17,63,18],[68,1,68,10],[68,11,68,22],[68,23,68,24],[68,25,70,25],[68,26,70,26],[68,27,68,28],[69,17,69,19],[69,21,69,22],[70,7,70,10],[70,23,70,24],[68,29,69,29],[68,30,68,31],[69,1,70,1],[69,3,70,3],[69,4,70,4],[69,5,70,5],[69,6,70,6],[69,7,69,10],[69,11,69,13],[69,14,69,16],[70,27,70,29],[70,30,70,31],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[123,1,123,2],[124,1,124,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both ROWS and COLUMNS have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON-RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE\n(drop down)","PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,null,"CAPACITORS",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"UNITS ADDED ",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"MVAR ADDED",null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,"KBH","Zone substation","KBH000365","KBH 2nd transformer","Demand growth","66/22",46.7,93.4,0,46.7,1,46.7,959303.57310000272,7,null,330426.78629000095,0,null,0,696334.0695711209,7171,853971.61771460145,1480531.560397597,2248350.867002063,6568918.4740753863,"2021/22,2022/23",0,0,6568918.4740753863,0,0]
[null,"EM","Zone substation","EM000347","EM New switchboard","Demand growth","66/11",63.9,63.9,38,38,0,0,0,7,null,330426.78629000095,0,null,0,382925.35086250119,2378,283073.76888125623,898708.27504396404,954478.49531933072,2849612.6763970531,"2022/23,2023/24",0,0,2849612.6763970535,0,0]
[null,"DC","Zone substation","DC000295","DC 4th transformer","Demand growth","66/22",110.4,147.19999999999999,81.400000000000006,108.5,1,46.7,916667.85874000262,7,null,508430.89374300145,0,null,0,697474.72284851305,10142,1083360.684513015,1094842.0197003791,2131368.413549941,6432144.5930948518,"2023/24,2024/25",0,0,6432144.5930948518,0,0]
[null,"MTN","Zone substation","MTN000376","MTN 3rd Transformer","Demand growth","66/22",92.9,139.4,46.7,93.4,1,46.7,906008.93015000259,7,null,421027.67930500116,0,null,0,762934.13168643205,6220,718175.28069797414,1603811.6786872395,2662552.4205980035,7074510.1211246531,"2024/25,2025/26",0,0,7074510.1211246522,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N17,Q17,T17,U17,W17,X17,Y17)<>0,SUM(N17,Q17,T17,U17,W17,X17,Y17),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2536222.7775607668,"2019/20,2020/21,2021/22,2022/23,2023/24,2024/25,2025/26"]
[]
[]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID",null,"PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)\n(drop down)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N72,Q72,T72,U72,W72,X72,Y72)<>0,SUM(N72,Q72,T72,U72,W72,X72,Y72),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N73,Q73,T73,U73,W73,X73,Y73)<>0,SUM(N73,Q73,T73,U73,W73,X73,Y73),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(N74,Q74,T74,U74,W74,X74,Y74)<>0,SUM(N74,Q74,T74,U74,W74,X74,Y74),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,"Non material projects - [forecast]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1165144.8147047183,"2019/20,2022/23,2023/24,2024/25,2025/26"]

{"sheet":"2.3 Augex (b)","index":12,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,9,9],[29,1,30,1],[29,2,30,2],[29,3,29,9],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[45,1,46,2],[45,3,45,9],[47,1,47,2],[63,1,63,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[60,1,61,2],[60,3,60,9],[62,1,62,2],[68,3,68,9],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[68,1,69,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUMES (0's)"]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0.36,1.6]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",1.05,1.6600000000000001,1.36,2,5.1099999999999994,7.2,5.7999999999999989]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",11.272588309085414,12.578239740047751,12.232916918292801,12.808470312507662,12.463124453817796,10.393454579726743,9.1250353920934852]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0.98022507035525341,1.0937599773954567,1.0637319059385044,1.1137800271745795,1.0837499525058953,0.90377865910667354,0.79348133844291158]
[null,"Distribution Substation Augmentations - Indoor","Number",0.24505626758881338,0.27343999434886418,0.26593297648462616,0.27844500679364487,0.27093748812647384,0.22594466477666839,0.19837033461072792]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0.65,0,0.26,2.516,2.97,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0.23,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",73.516880276644017,82.031998304659254,79.779892945387843,83.533502038093459,81.281246437942158,67.783399433000511,59.511100383218384]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",2.4505626758881336,2.7343999434886421,2.6593297648462615,2.784450067936449,2.7093748812647385,2.2594466477666839,1.9837033461072793]
[null,"Distribution Substation Augmentations - Indoor","Number",0.24505626758881338,0.27343999434886418,0.26593297648462616,0.27844500679364487,0.27093748812647384,0.22594466477666839,0.19837033461072792]
[]
[null,"COST METRICS"]
[null,"PROJECT TYPE",null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,282980.3873320276,282980.3873320276,69459.865815806887,626029.48131614656,1091089.9877608386,1293334.6378743863,768456.71357290645]
[null,"HV Feeder Augmentations - Underground Cables",null,1008474.5919160281,1072495.7394996318,1501087.6236646299,2885963.7426094799,4171397.3517592149,4604522.0290206205,2298728.3858449254]
[null,"HV Feeder Non-Material Projects",null,1162423.8795122374,1026007.5443426644,725161.70286029519,544656.19964317675,493634.50689522794,802852.22933467547,2923695.2194557586]
[null,"LV Feeder Augmentations - Overhead Lines",null,0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Underground Cables",null,0,0,0,0,0,0,0]
[null,"LV Feeder Non-Material Projects",null,1280652.536420011,1428984.5583918127,1405799.4725673154,1491070.4216455675,1474581.703027284,1244587.4765379948,1103949.5007896503]
[null,"Distribution Substation Augmentations - Pole Mounted",null,3498442.0645619361,3903650.3239687523,3840314.1127700112,4073254.3261821526,4028211.0180525454,3399920.788131332,3015730.8566388707]
[null,"Distribution Substation Augmentations - Ground Mounted",null,258777.0856381194,288750.03088365431,284065.09974948014,301295.50929815555,297963.69022264396,251489.54212087335,223071.30652674552]
[null,"Distribution Substation Augmentations - Indoor",null,42652.523684117434,47592.766958808723,46820.580597461958,49660.555588097915,49111.393780826525,41451.365854776042,36767.375138401672]
[]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,324843.37367286795,560660.37354060437,4690531.5780654717,4298471.1363442484,5835849.0075422032,7730514.9478211692,2988333.4913983135]
[null,"Subtransmission Lines",null,0,0,0,0,0,489775.18137136876,745938.95210431423]
[null,"HV Feeders",null,2662365.8966261675,2381483.8900863035,2295709.1923407321,4056649.4235688034,5756121.8464152804,6700708.8962296816,5990880.3188735899]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,3799417.2929903716,4239486.1120935865,4171199.7931169537,4424210.3910684055,4375286.1020560162,3692861.696106981,3275569.5383040183]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,1281106.9173138123,1429491.5681094413,1405799.4725673154,1491070.4216455675,1474581.703027284,1244587.4765379948,1103949.5007896503]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,13772827.506757045,12087086.889974263,25710541.023808196,24965271.831730928,17901345.022849627,18135837.328912821,17092169.878698483]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,1166695.3005064069,1455934.2041556612,5355580.5003866246,2465324.5320404884,4843737.2258553039,10188893.154772675,5570273.7872103183]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,20673865.686853856,19242274.629648536,32918198.151480258,36770347.046114177,30499445.601235945,27805390.527092073,25626568.283872306]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,0,117908.4999338682,4571261.6975395177,2221268.3763172999,4488123.9559039446,7233393.0030054962,2611652.7936206507]
[null,"Subtransmission Lines",null,0,0,0,0,0,389356.54379390192,393365.8213184161]
[null,"HV Feeders",null,1166695.3005064069,1338025.704221793,784318.80284710741,244056.15572318889,355613.26995135989,2566143.6079732771,2565255.1722712507]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,0,0,0,0,0,0,0]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,0,0,0,0,0,0,0]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,0,0,0,0,0]

{"sheet":"2.5 Connections","index":13,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,10],[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,54,10],[102,1,103,1],[102,2,103,3],[102,4,102,10],[159,4,159,10],[177,4,177,10],[195,4,195,10],[120,1,121,1],[120,2,121,3],[120,4,120,10],[138,1,139,1],[138,2,139,3],[138,4,138,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Underground connections","0's",8832.8037306041606,8732.6440858613714,8944.9346476269639,9245.0145394460014,9395.0544853555166,9468.478288672939,9517.161462611668]
[null,null,"Overhead connections","0's",323.4462693958402,319.77854797644306,327.55236389325302,338.54091571551061,344.0351916266394,346.72387983846829,348.50659702239847]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0.22539016345017723,0.22283434998616125,0.22825145262702387,0.23590871049531092,0.23973733942945441,0.24161092380148208,0.24285319170032654]
[null,null,"Augmentation LV","total spend $0s",15469573.513785966,15294156.167865014,15665957.076350858,16191510.240225587,16454286.822162947,16582879.617579101,16668142.23193112]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993]
[null,null,"Volume of GSL breaches for residential customers","0's",353.25,353.25,353.25,353.25,353.25,353.25,353.25]
[null,null,"Volume of customer complaints relating to connection services","0's",402,402,402,402,402,402,402]
[null,null,"GSL payments","$0's",69790,69790,69790,69790,69790,69790,69790]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1844.4898914557079,1889.0297510145749,1858.1651165289156,1725.3637978311228,1678.1879881518853,1685.1504504479515,1687.5144552643733]
[null,null,"Overhead connections","0's",1666.7701816167921,1707.0185506374155,1679.127775705276,1559.1220878941181,1516.4917469899865,1522.7833643089382,1524.9195932768839]
[null,null,"Distribution substations installed","MVA added",145.99725000000001,150.44647886311466,162.34499614996096,151.8965669867427,161.54681560007205,151.61941819774361,132.49739936966307]
[null,null,"Distribution substations installed","0's",221.75,228.50777454983347,246.58000678953772,230.71026152417383,245.36767890707509,230.28931014351053,201.24555983227617]
[null,null,"Distribution substations installed ","total spend $0s",20503600.879896771,21128442.874061864,22799450.030101094,21332090.738165796,22687354.936357763,21293168.442341842,18607705.243077233]
[null,null,"Augmentation HV ","net circuit KM added",25.381999999999998,26.155509959972367,28.224098003752186,26.407611535542646,28.085332248114462,26.359428500845933,23.03501600749869]
[null,null,"Augmentation HV","total spend $0s",20475873.437116161,21099870.444552258,22768617.863115303,21303242.911445115,22656674.35788152,21264373.25104538,18582541.659108341]
[null,null,"Augmentation LV","net circuit KM added",16.504250000000003,17.007212798710661,18.352279941628989,17.171137920001566,18.262049671260858,17.13980765247366,14.978160229365702]
[null,null,"Augmentation LV","total spend $0s",5556899.7742094174,5726244.8739619656,6179122.3632619558,5781437.6557902023,6148742.2751612831,5770888.9088582462,5043072.8567874776]
[null,"SUBDIVISION","Underground connections","0's",797.48786534446765,727.93830217686298,691.28519409984506,710.77530881262362,786.51988043433948,812.36793152108351,817.34022194035856]
[null,null,"Overhead connections","0's",1.6683846555323592,1.522883477357454,1.4462033349369143,1.4869776334992124,1.6454390804065677,1.6995145010901329,1.7099167823020054]
[null,null,"Distribution substations installed","MVA added",6.1715000000000009,5.6694081078748937,5.4341752334711622,5.587251460672185,6.1172225859409446,6.2979185780404965,6.3363889230413992]
[null,null,"Distribution substations installed","0's",27.75,25.49235599020146,24.434637078315607,25.122940619566254,27.50594292471218,28.318438068641949,28.49141904146461]
[null,null,"Distribution substations installed ","total spend $0s",1329420.5264277121,1221263.4710045499,1170591.2824405197,1203565.8718513844,1317728.4728959086,1356652.7151288122,1364939.7225505016]
[null,null,"Augmentation HV ","net circuit KM added",5.0687500000000005,4.6563740333453572,4.4631735744400798,4.5888974870423951,5.0241711062931484,5.1725795661415805,5.204175865456711]
[null,null,"Augmentation HV","total spend $0s",774346.36022846855,711348.21890669898,681833.23549900064,701039.91448638111,767536.10048298643,790208.26831741235,795035.19396404328]
[null,null,"Augmentation LV","net circuit KM added",11.307044398238748,10.387142378267223,9.9561631098870365,10.236619999991039,11.207600643788885,11.538660775888605,11.609143786330275]
[null,null,"Augmentation LV","total spend $0s",3749980.688361404,3444895.2311383649,3301960.9791280371,3394974.4921882427,3717000.1723546544,3826796.2479987643,3850171.9347569244]
[null,null,"Cost per lot","$0's",7324.9099597451495,7371.8890419464515,7440.6696681491512,7440.4898018237,7361.7356689911967,7338.0372359003259,7337.9474187557298]
[null,"EMBEDDED GENERATION","Underground connections","0's",7928.4589535087352,7625.3685930287284,7625.3685930287284,7596.5028444115851,7596.5028444115851,7596.5028444115851,7582.0699701030135]
[null,null,"Overhead connections","0's",5255.5410464912648,5054.6314069712716,5054.6314069712716,5035.4971555884149,5035.4971555884149,5035.4971555884149,5025.9300298969865]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Underground connections","0's",8832.8037306041606,8732.6440858613714,8944.9346476269639,9245.0145394460014,9395.0544853555166,9468.478288672939,9517.1614626116661]
[null,null,"Overhead connections","0's",323.4462693958402,319.77854797644306,327.55236389325302,338.54091571551066,344.03519162663935,346.72387983846829,348.50659702239841]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0.22539016345017723,0.22283434998616125,0.22825145262702387,0.23590871049531092,0.23973733942945441,0.24161092380148208,0.24285319170032654]
[null,null,"Augmentation LV","total spend $0s",3142554.246261891,3106919.2286060639,3182448.4293745905,3289211.5101601761,3342593.0505529679,3368715.9320217818,3386036.5382130612]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993,8.4499999999999993]
[null,null,"Volume of GSL breaches for residential customers","0's",353.25,353.25,353.25,353.25,353.25,353.25,353.25]
[null,null,"Volume of customer complaints relating to connection services","0's",402,402,402,402,402,402,402]
[null,null,"GSL payments","$0's",69790,69790,69790,69790,69790,69790,69790]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",1844.4898914557079,1889.0297510145749,1858.1651165289156,1725.3637978311228,1678.1879881518853,1685.1504504479515,1687.5144552643733]
[null,null,"Overhead connections","0's",1666.7701816167921,1707.0185506374155,1679.127775705276,1559.1220878941181,1516.4917469899865,1522.7833643089382,1524.9195932768839]
[null,null,"Distribution substations installed","MVA added",145.99725000000001,150.44647886311469,162.34499614996096,151.8965669867427,161.54681560007205,151.61941819774361,132.49739936966307]
[null,null,"Distribution substations installed","0's",221.74999999999997,228.50777454983347,246.58000678953772,230.71026152417383,245.36767890707509,230.28931014351053,201.24555983227617]
[null,null,"Distribution substations installed ","total spend $0s",7784575.6134917,7974029.0946108028,8476554.7170990035,7978383.4290503608,8069659.4924132666,8087602.3150400007,7181407.2522378704]
[null,null,"Augmentation HV ","net circuit KM added",25.381999999999998,26.15550995997237,28.224098003752186,26.407611535542646,28.085332248114465,26.359428500845937,23.03501600749869]
[null,null,"Augmentation HV","total spend $0s",7774048.3711717399,7963245.6504369304,8465091.6971508581,7967594.096420126,8058746.7252780916,8076665.2834553448,7171695.6869456526]
[null,null,"Augmentation LV","net circuit KM added",16.504250000000003,17.007212798710661,18.352279941628989,17.171137920001566,18.262049671260858,17.13980765247366,14.978160229365702]
[null,null,"Augmentation LV","total spend $0s",2109780.946396668,2161126.7569506643,2297321.5909457542,2162306.8716147048,2187044.5720246546,2191907.4479451925,1946309.8492905996]
[null,"SUBDIVISION","Underground connections","0's",797.48786534446765,727.93830217686298,691.28519409984506,710.77530881262362,786.51988043433948,812.36793152108351,817.34022194035856]
[null,null,"Overhead connections","0's",1.6683846555323592,1.522883477357454,1.4462033349369143,1.4869776334992124,1.6454390804065677,1.6995145010901329,1.7099167823020054]
[null,null,"Distribution substations installed","MVA added",6.1715000000000009,5.6694081078748946,5.4341752334711622,5.587251460672185,6.1172225859409446,6.2979185780404965,6.3363889230413992]
[null,null,"Distribution substations installed","0's",27.75,25.49235599020146,24.434637078315603,25.122940619566254,27.50594292471218,28.318438068641949,28.491419041464606]
[null,null,"Distribution substations installed ","total spend $0s",777866.27573215915,685949.78302409756,641515.41742888663,668961.11829668179,766767.55291706172,800122.70501422952,807045.19936784077]
[null,null,"Augmentation HV ","net circuit KM added",5.0687500000000005,4.6563740333453572,4.4631735744400798,4.5888974870423951,5.0241711062931484,5.1725795661415805,5.2041758654567118]
[null,null,"Augmentation HV","total spend $0s",453083.05941101641,399544.54382580199,373662.89946743677,389649.1717931726,446618.39646636567,466046.74145417206,470078.88041987992]
[null,null,"Augmentation LV","net circuit KM added",11.307044398238748,10.387142378267223,9.9561631098870365,10.236619999991039,11.207600643788885,11.538660775888605,11.609143786330275]
[null,null,"Augmentation LV","total spend $0s",2194176.6763308784,1934902.0030840717,1809563.1734442301,1886981.0003746855,2162869.8058600812,2256956.7961955187,2276483.5145102181]
[null,null,"Cost per lot","$0's",4285.927828849557,4140.5853927993658,4077.6865330497621,4135.5429685344589,4283.6898194431924,4327.8063259735809,4338.6935991976306]
[null,"EMBEDDED GENERATION","Underground connections","0's",7928.4589535087352,7625.3685930287284,7625.3685930287284,7596.5028444115851,7596.5028444115851,7596.5028444115851,7582.0699701030135]
[null,null,"Overhead connections","0's",5255.5410464912648,5054.6314069712716,5054.6314069712716,5035.4971555884149,5035.4971555884149,5035.4971555884149,5025.9300298969865]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0s",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0s",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,15303186.385206738,15129655.787389396,15742099.269037437,16563987.087236922,17134665.800070096,17531733.871631753,17871939.238735758]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,4280129.1793361949,4384199.9790939828,4375979.5316435657,4153722.7944338126,4197066.4468327332,4351789.0898390515,4458814.3560885033]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,19770216.526104975,20250926.840922035,20212956.018260695,19186336.578773607,19386543.945667095,20101218.672891229,20595575.875410024]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,2689409.3302978249,2754801.9780785069,2749636.6788209258,2609982.1689385478,2637217.0532812029,2734436.6703241784,2801685.7503329092]
[null,null,"Complex connection HV (customer connected at HV)",null,19923436.736025516,20684416.478881262,25352403.713860925,24268615.740186147,28138507.264450129,24612372.765262108,18069385.845494147]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,2469130.9472360048,2253139.1886812616,2172538.5442909272,2274127.7756894873,2562852.2195432065,2687811.6741649644,2742639.5738418265]
[null,null,"Complex connection HV (no upstream asset works)",null,2831720.3249268588,2619467.2897344069,2575852.4506664262,2696163.7136975368,2970816.7252507531,3094330.636388272,3157368.4948611697]
[null,null,"Complex connection HV (with upstream asset works)",null,489586.34202669526,446758.87874569558,430777.15258563444,450920.55577184487,508169.66379435395,532946.98164313054,543818.41431212297]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,3108753.6649482548,3073501.9292400107,3197916.2747378564,3364878.0239245393,3480808.0985750761,3561470.1771533312,3630580.9267186644]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,2635079.6127880923,2706752.3321555564,2696156.128491363,2537355.9985668017,2561409.1621182575,2662950.5569123956,2731917.051757711]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,10621343.370286105,10910389.968664106,10867568.728703965,10227046.384146336,10323946.054335793,10733359.48967158,11011407.554282483]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,929879.19338147203,961380.18791885418,953119.59805247642,879138.32681426336,885476.8024218448,926443.58215313952,953293.31513762346]
[null,null,"Complex connection HV (customer connected at HV)",null,3529930.4428648613,3563463.6124332286,5073257.8011128772,5143299.360486812,5572254.1524803303,5354926.332595774,3029171.1974370065]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,1465205.5675645536,1279393.7719889907,1199653.5855803832,1274962.5214944263,1511124.8060376702,1608053.7370312989,1645227.7336314593]
[null,null,"Complex connection HV (no upstream asset works)",null,1453264.5678832792,1279980.9147012227,1225728.1292452214,1305927.4420271241,1517127.0500386795,1605200.3238579459,1643118.5478156514]
[null,null,"Complex connection HV (with upstream asset works)",null,471384.02576401137,430148.8434852598,414761.30145375268,434155.79364321358,489276.43875626213,513132.56143084826,523599.80542323214]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,12194432.720258484,12056153.858149385,12544182.994299581,13199109.063312382,13653857.701495022,13970263.694478424,14241358.312017092]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1645049.5665481028,1677447.6469384264,1679823.4031522027,1616366.7958670114,1635657.284714476,1688838.5329266556,1726897.3043307927]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,9148873.1558188703,9340536.8722579293,9345387.2895567305,8959290.194627272,9062597.8913313039,9367859.1832196489,9584168.3211275414]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,1759530.1369163529,1793421.7901596527,1796517.0807684495,1730843.8421242842,1751740.2508593579,1807993.088171039,1848392.4351952856]
[null,null,"Complex connection HV (customer connected at HV)",null,16393506.293160655,17120952.866448034,20279145.912748046,19125316.379699335,22566253.111969799,19257446.432666335,15040214.648057142]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,1003925.3796714512,973745.4166922709,972884.95871054428,999165.25419506128,1051727.4135055363,1079757.9371336654,1097411.8402103672]
[null,null,"Complex connection HV (no upstream asset works)",null,1378455.7570435796,1339486.3750331842,1350124.3214212051,1390236.271670413,1453689.6752120738,1489130.312530326,1514249.9470455186]
[null,null,"Complex connection HV (with upstream asset works)",null,18202.316262683864,16610.035260435787,16015.851131881851,16764.762128631355,18893.225038091852,19814.420212282152,20218.608888890871]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,9156.25,9052.4226338378139,9272.4870115202175,9583.5554551615114,9739.0896769821557,9815.2021685114069,9865.6680596340648]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,883.88618602046483,905.37776686295638,889.63644176427533,829.47439104465843,823.36474431685974,840.90302433548163,849.52840795119732]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1375.3602164922368,1408.8019262369858,1384.3078311396612,1290.6934128909825,1281.1865723280939,1308.4767970027385,1321.8982189738751]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,18.802249842371346,19.259424169676301,18.924570732620161,17.644788418391911,17.514822472502541,17.887901187761432,18.071382523134659]
[null,null,"Complex connection HV (customer connected at HV)",null,1233.211420717427,1262.609184382372,1244.4240485976352,1146.673293371208,1072.6135960244153,1040.6660922309079,1022.93603909305]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,334.9375,305.63822783628092,290.12486711106646,298.30498908155795,330.25558313100703,341.15920453402686,343.2475415547288]
[null,null,"Complex connection HV (no upstream asset works)",null,417.8125,381.4761796562604,362.40915883090582,372.62655386893937,412.15217518299772,425.63996207659335,428.24497455095366]
[null,null,"Complex connection HV (with upstream asset works)",null,46.40625,42.346778161679147,40.197371492809637,41.330743495625448,45.757561200741314,47.268279411553443,47.557622616978186]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,9156.25,9052.4226338378139,9272.4870115202175,9583.5554551615114,9739.0896769821557,9815.2021685114069,9865.6680596340648]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,883.88618602046483,905.37776686295638,889.63644176427533,829.47439104465843,823.36474431685974,840.90302433548163,849.52840795119732]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1375.3602164922368,1408.8019262369858,1384.3078311396612,1290.6934128909825,1281.1865723280939,1308.4767970027385,1321.8982189738751]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,18.802249842371346,19.259424169676301,18.924570732620161,17.644788418391911,17.514822472502541,17.887901187761432,18.071382523134659]
[null,null,"Complex connection HV (customer connected at HV)",null,1233.211420717427,1262.609184382372,1244.4240485976352,1146.673293371208,1072.6135960244153,1040.6660922309079,1022.93603909305]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,334.9375,305.63822783628092,290.12486711106646,298.30498908155795,330.25558313100703,341.15920453402686,343.2475415547288]
[null,null,"Complex connection HV (no upstream asset works)",null,417.8125,381.4761796562604,362.40915883090582,372.62655386893937,412.15217518299772,425.63996207659335,428.24497455095366]
[null,null,"Complex connection HV (with upstream asset works)",null,46.40625,42.346778161679147,40.197371492809637,41.330743495625448,45.757561200741314,47.268279411553443,47.557622616978186]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RESIDENTIAL","Simple connection LV",null,435624.91666666669,440717.00596717116]
[null,null,"Complex connection LV",null,0,0]
[null,null,"Complex connection HV",null,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,21826.510817171791,22075.754796365749]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,34765.270503622705,35127.964375474025]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,507.6822619525343,511.62504364252959]
[null,null,"Complex connection HV (customer connected at HV)",null,30718.463156992126,31057.297492575504]
[null,null,"Complex connection sub-transmission",null,0,0]
[null,"SUBDIVISION","Complex connection LV",null,84057.765415299727,84363.403643136015]
[null,null,"Complex connection HV (no upstream asset works)",null,89787.316228004784,90168.792407661051]
[null,null,"Complex connection HV (with upstream asset works)",null,9005.0746066954962,9047.4213848571762]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0]

{"sheet":"2.6 Non-network","index":14,"n_rows":115,"n_cols":11,"rows_kept":115,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[12,1,16,1],[19,1,29,1],[32,1,36,1],[39,1,49,1],[55,1,56,3],[55,4,55,10],[57,1,57,3],[58,1,58,3],[59,1,59,3],[62,4,62,10],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1],[84,1,88,1],[94,4,94,10],[97,1,97,3],[98,1,98,3],[99,1,99,3],[100,1,100,3],[101,1,101,3],[102,1,102,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[106,1,106,3],[108,1,108,3],[109,1,109,3],[116,1,116,3],[117,1,117,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,115,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2021)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,21262196.902048059,21668886.853003982,22787969.701184019,23219344.780612499,23954334.794101182,24533486.504942477,24977058.603360701]
[null,"MOTOR VEHICLES","Car",null,316239.3040125969,322288.13084040367,328452.65582947171,334887.88354794908,341271.20052991225,347652.11535757844,354312.37648871634]
[null,null,"Light commercial vehicle",null,2776880.1685577082,2829994.5887074168,2884124.9481330733,2940632.333536631,2996683.8935796712,3052714.3604361764,3111197.7520254012]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,3916660.5580915455,3991575.9818184236,4067924.3407279495,4147625.3844233081,4226683.5076098405,4305711.8798360396,4388199.9885180611]
[null,null,"Heavy commercial vehicle",null,1385059.1517543837,1411551.693474933,1438550.9678977833,1466735.8612111886,1494693.3968249944,1522640.4115271019,1551810.9020882281]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,4870584.8898916226,4963746.3792298147,5058689.8030362306,5157802.4765430605,5256115.6426968165,5354391.811879375,5456970.3554583872]
[null,"OTHER","Other expenditure",null,0,0,0,0,0,0,0]
[null,"OTHER - DNSP nominated","Office furniture and equipment"]
[null,null,"Plant and equipment"]
[null,null,"Crane borer plant HCV"]
[null,null,"Other fleet assets"]
[null,null,"EWP Hired"]
[null,null,"Car Hired"]
[null,null,"LCV Hired"]
[null,null,"Other Hire"]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,28773136.064881667,24673033.950844131,56262617.58287093,38431417.151463956,39809519.360348433,35614308.745686792,24143290.087472178]
[null,"MOTOR VEHICLES","Car",null,24007.656146233097,149312.92270294443,134170.98432203502,122298.76571250128,360922.82300937647,0,87469.589083966071]
[null,null,"Light commercial vehicle",null,301634.65414497996,821758.1717104495,330103.21539548301,697317.52379934932,1156249.7623354276,1325933.0781556077,499670.02764215617]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,1256313.8747421829,2030226.0712846399,4259396.3276836518,268199.04761513433,405227.72044465918,271707.5979827065,546684.93177478795]
[null,null,"Heavy commercial vehicle",null,477882.86046652583,1579064.7221102754,745394.35734463914,268199.04761513433,135075.90681488637,0,820027.39766218199]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,1588564.8165809163,1588564.8165809163,15774141.875035444,15478839.834059861,17988058.510538418,12366771.322182888,9435781.9224328399]
[null,"OTHER","Other expenditure",null,328928.23092124454,328928.23092124454,421297.53409864247,421297.53409864247,421297.53409864247,421297.53409864247,421297.53409864247]
[null,"OTHER - DNSP nominated"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Employee numbers",null,null,215,215,215,215,215,215,215]
[null,"User numbers",null,null,1142,1142,1142,1142,1142,1142,1142]
[null,"Number of devices",null,null,893,893,893,893,893,893,893]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"CAR","Average kilometres travelled ","0's",19101.366666666669,19101.366666666669,19101.366666666669,19101.366666666669,19101.366666666669,19101.366666666669,19101.366666666669]
[null,null,"Number purchased","0's",1,2,3,3,9,null,2]
[null,null,"Number leased","0's",1,2.5,2,2,1,2.5,2]
[null,null,"Number in fleet","0's",33,34.5,32.5,26.75,35.75,31.5,30.5]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",23398.828671328672,23398.828671328672,23398.828671328672,23398.828671328672,23398.828671328672,23398.828671328672,23398.828671328672]
[null,null,"Number purchased","0's",8,12,5,7,17,30,8]
[null,null,"Number leased","0's"]
[null,null,"Number in fleet","0's",175.5,187.5,192.5,192.45833333333331,209.45833333333331,214.5,216]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's"]
[null,null,"Number leased","0's"]
[null,null,"Number in fleet","0's"]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0,0,0,0,0,0,0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",18036.727611940296,18036.727611940296,18036.727611940296,18036.727611940296,18036.727611940296,18036.727611940296,18036.727611940296]
[null,null,"Number purchased","0's",5,5,15,1,3,1,1]
[null,null,"Number leased","0's",0,0,11,11,5.5,5.5,0]
[null,null,"Number in fleet","0's",81,86,95.5,85.75,88.75,62,60.5]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",13593.663461538461,13593.663461538461,13593.663461538461,13593.663461538461,13593.663461538461,13593.663461538461,13593.663461538461]
[null,null,"Number purchased","0's",1,7,5,1,1,null,3]
[null,null,"Number leased","0's",0,1.5,1.5,4,4,0,1.5]
[null,null,"Number in fleet","0's",45.5,51,53.5,49,42,32,46.5]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",1,1,1,1,1,1,1]
[]
[]
[null,"Table 2.6.4 intentionally omitted"]
[]
[null,"2.6.5 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2021)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"RECURRENT"]
[null,"Market Compliance","Market Compliance","Market Compliance",1562765.4184530757,1738027.2097463524,4551978.8905780977,2091529.2570767682,2803730.6877271822,2017809.9217848768,4829606.6980463201]
[null,"Customer Engagement","Customer Engagement","Customer Engagement",1046543.8595044198,1163912.1793545505,3052949.055477811,1207072.7056395716,611913.99086648982,0,209495.63485928776]
[null,"Corporate Services","Corporate Services","Corporate Services",7273826.8348198934,8089575.574569677,4020262.5038308282,5203444.0852240063,3798966.0713538812,12259757.696012871,3606449.8403589246]
[null,"Field Work & Construction","Field Work & Construction","Field Work & Construction",1569079.1999492494,1745049.0723414472,2658601.9302568776,3413569.0704011731,1368460.1280240624,654788.31077130046,1254083.0932587995]
[null,"Service Management and Ops","Service Management and Ops","Service Management and Ops",1332264.1731523136,1481675.5964570723,786450.75291822141,537248.41628065729,546022.54919921805,617204.26651005715,770019.38925927959]
[null,"Network Assets and Network Operations","Network Assets and Network Operations","Network Assets and Network Operations",9918783.3590129539,11031159.994958302,6865527.4985329164,6365515.0015448965,5454327.1111747855,5232638.4683456682,7395778.073353448]
[null,"Cyber Security","Cyber Security","Cyber Security",1289662.6595240047,1434296.387147672,4696327.4054190041,2462260.1328989947,1788797.1915532434,1993295.7667875916,2692937.617733052]
[]
[]
[]
[null,"NON-RECURRENT"]
[null,"Market Compliance","Market Compliance","Market Compliance",1808058.5213471141,2010829.5652111638,14447566.175567403,3109288.299764378,123661.35288152,145944.03785362007,246378.88320786672]
[null,"Customer Engagement","Customer Engagement","Customer Engagement",1526898.9823055046,1698138.4067276539,9046495.8039410226,1098347.4569138922,1954188.730138917,914680.42180406046,0]
[null,"Corporate Services","Corporate Services","Corporate Services",221739.35070183148,246607.0853888964,0,0,0,0,0]
[null,"Field Work & Construction","Field Work & Construction","Field Work & Construction",1184705.4153670678,1317568.3459133597,0,3647516.3008077624,11421648.405982556,8697026.4706891477,0]
[null,"Service Management and Ops","Service Management and Ops","Service Management and Ops",0,0,0,0,0,0,0]
[null,"Network Assets and Network Operations","Network Assets and Network Operations","Network Assets and Network Operations",38808.29074423237,43160.582183850434,4166568.704726004,8230229.8994365092,9171175.7736380473,2253103.4902349273,1972196.2086955495]
[null,"Cyber Security","Cyber Security","Cyber Security",0,0,1969888.8616227314,1065396.5254753451,766627.3678085329,828059.89489266055,1166344.6486996557]

{"sheet":"2.10 Overheads","index":15,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[23,3,23,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE ($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE ($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",16183565.146717999,16493114.218534598,27898032.017861366,27037328.577475421,27652194.363200709,28234500.32955689,28831060.35180705]
[null,"Alternative Control Services","Total  ",681665.84641924116,{"$f":"D13","v":681665.84641924116},{"$f":"E13","v":681665.84641924116},681665.84641924116,681665.84641924116,681665.84641924116,681665.84641924116]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",22311277.895483259,22738034.008921564,23172952.845320437,23626970.268600453,24077325.291750468,24527510.83839523,24997404.792333938]
[null,"Alternative Control Services","Total  ",1040643.0765921297,{"$f":"D16","v":1040643.0765921297},{"$f":"E16","v":1040643.0765921297},1040643.0765921297,1040643.0765921297,1040643.0765921297,1040643.0765921297]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",487464.46850274556,{"$f":"D18","v":487464.46850274556},487464.46850274556,487464.46850274556,487464.46850274556,487464.46850274556,487464.46850274556]
[null,"Unregulated Distribution Services","Total  ",0,{"$f":"D19","v":0},0,0,0,0,0]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",54578305.008656576,55622244.554954819,58176572.269067995,59290364.58553277,60702334.133466512,61957735.736033939,63106621.073840901]
[null,"Alternative Control Services","Total  ",9075677.9001396056,{"$f":"D28","v":9075677.9001396056},9075677.9001396056,9075677.9001396056,9075677.9001396056,9075677.9001396056,9075677.9001396056]
[null,"CAPEX"]
[null,"Standard Control Services","Total",0,{"$f":"D30","v":0},0,0,0,0,0]
[null,"Alternative Control Services","Total",0,{"$f":"D31","v":0},0,0,0,0,0]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0,{"$f":"D33","v":0},0,0,0,0,0]
[null,"Unregulated Distribution Services","Total",0,{"$f":"D34","v":0},0,0,0,0,0]

{"sheet":"2.11 Labour","index":16,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[8,2,8,8],[9,2,9,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"($0's, real \", dms_DollarReal,\")\")","v":"($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"In-house labour expenditure"]
[null,"Labour expenditure outsourced to related parties"]
[null,"Labour expenditure outsourced to unrelated parties"]
[null,"Controllable non-labour expenditure"]
[null,"Uncontrollable non-labour expenditure"]
[null,"Total",{"$f":"SUM(C13:C17)","v":0},0,0,0,0,0,0]
[null,"CAPEX"]
[null,"In-house labour expenditure"]
[null,"Labour expenditure outsourced to related parties"]
[null,"Labour expenditure outsourced to unrelated parties"]
[null,"Controllable non-labour expenditure"]
[null,"Uncontrollable non-labour expenditure"]
[null,"Total",{"$f":"SUM(C20:C24)","v":0},0,0,0,0,0,0]

{"sheet":"2.14 Forecast price changes","index":17,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[[11,4,11,8],[12,2,12,8],[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,1,13,1],[11,2,11,3]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet. It has been grouped for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"United Energy must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"OPEX"]
[null,"CPI",0.02,0.02,2.3998043050028173E-2,2.3998043050028173E-2,2.3998043050028173E-2,2.3998043050028173E-2,2.3998043050028173E-2]
[null,"Real labour escalation",1.43E-2,1.38E-2,2.0036529680365511E-2,2.1723181818181558E-2,2.1601809954751472E-2,1.9069819819819811E-2,1.7140807174887973E-2]
[null,"Real non-labour escalation",0,0,0,0,0,0,0]
[null,"CAPEX"]
[null,"CPI"]
[null,"Real labour escalation",{"$f":"C17","v":1.43E-2},{"$f":"D17","v":1.38E-2},2.0036529680365511E-2,2.1723181818181558E-2,2.1601809954751472E-2,1.9069819819819811E-2,1.7140807174887973E-2]
[null,"Real materials escalation",0,0,0,0,0,0,0]
[null,"Real contracts escalaction",4.7000000000000002E-3,5.5999999999999999E-3,1.4310502283105153E-2,1.9211818181818163E-2,1.8789140271493032E-2,1.3946846846846661E-2,1.4428699551569668E-2]

{"sheet":"2.16 Opex Summary","index":18,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[[5,1,5,6],[7,9,7,11],[8,1,8,7],[8,9,8,10],[8,11,9,11],[9,1,9,7],[9,9,9,10],[42,2,42,11],[43,2,43,11],[56,2,56,11],[57,2,57,11],[10,1,10,7],[10,9,10,10],[14,2,14,11],[15,2,15,11],[28,2,28,11],[29,2,29,11]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nUnited Energy's total forecast opex must reconcile to Table 2.16.1 (and if United Energy owns any dual function assets Table 2.16.3). If United Energy did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if United Energy owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has United Energy used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If United Energy does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,2019]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Base year total opex, excluding category specific",null,null,123313865.97117098,{"$f":"E18","v":123313865.97117098},{"$f":"F18","v":123313865.97117098},{"$f":"G25-G24","v":126853177.80749485},{"$f":"H18","v":126853177.80749485},{"$f":"I18","v":126853177.80749485},126853177.80749485,126853177.80749485]
[null,"Increment from base year to final year",null,null,null,null,3539311.8363238852]
[null,"Price growth",null,null,null,null,null,1572995.745938719,3310132.5357921976,5070613.0302832695,6656109.5117503786,8110140.9964864627]
[null,"Output growth",null,null,null,null,null,1658324.037737862,3277806.5618707216,4865744.6253939373,6640931.4890965903,8676924.3426168784]
[null,"Productivity growth",null,null,null,null,null,-682446.15104585676,-1378263.1679064159,-2087343.1924727438,-2809681.2336420887,-3545857.7062968686]
[null,"Step changes",null,null,null,null,null,14992684.254744191,13814851.648379015,14881650.74233686,15165131.392520387,14960299.879567061]
[null,"Category specific",null,null,null,null,6404732.6179999039,{"$f":"G24","v":6404732.6179999039},{"$f":"H24","v":6404732.6179999039},6404732.6179999039,6404732.6179999039,6404732.6179999039]
[null,"Total opex",{"$f":"SUM(C18:C24)","v":0},0,123313865.97117098,123313865.97117098,133257910.42549476,150799468.31286967,152282438.00363028,155988575.63103607,158910401.58522004,161459417.9378683]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C32:C38)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,2017,2018,2019,2020,2021,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Base year total opex, excluding category specific"]
[null,"Increment from base year to final year"]
[null,"Price growth"]
[null,"Output growth"]
[null,"Productivity growth"]
[null,"Step changes"]
[null,"Category specific"]
[null,"Total opex",{"$f":"SUM(C46:C52)","v":0},0,0,0,0,0,0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C60:C66)","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"2.17 Step Changes","index":19,"n_rows":89,"n_cols":11,"rows_kept":89,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[9,4,9,10],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,1,21,3],[22,1,22,3],[25,4,25,10],[26,4,26,10],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,2,30,3],[31,2,31,3],[32,2,32,3],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,1,38,3],[41,4,41,10],[42,4,42,10],[43,2,43,3],[44,2,44,3],[45,2,45,3],[46,2,46,3],[47,2,47,3],[48,2,48,3],[49,2,49,3],[50,2,50,3],[51,2,51,3],[52,2,52,3],[53,2,53,3],[54,1,54,3],[55,1,55,3],[58,4,58,10],[59,4,59,10],[60,2,60,3],[61,2,61,3],[62,2,62,3],[63,2,63,3],[64,2,64,3],[65,2,65,3],[66,2,66,3],[76,3,76,10],[88,1,88,2],[67,2,67,3],[68,2,68,3],[69,2,69,3],[70,2,70,3],[71,1,71,3],[75,3,75,10]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Security of critical infrastructure","To comply with new critical infrastructure system and data control regulatory obligations",null,null,null,10050225.043777829,8811196.5105774868,8921952.153058378,9020954.9153566081,9110930.4869439863]
[null,"Demand management programs","Reducing costs for customers through efficient demand management initiatives",null,null,null,1482883.5447925481,1627236.3495269245,2057858.5560298443,1972201.2767004871,1474029.0399147184]
[null,"IT cloud solutions","Reducing costs and delivering customer benefits by migrating IT infrastructure to cloud\n",null,null,null,704613.98721916752,703319.63838981884,1009130.4169239444,1159264.400494904,1155037.0578174996]
[null,"Solar enablement","Operating expenditure associated with enabling more solar on the network",null,null,null,929932.49500403716,794608.08899863705,832283.95072825789,791511.11196391017,829709.94966698403]
[null,"5 minute settlement","To comply with the 5-minute settlement rule change ",null,null,null,591623.09301145247,619115.46587096003,774888.86576339754,909816.4999491442,1053566.8527390151]
[null,"ESV levy","Material increase in ESV levy",null,null,null,447599.73045345896,469109.29008480662,490779.40813444095,512611.28309299238,534606.12239724281]
[null,"Increasing insurance premiums","Material increase in insurance premiums due to worsening global insurance market conditions",null,null,null,432976.62492484221,432976.62492484221,432976.62492484221,432976.62492484221,432976.62492484221]
[null,"Financial year RIN","Prepare and audit an additional RIN on annual basis for calendar year accounts",null,null,null,352829.73556085426,357289.68000553781,361780.76677375386,365795.2800375013,369443.74516277434]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E12:E21)","v":0},0,14992684.254744191,13814851.648379013,14881650.742336862,15165131.39252039,14960299.879567062]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$22,0)-ROUND('2.16 Opex Summary'!H$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(H$22,0)-ROUND('2.16 Opex Summary'!I$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(I$22,0)-ROUND('2.16 Opex Summary'!J$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(J$22,0)-ROUND('2.16 Opex Summary'!K$23,0)=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(ROUND(K$22,0)-ROUND('2.16 Opex Summary'!L$23,0)=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E29:E38)","v":0},0,0,0,0,0,0]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E45:E54)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(ROUND(G$22,0)-ROUND('2.16 Opex Summary'!H$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(H$22,0)-ROUND('2.16 Opex Summary'!I$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(I$22,0)-ROUND('2.16 Opex Summary'!J$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(J$22,0)-ROUND('2.16 Opex Summary'!K$51,0)=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(ROUND(K$22,0)-ROUND('2.16 Opex Summary'!L$51,0)=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E62:E71)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,"Category","Description",{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Communications network","Reclassification from metering services to standard control",null,null,null,933370.30553717096,{"$f":"G79","v":933370.30553717096},{"$f":"H79","v":933370.30553717096},933370.30553717096,933370.30553717096]
[null,"Wasted truck visits","Reclassification from alternative control services to standard control",null,null,null,221838.3452600537,{"$f":"G80","v":221838.3452600537},221838.3452600537,221838.3452600537,221838.3452600537]
[null,"Replacement expenditure on faults and minor repairs","Reclassification from capital expenditure to operating expenditure",null,null,null,5249523.9672026793,{"$f":"G81","v":5249523.9672026793},5249523.9672026793,5249523.9672026793,5249523.9672026793]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D86:D88)","v":0},0,0,{"$f":"SUM(G79:G88)","v":6404732.6179999039},{"$f":"SUM(H79:H88)","v":6404732.6179999039},6404732.6179999039,6404732.6179999039,6404732.6179999039]

{"sheet":"3.1 Revenue","index":20,"n_rows":53,"n_cols":17,"rows_kept":53,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[9,2,9,8],[9,10,9,16],[10,2,10,8],[10,10,10,16],[29,2,29,8],[29,10,29,16],[30,2,30,8],[30,10,30,16],[31,2,31,8],[31,10,31,16],[43,2,43,8],[43,10,43,16],[44,2,44,8],[44,10,44,16],[45,2,45,8],[45,10,45,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0101","Revenue from Fixed Customer Charges ",20114674.131905623,24957004.993705265,57249218.996008568,56711434.345888779,56135414.698652357,55533719.817961328,54905105.526219003,null,0,0,0,0,0,0,0]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",230722557.85436478,214250303.50832072,184180911.44832331,175538234.63766146,165148873.58568633,154783151.97729582,144439363.09761295,null,0,0,0,0,0,0,0]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",47423492.584347956,44034560.220140964,47467955.820492215,52757294.025363907,59179638.615683556,65599095.224626847,72017218.353735223,null,0,0,0,0,0,0,0]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",1883523.2602642127,1748972.5654395367,1581992.5103441582,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",28453658.608759917,26416864.728507489,28054063.015430108,32385022.746855766,36736419.769760527,41085615.767036587,45433653.569220819,null,0,0,0,0,0,0,0]
["DREV0106","Revenue from controlled load customer charges",1966716.7302103369,1826223.0563833434,1651867.6476152793,1670807.862308441,1673985.7866213301,1677281.8604499993,1680701.9468373146,null,0,0,0,0,0,0,0]
["DREV0107","Revenue from unmetered supplies",3327212.8026443361,3089531.217356903,2794563.7015208285,2826606.0001619649,2831982.2855706676,2837558.4516106211,2843344.417143547,null,0,0,0,0,0,0,0]
["DREV0108","Revenue from Contracted Maximum Demand charges",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0109","Revenue from Measured Maximum Demand charges",112722066.77996285,105175167.94896555,95166515.654215828,96257689.175710186,96440774.051975623,96630665.694969118,96827701.883181319,null,0,0,0,0,0,0,0]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,39328706.328697748,19664371.960070539,30882141.197633091,30882141.197633091,30882141.197633084,30882141.197633084,30882141.197633084]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,{"$f":"SUM('4.2 Metering'!E44:E46)","v":10368184.337279599},{"$f":"SUM('4.2 Metering'!F44:F46)","v":13182785.147727612},{"$f":"SUM('4.2 Metering'!G44:G46)","v":11098143.31484223},{"$f":"SUM('4.2 Metering'!H44:H46)","v":10934742.260251457},{"$f":"SUM('4.2 Metering'!I44:I46)","v":10794779.016709179},{"$f":"SUM('4.2 Metering'!J44:J46)","v":10729215.194288487},{"$f":"SUM('4.2 Metering'!K44:K46)","v":10640581.863130575}]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,4610914.1509809289,4703132.434000548,6907949.9672736516,6746595.8670628918,6603494.8118720474,6446218.5916475533,6356693.0994926011]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,{"$f":"L25/1.02","v":3979208.1689151321},{"$f":"M25/1.02","v":4058792.332293435},4139968.1789393038,4198880.86091353,4264623.7953594029,4338014.2198798563,4419967.4166632574]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":446613902.75246},421498628.23881984,418147088.7939502,418147088.79395056,418147088.79395044,418147088.79395026,418147088.7939502,null,{"$f":"SUM(K13:K25)","v":58287012.985873401},41609081.874092132,53028202.658688277,52762360.185860969,52545038.821573719,52395589.203448981,52299383.576919518]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0201","Revenue from residential Customers ",209038663.23411843,199865675.45009077,211552081.58331755,209323254.30280989,209007400.3819102,208680187.67104408,208341049.80396178,null,0,0,0,0,0,0,0]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",56562470.547532693,52825324.826654039,31807879.367646459,30516930.449596606,28965544.261766639,27421302.392282654,25883941.345781431,null,0,0,0,0,0,0,0]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",152539928.73312134,142057129.3711915,130488033.5448477,131963960.41135398,132203368.13729724,132451604.41006608,132709107.84408593,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",23198116.478517909,21540944.116138641,19484360.664576408,19707767.167318217,19745251.903802071,19784130.255434886,19824471.378872141,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",3327212.8026443361,3089531.217356903,2794563.7015208285,2826606.0001619649,2831982.2855706676,2837558.4516106211,2843344.417143547,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",1947510.9565253342,2120023.2573879361,22020169.932041433,23808570.46270987,25393541.823603634,26972305.613511935,28545174.00410533,null,{"$f":"K26","v":58287012.985873401},{"$f":"L26","v":41609081.874092132},53028202.658688277,52762360.185860969,52545038.821573719,52395589.203448981,52299383.576919518]
["DREV02","Total revenue by customer class",{"$f":"SUM(C34:C39)","v":446613902.75246},421498628.23881984,418147088.79395032,418147088.7939505,418147088.7939505,418147088.79395026,418147088.79395014,null,{"$f":"SUM(K34:K39)","v":58287012.985873401},41609081.874092132,53028202.658688277,52762360.185860969,52545038.821573719,52395589.203448981,52299383.576919518]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DREV0301","EBSS",5236890.0925777182,0,31222586.835180152,30296272.10191245,12309280.957677422,-1389150.124589989,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",17680471.728818342,9458581.3884520326,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",114750,2550,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",-160892.01483995916,-80446.007419979578,8089940.4606836922,8089940.4606836922,8089940.4606836922,8089940.4606836922,8089940.4606836922,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C48:C52)","v":22871219.806556102},9380685.3810320534,39312527.295863844,38386212.562596142,20399221.418361112,6700790.3360937033,8089940.4606836922,null,{"$f":"SUM(K48:K52)","v":0},0,0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":21,"n_rows":85,"n_cols":17,"rows_kept":85,"cut":false,"hidden":false,"merged":[[9,2,9,8],[9,10,9,16],[10,2,10,8],[10,10,10,16],[11,2,11,8],[11,10,11,16],[80,2,80,8],[81,2,81,8],[82,2,82,8],[67,2,67,8],[67,10,67,16],[68,2,68,8],[68,10,68,16],[69,2,69,8],[69,10,69,16]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0101","Maintenance",{"$f":"'2.1 Expenditure summary'!C26","v":24835105.907987371},{"$f":"'2.1 Expenditure summary'!D26","v":26414613.05007799},{"$f":"'2.17 Step Changes'!G$13+(('2.16 Opex Summary'!H$25-'2.17 Step Changes'!G$13-'3.2 Operating expenditure'!E$17)*'3.2 Operating expenditure'!$D14/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":29088309.013325009},{"$f":"'2.17 Step Changes'!H$13+(('2.16 Opex Summary'!I$25-'2.17 Step Changes'!H$13-'3.2 Operating expenditure'!F$17)*'3.2 Operating expenditure'!$D14/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":29706499.960771274},{"$f":"'2.17 Step Changes'!I$13+(('2.16 Opex Summary'!J$25-'2.17 Step Changes'!I$13-'3.2 Operating expenditure'!G$17)*'3.2 Operating expenditure'!$D14/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":30682176.968218092},{"$f":"'2.17 Step Changes'!J$13+(('2.16 Opex Summary'!K$25-'2.17 Step Changes'!J$13-'3.2 Operating expenditure'!H$17)*'3.2 Operating expenditure'!$D14/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":31107132.333813109},{"$f":"'2.17 Step Changes'!K$13+(('2.16 Opex Summary'!L$25-'2.17 Step Changes'!K$13-'3.2 Operating expenditure'!I$17)*'3.2 Operating expenditure'!$D14/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":31177177.212056547}]
["DOPEX0102","Vegetation Management",{"$f":"'2.1 Expenditure summary'!C25","v":16480082.346490407},{"$f":"'2.1 Expenditure summary'!D25","v":17528211.871887408},{"$f":"(('2.16 Opex Summary'!H$25-'2.17 Step Changes'!G$13-'3.2 Operating expenditure'!E$17)*'3.2 Operating expenditure'!$D15/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":18318411.30925085},{"$f":"(('2.16 Opex Summary'!I$25-'2.17 Step Changes'!H$13-'3.2 Operating expenditure'!F$17)*'3.2 Operating expenditure'!$D15/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":18632840.876804601},{"$f":"(('2.16 Opex Summary'!J$25-'2.17 Step Changes'!I$13-'3.2 Operating expenditure'!G$17)*'3.2 Operating expenditure'!$D15/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":18994528.402365599},{"$f":"(('2.16 Opex Summary'!K$25-'2.17 Step Changes'!J$13-'3.2 Operating expenditure'!H$17)*'3.2 Operating expenditure'!$D15/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":19333360.798196316},{"$f":"(('2.16 Opex Summary'!L$25-'2.17 Step Changes'!K$13-'3.2 Operating expenditure'!I$17)*'3.2 Operating expenditure'!$D15/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":19710418.374719668}]
["DOPEX0103","Emergency",{"$f":"'2.1 Expenditure summary'!C27","v":15580195.765976164},{"$f":"'2.1 Expenditure summary'!D27","v":16571092.707535598},{"$f":"(('2.16 Opex Summary'!H$25-'2.17 Step Changes'!G$13-'3.2 Operating expenditure'!E$17)*'3.2 Operating expenditure'!$D16/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":17318143.703364421},{"$f":"(('2.16 Opex Summary'!I$25-'2.17 Step Changes'!H$13-'3.2 Operating expenditure'!F$17)*'3.2 Operating expenditure'!$D16/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":17615404.003046229},{"$f":"(('2.16 Opex Summary'!J$25-'2.17 Step Changes'!I$13-'3.2 Operating expenditure'!G$17)*'3.2 Operating expenditure'!$D16/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":17957341.763785146},{"$f":"(('2.16 Opex Summary'!K$25-'2.17 Step Changes'!J$13-'3.2 Operating expenditure'!H$17)*'3.2 Operating expenditure'!$D16/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":18277672.387619775},{"$f":"(('2.16 Opex Summary'!L$25-'2.17 Step Changes'!K$13-'3.2 Operating expenditure'!I$17)*'3.2 Operating expenditure'!$D16/SUM('3.2 Operating expenditure'!$D$14:$D$16))","v":18634140.92544413}]
["DOPEX0104","Overheads",{"$f":"'2.10 Overheads'!D12+'2.10 Overheads'!D27","v":70761870.155374572},{"$f":"'2.10 Overheads'!E12+'2.10 Overheads'!E27","v":72115358.773489416},{"$f":"'2.10 Overheads'!F12+'2.10 Overheads'!F27","v":86074604.286929369},{"$f":"'2.10 Overheads'!G12+'2.10 Overheads'!G27","v":86327693.163008183},{"$f":"'2.10 Overheads'!H12+'2.10 Overheads'!H27","v":88354528.496667221},{"$f":"'2.10 Overheads'!I12+'2.10 Overheads'!I27","v":90192236.065590829},{"$f":"'2.10 Overheads'!J12+'2.10 Overheads'!J27","v":91937681.425647944}]
["DOPEX0105","Public Lighting",null,null,null,null,null,null,null,null,{"$f":"'2.1 Expenditure summary'!C52","v":2749666.4436546406},{"$f":"'2.1 Expenditure summary'!D52","v":3394785.0840796423},{"$f":"'2.1 Expenditure summary'!E52","v":4039903.7245046441},{"$f":"'2.1 Expenditure summary'!F52","v":3973100.457610867},{"$f":"'2.1 Expenditure summary'!G52","v":3918291.7182181505},{"$f":"'2.1 Expenditure summary'!H52","v":3855224.4964738726},{"$f":"'2.1 Expenditure summary'!I52","v":3837635.9636825565}]
["DOPEX0106","Connections",null,null,null,null,null,null,null,null,{"$f":"'2.1 Expenditure summary'!C50","v":10368184.337279599},{"$f":"'2.1 Expenditure summary'!D50","v":13182785.147727612},{"$f":"'2.1 Expenditure summary'!E50","v":11098143.31484223},{"$f":"'2.1 Expenditure summary'!F50","v":10934742.260251457},{"$f":"'2.1 Expenditure summary'!G50","v":10794779.016709179},{"$f":"'2.1 Expenditure summary'!H50","v":10729215.194288487},{"$f":"'2.1 Expenditure summary'!I50","v":10640581.863130575}]
["DOPEX0107","Metering",null,null,null,null,null,null,null,null,{"$f":"'2.1 Expenditure summary'!C51","v":7638696.0770764677},{"$f":"'2.1 Expenditure summary'!D51","v":7857970.6789677124},{"$f":"'2.1 Expenditure summary'!E51","v":7017502.5630530277},{"$f":"'2.1 Expenditure summary'!F51","v":7205805.2039582543},{"$f":"'2.1 Expenditure summary'!G51","v":7396434.421316511},{"$f":"'2.1 Expenditure summary'!H51","v":7580823.2839377625},{"$f":"'2.1 Expenditure summary'!I51","v":7754817.9482922675}]
["DOPEX0108","Fee and quoted",null,null,null,null,null,null,null,null,{"$f":"'2.1 Expenditure summary'!C53","v":5022068.7158067375},{"$f":"'2.1 Expenditure summary'!D53","v":5167244.4171425831},{"$f":"'2.1 Expenditure summary'!E53","v":4083384.3601804958},{"$f":"'2.1 Expenditure summary'!F53","v":4142297.0421547252},{"$f":"'2.1 Expenditure summary'!G53","v":4208039.9766005948},{"$f":"'2.1 Expenditure summary'!H53","v":4281430.4011210501},{"$f":"'2.1 Expenditure summary'!I53","v":4363383.5979044521}]
["DOPEX0109"]
["DOPEX0110"]
["DOPEX0111"]
["DOPEX0112"]
["DOPEX0113"]
["DOPEX0114"]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C14:C62)","v":127657254.17582852},132629276.40299042,150799468.31286967,152282438.00363028,155988575.63103604,158910401.58522004,161459417.9378683,null,{"$f":"SUM(K14:K62)","v":25778615.573817447},29602785.327917553,26238933.962580398,26255944.963975303,26317545.132844437,26446693.375821173,26596419.373009849]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0201","Opex for network services",{"$f":"C63-C74","v":125104109.09231195},{"$f":"D63-D74","v":129976690.87493061},147783478.94661227,149236789.24355766,152868804.11841533,155732193.55351564,158230229.57911092]
["DOPEX0202","Opex for metering",null,null,null,null,null,null,null,null,{"$f":"K20","v":7638696.0770764677},{"$f":"L20","v":7857970.6789677124},7017502.5630530277,7205805.2039582543,7396434.421316511,7580823.2839377625,7754817.9482922675]
["DOPEX0203","Opex for connection services",{"$f":"C63*0.02","v":2553145.0835165703},{"$f":"D63*0.02","v":2652585.5280598085},3015989.3662573933,3045648.7600726057,3119771.512620721,3178208.0317044007,3229188.358757366,null,{"$f":"K19","v":10368184.337279599},{"$f":"L19","v":13182785.147727612},11098143.31484223,10934742.260251457,10794779.016709179,10729215.194288487,10640581.863130575]
["DOPEX0204","Opex for public lighting",null,null,null,null,null,null,null,null,{"$f":"K18","v":2749666.4436546406},{"$f":"L18","v":3394785.0840796423},4039903.7245046441,3973100.457610867,3918291.7182181505,3855224.4964738726,3837635.9636825565]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP"]
["DOPEX0207","Opex for transmission connection point planning"]
[]
[]
[null,"3.2.4 - OPEX FOR HIGH VOLTAGE CUSTOMERS"]
[null,null,"End user costs (not standard control services)"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPEX0401","Opex for high voltage customers"]

{"sheet":"3.3 Assets (RAB)","index":22,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,10,8,16],[8,18,8,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[21,2,21,8],[21,10,21,16],[21,18,21,24],[22,2,22,8],[22,10,22,16],[22,18,22,24],[97,2,97,8],[97,10,97,16],[97,18,97,24],[98,2,98,8],[98,10,98,16],[98,18,98,24],[114,2,114,8],[114,10,114,16],[114,18,114,24],[115,2,115,8],[115,10,115,16],[115,18,115,24]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",2288414511.1053491,{"$f":"C18","v":2320570786.6546392},2386036194.8387709,2497732784.0514221,2587722036.7036576,2666523673.9992485,2727681018.7276235,null,2372831834.857039,{"$f":"K18","v":2405672678.4436722},2473302106.2427373,2589119070.9764171,2682427937.2032266,2764136488.1263371,2827549866.1671538,null,0,{"$f":"S18","v":0},0,0,0,0,0]
["DRAB0102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-140956105.29488209,-137800191.95468083,-142737998.03542268,-155386252.86781585,-168506267.44280171,-178164653.72355697,-186869650.75913671,null,-146155835.11555511,-142883503.28697285,-148003460.09806457,-161118296.40767634,-174722295.20520085,-184736969.70106077,-193763085.37552518,null,0,0,0,0,0,0,0]
["DRAB0105","Actual additions (recognised in RAB)",173112380.84417218,203265600.13881248,254434587.24807429,245375505.52005148,247307904.73839289,239321998.45193189,204163820.70572791,null,179498323.5255484,210763864.93796879,263820424.83174428,254427162.63448551,256430846.12831137,248150347.74187753,211695219.96371138,null,0,0,0,0,0,0,0]
["DRAB0106","Disposals ",0,0,0,0,0,0,0,null,-501644.82336006337,-250933.8519306384,0,0,0,0,-2671555.6085316357,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":2320570786.6546392},{"$f":"SUM(D13+D14+D15+D16+D17)","v":2386036194.8387709},2497732784.0514221,2587722036.7036576,2666523673.9992485,2727681018.7276235,2744975188.6742148,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":2405672678.4436722},2473302106.2427373,2589119070.9764171,2682427937.2032266,2764136488.1263371,2827549866.1671538,2842810445.1468086,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":0},0,0,0,0,0,0]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",933084929.19612491,{"$f":"C31","v":945128533.41611993},962521827.87945175,1010633249.2599051,1053375980.5974007,1090081541.5857055,1120549719.2426915,null,967505499.49644411,{"$f":"K31","v":979993380.236992},998028295.94625366,1047914499.5679128,1092233967.537622,1130293559.9788826,1161885678.2527945,null,0,{"$f":"S31","v":0},0,0,0,0,0]
["DRAB0202","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-44210838.868094578,-45328475.898459606,-46777300.21053683,-53349830.203975946,-58887197.931469932,-64367341.078691393,-69640478.989748523,null,-45841732.519550689,-47000598.062744722,-48502868.055409275,-55317852.110222027,-61059487.797876008,-66741787.947694495,-72209446.64511475,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",56254443.08808957,62721770.361791357,94888721.590990156,96092561.541471437,95592758.919774726,94835518.735677451,81297473.759550095,null,58329613.260098532,65035513.772006407,98389071.677068532,99637320.079931065,99119080.239136606,98333906.221606404,84296456.299317136,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-1138940.7396295043,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":945128533.41611993},962521827.87945175,1010633249.2599051,1053375980.5974007,1090081541.5857055,1120549719.2426915,1132206714.0124931,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":979993380.236992},998028295.94625366,1047914499.5679128,1092233967.537622,1130293559.9788826,1161885678.2527945,1172833747.1673675,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",418892657.63388139,{"$f":"C38","v":424299429.53786093},432107854.16757894,453706661.02213228,472895285.51306659,489373624.74160826,503051796.48422945,null,434345189.03720868,{"$f":"K38","v":439951411.35196602},448047880.96075523,470443446.20940316,490339919.8763237,507426128.56679863,521608874.39192307,null,0,{"$f":"S38","v":0},0,0,0,0,0]
["DRAB0302","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-19847706.473658852,-20349450.667858817,-20999875.776592992,-23950501.673746906,-26436409.023750298,-28896626.368736684,-31263912.222914707,null,-20579868.525151037,-21100121.561117545,-21774540.201929837,-24834011.738901798,-27411621.726064477,-29962594.029605519,-32417206.692539189,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",25254478.377638374,28157875.297576834,42598682.631146289,43139126.164681211,42914748.252291948,42574798.111357875,36497122.369555146,null,26186090.839908332,29196591.169906761,44170105.450577721,44730485.405822314,44497830.416539431,44145339.85472995,37843464.730226338,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-511308.13324991695,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":424299429.53786093},432107854.16757894,453706661.02213228,472895285.51306659,489373624.74160826,503051796.48422945,508285006.63086987,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":439951411.35196602},448047880.96075523,470443446.20940316,490339919.8763237,507426128.56679863,521608874.39192307,526523824.29636025,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",212173611.89488715,{"$f":"C45","v":214912199.6993117},218867250.29927778,229807277.00883153,239526520.57001761,247872975.6544719,254801115.95452711,null,212173611.89488715,{"$f":"K45","v":214912199.6993117},218867250.29927778,229807277.00883153,239526520.57001761,247872975.6544719,254801115.95452711,null,0,{"$f":"S45","v":0},0,0,0,0,0]
["DRAB0402","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-10053075.635492161,-10307214.436902571,-10636661.711931851,-12131185.29104149,-13390323.955026528,-14636450.356670074,-15835505.964151315,null,-10053075.635492161,-10307214.436902571,-10636661.711931851,-12131185.29104149,-13390323.955026528,-14636450.356670074,-15835505.964151315,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",12791663.4399167,14262265.03686865,21576688.421485603,21850428.852227557,21736779.039480843,21564590.65672528,18486182.881931376,null,12791663.4399167,14262265.03686865,21576688.421485603,21850428.852227557,21736779.039480843,21564590.65672528,18486182.881931376,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-249769.29907602482,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":214912199.6993117},218867250.29927778,229807277.00883153,239526520.57001761,247872975.6544719,254801115.95452711,257451792.87230715,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":214912199.6993117},218867250.29927778,229807277.00883153,239526520.57001761,247872975.6544719,254801115.95452711,257202023.57323113,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",378217265.3360213,{"$f":"C52","v":383099027.87482923},390149237.41231793,409650752.9299041,426976120.05740362,441854376.5432108,454204367.92408669,null,378217265.3360213,{"$f":"K52","v":383099027.87482923},390149237.41231793,409650752.9299041,426976120.05740362,441854376.5432108,454204367.92408669,null,0,{"$f":"S52","v":0},0,0,0,0,0]
["DRAB0502","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-17920450.809668545,-18373474.54634716,-18960741.955904704,-21624855.631601013,-23869375.946442053,-26090700.811883513,-28228118.037320796,null,-17920450.809668545,-18373474.54634716,-18960741.955904704,-21624855.631601013,-23869375.946442053,-26090700.811883513,-28228118.037320796,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",22802213.348476451,25423684.083835866,38462257.473490894,38950222.759100579,38747632.432249241,38440692.19275941,32953172.044643592,null,22802213.348476451,25423684.083835866,38462257.473490894,38950222.759100579,38747632.432249241,38440692.19275941,32953172.044643592,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-445234.73215052229,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":383099027.87482923},390149237.41231793,409650752.9299041,426976120.05740362,441854376.5432108,454204367.92408669,458929421.93140948,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":383099027.87482923},390149237.41231793,409650752.9299041,426976120.05740362,441854376.5432108,454204367.92408669,458484187.19925898,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",100900603.4691487,{"$f":"C59","v":102202957.51615706},104083808.71496353,109286412.78577247,113908465.13162757,117877678.58531003,121172402.80172585,null,100900603.4691487,{"$f":"K59","v":102202957.51615706},104083808.71496353,109286412.78577247,113908465.13162757,117877678.58531003,121172402.80172585,null,0,{"$f":"S59","v":0},0,0,0,0,0]
["DRAB0602","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-4780808.4581445456,-4901665.8927624766,-5058336.7839484597,-5769067.6315985508,-6367859.582740753,-6960463.464070553,-7530682.5092544621,null,-4780808.4581445456,-4901665.8927624766,-5058336.7839484597,-5769067.6315985508,-6367859.582740753,-6960463.464070553,-7530682.5092544621,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",6083162.5051529035,6782517.0915689403,10260940.854757413,10391119.977453649,10337073.036423203,10255187.680486387,8791229.9365106411,null,6083162.5051529035,6782517.0915689403,10260940.854757413,10391119.977453649,10337073.036423203,10255187.680486387,8791229.9365106411,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-118779.48807942451,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":102202957.51615706},104083808.71496353,109286412.78577247,113908465.13162757,117877678.58531003,121172402.80172585,122432950.22898203,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":102202957.51615706},104083808.71496353,109286412.78577247,113908465.13162757,117877678.58531003,121172402.80172585,122314170.7409026,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",176286479.27151465,{"$f":"C66","v":178561861.20005098},181847952.90288782,190937578.96213126,199012905.64051503,205947637.85389328,211703949.63313985,null,176286479.27151465,{"$f":"K66","v":178561861.20005098},181847952.90288782,190937578.96213126,199012905.64051503,205947637.85389328,211703949.63313985,null,0,{"$f":"S66","v":0},0,0,0,0,0]
["DRAB0702","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-8352694.2573289154,-8563847.9165743403,-8837572.343009036,-10079311.584739173,-11125479.013413228,-12160835.079189455,-13157081.924430292,null,-8352694.2573289154,-8563847.9165743403,-8837572.343009036,-10079311.584739173,-11125479.013413228,-12160835.079189455,-13157081.924430292,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",10628076.185865255,11849939.619411176,17927198.402252451,18154638.263122961,18060211.226791456,17917146.858436018,15359422.250112314,null,10628076.185865255,11849939.619411176,17927198.402252451,18154638.263122961,18060211.226791456,17917146.858436018,15359422.250112314,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,-207523.2163462427,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":178561861.20005098},181847952.90288782,190937578.96213126,199012905.64051503,205947637.85389328,211703949.63313985,213906289.95882189,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":178561861.20005098},181847952.90288782,190937578.96213126,199012905.64051503,205947637.85389328,211703949.63313985,213698766.74247566,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",0,{"$f":"C72","v":0},0,0,0,0,0,null,0,{"$f":"K72","v":0},0,0,0,0,0,null,0,{"$f":"S72","v":0},0,0,0,0,0]
["DRAB0802","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},0,0,0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",0,{"$f":"C79","v":0},0,0,0,0,0,null,0,{"$f":"K79","v":0},0,0,0,0,0,null,145508234.02333027,{"$f":"S79","v":140606630.59111637},135491782.96377593,130101303.33666754,121554107.8179937,111884431.6417255,102167877.35807636]
["DRAB0902","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0903","Straight line depreciation",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-18449038.747280806,-18197040.859883536,-17903374.996923842,-18850457.037115205,-19549922.890743211,-20230546.816255517,-20945869.257919334]
["DRAB0905","Actual additions (recognised in RAB)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,13547435.315066898,13082193.232543105,12512895.369815432,10303261.518441366,9880246.7144750021,10513992.532606389,12646550.364788888]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":140606630.59111637},135491782.96377593,130101303.33666754,121554107.8179937,111884431.6417255,102167877.35807636,93868558.464945912]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",24286510.099498756,{"$f":"C86","v":28199978.115573466},37284926.331673332,61237045.006688863,72820463.752351269,82682456.228646487,85107332.422125727,null,24286510.099498756,{"$f":"K86","v":27710827.047774736},36551091.06520877,60503209.740224302,72086628.485886708,81948620.962181926,84373497.155661166,null,0,{"$f":"S86","v":0},0,0,0,0,0]
["DRAB1002","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-7970395.4098931672,-4289855.5287040509,-4297804.4562082179,-5863723.9277855754,-10689589.734066829,-12046229.807910627,-13294530.419940786,null,-7970395.4098931672,-4289855.5287040509,-4297804.4562082179,-5863723.9277855754,-10689589.734066829,-12046229.807910627,-13294530.419940786,null,0,0,0,0,0,0,0]
["DRAB1005","Actual additions (recognised in RAB)",11883863.425967878,13374803.744803917,28249923.131223753,17447142.673447981,20551582.21036204,14471106.001389859,11917761.126838055,null,11883863.425967878,13374803.744803917,28249923.131223753,17447142.673447981,20551582.21036204,14471106.001389859,11917761.126838055,null,0,0,0,0,0,0,0]
["DRAB1006","Disposals ",0,0,0,0,0,0,0,null,-489151.06779873092,-244684.1986658329,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":28199978.115573466},37284926.331673332,61237045.006688863,72820463.752351269,82682456.228646487,85107332.422125727,83730563.129023001,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":27710827.047774736},36551091.06520877,60503209.740224302,72086628.485886708,81948620.962181926,84373497.155661166,82996727.862558439,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":0},0,0,0,0,0,0]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",79116676.252315566,{"$f":"C93","v":79253507.272151828},95745332.349898875,70594637.181063563,48362153.312656283,30934253.390413888,17818723.462121591,null,79116676.252315566,{"$f":"K93","v":79241013.516590491},95726588.941072717,70575893.772237405,48343409.903830126,30915509.98158773,17799980.053295434,null,20996141.853353489,{"$f":"S93","v":20874026.712060578},20628639.2260415,20307553.111424919,21073780.89536,21795001.826693568,22697068.071098343]
["DRAB1102","Inflation addition",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,-492057.88966205926,-489196.0439410666,-483445.23270329909,-475920.37613386271,-493877.40981161501,-510779.67937765043,-531920.17345781869]
["DRAB1103","Straight line depreciation",-30656809.500326041,-28346725.341820002,-29934934.589723196,-25498288.491786696,-20808557.449570946,-16137908.204036547,-11090513.182773583,null,-30656809.500326041,-28346725.341820002,-29934934.589723196,-25498288.491786696,-20808557.449570946,-16137908.204036547,-11090513.182773583,null,-1568961.2966153526,-1610015.8920780118,-1634724.8843550493,-1674499.6273666027,-1741603.2199919543,-1574151.0982487146,-1646366.8196575388]
["DRAB1105","Actual additions (recognised in RAB)",30793640.520162303,44838550.419567041,4784239.4208878847,3265804.6233794182,3380657.5273285517,3022378.2757442519,2047530.6941319315,null,30793640.520162303,44838550.419567041,4784239.4208878847,3265804.6233794182,3380657.5273285517,3022378.2757442519,2047530.6941319315,null,1938904.0449845016,1853824.4499999979,1797084.0024417678,2916647.7874355484,2956701.5611371412,2986997.0220311354,3004074.516491455]
["DRAB1106","Disposals ",0,0,0,0,0,0,0,null,-12493.755561332484,-6249.6532648054936,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":79253507.272151828},95745332.349898875,70594637.181063563,48362153.312656283,30934253.390413888,17818723.462121591,8775740.9734799396,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":79241013.516590491},95726588.941072717,70575893.772237405,48343409.903830126,30915509.98158773,17799980.053295434,8756997.5646537822,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":20874026.712060578},20628639.2260415,20307553.111424919,21073780.89536,21795001.826693568,22697068.071098343,23522855.594474439]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2021)"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",939106731.30612242,953825180.6477859,986577538.56967843,1032004614.9286529,1071728761.0915531,1105315630.4141984,1126378216.6275923,null,973749439.86671805,989010838.09162283,1022971397.7570832,1070074233.5527674,1111263763.7582521,1146089619.1158385,1167359712.7100811,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",421596043.58587116,428203641.8527199,442907257.59485561,463300973.26759946,481134455.12733746,496212710.61291885,505668401.55754966,null,437148300.19458735,443999646.15636063,459245663.58507907,480391683.04286331,498883024.22156107,514517501.4793607,524066349.34414154,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",213542905.79709941,216889724.99929476,224337263.65405464,234666898.78942457,243699748.11224476,251337045.80449951,256126454.41341713,null,213542905.79709941,216889724.99929476,224337263.65405464,234666898.78942454,243699748.11224473,251337045.80449948,256001569.76387909,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",380658146.60542524,386624132.64357358,399899995.17111099,418313436.49365389,434415248.30030721,448029372.23364878,456566894.92774808,null,380658146.60542524,386624132.64357358,399899995.17111099,418313436.49365389,434415248.30030721,448029372.23364878,456344277.56167281,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",101551780.49265288,103143383.11556029,106685110.750368,111597438.95870003,115893071.8584688,119525040.69351794,121802676.51535395,null,101551780.49265288,103143383.11556029,106685110.75036798,111597438.9587,115893071.85846879,119525040.69351792,121743286.7713142,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",177424170.2357828,180204907.05146939,186392765.93250954,194975242.30132315,202480271.74720415,208825793.74351656,212805119.79598087,null,177424170.2357828,180204907.05146939,186392765.93250954,194975242.30132315,202480271.74720415,208825793.74351656,212701358.18780774,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,{"$f":"AVERAGE(S74,S79)","v":143057432.30722332},{"$f":"AVERAGE(T74,T79)","v":138049206.77744615},132796543.15022174,125827705.57733062,116719269.72985959,107026154.49990094,98018217.911511138]
["DRAB1209","“Other” assets with long lives",26243244.107536111,32742452.223623399,49260985.669181094,67028754.379520066,77751459.990498871,83894894.325386107,84418947.775574356,null,25998668.573636748,32130959.056491755,48527150.402716532,66294919.113055505,77017624.724034309,83161059.058921546,83685112.509109795,null,0,0,0,0,0,0,0]
["DRAB1210","“Other” assets with short lives",79185091.762233704,87499419.811025351,83169984.765481219,59478395.246859923,39648203.351535082,24376488.426267739,13297232.217800766,null,79178844.884453028,87483801.228831604,83151241.356655076,59459651.83803378,39629459.942708939,24357745.017441597,13278488.808974624,null,{"$f":"AVERAGE(S88,S93)","v":20935084.282707036},{"$f":"AVERAGE(T88,T93)","v":20751332.969051041},20468096.168733209,20690667.003392458,21434391.361026786,22246034.948895954,23109961.832786389]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,42.456714809991773,42.456714809991773,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,40.1640103064477,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,15,15,15,15,15,15,15]
["DRAB1408","“Other” assets with long lives",9.4492469336647211,9.4492469336647211,15.069660349990084,15.069660349990084,15.069660349990084,15.069660349990084,15.069660349990084,null,9.4492469336647211,9.4492469336647211,15.069660349990084,15.069660349990084,15.069660349990084,15.069660349990084,15.069660349990084,null,0,0,0,0,0,0,0]
["DRAB1409","“Other” assets with short lives",5,5,5,5,5,5,5,null,5,5,5,5,5,5,5,null,25,25,25,25,25,25,25]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",21,21,21,19,18,17,16,null,21,21,21,19,18,17,16,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,{"$f":"-S74/S76","v":7.8870360681949707},{"$f":"-T74/T76","v":7.7268953602831161},7.5679464339576272,6.9017585664107433,6.2176259465222214,5.5304699698885473,4.8777100677952596]
["DRAB1508","“Other” assets with long lives",3,6,9,10,7,7,6,null,3,6,9,10,7,7,6,null,0,0,0,0,0,0,0]
["DRAB1509","“Other” assets with short lives",3,3,3,3,2,2,2,null,3,3,3,3,2,2,2,null,{"$f":"-S88/S90","v":13.382192345118705},{"$f":"-T88/T90","v":12.965106005953107},12.619028084459698,12.127535163063332,12.100219299926051,13.845558949799097,13.786154944388132]

{"sheet":"3.4 Operational data","index":23,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":false,"merged":[[8,3,8,9],[9,3,9,9],[43,3,43,9],[44,3,44,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOPED01","Total energy delivered","GWh"]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",3291.2100689570889,3421.001156395675,3358.3776213847846,3198.5609170165226,3037.945129126419,2876.5262622968653,2714.3003011331634]
["DOPED0202","Energy Delivery at On-peak times","GWh",1766.4274635422689,1775.2678099837497,1802.4770036145603,1875.2114275371889,1948.3095235794306,2021.7731101018828,2095.6040145569477]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",42.241362762244719,42.996208923901236,43.103431390045628,0,0,0,0]
["DOPED0204","Energy Delivery at Off-peak times","GWh",2243.3263460150097,2184.1619283415166,2238.0553885014201,2405.451167561554,2530.3649769699909,2655.9033554254711,2782.069425773228]
["DOPED0205","Controlled load energy deliveries","GWh",91.308656792203607,92.940327377585675,93.172098767554701,93.637959261392453,94.106149057699412,94.576679802987897,95.049563202002844]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",85.937066808070909,87.472698047973353,87.690884498031537,88.129432150196493,88.570166000035371,89.013098820272816,89.458241001842467]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",0,0,0,0,0,0,0]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",0,0,0,0,0,0,0]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",0,0,0,0,0,0,0]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",{"$f":"SUM(D14:D19)*(1+'3.6 Quality of service'!D16)-SUM(D26:D33)","v":7563.3268673845841},{"$f":"SUM(E14:E19)*(1+'3.6 Quality of service'!E16)-SUM(E26:E33)","v":7614.8956394385223},{"$f":"SUM(F14:F19)*(1+'3.6 Quality of service'!F16)-SUM(F26:F33)","v":7599.2562236607446},{"$f":"SUM(G14:G19)*(1+'3.6 Quality of service'!G16)-SUM(G26:G33)","v":7603.6368550907328},{"$f":"SUM(H14:H19)*(1+'3.6 Quality of service'!H16)-SUM(H26:H33)","v":7608.1905512062649},{"$f":"SUM(I14:I19)*(1+'3.6 Quality of service'!I16)-SUM(I26:I33)","v":7612.9179204480934},{"$f":"SUM(J14:J19)*(1+'3.6 Quality of service'!J16)-SUM(J26:J33)","v":7617.8832728444204}]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",111.64999999999999,113.32474999999998,115.02462124999997,116.74999056874995,118.50124042728119,120.27875903369039,122.08294041919574]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",176.15658387309878,209.96893912356768,243.78182971000734,277.4662396634597,311.15064961691206,344.83505957036442,378.45576454329387]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",2747.37373904078,2796.4688530697354,2803.4425908579387,2817.459803812229,2831.54710283129,2845.7048383454462,2859.9333625371733]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",387.43104759022691,525.22636095169241,395.33780366349686,376.2485807879483,357.06391179802205,337.7833194631462,318.40632416659605]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",2916.8172131081587,2958.5505932725387,2976.3440950083254,2991.2258154833671,3006.1819445607834,3021.2128542835876,3036.318918555005]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",1043.596519780009,1062.2454168742606,1064.8944079387848,1070.2188799784788,1075.5699743783707,1080.9478242502626,1086.352563371514]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",425.23244535771209,261.34890490217549,382.85753068785107,405.83782346483076,428.93301116510884,452.14367010503702,475.47037703689784]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2452.8358882031198,2459.4540531127168,2471.2734944190147,2507.4074882960458,2522.655107198826,2573.9360318651752,2622.9245285204802]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2300.9722230380494,2307.2916411899005,2318.476122456856,2352.3612917409187,2366.6446752260258,2414.7482425792878,2460.6719072957158]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2200.6648480638523,2206.4093248685581,2216.926435486339,2249.2334235315075,2262.7664811452269,2308.6526487317769,2352.4556726482388]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2063.7089314625587,2069.1937996052015,2079.1456874405599,2109.440518422784,2122.1235516953307,2165.1608210017334,2206.2168739398639]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2286.5016768559767,2292.8032999781503,2304.3155085172357,2339.1264271919399,2353.9465726272661,2403.0638924563596,2450.0373965736649]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2072.9808899377185,2078.3498578830663,2095.4133612793557,2133.3657386723244,2151.357714657931,2180.657672381788,2224.860457318503]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2242,2248,2259,2293,2307,2355,2401]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2012,2018,2035,2073,2091,2117,2160]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2462.8057945311211,2469.5923781029028,2481.5801901107716,2517.9261817100883,2533.2085889273853,2584.8858673469463,2634.3995373020152]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2310.8729233338981,2317.3463821131472,2328.688626632018,2362.7853574956825,2377.099634959377,2425.595548713713,2472.0328994825363]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2205.5744306160636,2211.4506131159974,2222.0738938583913,2254.4839055173766,2268.0053086633143,2314.0962060583497,2358.2308123368343]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2068.72200036289,2074.3262059698013,2084.3760178347989,2114.7763295987561,2127.4456823515229,2170.6897271575822,2212.072210746795]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2343.1889561066182,2349.5704941854142,2361.3098792855108,2396.9470219309492,2412.1209551933803,2462.4544853715201,2510.6022914133491]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2124.5587040695132,2129.9932822190544,2147.4198319353663,2186.273485257344,2204.6940121696352,2234.7430088619885,2280.0522697695619]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2293.1607971488038,2299.2977127522349,2310.5487246918588,2345.3245797779691,2359.6440495193087,2408.7393743467587,2455.7890606397314]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2057.9123656839397,2064.0492812873708,2081.4372088304262,2120.3043409854904,2138.7150877957843,2165.3083887439861,2209.2896172352434]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.97768983439259272,0.97768983439259283,0.97768983439259283,0.97768983439259283,0.97768983439259283,0.97768983439259272,0.97768983439259283]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.92313364178031954,0.92313364178031954,0.92313364178031954,0.92313364178031954,0.92313364178031954,0.92313364178031954,0.92313364178031954]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0.97762142649275308,0.97762142649275297,0.97762142649275319,0.97762142649275297,0.97762142649275308,0.97762142649275297,0.97762142649275297]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.98809469004631822,0.98806688843509016,0.98801946563069132,0.98779532605080667,0.98770986121522908,0.98731406527358889,0.98697140295066277]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",0.90847656112251873,0.90847656112251873,0.90847656112251873,0.90847656112251873,0.90847656112251873,0.90847656112251873,0.90847656112251873]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.98305902396592382,0.98288295386505331,0.98267785825894327,0.98224070532813601,0.98209059360898554,0.98152296324188504,0.98097309307012692]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.97768983439259272,0.97768983439259283,0.97768983439259283,0.97768983439259283,0.97768983439259283,0.97768983439259272,0.97768983439259283]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW "]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW "]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA"]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA"]

{"sheet":"3.5 Physical assets","index":24,"n_rows":95,"n_cols":10,"rows_kept":95,"cut":false,"hidden":false,"merged":[[8,3,8,9],[75,3,75,9],[91,3,91,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"CIRCUIT LENGTH"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",5808.7610833879944,5798.6008446511623,5788.4583774235571,5778.3336506206188,5768.2266332121608,5758.1372942222697,5748.0656027292134]
["DPA0102","Overhead 2.2 kV","km"]
["DPA0103","Overhead 7.6 kV","km",19.521529287547946,19.487383727897235,19.453297893036865,19.419271678500824,19.385304980005817,19.351397693450956,19.317549714917437]
["DPA0104","Overhead 11 kV","km",640.61308411399034,639.49257291046524,638.37402161907494,637.25742681169152,636.14278506618359,635.03009296640516,633.91934710218584]
["DPA0105","Overhead SWER","km",37.189559622832533,37.124510501537763,37.059575159169775,36.994753396715204,36.930045015508789,36.865449817232758,36.800967603916227]
["DPA0106","Overhead 22 kV","km",2906.0123183253577,2900.929344778589,2895.8552619787429,2890.7900543748083,2885.7337064429739,2880.686202686582,2875.6475276360798]
["DPA0107","Overhead 33 kV","km"]
["DPA0108","Overhead 44 kV","km"]
["DPA0109","Overhead 66 kV","km",596.78181991221413,595.73797498950762,594.69595588016591,593.65575939061648,592.61738233287281,591.58082152452448,590.54607378872765]
["DPA0110","Overhead 132 kV","km"]
["DPA0111","Overhead 6.6kv","km"]
["DPA0112","Overhead 110kV","km"]
["DPA0113","Overhead 220kV","km"]
["DPA0114","Other ","km"]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D13:D26)","v":10008.879394649937},9991.3726315591593,9973.8964899537477,9956.4509162729501,9939.0358570497065,9921.6512589104659,9904.2970685750406]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",2435.1006996316705,2561.7858801673819,2695.0618086626309,2835.2713662538099,2982.7752723370072,3137.9530125966303,3301.2038153143635]
["DPA0202","Underground 5 kV","km"]
["DPA0203","Underground 6.6 Kv","km",1.5051878800476646,1.5834947025757211,1.6658754075311635,1.7525419370857767,1.8437172596215963,1.9396359433652701,2.0405447598655293]
["DPA0204","Underground 7.6 kV","km"]
["DPA0205","Underground 11 kV","km",241.92574904383747,254.51184340884325,267.7527245089978,281.68245737322053,296.33687925050344,311.75369180898116,327.97255813162207]
["DPA0206","Underground SWER","km",0.58658057090092808,0.61709720026847947,0.64920144558199744,0.68297590195254521,0.71850746147018074,0.75588753675264186,0.7952122961240663]
["DPA0207","Underground 22 kV","km",989.00804521278928,1040.4608096828604,1094.5903845028845,1151.5360297053094,1211.444250272393,1274.4691730519403,1340.7729432819376]
["DPA0208","Underground 33 kV","km"]
["DPA0209","Underground 66 kV","km",4.1281991121895505,4.3429670886819407,4.5689082868317943,4.8066039892131966,5.0566657194033491,5.3197368152591604,5.5964940840429591]
["DPA0210","Underground 110 kV","km"]
["DPA0211","Underground 132 kV","km"]
["DPA0212","Other ","km"]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D29:D40)","v":3672.2544614514354},3863.3020922506116,4064.2889028144577,4275.731975160591,4498.1752923003987,4732.1911377529295,4978.3815678679557]
[]
[null,"CIRCUIT CAPACITY MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",0.19362682081636667,0.19439762679893824,0.19515162112848539,0.19587836487235277,0.19655587582963194,0.19708835089905447,0.19746623030612689]
["DPA0302","Overhead 6.6 kV","MVA",2.9967769867475957,2.9967769867475957,2.9967769867475957,2.9967769867475957,2.9967769867475957,2.9967769867475957,2.9967769867475957]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",5.7221465880067175,5.7288518255805485,5.7288518255805485,5.7312295493017835,5.7447687492017563,5.747009764221346,5.7557169074271624]
["DPA0305","Overhead SWER","MVA",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
["DPA0306","Overhead 22 kV","MVA",11.758730326621231,11.760828708625207,11.790573039955961,11.816260231794157,11.816260231794157,11.824476408859061,11.825823597275409]
["DPA0307","Overhead 33 kV","MVA",0,0,0,0,0,0,0]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",101.04234673491818,101.04234673491818,101.04234673491818,101.04234673491818,101.04234673491818,101.04234673491818,101.51451884637284]
["DPA0310","Overhead 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0311","Overhead 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0312","Overhead 220 kV","MVA",0,0,0,0,0,0,0]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.19362682081636667,0.19439762679893824,0.19515162112848539,0.19587836487235277,0.19655587582963194,0.19708835089905447,0.19746623030612689]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",3.1190944147781097,3.1190944147781097,3.1190944147781097,3.1190944147781097,3.1190944147781097,3.1190944147781097,3.1190944147781097]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",5.9557035915988283,5.9626825123389384,5.9626825123389384,5.9651572860079796,5.9792491063120314,5.9815815913324215,5.9906441281384755]
["DPA0406","Underground SWER","MVA",0,0,0,0,0,0,0]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",12.238678503218017,12.240862533467054,12.271820919137836,12.298556567785756,12.298556567785756,12.307108099016576,12.308510274715221]
["DPA0409","Underground 33 kV","MVA",0,0,0,0,0,0,0]
["DPA0410","Underground 66 kV","MVA",134.16049863234707,134.16049863234707,134.16049863234707,134.16049863234707,134.16049863234707,134.16049863234707,134.16049863234707]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",0,0,0,0,0,0,0]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",5262.3481444700656,5436.7795087236309,5621.7048585551165,5798.4735882613213,5984.7362697885665,6157.9661867857676,6309.3374417955492]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",299.69903151200003,299.69903151200003,299.69903151200003,299.69903151200003,299.69903151200003,299.69903151200003,299.69903151200003]
["DPA0503","Cold spare capacity included in DPA0501","MVA",23,23,23,23,23,23,23]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",0,0,0,0,0,0,0]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",3384.5,3384.5,3384.5,3417.5,3417.5,3450.5,3483.5]
["DPA0604","Total zone substation transformer  capacity ","MVA",3384.5,3384.5,3384.5,3417.5,3417.5,3450.5,3483.5]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DPA0701","Public lighting luminaires","0's",82532.484679478424,89045.619810209624,95558.754940940824,97263.860514210159,98873.036060578001,99678.301270714612,99698.633841754112]
["DPA0702","Public lighting poles","0's",35125,35234.254672237294,35343.849176030621,35453.784568410163,35564.061909693955,35674.682263498093,35785.646696747004]

{"sheet":"3.6 Quality of service","index":25,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[6,3,6,9],[13,3,13,9],[18,3,18,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS0201","Energy Not Supplied (planned)","GWh",0.84079547685772882,0.85011848586347971,0.85224676703203817,0.85650801129038834,0.86079056103878471,0.86509452301058587,0.86942000419939014]
["DQS0202","Energy Not Supplied (unplanned)","GWh",1.1120944984294419,1.124425757706492,1.1272407702081177,1.1328769878455935,1.1385413856040603,1.1442341046564719,1.1499552865199933]
["DQS02","Total",null,{"$f":"SUM(D9:D10)","v":1.9528899752871707},1.9745442435699716,1.9794875372401559,1.9893849991359818,1.999331946642845,2.0093286276670579,2.0193752907193834]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS03","System losses","%",4.3971098E-2,4.3971098E-2,4.3971098E-2,4.3971098E-2,4.3971098E-2,4.3971098E-2,4.3971098E-2]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DQS04","Overall utilisation","%",0.6827811857981676,0.68469386382424202,0.68804509576954287,0.69137830504628606,0.69556682807882286,0.70296929393239038,0.70964056250395757]

{"sheet":"3.7 Operating Environment","index":26,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[8,3,8,9],[15,3,15,9],[33,3,33,9]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0101","Customer density","Customer / km",101.52017173194093]
["DOEF0102","Energy density","MWh/customer",10.705597800671894]
["DOEF0103","Demand density","kVA / customer",3.2896000786677035]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0201","Rural proportion","%",12]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",47170]
["DOEF0203","Rural vegetation maintenance spans","0's",11135]
["DOEF0204","Total vegetation maintenance spans","0's",57012]
["DOEF0205","Total number of spans","0's",184045]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",2.2738370869290674]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",1.5934769355821987]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",3.34]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",10.173333333333334]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",1]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",1]
["DOEF0212","Tropical proportion","Spans",0]
["DOEF0213","Standard vehicle access","km",69,{"$f":"D30","v":69},69,69,69,69,69]
["DOEF0214","Bushfire risk","Spans",17952]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
["DOEF0301","Route Line length","km",6919.5940544598479,6907.1230304402616,6894.6744826582808,6882.2483706055027,6869.8446538465323,6857.4632920188506,6845.1042448326825]

{"sheet":"4.1 Public lighting","index":27,"n_rows":162,"n_cols":10,"rows_kept":162,"cut":false,"hidden":false,"merged":[[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[5,1,5,2],[8,3,8,9],[31,3,31,9],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[95,1,95,2],[93,1,93,2],[96,1,96,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[212,1,212,2],[213,1,213,2],[214,1,214,2],[215,1,215,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",13264,13264,13264,13264,13264,13264,13264]
[null,"Number of poles installed ","0's",0,0,0,0,0,0,0]
[null,"Total expenditure","$0's",5849373.5321300151,5922508.5982219642,6022996.5347563177,6150067.6732174363,6284215.4055679077,6411194.4227877334,6526150.4805518519]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",1912.2662818818335,1844.3406877380312,1776.4150935942287,1746.3854406543319,1719.9157280314478,1688.3029797369827,1669.1298040753672]
[null,"Number of poles replaced","0's",208,208,224.81454545454545,224.81454545454545,224.81454545454545,224.81454545454545,224.81454545454545]
[null,"Total expenditure","$0's",1873644.5249999976,1835364.2637208826,1797084.0024417676,2916647.7874355479,2956701.5611371407,2986997.0220311349,3004074.5164914541]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",17503.444656788532,17560.88931357706,17618.333970365591,17675.778627154123,17733.223283942651,17790.667940731182,17848.11259751971]
[null,"Number of poles maintained","0's",4398.9385741447113,4417.2627150459466,4435.6856438871346,4454.2078932475179,4472.8299985775484,4491.5524982143597,4510.3759333973376]
[null,"Total expenditure","$0's",2749666.4436546406,3394785.0840796423,4039903.7245046441,3973100.457610867,3918291.7182181505,3855224.4964738726,3837635.9636825565]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",3,3,3,3,3,3,3]
[null,"GSO breaches","0's",228,228,228,228,228,228,228]
[null,"GSL payments ","$0's",3250,3250,3250,3250,3250,3250,3250]
[null,"Customer complaints ","0's",130,130,130,130,130,130,130]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2021)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"LIGHT INSTALLATION"]
[null,"New Light Major Road (CNJ)",null,1319.8713394164652,1335.0280592404583,1351.7199946777912,1374.6547951571315,1403.6567958728301,1434.273918507866,1463.2548939904686]
[null,"Pb.Light CapProj - Major Scheme (CLJ)",null,1893.446956648927,1915.190322207731,1939.1360610161601,1972.0376226093958,2013.6430036430866,2057.565389063082,2099.1406079420008]
[null,"New Light Minor Road (CNM)",null,528.51335670416017,534.58253074527897,541.26644800631607,550.45018283310264,562.06339413002127,574.32334536407097,585.92813757028944]
[null,"New Light Watchman (CNW)",null,1495.8163326345336,1512.9935137618381,1531.9105618897884,1557.902678028835,1590.7707804370593,1625.4693080344607,1658.3135824481499]
[null,"New Sustainable Light (CNG)",null,682.50136962104261,690.33886235985096,698.97021032338989,710.8297244075851,725.8265688871129,741.65858789398521,756.64456029079088]
[null,"New Sustainable Lantern & Bracket (CNS)",null,2308.3348504446758,2334.8425739956829,2364.0352499336291,2404.1461286635686,2454.8679884277685,2508.4145494357817,2559.0996379808144]
[null,"Pb.Light CapProj - Minor Scheme (CLN)",null,203.10974083886364,205.4421480542363,208.01080348263176,211.54014853501343,216.00315085445041,220.71469784991984,225.17446468001958]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[null,"SINGLE MAJOR RD REPL (RLJ)",null,781.64699833012514,781.64699833012514,791.41997736274141,804.84809808866532,821.82851033400141,839.75456202972134,856.72266418896982]
[null,"SINGLE MINOR RD REPL (RLM)",null,607.07139305555086,607.07139305555086,614.66164288483162,625.0906830687253,638.27863432863671,652.20102282133894,665.37941337018015]
[null,"SINGLE SUSTAINABLE LANTERN REPL (RLG)",null,364.98942710622629,364.98942710622629,369.55291167900174,375.82316167847557,383.7521512999968,392.12270649009565,400.04594792697804]
[null,"Single Sustainable Lantern Replacement (RLS)",null,2417.5252543209881,2417.5252543209881,2447.751716741715,2489.2830231272628,2541.8010722204981,2597.2438523722153,2649.7238280844185]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"PL Luminaires (MLF)",null,256.86869265796099,260.08033724029144,264.49315251763556,270.07333935846134,275.96428690055615,281.54042834016292,286.58859497010792]
[null,"PL Poles (MLR)",null,275.10681966983202,278.54649664179868,283.27262953163711,289.24901941028685,295.5582345442055,301.53029179106534,306.93688709217821]
[null,"MINOR LAMP BULK (MRB)",null,57.518475869909004,58.237632803749428,59.225757928776865,60.475282885798414,61.794393909196138,63.043013013075409,64.173407096866725]
[null,"PL Luminaires (MRF)",null,224.29114823991401,227.09547384166643,230.94863085852435,235.8211067565064,240.96493092116211,245.83387447865101,250.24180398621644]
[null,"PL Poles (MRR)",null,258.30942144511005,261.53907954538221,265.97664548399473,271.58813055636466,277.51211932905733,283.11953631030417,288.1960171692462]
[null,"Bulk Change Sustainable Lantern - Minor Rd (MRS)",null,65.935354607462656,66.759748278088253,67.892469191322888,69.324841483635169,70.836982613575017,72.268316496102358,73.564125079930832]

{"sheet":"4.2 Metering","index":28,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,4,8,10],[10,1,13,1],[14,1,17,1],[18,1,21,1],[26,4,26,10],[27,2,27,3],[28,1,30,1],[31,1,33,1],[34,1,36,1],[37,1,39,1],[40,1,42,1],[43,1,45,1],[46,1,48,1],[49,1,51,1],[54,1,56,1],[64,4,64,10],[65,2,65,3],[84,1,86,1],[87,1,89,1],[66,1,68,1],[69,1,71,1],[72,1,74,1],[75,1,77,1],[78,1,80,1],[81,1,83,1]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,null,"VOLUMES (0's)"]
[null,"ASSET CATEGORY","ASSET SUBCATEGORY",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter Type 4","Single phase meter population ",null,583315.59374109702,595740.26423819247,610605.59561839746,618581.12848192721,625236.3841182224,631677.48548782815,637870.0133132115]
[null,null,"Multi phase meter population ",null,111216.15042804064,117694.40063780514,124966.46892391154,128950.09446728881,132626.14665620608,136215.77696374353,139706.77832282972]
[null,null,"Current transformer connected meter population ",null,3783.7882165968831,4227.6171665402107,4756.1942799148264,5066.0704951637854,5361.2278609911,5650.2383432903516,5932.2909491503942]
[null,null,"Direct connect meter population ",null,690747.95595254085,709207.04770945734,730815.87026239419,742465.15245405224,752501.30291343736,762243.02410828136,771644.50068689079]
[null,"Meter Type 5","Single phase meter population ",null,205.57731863772642,156.86934319506668,100.96128705076158,84.628861725397471,83.632223996165763,82.641101778310855,81.65497925110985]
[null,null,"Multi phase meter population ",null,392.83586630773459,299.76023006582045,192.92602377026714,161.71653775249217,159.81207159663359,157.91814498231676,156.0337722323188]
[null,null,"Current transformer connected meter population ",null,105.16331481467853,80.246693713647971,51.64686301276582,43.291991971737978,42.7821607901178,42.27515107471347,41.770698956838366]
[null,null,"Direct connect meter population ",null,493.24987013078248,376.38287954723916,242.2404478082629,203.05340750615167,200.66213480268152,198.28409568591414,195.91805252659026]
[null,"Meter Type 6","Single phase meter population ",null,10303.290959843278,7862.1051015190842,5060.0597529797533,4241.4980005342768,4191.5477016692184,4141.8738336812821,4092.4505442486929]
[null,null,"Multi phase meter population ",null,5079.0488690495713,3875.6564460668951,2494.3768807326778,2090.8635606479393,2066.2403591923994,2041.7534254535813,2017.3900154251101]
[null,null,"Current transformer connected meter population ",null,65.811880884024617,50.218898646605496,32.320940078956667,27.092407879087631,26.773352236396292,26.45606228546584,26.140372895569808]
[null,null,"Direct connect meter population ",null,15316.527948008825,11687.542648939374,7522.1156936334746,6305.2691533031284,6231.0147086252218,6157.1711968493973,6083.7001867782328]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2021)"}]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter purchase ",null,"Meter Type 4",6971423.7181626186,7799339.6047307551,7135126.2772513703,7257337.9577821409,7363594.5492834803,7730922.0951603027,8276490.422246811]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4",178675.87351039998,183804.90085174673,190990.52818581456,196115.43131511621,201303.65527139819,206322.03979597654,211057.53259387624]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",5726.2666137599981,5890.643468053684,4284.6516685522856,4399.6229446292218,4516.0147502452528,4628.5964045865212,4734.8317101310895]
[null,"Meter investigation ",null,"Meter Type 4",99147.816069119974,101993.92981387094,105981.25749982138,108825.08270606269,111704.0448425646,114488.76253293623,117116.50269560277]
[null,null,null,"Meter Type 5",14628.366305279997,15048.284726636699,10945.605282768438,11239.311820462211,11536.647254232083,11824.249245204888,12095.63880298848]
[null,null,null,"Meter Type 6",26005.984542719994,26752.506180687466,19458.85383603278,19980.998791932823,20509.59511863481,21020.887547030914,21503.357871979522]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",47926.496695225331,49302.263367553744,35860.772451568824,36823.034751704552,37797.186299905909,38739.448448818817,39628.594268167042]
[null,null,null,"Meter Type 6",431192.9359739903,443570.65835225786,322638.05673131201,331295.49541311641,340059.90122445114,348537.39927799447,356537.01165925898]
[null,"Special meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4",10368184.337279599,13182785.147727612,11098143.31484223,10934742.260251457,10794779.016709179,10729215.194288487,10640581.863130575]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",4777912.4624555875,2963192.8919369783,2916070.5163914803,2769807.7092560632,2130001.5734226648,2494815.0236493004,3096396.1113773668]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Remote meter re-configuration ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Other metering ",null,"Meter Type 4",1993259.1204758738,2050477.1450835133,2130638.0360788931,2187810.0521062347,2245688.4579410804,2301672.1815806828,2354500.042577887]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 7",0,0,0,0,0,0,0]
[null,"IT infrastructure capex ",null,"Meter Type 4",880195.75114239997,891200.89110825385,1705836.1565689771,0,114825.8824645861,0,894317.00496801292]
[null,"IT infrastructure opex ",null,"Meter Type 4",3801198.1812098552,3910314.4766461728,4063183.4287686911,4172211.9846181422,4282587.6446267702,4389350.0952736316,4490094.2318873582]
[null,"Communications infrastructure capex ",null,"Meter Type 4",1219338.3094241279,1219338.3094241279,156242.32035708381,163327.78983465931,170184.83312492055,187045.54080291424,265984.30177131837]
[null,"Communications infrastructure opex ",null,"Meter Type 4",1040935.035680243,1070815.8704772196,133521.37254957427,137104.18949085328,140731.27398722887,144239.62383089936,147550.20422501731]
[]
[null,"VOLUMES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Meter purchase ",null,"Meter Type 4",8424.2652674445781,22191.61369490574,25927.465691222602,24082.198363414107,24460.979199278132,24770.424919527195,26022.096278690082]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4",890.90429384049605,915.15184388446733,943.54839246954862,958.88889441907133,972.14128580325587,985.008115860418,997.42957507002438]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter investigation ",null,"Meter Type 4",375.65780131984047,385.88199868861182,397.85565857586954,404.32411907532264,409.91210899077379,415.33752350796431,420.57514340510244]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",3765.5251433642957,2873.3493555532018,1849.290901424841,1550.1326157622307,1531.8773702267986,1513.7231513849017,1495.6605110351802]
[null,null,null,"Meter Type 6",64255.463824767387,49031.247579643517,31556.566506367744,26451.686397905916,26140.176256702554,25830.390049560086,25522.166551008613]
[null,"Special meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4",18405.777182976111,23402.304413868562,19701.612775464819,19396.236042496101,19134.661732858447,19012.13090867304,18846.485973461793]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",10509.83651192963,7232.161277354041,6733.585587949291,6475.7431567820349,6482.7631866687452,7517.9653700170447,9338.0483479303766]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",251238479.02616379,258076382.53081211,266084319.77551192,270410401.04365999,274147627.00366646,277776123.16851747,281279023.02059269]
[null,"Remote meter re-configuration ",null,"Meter Type 4",6950.6957118523487,7139.8712981401077,7361.4167209720999,7481.1009136013263,7584.4939947691801,7684.8789868741369,7781.7892654080706]

{"sheet":"4.3 Fee-based services","index":29,"n_rows":28,"n_cols":16,"rows_kept":28,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,1,9,1],[8,2,8,8],[8,9,8,15]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"COMMON FEE-BASED SERVICES"]
[null,"Energisation"]
[null,"De-energisation",184824.88080347897,190661.45598674676,196739.6323213916,220348.38819995863,246790.19478395372,276405.01815802814,309573.62033699156,3758,3825,3868,4332.1600000000008,4852.0192000000015,5434.2615040000019,6086.3728844800025]
[null,"Re-energisation",253237.43850499904,257446.01716044819,276072.91706486,309201.66711264319,346305.86716616037,387862.57122609974,434406.0797732317,4624,4689,4758,5328.9600000000009,5968.4352000000008,6684.6474240000016,7486.8051148800023]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Service  (DNSP to nominate)",206641.72454852751,202508.89005755694,217517.60478792369,219692.78083580293,221889.70864416094,224108.60573060258,226349.69178790861,704.94749999999999,726.75,765,772.65,780.37649999999996,788.18026499999996,796.06206765000002]
[null,null,30793.668756251158,30177.795381126136,32414.388164474905,32414.388164474905,32414.388164474905,32414.388164474905,32414.388164474905,105.05099999999999,108.3,114,114,114,114,114]
[null,null,3154.1304563299509,3253.7345760035282,3320.1373224525801,3320.1373224525801,3320.1373224525801,3320.1373224525801,3320.1373224525801,139,139,139,139,139,139,139]
[null,null,1122881.7213370022,1150953.764370427,0,0,0,0,0,2089,2089,0,0,0,0,0]
[null,null,321045.61499999999,324256.07114999997,0,0,0,0,0,932,932,0,0,0,0,0]
[null,null,375663.53995014873,383330.14280627423,391153.20694517781,391153.20694517781,391153.20694517781,391153.20694517781,391153.20694517781,5768,5768,5768,5768,5768,5768,5768]
[null,null,514138.7,523875.48599999998,0,0,0,0,0,45499,45953.99,0,0,0,0,0]
[null,null,463639.00000000006,523875.48599999998,0,0,0,0,0,41030,45953.99,0,0,0,0,0]
[null,null,0,0,188603.01237248661,188603.01237248661,188603.01237248661,188603.01237248661,188603.01237248661,0,0,550.66046668921206,550.66046668921206,550.66046668921206,550.66046668921206,550.66046668921206]
[null,null,0,0,51745.052355698164,51745.052355698164,51745.052355698164,51745.052355698164,51745.052355698164,0,0,86.18802840716944,86.18802840716944,86.18802840716944,86.18802840716944,86.18802840716944]
[null,null,0,0,837615.54722090194,837615.54722090194,837615.54722090194,837615.54722090194,837615.54722090194,0,0,1413.501521812648,1413.501521812648,1413.501521812648,1413.501521812648,1413.501521812648]
[null,null,0,0,132933.71008370799,132933.71008370799,132933.71008370799,132933.71008370799,132933.71008370799,0,0,169.64998309097058,169.64998309097058,169.64998309097058,169.64998309097058,169.64998309097058]
[null,null,0,0,191292.38906241994,191292.38906241994,191292.38906241994,191292.38906241994,191292.38906241994,0,0,577,577,577,577,577]

{"sheet":"4.4 Quoted services","index":30,"n_rows":19,"n_cols":16,"rows_kept":19,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,1,9,1],[8,2,8,8],[8,9,8,15]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2021)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Service (DNSP to nominate)"]
[null,"Connection services",12737.744999999999,12928.811174999997,0,0,0,0,0,57,57,0,0,0,0,0]
[null,"Ancillary services",1533310.5514499999,1563976.762479,0,0,0,0,0,680,680,0,0,0,0,0]
[null,"Audit design and construction",0,0,619789.69171646913,619789.69171646913,619789.69171646913,619789.69171646913,619789.69171646913,0,0,305,305,305,305,305]
[null,"Specification and design enquiry",0,0,746040.46251009672,746040.46251009672,746040.46251009672,746040.46251009672,746040.46251009672,0,0,313,313,313,313,313]
[null,"High load escorts–surveying and  lifting overhead lines",0,0,32833.822650302973,32833.822650302973,32833.822650302973,32833.822650302973,32833.822650302973,0,0,25,25,25,25,25]
[null,"No-go zone safety-related services  ",0,0,94579.166846248307,94579.166846248307,94579.166846248307,94579.166846248307,94579.166846248307,0,0,54,54,54,54,54]
[null,"Elective undergrounding ",0,0,64937.358560351706,64937.358560351706,64937.358560351706,64937.358560351706,64937.358560351706,0,0,36,36,36,36,36]
[null,"Reserve feeder maintenance",0,0,5796.260195531202,5796.260195531202,5796.260195531202,5796.260195531202,5796.260195531202,0,0,4,4,4,4,4]

{"sheet":"5.4 MD & utilisation-Spatial","index":31,"n_rows":11579,"n_cols":12,"rows_kept":11579,"cut":false,"hidden":false,"merged":[[5,1,5,2],[11,2,12,2],[11,3,12,3],[13,2,14,2],[13,3,14,3],[15,2,16,2],[15,3,16,3],[17,2,18,2],[17,3,18,3],[19,2,20,2],[19,3,20,3],[21,2,22,2],[21,3,22,3],[23,2,24,2],[23,3,24,3],[25,2,26,2],[25,3,26,3],[27,2,28,2],[27,3,28,3],[29,2,30,2],[29,3,30,3],[31,2,32,2],[31,3,32,3],[33,2,34,2],[33,3,34,3],[35,2,36,2],[35,3,36,3],[37,2,38,2],[37,3,38,3],[39,2,40,2],[39,3,40,3],[9,5,9,11],[41,2,42,2],[41,3,42,3],[43,2,44,2],[43,3,44,3],[45,2,46,2],[45,3,46,3],[47,2,48,2],[47,3,48,3],[49,2,50,2],[49,3,50,3],[51,2,52,2],[51,3,52,3],[53,2,54,2],[53,3,54,3],[55,2,56,2],[55,3,56,3],[57,2,58,2],[57,3,58,3],[59,2,60,2],[59,3,60,3],[61,2,62,2],[61,3,62,3],[63,2,64,2],[63,3,64,3],[65,2,66,2],[65,3,66,3],[67,2,68,2],[67,3,68,3],[69,2,70,2],[69,3,70,3],[71,2,72,2],[71,3,72,3],[73,2,74,2],[73,3,74,3],[75,2,76,2],[75,3,76,3],[77,2,78,2],[77,3,78,3],[79,2,80,2],[79,3,80,3],[81,2,82,2],[81,3,82,3],[83,2,84,2],[83,3,84,3],[85,2,86,2],[85,3,86,3],[87,2,88,2],[87,3,88,3],[89,2,90,2],[89,3,90,3],[91,2,92,2],[91,3,92,3],[93,2,94,2],[93,3,94,3],[95,2,96,2],[95,3,96,3],[97,2,98,2],[97,3,98,3],[99,2,100,2],[99,3,100,3],[101,2,102,2],[101,3,102,3],[103,2,104,2],[103,3,104,3],[105,2,106,2],[105,3,106,3],[107,2,108,2],[107,3,108,3],[109,2,110,2],[109,3,110,3],[111,2,112,2],[111,3,112,3],[113,2,114,2],[113,3,114,3],[115,2,116,2],[115,3,116,3],[117,2,118,2],[117,3,118,3],[119,2,120,2],[119,3,120,3],[121,2,122,2],[121,3,122,3],[123,2,124,2],[123,3,124,3],[125,2,126,2],[125,3,126,3],[127,2,128,2],[127,3,128,3],[129,2,130,2],[129,3,130,3],[131,2,132,2],[131,3,132,3],[133,2,134,2],[133,3,134,3],[135,2,136,2],[135,3,136,3],[137,2,138,2],[137,3,138,3],[139,2,140,2],[139,3,140,3],[141,2,142,2],[141,3,142,3],[143,2,144,2],[143,3,144,3],[145,2,146,2],[145,3,146,3],[147,2,148,2],[147,3,148,3],[149,2,150,2],[149,3,150,3],[151,2,152,2],[151,3,152,3],[153,2,154,2],[153,3,154,3],[155,2,156,2],[155,3,156,3],[157,2,158,2],[157,3,158,3],[159,2,160,2],[159,3,160,3],[161,2,162,2],[161,3,162,3],[163,2,164,2],[163,3,164,3],[165,2,166,2],[165,3,166,3],[167,2,168,2],[167,3,168,3],[169,2,170,2],[169,3,170,3],[171,2,172,2],[171,3,172,3],[173,2,174,2],[173,3,174,3],[175,2,176,2],[175,3,176,3],[177,2,178,2],[177,3,178,3],[179,2,180,2],[179,3,180,3],[181,2,182,2],[181,3,182,3],[183,2,184,2],[183,3,184,3],[185,2,186,2],[185,3,186,3],[187,2,188,2],[187,3,188,3],[189,2,190,2],[189,3,190,3],[191,2,192,2],[191,3,192,3],[193,2,194,2],[193,3,194,3],[195,2,196,2],[195,3,196,3],[197,2,198,2],[197,3,198,3],[199,2,200,2],[199,3,200,3],[201,2,202,2],[201,3,202,3],[203,2,204,2],[203,3,204,3],[205,2,206,2],[205,3,206,3],[207,2,208,2],[207,3,208,3],[209,2,210,2],[209,3,210,3],[211,2,212,2],[211,3,212,3],[213,2,214,2],[213,3,214,3],[215,2,216,2],[215,3,216,3],[217,2,218,2],[217,3,218,3],[219,2,220,2],[219,3,220,3],[221,2,222,2],[221,3,222,3],[223,2,224,2],[223,3,224,3],[225,2,226,2],[225,3,226,3],[227,2,228,2],[227,3,228,3],[229,2,230,2],[229,3,230,3],[231,2,232,2],[231,3,232,3],[233,2,234,2],[233,3,234,3],[235,2,236,2],[235,3,236,3],[237,2,238,2],[237,3,238,3],[239,2,240,2],[239,3,240,3],[241,2,242,2],[241,3,242,3],[243,2,244,2],[243,3,244,3],[245,2,246,2],[245,3,246,3],[247,2,248,2],[247,3,248,3],[249,2,250,2],[249,3,250,3],[251,2,252,2],[251,3,252,3],[253,2,254,2],[253,3,254,3],[255,2,256,2],[255,3,256,3],[257,2,258,2],[257,3,258,3],[259,2,260,2],[259,3,260,3],[261,2,262,2],[261,3,262,3],[263,2,264,2],[263,3,264,3],[265,2,266,2],[265,3,266,3],[267,2,268,2],[267,3,268,3],[269,2,270,2],[269,3,270,3],[271,2,272,2],[271,3,272,3],[273,2,274,2],[273,3,274,3],[275,2,276,2],[275,3,276,3],[277,2,278,2],[277,3,278,3],[279,2,280,2],[279,3,280,3],[281,2,282,2],[281,3,282,3],[283,2,284,2],[283,3,284,3],[285,2,286,2],[285,3,286,3],[287,2,288,2],[287,3,288,3],[289,2,290,2],[289,3,290,3],[291,2,292,2],[291,3,292,3],[293,2,294,2],[293,3,294,3],[295,2,296,2],[295,3,296,3],[297,2,298,2],[297,3,298,3],[299,2,300,2],[299,3,300,3],[301,2,302,2],[301,3,302,3],[303,2,304,2],[303,3,304,3],[305,2,306,2],[305,3,306,3],[307,2,308,2],[307,3,308,3],[309,2,310,2],[309,3,310,3],[311,2,312,2],[311,3,312,3],[313,2,314,2],[313,3,314,3],[315,2,316,2],[315,3,316,3],[317,2,318,2],[317,3,318,3],[319,2,320,2],[319,3,320,3],[321,2,322,2],[321,3,322,3],[323,2,324,2],[323,3,324,3],[325,2,326,2],[325,3,326,3],[327,2,328,2],[327,3,328,3],[329,2,330,2],[329,3,330,3],[331,2,332,2],[331,3,332,3],[333,2,334,2],[333,3,334,3],[335,2,336,2],[335,3,336,3],[337,2,338,2],[337,3,338,3],[339,2,340,2],[339,3,340,3],[341,2,342,2],[341,3,342,3],[343,2,344,2],[343,3,344,3],[345,2,346,2],[345,3,346,3],[347,2,348,2],[347,3,348,3],[349,2,350,2],[349,3,350,3],[351,2,352,2],[351,3,352,3],[353,2,354,2],[353,3,354,3],[355,2,356,2],[355,3,356,3],[357,2,358,2],[357,3,358,3],[359,2,360,2],[359,3,360,3],[361,2,362,2],[361,3,362,3],[363,2,364,2],[363,3,364,3],[365,2,366,2],[365,3,366,3],[367,2,368,2],[367,3,368,3],[369,2,370,2],[369,3,370,3],[371,2,372,2],[371,3,372,3],[373,2,374,2],[373,3,374,3],[375,2,376,2],[375,3,376,3],[377,2,378,2],[377,3,378,3],[379,2,380,2],[379,3,380,3],[381,2,382,2],[381,3,382,3],[383,2,384,2],[383,3,384,3],[385,2,386,2],[385,3,386,3],[387,2,388,2],[387,3,388,3],[389,2,390,2],[389,3,390,3],[391,2,392,2],[391,3,392,3],[393,2,394,2],[393,3,394,3],[395,2,396,2],[395,3,396,3],[397,2,398,2],[397,3,398,3],[399,2,400,2],[399,3,400,3],[401,2,402,2],[401,3,402,3],[403,2,404,2],[403,3,404,3],[405,2,406,2],[405,3,406,3],[407,2,408,2],[407,3,408,3],[409,2,410,2],[409,3,410,3],[411,2,412,2],[411,3,412,3],[413,2,414,2],[413,3,414,3],[415,2,416,2],[415,3,416,3],[417,2,418,2],[417,3,418,3],[419,2,420,2],[419,3,420,3],[421,2,422,2],[421,3,422,3],[423,2,424,2],[423,3,424,3],[425,2,426,2],[425,3,426,3],[427,2,428,2],[427,3,428,3],[429,2,430,2],[429,3,430,3],[431,2,432,2],[431,3,432,3],[433,2,434,2],[433,3,434,3],[435,2,436,2],[435,3,436,3],[437,2,438,2],[437,3,438,3],[439,2,440,2],[439,3,440,3],[441,2,442,2],[441,3,442,3],[443,2,444,2],[443,3,444,3],[445,2,446,2],[445,3,446,3],[447,2,448,2],[447,3,448,3],[449,2,450,2],[449,3,450,3],[451,2,452,2],[451,3,452,3],[453,2,454,2],[453,3,454,3],[455,2,456,2],[455,3,456,3],[457,2,458,2],[457,3,458,3],[459,2,460,2],[459,3,460,3],[461,2,462,2],[461,3,462,3],[463,2,464,2],[463,3,464,3],[465,2,466,2],[465,3,466,3],[467,2,468,2],[467,3,468,3],[469,2,470,2],[469,3,470,3],[471,2,472,2],[471,3,472,3],[473,2,474,2],[473,3,474,3],[475,2,476,2],[475,3,476,3],[477,2,478,2],[477,3,478,3],[479,2,480,2],[479,3,480,3],[481,2,482,2],[481,3,482,3],[483,2,484,2],[483,3,484,3],[485,2,486,2],[485,3,486,3],[487,2,488,2],[487,3,488,3],[489,2,490,2],[489,3,490,3],[491,2,492,2],[491,3,492,3],[493,2,494,2],[493,3,494,3],[495,2,496,2],[495,3,496,3],[497,2,498,2],[497,3,498,3],[499,2,500,2],[499,3,500,3],[501,2,502,2],[501,3,502,3],[503,2,504,2],[503,3,504,3],[505,2,506,2],[505,3,506,3],[507,2,508,2],[507,3,508,3],[509,2,510,2],[509,3,510,3],[511,2,512,2],[511,3,512,3],[513,2,514,2],[513,3,514,3],[515,2,516,2],[515,3,516,3],[517,2,518,2],[517,3,518,3],[519,2,520,2],[519,3,520,3],[521,2,522,2],[521,3,522,3],[523,2,524,2],[523,3,524,3],[525,2,526,2],[525,3,526,3],[527,2,528,2],[527,3,528,3],[529,2,530,2],[529,3,530,3],[531,2,532,2],[531,3,532,3],[533,2,534,2],[533,3,534,3],[535,2,536,2],[535,3,536,3],[537,2,538,2],[537,3,538,3],[539,2,540,2],[539,3,540,3],[541,2,542,2],[541,3,542,3],[543,2,544,2],[543,3,544,3],[545,2,546,2],[545,3,546,3],[547,2,548,2],[547,3,548,3],[549,2,550,2],[549,3,550,3],[551,2,552,2],[551,3,552,3],[553,2,554,2],[553,3,554,3],[555,2,556,2],[555,3,556,3],[557,2,558,2],[557,3,558,3],[559,2,560,2],[559,3,560,3],[561,2,562,2],[561,3,562,3],[563,2,564,2],[563,3,564,3],[565,2,566,2],[565,3,566,3],[567,2,568,2],[567,3,568,3],[569,2,570,2],[569,3,570,3],[571,2,572,2],[571,3,572,3],[573,2,574,2],[573,3,574,3],[575,2,576,2],[575,3,576,3],[577,2,578,2],[577,3,578,3],[579,2,580,2],[579,3,580,3],[581,2,582,2],[581,3,582,3],[583,2,584,2],[583,3,584,3],[585,2,586,2],[585,3,586,3],[587,2,588,2],[587,3,588,3],[589,2,590,2],[589,3,590,3],[591,2,592,2],[591,3,592,3],[593,2,594,2],[593,3,594,3],[595,2,596,2],[595,3,596,3],[597,2,598,2],[597,3,598,3],[599,2,600,2],[599,3,600,3],[601,2,602,2],[601,3,602,3],[603,2,604,2],[603,3,604,3],[605,2,606,2],[605,3,606,3],[607,2,608,2],[607,3,608,3],[609,2,610,2],[609,3,610,3],[611,2,612,2],[611,3,612,3],[613,2,614,2],[613,3,614,3],[615,2,616,2],[615,3,616,3],[617,2,618,2],[617,3,618,3],[619,2,620,2],[619,3,620,3],[621,2,622,2],[621,3,622,3],[623,2,624,2],[623,3,624,3],[625,2,626,2],[625,3,626,3],[627,2,628,2],[627,3,628,3],[629,2,630,2],[629,3,630,3],[631,2,632,2],[631,3,632,3],[633,2,634,2],[633,3,634,3],[635,2,636,2],[635,3,636,3],[637,2,638,2],[637,3,638,3],[639,2,640,2],[639,3,640,3],[641,2,642,2],[641,3,642,3],[643,2,644,2],[643,3,644,3],[645,2,646,2],[645,3,646,3],[647,2,648,2],[647,3,648,3],[649,2,650,2],[649,3,650,3],[651,2,652,2],[651,3,652,3],[653,2,654,2],[653,3,654,3],[655,2,656,2],[655,3,656,3],[657,2,658,2],[657,3,658,3],[659,2,660,2],[659,3,660,3],[661,2,662,2],[661,3,662,3],[663,2,664,2],[663,3,664,3],[665,2,666,2],[665,3,666,3],[667,2,668,2],[667,3,668,3],[669,2,670,2],[669,3,670,3],[671,2,672,2],[671,3,672,3],[673,2,674,2],[673,3,674,3],[675,2,676,2],[675,3,676,3],[677,2,678,2],[677,3,678,3],[679,2,680,2],[679,3,680,3],[681,2,682,2],[681,3,682,3],[683,2,684,2],[683,3,684,3],[685,2,686,2],[685,3,686,3],[687,2,688,2],[687,3,688,3],[689,2,690,2],[689,3,690,3],[691,2,692,2],[691,3,692,3],[693,2,694,2],[693,3,694,3],[695,2,696,2],[695,3,696,3],[697,2,698,2],[697,3,698,3],[699,2,700,2],[699,3,700,3],[701,2,702,2],[701,3,702,3],[703,2,704,2],[703,3,704,3],[705,2,706,2],[705,3,706,3],[707,2,708,2],[707,3,708,3],[709,2,710,2],[709,3,710,3],[711,2,712,2],[711,3,712,3],[713,2,714,2],[713,3,714,3],[715,2,716,2],[715,3,716,3],[717,2,718,2],[717,3,718,3],[719,2,720,2],[719,3,720,3],[721,2,722,2],[721,3,722,3],[723,2,724,2],[723,3,724,3],[725,2,726,2],[725,3,726,3],[727,2,728,2],[727,3,728,3],[729,2,730,2],[729,3,730,3],[731,2,732,2],[731,3,732,3],[733,2,734,2],[733,3,734,3],[735,2,736,2],[735,3,736,3],[737,2,738,2],[737,3,738,3],[739,2,740,2],[739,3,740,3],[741,2,742,2],[741,3,742,3],[743,2,744,2],[743,3,744,3],[745,2,746,2],[745,3,746,3],[747,2,748,2],[747,3,748,3],[749,2,750,2],[749,3,750,3],[751,2,752,2],[751,3,752,3],[753,2,754,2],[753,3,754,3],[755,2,756,2],[755,3,756,3],[757,2,758,2],[757,3,758,3],[759,2,760,2],[759,3,760,3],[761,2,762,2],[761,3,762,3],[763,2,764,2],[763,3,764,3],[765,2,766,2],[765,3,766,3],[767,2,768,2],[767,3,768,3],[769,2,770,2],[769,3,770,3],[771,2,772,2],[771,3,772,3],[773,2,774,2],[773,3,774,3],[775,2,776,2],[775,3,776,3],[777,2,778,2],[777,3,778,3],[779,2,780,2],[779,3,780,3],[781,2,782,2],[781,3,782,3],[783,2,784,2],[783,3,784,3],[785,2,786,2],[785,3,786,3],[787,2,788,2],[787,3,788,3],[789,2,790,2],[789,3,790,3],[791,2,792,2],[791,3,792,3],[793,2,794,2],[793,3,794,3],[795,2,796,2],[795,3,796,3],[797,2,798,2],[797,3,798,3],[799,2,800,2],[799,3,800,3],[801,2,802,2],[801,3,802,3],[803,2,804,2],[803,3,804,3],[805,2,806,2],[805,3,806,3],[807,2,808,2],[807,3,808,3],[809,2,810,2],[809,3,810,3],[811,2,812,2],[811,3,812,3],[813,2,814,2],[813,3,814,3],[815,2,816,2],[815,3,816,3],[817,2,818,2],[817,3,818,3],[819,2,820,2],[819,3,820,3],[821,2,822,2],[821,3,822,3],[823,2,824,2],[823,3,824,3],[825,2,826,2],[825,3,826,3],[827,2,828,2],[827,3,828,3],[829,2,830,2],[829,3,830,3],[831,2,832,2],[831,3,832,3],[833,2,834,2],[833,3,834,3],[835,2,836,2],[835,3,836,3],[837,2,838,2],[837,3,838,3],[839,2,840,2],[839,3,840,3],[841,2,842,2],[841,3,842,3],[843,2,844,2],[843,3,844,3],[845,2,846,2],[845,3,846,3],[847,2,848,2],[847,3,848,3],[849,2,850,2],[849,3,850,3],[851,2,852,2],[851,3,852,3],[853,2,854,2],[853,3,854,3],[855,2,856,2],[855,3,856,3],[857,2,858,2],[857,3,858,3],[859,2,860,2],[859,3,860,3],[861,2,862,2],[861,3,862,3],[863,2,864,2],[863,3,864,3],[865,2,866,2],[865,3,866,3],[867,2,868,2],[867,3,868,3],[869,2,870,2],[869,3,870,3],[871,2,872,2],[871,3,872,3],[873,2,874,2],[873,3,874,3],[875,2,876,2],[875,3,876,3],[877,2,878,2],[877,3,878,3],[879,2,880,2],[879,3,880,3],[881,2,882,2],[881,3,882,3],[883,2,884,2],[883,3,884,3],[885,2,886,2],[885,3,886,3],[887,2,888,2],[887,3,888,3],[889,2,890,2],[889,3,890,3],[891,2,892,2],[891,3,892,3],[893,2,894,2],[893,3,894,3],[895,2,896,2],[895,3,896,3],[897,2,898,2],[897,3,898,3],[899,2,900,2],[899,3,900,3],[901,2,902,2],[901,3,902,3],[903,2,904,2],[903,3,904,3],[905,2,906,2],[905,3,906,3],[907,2,908,2],[907,3,908,3],[909,2,910,2],[909,3,910,3],[911,2,912,2],[911,3,912,3],[913,2,914,2],[913,3,914,3],[915,2,916,2],[915,3,916,3],[917,2,918,2],[917,3,918,3],[919,2,920,2],[919,3,920,3],[921,2,922,2],[921,3,922,3],[923,2,924,2],[923,3,924,3],[925,2,926,2],[925,3,926,3],[927,2,928,2],[927,3,928,3],[929,2,930,2],[929,3,930,3],[931,2,932,2],[931,3,932,3],[933,2,934,2],[933,3,934,3],[935,2,936,2],[935,3,936,3],[937,2,938,2],[937,3,938,3],[939,2,940,2],[939,3,940,3],[941,2,942,2],[941,3,942,3],[943,2,944,2],[943,3,944,3],[945,2,946,2],[945,3,946,3],[947,2,948,2],[947,3,948,3],[949,2,950,2],[949,3,950,3],[951,2,952,2],[951,3,952,3],[953,2,954,2],[953,3,954,3],[955,2,956,2],[955,3,956,3],[957,2,958,2],[957,3,958,3],[959,2,960,2],[959,3,960,3],[961,2,962,2],[961,3,962,3],[963,2,964,2],[963,3,964,3],[965,2,966,2],[965,3,966,3],[967,2,968,2],[967,3,968,3],[969,2,970,2],[969,3,970,3],[971,2,972,2],[971,3,972,3],[973,2,974,2],[973,3,974,3],[975,2,976,2],[975,3,976,3],[977,2,978,2],[977,3,978,3],[979,2,980,2],[979,3,980,3],[981,2,982,2],[981,3,982,3],[983,2,984,2],[983,3,984,3],[985,2,986,2],[985,3,986,3],[987,2,988,2],[987,3,988,3],[989,2,990,2],[989,3,990,3],[991,2,992,2],[991,3,992,3],[993,2,994,2],[993,3,994,3],[995,2,996,2],[995,3,996,3],[997,2,998,2],[997,3,998,3],[999,2,1000,2],[999,3,1000,3],[1001,2,1002,2],[1001,3,1002,3],[1003,2,1004,2],[1003,3,1004,3],[1005,2,1006,2],[1005,3,1006,3],[1007,2,1008,2],[1007,3,1008,3]],"merged_total":11556,"flags":["merged_cut"]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"Demand"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"BOX HILL","Substation Rating","MVA","Non-Coincident",108.9,108.9,108.9,108.9,108.9,108.9,108.9]
[null,null,null,null,"Coincident",108.9,108.9,108.9,108.9,108.9,108.9,108.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",48.195282762671788,48.81269339938752,50.073033805659968,51.862353260586765,52.586459828264772,53.724175256308122,54.750480291829206]
[null,null,null,null,"Coincident",46.018283693735412,46.607805659522491,47.811216015098715,49.51971123652973,50.211109637904237,51.297434031688866,52.277380482329846]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",48.199898253213519,48.814333288326019,50.073242877790022,51.870480559772396,52.600870922501471,53.751798055947404,54.793334865501549]
[null,null,null,null,"Coincident",46.494884306096857,47.087584434240043,48.301961597579016,50.035624138842934,50.740177813105355,51.85039227109435,52.855085957507534]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",46.033500502987117,46.623217405277323,47.827025691075235,49.536085858519122,50.227712883752368,51.31439649108777,52.294666979415929]
[null,null,null,null,"Coincident",43.954149952677582,44.517229120450416,45.666660932719481,47.298522208902519,47.958908180993731,48.996505880626344,49.93249718190409]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",46.037908967342865,46.624783737580984,47.827225385349287,49.543848610591603,50.241477573484772,51.340780279877855,52.335599326434526]
[null,null,null,null,"Coincident",44.409372814153507,44.975487588940801,46.135394296712576,47.791294021552339,48.464245191446928,49.524661374954484,50.484289883549323]
[null,"BEAUMARIS","Substation Rating","MVA","Non-Coincident",63,63,63,63,63,63,63]
[null,null,null,null,"Coincident",63,63,63,63,63,63,63]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.613798485902727,30.556253905213598,30.492019661855853,30.806068267062525,30.907289348119708,31.542007742942207,32.148695004815032]
[null,null,null,null,"Coincident",26.345924409218267,26.29640212684961,26.241122788652955,26.511389832365463,26.598499667865948,27.144731879423567,27.666840782332081]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.023734437195536,30.967996633931588,30.905788613271671,31.210024537401203,31.308132577190506,31.923864836568672,32.513231782008489]
[null,null,null,null,"Coincident",26.751189593367666,26.703127921564416,26.64948710155706,26.911824084359001,26.996420823618433,27.527355306787214,28.035555469776675]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.928185867756028,29.871930029156339,29.809134346511126,30.116149662903926,30.215103842961312,30.835607375140729,31.428707546793422]
[null,null,null,null,"Coincident",25.755893145374383,25.707479941374,25.653438613932785,25.917652880642667,26.002811844139753,26.536810889112228,27.047226880014229]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.328941081122188,30.274451556187476,30.213636717884004,30.511059113513546,30.606969970550367,31.208912572084405,31.785080325182957]
[null,null,null,null,"Coincident",26.152082195960144,26.105096891359505,26.052657386604213,26.309119190417881,26.391821339827022,26.91086525733348,27.407684002089258]
[null,"BENTLEIGH","Substation Rating","MVA","Non-Coincident",62.1,62.1,62.1,62.1,62.1,62.1,62.1]
[null,null,null,null,"Coincident",62.1,62.1,62.1,62.1,62.1,62.1,62.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",32.267909788048776,32.482658059788427,32.67259391271751,33.009101059851766,33.051400167885248,33.730150459601546,34.378925033232576]
[null,null,null,null,"Coincident",30.640943718252171,30.844864261949851,31.025223442879312,31.344763711333552,31.384930074667885,32.029457396822764,32.645520393373729]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",32.386092229254935,32.594496075766045,32.77900101364137,33.106293146451797,33.147470110111627,33.809285610997783,34.443685965742212]
[null,null,null,null,"Coincident",30.804535796530768,31.002762359480744,31.178257103433925,31.489566110698913,31.528732220709117,32.158228337234426,32.761648110719896]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.672516287792511,31.883302117402355,32.069733356210399,32.400031419164442,32.441550042370885,33.107776327585391,33.744579993686038]
[null,null,null,null,"Coincident",30.07557029148245,30.275728181600034,30.452759453013744,30.766403702786967,30.805828933776027,31.438463716845813,32.043159385723428]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",31.788518077763413,31.993076546732063,32.174177079379476,32.495430159464135,32.535847343619054,33.185451311431493,33.80814598550878]
[null,null,null,null,"Coincident",30.236143839563702,30.430712811800991,30.602969402723339,30.908534270974851,30.946977704881039,31.564858631619419,32.15714436470936]
[null,"BULLEEN","Substation Rating","MVA","Non-Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,null,null,"Coincident",59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",31.273754350542383,31.0323164768932,30.926540973105428,31.259063516893264,31.306894494894532,31.825150093398566,32.31102467348132]
[null,null,null,null,"Coincident",28.611869054203602,28.390981317216696,28.294208962046437,28.59842864011215,28.64218845429906,29.116332401162545,29.56085146037978]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.612245579135411,31.362958397540652,31.253756958297949,31.597075979500993,31.646466287779297,32.181716663534274,32.683683668693881]
[null,null,null,null,"Coincident",28.964444863629467,28.736037653251579,28.635982785018431,28.950545849998353,28.995799290072501,29.48621778811885,29.94614068755067]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",30.564696996910779,30.328733147833042,30.225355849836429,30.550339242671097,30.597085767993512,31.103591164105435,31.57844970370617]
[null,null,null,null,"Coincident",27.963163563758524,27.747283926294369,27.652705652119074,27.950027878812815,27.992795544193569,28.456189414541296,28.89063007049954]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.89551374894166,30.651878556145384,30.545152997561406,30.880688083586826,30.928958585113104,31.452073442672564,31.942659550217535]
[null,null,null,null,"Coincident",28.307745562541001,28.084516937705661,27.986730573576374,28.294161675700003,28.338389102584241,28.817688537709682,29.267183788759716]
[null,"BURWOOD","Substation Rating","MVA","Non-Coincident",38.1,38.1,38.1,38.1,38.1,38.1,38.1]
[null,null,null,null,"Coincident",38.1,38.1,38.1,38.1,38.1,38.1,38.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.084799498403765,23.938864256914957,23.832430786986997,24.100878088336753,24.137755986775119,24.479731539484785,24.826680658506703]
[null,null,null,null,"Coincident",22.907088703610384,22.768289477900055,22.667060446002388,22.922381074462312,22.957455698637048,23.282709156566217,23.612692980828538]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.213308652887822,24.063115980418022,23.953607855067826,24.22985922244446,24.267821819405899,24.619997221018082,24.977547304659776]
[null,null,null,null,"Coincident",23.020695538561512,22.877900523034473,22.77378615977975,23.036430918976272,23.072523689238718,23.407352886392566,23.747292038587734]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.573834685679074,23.430995495429649,23.326820037158914,23.589572164460421,23.625667689415856,23.960388148544265,24.299976658579681]
[null,null,null,null,"Coincident",22.421109308586402,22.285254741824804,22.186173308180109,22.436077248113545,22.470407755702464,22.788760883312094,23.111744021395669]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.699617487549787,23.552611188741359,23.445426304602496,23.715816932793576,23.752974144132093,24.097678059915925,24.447642632557631]
[null,null,null,null,"Coincident",22.532305947216447,22.39254036227992,22.290634810276707,22.547707497752022,22.583034551214581,22.910760266438682,23.243487527779177]
[null,"CLARINDA","Substation Rating","MVA","Non-Coincident",59.4,59.4,59.4,59.4,59.4,59.4,59.4]
[null,null,null,null,"Coincident",59.4,59.4,59.4,59.4,59.4,59.4,59.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.675770805164291,36.379850949771495,36.928047229753702,37.395299506743207,37.449185889318791,38.233921405007223,38.945154593240325]
[null,null,null,null,"Coincident",30.715612157465024,31.321800956233631,31.793779106728454,32.196067253439622,32.242461576264482,32.918091876663908,33.530439200078234]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.001410688311829,36.736853010235521,37.310062668868461,37.799026521337929,37.855439304858479,38.677474644998938,39.423302074312012]
[null,null,null,null,"Coincident",31.046333402474332,31.680552648003665,32.174868227065531,32.596533225611097,32.645181599434657,33.354075577494875,33.997250569487107]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",35.078433928080919,35.770725314511239,36.309742876093736,36.769171719709611,36.82215585622972,37.593752161420426,38.29307682456917]
[null,null,null,null,"Coincident",30.201325642282338,30.797364725549158,31.261440315059165,31.656992754599312,31.702610274588938,32.366928166465854,32.969022659188553]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",35.39862146341752,36.121749914892497,36.685362043894706,37.166138935464687,37.22160717216326,38.029878772604491,38.763218448537209]
[null,null,null,null,"Coincident",30.52650945975412,31.150109662303848,31.636148673890744,32.050753529159181,32.098587359469335,32.795611978985058,33.428017977555037]
[null,"CAULFIELD","Substation Rating","MVA","Non-Coincident",84.2,84.2,84.2,84.2,84.2,84.2,84.2]
[null,null,null,null,"Coincident",84.2,84.2,84.2,84.2,84.2,84.2,84.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",55.046915795432227,56.099634894973349,56.487057336874564,57.123324708793362,57.267771434469118,58.366642231837218,59.076652027415854]
[null,null,null,null,"Coincident",49.701435340423387,50.651927288998884,51.001728021107837,51.576208919586577,51.70662875315162,52.698790713429915,53.339853076981029]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",55.4855062742635,56.579751795897728,56.98274378361738,57.644903608831186,57.795283146077352,58.939927644730929,59.68009430100188]
[null,null,null,null,"Coincident",50.097454351049613,51.085440561321221,51.44929905454341,52.047158276603618,52.18293485157588,53.216425926452786,53.884716940892034]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.503517277937398,52.488472303093047,52.850956161488902,53.446266672704262,53.581415287737116,54.609551201996005,55.273857298816843]
[null,null,null,null,"Coincident",46.502128172023681,47.391436460937129,47.718720338510948,48.256221603624518,48.378246244866276,49.306542225218827,49.906339071968418]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.913875460189992,52.937683830112704,53.31473501458818,53.934271268451923,54.074970796897603,55.145933935551639,55.838455680302452]
[null,null,null,null,"Coincident",46.872655233557474,47.797044259096843,48.13748099241058,48.696855706292503,48.82389227271905,49.790856991129921,50.416129766388991]
[null,"CHELTENHAM","Substation Rating","MVA","Non-Coincident",61.8,61.8,61.8,61.8,61.8,61.8,61.8]
[null,null,null,null,"Coincident",61.8,61.8,61.8,61.8,61.8,61.8,61.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.173600041471708,28.526361252396448,28.863165589196694,29.720921606795773,30.624907304836313,31.759889822159856,32.539716316155292]
[null,null,null,null,"Coincident",26.087635680062096,26.414278563439289,26.726146014562897,27.52039405019082,28.35744893546477,29.408397709195913,30.130486098293041]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.180804824461493,28.537074165618701,28.877823884746999,29.748118538315424,30.6689210318623,31.829766789174755,32.630157146785372]
[null,null,null,null,"Coincident",26.18846492245931,26.519546564802774,26.836205798714477,27.644971948196375,28.500675110436571,29.579450843959073,30.323254824545383]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.026790491719218,27.365192517986149,27.68828719647961,28.511128159172952,29.378317017980077,30.467099944631759,31.215183513720632]
[null,null,null,null,"Coincident",25.025735543610942,25.339082391782686,25.638255243328,26.400173323579633,27.203155795861061,28.211325581878832,28.904021282105422]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.033702003209285,27.375469360874089,27.702348824465407,28.53721803654458,29.420539161310714,30.534132561866635,31.301942940195705]
[null,null,null,null,"Coincident",25.122460520386966,25.44006544734339,25.743835031620943,26.519680264273713,27.340551933315812,28.375415979605449,29.088943335733948]
[null,"CARRUM","Substation Rating","MVA","Non-Coincident",110.8,110.8,110.8,110.8,110.8,110.8,110.8]
[null,null,null,null,"Coincident",110.8,110.8,110.8,110.8,110.8,110.8,110.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",88.677452711118164,88.527410267801415,88.806188774428421,89.85095587883859,90.34731822764094,92.080929072520462,93.848290972649096]
[null,null,null,null,"Coincident",79.149602560307216,79.015681260217704,79.264506720662141,80.197019987044911,80.640051236054617,82.187396194343535,83.764865863337221]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",88.855288912252945,88.702600023472783,88.986307996544483,90.050019625908845,90.55563738620269,92.322816040207783,94.126301153213916]
[null,null,null,null,"Coincident",79.335180539165705,79.198851000361756,79.452162013578672,80.401905750730535,80.853350755161657,82.431190850858201,84.041447469137111]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",83.73086715995548,83.589194350175561,83.852422097385201,84.838910240176546,85.307584617034948,86.944491575025026,88.613266894556546]
[null,null,null,null,"Coincident",74.734497384919194,74.608046452411998,74.842991987466547,75.723488010359205,76.141806190735736,77.60283750356767,79.092313117325446]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",83.89878334245968,83.754611710636851,84.022493949912189,85.026869858464195,85.504283363549803,87.172885658751483,88.875769174294106]
[null,null,null,null,"Coincident",74.909723495058287,74.78099865966233,75.020179535402121,75.916944882852079,76.343207484453714,77.83303286185604,79.35346651073155]
[null,"DONCASTER","Substation Rating","MVA","Non-Coincident",110.4,110.4,110.4,110.4,147.20000000000002,147.20000000000002,147.20000000000002]
[null,null,null,null,"Coincident",110.4,110.4,110.4,110.4,147.20000000000002,147.20000000000002,147.20000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",95.101365492913132,96.078693772393819,97.283330465988286,99.277822228456444,100.18465643350865,101.84311729072769,103.39795620594825]
[null,null,null,null,"Coincident",92.123104661409187,93.069826245400151,94.236737694334565,96.168768558748013,97.04720371001612,98.65372704787319,100.15987354089246]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",95.124260289691591,96.095839641934717,97.294592671798512,99.282139493542488,100.18692208571424,101.84333946623221,103.39818920685603]
[null,null,null,null,"Coincident",92.088857009673958,93.029433385982074,94.189934356195707,96.114058806784968,96.989969899303347,98.593531207830949,100.09876588718384]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",88.791185129039647,89.703665572884404,90.828372028147129,92.69052496782129,93.537188770857185,95.085607179356003,96.537279184817081]
[null,null,null,null,"Coincident",86.01053831622032,86.89444288472059,87.983927246532957,89.787763703223334,90.607912790839904,92.107839846213466,93.514050276526305]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",88.812560806756906,89.719673777064358,90.838886962353115,92.694555773073347,93.539304092160748,95.085814613037428,96.537496725612954]
[null,null,null,null,"Coincident",85.978563069916589,86.856730178495042,87.940229410652208,89.736684061098984,90.55447656669844,92.051638129766104,93.45699724721257]
[null,"DROMANA","Substation Rating","MVA","Non-Coincident",89.6,89.6,89.6,89.6,89.6,89.6,89.6]
[null,null,null,null,"Coincident",89.6,89.6,89.6,89.6,89.6,89.6,89.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.873659358595191,47.176078451809332,47.63922747730129,48.75677887605044,49.562280762484363,50.969391743636535,52.359782585940799]
[null,null,null,null,"Coincident",36.329100274234086,36.563488067134344,36.922448464492902,37.788598822333988,38.412897398629731,39.503468875889048,40.581081527037568]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.111309082581968,47.419431292666864,47.891382724747324,49.030500259341459,49.851818741202571,51.287070373349898,52.705861412891359]
[null,null,null,null,"Coincident",36.499361936849034,36.738078803046839,37.103721925082006,37.986250218042017,38.622564536591817,39.734521937316366,40.833726537515602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.204293782871524,41.470135309495582,41.877266495171227,42.859650136252903,43.567726630075754,44.804647643836269,46.026870818285609]
[null,null,null,null,"Coincident",31.935098327083171,32.141136934052099,32.456681098334762,33.218070635507289,33.766860345931327,34.725527284999167,35.672802767000135]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.413199790607266,41.684054642545291,42.098923584394278,43.100264938811712,43.822245012033832,45.0839030671671,46.331091437132756]
[null,null,null,null,"Coincident",32.084766854404158,32.294610933580728,32.616029547492737,33.391816109762757,33.951168259318493,34.928634496016116,35.894890382453283]
[null,"DANDENONG","Substation Rating","MVA","Non-Coincident",126.2,126.2,126.2,126.2,126.2,126.2,126.2]
[null,null,null,null,"Coincident",126.2,126.2,126.2,126.2,126.2,126.2,126.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",2.8736124038696262,2.8736124038696262,2.8736124038696262,2.8736124038696262,2.8736124038696262,2.8736124038696262,2.8736124038696262]
[null,null,null,null,"Coincident",3.5867835879325867,3.5867835879325867,3.5867835879325867,3.5867835879325867,3.5867835879325867,3.5867835879325867,3.5867835879325867]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",89.157754970432393,88.658863628396944,88.402686152922513,89.398449562116156,89.713777256640668,91.435231531523996,93.190200189702765]
[null,null,null,null,"Coincident",82.810880526680819,82.347503770112709,82.109562804437033,83.03444078884705,83.327321246039844,84.92623032957141,86.556268007490829]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",85.438197978640147,84.957938950900342,84.711461513881659,85.670023787144373,85.973850042902484,87.634802458302147,89.331908521569716]
[null,null,null,null,"Coincident",79.156942103275611,78.711990817401357,78.483633938704898,79.371724513672447,79.653214033647018,81.192056346484136,82.764394358889007]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",81.626391726882247,81.169642898609922,80.93510533122037,81.846754285740275,82.135445515394139,83.71148453777802,85.318206905433073]
[null,null,null,null,"Coincident",75.815652551598916,75.391418309032986,75.173576770979935,76.020328157665901,76.28846832041333,77.752313829211758,79.24465842752015]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",78.221034378402734,77.781343949435993,77.555687035658877,78.433277320855055,78.711438665066197,80.232086560968085,81.785834121887333]
[null,null,null,null,"Coincident",72.470370818185017,72.063005603883724,71.853938562657902,72.667010058068414,72.924721502598118,74.33357422074026,75.773093178683851]
[null,"DANDENONG SOUTH","Substation Rating","MVA","Non-Coincident",144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001]
[null,null,null,null,"Coincident",144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001,144.80000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",69.14703774974727,68.812702634595468,68.621657537932521,69.394608436011424,69.639378250227878,70.975639068297482,72.337915074741744]
[null,null,null,null,"Coincident",48.303622257762768,48.070067825998883,47.93661062401717,48.476566194344386,48.647553542910266,49.581017070697023,50.532653869141619]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",70.030520296412817,69.670281987853699,69.464554996865218,70.297441658938595,70.56148339614721,72.005344510805855,73.481294196838121]
[null,null,null,null,"Coincident",48.804491708317208,48.553440488525084,48.410068696006945,48.99051005244808,49.174521576562199,50.180752966819753,51.209346984241968]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",67.96310748183798,67.634496826841456,67.446722789645918,68.206439281832331,68.447018166094992,69.760399629100121,71.099350850423235]
[null,null,null,null,"Coincident",47.476571348545313,47.247015817818529,47.115843659795871,47.646554152331753,47.814613868652138,48.732094705632441,49.667437651926605]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",68.831463108215885,68.477392772299467,68.275188223045063,69.09381426367959,69.353335098549564,70.772474534132272,72.223153123034834]
[null,null,null,null,"Coincident",47.968864950848257,47.7221122107536,47.581195219051963,48.151698303182371,48.332559196117884,49.321561969818383,50.332544479499319]
[null,"DANDENONG VALLEY","Substation Rating","MVA","Non-Coincident",131.6,131.6,131.6,131.6,131.6,131.6,131.6]
[null,null,null,null,"Coincident",131.6,131.6,131.6,131.6,131.6,131.6,131.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",83.518865518329775,84.096316551798921,85.106185200550854,86.520308681736836,86.825484549996219,88.491517417164843,90.189985687880181]
[null,null,null,null,"Coincident",64.892726807828325,65.341396362033265,66.126046990709099,67.224796694355362,67.461913112596847,68.75639209086205,70.076072821667779]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",87.490590341102205,88.135589165880575,89.264027098823462,90.845087970774259,91.186423662942104,93.050665548905485,94.95253906116271]
[null,null,null,null,"Coincident",67.089776196521541,67.584375977283003,68.449687870569406,69.662081336411916,69.923825314891701,71.353368428246455,72.811768329241133]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",81.939926660748071,82.506460880759121,83.497237784901358,84.884627012694338,85.18403347743272,86.818569699913283,88.484928128925688]
[null,null,null,null,"Coincident",63.665918382026291,64.106105759312868,64.875922429702101,65.95390007674682,66.186533767352955,67.456540392618379,68.751272326855343]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",85.836565326454334,86.469370334886946,87.576474950026309,89.127645587819444,89.462528268628731,91.291526333505573,93.157444592155457]
[null,null,null,null,"Coincident",65.82143216519728,66.306681450020491,67.155634469611016,68.345107423518698,68.601903086000704,70.004420435101409,71.43524902919097]
[null,"EAST BURWOOD","Substation Rating","MVA","Non-Coincident",101.8,101.8,101.8,101.8,101.8,101.8,101.8]
[null,null,null,null,"Coincident",101.8,101.8,101.8,101.8,101.8,101.8,101.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",64.512880827374261,65.408525787367722,66.345880122413874,68.256181613480422,69.321367806980177,70.303489470790609,71.611285614182634]
[null,null,null,null,"Coincident",59.802504013269356,60.632753889380076,61.501667750682444,63.272489501640223,64.259901640033192,65.170314165226458,66.382622205275311]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.514180916537256,65.408666791598264,66.346051244652514,68.260134204877914,69.329473818276114,70.316649005954588,71.632911621269827]
[null,null,null,null,"Coincident",59.966501116975543,60.797933640242924,61.66924077074551,63.448397792375125,64.442358410184525,65.359946468400082,66.583424197949938]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.555893362887176,61.396602690897183,62.276463091305921,64.069593577813421,65.06944509146372,65.991326954129661,67.218907598242495]
[null,null,null,null,"Coincident",56.13443407606335,56.913759418809128,57.729377237324428,59.391583167991513,60.31843100660754,61.173002110622583,62.310951547303432]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",60.557113709269274,61.39673504643671,62.276623717523542,64.073303731508375,65.077053909258538,66.003679330862411,67.239207144042368]
[null,null,null,null,"Coincident",56.288372188832298,57.068807639422992,57.886671932636347,59.556701878530802,60.489696536450886,61.351003052168942,62.499437069876784]
[null,"ELSTERNWICK","Substation Rating","MVA","Non-Coincident",66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006]
[null,null,null,null,"Coincident",66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006,66.900000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.2853093660108,35.524532770998725,35.790197203529146,36.193336184186926,36.303658507809708,37.000263756671281,37.710430966286957]
[null,null,null,null,"Coincident",34.472627163174245,34.706340836003697,34.965886553405262,35.359740540371988,35.46752194850913,36.148083163796272,36.841893984232925]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.303805240303475,35.540593450860172,35.80377211597191,36.203567475855579,36.313062894121423,37.005292728458457,37.712442624973441]
[null,null,null,null,"Coincident",34.505080212810661,34.736511248164867,34.993735671656019,35.38448592839454,35.49150408591273,36.168072682326581,36.85922378447107]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.37748957957816,32.59699887229386,32.840770219363407,33.210687002860347,33.311917796855653,33.951116647350105,34.6027598337703]
[null,null,null,null,"Coincident",31.631779536882732,31.846233147821728,32.084390015696265,32.445786970633385,32.544686242923575,33.169163229299379,33.805797936844982]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.394461231178674,32.611736010899079,32.853226439644779,33.220075146122781,33.320547179034264,33.955731187637852,34.604605714090738]
[null,null,null,null,"Coincident",31.66155816984098,31.873917252705919,32.109944121701439,32.468493121074978,32.566692041309146,33.187505435717419,33.821699609147366]
[null,"EAST MALVERN","Substation Rating","MVA","Non-Coincident",63.9,63.9,63.9,63.9,63.9,63.9,63.9]
[null,null,null,null,"Coincident",63.9,63.9,63.9,63.9,63.9,63.9,63.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.958366345685022,37.099684127106393,38.068873140513588,38.534812721398438,38.632255010524815,39.373542052157305,40.129260948534757]
[null,null,null,null,"Coincident",33.5294670255944,34.593691594363904,35.497414270588997,35.931880777298716,36.022741079147586,36.713956001982908,37.418627943224948]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.072283440352571,37.186883488808782,38.136725380166119,38.594384622636056,38.690175787502326,39.419784560813959,40.165140978808054]
[null,null,null,null,"Coincident",33.557622780229266,34.594522150316749,35.478148936620286,35.903903969458362,35.993017368158959,36.671763864272052,37.365160209785579]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.606845588759498,33.641786172787953,34.520641352210831,34.943152759474103,35.031512882534592,35.70370782796374,36.388989498599038]
[null,null,null,null,"Coincident",30.404333263270008,31.369366153030182,32.188856823864512,32.582828623405724,32.665220237197424,33.292010065213127,33.931002642292981]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.710144973387706,33.720858066520115,34.582169383821949,34.997172226499103,35.084035119310606,35.745640276309942,36.421525309475271]
[null,null,null,null,"Coincident",30.429864744177351,31.370119296525267,32.171387126718244,32.557459410451301,32.638266942233642,33.253750470598298,33.882518400504068]
[null,"ELWOOD","Substation Rating","MVA","Non-Coincident",58.8,58.8,58.8,58.8,58.8,58.8,58.8]
[null,null,null,null,"Coincident",58.8,58.8,58.8,58.8,58.8,58.8,58.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.460351771355008,26.479160234680499,26.509355972083316,26.807956024039051,26.942512450001889,27.459493282282253,27.986539031198646]
[null,null,null,null,"Coincident",22.323183179380109,22.339050873648336,22.364525401844489,22.616438290787876,22.729956348699066,23.166105418784991,23.610745720570812]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.565009229991553,26.584131690321009,26.614832097158803,26.918459931223648,27.055303696837232,27.581193752615583,28.117511426365791]
[null,null,null,null,"Coincident",22.393733202676263,22.409853026730872,22.435732811450205,22.691684565507121,22.807040925863301,23.250354967318454,23.702459267146168]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.600710584168869,24.618197183243648,24.646270755475083,24.923885109284736,25.048984870654326,25.52963214028965,26.019636961304347]
[null,null,null,null,"Coincident",20.754303399239898,20.769055907358602,20.792740078333996,21.026948456471548,21.132488432390286,21.5379848194925,21.951375672071116]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.698012686296607,24.71579121457496,24.744333987927295,25.026622769863046,25.153849115990159,25.642779466315321,26.141404578600739]
[null,null,null,null,"Coincident",20.819895146462773,20.834882064613439,20.858943010566172,21.09690640120715,21.204155483142547,21.616313285350707,22.03664356402675]
[null,"FRANKSTON SOUTH","Substation Rating","MVA","Non-Coincident",93,93,93,93,93,93,93]
[null,null,null,null,"Coincident",93,93,93,93,93,93,93]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",73.967857941417805,73.540994487029721,73.353371480509821,73.812394323972555,74.057460174858207,75.106681191486558,76.171161691610322]
[null,null,null,null,"Coincident",68.130546504350576,67.737369775436392,67.564553388336009,67.987351588168508,68.213077610458029,69.179497394080201,70.159972430603418]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",74.557654164446575,74.144272529324951,73.962650829163181,74.407073149459038,74.644456488284973,75.661651260465945,76.6950310398082]
[null,null,null,null,"Coincident",68.31590761708955,67.937133071242357,67.770716203268705,68.177932799828184,68.39544310680887,69.327481337674229,70.274349614715305]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",66.636590963038614,66.252035749480086,66.083008852004909,66.496536001685826,66.717312340476255,67.662540628285541,68.621515967696567]
[null,null,null,null,"Coincident",61.377840130159484,61.023632808357753,60.867944983680736,61.248837867241875,61.452191229575732,62.322825064488491,63.206121076791746]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",67.167929990006783,66.795520355634949,66.631899949684069,67.032273695748941,67.246128968715098,68.162505268502613,69.093462410996082]
[null,null,null,null,"Coincident",61.544829319704803,61.203596719744688,61.053674130810279,61.42052976964446,61.616481710932199,62.456141694073501,63.309161854844348]
[null,"FRANKSTON","Substation Rating","MVA","Non-Coincident",91.2,91.2,91.2,91.2,91.2,91.2,91.2]
[null,null,null,null,"Coincident",91.2,91.2,91.2,91.2,91.2,91.2,91.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",57.369743795813349,56.882117757358486,56.552098256238409,56.905983898049165,56.993058447243421,57.80051679895552,58.619718527130651]
[null,null,null,null,"Coincident",53.659741336309025,53.203649233379913,52.89497152463732,53.225971991883341,53.30741558004663,54.062656991737853,54.828882355974926]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.5530601922326,57.053803053436432,56.716076307936817,57.078231754807199,57.167364674304807,57.99434413867975,58.834126722447365]
[null,null,null,null,"Coincident",53.993533856096143,53.525154639831172,53.208315528125631,53.548072481386725,53.631692731821929,54.407525390569951,55.195369324792864]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",53.349494038848626,52.896038947183506,52.589145936289597,52.918232641041357,52.999205342605229,53.750080136025993,54.51187537550696]
[null,null,null,null,"Coincident",49.899474202575909,49.475343270198302,49.188296501415451,49.496101736123265,49.571838072626427,50.274155087224166,50.98668634145583]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",53.519964331217366,53.055693201737398,52.741633040340851,53.078410034198683,53.161296863436185,53.930324805445942,54.711258673759794]
[null,null,null,null,"Coincident",50.209875833581528,49.774318821247931,49.47968256905601,49.795630669106316,49.873391135808028,50.594856442509332,51.327491320956106]
[null,"GLEN WAVERLEY","Substation Rating","MVA","Non-Coincident",103.4,103.4,103.4,103.4,103.4,103.4,103.4]
[null,null,null,null,"Coincident",103.4,103.4,103.4,103.4,103.4,103.4,103.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",72.741455193593723,73.608353084291849,73.952656656596758,74.888383016488774,75.11847144158304,76.692554589843169,78.11920108882174]
[null,null,null,null,"Coincident",71.150693565644985,71.998633519686464,72.335407617777108,73.250670851331947,73.475727539891651,75.015387523743129,76.410835107313943]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",72.747924367604369,73.619532513149409,73.96604311158832,74.908705544380226,75.140705305226675,76.729964730783479,78.173400096056753]
[null,null,null,null,"Coincident",71.210551702749697,72.063740263831349,72.402928097713698,73.325669364795957,73.552766304102434,75.108440111657714,76.521371540312231]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",68.470365818881021,69.286362908102632,69.610450341956181,70.491234565995441,70.707813112506045,72.18947234937265,73.532351831496229]
[null,null,null,null,"Coincident",66.973007396418751,67.771159683737565,68.088159744201306,68.949682355417792,69.161524608980869,70.610781872950042,71.924294316080008]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",68.476455148684437,69.29688592529395,69.623050797471549,70.510363835754873,70.728741491972684,72.224685915401849,73.583368488264028]
[null,null,null,null,"Coincident",67.029350901424095,67.832443618421195,68.151715689696488,69.020277254008789,69.234039962897128,70.698370782437053,72.028340488700081]
[null,"HASTINGS","Substation Rating","MVA","Non-Coincident",79.8,79.8,79.8,79.8,79.8,79.8,79.8]
[null,null,null,null,"Coincident",79.8,79.8,79.8,79.8,79.8,79.8,79.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.513472679420317,50.259481581781415,50.387043758032931,50.910898580419193,50.988799764781575,51.711191812787909,52.444090064310068]
[null,null,null,null,"Coincident",44.290946303633284,44.068243221259209,44.180091589606143,44.639415104274377,44.70771999385267,45.341123830715688,45.98373965937202]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.522205693650115,50.267011842368241,50.395167692498674,50.921678573683899,51.000004256030628,51.726687464861008,52.464574451946504]
[null,null,null,null,"Coincident",44.476113883262414,44.251459582522976,44.364278769788271,44.82778105736385,44.896733351116836,45.536452949840864,46.18603554862112]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",45.300778206420553,45.072997502180179,45.187396009100738,45.657192082554076,45.727054321034771,46.374899741453653,47.032167186730781]
[null,null,null,null,"Coincident",39.720380101105313,39.520658672239378,39.620964944179747,40.032888962847672,40.094145187950978,40.662185459324313,41.238487098901665]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.308610024739764,45.079750683986653,45.194681601119562,45.666859643662974,45.737102574422742,46.388796333006212,47.050537705560515]
[null,null,null,null,"Coincident",39.886439471226907,39.684968178300693,39.786145086334102,40.201816653024551,40.263653473984213,40.83735775759218,41.41990723742795]
[null,"HEATHERTON","Substation Rating","MVA","Non-Coincident",92.8,92.8,92.8,92.8,92.8,92.8,92.8]
[null,null,null,null,"Coincident",92.8,92.8,92.8,92.8,92.8,92.8,92.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",53.79108160420963,55.078763325116398,55.805382192864094,56.205111105574275,56.318911259471982,57.475487902287071,58.580986533332378]
[null,null,null,null,"Coincident",47.223262189978783,48.353719687953031,48.991619359804019,49.342541904710622,49.442447211399056,50.457807386684848,51.428326107402107]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",53.794914177533251,55.078909805632421,55.808202443927513,56.210801645827331,56.325596566495093,57.496617832353429,58.622997443418612]
[null,null,null,null,"Coincident",47.105819774104603,48.230157782124657,48.868766990956843,49.221305251047824,49.321826070285724,50.347237441314633,51.333558095734823]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",51.037949560743272,52.259725229905271,52.949154332574381,53.328424343075092,53.436399984044193,54.533780787677465,55.582697851400262]
[null,null,null,null,"Coincident",44.806283901851756,45.8788823892125,46.484133116764291,46.817094764169966,46.911886723200141,47.875278792419437,48.796124479817699]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.041585975519574,52.259864213263953,52.951830237710155,53.333823630424355,53.442743124067931,54.553829246879005,55.622558561503823]
[null,null,null,null,"Coincident",44.694852416949075,45.761644621738341,46.367568570790382,46.702063237938845,46.797439206390592,47.770368031630838,48.706206879070514]
[null,"GARDINER","Substation Rating","MVA","Non-Coincident",73.5,73.5,73.5,73.5,73.5,73.5,73.5]
[null,null,null,null,"Coincident",73.5,73.5,73.5,73.5,73.5,73.5,73.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.778191261276184,46.509020847244955,47.513648807333055,48.740993159891715,49.32345529191749,50.269888220735048,51.234746916883523]
[null,null,null,null,"Coincident",44.967529791548401,45.685417507819864,46.672255049452886,47.877865018251633,48.450012640354686,49.379685695356017,50.327458225643653]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.27355846368971,46.979765957316005,47.952231927315168,49.142776552270959,49.708680982266081,50.629387951949489,51.569450958538795]
[null,null,null,null,"Coincident",45.312402037865517,46.003940768314742,46.956207472318546,48.122023080217986,48.676173007266918,49.5777558064825,50.498292594871579]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.825363330101503,43.509052259025509,44.448878761929421,45.597055795169588,46.141947407152728,47.027332629405258,47.929955102821317]
[null,null,null,null,"Coincident",42.066991908638784,42.738573756512018,43.661757375257729,44.789601956392879,45.324844374669532,46.19455078424356,47.081189199732719]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.288777891504687,43.949432925434991,44.859171981171826,45.972922977436284,46.5023249078519,47.363643570972663,48.2430697497092]
[null,null,null,null,"Coincident",42.389618881091756,43.0365513301983,43.927394031985386,45.018011105500683,45.53641673297016,46.379844790846228,47.241004249866499]
[null,"KEYSBOROUGH","Substation Rating","MVA","Non-Coincident",46.7,46.7,93.4,93.4,93.4,93.4,93.4]
[null,null,null,null,"Coincident",46.7,46.7,93.4,93.4,93.4,93.4,93.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.344573691058045,37.572425060480782,38.485067357848735,39.35128673579387,40.081727247304038,41.038480524673425,42.002664736212218]
[null,null,null,null,"Coincident",32.447578315213853,33.543775062696653,34.358560583895631,35.131900817377193,35.784020880836962,36.638187644757998,37.498988571469511]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",37.183835960313623,38.511054749178648,39.499200576800369,40.438276212579133,41.230996467556793,42.270416756184417,43.319078700214021]
[null,null,null,null,"Coincident",33.178650185662121,34.36291014105214,35.244619730726384,36.082544630423016,36.789878539250076,37.717339659427765,38.6530469877709]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.27730964829108,34.401537726179129,35.237158487225862,36.030274144827381,36.699069857986629,37.575078896878495,38.457891743662934]
[null,null,null,null,"Coincident",29.709197309919325,30.712881626359927,31.458904136249856,32.166979092137403,32.764064133334436,33.546144345249878,34.334298836404706]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.045743215501048,35.26095269858704,36.165704944766915,37.02552822899667,37.751347648797818,38.70304709899353,39.66320826430217]
[null,null,null,null,"Coincident",30.378571099108875,31.462886616868847,32.27018520523216,33.037394268853078,33.685033438013704,34.534222402101001,35.390961643841244]
[null,"LYNDALE","Substation Rating","MVA","Non-Coincident",101.1,101.1,101.1,101.1,101.1,101.1,101.1]
[null,null,null,null,"Coincident",101.1,101.1,101.1,101.1,101.1,101.1,101.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.385263291848105,58.037925572253926,57.734743104286224,58.096029373907264,58.48344080364906,59.312014387877383,60.152638440722789]
[null,null,null,null,"Coincident",55.377805779708282,55.048359619989775,54.760794250231953,55.103470462377132,55.470926113058006,56.256819409320649,57.054142447833414]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",58.538781868719767,58.199888861938355,57.904306757713513,58.2565605935797,58.634622615262522,59.444337709185646,60.267360318382494]
[null,null,null,null,"Coincident",55.33144125283664,55.011116198280924,54.7317290413704,55.064682885012495,55.422030883636459,56.187381677088531,56.965310866880323]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.582408886304037,54.257694594312952,53.97425955436028,54.312013874228469,54.674191723109502,55.448797156344831,56.234668165313572]
[null,null,null,null,"Coincident",51.770838527954346,51.462850450451086,51.194015307665076,51.514371713928462,51.857893579588129,52.592598654449063,53.33798900894714]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.725928213990663,54.409108598527276,54.132778881700823,54.462089084600969,54.815526487952646,55.572501756129519,56.341917770463517]
[null,null,null,null,"Coincident",51.727493899175712,51.428032834542151,51.166843226475393,51.478110519098472,51.812183082548216,52.527683665988945,53.25494336694392]
[null,"LANGWARRIN","Substation Rating","MVA","Non-Coincident",90.8,90.8,90.8,90.8,90.8,90.8,90.8]
[null,null,null,null,"Coincident",90.8,90.8,90.8,90.8,90.8,90.8,90.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.180121525208548,46.794874753459403,46.649719869140689,46.964326515993818,47.12997986767634,47.797701462147444,48.475134153221546]
[null,null,null,null,"Coincident",38.50208315677208,38.187696445541619,38.069240510160775,38.325980232044287,38.461164265393386,39.006069016055434,39.558898660441045]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.766758427394286,47.366722209244031,47.216017220386242,47.542668616671122,47.714687033364477,48.408222135900395,49.112092595833403]
[null,null,null,null,"Coincident",39.119521135019532,38.791903649430907,38.668480851006429,38.93599840131651,39.076876248358964,39.644860386172518,40.221308867086677]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.124455853743704,43.764159957435766,43.628406167957834,43.922637014585646,44.077561668593475,44.702037635703682,45.335595750962263]
[null,null,null,null,"Coincident",36.008458935834611,35.714433780488619,35.60364975699828,35.843761485368852,35.970190195571647,36.479803669166373,36.99682877316701]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.673098656175682,44.298971166100472,44.158026729909452,44.463522236258129,44.624399715756809,45.273017354406107,45.931300971150797]
[null,null,null,null,"Coincident",36.585907953193498,36.279508927238339,36.164079724337356,36.414271244773602,36.546025003383022,37.077223105558105,37.616337349561576]
[null,"MENTONE","Substation Rating","MVA","Non-Coincident",81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994]
[null,null,null,null,"Coincident",81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994,81.599999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.072259685350588,41.7758055968905,41.68538181162905,42.114714999808321,42.17915672582474,43.045356487002138,43.873302180132036]
[null,null,null,null,"Coincident",39.594385743497675,39.315391517337467,39.230293301534346,39.634340623745913,39.694987011103123,40.5101713565954,41.289354633025575]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.266081827175192,41.979442873224095,41.892075827894672,42.307157148942395,42.369516383774915,43.20911618722392,44.013964973389101]
[null,null,null,null,"Coincident",39.630874083632328,39.36210650924609,39.280186628745525,39.669388439222629,39.727859697422161,40.515112091130824,41.269780125686331]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",37.812276002484403,37.545839069960408,37.464571052718966,37.850432547439532,37.908349292307356,38.686842881381928,39.430955778997379]
[null,null,null,null,"Coincident",35.585296655774144,35.33455170502593,35.258070022146725,35.621205945431782,35.675711644779867,36.408355331978619,37.108643201592542]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",37.986472881303733,37.72885726186896,37.650336477479811,38.023389163318726,38.07943427752047,38.834021260417892,39.557375904792721]
[null,null,null,null,"Coincident",35.618090406296758,35.376536618142389,35.302911451470955,35.652705030149384,35.705255840821032,36.412795797485003,37.091050691001008]
[null,"MORDIALLOC","Substation Rating","MVA","Non-Coincident",83.1,83.1,83.1,83.1,83.1,83.1,83.1]
[null,null,null,null,"Coincident",83.1,83.1,83.1,83.1,83.1,83.1,83.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.623242254837784,63.383451076577003,63.347848315500393,64.000291270311081,64.098221156219864,65.41455529296708,66.672756031510701]
[null,null,null,null,"Coincident",53.602996838326554,53.400971205638939,53.370975647069614,53.920663094682304,54.00316966270222,55.112189763998252,56.172232097898736]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",64.15252809559864,63.901991840687714,63.864799907741578,64.54661808072639,64.649002703348728,66.026332979146602,67.344699541928222]
[null,null,null,null,"Coincident",53.896306178467718,53.685823768743134,53.654577801281853,54.227392031680886,54.313408173719708,55.470541282217866,56.578137351031359]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",62.205092382290346,61.970646103422254,61.935836921064578,62.57373704749341,62.669484095019584,63.956477396215213,65.186633081508361]
[null,null,null,null,"Coincident",52.40819631511598,52.210673795050319,52.181346831731005,52.718781851517861,52.799449363954082,53.883749619804227,54.92016381330447]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.722580543130874,62.47762869331121,62.441265761420318,63.107886338041745,63.207988827054152,64.55461867505467,65.843599099898029]
[null,null,null,null,"Coincident",52.694967846296194,52.489177049132458,52.458627548295674,53.018673859314234,53.102772718037308,54.234113551382869,55.31702151616151]
[null,"MULGRAVE","Substation Rating","MVA","Non-Coincident",111.6,111.6,111.6,111.6,111.6,111.6,111.6]
[null,null,null,null,"Coincident",111.6,111.6,111.6,111.6,111.6,111.6,111.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",84.348089457841013,83.920492717597114,83.981809028261324,84.927775899941778,85.057727924210567,86.689840558685091,88.35372821571535]
[null,null,null,null,"Coincident",83.364118864082911,82.941510293945669,83.002111313404114,83.937042919314052,84.065478975985926,85.678552046572918,87.323029465192818]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",84.424947108504057,83.991714527662836,84.053827519782843,85.012569181619938,85.144346179151967,86.800774319495034,88.492006565245859]
[null,null,null,null,"Coincident",83.43504968121988,83.006896828964557,83.068281535273243,84.015781781663989,84.146013670607871,85.783019898225305,87.454422146962841]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",79.545143480809401,79.141894939280448,79.199719778714851,80.091821437680409,80.214373738301859,81.753550671894502,83.322693295813366]
[null,null,null,null,"Coincident",78.617202106387325,78.21865769875626,78.275807977071864,79.157502739986697,79.278625395185415,80.799846915075392,82.35068455770454]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",79.617624705800807,79.209061239513872,79.267637395796314,80.171786423261594,80.296059779582194,81.858167646353692,83.453097804373002]
[null,null,null,null,"Coincident",78.684093983401212,78.280320995971664,78.338210336468137,79.231758056774538,79.354574286026491,80.898366161951458,82.474595481957891]
[null,"MOORABBIN","Substation Rating","MVA","Non-Coincident",79.8,79.8,79.8,79.8,79.8,79.8,79.8]
[null,null,null,null,"Coincident",79.8,79.8,79.8,79.8,79.8,79.8,79.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",50.329488009954062,50.383279845780955,50.506922716722208,51.027112222316354,51.094374456949559,52.143658946912367,53.146603779351288]
[null,null,null,null,"Coincident",46.87090115087684,46.920996471124639,47.036142740459859,47.520585397448635,47.583225445566278,48.560404263647406,49.494427834316951]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.360650442073364,50.415034693704222,50.540057999362688,51.06633741332687,51.134419913418519,52.197442692758578,53.215107613222543]
[null,null,null,null,"Coincident",46.94389906102429,46.994593577410747,47.11113459484374,47.601708236569181,47.665171634759417,48.65607293597094,49.604693712010281]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",48.943601053713635,48.995911662399692,49.116149868424905,49.622015289290964,49.687425372088107,50.707816468823125,51.68314392989457]
[null,null,null,null,"Coincident",45.580250816436973,45.628966697837974,45.740942267071901,46.212045174623242,46.272960348734465,47.223231295676015,48.131535330252603]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.973905388325761,49.026792099887359,49.148372728590644,49.660160364394741,49.726368125589651,50.760119210296487,51.749761422903468]
[null,null,null,null,"Coincident",45.651238635572049,45.700537213478086,45.813869124633356,46.290934192398964,46.352650044583307,47.31626560849508,48.23876489568336]
[null,"MORNINGTON","Substation Rating","MVA","Non-Coincident",92.9,92.9,92.9,92.9,92.9,139.35000000000002,139.35000000000002]
[null,null,null,null,"Coincident",92.9,92.9,92.9,92.9,92.9,139.35000000000002,139.35000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",66.904804360281375,66.726446423885534,67.133002624430944,68.707851440375975,69.42476441251344,71.395786465289802,73.343387648755836]
[null,null,null,null,"Coincident",61.121512730581848,60.958572161750432,61.329985399184324,62.768703333911148,63.42364591646853,65.224291634559108,67.003540997404329]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",66.925107286865128,66.745881461276397,67.154440204949466,68.737839988834807,69.459047250536628,71.443093120909566,73.405205641467134]
[null,null,null,null,"Coincident",61.129621219588415,60.965915739311093,61.339094689023248,62.785377451233863,63.444130623487673,65.256364887353996,67.048565154703226]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",64.419041870793791,64.247310595550829,64.638761720117799,66.155099041249855,66.845376028252829,68.743167275983254,70.618407826866445]
[null,null,null,null,"Coincident",58.850621049496318,58.693734329232122,59.051348182562883,60.436612391368342,61.06722141940665,62.800966447394572,64.514110074367835]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",64.438590468091164,64.266023548968946,64.659402814733298,66.18397340352152,66.878385131248976,68.788716313279991,70.677929051073207]
[null,null,null,null,"Coincident",58.858428277957969,58.700805065554945,59.060119028381173,60.45266700317449,61.08694504331968,62.831848059477316,64.557461416651364]
[null,"NORTH BRIGHTON","Substation Rating","MVA","Non-Coincident",90.8,90.8,90.8,90.8,90.8,90.8,90.8]
[null,null,null,null,"Coincident",90.8,90.8,90.8,90.8,90.8,90.8,90.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",49.762192974376923,49.496096492289013,49.517590670287873,50.027590678672098,50.096251688911678,51.125038526232444,52.108390945945253]
[null,null,null,null,"Coincident",44.160734865913149,43.924591410573733,43.943666106422789,44.396258201057087,44.45719041661232,45.370172342064379,46.242834153995616]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",50.735305321854469,50.453212176827996,50.475996305853691,51.016715909131435,51.089528960800315,52.180975696045429,53.224972482084603]
[null,null,null,null,"Coincident",44.953824436154498,44.703876877236389,44.724064668157411,45.203167217373057,45.26768294504275,46.234755176230998,47.159784560282006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.232043487642933,46.979476631910579,46.99987794240942,47.48394709481002,47.549117048698733,48.525595409788437,49.458949457819834]
[null,null,null,null,"Coincident",41.915390479416388,41.69125369433425,41.709358540805148,42.138938674199544,42.196772802538405,43.063334331058414,43.891625814763017]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",48.155678118015594,47.887927946709503,47.909553620914089,48.422780436094563,48.491891321634981,49.527843649742536,50.518758612524664]
[null,null,null,null,"Coincident",42.668155557324496,42.430916535753866,42.450077882183919,42.904820551005727,42.966055988449185,43.88395761112676,44.76195404744422]
[null,"NOTTING HILL","Substation Rating","MVA","Non-Coincident",111,111,111,111,111,111,111]
[null,null,null,null,"Coincident",111,111,111,111,111,111,111]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.173149129198478,59.095367927585308,60.383703860854737,61.715959266039462,63.451756996719404,65.211023456227352,66.424088776664036]
[null,null,null,null,"Coincident",53.738487061947929,54.590403172855545,55.780526535915705,57.011221296753313,58.614695499003155,60.239849359297352,61.360440147373922]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",61.275580497148795,62.099192279924509,63.255100712117709,64.456621314797403,66.030989065854882,67.636258245108166,68.748424211264165]
[null,null,null,null,"Coincident",55.457104268923146,56.202509276006381,57.24865741412885,58.336086579278373,59.760958866405666,61.213798309643259,62.220357585770081]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",56.222009876145258,57.113297268473254,58.358422152518962,59.64599344045957,61.323572162225823,63.023832466882112,64.196211329758029]
[null,null,null,null,"Coincident",51.936087276552229,52.759429947837233,53.909636331252969,55.099053339513283,56.648746690904943,58.219392560200951,59.302398505339582]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.220385065041768,60.016372741116953,61.133511769405644,62.294733126706099,63.816296263198062,65.367724387699411,66.442588081158135]
[null,null,null,null,"Coincident",53.597061712872986,54.317465684418117,55.328525801222263,56.379482371011235,57.756564151837637,59.160675064670436,60.133474137961855]
[null,"NOBLE PARK","Substation Rating","MVA","Non-Coincident",108,108,108,108,108,108,108]
[null,null,null,null,"Coincident",108,108,108,108,108,108,108]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",63.494087236102843,63.020936318881738,62.658889390272506,63.451715194439281,63.493971664072674,64.824467198586404,66.030341741058123]
[null,null,null,null,"Coincident",61.009525433651611,60.554889196251807,60.207009381600329,60.968811435449922,61.00941438402446,62.287846828457177,63.446534775181284]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",63.497324251733772,63.022433720588474,62.659498431146005,63.454770030679001,63.497208175791023,64.835991003437314,66.053506330084488]
[null,null,null,null,"Coincident",61.403675514610882,60.944443185957113,60.593474684396703,61.362524401359792,61.403563265951469,62.698203430746787,63.87557455516022]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",59.107812584135345,58.667347700608133,58.33031156174183,59.068367671916292,59.107704996008692,60.346287738455779,61.468858509358526]
[null,null,null,null,"Coincident",56.79488834558537,56.371659117732094,56.047811405585897,56.756986936493405,56.794784967446788,57.98490122261898,59.063545124432927]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",59.110825981470022,58.668741659373389,58.330878529082788,59.071211475107937,59.110717924241889,60.357015460154507,61.490422850958829]
[null,null,null,null,"Coincident",57.161809898906249,56.734302085246256,56.407579057698399,57.123501571382313,57.161705404566504,58.366909724459532,59.462946139709103]
[null,"NUNAWADING","Substation Rating","MVA","Non-Coincident",133,133,133,133,133,133,133]
[null,null,null,null,"Coincident",133,133,133,133,133,133,133]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",66.457200201244987,66.41537270974105,66.452312188743335,67.287883998330116,67.378341166838609,68.83608102063036,70.151072199926602]
[null,null,null,null,"Coincident",61.726226062594044,61.687376198495272,61.72168601932168,62.497774904407123,62.581792582182132,63.935758435138979,65.157137646989014]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",67.054505559357082,67.014396703960216,67.049818202016695,67.851798567637729,67.938703670738207,69.341401765032657,70.610157633151246]
[null,null,null,null,"Coincident",61.954082510384723,61.917024488467689,61.949751691433789,62.69073035243386,62.771025119849519,64.067028613517081,65.239278040803853]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",61.598069733263308,61.559300529465602,61.593539116053705,62.368016681136432,62.451859920947719,63.803014662569524,65.021858040196477]
[null,null,null,null,"Coincident",57.213008761443632,57.17699947079285,57.208800671105251,57.92814450620422,58.006019089526113,59.260987441703712,60.393063449035836]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.151702101007139,62.114525872334006,62.14735746771769,62.890699684010862,62.97125057367743,64.271388027037176,65.447376666374879]
[null,null,null,null,"Coincident",57.424205100104935,57.389856638067563,57.420190936298248,58.106991690662369,58.181415570505457,59.382659579216977,60.46919800918586]
[null,"OAKLEIGH","Substation Rating","MVA","Non-Coincident",87.2,87.2,87.2,87.2,87.2,87.2,87.2]
[null,null,null,null,"Coincident",87.2,87.2,87.2,87.2,87.2,87.2,87.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",45.132909641531711,45.010051497929268,45.116610593390675,45.679418028601049,45.90303000517688,47.081768929604713,48.236663806207396]
[null,null,null,null,"Coincident",43.971220778425895,43.851524915702271,43.955341256144266,44.503662429893765,44.721518793882055,45.869917820175843,46.995086527407594]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",45.187187450399357,45.06263040596437,45.170661721118044,45.74152248770514,45.968461198818112,47.165880044772791,48.340841163267292]
[null,null,null,null,"Coincident",44.041744455856467,43.920344788590079,44.025637634719324,44.58202774042131,44.803213817402757,45.970279479058497,47.115456690698494]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.676539435994705,42.560367878430029,42.661127467737295,43.193303963655566,43.404745800942251,44.519331556494684,45.611370982652318]
[null,null,null,null,"Coincident",41.578075787795299,41.46489440315996,41.563060512594582,42.081539165554688,42.287538640947986,43.373435755119097,44.437366866312864]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.727863161166368,42.61008516588354,42.712236848947988,43.252028371613257,43.466615885054992,44.598864902604788,45.709878460282638]
[null,null,null,null,"Coincident",41.644761195958473,41.529968736780454,41.629530992700865,42.15563942391838,42.364787391819512,43.468335204926028,44.551185852533827]
[null,"OAKLEIGH EAST","Substation Rating","MVA","Non-Coincident",64.8,64.8,64.8,64.8,64.8,64.8,64.8]
[null,null,null,null,"Coincident",64.8,64.8,64.8,64.8,64.8,64.8,64.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.652139281517671,15.684589847809566,15.718542730136763,15.917430172950029,15.928030586235685,16.261797289013487,16.564301701515387]
[null,null,null,null,"Coincident",15.068142204350545,15.099382007338711,15.132068073438182,15.323534825494795,15.333739726686913,15.655053257705113,15.946270925976474]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.540351569223517,16.567597402317546,16.596132090046829,16.763838325518766,16.772803218631658,17.056402851420494,17.315594236908499]
[null,null,null,null,"Coincident",15.351405577397623,15.376692937969738,15.40317650831728,15.558827760820199,15.567148243583702,15.830362297186001,16.070922605964295]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.916584411589852,14.947509999625508,14.979867304025966,15.169408252759567,15.179510511417586,15.49759221936929,15.785880773592114]
[null,null,null,null,"Coincident",14.360031627270358,14.389803350476569,14.420953371268379,14.603422356350682,14.613147689565926,14.919361448708647,15.196893666687666]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.763056151118796,15.789021596602089,15.81621532843112,15.97604039596812,15.984583993904106,16.254856177501768,16.501867152222275]
[null,null,null,null,"Coincident",14.629983353278682,14.654082362477103,14.679321366903539,14.827657961982977,14.835587432916929,15.086432034939582,15.315687479670178]
[null,"ORMOND","Substation Rating","MVA","Non-Coincident",64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994]
[null,null,null,null,"Coincident",64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994,64.599999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",38.642823133089223,38.486299839953134,38.429100655738843,39.040008540163328,39.231118975715219,40.238530621097226,41.225563901979427]
[null,null,null,null,"Coincident",34.641885770309685,34.501568329667776,34.450291340952901,34.997948044903524,35.169271601029365,36.072379508616997,36.957218953448773]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",39.349453958415836,39.204020831716939,39.15090780493739,39.719090092098853,39.897242533569816,40.839428081726801,41.767330585588844]
[null,null,null,null,"Coincident",34.782023762114406,34.653471572445255,34.606523562404853,35.108754923331681,35.266228581265281,36.099051322819697,36.919248903511978]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",36.115867033412705,35.969579211141912,35.916120432408583,36.487079439403225,36.665692659646432,37.607227001151969,38.529715573146859]
[null,null,null,null,"Coincident",32.376561514623418,32.245419801419949,32.197495950206438,32.709339938201751,32.869460195239441,33.713511495397412,34.540488955750178]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.776289405797648,36.640366534737709,36.590726708829919,37.121754058027193,37.288256641590607,38.16883019235955,39.036054704762122]
[null,null,null,null,"Coincident",32.507535513622344,32.387389690607421,32.34351173473803,32.812900862669302,32.960076902877532,33.738439169340047,34.505001867499757]
[null,"ROSEBUD","Substation Rating","MVA","Non-Coincident",91.6,91.6,91.6,91.6,91.6,91.6,91.6]
[null,null,null,null,"Coincident",91.6,91.6,91.6,91.6,91.6,91.6,91.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.953686158417419,46.869102499989708,47.094991536352573,48.199775901099208,48.862028263610988,50.249258541825654,51.620004915660033]
[null,null,null,null,"Coincident",38.394352650408862,38.325188010189173,38.50989903144351,39.413288817702835,39.954817136992958,41.089164892553583,42.21003364593966]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.954265127428911,46.869559725514279,47.095805297476076,48.203742478246262,48.868960516026831,50.264851850772601,51.647195511604387]
[null,null,null,null,"Coincident",38.476846221295055,38.407434066409074,38.592831837133375,39.500735057674824,40.045850439075238,41.189718756104355,42.322485381637939]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",40.15244518345046,40.080113467108198,40.273282478791351,41.218038839247406,41.784363953609017,42.970653939764908,44.142847714926724]
[null,null,null,null,"Coincident",32.8329310492961,32.773784906527155,32.931740538182375,33.704274322850182,34.167362270455008,35.137399764858479,36.095910690418869]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.152940288806377,40.080504463520064,40.273978366624171,41.221430857733999,41.790292069331088,42.983988558065342,44.166099753317866]
[null,null,null,null,"Coincident",32.903475427256531,32.844117622318251,33.002660527789516,33.77905397582839,34.245209399632365,35.223388402269912,36.192073793315096]
[null,"SURREY HILLS","Substation Rating","MVA","Non-Coincident",21.6,21.6,21.6,21.6,21.6,21.6,21.6]
[null,null,null,null,"Coincident",21.6,21.6,21.6,21.6,21.6,21.6,21.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0143070754481247,7.9933580580673382,8.0121574255316101,8.1024059636726609,8.1920361914977473,8.30809818607338,8.4258481434924981]
[null,null,null,null,"Coincident",7.120101469813445,7.1014898633401877,7.11819166957918,7.1983706224215487,7.2780002536384716,7.3811124965794788,7.4857243659522847]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.1977612788210852,8.1763327208812893,8.1955624216169962,8.2878768244066539,8.3795587632391904,8.4982775141078264,8.6187228667036155]
[null,null,null,null,"Coincident",7.3176937287503652,7.2985656255135307,7.315730929026695,7.3981349541490715,7.4799744132423482,7.5859481576792476,7.6934631451703304]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3994403373691373,7.380098552386813,7.3974556110348777,7.4807801788637383,7.5635338738460884,7.6706914604238943,7.7794075074193616]
[null,null,null,null,"Coincident",6.5738392010581883,6.5566554981647274,6.5720759228662375,6.6461034554132938,6.7196238109136948,6.8148251655051189,6.9114110934858548]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.5688197259698544,7.5490351913246663,7.5667895675869925,7.6520215045830851,7.7366695009749309,7.8462800144865241,7.9574846628804217]
[null,null,null,null,"Coincident",6.7562719575479919,6.7386113841090731,6.7544597460476368,6.8305416408030855,6.9061022836761818,7.0039456021198534,7.1032119177007012]
[null,"SANDRINGHAM","Substation Rating","MVA","Non-Coincident",73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994]
[null,null,null,null,"Coincident",73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994,73.099999999999994]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.176939902829361,35.241041495274196,35.34544787302459,35.709483733161932,35.824437721812721,36.560135678048766,37.263342930706209]
[null,null,null,null,"Coincident",30.298459162036625,30.353670885576999,30.443597763277694,30.757147653414698,30.856159356543799,31.489827735435927,32.095511353338566]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.188769272560023,35.252386036580404,35.356026288924795,35.717615731587784,35.831868625188157,36.563864626068806,37.264749957936708]
[null,null,null,null,"Coincident",30.440149642828036,30.495181513979126,30.584835822885115,30.897629846986188,30.996464652812531,31.629679973080467,32.235982916478918]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.616206295499126,32.675641561011879,32.772447592596187,33.109983169766842,33.216568990440322,33.898711222767979,34.550727938392569]
[null,null,null,null,"Coincident",28.092858480429033,28.144051022187845,28.227431600563854,28.518156374489315,28.609960441126383,29.197500421180699,29.759092813409442]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.627174536754531,32.686160267317575,32.782255944210448,33.117523192832664,33.223458955233298,33.902168719020437,34.552032539945181]
[null,null,null,null,"Coincident",28.224234488813131,28.275260270681866,28.358388122127604,28.648412053892613,28.740052100608224,29.327172002804961,29.889338636232377]
[null,"SPRINGVALE","Substation Rating","MVA","Non-Coincident",80,80,80,80,80,80,80]
[null,null,null,null,"Coincident",80,80,80,80,80,80,80]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",56.697722509315469,56.599046249688918,56.857950028727927,57.379597277426441,57.457834206561643,58.661844442984091,59.753080944959891]
[null,null,null,null,"Coincident",51.637471075579107,51.547601636793893,51.783398346252341,52.258488764776637,52.329743075998699,53.426295829907829,54.420139864791828]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",57.135846341590678,57.032462098170889,57.303756076807993,57.850731337924991,57.932808264451445,59.197228047257525,60.345260668036225]
[null,null,null,null,"Coincident",51.011668189486691,50.919365317313911,51.161580306784856,51.649927330842978,51.72320673790643,52.852098082704373,53.877077371043718]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",54.291483538420756,54.196995077719933,54.444911036873698,54.944419690169688,55.019336261105011,56.172248565829058,57.217173228787246]
[null,null,null,null,"Coincident",49.445988071299837,49.359932671885637,49.585722220449497,50.040649905284376,50.108880199087068,51.158895493406625,52.110561004323699]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",54.711013490860225,54.612016852170981,54.871797173555656,55.395558923950091,55.474152523625335,56.684910606766877,57.784220973639833]
[null,null,null,null,"Coincident",48.846744123132424,48.758358564712616,48.990294002885811,49.45791568580848,49.528085130826959,50.609066573294839,51.590545964304852]
[null,"SPRINGVALE WEST","Substation Rating","MVA","Non-Coincident",80,80,80,80,80,80,80]
[null,null,null,null,"Coincident",80,80,80,80,80,80,80]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",58.703528192111293,60.119831076913641,61.119231346704026,62.501894521087088,63.369969315319544,64.697866420927951,65.901385916587373]
[null,null,null,null,"Coincident",37.895225613058813,38.809499746299473,39.454648340733492,40.347206838557398,40.907580144720434,41.764785187716825,42.541700038021467]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",59.223973786347017,60.727379161654923,61.791017931083687,63.266099064373613,64.19418550955919,65.616678193906438,66.908694704613907]
[null,null,null,null,"Coincident",39.242021333958327,40.238183226509697,40.942954159850395,41.920348306192309,42.535301774413078,43.477850622417314,44.333945481231012]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",55.955425938698049,57.305427099070755,58.258042205889595,59.575978439622702,60.403415841663765,61.669149783649686,62.816328634378451]
[null,null,null,null,"Coincident",36.121227386580074,36.992701386963745,37.607648486517448,38.458423430699639,38.992563847752848,39.809640346812557,40.550185297102921]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",56.451507789316565,57.884533890551594,58.898380284818188,60.304408093526064,61.189047806804311,62.544949002160891,63.776482036084772]
[null,null,null,null,"Coincident",37.404975238476226,38.354503566981393,39.026281890683443,39.957921051954528,40.544086556933436,41.44251164112103,42.258529927314726]
[null,"SPRINGVALE SOUTH","Substation Rating","MVA","Non-Coincident",80.2,80.2,80.2,80.2,80.2,80.2,80.2]
[null,null,null,null,"Coincident",80.2,80.2,80.2,80.2,80.2,80.2,80.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",7.9454901314010611,7.9454901314010611,7.9454901314010611,7.9454901314010611,7.9454901314010611,7.9454901314010611,7.9454901314010611]
[null,null,null,null,"Coincident",7.3603980905927795,7.3603980905927795,7.3603980905927795,7.3603980905927795,7.3603980905927795,7.3603980905927795,7.3603980905927795]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",46.488501555413983,46.00163480728142,45.660571556557308,46.238316864769907,46.269109854786137,47.238664009839113,48.117404781827787]
[null,null,null,null,"Coincident",42.693516628573384,42.246394159321071,41.933172844824014,42.463755206009672,42.492034479105506,43.38244124757739,44.189447980551662]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",40.45766931065338,40.041363495947991,39.751722667420353,40.243330817245102,40.269664999720774,41.10544466421004,41.873590685733376]
[null,null,null,null,"Coincident",37.134640148819294,36.752528008294313,36.486677104793365,36.937906551497107,36.962077750839768,37.72920985739286,38.43426347459431]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.270668873955223,41.827974822577389,41.517855733898031,42.043183068611661,42.071182256390678,42.952770203353424,43.751784130582294]
[null,null,null,null,"Coincident",38.819997291587384,38.413441579712241,38.128638369748849,38.611081781552656,38.636795318213011,39.446416803395515,40.180205014399604]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",36.787005079182748,36.408470072569607,36.145107926115479,36.59211319885393,36.61605812007641,37.376008737265032,38.074462011435529]
[null,null,null,null,"Coincident",33.765469416413531,33.418025742721518,33.176295096739416,33.586585166103255,33.608563348438992,34.306094698638191,34.947179848599021]
[null,"SORRENTO","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",72,72,72,72,72,72,72]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,null,null,"Coincident",0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.247650587799363,47.106818006205728,47.156776771384955,48.26301053360271,48.766597497837409,50.151118423770583,51.519187639476556]
[null,null,null,null,"Coincident",38.685988429825464,38.570675868157466,38.611581694958318,39.517356818026329,39.9296896902311,41.063324058398663,42.183487901289688]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.256349432651525,47.121304958723982,47.169204540665071,48.231475379626382,48.716050700614424,50.05134588622299,51.374890175248844]
[null,null,null,null,"Coincident",38.771419095274219,38.660622007517624,38.699921166005801,39.571460089018764,39.96902936973585,41.064570812921481,42.150471246134423]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.022341467510095,42.89410339980315,42.939594403654056,43.946898810728854,44.405450507254621,45.666155141313013,46.911879324781502]
[null,null,null,null,"Coincident",35.226340009081419,35.121339731991341,35.158587392493885,35.983359971714378,36.358818336428364,37.391072941257413,38.411061676122898]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",43.030262383554529,42.907294798958659,42.950910770224596,43.918183813353927,44.359424058464853,45.57530515986312,46.780486235354459]
[null,null,null,null,"Coincident",35.304130697401526,35.203242080004308,35.239026754899882,36.032624842457956,36.394639908587394,37.392208199797032,38.380997666705852]
[null,"WEST DONCASTER","Substation Rating","MVA","Non-Coincident",94.9,94.9,94.9,94.9,94.9,94.9,94.9]
[null,null,null,null,"Coincident",94.9,94.9,94.9,94.9,94.9,94.9,94.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.413098285545708,54.04570445816654,53.932845932776679,54.512732546636286,54.705010761307328,55.610599723441346,56.459606773195432]
[null,null,null,null,"Coincident",49.972140710409342,49.634731950085097,49.531084440774826,50.063643261663969,50.24022857479325,51.071907351915492,51.851622183292974]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",55.082386449527242,54.701187223470328,54.584100856302001,55.185775658110622,55.385313467067569,56.325321260562774,57.20692575215385]
[null,null,null,null,"Coincident",50.340274625965257,49.991893320001068,49.884887065222848,50.434762927742405,50.617122276140648,51.476203618203712,52.281909671968208]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",50.50338654386605,50.162390844988721,50.057641475588284,50.595861844104682,50.774324407448105,51.614844628599748,52.402848483612502]
[null,null,null,null,"Coincident",46.381522431937682,46.068357301062044,45.972157114122936,46.466450305213925,46.630347539665408,47.402268200035003,48.125958648911777]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",51.124584746501256,50.770775599983885,50.662102169386571,51.220545192240806,51.405745730592542,52.278211707442566,53.096470799839437]
[null,null,null,null,"Coincident",46.723205041879524,46.399855769110033,46.300538170628208,46.810904132335331,46.980160523759942,47.777514808993857,48.525328948531843]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,"VOLUMES"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"BOX HILL",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"BEAUMARIS",null,"MWh","Non-Coincident",0,0,0,0,0,5.7736485161088275E-4,2.3987530323926545E-3]
[null,"BENTLEIGH",null,"MWh","Non-Coincident",6.6958581279353661E-3,8.7288485794550404E-3,1.0911924014978484E-2,1.534511687107637E-2,1.6069998247439987E-2,3.2737720263206226E-2,6.0409126493522876E-2]
[null,"BULLEEN",null,"MWh","Non-Coincident",1.8793781577280157E-2,1.3712224469928518E-2,1.1930997225998335E-2,1.8923977792274987E-2,2.0384916144776194E-2,3.637157463065515E-2,5.8146140667343582E-2]
[null,"BURWOOD",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"CLARINDA",null,"MWh","Non-Coincident",0.31231879399143742,0.38356959020016435,0.4509776994014566,0.51557271786118675,0.52906269812891937,0.61797538550858289,0.73645341720659041]
[null,"CAULFIELD",null,"MWh","Non-Coincident",0.90286737303698417,1.0549291831315073,1.121177754941012,1.2295655448821883,1.2594202096494274,1.4178526429154297,1.5436253879583368]
[null,"CHELTENHAM",null,"MWh","Non-Coincident",0,0,0,0,0,8.9514001805430926E-3,4.1778072299223867E-2]
[null,"CARRUM",null,"MWh","Non-Coincident",0.70048889141215853,0.68154401418606636,0.7273600417454531,0.88643916542770207,0.97390602871163523,1.2526415980384842,1.6250089035800652]
[null,"DONCASTER",null,"MWh","Non-Coincident",4.1838944845298451,4.6521384719867145,5.6304489900406818,7.692862069868144,8.7504431873351969,11.171904090796778,18.805075250169562]
[null,"DROMANA",null,"MWh","Non-Coincident",1.0926310671192568E-2,1.3185516013181568E-2,1.7144336669110707E-2,2.7714672945524609E-2,3.6968202002570866E-2,5.3496695691103865E-2,7.2218674820240344E-2]
[null,"DANDENONG",null,"MWh","Non-Coincident",4.6744363848799278E-2,3.9624979178413296E-2,3.6423745387403332E-2,5.1412747634376893E-2,5.6642029946630763E-2,8.4859634870554257E-2,0.11528343237882194]
[null,"DANDENONG SOUTH",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"DANDENONG VALLEY",null,"MWh","Non-Coincident",0,7.6441378761521787E-4,9.562281346175221E-3,4.3828928428116545E-2,5.7623297171097737E-2,0.19307116308486119,0.51574853986709202]
[null,"EAST BURWOOD",null,"MWh","Non-Coincident",0,0,0,1.0825190668514045E-3,7.0641293071936687E-3,1.282867187774123E-2,3.0025378411814237E-2]
[null,"ELSTERNWICK",null,"MWh","Non-Coincident",2.1507997708735009E-2,2.8095894337887378E-2,3.5904375852425473E-2,5.0497268804032165E-2,5.4987400591962485E-2,8.3483974124764632E-2,0.11968040694180304]
[null,"EAST MALVERN",null,"MWh","Non-Coincident",1.8408292638437713,2.2982078094989893,3.2664732544363151,5.2044063851573332,9.0811846769395448,15.489519979045118,25.918803445751387]
[null,"ELWOOD",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"FRANKSTON SOUTH",null,"MWh","Non-Coincident",0.69278438726738778,0.64791009375767339,0.6347359142432184,0.69013189764444749,0.72298808331068698,0.82741657034986693,0.96352011746257393]
[null,"FRANKSTON",null,"MWh","Non-Coincident",0.51049685605473849,0.46673448420719144,0.4426594397639208,0.47844753084589392,0.48996422619334606,0.55456497041898845,0.64007327081721643]
[null,"GLEN WAVERLEY",null,"MWh","Non-Coincident",3.6274771841597012E-2,7.3079239826686446E-2,9.1672203318869702E-2,0.14863364817519373,0.16432240582641303,0.2671832578863842,0.38096582109414451]
[null,"HASTINGS",null,"MWh","Non-Coincident",0.45849504536489399,0.43532284880845568,0.45089373116797382,0.50713945733754451,0.51866185339822257,0.58366537787603012,0.66984408524218275]
[null,"HEATHERTON",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"GARDINER",null,"MWh","Non-Coincident",0.60830256988624953,0.70261166272998821,0.85448393565346192,1.06154877948115,1.168943624529722,1.3185502670037919,1.5015829681891295]
[null,"KEYSBOROUGH",null,"MWh","Non-Coincident",5.5248061552622465,6.1386668725916484,6.8095985582787399,7.564589545208289,8.2732332736965972,9.237571966940191,10.764085759430515]
[null,"LYNDALE",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"LANGWARRIN",null,"MWh","Non-Coincident",1.4117868759955526E-2,1.0257751969549877E-2,9.0233403263142373E-3,1.2107946689219289E-2,1.382573268903175E-2,2.1459516609912559E-2,3.0202591072787891E-2]
[null,"MENTONE",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"MORDIALLOC",null,"MWh","Non-Coincident",0.47453449893053973,0.44167440491590759,0.44076085837612716,0.5442307333754044,0.56523740609813766,0.79959201169338923,1.1370892348778596]
[null,"MULGRAVE",null,"MWh","Non-Coincident",0.72758523787753204,0.67288341993240808,0.68357781983796562,0.81167069380094881,0.83153061094290115,1.0548745048698782,1.3129621259302526]
[null,"MOORABBIN",null,"MWh","Non-Coincident",0.33804814922992682,0.34221987011372113,0.35471603789834383,0.39964024755535421,0.40773023674922509,0.48735153787363739,0.58138576727614533]
[null,"MORNINGTON",null,"MWh","Non-Coincident",5.0816950058520867,5.3450631969747491,5.6832384837247503,6.3396758425412969,7.3071991390366087,9.0216749385843489,12.08377673610835]
[null,"NORTH BRIGHTON",null,"MWh","Non-Coincident",7.0860397870900579E-2,6.1559142752508511E-2,6.3214038399473413E-2,8.4365837741025088E-2,8.8213630467463222E-2,0.13726579901669039,0.20300103438763947]
[null,"NOTTING HILL",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"NOBLE PARK",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"NUNAWADING",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"OAKLEIGH",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"OAKLEIGH EAST",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"ORMOND",null,"MWh","Non-Coincident",0.12033908989993192,0.11458823901088443,0.11366569447986367,0.13980073860464773,0.1494005149275737,0.19165725648622683,0.24458344874801624]
[null,"ROSEBUD",null,"MWh","Non-Coincident",6.8399984994443113E-3,6.0582514773281308E-3,8.1925631363162239E-3,2.029735014222709E-2,3.3757042847038371E-2,7.8707344345034722E-2,0.16312564872017382]
[null,"SURREY HILLS",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,"SANDRINGHAM",null,"MWh","Non-Coincident",0,0,0,0,0,7.9642310448384455E-5,1.3980054888087356E-3]
[null,"SPRINGVALE SOUTH",null,"MWh","Non-Coincident",0.24886365877931582,0.21331534462314239,0.19313615963419034,0.23483245303427366,0.23915605562506326,0.31473555529985997,0.401633597798709]
[null,"SORRENTO",null,"MWh","Non-Coincident",0.12538793829705994,0.12316238327390237,0.12439380839378249,0.14447005756339532,0.15550136361084604,0.18435212006747889,0.21933860278556797]
[null,"SPRINGVALE",null,"MWh","Non-Coincident",0,0,0,2.5158328019116443E-3,7.5640430877508E-3,6.6586995961728443E-2,0.23719368927656956]
[null,"SPRINGVALE WEST",null,"MWh","Non-Coincident",0,0,0,2.5158328019116443E-3,7.5640430877508E-3,6.6586995961728443E-2,0.23719368927656956]
[null,"WEST DONCASTER",null,"MWh","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]
[null,null,null,"MWh","Non-Coincident"]

{"sheet":"6.1 Telephone answering","index":32,"n_rows":1833,"n_cols":4,"rows_kept":1833,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"6.1 TELEPHONE ANSWERING"]
[]
[null,"6.1.1 - TELEPHONE ANSWERING DATA"]
["C10 starts at first day of PRCP_y5 and goes for 5 full years","Date","Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) "]
[null,"2015-01-01"]
[null,{"$f":"B8+1","v":"2015-01-02"}]
[null,"2015-01-03"]
[null,"2015-01-04"]
[null,"2015-01-05"]
[null,"2015-01-06"]
[null,"2015-01-07"]
[null,"2015-01-08"]
[null,"2015-01-09"]
[null,"2015-01-10"]
[null,"2015-01-11"]
[null,"2015-01-12"]
[null,"2015-01-13"]
[null,"2015-01-14"]
[null,"2015-01-15"]
[null,"2015-01-16"]
[null,"2015-01-17"]
[null,"2015-01-18"]
[null,"2015-01-19"]
[null,"2015-01-20"]
[null,"2015-01-21"]
[null,"2015-01-22"]
[null,"2015-01-23"]
[null,"2015-01-24"]
[null,"2015-01-25"]
[null,"2015-01-26"]
[null,"2015-01-27"]
[null,"2015-01-28"]
[null,"2015-01-29"]
[null,"2015-01-30"]
[null,"2015-01-31"]
[null,"2015-02-01"]
[null,"2015-02-02"]
[null,"2015-02-03"]
[null,"2015-02-04"]
[null,"2015-02-05"]
[null,"2015-02-06"]
[null,"2015-02-07"]
[null,"2015-02-08"]
[null,"2015-02-09"]
[null,"2015-02-10"]
[null,"2015-02-11"]
[null,"2015-02-12"]
[null,"2015-02-13"]
[null,"2015-02-14"]
[null,"2015-02-15"]
[null,"2015-02-16"]
[null,"2015-02-17"]
[null,"2015-02-18"]
[null,"2015-02-19"]
[null,"2015-02-20"]
[null,"2015-02-21"]
[null,"2015-02-22"]
[null,"2015-02-23"]
[null,"2015-02-24"]
[null,"2015-02-25"]
[null,"2015-02-26"]
[null,"2015-02-27"]
[null,"2015-02-28"]
[null,"2015-03-01"]
[null,"2015-03-02"]
[null,"2015-03-03"]
[null,"2015-03-04"]
[null,"2015-03-05"]
[null,"2015-03-06"]
[null,{"$f":"B72+1","v":"2015-03-07"}]
[null,"2015-03-08"]
[null,"2015-03-09"]
[null,"2015-03-10"]
[null,"2015-03-11"]
[null,"2015-03-12"]
[null,"2015-03-13"]
[null,"2015-03-14"]
[null,"2015-03-15"]
[null,"2015-03-16"]
[null,"2015-03-17"]
[null,"2015-03-18"]
[null,"2015-03-19"]
[null,"2015-03-20"]
[null,"2015-03-21"]
[null,"2015-03-22"]
[null,"2015-03-23"]
[null,"2015-03-24"]
[null,"2015-03-25"]
[null,"2015-03-26"]
[null,"2015-03-27"]
[null,"2015-03-28"]
[null,"2015-03-29"]
[null,"2015-03-30"]
[null,"2015-03-31"]
[null,"2015-04-01"]
[null,"2015-04-02"]
[null,"2015-04-03"]
[null,"2015-04-04"]
[null,"2015-04-05"]
[null,"2015-04-06"]
[null,"2015-04-07"]
[null,"2015-04-08"]
[null,"2015-04-09"]
[null,"2015-04-10"]
[null,"2015-04-11"]
[null,"2015-04-12"]
[null,"2015-04-13"]
[null,"2015-04-14"]
[null,"2015-04-15"]
[null,"2015-04-16"]
[null,"2015-04-17"]
[null,"2015-04-18"]
[null,"2015-04-19"]
[null,"2015-04-20"]
[null,"2015-04-21"]
[null,"2015-04-22"]
[null,"2015-04-23"]
[null,"2015-04-24"]
[null,"2015-04-25"]
[null,"2015-04-26"]
[null,"2015-04-27"]
[null,"2015-04-28"]
[null,"2015-04-29"]
[null,"2015-04-30"]
[null,"2015-05-01"]
[null,"2015-05-02"]
[null,"2015-05-03"]
[null,"2015-05-04"]
[null,"2015-05-05"]
[null,"2015-05-06"]
[null,"2015-05-07"]
[null,"2015-05-08"]
[null,"2015-05-09"]
[null,{"$f":"B136+1","v":"2015-05-10"}]
[null,"2015-05-11"]
[null,"2015-05-12"]
[null,"2015-05-13"]
[null,"2015-05-14"]
[null,"2015-05-15"]
[null,"2015-05-16"]
[null,"2015-05-17"]
[null,"2015-05-18"]
[null,"2015-05-19"]
[null,"2015-05-20"]
[null,"2015-05-21"]
[null,"2015-05-22"]
[null,"2015-05-23"]
[null,"2015-05-24"]
[null,"2015-05-25"]
[null,"2015-05-26"]
[null,"2015-05-27"]
[null,"2015-05-28"]
[null,"2015-05-29"]
[null,"2015-05-30"]
[null,"2015-05-31"]
[null,"2015-06-01"]
[null,"2015-06-02"]
[null,"2015-06-03"]
[null,"2015-06-04"]
[null,"2015-06-05"]
[null,"2015-06-06"]
[null,"2015-06-07"]
[null,"2015-06-08"]
[null,"2015-06-09"]
[null,"2015-06-10"]
[null,"2015-06-11"]
[null,"2015-06-12"]
[null,"2015-06-13"]
[null,"2015-06-14"]
[null,"2015-06-15"]
[null,"2015-06-16"]
[null,"2015-06-17"]
[null,"2015-06-18"]
[null,"2015-06-19"]
[null,"2015-06-20"]
[null,"2015-06-21"]
[null,"2015-06-22"]
[null,"2015-06-23"]
[null,"2015-06-24"]
[null,"2015-06-25"]
[null,"2015-06-26"]
[null,"2015-06-27"]
[null,"2015-06-28"]
[null,"2015-06-29"]
[null,"2015-06-30"]
[null,"2015-07-01"]
[null,"2015-07-02"]
[null,"2015-07-03"]
[null,"2015-07-04"]
[null,"2015-07-05"]
[null,"2015-07-06"]
[null,"2015-07-07"]
[null,"2015-07-08"]
[null,"2015-07-09"]
[null,"2015-07-10"]
[null,"2015-07-11"]
[null,"2015-07-12"]
[null,{"$f":"B200+1","v":"2015-07-13"}]
[null,"2015-07-14"]
[null,"2015-07-15"]
[null,"2015-07-16"]
[null,"2015-07-17"]
[null,"2015-07-18"]
[null,"2015-07-19"]
[null,"2015-07-20"]
[null,"2015-07-21"]
[null,"2015-07-22"]
[null,"2015-07-23"]
[null,"2015-07-24"]
[null,"2015-07-25"]
[null,"2015-07-26"]
[null,"2015-07-27"]
[null,"2015-07-28"]
[null,"2015-07-29"]
[null,"2015-07-30"]
[null,"2015-07-31"]
[null,"2015-08-01"]
[null,"2015-08-02"]
[null,"2015-08-03"]
[null,"2015-08-04"]
[null,"2015-08-05"]
[null,"2015-08-06"]
[null,"2015-08-07"]
[null,"2015-08-08"]
[null,"2015-08-09"]
[null,"2015-08-10"]
[null,"2015-08-11"]
[null,"2015-08-12"]
[null,"2015-08-13"]
[null,"2015-08-14"]
[null,"2015-08-15"]
[null,"2015-08-16"]
[null,"2015-08-17"]
[null,"2015-08-18"]
[null,"2015-08-19"]
[null,"2015-08-20"]
[null,"2015-08-21"]
[null,"2015-08-22"]
[null,"2015-08-23"]
[null,"2015-08-24"]
[null,"2015-08-25"]
[null,"2015-08-26"]
[null,"2015-08-27"]
[null,"2015-08-28"]
[null,"2015-08-29"]
[null,"2015-08-30"]
[null,"2015-08-31"]
[null,"2015-09-01"]
[null,"2015-09-02"]
[null,"2015-09-03"]
[null,"2015-09-04"]
[null,"2015-09-05"]
[null,"2015-09-06"]
[null,"2015-09-07"]
[null,"2015-09-08"]
[null,"2015-09-09"]
[null,"2015-09-10"]
[null,"2015-09-11"]
[null,"2015-09-12"]
[null,"2015-09-13"]
[null,"2015-09-14"]
[null,{"$f":"B264+1","v":"2015-09-15"}]
[null,"2015-09-16"]
[null,"2015-09-17"]
[null,"2015-09-18"]
[null,"2015-09-19"]
[null,"2015-09-20"]
[null,"2015-09-21"]
[null,"2015-09-22"]
[null,"2015-09-23"]
[null,"2015-09-24"]
[null,"2015-09-25"]
[null,"2015-09-26"]
[null,"2015-09-27"]
[null,"2015-09-28"]
[null,"2015-09-29"]
[null,"2015-09-30"]
[null,"2015-10-01"]
[null,"2015-10-02"]
[null,"2015-10-03"]
[null,"2015-10-04"]
[null,"2015-10-05"]
[null,"2015-10-06"]
[null,"2015-10-07"]
[null,"2015-10-08"]
[null,"2015-10-09"]
[null,"2015-10-10"]
[null,"2015-10-11"]
[null,"2015-10-12"]
[null,"2015-10-13"]
[null,"2015-10-14"]
[null,"2015-10-15"]
[null,"2015-10-16"]
[null,"2015-10-17"]
[null,"2015-10-18"]
[null,"2015-10-19"]
[null,"2015-10-20"]
[null,"2015-10-21"]
[null,"2015-10-22"]
[null,"2015-10-23"]
[null,"2015-10-24"]
[null,"2015-10-25"]
[null,"2015-10-26"]
[null,"2015-10-27"]
[null,"2015-10-28"]
[null,"2015-10-29"]
[null,"2015-10-30"]
[null,"2015-10-31"]
[null,"2015-11-01"]
[null,"2015-11-02"]
[null,"2015-11-03"]
[null,"2015-11-04"]
[null,"2015-11-05"]
[null,"2015-11-06"]
[null,"2015-11-07"]
[null,"2015-11-08"]
[null,"2015-11-09"]
[null,"2015-11-10"]
[null,"2015-11-11"]
[null,"2015-11-12"]
[null,"2015-11-13"]
[null,"2015-11-14"]
[null,"2015-11-15"]
[null,"2015-11-16"]
[null,"2015-11-17"]
[null,{"$f":"B328+1","v":"2015-11-18"}]
[null,"2015-11-19"]
[null,"2015-11-20"]
[null,"2015-11-21"]
[null,"2015-11-22"]
[null,"2015-11-23"]
[null,"2015-11-24"]
[null,"2015-11-25"]
[null,"2015-11-26"]
[null,"2015-11-27"]
[null,"2015-11-28"]
[null,"2015-11-29"]
[null,"2015-11-30"]
[null,"2015-12-01"]
[null,"2015-12-02"]
[null,"2015-12-03"]
[null,"2015-12-04"]
[null,"2015-12-05"]
[null,"2015-12-06"]
[null,"2015-12-07"]
[null,"2015-12-08"]
[null,"2015-12-09"]
[null,"2015-12-10"]
[null,"2015-12-11"]
[null,"2015-12-12"]
[null,"2015-12-13"]
[null,"2015-12-14"]
[null,"2015-12-15"]
[null,"2015-12-16"]
[null,"2015-12-17"]
[null,"2015-12-18"]
[null,"2015-12-19"]
[null,"2015-12-20"]
[null,"2015-12-21"]
[null,"2015-12-22"]
[null,"2015-12-23"]
[null,"2015-12-24"]
[null,"2015-12-25"]
[null,"2015-12-26"]
[null,"2015-12-27"]
[null,"2015-12-28"]
[null,"2015-12-29"]
[null,"2015-12-30"]
[null,"2015-12-31"]
[null,"2016-01-01"]
[null,"2016-01-02"]
[null,"2016-01-03"]
[null,"2016-01-04"]
[null,"2016-01-05"]
[null,"2016-01-06"]
[null,"2016-01-07"]
[null,"2016-01-08"]
[null,"2016-01-09"]
[null,"2016-01-10"]
[null,"2016-01-11"]
[null,"2016-01-12"]
[null,"2016-01-13"]
[null,"2016-01-14"]
[null,"2016-01-15"]
[null,"2016-01-16"]
[null,"2016-01-17"]
[null,"2016-01-18"]
[null,"2016-01-19"]
[null,"2016-01-20"]
[null,{"$f":"B392+1","v":"2016-01-21"}]
[null,"2016-01-22"]
[null,"2016-01-23"]
[null,"2016-01-24"]
[null,"2016-01-25"]
[null,"2016-01-26"]
[null,"2016-01-27"]
[null,"2016-01-28"]
[null,"2016-01-29"]
[null,"2016-01-30"]
[null,"2016-01-31"]
[null,"2016-02-01"]
[null,"2016-02-02"]
[null,"2016-02-03"]
[null,"2016-02-04"]
[null,"2016-02-05"]
[null,"2016-02-06"]
[null,"2016-02-07"]
[null,"2016-02-08"]
[null,"2016-02-09"]
[null,"2016-02-10"]
[null,"2016-02-11"]
[null,"2016-02-12"]
[null,"2016-02-13"]
[null,"2016-02-14"]
[null,"2016-02-15"]
[null,"2016-02-16"]
[null,"2016-02-17"]
[null,"2016-02-18"]
[null,"2016-02-19"]
[null,"2016-02-20"]
[null,"2016-02-21"]
[null,"2016-02-22"]
[null,"2016-02-23"]
[null,"2016-02-24"]
[null,"2016-02-25"]
[null,"2016-02-26"]
[null,"2016-02-27"]
[null,"2016-02-28"]
[null,"2016-02-29"]
[null,"2016-03-01"]
[null,"2016-03-02"]
[null,"2016-03-03"]
[null,"2016-03-04"]
[null,"2016-03-05"]
[null,"2016-03-06"]
[null,"2016-03-07"]
[null,"2016-03-08"]
[null,"2016-03-09"]
[null,"2016-03-10"]
[null,"2016-03-11"]
[null,"2016-03-12"]
[null,"2016-03-13"]
[null,"2016-03-14"]
[null,"2016-03-15"]
[null,"2016-03-16"]
[null,"2016-03-17"]
[null,"2016-03-18"]
[null,"2016-03-19"]
[null,"2016-03-20"]
[null,"2016-03-21"]
[null,"2016-03-22"]
[null,"2016-03-23"]
[null,"2016-03-24"]
[null,{"$f":"B456+1","v":"2016-03-25"}]
[null,"2016-03-26"]
[null,"2016-03-27"]
[null,"2016-03-28"]
[null,"2016-03-29"]
[null,"2016-03-30"]
[null,"2016-03-31"]
[null,"2016-04-01"]
[null,"2016-04-02"]
[null,"2016-04-03"]
[null,"2016-04-04"]
[null,"2016-04-05"]
[null,"2016-04-06"]
[null,"2016-04-07"]
[null,"2016-04-08"]
[null,"2016-04-09"]
[null,"2016-04-10"]
[null,"2016-04-11"]
[null,"2016-04-12"]
[null,"2016-04-13"]
[null,"2016-04-14"]
[null,"2016-04-15"]
[null,"2016-04-16"]
[null,"2016-04-17"]
[null,"2016-04-18"]
[null,"2016-04-19"]
[null,"2016-04-20"]
[null,"2016-04-21"]
[null,"2016-04-22"]
[null,"2016-04-23"]
[null,"2016-04-24"]
[null,"2016-04-25"]
[null,"2016-04-26"]
[null,"2016-04-27"]
[null,"2016-04-28"]
[null,"2016-04-29"]
[null,"2016-04-30"]
[null,"2016-05-01"]
[null,"2016-05-02"]
[null,"2016-05-03"]
[null,"2016-05-04"]
[null,"2016-05-05"]
[null,"2016-05-06"]
[null,"2016-05-07"]
[null,"2016-05-08"]
[null,"2016-05-09"]
[null,"2016-05-10"]
[null,"2016-05-11"]
[null,"2016-05-12"]
[null,"2016-05-13"]
[null,"2016-05-14"]
[null,"2016-05-15"]
[null,"2016-05-16"]
[null,"2016-05-17"]
[null,"2016-05-18"]
[null,"2016-05-19"]
[null,"2016-05-20"]
[null,"2016-05-21"]
[null,"2016-05-22"]
[null,"2016-05-23"]
[null,"2016-05-24"]
[null,"2016-05-25"]
[null,"2016-05-26"]
[null,"2016-05-27"]
[null,{"$f":"B520+1","v":"2016-05-28"}]
[null,"2016-05-29"]
[null,"2016-05-30"]
[null,"2016-05-31"]
[null,"2016-06-01"]
[null,"2016-06-02"]
[null,"2016-06-03"]
[null,"2016-06-04"]
[null,"2016-06-05"]
[null,"2016-06-06"]
[null,"2016-06-07"]
[null,"2016-06-08"]
[null,"2016-06-09"]
[null,"2016-06-10"]
[null,"2016-06-11"]
[null,"2016-06-12"]
[null,"2016-06-13"]
[null,"2016-06-14"]
[null,"2016-06-15"]
[null,"2016-06-16"]
[null,"2016-06-17"]
[null,"2016-06-18"]
[null,"2016-06-19"]
[null,"2016-06-20"]
[null,"2016-06-21"]
[null,"2016-06-22"]
[null,"2016-06-23"]
[null,"2016-06-24"]
[null,"2016-06-25"]
[null,"2016-06-26"]
[null,"2016-06-27"]
[null,"2016-06-28"]
[null,"2016-06-29"]
[null,"2016-06-30"]
[null,"2016-07-01"]
[null,"2016-07-02"]
[null,"2016-07-03"]
[null,"2016-07-04"]
[null,"2016-07-05"]
[null,"2016-07-06"]
[null,"2016-07-07"]
[null,"2016-07-08"]
[null,"2016-07-09"]
[null,"2016-07-10"]
[null,"2016-07-11"]
[null,"2016-07-12"]
[null,"2016-07-13"]
[null,"2016-07-14"]
[null,"2016-07-15"]
[null,"2016-07-16"]
[null,"2016-07-17"]
[null,"2016-07-18"]
[null,"2016-07-19"]
[null,"2016-07-20"]
[null,"2016-07-21"]
[null,"2016-07-22"]
[null,"2016-07-23"]
[null,"2016-07-24"]
[null,"2016-07-25"]
[null,"2016-07-26"]
[null,"2016-07-27"]
[null,"2016-07-28"]
[null,"2016-07-29"]
[null,"2016-07-30"]
[null,{"$f":"B584+1","v":"2016-07-31"}]
[null,"2016-08-01"]
[null,"2016-08-02"]
[null,"2016-08-03"]
[null,"2016-08-04"]
[null,"2016-08-05"]
[null,"2016-08-06"]
[null,"2016-08-07"]
[null,"2016-08-08"]
[null,"2016-08-09"]
[null,"2016-08-10"]
[null,"2016-08-11"]
[null,"2016-08-12"]
[null,"2016-08-13"]
[null,"2016-08-14"]
[null,"2016-08-15"]
[null,"2016-08-16"]
[null,"2016-08-17"]
[null,"2016-08-18"]
[null,"2016-08-19"]
[null,"2016-08-20"]
[null,"2016-08-21"]
[null,"2016-08-22"]
[null,"2016-08-23"]
[null,"2016-08-24"]
[null,"2016-08-25"]
[null,"2016-08-26"]
[null,"2016-08-27"]
[null,"2016-08-28"]
[null,"2016-08-29"]
[null,"2016-08-30"]
[null,"2016-08-31"]
[null,"2016-09-01"]
[null,"2016-09-02"]
[null,"2016-09-03"]
[null,"2016-09-04"]
[null,"2016-09-05"]
[null,"2016-09-06"]
[null,"2016-09-07"]
[null,"2016-09-08"]
[null,"2016-09-09"]
[null,"2016-09-10"]
[null,"2016-09-11"]
[null,"2016-09-12"]
[null,"2016-09-13"]
[null,"2016-09-14"]
[null,"2016-09-15"]
[null,"2016-09-16"]
[null,"2016-09-17"]
[null,"2016-09-18"]
[null,"2016-09-19"]
[null,"2016-09-20"]
[null,"2016-09-21"]
[null,"2016-09-22"]
[null,"2016-09-23"]
[null,"2016-09-24"]
[null,"2016-09-25"]
[null,"2016-09-26"]
[null,"2016-09-27"]
[null,"2016-09-28"]
[null,"2016-09-29"]
[null,"2016-09-30"]
[null,"2016-10-01"]
[null,"2016-10-02"]
[null,{"$f":"B648+1","v":"2016-10-03"}]
[null,"2016-10-04"]
[null,"2016-10-05"]
[null,"2016-10-06"]
[null,"2016-10-07"]
[null,"2016-10-08"]
[null,"2016-10-09"]
[null,"2016-10-10"]
[null,"2016-10-11"]
[null,"2016-10-12"]
[null,"2016-10-13"]
[null,"2016-10-14"]
[null,"2016-10-15"]
[null,"2016-10-16"]
[null,"2016-10-17"]
[null,"2016-10-18"]
[null,"2016-10-19"]
[null,"2016-10-20"]
[null,"2016-10-21"]
[null,"2016-10-22"]
[null,"2016-10-23"]
[null,"2016-10-24"]
[null,"2016-10-25"]
[null,"2016-10-26"]
[null,"2016-10-27"]
[null,"2016-10-28"]
[null,"2016-10-29"]
[null,"2016-10-30"]
[null,"2016-10-31"]
[null,"2016-11-01"]
[null,"2016-11-02"]
[null,"2016-11-03"]
[null,"2016-11-04"]
[null,"2016-11-05"]
[null,"2016-11-06"]
[null,"2016-11-07"]
[null,"2016-11-08"]
[null,"2016-11-09"]
[null,"2016-11-10"]
[null,"2016-11-11"]
[null,"2016-11-12"]
[null,"2016-11-13"]
[null,"2016-11-14"]
[null,"2016-11-15"]
[null,"2016-11-16"]
[null,"2016-11-17"]
[null,"2016-11-18"]
[null,"2016-11-19"]
[null,"2016-11-20"]
[null,"2016-11-21"]
[null,"2016-11-22"]
[null,"2016-11-23"]
[null,"2016-11-24"]
[null,"2016-11-25"]
[null,"2016-11-26"]
[null,"2016-11-27"]
[null,"2016-11-28"]
[null,"2016-11-29"]
[null,"2016-11-30"]
[null,"2016-12-01"]
[null,"2016-12-02"]
[null,"2016-12-03"]
[null,"2016-12-04"]
[null,"2016-12-05"]
[null,{"$f":"B712+1","v":"2016-12-06"}]
[null,"2016-12-07"]
[null,"2016-12-08"]
[null,"2016-12-09"]
[null,"2016-12-10"]
[null,"2016-12-11"]
[null,"2016-12-12"]
[null,"2016-12-13"]
[null,"2016-12-14"]
[null,"2016-12-15"]
[null,"2016-12-16"]
[null,"2016-12-17"]
[null,"2016-12-18"]
[null,"2016-12-19"]
[null,"2016-12-20"]
[null,"2016-12-21"]
[null,"2016-12-22"]
[null,"2016-12-23"]
[null,"2016-12-24"]
[null,"2016-12-25"]
[null,"2016-12-26"]
[null,"2016-12-27"]
[null,"2016-12-28"]
[null,"2016-12-29"]
[null,"2016-12-30"]
[null,"2016-12-31"]
[null,"2017-01-01"]
[null,"2017-01-02"]
[null,"2017-01-03"]
[null,"2017-01-04"]
[null,"2017-01-05"]
[null,"2017-01-06"]
[null,"2017-01-07"]
[null,"2017-01-08"]
[null,"2017-01-09"]
[null,"2017-01-10"]
[null,"2017-01-11"]
[null,"2017-01-12"]
[null,"2017-01-13"]
[null,"2017-01-14"]
[null,"2017-01-15"]
[null,"2017-01-16"]
[null,"2017-01-17"]
[null,"2017-01-18"]
[null,"2017-01-19"]
[null,"2017-01-20"]
[null,"2017-01-21"]
[null,"2017-01-22"]
[null,"2017-01-23"]
[null,"2017-01-24"]
[null,"2017-01-25"]
[null,"2017-01-26"]
[null,"2017-01-27"]
[null,"2017-01-28"]
[null,"2017-01-29"]
[null,"2017-01-30"]
[null,"2017-01-31"]
[null,"2017-02-01"]
[null,"2017-02-02"]
[null,"2017-02-03"]
[null,"2017-02-04"]
[null,"2017-02-05"]
[null,"2017-02-06"]
[null,"2017-02-07"]
[null,{"$f":"B776+1","v":"2017-02-08"}]
[null,"2017-02-09"]
[null,"2017-02-10"]
[null,"2017-02-11"]
[null,"2017-02-12"]
[null,"2017-02-13"]
[null,"2017-02-14"]
[null,"2017-02-15"]
[null,"2017-02-16"]
[null,"2017-02-17"]
[null,"2017-02-18"]
[null,"2017-02-19"]
[null,"2017-02-20"]
[null,"2017-02-21"]
[null,"2017-02-22"]
[null,"2017-02-23"]
[null,"2017-02-24"]
[null,"2017-02-25"]
[null,"2017-02-26"]
[null,"2017-02-27"]
[null,"2017-02-28"]
[null,"2017-03-01"]
[null,"2017-03-02"]
[null,"2017-03-03"]
[null,"2017-03-04"]
[null,"2017-03-05"]
[null,"2017-03-06"]
[null,"2017-03-07"]
[null,"2017-03-08"]
[null,"2017-03-09"]
[null,"2017-03-10"]
[null,"2017-03-11"]
[null,"2017-03-12"]
[null,"2017-03-13"]
[null,"2017-03-14"]
[null,"2017-03-15"]
[null,"2017-03-16"]
[null,"2017-03-17"]
[null,"2017-03-18"]
[null,"2017-03-19"]
[null,"2017-03-20"]
[null,"2017-03-21"]
[null,"2017-03-22"]
[null,"2017-03-23"]
[null,"2017-03-24"]
[null,"2017-03-25"]
[null,"2017-03-26"]
[null,"2017-03-27"]
[null,"2017-03-28"]
[null,"2017-03-29"]
[null,"2017-03-30"]
[null,"2017-03-31"]
[null,"2017-04-01"]
[null,"2017-04-02"]
[null,"2017-04-03"]
[null,"2017-04-04"]
[null,"2017-04-05"]
[null,"2017-04-06"]
[null,"2017-04-07"]
[null,"2017-04-08"]
[null,"2017-04-09"]
[null,"2017-04-10"]
[null,"2017-04-11"]
[null,"2017-04-12"]
[null,{"$f":"B840+1","v":"2017-04-13"}]
[null,"2017-04-14"]
[null,"2017-04-15"]
[null,"2017-04-16"]
[null,"2017-04-17"]
[null,"2017-04-18"]
[null,"2017-04-19"]
[null,"2017-04-20"]
[null,"2017-04-21"]
[null,"2017-04-22"]
[null,"2017-04-23"]
[null,"2017-04-24"]
[null,"2017-04-25"]
[null,"2017-04-26"]
[null,"2017-04-27"]
[null,"2017-04-28"]
[null,"2017-04-29"]
[null,"2017-04-30"]
[null,"2017-05-01"]
[null,"2017-05-02"]
[null,"2017-05-03"]
[null,"2017-05-04"]
[null,"2017-05-05"]
[null,"2017-05-06"]
[null,"2017-05-07"]
[null,"2017-05-08"]
[null,"2017-05-09"]
[null,"2017-05-10"]
[null,"2017-05-11"]
[null,"2017-05-12"]
[null,"2017-05-13"]
[null,"2017-05-14"]
[null,"2017-05-15"]
[null,"2017-05-16"]
[null,"2017-05-17"]
[null,"2017-05-18"]
[null,"2017-05-19"]
[null,"2017-05-20"]
[null,"2017-05-21"]
[null,"2017-05-22"]
[null,"2017-05-23"]
[null,"2017-05-24"]
[null,"2017-05-25"]
[null,"2017-05-26"]
[null,"2017-05-27"]
[null,"2017-05-28"]
[null,"2017-05-29"]
[null,"2017-05-30"]
[null,"2017-05-31"]
[null,"2017-06-01"]
[null,"2017-06-02"]
[null,"2017-06-03"]
[null,"2017-06-04"]
[null,"2017-06-05"]
[null,"2017-06-06"]
[null,"2017-06-07"]
[null,"2017-06-08"]
[null,"2017-06-09"]
[null,"2017-06-10"]
[null,"2017-06-11"]
[null,"2017-06-12"]
[null,"2017-06-13"]
[null,"2017-06-14"]
[null,"2017-06-15"]
[null,{"$f":"B904+1","v":"2017-06-16"}]
[null,"2017-06-17"]
[null,"2017-06-18"]
[null,"2017-06-19"]
[null,"2017-06-20"]
[null,"2017-06-21"]
[null,"2017-06-22"]
[null,"2017-06-23"]
[null,"2017-06-24"]
[null,"2017-06-25"]
[null,"2017-06-26"]
[null,"2017-06-27"]
[null,"2017-06-28"]
[null,"2017-06-29"]
[null,"2017-06-30"]
[null,"2017-07-01"]
[null,"2017-07-02"]
[null,"2017-07-03"]
[null,"2017-07-04"]
[null,"2017-07-05"]
[null,"2017-07-06"]
[null,"2017-07-07"]
[null,"2017-07-08"]
[null,"2017-07-09"]
[null,"2017-07-10"]
[null,"2017-07-11"]
[null,"2017-07-12"]
[null,"2017-07-13"]
[null,"2017-07-14"]
[null,"2017-07-15"]
[null,"2017-07-16"]
[null,"2017-07-17"]
[null,"2017-07-18"]
[null,"2017-07-19"]
[null,"2017-07-20"]
[null,"2017-07-21"]
[null,"2017-07-22"]
[null,"2017-07-23"]
[null,"2017-07-24"]
[null,"2017-07-25"]
[null,"2017-07-26"]
[null,"2017-07-27"]
[null,"2017-07-28"]
[null,"2017-07-29"]
[null,"2017-07-30"]
[null,"2017-07-31"]
[null,"2017-08-01"]
[null,"2017-08-02"]
[null,"2017-08-03"]
[null,"2017-08-04"]
[null,"2017-08-05"]
[null,"2017-08-06"]
[null,"2017-08-07"]
[null,"2017-08-08"]
[null,"2017-08-09"]
[null,"2017-08-10"]
[null,"2017-08-11"]
[null,"2017-08-12"]
[null,"2017-08-13"]
[null,"2017-08-14"]
[null,"2017-08-15"]
[null,"2017-08-16"]
[null,"2017-08-17"]
[null,"2017-08-18"]
[null,{"$f":"B968+1","v":"2017-08-19"}]
[null,"2017-08-20"]
[null,"2017-08-21"]
[null,"2017-08-22"]
[null,"2017-08-23"]
[null,"2017-08-24"]
[null,"2017-08-25"]
[null,"2017-08-26"]
[null,"2017-08-27"]
[null,"2017-08-28"]
[null,"2017-08-29"]
[null,"2017-08-30"]
[null,"2017-08-31"]
[null,"2017-09-01"]
[null,"2017-09-02"]
[null,"2017-09-03"]
[null,"2017-09-04"]
[null,"2017-09-05"]
[null,"2017-09-06"]
[null,"2017-09-07"]
[null,"2017-09-08"]
[null,"2017-09-09"]
[null,"2017-09-10"]
[null,"2017-09-11"]
[null,"2017-09-12"]
[null,"2017-09-13"]
[null,"2017-09-14"]
[null,"2017-09-15"]
[null,"2017-09-16"]
[null,"2017-09-17"]
[null,"2017-09-18"]
[null,"2017-09-19"]
[null,"2017-09-20"]
[null,"2017-09-21"]
[null,"2017-09-22"]
[null,"2017-09-23"]
[null,"2017-09-24"]
[null,"2017-09-25"]
[null,"2017-09-26"]
[null,"2017-09-27"]
[null,"2017-09-28"]
[null,"2017-09-29"]
[null,"2017-09-30"]
[null,"2017-10-01"]
[null,"2017-10-02"]
[null,"2017-10-03"]
[null,"2017-10-04"]
[null,"2017-10-05"]
[null,"2017-10-06"]
[null,"2017-10-07"]
[null,"2017-10-08"]
[null,"2017-10-09"]
[null,"2017-10-10"]
[null,"2017-10-11"]
[null,"2017-10-12"]
[null,"2017-10-13"]
[null,"2017-10-14"]
[null,"2017-10-15"]
[null,"2017-10-16"]
[null,"2017-10-17"]
[null,"2017-10-18"]
[null,"2017-10-19"]
[null,"2017-10-20"]
[null,"2017-10-21"]
[null,{"$f":"B1032+1","v":"2017-10-22"}]
[null,"2017-10-23"]
[null,"2017-10-24"]
[null,"2017-10-25"]
[null,"2017-10-26"]
[null,"2017-10-27"]
[null,"2017-10-28"]
[null,"2017-10-29"]
[null,"2017-10-30"]
[null,"2017-10-31"]
[null,"2017-11-01"]
[null,"2017-11-02"]
[null,"2017-11-03"]
[null,"2017-11-04"]
[null,"2017-11-05"]
[null,"2017-11-06"]
[null,"2017-11-07"]
[null,"2017-11-08"]
[null,"2017-11-09"]
[null,"2017-11-10"]
[null,"2017-11-11"]
[null,"2017-11-12"]
[null,"2017-11-13"]
[null,"2017-11-14"]
[null,"2017-11-15"]
[null,"2017-11-16"]
[null,"2017-11-17"]
[null,"2017-11-18"]
[null,"2017-11-19"]
[null,"2017-11-20"]
[null,"2017-11-21"]
[null,"2017-11-22"]
[null,"2017-11-23"]
[null,"2017-11-24"]
[null,"2017-11-25"]
[null,"2017-11-26"]
[null,"2017-11-27"]
[null,"2017-11-28"]
[null,"2017-11-29"]
[null,"2017-11-30"]
[null,"2017-12-01"]
[null,"2017-12-02"]
[null,"2017-12-03"]
[null,"2017-12-04"]
[null,"2017-12-05"]
[null,"2017-12-06"]
[null,"2017-12-07"]
[null,"2017-12-08"]
[null,"2017-12-09"]
[null,"2017-12-10"]
[null,"2017-12-11"]
[null,"2017-12-12"]
[null,"2017-12-13"]
[null,"2017-12-14"]
[null,"2017-12-15"]
[null,"2017-12-16"]
[null,"2017-12-17"]
[null,"2017-12-18"]
[null,"2017-12-19"]
[null,"2017-12-20"]
[null,"2017-12-21"]
[null,"2017-12-22"]
[null,"2017-12-23"]
[null,"2017-12-24"]
[null,{"$f":"B1096+1","v":"2017-12-25"}]
[null,"2017-12-26"]
[null,"2017-12-27"]
[null,"2017-12-28"]
[null,"2017-12-29"]
[null,"2017-12-30"]
[null,"2017-12-31"]
[null,"2018-01-01"]
[null,"2018-01-02"]
[null,"2018-01-03"]
[null,"2018-01-04"]
[null,"2018-01-05"]
[null,"2018-01-06"]
[null,"2018-01-07"]
[null,"2018-01-08"]
[null,"2018-01-09"]
[null,"2018-01-10"]
[null,"2018-01-11"]
[null,"2018-01-12"]
[null,"2018-01-13"]
[null,"2018-01-14"]
[null,"2018-01-15"]
[null,"2018-01-16"]
[null,"2018-01-17"]
[null,"2018-01-18"]
[null,"2018-01-19"]
[null,"2018-01-20"]
[null,"2018-01-21"]
[null,"2018-01-22"]
[null,"2018-01-23"]
[null,"2018-01-24"]
[null,"2018-01-25"]
[null,"2018-01-26"]
[null,"2018-01-27"]
[null,"2018-01-28"]
[null,"2018-01-29"]
[null,"2018-01-30"]
[null,"2018-01-31"]
[null,"2018-02-01"]
[null,"2018-02-02"]
[null,"2018-02-03"]
[null,"2018-02-04"]
[null,"2018-02-05"]
[null,"2018-02-06"]
[null,"2018-02-07"]
[null,"2018-02-08"]
[null,"2018-02-09"]
[null,"2018-02-10"]
[null,"2018-02-11"]
[null,"2018-02-12"]
[null,"2018-02-13"]
[null,"2018-02-14"]
[null,"2018-02-15"]
[null,"2018-02-16"]
[null,"2018-02-17"]
[null,"2018-02-18"]
[null,"2018-02-19"]
[null,"2018-02-20"]
[null,"2018-02-21"]
[null,"2018-02-22"]
[null,"2018-02-23"]
[null,"2018-02-24"]
[null,"2018-02-25"]
[null,"2018-02-26"]
[null,{"$f":"B1160+1","v":"2018-02-27"}]
[null,"2018-02-28"]
[null,"2018-03-01"]
[null,"2018-03-02"]
[null,"2018-03-03"]
[null,"2018-03-04"]
[null,"2018-03-05"]
[null,"2018-03-06"]
[null,"2018-03-07"]
[null,"2018-03-08"]
[null,"2018-03-09"]
[null,"2018-03-10"]
[null,"2018-03-11"]
[null,"2018-03-12"]
[null,"2018-03-13"]
[null,"2018-03-14"]
[null,"2018-03-15"]
[null,"2018-03-16"]
[null,"2018-03-17"]
[null,"2018-03-18"]
[null,"2018-03-19"]
[null,"2018-03-20"]
[null,"2018-03-21"]
[null,"2018-03-22"]
[null,"2018-03-23"]
[null,"2018-03-24"]
[null,"2018-03-25"]
[null,"2018-03-26"]
[null,"2018-03-27"]
[null,"2018-03-28"]
[null,"2018-03-29"]
[null,"2018-03-30"]
[null,"2018-03-31"]
[null,"2018-04-01"]
[null,"2018-04-02"]
[null,"2018-04-03"]
[null,"2018-04-04"]
[null,"2018-04-05"]
[null,"2018-04-06"]
[null,"2018-04-07"]
[null,"2018-04-08"]
[null,"2018-04-09"]
[null,"2018-04-10"]
[null,"2018-04-11"]
[null,"2018-04-12"]
[null,"2018-04-13"]
[null,"2018-04-14"]
[null,"2018-04-15"]
[null,"2018-04-16"]
[null,"2018-04-17"]
[null,"2018-04-18"]
[null,"2018-04-19"]
[null,"2018-04-20"]
[null,"2018-04-21"]
[null,"2018-04-22"]
[null,"2018-04-23"]
[null,"2018-04-24"]
[null,"2018-04-25"]
[null,"2018-04-26"]
[null,"2018-04-27"]
[null,"2018-04-28"]
[null,"2018-04-29"]
[null,"2018-04-30"]
[null,"2018-05-01"]
[null,{"$f":"B1224+1","v":"2018-05-02"}]
[null,"2018-05-03"]
[null,"2018-05-04"]
[null,"2018-05-05"]
[null,"2018-05-06"]
[null,"2018-05-07"]
[null,"2018-05-08"]
[null,"2018-05-09"]
[null,"2018-05-10"]
[null,"2018-05-11"]
[null,"2018-05-12"]
[null,"2018-05-13"]
[null,"2018-05-14"]
[null,"2018-05-15"]
[null,"2018-05-16"]
[null,"2018-05-17"]
[null,"2018-05-18"]
[null,"2018-05-19"]
[null,"2018-05-20"]
[null,"2018-05-21"]
[null,"2018-05-22"]
[null,"2018-05-23"]
[null,"2018-05-24"]
[null,"2018-05-25"]
[null,"2018-05-26"]
[null,"2018-05-27"]
[null,"2018-05-28"]
[null,"2018-05-29"]
[null,"2018-05-30"]
[null,"2018-05-31"]
[null,"2018-06-01"]
[null,"2018-06-02"]
[null,"2018-06-03"]
[null,"2018-06-04"]
[null,"2018-06-05"]
[null,"2018-06-06"]
[null,"2018-06-07"]
[null,"2018-06-08"]
[null,"2018-06-09"]
[null,"2018-06-10"]
[null,"2018-06-11"]
[null,"2018-06-12"]
[null,"2018-06-13"]
[null,"2018-06-14"]
[null,"2018-06-15"]
[null,"2018-06-16"]
[null,"2018-06-17"]
[null,"2018-06-18"]
[null,"2018-06-19"]
[null,"2018-06-20"]
[null,"2018-06-21"]
[null,"2018-06-22"]
[null,"2018-06-23"]
[null,"2018-06-24"]
[null,"2018-06-25"]
[null,"2018-06-26"]
[null,"2018-06-27"]
[null,"2018-06-28"]
[null,"2018-06-29"]
[null,"2018-06-30"]
[null,"2018-07-01"]
[null,"2018-07-02"]
[null,"2018-07-03"]
[null,"2018-07-04"]
[null,{"$f":"B1288+1","v":"2018-07-05"}]
[null,"2018-07-06"]
[null,"2018-07-07"]
[null,"2018-07-08"]
[null,"2018-07-09"]
[null,"2018-07-10"]
[null,"2018-07-11"]
[null,"2018-07-12"]
[null,"2018-07-13"]
[null,"2018-07-14"]
[null,"2018-07-15"]
[null,"2018-07-16"]
[null,"2018-07-17"]
[null,"2018-07-18"]
[null,"2018-07-19"]
[null,"2018-07-20"]
[null,"2018-07-21"]
[null,"2018-07-22"]
[null,"2018-07-23"]
[null,"2018-07-24"]
[null,"2018-07-25"]
[null,"2018-07-26"]
[null,"2018-07-27"]
[null,"2018-07-28"]
[null,"2018-07-29"]
[null,"2018-07-30"]
[null,"2018-07-31"]
[null,"2018-08-01"]
[null,"2018-08-02"]
[null,"2018-08-03"]
[null,"2018-08-04"]
[null,"2018-08-05"]
[null,"2018-08-06"]
[null,"2018-08-07"]
[null,"2018-08-08"]
[null,"2018-08-09"]
[null,"2018-08-10"]
[null,"2018-08-11"]
[null,"2018-08-12"]
[null,"2018-08-13"]
[null,"2018-08-14"]
[null,"2018-08-15"]
[null,"2018-08-16"]
[null,"2018-08-17"]
[null,"2018-08-18"]
[null,"2018-08-19"]
[null,"2018-08-20"]
[null,"2018-08-21"]
[null,"2018-08-22"]
[null,"2018-08-23"]
[null,"2018-08-24"]
[null,"2018-08-25"]
[null,"2018-08-26"]
[null,"2018-08-27"]
[null,"2018-08-28"]
[null,"2018-08-29"]
[null,"2018-08-30"]
[null,"2018-08-31"]
[null,"2018-09-01"]
[null,"2018-09-02"]
[null,"2018-09-03"]
[null,"2018-09-04"]
[null,"2018-09-05"]
[null,"2018-09-06"]
[null,{"$f":"B1352+1","v":"2018-09-07"}]
[null,"2018-09-08"]
[null,"2018-09-09"]
[null,"2018-09-10"]
[null,"2018-09-11"]
[null,"2018-09-12"]
[null,"2018-09-13"]
[null,"2018-09-14"]
[null,"2018-09-15"]
[null,"2018-09-16"]
[null,"2018-09-17"]
[null,"2018-09-18"]
[null,"2018-09-19"]
[null,"2018-09-20"]
[null,"2018-09-21"]
[null,"2018-09-22"]
[null,"2018-09-23"]
[null,"2018-09-24"]
[null,"2018-09-25"]
[null,"2018-09-26"]
[null,"2018-09-27"]
[null,"2018-09-28"]
[null,"2018-09-29"]
[null,"2018-09-30"]
[null,"2018-10-01"]
[null,"2018-10-02"]
[null,"2018-10-03"]
[null,"2018-10-04"]
[null,"2018-10-05"]
[null,"2018-10-06"]
[null,"2018-10-07"]
[null,"2018-10-08"]
[null,"2018-10-09"]
[null,"2018-10-10"]
[null,"2018-10-11"]
[null,"2018-10-12"]
[null,"2018-10-13"]
[null,"2018-10-14"]
[null,"2018-10-15"]
[null,"2018-10-16"]
[null,"2018-10-17"]
[null,"2018-10-18"]
[null,"2018-10-19"]
[null,"2018-10-20"]
[null,"2018-10-21"]
[null,"2018-10-22"]
[null,"2018-10-23"]
[null,"2018-10-24"]
[null,"2018-10-25"]
[null,"2018-10-26"]
[null,"2018-10-27"]
[null,"2018-10-28"]
[null,"2018-10-29"]
[null,"2018-10-30"]
[null,"2018-10-31"]
[null,"2018-11-01"]
[null,"2018-11-02"]
[null,"2018-11-03"]
[null,"2018-11-04"]
[null,"2018-11-05"]
[null,"2018-11-06"]
[null,"2018-11-07"]
[null,"2018-11-08"]
[null,"2018-11-09"]
[null,{"$f":"B1416+1","v":"2018-11-10"}]
[null,"2018-11-11"]
[null,"2018-11-12"]
[null,"2018-11-13"]
[null,"2018-11-14"]
[null,"2018-11-15"]
[null,"2018-11-16"]
[null,"2018-11-17"]
[null,"2018-11-18"]
[null,"2018-11-19"]
[null,"2018-11-20"]
[null,"2018-11-21"]
[null,"2018-11-22"]
[null,"2018-11-23"]
[null,"2018-11-24"]
[null,"2018-11-25"]
[null,"2018-11-26"]
[null,"2018-11-27"]
[null,"2018-11-28"]
[null,"2018-11-29"]
[null,"2018-11-30"]
[null,"2018-12-01"]
[null,"2018-12-02"]
[null,"2018-12-03"]
[null,"2018-12-04"]
[null,"2018-12-05"]
[null,"2018-12-06"]
[null,"2018-12-07"]
[null,"2018-12-08"]
[null,"2018-12-09"]
[null,"2018-12-10"]
[null,"2018-12-11"]
[null,"2018-12-12"]
[null,"2018-12-13"]
[null,"2018-12-14"]
[null,"2018-12-15"]
[null,"2018-12-16"]
[null,"2018-12-17"]
[null,"2018-12-18"]
[null,"2018-12-19"]
[null,"2018-12-20"]
[null,"2018-12-21"]
[null,"2018-12-22"]
[null,"2018-12-23"]
[null,"2018-12-24"]
[null,"2018-12-25"]
[null,"2018-12-26"]
[null,"2018-12-27"]
[null,"2018-12-28"]
[null,"2018-12-29"]
[null,"2018-12-30"]
[null,"2018-12-31"]
[null,"2019-01-01",55,51]
[null,"2019-01-02",110,106]
[null,"2019-01-03",146,141]
[null,"2019-01-04",267,216]
[null,"2019-01-05",106,101]
[null,"2019-01-06",69,57]
[null,"2019-01-07",199,187]
[null,"2019-01-08",180,158]
[null,"2019-01-09",272,230]
[null,"2019-01-10",201,153]
[null,"2019-01-11",205,180]
[null,"2019-01-12",185,147]
[null,{"$f":"B1480+1","v":"2019-01-13"},89,82]
[null,"2019-01-14",321,258]
[null,"2019-01-15",262,220]
[null,"2019-01-16",178,146]
[null,"2019-01-17",244,187]
[null,"2019-01-18",223,186]
[null,"2019-01-19",128,108]
[null,"2019-01-20",115,94]
[null,"2019-01-21",250,201]
[null,"2019-01-22",296,244]
[null,"2019-01-23",221,163]
[null,"2019-01-24",555,363]
[null,"2019-01-25",1505,661]
[null,"2019-01-26",181,139]
[null,"2019-01-27",199,146]
[null,"2019-01-28",100,98]
[null,"2019-01-29",315,234]
[null,"2019-01-30",759,540]
[null,"2019-01-31",426,324]
[null,"2019-02-01",250,191]
[null,"2019-02-02",168,142]
[null,"2019-02-03",228,188]
[null,"2019-02-04",250,194]
[null,"2019-02-05",206,180]
[null,"2019-02-06",503,403]
[null,"2019-02-07",325,280]
[null,"2019-02-08",232,200]
[null,"2019-02-09",154,118]
[null,"2019-02-10",101,80]
[null,"2019-02-11",218,197]
[null,"2019-02-12",309,263]
[null,"2019-02-13",440,329]
[null,"2019-02-14",196,176]
[null,"2019-02-15",160,156]
[null,"2019-02-16",101,96]
[null,"2019-02-17",71,70]
[null,"2019-02-18",239,211]
[null,"2019-02-19",206,197]
[null,"2019-02-20",215,194]
[null,"2019-02-21",182,165]
[null,"2019-02-22",186,171]
[null,"2019-02-23",119,108]
[null,"2019-02-24",77,75]
[null,"2019-02-25",270,226]
[null,"2019-02-26",187,179]
[null,"2019-02-27",201,180]
[null,"2019-02-28",293,262]
[null,"2019-03-01",499,353]
[null,"2019-03-02",411,281]
[null,"2019-03-03",230,198]
[null,"2019-03-04",260,218]
[null,"2019-03-05",233,203]
[null,"2019-03-06",320,290]
[null,"2019-03-07",215,194]
[null,"2019-03-08",176,142]
[null,"2019-03-09",143,123]
[null,"2019-03-10",92,88]
[null,"2019-03-11",69,65]
[null,"2019-03-12",235,201]
[null,"2019-03-13",147,138]
[null,"2019-03-14",288,250]
[null,"2019-03-15",208,175]
[null,"2019-03-16",108,97]
[null,"2019-03-17",52,51]
[null,{"$f":"B1544+1","v":"2019-03-18"},212,192]
[null,"2019-03-19",200,189]
[null,"2019-03-20",208,183]
[null,"2019-03-21",143,139]
[null,"2019-03-22",253,233]
[null,"2019-03-23",168,155]
[null,"2019-03-24",139,105]
[null,"2019-03-25",434,327]
[null,"2019-03-26",241,205]
[null,"2019-03-27",184,160]
[null,"2019-03-28",230,203]
[null,"2019-03-29",226,173]
[null,"2019-03-30",205,163]
[null,"2019-03-31",94,84]
[null,"2019-04-01",170,142]
[null,"2019-04-02",227,214]
[null,"2019-04-03",188,146]
[null,"2019-04-04",149,126]
[null,"2019-04-05",219,173]
[null,"2019-04-06",88,84]
[null,"2019-04-07",90,79]
[null,"2019-04-08",224,196]
[null,"2019-04-09",180,141]
[null,"2019-04-10",128,108]
[null,"2019-04-11",135,114]
[null,"2019-04-12",156,133]
[null,"2019-04-13",66,57]
[null,"2019-04-14",44,43]
[null,"2019-04-15",200,174]
[null,"2019-04-16",180,156]
[null,"2019-04-17",185,156]
[null,"2019-04-18",164,146]
[null,"2019-04-19",82,73]
[null,"2019-04-20",59,57]
[null,"2019-04-21",34,30]
[null,"2019-04-22",39,39]
[null,"2019-04-23",182,168]
[null,"2019-04-24",149,126]
[null,"2019-04-25",51,50]
[null,"2019-04-26",220,189]
[null,"2019-04-27",101,95]
[null,"2019-04-28",62,59]
[null,"2019-04-29",183,164]
[null,"2019-04-30",208,177]
[null,"2019-05-01",196,143]
[null,"2019-05-02",205,164]
[null,"2019-05-03",171,141]
[null,"2019-05-04",100,84]
[null,"2019-05-05",59,54]
[null,"2019-05-06",189,177]
[null,"2019-05-07",250,181]
[null,"2019-05-08",265,212]
[null,"2019-05-09",182,170]
[null,"2019-05-10",198,163]
[null,"2019-05-11",190,129]
[null,"2019-05-12",87,81]
[null,"2019-05-13",204,172]
[null,"2019-05-14",166,145]
[null,"2019-05-15",191,156]
[null,"2019-05-16",140,124]
[null,"2019-05-17",186,157]
[null,"2019-05-18",147,111]
[null,"2019-05-19",68,54]
[null,"2019-05-20",219,203]
[null,{"$f":"B1608+1","v":"2019-05-21"},170,167]
[null,"2019-05-22",184,169]
[null,"2019-05-23",190,176]
[null,"2019-05-24",252,212]
[null,"2019-05-25",109,93]
[null,"2019-05-26",89,75]
[null,"2019-05-27",300,239]
[null,"2019-05-28",214,190]
[null,"2019-05-29",253,204]
[null,"2019-05-30",289,254]
[null,"2019-05-31",247,201]
[null,"2019-06-01",160,130]
[null,"2019-06-02",82,73]
[null,"2019-06-03",211,168]
[null,"2019-06-04",225,187]
[null,"2019-06-05",178,151]
[null,"2019-06-06",192,165]
[null,"2019-06-07",168,158]
[null,"2019-06-08",176,109]
[null,"2019-06-09",68,61]
[null,"2019-06-10",81,78]
[null,"2019-06-11",177,169]
[null,"2019-06-12",199,154]
[null,"2019-06-13",199,160]
[null,"2019-06-14",155,139]
[null,"2019-06-15",111,97]
[null,"2019-06-16",54,49]
[null,"2019-06-17",193,146]
[null,"2019-06-18",130,120]
[null,"2019-06-19",164,134]
[null,"2019-06-20",185,147]
[null,"2019-06-21",218,156]
[null,"2019-06-22",184,106]
[null,"2019-06-23",121,90]
[null,"2019-06-24",252,191]
[null,"2019-06-25",241,212]
[null,"2019-06-26",168,152]
[null,"2019-06-27",168,146]
[null,"2019-06-28",192,185]
[null,"2019-06-29",237,165]
[null,"2019-06-30",100,74]
[null,"2019-07-01",242,188]
[null,"2019-07-02",198,176]
[null,"2019-07-03",194,158]
[null,"2019-07-04",159,136]
[null,"2019-07-05",198,184]
[null,"2019-07-06",214,171]
[null,"2019-07-07",179,121]
[null,"2019-07-08",236,199]
[null,"2019-07-09",172,148]
[null,"2019-07-10",346,296]
[null,"2019-07-11",346,284]
[null,"2019-07-12",215,179]
[null,"2019-07-13",430,287]
[null,"2019-07-14",147,109]
[null,"2019-07-15",288,204]
[null,"2019-07-16",218,184]
[null,"2019-07-17",200,145]
[null,"2019-07-18",180,148]
[null,"2019-07-19",172,150]
[null,"2019-07-20",130,114]
[null,"2019-07-21",75,70]
[null,"2019-07-22",212,180]
[null,"2019-07-23",421,206]
[null,{"$f":"B1672+1","v":"2019-07-24"},205,158]
[null,"2019-07-25",201,161]
[null,"2019-07-26",123,117]
[null,"2019-07-27",85,64]
[null,"2019-07-28",85,75]
[null,"2019-07-29",193,163]
[null,"2019-07-30",155,130]
[null,"2019-07-31",174,158]
[null,"2019-08-01",184,137]
[null,"2019-08-02",162,131]
[null,"2019-08-03",77,61]
[null,"2019-08-04",73,46]
[null,"2019-08-05",172,124]
[null,"2019-08-06",163,114]
[null,"2019-08-07",145,107]
[null,"2019-08-08",185,128]
[null,"2019-08-09",542,363]
[null,"2019-08-10",156,114]
[null,"2019-08-11",103,92]
[null,"2019-08-12",248,203]
[null,"2019-08-13",174,139]
[null,"2019-08-14",250,226]
[null,"2019-08-15",267,202]
[null,"2019-08-16",207,174]
[null,"2019-08-17",113,96]
[null,"2019-08-18",138,101]
[null,"2019-08-19",276,228]
[null,"2019-08-20",247,157]
[null,"2019-08-21",190,173]
[null,"2019-08-22",163,115]
[null,"2019-08-23",176,163]
[null,"2019-08-24",139,115]
[null,"2019-08-25",43,41]
[null,"2019-08-26",205,183]
[null,"2019-08-27",142,139]
[null,"2019-08-28",192,167]
[null,"2019-08-29",178,158]
[null,"2019-08-30",232,213]
[null,"2019-08-31",119,105]
[null,"2019-09-01",70,58]
[null,"2019-09-02",151,142]
[null,"2019-09-03",180,161]
[null,"2019-09-04",179,128]
[null,"2019-09-05",182,150]
[null,"2019-09-06",173,136]
[null,"2019-09-07",144,128]
[null,"2019-09-08",103,90]
[null,"2019-09-09",262,216]
[null,"2019-09-10",197,184]
[null,"2019-09-11",161,150]
[null,"2019-09-12",159,151]
[null,"2019-09-13",175,148]
[null,"2019-09-14",111,102]
[null,"2019-09-15",48,45]
[null,"2019-09-16",234,194]
[null,"2019-09-17",170,160]
[null,"2019-09-18",201,127]
[null,"2019-09-19",177,146]
[null,"2019-09-20",158,127]
[null,"2019-09-21",184,124]
[null,"2019-09-22",61,59]
[null,"2019-09-23",179,109]
[null,"2019-09-24",167,130]
[null,"2019-09-25",299,208]
[null,{"$f":"B1736+1","v":"2019-09-26"},155,134]
[null,"2019-09-27",124,109]
[null,"2019-09-28",95,85]
[null,"2019-09-29",87,54]
[null,"2019-09-30",213,190]
[null,"2019-10-01",185,157]
[null,"2019-10-02",174,140]
[null,"2019-10-03",182,147]
[null,"2019-10-04",189,136]
[null,"2019-10-05",126,100]
[null,"2019-10-06",58,52]
[null,"2019-10-07",124,100]
[null,"2019-10-08",179,129]
[null,"2019-10-09",142,121]
[null,"2019-10-10",131,105]
[null,"2019-10-11",149,108]
[null,"2019-10-12",111,102]
[null,"2019-10-13",47,40]
[null,"2019-10-14",162,119]
[null,"2019-10-15",133,115]
[null,"2019-10-16",228,160]
[null,"2019-10-17",236,170]
[null,"2019-10-18",156,114]
[null,"2019-10-19",104,88]
[null,"2019-10-20",52,51]
[null,"2019-10-21",187,144]
[null,"2019-10-22",152,121]
[null,"2019-10-23",160,123]
[null,"2019-10-24",202,168]
[null,"2019-10-25",174,137]
[null,"2019-10-26",124,73]
[null,"2019-10-27",52,48]
[null,"2019-10-28",233,199]
[null,"2019-10-29",205,182]
[null,"2019-10-30",199,176]
[null,"2019-10-31",187,144]
[null,"2019-11-01",188,135]
[null,"2019-11-02",191,148]
[null,"2019-11-03",64,55]
[null,"2019-11-04",170,156]
[null,"2019-11-05",68,62]
[null,"2019-11-06",190,148]
[null,"2019-11-07",221,157]
[null,"2019-11-08",183,118]
[null,"2019-11-09",102,79]
[null,"2019-11-10",43,43]
[null,"2019-11-11",368,183]
[null,"2019-11-12",200,144]
[null,"2019-11-13",197,171]
[null,"2019-11-14",160,135]
[null,"2019-11-15",147,125]
[null,"2019-11-16",101,85]
[null,"2019-11-17",61,59]
[null,"2019-11-18",146,127]
[null,"2019-11-19",168,143]
[null,"2019-11-20",188,146]
[null,"2019-11-21",987,638]
[null,"2019-11-22",394,162]
[null,"2019-11-23",152,101]
[null,"2019-11-24",66,61]
[null,"2019-11-25",258,100]
[null,"2019-11-26",377,131]
[null,"2019-11-27",238,167]
[null,"2019-11-28",186,133]
[null,{"$f":"B1800+1","v":"2019-11-29"},170,140]
[null,"2019-11-30",158,117]
[null,"2019-12-01",90,73]
[null,"2019-12-02",232,131]
[null,"2019-12-03",252,161]
[null,"2019-12-04",193,147]
[null,"2019-12-05",147,132]
[null,"2019-12-06",151,125]
[null,"2019-12-07",100,81]
[null,"2019-12-08",76,67]
[null,"2019-12-09",262,163]
[null,"2019-12-10",232,139]
[null,"2019-12-11",210,118]
[null,"2019-12-12",164,130]
[null,"2019-12-13",152,141]
[null,"2019-12-14",129,111]
[null,"2019-12-15",78,71]
[null,"2019-12-16",168,131]
[null,"2019-12-17",161,111]
[null,"2019-12-18",462,178]
[null,"2019-12-19",246,200]
[null,"2019-12-20",885,276]
[null,"2019-12-21",349,135]
[null,"2019-12-22",52,43]
[null,"2019-12-23",148,129]
[null,"2019-12-24",94,92]
[null,"2019-12-25",53,49]
[null,"2019-12-26",53,51]
[null,"2019-12-27",109,93]
[null,"2019-12-28",70,61]
[null,"2019-12-29",85,68]
[null,"2019-12-30",736,532]
[null,"2019-12-31",291,196]

{"sheet":"6.2 Reliability & Cust serv","index":33,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[[5,1,5,7],[8,4,8,8],[16,1,16,3],[20,4,20,8],[28,1,28,3],[32,4,32,8],[70,4,70,8],[40,1,40,3],[44,4,44,8],[52,1,52,3],[55,1,55,8],[58,2,58,8],[67,1,67,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIDI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total sustained minutes off supply after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,51.49466569183322,51.49466569183322,51.49466569183322,51.49466569183322,51.49466569183322]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,121.52419302123414,121.52419302123414,121.52419302123414,121.52419302123414,121.52419302123414]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E12:E16)","v":173.01885871306735},{"$f":"SUM(F12:F16)","v":173.01885871306735},{"$f":"SUM(G12:G16)","v":173.01885871306735},{"$f":"SUM(H12:H16)","v":173.01885871306735},{"$f":"SUM(I12:I16)","v":173.01885871306735}]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"SAIFI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total sustained interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,0.65709083829821269,0.65709083829821269,0.65709083829821269,0.65709083829821269,0.65709083829821269]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,1.6105015870065968,1.6105015870065968,1.6105015870065968,1.6105015870065968,1.6105015870065968]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E24:E28)","v":2.2675924253048096},{"$f":"SUM(F24:F28)","v":2.2675924253048096},{"$f":"SUM(G24:G28)","v":2.2675924253048096},{"$f":"SUM(H24:H28)","v":2.2675924253048096},{"$f":"SUM(I24:I28)","v":2.2675924253048096}]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFI",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},null,null,1.5637975209211823,1.5637975209211823,1.5637975209211823,1.5637975209211823,1.5637975209211823]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},null,null,4.7274014707913574,4.7274014707913574,4.7274014707913574,4.7274014707913574,4.7274014707913574]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E36:E40)","v":6.2911989917125393},{"$f":"SUM(F36:F40)","v":6.2911989917125393},{"$f":"SUM(G36:G40)","v":6.2911989917125393},{"$f":"SUM(H36:H40)","v":6.2911989917125393},{"$f":"SUM(I36:I40)","v":6.2911989917125393}]
[]
[]
[null,"6.2.3(B) - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFIe)"]
[null,null,null,null,"Proposed target"]
[null,"MAIFIe",null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Total momentary interruptions after removing excluded events"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",null,null,{"$f":"SUM(E48:E52)","v":0},{"$f":"SUM(F48:F52)","v":0},{"$f":"SUM(G48:G52)","v":0},{"$f":"SUM(H48:H52)","v":0},{"$f":"SUM(I48:I52)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - DISTRIBUTION CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},645560.22071270435,657448.2844416172,667473.25090973475,677070.75869249692,686277.06981915596,695213.8963309055,703839.3391858039]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},56918.156011376821,57966.310225786779,58850.197719367447,59696.396769080537,60508.104548128547,61296.052239640267,62056.545662764001]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C61:C65)","v":702478.37672408111},715414.59466740396,726323.4486291022,736767.15546157747,746785.17436728452,756509.94857054576,765895.88484856789]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,null,null,"Proposed target"]
[null,null,null,null,{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"}]
[null,"Number of calls received",null,null,500004,500004,500004,500004,500004]
[null,"Number of calls answered within 30 seconds",null,null,363367,363367,363367,363367,363367]
[null,"Percentage of calls answered within 30 seconds",null,null,{"$f":"IFERROR((E74/E73),\"\")","v":0.72672818617451063},{"$f":"IFERROR((F74/F73),\"\")","v":0.72672818617451063},{"$f":"IFERROR((G74/G73),\"\")","v":0.72672818617451063},{"$f":"IFERROR((H74/H73),\"\")","v":0.72672818617451063},{"$f":"IFERROR((I74/I73),\"\")","v":0.72672818617451063}]

{"sheet":"7.1  Policies and Procedures","index":34,"n_rows":216,"n_cols":5,"rows_kept":216,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[null,"Governance framework"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Connection policy, United Energy to apply from 1 July 2021","This connection policy provides an outline of our connection services, when connection charges may be payable by customers and how those charges are calculated.","Connections capex","No "]
[null,"Cost allocation method, January 2020 Version number 3","The cost allocation method governs the manner in which we allocate costs for the services we provide. ","Opex and capex","Yes"]
[null,"UE Model Standing Offer Basic Connection Service for Retail Customers (Without Generation) 2019","Provides the connection arrangements for residential customers","Connections capex","No "]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"UE Motor Vehicle Policy Document No. U PO 005 (July 2019)","This document details the management and replacement of our fleet vehicels"]
[null,"Asset management policy ","The purpose of this document is to describe the framework for the management of our electricity distribution system.","Augex, Repex and Opex","No"]
[null,"Asset Management Strategies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[null,"Asset Management Plans"]
[null,"Fire prevention plan","This document outlines our activities to mitigate the risk of fires","Augex and Repex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"Strategic asset management plan, November 2019","This document assists us in managing and maintaining the assets operating in our network","Augex, Repex and Opex","No"]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Network planning guidelines","The document provides criteria to be used in relation to network planning","Augex, Repex and Opex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Information technology policies or strategies"]
[null,"IT deliverability plan 2021-2026, Jan2020","This document provides an overview of our delivery framework and operating model and highlights how our flexible resourcing model ensures delivery of projects on time and within budget.","IT Capex","No"]
[null,"VPN & UE, Cyber strategy and program review Nov2019","This document outlines our cyber security strategy which informs our cyber security program","IT Capex","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"Demand side engagement strategy ","The Demand Side Engagement Strategy assists non-network providers in understanding our framework and processes for assessing demand side options and consultation process.","Augex","No"]
[]
[]
[null,"Self insurance guidelines or policy"]
[null,"Insurance Credit Management Policy, Appendix C, Nov2019","Support of our nominated pass through events in the event of an insurer credit risk event","Pass through event","No"]
[]
[null,"Land and easement acquisition polices"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"<insert relevant policy, plan, strategy etc>"]

{"sheet":"7.2 Contingent projects","index":35,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2021-22 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2021-22"}]
[null,null,null,null,null,{"$f":"+E8*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":36,"n_rows":304,"n_cols":5,"rows_kept":304,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"LEGISLATION"]
[null,"The National Electricity Law (NEL) and associated regulations","This law states the market objectives to govern the National Electricity Market's (NEM) development; establishes the governance arrangements for the NEM and Victoria's participation in the national market; provides for the making of rules; confers powers and responsibilities with respect to the safety and security of the national system; and provides immunity for service providers in certain circumstances.","Relevant to capital and operating expenditure forecasts.","Yes"]
[null,"Electricity Safety Act 1998 Version 75 (incorp amendments as at 1 April 2019)","This Act regulates the safety of electricity supply and use in Victoria, and the efficiency of electrical equipment. It is administered by Energy Safe Victoria.","Relevant to capital expenditure, the expulsion dropout (EDO) fuse replacement step change and hazardous bushfire risk area (HBRA) reclassification step change","Yes"]
[null,"Electricity Safety (Electric Line Clearance) Regulations 2015","These Regulations prescribe the Code of Practice for Electric Line Clearance 2015, and make it an offence to breach those prescribed provisions.","Relevant to vegetation management expenditure, connections and HBRA reclassification step change","Yes"]
[null,"Electricity Safety (Bushfire Mitigation) Regulations 2013","Safety obligations related to bushfire mitigation","Relevant to capital expenditure, on-going operating expenditure step change for operation of rapid earth fault current limiters (REFCLs) and the HBRA reclassification step change","Yes"]
[null,"Electricity Safety (Management) Regulations 2009","Risk management obligations in managing the network in a safe manner.","Generally relevant all expenditure.","Yes"]
[null,"National Electricity (Victoria) Act 2005","This Act provides for the regulation of the national electricity wholesale market. It is part of a national scheme which gives effect to the National Electricity Law and the National Electricity Rules made under that Law. The lead legislation under the national scheme is the National Electricity (South Australia) Act 1996. The economic regulator is the Australian Energy Regulator (AER) and the rule-maker is the Australian Energy Market Commission (AEMC). The national electricity wholesale market is administered by the Australian Energy Market Operator (AEMO).","Application of F-Factor Scheme for 2016-2020. Applied in the EDO fuse replacement step change","Yes"]
[null,"Environment Protection Act 1970 ","An Act to establish an Environment Protection Authority (EPA), to make provision with respect to its powers, duties, and functions and to make further provision for the protection of the environment and for other purposes.","Relevant to capital and operating expenditure forecast on envrionmental expenditure, including operating expenditure step change and replacement capital expenditure","Yes"]
[null,"Environment Protection Act 2017","The main purposes of this Act are— (a) to provide for the continuation of the EPA; and (b) to specify a new objective of the EPA; and (c) to provide for a new governance structure of the continued EPA; and to provide for the governing board of the EPA; and (e) to make consequential amendments to the Environment Protection Act 1970","Relevant to capital and operating expenditure forecast on envrionmental expenditure, including operating expenditure step change and replacement capital expenditure","Yes"]
[null,"Environment Protection Amendment Act 2018","The Environment Protection Amendment Act 2018 provides the foundation for a transformation of Victoria’s environment protection laws and the EPA. The Victorian Government intends this new legislation to take effect from 1 July 2020.","Relevant to capital and operating expenditure forecast on envrionmental expenditure, including operating expenditure step change and replacement capital expenditure","Yes"]
[null,"Environment Protection (Industrial Waste Resource) Regulations 2009","The Environment Protection (Industrial Waste Resource) Regulations 2009, administered by the EPA, contains a number of provisions relevant to contamination of land. This includes the transport and disposal of contaminants.","Section 45 makes it an offence to pollute land and Section 57 provides for environmental audits by accredited auditors. \nThese are relevant to our step change for decommissioning zone substations. Step change reference relevant to CitiPower only.","Yes"]
[null,"Environment Protection Regulations DRAFT"," The objectives of these Regulations are to further the purposes of, and give effect to, the Environment Protection Act 2017 by—\n(a) imposing obligations in relation to environmental protection, pollution incidents, contaminated land and waste; and\n(b) providing for activities and other matters for the purposes of permissions under the Act; and (l) prescribing other matters necessary to give effect to the Act.\n(c) specifying matters in relation to litter, water, air, land, noise and vehicle emissions; and\n(d) encouraging retailers and consumers to reduce the overall use of plastic bags that often enter the environment as litter, by banning thin, single-use plastic shopping bags; and\n(e) setting out additional matters in relation to environmental audits; and\n(f) prescribing activities in respect of which—\n(i) the environment protection levy is payable; and\n(ii) the waste levy is payable; and\n(iii) the Authority may require a financial assurance; and\n(g) prescribing the form and manner of certain applications; and \n(h) prescribing infringement offences and infringement penalties; and\n(i) providing for exemptions from certain provisions of the Act; and\n(j) prescribing the fees payable under the Act; and\n(k) providing for transitional arrangements; and\n","Relevant to capital and operating expenditure forecast on envrionmental expenditure, including operating expenditure step change and replacement capital expenditure","Yes"]
[null,"Environment Reference Standard (standards) DRAFT","This environment reference standard sets out the environmental values of the ambient air, acoustic, land and water environments that are sought to be achieved or maintained in Victoria. ","Relevant to capital and operating expenditure forecast on envrionmental spen, including the step change due to change in legislation","Yes"]
[null,"Superannuation Guarantee (Administration) Act 1992, No. 111","The Act sets out relevant superannuation payment requirements.","The Superannuation Guarantee (Administration) Act 1992 required, from 1 July 2014, that we increase our employee superannuation contributions by an increment of 25 basis points.","Yes"]
[null,"Minerals Resource Rent Tax Repeal and Other Measures Bill 2014","The bill: repeals the Minerals Resource Rent Tax Act 2012, Minerals Resource Rent Tax (Imposition—Customs) Act 2012, Minerals Resource Rent Tax (Imposition—Excise) Act 2012 and Minerals Resource Rent Tax (Imposition—General) Act 2012; amends the: Income Tax Assessment Act 1997 and Income Tax (Transitional Provisions) Act 1997 to provide that companies can carry tax losses forward to use as a deduction for a future year; Income Tax Assessment Act 1997 to: amend the instant asset write-off threshold provisions for small business entities; provide that motor vehicle purchases made by small business entities will be treated as normal business assets for depreciation purposes; and provide that geothermal energy exploration and prospecting expenditure are no longer immediately deductible; Superannuation Guarantee (Administration) Act 1992 to enable the Treasurer by non-disallowable legislative instrument to vary the superannuation guarantee charge percentage for a particular year commencing on 1 July; Superannuation (Government Co-contribution for Low Income Earners) Act 2003 to abolish the low income superannuation contribution; Social Security Act 1991 and Social Security (Administration) Act 1999 to abolish the income support bonus payment; and A New Tax System (Family Assistance) Act 1999, A New Tax System (Family Assistance) (Administration) Act 1999, Income Tax Assessment Act 1997 and Social Security (Administration) Act 1999 to abolish the schoolkids bonus payment; and makes consequential amendments to 13 Acts.","Relevant to all expenditure that includes labour","Yes"]
[null,"Occupational Health and Safety Act 2004 (Vic)","Safety obligations relating to employee health and safety","Relevant to all expenditure","No"]
[null,"Roads Management Act 2004 (Vic)","Safety obligations when carrying out works on public roadways.","Relevant to all capex categories and public lighting","No"]
[null,"The Australian Privacy Principles (APPS) within the Privacy Act 1988 (Cth)","The Australian Privacy Principles (or APPs) are the cornerstone of the privacy protection framework in the Privacy Act 1988 (Privacy Act). They apply to any organisation or agency the Privacy Act covers.\n\nThere are 13 Australian Privacy Principles and they govern standards, rights and obligations around:\n- the collection, use and disclosure of personal information\n- an organisation or agency’s governance and accountability\n- integrity and correction of personal information\n- the rights of individuals to access their personal information","Relevant to ICT cyber security expenditure","No"]
[null,"Corporations Act 2001 (Cth)","Regulates matters such as the formation and operation of companies (in conjunction with a constitution that may be adopted by a company), duties of officers, takeovers, fundraising and financial reporting obligations","Relevant to SAP upgrade expenditure","No"]
[null,"Foreign Acquisitions and Takeovers Act 1975","An Act relating to the foreign acquisition of certain land interests and to the foreign control of certain business enterprises and mineral rights","Relevant to the security of critical infrastructure step change","Yes"]
[null,"Security of Critical Infrastructure Act 2018 ","The object of this Act is to provide a framework for managing risks to national security relating to critical infrastructure, including by:\n(a)  improving the transparency of the ownership and operational control of critical infrastructure in Australia in order to better understand those risks; and\n(b)  facilitating cooperation and collaboration between all levels of government, and regulators, owners and operators of critical infrastructure, in order to identify and manage those risks.","Relevant to cyber security expenditure and security of critical infrastructure step change","Yes"]
[null,"Regulatory Powers (Standard Provisions) Act 2014","An Act in relation to monitoring, investigation and enforcement by regulatory agencies, and for related purposes","Relevant to the security of critical infrastructure step change","Yes"]
[null,"Criminal Code Act 1995 ","The only offences against laws of the Commonwealth are those offences created by, or under the authority of, this Code or any other Act.","Relevant to the security of critical infrastructure step change","Yes"]
[null,"Australian Energy Market Act 2004 ","An Act relating to the regulation of energy markets, and for related purposes","Relevant to the security of critical infrastructure step change","Yes"]
[null,"Energy Safety Legislation Amendment Bill 2019","A Bill for an Act to amend the Electricity Safety Act 1998 and the Energy Safe Victoria Act 2005 in relation to Energy Safe Victoria and certain classes of electrical work and to make consequential and related amendments to certain other Acts and for other purposes.","Relevant to our obligation to pay Energy Safe Victoria (ESV) levy and the ESV levy step change","Yes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENCES"]
[null,"Electricity Distribution Licence (2005)","The Licence authorises the distribution or supply electricity to supply points located in the Licensee’s distribution area.","Relevant to all expenditure chapters","No"]
[]
[]
[]
[null,"RULES"]
[null,"National Electricity Rules(NER)","These Rules are made under the National Electricity Law and set out the rights and obligations of participants in the National Electricity Market, AEMO as market operator, and the market institutions. It includes connections, planning and expansation, economic regulation, metering and transitional requirements. It also includes all procedures established under the Rules","The regulatory proposal is developed in accordance with the NER and positions are consistent with the objectives and requirements in the NER.\n","Yes"]
[null,"AEMC, National Electricity Amendment (Retailer insolvency events – costs pass through provisions) Rule 2015, Consultation, 30 October 2014","Change in definition of the retailer insolvency event","Pass through event in the regulatory proposal.","No"]
[null,"AEMC, Rule determination, National Electricity Amendment (Five Minute Settlement) Rule 2017, page 8","In 2017/2018, the AEMC made a rule change to reduce the time interval for wholesale market financial settlement from 30 minutes to five minutes to align with the time period for physical dispatch of energy.","Information and communications technology expenditure and 5-minute settlement step change","Yes"]
[]
[null,"ORDERS"]
[null,"Advanced Metering Infrastructure (Oligations to install meters) Order 2017","Objectives\nThe objectives of this Order are:\n(a) to regulate the installation and operation of remotely read interval meters on and after\n1 December 2017; and\n(b) to make consequential amendments to the Cost Recovery Order; and\n(c) to revoke the AMI Specifications Order.","Relevant to metering expenditure forecasts","No"]
[]
[]
[null,"CODES"]
[null,"Electricity Distribution Code (2018)","The purpose of this Code is to regulate the following activities so that they are undertaken in a safe, efficient and reliable manner:\n(a) the distribution of electricity by a distributor for supply to its customers;\n(b) the connection of a customer’s electrical installation to the distribution system;\n(c) the connection of embedded generating units to the distribution system; and\n(d) the transfer of electricity between distribution systems.","Relevant to all expenditure, service target performance incentive scheme and guranteed service level payments,","No"]
[null,"Electricity System Code (2000)","The purpose of this code is to regulate the following activities so that they are undertaken in a safe, efficient and reliable manner:\n(a) the provision of shared transmission network services by transmitters;\n(b) the connection of distributors and EHV consumers to the transmission network;\n(c) the connection of generating Units to the transmission network; and\n(d) the transfer of electricity between transmission networks.","Relevant to augmentation and replacement capital expenditure","No"]
[null,"Public Lighting Code (2015)","The purpose of this Code is to regulate the provision of public lighting or the arrangements for such provision by specifying minimum standards and certain obligations of distributors and public lighting customers. The objective of such regulation is to provide a safe visual environment for pedestrian and vehicular movement during times of inadequate natural light.","Relevant to public lighting expenditure","No"]
[null,"Code of Practice for Electric Line Clearance 2010 (as contained in the Schedule to the Electricity Safety (Electric Line Clearance) Regulations 2010)","The Code includes the clearance spaces required to be maintained for vegetation in the vicinity of powerlines.","Relevant to our vegetation management expenditure, including the HBRA reclassification step change","Yes"]
[null,"Building Code of Australia (BCA) and National Construction Code(NCC)","The BCA is contained within the NCC and provides the minimum necessary requirements for safety, health, amenity and sustainability in the design and construction of new buildings (and new building work in existing buildings) throughout Australia.","Relevant to property expenditure","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"Electricity Industry Guideline 11 – Voltage Variation Compensation","Broadly speaking, this guideline requires a distributor to compensate any person whose property is damaged due to an unauthorised voltage variation affecting an electrical installation where the aggregate consumption of electricity which is taken from the relevant customer’s point of supply is, or is reasonably expected to be, less than 160 megawatt hours in any year.","This guideline is a relevant guideline for the purposes of clause 4.2.7 of the Electricity Distribution Code (relating to compensation for property damage due to voltage variations outside limits).","No"]
[null,"Electricity Industry Guideline No 14 – Provision of Services by Electricity Distributors","The objective of this guideline is to facilitate efficiency in the following aspects of electricity distribution, by way of regulation that is flexible and encourages transparency:\n(a) the undergrounding of distribution fixed assets;\n(b) the determination of customer contributions to the capital cost of new works and augmentation;\n(c) the contestability of connection and augmentation works; and\n(d) the provision of excluded services.","This guideline is a relevant guideline for the purposes of the Distribution Licence","No"]
[null,"Electricity Industry Guideline No 15 – Connection of Embedded Generation","The objective of this guideline is to provide clarity and transparency about arrangements for connecting embedded generating units to distribution systems, in particular in respect of:\n(a) the way in which distributors negotiate connection agreements with embedded generators;\n(b) the charges under, and other terms and conditions of, connection agreements, including principles distributors must observe in setting those charges and other terms and conditions;\n(c) the payment to embedded generators of a share of distributors’ avoided distribution system costs; and\n(d) the payment to embedded generators of distributors’ avoided customer TUOS usage charges.\n1.1.2 By regulating these arrangements, the Commission also intends to make it clear that, if a dispute arises between a distributor and an embedded generator, that dispute must be resolved in accordance with the procedures specified by the Commission in the distributor’s distribution licence, in this guideline and in guideline 14.","This guideline is a relevant guideline for the purposes of clauses 10.3 and 11.1 of Distribution Licence","No"]
[null,"Forecast Expenditure Assessment Guideline, November 2013","The Guideline must specify:\n- the approach the AER proposes to use to assess the forecasts of operating expenditure (opex) and capital expenditure (capex) that form part of the regulatory proposals DNSPs\n- the information the AER requires for the purposes of that assessment.","Our proposed operating and capital expenditure is developed taking into consideration the AER's assessment approach as set out in the Guideline.\nChapters 7,9, 10.","Yes"]
[null,"Capital Expenditure Incentive Guideline, November 2013","This guideline is specifically concerned with further improving the incentives facing distributors to undertake efficient and prudent capital expenditure","Our regulatory proposal has been prepared consistent with the guideline","No"]
[null,"Consumer Engagement Guideline for Network Service Providers, November 2013","Sets out the framework for engaging consumers and integrating the long-term interests of consumers into our expenditure plans","Referred to throughout regulatory proposal","Yes"]
[null,"Connection charge guidelines for electricity retail customers —under chapter 5A of the National Electricity Rules, June 2012","The AER is required to develop and publish guidelines for the development of connection policies by distribution network service providers.","This guideline impacts the connection charging methodology.","No"]
[null,"Shared Asset Guideline (Nov 2013)","Shared Asset Guideline sets out how electricity consumers will share in the benefits of using assets paid for by electricity consumers to also provide other, unregulated, services","We have applied the guideline to determine whether the shared asset reduction is to be applied","No"]
[null,"Confidentiality guideline (2017)","Sets out how energy network businesses must make confidentilaity claims over information supplied to the AER","Confidentiality claim template is lodged with regulatory proposal identifies any components of the regulatory proposal and reset regulatory information notice which we are proposing to claim confidentiality over and why","No"]
[null,"Service target performance incentives scheme, November 2018","The service traget performance incentive scheme (STPIS) is designed to ensure distributors improve efficiency without a deterioration in service performance for customers, and improving service performance where customers are willing to pay for these improvements, in accordance with clause 6.6.2 of the National Electricity Rules","Our regulatory proposal is based on the guideline.","No"]
[null,"Demand management incentive scheme and innovation allowance mechanism 2017","The role of the scheme, as set out in clause 6.6.3(a) of the NER, is to provide incentives for distributors to implement efficient non-network alternatives, or to manage the expected demand for standard control services in some other way. The scheme is designed to complement the existing incentives within the regulatory framework for distributors to implement non-network alternatives and manage demand","Our regulatory proposal is based on the guideline","No"]
[null,"Efficiency benefit sharing scheme, Nov 2013","The efficiency benefits sharing scheme provides for a sharing between distributors and network users of efficiency gains and efficiency losses.","Our regulatory proposal has been prepared in accordance with the guideline. ","No"]
[null,"National guidelines for prevention of unauthorised access to electricity infrastructure ","The Energy Networks Association has produced a National Electricity Network\nSafety Code as the peak hierarchical document on electricity industry safety in Australia with the objectives to:\n• promote safety as a priority for customers, the public and industry workers;\n• promote nationally consistent practices;\n• promote economic efficiencies through standardisation; and\n• simplify the interpretation of regulatory requirements. ","Relevant to property and information and communications technology expenditure","No"]
[null,"Distribution Reliability Measures Guideline, November 2018.","The purpose of the Distribution Reliability Measures Guideline is to outline a set of common definitions of reliability measures that can be used to assess and compare the reliability performance of distributors, as required under National Electricity Rules 6.2.8","Our proposed STPIS targets are calculated in accordance with the defintions in the Guideline","No"]
[null,"Customer Service Incentive Scheme, December 2019, DRAFT ","Sets out the factors the AER will consider should distributors choose to propose a customer incentive scheme","Relevant for our proposed incentive arrangements","No"]
[null,"Application guidelines for the\nregulatory investment tests, December 2018","Guidelines to identify the credible option that maximises the present value of net economic benefit to all those who produce, consume and transport electricity in the relevant market (the preferred option)","Relevant to augmentation and demand management forecasts and business cases","No"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[null,"Use of System Agreement (2011)","This agreement sets out the rights and obligations of the parties in respect of: \n(a) the provision of the distribution services by the distributor to the retailer in respect of customers, and the payment for those distribution services by the retailer; and \n(b) the provision of retail services by the retailer, and the payment for those retail services by the distributor. \n","Sets out credit support arrangements.","No"]
[]
[]
[null,"OTHER"]
[null,"Victoria Fire Factor Scheme 2017","Financial incentive scheme to encourage improvements in the management of electricity distribution assets, with the aim of reducing the number of fires started by those assets","Relevant to replacement capital expenditure and incentive arrangements","Yes"]
[null,"NEM Metrology Procedure Part A","These procedures set out the obligations as a responsible person and financially responsible metering provider in relation to the engagement of metering service providers for the provision, installation, routine testing and maintenance of metering installations","Provision, installation, routine testing and maintenance of metering installations. Measurement of electrical energy and the provision of data to AEMO","No"]
[null,"Regulatory Information Notices (RINs)","Refers to the RIN issued under Division 4 of Part 3 of the National Electricity (Victoria) Law on 4 October 2019 (Reset RIN)","A completed Reset RIN forms part of our regulatory proposal","No"]
[null,"Distribution Roll Forward Model (RFM)","This handbook sets out the AER's RFM which forms part of a distributor's revenue proposal.  Distributors are required to submit a completed RFM to the AER as part of their regulatory proposal. However, the AER recognises that there may be a need for some flexibility in applying the RFM in order to account for the particular circumstances a distributor may face. A number of elements of the RFM where this may be the case have been identified in this handbook.","Population of the roll forward model","No"]
[null,"Distribution post tax revenue model (PTRM)","This handbook sets out the PTRM to be used as part of the building block determinations for standard control services of distributors.  Distributors are required to submit a completed PTRM to the AER as part of their regulatory proposals. However, the AER recognises that there may be a need for some flexibility in applying the PTRM in order to account for the particular circumstances a DNSP may face. A number of elements of the PTRM where this may be the case have been identified in this handbook.","Population of the PTRM","No"]
[null,"Electricity distribution network service providers, Annual Benchmarking Report 2019","The AER must have regard to the benchmarking report in assessing a distributor's expenditure forecasts","Relevant to the assessment of the efficiency of historical and forecast expenditure\n","No"]
[null,"Victorian Electricity Distribution Network Service Providers - Distribution Determination 2016-2020 – Final Decision","Contains obligations relating to the distributor in the current regulatory control period","Relevant to all expenditure","No"]
[null,"Electricity network service providers, Replacement expenditure model handbook, November 2013","Obligations related to populating an expenditure forecasting model related to the AER's Forecast Expenditure Assessment Guideline","Relevant to a comparison against replacement capex.","Yes"]
[null,"AER, Final framework and approach, AusNet Services, CitiPower, Jemena, Powercor and United Energy, Regulatory control period commencing 1 January 2021, January 2019 (F&A)","The F&A determines, amongst other things, which services we will regulate and the broad nature of the regulatory arrangements. This includes an assessment of services and whether we need to directly control the prices set for those services.","Sets out reclassification of services and form of price control","Yes"]
[null,"Australian Energy Sector Cyber Security Framework (AESCSF)","In 2018 AEMO, in collaboration with industry and government partners, developed a tailored cyber security framework for the Australian energy sector – AESCSF. The framework enables participants to undertake assessments of their own cyber security capability and maturity and use the results to inform and prioritise investment to improve cyber security posture.","Relevant for information and communications technology expenditure on cyber security","No"]

{"sheet":"7.3(b) Obligations cont.","index":37,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[5,2,6,2],[5,1,6,1]]}
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"OTHER"]
[null,"Bushfire Mitigation Plan","Section 113A (1) of the Electricity Safety Act 1998 requires that a major electricity company must prepare and submit to Energy Safe Victoria, for acceptance, a plan for the company's proposals for mitigation of bushfire in relation to the company’s supply network at the end of each period of 5 years","Relevant to HBRA reclassification and EDO fuse replacement step changes","Yes"]
[null,null,null,"Relevant to bushfire capital expenditure","No"]
[null,"Fire Prevention Plan","Information on asset management approach, processes and strategies applied to the management of the electricity network to prevent fire ignition emanating from the United Energy supply network.","Relevant to network communications busines cases","No"]
[null,"Power System Data\nCommunication Standard","Sets out the standards with which data communication providers must comply when transmitting data to and from AEMO","Relevant to network communications busines cases","No"]
[null,"Industry practice application note - Asset replacement planning Jan 2019","Provides clarity on how distributors might apply the National Electricity Rule requirements to their replacement expenditure planning of network assets and demonstrate the prudancy and efficiency of network assets investment on asset retirement and de-rating decisions.","Relevent to replacement expenditure","No"]
[null,"Demand Side Engagement Strategy V3.1 30 July 2019","Used to assist non-network providers in understanding our framework and processes for assessing demand side options. Also discusses the consultation process with non-network providers, which provides information on how CitiPower and Powercor will engage with non-network providers and how it will consider non-network options. It is aligned with clauses 5.13.1 (e)to (j) of the National Electricity Rules ","Presents our demand side engagement strategy outlining our process for engaging and consulting with non-network service providers, and for investigating, developing, assessing and reporting on non-network options as alternatives to network augmentation","Yes"]
[null,"Demand Side Engagement Document 18 July 2016 (Document no. UE PL 2202)","Prepared by United Energy as required under clause 5.13.1(e) to (j) of the National Electricity Rules. The purpose of the document is to present United Energy's demand side engagement strategy outlining United Energy's process for engaging and consulting with non-network service providers, and for investigating, developing, assessing and reporting on non-network options as alternatives to network augmentation","Presents our demand side engagement strategy outlining our process for engaging and consulting with non-network service providers, and for investigating, developing, assessing and reporting on non-network options as alternatives to network augmentation.","Yes"]

{"sheet":"7.4 Shared Assets","index":38,"n_rows":26,"n_cols":19,"rows_kept":26,"cut":false,"hidden":false,"merged":[[6,1,7,1],[6,2,7,2],[6,3,6,10],[6,11,6,18],[25,1,26,1],[25,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[32,2,32,8],[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service","Shared asset unregulated revenue  ($0's, nominal)",null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Shared asset unregulated revenue  ($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  ($0's, real June 2021)"}]
[null,null,null,{"$f":"PRCP_y1","v":"2011-12"},{"$f":"PRCP_y2","v":"2012-13"},{"$f":"PRCP_y3","v":"2013-14"},{"$f":"PRCP_y4","v":"2014-15"},{"$f":"PRCP_y5","v":"2015-16"},{"$f":"CRCP_y1","v":"2016-17"},{"$f":"CRCP_y2","v":"2017-18"},{"$f":"CRCP_y3","v":"2018-19"},{"$f":"CRCP_y4","v":"2019-20"},{"$f":"CRCP_y5","v":"2020-21"},{"$f":"FRCP_y1","v":"2021-22"},{"$f":"FRCP_y2","v":"2022-23"},{"$f":"FRCP_y3","v":"2023-24"},{"$f":"FRCP_y4","v":"2024-25"},{"$f":"FRCP_y5","v":"2025-26"},{"$f":"CONCATENATE(\"Total \",dms_Header_Span)","v":"Total 2021-22 to 2025-26"}]
[null,"Joint Use Poles","Network poles used to carry the service cables of telco providers.",5231907.8599999994,5378658.620000001,5359535.7050000001,5603382.1633333331,5807930.2933333339,8236691.1849999996,9789196.589999998,8930866.0899557509,9458173.1013995223,{"$f":"L9","v":9458173.1013995223},{"$f":"M9","v":9458173.1013995223},9458173.1013995223,9458173.1013995223,9458173.1013995223,9458173.1013995223,{"$f":"SUM(N9:R9)","v":47290865.506997615}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]

{"sheet":"7.7 TSS-LRMC","index":39,"n_rows":152,"n_cols":22,"rows_kept":152,"cut":false,"hidden":false,"merged":[[5,3,6,4],[10,1,11,1],[10,2,10,21],[21,1,22,1],[21,2,21,21],[32,1,33,1],[32,2,32,21],[109,2,109,21],[124,2,124,21],[139,2,139,21],[46,1,47,1],[46,2,46,21],[66,1,67,1],[66,2,66,21],[86,1,87,1],[86,2,86,21]]}
[null,{"$f":"INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"dms_Header_Span","v":"2021-22 to 2025-26"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[null,null,null,{"$f":"\"Is \"&dms_TradingName&\" using the 'Average Incremental Cost' approach?\"","v":"Is United Energy using the 'Average Incremental Cost' approach?"},null,"YES / NO?"]
[null,null,null,null,null,"NO"]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C12,4)+1)&\"-\"&MID(C12,3,2)+2),VALUE(LEFT(C12,4)+1))","v":"2020-21"},"2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37","2037-38","2038-39"]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C23,4)+1)&\"-\"&MID(C23,3,2)+2),VALUE(LEFT(C23,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D23,4)+1)&\"-\"&MID(D23,3,2)+2),VALUE(LEFT(D23,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E23,4)+1)&\"-\"&MID(E23,3,2)+2),VALUE(LEFT(E23,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F23,4)+1)&\"-\"&MID(F23,3,2)+2),VALUE(LEFT(F23,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G23,4)+1)&\"-\"&MID(G23,3,2)+2),VALUE(LEFT(G23,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H23,4)+1)&\"-\"&MID(H23,3,2)+2),VALUE(LEFT(H23,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I23,4)+1)&\"-\"&MID(I23,3,2)+2),VALUE(LEFT(I23,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J23,4)+1)&\"-\"&MID(J23,3,2)+2),VALUE(LEFT(J23,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K23,4)+1)&\"-\"&MID(K23,3,2)+2),VALUE(LEFT(K23,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L23,4)+1)&\"-\"&MID(L23,3,2)+2),VALUE(LEFT(L23,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M23,4)+1)&\"-\"&MID(M23,3,2)+2),VALUE(LEFT(M23,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N23,4)+1)&\"-\"&MID(N23,3,2)+2),VALUE(LEFT(N23,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O23,4)+1)&\"-\"&MID(O23,3,2)+2),VALUE(LEFT(O23,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P23,4)+1)&\"-\"&MID(P23,3,2)+2),VALUE(LEFT(P23,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q23,4)+1)&\"-\"&MID(Q23,3,2)+2),VALUE(LEFT(Q23,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R23,4)+1)&\"-\"&MID(R23,3,2)+2),VALUE(LEFT(R23,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S23,4)+1)&\"-\"&MID(S23,3,2)+2),VALUE(LEFT(S23,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T23,4)+1)&\"-\"&MID(T23,3,2)+2),VALUE(LEFT(T23,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U23,4)+1)&\"-\"&MID(U23,3,2)+2),VALUE(LEFT(U23,4)+1))","v":"2038-39"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C34,4)+1)&\"-\"&MID(C34,3,2)+2),VALUE(LEFT(C34,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D34,4)+1)&\"-\"&MID(D34,3,2)+2),VALUE(LEFT(D34,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E34,4)+1)&\"-\"&MID(E34,3,2)+2),VALUE(LEFT(E34,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F34,4)+1)&\"-\"&MID(F34,3,2)+2),VALUE(LEFT(F34,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G34,4)+1)&\"-\"&MID(G34,3,2)+2),VALUE(LEFT(G34,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H34,4)+1)&\"-\"&MID(H34,3,2)+2),VALUE(LEFT(H34,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I34,4)+1)&\"-\"&MID(I34,3,2)+2),VALUE(LEFT(I34,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J34,4)+1)&\"-\"&MID(J34,3,2)+2),VALUE(LEFT(J34,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K34,4)+1)&\"-\"&MID(K34,3,2)+2),VALUE(LEFT(K34,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L34,4)+1)&\"-\"&MID(L34,3,2)+2),VALUE(LEFT(L34,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M34,4)+1)&\"-\"&MID(M34,3,2)+2),VALUE(LEFT(M34,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N34,4)+1)&\"-\"&MID(N34,3,2)+2),VALUE(LEFT(N34,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O34,4)+1)&\"-\"&MID(O34,3,2)+2),VALUE(LEFT(O34,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P34,4)+1)&\"-\"&MID(P34,3,2)+2),VALUE(LEFT(P34,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q34,4)+1)&\"-\"&MID(Q34,3,2)+2),VALUE(LEFT(Q34,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R34,4)+1)&\"-\"&MID(R34,3,2)+2),VALUE(LEFT(R34,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S34,4)+1)&\"-\"&MID(S34,3,2)+2),VALUE(LEFT(S34,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T34,4)+1)&\"-\"&MID(T34,3,2)+2),VALUE(LEFT(T34,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U34,4)+1)&\"-\"&MID(U34,3,2)+2),VALUE(LEFT(U34,4)+1))","v":"2038-39"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"Total capex"]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C48,4)+1)&\"-\"&MID(C48,3,2)+2),VALUE(LEFT(C48,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D48,4)+1)&\"-\"&MID(D48,3,2)+2),VALUE(LEFT(D48,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E48,4)+1)&\"-\"&MID(E48,3,2)+2),VALUE(LEFT(E48,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F48,4)+1)&\"-\"&MID(F48,3,2)+2),VALUE(LEFT(F48,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G48,4)+1)&\"-\"&MID(G48,3,2)+2),VALUE(LEFT(G48,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H48,4)+1)&\"-\"&MID(H48,3,2)+2),VALUE(LEFT(H48,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I48,4)+1)&\"-\"&MID(I48,3,2)+2),VALUE(LEFT(I48,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J48,4)+1)&\"-\"&MID(J48,3,2)+2),VALUE(LEFT(J48,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K48,4)+1)&\"-\"&MID(K48,3,2)+2),VALUE(LEFT(K48,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L48,4)+1)&\"-\"&MID(L48,3,2)+2),VALUE(LEFT(L48,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M48,4)+1)&\"-\"&MID(M48,3,2)+2),VALUE(LEFT(M48,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N48,4)+1)&\"-\"&MID(N48,3,2)+2),VALUE(LEFT(N48,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O48,4)+1)&\"-\"&MID(O48,3,2)+2),VALUE(LEFT(O48,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P48,4)+1)&\"-\"&MID(P48,3,2)+2),VALUE(LEFT(P48,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q48,4)+1)&\"-\"&MID(Q48,3,2)+2),VALUE(LEFT(Q48,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R48,4)+1)&\"-\"&MID(R48,3,2)+2),VALUE(LEFT(R48,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S48,4)+1)&\"-\"&MID(S48,3,2)+2),VALUE(LEFT(S48,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T48,4)+1)&\"-\"&MID(T48,3,2)+2),VALUE(LEFT(T48,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U48,4)+1)&\"-\"&MID(U48,3,2)+2),VALUE(LEFT(U48,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C68,4)+1)&\"-\"&MID(C68,3,2)+2),VALUE(LEFT(C68,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D68,4)+1)&\"-\"&MID(D68,3,2)+2),VALUE(LEFT(D68,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E68,4)+1)&\"-\"&MID(E68,3,2)+2),VALUE(LEFT(E68,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F68,4)+1)&\"-\"&MID(F68,3,2)+2),VALUE(LEFT(F68,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G68,4)+1)&\"-\"&MID(G68,3,2)+2),VALUE(LEFT(G68,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H68,4)+1)&\"-\"&MID(H68,3,2)+2),VALUE(LEFT(H68,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I68,4)+1)&\"-\"&MID(I68,3,2)+2),VALUE(LEFT(I68,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J68,4)+1)&\"-\"&MID(J68,3,2)+2),VALUE(LEFT(J68,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K68,4)+1)&\"-\"&MID(K68,3,2)+2),VALUE(LEFT(K68,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L68,4)+1)&\"-\"&MID(L68,3,2)+2),VALUE(LEFT(L68,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M68,4)+1)&\"-\"&MID(M68,3,2)+2),VALUE(LEFT(M68,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N68,4)+1)&\"-\"&MID(N68,3,2)+2),VALUE(LEFT(N68,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O68,4)+1)&\"-\"&MID(O68,3,2)+2),VALUE(LEFT(O68,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P68,4)+1)&\"-\"&MID(P68,3,2)+2),VALUE(LEFT(P68,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q68,4)+1)&\"-\"&MID(Q68,3,2)+2),VALUE(LEFT(Q68,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R68,4)+1)&\"-\"&MID(R68,3,2)+2),VALUE(LEFT(R68,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S68,4)+1)&\"-\"&MID(S68,3,2)+2),VALUE(LEFT(S68,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T68,4)+1)&\"-\"&MID(T68,3,2)+2),VALUE(LEFT(T68,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U68,4)+1)&\"-\"&MID(U68,3,2)+2),VALUE(LEFT(U68,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C88,4)+1)&\"-\"&MID(C88,3,2)+2),VALUE(LEFT(C88,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D88,4)+1)&\"-\"&MID(D88,3,2)+2),VALUE(LEFT(D88,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E88,4)+1)&\"-\"&MID(E88,3,2)+2),VALUE(LEFT(E88,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F88,4)+1)&\"-\"&MID(F88,3,2)+2),VALUE(LEFT(F88,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G88,4)+1)&\"-\"&MID(G88,3,2)+2),VALUE(LEFT(G88,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H88,4)+1)&\"-\"&MID(H88,3,2)+2),VALUE(LEFT(H88,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I88,4)+1)&\"-\"&MID(I88,3,2)+2),VALUE(LEFT(I88,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J88,4)+1)&\"-\"&MID(J88,3,2)+2),VALUE(LEFT(J88,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K88,4)+1)&\"-\"&MID(K88,3,2)+2),VALUE(LEFT(K88,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L88,4)+1)&\"-\"&MID(L88,3,2)+2),VALUE(LEFT(L88,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M88,4)+1)&\"-\"&MID(M88,3,2)+2),VALUE(LEFT(M88,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N88,4)+1)&\"-\"&MID(N88,3,2)+2),VALUE(LEFT(N88,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O88,4)+1)&\"-\"&MID(O88,3,2)+2),VALUE(LEFT(O88,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P88,4)+1)&\"-\"&MID(P88,3,2)+2),VALUE(LEFT(P88,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q88,4)+1)&\"-\"&MID(Q88,3,2)+2),VALUE(LEFT(Q88,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R88,4)+1)&\"-\"&MID(R88,3,2)+2),VALUE(LEFT(R88,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S88,4)+1)&\"-\"&MID(S88,3,2)+2),VALUE(LEFT(S88,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T88,4)+1)&\"-\"&MID(T88,3,2)+2),VALUE(LEFT(T88,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U88,4)+1)&\"-\"&MID(U88,3,2)+2),VALUE(LEFT(U88,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C111,4)+1)&\"-\"&MID(C111,3,2)+2),VALUE(LEFT(C111,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D111,4)+1)&\"-\"&MID(D111,3,2)+2),VALUE(LEFT(D111,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E111,4)+1)&\"-\"&MID(E111,3,2)+2),VALUE(LEFT(E111,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F111,4)+1)&\"-\"&MID(F111,3,2)+2),VALUE(LEFT(F111,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G111,4)+1)&\"-\"&MID(G111,3,2)+2),VALUE(LEFT(G111,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H111,4)+1)&\"-\"&MID(H111,3,2)+2),VALUE(LEFT(H111,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I111,4)+1)&\"-\"&MID(I111,3,2)+2),VALUE(LEFT(I111,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J111,4)+1)&\"-\"&MID(J111,3,2)+2),VALUE(LEFT(J111,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K111,4)+1)&\"-\"&MID(K111,3,2)+2),VALUE(LEFT(K111,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L111,4)+1)&\"-\"&MID(L111,3,2)+2),VALUE(LEFT(L111,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M111,4)+1)&\"-\"&MID(M111,3,2)+2),VALUE(LEFT(M111,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N111,4)+1)&\"-\"&MID(N111,3,2)+2),VALUE(LEFT(N111,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O111,4)+1)&\"-\"&MID(O111,3,2)+2),VALUE(LEFT(O111,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P111,4)+1)&\"-\"&MID(P111,3,2)+2),VALUE(LEFT(P111,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q111,4)+1)&\"-\"&MID(Q111,3,2)+2),VALUE(LEFT(Q111,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R111,4)+1)&\"-\"&MID(R111,3,2)+2),VALUE(LEFT(R111,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S111,4)+1)&\"-\"&MID(S111,3,2)+2),VALUE(LEFT(S111,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T111,4)+1)&\"-\"&MID(T111,3,2)+2),VALUE(LEFT(T111,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U111,4)+1)&\"-\"&MID(U111,3,2)+2),VALUE(LEFT(U111,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C126,4)+1)&\"-\"&MID(C126,3,2)+2),VALUE(LEFT(C126,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D126,4)+1)&\"-\"&MID(D126,3,2)+2),VALUE(LEFT(D126,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E126,4)+1)&\"-\"&MID(E126,3,2)+2),VALUE(LEFT(E126,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F126,4)+1)&\"-\"&MID(F126,3,2)+2),VALUE(LEFT(F126,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G126,4)+1)&\"-\"&MID(G126,3,2)+2),VALUE(LEFT(G126,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H126,4)+1)&\"-\"&MID(H126,3,2)+2),VALUE(LEFT(H126,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I126,4)+1)&\"-\"&MID(I126,3,2)+2),VALUE(LEFT(I126,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J126,4)+1)&\"-\"&MID(J126,3,2)+2),VALUE(LEFT(J126,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K126,4)+1)&\"-\"&MID(K126,3,2)+2),VALUE(LEFT(K126,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L126,4)+1)&\"-\"&MID(L126,3,2)+2),VALUE(LEFT(L126,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M126,4)+1)&\"-\"&MID(M126,3,2)+2),VALUE(LEFT(M126,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N126,4)+1)&\"-\"&MID(N126,3,2)+2),VALUE(LEFT(N126,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O126,4)+1)&\"-\"&MID(O126,3,2)+2),VALUE(LEFT(O126,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P126,4)+1)&\"-\"&MID(P126,3,2)+2),VALUE(LEFT(P126,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q126,4)+1)&\"-\"&MID(Q126,3,2)+2),VALUE(LEFT(Q126,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R126,4)+1)&\"-\"&MID(R126,3,2)+2),VALUE(LEFT(R126,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S126,4)+1)&\"-\"&MID(S126,3,2)+2),VALUE(LEFT(S126,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T126,4)+1)&\"-\"&MID(T126,3,2)+2),VALUE(LEFT(T126,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U126,4)+1)&\"-\"&MID(U126,3,2)+2),VALUE(LEFT(U126,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2021"}]
[null,null,{"$f":"CRCP_y4","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C141,4)+1)&\"-\"&MID(C141,3,2)+2),VALUE(LEFT(C141,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(D141,4)+1)&\"-\"&MID(D141,3,2)+2),VALUE(LEFT(D141,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(E141,4)+1)&\"-\"&MID(E141,3,2)+2),VALUE(LEFT(E141,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F141,4)+1)&\"-\"&MID(F141,3,2)+2),VALUE(LEFT(F141,4)+1))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(G141,4)+1)&\"-\"&MID(G141,3,2)+2),VALUE(LEFT(G141,4)+1))","v":"2024-25"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(H141,4)+1)&\"-\"&MID(H141,3,2)+2),VALUE(LEFT(H141,4)+1))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(I141,4)+1)&\"-\"&MID(I141,3,2)+2),VALUE(LEFT(I141,4)+1))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(J141,4)+1)&\"-\"&MID(J141,3,2)+2),VALUE(LEFT(J141,4)+1))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(K141,4)+1)&\"-\"&MID(K141,3,2)+2),VALUE(LEFT(K141,4)+1))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(L141,4)+1)&\"-\"&MID(L141,3,2)+2),VALUE(LEFT(L141,4)+1))","v":"2029-30"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(M141,4)+1)&\"-\"&MID(M141,3,2)+2),VALUE(LEFT(M141,4)+1))","v":"2030-31"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(N141,4)+1)&\"-\"&MID(N141,3,2)+2),VALUE(LEFT(N141,4)+1))","v":"2031-32"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(O141,4)+1)&\"-\"&MID(O141,3,2)+2),VALUE(LEFT(O141,4)+1))","v":"2032-33"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(P141,4)+1)&\"-\"&MID(P141,3,2)+2),VALUE(LEFT(P141,4)+1))","v":"2033-34"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(Q141,4)+1)&\"-\"&MID(Q141,3,2)+2),VALUE(LEFT(Q141,4)+1))","v":"2034-35"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(R141,4)+1)&\"-\"&MID(R141,3,2)+2),VALUE(LEFT(R141,4)+1))","v":"2035-36"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(S141,4)+1)&\"-\"&MID(S141,3,2)+2),VALUE(LEFT(S141,4)+1))","v":"2036-37"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(T141,4)+1)&\"-\"&MID(T141,3,2)+2),VALUE(LEFT(T141,4)+1))","v":"2037-38"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(U141,4)+1)&\"-\"&MID(U141,3,2)+2),VALUE(LEFT(U141,4)+1))","v":"2038-39"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]

{"sheet":"8.2 Capex","index":40,"n_rows":61,"n_cols":5,"rows_kept":61,"cut":false,"hidden":false,"merged":[[8,2,8,3],[7,2,7,4]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"United Energy"}]
[null,{"$f":"CONCATENATE(\"Annual Reporting RIN Response \",IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result)))","v":"Annual Reporting RIN Response 2021-22 to 2025-26"}]
[null,"8.2 - CAPEX"]
[]
[null,"8.2.7 - IMMEDIATE EXPENSING OF CAPEX"]
[null,"ESTIMATED - AS INCURRED"]
[null,null,"Estimate"]
[null,null,"CALENDAR YEARS",null,"6 MONTHS"]
[null,null,2019,2020,"1 January 2021 \nto \n30 June 2021"]
[null,"Subtransmission",3502641.9495572443,{"$f":"C11","v":3502641.9495572443},{"$f":"D11/2","v":1751320.9747786222}]
[null,"Distribution system assets",24788926.703239989,{"$f":"C12","v":24788926.703239989},{"$f":"D12/2","v":12394463.351619994}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",{"$f":"SUM(C11:C60)","v":28291568.652797233},{"$f":"SUM(D11:D60)","v":28291568.652797233},14145784.326398617]

{"sheet":"Sheet1","index":41,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}