{"text_format":"1","workbook":"xlsx","n_sheets":23,"sheets":["AER only","Instructions","Contents","Business & other details","2.1 Expenditure summary","2.2 Repex","2.3(a) Augex","2.3(b) Augex","2.5 Connections","2.6 Non-network","2.7 Vegetation management","2.8 Maintenance","2.9 Emergency Response","2.10 network overheads","2.11 Labour","2.12 Input tables","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.2 Asset Age Profile","5.4 MD & utilisation-Spatial","6.3 Sustained interruptions","Amendments"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":738,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AER only","index":0,"n_rows":148,"n_cols":41,"rows_kept":148,"cut":false,"hidden":true,"merged":[[56,35,60,35],[64,35,65,35],[70,14,70,15],[70,24,70,27],[108,1,108,8],[53,35,55,35],[0,1,0,11],[4,27,4,38],[6,27,6,30],[6,33,6,37],[51,24,51,28],[51,29,51,32],[52,1,52,5],[52,14,52,21],[52,24,52,28],[52,29,52,32],[53,2,53,3]]}
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,"2018-03-28","major changes to accommodate STPIS"]
[null,null,"Template Version",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_ContactName1_List","dms_ContactPh1_List","dms_ContactEmail_List","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5","dms_Public_Lighting_List","Column1"]
[null,"ActewAGL Distribution","ActewAGL Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,null,null,null,"NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution"]
[null,"ActewAGL Distribution (Tx Assets)","ActewAGL Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,null,null,null,"NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Distribution (Tx Assets)"]
[null,"ActewAGL Gas","ActewAGL Gas",76670568688,"ACT","Gas","Distribution","Weighted average price cap","Financial","June",5,5,"x",null,"40 Bunda Street",null,"CANBERRA","ACT",2600,"GPO BOX 366",null,"CANBERRA","ACT",2601,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ActewAGL Gas"]
[null,"AEMO","Australian Energy Market Operator Ltd",94072010327,"Vic","Electricity","Transmission","-","Financial","March",5,5,"x","-","Level 22","530 Collins Street","MELBOURNE","VIC",3000,"GPO Box 2008",null,"MELBOURNE","VIC",3001,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AEMO"]
[null,"AGN (Albury and Victoria)","Australian Gas Networks Limited (reporting data for Albury and Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Albury)"]
[null,"AGN (Albury)","Australian Gas Networks Limited (reporting data for Albury)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"AGN (SA)","Australian Gas Networks Limited (reporting data for SA)",19078551685,"SA","Gas","Distribution","Weighted average price cap","Financial","June",5,5,5,"distribution determination","Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (SA)"]
[null,"AGN (Victoria)","Australian Gas Networks Limited (reporting data for Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA",5000,"PO Box 6468","Halifax Street","ADELAIDE","SA",5000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AGN (Victoria)"]
[null,"Amadeus","APT Pipelines (NT) Pty Ltd",39009737393,"NT","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Amadeus"]
[null,"APA GasNet","APA GasNet Australia (Operations) Pty Ltd","065083009","Vic","Gas","Transmission","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","APA GasNet"]
[null,"Ausgrid","Ausgrid",78508211731,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,null,null,null,"YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ausgrid"]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW",2001,null,null,null,"YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Ausgrid (Tx Assets)"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","VIC",8001,null,null,null,null,"YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","AusNet (D)"]
[null,"AusNet (Gas)","AusNet Gas Services","086015036","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"X",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (Gas)"]
[null,"AusNet (T)","Ausnet Services (Transmission) Ltd",48116124362,"Vic","Electricity","Transmission","Revenue cap","Financial","March",5,5,2,"transmission determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic",3006,"Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic",8001,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","AusNet (T)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"-","Electricity","Distribution","Revenue cap","Financial","June",5,5,2,"distribution determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co."]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic",3000,"PO Box 123",null,"MELBOURNE","VIC",3000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Australian Distribution Co. (Vic)"]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"-","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","123 Straight Street",null,"SYDNEY","NSW",2000,"PO Box 123",null,"SYDNEY","NSW",2000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Australian Transmission Co."]
[null,"Central Ranges Pipeline (D)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",15,5,5,"distribution determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"Central Ranges Pipeline (T)","Central Ranges Pipeline Pty Ltd",108218355,"NSW","Gas","Distribution","Weighted average price cap","Financial","June",14,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO"]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked Bag 14090",null,"MELBOURNE","VIC",8001,null,null,null,"YES","YES","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","CitiPower"]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",9,5,5,"transmission determination","Level 19, HSBC Building","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Directlink"]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","52-55 East Terrace","Rymill Park","ADELAIDE","SA",5000,"PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","ElectraNet"]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","51 Huntingwood Drive",null,"HUNTINGWOOD","NSW",2148,"PO Box 811",null,"SEVEN HILLS","NSW",1730,null,null,null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Endeavour Energy"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","26 Reddacliff Street",null,"NEWSTEAD","Qld",4006,"26 Reddacliff Street",null,"NEWSTEAD","QLD",4006,null,null,null,"YES","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","22 Walker Street",null,"TOWNSVILLE","Qld",4810,"Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,null,null,null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Ergon Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","8 Buller Street",null,"PORT MACQUARIE","NSW",2444,"PO Box 5730",null,"PORT MACQUARIE","NSW",2444,null,null,null,"NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Essential Energy"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","VIC",3000,"PO Box 16182",null,"MELBOURNE","VIC",8001,null,null,null,"NO","NO","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Jemena Electricity"]
[null,"JGN","Jemena Gas Networks (NSW) Ltd","003 004 322","NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","JGN"]
[null,"Multinet Gas","Multinet Gas (DB No.1) Pty Ltd (ACN 086 026 986), Multinet Gas (DB No.2) Pty Ltd (ACN 086 230 122)","086026986","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"43-45 Centreway",null,"MT WAVERLEY","Vic",3149,null,null,null,null,null,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Multinet Gas"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Murraylink"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,"x","distribution determination","GPO Box 1921",null,"DARWIN","NT",801,"GPO Box 1921",null,"DARWIN","NT",801,null,null,null,"YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Power and Water"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic",3000,"Locked bag 14090",null,"MELBOURNE","VIC",8001,null,null,null,null,null,"YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","Powercor Australia"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","33 Harold St",null,"VIRGINIA","Qld",4014,"PO Box 1193",null,"VIRGINIA","QLD",4014,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Powerlink"]
[null,"Roma to Brisbane Pipeline","APT Petroleum Pipelines Limited t/a Roma to Brisbane Pipeline","009 737 393","Qld","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","580 George Street",null,"SYDNEY","NSW",2000,"PO Box R41",null,"ROYAL EXCHANGE","NSW",1225,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","Roma to Brisbane Pipeline"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","1 Anzac Highway",null,"KESWICK","SA",5035,"GPO Box 77",null,"ADELAIDE","SA",5000,null,null,null,"NO","NO","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","SA Power Networks"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,null,null,null,"YES","YES","YES","YES","YES",null,"Critical Infrastructure","High density commercial","Urban","High density rural","Low density rural","YES","TasNetworks (D)"]
[null,"TasNetworks (T)","TasNetworks (T)",24167357299,"Tas","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","1-7 Maria Street",null,"LENAH VALLEY","Tas",7008,"PO Box 606",null,"MOONAH","Tas",7009,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TasNetworks (T)"]
[null,"TransGrid","NSW Electricity Networks Operations Pty Ltd trading as TransGrid","70 250 995 390","NSW","Electricity","Transmission","Revenue cap","Financial","June",4,5,5,"transmission determination","180 Thomas Street",null,"SYDNEY","NSW",2000,"PO Box A1000",null,"SYDNEY SOUTH","NSW",1235,null,null,null,"NO","NO","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"NO","TransGrid"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 3","6 Nexus Court","MULGRAVE","Vic",3149,"PO Box 449",null,"MOUNT WAVERLEY","VIC",3170,null,null,null,"NO","NO","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"YES","United Energy"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For EB & Reset RINs only",null,null,null,null,"For AARs only"]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68",null,null,null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2014-15"},null,null,null,null,null,null,"Drop down selector box for CA & Reset RINs.","For CA & Reset RINs only",null,null,null,null,null,null,null,null,null,"for DNSP only",null,null,null,null,"For DNSPs only",null,null,null,null,null,"Reason for interruption","dms_Reason_Interruption_Detailed","dms_Reason_Interruption","dms_STPIS_Exclusion_List","dms_020301_ProjectType_List","dms_020302_ProjectType_List"]
[null,"dms_Model_List ","DELETE NR 'CRY' IF NOT AN ANNUAL RIN (EB, CA , ARR)",null,"dms_RYE_Formula_Result",null,null,null,null,null,null,null,null,"dms_0203_ProjectType","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020603_01_UOM","dms_020701_01_UOM","dms_020701_02_UOM","dms_040102_01_UOM","dms_040102_04_UOM","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM","dms_030605_UOM","dms_03060703_UOM",null,null,null,null,"Animal","Animal impact","Animal","Weather","New substation establishment","New line on new route - single circuit"]
[null,"ARR","ANNUAL REPORTING STATEMENT",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"2018"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","0's","days","minutes/customer","minutes/customer","Customer / km","%","km","number","number",null,null,null,null,null,"Animal nesting/burrowing, etc and other","Asset failure","Equipment failure","Capacity upgrade","New line on new route - dual circuit"]
[null,"CA","CATEGORY ANALYSIS",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"2018"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - dual circuit","Circuit line length in km","0's","0's","0's","0's","0's","0's","0's","0's","0's","minutes/customer","minutes/customer","MWh/customer","Number of spans",null,"number","number",null,null,null,null,null,"Other","Other","Operational error","Voltage upgrade","New line on new route - other"]
[null,"CPI","CPI",null,null,null,null,null,null,null,null,null,null,"New line on new route - other","Circuit line length in km","MVA added","MVA added","MVA added","MVA added","0's","km","km","0's","$0s","interruptions/customer","interruptions/customer","kVA / customer","Number of spans",null,"number","number",null,null,null,null,"Asset failure","LV","Overloads","Vegetation","Other","Line rebuild over existing route - single circuit"]
[null,"EB","ECONOMIC BENCHMARKING",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":"2018"},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Line rebuild over existing route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","km","km","$0s","0's","interruptions/customer","interruptions/customer",null,"Number of spans",null,"number","number",null,null,null,null,null,"Distribution substation","Planned","Animals",null,"Line rebuild over existing route - dual circuit"]
[null,"PTRM","POST TAX REVENUE MODEL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Line rebuild over existing route - dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","(per cent)","0's","0's",null,null,null,null,null,"Number of spans",null,"number","(per cent)",null,null,null,null,null,"HV","Network business","Third party impacts",null,"Reconductor - Single circuit"]
[null,"Reset","REGULATORY REPORTING STATEMENT",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Reconductor - Single circuit","Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,"years","years",null,null,null,null,null,"Years",null,"number",null,null,null,null,null,null,"Zone substation","Third party","Transmission failure",null,"Reconductor - Dual circuit"]
[null,"RFM","ROLL FORWARD MODEL",null,{"$f":"LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)","v":"2018"},"=LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)",null,null,null,null,null,null,null,"Reconductor - Dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,"Years",null,"number",null,null,null,null,null,null,"Subtransmission","Unknown","Load shedding",null,"Reconductor - Other"]
[null,"WACC","WEIGHTED AVERAGE COST OF CAPITAL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2025"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Other",null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,null,null,null,null,null,null,null,"Trees",null,"number",null,null,null,null,null,"Other","insert description of 'other'","Vegetation","Inter-distributor connection failure",null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,null,null,"Trees",null,"number",null,null,null,null,null,"Overloads","-","Weather","Other",null,"Line upgrade - voltage upgrade"]
[null,"dms_DataQuality_List",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,"$0s",null,null,null,null,null,null,null,null,null,"Defects",null,"number",null,null,null,null,null,"Planned","-","2 - STPIS Exclusion (3.3)(a)",null,null,"Line upgrade - capacity"]
[null,"Actual",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,"Defects",null,"number",null,null,null,null,null,"Network business","Network error","3 - STPIS Exclusion (3.3)(a)",null,null,"String spare circuit"]
[null,"Estimate",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"number",null,null,null,null,null,null,"Switching and protection error","4 - STPIS Exclusion (3.3)(a)",null,null,"Other"]
[null,"Consolidated",null,null,null,null,null,null,null,null,null,null,null,null,null,"$0s",null,null,null,null,null,null,null,null,null,null,null,"km",null,"(per cent)",null,null,null,null,null,"Third party","Fire","5 - STPIS Exclusion (3.3)(a)"]
[null,"Recast",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,"(per cent)",null,null,null,null,null,null,"Other","6 - STPIS Exclusion (3.3)(a)"]
[null,"Public",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dig-in","7 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unauthorised access"]
[null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above.",null,null,null,null,null,null,null,null,null,null,null,"For PTRM files - this field set the text for the named range \"DMS_Xfactor\" which in all cases is simply the text \"x factors\" - this saves putting in each old gas PTRM file ",null,null,null,null,null,null,null,null,null,"for TNSP only",null,null,null,null,null,null,null,null,null,null,null,"Vehicle impact"]
[null,"dms_SourceList","dms_FormControl_Choices",null,null,null,null,null,null,null,null,null,null,null,"DMS_Xfactor",null,null,null,null,null,null,null,null,null,"dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM",null,null,null,null,null,null,null,"Unknown","Unknown"]
[null,"After appeal","Revenue cap",null,null,null,null,null,null,null,null,null,null,null,"x factors",null,null,null,null,null,null,null,null,null,"%",null,"Number of spans","km",null,null,null,null,null,null,null,"Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,"Draft decision","Revenue yield",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Years","%",null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility"]
[null,"Final decision","Weighted average price cap",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Trees","km",null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,"PTRM update 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"Defects","number",null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,"PTRM update 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans",null,null,null,null,null,null,null,null,"Weather"]
[null,"PTRM update 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"km",null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"km",null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans",null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,"Regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[null,"Reporting",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Revised regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[]
[]
[]
[null,"These are indeces and lookup values for various dates. All step from the value placed in FRCP_y1 on the business and other details worksheet",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"},null,null,null,null,null,null,null,null,"These date tables are currently used in the Recast templates to provide column headings and conditional formatting"]
[null,"dms_FRCPlength_Num_List","dms_FinalYear_List","dms_CRCPlength_Num_List","dms_CFinalYear_List","dms_FRCP_years",null,"dms_CRCP_years",null,"dms_CRCP_index",null,"CRY from input cell on business sheet","CRY - financial","dms_FinYears","CRY calendar","dms_CalYears",null,null,null,null,null,null,null,null,"These \"row descriptions\" are the column headings in the various templates but become row descriptions in the ETL process"]
[null,1,"dms_FRCP_y1",1,"CRCP_y1",{"$f":"FRCP_y1","v":"2020-21"},"dms_FRCP_y1",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)-1)&\"-\"&TEXT(VALUE(MID(dms_FRCP_y1,3,2)),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)-1))","v":"2019-20"},"dms_CRCP_yZ",1,null,{"$f":"CRY","v":"2017-18"},{"$f":"VALUE(LEFT(CRY,4))&\"-\"&TEXT(MID(CRY,3,2)+1,\"00\")","v":"2017-18"},"dms_CRYf_y1",{"$f":"VALUE(LEFT(CRY,4)+1)","v":2018},"dms_CRYc_y1",null,null,null,null,null,null,null,null,null,"Table 6.3 sustained interruptions - row descriptions"]
[null,2,"dms_FRCP_y2",2,"CRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y1,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)+1))","v":"2021-22"},"dms_FRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yZ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yZ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yZ,4)-1))","v":"2018-19"},"dms_CRCP_yY",2,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y1,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y1,3,2)+2,\"00\")","v":"2018-19"},"dms_CRYf_y2",{"$f":"VALUE(LEFT(dms_CRYc_y1,4)+1)","v":2019},"dms_CRYc_y2",null,null,null,null,null,null,null,null,null,"dms_060301_CustNo_Affected_Row","dms_060301_Avg_Duration_Sustained_Int_Row","dms_060301_Effect_unplanned_SAIDI_Row","dms_060301_Effect_unplanned_SAIFI_Row"]
[null,3,"=IF(dms_Model=\"ARR\",15,9)",3,"=IF(dms_Model=\"ARR\",15,9)",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y2,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y2,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y2,4)+1))","v":"2022-23"},"dms_FRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yY,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yY,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yY,4)-1))","v":"2017-18"},"dms_CRCP_yX",3,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y2,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y2,3,2)+2,\"00\")","v":"2019-20"},"dms_CRYf_y3",{"$f":"VALUE(LEFT(dms_CRYc_y2,4)+1)","v":2020},"dms_CRYc_y3",null,null,null,null,null,null,null,null,null,"Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI"]
[null,4,"dms_FRCP_y4",4,"CRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y3,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y3,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y3,4)+1))","v":"2023-24"},"dms_FRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yX,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yX,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yX,4)-1))","v":"2016-17"},"dms_CRCP_yW",4,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y3,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y3,3,2)+2,\"00\")","v":"2020-21"},"dms_CRYf_y4",{"$f":"VALUE(LEFT(dms_CRYc_y3,4)+1)","v":2021},"dms_CRYc_y4"]
[null,5,"dms_FRCP_y5",5,"CRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y4,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y4,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y4,4)+1))","v":"2024-25"},"dms_FRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yW,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yW,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yW,4)-1))","v":"2015-16"},"dms_CRCP_yV",5,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y4,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y4,3,2)+2,\"00\")","v":"2021-22"},"dms_CRYf_y5",{"$f":"VALUE(LEFT(dms_CRYc_y4,4)+1)","v":2022},"dms_CRYc_y5"]
[null,6,"dms_FRCP_y6",6,"CRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y5,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y5,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y5,4)+1))","v":"2025-26"},"dms_FRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yV,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yV,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yV,4)-1))","v":"2014-15"},"dms_CRCP_yU",6,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y5,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y5,3,2)+2,\"00\")","v":"2022-23"},"dms_CRYf_y6",{"$f":"VALUE(LEFT(dms_CRYc_y5,4)+1)","v":2023},"dms_CRYc_y6"]
[null,7,"dms_FRCP_y7",7,"CRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y6,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y6,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y6,4)+1))","v":"2026-27"},"dms_FRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yU,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yU,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yU,4)-1))","v":"2013-14"},"dms_CRCP_yT",7,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y6,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y6,3,2)+2,\"00\")","v":"2023-24"},"dms_CRYf_y7",{"$f":"VALUE(LEFT(dms_CRYc_y6,4)+1)","v":2024},"dms_CRYc_y7",null,null,null,null,null,null,null,null,null,"Table 6.1 telephone answering - row descriptions and start date"]
[null,8,"dms_FRCP_y8",8,"CRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y7,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y7,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y7,4)+1))","v":"2027-28"},"dms_FRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yT,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yT,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yT,4)-1))","v":"2012-13"},"dms_CRCP_yS",8,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y7,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y7,3,2)+2,\"00\")","v":"2024-25"},"dms_CRYf_y8",{"$f":"VALUE(LEFT(dms_CRYc_y7,4)+1)","v":2025},"dms_CRYc_y8",null,null,null,null,null,null,null,null,null,"dms_060101_Rows","dms_060102_Rows","dms_060101_StartDateTxt"]
[null,9,"dms_FRCP_y9",9,"CRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y8,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y8,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y8,4)+1))","v":"2028-29"},"dms_FRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yS,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yS,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yS,4)-1))","v":"2011-12"},"dms_CRCP_yR",9,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y8,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y8,3,2)+2,\"00\")","v":"2025-26"},"dms_CRYf_y9",{"$f":"VALUE(LEFT(dms_CRYc_y8,4)+1)","v":2026},"dms_CRYc_y9",null,null,null,null,null,null,null,null,null,"Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) ",{"$f":"dms_060701_StartDateTxt","v":"1-Jul-2017"}]
[null,10,"=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")",10,"=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y9,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y9,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y9,4)+1))","v":"2029-30"},"dms_FRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yR,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yR,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yR,4)-1))","v":"2010-11"},"dms_CRCP_yQ",10,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y9,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y9,3,2)+2,\"00\")","v":"2026-27"},"dms_CRYf_y10",{"$f":"VALUE(LEFT(dms_CRYc_y9,4)+1)","v":2027},"dms_CRYc_y10"]
[null,11,"dms_FRCP_y11",11,"CRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y10,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y10,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y10,4)+1))","v":"2030-31"},"dms_FRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yQ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yQ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yQ,4)-1))","v":"2009-10"},"dms_CRCP_yP",11,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y10,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y10,3,2)+2,\"00\")","v":"2027-28"},"dms_CRYf_y11",{"$f":"VALUE(LEFT(dms_CRYc_y10,4)+1)","v":2028},"dms_CRYc_y11"]
[null,12,"dms_FRCP_y12",12,"CRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y11,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y11,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y11,4)+1))","v":"2031-32"},"dms_FRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yP,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yP,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yP,4)-1))","v":"2008-09"},"dms_CRCP_yO",12,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y11,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y11,3,2)+2,\"00\")","v":"2028-29"},"dms_CRYf_y12",{"$f":"VALUE(LEFT(dms_CRYc_y11,4)+1)","v":2029},"dms_CRYc_y12"]
[null,13,"dms_FRCP_y13",13,"CRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y12,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y12,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y12,4)+1))","v":"2032-33"},"dms_FRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yO,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yO,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yO,4)-1))","v":"2007-08"},"dms_CRCP_yN",13,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y12,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y12,3,2)+2,\"00\")","v":"2029-30"},"dms_CRYf_y13",{"$f":"VALUE(LEFT(dms_CRYc_y12,4)+1)","v":2030},"dms_CRYc_y13",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dms_0603_FeederList",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,14,"dms_FRCP_y14",14,"CRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y13,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y13,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y13,4)+1))","v":"2033-34"},"dms_FRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yN,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yN,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yN,4)-1))","v":"2006-07"},"dms_CRCP_yM",14,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y13,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y13,3,2)+2,\"00\")","v":"2030-31"},"dms_CRYf_y14",{"$f":"VALUE(LEFT(dms_CRYc_y13,4)+1)","v":2031},"dms_CRYc_y14",null,null,null,null,null,null,null,null,null,"Table 6.7.1 - daily performance data - unplanned - MAIFI  -- row descriptions and header named range values"]
[null,15,"dms_FRCP_y15",15,"CRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y14,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y14,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y14,4)+1))","v":"2034-35"},"dms_FRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yM,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yM,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yM,4)-1))","v":"2005-06"},"dms_CRCP_yL",15,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y14,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y14,3,2)+2,\"00\")","v":"2031-32"},"dms_CRYf_y15",{"$f":"VALUE(LEFT(dms_CRYc_y14,4)+1)","v":2032},"dms_CRYc_y15",null,null,null,null,null,null,null,null,null,"These headings (Lists) are determined from the INDEX/MATCH function on the NSP selected on the Business & other details sheet"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y15,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y15,3,2)+2,\"00\")","v":"2032-33"},"dms_CRYf_y16",{"$f":"VALUE(LEFT(dms_CRYc_y15,4)+1)","v":2033},"dms_CRYc_y16",null,null,null,null,null,null,null,null,"dms_060701_Feeder_Header_Lvl4",{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},{"$f":"IF((INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))=0),\"Network\",(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))))","v":"Network"},"Network","Network"]
[null,"These are drop down lists for businesses to select the correct FRCP_y1 on the business and other details worksheet.\nThis also populates the column headings in the worksheets",null,null,null,null,null,null,null,null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y16,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y16,3,2)+2,\"00\")","v":"2033-34"},"dms_CRYf_y17",{"$f":"VALUE(LEFT(dms_CRYc_y16,4)+1)","v":2034},"dms_CRYc_y17"]
[null,"dms_RCP_fyear_list","dms_CRY_ListF","dms_CRY_ListC","dms_RCP_cyear_list","dms_FRCP_fyear_list","dms_FRCP_ListF","dms_FRCP_ListC","dms_FRCP_cyear_list",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y17,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y17,3,2)+2,\"00\")","v":"2034-35"},"dms_CRYf_y18",{"$f":"VALUE(LEFT(dms_CRYc_y17,4)+1)","v":2035},"dms_CRYc_y18",null,null,null,null,null,null,null,null,"dms_060701_Rows","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events","All events","After removing excluded events"]
[null,"dms_fy1","2005-06","2006","dms_cy1","dms_frcp_fy1","2010-11",2011,"dms_crcp_cy1",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y18,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y18,3,2)+2,\"00\")","v":"2035-36"},"dms_CRYf_y19",{"$f":"VALUE(LEFT(dms_CRYc_y18,4)+1)","v":2036},"dms_CRYc_y19",null,null,null,null,null,null,null,null,null,"the number of column headings changes from 10 to 12 depending on the number of feeder categories for the NSP"]
[null,"dms_fy2","2006-07","2007","dms_cy2","dms_frcp_fy2","2011-12",2012,"dms_crcp_cy2",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y19,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y19,3,2)+2,\"00\")","v":"2036-37"},"dms_CRYf_y20",{"$f":"VALUE(LEFT(dms_CRYc_y19,4)+1)","v":2037},"dms_CRYc_y20"]
[null,"dms_fy3","2007-08","2008","dms_cy3","dms_frcp_fy3","2012-13",2013,"dms_crcp_cy3"]
[null,"dms_fy4","2008-09","2009","dms_cy4","dms_frcp_fy4","2013-14",2014,"dms_crcp_cy4"]
[null,"dms_fy5","2009-10",2010,"dms_cy5","dms_frcp_fy5","2014-15",2015,"dms_crcp_cy5"]
[null,"dms_fy6","2010-11",2011,"dms_cy6","dms_frcp_fy6","2015-16",2016,"dms_crcp_cy6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table 6.8.1 - row descriptions"]
[null,"dms_fy7","2011-12",2012,"dms_cy7","dms_frcp_fy7","2016-17",2017,"dms_crcp_cy7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dms_060801_01_Rows","dms_060801_02_Rows","dms_060801_03_Rows","dms_060801_04_Rows"]
[null,"dms_fy8","2012-13",2013,"dms_cy8","dms_frcp_fy8","2017-18",2018,"dms_crcp_cy8",null,null,"2005-06","2006",null,null,null,null,null,null,null,null,null,null,null,null,"Number of interruptions","Duration of interruptions","Total unplanned minutes off supply","Effect on unplanned MAIFI"]
[null,"dms_fy9","2013-14",2014,"dms_cy9","dms_frcp_fy9","2018-19",2019,"dms_crcp_cy9",null,null,"2006-07","2007"]
[null,"dms_fy10","2014-15",2015,"dms_cy10","dms_frcp_fy10","2019-20",2020,"dms_crcp_cy10",null,null,"2007-08","2008"]
[null,"dms_fy11","2015-16",2016,"dms_cy11","dms_frcp_fy11","2020-21",2021,"dms_crcp_cy11",null,null,"2008-09","2009"]
[null,"dms_fy12","2016-17",2017,"dms_cy12","dms_frcp_fy12","2021-22",2022,"dms_crcp_cy12",null,null,"2009-10",2010]
[null,"dms_fy13","2017-18",2018,"dms_cy13","dms_frcp_fy13","2022-23",2023,"dms_crcp_cy13",null,null,"2010-11",2011,null,null,null,null,null,null,null,null,null,null,null,null,"Table 7.9.4 - market impact component - row descriptions"]
[null,"dms_fy14","2018-19",2019,"dms_cy14","dms_frcp_fy14","2023-24",2024,"dms_crcp_cy14",null,null,"2011-12",2012,null,null,null,null,null,null,null,null,null,null,null,"dms_070904_01_Rows","without exclusions","with exclusions"]
[null,"dms_fy15","2019-20",2020,"dms_cy15","dms_frcp_fy15","2024-25",2025,"dms_crcp_cy15",null,null,"2012-13",2013]
[null,"dms_fy16","2020-21",2021,"dms_cy16",null,null,null,null,null,null,"2013-14",2014]
[null,"dms_fy17","2021-22",2022,"dms_cy17",null,null,null,null,null,null,"2014-15",2015]
[null,"dms_fy18","2022-23",2023,"dms_cy18",null,null,null,null,null,null,"2015-16",2016]
[null,"dms_fy19","2023-24",2024,"dms_cy19",null,null,null,null,null,null,"2016-17",2017,null,null,null,null,null,null,null,null,null,null,null,null,"Use this to add to existing files"]
[null,"dms_fy20","2024-25",2025,"dms_cy20",null,null,null,null,null,null,"2017-18",2018,null,null,null,null,null,null,null,null,null,null,null,null,"ARR's  6.8 STPIS exclusions"]
[null,null,null,null,null,null,null,null,null,null,null,"2018-19",2019,null,null,null,null,null,null,null,null,null,null,null,null,"dms_060801_Event_Date","dms_060801_OutageID","dms_060801_FeederID","dms_060801_FeederClass","dms_060801_CauseID","dms_060801_01_Values","dms_060801_02_Values","dms_060801_03_Values","dms_060801_Excl_Cat","dms_060801_04_Values"]
[null,null,null,null,null,null,null,null,null,null,null,"2019-20",2020]
[null,null,null,null,null,null,null,null,null,null,null,"2020-21",2021]
[null,null,null,null,null,null,null,null,null,null,null,"2021-22",2022,null,null,null,null,null,null,null,null,null,null,null,null,"CA 6.3 sustained interruptions"]
[null,null,null,null,null,null,null,null,null,null,null,"2022-23",2023,null,null,null,null,null,null,null,null,null,null,null,null,"dms_060301_Event_Date","dms_060301_Event_Time","dms_060301_AssetID","dms_060301_FeederClass","dms_060301_Reason","dms_060301_DetailedReason","dms_060301_CustNo_Affected_Values","dms_060301_Avg_Duration_Sustained_Int_Values","dms_060301_Effect_unplanned_SAIDI_Values","dms_060301_Effect_unplanned_SAIFI_Values","dms_060301_MED"]
[null,null,null,null,null,null,null,null,null,null,null,"2023-24",2024]
[null,null,null,null,null,null,null,null,null,null,null,"2024-25",2025]
[null,null,null,null,null,null,null,null,null,null,null,"2025-26",2026]
[null,null,null,null,null,null,null,null,null,null,null,"2026-27",2027]
[null,null,null,null,null,null,null,null,null,null,null,"2027-28",2028]
[null,null,null,null,null,null,null,null,null,null,null,"2028-29",2029]
[null,null,null,null,null,null,null,null,null,null,null,"2029-30",2030]
[null,null,null,null,null,null,null,null,null,null,null,"2030-31",2031]
[null,null,null,null,null,null,null,null,null,null,null,"2031-32",2032]
[null,null,null,null,null,null,null,null,null,null,null,"2032-33",2033]
[null,null,null,null,null,null,null,null,null,null,null,"2033-34",2034]
[null,null,null,null,null,null,null,null,null,null,null,"2034-35",2035]
[null,null,null,null,null,null,null,null,null,null,null,"2035-36",2036]

{"sheet":"Instructions","index":1,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[25,2,25,3],[26,2,26,4],[7,2,7,3],[1,1,1,5],[2,1,2,5],[3,2,3,4],[4,2,4,4],[5,2,5,4],[24,2,24,4],[12,2,12,4],[8,2,8,4],[10,2,10,4],[20,2,20,4],[22,2,22,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Segment,\" Network Service Provider\")","v":"Distribution Network Service Provider"}]
[null,"Annual Reporting RIN Template"]
[null,null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingName,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Power and Water to fulfil its reporting obligations to the AER."}]
[null,null,"INSTRUCTIONS"]
[null,null,"Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,null,"Identifying CONFIDENTIAL INFORMATION:\n\nPlease use the macro at the top of each \nworksheet to identify confidential information. \n\n"]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selection CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return selection to NON-CONFIDENTIAL macro."]
[]
[null,null,"UNITS OF MEASURE\n\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,null,"COLOUR CODING OF INPUT / NON-INPUT CELLS:"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null,"\nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,null,"WORKSHEET NAVIGATION\n\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin of excel (for Row groupings) or above the columns (for column groupings). \n\n\n"]
[]
[null,null,"RETURNING COMPLETED RESPONSES\n\nPlease return four (4) files - using the locked template - to the AER:\n \n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro.\n\n2. An actual and an estimate version with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER.\n\n3. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. If the confidential and public versions of the consolidated file are exactly the same, only the public version of the file needs to be submitted to the AER."]
[]
[null,null,"SUBMITTING AMENDED DATA TO THE AER\n\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]

{"sheet":"Contents","index":2,"n_rows":34,"n_cols":19,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE((LOOKUP(dms_Model,dms_Model_List,dms_Worksheet_List))&\" \"&CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"CONTENTS"]
[]
[]
[null,null,null,null,"1. Business details",null,null,null,null,null,null,"2. Expenditure"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"4. Alternative control services",null,null,null,null,null,null,"5. Network information",null,null,null,null,null,null,"6. Service & quality"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"8. Capex",null,null,null,null,null,null,"9. TAX"]

{"sheet":"Business & other details","index":3,"n_rows":144,"n_cols":9,"rows_kept":144,"cut":false,"hidden":false,"merged":[[59,2,59,8],[18,4,18,7],[19,2,19,3],[19,4,19,7],[22,2,22,3],[22,4,22,7],[23,4,23,7],[24,2,24,3],[24,4,24,7],[32,1,32,8],[57,2,57,3],[58,4,58,8],[7,1,7,8],[11,1,11,8],[13,2,13,4],[14,2,14,4],[17,2,17,3],[17,4,17,7]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"CATEGORY ANALYSIS"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result))","v":"2017-18"}]
[null,"BUSINESS & OTHER DETAILS"]
[]
[]
[null,"Instructions"]
[null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,"SUBMISSION PARTICULARS INPUT SHEETS"]
[]
[null,"ENTITY DETAILS"]
[]
[null,"Short name","Power and Water",null,null,"Select business name from drop down list first"]
[null,"ACN / ABN",{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":15947352360}]
[]
[]
[null,"Business address","Address 1",null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 1921"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"DARWIN"}]
[null,null,null,"State",{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},"p/code",{"$f":"INDEX(dms_PostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":801}]
[]
[null,"Postal address","Address 1",null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"GPO Box 1921"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"DARWIN"}]
[null,null,null,"State",{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},"p/code",{"$f":"INDEX(dms_PPostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":801}]
[]
[]
[null,"Contact name/s","Jodi Triggs"]
[null,"Contact phone/s"]
[null,"Contact email address/s"]
[]
[null,"REGULATORY CONTROL PERIODS"]
[]
[null,"Forthcoming regulatory control period","2020-21",{"$f":"dms_FRCP_y2","v":"2021-22"},{"$f":"dms_FRCP_y3","v":"2022-23"},{"$f":"dms_FRCP_y4","v":"2023-24"},{"$f":"dms_FRCP_y5","v":"2024-25"}]
[null,null,{"$f":"dms_FRCP_y6","v":"2025-26"},{"$f":"dms_FRCP_y7","v":"2026-27"},{"$f":"dms_FRCP_y8","v":"2027-28"},{"$f":"dms_FRCP_y9","v":"2028-29"},{"$f":"dms_FRCP_y10","v":"2029-30"}]
[]
[]
[null,"Current regulatory control period",{"$f":"dms_CRCP_FirstYear_Result","v":"2015-16"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+1)&\"-\"&TEXT(MID(CRCP_y1,3,2)+2,\"00\"),VALUE(LEFT(CRCP_y1,4)+1))","v":"2016-17"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+2)&\"-\"&TEXT(VALUE(MID(CRCP_y1,3,2)+3),\"00\"),VALUE(LEFT(CRCP_y1,4)+2))","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+3)&\"-\"&TEXT(MID(CRCP_y1,3,2)+4,\"00\"),VALUE(LEFT(CRCP_y1,4)+3))","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+4)&\"-\"&TEXT(MID(CRCP_y1,3,2)+5,\"00\"),VALUE(LEFT(CRCP_y1,4)+4))","v":"2019-20"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+5)&\"-\"&TEXT(MID(CRCP_y1,3,2)+6,\"00\"),VALUE(LEFT(CRCP_y1,4)+5))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+6)&\"-\"&TEXT(MID(CRCP_y1,3,2)+7,\"00\"),VALUE(LEFT(CRCP_y1,4)+6))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+7)&\"-\"&TEXT(MID(CRCP_y1,3,2)+8,\"00\"),VALUE(LEFT(CRCP_y1,4)+7))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+8)&\"-\"&TEXT(MID(CRCP_y1,3,2)+9,\"00\"),VALUE(LEFT(CRCP_y1,4)+8))","v":"2023-24"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+9)&\"-\"&TEXT(MID(CRCP_y1,3,2)+10,\"00\"),VALUE(LEFT(CRCP_y1,4)+9))","v":"2024-25"}]
[null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+10)&\"-\"&TEXT(MID(CRCP_y1,3,2)+11,\"00\"),VALUE(LEFT(CRCP_y1,4)+10))","v":"2025-26"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+11)&\"-\"&TEXT(MID(CRCP_y1,3,2)+12,\"00\"),VALUE(LEFT(CRCP_y1,4)+11))","v":"2026-27"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+12)&\"-\"&TEXT(MID(CRCP_y1,3,2)+13,\"00\"),VALUE(LEFT(CRCP_y1,4)+12))","v":"2027-28"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+13)&\"-\"&TEXT(MID(CRCP_y1,3,2)+14,\"00\"),VALUE(LEFT(CRCP_y1,4)+13))","v":"2028-29"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+14)&\"-\"&TEXT(MID(CRCP_y1,3,2)+15,\"00\"),VALUE(LEFT(CRCP_y1,4)+14))","v":"2029-30"}]
[]
[]
[null,"Previous regulatory control period",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y2,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y2,3,2)),\"00\"),VALUE(LEFT(PRCP_y2,4)-1))","v":"2010-11"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y3,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y3,3,2)),\"00\"),VALUE(LEFT(PRCP_y3,4)-1))","v":"2011-12"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y4,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y4,3,2)),\"00\"),VALUE(LEFT(PRCP_y4,4)-1))","v":"2012-13"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y5,4)-1)&\"-\"&TEXT(VALUE(RIGHT(PRCP_y5,2)-1),\"00\"),VALUE(LEFT(PRCP_y5,4)-1))","v":"2013-14"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2014-15"}]
[]
[]
[]
[null,"Commencing regulatory year","2017-18","CRY"]
[]
[null,"Last completed regulatory year","2017-18","dms_FinalYear"]
[]
[]
[]
[null,null,"IF THIS IS AN ABC RIN - make sure the the named range CRY is applied and the named range dms_dollar_nom_UOM is applied"]
[null,null,"IF THIS IS A RESET RIN - make sure the named ranges CRY and dms_dollar_nom_UOM are NOT present in the workbook"]
[null,null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS - make sure MultiYear Flag is set and final year entered as required"]
[]
[null,"Source","Reporting",null,"Please select the correct submission type from the dropdown list."]
[null,"Data quality (actual, estimate, public, consolidated)","Consolidated",null,"Use Consolidated for Consolidated Confidential version\nUse Public for Consolidated Public version"]
[null,"Amended RIN submission - amendment reason","20190906 - updated confidentiality for 4.2.2 D19/138370"]
[null,"Submission Date","2019-09-06","dms_SubmissionDate","Please enter date this file submitted to AER (dd/mm/yyyy)"]
[null,"EBSS - First application of scheme in forthcoming period?","No"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))","v":"2018"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Model or RIN Type","CA","dms_Model","Drop down selection"]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an ABC RIN make the NAMED RANGE on this field is set"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"NT"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FOR RESET RINS"]
[null,"CRY-1",{"$f":"VALUE(LEFT(CRY,4)-1)","v":2016},"dms_Left_CRY_minus1","=VALUE(LEFT(CRY,4)-1)",null,"Not used in Reset RINS but may be useful in other cases"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))","v":"June 2018"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))"]
[null,"Dollar $ real previous year (PRCP_y5)",{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)","v":"June 2017"},"dms_DollarReal_Prev","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(CRY,2))&RIGHT(CRY,2))-1),CONCATENATE(dms_RPTMonth)&\" \"&VALUE(((LEFT(dms_CRCP_FirstYear_Result,2)&RIGHT(dms_CRCP_FirstYear_Result,2))))-1)"]
[null,"FOR PTRM/ RFMs"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FOR EB RINS"]
[null,"Calendar Year for table 3.6 data",{"$f":"VALUE(dms_RYE)-1","v":2017},"dms_0306_Year","=VALUE(dms_RYE)-1"]
[null,"FOR ABC RINS THAT SPAN MULTIPLE YEARS"]
[null,"Is this a multi year ABC RIN?","No"]
[null,"Backcast Multiyear EB, CA or ARR?",{"$f":"IF(dms_MultiYear_ResponseFlag=\"No\",0,1)","v":0},"dms_MultiYear_Flag","This is set from the answer provided above"]
[null,null,{"$f":"IF(dms_MultiYear_Flag=1,\"Specify Final Reg Year here eg 2016 or 2015-16\",\"not a Multi Reg Year submission\")","v":"not a Multi Reg Year submission"},"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if response to Q in C73 is \"yes\" and dms_MultiYear_Flag is set to 1"]
[null,"This block works out the various RYE's for ALL RIN types and MODELS"]
[null,"Single Year Model T/F",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":1},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Single Year Final Year Reference","CRY","dms_SingleYear_FinalYear_Ref","This is the reference for EB, CA & ARR RINs"]
[null,"Single Year Final Year Result",{"$f":"IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")","v":"2017-18"},"dms_SingleYear_FinalYear_Result","=IFERROR(IF(SUM(dms_SingleYear_Model)<>0,(INDIRECT(dms_SingleYear_FinalYear_Ref)),\"not a single year RIN\"),\"CRY not present\")"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Multi Year Final Year Reference",{"$f":"INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))","v":"dms_FRCP_y5"},"dms_MultiYear_FinalYear_Ref","=INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))"]
[null,"Multi Year Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)","v":"2024-25"},"dms_MultiYear_FinalYear_Result","=IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)",null,null,null,"Formula errors OK"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP Final Year Reference",{"$f":"INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))","v":"CRCP_y5"},"dms_CRCP_FinalYear_Ref","=INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))"]
[null,"CRCP First Year Result",{"$f":"INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))","v":"2015-16"},"dms_CRCP_FirstYear_Result","=INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))"]
[null,"CRCP Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)","v":"2017-18"},"dms_CRCP_FinalYear_Result","=IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)"]
[null,"FOR CA RINS"]
[null,"How many rows in tables 6.3 sustained interruptions?",{"$f":"IF(dms_Model<>\"CA\",\"not a CA\",\"Is a CA\")","v":"Is a CA"},"dms_060301_MaxRows only returns a valid value when cover sheet is attached to a CA file"]
[null,"Table 6.3.1 - last row reference",{"$f":"IFERROR(IF(dms_Model=\"CA\",\nLOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),\n(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\n\"not a CA\"),\"no data in 6.3 or 6.3 not present\")","v":15},"dms_060301_LastRow","=IFERROR(IF(dms_Model=\"CA\",LOOKUP(2,1/(dms_060301_Avg_Duration_Sustained_Int_Values<>\"\"),(ROW(dms_060301_Avg_Duration_Sustained_Int_Values))),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.3.1 - max number rows",{"$f":"IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-14),\"not a CA\"),\"no data in 6.3 or 6.3 not present\")","v":1},"dms_060301_MaxRows","=IFERROR(IF(dms_Model=\"CA\",(dms_060301_LastRow-14),\"not a CA\"),\"6.3 not present\")"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"x"},"dms_663","=INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"FOR ARR or RESET RINS"]
[null,"How many rows in tables 6.1 or 6.7?  (leap year?)","insert dms_LeapYear NR if required","dms_LeapYear is used to determine dms_060701_Max_Rows BUT it is only found on worksheet 6.1 or 6.7 and the date value in the cell is used to determine whether it is a leap year"]
[null,"Is dms_LeapYear named range present?",{"$f":"IFERROR(IF(dms_LeapYear,\"yes\"),\"no\")","v":"no"}]
[null,"Table 6.7.1 - includes a leap year?",{"$f":"\nIFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\n\"dms_LeapYear not present\")","v":"dms_LeapYear not present"},"dms_LeapYear_Result","=IFERROR(IF(MONTH(DATE(YEAR(dms_LeapYear),2,29))=2,\"is a leap year\",\"not a leap year\"),\"dms_LeapYear not present\")"]
[null,"Table 6.7.1 - Last row  (leap year/ non leap year)",{"$f":"\nIFERROR(IF(dms_Model=\"ARR\",\nIF(dms_LeapYear_Result=\"is a leap year\",366,365),\n(IF(dms_Model=\"Reset\",\n(IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)),\n\"not a relevant RIN type\"))),\n\"dms_LeapYear in either 6.1 or 6.7 not present\")","v":"not a relevant RIN type"},"dms_060701_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",IF(dms_LeapYear_Result=\"is a leap year\",366,365),(IF(dms_Model=\"Reset\",(IF(dms_LeapYear_Result=\"is a leap year\",1827,1826)),\"not a relevant RIN type\"))),\"dms_LeapYear in either 6.1 or 6.7 not present\")"]
[null,"How many columns in 6.7?   (4 or 5 feeder categories)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",\"This NSP has only 4 feeder categories\",\"This NSP has 5 feeder categories\")","v":"This NSP has only 4 feeder categories"}]
[null,"Table 6.7.1 - Last column (# of feeder categories > 4)",{"$f":"IF(dms_FifthFeeder_flag_NSP=\"NO\",10,12)","v":10},"dms_060701_MaxCols","=IF(dms_FifthFeeder_flag_NSP=\"NO\",8,10)"]
[null,"Table 6.7.1 - Number of offset rows",{"$f":"IF(dms_Model=\"ARR\",15,9)","v":9},"dms_060701_OffsetRows","=IF(dms_Model=\"ARR\",15,9)"]
[null,"Start date for telephone answering in 6.1 or 6.7?",null,null,"Using 060701 as naming standard not 060101 "]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Text",{"$f":"IF(SUM(dms_SingleYear_Model)>0,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))","v":"1-Jul-2017"},"dms_060701_StartDateTxt","=IF(SUM(dms_SingleYear_Model)>1,(CONCATENATE(IF(LEN(CRY)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRY,4))),(CONCATENATE(IF(LEN(CRCP_y4)=4,\"1-Jan-\",\"1-Jul-\"),LEFT(CRCP_y4,4))))"]
[null,"Table 6.1.1 and 6.7.1 - Start Date as Date Value",{"$f":"DATEVALUE(dms_060701_StartDateTxt)","v":42917},"dms_060701_StartDateVal","=DATEVALUE(dms_060701_StartDateTxt)"]
[null,"FOR ARRs"]
[null,"How many rows in table 6.8?","insert dms_060801_StartCell NR if required","dms_060801_StartCell is only found on worksheet 6.8 and is used to determine the starting date for the date range"]
[null,"Table 6.8 - Number of offset rows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 not present\")","v":"not an ARR"},"dms_0608_OffsetRows","=IFERROR(IF(dms_Model=\"ARR\",(ROW(dms_060801_StartCell)-1),\"not an ARR\"),\"6.8 not present\")"]
[null,"Table 6.8 - Last row",{"$f":"IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"6.8 not present\")","v":"6.8 not present"},"dms_0608_LastRow","=IFERROR(IF(dms_060801_StartCell<>\"\",IF(dms_Model=\"ARR\",(LOOKUP(2,1/(dms_060801_01_Values<>\"\"),(ROW(dms_060801_01_Values)))),\"not an ARR\"),0),\"6.8 not present\")"]
[null,"Table 6.8 - MaxRows",{"$f":"IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")","v":"not an ARR"},"dms_060801_MaxRows","=IFERROR(IF(dms_Model=\"ARR\",(MAX(0,dms_0608_LastRow-dms_0608_OffsetRows)),\"not an ARR\"),\"6.8 not present\")"]
[null,"FOR TNSP RESET RINS"]
[null,"Table 7.9.4 only appears in TNSPs Reset RIN"]
[null,"Table 7.9.4 - first year",{"$f":"LEFT(PRCP_y3,4)","v":"2012"},"dms_070904_Start_Year","=LEFT(PRCP_y3,4)"]
[null,"FOR SUBSET FILES"]
[null,"Is this Submission File a Subset File","NO","dms_Partial"]
[null,"MISC"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"distribution determination"},"dms_DeterminationRef"]
[null,"Public lighting NSP?",{"$f":"INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_Public_Lighting","=INDEX(dms_Public_Lighting_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[null,"Fifth Feeder Category (eg. TasNetworks (D))",{"$f":"INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"NO"},"dms_FifthFeeder_flag_NSP","=INDEX(dms_FeederType_5_flag,MATCH(dms_TradingName,dms_TradingName_List))"]
[]
[null,"DISCARD FILES"]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]
[]
[null,"REGULATORY YEARS FOR MULTI RYE SUBMISSIONS"]
[null,"Multiple RYE flag","NO","dms_Multi_RYE_flag"]
[null,null,"Manually specify RYE","Named ranges to apply"]
[null,null,2013,"dms_RYE_01"]
[null,null,2014,"dms_RYE_02"]
[null,null,2015,"dms_RYE_03"]
[null,null,2016,"dms_RYE_04"]
[null,null,2017,"dms_RYE_05"]

{"sheet":"2.1 Expenditure summary","index":4,"n_rows":158,"n_cols":3,"rows_kept":158,"cut":false,"hidden":false,"merged":[]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[null,"There are EIGHT tables on this worksheet - see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Replacement expenditure",18664842]
[null,"Connections",2622909]
[null,"Augmentation Expenditure",17626042]
[null,"Non-network",4098856]
[null,"capitalised network overheads",8183999]
[null,"capitalised corporate overheads",3048697]
[null,"Metering",0]
[null,"Public Lighting",0]
[]
[]
[]
[]
[]
[]
[null,"balancing item",47062]
[null,"capcons (included in the above)",11825296]
[null,"TOTAL GROSS CAPEX (includes capcons)",{"$f":"+SUM(C11:C25)","v":54292407}]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Vegetation management",4110818]
[null,"Maintenance",14092166]
[null,"Emergency response",8947734]
[null,"Non-network",7139659]
[null,"Network overheads",37977440]
[null,"Corporate overheads",13381113]
[null,"Metering",0]
[null,"Public Lighting",0]
[]
[]
[]
[]
[]
[]
[null,"balancing tem",102069]
[null,"TOTAL OPEX",{"$f":"+SUM(C32:C46)","v":85750999}]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Connections",0]
[null,"Capitalised network overheads",303490.36]
[null,"Capitalised corporate overheads",380100.8]
[null,"Metering",3447199.51]
[null,"Public lighting",0]
[null,"Fee and quoted",28661.19]
[null,"Non-network",366118.32]
[]
[]
[]
[]
[]
[null,"balancing tem",0]
[null,"TOTAL CAPEX",{"$f":"+SUM(C52:C64)","v":4525570.18}]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Connections",507355.73]
[null,"Network overheads",2165072]
[null,"Corporate overheads",1668310]
[null,"Metering",3645825.98]
[null,"Public lighting",0]
[null,"Fee and quoted",2936483.13]
[null,"Non-network",482576.26]
[]
[]
[]
[]
[]
[null,"balancing tem",0]
[null,"TOTAL OPEX",{"$f":"+SUM(C70:C82)","v":11405623.1}]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Replacement expenditure",0]
[null,"Connections",0]
[null,"Augmentation Expenditure",0]
[null,"Non-network",0]
[null,"Capitalised network overheads",0]
[null,"Capitalised corporate overheads",0]
[]
[]
[]
[]
[]
[]
[null,"balancing tem",0]
[null,"capcons (included in the above)",0]
[null,"TOTAL GROSS CAPEX (includes capcons)",{"$f":"SUM(C88:C100)","v":0}]
[]
[null,"2.1.6 - DUAL FUNCTION ASSETS OPEX"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Vegetation management",0]
[null,"Maintenance",0]
[null,"Emergency response",0]
[null,"Non-network",0]
[null,"Network overheads",0]
[null,"Corporate overheads",0]
[null,"Metering",0]
[]
[]
[]
[]
[]
[null,"balancing tem",0]
[null,"TOTAL OPEX",{"$f":"SUM(C107:C119)","v":0}]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Replacement expenditure",0]
[null,"Connections",8726992.7799999993]
[null,"Augmentation Expenditure",3098303.15]
[null,"Non-network",0]
[null,"Capitalised network overheads",0]
[null,"Capitalised corporate overheads",0]
[null,"Metering",0]
[null,"Public Lighting",0]
[]
[]
[]
[]
[]
[]
[]
[null,"TOTAL CAPCONS",{"$f":"+SUM(C125:C139)","v":11825295.93}]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,"EXPENDITURE ($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Vegetation management",0]
[null,"Maintenance",0]
[null,"Emergency response",0]
[null,"Non-network",0]
[null,"Metering",0]
[null,"Public Lighting",0]
[]
[]
[]
[]
[]
[]
[null,"capcons (included in the above)",0]
[null,"TOTAL CAPITALISED OVERHEADS",{"$f":"+SUM(C145:C156)","v":0}]

{"sheet":"2.2 Repex","index":5,"n_rows":528,"n_cols":5,"rows_kept":528,"cut":false,"hidden":false,"merged":[[66,1,81,1],[82,1,110,1],[111,1,124,1],[125,1,133,1],[134,1,141,1],[11,1,35,1],[36,1,42,1],[49,1,57,1],[58,1,65,1],[43,1,48,1],[485,1,488,1],[281,1,289,1],[290,1,297,1],[205,1,213,1],[214,1,221,1],[222,1,237,1],[238,1,266,1],[355,1,360,1],[167,1,191,1],[192,1,198,1],[199,1,204,1],[323,1,347,1],[348,1,354,1],[267,1,280,1],[522,1,525,1],[526,1,527,1],[361,1,369,1],[370,1,377,1],[378,1,393,1],[394,1,422,1],[423,1,436,1],[496,1,499,1],[500,1,501,1],[489,1,495,1],[437,1,445,1],[446,1,453,1],[481,1,484,1],[507,1,510,1],[511,1,514,1],[515,1,521,1]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.2 REPEX"]
[]
[null,"There are TWO tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for ease of navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,"EXPENDITURE ($0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRY","v":"2017-18"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - replacement of staked pole",null,0]
[null,null,"˂ = 1 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of staked pole",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of staked pole",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of staked pole",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of staked pole",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"> 132 kV; Wood - replacement of staked pole",null,0]
[null,null,"> 132 kV; Wood - replacement of unstaked pole",null,0]
[null,null,"˂ = 1 kV; Concrete",null,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0]
[null,null,"> 132 kV; Concrete",null,0]
[null,null,"˂ = 1 kV; Steel",null,719677]
[null,null,"> 1 kV & < = 11 kV; Steel",null,404061]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,234826]
[null,null,"> 22 kV & < = 66 kV; Steel",null,111385]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0]
[null,null,"> 132 kV; Steel",null,0]
[null,null,"Other",null,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,24036]
[null,null,"> 1 kV & < = 11 kV",null,287644]
[null,null,"˃ 11 kV & < = 22 kV",null,439647]
[null,null,"> 22 kV & < = 66 kV",null,73923]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0]
[null,null,"> 1 kV & < = 11 kV",null,0]
[null,null,"˃ 11 kV & < = 22 kV",null,0]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,"OVERHEAD CONDUCTORS BY: \nHIGHEST OPERATING VOLTAGE; NUMBER OF PHASES (AT HV)","˂ = 1 kV",null,441005]
[null,null,"> 1 kV & < = 11 kV",null,990221]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,191059]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"UNDERGROUND CABLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,294624]
[null,null,"> 1 kV & < = 11 kV",null,2584815]
[null,null,"> 11 kV & < = 22 kV",null,74620]
[null,null,"> 22 kV & < = 33 kV",null,0]
[null,null,"> 33 kV & < = 66 kV",null,77736]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,">  132 kV",null,0]
[null,null,"Other",null,0]
[null,"SERVICE LINES BY: \nCONNECTION VOLTAGE; CUSTOMER TYPE; CONNECTION COMPLEXITY ","˂ = 11 kV ; Residential ; Simple Type",null,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 132 kV ; Subdivision  ",null,0]
[null,null,"Other",null,0]
[null,"TRANSFORMERS BY: \nMOUNTING TYPE; HIGHEST OPERATING VOLTAGE ; AMPERE RATING; NUMBER OF PHASES (AT LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,77820]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,45269]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,114665]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,957677]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,65664]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,9371]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,41761]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,1467231]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,11658]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,639344]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,324819]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,219088]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0]
[null,null,"Other",null,0]
[null,"SWITCHGEAR BY: \nHIGHEST OPERATING VOLTAGE ; SWITCH FUNCTION","˂ = 11 kV ;  FUSE",null,0]
[null,null,"˂ = 11 kV  ; Switch",null,3139249]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,194845]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,174227]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,99988]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,454161]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,29996]
[null,null,"> 132 kV ; Switch",null,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0]
[null,null,"Other",null,0]
[null,"PUBLIC LIGHTING BY: \nASSET TYPE ; LIGHTING OBLIGATION","Luminaires ;  Major Road",null,0]
[null,null,"Luminaires ;  Minor Road",null,0]
[null,null,"Brackets ; Major Road",null,0]
[null,null,"Brackets ; Minor Road",null,0]
[null,null,"Lamps ; Major Road",null,0]
[null,null,"Lamps ; Minor Road",null,0]
[null,null,"Poles / Columns ; Major Road",null,0]
[null,null,"Poles / Columns ; Minor Road",null,0]
[null,null,"Other",null,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFUNCTION","Field Devices",null,795589]
[null,null,"Local Network Wiring Assets",null,116019]
[null,null,"Communications Network Assets",null,357939]
[null,null,"Master Station Assets",null,0]
[null,null,"Communications Site Infrastructure",null,0]
[null,null,"Communications Linear Assets",null,0]
[null,null,"AFLC",null,0]
[null,null,"Other",null,0]
[null,"OTHER BY: \nDNSP DEFINED","Buildings",null,102805]
[null,null,"Instrument Transformers",null,108969]
[null,null,"Metering Units",null,52235]
[null,null,"Pillars",null,605245]
[null,null,"Substation Auxiliary Plant",null,330353]
[null,null,"Voltage Regulators",null,102597]
[null,null,"Civil and Grounds",null,284533]
[null,null,"Fire Systems",null,320]
[null,null,"Power Transformer Refurbishment",null,78890]
[null,null,"Tower Refurbishment",null,713234]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRY","v":"2017-18"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - Staked",null,0]
[null,null,"˂ = 1 kV; Wood - Unstaked",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Staked",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Unstaked",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Staked",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Unstaked",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Staked",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Unstaked",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Staked",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Untaked",null,0]
[null,null,"> 132 kV; Wood - Staked",null,0]
[null,null,"> 132 kV; Wood - Unstaked",null,0]
[null,null,"˂ = 1 kV; Concrete",null,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0]
[null,null,"> 132 kV; Concrete",null,0]
[null,null,"˂ = 1 kV; Steel",null,37]
[null,null,"> 1 kV & < = 11 kV; Steel",null,12]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,14]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0]
[null,null,"> 132 kV; Steel",null,0]
[null,null,"Other",null,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,22]
[null,null,"> 1 kV & < = 11 kV",null,178]
[null,null,"˃ 11 kV & < = 22 kV",null,291]
[null,null,"> 22 kV & < = 66 kV",null,8]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0]
[null,null,"> 1 kV & < = 11 kV",null,0]
[null,null,"˃ 11 kV & < = 22 kV",null,0]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,"OVERHEAD CONDUCTORS BY: \nHIGHEST OPERATING VOLTAGE; NUMBER OF PHASES (AT HV)","˂ = 1 kV",null,3.2]
[null,null,"> 1 kV & < = 11 kV",null,4.8]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,0.5]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"UNDERGROUND CABLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,0.4]
[null,null,"> 1 kV & < = 11 kV",null,1.8]
[null,null,"> 11 kV & < = 22 kV",null,0.1]
[null,null,"> 22 kV & < = 33 kV",null,0]
[null,null,"> 33 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,">  132 kV",null,0]
[null,null,"Other",null,0]
[null,"SERVICE LINES BY: \nCONNECTION VOLTAGE; CUSTOMER TYPE; CONNECTION COMPLEXITY ","˂ = 11 kV ; Residential ; Simple Type",null,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 132 kV ; Subdivision  ",null,0]
[null,null,"Other",null,0]
[null,"TRANSFORMERS BY: \nMOUNTING TYPE; HIGHEST OPERATING VOLTAGE ; AMPERE RATING; NUMBER OF PHASES (AT LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,1]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,10]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,55]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,1]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,2]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,29]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,7]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,3]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0]
[null,null,"Other",null,0]
[null,"SWITCHGEAR BY: \nHIGHEST OPERATING VOLTAGE ; SWITCH FUNCTION","˂ = 11 kV ;  FUSE",null,0]
[null,null,"˂ = 11 kV  ; Switch",null,38]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,10]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,6]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,24]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,9]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0]
[null,null,"> 132 kV ; Switch",null,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0]
[null,null,"Other",null,0]
[null,"PUBLIC LIGHTING BY: \nASSET TYPE ; LIGHTING OBLIGATION","Luminaires ;  Major Road",null,0]
[null,null,"Luminaires ;  Minor Road",null,0]
[null,null,"Brackets ; Major Road",null,0]
[null,null,"Brackets ; Minor Road",null,0]
[null,null,"Lamps ; Major Road",null,0]
[null,null,"Lamps ; Minor Road",null,0]
[null,null,"Poles / Columns ; Major Road",null,0]
[null,null,"Poles / Columns ; Minor Road",null,0]
[null,null,"Other",null,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFUNCTION","Field Devices",null,61]
[null,null,"Local Network Wiring Assets",null,0]
[null,null,"Communications Network Assets",null,0]
[null,null,"Master Station Assets",null,0]
[null,null,"Communications Site Infrastructure",null,0]
[null,null,"Communications Linear Assets",null,0]
[null,null,"AFLC",null,0]
[null,null,"Other",null,0]
[null,"OTHER BY: \nDNSP DEFINED",{"$f":"IF(ISBLANK(C143),\"\",C143)","v":"Buildings"},null,0]
[null,null,"Instrument Transformers",null,6]
[null,null,"Metering Units",null,2]
[null,null,"Pillars",null,82]
[null,null,"Substation Auxiliary Plant",null,5]
[null,null,"Voltage Regulators",null,6]
[null,null,"Civil and Grounds",null,6]
[null,null,"Fire Systems",null,0]
[null,null,"Power Transformer Refurbishment",null,0]
[null,null,"Tower Refurbishment",null,4]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRY","v":"2017-18"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - Staked",null,0]
[null,null,"˂ = 1 kV; Wood - Unstaked",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Staked",null,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Unstaked",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Staked",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Unstaked",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Staked",null,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Unstaked",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Staked",null,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Untaked",null,0]
[null,null,"> 132 kV; Wood - Staked",null,0]
[null,null,"> 132 kV; Wood - Unstaked",null,0]
[null,null,"˂ = 1 kV; Concrete",null,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0]
[null,null,"> 132 kV; Concrete",null,0]
[null,null,"˂ = 1 kV; Steel",null,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0]
[null,null,"> 132 kV; Steel",null,0]
[null,null,"Other",null,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,71]
[null,null,"> 1 kV & < = 11 kV",null,5]
[null,null,"˃ 11 kV & < = 22 kV",null,7]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv",null,0]
[null,null,"> 1 kV & < = 11 kV",null,0]
[null,null,"˃ 11 kV & < = 22 kV",null,0]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,"> 132 kV",null,0]
[null,"OVERHEAD CONDUCTORS BY: \nHIGHEST OPERATING VOLTAGE; NUMBER OF PHASES (AT HV)","˂ = 1 kV",null,3]
[null,null,"> 1 kV & < = 11 kV",null,11]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",null,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",null,8]
[null,null,"> 22 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,1]
[null,null,"> 132 kV",null,0]
[null,null,"Other",null,0]
[null,"UNDERGROUND CABLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,4]
[null,null,"> 1 kV & < = 11 kV",null,44]
[null,null,"> 11 kV & < = 22 kV",null,4]
[null,null,"> 22 kV & < = 33 kV",null,0]
[null,null,"> 33 kV & < = 66 kV",null,0]
[null,null,"> 66 kV & < = 132 kV",null,0]
[null,null,">  132 kV",null,0]
[null,null,"Other",null,0]
[null,"SERVICE LINES BY: \nCONNECTION VOLTAGE; CUSTOMER TYPE; CONNECTION COMPLEXITY ","˂ = 11 kV ; Residential ; Simple Type",null,70]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",null,31]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",null,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",null,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",null,0]
[null,null,"> 132 kV ; Subdivision  ",null,0]
[null,null,"Other",null,0]
[null,"TRANSFORMERS BY: \nMOUNTING TYPE; HIGHEST OPERATING VOLTAGE ; AMPERE RATING; NUMBER OF PHASES (AT LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,10]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,11]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,3]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,6]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,2]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0]
[null,null,"Other",null,0]
[null,"SWITCHGEAR BY: \nHIGHEST OPERATING VOLTAGE ; SWITCH FUNCTION","˂ = 11 kV ;  FUSE"]
[null,null,"˂ = 11 kV  ; Switch",null,11]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,4]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,15]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,5]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,1]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,1]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0]
[null,null,"> 132 kV ; Switch",null,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0]
[null,null,"Other",null,0]
[null,"PUBLIC LIGHTING BY: \nASSET TYPE ; LIGHTING OBLIGATION","Luminaires ;  Major Road",null,0]
[null,null,"Luminaires ;  Minor Road",null,0]
[null,null,"Brackets ; Major Road",null,0]
[null,null,"Brackets ; Minor Road",null,0]
[null,null,"Lamps ; Major Road",null,0]
[null,null,"Lamps ; Minor Road",null,0]
[null,null,"Poles / Columns ; Major Road",null,0]
[null,null,"Poles / Columns ; Minor Road",null,0]
[null,null,"Other",null,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFUNCTION","Field Devices",null,1]
[null,null,"Local Network Wiring Assets",null,0]
[null,null,"Communications Network Assets",null,0]
[null,null,"Master Station Assets",null,0]
[null,null,"Communications Site Infrastructure",null,0]
[null,null,"Communications Linear Assets",null,0]
[null,null,"AFLC",null,0]
[null,null,"Other",null,0]
[null,"OTHER BY: \nDNSP DEFINED",{"$f":"IF(ISBLANK(C299),\"\",C299)","v":"Buildings"},null,0]
[null,null,"Instrument Transformers",null,0]
[null,null,"Metering Units",null,0]
[null,null,"Pillars",null,8]
[null,null,"Substation Auxiliary Plant",null,0]
[null,null,"Voltage Regulators",null,0]
[null,null,"Civil and Grounds",null,0]
[null,null,"Fire Systems",null,0]
[null,null,"Power Transformer Refurbishment",null,0]
[null,null,"Tower Refurbishment",null,0]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[]
[]
[]
[null,"2.2.2 - SELECTED ASSET CHARACTERISTICS"]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"TOTAL POLES BY: \nFEEDER TYPE","Total CBD poles","Number",0]
[null,null,"Total urban poles","Number",14]
[null,null,"Total rural long poles","Number",0]
[null,null,"Total rural short poles","Number",49]
[null,"OVERHEAD CONDUCTORS BY:\nCONDUCTOR LENGTH BY FEEDER TYPE","Conductors CBD (km)","KM",0]
[null,null,"Conductors urban (km)","KM",2.2000000000000002]
[null,null,"Conductors rural long (km)","KM",0]
[null,null,"Conductors rural short (km)","KM",6.3]
[null,"OVERHEAD CONDUCTORS BY: \nCONDUCTOR LENGTH MATERIAL TYPE","OH conductor LV ABC","KM",2.5]
[null,null,"OH conductor steel","KM",0.8]
[null,null,"OH conductor ACSR","KM",0.3]
[null,null,"OH conductor AAAC","KM",0]
[null,null,"OH conductor AAC","KM",5]
[null,null,"OH conductor HDBC","KM",0]
[null,null,"Other","KM",0]
[null,"UNDERGROUND CABLES BY: \nCABLE LENGTH BY FEEDER TYPE","Cable CBD (km)","KM",0.7]
[null,null,"Cable urban (km)","KM",1]
[null,null,"Cable rural long (km)","KM",0]
[null,null,"Cable rural short (km)","KM",0.6]
[null,"TRANSFORMERS BY: \nTOTAL MVA","Total MVA replaced","MVA",35]
[null,null,"Total MVA disposed of","MVA",32]
[]
[]
[null,"ASSETS IN COMMISSION"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"TOTAL POLES BY: \nFEEDER TYPE","Total CBD poles","Number",248]
[null,null,"Total urban poles","Number",7021]
[null,null,"Total rural long poles","Number",5765]
[null,null,"Total rural short poles","Number",31933]
[null,"OVERHEAD CONDUCTORS BY:\nCONDUCTOR LENGTH BY FEEDER TYPE","Conductors CBD (km)","KM",1]
[null,null,"Conductors urban (km)","KM",489]
[null,null,"Conductors rural long (km)","KM",949]
[null,null,"Conductors rural short (km)","KM",3988]
[null,"OVERHEAD CONDUCTORS BY: \nCONDUCTOR LENGTH MATERIAL TYPE","OH conductor LV ABC","KM",245]
[null,null,"OH conductor steel","KM",187]
[null,null,"OH conductor ACSR","KM",3054]
[null,null,"OH conductor AAAC","KM",1079]
[null,null,"OH conductor AAC","KM",862]
[null,null,"OH conductor HDBC","KM",1]
[null,null,"Other","KM",0]
[null,"UNDERGROUND CABLES BY: \nCABLE LENGTH BY FEEDER TYPE","Cable CBD (km)","KM",54]
[null,null,"Cable urban (km)","KM",564]
[null,null,"Cable rural long (km)","KM",3]
[null,null,"Cable rural short (km)","KM",1000]
[null,"TRANSFORMERS BY: \nTOTAL MVA","Total MVA replaced","MVA",0]
[null,null,"Total MVA disposed of","MVA",0]

{"sheet":"2.3(a) Augex","index":6,"n_rows":130,"n_cols":34,"rows_kept":130,"cut":false,"hidden":false,"merged":[[73,5,74,5],[6,1,6,3],[12,21,12,22],[11,11,11,22],[13,17,13,19],[73,11,73,13],[73,14,73,16],[72,1,72,10],[73,1,74,1],[73,2,74,2],[73,3,74,3],[73,4,74,4],[73,6,74,6],[12,3,13,3],[12,4,13,4],[12,5,13,5],[74,7,74,10],[73,7,73,10],[72,11,72,22],[73,17,73,19],[73,21,73,22],[72,23,72,24],[72,25,74,25],[72,26,74,26],[72,30,72,31],[74,23,74,24],[74,27,74,29],[74,30,74,31],[72,29,73,29],[72,27,72,28],[11,30,11,31],[11,23,11,24],[11,25,13,25],[11,26,13,26],[11,27,11,28],[11,29,12,29],[13,30,13,31],[12,1,13,1],[12,2,13,2],[13,27,13,29],[12,6,13,6],[12,16,12,19],[13,23,13,24],[12,7,12,8],[12,9,12,10],[12,11,12,13],[12,14,12,15]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both rows and columns have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"NOTE: DNSP MUST PROVIDE EXPENDITURE INFORMATION ON A PROJECT CLOSE BASIS. "]
[null,"AUG231_1","AUG231_2","AUG231_3","AUG231_4","AUG231_5","AUG231_6","ED_AUG231_00001","ED_AUG231_00002","ED_AUG231_00003","ED_AUG231_00004","ED_AUG231_00005","ED_AUG231_00006","ED_AUG231_00007","ED_AUG231_00008","ED_AUG231_00009","ED_AUG231_00010","ED_AUG231_00011",null,null,"ED_AUG231_00012","ED_AUG231_00013","ED_AUG231_00014","ED_AUG231_00015","ED_AUG231_00016","ED_AUG231_00017","ED_AUG231_00018","ED_AUG231_00019","ED_AUG231_00020","ED_AUG231_00021","ED_AUG231_00022","ED_AUG231_00023"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTYCONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE\n(drop down)","PROJECT ID","PROJECT TYPE\n(drop down)","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,"CAPACITORS",null,null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED","EXPENDITURE ($0's)","UNITS ADDED ","EXPENDITURE ($0's)","MVAR ADDED","EXPENDITURE ($0's)",null,null,"EXPENDITURE ($0's)","VOLUME","EXPENDITURE ($0's)","EXPENDITURE ($0's)",null,null,null,"EXPENDITURE ($0's)",null,null,"EXPENDITURE ($0's)"]
[null,"No Material projects in this category",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,0,0,0,0,{"$f":"SUM(N15,P15,R15,U15,W15,X15,Y15)","v":0},0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N47,P47,R47,U47,W47,X47,Y47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Non material projects - [actual]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221978,"2014-15 to 2017-18",null,null,null,0,0]
[]
[]
[null,"AUG232_1","AUG232_2","AUG232_3","AUG232_4","AUG232_5","AUG232_6","ED_AUG232_00001","ED_AUG232_00002","ED_AUG232_00003","ED_AUG232_00004","ED_AUG232_00005","ED_AUG232_00006","ED_AUG232_00007","ED_AUG232_00008","ED_AUG232_00009","ED_AUG232_00010","ED_AUG232_00011","ED_AUG232_00012","ED_AUG232_00013","ED_AUG232_00014","ED_AUG232_00015","ED_AUG232_00016","ED_AUG232_00017","ED_AUG232_00018","ED_AUG232_00019","ED_AUG232_00020","ED_AUG232_00021"]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"NOTE: DNSP MUST PROVIDE EXPENDITURE INFORMATION ON A PROJECT CLOSE BASIS."]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTYCONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID","PROJECT ID","PROJECT TYPE","PROJECT TRIGGER","PROJECT TRIGGER\n(drop down)","VOLTAGE (KV)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED","EXPENDITURE ($0's)","CIRCUIT KM ADDED","CIRCUIT KM UPGRADED","EXPENDITURE ($0's)","CIRCUIT KM ADDED","CIRCUIT KM UPGRADED","EXPENDITURE ($0's)","EXPENDITURE ($0's)","VOLUME","EXPENDITURE ($0's)","EXPENDITURE ($0's)",null,null,null,"EXPENDITURE ($0's)",null,null,"EXPENDITURE ($0's)"]
[null,"132 CI-HC A and B","PRD30003","Line rebuild over existing rout - dual circuit",null,"Other",132,0,0,null,null,null,6,2980970,0,4.2,1930714,0,0,0,0,24327,2811801,913325,0,{"$f":"SUM(N76,Q76,T76,U76,W76,X76,Y76)","v":8636810},"2011-12 to 2017-18",0,0,8063662,52084,0,null,"New line on new route - single circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"New line on new route - dual circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"New line on new route - other"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Line rebuild over existing route - single circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Line rebuild over existing route - dual circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Reconductor - Single circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Reconductor - Dual circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Reconductor - Other"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Line upgrade - raising/retensoring"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Line upgrade - voltage upgrade"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Line upgrade - capacity"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"String spare circuit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,"Other"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N108,Q108,T108,U108,W108,X108,Y108)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,"Non material projects - [actual]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,136080,"2015-16 to 2017-18",null,null,null,0,0]

{"sheet":"2.3(b) Augex","index":7,"n_rows":76,"n_cols":4,"rows_kept":76,"cut":false,"hidden":false,"merged":[[58,1,59,2],[65,1,66,2],[5,1,5,2],[29,1,30,2],[44,1,45,2],[9,1,10,1],[9,2,10,2],[60,1,60,2],[61,1,61,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.3 AUGEX  PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP MUST PROVIDE EXPENDITURE INFORMATION ON AN AS INCURRED BASIS."]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUME (0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",4]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0]
[null,"Distribution Substation Augmentations - Indoor","Number",0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",1]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0]
[null,"Distribution Substation Augmentations - Indoor","Number",0]
[]
[null,"COST METRICS"]
[null,"TOTAL DIRECT EXPENDITURE - Project Type",null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,0]
[null,"HV Feeder Augmentations - Underground Cables",null,0]
[null,"HV Feeder Non-Material Projects",null,1153235]
[null,"LV Feeder Augmentations - Overhead Lines",null,0]
[null,"LV Feeder Augmentations - Underground Cables",null,0]
[null,"LV Feeder Non-Material Projects",null,109651]
[null,"Distribution Substation Augmentations - Pole Mounted",null,167283]
[null,"Distribution Substation Augmentations - Ground Mounted",null,0]
[null,"Distribution Substation Augmentations - Indoor",null,0]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,"AUGMENTATION CAPEX (as incurred)",null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,5994274]
[null,"Subtransmission Lines",null,8769622]
[null,"HV Feeders",null,1153235]
[null,"HV Feeders - Land Purchases and Easements",null,0]
[null,"Distribution Substations",null,167283]
[null,"Distribution Substations - Land Purchases And Easements",null,0]
[null,"LV Feeders",null,109651]
[null,"LV Feeders - Land Purchases And Easements",null,0]
[null,"Other Assets",null,1431977]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,"AUGMENTATION CAPEX (as incurred)",null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,4150532]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,13475510]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVER"]
[null,"AUGMENTATION CAPEX (as incurred)",null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,619661]
[null,"Subtransmission Lines",null,2478643]
[null,"HV Feeders",null,25544]
[null,"HV Feeders - Land Purchases and Easements",null,0]
[null,"Distribution Substations",null,0]
[null,"Distribution Substations - Land Purchases And Easements",null,0]
[null,"LV Feeders",null,0]
[null,"LV Feeders - Land Purchases And Easements",null,0]
[null,"Other Assets",null,1026685]

{"sheet":"2.5 Connections","index":8,"n_rows":209,"n_cols":5,"rows_kept":209,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,null,null,null,"VOLUMES AND EXPENDITURE"]
[null,null,null,"Units",{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Underground connections","0's",117]
[null,null,"Overhead connections","0's",94]
[null,null,"Distribution substation installed (MVA added)","MVA",0.43]
[null,null,"Distribution substations installed","0's",6]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",149415]
[null,null,"Augmentation HV (net circuit KM added)","KM",0.2]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",62238]
[null,null,"Augmentation LV (net circuit KM added)","KM",0.5]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",142237]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",3]
[null,null,"Volume of GSL breaches for residential customers","0's",656]
[null,null,"Volume of customer complaints relating to connection services","0's",27]
[null,null,"GSL payments","$0s",42120]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",58]
[null,null,"Overhead connections","0's",12]
[null,null,"Distribution substation installed (MVA added)","MVA",5]
[null,null,"Distribution substations installed (0's)","0's",20]
[null,null,"Distribution substation installed (total spend ($0's)","total spend $0s",1188795]
[null,null,"Augmentation HV (net circuit KM added)","KM",0.2]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",274168]
[null,null,"Augmentation LV (net circuit KM added)","KM",0.5]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",196997]
[null,"SUBDIVISION","Underground connections","0's",404]
[null,null,"Overhead connections","0's",2]
[null,null,"Distribution substation installed (MVA added)","MVA",0]
[null,null,"Distribution substations installed","0's",5]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",192543]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",109754]
[null,null,"Augmentation LV (net circuit KM added)","KM",1]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",306760]
[null,null,"Cost per lot ($)","$0s",29003]
[null,"EMBEDDED GENERATION","Underground connections","0's",1157]
[null,null,"Overhead connections","0's",841]
[null,null,"Distribution substation installed (MVA added)","MVA",0]
[null,null,"Distribution substations installed","0's",0]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",0]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",0]
[null,null,"Augmentation LV (net circuit KM added)","KM",0]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES AND EXPENDITURE"]
[null,null,null,"Units",{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Underground connections","0's",117]
[null,null,"Overhead connections","0's",94]
[null,null,"Distribution substation installed (MVA added)","MVA",0]
[null,null,"Distribution substations installed","0's",6]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",149415]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",62238]
[null,null,"Augmentation LV (net circuit KM added)","KM",0]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",142237]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",3]
[null,null,"Volume of GSL breaches for residential customers","0's",656]
[null,null,"Volume of customer complaints relating to connection services","0's",27]
[null,null,"GSL payments","$0s",42120]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",58]
[null,null,"Overhead connections","0's",12]
[null,null,"Distribution substation installed (MVA added)","MVA",5]
[null,null,"Distribution substations installed (0's)","0's",20]
[null,null,"Distribution substation installed (total spend ($0's)","total spend $0s",1188795]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",274168]
[null,null,"Augmentation LV (net circuit KM added)","KM",1]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",196997]
[null,"SUBDIVISION","Underground connections","0's",404]
[null,null,"Overhead connections","0's",2]
[null,null,"Distribution substation installed (MVA added)","MVA",0]
[null,null,"Distribution substations installed","0's",5]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",192543]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",109754]
[null,null,"Augmentation LV (net circuit KM added)","KM",1]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",306760]
[null,null,"Cost per lot ($)","$0s",29003]
[null,"EMBEDDED GENERATION","Underground connections","0's",1157]
[null,null,"Overhead connections","0's",841]
[null,null,"Distribution substation installed (MVA added)","MVA",0]
[null,null,"Distribution substations installed","0's",0]
[null,null,"Distribution substation installed (total spend $0's)","total spend $0s",0]
[null,null,"Augmentation HV (net circuit KM added)","KM",0]
[null,null,"Augmentation HV (total spend $0's)","total spend $0s",0]
[null,null,"Augmentation LV (net circuit KM added)","KM",0]
[null,null,"Augmentation LV (total spend $0's)","total spend $0s",0]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,77223]
[null,null,"Complex connection LV",null,33572]
[null,null,"Complex connection HV",null,243096]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,131561]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1528401]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,261007]
[null,null,"Complex connection HV (no upstream asset works)",null,348050]
[null,null,"Complex connection HV (with upstream asset works)",null,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0]
[null,null,"Complex connection HV (small capacity)",null,0]
[null,null,"Complex connection HV (large capacity)",null,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,77223]
[null,null,"Complex connection LV",null,33572]
[null,null,"Complex connection HV",null,243096]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,131561]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1528401]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,261007]
[null,null,"Complex connection HV (no upstream asset works)",null,348050]
[null,null,"Complex connection HV (with upstream asset works)",null,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0]
[null,null,"Complex connection HV (small capacity)",null,0]
[null,null,"Complex connection HV (large capacity)",null,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,0]
[null,null,"Complex connection LV",null,0]
[null,null,"Complex connection HV",null,98842]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,10808]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1514102]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,838623]
[null,null,"Complex connection HV (customer connected at HV)",null,975013]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,498455]
[null,null,"Complex connection HV (no upstream asset works)",null,913699]
[null,null,"Complex connection HV (with upstream asset works)",null,3877449]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0]
[null,null,"Complex connection HV (small capacity)",null,0]
[null,null,"Complex connection HV (large capacity)",null,0]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,201]
[null,null,"Complex connection LV",null,2]
[null,null,"Complex connection HV",null,8]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,30]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,40]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,394]
[null,null,"Complex connection HV (no upstream asset works)",null,12]
[null,null,"Complex connection HV (with upstream asset works)",null,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,1998]
[null,null,"Complex connection HV (small capacity)",null,0]
[null,null,"Complex connection HV (large capacity)",null,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,201]
[null,null,"Complex connection LV",null,2]
[null,null,"Complex connection HV",null,8]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,30]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,40]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,394]
[null,null,"Complex connection HV (no upstream asset works)",null,12]
[null,null,"Complex connection HV (with upstream asset works)",null,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,1998]
[null,null,"Complex connection HV (small capacity)",null,0]
[null,null,"Complex connection HV (large capacity)",null,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"RESIDENTIAL","Simple connection LV",null,64155]
[null,null,"Complex connection LV",null,279]
[null,null,"Complex connection HV",null,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,10115]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,1220]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,567]
[null,null,"Complex connection HV (customer connected at HV)",null,47]
[null,null,"Complex connection sub-transmission",null,0]
[null,"SUBDIVISION","Complex connection LV",null,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,8890]
[null,null,"Complex connection HV (small capacity)",null,3]
[null,null,"Complex connection HV (large capacity)",null,0]

{"sheet":"2.6 Non-network","index":9,"n_rows":142,"n_cols":6,"rows_kept":142,"cut":false,"hidden":false,"merged":[[5,1,5,2],[108,1,112,1],[88,1,92,1],[93,1,97,1],[98,1,102,1],[103,1,107,1],[83,1,83,4],[82,1,82,4],[81,1,81,4],[9,2,9,4],[120,1,120,4],[121,1,121,4],[128,1,128,4],[125,1,125,4],[127,1,127,4],[122,1,122,4],[123,1,123,4],[124,1,124,4],[144,1,144,4],[145,1,145,4],[146,1,146,4],[138,1,138,4],[139,1,139,4],[141,1,141,4],[142,1,142,4],[143,1,143,4],[134,1,134,4],[135,1,135,4],[136,1,136,4],[137,1,137,4],[129,1,129,4],[130,1,130,4],[131,1,131,4],[132,1,132,4]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,null,"EXPENDITURE\n($0's)"]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,null,{"$f":"CRY","v":"2017-18"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total",null,null,1655419.05]
[null,"MOTOR VEHICLES","Car",null,null,646231.64]
[null,null,"Light commercial vehicle",null,null,2015392.79]
[null,null,"Elevated work platform (LCV)  ",null,null,0]
[null,null,"Elevated work platform (HCV)",null,null,1044022.54]
[null,null,"Heavy commercial vehicle",null,null,924321.42]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,null,1336847.78]
[null,"OTHER","Other expenditure",null,null,0]
[null,"OTHER - DNSP nominated"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total",null,null,2949776.36]
[null,"MOTOR VEHICLES","Car",null,null,0]
[null,null,"Light commercial vehicle",null,null,7968.88]
[null,null,"Elevated work platform (LCV)  ",null,null,0]
[null,null,"Elevated work platform (HCV)",null,null,0]
[null,null,"Heavy commercial vehicle",null,null,1080.51]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,null,478369.7]
[null,"OTHER","Other expenditure",null,null,399647.6]
[null,"OTHER - DNSP nominated","Test Equipment",null,null,244990.82]
[null,null,"Tools",null,null,383140.39]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.3 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Employee numbers",null,null,null,413.03]
[null,"User numbers",null,null,null,745.31]
[null,"Number of devices",null,null,null,969.41]
[]
[null,"MOTOR VEHICLES"]
[null,null,null,null,null,"VOLUMES / %"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC",null,"Units",{"$f":"CRY","v":"2017-18"}]
[null,"CAR","Average kilometres travelled",null,"0's",13982.19]
[null,null,"Number purchased",null,"0's",0]
[null,null,"Number leased",null,"0's",71.83]
[null,null,"Number in fleet",null,"0's",71.83]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure",null,"(per cent)",0.74299999999999999]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled",null,"0's",20612.34]
[null,null,"Number purchased",null,"0's",0.92]
[null,null,"Number leased",null,"0's",140.08000000000001]
[null,null,"Number in fleet",null,"0's",141]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure",null,"(per cent)",0.56230000000000002]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled",null,"0's",0]
[null,null,"Number purchased",null,"0's",0]
[null,null,"Number leased",null,"0's",0]
[null,null,"Number in fleet",null,"0's",0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure",null,"(per cent)",0]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled",null,"0's",16310.88]
[null,null,"Number purchased",null,"0's",0]
[null,null,"Number leased",null,"0's",19.420000000000002]
[null,null,"Number in fleet",null,"0's",19.420000000000002]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure",null,"(per cent)",1]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled",null,"0's",12434.5]
[null,null,"Number purchased",null,"0's",1]
[null,null,"Number leased",null,"0's",29]
[null,null,"Number in fleet",null,"0's",30]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure",null,"(per cent)",0.80710000000000004]
[]
[]
[]
[null,"2.6.4 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX BY PURPOSE"]
[null,null,null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"ICT CAPABILITY GROWTH"]
[null,"Audio Visual",null,null,null,44334.42]
[null,"Business Analytics",null,null,null,77184.100000000006]
[null,"Mobility",null,null,null,1091.31]
[null,"Outage Management Systems",null,null,null,1028824.64]
[null,"Portable Radio",null,null,null,29365.03]
[null,"Miscelleanous",null,null,null,11507.51]
[null,"ICT ASSET EXTENSIONS"]
[null,"Miscelleanous",null,null,null,16260.21]
[]
[]
[]
[]
[]
[null,"ICT ASSET REMEDIATION"]
[]
[]
[]
[]
[]
[]
[null,"ICT ASSET REPLACEMENT"]
[null,"400 MHZ Band Relocation",null,null,null,1741209.13]

{"sheet":"2.7 Vegetation management","index":10,"n_rows":406,"n_cols":5,"rows_kept":406,"cut":false,"hidden":false,"merged":[[59,1,64,1],[95,1,100,1],[101,1,106,1],[107,1,112,1],[113,1,118,1],[65,1,70,1],[71,1,76,1],[77,1,82,1],[83,1,88,1],[89,1,94,1],[5,1,5,2],[235,2,235,3],[9,1,10,1],[9,2,10,2],[9,3,10,3],[121,1,122,1],[121,2,122,2],[121,3,122,3],[11,1,16,1],[17,1,22,1],[23,1,28,1],[29,1,34,1],[35,1,40,1],[41,1,46,1],[47,1,52,1],[53,1,58,1]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.7 VEGETATION MANAGEMENT"]
[]
[null,"There are THREE tables on this worksheet. Each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group and ungroup data."]
[]
[null,"2.7.1 - DESCRIPTOR METRICS BY ZONE"]
[null,"URBAN AND CBD"]
[null,"ZONES","ASSET","Units","VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"ZONE 1","Route line length within zone","KM",259]
[null,null,"Number of maintenance spans","0's",3518]
[null,null,"Total length of maintenance spans","KM",126]
[null,null,"Length of vegetation corridors","KM",1]
[null,null,"Average number of trees per maintenance span","0's",3.5]
[null,null,"Average frequency of cutting cycle","years",0.5]
[null,"ZONE 2","Route line length within zone","KM",35]
[null,null,"Number of maintenance spans","0's",552]
[null,null,"Total length of maintenance spans","KM",20]
[null,null,"Length of vegetation corridors","KM",1]
[null,null,"Average number of trees per maintenance span","0's",3.4]
[null,null,"Average frequency of cutting cycle","years",0.5]
[null,"ZONE 3","Route line length within zone","KM",34]
[null,null,"Number of maintenance spans","0's",0]
[null,null,"Total length of maintenance spans","KM",0]
[null,null,"Length of vegetation corridors","KM",0]
[null,null,"Average number of trees per maintenance span","0's",0]
[null,null,"Average frequency of cutting cycle","years",1.5]
[null,"ZONE 4","Route line length within zone","KM",75]
[null,null,"Number of maintenance spans","0's",0]
[null,null,"Total length of maintenance spans","KM",0]
[null,null,"Length of vegetation corridors","KM",0]
[null,null,"Average number of trees per maintenance span","0's",0]
[null,null,"Average frequency of cutting cycle","years",1.5]
[null,"ZONE 5","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 6","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 7","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 8","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 9","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 10","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 11","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 12","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 13","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 14","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 15","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 16","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 17","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,"ZONE 18","Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[]
[null,"RURAL"]
[null,"ZONES","ASSET","Units","VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,{"$f":"IF(ISBLANK(B12),\"\",B12)","v":"ZONE 1"},"Route line length within zone","KM",2334]
[null,null,"Number of maintenance spans","0's",7777]
[null,null,"Total length of maintenance spans","KM",704]
[null,null,"Length of vegetation corridors","KM",254]
[null,null,"Average number of trees per maintenance span","0's",4.3]
[null,null,"Average frequency of cutting cycle","years",0.5]
[null,{"$f":"IF(ISBLANK(B18),\"\",B18)","v":"ZONE 2"},"Route line length within zone","KM",1150]
[null,null,"Number of maintenance spans","0's",2492]
[null,null,"Total length of maintenance spans","KM",281]
[null,null,"Length of vegetation corridors","KM",365]
[null,null,"Average number of trees per maintenance span","0's",5.3]
[null,null,"Average frequency of cutting cycle","years",0.5]
[null,{"$f":"IF(ISBLANK(B24),\"\",B24)","v":"ZONE 3"},"Route line length within zone","KM",327]
[null,null,"Number of maintenance spans","0's",0]
[null,null,"Total length of maintenance spans","KM",0]
[null,null,"Length of vegetation corridors","KM",0]
[null,null,"Average number of trees per maintenance span","0's",0]
[null,null,"Average frequency of cutting cycle","years",1.5]
[null,{"$f":"IF(ISBLANK(B30),\"\",B30)","v":"ZONE 4"},"Route line length within zone","KM",506]
[null,null,"Number of maintenance spans","0's",0]
[null,null,"Total length of maintenance spans","KM",0]
[null,null,"Length of vegetation corridors","KM",0]
[null,null,"Average number of trees per maintenance span","0's",0]
[null,null,"Average frequency of cutting cycle","years",1.5]
[null,{"$f":"IF(ISBLANK(B36),\"\",B36)","v":"ZONE 5"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B42),\"\",B42)","v":"ZONE 6"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B48),\"\",B48)","v":"ZONE 7"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B54),\"\",B54)","v":"ZONE 8"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B60),\"\",B60)","v":"ZONE 9"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B66),\"\",B66)","v":"ZONE 10"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B72),\"\",B72)","v":"ZONE 11"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B78),\"\",B78)","v":"ZONE 12"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B84),\"\",B84)","v":"ZONE 13"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B90),\"\",B90)","v":"ZONE 14"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B96),\"\",B96)","v":"ZONE 15"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B102),\"\",B102)","v":"ZONE 16"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B108),\"\",B108)","v":"ZONE 17"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[null,{"$f":"IF(ISBLANK(B114),\"\",B114)","v":"ZONE 18"},"Route line length within zone","KM"]
[null,null,"Number of maintenance spans","0's"]
[null,null,"Total length of maintenance spans","KM"]
[null,null,"Length of vegetation corridors","KM"]
[null,null,"Average number of trees per maintenance span","0's"]
[null,null,"Average frequency of cutting cycle","years"]
[]
[]
[null,"2.7.2 - EXPENDITURE METRICS BY ZONE"]
[null,null,null,null,"EXPENDITURE\n($0's)"]
[null,"ZONES","SERVICE SUBCATEGORY",null,{"$f":"CRY","v":"2017-18"}]
[null,{"$f":"IF(ISBLANK(B12),\"\",B12)","v":"ZONE 1"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B18),\"\",B18)","v":"ZONE 2"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B24),\"\",B24)","v":"ZONE 3"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B30),\"\",B30)","v":"ZONE 4"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B36),\"\",B36)","v":"ZONE 5"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B42),\"\",B42)","v":"ZONE 6"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B48),\"\",B48)","v":"ZONE 7"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B54),\"\",B54)","v":"ZONE 8"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B60),\"\",B60)","v":"ZONE 9"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B66),\"\",B66)","v":"ZONE 10"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B72),\"\",B72)","v":"ZONE 11"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B78),\"\",B78)","v":"ZONE 12"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B84),\"\",B84)","v":"ZONE 13"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B90),\"\",B90)","v":"ZONE 14"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B96),\"\",B96)","v":"ZONE 15"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B102),\"\",B102)","v":"ZONE 16"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B108),\"\",B108)","v":"ZONE 17"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[null,{"$f":"IF(ISBLANK(B114),\"\",B114)","v":"ZONE 18"},"Tree trimming (excluding hazard trees) "]
[null,null,"Hazard tree cutting "]
[null,null,"Ground clearance "]
[null,null,"Vegetation corridor clearance "]
[null,null,"Inspection "]
[null,null,"Vegetation audit "]
[null,null,"Contractor liaison expenditure "]
[null,null,"Tree replacement program costs "]
[null,null,"Other vegetation management costs not specified in sheet "]
[]
[null,"2.7.3 - DESCRIPTOR METRICS ACROSS ALL ZONES - UNPLANNED VEGETATION EVENTS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,"DESCRIPTOR METRIC",null,null,{"$f":"CRY","v":"2017-18"}]
[null,"Number of fire starts caused by vegetation grow-ins (NSP responsibility)",null,null,0]
[null,"Number of fire starts caused by vegetation blow-ins and fall-ins (NSP responsibility)",null,null,0]
[null,"Number of fire starts caused by vegetation grow-ins (other party responsibility)",null,null,0]
[null,"Number of fire starts caused by vegetation blow-ins and fall-ins (other party responsibility)",null,null,0]

{"sheet":"2.8 Maintenance","index":11,"n_rows":166,"n_cols":10,"rows_kept":166,"cut":false,"hidden":false,"merged":[[9,9,11,9],[149,1,150,1],[68,1,69,1],[5,1,5,2],[29,1,30,1],[110,1,111,1],[9,7,10,7],[9,8,11,8]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.8 MAINTENANCE"]
[]
[null,"There are TWO tables on this worksheet. It has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.8.1 - DESCRIPTOR METRICS FOR ROUTINE AND NON-ROUTINE MAINTENANCE"]
[null,"ASSET QUANTITY AT YEAR END"]
[null,null,null,null,null,"VOLUME",null,"AVERAGE AGE OF ASSET GROUP ","INSPECTION \nCYCLE \n(YEARS)","MAINTENANCE \nCYCLE \n(YEARS)"]
[null,null,null,null,null,"(0's)"]
[null,"MAINTENANCE ACTIVITY","MAINTENANCE ASSET CATEGORY","ASSET QUANTITY","Units",{"$f":"CRY","v":"2017-18"},null,{"$f":"CRY","v":"2017-18"}]
[null,"Pole top, overhead line & service line maintenance","Pole tops and overhead lines","Number of poles","Number",44966,null,30,3,0]
[null,null,"Service lines","Number of customers","Number",55683,null,27,0,0]
[null,"Pole inspection and treatment","All poles","Number of poles","Number",44966,null,30,3,0]
[null,"Overhead asset inspection","All overhead assets","Line patrolled (route KM)","KM",5428,null,29,3,0]
[null,"Network underground cable maintenance: by voltage","LV - 11 to 22 KV","Length (KM)","KM",1586,null,22,0,0]
[null,null,"33 KV and above","Length (KM)","KM",35,null,15,0,0]
[null,"Network underground cable maintenance: by location","Cbd","Length (KM)","KM",73,null,29,0,0]
[null,null,"Non-CBD","Length (KM)","KM",1548,null,23,0,0]
[null,"Distribution substation equipment & property maintenance","Distribution substation transformers","Number of installed transformers","Number",4757,null,18,3,0]
[null,null,"Distribution substation switchgear\n (within-substations and stand-alone switchgear)","Number of switches","Number",6368,null,23,3,0]
[null,null,"Distribution substation - other equipment","Earth mat","Number",1928,null,21,3,6]
[null,null,"Distribution substation - property","Number of distribution substation properties maintained","Number",343,null,21,3,0]
[null,"Zone substation equipment maintenance","Transformers - zone substation","Number","Number",69,null,22,0.08,6]
[null,null,"Transformers - distribution","Number of distribution transformers within zone substation","Number",0,null,0,0,0]
[null,null,"Transformers - HV","Number of HV transformers","Number",0,null,0,0,0]
[null,null,"Zone substation - other equipment","Other ZSS assets",null,1175,null,18,0.08,3]
[null,"Zone substation property maintenance","All zone substation properties","Number of zone substation properties maintained","Number",36,null,28,0.08,0.08]
[null,"Public lighting maintenance","Minor roads","Number of public lights maintained","Number",0,null,0,0,0]
[null,null,"Major roads","Number of public lights maintained","Number",0,null,0,0,0]
[null,"SCADA & network control maintenance","SCADA & network control","Number of systems","Number",110,null,10,3,1]
[null,"Protection systems maintenance","Protection systems","Number of systems","Number",1310,null,12,0,3]
[null,"Subtransmission asset maintenance","Subtransmission asset maintenance\n- for DNSPs with dual function assets",0,null,0,null,0,0,0]
[null,"Various assets"," includes rates, electricity, communications equip, metering","Various","Number",0,null,0,0,0]
[null,"Ground clearance - access tracks","Access tracks","Number","Number",0,null,0,0,0]
[null,"Other","Pillars","Number of pillars",null,7431,null,18,10,0]
[null,null,"Communications","Number of assets",null,761,null,10,3,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET QUANTITY INSPECTED / MAINTAINED"]
[null,null,null,null,null,"VOLUME"]
[null,null,null,null,null,"(0's)"]
[null,"MAINTENANCE ACTIVITY","MAINTENANCE ASSET CATEGORY","ASSET QUANTITY","Units",{"$f":"CRY","v":"2017-18"}]
[null,"Pole top, overhead line & service line maintenance","Pole tops and overhead lines","Number of poles","Number",15182]
[null,null,"Service lines","Number of customers","Number",6]
[null,"Pole inspection and treatment","All poles","Number of poles","Number",14989]
[null,"Overhead asset inspection","All overhead assets","Line patrolled (route KM)","KM",1809]
[null,"Network underground cable maintenance: by voltage","LV - 11 to 22 KV","Length (KM)","KM",32]
[null,null,"33 KV and above","Length (KM)","KM",1]
[null,"Network underground cable maintenance: by location","Cbd","Length (KM)","KM",1]
[null,null,"Non-CBD","Length (KM)","KM",32]
[null,"Distribution substation equipment & property maintenance","Distribution substation transformers","Number of installed transformers","Number",2114]
[null,null,"Distribution substation switchgear\n (within-substations and stand-alone switchgear)","Number of switches","Number",2395]
[null,null,"Distribution substation - other equipment","Earth mat","Number",156]
[null,null,"Distribution substation - property","Number of distribution substation properties maintained","Number",126]
[null,"Zone substation equipment maintenance","Transformers - zone substation","Number","Number",1062]
[null,null,"Transformers - distribution","Number of distribution transformers within zone substation","Number",0]
[null,null,"Transformers - HV","Number of HV transformers","Number",0]
[null,null,"Zone substation - other equipment",{"$f":"IF(ISBLANK(D28),\"\",D28)","v":"Other ZSS assets"},{"$f":"IF(ISBLANK(E28),\"\",E28)","v":""},14957]
[null,"Zone substation property maintenance","All zone substation properties","Number of zone substation properties maintained","Number",826]
[null,"Public lighting maintenance","Minor roads","Number of public lights maintained","Number",0]
[null,null,"Major roads","Number of public lights maintained","Number",0]
[null,"SCADA & network control maintenance","SCADA & network control","Number of systems","Number",159]
[null,"Protection systems maintenance","Protection systems","Number of systems","Number",174]
[null,"Subtransmission asset maintenance","Subtransmission asset maintenance\n- for DNSPs with dual function assets",{"$f":"IF(ISBLANK(D34),\"\",D34)","v":0},{"$f":"IF(ISBLANK(E34),\"\",E34)","v":""},0]
[null,"Various assets"," includes rates, electricity, communications equip, metering","Various","Number",0]
[null,"Ground clearance - access tracks","Access tracks","Number","Number",0]
[null,"Other",{"$f":"IF(ISBLANK(C37),\"\",C37)","v":"Pillars"},"Number of pillars",null,752]
[null,null,"Communications","Number of assets",null,379]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[]
[]
[]
[null,"2.8.2 - COST METRICS FOR ROUTINE AND NON-ROUTINE MAINTENANCE"]
[null,"ROUTINE MAINTENANCE"]
[null,null,null,null,null,"EXPENDITURE"]
[null,null,null,null,null,"($0'S)"]
[null,"MAINTENANCE ACTIVITY","MAINTENANCE ASSET CATEGORY","ASSET QUANTITY","Units",{"$f":"CRY","v":"2017-18"}]
[null,"Pole top, overhead line & service line maintenance","Pole tops and overhead lines","Number of poles","Number",147968]
[null,null,"Service lines","Number of customers","Number",0]
[null,"Pole inspection and treatment","All poles","Number of poles","Number",106238]
[null,"Overhead asset inspection","All overhead assets","Line patrolled (route KM)","KM",174413]
[null,"Network underground cable maintenance: by voltage","LV - 11 to 22 KV","Length (KM)","KM",40689]
[null,null,"33 KV and above","Length (KM)","KM",0]
[null,"Network underground cable maintenance: by location","Cbd","Length (KM)","KM",3112]
[null,null,"Non-CBD","Length (KM)","KM",37578]
[null,"Distribution substation equipment & property maintenance","Distribution substation transformers","Number of installed transformers","Number",339209]
[null,null,"Distribution substation switchgear\n (within-substations and stand-alone switchgear)","Number of switches","Number",394395]
[null,null,"Distribution substation - other equipment","Earth mat","Number",136770]
[null,null,"Distribution substation - property","Number of distribution substation properties maintained","Number",18410]
[null,"Zone substation equipment maintenance","Transformers - zone substation","Number","Number",298529]
[null,null,"Transformers - distribution","Number of distribution transformers within zone substation","Number",0]
[null,null,"Transformers - HV","Number of HV transformers","Number",0]
[null,null,"Zone substation - other equipment",{"$f":"IF(ISBLANK(D28),\"\",D28)","v":"Other ZSS assets"},{"$f":"IF(ISBLANK(E28),\"\",E28)","v":""},813713]
[null,"Zone substation property maintenance","All zone substation properties","Number of zone substation properties maintained","Number",454205]
[null,"Public lighting maintenance","Minor roads","Number of public lights maintained","Number",0]
[null,null,"Major roads","Number of public lights maintained","Number",0]
[null,"SCADA & network control maintenance","SCADA & network control","Number of systems","Number",78409]
[null,"Protection systems maintenance","Protection systems","Number of systems","Number",317821]
[null,"Subtransmission asset maintenance","Subtransmission asset maintenance\n- for DNSPs with dual function assets",{"$f":"IF(ISBLANK(D34),\"\",D34)","v":0},{"$f":"IF(ISBLANK(E34),\"\",E34)","v":""},0]
[null,"Various assets"," includes rates, electricity, communications equip, metering","Various","Number",0]
[null,"Ground clearance - access tracks","Access tracks","Number","Number",0]
[null,"Other",{"$f":"IF(ISBLANK(C37),\"\",C37)","v":"Pillars"},"Number of pillars",null,161545]
[null,null,"Communications","Number of assets",null,154751]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[]
[null,"NON-ROUTINE MAINTENANCE"]
[null,null,null,null,null,"EXPENDITURE"]
[null,null,null,null,null,"($0'S)"]
[null,"MAINTENANCE ACTIVITY","MAINTENANCE ASSET CATEGORY","ASSET QUANTITY","Units",{"$f":"CRY","v":"2017-18"}]
[null,"Pole top, overhead line & service line maintenance","Pole tops and overhead lines","Number of poles","Number",1247923]
[null,null,"Service lines","Number of customers","Number",48153]
[null,"Pole inspection and treatment","All poles","Number of poles","Number",0]
[null,"Overhead asset inspection","All overhead assets","Line patrolled (route KM)","KM",0]
[null,"Network underground cable maintenance: by voltage","LV - 11 to 22 KV","Length (KM)","KM",609464]
[null,null,"33 KV and above","Length (KM)","KM",3489]
[null,"Network underground cable maintenance: by location","Cbd","Length (KM)","KM",21297]
[null,null,"Non-CBD","Length (KM)","KM",591656]
[null,"Distribution substation equipment & property maintenance","Distribution substation transformers","Number of installed transformers","Number",2128371]
[null,null,"Distribution substation switchgear\n (within-substations and stand-alone switchgear)","Number of switches","Number",691959]
[null,null,"Distribution substation - other equipment","Earth mat","Number",708905]
[null,null,"Distribution substation - property","Number of distribution substation properties maintained","Number",95005]
[null,"Zone substation equipment maintenance","Transformers - zone substation","Number","Number",1005550]
[null,null,"Transformers - distribution","Number of distribution transformers within zone substation","Number",0]
[null,null,"Transformers - HV","Number of HV transformers","Number",0]
[null,null,"Zone substation - other equipment",{"$f":"IF(ISBLANK(D28),\"\",D28)","v":"Other ZSS assets"},{"$f":"IF(ISBLANK(E28),\"\",E28)","v":""},1149554]
[null,"Zone substation property maintenance","All zone substation properties","Number of zone substation properties maintained","Number",799420]
[null,"Public lighting maintenance","Minor roads","Number of public lights maintained","Number",0]
[null,null,"Major roads","Number of public lights maintained","Number",0]
[null,"SCADA & network control maintenance","SCADA & network control","Number of systems","Number",331541]
[null,"Protection systems maintenance","Protection systems","Number of systems","Number",661808]
[null,"Subtransmission asset maintenance","Subtransmission asset maintenance\n- for DNSPs with dual function assets",{"$f":"IF(ISBLANK(D34),\"\",D34)","v":0},{"$f":"IF(ISBLANK(E34),\"\",E34)","v":""},0]
[null,"Various assets"," includes rates, electricity, communications equip, metering","Various","Number",0]
[null,"Ground clearance - access tracks","Access tracks","Number","Number",0]
[null,"Other",{"$f":"IF(ISBLANK(C37),\"\",C37)","v":"Pillars"},"Number of pillars",null,598284]
[null,null,"Communications","Number of assets",null,375673]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]
[null,null,"",""]

{"sheet":"2.9 Emergency Response","index":12,"n_rows":159,"n_cols":3,"rows_kept":159,"cut":false,"hidden":false,"merged":[]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.9 EMERGENCY RESPONSE"]
[]
[null,"There is ONE table on this worksheet. It has been 'sub-grouped' for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.9.1 - EMERGENCY RESPONSE EXPENDITURE (OPEX)"]
[null,null,"EXPENDITURE\n($0's)"]
[null,null,{"$f":"CRY","v":"2017-18"}]
[null,"(A) TOTAL EMERGENCY RESPONSE EXPENDITURE"]
[null,"Total Expenditure",8947734]
[null,"(B) MAJOR EVENTS O&M EXPENDITURE"]
[null,"Cyclone Marcus",2732798]
[null,"Tennant Creek UFLS",0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"(C) MAJOR EVENT DAYS O&M EXPENDITURE"]
[null,"Sunday, 18 March 2018",160455]
[null,"Monday, 19 March 2018",147823]
[null,"Tuesday, 20 March 2018",162392]
[null,"Wednesday, 21 March 2018",139312]
[null,"Thursday, 22 March 2018",126377]
[null,"Friday, 23 March 2018",105775]
[null,"Saturday, 24 March 2018",80095]
[null,"Sunday, 25 March 2018",82388]
[null,"Monday, 26 March 2018",161082]
[null,"Tuesday, 27 March 2018",86799]
[null,"Wednesday, 28 March 2018",92565]
[null,"Thursday, 29 March 2018",128141]
[null,"Friday, 30 March 2018",334515]
[null,"Saturday, 31 March 2018",0]
[null,"Sunday, 1 April 2018",366]
[null,"Monday, 2 April 2018",806]
[null,"Tuesday, 3 April 2018",53275]
[null,"Wednesday, 4 April 2018",9141]
[null,"Thursday, 5 April 2018",43294]
[null,"Friday, 6 April 2018",26543]
[null,"Saturday, 7 April 2018",779]
[null,"Sunday, 8 April 2018",5129]
[null,"Monday, 9 April 2018",46525]
[null,"Tuesday, 10 April 2018",94520]
[null,"Wednesday, 11 April 2018",8308]
[null,"Thursday, 12 April 2018",16657]
[null,"Friday, 13 April 2018",16627]
[null,"Saturday, 14 April 2018",0]
[null,"Sunday, 15 April 2018",0]
[null,"Monday, 16 April 2018",38499]
[null,"Tuesday, 17 April 2018",44405]
[null,"Wednesday, 18 April 2018",9297]
[null,"Thursday, 19 April 2018",8368]
[null,"Friday, 20 April 2018",12597]
[null,"Saturday, 21 April 2018","(141)"]
[null,"Sunday, 22 April 2018",0]
[null,"Monday, 23 April 2018",31691]
[null,"Tuesday, 24 April 2018",18247]
[null,"Wednesday, 25 April 2018",0]
[null,"Thursday, 26 April 2018",25442]
[null,"Friday, 27 April 2018",10390]
[null,"Saturday, 28 April 2018",0]
[null,"Sunday, 29 April 2018",0]
[null,"Monday, 30 April 2018",22223]
[null,"Tuesday, 1 May 2018",12908]
[null,"Wednesday, 2 May 2018",26449]
[null,"Thursday, 3 May 2018",0]
[null,"Friday, 4 May 2018",85]
[null,"Saturday, 5 May 2018",0]
[null,"Sunday, 6 May 2018",1374]
[null,"Monday, 7 May 2018",0]
[null,"Tuesday, 8 May 2018",32153]
[null,"Wednesday, 9 May 2018",3004]
[null,"Thursday, 10 May 2018",1712]
[null,"Friday, 11 May 2018",2401]
[null,"Saturday, 12 May 2018",626]
[null,"Sunday, 13 May 2018",0]
[null,"Monday, 14 May 2018",979]
[null,"Tuesday, 15 May 2018",4749]
[null,"Wednesday, 16 May 2018",17330]
[null,"Thursday, 17 May 2018",5527]
[null,"Friday, 18 May 2018",2073]
[null,"Saturday, 19 May 2018",902]
[null,"Sunday, 20 May 2018",0]
[null,"Monday, 21 May 2018",70408]
[null,"Tuesday, 22 May 2018",24871]
[null,"Wednesday, 23 May 2018",2065]
[null,"Thursday, 24 May 2018",182]
[null,"Friday, 25 May 2018",3082]
[null,"Saturday, 26 May 2018",0]
[null,"Sunday, 27 May 2018",3664]
[null,"Monday, 28 May 2018",33440]
[null,"Tuesday, 29 May 2018",3125]
[null,"Wednesday, 30 May 2018",12100]
[null,"Thursday, 31 May 2018",8341]
[null,"Friday, 1 June 2018",1888]
[null,"Saturday, 2 June 2018",0]
[null,"Sunday, 3 June 2018",3664]
[null,"Monday, 4 June 2018",4633]
[null,"Tuesday, 5 June 2018",4053]
[null,"Wednesday, 6 June 2018",2043]
[null,"Thursday, 7 June 2018",57077]
[null,"Friday, 8 June 2018","(1,094)"]
[null,"Saturday, 9 June 2018",0]
[null,"Sunday, 10 June 2018",0]
[null,"Monday, 11 June 2018",0]
[null,"Tuesday, 12 June 2018",929]
[null,"Wednesday, 13 June 2018",0]
[null,"Thursday, 14 June 2018",3448]
[null,"Friday, 15 June 2018",12255]
[null,"Saturday, 16 June 2018",0]
[null,"Sunday, 17 June 2018",0]
[null,"Monday, 18 June 2018",123]
[null,"Tuesday, 19 June 2018",1206]
[null,"Wednesday, 20 June 2018",5576]
[null,"Thursday, 21 June 2018",1139]
[null,"Friday, 22 June 2018",1666]
[null,"Saturday, 23 June 2018",0]
[null,"Sunday, 24 June 2018",0]
[null,"Monday, 25 June 2018",921]
[null,"Tuesday, 26 June 2018",4307]
[null,"Wednesday, 27 June 2018",4710]

{"sheet":"2.10 network overheads","index":13,"n_rows":34,"n_cols":4,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,"Power and Water Corporation"]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",37977439.82]
[null,"Alternative Control Services","Total  ",2165072.2999999998]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",8183999.0700000003]
[null,"Alternative Control Services","Total  ",303490.36]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",0]
[null,"Unregulated Services","Total  ",1734681.51]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,"EXPENDITURE\n($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"OPEX"]
[null,"Standard Control Services","Total",13381112.630000001]
[null,"Alternative Control Services","Total",1668310.19]
[null,"CAPEX"]
[null,"Standard Control Services","Total",3048696.56]
[null,"Alternative Control Services","Total",380100.8]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",0]
[null,"Unregulated Services","Total",956089.92]

{"sheet":"2.11 Labour","index":14,"n_rows":176,"n_cols":4,"rows_kept":176,"cut":false,"hidden":false,"merged":[[5,1,5,3],[43,1,43,2],[76,1,76,2],[10,1,10,2],[109,1,109,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.11 LABOUR"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.11.1 - COST METRICS PER ANNUM"]
[null,"AVERAGE STAFFING LEVEL (ASL)"]
[null,null,null,"VOLUME\n(0's)"]
[null,"INTERNAL LABOUR",null,{"$f":"CRY","v":"2017-18"}]
[null,"CORPORATE OVERHEADS","Executive manager",3.79]
[null,null,"Senior manager",3.9]
[null,null,"Manager",10.73]
[null,null,"Professional",6.77]
[null,null,"Semi professional",0]
[null,null,"Support staff",26.68]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NETWORK OVERHEADS ","Executive manager",2.13]
[null,null,"Senior manager",15.69]
[null,null,"Manager",33.950000000000003]
[null,null,"Professional",65.7]
[null,null,"Semi professional",6.04]
[null,null,"Support staff",49.35]
[null,null,"Intern, junior staff, apprentice",1.43]
[null,"NON-NETWORK LABOUR ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"DIRECT OPEX LABOUR ","Skilled electrical worker",87.41]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",26.26]
[null,null,"Unskilled worker",0]
[null,"DIRECT CAPEX LABOUR","Skilled electrical worker",56.29]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",16.91]
[null,null,"Unskilled worker",0]
[]
[null,"TOTAL LABOUR EXPENDITURE"]
[null,null,null,"EXPENDITURE \n($0's)"]
[null,"INTERNAL LABOUR",null,{"$f":"CRY","v":"2017-18"}]
[null,"CORPORATE OVERHEADS","Executive manager",503333.32]
[null,null,"Senior manager",680621.17]
[null,null,"Manager",1386851.25]
[null,null,"Professional",706060.44]
[null,null,"Semi professional",0]
[null,null,"Support staff",2268260.35]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NETWORK OVERHEADS ","Executive manager",575229.56000000006]
[null,null,"Senior manager",3400366.47]
[null,null,"Manager",6051258.4299999997]
[null,null,"Professional",10718683.99]
[null,null,"Semi professional",1046118.01]
[null,null,"Support staff",4959967.9800000004]
[null,null,"Intern, junior staff, apprentice",111775.38]
[null,"NON-NETWORK LABOUR ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"DIRECT OPEX LABOUR ","Skilled electrical worker",14681503.310000001]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",3105921.4]
[null,null,"Unskilled worker",0]
[null,"DIRECT CAPEX LABOUR","Skilled electrical worker",9455078.9800000004]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",2000253.76]
[null,null,"Unskilled worker",0]
[]
[null,"AVERAGE PRODUCTIVE WORK HOURS PER ASL "]
[null,null,null,"VOLUME\n(0's)"]
[null,"INTERNAL LABOUR",null,{"$f":"CRY","v":"2017-18"}]
[null,"CORPORATE OVERHEADS","Executive manager",543.66]
[null,null,"Senior manager",562.5]
[null,null,"Manager",553.88]
[null,null,"Professional",595.39]
[null,null,"Semi professional",0]
[null,null,"Support staff",580.87]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NETWORK OVERHEADS ","Executive manager",921.67]
[null,null,"Senior manager",973.78]
[null,null,"Manager",868.63]
[null,null,"Professional",1014.88]
[null,null,"Semi professional",503.42]
[null,null,"Support staff",538.51]
[null,null,"Intern, junior staff, apprentice",697.61]
[null,"NON-NETWORK LABOUR ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"DIRECT OPEX LABOUR ","Skilled electrical worker",673.05]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",651.65]
[null,null,"Unskilled worker",0]
[null,"DIRECT CAPEX LABOUR","Skilled electrical worker",433.45]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",419.67]
[null,null,"Unskilled worker",0]
[]
[null,"STAND DOWN OCCURRENCES PER ASL"]
[null,null,null,"VOLUME\n(0's)"]
[null,"INTERNAL LABOUR",null,{"$f":"CRY","v":"2017-18"}]
[null,"CORPORATE OVERHEADS","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NETWORK OVERHEADS ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NON-NETWORK LABOUR ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"DIRECT OPEX LABOUR ","Skilled electrical worker",0.46]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",0.43]
[null,null,"Unskilled worker",0]
[null,"DIRECT CAPEX LABOUR","Skilled electrical worker",0.3]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",0.27]
[null,null,"Unskilled worker",0]
[]
[]
[]
[null,"2.11.2 - EXTRA DESCRIPTOR METRICS FOR CURRENT YEAR"]
[null,"AVERAGE PRODUCTIVE WORK HOURS PER ASL"]
[null,null,null,"ORDINARY TIME"]
[null,null,null,"PER ASL\n(0s)"]
[null,null,null,{"$f":"CRY","v":"2017-18"}]
[null,"CORPORATE OVERHEADS","Executive manager",561.73]
[null,null,"Senior manager",593.65]
[null,null,"Manager",599.04]
[null,null,"Professional",629.05999999999995]
[null,null,"Semi professional",0]
[null,null,"Support staff",610.01]
[null,null,"Intern, junior staff, apprentice",0]
[null,"NETWORK OVERHEADS ","Executive manager",1019.22]
[null,null,"Senior manager",1130.96]
[null,null,"Manager",993.84]
[null,null,"Professional",1164.6300000000001]
[null,null,"Semi professional",541.77]
[null,null,"Support staff",585.77]
[null,null,"Intern, junior staff, apprentice",749.6]
[null,"NON-NETWORK LABOUR ","Executive manager",0]
[null,null,"Senior manager",0]
[null,null,"Manager",0]
[null,null,"Professional",0]
[null,null,"Semi professional",0]
[null,null,"Support staff",0]
[null,null,"Intern, junior staff, apprentice",0]
[null,"DIRECT OPEX LABOUR ","Skilled electrical worker",804.21]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",791.69]
[null,null,"Unskilled worker",0]
[null,"DIRECT CAPEX LABOUR","Skilled electrical worker",517.91999999999996]
[null,null,"Skilled non electical worker",0]
[null,null,"Apprentice",509.86]
[null,null,"Unskilled worker",0]

{"sheet":"2.12 Input tables","index":15,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[[9,3,9,8],[5,1,5,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"2.12 INPUT TABLES"]
[]
[null,"There are SIX tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.12  INPUT TABLES"]
[null,null,null,"DIRECT MATERIAL EXPENDITURE","DIRECT LABOUR EXPENDITURE","CONTRACT EXPENDITURE","OTHER EXPENDITURE","RELATED PARTY CONTRACT EXPENDITURE","RELATED PARTY CONTRACT MARGIN\nEXPENDITURE"]
[null,null,null,"EXPENDITURE ($0's)"]
[null,null,null,{"$f":"CRY","v":"2017-18"},"2017-18","2017-18","2017-18","2017-18","2017-18"]
[null,"VEGETATION MANAGEMENT","All zones",0,228201.23,3882616.35,0,0,0]
[null,"MAINTENANCE","All maintenance expenditure",765813.73,10540633.470000001,2785718.77,0,0,0]
[null,"OVERHEADS","Network overheads - opex",648567.42000000004,28464384.620000001,6466190.5599999996,4563369.5199999996,0,0]
[null,null,"Network overheads - capex",0,8414403.5099999998,73085.91,0,0,0]
[null,null,"Corporate overheads - opex",145614.32999999999,6650163.1699999999,2170268.67,6083376.6600000001,0,0]
[null,null,"Corporate overheads - capex",33176.160000000003,1515145.28,494464.91,1386011.02,0,0]
[null,"AUGMENTATION","All augex",2472462.6,1997276.75,13156302.380000001,0,0,0]
[null,"CONNECTIONS","Simple and complex customer connections",773493.63,1220988.67,628426.34,0,0,0]
[null,"EMERGENCY RESPONSE","All major storms and major event days",754299.97,7038644,1154790.23,0,0,0]
[null,"PUBLIC LIGHTING","All public lighting services",0,0,0,0,0,0]
[null,"METERING","All metering services",1908436.46,1912023.2,2003936.7,47251.199999999997,0,0]
[null,"FEE-BASED SERVICES","All fee-based services",14812.81,1734756.42,13211.06,0,0,0]
[null,"QUOTED SERVICES","All quoted services",377263.88,1592742.75,961091.06,0,0,0]
[null,"REPLACEMENT","All replacement expenditure",3806868.5,7407860.46,7450112.71,0,0,0]
[null,"NON-NETWORK EXPENDITURE","Opex",0,0,0,7622235.2199999997,0,0]
[null,null,"Capex",950525.14,829206.86,2685242.25,0,0,0]

{"sheet":"4.2 Metering","index":16,"n_rows":100,"n_cols":5,"rows_kept":100,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,"VOLUMES\n(0's)"]
[null,"Asset Category","Asset Subcategory",{"$f":"CRY","v":"2017-18"}]
[null,"Meter Type 1","Single phase meter population ",0]
[null,null,"Multi phase meter population ",0]
[null,null,"Current transformer connected meter population ",0]
[null,null,"Direct connect meter population ",0]
[null,"Meter Type 2","Single phase meter population ",0]
[null,null,"Multi phase meter population ",14]
[null,null,"Current transformer connected meter population ",14]
[null,null,"Direct connect meter population ",0]
[null,"Meter Type 3","Single phase meter population ",0]
[null,null,"Multi phase meter population ",326]
[null,null,"Current transformer connected meter population ",318]
[null,null,"Direct connect meter population ",8]
[null,"Meter Type 4","Single phase meter population ",4545]
[null,null,"Multi phase meter population ",3156]
[null,null,"Current transformer connected meter population ",1725]
[null,null,"Direct connect meter population ",5976]
[null,"Meter Type 5","Single phase meter population ",0]
[null,null,"Multi phase meter population ",0]
[null,null,"Current transformer connected meter population ",0]
[null,null,"Direct connect meter population ",0]
[null,"Meter Type 6","Single phase meter population ",93669]
[null,null,"Multi phase meter population ",5834]
[null,null,"Current transformer connected meter population ",704]
[null,null,"Direct connect meter population ",98799]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,null,null,"VOLUMES\n(0's)","EXPENDITURE\n($0's)"]
[null,"Service Subcategory","Meter Type",{"$f":"CRY","v":"2017-18"},{"$f":"CRY","v":"2017-18"}]
[null,"Meter purchase ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Meter testing ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Meter investigation ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Scheduled meter reading ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Special meter reading ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"New meter installation ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Meter replacement ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Meter maintenance ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,"Remote meter reading ","Meter Type 4"]
[null,"Remote meter re-configuration ","Meter Type 4"]
[null,"Other metering ","Meter Type 1"]
[null,null,"Meter Type 2"]
[null,null,"Meter Type 3"]
[null,null,"Meter Type 4"]
[null,null,"Meter Type 5"]
[null,null,"Meter Type 6"]
[null,null,"Meter Type 7"]
[null,"IT infrastructure capex ","Meter Type 4"]
[null,"IT infrastructure opex ","Meter Type 4"]
[null,"Communications infrastructure capex ","Meter Type 4"]
[null,"Communications infrastructure opex ","Meter Type 4"]

{"sheet":"4.3 Fee-based services","index":17,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There is ONE table on this worksheet. The COLUMNS AND ROWS have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"COMMON FEE-BASED SERVICES"]
[null,null,"EXPENDITURE \n($0's)","VOLUMES \n(0's)"]
[null,"SERVICE SUBCATEGORY",{"$f":"CRY","v":"2017-18"},{"$f":"CRY","v":"2017-18"}]
[null,"Energisation",0,0]
[null,"De-energisation",124530.34,2465]
[null,"Re-energisation",124530.34,2465]
[]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Disconnection - with comms (remote change)",0,0]
[null,"Reconnection - with comms (remote change)",0,0]
[null,"Remove and Reinstate Cable",65522,100]
[null,"Provision of three phase service",53131.99,32]
[null,"Standard temporary builder's connection",0,0]
[null,"Temporary disconnection and reconnection",139641.06,305]
[null,"Disconnection - physical disconnection of the service mains at the connection to the network (Pillar Box, Pit or Pole Top) due to action or inaction of the network user or their agent",0,0]
[null,"After hours attendance charge",34046.629999999997,95]
[null,"Wasted visit fee",0,0]
[null,"Special Meter Test",2495.17,6]
[null,"Exchange or Replace Meter - 3 Phase #",261825.72,345]
[null,"Exchange or Replace Meter - Standard #",729827.44,1135]
[null,"Relocation of Meter",634.91,2]
[null,"Remove Meter - Permanent removal of connection point (meter) from meter panel",10964.53,26]
[null,"General Meter Inspection",178.06,1]
[null,"Special Meter Read",637.28,8]
[null,"Meter Program Change - no comms",89205.16,410]
[null,"Meter Program Change - with comms",0,0]
[null,"Meter Data Processing Services",0,0]
[null,"Historical Data requests",104158.69,493]
[null,"Standing Data requests",21450.99,123]
[null,"Customer Transfers",0,0]
[null,"Network Tariff change request",0,0]
[null,"Installation of Minor Apparatus",0,0]

{"sheet":"4.4 Quoted services","index":18,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,1,9,1]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There is ONE table on this worksheet. The COLUMNS  have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY","EXPENDITURE \n($0's)","VOLUMES \n(0's)"]
[null,null,{"$f":"CRY","v":"2017-18"},{"$f":"CRY","v":"2017-18"}]
[null,"Design related services",121603.41,4]
[null,"Connection applications",256573.36,23]
[null,"Access permits, oversights and facilitation",949805.63,76]
[null,"Notices of arrangement and completion notices",0,0]
[null,"Network related property services",8283.5499999999993,1]
[null,"Site establishment services",1193.1500000000001,1]
[null,"Network safety services",161191.70000000001,90]
[null,"Network tariff change request",137.68,1]
[null,"Planned interruption - customer request",1861.84,2]
[null,"Performance of a statutory right (access prevented)",0,0]
[null,"Provision of network related training to third parties",0,0]
[null,"Non-standard reporting services",1101.3699999999999,1]
[null,"Services provided for retailer of last resort event",0,0]
[null,"Rectification of illegal connections service",0,0]
[null,"Rearrangement and connection of network assets at customer request",1429346,180]

{"sheet":"5.2 Asset Age Profile","index":19,"n_rows":139,"n_cols":123,"rows_kept":139,"cut":false,"hidden":false,"merged":[[8,3,8,4]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"5.2 ASSET AGE PROFILE"]
[]
[null,"There is ONE table on this worksheet. Both ROWS and COLUMNS have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"5.2.1 - ASSET AGE PROFILE"]
[null,null,null,"ECONOMIC LIFE (YEARS)",null,"INSTALLED ASSETS -˃ QUANTITY CURRENTLY IN COMMISSION BY YEAR"]
[null,"ASSET GROUP","ASSET CATEGORY","MEAN ","STANDARD DEVIATION ",{"$f":"CRY","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(F10,4)-1)&\"-\"&MID(F10,3,2)),VALUE(LEFT(F10,4)-1))","v":"2016-17"},"2015-16","2014-15","2013-14","2012-13","2011-12","2010-11","2009-10","2008-09","2007-08","2006-07","2005-06","2004-05","2003-04","2002-03","2001-02","2000-01","1999-00","1998-99","1997-98","1996-97","1995-96","1994-95","1993-94","1992-93","1991-92","1990-91","1989-90","1988-89","1987-88","1986-87","1985-86",{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(AL10,4)-1)&\"-\"&MID(AL10,3,2)),VALUE(LEFT(AL10,4)-1))","v":"1984-85"},"1983-84","1982-83","1981-82","1980-81","1979-80","1978-79","1977-78","1976-77","1975-76","1974-75","1973-74","1972-73","1971-72","1970-71","1969-70","1968-69","1967-68","1966-67","1965-66","1964-65","1963-64","1962-63","1961-62","1960-61","1959-60","1958-59","1957-58","1956-57","1955-56","1954-55","1953-54",{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(BR10,4)-1)&\"-\"&MID(BR10,3,2)),VALUE(LEFT(BR10,4)-1))","v":"1952-53"},"1951-52","1950-51","1949-50","1948-49","1947-48","1946-47","1945-46","1944-45","1943-44","1942-43","1941-42","1940-41","1939-40","1938-39","1937-38","1936-37","1935-36","1934-35","1933-34","1932-33","1931-32","1930-31","1929-30","1928-29","1927-28","1926-27","1925-26","1924-25","1923-24","1922-23","1921-22",{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(CX10,4)-1)&\"-\"&MID(CX10,3,2)),VALUE(LEFT(CX10,4)-1))","v":"1920-21"},"1919-20","1918-19","1917-18","1916-17","1915-16","1914-15","1913-14","1912-13","1911-12","1910-11","1909-10","1908-09","1907-08","1906-07","1905-06","1904-05","1903-04","1902-03","1901-02","1900-01"]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood - Staked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood - Unstaked",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",60,7.7,1,"-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",68,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Concrete",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",60,7.7,91,100,189,111,293,59,134,392,252,491,156,233,449,78,70,75,56,53,87,129,26,80,66,91,60,54,64,6,95,100,63,174,76,"3,670",34,172,247,41,"1,224",75,158,88,177,583,446,91,328,175,122,227,156,175,"-",161,"-",18,86,4,202,"-","-","-",1,66,"-","-","-","-",22,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",60,7.7,29,71,152,40,44,76,35,146,112,24,28,37,16,21,88,10,34,8,62,87,30,27,2,11,10,3,"-","-",3,410,124,114,6,"1,084","-",8,715,19,617,3,"-","-",10,348,149,54,60,"-",156,223,67,226,"-",114,"-","-",3,"-",11,"-","-","-","-",40,"-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",60,7.7,280,127,154,246,690,161,120,184,213,273,716,792,"1,007",126,271,254,167,291,295,257,216,265,266,136,154,39,189,313,301,178,212,454,103,"5,307",194,512,78,103,"3,360",40,175,124,83,816,182,253,392,187,229,257,23,89,"-",81,"-",375,140,64,163,"-","-","-","-","-","-","-","-","-",44,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",45,6.7,1,14,8,9,2,6,144,295,3,"-",12,"-","-","-",66,"-","-","-","-",57,72,1,1,4,1,"-","-","-","-",22,"-","-","-","1,259","-","-",61,"-",22,"-","-","-","-",76,"-","-",106,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",45,6.7,6,2,"-","-","-",3,22,"-","-","-",17,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",55,146,449,"-","-","-","-",32,"-","-","-","-",164,"-","-",24,"-","-","-","-","-","-",44,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHIGHEST OPERATING VOLTAGE; NUMBER OF PHASES (AT HV)","˂ = 1 kV",60,7.7,11.2,5.0999999999999996,5.5,8.4,12.5,8.3000000000000007,8.1999999999999993,16.399999999999999,11.6,6.4,20.6,28.5,34.799999999999997,7.3,7.2,10.5,11.4,11.2,36.6,18.8,15.1,23.1,5.6,5.3,4.9000000000000004,1.3,2.2000000000000002,1.2,11.4,13.1,1.3,12.9,3.3,322.60000000000002,26.7,21.4,27.8,4.2,147.5,2.6,5.8,3.4,13.2,51.3,20.9,6,24,5,5.3,14.9,5.3,8.6,0,49.7,0,0.3,29.1,0,7.8,0.1,0,0,0,0.2,0,0,0,0,2.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",60,7.7,4.2,2.2999999999999998,20.9,1.6,2,3.5,1.4,7.6,6.7,1.1000000000000001,1.6,1.9,0.8,1.8,4.2,0.3,2.2999999999999998,1.7,4.5999999999999996,5.5,2.2999999999999998,1.7,0.4,1.6,0.7,0,0,0,0.2,0.9,9.1999999999999993,7.7,0.2,70.900000000000006,0,0,71.8,1.3,31.2,0.6,0,1,0.7,19.600000000000001,6,2.1,5.0999999999999996,8.6,4.0999999999999996,11.1,0,8.3000000000000007,0,2.4,0,0,25.8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER",60,7.7,0,0,0,0,0,0,0,0,0,0,0,0.3,0,0,0,0,0,0,0,0,0,0,8.3000000000000007,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase",60,7.7,31.5,10,11.8,124.3,13.1,42,8.5,14.6,18.399999999999999,42.9,116,111.2,124.7,19.100000000000001,35.299999999999997,38.700000000000003,22.5,61.3,28,87.6,34,27.8,40,7.2,9.3000000000000007,2.7,25.4,66.7,29.5,23.2,18.5,50.8,21.6,765.4,54.2,149.80000000000001,3.7,7.1,421.1,2.7,12.9,13.3,14,91,23.9,17.399999999999999,30.7,11.1,43.3,33.799999999999997,3.4,15.2,0,32.5,0,41.4,16.399999999999999,0,7.6,0,0,0,0,0,0,0,0,0,2.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV",45,6.7,0.1,1,0,0.3,0.1,0,28.1,39.4,0,0,1.9,0,0,0,5.6,0.1,0,0,0,0,6.1,13.3,0,0,66.099999999999994,0,0,0.1,10,0.1,0,0,39.4,86.6,0,0,24,0,20.100000000000001,0,5.8,0,0,4.0999999999999996,0,0,0.2,2.5,0,0,0,19,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",45,6.7,4.2,0,0,0,0,0,0,0,0,0,4.2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0.1,0,340.1,2.2999999999999998,0,0,0,0,0,0,0,0,0,2.8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",55,7.4,7.2,17.100000000000001,23.7,28.2,17.100000000000001,19,4.0999999999999996,21.3,50.5,6.9,13.4,25.4,15.8,21.5,7.9,5.4,5,8.6,11.6,23,21.4,32.700000000000003,7.6,4.5999999999999996,1.8,10.3,1.1000000000000001,0.3,1.5,12.8,0.6,4.5,9.5,87.7,2.2000000000000002,66.5,90.8,5.8,7.7,0,0,1,0.2,12.9,1.1000000000000001,0,0.4,0,0.2,0,0,0,0,0,0,0.1,6.9,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV",55,7.4,7.5,18.8,25.6,19.399999999999999,19.399999999999999,20,19.8,35.799999999999997,32.1,16.8,17.600000000000001,13.7,11.6,11.6,5.5,11.1,6.4,11.1,8.1999999999999993,9.8000000000000007,18.2,26.8,11.9,0.7,4,5,0,0.5,1.4,33.6,1,1.2,4.5999999999999996,46.9,1.4,32.799999999999997,203.7,2.8,22.5,0,0,0.1,0.2,16.600000000000001,0.7,0.2,0.1,2,0.1,0,0,0,0,0,0,0,6.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV",55,7.4,4.7,8.1999999999999993,8.6999999999999993,3.9,1.1000000000000001,14.3,4.3,1.2,0.9,0.5,3,0.9,0.2,0,1.6,0.1,0.4,4.5,5.2,2.2000000000000002,3.6,0.1,0.1,0,0.1,0.1,0.1,0.1,3.1,0.6,6,0.8,0.3,2.1,0.7,0,0.6,0,2.9,0,0.3,1.1000000000000001,0,1.3,2.5,0,0.4,0.2,0.4,0,0,0,0,0.3,0,0,0,0,0.2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV",60,7.7,1.6,0.1,0.5,1.5,0,5,0.9,14.1,0,0,0.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.6,7.2,0,0,0,0,0,1.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,">  132 kV",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nCONNECTION VOLTAGE; CUSTOMER TYPE; CONNECTION COMPLEXITY ","˂ = 11 kV ; Residential ; Simple Type",35,5.9,318,426,658,561,647,422,310,869,"1,739",628,446,936,746,969,281,261,290,433,555,658,766,"1,366",287,306,104,336,46,1,184,764,216,392,511,"8,993",232,"3,155","8,859",343,"1,227",42,180,122,289,"1,466",897,159,513,267,84,364,108,189,"-",515,1,4,718,"-",298,"-","-","-","-","-","-","-","-","-",5,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type",35,5.9,151,163,524,624,696,302,189,434,145,270,152,154,217,66,104,84,78,182,152,179,70,82,43,43,40,49,8,6,224,206,8,61,67,942,38,93,176,24,974,"-",59,28,20,259,49,63,178,44,82,62,6,28,"-",20,1,10,204,"-",40,"-","-","-","-",18,"-","-","-","-",30,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Residential ; Complex Type",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMOUNTING TYPE; HIGHEST OPERATING VOLTAGE ; AMPERE RATING; NUMBER OF PHASES (AT LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",45,6.7,2,"-","-",1,1,2,"-",3,4,2,12,5,7,12,2,3,10,1,"-","-",7,4,14,2,4,2,1,"-",1,8,"-","-",6,"-",3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",45,6.7,"-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",45,6.7,7,14,14,13,14,24,23,11,26,31,73,48,25,10,13,5,3,11,8,16,38,18,27,18,17,10,14,"-",4,8,16,"-",40,6,4,"-",5,5,"-","-",3,1,"-",7,9,3,1,1,9,1,2,"-","-",2,2,4,"-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",45,6.7,58,61,109,65,40,108,65,77,127,114,84,96,94,105,66,44,38,57,24,50,75,46,54,24,39,14,26,1,24,46,7,10,39,5,9,5,21,9,10,"-","-",10,2,10,19,3,15,8,10,2,2,1,2,5,"-",5,2,"-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",45,6.7,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",45,6.7,"-","-","-","-","-","-","-","-","-",2,"-",3,"-","-","-","-","-","-","-",4,"-","-",1,"-","-","-","-","-","-",3,"-","-","-","-",7,36,56,94,92,4,"-",1,"-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",45,6.7,"-","-",1,"-",1,"-","-",3,4,3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",45,6.7,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",45,6.7,5,25,24,22,32,41,42,37,58,46,49,28,32,37,39,6,17,11,6,23,67,24,16,30,17,13,2,1,11,14,8,12,26,50,22,21,23,26,8,"-",5,18,42,10,"-","-",1,1,1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",45,6.7,9,9,6,17,11,18,16,14,11,5,11,8,13,4,7,11,2,3,4,3,3,2,7,1,"-","-","-","-",9,"-",1,"-",3,2,"-",1,3,"-",1,"-","-",2,"-","-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",45,6.7,1,6,1,1,1,1,"-",2,3,4,2,2,2,"-",1,1,1,"-","-","-",1,2,2,"-","-","-","-",4,"-","-","-","-","-","-",1,"-",5,2,2,"-","-",2,"-",1,11,2,2,1,6,3,"-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",45,6.7,7,5,18,8,8,4,5,15,1,6,8,8,8,2,6,2,5,5,1,3,6,6,10,"-","-","-","-","-",1,13,"-","-",6,9,1,12,5,3,6,"-","-",1,1,3,"-","-","-",1,"-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",45,6.7,"-",5,2,3,"-",1,1,"-","-",1,1,2,2,1,"-","-",2,"-","-",2,9,2,3,6,"-",1,"-","-",2,"-","-","-",2,6,2,"-",1,"-","-","-","-",1,"-",1,"-",1,2,"-",3,2,"-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",45,6.7,"-","-","-",2,"-",1,"-",2,2,1,"-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-",3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",2,"-","-","-",2,"-",2,"-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",45,6.7,2,2,"-","-","-",5,1,"-",4,2,"-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",2,"-","-","-","-","-","-","-","-",2,"-","-","-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",0,0,"-","-","-","-","-","-","-","-","-","-",4,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",45,6.7,"-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",45,6.7,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,"-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-",3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"SWITCHGEAR BY: \nHIGHEST OPERATING VOLTAGE ; SWITCH FUNCTION","˂ = 11 kV ;  Fuse",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV  ; Switch",35,5.9,63,126,181,128,120,153,81,87,187,90,71,46,26,44,33,29,33,29,41,47,36,23,23,13,4,6,"-","-",24,3,21,10,10,92,3,31,445,3,195,"-",3,21,3,102,45,10,45,10,24,48,"-",38,3,34,"-","-",38,"-","-","-","-","-","-",3,"-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ;  Circuit Breaker",45,6.7,3,18,"-","-",1,26,29,22,45,30,"-",29,11,7,"-","-","-","-",2,"-",1,4,"-",1,"-","-","-","-","-","-","-",10,4,3,7,26,2,"-","-","-","-","-","-",2,"-","-","-",11,"-","-","-","-",9,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Switch",35,5.9,32,73,68,54,45,59,61,70,86,101,185,137,114,60,44,52,55,73,61,161,33,37,32,8,19,"-",7,7,78,58,20,33,13,184,22,7,16,16,653,11,7,33,24,128,20,18,31,22,71,2,16,4,"-",31,"-",33,2,"-",14,"-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",45,6.7,16,36,12,8,5,12,4,5,24,11,14,11,3,"-",2,"-",1,4,1,1,"-",2,"-","-","-","-","-",1,12,1,1,"-",5,7,3,"-","-","-",3,"-","-","-",1,5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Switch",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Switch",45,6.7,24,1,"-",2,"-","-",5,4,"-",11,1,"-","-","-",3,4,1,"-","-","-",1,"-","-",2,"-","-","-",9,"-",5,"-","-",28,2,"-","-",2,"-",11,2,"-","-","-",4,"-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",45,6.7,9,6,"-",16,12,"-","-",2,3,17,1,6,"-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-",1,"-","-",5,"-","-",5,"-","-",2,"-",1,"-",1,"-","-",3,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Switch",45,6.7,"-",4,"-","-","-","-","-","-",13,"-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",7,"-",100,5,"-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",45,6.7,"-","-","-",2,"-","-","-",2,3,"-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",2,4,"-",9,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Switch",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nASSET TYPE ; LIGHTING OBLIGATION","Luminaires ;  Major Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Luminaires ;  Minor Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Brackets ; Major Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Brackets ; Minor Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Lamps ; Major Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Lamps ; Minor Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Major Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Poles / Columns ; Minor Road",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFUNCTION","Field Devices",15,3.9,47,57,254,76,27,136,188,49,9,51,41,5,9,8,7,6,"-",24,14,1,"-",5,5,66,5,17,"-",14,12,65,23,89,47,6,8,46,"-","-","-","-","-","-","-","-","-","-","-","-","-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Local Network Wiring Assets",45,6.7,"-",17,15,116,1,14,111,19,50,13,11,5,"-","-","-",3,"-","-","-","-","-","-","-","-","-","-",17,2,"-",14,32,"-",37,41,26,10,72,"-","-","-","-","-","-","-","-","-","-","-","-","-",2,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",15,3.9,4,15,28,61,23,16,46,82,63,36,45,"-",15,"-","-",5,"-",1,"-","-","-","-",8,"-","-",11,"-",18,"-","-",31,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Master Station Assets",15,3.9,"-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",15,3.9,"-",33,12,3,17,7,15,33,11,34,20,3,5,"-","-","-",2,6,"-","-","-","-",2,"-","-","-","-",9,"-",18,2,"-",21,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",15,3.9,11291,"8,508","39,765","11,810","16,292","17,414",856,"22,933","43,775","4,993","2,584","2,650","5,225",730,325,"34,882","5,883","29,285","-","-","-","-","21,105","4,213","-","-","-","5,598","-","-","-","28,617","-","15,241","28,079","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"AFLC",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"OTHER BY: \nDNSP DEFINED","Buildings",60,7.7,1,2,"-",1,1,"-",2,"-",1,"-",1,"-","-","-","-",1,"-","-","-","-","-","-","-",1,"-","-","-",2,1,"-",2,1,2,2,1,1,1,"-",1,"-",1,3,"-",5,"-","-",1,"-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Instrument Transformers",45,6.7,"-",53,1,19,12,4,13,1,5,25,"-","-","-","-","-",9,3,"-","-","-","(1)","-","-","-","-",1,"-",3,3,8,3,"-",77,11,4,"-",11,"-",13,"-","-",1,8,7,"-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Metering Units",25,5,"-",7,6,7,3,7,2,2,"-","-","-",1,"-",2,2,2,"-","-",1,"-",3,"-","-",2,"-","-","-","-",2,"-",1,"-","-",6,"-","-","-","-",2,"-","-","-","-",17,"-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Pillars",35,5.9,76,196,291,413,282,325,19,64,535,161,243,363,138,283,180,107,109,110,185,258,219,318,90,50,16,111,13,3,15,92,4,60,119,457,44,411,759,79,65,"-","-",6,6,128,8,4,"-","-","-","-","-","-","-","-","-","-",4,"-",4,"-","-","-","-",8,"-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Substation Auxiliary Plant",15,3.9,2,4,10,4,2,1,8,4,"-",6,2,8,8,5,7,3,6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Voltage Regulators",35,5.9,"-","-","-",2,"-",5,1,"-","-",1,"-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-",1,"-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Civil and Grounds",60,7.7,1,2,"-",1,1,"-",2,"-",1,"-",1,"-","-","-","-",1,"-","-","-","-","-","-","-",1,"-","-","-",2,1,"-",2,1,2,2,1,1,1,"-",1,"-",1,3,"-",5,"-","-",1,"-","-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Fire Systems",15,3.9,2,1,3,1,1,1,10,4,"-","-","-",2,"-","-","-","-","-",4,"-",4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Capacitor Banks",45,6.7,"-",2,8,1,3,2,2,"-",2,"-","-","-","-","-","-","-","-","-",1,"-","-","-","-","-",1,"-","-","-","-","-","-","-","-",1,"-",1,"-","-","-","-","-","-",1,9,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Power Transformer Refurbishment",60,7.7,"-",2,"-",3,2,"-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,"Tower Refurbishment",45,6.7,4,"-","-","-","-","-","-",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"5.4 MD & utilisation-Spatial","index":20,"n_rows":11432,"n_cols":6,"rows_kept":11432,"cut":false,"hidden":false,"merged":[[11410,1,11431,1],[11410,2,11411,2],[11410,3,11411,3],[11412,2,11413,2],[11412,3,11413,3],[11414,2,11415,2],[11414,3,11415,3],[11416,2,11417,2],[11416,3,11417,3],[11418,2,11419,2],[11418,3,11419,3],[11420,2,11421,2],[11420,3,11421,3],[11422,2,11423,2],[11422,3,11423,3],[11424,2,11425,2],[11424,3,11425,3],[11426,2,11427,2],[11426,3,11427,3],[11428,2,11429,2],[11428,3,11429,3],[11430,2,11431,2],[11430,3,11431,3],[44,3,45,3],[46,2,47,2],[46,3,47,3],[48,2,49,2],[48,3,49,3],[50,2,51,2],[50,3,51,3],[52,2,53,2],[52,3,53,3],[68,2,69,2],[108,2,109,2],[108,3,109,3],[110,2,111,2],[110,3,111,3],[114,2,115,2],[114,3,115,3],[116,2,117,2],[116,3,117,3],[118,2,119,2],[118,3,119,3],[134,2,135,2],[134,3,135,3],[120,1,141,1],[120,2,121,2],[120,3,121,3],[122,2,123,2],[122,3,123,3],[124,2,125,2],[124,3,125,3],[126,2,127,2],[126,3,127,3],[128,2,129,2],[128,3,129,3],[130,2,131,2],[130,3,131,3],[132,2,133,2],[132,3,133,3],[136,2,137,2],[136,3,137,3],[138,2,139,2],[138,3,139,3],[24,2,25,2],[24,3,25,3],[10,1,31,1],[10,2,11,2],[10,3,11,3],[12,2,13,2],[12,3,13,3],[14,2,15,2],[14,3,15,3],[16,2,17,2],[16,3,17,3],[18,2,19,2],[18,3,19,3],[20,2,21,2],[20,3,21,3],[22,2,23,2],[22,3,23,3],[26,2,27,2],[26,3,27,3],[28,2,29,2],[28,3,29,3],[30,2,31,2],[30,3,31,3],[90,2,91,2],[90,3,91,3],[76,1,97,1],[76,2,77,2],[76,3,77,3],[78,2,79,2],[78,3,79,3],[80,2,81,2],[80,3,81,3],[82,2,83,2],[82,3,83,3],[84,2,85,2],[84,3,85,3],[86,2,87,2],[86,3,87,3],[88,2,89,2],[88,3,89,3],[92,2,93,2],[92,3,93,3],[94,2,95,2],[94,3,95,3],[96,2,97,2],[96,3,97,3],[32,1,53,1],[32,2,33,2],[32,3,33,3],[34,2,35,2],[34,3,35,3],[42,2,43,2],[42,3,43,3],[44,2,45,2],[36,2,37,2],[36,3,37,3],[38,2,39,2],[38,3,39,3],[40,2,41,2],[40,3,41,3],[140,2,141,2],[140,3,141,3],[68,3,69,3],[54,1,75,1],[54,2,55,2],[54,3,55,3],[56,2,57,2],[56,3,57,3],[58,2,59,2],[58,3,59,3],[60,2,61,2],[60,3,61,3],[62,2,63,2],[62,3,63,3],[64,2,65,2],[64,3,65,3],[66,2,67,2],[66,3,67,3],[70,2,71,2],[70,3,71,3],[72,2,73,2],[72,3,73,3],[74,2,75,2],[74,3,75,3],[112,2,113,2],[112,3,113,3],[98,1,119,1],[98,2,99,2],[98,3,99,3],[100,2,101,2],[100,3,101,3],[102,2,103,2],[102,3,103,3],[104,2,105,2],[104,3,105,3],[106,2,107,2],[106,3,107,3],[156,2,157,2],[156,3,157,3],[142,1,163,1],[142,2,143,2],[142,3,143,3],[144,2,145,2],[144,3,145,3],[146,2,147,2],[146,3,147,3],[148,2,149,2],[148,3,149,3],[150,2,151,2],[150,3,151,3],[152,2,153,2],[152,3,153,3],[154,2,155,2],[154,3,155,3],[158,2,159,2],[158,3,159,3],[160,2,161,2],[160,3,161,3],[162,2,163,2],[162,3,163,3],[178,2,179,2],[178,3,179,3],[164,1,185,1],[164,2,165,2],[164,3,165,3],[166,2,167,2],[166,3,167,3],[168,2,169,2],[168,3,169,3],[170,2,171,2],[170,3,171,3],[172,2,173,2],[172,3,173,3],[174,2,175,2],[174,3,175,3],[176,2,177,2],[176,3,177,3],[180,2,181,2],[180,3,181,3],[182,2,183,2],[182,3,183,3],[184,2,185,2],[184,3,185,3],[200,2,201,2],[200,3,201,3],[186,1,207,1],[186,2,187,2],[186,3,187,3],[188,2,189,2],[188,3,189,3],[190,2,191,2],[190,3,191,3],[192,2,193,2],[192,3,193,3],[194,2,195,2],[194,3,195,3],[196,2,197,2],[196,3,197,3],[198,2,199,2],[198,3,199,3],[202,2,203,2],[202,3,203,3],[204,2,205,2],[204,3,205,3],[206,2,207,2],[206,3,207,3],[222,2,223,2],[222,3,223,3],[208,1,229,1],[208,2,209,2],[208,3,209,3],[210,2,211,2],[210,3,211,3],[212,2,213,2],[212,3,213,3],[214,2,215,2],[214,3,215,3],[216,2,217,2],[216,3,217,3],[218,2,219,2],[218,3,219,3],[220,2,221,2],[220,3,221,3],[224,2,225,2],[224,3,225,3],[226,2,227,2],[226,3,227,3],[228,2,229,2],[228,3,229,3],[244,2,245,2],[244,3,245,3],[230,1,251,1],[230,2,231,2],[230,3,231,3],[232,2,233,2],[232,3,233,3],[234,2,235,2],[234,3,235,3],[236,2,237,2],[236,3,237,3],[238,2,239,2],[238,3,239,3],[240,2,241,2],[240,3,241,3],[242,2,243,2],[242,3,243,3],[246,2,247,2],[246,3,247,3],[248,2,249,2],[248,3,249,3],[250,2,251,2],[250,3,251,3],[266,2,267,2],[266,3,267,3],[252,1,273,1],[252,2,253,2],[252,3,253,3],[254,2,255,2],[254,3,255,3],[256,2,257,2],[256,3,257,3],[258,2,259,2],[258,3,259,3],[260,2,261,2],[260,3,261,3],[262,2,263,2],[262,3,263,3],[264,2,265,2],[264,3,265,3],[268,2,269,2],[268,3,269,3],[270,2,271,2],[270,3,271,3],[272,2,273,2],[272,3,273,3],[288,2,289,2],[288,3,289,3],[274,1,295,1],[274,2,275,2],[274,3,275,3],[276,2,277,2],[276,3,277,3],[278,2,279,2],[278,3,279,3],[280,2,281,2],[280,3,281,3],[282,2,283,2],[282,3,283,3],[284,2,285,2],[284,3,285,3],[286,2,287,2],[286,3,287,3],[290,2,291,2],[290,3,291,3],[292,2,293,2],[292,3,293,3],[294,2,295,2],[294,3,295,3],[310,2,311,2],[310,3,311,3],[296,1,317,1],[296,2,297,2],[296,3,297,3],[298,2,299,2],[298,3,299,3],[300,2,301,2],[300,3,301,3],[302,2,303,2],[302,3,303,3],[304,2,305,2],[304,3,305,3],[306,2,307,2],[306,3,307,3],[308,2,309,2],[308,3,309,3],[312,2,313,2],[312,3,313,3],[314,2,315,2],[314,3,315,3],[316,2,317,2],[316,3,317,3],[332,2,333,2],[332,3,333,3],[318,1,339,1],[318,2,319,2],[318,3,319,3],[320,2,321,2],[320,3,321,3],[322,2,323,2],[322,3,323,3],[324,2,325,2],[324,3,325,3],[326,2,327,2],[326,3,327,3],[328,2,329,2],[328,3,329,3],[330,2,331,2],[330,3,331,3],[334,2,335,2],[334,3,335,3],[336,2,337,2],[336,3,337,3],[338,2,339,2],[338,3,339,3],[354,2,355,2],[354,3,355,3],[340,1,361,1],[340,2,341,2],[340,3,341,3],[342,2,343,2],[342,3,343,3],[344,2,345,2],[344,3,345,3],[346,2,347,2],[346,3,347,3],[348,2,349,2],[348,3,349,3],[350,2,351,2],[350,3,351,3],[352,2,353,2],[352,3,353,3],[356,2,357,2],[356,3,357,3],[358,2,359,2],[358,3,359,3],[360,2,361,2],[360,3,361,3],[376,2,377,2],[376,3,377,3],[362,1,383,1],[362,2,363,2],[362,3,363,3],[364,2,365,2],[364,3,365,3],[366,2,367,2],[366,3,367,3],[368,2,369,2],[368,3,369,3],[370,2,371,2],[370,3,371,3],[372,2,373,2],[372,3,373,3],[374,2,375,2],[374,3,375,3],[378,2,379,2],[378,3,379,3],[380,2,381,2],[380,3,381,3],[382,2,383,2],[382,3,383,3],[398,2,399,2],[398,3,399,3],[384,1,405,1],[384,2,385,2],[384,3,385,3],[386,2,387,2],[386,3,387,3],[388,2,389,2],[388,3,389,3],[390,2,391,2],[390,3,391,3],[392,2,393,2],[392,3,393,3],[394,2,395,2],[394,3,395,3],[396,2,397,2],[396,3,397,3],[400,2,401,2],[400,3,401,3],[402,2,403,2],[402,3,403,3],[404,2,405,2],[404,3,405,3],[420,2,421,2],[420,3,421,3],[406,1,427,1],[406,2,407,2],[406,3,407,3],[408,2,409,2],[408,3,409,3],[410,2,411,2],[410,3,411,3],[412,2,413,2],[412,3,413,3],[414,2,415,2],[414,3,415,3],[416,2,417,2],[416,3,417,3],[418,2,419,2],[418,3,419,3],[422,2,423,2],[422,3,423,3],[424,2,425,2],[424,3,425,3],[426,2,427,2],[426,3,427,3],[442,2,443,2],[442,3,443,3],[428,1,449,1],[428,2,429,2],[428,3,429,3],[430,2,431,2],[430,3,431,3],[432,2,433,2],[432,3,433,3],[434,2,435,2],[434,3,435,3],[436,2,437,2],[436,3,437,3],[438,2,439,2],[438,3,439,3],[440,2,441,2],[440,3,441,3],[444,2,445,2],[444,3,445,3],[446,2,447,2],[446,3,447,3],[448,2,449,2],[448,3,449,3],[464,2,465,2],[464,3,465,3],[450,1,471,1],[450,2,451,2],[450,3,451,3],[452,2,453,2],[452,3,453,3],[454,2,455,2],[454,3,455,3],[456,2,457,2],[456,3,457,3],[458,2,459,2],[458,3,459,3],[460,2,461,2],[460,3,461,3],[462,2,463,2],[462,3,463,3],[466,2,467,2],[466,3,467,3],[468,2,469,2],[468,3,469,3],[470,2,471,2],[470,3,471,3],[486,2,487,2],[486,3,487,3],[472,1,493,1],[472,2,473,2],[472,3,473,3],[474,2,475,2],[474,3,475,3],[476,2,477,2],[476,3,477,3],[478,2,479,2],[478,3,479,3],[480,2,481,2],[480,3,481,3],[482,2,483,2],[482,3,483,3],[484,2,485,2],[484,3,485,3],[488,2,489,2],[488,3,489,3],[490,2,491,2],[490,3,491,3],[492,2,493,2],[492,3,493,3],[508,2,509,2],[508,3,509,3],[494,1,515,1],[494,2,495,2],[494,3,495,3],[496,2,497,2],[496,3,497,3],[498,2,499,2],[498,3,499,3],[500,2,501,2],[500,3,501,3],[502,2,503,2],[502,3,503,3],[504,2,505,2],[504,3,505,3],[506,2,507,2],[506,3,507,3],[510,2,511,2],[510,3,511,3],[512,2,513,2],[512,3,513,3],[514,2,515,2],[514,3,515,3],[530,2,531,2],[530,3,531,3],[516,1,537,1],[516,2,517,2],[516,3,517,3],[518,2,519,2],[518,3,519,3],[520,2,521,2],[520,3,521,3],[522,2,523,2],[522,3,523,3],[524,2,525,2],[524,3,525,3],[526,2,527,2],[526,3,527,3],[528,2,529,2],[528,3,529,3],[532,2,533,2],[532,3,533,3],[534,2,535,2],[534,3,535,3],[536,2,537,2],[536,3,537,3],[552,2,553,2],[552,3,553,3],[538,1,559,1],[538,2,539,2],[538,3,539,3],[540,2,541,2],[540,3,541,3],[542,2,543,2],[542,3,543,3],[544,2,545,2],[544,3,545,3],[546,2,547,2],[546,3,547,3],[548,2,549,2],[548,3,549,3],[550,2,551,2],[550,3,551,3],[554,2,555,2],[554,3,555,3],[556,2,557,2],[556,3,557,3],[558,2,559,2],[558,3,559,3],[574,2,575,2],[574,3,575,3],[560,1,581,1],[560,2,561,2],[560,3,561,3],[562,2,563,2],[562,3,563,3],[564,2,565,2],[564,3,565,3],[566,2,567,2],[566,3,567,3],[568,2,569,2],[568,3,569,3],[570,2,571,2],[570,3,571,3],[572,2,573,2],[572,3,573,3],[576,2,577,2],[576,3,577,3],[578,2,579,2],[578,3,579,3],[580,2,581,2],[580,3,581,3],[596,2,597,2],[596,3,597,3],[582,1,603,1],[582,2,583,2],[582,3,583,3],[584,2,585,2],[584,3,585,3],[586,2,587,2],[586,3,587,3],[588,2,589,2],[588,3,589,3],[590,2,591,2],[590,3,591,3],[592,2,593,2],[592,3,593,3],[594,2,595,2],[594,3,595,3],[598,2,599,2],[598,3,599,3],[600,2,601,2],[600,3,601,3],[602,2,603,2],[602,3,603,3],[618,2,619,2],[618,3,619,3],[604,1,625,1],[604,2,605,2],[604,3,605,3],[606,2,607,2],[606,3,607,3],[608,2,609,2],[608,3,609,3],[610,2,611,2],[610,3,611,3],[612,2,613,2],[612,3,613,3],[614,2,615,2],[614,3,615,3],[616,2,617,2],[616,3,617,3],[620,2,621,2],[620,3,621,3],[622,2,623,2],[622,3,623,3],[624,2,625,2],[624,3,625,3],[640,2,641,2],[640,3,641,3],[626,1,647,1],[626,2,627,2],[626,3,627,3],[628,2,629,2],[628,3,629,3],[630,2,631,2],[630,3,631,3],[632,2,633,2],[632,3,633,3],[634,2,635,2],[634,3,635,3],[636,2,637,2],[636,3,637,3],[638,2,639,2],[638,3,639,3],[642,2,643,2],[642,3,643,3],[644,2,645,2],[644,3,645,3],[646,2,647,2],[646,3,647,3],[662,2,663,2],[662,3,663,3],[648,1,669,1],[648,2,649,2],[648,3,649,3],[650,2,651,2],[650,3,651,3],[652,2,653,2],[652,3,653,3],[654,2,655,2],[654,3,655,3],[656,2,657,2],[656,3,657,3],[658,2,659,2],[658,3,659,3],[660,2,661,2],[660,3,661,3],[664,2,665,2],[664,3,665,3],[666,2,667,2],[666,3,667,3],[668,2,669,2],[668,3,669,3],[684,2,685,2],[684,3,685,3],[670,1,691,1],[670,2,671,2],[670,3,671,3],[672,2,673,2],[672,3,673,3],[674,2,675,2],[674,3,675,3],[676,2,677,2],[676,3,677,3],[678,2,679,2],[678,3,679,3],[680,2,681,2],[680,3,681,3],[682,2,683,2],[682,3,683,3],[686,2,687,2],[686,3,687,3],[688,2,689,2],[688,3,689,3],[690,2,691,2],[690,3,691,3],[706,2,707,2],[706,3,707,3],[692,1,713,1],[692,2,693,2],[692,3,693,3],[694,2,695,2],[694,3,695,3],[696,2,697,2],[696,3,697,3],[698,2,699,2],[698,3,699,3],[700,2,701,2],[700,3,701,3],[702,2,703,2],[702,3,703,3],[704,2,705,2],[704,3,705,3],[708,2,709,2],[708,3,709,3],[710,2,711,2],[710,3,711,3],[712,2,713,2],[712,3,713,3],[728,2,729,2],[728,3,729,3],[714,1,735,1],[714,2,715,2],[714,3,715,3],[716,2,717,2],[716,3,717,3],[718,2,719,2],[718,3,719,3],[720,2,721,2],[720,3,721,3],[722,2,723,2],[722,3,723,3],[724,2,725,2],[724,3,725,3],[726,2,727,2],[726,3,727,3],[730,2,731,2],[730,3,731,3],[732,2,733,2],[732,3,733,3],[734,2,735,2],[734,3,735,3],[750,2,751,2],[750,3,751,3],[736,1,757,1],[736,2,737,2],[736,3,737,3],[738,2,739,2],[738,3,739,3],[740,2,741,2],[740,3,741,3],[742,2,743,2],[742,3,743,3],[744,2,745,2],[744,3,745,3],[746,2,747,2],[746,3,747,3],[748,2,749,2],[748,3,749,3],[752,2,753,2],[752,3,753,3],[754,2,755,2],[754,3,755,3],[756,2,757,2],[756,3,757,3],[772,2,773,2],[772,3,773,3],[758,1,779,1],[758,2,759,2],[758,3,759,3],[760,2,761,2],[760,3,761,3],[762,2,763,2],[762,3,763,3],[764,2,765,2],[764,3,765,3],[766,2,767,2],[766,3,767,3],[768,2,769,2],[768,3,769,3],[770,2,771,2],[770,3,771,3],[774,2,775,2],[774,3,775,3],[776,2,777,2],[776,3,777,3],[778,2,779,2],[778,3,779,3],[794,2,795,2],[794,3,795,3],[780,1,801,1],[780,2,781,2],[780,3,781,3],[782,2,783,2],[782,3,783,3],[784,2,785,2],[784,3,785,3],[786,2,787,2],[786,3,787,3],[788,2,789,2],[788,3,789,3],[790,2,791,2],[790,3,791,3],[792,2,793,2],[792,3,793,3],[796,2,797,2],[796,3,797,3],[798,2,799,2],[798,3,799,3],[800,2,801,2],[800,3,801,3],[816,2,817,2],[816,3,817,3],[802,1,823,1],[802,2,803,2],[802,3,803,3],[804,2,805,2],[804,3,805,3],[806,2,807,2],[806,3,807,3],[808,2,809,2],[808,3,809,3],[810,2,811,2],[810,3,811,3],[812,2,813,2],[812,3,813,3],[814,2,815,2],[814,3,815,3],[818,2,819,2],[818,3,819,3],[820,2,821,2],[820,3,821,3],[822,2,823,2],[822,3,823,3],[838,2,839,2],[838,3,839,3],[824,1,845,1],[824,2,825,2],[824,3,825,3],[826,2,827,2],[826,3,827,3],[828,2,829,2],[828,3,829,3],[830,2,831,2],[830,3,831,3],[832,2,833,2],[832,3,833,3],[834,2,835,2],[834,3,835,3],[836,2,837,2],[836,3,837,3],[840,2,841,2],[840,3,841,3],[842,2,843,2],[842,3,843,3],[844,2,845,2],[844,3,845,3],[860,2,861,2],[860,3,861,3],[846,1,867,1],[846,2,847,2],[846,3,847,3],[848,2,849,2],[848,3,849,3],[850,2,851,2],[850,3,851,3],[852,2,853,2],[852,3,853,3],[854,2,855,2],[854,3,855,3],[856,2,857,2],[856,3,857,3],[858,2,859,2],[858,3,859,3],[862,2,863,2],[862,3,863,3],[864,2,865,2],[864,3,865,3],[866,2,867,2],[866,3,867,3],[882,2,883,2],[882,3,883,3],[868,1,889,1],[868,2,869,2],[868,3,869,3],[870,2,871,2],[870,3,871,3],[872,2,873,2],[872,3,873,3],[874,2,875,2],[874,3,875,3],[876,2,877,2],[876,3,877,3],[878,2,879,2],[878,3,879,3],[880,2,881,2],[880,3,881,3],[884,2,885,2],[884,3,885,3],[886,2,887,2],[886,3,887,3],[888,2,889,2],[888,3,889,3],[904,2,905,2],[904,3,905,3],[890,1,911,1],[890,2,891,2],[890,3,891,3],[892,2,893,2],[892,3,893,3],[894,2,895,2],[894,3,895,3],[896,2,897,2],[896,3,897,3],[898,2,899,2],[898,3,899,3],[900,2,901,2],[900,3,901,3],[902,2,903,2],[902,3,903,3],[906,2,907,2],[906,3,907,3],[908,2,909,2],[908,3,909,3],[910,2,911,2],[910,3,911,3],[926,2,927,2],[926,3,927,3],[912,1,933,1],[912,2,913,2],[912,3,913,3],[914,2,915,2],[914,3,915,3],[916,2,917,2],[916,3,917,3],[918,2,919,2],[918,3,919,3],[920,2,921,2],[920,3,921,3],[922,2,923,2],[922,3,923,3],[924,2,925,2],[924,3,925,3],[928,2,929,2],[928,3,929,3],[930,2,931,2],[930,3,931,3],[932,2,933,2],[932,3,933,3],[948,2,949,2],[948,3,949,3],[934,1,955,1],[934,2,935,2],[934,3,935,3],[936,2,937,2],[936,3,937,3],[938,2,939,2],[938,3,939,3],[940,2,941,2],[940,3,941,3]],"merged_total":11938,"flags":["merged_cut"]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There is ONE table on this worksheet - sub-divided by Network Level. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"5.4.1 NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRY","v":"2017-18"}]
[null,"Hudson Creek (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",394.5]
[null,null,null,null,"Coincident",394.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",209.01]
[null,null,null,null,"Coincident",203.65]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",210.57]
[null,null,null,null,"Coincident",205.17]
[null,null,"Date MD occurred",null,"Non-Coincident","06/12/2017"]
[null,null,null,null,"Coincident","17/10/2017"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:30"]
[null,null,null,null,"Coincident","16:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",229.82]
[null,null,null,null,"Coincident",218.64]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",231.54]
[null,null,null,null,"Coincident",220.27]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",224.66]
[null,null,null,null,"Coincident",213.42]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",226.34]
[null,null,null,null,"Coincident",215.02]
[null,"Pine Creek (132/66kV) - (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",30]
[null,null,null,null,"Coincident",30]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",23.98]
[null,null,null,null,"Coincident",19.97]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",24.3]
[null,null,null,null,"Coincident",20.23]
[null,null,"Date MD occurred",null,"Non-Coincident","26/08/2017"]
[null,null,null,null,"Coincident","17/10/2017"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","21:00"]
[null,null,null,null,"Coincident","16:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",27.7]
[null,null,null,null,"Coincident",21.43]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.07]
[null,null,null,null,"Coincident",21.72]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.12]
[null,null,null,null,"Coincident",20.92]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.48]
[null,null,null,null,"Coincident",21.2]
[null,"Pine Creek (66/11 kV) - (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",40]
[null,null,null,null,"Coincident",40]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",28.06]
[null,null,null,null,"Coincident",24.24]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",28.23]
[null,null,null,null,"Coincident",24.39]
[null,null,"Date MD occurred",null,"Non-Coincident","16/07/2017"]
[null,null,null,null,"Coincident","17/10/2017"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","8:30"]
[null,null,null,null,"Coincident","16:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",34.29]
[null,null,null,null,"Coincident",26.03]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.49]
[null,null,null,null,"Coincident",26.19]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",33.6]
[null,null,null,null,"Coincident",25.41]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",33.799999999999997]
[null,null,null,null,"Coincident",25.56]
[null,"Owen Springs (Alice Springs System)","Substation Rating","MVA","Non-Coincident",187.5]
[null,null,null,null,"Coincident",187.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",27.14]
[null,null,null,null,"Coincident",10]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",27.74]
[null,null,null,null,"Coincident",10.220000000000001]
[null,null,"Date MD occurred",null,"Non-Coincident","24/01/2018"]
[null,null,null,null,"Coincident","21/02/2018"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:00"]
[null,null,null,null,"Coincident","17:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",29.82]
[null,null,null,null,"Coincident",10.92]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.48]
[null,null,null,null,"Coincident",11.16]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.62]
[null,null,null,null,"Coincident",10.52]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.25]
[null,null,null,null,"Coincident",10.75]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[null,"ZONE SUBSTATION"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRY","v":"2017-18"}]
[null,"Archer (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",60.6]
[null,null,null,null,"Coincident",60.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",25.853000000000002]
[null,null,null,null,"Coincident",20.385000000000002]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",26.504999999999999]
[null,null,null,null,"Coincident",20.9]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-11"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","19:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",27.422000000000001]
[null,null,null,null,"Coincident",21.885999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.114000000000001]
[null,null,null,null,"Coincident",22.437999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.725000000000001]
[null,null,null,null,"Coincident",21.364000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",27.399000000000001]
[null,null,null,null,"Coincident",21.902999999999999]
[null,"Batchelor (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",33.6]
[null,null,null,null,"Coincident",33.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",1.9650000000000001]
[null,null,null,null,"Coincident",1.6279999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",1.9650000000000001]
[null,null,null,null,"Coincident",1.6279999999999999]
[null,null,"Date MD occurred",null,"Non-Coincident","10/10/2017"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",2.0529999999999999]
[null,null,null,null,"Coincident",1.748]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0529999999999999]
[null,null,null,null,"Coincident",1.748]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0019999999999998]
[null,null,null,null,"Coincident",1.706]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0019999999999998]
[null,null,null,null,"Coincident",1.706]
[null,"Berrimah (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",76.2]
[null,null,null,null,"Coincident",76.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",26.946999999999999]
[null,null,null,null,"Coincident",23.873999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",27.428000000000001]
[null,null,null,null,"Coincident",24.3]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-16"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","14:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",29.021999999999998]
[null,null,null,null,"Coincident",25.631]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.54]
[null,null,null,null,"Coincident",26.088000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.376999999999999]
[null,null,null,null,"Coincident",25.02]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.882999999999999]
[null,null,null,null,"Coincident",25.466000000000001]
[null,"Casuarina (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",81]
[null,null,null,null,"Coincident",81]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",41.933]
[null,null,null,null,"Coincident",38.673999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",43.088999999999999]
[null,null,null,null,"Coincident",39.74]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-08"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","17:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",45.02]
[null,null,null,null,"Coincident",41.521000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",46.26]
[null,null,null,null,"Coincident",42.664999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",43.945999999999998]
[null,null,null,null,"Coincident",40.530999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",45.156999999999996]
[null,null,null,null,"Coincident",41.648000000000003]
[null,"Centre Yard (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",1]
[null,null,null,null,"Coincident",1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",0.47399999999999998]
[null,null,null,null,"Coincident",0.28699999999999998]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",0.47899999999999998]
[null,null,null,null,"Coincident",0.28999999999999998]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-17"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","20:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",0.49399999999999999]
[null,null,null,null,"Coincident",0.308]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.499]
[null,null,null,null,"Coincident",0.311]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.48199999999999998]
[null,null,null,null,"Coincident",0.30099999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.48699999999999999]
[null,null,null,null,"Coincident",0.30399999999999999]
[null,null,"Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Darwin (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",114]
[null,null,null,null,"Coincident",114]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",28.169]
[null,null,null,null,"Coincident",25.693000000000001]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",28.439]
[null,null,null,null,"Coincident",25.94]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-08"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",30.251999999999999]
[null,null,null,null,"Coincident",27.584]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.542000000000002]
[null,null,null,null,"Coincident",27.849]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",29.527000000000001]
[null,null,null,null,"Coincident",26.927]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.811]
[null,null,null,null,"Coincident",27.184999999999999]
[null,"Frances Bay (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",88.6]
[null,null,null,null,"Coincident",88.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",23]
[null,null,null,null,"Coincident",20.739000000000001]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",23.501000000000001]
[null,null,null,null,"Coincident",21.19]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-03-07"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","15:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",25.065000000000001]
[null,null,null,null,"Coincident",22.265000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.61]
[null,null,null,null,"Coincident",22.75]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.48]
[null,null,null,null,"Coincident",21.734000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.012]
[null,null,null,null,"Coincident",22.207000000000001]
[null,"Humpty Doo (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",5.4]
[null,null,null,null,"Coincident",5.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",2.4180000000000001]
[null,null,null,null,"Coincident",1.7709999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",2.484]
[null,null,null,null,"Coincident",1.82]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-09-12"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",1.9910000000000001]
[null,null,null,null,"Coincident",1.9019999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0459999999999998]
[null,null,null,null,"Coincident",1.954]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9470000000000001]
[null,null,null,null,"Coincident",1.857]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0009999999999999]
[null,null,null,null,"Coincident",1.907]
[null,"Katherine (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",62.3]
[null,null,null,null,"Coincident",62.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",26.494]
[null,null,null,null,"Coincident",25.405000000000001]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",27.198]
[null,null,null,null,"Coincident",26.08]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-31"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",28.512]
[null,null,null,null,"Coincident",27.274999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.27]
[null,null,null,null,"Coincident",27.998999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.856000000000002]
[null,null,null,null,"Coincident",26.623999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.596]
[null,null,null,null,"Coincident",27.332000000000001]
[null,"Leanyer (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",54]
[null,null,null,null,"Coincident",54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",11.824999999999999]
[null,null,null,null,"Coincident",7.6420000000000003]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",12.534000000000001]
[null,null,null,null,"Coincident",8.1]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-11"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","19:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",13.207000000000001]
[null,null,null,null,"Coincident",8.2050000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.997999999999999]
[null,null,null,null,"Coincident",8.6959999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.906000000000001]
[null,null,null,null,"Coincident",8.0090000000000003]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.679]
[null,null,null,null,"Coincident",8.4890000000000008]
[null,"Manton (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",32.4]
[null,null,null,null,"Coincident",32.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",3.419]
[null,null,null,null,"Coincident",3.1429999999999998]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",3.5249999999999999]
[null,null,null,null,"Coincident",3.24]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-09-21"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","17:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",3.214]
[null,null,null,null,"Coincident",3.3740000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3130000000000002]
[null,null,null,null,"Coincident",3.4780000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1349999999999998]
[null,null,null,null,"Coincident",3.294]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2309999999999999]
[null,null,null,null,"Coincident",3.3959999999999999]
[null,"Marrakai (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",5]
[null,null,null,null,"Coincident",5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",0.85599999999999998]
[null,null,null,null,"Coincident",0.59799999999999998]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",0.90200000000000002]
[null,null,null,null,"Coincident",0.63]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-09-26"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","18:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",0.76400000000000001]
[null,null,null,null,"Coincident",0.64200000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.80600000000000005]
[null,null,null,null,"Coincident",0.67600000000000005]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.746]
[null,null,null,null,"Coincident",0.627]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.78600000000000003]
[null,null,null,null,"Coincident",0.66]
[null,"Mary River (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",7.5]
[null,null,null,null,"Coincident",7.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",2.4300000000000002]
[null,null,null,null,"Coincident",0.45600000000000002]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",2.823]
[null,null,null,null,"Coincident",0.53]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-09-08"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","12:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",2.512]
[null,null,null,null,"Coincident",0.49]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9180000000000001]
[null,null,null,null,"Coincident",0.56899999999999995]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.452]
[null,null,null,null,"Coincident",0.47799999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8479999999999999]
[null,null,null,null,"Coincident",0.55500000000000005]
[null,"Palmerston (66/11 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",76.2]
[null,null,null,null,"Coincident",76.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",29.963000000000001]
[null,null,null,null,"Coincident",27.196999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",30.946000000000002]
[null,null,null,null,"Coincident",28.09]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-06"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","15:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",32.445999999999998]
[null,null,null,null,"Coincident",29.199000000000002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",33.51]
[null,null,null,null,"Coincident",30.157]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",31.722000000000001]
[null,null,null,null,"Coincident",28.503]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.762999999999998]
[null,null,null,null,"Coincident",29.437999999999999]
[null,"Palmerston (11/22 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",19]
[null,null,null,null,"Coincident",19]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",6.1970000000000001]
[null,null,null,null,"Coincident",2.8359999999999999]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",6.2290000000000001]
[null,null,null,null,"Coincident",2.85]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-09-20"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","19:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",6.516]
[null,null,null,null,"Coincident",3.044]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5490000000000004]
[null,null,null,null,"Coincident",3.06]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4189999999999996]
[null,null,null,null,"Coincident",2.972]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.452]
[null,null,null,null,"Coincident",2.9870000000000001]
[null,"Pine Creek (11/22 kV) (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",1.8]
[null,null,null,null,"Coincident",1.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",0.92800000000000005]
[null,null,null,null,"Coincident",0.57499999999999996]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",0.95299999999999996]
[null,null,null,null,"Coincident",0.59]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-01-05"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","14:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",1.05]
[null,null,null,null,"Coincident",0.61699999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0780000000000001]
[null,null,null,null,"Coincident",0.63300000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0269999999999999]
[null,null,null,null,"Coincident",0.60199999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.054]
[null,null,null,null,"Coincident",0.61799999999999999]
[null,"Strangways (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",54]
[null,null,null,null,"Coincident",54]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",27.251999999999999]
[null,null,null,null,"Coincident",23]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",27.998000000000001]
[null,null,null,null,"Coincident",23.63]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-12"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","19:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",27.997]
[null,null,null,null,"Coincident",24.693000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.763999999999999]
[null,null,null,null,"Coincident",25.369]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.266999999999999]
[null,null,null,null,"Coincident",24.103999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",28.013999999999999]
[null,null,null,null,"Coincident",24.763999999999999]
[null,"Tindal (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",13.2]
[null,null,null,null,"Coincident",13.2]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",3.9510000000000001]
[null,null,null,null,"Coincident",3.2120000000000002]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",4.391]
[null,null,null,null,"Coincident",3.57]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-13"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","15:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",4.5640000000000001]
[null,null,null,null,"Coincident",3.448]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.0730000000000004]
[null,null,null,null,"Coincident",3.8330000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4640000000000004]
[null,null,null,null,"Coincident",3.3660000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.9619999999999997]
[null,null,null,null,"Coincident",3.7410000000000001]
[null,"Weddell (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",29.1]
[null,null,null,null,"Coincident",29.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",16.957999999999998]
[null,null,null,null,"Coincident",14.492000000000001]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",18.582999999999998]
[null,null,null,null,"Coincident",15.88]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-19"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","15:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",17.817]
[null,null,null,null,"Coincident",15.558999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.523]
[null,null,null,null,"Coincident",17.048999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.408000000000001]
[null,null,null,null,"Coincident",15.188000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.074999999999999]
[null,null,null,null,"Coincident",16.641999999999999]
[null,"Wishart Modular Substation (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",12]
[null,null,null,null,"Coincident",12]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",3.206]
[null,null,null,null,"Coincident",2.3849999999999998]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",3.427]
[null,null,null,null,"Coincident",2.5499999999999998]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-11-06"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","12:30:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",3.5169999999999999]
[null,null,null,null,"Coincident",2.5609999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.76]
[null,null,null,null,"Coincident",2.738]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.4409999999999998]
[null,null,null,null,"Coincident",2.5]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.6789999999999998]
[null,null,null,null,"Coincident",2.6720000000000002]
[null,"Woolner (Darwin Katherine System)","Substation Rating","MVA","Non-Coincident",87]
[null,null,null,null,"Coincident",87]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",32.816000000000003]
[null,null,null,null,"Coincident",32.552999999999997]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",33.146000000000001]
[null,null,null,null,"Coincident",32.880000000000003]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-12-07"]
[null,null,null,null,"Coincident","2017-10-17"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","15:00:00"]
[null,null,null,null,"Coincident","16:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",35.133000000000003]
[null,null,null,null,"Coincident",34.948999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",35.485999999999997]
[null,null,null,null,"Coincident",35.299999999999997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.290999999999997]
[null,null,null,null,"Coincident",34.116]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.634999999999998]
[null,null,null,null,"Coincident",34.457999999999998]
[null,"Lovegrove (22/11 kV) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",38.9]
[null,null,null,null,"Coincident",38.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",21.498999999999999]
[null,null,null,null,"Coincident",19.834]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",21.939]
[null,null,null,null,"Coincident",20.239999999999998]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-02-19"]
[null,null,null,null,"Coincident","2018-02-21"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","17:00:00"]
[null,null,null,null,"Coincident","17:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",25.087]
[null,null,null,null,"Coincident",21.661999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.6]
[null,null,null,null,"Coincident",22.106000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.19]
[null,null,null,null,"Coincident",20.863]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.684999999999999]
[null,null,null,null,"Coincident",21.29]
[null,"Lovegrove (66/22 kV) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",120]
[null,null,null,null,"Coincident",120]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",21.911000000000001]
[null,null,null,null,"Coincident",19.292000000000002]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",28.614999999999998]
[null,null,null,null,"Coincident",25.195]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-01-24"]
[null,null,null,null,"Coincident","2018-02-21"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:00:00"]
[null,null,null,null,"Coincident","17:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",24.495999999999999]
[null,null,null,null,"Coincident",21.07]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.991]
[null,null,null,null,"Coincident",27.516999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.673999999999999]
[null,null,null,null,"Coincident",20.292999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",30.917999999999999]
[null,null,null,null,"Coincident",26.501999999999999]
[null,"Lovegrove (22 kV loads) (Alice Springs System)","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",0.48499999999999999]
[null,null,null,null,"Coincident",0.127]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",0.495]
[null,null,null,null,"Coincident",0.13]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-02-05"]
[null,null,null,null,"Coincident","2018-02-21"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","12:30:00"]
[null,null,null,null,"Coincident","17:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",0.63300000000000001]
[null,null,null,null,"Coincident",0.13900000000000001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.64600000000000002]
[null,null,null,null,"Coincident",0.14199999999999999]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.61099999999999999]
[null,null,null,null,"Coincident",0.13400000000000001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.624]
[null,null,null,null,"Coincident",0.13700000000000001]
[null,"Sadadeen (Ron Goodin 11kV load) (Alice Springs System)","Substation Rating","MVA","Non-Coincident",41.4]
[null,null,null,null,"Coincident",41.4]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",18.934999999999999]
[null,null,null,null,"Coincident",18.077000000000002]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",19.306999999999999]
[null,null,null,null,"Coincident",18.431999999999999]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-02-12"]
[null,null,null,null,"Coincident","2018-02-21"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:30:00"]
[null,null,null,null,"Coincident","17:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",20.529]
[null,null,null,null,"Coincident",19.742999999999999]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.931999999999999]
[null,null,null,null,"Coincident",20.131]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.779]
[null,null,null,null,"Coincident",19.013999999999999]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.167999999999999]
[null,null,null,null,"Coincident",19.388000000000002]
[null,"Brewer + Sadadeen 22kV (Balance Loads)(Alice Springs System)","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",9.4610000000000003]
[null,null,null,null,"Coincident",9.1199999999999992]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",9.7970000000000006]
[null,null,null,null,"Coincident",9.4429999999999996]
[null,null,"Date MD occurred",null,"Non-Coincident","2018-02-12"]
[null,null,null,null,"Coincident","2018-02-21"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","13:30:00"]
[null,null,null,null,"Coincident","17:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",10.69]
[null,null,null,null,"Coincident",9.9600000000000009]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.069000000000001]
[null,null,null,null,"Coincident",10.313000000000001]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.295]
[null,null,null,null,"Coincident",9.5920000000000005]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.66]
[null,null,null,null,"Coincident",9.9320000000000004]
[null,"Tennant Creek (Tennant Creek System)","Substation Rating","MVA","Non-Coincident",16.600000000000001]
[null,null,null,null,"Coincident",16.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident",6.9039999999999999]
[null,null,null,null,"Coincident",6.8860000000000001]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident",7.11]
[null,null,null,null,"Coincident",7.0910000000000002]
[null,null,"Date MD occurred",null,"Non-Coincident","2017-10-19"]
[null,null,null,null,"Coincident","2018-02-22"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident","16:30:00"]
[null,null,null,null,"Coincident","15:00:00"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer"]
[null,null,null,null,"Coincident","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident",8.8049999999999997]
[null,null,null,null,"Coincident",7.3710000000000004]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0679999999999996]
[null,null,null,null,"Coincident",7.5910000000000002]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4689999999999994]
[null,null,null,null,"Coincident",6.9740000000000002]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.7219999999999995]
[null,null,null,null,"Coincident",7.1820000000000004]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]

{"sheet":"6.3 Sustained interruptions","index":21,"n_rows":5616,"n_cols":12,"rows_kept":5616,"cut":false,"hidden":false,"merged":[[5,1,5,4],[9,1,9,4],[8,1,8,4],[12,7,13,7],[12,11,13,11]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Power and Water Corporation"}]
[null,{"$f":"CONCATENATE(\"CATEGORY ANALYSIS \", CRY)","v":"CATEGORY ANALYSIS 2017-18"}]
[null,"6.3 SUSTAINED INTERRUPTIONS TO SUPPLY"]
[]
[null,"There is ONE table on this worksheet. It has been grouped into five subgroups of 10000 rows each for navigation purposes. See the Instructions sheet on how to group and ungroup data."]
[]
[null,"Definitions:"]
[null,"Feeder classification definitions\n(column E)",null,null,null,null,null,null,"Average duration of sustained customer interruption \n(column I)","Effect on unplanned SAIDI \n(column J)","Effect on unplanned SAIFI \n(column K)"]
[null,"CBD feeder: a feeder supplying predominantly commercial, high-rise buildings, supplied by a predominantly underground distribution network containing significant interconnection and redundancy when compared to urban areas.\nUrban feeder: a feeder, that is not a CBD feeder, with actual maximum demand over the reporting period per total feeder route length greater than 0.3 MVA/km.\nShort rural feeder: a feeder that is not a CBD or urban feeder with a total feeder route length less than 200 km.\nLong rural feeder: a feeder that is not a CBD or urban feeder with a total feeder route length greater than 200 km.\n",null,null,null,null,null,null,"\nThe average duration of an  interruption experienced by an affected customer.","\nThe sum of the duration of each unplanned sustained customer\ninterruption (in minutes) divided by the total number of distribution\ncustomers. Unplanned SAIDI excludes momentary interruptions (one minute or less).","\nThe total number of unplanned sustained customer interruptions\ndivided by the total number of distribution customers. Unplanned SAIFI excludes momentary interruptions (one minute or less). SAIFI is expressed per 0.01 interruptions."]
[]
[null,{"$f":"CONCATENATE(\"6.3.1 - SUSTAINED INTERRUPTIONS TO SUPPLY (for \",CRY,\")\")","v":"6.3.1 - SUSTAINED INTERRUPTIONS TO SUPPLY (for 2017-18)"}]
[null,"Date of event","Time of interruption","Asset ID","Feeder classification","Reason for interruption","Detailed reason for interruption","Number of customers affected by the interruption","Average duration of sustained customer interruption","Effect on unplanned SAIDI","Effect on unplanned SAIFI","MED"]
[null,"(DD/MM/YYYY)","(HH:MM)","(eg. Feeder ID)","(CBD, Urban, Short rural, Long rural)","(select from options in drop-down box)","(choose from options in column 'O' that correspond with reason in column 'F')",null,"(minutes)","(by feeder classification)","(by feeder classification)"]
[null,"02-07-2017","08:06","DT-0389","Rural Short","Unknown","Unknown",8,101.22,1.7951000000000002E-2,1.7699999999999999E-4,"No"]
[null,"03-07-2017","09:33","NMI-25000633381","Urban","Asset Failure","LV",1,222.03,6.9170000000000004E-3,3.1000000000000001E-5,"No"]
[null,"03-07-2017","14:58","DT-1358","CBD","Overloads",null,67,45.82,0.82519299999999995,1.8010999999999999E-2,"No"]
[null,"03-07-2017","17:26","NMI-25000855828","Urban","Asset Failure","LV",1,48.3,1.505E-3,3.1000000000000001E-5,"No"]
[null,"04-07-2017","08:58","NMI-25010154825","Rural Short","Third Party","Other",1,77.55,1.719E-3,2.1999999999999999E-5,"No"]
[null,"04-07-2017","09:05","22PA202 HOWARD SPRINGS","Rural Short","Planned",null,145,222.43,null,null,"No"]
[null,"04-07-2017","09:54","11LG06 BRADSHAW","Urban","Planned",null,83,186.55,null,null,"No"]
[null,"05-07-2017","09:19","11CA12 MARRARA","Urban","Planned",null,583,106.32,null,null,"No"]
[null,"05-07-2017","09:32","NMI-25000167373","Rural Short","Third Party","Other",1,199.97,4.4330000000000003E-3,2.1999999999999999E-5,"No"]
[null,"05-07-2017","10:20","22SY06 WHITEWOOD","Urban","Unknown","Unknown",1,10.82,3.3700000000000001E-4,3.1000000000000001E-5,"No"]
[null,"05-07-2017","11:17","DT-6860","Rural Short","Unknown","Unknown",2,80.98,3.591E-3,4.3999999999999999E-5,"No"]
[null,"05-07-2017","11:43","NMI-25000358541","Urban","Third Party","Unauthorised Access",1,78.38,2.4420000000000002E-3,3.1000000000000001E-5,"No"]
[null,"06-07-2017","07:25","22RG04 BREWER 2","Rural Short","Unknown","Unknown",194,15.4,6.6231999999999999E-2,4.3010000000000001E-3,"No"]
[null,"06-07-2017","09:00","11WN24 PARAP","Urban","Planned",null,255,326.97000000000003,null,null,"No"]
[null,"06-07-2017","09:04","DT-1999","Urban","Planned",null,1,163.02000000000001,null,null,"No"]
[null,"06-07-2017","09:13","11CA23 MOIL","Rural Short","Planned",null,18,302,null,null,"No"]
[null,"06-07-2017","14:55","NMI-25000340096","Rural Short","Asset Failure","LV",1,76.48,1.696E-3,2.1999999999999999E-5,"No"]
[null,"07-07-2017","08:30","22MT06 LAKE BENNETT","Rural Short","Planned",null,6,328.67,null,null,"No"]
[null,"07-07-2017","10:51","REC-10050","Rural Long","Asset Failure","HV",18,4.8499999999999996,0.10045999999999999,2.0712999999999999E-2,"No"]
[null,"07-07-2017","13:41","DT-7002","Rural Long","Unknown","Unknown",1,1.52,1.745E-3,1.1509999999999999E-3,"No"]
[null,"07-07-2017","14:02","NMI-25000658802","Urban","Asset Failure","LV",1,53.68,1.6720000000000001E-3,3.1000000000000001E-5,"No"]
[null,"09-07-2017","09:07","11PA08 YARRAWONGA","Rural Short","Planned",null,112,225,null,null,"No"]
[null,"09-07-2017","09:07","11PA08 YARRAWONGA","Rural Short","Planned",null,482,225,null,null,"No"]
[null,"09-07-2017","09:26","NMI-25000453573","Rural Short","Asset Failure","LV",1,170.15,3.7720000000000002E-3,2.1999999999999999E-5,"No"]
[null,"09-07-2017","13:05","DT-1916","CBD","Planned",null,1,300.7,null,null,"No"]
[null,"09-07-2017","21:32","DT-8197","Rural Short","Asset Failure","HV",3,272.14999999999998,1.8100000000000002E-2,6.7000000000000002E-5,"No"]
[null,"09-07-2017","22:36","REC-10007","Rural Short","Network Business","Network Error",165,2.17,7.9249999999999998E-3,3.6579999999999998E-3,"No"]
[null,"10-07-2017","13:02","PSPT127375","Rural Short","Asset Failure","LV",1,45.9,1.018E-3,2.1999999999999999E-5,"No"]
[null,"11-07-2017","07:39","22MK103 CORROBOREE","Rural Short","Unknown","Unknown",66,178.8,0.26161200000000001,1.4630000000000001E-3,"No"]
[null,"11-07-2017","11:00","22SY06 WHITEWOOD","Urban","Unknown","Unknown",1,116.87,3.6410000000000001E-3,3.1000000000000001E-5,"No"]
[null,"11-07-2017","13:09","SWH-0111","Rural Short","Network Business","Network Error",259,3.93,2.2584E-2,5.7419999999999997E-3,"No"]
[null,"11-07-2017","13:28","DT-1514","Rural Short","Network Business","Switching and Protection Error",45,323.14999999999998,0.322376,9.9799999999999997E-4,"No"]
[null,"11-07-2017","14:28","NMI-25000110963","Rural Short","Third Party","Other",1,46.07,1.021E-3,2.1999999999999999E-5,"No"]
[null,"11-07-2017","14:40","11LG13 ELDER","Urban","Asset Failure","HV",625,111.88,2.1784819999999998,1.9470999999999999E-2,"No"]
[null,"11-07-2017","15:56","NMI-25000662357","Urban","Asset Failure","LV",1,126.33,3.9360000000000003E-3,3.1000000000000001E-5,"No"]
[null,"11-07-2017","21:47","NMI-25000885874","Rural Short","Third Party","Other",1,185.83,4.1200000000000004E-3,2.1999999999999999E-5,"No"]
[null,"12-07-2017","08:42","11LG06 BRADSHAW","Urban","Planned",null,363,251.35,null,null,"No"]
[null,"12-07-2017","10:40","REC-10019","Rural Short","Third Party","Blow-in/Fall-in Other Responsibile Party",278,20.2,0.12449200000000001,6.1630000000000001E-3,"No"]
[null,"12-07-2017","10:59","11CP4307 BELYUEN","Rural Short","Planned",null,100,130,null,null,"No"]
[null,"12-07-2017","11:51","NMI-25010185763","Rural Short","Asset Failure","LV",1,107.38,2.3809999999999999E-3,2.1999999999999999E-5,"No"]
[null,"12-07-2017","14:36","11LG07 ARALUEN","Urban","Unknown","Unknown",648,112.88,2.2788369999999998,2.0188000000000001E-2,"No"]
[null,"13-07-2017","09:37","22SY11 HERBERT","Rural Short","Planned",null,33,200.23,null,null,"No"]
[null,"13-07-2017","11:15","DT-1846","Rural Short","Asset Failure","HV",9,75.849999999999994,1.5134E-2,2.0000000000000001E-4,"No"]
[null,"13-07-2017","17:07","NMI-25000852998","Urban","Third Party","Other",1,88.13,2.7460000000000002E-3,3.1000000000000001E-5,"No"]
[null,"14-07-2017","07:35","NMI-25000683345","Rural Short","Asset Failure","LV",1,128.72999999999999,2.8540000000000002E-3,2.1999999999999999E-5,"No"]
[null,"14-07-2017","10:09","22PC308 TOWNSHIP","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,175,57.38,null,null,"No"]
[null,"14-07-2017","15:17","DT-6811","Rural Long","Unknown","Unknown",1,271.68,0.312639,1.1509999999999999E-3,"No"]
[null,"16-07-2017","07:00","11LG13 ELDER","Urban","Planned",null,201,134.16999999999999,null,null,"No"]
[null,"16-07-2017","11:08","NMI-25000567522","Urban","Third Party","Other",1,189.55,5.9049999999999997E-3,3.1000000000000001E-5,"No"]
[null,"16-07-2017","16:52","NMI-25000436506","Rural Short","Asset Failure","LV",1,280.13,6.2100000000000002E-3,2.1999999999999999E-5,"No"]
[null,"17-07-2017","10:00","DT-0159","Rural Short","Animal","Animal Impact",2,73.349999999999994,3.2520000000000001E-3,4.3999999999999999E-5,"No"]
[null,"17-07-2017","12:18","22RG04 BREWER 2","Rural Short","Unknown","Unknown",194,14.95,6.4297000000000007E-2,4.3010000000000001E-3,"No"]
[null,"17-07-2017","14:26","DT-8166","Rural Short","Animal","Animal Impact",1,41.13,9.1200000000000005E-4,2.1999999999999999E-5,"No"]
[null,"18-07-2017","06:03","DT-8575","Rural Short","Planned",null,16,11.48,null,null,"No"]
[null,"19-07-2017","16:38","NMI-25000695052","Rural Short","Asset Failure","LV",1,45.83,1.016E-3,2.1999999999999999E-5,"No"]
[null,"20-07-2017","08:16","DT-0419","Rural Short","Unknown","Unknown",1,219.1,4.8570000000000002E-3,2.1999999999999999E-5,"No"]
[null,"20-07-2017","09:16","DT-6701","Rural Long","Animal","Animal Impact",1,109,0.12543199999999999,1.1509999999999999E-3,"No"]
[null,"20-07-2017","10:56","11PA03 PALM SHOPS","Urban","Asset Failure","HV",25,73.819999999999993,5.7491E-2,7.7899999999999996E-4,"No"]
[null,"20-07-2017","11:11","DT-0162","Rural Short","Network Business","Network Error",1,8.1300000000000008,1.8000000000000001E-4,2.1999999999999999E-5,"No"]
[null,"21-07-2017","09:35","DT-1176","Urban","Planned",null,3,303.82,null,null,"No"]
[null,"22-07-2017","16:09","DT-8405","Rural Short","Animal","Animal Impact",26,22.38,1.2902E-2,5.7600000000000001E-4,"No"]
[null,"22-07-2017","21:10","NMI-25010121513","Rural Short","Asset Failure","LV",1,46.72,1.036E-3,2.1999999999999999E-5,"No"]
[null,"23-07-2017","11:21","DT-6257","Rural Short","Animal","Animal Impact",1,23.68,5.2499999999999997E-4,2.1999999999999999E-5,"No"]
[null,"25-07-2017","08:59","DT-6398","Rural Short","Planned",null,1,115.42,null,null,"No"]
[null,"25-07-2017","09:15","11BE03 TDZ","Rural Short","Planned",null,1,194,null,null,"No"]
[null,"25-07-2017","09:25","DT-1173","Urban","Planned",null,66,330,null,null,"No"]
[null,"26-07-2017","00:00","DT-2183-1","CBD","Planned",null,1,269.37,null,null,"No"]
[null,"26-07-2017","00:00","DT-2183-2","CBD","Planned",null,0,269.18,null,null,"No"]
[null,"26-07-2017","09:39","DT-8008","Rural Short","Planned",null,2,20.149999999999999,null,null,"No"]
[null,"26-07-2017","10:02","22MT06 LAKE BENNETT","Rural Short","Planned",null,15,250.72,null,null,"No"]
[null,"27-07-2017","07:37","DT-0716","Rural Short","Animal","Animal Impact",5,70.62,7.8279999999999999E-3,1.11E-4,"No"]
[null,"27-07-2017","14:34","DT-8037","Rural Short","Planned",null,3,112,null,null,"No"]
[null,"28-07-2017","19:22","DT-2731","Rural Short","Unknown","Unknown",77,76.78,0.13106999999999999,1.707E-3,"No"]
[null,"30-07-2017","08:44","11BE19 HIDDEN VALLEY","Urban","Planned",null,34,234.1,null,null,"No"]
[null,"30-07-2017","09:31","DT-8477","Rural Short","Third Party","Vehicle impact",4,668.22,5.9255000000000002E-2,8.8999999999999995E-5,"No"]
[null,"30-07-2017","10:23","11CP4306 WAGAIT","Rural Short","Asset Failure","Subtransmission",278,101.22,0.62379700000000005,6.1630000000000001E-3,"No"]
[null,"30-07-2017","10:23","11CP4307 BELYUEN","Rural Short","Asset Failure","Subtransmission",1,101.45,2.2490000000000001E-3,2.1999999999999999E-5,"No"]
[null,"30-07-2017","16:52","22SY15 DARWIN RIVER","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",719,153.93,2.453624,1.5939999999999999E-2,"No"]
[null,"31-07-2017","08:52","22TC01 ALI CURUNG","Rural Long","Asset Failure","HV",98,500.43,56.435519999999997,0.112773,"No"]
[null,"31-07-2017","09:56","DT-10473","Rural Short","Planned",null,0,132.37,null,null,"No"]
[null,"01-08-2017","07:38","11LG13 ELDER","Urban","Third Party","Vehicle impact",625,38,0.73989799999999994,1.9470999999999999E-2,"No"]
[null,"01-08-2017","07:38","DT-8528","Urban","Third Party","Vehicle impact",17,67,3.5484000000000002E-2,5.2999999999999998E-4,"No"]
[null,"01-08-2017","08:30","DT-3388","Rural Short","Planned",null,23,354,null,null,"No"]
[null,"01-08-2017","09:17","SP-114935","Rural Short","Network Business","Switching and Protection Error",9,72.17,1.4399E-2,2.0000000000000001E-4,"No"]
[null,"01-08-2017","09:37","DT-0536","Rural Short","Planned",null,21,72,null,null,"No"]
[null,"01-08-2017","21:43","11LG16 BRAITLING","Rural Short","Planned",null,126,177.22,null,null,"No"]
[null,"01-08-2017","22:09","NMI-25000630209","Rural Short","Asset Failure","LV",1,263.55,5.8430000000000001E-3,2.1999999999999999E-5,"No"]
[null,"02-08-2017","00:11","DT-0431","Rural Short","Planned",null,19,246.27,null,null,"No"]
[null,"02-08-2017","10:20","DT-9555","Rural Short","Planned",null,1,110,null,null,"No"]
[null,"02-08-2017","12:40","DT-8467","Rural Short","Planned",null,1,130,null,null,"No"]
[null,"02-08-2017","13:13","DT-0028","Rural Short","Network Business","Network Error",22,6,2.9260000000000002E-3,4.8799999999999999E-4,"No"]
[null,"03-08-2017","09:01","22MT06 LAKE BENNETT","Rural Short","Planned",null,44,276.27999999999997,null,null,"No"]
[null,"03-08-2017","09:57","DT-8438","Rural Short","Planned",null,1,105.35,null,null,"No"]
[null,"03-08-2017","10:04","DT-8201","Rural Short","Planned",null,0,101.2,null,null,"No"]
[null,"03-08-2017","12:01","DT-8164","Rural Short","Planned",null,14,33.799999999999997,null,null,"No"]
[null,"03-08-2017","13:30","DT-8462","Rural Short","Planned",null,1,90,null,null,"No"]
[null,"04-08-2017","09:02","DT-0547","Rural Short","Planned",null,14,130.19999999999999,null,null,"No"]
[null,"04-08-2017","09:50","DT-8433","Rural Short","Planned",null,1,165.58,null,null,"No"]
[null,"04-08-2017","09:58","DT-3388","Rural Short","Planned",null,23,103.23,null,null,"No"]
[null,"04-08-2017","10:08","22MT01 DARWIN RIVER DAM 1","Rural Short","Planned",null,8,201.53,null,null,"No"]
[null,"04-08-2017","13:06","DT-8379","Rural Short","Planned",null,1,74.930000000000007,null,null,"No"]
[null,"04-08-2017","15:34","REC-10018","Rural Short","Planned",null,0,24,null,null,"No"]
[null,"04-08-2017","15:34","REC-10019","Rural Short","Planned",null,294,24,null,null,"No"]
[null,"05-08-2017","08:01","DT-6172","Rural Short","Asset Failure","HV",8,68.599999999999994,1.2166E-2,1.7699999999999999E-4,"No"]
[null,"05-08-2017","12:48","NMI-25010219702","Urban","Network Business","Network Error",1,146.88,4.5760000000000002E-3,3.1000000000000001E-5,"No"]
[null,"05-08-2017","13:00","DT-7084","Urban","Planned",null,19,219.4,null,null,"No"]
[null,"05-08-2017","14:55","DT-8237","Urban","Overloads",null,54,5.17,8.6920000000000001E-3,1.6819999999999999E-3,"No"]
[null,"06-08-2017","06:09","22SY15 DARWIN RIVER","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",719,74.63,1.1896199999999999,1.5939999999999999E-2,"No"]
[null,"06-08-2017","09:39","DT-1364","CBD","Planned",null,1,159.30000000000001,null,null,"No"]
[null,"06-08-2017","12:23","DT-2187","Urban","Planned",null,9,120.97,null,null,"No"]
[null,"06-08-2017","23:49","GCR-6486","Rural Short","Animal","Animal Impact",25,117.15,6.4928E-2,5.5400000000000002E-4,"No"]
[null,"08-08-2017","08:46","DT-1675","Rural Short","Planned",null,9,194.4,null,null,"No"]
[null,"08-08-2017","09:50","DT-0534","Rural Short","Planned",null,18,77.47,null,null,"No"]
[null,"08-08-2017","09:50","DT-7088","Rural Long","Planned",null,1,81.38,null,null,"No"]
[null,"08-08-2017","09:54","DT-0655","Rural Short","Planned",null,8,74,null,null,"No"]
[null,"08-08-2017","10:24","DT-8231","Rural Short","Planned",null,123,36.57,null,null,"No"]
[null,"08-08-2017","10:40","DT-0172","Rural Short","Planned",null,2,74.78,null,null,"No"]
[null,"08-08-2017","11:45","DT-8217","Rural Short","Planned",null,1,35.450000000000003,null,null,"No"]
[null,"08-08-2017","16:51","DT-6134","Rural Short","Unknown","Unknown",24,141.66999999999999,7.5374999999999998E-2,5.3200000000000003E-4,"No"]
[null,"08-08-2017","20:05","22BA04 TOWN","Rural Short","Asset Failure","HV",314,10.68,7.4367000000000003E-2,6.9610000000000002E-3,"No"]
[null,"08-08-2017","20:05","22BA05 MANTON","Rural Short","Asset Failure","HV",6,10.85,1.4430000000000001E-3,1.3300000000000001E-4,"No"]
[null,"08-08-2017","20:07","22KA03 FLORINA","Rural Short","Asset Failure","HV",238,12.53,6.6128999999999993E-2,5.2760000000000003E-3,"No"]
[null,"08-08-2017","20:07","22KA06 TINDAL 2","Rural Short","Asset Failure","HV",245,12.72,6.9069000000000005E-2,5.4310000000000001E-3,"No"]
[null,"08-08-2017","20:07","22KA07 KATH EAST","Rural Short","Asset Failure","HV",1210,13.23,0.35497800000000002,2.6825000000000002E-2,"No"]
[null,"08-08-2017","20:07","22KA09 PINE CREEK","Rural Short","Asset Failure","HV",108,12.57,3.0088E-2,2.3939999999999999E-3,"No"]
[null,"08-08-2017","20:07","22KA10 MATARANKA 1","Rural Long","Asset Failure","HV",226,13.25,3.4459149999999998,0.26006899999999999,"No"]
[null,"08-08-2017","20:07","22KA15 OPS","Rural Short","Asset Failure","HV",325,14.95,0.107714,7.2049999999999996E-3,"No"]
[null,"08-08-2017","20:07","22KA19 TINDAL 1","Rural Short","Asset Failure","HV",245,12.15,6.5991999999999995E-2,5.4310000000000001E-3,"No"]
[null,"08-08-2017","20:07","22KA22 KATHERINE","Urban","Asset Failure","HV",1442,14.03,0.63042699999999996,4.4923999999999999E-2,"No"]
[null,"08-08-2017","20:07","22KA18 GORGE","Rural Short","Asset Failure","HV",203,13.57,6.1053999999999997E-2,4.4999999999999997E-3,"No"]
[null,"08-08-2017","21:21","NMI-25000119821","Rural Short","Asset Failure","LV",1,253.3,5.6150000000000002E-3,2.1999999999999999E-5,"No"]
[null,"08-08-2017","22:59","NMI-25000812993","Rural Short","Asset Failure","LV",1,197.4,4.3759999999999997E-3,2.1999999999999999E-5,"No"]
[null,"09-08-2017","00:00","DT-1478","Urban","Planned",null,2,203.78,null,null,"No"]
[null,"09-08-2017","09:04","DT-7086","Rural Short","Planned",null,29,34.72,null,null,"No"]
[null,"09-08-2017","09:10","DT-8074","Urban","Planned",null,167,94.83,null,null,"No"]
[null,"09-08-2017","10:09","22HD402 LAMBELLS","Rural Short","Network Business","Network Error",88,3.15,6.1450000000000003E-3,1.951E-3,"No"]
[null,"09-08-2017","13:30","DT-8515","Rural Short","Planned",null,1,34.020000000000003,null,null,"No"]
[null,"09-08-2017","22:20","11CA07 JINGILI","Urban","Asset Failure","HV",606,81.02,1.5295209999999999,1.8879E-2,"No"]
[null,"10-08-2017","08:30","DT-1176","Urban","Planned",null,3,328.78,null,null,"No"]
[null,"10-08-2017","09:12","NMI-25000153779","Urban","Asset Failure","LV",1,85.35,2.6589999999999999E-3,3.1000000000000001E-5,"No"]
[null,"10-08-2017","09:33","SEC-22BR104","Rural Short","Planned",null,200,102.83,null,null,"No"]
[null,"10-08-2017","09:52","DT-0495","Rural Short","Planned",null,19,77,null,null,"No"]
[null,"10-08-2017","10:47","DT-8530","Urban","Network Business","Network Error",74,7.88,1.8173999999999999E-2,2.3050000000000002E-3,"No"]
[null,"10-08-2017","11:32","NMI-25000246333","CBD","Third Party","Unauthorised Access",1,112.18,3.0157E-2,2.6899999999999998E-4,"No"]
[null,"11-08-2017","07:07","22RG04 BREWER 2","Rural Short","Unknown","Unknown",194,15.72,6.7594000000000001E-2,4.3010000000000001E-3,"No"]
[null,"11-08-2017","15:51","11BE10 KARAMA 2","Rural Short","Asset Failure","HV",1803,47.93,1.9159310000000001,3.9971E-2,"No"]
[null,"11-08-2017","17:14","11BE10 KARAMA 2","Rural Short","Asset Failure","HV",46,107.22,0.109337,1.0200000000000001E-3,"No"]
[null,"11-08-2017","17:19","NMI-25000715445","Rural Short","Asset Failure","HV",1,114.68,2.542E-3,2.1999999999999999E-5,"No"]
[null,"12-08-2017","02:58","GCR-6486","Rural Short","Unknown","Unknown",25,14.37,7.9620000000000003E-3,5.5400000000000002E-4,"No"]
[null,"12-08-2017","08:53","DT-6470","Rural Short","Unknown","Unknown",1,34.1,7.5600000000000005E-4,2.1999999999999999E-5,"No"]
[null,"12-08-2017","09:18","NMI-25000794984","Rural Short","Asset Failure","LV",1,291.88,6.4710000000000002E-3,2.1999999999999999E-5,"No"]
[null,"12-08-2017","22:59","NMI-25010183098","Rural Short","Animal","Animal Impact",1,32.630000000000003,7.2300000000000001E-4,2.1999999999999999E-5,"No"]
[null,"13-08-2017","06:57","11LG15 LARAPINTA","Rural Short","Asset Failure","HV",993,93.22,2.0520559999999999,2.2013999999999999E-2,"No"]
[null,"13-08-2017","08:30","DT-2359","Rural Short","Planned",null,11,139.22,null,null,"No"]
[null,"13-08-2017","08:57","DT-1083","Urban","Planned",null,10,147.25,null,null,"No"]
[null,"13-08-2017","09:17","FH-6597","Rural Short","Unknown","Unknown",4,51,4.522E-3,8.8999999999999995E-5,"No"]
[null,"13-08-2017","13:07","DT-2182","Urban","Planned",null,13,76.88,null,null,"No"]
[null,"14-08-2017","07:13","22KA03 FLORINA","Rural Short","Unknown","Unknown",238,20.350000000000001,0.10737099999999999,5.2760000000000003E-3,"No"]
[null,"14-08-2017","09:55","DT-0109","Rural Short","Planned",null,7,73.2,null,null,"No"]
[null,"14-08-2017","10:35","DT-0215","Rural Short","Planned",null,15,139.68,null,null,"No"]
[null,"14-08-2017","14:44","22KA03 FLORINA","Rural Short","Asset Failure","HV",238,87.05,0.45929500000000001,5.2760000000000003E-3,"No"]
[null,"15-08-2017","01:54","DT-2053","Rural Short","Unknown","Unknown",36,188.72,0.150612,7.9799999999999999E-4,"No"]
[null,"15-08-2017","07:26","DT-6434","Rural Short","Unknown","Unknown",1,66.930000000000007,1.4840000000000001E-3,2.1999999999999999E-5,"No"]
[null,"15-08-2017","08:30","DT-2502","Urban","Planned",null,60,133.77000000000001,null,null,"No"]
[null,"15-08-2017","09:51","REC-10022","Rural Long","Planned",null,540,360.22,null,null,"No"]
[null,"15-08-2017","10:23","DT-6412","Rural Short","Unknown","Unknown",1,111.4,2.47E-3,2.1999999999999999E-5,"No"]
[null,"15-08-2017","13:42","DT-0722","Rural Short","Asset Failure","HV",1,157.75,3.4970000000000001E-3,2.1999999999999999E-5,"No"]
[null,"16-08-2017","05:15","GCR-6486","Rural Short","Unknown","Unknown",25,15,8.3129999999999992E-3,5.5400000000000002E-4,"No"]
[null,"16-08-2017","06:23","DT-0794","Rural Short","Unknown","Unknown",8,241.58,4.2845000000000001E-2,1.7699999999999999E-4,"No"]
[null,"16-08-2017","08:41","DT-1530","Rural Short","Planned",null,9,310.05,null,null,"No"]
[null,"16-08-2017","09:00","DT-8020","Rural Short","Planned",null,47,174.25,null,null,"No"]
[null,"16-08-2017","11:19","REC-10050","Rural Long","Weather",null,18,15.1,0.31277300000000002,2.0712999999999999E-2,"No"]
[null,"16-08-2017","17:57","DT-6412","Rural Short","Asset Failure","HV",1,97.83,2.1689999999999999E-3,2.1999999999999999E-5,"No"]
[null,"16-08-2017","18:14","DT-1847","Rural Short","Network Business","Network Error",9,17.100000000000001,3.4120000000000001E-3,2.0000000000000001E-4,"No"]
[null,"17-08-2017","00:37","REC-10022","Rural Long","Unknown","Unknown",540,15.48,9.6214040000000001,0.62140399999999996,"No"]
[null,"17-08-2017","02:29","GCR-6486","Rural Short","Unknown","Unknown",25,14.92,8.267E-3,5.5400000000000002E-4,"No"]
[null,"17-08-2017","07:30","DT-6746","Rural Short","Animal","Animal Impact",1,89.75,1.99E-3,2.1999999999999999E-5,"No"]
[null,"17-08-2017","08:30","DT-1666","Rural Short","Planned",null,9,165,null,null,"No"]
[null,"17-08-2017","09:02","DT-0596","Rural Short","Planned",null,15,381.15,null,null,"No"]
[null,"18-08-2017","09:10","DT-1953","Urban","Planned",null,91,233,null,null,"No"]
[null,"18-08-2017","09:32","DT-8325","Rural Short","Planned",null,46,158,null,null,"No"]
[null,"18-08-2017","09:39","22BA05 MANTON","Rural Short","Network Business","Network Error",6,3,3.9899999999999999E-4,1.3300000000000001E-4,"No"]
[null,"18-08-2017","09:39","DT-0163","Rural Short","Planned",null,1,106,null,null,"No"]
[null,"18-08-2017","09:50","DT-0130","Rural Short","Planned",null,26,200,null,null,"No"]
[null,"18-08-2017","15:02","DT-8200","Rural Short","Network Business","Network Error",1,6.73,1.4899999999999999E-4,2.1999999999999999E-5,"No"]
[null,"19-08-2017","18:25","NMI-25000682784","Rural Long","Unknown","Unknown",1,81.55,9.3842999999999996E-2,1.1509999999999999E-3,"No"]
[null,"20-08-2017","01:15","NMI-25000692288","Rural Short","Asset Failure","HV",1,246.55,5.4660000000000004E-3,2.1999999999999999E-5,"No"]
[null,"20-08-2017","02:09","11BE10 KARAMA 2","Rural Short","Asset Failure","HV",120,128.30000000000001,0.34131400000000001,2.66E-3,"No"]
[null,"20-08-2017","04:10","REC-10040","Rural Short","Unknown","Unknown",12,250,6.6506999999999997E-2,2.6600000000000001E-4,"No"]
[null,"20-08-2017","10:09","SWH-6486","Rural Short","Animal","Animal Impact",25,114.13,6.3256000000000007E-2,5.5400000000000002E-4,"No"]
[null,"20-08-2017","12:00","REC-10026","Rural Short","Animal","Animal Impact",84,144.16999999999999,0.26846700000000001,1.8619999999999999E-3,"No"]
[null,"21-08-2017","07:34","NMI-25010222092","Rural Short","Unknown","Unknown",1,165.25,3.663E-3,2.1999999999999999E-5,"No"]
[null,"21-08-2017","12:46","11PA15 MOULDEN","Urban","Network Business","Switching and Protection Error",1543,14,0.67298000000000002,4.8070000000000002E-2,"No"]
[null,"21-08-2017","12:46","11PA17 THORNGATE","Urban","Network Business","Switching and Protection Error",1,14,4.3600000000000003E-4,3.1000000000000001E-5,"No"]
[null,"21-08-2017","12:46","11PA18 WOODROFFE","Urban","Network Business","Switching and Protection Error",714,14,0.31141200000000002,2.2244E-2,"No"]
[null,"21-08-2017","12:46","11PA22 PALM CIVIC","Urban","Network Business","Switching and Protection Error",89,14,3.8816999999999997E-2,2.7729999999999999E-3,"No"]
[null,"21-08-2017","12:46","11PA23 GEORGINA","Urban","Network Business","Switching and Protection Error",342,14,0.14916399999999999,1.0655E-2,"No"]
[null,"21-08-2017","12:46","11PA25 PINELANDS","Urban","Network Business","Switching and Protection Error",3,14,1.3079999999999999E-3,9.2999999999999997E-5,"No"]
[null,"21-08-2017","12:46","11PA26 GATEWAY","Urban","Network Business","Switching and Protection Error",18,14,7.8510000000000003E-3,5.6099999999999998E-4,"No"]
[null,"21-08-2017","12:46","22PA202 HOWARD SPRINGS","Rural Short","Network Business","Switching and Protection Error",906,14,0.281192,2.0084999999999999E-2,"No"]
[null,"21-08-2017","12:46","DT-8253","Rural Short","Planned",null,1,132,null,null,"No"]
[null,"22-08-2017","08:15","DT-2133","Urban","Planned",null,1,323.17,null,null,"No"]
[null,"22-08-2017","09:16","22SY03 VIRGINIA","Rural Short","Planned",null,161,273.38,null,null,"No"]
[null,"22-08-2017","09:35","DT-8013","Rural Short","Planned",null,66,175,null,null,"No"]
[null,"22-08-2017","09:50","DT-1032","Urban","Planned",null,57,235.25,null,null,"No"]
[null,"22-08-2017","18:13","REC-10030","Rural Long","Third Party","Vehicle impact",17,546.41999999999996,10.689394,1.9563000000000001E-2,"No"]
[null,"22-08-2017","19:46","NMI-25010154437","Urban","Asset Failure","LV",1,240.22,7.4840000000000002E-3,3.1000000000000001E-5,"No"]
[null,"23-08-2017","01:00","DT-2039","Rural Short","Planned",null,37,66.17,null,null,"No"]
[null,"23-08-2017","05:24","DT-6327","Rural Short","Unknown","Unknown",1,205.22,4.5490000000000001E-3,2.1999999999999999E-5,"No"]
[null,"23-08-2017","07:26","NMI-25000419823","Rural Long","Asset Failure","LV",1,108.5,0.12485599999999999,1.1509999999999999E-3,"No"]
[null,"23-08-2017","09:52","22MT06 LAKE BENNETT","Rural Short","Planned",null,11,157.80000000000001,null,null,"No"]
[null,"24-08-2017","04:33","DT-6552","Rural Short","Unknown","Unknown",42,105.27,9.8014000000000004E-2,9.3099999999999997E-4,"No"]
[null,"24-08-2017","08:30","DT-1846","Rural Short","Planned",null,9,348.3,null,null,"No"]
[null,"24-08-2017","08:52","DT-8023","Rural Short","Planned",null,99,188,null,null,"No"]
[null,"24-08-2017","13:01","NMI-25000449720","Rural Short","Third Party","Other",1,55.97,1.2409999999999999E-3,2.1999999999999999E-5,"No"]
[null,"24-08-2017","22:15","11LG16 BRAITLING","Rural Short","Planned",null,126,158.18,null,null,"No"]
[null,"25-08-2017","01:43","DT-8032","Rural Short","Planned",null,15,67.55,null,null,"No"]
[null,"25-08-2017","04:32","GCR-6486","Rural Short","Unknown","Unknown",25,15,8.3129999999999992E-3,5.5400000000000002E-4,"No"]
[null,"25-08-2017","07:13","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,875,10,null,null,"No"]
[null,"25-08-2017","07:13","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,648,8.3000000000000007,null,null,"No"]
[null,"25-08-2017","17:41","11BE18 PORT","Rural Short","Asset Failure","HV",8,39.880000000000003,7.0730000000000003E-3,1.7699999999999999E-4,"No"]
[null,"26-08-2017","08:00","DT-1062","Urban","Planned",null,1,232.28,null,null,"No"]
[null,"26-08-2017","17:13","DT-6405","Rural Short","Unknown","Unknown",2,358.75,1.5906E-2,4.3999999999999999E-5,"No"]
[null,"26-08-2017","20:10","66PC301 COSMO HOWLEY","Rural Short","Network Business","Network Error",2,61.43,2.7239999999999999E-3,4.3999999999999999E-5,"No"]
[null,"27-08-2017","10:49","DT-1994","Rural Short","Unknown","Unknown",3,138.69999999999999,9.2250000000000006E-3,6.7000000000000002E-5,"No"]
[null,"27-08-2017","20:23","22WD101 JENKINS","Rural Short","Weather",null,720,605.25,9.6608140000000002,1.5962E-2,"No"]
[null,"28-08-2017","08:52","DT-6466","Rural Short","Planned",null,20,193.53,null,null,"No"]
[null,"29-08-2017","08:00","DT-3380","Rural Short","Planned",null,42,441.45,null,null,"No"]
[null,"29-08-2017","09:07","DT-1932","Urban","Planned",null,96,143,null,null,"No"]
[null,"29-08-2017","09:11","22KA09 PINE CREEK","Rural Short","Planned",null,2,151.18,null,null,"No"]
[null,"29-08-2017","10:06","DT-0489","Rural Short","Planned",null,1,53.3,null,null,"No"]
[null,"30-08-2017","07:51","11BE04 MCMILLANS","Rural Short","Network Business","Switching and Protection Error",378,29,0.24301700000000001,8.3800000000000003E-3,"No"]
[null,"30-08-2017","07:51","11BE06 KARAMA 1","Rural Short","Network Business","Switching and Protection Error",757,157,2.6347649999999998,1.6781999999999998E-2,"No"]
[null,"30-08-2017","07:51","11BE07 NAVY","Urban","Network Business","Switching and Protection Error",2,332,2.0686E-2,6.2000000000000003E-5,"No"]
[null,"30-08-2017","07:51","11BE09 JAIL","Rural Short","Network Business","Switching and Protection Error",208,94,0.43344899999999997,4.6109999999999996E-3,"No"]
[null,"30-08-2017","07:51","11BE10 KARAMA 2","Rural Short","Network Business","Switching and Protection Error",1803,155,6.1954640000000003,3.9971E-2,"No"]
[null,"30-08-2017","07:51","11BE13 KORMILDA","Rural Short","Network Business","Switching and Protection Error",315,216,1.5083800000000001,6.9829999999999996E-3,"No"]
[null,"30-08-2017","07:51","11BE14 ROBERTSON","Urban","Network Business","Switching and Protection Error",4,401,4.9970000000000001E-2,1.25E-4,"No"]
[null,"30-08-2017","07:51","11BE16 ANULA","Rural Short","Network Business","Switching and Protection Error",981,68,1.4788509999999999,2.1748E-2,"No"]
[null,"30-08-2017","07:51","11BE19 HIDDEN VALLEY","Urban","Network Business","Switching and Protection Error",229,222,1.583788,7.1339999999999997E-3,"No"]
[null,"30-08-2017","09:45","DT-8084","Urban","Planned",null,63,152,null,null,"No"]
[null,"30-08-2017","12:33","NMI-25000794679","Urban","Network Business","Network Error",1,202.62,6.3119999999999999E-3,3.1000000000000001E-5,"No"]
[null,"01-09-2017","19:13","11LE08 PARKSIDE","Rural Short","Asset Failure","HV",838,205.67,3.8208000000000002,1.8578000000000001E-2,"No"]
[null,"02-09-2017","07:15","DT-6976","Rural Long","Unknown","Unknown",4,88.3,0.40644400000000003,4.6030000000000003E-3,"No"]
[null,"02-09-2017","19:12","PSPT128630","Rural Short","Asset Failure","LV",1,151.85,3.3660000000000001E-3,2.1999999999999999E-5,"No"]
[null,"03-09-2017","10:06","DT-6170","Rural Short","Animal","Animal Impact",1,66.37,1.4710000000000001E-3,2.1999999999999999E-5,"No"]
[null,"03-09-2017","21:32","NMI-25000731475","Rural Short","Asset Failure","LV",1,182.78,4.052E-3,2.1999999999999999E-5,"No"]
[null,"04-09-2017","00:47","22MT06 LAKE BENNETT","Rural Short","Unknown","Unknown",229,71.72,0.36408400000000002,5.0769999999999999E-3,"No"]
[null,"04-09-2017","09:47","DT-10096","Rural Long","Planned",null,1,25.28,null,null,"No"]
[null,"05-09-2017","07:00","DT-6412","Rural Short","Animal","Animal Impact",1,104.53,2.317E-3,2.1999999999999999E-5,"No"]
[null,"05-09-2017","07:02","DT-6878","Rural Long","Animal","Animal Impact",0,99.18,0,0,"No"]
[null,"05-09-2017","07:46","DT-2268","Urban","Planned",null,32,228,null,null,"No"]
[null,"05-09-2017","07:50","22BA01 MINE","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,124,null,null,"No"]
[null,"05-09-2017","07:50","22BA04 TOWN","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,328,124,null,null,"No"]
[null,"05-09-2017","07:50","22BA05 MANTON","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,6,124,null,null,"No"]
[null,"05-09-2017","07:50","22KA03 FLORINA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,243,45,null,null,"No"]
[null,"05-09-2017","07:50","22KA06 TINDAL 2","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,46,null,null,"No"]
[null,"05-09-2017","07:50","22KA07 KATH EAST","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1253,42,null,null,"No"]
[null,"05-09-2017","07:50","22KA09 PINE CREEK","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,110,45,null,null,"No"]
[null,"05-09-2017","07:50","22KA10 MATARANKA 1","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,234,44,null,null,"No"]
[null,"05-09-2017","07:50","22KA15 OPS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,328,43,null,null,"No"]
[null,"05-09-2017","07:50","22KA18 GORGE","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,204,44,null,null,"No"]
[null,"05-09-2017","07:50","22KA19 TINDAL 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,43,null,null,"No"]
[null,"05-09-2017","07:50","22KA22 KATHERINE","Urban","3 - STPIS Exclusion (3.3)(a)",null,1469,42,null,null,"No"]
[null,"05-09-2017","07:50","22MT01 DARWIN RIVER DAM 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,0,100,null,null,"No"]
[null,"05-09-2017","07:50","22MT06 LAKE BENNETT","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,229,221,null,null,"No"]
[null,"05-09-2017","07:50","22MT07 ACACIA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,162,98,null,null,"No"]
[null,"05-09-2017","08:30","DT-3381","Rural Short","Planned",null,74,385,null,null,"No"]
[null,"05-09-2017","08:35","DT-8017","Rural Short","Planned",null,57,135,null,null,"No"]
[null,"05-09-2017","10:54","NMI-25000515664","Rural Short","Asset Failure","LV",1,115.55,2.562E-3,2.1999999999999999E-5,"No"]
[null,"05-09-2017","13:07","DT-8016","Rural Short","Planned",null,67,157.37,null,null,"No"]
[null,"06-09-2017","09:22","22MR103 MT BUNDY","Rural Short","Planned",null,12,201.65,null,null,"No"]
[null,"06-09-2017","09:48","DT-8405","Rural Short","Planned",null,26,167,null,null,"No"]
[null,"06-09-2017","16:06","DT-8157","Rural Short","Animal","Animal Impact",8,63.98,1.1348E-2,1.7699999999999999E-4,"No"]
[null,"06-09-2017","17:10","22MT06 LAKE BENNETT","Rural Short","Unknown","Unknown",229,15.1,7.6658000000000004E-2,5.0769999999999999E-3,"No"]
[null,"08-09-2017","07:07","DT-6746","Rural Short","Animal","Animal Impact",1,113.88,2.5249999999999999E-3,2.1999999999999999E-5,"No"]
[null,"08-09-2017","09:24","DT-8039","Rural Short","Network Business","Network Error",85,5.13,9.6729999999999993E-3,1.884E-3,"No"]
[null,"08-09-2017","13:18","DT-0299","Rural Short","Unknown","Unknown",3,142.32,9.4649999999999995E-3,6.7000000000000002E-5,"No"]
[null,"08-09-2017","15:21","NMI-25000140317","Rural Short","Asset Failure","LV",1,530.73,1.1766E-2,2.1999999999999999E-5,"No"]
[null,"08-09-2017","15:37","DT-6045","Rural Short","Unknown","Unknown",2,75.73,3.3579999999999999E-3,4.3999999999999999E-5,"No"]
[null,"09-09-2017","04:16","REC-10026","Rural Short","Animal","Animal Impact",84,185.42,0.34528199999999998,1.8619999999999999E-3,"No"]
[null,"09-09-2017","11:47","DT-6746","Rural Short","Animal","Animal Impact",1,168.25,3.7299999999999998E-3,2.1999999999999999E-5,"No"]
[null,"09-09-2017","13:02","22TC07 THREE WAYS","Rural Short","Planned",null,2,150,null,null,"No"]
[null,"10-09-2017","05:22","22BR102 BOREFIELDS","Rural Short","Asset Failure","HV",8,17.329999999999998,3.0739999999999999E-3,1.7699999999999999E-4,"No"]
[null,"10-09-2017","05:22","22BR104 HERMANNSBURG","Rural Short","Asset Failure","HV",1,17.22,3.8200000000000002E-4,2.1999999999999999E-5,"No"]
[null,"10-09-2017","05:22","22BR101 BR-SD 1","Rural Short","Asset Failure","HV",238,491.27,2.5920339999999999,5.2760000000000003E-3,"No"]
[null,"10-09-2017","05:22","22RG04 BREWER 2","Rural Short","Asset Failure","HV",9,16.100000000000001,3.212E-3,2.0000000000000001E-4,"No"]
[null,"10-09-2017","08:59","DT-2047","Urban","Planned",null,9,111.22,null,null,"No"]
[null,"10-09-2017","10:16","REC-10007","Rural Short","Network Business","Network Error",165,2.12,7.7429999999999999E-3,3.6579999999999998E-3,"No"]
[null,"10-09-2017","12:11","DT-2066","Urban","Planned",null,19,11.05,null,null,"No"]
[null,"10-09-2017","19:29","22KA09 PINE CREEK","Rural Short","Asset Failure","HV",110,124.1,0.30262899999999998,2.4390000000000002E-3,"No"]
[null,"11-09-2017","07:10","DT-6755","Rural Short","Unknown","Unknown",1,79.27,1.7570000000000001E-3,2.1999999999999999E-5,"No"]
[null,"11-09-2017","16:15","NMI-25000481873","Rural Short","Asset Failure","LV",1,162.52000000000001,3.6029999999999999E-3,2.1999999999999999E-5,"No"]
[null,"11-09-2017","19:00","DT-6412","Rural Short","Unknown","Unknown",1,77.930000000000007,1.7279999999999999E-3,2.1999999999999999E-5,"No"]
[null,"11-09-2017","19:46","NMI-25000546337","Rural Short","Asset Failure","LV",1,83.13,1.843E-3,2.1999999999999999E-5,"No"]
[null,"12-09-2017","00:05","REC-10022","Rural Long","Animal","Animal Impact",540,181.33,112.68124299999999,0.62140399999999996,"No"]
[null,"12-09-2017","08:21","NMI-25000682743","Urban","Asset Failure","LV",1,113.58,3.539E-3,3.1000000000000001E-5,"No"]
[null,"12-09-2017","23:50","GCR-6486","Rural Short","Unknown","Unknown",25,14.85,8.2299999999999995E-3,5.5400000000000002E-4,"No"]
[null,"13-09-2017","06:49","DT-6412","Rural Short","Unknown","Unknown",1,67.5,1.4959999999999999E-3,2.1999999999999999E-5,"No"]
[null,"13-09-2017","07:21","DT-6746","Rural Short","Unknown","Unknown",1,65.02,1.441E-3,2.1999999999999999E-5,"No"]
[null,"13-09-2017","09:25","DT-10511-A","Rural Short","Planned",null,1,238.13,null,null,"No"]
[null,"13-09-2017","10:59","DT-10209","Rural Short","Planned",null,1,186,null,null,"No"]
[null,"13-09-2017","10:59","DT-10209","Rural Short","Planned",null,1,185.4,null,null,"No"]
[null,"13-09-2017","14:38","DT-6050","Urban","Asset Failure","LV",47,85.92,0.125801,1.464E-3,"No"]
[null,"14-09-2017","13:18","NMI-25010208844","Rural Short","Third Party","Other",1,24.03,5.3300000000000005E-4,2.1999999999999999E-5,"No"]
[null,"14-09-2017","13:40","DT-6050","Urban","Overloads",null,47,82.67,0.121042,1.464E-3,"No"]
[null,"14-09-2017","14:24","NMI-25000384357","Rural Short","Asset Failure","LV",1,91.22,2.0219999999999999E-3,2.1999999999999999E-5,"No"]
[null,"14-09-2017","15:27","NMI-25000369366","Rural Short","Asset Failure","LV",1,102.37,2.2690000000000002E-3,2.1999999999999999E-5,"No"]
[null,"14-09-2017","17:37","NMI-25000176847","Rural Short","Asset Failure","LV",1,42.72,9.4700000000000003E-4,2.1999999999999999E-5,"No"]
[null,"14-09-2017","20:05","DT-1086","Urban","Network Business","Network Error",31,154.53,0.14924200000000001,9.6599999999999995E-4,"No"]
[null,"14-09-2017","22:36","22TC01 ALI CURUNG","Rural Long","Asset Failure","HV",46,100.7,5.330495,5.2934000000000002E-2,"No"]
[null,"15-09-2017","04:21","DT-6746","Rural Short","Animal","Animal Impact",1,200.87,4.4530000000000004E-3,2.1999999999999999E-5,"No"]
[null,"15-09-2017","09:02","DT-10376","Rural Long","Animal","Animal Impact",1,200.3,0.23049500000000001,1.1509999999999999E-3,"No"]
[null,"15-09-2017","10:48","DT-10737","Rural Short","Unknown","Unknown",1,154.13,3.4169999999999999E-3,2.1999999999999999E-5,"No"]
[null,"15-09-2017","11:50","REC-10035","Rural Long","Unknown","Unknown",26,69.430000000000007,2.077407,2.9919000000000001E-2,"No"]
[null,"16-09-2017","02:08","DT-6730","Rural Short","Animal","Animal Impact",2,68.099999999999994,3.019E-3,4.3999999999999999E-5,"No"]
[null,"16-09-2017","07:53","REC-10015","Rural Short","Unknown","Unknown",0,14.45,0,0,"No"]
[null,"16-09-2017","11:44","FH-6110","Rural Short","Animal","Animal Impact",6,345.3,4.5929999999999999E-2,1.3300000000000001E-4,"No"]
[null,"16-09-2017","19:39","DT-6138","Rural Long","Overloads",null,13,1.22,1.8200999999999998E-2,1.4959999999999999E-2,"No"]
[null,"16-09-2017","19:46","NMI-25000707540","Urban","Asset Failure","LV",1,33.130000000000003,1.0319999999999999E-3,3.1000000000000001E-5,"No"]
[null,"16-09-2017","20:38","DT-8518","Rural Short","Animal","Animal Impact",2,70.2,3.1129999999999999E-3,4.3999999999999999E-5,"No"]
[null,"17-09-2017","07:28","DT-6877","Rural Long","Animal","Animal Impact",1,69.28,7.9727999999999993E-2,1.1509999999999999E-3,"No"]
[null,"17-09-2017","08:03","11WN22 LUDMILLA","Rural Short","Planned",null,28,139.47999999999999,null,null,"No"]
[null,"17-09-2017","18:42","NMI-25000123007","Rural Short","Asset Failure","LV",1,54.73,1.2130000000000001E-3,2.1999999999999999E-5,"No"]
[null,"17-09-2017","19:58","NMI-25000336696","Rural Short","Unknown","Unknown",1,169.95,3.7680000000000001E-3,2.1999999999999999E-5,"No"]
[null,"17-09-2017","21:47","NMI-25010186745","Urban","Asset Failure","LV",1,97.28,3.0309999999999998E-3,3.1000000000000001E-5,"No"]
[null,"17-09-2017","22:46","NMI-25000161130","Rural Short","Animal","Animal Impact",1,209.12,4.6360000000000004E-3,2.1999999999999999E-5,"No"]
[null,"18-09-2017","07:37","FH-6552","Rural Short","Animal","Animal Impact",1,98.75,2.189E-3,2.1999999999999999E-5,"No"]
[null,"18-09-2017","09:57","NMI-25010150890","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",1,98.62,2.186E-3,2.1999999999999999E-5,"No"]
[null,"18-09-2017","11:14","DT-6878","Rural Long","Animal","Animal Impact",0,83.9,0,0,"No"]
[null,"19-09-2017","14:48","DT-0162","Rural Short","Planned",null,1,74.23,null,null,"No"]
[null,"19-09-2017","18:09","NMI-25010181549","Rural Short","Third Party","Other",1,28.43,6.3000000000000003E-4,2.1999999999999999E-5,"No"]
[null,"20-09-2017","02:34","NMI-25000716674","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",1,196.15,4.3480000000000003E-3,2.1999999999999999E-5,"No"]
[null,"20-09-2017","04:31","DT-1350","Urban","Asset Failure","LV",126,241.68,0.94869300000000001,3.9249999999999997E-3,"No"]
[null,"20-09-2017","09:01","22SY12 NOONAMAH","Rural Short","Planned",null,881,329.62,null,null,"No"]
[null,"20-09-2017","09:22","11LG16 BRAITLING","Rural Short","Planned",null,126,237.18,null,null,"No"]
[null,"20-09-2017","12:07","NMI-25000414394","Urban","Asset Failure","LV",1,84.13,2.6210000000000001E-3,3.1000000000000001E-5,"No"]
[null,"20-09-2017","19:14","NMI-25010192099","Rural Short","Network Business","Network Error",1,50.65,1.1230000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-09-2017","23:40","DT-2637","Urban","Planned",null,45,337,null,null,"No"]
[null,"21-09-2017","00:00","DT-2637","Urban","Planned",null,45,317.05,null,null,"No"]
[null,"21-09-2017","06:53","DT-6878","Rural Long","Unknown","Unknown",0,54.28,0,0,"No"]
[null,"21-09-2017","07:48","DT-6802","Rural Long","Unknown","Unknown",1,20.170000000000002,2.3206999999999998E-2,1.1509999999999999E-3,"No"]
[null,"21-09-2017","08:31","DT-0170","Rural Short","Planned",null,1,172.18,null,null,"No"]
[null,"21-09-2017","09:02","DT-6878","Rural Long","Unknown","Unknown",0,85.57,0,0,"No"]
[null,"21-09-2017","10:17","22MK303 MARRAKAI","Rural Short","Planned",null,67,94.27,null,null,"No"]
[null,"21-09-2017","13:21","22BR101 BR-SD 1","Rural Short","Weather",null,238,63,0.33240199999999998,5.2760000000000003E-3,"No"]
[null,"21-09-2017","13:48","NMI-25000763139","Rural Short","Asset Failure","LV",1,73.28,1.6249999999999999E-3,2.1999999999999999E-5,"No"]
[null,"21-09-2017","19:40","PSPT106741","Rural Short","Asset Failure","LV",1,23.3,5.1699999999999999E-4,2.1999999999999999E-5,"No"]
[null,"22-09-2017","04:24","11LE01 DARWIN PRIVATE HOSPITAL","Rural Short","Asset Failure","HV",1,11.82,2.6200000000000003E-4,2.1999999999999999E-5,"No"]
[null,"22-09-2017","04:24","11LE03 LYONS 1","Rural Short","Asset Failure","HV",792,12.23,0.21479100000000001,1.7558000000000001E-2,"No"]
[null,"22-09-2017","04:24","11LE04 TAMBLING","Rural Short","Asset Failure","HV",621,12.07,0.16612099999999999,1.3767E-2,"No"]
[null,"22-09-2017","04:24","11LE12 MUIRHEAD","Rural Short","Asset Failure","HV",993,12.53,0.27590700000000001,2.2013999999999999E-2,"No"]
[null,"22-09-2017","04:24","11LE13 ROSEWOOD","Rural Short","Asset Failure","HV",941,13.2,0.275366,2.0861000000000001E-2,"No"]
[null,"22-09-2017","04:54","GCR-6486","Rural Short","Animal","Animal Impact",25,90.38,5.0092999999999999E-2,5.5400000000000002E-4,"No"]
[null,"22-09-2017","07:08","DT-6914","Rural Long","Animal","Animal Impact",3,164,0.566168,3.4520000000000002E-3,"No"]
[null,"22-09-2017","14:34","DT-10153","Rural Short","Planned",null,5,35.92,null,null,"No"]
[null,"22-09-2017","16:00","DT-8038","Rural Short","Network Business","Network Error",153,2.1,7.123E-3,3.392E-3,"No"]
[null,"22-09-2017","18:39","DT-0714","Rural Short","Unknown","Unknown",6,220.85,2.9375999999999999E-2,1.3300000000000001E-4,"No"]
[null,"23-09-2017","03:42","FH-6311","Rural Long","Animal","Animal Impact",1,95.58,0.10999200000000001,1.1509999999999999E-3,"No"]
[null,"23-09-2017","08:50","DT-0597","Rural Short","Planned",null,1,153.22,null,null,"No"]
[null,"23-09-2017","14:23","DT-0167","Rural Short","Planned",null,2,99,null,null,"No"]
[null,"24-09-2017","09:44","DT-0529","Rural Short","Planned",null,1,101,null,null,"No"]
[null,"24-09-2017","10:00","NMI-25000497218","Rural Short","Third Party","Unauthorised Access",1,60.58,1.343E-3,2.1999999999999999E-5,"No"]
[null,"25-09-2017","00:10","DT-6245","Rural Short","Unknown","Unknown",1,77.2,1.7110000000000001E-3,2.1999999999999999E-5,"No"]
[null,"25-09-2017","08:47","22BA01 MINE","Rural Short","Overloads",null,1,4,8.8999999999999995E-5,2.1999999999999999E-5,"No"]
[null,"25-09-2017","08:47","22BA04 TOWN","Rural Short","Overloads",null,328,4,2.9086000000000001E-2,7.2709999999999997E-3,"No"]
[null,"25-09-2017","08:47","22BA05 MANTON","Rural Short","Overloads",null,6,4,5.3200000000000003E-4,1.3300000000000001E-4,"No"]
[null,"25-09-2017","08:47","22KA03 FLORINA","Rural Short","Overloads",null,243,5,2.6935000000000001E-2,5.3870000000000003E-3,"No"]
[null,"25-09-2017","08:47","22KA06 TINDAL 2","Rural Short","Overloads",null,245,5,2.7157000000000001E-2,5.4310000000000001E-3,"No"]
[null,"25-09-2017","08:47","22KA07 KATH EAST","Rural Short","Overloads",null,1253,6,0.16666700000000001,2.7778000000000001E-2,"No"]
[null,"25-09-2017","08:47","22KA09 PINE CREEK","Rural Short","Overloads",null,110,6,1.4631999999999999E-2,2.4390000000000002E-3,"No"]
[null,"25-09-2017","08:47","22KA10 MATARANKA 1","Rural Long","Overloads",null,234,7,1.884925,0.26927499999999999,"No"]
[null,"25-09-2017","08:47","22KA15 OPS","Rural Short","Overloads",null,328,7,5.0900000000000001E-2,7.2709999999999997E-3,"No"]
[null,"25-09-2017","08:47","22KA18 GORGE","Rural Short","Overloads",null,204,4,1.8089999999999998E-2,4.522E-3,"No"]
[null,"25-09-2017","08:47","22KA19 TINDAL 1","Rural Short","Overloads",null,245,9,4.8883000000000003E-2,5.4310000000000001E-3,"No"]
[null,"25-09-2017","08:47","22KA22 KATHERINE","Urban","Overloads",null,1469,8,0.36611700000000003,4.5765E-2,"No"]
[null,"25-09-2017","11:21","22KA03 FLORINA","Rural Short","Overloads",null,243,18,9.6966999999999998E-2,5.3870000000000003E-3,"No"]
[null,"25-09-2017","11:21","22KA06 TINDAL 2","Rural Short","Overloads",null,245,27,0.146648,5.4310000000000001E-3,"No"]
[null,"25-09-2017","11:21","22KA09 PINE CREEK","Rural Short","Overloads",null,110,9,2.1947000000000001E-2,2.4390000000000002E-3,"No"]
[null,"25-09-2017","11:21","22KA22 KATHERINE","Urban","Overloads",null,1469,28,1.2814110000000001,4.5765E-2,"No"]
[null,"25-09-2017","11:21","22KA19 TINDAL 1","Rural Short","Overloads",null,245,28.23,0.15334700000000001,5.4310000000000001E-3,"No"]
[null,"25-09-2017","12:50","22KA06 TINDAL 2","Rural Short","Overloads",null,245,9,4.8883000000000003E-2,5.4310000000000001E-3,"No"]
[null,"25-09-2017","12:50","22KA09 PINE CREEK","Rural Short","Overloads",null,110,8,1.9508999999999999E-2,2.4390000000000002E-3,"No"]
[null,"25-09-2017","12:50","22KA19 TINDAL 1","Rural Short","Overloads",null,245,9,4.8883000000000003E-2,5.4310000000000001E-3,"No"]
[null,"25-09-2017","12:50","22KA22 KATHERINE","Urban","Overloads",null,1469,7,0.320353,4.5765E-2,"No"]
[null,"25-09-2017","13:32","DT-6050","Urban","Overloads",null,47,45.75,6.6988000000000006E-2,1.464E-3,"No"]
[null,"25-09-2017","14:58","11CA16 NAKARA","Urban","7 - STPIS Exclusion (3.3)(a)",null,1451,143,null,null,"No"]
[null,"25-09-2017","18:07","NMI-25000539786","Rural Short","Asset Failure","LV",1,91.93,2.0379999999999999E-3,2.1999999999999999E-5,"No"]
[null,"26-09-2017","05:45","GCR-6486","Rural Short","Animal","Animal Impact",25,51.25,2.8403999999999999E-2,5.5400000000000002E-4,"No"]
[null,"26-09-2017","07:53","DT-6345","Rural Long","Animal","Animal Impact",1,92.72,0.106694,1.1509999999999999E-3,"No"]
[null,"26-09-2017","09:35","22MT07 ACACIA","Rural Short","Planned",null,17,194,null,null,"No"]
[null,"26-09-2017","15:06","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,655,8,null,null,"No"]
[null,"26-09-2017","15:06","11LG15 LARAPINTA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1002,10,null,null,"No"]
[null,"26-09-2017","15:06","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,890,17,null,null,"No"]
[null,"26-09-2017","15:07","DT-10230","Rural Short","Planned",null,0,71.75,null,null,"No"]
[null,"26-09-2017","18:20","NMI-25000527163","Urban","Asset Failure","LV",1,27.57,8.5899999999999995E-4,3.1000000000000001E-5,"No"]
[null,"27-09-2017","09:02","22BA04 TOWN","Rural Short","Planned",null,17,250.93,null,null,"No"]
[null,"27-09-2017","14:43","DT-0437","Rural Short","Planned",null,6,44.15,null,null,"No"]
[null,"27-09-2017","19:39","NMI-25000258337","Rural Short","Third Party","Unauthorised Access",1,152.63,3.3839999999999999E-3,2.1999999999999999E-5,"No"]
[null,"28-09-2017","01:42","22MT07 ACACIA","Rural Short","Unknown","Unknown",162,15.3,5.4947999999999997E-2,3.591E-3,"No"]
[null,"28-09-2017","08:26","DT-7049","Rural Short","Planned",null,50,161,null,null,"No"]
[null,"28-09-2017","09:48","22BA04 TOWN","Rural Short","Planned",null,29,280,null,null,"No"]
[null,"29-09-2017","00:54","GCR-0689","Rural Short","Unknown","Unknown",0,123.25,0,0,"No"]
[null,"29-09-2017","03:07","DT-6338","Rural Long","Unknown","Unknown",1,97.47,0.11216,1.1509999999999999E-3,"No"]
[null,"29-09-2017","04:50","GCR-0689","Rural Short","Unknown","Unknown",0,13,0,0,"No"]
[null,"29-09-2017","06:48","11WN04 BULLOCKY POINT","Urban","Unknown","Unknown",304,15.13,0.14332300000000001,9.4710000000000003E-3,"No"]
[null,"29-09-2017","08:44","DT-0657","Rural Short","Planned",null,2,206.2,null,null,"No"]
[null,"29-09-2017","13:10","22KA09 PINE CREEK","Rural Short","Planned",null,11,2.2000000000000002,null,null,"No"]
[null,"29-09-2017","17:05","NMI-25000247595","Rural Short","7 - STPIS Exclusion (3.3)(a)",null,1,17.02,null,null,"No"]
[null,"30-09-2017","06:56","DT-6878","Rural Long","Animal","Animal Impact",0,77.97,0,0,"No"]
[null,"30-09-2017","07:44","NMI-25000514666","Rural Short","Asset Failure","LV",1,205.87,4.5640000000000003E-3,2.1999999999999999E-5,"No"]
[null,"30-09-2017","07:47","PSPT109316","Rural Short","Asset Failure","LV",6,94.3,1.2543E-2,1.3300000000000001E-4,"No"]
[null,"30-09-2017","10:13","NMI-25010218217","Urban","Asset Failure","LV",1,53.3,1.66E-3,3.1000000000000001E-5,"No"]
[null,"30-09-2017","17:42","GCR-4440","Urban","Unknown","Unknown",893,18.95,0.52719199999999999,2.7820000000000001E-2,"No"]
[null,"30-09-2017","18:09","GCR-4440","Urban","Weather",null,893,6.57,0.18268599999999999,2.7820000000000001E-2,"No"]
[null,"30-09-2017","19:23","SWH-7571","Rural Long","Unknown","Unknown",18,235,4.8676640000000004,2.0712999999999999E-2,"No"]
[null,"30-09-2017","19:23","REC-10050","Rural Long","Asset Failure","HV",18,234.22,4.8514379999999999,2.0712999999999999E-2,"No"]
[null,"30-09-2017","19:40","NMI-25010196119","Rural Short","Asset Failure","LV",1,206.35,4.5750000000000001E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","10:07","22MT06 LAKE BENNETT","Rural Short","Animal","Animal Impact",229,130.19999999999999,0.66098699999999999,5.0769999999999999E-3,"No"]
[null,"01-10-2017","10:31","NMI-25000531083","Urban","Asset Failure","LV",1,261.27999999999997,8.1399999999999997E-3,3.1000000000000001E-5,"No"]
[null,"01-10-2017","10:52","NMI-25000712617","Rural Short","Asset Failure","LV",1,333.6,7.3959999999999998E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","11:25","NMI-25000803003","Rural Short","Asset Failure","LV",1,298.37,6.6140000000000001E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","11:32","NMI-25000242992","Urban","Asset Failure","LV",1,279.14999999999998,8.6969999999999999E-3,3.1000000000000001E-5,"No"]
[null,"01-10-2017","11:37","NMI-25000569791","Rural Short","Asset Failure","LV",1,563.28,1.2487E-2,2.1999999999999999E-5,"No"]
[null,"01-10-2017","11:39","NMI-25000744659","Rural Short","Asset Failure","LV",1,157.57,3.493E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","12:51","NMI-25000645551","Rural Short","Asset Failure","LV",1,260.87,5.7829999999999999E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","13:00","PSPT112789","Urban","Asset Failure","LV",4,371.12,4.6247000000000003E-2,1.25E-4,"No"]
[null,"01-10-2017","14:29","NMI-25000135348","Urban","Asset Failure","LV",1,48.4,1.508E-3,3.1000000000000001E-5,"No"]
[null,"01-10-2017","22:56","NMI-25000472962","Rural Short","Asset Failure","LV",1,248.45,5.5079999999999999E-3,2.1999999999999999E-5,"No"]
[null,"01-10-2017","23:07","NMI-25000645428","Rural Short","Asset Failure","LV",1,141.78,3.143E-3,2.1999999999999999E-5,"No"]
[null,"02-10-2017","04:55","NMI-25000711387","Urban","Network Business","Switching and Protection Error",1,62.48,1.9469999999999999E-3,3.1000000000000001E-5,"No"]
[null,"02-10-2017","06:27","DT-7025","Urban","Asset Failure","LV",1,54.97,1.712E-3,3.1000000000000001E-5,"No"]
[null,"02-10-2017","07:07","NMI-25000814379","Rural Short","Asset Failure","LV",1,128.80000000000001,2.8549999999999999E-3,2.1999999999999999E-5,"No"]
[null,"02-10-2017","12:43","DT-6061","Rural Short","Unknown","Unknown",2,120.88,5.3600000000000002E-3,4.3999999999999999E-5,"No"]
[null,"02-10-2017","13:43","NMI-25000534036","Rural Short","Asset Failure","LV",1,72.02,1.5969999999999999E-3,2.1999999999999999E-5,"No"]
[null,"02-10-2017","15:33","DT-6891","Rural Short","Weather",null,0,118.85,0,0,"No"]
[null,"02-10-2017","16:47","NMI-25000598832","Rural Short","Weather",null,1,136.41999999999999,3.0240000000000002E-3,2.1999999999999999E-5,"No"]
[null,"02-10-2017","21:28","NMI-25000681630","Rural Short","Asset Failure","LV",1,67.180000000000007,1.4890000000000001E-3,2.1999999999999999E-5,"No"]
[null,"03-10-2017","00:00","NMI-25000681630","Rural Short","Asset Failure","LV",1,117.45,2.604E-3,2.1999999999999999E-5,"No"]
[null,"03-10-2017","06:07","DT-6803","Rural Long","Animal","Animal Impact",2,79.83,0.18373600000000001,2.3010000000000001E-3,"No"]
[null,"03-10-2017","09:00","22MT06 LAKE BENNETT","Rural Short","Planned",null,42,265.3,null,null,"No"]
[null,"03-10-2017","12:06","NMI-25000114830","Rural Short","Asset Failure","LV",1,72.069999999999993,1.598E-3,2.1999999999999999E-5,"No"]
[null,"03-10-2017","13:48","DT-0588","Rural Short","Unknown","Unknown",2,115.02,5.1000000000000004E-3,4.3999999999999999E-5,"No"]
[null,"03-10-2017","15:46","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,919,14.18,0.288962,2.0372999999999999E-2,"No"]
[null,"03-10-2017","23:33","22KA22 KATHERINE","Urban","Asset Failure","HV",1469,6.82,0.31196200000000002,4.5765E-2,"No"]
[null,"04-10-2017","05:09","DT-8538","Urban","Planned",null,0,106.5,null,null,"No"]
[null,"04-10-2017","05:23","CB22TL01","Rural Short","Unknown","Unknown",0,15.72,0,0,"No"]
[null,"04-10-2017","06:53","DT-6050","Urban","Network Business","Switching and Protection Error",47,81.319999999999993,0.119065,1.464E-3,"No"]
[null,"04-10-2017","08:31","DT-0464","Rural Short","Planned",null,1,139.28,null,null,"No"]
[null,"04-10-2017","09:01","DT-0160","Rural Short","Planned",null,2,79.42,null,null,"No"]
[null,"04-10-2017","09:02","NMI-25000416177","Urban","Asset Failure","LV",1,306.33,9.5429999999999994E-3,3.1000000000000001E-5,"No"]
[null,"04-10-2017","11:01","FH-1659","Rural Short","Network Business","Network Error",341,6.6,4.9894000000000001E-2,7.5599999999999999E-3,"No"]
[null,"04-10-2017","12:49","NMI-25000135348","Urban","Third Party","Other",1,193.57,6.0299999999999998E-3,3.1000000000000001E-5,"No"]
[null,"04-10-2017","14:45","DT-0431","Rural Short","Unknown","Unknown",19,55.05,2.3188E-2,4.2099999999999999E-4,"No"]
[null,"04-10-2017","15:53","DT-10085","Rural Long","Animal","Animal Impact",2,319.33,0.73494400000000004,2.3010000000000001E-3,"No"]
[null,"04-10-2017","16:30","NMI-25000563218","Rural Short","Planned",null,1,56.62,null,null,"No"]
[null,"04-10-2017","19:00","NMI-25000764006","Urban","Planned",null,1,52.65,null,null,"No"]
[null,"04-10-2017","20:28","11CA12 MARRARA","Urban","Asset Failure","HV",667,37,0.76883999999999997,2.0778999999999999E-2,"No"]
[null,"04-10-2017","20:28","11CA23 MOIL","Rural Short","Asset Failure","HV",878,37,0.72018300000000002,1.9463999999999999E-2,"No"]
[null,"04-10-2017","20:28","11CA24 PARER","Rural Short","Asset Failure","HV",391,37,0.32071899999999998,8.6680000000000004E-3,"No"]
[null,"05-10-2017","03:27","NMI-25000711387","Urban","Asset Failure","LV",1,93.67,2.918E-3,3.1000000000000001E-5,"No"]
[null,"05-10-2017","08:02","22MT06 LAKE BENNETT","Rural Short","Planned",null,2,223,null,null,"No"]
[null,"05-10-2017","08:36","11CP4307 BELYUEN","Rural Short","Asset Failure","HV",1,198,4.3889999999999997E-3,2.1999999999999999E-5,"No"]
[null,"05-10-2017","08:36","11CP4306 WAGAIT","Rural Short","Asset Failure","HV",281,197.35,1.2293909999999999,6.2290000000000002E-3,"No"]
[null,"05-10-2017","08:37","DT-1644","Rural Short","Planned",null,93,176.8,null,null,"No"]
[null,"05-10-2017","09:10","DT-6301","Rural Short","Planned",null,7,140.47,null,null,"No"]
[null,"05-10-2017","13:03","22MT06 LAKE BENNETT","Rural Short","Planned",null,15,37.33,null,null,"No"]
[null,"05-10-2017","14:54","NMI-25000423602","Urban","Asset Failure","LV",1,163.83000000000001,5.104E-3,3.1000000000000001E-5,"No"]
[null,"05-10-2017","16:07","NMI-25000527781","Rural Short","Third Party","Other",1,186.47,4.1339999999999997E-3,2.1999999999999999E-5,"No"]
[null,"06-10-2017","08:44","22BA04 TOWN","Rural Short","Planned",null,9,157.35,null,null,"No"]
[null,"06-10-2017","13:06","22BA05 MANTON","Rural Short","Planned",null,4,50.53,null,null,"No"]
[null,"06-10-2017","13:59","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,919,15,0.30559999999999998,2.0372999999999999E-2,"No"]
[null,"06-10-2017","18:32","GCR-4440","Urban","Unknown","Unknown",893,14.35,0.39922000000000002,2.7820000000000001E-2,"No"]
[null,"06-10-2017","23:36","NMI-25000418486","Urban","Asset Failure","LV",1,51.17,1.5939999999999999E-3,3.1000000000000001E-5,"No"]
[null,"07-10-2017","04:52","22RG04 BREWER 2","Rural Short","Unknown","Unknown",198,15.33,6.7305000000000004E-2,4.3889999999999997E-3,"No"]
[null,"07-10-2017","09:15","DT-0483","Rural Short","Planned",null,1,165.3,null,null,"No"]
[null,"07-10-2017","09:20","DT-0482","Rural Short","Planned",null,2,68.38,null,null,"No"]
[null,"07-10-2017","10:35","REC-10049","Rural Long","Unknown","Unknown",39,15.02,0.67393599999999998,4.4879000000000002E-2,"No"]
[null,"07-10-2017","14:00","DT-0603","Rural Short","Planned",null,1,55.48,null,null,"No"]
[null,"07-10-2017","17:24","11PA15 MOULDEN","Urban","Asset Failure","HV",1617,267.75,13.488014,5.0375000000000003E-2,"No"]
[null,"08-10-2017","08:53","DT-0333","Rural Short","Planned",null,2,114.23,null,null,"No"]
[null,"08-10-2017","14:27","NMI-25000741014","Rural Short","Asset Failure","LV",1,184.4,4.0879999999999996E-3,2.1999999999999999E-5,"No"]
[null,"09-10-2017","07:46","22SY06 WHITEWOOD","Urban","Unknown","Unknown",1,52.27,1.6280000000000001E-3,3.1000000000000001E-5,"No"]
[null,"09-10-2017","08:08","NMI-25000711387","Urban","Network Business","Network Error",1,81.3,2.5330000000000001E-3,3.1000000000000001E-5,"No"]
[null,"09-10-2017","13:16","NMI-25000240171","Urban","Network Business","Network Error",1,84.53,2.6340000000000001E-3,3.1000000000000001E-5,"No"]
[null,"10-10-2017","06:55","DT-6878","Rural Long","Overloads",null,0,184.17,0,0,"No"]
[null,"10-10-2017","09:40","DT-0276","Urban","Planned",null,1,178.23,null,null,"No"]
[null,"10-10-2017","16:24","NMI-25000676688","Urban","Third Party","Other",1,51.05,1.5900000000000001E-3,3.1000000000000001E-5,"No"]
[null,"11-10-2017","07:19","NMI-25000638200","Rural Short","Asset Failure","LV",1,66.25,1.469E-3,2.1999999999999999E-5,"No"]
[null,"11-10-2017","08:16","NMI-25000867483","Urban","Third Party","Other",1,82.25,2.562E-3,3.1000000000000001E-5,"No"]
[null,"11-10-2017","09:56","NMI-25000517040","Rural Short","Asset Failure","LV",1,177.47,3.934E-3,2.1999999999999999E-5,"No"]
[null,"11-10-2017","21:14","NMI-25000144084","Rural Short","Third Party","Other",1,195.32,4.3299999999999996E-3,2.1999999999999999E-5,"No"]
[null,"12-10-2017","05:10","DT-8063-1","Urban","Planned",null,1,87,null,null,"No"]
[null,"12-10-2017","09:22","DT-6419","Rural Short","Planned",null,5,106.92,null,null,"No"]
[null,"12-10-2017","18:52","NMI-25000598543","Urban","Network Business","Network Error",1,69.099999999999994,2.153E-3,3.1000000000000001E-5,"No"]
[null,"12-10-2017","20:04","22PA202 HOWARD SPRINGS","Rural Short","Unknown","Unknown",919,13.5,0.27504000000000001,2.0372999999999999E-2,"No"]
[null,"12-10-2017","21:47","DT-1098","Rural Short","Third Party","Other",100,325.98,0.72267300000000001,2.2169999999999998E-3,"No"]
[null,"12-10-2017","21:47","11WN01 BAGOT","Rural Short","7 - STPIS Exclusion (3.3)(a)",null,782,2.13,null,null,"No"]
[null,"14-10-2017","07:46","DT-6543","Rural Long","Asset Failure","HV",1,121.53,0.13985400000000001,1.1509999999999999E-3,"No"]
[null,"14-10-2017","08:33","DT-6543","Rural Long","Unknown","Unknown",1,37.15,4.2750000000000003E-2,1.1509999999999999E-3,"No"]
[null,"14-10-2017","09:23","22SY03 VIRGINIA","Rural Short","Planned",null,37,289,null,null,"No"]
[null,"14-10-2017","11:02","NMI-25000112743","Rural Short","Asset Failure","LV",1,77.95,1.7279999999999999E-3,2.1999999999999999E-5,"No"]
[null,"14-10-2017","12:31","NMI-25000633417","Urban","Asset Failure","LV",1,83.92,2.614E-3,3.1000000000000001E-5,"No"]
[null,"15-10-2017","12:32","DT-2681","Rural Short","Planned",null,1,189.13,null,null,"No"]
[null,"15-10-2017","13:59","NMI-25000190089","Rural Short","Asset Failure","LV",1,90.35,2.003E-3,2.1999999999999999E-5,"No"]
[null,"16-10-2017","04:33","22WD101 JENKINS","Rural Short","Weather",null,4,41,3.6359999999999999E-3,8.8999999999999995E-5,"No"]
[null,"16-10-2017","04:33","22WD102 WICKHAM","Urban","Weather",null,2,49,3.0530000000000002E-3,6.2000000000000003E-5,"No"]
[null,"16-10-2017","04:40","22SY15 DARWIN RIVER","Rural Short","Weather",null,770,34,0.58038500000000004,1.7069999999999998E-2,"No"]
[null,"16-10-2017","07:12","DT-0087","Rural Short","Asset Failure","HV",13,46.48,1.3396E-2,2.8800000000000001E-4,"No"]
[null,"16-10-2017","09:26","DT-0159","Rural Short","Animal","Animal Impact",2,32.57,1.444E-3,4.3999999999999999E-5,"No"]
[null,"16-10-2017","10:38","DT-0134","Rural Short","Planned",null,1,113.75,null,null,"No"]
[null,"16-10-2017","11:18","DT-8177-1","Rural Short","Planned",null,2,13.78,null,null,"No"]
[null,"16-10-2017","17:41","NMI-25000335938","Rural Short","Asset Failure","LV",1,77.099999999999994,1.709E-3,2.1999999999999999E-5,"No"]
[null,"16-10-2017","18:12","11CA07 JINGILI","Urban","Asset Failure","HV",606,40,0.75516399999999995,1.8879E-2,"No"]
[null,"17-10-2017","04:20","DT-8063-1","Urban","Planned",null,1,155.25,null,null,"No"]
[null,"17-10-2017","08:59","DT-7131","Rural Long","Planned",null,1,420.73,null,null,"No"]
[null,"17-10-2017","09:09","22SY11 HERBERT","Rural Short","Planned",null,1,114.37,null,null,"No"]
[null,"17-10-2017","09:59","22SY03 VIRGINIA","Rural Short","Planned",null,105,253.77,null,null,"No"]
[null,"17-10-2017","10:02","DT-0448","Rural Short","Planned",null,5,96.87,null,null,"No"]
[null,"17-10-2017","13:35","DT-1481","Urban","Asset Failure","HV",1,925.15,2.8822E-2,3.1000000000000001E-5,"No"]
[null,"17-10-2017","13:35","11CA17 CAS SQUARE","Urban","Asset Failure","HV",4,59.9,7.4640000000000001E-3,1.25E-4,"No"]
[null,"18-10-2017","08:31","DT-1648","Rural Short","Planned",null,7,151.6,null,null,"No"]
[null,"18-10-2017","10:32","DT-0117","Rural Short","Planned",null,16,134.30000000000001,null,null,"No"]
[null,"18-10-2017","14:26","NMI-25000472962","Rural Short","Asset Failure","LV",1,58.67,1.3010000000000001E-3,2.1999999999999999E-5,"No"]
[null,"19-10-2017","08:34","22SY03 VIRGINIA","Rural Short","Planned",null,1,300.42,null,null,"No"]
[null,"19-10-2017","13:49","NMI-25000700191","Rural Short","Asset Failure","LV",1,61.02,1.353E-3,2.1999999999999999E-5,"No"]
[null,"19-10-2017","13:55","DT-0602","Rural Short","Unknown","Unknown",1,95.55,2.1180000000000001E-3,2.1999999999999999E-5,"No"]
[null,"19-10-2017","17:50","DT-7040","Rural Short","Asset Failure","HV",2,40.83,1.81E-3,4.3999999999999999E-5,"No"]
[null,"19-10-2017","17:55","NMI-25000726815","Urban","Third Party","Other",1,60.4,1.882E-3,3.1000000000000001E-5,"No"]
[null,"19-10-2017","18:49","DT-8341","Urban","Planned",null,29,32.979999999999997,null,null,"No"]
[null,"19-10-2017","22:45","DT-1995","Rural Short","Planned",null,11,282.83,null,null,"No"]
[null,"20-10-2017","15:48","DT-1904","Rural Short","Unknown","Unknown",51,23.57,2.6644999999999999E-2,1.1310000000000001E-3,"No"]
[null,"20-10-2017","17:17","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,655,15,null,null,"No"]
[null,"20-10-2017","17:17","11LG15 LARAPINTA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1002,16,null,null,"No"]
[null,"20-10-2017","17:17","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,890,14.27,null,null,"No"]
[null,"20-10-2017","18:16","22TC08 TCK WEST","Urban","Vegetation","Blow-in/Fall-in NSP Responsibility",214,18.399999999999999,0.12267,6.6670000000000002E-3,"No"]
[null,"21-10-2017","15:59","11AR12 FAIRWAY WATERS","Rural Short","Asset Failure","HV",1493,81.93,2.7118570000000002,3.3098000000000002E-2,"No"]
[null,"21-10-2017","21:33","NMI-25000778292","Urban","Asset Failure","LV",1,76.7,2.3890000000000001E-3,3.1000000000000001E-5,"No"]
[null,"22-10-2017","12:16","DT-1974","Rural Short","Overloads",null,56,50.5,6.2694E-2,1.2409999999999999E-3,"No"]
[null,"23-10-2017","10:15","DT-8201","Rural Short","Animal","Animal Impact",0,40.799999999999997,0,0,"No"]
[null,"23-10-2017","10:38","DT-0588","Rural Short","Animal","Animal Impact",2,90.48,4.0119999999999999E-3,4.3999999999999999E-5,"No"]
[null,"23-10-2017","12:25","NMI-25000169801","Urban","Asset Failure","LV",1,150.63,4.6930000000000001E-3,3.1000000000000001E-5,"No"]
[null,"23-10-2017","12:39","NMI-25000396857","CBD","Third Party","Other",1,93.25,2.5066999999999999E-2,2.6899999999999998E-4,"No"]
[null,"24-10-2017","09:08","DT-0276","Urban","Planned",null,1,275.37,null,null,"No"]
[null,"24-10-2017","18:15","NMI-25000417217","CBD","Third Party","Other",1,24.05,6.4650000000000003E-3,2.6899999999999998E-4,"No"]
[null,"25-10-2017","01:00","DT-1396","CBD","Planned",null,4,326.27,null,null,"No"]
[null,"25-10-2017","10:28","DT-10096","Rural Long","Planned",null,1,152,null,null,"No"]
[null,"25-10-2017","16:18","NMI-25000139110","Rural Short","Network Business","Network Error",1,67.13,1.488E-3,2.1999999999999999E-5,"No"]
[null,"25-10-2017","16:19","NMI-25000490504","Rural Short","Asset Failure","LV",1,59.53,1.32E-3,2.1999999999999999E-5,"No"]
[null,"25-10-2017","16:39","NMI-25000381363","Urban","Asset Failure","LV",1,150.35,4.6839999999999998E-3,3.1000000000000001E-5,"No"]
[null,"25-10-2017","17:24","NMI-25000767329","Rural Short","Network Business","Network Error",1,62.28,1.3810000000000001E-3,2.1999999999999999E-5,"No"]
[null,"26-10-2017","10:10","22SY04 DUNDEE","Rural Long","Planned",null,27,235,null,null,"No"]
[null,"26-10-2017","10:14","DT-7069","Rural Short","Planned",null,3,120.27,null,null,"No"]
[null,"26-10-2017","14:04","NMI-25000707581","Rural Short","Network Business","Network Error",1,50.85,1.127E-3,2.1999999999999999E-5,"No"]
[null,"26-10-2017","15:34","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,46,20,null,null,"No"]
[null,"26-10-2017","15:34","22TC09 WARREGO","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,19,null,null,"No"]
[null,"27-10-2017","10:16","DT-10037","Rural Long","Planned",null,1,63.15,null,null,"No"]
[null,"27-10-2017","10:30","11LG06 BRADSHAW","Urban","Animal","Animal Impact",1881,32.200000000000003,1.886919,5.8599999999999999E-2,"No"]
[null,"27-10-2017","10:35","DT-10341","Rural Long","Asset Failure","HV",1,110.53,0.127196,1.1509999999999999E-3,"No"]
[null,"27-10-2017","12:49","NMI-25000821657","Rural Short","Asset Failure","LV",1,174.83,3.8760000000000001E-3,2.1999999999999999E-5,"No"]
[null,"27-10-2017","14:27","11RG20 WILLS","Urban","Weather",null,611,18.12,0.34484799999999999,1.9035E-2,"No"]
[null,"28-10-2017","10:03","DT-6002","Urban","Unknown","Unknown",14,35.880000000000003,1.5651000000000002E-2,4.3600000000000003E-4,"No"]
[null,"28-10-2017","10:52","NMI-25000607759","Rural Short","Asset Failure","LV",1,40.950000000000003,9.0799999999999995E-4,2.1999999999999999E-5,"No"]
[null,"28-10-2017","16:57","22BA01 MINE","Rural Short","Weather",null,1,4.4800000000000004,9.8999999999999994E-5,2.1999999999999999E-5,"No"]
[null,"28-10-2017","16:58","NMI-25000768567","Rural Short","Weather",null,1,152.5,3.3809999999999999E-3,2.1999999999999999E-5,"No"]
[null,"28-10-2017","18:33","NMI-25000347966","Rural Short","Weather",null,1,59.07,1.3090000000000001E-3,2.1999999999999999E-5,"No"]
[null,"28-10-2017","23:07","DT-0452","Rural Short","Asset Failure","HV",4,341.72,3.0301999999999999E-2,8.8999999999999995E-5,"No"]
[null,"29-10-2017","12:13","NMI-25000708639","Rural Short","Asset Failure","LV",1,166.68,3.6949999999999999E-3,2.1999999999999999E-5,"No"]
[null,"29-10-2017","18:04","DT-2628","Urban","Overloads",null,98,147.32,0.449766,3.0530000000000002E-3,"No"]
[null,"29-10-2017","19:33","22TC01 ALI CURUNG","Rural Long","Asset Failure","HV",46,103.18,5.4619489999999997,5.2934000000000002E-2,"Yes"]
[null,"29-10-2017","19:33","22TC02 TCK EAST","Urban","Asset Failure","HV",643,95.43,1.911699,2.0032000000000001E-2,"Yes"]
[null,"29-10-2017","19:33","22TC07 THREE WAYS","Rural Short","Asset Failure","HV",564,83.57,1.044861,1.2503E-2,"Yes"]
[null,"29-10-2017","19:33","22TC08 TCK WEST","Urban","Asset Failure","HV",214,80.400000000000006,0.53601699999999997,6.6670000000000002E-3,"Yes"]
[null,"29-10-2017","19:33","22TC09 WARREGO","Rural Short","Asset Failure","HV",1,79.58,1.7639999999999999E-3,2.1999999999999999E-5,"Yes"]
[null,"30-10-2017","04:59","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,919,14.47,0.294734,2.0372999999999999E-2,"No"]
[null,"30-10-2017","06:49","DT-6277","Rural Long","Unknown","Unknown",2,430.87,0.99163800000000002,2.3010000000000001E-3,"No"]
[null,"30-10-2017","08:57","CBH-22RG04","Rural Short","Unknown","Unknown",198,15.25,6.6938999999999999E-2,4.3889999999999997E-3,"No"]
[null,"30-10-2017","09:14","NMI-25000744922","Rural Short","Asset Failure","LV",1,53.3,1.1820000000000001E-3,2.1999999999999999E-5,"No"]
[null,"30-10-2017","09:59","11CA17 CAS SQUARE","Urban","Asset Failure","HV",4,51.28,6.391E-3,1.25E-4,"No"]
[null,"30-10-2017","10:11","22TC01 ALI CURUNG","Rural Long","Asset Failure","HV",46,2.42,0.12792500000000001,5.2934000000000002E-2,"No"]
[null,"30-10-2017","10:11","22TC07 THREE WAYS","Rural Short","Asset Failure","HV",564,1.1200000000000001,1.3962E-2,1.2503E-2,"No"]
[null,"30-10-2017","10:11","22TC09 WARREGO","Rural Short","Asset Failure","HV",1,1.93,4.3000000000000002E-5,2.1999999999999999E-5,"No"]
[null,"30-10-2017","20:58","NMI-25000116588","Rural Short","Asset Failure","LV",1,84.33,1.8699999999999999E-3,2.1999999999999999E-5,"No"]
[null,"30-10-2017","21:53","11BE18 PORT","Rural Short","Asset Failure","HV",7,37.17,5.7679999999999997E-3,1.55E-4,"No"]
[null,"31-10-2017","07:35","DT-7131","Rural Long","Planned",null,1,493,null,null,"No"]
[null,"31-10-2017","09:04","22SY12 NOONAMAH","Rural Short","Planned",null,114,252.35,null,null,"No"]
[null,"31-10-2017","12:51","DT-2452","Rural Short","Asset Failure","HV",2,72.98,3.2360000000000002E-3,4.3999999999999999E-5,"No"]
[null,"31-10-2017","13:54","DT-1298","Rural Short","Overloads",null,10,172.15,3.8163999999999997E-2,2.22E-4,"No"]
[null,"31-10-2017","17:06","CB66BE202","N/A","Network Business","Network Error",0,87,null,null,"No"]
[null,"31-10-2017","23:22","REC-10031","Rural Short","Weather",null,7,389,6.0366000000000003E-2,1.55E-4,"No"]
[null,"01-11-2017","01:00","22KA09 PINE CREEK","Rural Short","Network Business","Network Error",110,25.2,6.1453000000000001E-2,2.4390000000000002E-3,"No"]
[null,"01-11-2017","02:25","GCR-0453","Rural Long","Weather",null,21,208,5.0264670000000002,2.4166E-2,"No"]
[null,"01-11-2017","07:59","22KA03 FLORINA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,243,4.32,null,null,"No"]
[null,"01-11-2017","07:59","22KA05 CAP BANK 1","N/A","3 - STPIS Exclusion (3.3)(a)",null,0,14.82,null,null,"No"]
[null,"01-11-2017","07:59","22KA06 TINDAL 2","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,4.9800000000000004,null,null,"No"]
[null,"01-11-2017","07:59","22KA09 PINE CREEK","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,110,3.62,null,null,"No"]
[null,"01-11-2017","07:59","22KA17 CAP BANK 2","N/A","3 - STPIS Exclusion (3.3)(a)",null,0,14.55,null,null,"No"]
[null,"01-11-2017","07:59","22KA19 TINDAL 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,3.48,null,null,"No"]
[null,"01-11-2017","07:59","22KA22 KATHERINE","Urban","3 - STPIS Exclusion (3.3)(a)",null,1469,2.0299999999999998,null,null,"No"]
[null,"01-11-2017","09:22","DT-0832","Rural Short","Planned",null,0,40.17,null,null,"No"]
[null,"01-11-2017","15:34","NMI-25010196174","Rural Short","Asset Failure","LV",1,55.7,1.235E-3,2.1999999999999999E-5,"No"]
[null,"01-11-2017","16:07","11PA25 PINELANDS","Urban","Weather",null,3,82.15,7.6779999999999999E-3,9.2999999999999997E-5,"No"]
[null,"01-11-2017","16:14","NMI-25000316138","Rural Short","Weather",null,1,135.62,3.006E-3,2.1999999999999999E-5,"No"]
[null,"02-11-2017","08:35","DT-6062","Rural Short","Planned",null,2,166.28,null,null,"No"]
[null,"02-11-2017","08:41","DT-8448","Rural Short","Planned",null,1,229.17,null,null,"No"]
[null,"02-11-2017","08:48","22TC01 ALI CURUNG","Rural Long","Planned",null,4,229.17,null,null,"No"]
[null,"02-11-2017","09:17","DT-3139","Urban","Planned",null,1,181.48,null,null,"No"]
[null,"03-11-2017","06:12","FH-6187","Rural Short","Unknown","Unknown",9,19.23,3.8370000000000001E-3,2.0000000000000001E-4,"No"]
[null,"03-11-2017","17:29","DT-0360","Rural Short","Unknown","Unknown",1,295.37,6.548E-3,2.1999999999999999E-5,"No"]
[null,"03-11-2017","18:21","NMI-25000136296","Rural Short","Asset Failure","LV",1,114.17,2.5309999999999998E-3,2.1999999999999999E-5,"No"]
[null,"04-11-2017","04:45","REC-10022","Rural Long","Unknown","Unknown",540,14.22,8.8342919999999996,0.62140399999999996,"No"]
[null,"04-11-2017","10:42","DT-0899","Rural Short","Unknown","Unknown",1,81.83,1.8140000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-11-2017","00:32","NMI-25000138747","Urban","Third Party","Other",1,96.03,2.9919999999999999E-3,3.1000000000000001E-5,"No"]
[null,"05-11-2017","03:24","DT-6484",null,"Unknown","Unknown",1,45.25,null,null,"No"]
[null,"05-11-2017","17:29","DT-2025","Urban","Unknown","Unknown",77,86.8,0.20821799999999999,2.3990000000000001E-3,"No"]
[null,"06-11-2017","10:36","NMI-25000466691","Urban","Unknown","Unknown",1,113.12,3.5239999999999998E-3,3.1000000000000001E-5,"No"]
[null,"06-11-2017","10:55","22SY04 DUNDEE","Rural Long","Planned",null,1,173.32,null,null,"No"]
[null,"06-11-2017","11:05","DT-6365",null,"Unknown","Unknown",0,65.349999999999994,null,null,"No"]
[null,"06-11-2017","11:40","NMI-25000382007","Rural Short","Asset Failure","LV",1,167.63,3.7160000000000001E-3,2.1999999999999999E-5,"No"]
[null,"06-11-2017","22:11","DT-0485","Rural Short","Asset Failure","LV",1,163.83000000000001,3.6319999999999998E-3,2.1999999999999999E-5,"No"]
[null,"07-11-2017","09:22","DT-0123","Rural Short","Planned",null,3,187,null,null,"No"]
[null,"07-11-2017","09:45","NMI-25000608070","Rural Short","Network Business","Network Error",1,99.5,2.2060000000000001E-3,2.1999999999999999E-5,"No"]
[null,"07-11-2017","11:07","DT-1745","Urban","Third Party","Other",1,135.52000000000001,4.2220000000000001E-3,3.1000000000000001E-5,"No"]
[null,"08-11-2017","07:15","DT-6878","Rural Long","Asset Failure","LV",0,56.53,0,0,"No"]
[null,"08-11-2017","07:45","22BR101 BR-SD 1","Rural Short","Planned",null,24,328.95,null,null,"No"]
[null,"08-11-2017","09:00","11CA12 MARRARA","Urban","Planned",null,15,316.10000000000002,null,null,"No"]
[null,"08-11-2017","20:43","NMI-25000723272","Rural Short","Asset Failure","LV",1,170.62,3.7820000000000002E-3,2.1999999999999999E-5,"No"]
[null,"08-11-2017","21:00","DT-1206","CBD","Planned",null,28,359.65,null,null,"No"]
[null,"08-11-2017","21:07","NMI-25000110907","Rural Short","Asset Failure","LV",1,187.43,4.1549999999999998E-3,2.1999999999999999E-5,"No"]
[null,"09-11-2017","01:45","11WH02 BLESSER CREEK","Rural Short","Asset Failure","HV",33,64.5,4.7187E-2,7.3200000000000001E-4,"No"]
[null,"09-11-2017","08:15","DT-6416","Rural Short","Planned",null,13,67.97,null,null,"No"]
[null,"09-11-2017","09:19","DT-6700","Rural Long","Asset Failure","LV",1,142.37,0.163828,1.1509999999999999E-3,"No"]
[null,"09-11-2017","09:20","22SY03 VIRGINIA","Rural Short","Planned",null,17,292.25,null,null,"No"]
[null,"09-11-2017","09:48","11RG07 HOSPITAL","Urban","3 - STPIS Exclusion (3.3)(a)",null,50,367,null,null,"No"]
[null,"09-11-2017","09:48","22BR102 BOREFIELDS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,8,162,null,null,"No"]
[null,"09-11-2017","09:48","22BR103 BR-SD 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,191,162,null,null,"No"]
[null,"09-11-2017","09:48","22BR103 BR-SD 2","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,198,162,null,null,"No"]
[null,"09-11-2017","09:48","22BR104 HERMANNSBURG","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,162,null,null,"No"]
[null,"09-11-2017","09:48","22BR101 BR-SD 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,238,366.62,null,null,"No"]
[null,"09-11-2017","09:49","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,655,298,null,null,"No"]
[null,"09-11-2017","09:49","11LG15 LARAPINTA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1002,316,null,null,"No"]
[null,"09-11-2017","09:49","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,890,177,null,null,"No"]
[null,"09-11-2017","09:50","11LG06 BRADSHAW","Urban","3 - STPIS Exclusion (3.3)(a)",null,1881,313,null,null,"No"]
[null,"09-11-2017","09:50","11LG10 GHAN RD","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,129,293,null,null,"No"]
[null,"09-11-2017","09:50","11LG13 ELDER","Urban","3 - STPIS Exclusion (3.3)(a)",null,609,306,null,null,"No"]
[null,"09-11-2017","09:50","11LG16 BRAITLING","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1652,316,null,null,"No"]
[null,"09-11-2017","09:50","11LG21 STOKES","Urban","3 - STPIS Exclusion (3.3)(a)",null,17,327,null,null,"No"]
[null,"09-11-2017","09:50","11RG01 GAP","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,739,175,null,null,"No"]
[null,"09-11-2017","09:50","11RG06 SADADEEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,381,122,null,null,"No"]
[null,"09-11-2017","09:50","11RG08 CBD","Urban","3 - STPIS Exclusion (3.3)(a)",null,179,351,null,null,"No"]
[null,"09-11-2017","09:50","11RG19 NTH STUART HWY","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1937,80,null,null,"No"]
[null,"09-11-2017","09:50","11RG20 WILLS","Urban","3 - STPIS Exclusion (3.3)(a)",null,611,88,null,null,"No"]
[null,"09-11-2017","09:50","11RG21 GILLEN","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,216,86,null,null,"No"]
[null,"09-11-2017","09:50","22RG09 FARMS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,114,182,null,null,"No"]
[null,"09-11-2017","09:51","REC-10008","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,15,204,null,null,"No"]
[null,"09-11-2017","12:54","22MR103 MT BUNDY","Rural Short","Asset Failure","HV",12,135,3.5914000000000001E-2,2.6600000000000001E-4,"No"]
[null,"09-11-2017","12:54","22MR303 TOMS GULLY","Rural Short","Asset Failure","HV",5,135,1.4964E-2,1.11E-4,"No"]
[null,"09-11-2017","15:10","NMI-25000521729","Urban","Asset Failure","LV",1,82.17,2.5600000000000002E-3,3.1000000000000001E-5,"No"]
[null,"09-11-2017","16:11","NMI-25010204249","Urban","Asset Failure","LV",1,45.93,1.431E-3,3.1000000000000001E-5,"No"]
[null,"09-11-2017","16:34","NMI-25000402589","Rural Short","Network Business","Network Error",1,119.42,2.647E-3,2.1999999999999999E-5,"No"]
[null,"09-11-2017","16:40","NMI-25000873094","Rural Short","Network Business","Network Error",1,115.27,2.555E-3,2.1999999999999999E-5,"No"]
[null,"09-11-2017","18:45","NMI-25000625513","Urban","Asset Failure","LV",1,101.15,3.1510000000000002E-3,3.1000000000000001E-5,"No"]
[null,"09-11-2017","18:52","NMI-25000402589","Rural Short","Network Business","Network Error",1,97.83,2.1689999999999999E-3,2.1999999999999999E-5,"No"]
[null,"09-11-2017","20:49","PSPT113336","Urban","Asset Failure","LV",8,93.65,2.334E-2,2.4899999999999998E-4,"No"]
[null,"10-11-2017","08:36","NMI-25000418149","Urban","Asset Failure","LV",1,121.28,3.7780000000000001E-3,3.1000000000000001E-5,"No"]
[null,"10-11-2017","09:35","DT-8466","Rural Short","Planned",null,1,105.22,null,null,"No"]
[null,"10-11-2017","23:02","DT-6730","Rural Short","Asset Failure","HV",2,92.22,4.0889999999999998E-3,4.3999999999999999E-5,"No"]
[null,"11-11-2017","06:39","FH-6663","Rural Short","Weather",null,3,184.55,1.2274E-2,6.7000000000000002E-5,"No"]
[null,"11-11-2017","07:10","11LE13 ROSEWOOD","Rural Short","Asset Failure","HV",95,134.97999999999999,0.28428300000000001,2.1059999999999998E-3,"No"]
[null,"11-11-2017","07:14","DT-1573","Rural Short","Asset Failure","HV",1,180.98,4.0119999999999999E-3,2.1999999999999999E-5,"No"]
[null,"11-11-2017","08:35","22RG04 BREWER 2","Rural Short","Weather",null,198,17.27,7.5790999999999997E-2,4.3889999999999997E-3,"No"]
[null,"11-11-2017","09:00","DT-7134","Rural Long","Planned",null,0,190.28,null,null,"No"]
[null,"11-11-2017","09:33","22RG04 BREWER 2","Rural Short","Weather",null,198,14.22,6.2404000000000001E-2,4.3889999999999997E-3,"No"]
[null,"11-11-2017","11:06","DT-1335","Rural Short","Unknown","Unknown",75,137.85,0.22919999999999999,1.663E-3,"No"]
[null,"11-11-2017","13:41","DT-1335","Rural Short","Asset Failure","HV",1,97.75,2.1670000000000001E-3,2.1999999999999999E-5,"No"]
[null,"11-11-2017","13:44","22RG04 BREWER 2","Rural Short","Weather",null,198,6.65,2.9190000000000001E-2,4.3889999999999997E-3,"No"]
[null,"11-11-2017","14:33","DT-8162","Rural Short","Unknown","Unknown",17,66.12,2.4917999999999999E-2,3.77E-4,"No"]
[null,"12-11-2017","04:27","FH-6411","Rural Short","Weather",null,12,57.57,1.5313999999999999E-2,2.6600000000000001E-4,"No"]
[null,"12-11-2017","05:51","DT-2398","Rural Short","Planned",null,2,499.13,null,null,"No"]
[null,"12-11-2017","06:30","DT-2112","Rural Short","Planned",null,9,14.15,null,null,"No"]
[null,"12-11-2017","08:31","11BE09 JAIL","Rural Short","Planned",null,55,285.60000000000002,null,null,"No"]
[null,"12-11-2017","12:02","NMI-25010248700","Rural Short","Third Party","Other",1,32.270000000000003,7.1500000000000003E-4,2.1999999999999999E-5,"No"]
[null,"12-11-2017","16:42","DT-1441","Urban","Asset Failure","LV",85,106.35,0.28162100000000001,2.6480000000000002E-3,"No"]
[null,"12-11-2017","19:09","11LG07 ARALUEN","Urban","Weather",null,655,28.33,0.57815899999999998,2.0406000000000001E-2,"No"]
[null,"13-11-2017","06:34","FH-6397","Rural Short","Weather",null,1,48.23,1.0690000000000001E-3,2.1999999999999999E-5,"No"]
[null,"13-11-2017","08:40","NMI-25010229056","Rural Short","Asset Failure","LV",1,122.95,2.7260000000000001E-3,2.1999999999999999E-5,"No"]
[null,"13-11-2017","09:57","11LE08 PARKSIDE","Rural Short","Planned",null,838,253,null,null,"No"]
[null,"13-11-2017","10:07","NMI-25000791743","Urban","Asset Failure","LV",1,113.82,3.5460000000000001E-3,3.1000000000000001E-5,"No"]
[null,"13-11-2017","10:26","DT-10491","Rural Long","Planned",null,2,97.75,null,null,"No"]
[null,"13-11-2017","13:21","NMI-25000792491","Urban","Third Party","Other",1,62.7,1.9530000000000001E-3,3.1000000000000001E-5,"No"]
[null,"13-11-2017","14:24","NMI-25000429906","Rural Short","Asset Failure","LV",1,302.3,6.7019999999999996E-3,2.1999999999999999E-5,"No"]
[null,"13-11-2017","16:41","REC-10007","Rural Short","Weather",null,165,17.350000000000001,6.3464000000000007E-2,3.6579999999999998E-3,"No"]
[null,"13-11-2017","17:08","11LG06 BRADSHAW","Urban","3 - STPIS Exclusion (3.3)(a)",null,1881,98,null,null,"No"]
[null,"13-11-2017","17:08","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,655,72,null,null,"No"]
[null,"13-11-2017","17:08","11LG10 GHAN RD","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,129,114,null,null,"No"]
[null,"13-11-2017","17:08","11LG13 ELDER","Urban","3 - STPIS Exclusion (3.3)(a)",null,609,99,null,null,"No"]
[null,"13-11-2017","17:08","11LG15 LARAPINTA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1002,115,null,null,"No"]
[null,"13-11-2017","17:08","11LG16 BRAITLING","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1652,128,null,null,"No"]
[null,"13-11-2017","17:08","11LG21 STOKES","Urban","3 - STPIS Exclusion (3.3)(a)",null,17,120,null,null,"No"]
[null,"13-11-2017","17:08","11RG01 GAP","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,739,37,null,null,"No"]
[null,"13-11-2017","17:08","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,890,60,null,null,"No"]
[null,"13-11-2017","17:08","11RG06 SADADEEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,381,78,null,null,"No"]
[null,"13-11-2017","17:08","11RG19 NTH STUART HWY","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1937,40,null,null,"No"]
[null,"13-11-2017","17:08","11RG21 GILLEN","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,216,120,null,null,"No"]
[null,"13-11-2017","17:08","22BR102 BOREFIELDS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,8,196,null,null,"No"]
[null,"13-11-2017","17:08","22BR104 HERMANNSBURG","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,194,null,null,"No"]
[null,"13-11-2017","17:08","22RG09 FARMS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,114,103,null,null,"No"]
[null,"13-11-2017","17:08","REC-10008","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,15,127,null,null,"No"]
[null,"13-11-2017","17:09","11RG20 WILLS","Urban","3 - STPIS Exclusion (3.3)(a)",null,611,72,null,null,"No"]
[null,"13-11-2017","17:30","NMI-25000507604","Rural Short","Asset Failure","LV",1,79.900000000000006,1.771E-3,2.1999999999999999E-5,"No"]
[null,"13-11-2017","20:11","22BR103 BR-SD 2","Rural Short","Weather",null,209,12,5.5599999999999997E-2,4.633E-3,"No"]
[null,"13-11-2017","21:39","NMI-25000798036","Rural Short","Asset Failure","LV",1,75.08,1.665E-3,2.1999999999999999E-5,"No"]
[null,"13-11-2017","21:44","SWH-18306","Rural Short","Weather",null,22,37.880000000000003,1.8475999999999999E-2,4.8799999999999999E-4,"No"]
[null,"13-11-2017","22:28","NMI-25010140883","Rural Short","Asset Failure","LV",1,72.92,1.616E-3,2.1999999999999999E-5,"No"]
[null,"14-11-2017","07:06","22TC01 ALI CURUNG","Rural Long","Weather",null,46,24,1.2704260000000001,5.2934000000000002E-2,"No"]
[null,"14-11-2017","07:06","22TC02 TCK EAST","Urban","Weather",null,643,4,8.0127000000000004E-2,2.0032000000000001E-2,"No"]
[null,"14-11-2017","07:06","22TC07 THREE WAYS","Rural Short","Weather",null,564,13,0.16254299999999999,1.2503E-2,"No"]
[null,"14-11-2017","07:06","22TC09 WARREGO","Rural Short","Weather",null,1,287,6.3629999999999997E-3,2.1999999999999999E-5,"No"]
[null,"14-11-2017","07:23","DT-10140","Rural Long","Unknown","Unknown",2,103.75,0.23877999999999999,2.3010000000000001E-3,"No"]
[null,"14-11-2017","09:00","22MT07 ACACIA","Rural Short","Planned",null,70,158,null,null,"No"]
[null,"14-11-2017","10:53","66 PC-PK","N/A","Unknown","Unknown",0,205,null,null,"No"]
[null,"14-11-2017","15:28","11WN22 LUDMILLA","Rural Short","Weather",null,1224,49.6,1.34589,2.7134999999999999E-2,"No"]
[null,"14-11-2017","18:04","DT-0854","Rural Short","Weather",null,3,44.47,2.957E-3,6.7000000000000002E-5,"No"]
[null,"14-11-2017","18:36","DT-2423","Urban","Weather",null,57,152.33000000000001,0.270507,1.776E-3,"No"]
[null,"15-11-2017","04:14","DT-0536","Rural Short","Unknown","Unknown",21,121.18,5.6417000000000002E-2,4.66E-4,"No"]
[null,"15-11-2017","09:00","22SY15 DARWIN RIVER","Rural Short","Planned",null,103,256.22000000000003,null,null,"No"]
[null,"15-11-2017","09:01","NMI-25000732885","Rural Short","Asset Failure","HV",1,143.66999999999999,3.1849999999999999E-3,2.1999999999999999E-5,"No"]
[null,"15-11-2017","09:21","11LG16 BRAITLING","Rural Short","Planned",null,28,167,null,null,"No"]
[null,"15-11-2017","10:16","REC-10037","Rural Short","Third Party","Dig-in",27,115.6,6.9194000000000006E-2,5.9900000000000003E-4,"No"]
[null,"15-11-2017","11:23","PT-0958","Rural Short","Unknown","Unknown",0,156.68,0,0,"No"]
[null,"15-11-2017","16:59","REC-10014","Rural Short","Weather",null,2,20.02,8.8699999999999998E-4,4.3999999999999999E-5,"No"]
[null,"15-11-2017","18:47","22BR103 BR-SD 2","Rural Short","Weather",null,198,4,1.7558000000000001E-2,4.3889999999999997E-3,"No"]
[null,"15-11-2017","19:20","22BR103 BR-SD 2","Rural Short","Weather",null,198,4,1.7558000000000001E-2,4.3889999999999997E-3,"No"]
[null,"15-11-2017","19:35","22BR103 BR-SD 2","Rural Short","Weather",null,198,16,7.0231000000000002E-2,4.3889999999999997E-3,"No"]
[null,"15-11-2017","19:38","NMI-25010209941","Urban","Asset Failure","LV",1,100.15,3.1199999999999999E-3,3.1000000000000001E-5,"No"]
[null,"15-11-2017","19:40","PSPT128630","Rural Short","Asset Failure","LV",1,96.8,2.1459999999999999E-3,2.1999999999999999E-5,"No"]
[null,"15-11-2017","20:05","11WN01 BAGOT","Rural Short","Planned",null,313,228.82,null,null,"No"]
[null,"16-11-2017","09:00","DT-8293","Rural Short","Planned",null,1,198.15,null,null,"No"]
[null,"16-11-2017","09:03","DT-2301","Rural Short","Planned",null,7,117.2,null,null,"No"]
[null,"16-11-2017","17:03","NMI-25000185600","Rural Short","Third Party","Other",1,75.680000000000007,1.678E-3,2.1999999999999999E-5,"No"]
[null,"16-11-2017","18:41","NMI-25000387276","Urban","Asset Failure","LV",1,27.27,8.4900000000000004E-4,3.1000000000000001E-5,"No"]
[null,"17-11-2017","15:39","DT-0609","Rural Short","Unknown","Unknown",1,375.95,8.3339999999999994E-3,2.1999999999999999E-5,"No"]
[null,"18-11-2017","06:29","DT-8100","Urban","Unknown","Unknown",80,63.33,0.15784500000000001,2.4919999999999999E-3,"No"]
[null,"18-11-2017","07:19","REC-10022","Rural Long","Unknown","Unknown",540,15.75,9.7871120000000005,0.62140399999999996,"No"]
[null,"18-11-2017","08:03","11AR12 FAIRWAY WATERS","Rural Short","Asset Failure","HV",1493,19.52,0.64596900000000002,3.3098000000000002E-2,"No"]
[null,"18-11-2017","10:59","NMI-25020116047","Rural Short","Asset Failure","LV",1,60.2,1.335E-3,2.1999999999999999E-5,"No"]
[null,"18-11-2017","17:36","DT-1042","Urban","Unknown","Unknown",1,21.58,6.7199999999999996E-4,3.1000000000000001E-5,"No"]
[null,"18-11-2017","19:40","11CA23 MOIL","Rural Short","Unknown","Unknown",878,169.68,3.3027839999999999,1.9463999999999999E-2,"No"]
[null,"19-11-2017","08:30","11BE09 JAIL","Rural Short","Planned",null,20,215.6,null,null,"No"]
[null,"19-11-2017","13:40","NMI-25000158489","Urban","Asset Failure","LV",1,116.52,3.63E-3,3.1000000000000001E-5,"No"]
[null,"19-11-2017","16:38","22MT06 LAKE BENNETT","Rural Short","Weather",null,229,198.37,1.0070490000000001,5.0769999999999999E-3,"No"]
[null,"19-11-2017","16:49","NMI-25000506044","Rural Short","Asset Failure","LV",1,101.25,2.245E-3,2.1999999999999999E-5,"No"]
[null,"19-11-2017","18:28","NMI-25000516885","Urban","Asset Failure","LV",1,86.08,2.6819999999999999E-3,3.1000000000000001E-5,"No"]
[null,"19-11-2017","20:49","NMI-25000419766","Urban","Unknown","Unknown",1,88.17,2.7469999999999999E-3,3.1000000000000001E-5,"No"]
[null,"19-11-2017","21:21","DT-1234","Urban","Asset Failure","LV",86,75.45,0.20214599999999999,2.679E-3,"No"]
[null,"20-11-2017","08:19","NMI-25000657828","Urban","Asset Failure","LV",1,48.12,1.4989999999999999E-3,3.1000000000000001E-5,"No"]
[null,"20-11-2017","09:56","DT-0519","Rural Short","Planned",null,17,169.7,null,null,"No"]
[null,"20-11-2017","09:58","11LG16 BRAITLING","Rural Short","Weather",null,1652,28.92,1.059021,3.6623000000000003E-2,"No"]
[null,"20-11-2017","10:12","NMI-25000112059","Rural Short","Asset Failure","LV",1,89.38,1.9819999999999998E-3,2.1999999999999999E-5,"No"]
[null,"20-11-2017","10:15","DT-0726","Rural Short","Planned",null,4,65.569999999999993,null,null,"No"]
[null,"20-11-2017","11:16","NMI-25000310074","Rural Short","Asset Failure","LV",1,51.43,1.14E-3,2.1999999999999999E-5,"No"]
[null,"20-11-2017","12:35","DT-6753","Rural Long","Animal","Animal Impact",1,97.58,0.112294,1.1509999999999999E-3,"No"]
[null,"20-11-2017","13:58","DT-7111","Rural Long","Unknown","Unknown",1,31.68,3.6459999999999999E-2,1.1509999999999999E-3,"No"]
[null,"20-11-2017","15:48","REC-10031","Rural Short","Weather",null,7,42.5,6.5950000000000002E-3,1.55E-4,"No"]
[null,"20-11-2017","16:18","GCR-6486","Rural Short","Asset Failure","LV",25,79.13,4.3858000000000001E-2,5.5400000000000002E-4,"No"]
[null,"20-11-2017","18:13","DT-0474","Rural Short","Unknown","Unknown",1,190.42,4.2209999999999999E-3,2.1999999999999999E-5,"No"]
[null,"20-11-2017","18:40","NMI-25000801668","Rural Short","Unknown","Unknown",1,76,1.6850000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-11-2017","20:01","NMI-25000130556","Rural Short","Asset Failure","LV",1,118.08,2.6180000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-11-2017","20:01","22KA18 GORGE","Rural Short","Weather",null,204,14.33,6.4822000000000005E-2,4.522E-3,"No"]
[null,"21-11-2017","00:15","DT-6867","Rural Short","Animal","Animal Impact",1,66.33,1.4710000000000001E-3,2.1999999999999999E-5,"No"]
[null,"21-11-2017","08:58","DT-1293","Rural Short","Planned",null,2,216.9,null,null,"No"]
[null,"21-11-2017","09:00","DT-0079","Rural Short","Planned",null,4,150.22,null,null,"No"]
[null,"21-11-2017","09:15","DT-0898","Rural Short","Planned",null,10,100.32,null,null,"No"]
[null,"21-11-2017","16:16","22BR103 BR-SD 2","Rural Short","Weather",null,198,50.77,0.22283900000000001,4.3889999999999997E-3,"No"]
[null,"21-11-2017","17:53","22PC308 TOWNSHIP","Rural Short","Asset Failure","HV",178,2,7.8919999999999997E-3,3.9459999999999999E-3,"No"]
[null,"21-11-2017","17:54","22KA03 FLORINA","Rural Short","Asset Failure","HV",243,23,0.123903,5.3870000000000003E-3,"No"]
[null,"21-11-2017","17:54","22KA06 TINDAL 2","Rural Short","Asset Failure","HV",245,23,0.12492200000000001,5.4310000000000001E-3,"No"]
[null,"21-11-2017","17:54","22KA07 KATH EAST","Rural Short","Asset Failure","HV",1253,23,0.63888900000000004,2.7778000000000001E-2,"No"]
[null,"21-11-2017","17:54","22KA09 PINE CREEK","Rural Short","Weather",null,110,23,5.6087999999999999E-2,2.4390000000000002E-3,"No"]
[null,"21-11-2017","17:54","22KA10 MATARANKA 1","Rural Long","Asset Failure","HV",234,23,6.1933259999999999,0.26927499999999999,"No"]
[null,"21-11-2017","17:54","22KA15 OPS","Rural Short","Asset Failure","HV",328,23,0.167243,7.2709999999999997E-3,"No"]
[null,"21-11-2017","17:54","22KA18 GORGE","Rural Short","Asset Failure","HV",204,23,0.104017,4.522E-3,"No"]
[null,"21-11-2017","17:54","22KA19 TINDAL 1","Rural Short","Asset Failure","HV",245,23,0.12492200000000001,5.4310000000000001E-3,"No"]
[null,"21-11-2017","17:54","22KA22 KATHERINE","Urban","Asset Failure","HV",1469,23,1.0525869999999999,4.5765E-2,"No"]
[null,"22-11-2017","06:45","DT-1505","Rural Short","Animal","Animal Impact",1,139.57,3.094E-3,2.1999999999999999E-5,"No"]
[null,"22-11-2017","09:00","22SY11 HERBERT","Rural Short","Planned",null,50,220.17,null,null,"No"]
[null,"22-11-2017","09:04","DT-0446","Rural Short","Planned",null,10,131.27000000000001,null,null,"No"]
[null,"22-11-2017","09:06","22HD402 LAMBELLS","Rural Short","Planned",null,96,163,null,null,"No"]
[null,"22-11-2017","09:06","22HD402 LAMBELLS","Rural Short","Planned",null,80,179.42,null,null,"No"]
[null,"22-11-2017","14:13","DT-0419","Rural Short","Weather",null,1,708.32,1.5703000000000002E-2,2.1999999999999999E-5,"No"]
[null,"22-11-2017","14:32","132 MT-BA-PK","N/A","Weather",null,0,11.3,null,null,"No"]
[null,"22-11-2017","15:52","22KA03 FLORINA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,243,6.85,null,null,"No"]
[null,"22-11-2017","15:52","22KA06 TINDAL 2","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,6.6,null,null,"No"]
[null,"22-11-2017","15:52","22KA07 KATH EAST","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1253,7.93,null,null,"No"]
[null,"22-11-2017","15:52","22KA09 PINE CREEK","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,110,6.97,null,null,"No"]
[null,"22-11-2017","15:52","22KA10 MATARANKA 1","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,234,6.8,null,null,"No"]
[null,"22-11-2017","15:52","22KA15 OPS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,328,6.63,null,null,"No"]
[null,"22-11-2017","15:52","22KA18 GORGE","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,204,7.47,null,null,"No"]
[null,"22-11-2017","15:52","22KA19 TINDAL 1","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,245,11.78,null,null,"No"]
[null,"22-11-2017","15:52","22KA22 KATHERINE","Urban","3 - STPIS Exclusion (3.3)(a)",null,1469,7.23,null,null,"No"]
[null,"22-11-2017","15:52","22PC308 TOWNSHIP","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,178,16.100000000000001,null,null,"No"]
[null,"22-11-2017","16:14","DT-0726","Rural Short","Asset Failure","HV",4,265.83,2.3573E-2,8.8999999999999995E-5,"No"]
[null,"22-11-2017","17:24","NMI-25000585723","Rural Short","Weather",null,1,72.72,1.6119999999999999E-3,2.1999999999999999E-5,"No"]
[null,"22-11-2017","18:32","NMI-25000675946","Urban","Asset Failure","LV",1,111.2,3.4640000000000001E-3,3.1000000000000001E-5,"No"]
[null,"23-11-2017","09:20","DT-0372","Rural Short","Planned",null,30,82.8,null,null,"No"]
[null,"23-11-2017","09:21","22SY15 DARWIN RIVER","Rural Short","Planned",null,36,188.4,null,null,"No"]
[null,"23-11-2017","10:19","FH-6597","Rural Short","Weather",null,4,29.23,2.5920000000000001E-3,8.8999999999999995E-5,"No"]
[null,"23-11-2017","11:36","22BR101 BR-SD 1","Rural Short","Unknown","Unknown",238,38.25,0.201816,5.2760000000000003E-3,"No"]
[null,"23-11-2017","14:18","NMI-25000711000","Rural Short","Asset Failure","LV",1,53.7,1.1900000000000001E-3,2.1999999999999999E-5,"No"]
[null,"23-11-2017","14:35","22WD101 JENKINS","Rural Short","Weather",null,4,15.92,1.4109999999999999E-3,8.8999999999999995E-5,"No"]
[null,"24-11-2017","06:05","DT-6076","Rural Short","Unknown","Unknown",1,54.62,1.2110000000000001E-3,2.1999999999999999E-5,"No"]
[null,"24-11-2017","08:41","DT-6144","Rural Short","Planned",null,16,152.22999999999999,null,null,"No"]
[null,"24-11-2017","09:05","DT-0570","Rural Short","Planned",null,21,126,null,null,"No"]
[null,"24-11-2017","09:22","22SY12 NOONAMAH","Rural Short","Planned",null,83,206.17,null,null,"No"]
[null,"24-11-2017","09:26","DT-6002","Urban","Unknown","Unknown",14,32.049999999999997,1.3979E-2,4.3600000000000003E-4,"No"]
[null,"24-11-2017","09:40","DT-8252","Rural Short","Planned",null,17,95.38,null,null,"No"]
[null,"24-11-2017","10:25","DT-0325","Rural Short","Planned",null,10,66.17,null,null,"No"]
[null,"24-11-2017","12:58","REC-10049","Rural Long","Unknown","Unknown",39,15.07,0.67618,4.4879000000000002E-2,"No"]
[null,"25-11-2017","02:23","66 BE-HC 1","N/A","Animal","Animal Impact",0,143,null,null,"No"]
[null,"25-11-2017","10:11","22TC09 WARREGO","Rural Short","Weather",null,1,453.05,1.0044000000000001E-2,2.1999999999999999E-5,"No"]
[null,"25-11-2017","14:17","22TC01 ALI CURUNG","Rural Long","Weather",null,46,30.82,1.631262,5.2934000000000002E-2,"No"]
[null,"25-11-2017","14:23","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,919,17.37,0.35381699999999999,2.0372999999999999E-2,"No"]
[null,"25-11-2017","14:57","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,46,55.92,null,null,"No"]
[null,"25-11-2017","14:57","22TC02 TCK EAST","Urban","3 - STPIS Exclusion (3.3)(a)",null,643,53.15,null,null,"No"]
[null,"25-11-2017","14:57","22TC07 THREE WAYS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,564,43.87,null,null,"No"]
[null,"25-11-2017","14:57","22TC08 TCK WEST","Urban","3 - STPIS Exclusion (3.3)(a)",null,214,15.25,null,null,"No"]
[null,"25-11-2017","14:57","22TC09 WARREGO","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,167.87,null,null,"No"]
[null,"25-11-2017","15:04","11WN22 LUDMILLA","Rural Short","Weather",null,1224,23.17,0.62862499999999999,2.7134999999999999E-2,"No"]
[null,"26-11-2017","07:29","DT-0843","Rural Short","Asset Failure","HV",1,132.62,2.9399999999999999E-3,2.1999999999999999E-5,"No"]
[null,"26-11-2017","08:25","DT-1347","Rural Short","Planned",null,1,423,null,null,"No"]
[null,"26-11-2017","23:47","DT-6521","Rural Short","Unknown","Unknown",1,28.9,6.4099999999999997E-4,2.1999999999999999E-5,"No"]
[null,"27-11-2017","01:01","22TC01 ALI CURUNG","Rural Long","Asset Failure","HV",46,16,0.84695100000000001,5.2934000000000002E-2,"No"]
[null,"27-11-2017","01:01","22TC09 WARREGO","Rural Short","Weather",null,1,847,1.8776999999999999E-2,2.1999999999999999E-5,"No"]
[null,"27-11-2017","06:26","DT-0933","Rural Short","Unknown","Unknown",1,112.02,2.483E-3,2.1999999999999999E-5,"No"]
[null,"27-11-2017","08:22","NMI-25000493579","Rural Short","Unknown","Unknown",1,46.45,1.0300000000000001E-3,2.1999999999999999E-5,"No"]
[null,"27-11-2017","09:00","DT-0231","Rural Short","Planned",null,13,112.13,null,null,"No"]
[null,"27-11-2017","09:16","DT-1983","Rural Short","Planned",null,4,96.17,null,null,"No"]
[null,"27-11-2017","09:17","NMI-25000141652","Rural Short","Unknown","Unknown",1,17.149999999999999,3.8000000000000002E-4,2.1999999999999999E-5,"No"]
[null,"27-11-2017","09:46","NMI-25000592308","Rural Short","Unknown","Unknown",1,46.33,1.0269999999999999E-3,2.1999999999999999E-5,"No"]
[null,"27-11-2017","10:19","NMI-25000116507","Rural Short","Network Business","Switching and Protection Error",1,71.3,1.5809999999999999E-3,2.1999999999999999E-5,"No"]
[null,"27-11-2017","10:46","DT-1297","Rural Short","Planned",null,16,135,null,null,"No"]
[null,"27-11-2017","10:46","NMI-25000398521","Rural Short","Asset Failure","LV",1,112.87,2.5019999999999999E-3,2.1999999999999999E-5,"No"]
[null,"27-11-2017","13:52","NMI-25000278717","Urban","Asset Failure","LV",1,42.35,1.3190000000000001E-3,3.1000000000000001E-5,"No"]
[null,"27-11-2017","17:15","DT-10253","Rural Long","Unknown","Unknown",1,157.97999999999999,0.18179899999999999,1.1509999999999999E-3,"No"]
[null,"28-11-2017","05:17","DT-0431","Rural Short","Network Business","Network Error",19,91.05,3.8351000000000003E-2,4.2099999999999999E-4,"No"]
[null,"28-11-2017","09:00","22SY02 MCMINNS","Rural Short","Planned",null,74,296.33,null,null,"No"]
[null,"28-11-2017","09:46","DT-9549","Rural Short","Planned",null,1,98.32,null,null,"No"]
[null,"28-11-2017","18:30","DT-0452","Rural Short","Asset Failure","HV",4,204.27,1.8114000000000002E-2,8.8999999999999995E-5,"No"]
[null,"29-11-2017","07:36","11LG07 ARALUEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,655,19.420000000000002,null,null,"No"]
[null,"29-11-2017","07:36","11LG15 LARAPINTA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1002,18.600000000000001,null,null,"No"]
[null,"29-11-2017","07:36","11RG02 GOLF","Urban","3 - STPIS Exclusion (3.3)(a)",null,890,17,null,null,"No"]
[null,"29-11-2017","08:27","DT-2764","Urban","Unknown","Unknown",1,104.92,3.2690000000000002E-3,3.1000000000000001E-5,"No"]
[null,"29-11-2017","08:30","DT-1616","Rural Short","Planned",null,9,210.67,null,null,"No"]
[null,"29-11-2017","09:42","22SY12 NOONAMAH","Rural Short","Planned",null,57,169.83,null,null,"No"]
[null,"29-11-2017","10:02","22KA09 PINE CREEK","Rural Short","Planned",null,33,178,null,null,"No"]
[null,"30-11-2017","09:00","DT-1894","Rural Short","Planned",null,9,141.58000000000001,null,null,"No"]
[null,"30-11-2017","09:25","DT-1161","Urban","Planned",null,32,187,null,null,"No"]
[null,"30-11-2017","10:00","DT-9557","Rural Short","Planned",null,2,85.12,null,null,"No"]
[null,"30-11-2017","10:15","DT-8373","Rural Short","Planned",null,15,76.13,null,null,"No"]
[null,"30-11-2017","23:42","DT-2489","Rural Short","Asset Failure","LV",1,192.27,4.2620000000000002E-3,2.1999999999999999E-5,"No"]
[null,"01-12-2017","12:32","REC-10049","Rural Long","Unknown","Unknown",39,17.72,0.79510899999999995,4.4879000000000002E-2,"No"]
[null,"01-12-2017","13:01","NMI-25010252040","Rural Short","Third Party","Other",1,34.93,7.7399999999999995E-4,2.1999999999999999E-5,"No"]
[null,"01-12-2017","17:41","22RG04 BREWER 2","Rural Short","Weather",null,198,18.579999999999998,8.1571000000000005E-2,4.3889999999999997E-3,"No"]
[null,"01-12-2017","18:42","DT-8368","Rural Short","Weather",null,28,147.63,9.1641E-2,6.2100000000000002E-4,"No"]
[null,"02-12-2017","16:03","NMI-25010152290","Urban","Third Party","Other",1,36.799999999999997,1.1460000000000001E-3,3.1000000000000001E-5,"No"]
[null,"02-12-2017","17:47","SWH-6089",null,"Weather",null,1,14.65,null,null,"No"]
[null,"02-12-2017","20:03","SWH-6089",null,"Weather",null,1,8.6,null,null,"No"]
[null,"03-12-2017","01:41","11CA16 NAKARA","Urban","Weather",null,1451,16.38,0.740591,4.5204000000000001E-2,"No"]
[null,"03-12-2017","02:14","11WN11 BISHOP","Urban","Unknown","Unknown",356,15.33,0.17005700000000001,1.1091E-2,"No"]
[null,"03-12-2017","03:16","DT-1255","Rural Short","Weather",null,1,229.55,5.0889999999999998E-3,2.1999999999999999E-5,"No"]
[null,"03-12-2017","03:35","11BE19 HIDDEN VALLEY","Urban","Weather",null,360,191,2.1421230000000002,1.1214999999999999E-2,"No"]
[null,"03-12-2017","07:30","FH-6597","Rural Short","Weather",null,4,55.95,4.9610000000000001E-3,8.8999999999999995E-5,"No"]
[null,"03-12-2017","08:20","DT-6424","Rural Short","Weather",null,1,66.27,1.469E-3,2.1999999999999999E-5,"No"]
[null,"03-12-2017","08:38","DT-10152","Rural Long","Weather",null,1,260.73,0.30003800000000003,1.1509999999999999E-3,"No"]
[null,"03-12-2017","12:13","22BA01 MINE","Rural Short","Unknown","Unknown",1,18,3.9899999999999999E-4,2.1999999999999999E-5,"No"]
[null,"03-12-2017","13:10","DT-7566","Urban","Animal","Animal Impact",1,33.32,1.0380000000000001E-3,3.1000000000000001E-5,"No"]
[null,"03-12-2017","16:55","NMI-25000516521","Rural Short","Asset Failure","LV",1,144.05000000000001,3.1930000000000001E-3,2.1999999999999999E-5,"No"]
[null,"03-12-2017","22:40","DT-1250","Urban","Unknown","Unknown",1,238.62,7.4339999999999996E-3,3.1000000000000001E-5,"No"]
[null,"04-12-2017","09:50","DT-0542","Rural Short","Planned",null,20,165,null,null,"No"]
[null,"04-12-2017","10:03","11CP4306 WAGAIT","Rural Short","Planned",null,281,369.15,null,null,"No"]
[null,"04-12-2017","10:03","11CP4307 BELYUEN","Rural Short","Planned",null,1,369.03,null,null,"No"]
[null,"04-12-2017","13:01","22MT06 LAKE BENNETT","Rural Short","Planned",null,32,94.2,null,null,"No"]
[null,"05-12-2017","08:17","22MT07 ACACIA","Rural Short","Asset Failure","HV",162,385.85,1.385734,3.591E-3,"No"]
[null,"05-12-2017","08:41","22BA04 TOWN","Rural Short","Planned",null,44,356,null,null,"No"]
[null,"05-12-2017","11:06","DT-1004","Urban","Asset Failure","LV",8,102.83,2.5628999999999999E-2,2.4899999999999998E-4,"No"]
[null,"05-12-2017","16:45","REC-10011","Rural Short","Unknown","Unknown",219,15.93,7.7356999999999995E-2,4.8549999999999999E-3,"No"]
[null,"05-12-2017","17:40","NMI-25000235245","Urban","Network Business","Switching and Protection Error",1,113.52,3.5360000000000001E-3,3.1000000000000001E-5,"No"]
[null,"06-12-2017","04:55","CB22TL05","Rural Short","Weather",null,0,14.65,0,0,"No"]
[null,"06-12-2017","07:03","DT-1250","Urban","Unknown","Unknown",1,127.62,3.9760000000000004E-3,3.1000000000000001E-5,"No"]
[null,"06-12-2017","07:41","DT-1726","Rural Short","Planned",null,9,259,null,null,"No"]
[null,"06-12-2017","07:59","DT-6983","Rural Long","Unknown","Unknown",1,181.3,0.20863100000000001,1.1509999999999999E-3,"No"]
[null,"06-12-2017","09:30","11WN02 FANNIE BAY","Urban","Planned",null,221,248.83,null,null,"No"]
[null,"06-12-2017","10:07","NMI-25000801238","Urban","Network Business","Network Error",1,52.17,1.6249999999999999E-3,3.1000000000000001E-5,"No"]
[null,"06-12-2017","13:26","DT-0437","Rural Short","Planned",null,6,104,null,null,"No"]
[null,"06-12-2017","19:52","DT-1234","Urban","Asset Failure","LV",1,51.83,1.6149999999999999E-3,3.1000000000000001E-5,"No"]
[null,"07-12-2017","09:00","22MT06 LAKE BENNETT","Rural Short","Planned",null,229,289.62,null,null,"No"]
[null,"07-12-2017","09:28","22TC07 THREE WAYS","Rural Short","Unknown","Unknown",564,15.12,0.18900900000000001,1.2503E-2,"No"]
[null,"07-12-2017","09:41","DT-7087","Rural Short","Overloads",null,2,10.75,4.7699999999999999E-4,4.3999999999999999E-5,"No"]
[null,"07-12-2017","13:23","DT-2418","Rural Short","Asset Failure","LV",1,91.23,2.0230000000000001E-3,2.1999999999999999E-5,"No"]
[null,"08-12-2017","03:34","DT-6465","Rural Short","Unknown","Unknown",2,133.68,5.927E-3,4.3999999999999999E-5,"No"]
[null,"08-12-2017","09:18","DT-1905","Rural Short","Planned",null,94,247,null,null,"No"]
[null,"08-12-2017","10:23","DT-10491","Rural Long","Planned",null,2,114.27,null,null,"No"]
[null,"08-12-2017","21:07","NMI-25010190459","Rural Short","Asset Failure","LV",1,107.5,2.3830000000000001E-3,2.1999999999999999E-5,"No"]
[null,"09-12-2017","07:48","NMI-25000755879","Rural Short","Asset Failure","LV",1,72.67,1.611E-3,2.1999999999999999E-5,"No"]
[null,"09-12-2017","08:30","22MT06 LAKE BENNETT","Rural Short","Planned",null,5,241.17,null,null,"No"]
[null,"09-12-2017","18:06","DT-2662","Rural Short","Overloads",null,1,73.12,1.621E-3,2.1999999999999999E-5,"No"]
[null,"10-12-2017","05:53","DT-0787","Rural Short","Third Party","Other",19,214.05,9.0160000000000004E-2,4.2099999999999999E-4,"No"]
[null,"10-12-2017","06:00","DT-2112","Rural Short","Planned",null,9,329.57,null,null,"No"]
[null,"10-12-2017","08:30","DT-1594","Rural Short","Planned",null,6,227.3,null,null,"No"]
[null,"10-12-2017","08:42","11FB08 FRANCIS BAY","Urban","Planned",null,21,18.170000000000002,null,null,"No"]
[null,"10-12-2017","11:00","NMI-25000809149","Urban","Asset Failure","LV",1,35.68,1.1119999999999999E-3,3.1000000000000001E-5,"No"]
[null,"10-12-2017","17:07","DT-2560","Urban","Asset Failure","LV",1,95.27,2.9680000000000002E-3,3.1000000000000001E-5,"No"]
[null,"10-12-2017","18:58","DT-2613","Urban","Overloads",null,89,274.23,0.76035900000000001,2.7729999999999999E-3,"No"]
[null,"10-12-2017","21:41","NMI-25000572952","Rural Short","Overloads",null,1,42.87,9.5E-4,2.1999999999999999E-5,"No"]
[null,"11-12-2017","07:17","11BE18 PORT","Rural Short","Asset Failure","HV",7,12.4,1.9239999999999999E-3,1.55E-4,"No"]
[null,"11-12-2017","07:25","NMI-25000481584","Rural Short","Asset Failure","LV",1,274.48,6.0850000000000001E-3,2.1999999999999999E-5,"No"]
[null,"11-12-2017","09:24","NMI-25010142509","Urban","Third Party","Other",1,67.33,2.098E-3,3.1000000000000001E-5,"No"]
[null,"11-12-2017","10:00","DT-2057","Rural Short","Planned",null,1,112.27,null,null,"No"]
[null,"11-12-2017","10:29","DT-6860","Rural Short","Animal","Animal Impact",2,65.02,2.8830000000000001E-3,4.3999999999999999E-5,"No"]
[null,"11-12-2017","11:04","NMI-25000700448","Urban","Third Party","Other",1,131.65,4.1009999999999996E-3,3.1000000000000001E-5,"No"]
[null,"11-12-2017","17:16","NMI-25000806442","Rural Short","Weather",null,1,225.03,4.9890000000000004E-3,2.1999999999999999E-5,"No"]
[null,"11-12-2017","21:38","DT-1479","Rural Short","Network Business","Network Error",1,298.3,6.613E-3,2.1999999999999999E-5,"No"]
[null,"12-12-2017","08:33","11WN11 BISHOP","Urban","Planned",null,107,260.25,null,null,"No"]
[null,"12-12-2017","09:00","DT-1235","Urban","Planned",null,66,383.75,null,null,"No"]
[null,"12-12-2017","10:40","DT-0840","Rural Short","Weather",null,1,150.72999999999999,3.3419999999999999E-3,2.1999999999999999E-5,"No"]
[null,"12-12-2017","14:17","11RG02 GOLF","Urban","Asset Failure","HV",890,83.5,2.3151809999999999,2.7727000000000002E-2,"No"]
[null,"12-12-2017","14:58","22SY11 HERBERT","Rural Short","Weather",null,1774,17.149999999999999,0.67447199999999996,3.9328000000000002E-2,"No"]
[null,"12-12-2017","15:22","GCR-0013","Rural Short","Weather",null,158,188.03,0.65862500000000002,3.503E-3,"No"]
[null,"12-12-2017","15:59","NMI-25000630050","Urban","Asset Failure","LV",1,213.63,6.6550000000000003E-3,3.1000000000000001E-5,"No"]
[null,"12-12-2017","16:15","NMI-25000694815","Urban","Asset Failure","LV",1,91.85,2.8609999999999998E-3,3.1000000000000001E-5,"No"]
[null,"12-12-2017","16:26","DT-0638","Rural Short","Weather",null,1,157.35,3.4880000000000002E-3,2.1999999999999999E-5,"No"]
[null,"12-12-2017","17:49","DT-8041","Rural Short","Unknown","Unknown",57,66.67,8.4241999999999997E-2,1.2639999999999999E-3,"No"]
[null,"12-12-2017","20:32","FH-6411","Rural Short","Unknown","Unknown",12,82.78,2.2023000000000001E-2,2.6600000000000001E-4,"No"]
[null,"12-12-2017","20:49","22SY11 HERBERT","Rural Short","Weather",null,1774,58.95,2.3183760000000002,3.9328000000000002E-2,"No"]
[null,"12-12-2017","21:25","FH-6303","Rural Short","Weather",null,0,75.819999999999993,0,0,"No"]
[null,"12-12-2017","23:45","NMI-25000403629","Urban","Third Party","Other",1,85.47,2.663E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","09:05","DT-1185","Rural Short","Planned",null,5,227,null,null,"No"]
[null,"13-12-2017","10:37","NMI-25000735897","Urban","Third Party","Other",1,190.05,5.921E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","10:37","NMI-25000528807","Urban","Third Party","Other",1,186.75,5.8180000000000003E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","10:40","NMI-25000767576","Urban","Third Party","Other",1,188.93,5.8859999999999997E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","11:02","NMI-25000620828","Urban","Third Party","Vehicle impact",1,168.37,5.2449999999999997E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","11:42","NMI-25000432867","Rural Long","Asset Failure","LV",1,159.25,0.183257,1.1509999999999999E-3,"No"]
[null,"13-12-2017","16:02","REC-10027","Rural Short","Weather",null,175,14.93,5.7935E-2,3.8800000000000002E-3,"No"]
[null,"13-12-2017","17:48","FH-6504","Rural Short","Weather",null,12,93.58,2.4896000000000001E-2,2.6600000000000001E-4,"No"]
[null,"13-12-2017","19:09","NMI-25000112067","Rural Short","Asset Failure","LV",1,164.17,3.6389999999999999E-3,2.1999999999999999E-5,"No"]
[null,"13-12-2017","20:03","NMI-25000170710","Urban","Asset Failure","LV",1,81.22,2.5300000000000001E-3,3.1000000000000001E-5,"No"]
[null,"13-12-2017","21:48","FH-6186","Rural Short","Unknown","Unknown",1,80.03,1.774E-3,2.1999999999999999E-5,"No"]
[null,"13-12-2017","22:02","22KA22 KATHERINE","Urban","Weather",null,1469,14.85,0.67960500000000001,4.5765E-2,"No"]
[null,"14-12-2017","05:13","NMI-25000420039","Rural Short","Unknown","Unknown",1,65.92,1.4610000000000001E-3,2.1999999999999999E-5,"No"]
[null,"14-12-2017","09:00","22SY12 NOONAMAH","Rural Short","Planned",null,39,263.18,null,null,"No"]
[null,"14-12-2017","09:24","NMI-25000706917","Urban","Asset Failure","LV",1,75.599999999999994,2.3549999999999999E-3,3.1000000000000001E-5,"No"]
[null,"14-12-2017","10:40","DT-2119","Urban","Asset Failure","LV",45,15,2.1028999999999999E-2,1.402E-3,"No"]
[null,"14-12-2017","19:37","DT-2845","Rural Short","Asset Failure","HV",77,94.73,0.16171099999999999,1.707E-3,"No"]
[null,"14-12-2017","21:07","NMI-25000448391","Urban","Overloads",null,1,127.42,3.9690000000000003E-3,3.1000000000000001E-5,"No"]
[null,"15-12-2017","05:36","CB22TL05","Rural Short","Weather",null,0,1.1200000000000001,0,0,"No"]
[null,"15-12-2017","09:16","DT-8038","Rural Short","Planned",null,153,113.3,null,null,"No"]
[null,"15-12-2017","14:23","NMI-25000607675","Urban","Asset Failure","LV",1,41.18,1.2830000000000001E-3,3.1000000000000001E-5,"No"]
[null,"15-12-2017","14:34","DT-1109","Rural Short","Third Party","Vehicle impact",1,118.12,2.6189999999999998E-3,2.1999999999999999E-5,"No"]
[null,"16-12-2017","02:38","11CA19 CAS VILLAGE","Rural Short","Asset Failure","HV",825,42.27,0.773034,1.8289E-2,"No"]
[null,"16-12-2017","10:19","GCR-4440","Urban","Unknown","Unknown",893,20.149999999999999,0.56057699999999999,2.7820000000000001E-2,"No"]
[null,"16-12-2017","11:22","NMI-25000699739","Rural Short","Network Business","Network Error",1,105.08,2.33E-3,2.1999999999999999E-5,"No"]
[null,"16-12-2017","13:50","NMI-25000760657","Rural Short","Asset Failure","LV",1,407.93,9.0430000000000007E-3,2.1999999999999999E-5,"No"]
[null,"16-12-2017","13:53","DT-1248","Rural Short","Asset Failure","LV",96,402.78,0.85721400000000003,2.1280000000000001E-3,"No"]
[null,"16-12-2017","15:27","SEC-GCR0111","Rural Short","Weather",null,259,566.1,3.2504189999999999,5.7419999999999997E-3,"No"]
[null,"17-12-2017","00:04","NMI-25000120333","Rural Short","Asset Failure","LV",1,201.48,4.4669999999999996E-3,2.1999999999999999E-5,"No"]
[null,"17-12-2017","00:51","SEC-GCR0111","Rural Short","Network Business","Network Error",259,1.88,1.0814000000000001E-2,5.7419999999999997E-3,"No"]
[null,"17-12-2017","06:42","NMI-25000514106","Rural Short","Overloads",null,1,75.680000000000007,1.678E-3,2.1999999999999999E-5,"No"]
[null,"17-12-2017","06:57","DT-6119","Rural Short","Unknown","Unknown",1,59.25,1.3140000000000001E-3,2.1999999999999999E-5,"No"]
[null,"17-12-2017","07:15","SWH-6637","Rural Short","Network Business","Network Error",18,16.78,6.6969999999999998E-3,3.9899999999999999E-4,"No"]
[null,"17-12-2017","08:49","DT-2187","Urban","Planned",null,9,137.08000000000001,null,null,"No"]
[null,"17-12-2017","08:55","DT-3064","Urban","Planned",null,8,191.3,null,null,"No"]
[null,"17-12-2017","09:23","DT-6860","Rural Short","Unknown","Unknown",1,103.07,2.2850000000000001E-3,2.1999999999999999E-5,"No"]
[null,"17-12-2017","12:14","SWH-1166","Rural Short","Network Business","Network Error",25,2.12,1.173E-3,5.5400000000000002E-4,"No"]
[null,"17-12-2017","13:14","SWH-0337","Rural Short","Network Business","Network Error",44,6.1,5.9500000000000004E-3,9.7499999999999996E-4,"No"]
[null,"18-12-2017","06:26","22KA10 MATARANKA 1","Rural Long","Animal","Animal Impact",234,60.78,16.367433999999999,0.26927499999999999,"No"]
[null,"18-12-2017","06:28","DT-1505","Rural Short","Asset Failure","HV",1,92.58,2.052E-3,2.1999999999999999E-5,"No"]
[null,"18-12-2017","11:30","SWH-7517","Rural Long","Network Business","Network Error",10,43.17,0.49674000000000001,1.1507E-2,"No"]
[null,"18-12-2017","15:03","NMI-25000881314","Rural Short","Asset Failure","LV",1,585.67999999999995,1.2984000000000001E-2,2.1999999999999999E-5,"No"]
[null,"18-12-2017","18:16","22BR103 BR-SD 2","Rural Short","Weather",null,198,26.18,0.11493100000000001,4.3889999999999997E-3,"No"]
[null,"18-12-2017","18:21","NMI-25010243610","Rural Short","Overloads",null,1,211.63,4.692E-3,2.1999999999999999E-5,"No"]
[null,"19-12-2017","08:37","DT-8644","Rural Short","Planned",null,2,54.02,null,null,"No"]
[null,"19-12-2017","08:44","DT-0052","Rural Short","Planned",null,1,204.17,null,null,"No"]
[null,"19-12-2017","08:49","DT-6031","Urban","Planned",null,35,96.03,null,null,"No"]
[null,"19-12-2017","09:08","22SY03 VIRGINIA","Rural Short","Planned",null,100,169.88,null,null,"No"]
[null,"19-12-2017","09:48","DT-2018","Urban","Planned",null,57,210.65,null,null,"No"]
[null,"19-12-2017","13:50","REC-10015","Rural Short","Unknown","Unknown",0,14.18,0,0,"No"]
[null,"19-12-2017","14:27","REC-10015","Rural Short","Weather",null,0,94.18,0,0,"No"]
[null,"19-12-2017","17:49","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",198,11.75,5.1575999999999997E-2,4.3889999999999997E-3,"No"]
[null,"19-12-2017","18:09","REC-10015","Rural Short","Weather",null,0,10.33,0,0,"No"]
[null,"19-12-2017","19:49","NMI-25000843016","Rural Short","Overloads",null,1,124.02,2.7490000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-12-2017","01:40","REC-10049","Rural Long","Unknown","Unknown",39,16.13,0.724051,4.4879000000000002E-2,"No"]
[null,"20-12-2017","09:00","22SY15 DARWIN RIVER","Rural Short","Planned",null,32,92.78,null,null,"No"]
[null,"20-12-2017","12:41","DT-6205","Rural Short","Asset Failure","HV",9,7.2,1.4369999999999999E-3,2.0000000000000001E-4,"No"]
[null,"20-12-2017","15:24","SEC-22EV0134","Rural Short","Weather",null,107,322.67,0.76539299999999999,2.372E-3,"No"]
[null,"20-12-2017","15:36","DT-6442","Rural Long","Weather",null,1,417.07,0.479939,1.1509999999999999E-3,"No"]
[null,"20-12-2017","17:33","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",198,21.98,9.6494999999999997E-2,4.3889999999999997E-3,"No"]
[null,"20-12-2017","18:45","NMI-25000601366","Rural Short","Asset Failure","LV",1,35.28,7.8200000000000003E-4,2.1999999999999999E-5,"No"]
[null,"21-12-2017","00:00","DT-1482","Urban","Asset Failure","HV",1,31.2,9.7199999999999999E-4,3.1000000000000001E-5,"No"]
[null,"21-12-2017","00:00","DT-1478","Urban","Planned",null,2,179.6,null,null,"No"]
[null,"21-12-2017","01:17","DT-3289","Urban","Planned",null,18,25,null,null,"No"]
[null,"21-12-2017","11:55","NMI-25000137947","Rural Short","Weather",null,1,91.15,2.0209999999999998E-3,2.1999999999999999E-5,"No"]
[null,"21-12-2017","12:19","NMI-25000430137","Rural Short","Third Party","Other",1,99.62,2.2079999999999999E-3,2.1999999999999999E-5,"No"]
[null,"21-12-2017","13:39","DT-1706","Rural Short","Network Business","Network Error",9,4.8,9.5799999999999998E-4,2.0000000000000001E-4,"No"]
[null,"21-12-2017","22:29","REC-10033","Rural Short","Asset Failure","HV",1,106.13,2.3530000000000001E-3,2.1999999999999999E-5,"No"]
[null,"22-12-2017","11:44","DT-2116","Rural Short","Network Business","Network Error",1,8.2799999999999994,1.84E-4,2.1999999999999999E-5,"No"]
[null,"22-12-2017","13:00","DT-8155","Rural Short","Unknown","Unknown",13,78.099999999999994,2.2508E-2,2.8800000000000001E-4,"No"]
[null,"22-12-2017","14:09","22HD403 MIDDLE POINT","Rural Short","Unknown","Unknown",27,15.57,9.3179999999999999E-3,5.9900000000000003E-4,"No"]
[null,"22-12-2017","14:30","22HD403 MIDDLE POINT","Rural Short","Asset Failure","HV",27,168.93,0.101117,5.9900000000000003E-4,"No"]
[null,"22-12-2017","16:42","DT-6809","Rural Short","Network Business","Network Error",1,16.2,3.59E-4,2.1999999999999999E-5,"No"]
[null,"23-12-2017","04:03","FH-6260","Rural Long","Weather",null,15,109.08,1.882911,1.7260999999999999E-2,"No"]
[null,"23-12-2017","06:49","DT-8415","Rural Short","Animal","Animal Impact",3,75.63,5.0299999999999997E-3,6.7000000000000002E-5,"No"]
[null,"23-12-2017","07:46","DT-6116","Rural Long","Unknown","Unknown",1,70.180000000000007,8.0763000000000001E-2,1.1509999999999999E-3,"No"]
[null,"23-12-2017","11:13","NMI-25010229336","Urban","Third Party","Other",1,31.53,9.8200000000000002E-4,3.1000000000000001E-5,"No"]
[null,"23-12-2017","15:38","NMI-25000662992","Urban","Asset Failure","LV",1,331.7,1.0333999999999999E-2,3.1000000000000001E-5,"No"]
[null,"23-12-2017","16:18","DT-2427","Rural Short","Network Business","Network Error",72,11.93,1.9047999999999999E-2,1.596E-3,"No"]
[null,"23-12-2017","18:02","SEC-0279","Rural Short","Weather",null,217,49.43,0.23780799999999999,4.8110000000000002E-3,"No"]
[null,"24-12-2017","01:10","22KA06 TINDAL 2","Rural Short","Unknown","Unknown",245,10.17,5.5218999999999997E-2,5.4310000000000001E-3,"No"]
[null,"25-12-2017","06:34","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",198,26.23,0.11515,4.3889999999999997E-3,"No"]
[null,"25-12-2017","09:26","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,919,45,0.91679999999999995,2.0372999999999999E-2,"No"]
[null,"26-12-2017","00:56","22KA10 MATARANKA 1","Rural Long","Unknown","Unknown",234,14.95,4.0256619999999996,0.26927499999999999,"No"]
[null,"26-12-2017","22:33","DT-6666","Rural Short","Asset Failure","LV",1,123.73,2.7430000000000002E-3,2.1999999999999999E-5,"No"]
[null,"27-12-2017","05:35","66 MR-SY","Rural Short","Weather",null,5,15.23,1.689E-3,1.11E-4,"No"]
[null,"27-12-2017","16:03","NMI-25000553904","Urban","Asset Failure","LV",1,79.8,2.4859999999999999E-3,3.1000000000000001E-5,"No"]
[null,"27-12-2017","17:56","22TC07 THREE WAYS","Rural Short","Weather",null,564,15.65,0.19567699999999999,1.2503E-2,"No"]
[null,"27-12-2017","21:51","NMI-25000357668","Rural Short","Asset Failure","LV",1,121.35,2.6900000000000001E-3,2.1999999999999999E-5,"No"]
[null,"28-12-2017","07:43","DT-6764","Rural Short","Weather",null,2,47.9,2.124E-3,4.3999999999999999E-5,"No"]
[null,"28-12-2017","19:32","22KA22 KATHERINE","Urban","Unknown","Unknown",1469,15.35,0.702488,4.5765E-2,"No"]
[null,"28-12-2017","19:48","REC-10049","Rural Long","Weather",null,39,15.7,0.70460299999999998,4.4879000000000002E-2,"No"]
[null,"28-12-2017","21:33","REC-10049","Rural Long","Unknown","Unknown",39,15.67,0.70310700000000004,4.4879000000000002E-2,"No"]
[null,"28-12-2017","21:49","REC-10049","Rural Long","7 - STPIS Exclusion (3.3)(a)",null,39,17.68,null,null,"No"]
[null,"29-12-2017","11:30","DT-6309","Rural Short","Weather",null,1,114.67,2.542E-3,2.1999999999999999E-5,"No"]
[null,"29-12-2017","14:40","DT-6764","Rural Short","Unknown","Unknown",1,102.53,2.2729999999999998E-3,2.1999999999999999E-5,"No"]
[null,"29-12-2017","18:13","NMI-25000729049","Rural Short","Asset Failure","LV",1,136.91999999999999,3.0349999999999999E-3,2.1999999999999999E-5,"No"]
[null,"29-12-2017","19:04","NMI-25000116331","Rural Short","Weather",null,1,286.77,6.3569999999999998E-3,2.1999999999999999E-5,"No"]
[null,"30-12-2017","07:29","NMI-25000401278","Rural Short","Third Party","Other",1,127.73,2.8319999999999999E-3,2.1999999999999999E-5,"No"]
[null,"30-12-2017","13:56","REC-10015","Rural Short","Weather",null,0,15.45,0,0,"No"]
[null,"30-12-2017","17:49","22BA01 MINE","Rural Short","Weather",null,1,16.12,3.57E-4,2.1999999999999999E-5,"No"]
[null,"31-12-2017","00:06","NMI-25000604375","Rural Short","Asset Failure","LV",0,173.48,0,0,"No"]
[null,"31-12-2017","17:37","NMI-25000330022","Urban","Asset Failure","LV",1,64.099999999999994,1.9970000000000001E-3,3.1000000000000001E-5,"No"]
[null,"31-12-2017","18:14","NMI-25000803687","Urban","Weather",null,1,65.33,2.0349999999999999E-3,3.1000000000000001E-5,"No"]
[null,"01-01-2018","09:56","NMI-25000121596","Urban","Asset Failure","LV",1,45.1,1.405E-3,3.1000000000000001E-5,"No"]
[null,"01-01-2018","10:39","REC-10015","Rural Short","Weather",null,0,15.93,0,0,"No"]
[null,"01-01-2018","15:55","22SY12 NOONAMAH","Rural Short","Weather",null,908,111.47,2.2437649999999998,2.0129000000000001E-2,"No"]
[null,"01-01-2018","16:03","22SY15 DARWIN RIVER","Rural Short","Weather",null,817,124.75,2.2594829999999999,1.8112E-2,"No"]
[null,"01-01-2018","16:15","22SY04 DUNDEE","Rural Long","Weather",null,633,15.33,11.16916,0.72842300000000004,"No"]
[null,"01-01-2018","17:23","DT-1248","Rural Short","Asset Failure","HV",96,487.7,1.037936,2.1280000000000001E-3,"No"]
[null,"01-01-2018","17:34","SWH-1124","Urban","Asset Failure","HV",1373,278.77999999999997,11.924655,4.2774E-2,"No"]
[null,"01-01-2018","17:46","DT-10479","Rural Short","Weather",null,3,80.599999999999994,5.3600000000000002E-3,6.7000000000000002E-5,"No"]
[null,"01-01-2018","19:30","11CA23 MOIL","Rural Short","Network Business","Network Error",895,1.35,2.6786000000000001E-2,1.9841000000000001E-2,"No"]
[null,"01-01-2018","19:36","DT-1242","Urban","Asset Failure","HV",90,78.7,0.220661,2.8040000000000001E-3,"No"]
[null,"01-01-2018","20:51","NMI-25000666473","Rural Short","Asset Failure","LV",1,335.93,7.4469999999999996E-3,2.1999999999999999E-5,"No"]
[null,"02-01-2018","02:59","DT-6467","Rural Long","Weather",null,1,426.55,0.49085200000000001,1.1509999999999999E-3,"No"]
[null,"02-01-2018","09:30","DT-0102","Rural Short","Planned",null,20,98.15,null,null,"No"]
[null,"02-01-2018","10:02","DT-0226","Rural Short","Weather",null,3,190.17,1.2647E-2,6.7000000000000002E-5,"No"]
[null,"02-01-2018","10:52","DT-0194-1","Rural Short","Asset Failure","HV",5,133.28,1.4774000000000001E-2,1.11E-4,"No"]
[null,"02-01-2018","22:57","REC-10029","Rural Long","Weather",null,39,17.23,0.77341800000000005,4.4879000000000002E-2,"No"]
[null,"03-01-2018","09:00","11BE04 MCMILLANS","Rural Short","Planned",null,14,194.15,null,null,"No"]
[null,"03-01-2018","09:00","DT-0498","Rural Short","Planned",null,21,118.13,null,null,"No"]
[null,"03-01-2018","09:14","DT-0610","Rural Short","Planned",null,7,150.65,null,null,"No"]
[null,"03-01-2018","09:30","SWH-6087","Rural Long","Asset Failure","HV",39,1.33,5.9839000000000003E-2,4.4879000000000002E-2,"No"]
[null,"03-01-2018","19:50","22SY12 NOONAMAH","Rural Short","Asset Failure","HV",908,9.58,0.192907,2.0129000000000001E-2,"No"]
[null,"04-01-2018","09:10","22SY02 MCMINNS","Rural Short","Planned",null,128,269.45,null,null,"No"]
[null,"04-01-2018","09:20","DT-0849","Rural Short","Planned",null,1,85.2,null,null,"No"]
[null,"04-01-2018","11:28","PSPT104567","Urban","7 - STPIS Exclusion (3.3)(a)",null,114,11.55,null,null,"No"]
[null,"04-01-2018","14:20","22KA03 FLORINA","Rural Short","Asset Failure","Subtransmission",266,41.52,0.24482200000000001,5.8970000000000003E-3,"No"]
[null,"04-01-2018","14:20","22KA06 TINDAL 2","Rural Short","Asset Failure","Subtransmission",245,46.05,0.250116,5.4310000000000001E-3,"No"]
[null,"04-01-2018","14:20","22KA07 KATH EAST","Rural Short","Asset Failure","Subtransmission",1333,37.799999999999997,1.1170389999999999,2.9551000000000001E-2,"No"]
[null,"04-01-2018","14:20","22KA09 PINE CREEK","Rural Short","Asset Failure","Subtransmission",126,42.95,0.119972,2.7929999999999999E-3,"No"]
[null,"04-01-2018","14:20","22KA10 MATARANKA 1","Rural Long","Asset Failure","Subtransmission",303,28.17,9.821059,0.34867700000000001,"No"]
[null,"04-01-2018","14:20","22KA15 OPS","Rural Short","Asset Failure","Subtransmission",392,97.33,0.84585100000000002,8.6899999999999998E-3,"No"]
[null,"04-01-2018","14:20","22KA18 GORGE","Rural Short","Asset Failure","Subtransmission",234,45.43,0.23568800000000001,5.1879999999999999E-3,"No"]
[null,"04-01-2018","14:20","22KA19 TINDAL 1","Rural Short","Asset Failure","Subtransmission",245,46.7,0.25364700000000001,5.4310000000000001E-3,"No"]
[null,"04-01-2018","14:20","22KA22 KATHERINE","Urban","Asset Failure","Subtransmission",1638,36.270000000000003,1.8506739999999999,5.1029999999999999E-2,"No"]
[null,"04-01-2018","14:20","66PC301 COSMO HOWLEY","Rural Short","Asset Failure","Subtransmission",4,258.25,2.2901000000000001E-2,8.8999999999999995E-5,"No"]
[null,"04-01-2018","15:34","NMI-25010248865","Rural Short","Network Business","Network Error",1,54.63,1.2110000000000001E-3,2.1999999999999999E-5,"No"]
[null,"04-01-2018","17:44","DT-0657","Rural Short","Weather",null,2,135.32,6.0000000000000001E-3,4.3999999999999999E-5,"No"]
[null,"04-01-2018","18:19","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,949,16.38,0.34467900000000001,2.1038000000000001E-2,"No"]
[null,"04-01-2018","19:12","NMI-25000419766","Urban","Asset Failure","LV",1,340.77,1.0616E-2,3.1000000000000001E-5,"No"]
[null,"04-01-2018","20:11","DT-6741","Rural Short","Unknown","Unknown",1,14.2,3.1500000000000001E-4,2.1999999999999999E-5,"No"]
[null,"04-01-2018","21:51","NMI-25000499279","Rural Short","Asset Failure","LV",1,69.98,1.5510000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-01-2018","16:40","132 MT-BA-PK","N/A","Network Business","Network Error",0,1.1000000000000001,null,null,"No"]
[null,"05-01-2018","16:40","22PC308 TOWNSHIP","Rural Short","Asset Failure","Subtransmission",233,212,1.0950610000000001,5.1650000000000003E-3,"No"]
[null,"05-01-2018","16:40","66PC301 COSMO HOWLEY","Rural Short","Asset Failure","Subtransmission",4,212,1.8799E-2,8.8999999999999995E-5,"No"]
[null,"05-01-2018","17:17","22HD403 MIDDLE POINT","Rural Short","Weather",null,42,56.65,5.2747000000000002E-2,9.3099999999999997E-4,"No"]
[null,"05-01-2018","17:35","11BE14 ROBERTSON","Urban","Vegetation","Grow-in NSP Responsibility",4,38.479999999999997,4.7959999999999999E-3,1.25E-4,"No"]
[null,"05-01-2018","19:30","DT-0145","Rural Short","Weather",null,3,370.3,2.4628000000000001E-2,6.7000000000000002E-5,"No"]
[null,"05-01-2018","19:54","DT-10035","Rural Short","Weather",null,2,288.12,1.2775E-2,4.3999999999999999E-5,"No"]
[null,"06-01-2018","05:28","22SY02 MCMINNS","Rural Short","Unknown","Unknown",1238,16.47,0.451932,2.7445000000000001E-2,"No"]
[null,"06-01-2018","06:52","DT-0055","Rural Short","Asset Failure","LV",28,85.55,5.3103999999999998E-2,6.2100000000000002E-4,"No"]
[null,"06-01-2018","07:19","NMI-25010247890","Rural Short","Asset Failure","LV",1,108.83,2.4130000000000002E-3,2.1999999999999999E-5,"No"]
[null,"06-01-2018","08:11","NMI-25000876535","Rural Long","Asset Failure","LV",1,199.17,0.22919100000000001,1.1509999999999999E-3,"No"]
[null,"06-01-2018","10:51","DT-6348","Rural Short","Unknown","Unknown",0,392.7,0,0,"No"]
[null,"06-01-2018","10:53","NMI-25000603097","Urban","Asset Failure","LV",1,25.02,7.7899999999999996E-4,3.1000000000000001E-5,"No"]
[null,"06-01-2018","11:21","DT-10030","Rural Short","Overloads",null,1,214.85,4.7629999999999999E-3,2.1999999999999999E-5,"No"]
[null,"06-01-2018","14:11","NMI-25000179404","Rural Short","Asset Failure","LV",1,99.17,2.1979999999999999E-3,2.1999999999999999E-5,"No"]
[null,"06-01-2018","16:49","DT-10029","Rural Long","Asset Failure","HV",1,317.25,0.36507499999999998,1.1509999999999999E-3,"No"]
[null,"07-01-2018","08:16","DT-1317","Rural Short","Planned",null,3,114.2,null,null,"No"]
[null,"07-01-2018","08:53","DT-6463","Rural Short","Weather",null,1,275.37,6.1050000000000002E-3,2.1999999999999999E-5,"No"]
[null,"07-01-2018","12:20","NMI-25000383913","Urban","Asset Failure","LV",1,120.43,3.7520000000000001E-3,3.1000000000000001E-5,"No"]
[null,"07-01-2018","22:33","DT-1418","CBD","Planned",null,2,249.27,null,null,"No"]
[null,"07-01-2018","23:05","DT-6050","Urban","Planned",null,47,237,null,null,"No"]
[null,"08-01-2018","01:05","66 MR-SY","Rural Short","Unknown","Unknown",418,11.55,0.10703,9.2669999999999992E-3,"No"]
[null,"08-01-2018","02:33","DT-0339","Rural Short","Animal","Animal Impact",19,163.80000000000001,6.8994E-2,4.2099999999999999E-4,"No"]
[null,"08-01-2018","08:36","PSPT119809","Urban","Asset Failure","LV",3,73.38,6.8580000000000004E-3,9.2999999999999997E-5,"No"]
[null,"08-01-2018","09:15","NMI-25000387962","Rural Short","Asset Failure","LV",1,159.1,3.5270000000000002E-3,2.1999999999999999E-5,"No"]
[null,"08-01-2018","10:05","DT-6741","Rural Short","Weather",null,1,219.5,4.8659999999999997E-3,2.1999999999999999E-5,"No"]
[null,"08-01-2018","12:25","11AR05 BELLAMACK 1","Urban","3 - STPIS Exclusion (3.3)(a)",null,1151,52.58,null,null,"No"]
[null,"08-01-2018","12:25","11AR13 BONSON","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1444,53.02,null,null,"No"]
[null,"08-01-2018","12:25","11AR18 BELLAMACK 2","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,981,54.5,null,null,"No"]
[null,"08-01-2018","12:25","11BE01 LEANYER","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,11,37.380000000000003,null,null,"No"]
[null,"08-01-2018","12:25","11BE04 MCMILLANS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,433,38.85,null,null,"No"]
[null,"08-01-2018","12:25","11BE07 NAVY","Urban","3 - STPIS Exclusion (3.3)(a)",null,3,31.12,null,null,"No"]
[null,"08-01-2018","12:25","11BE13 KORMILDA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,360,29.73,null,null,"No"]
[null,"08-01-2018","12:25","11BE14 ROBERTSON","Urban","3 - STPIS Exclusion (3.3)(a)",null,4,62.4,null,null,"No"]
[null,"08-01-2018","12:25","11BE16 ANULA","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1021,34.53,null,null,"No"]
[null,"08-01-2018","12:25","11BE19 HIDDEN VALLEY","Urban","3 - STPIS Exclusion (3.3)(a)",null,383,30.92,null,null,"No"]
[null,"08-01-2018","12:25","11DA19 GARDENS","Urban","3 - STPIS Exclusion (3.3)(a)",null,875,41.18,null,null,"No"]
[null,"08-01-2018","12:25","11DA27 STUART PARK","Urban","3 - STPIS Exclusion (3.3)(a)",null,1399,42.78,null,null,"No"]
[null,"08-01-2018","12:25","11LE13 ROSEWOOD","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,952,58.58,null,null,"No"]
[null,"08-01-2018","12:25","11PA04 BAKEWELL","Urban","3 - STPIS Exclusion (3.3)(a)",null,2354,47.22,null,null,"No"]
[null,"08-01-2018","12:25","11PA15 MOULDEN","Urban","3 - STPIS Exclusion (3.3)(a)",null,1672,46.22,null,null,"No"]
[null,"08-01-2018","14:53","NMI-25000170149","Rural Short","Asset Failure","LV",1,423.38,9.3860000000000002E-3,2.1999999999999999E-5,"No"]
[null,"08-01-2018","16:17","DT-0525","Rural Short","Weather",null,2,153.53,6.8069999999999997E-3,4.3999999999999999E-5,"No"]
[null,"09-01-2018","08:30","DT-1444","Rural Short","Planned",null,65,302.39999999999998,null,null,"No"]
[null,"09-01-2018","09:09","DT-0938","Rural Short","Planned",null,8,209.75,null,null,"No"]
[null,"09-01-2018","11:10","NMI-25000592934","Rural Short","Network Business","Switching and Protection Error",1,87.03,1.9289999999999999E-3,2.1999999999999999E-5,"No"]
[null,"09-01-2018","17:55","REC-10015","Rural Short","Unknown","Unknown",0,104.73,0,0,"No"]
[null,"09-01-2018","20:20","REC-10029","Rural Long","Weather",null,39,16.13,0.724051,4.4879000000000002E-2,"No"]
[null,"09-01-2018","20:43","NMI-25000131744","Rural Short","Asset Failure","LV",1,104.68,2.3210000000000001E-3,2.1999999999999999E-5,"No"]
[null,"10-01-2018","08:28","22RG13 BREWER 1","Rural Short","Unknown","Unknown",493,17.77,0.19417799999999999,1.0928999999999999E-2,"No"]
[null,"10-01-2018","08:30","DT-2207","Urban","Planned",null,3,182.07,null,null,"No"]
[null,"10-01-2018","08:40","DT-6110","Rural Short","Planned",null,1,77.5,null,null,"No"]
[null,"10-01-2018","13:55","DT-1248","Rural Short","Network Business","Network Error",96,24.62,5.2389999999999999E-2,2.1280000000000001E-3,"No"]
[null,"10-01-2018","16:10","NMI-25000803687","Urban","Network Business","Network Error",1,35.270000000000003,1.0989999999999999E-3,3.1000000000000001E-5,"No"]
[null,"11-01-2018","04:15","REC-10032","Rural Long","Unknown","Unknown",207,16.2,3.8589180000000001,0.238205,"No"]
[null,"11-01-2018","09:00","22SY11 HERBERT","Rural Short","Planned",null,23,160.88,null,null,"No"]
[null,"11-01-2018","10:02","DT-1350","Urban","Planned",null,126,156.91999999999999,null,null,"No"]
[null,"11-01-2018","12:51","DT-2505","Rural Short","Overloads",null,38,336.6,0.28355900000000001,8.4199999999999998E-4,"No"]
[null,"11-01-2018","15:18","DT-8288","Urban","Third Party","Vehicle impact",35,17.12,1.8664E-2,1.09E-3,"No"]
[null,"11-01-2018","20:46","22RG10 LOVEGROVE 1","Urban","Weather",null,0,20.149999999999999,0,0,"No"]
[null,"11-01-2018","21:20","22LG29 JINDALEE","Rural Short","Weather",null,7,280.27,4.3492999999999997E-2,1.55E-4,"No"]
[null,"11-01-2018","22:04","DT-1283","Rural Short","Network Business","Network Error",6,64.2,8.5400000000000007E-3,1.3300000000000001E-4,"No"]
[null,"12-01-2018","02:39","SWH-18069","Rural Short","Asset Failure","HV",8,3.35,5.9400000000000002E-4,1.7699999999999999E-4,"No"]
[null,"12-01-2018","10:04","NMI-25000639594","CBD","Asset Failure","LV",1,81.87,2.2006999999999999E-2,2.6899999999999998E-4,"No"]
[null,"12-01-2018","15:33","11RG02 GOLF","Urban","Weather",null,940,15,0.43926599999999999,2.9284000000000001E-2,"No"]
[null,"12-01-2018","16:03","DT-8092","Rural Short","Weather",null,86,153.13,0.29195399999999999,1.9070000000000001E-3,"No"]
[null,"12-01-2018","16:25","NMI-25010202292","Urban","Network Business","Network Error",1,181.65,5.659E-3,3.1000000000000001E-5,"No"]
[null,"12-01-2018","19:03","DT-6968","Rural Long","Weather",null,1,472,0.543153,1.1509999999999999E-3,"No"]
[null,"13-01-2018","02:05","22LG29 JINDALEE","Rural Short","Network Business","Network Error",7,2.13,3.3100000000000002E-4,1.55E-4,"No"]
[null,"13-01-2018","06:14","22BA01 MINE","Rural Short","Asset Failure","Subtransmission",1,37.619999999999997,8.34E-4,2.1999999999999999E-5,"No"]
[null,"13-01-2018","06:14","22BA04 TOWN","Rural Short","Asset Failure","Subtransmission",383,37.479999999999997,0.31826100000000002,8.4910000000000003E-3,"No"]
[null,"13-01-2018","06:14","22BA05 MANTON","Rural Short","Asset Failure","Subtransmission",11,37.28,9.0919999999999994E-3,2.4399999999999999E-4,"No"]
[null,"13-01-2018","06:14","22KA03 FLORINA","Rural Short","Asset Failure","Subtransmission",266,16.98,0.10015,5.8970000000000003E-3,"No"]
[null,"13-01-2018","06:14","22KA06 TINDAL 2","Rural Short","Asset Failure","Subtransmission",245,17.8,9.6679000000000001E-2,5.4310000000000001E-3,"No"]
[null,"13-01-2018","06:14","22KA07 KATH EAST","Rural Short","Asset Failure","Subtransmission",1333,12.62,0.37283899999999998,2.9551000000000001E-2,"No"]
[null,"13-01-2018","06:14","22KA09 PINE CREEK","Rural Short","Asset Failure","Subtransmission",126,19.47,5.4376000000000001E-2,2.7929999999999999E-3,"No"]
[null,"13-01-2018","06:14","22KA10 MATARANKA 1","Rural Long","Asset Failure","Subtransmission",303,20.22,7.0490789999999999,0.34867700000000001,"No"]
[null,"13-01-2018","06:14","22KA15 OPS","Rural Short","Asset Failure","Subtransmission",392,13.72,0.119201,8.6899999999999998E-3,"No"]
[null,"13-01-2018","06:14","22KA19 TINDAL 1","Rural Short","Asset Failure","Subtransmission",245,17.55,9.5321000000000003E-2,5.4310000000000001E-3,"No"]
[null,"13-01-2018","06:14","22KA22 KATHERINE","Urban","Asset Failure","Subtransmission",1638,10.77,0.54941899999999999,5.1029999999999999E-2,"No"]
[null,"13-01-2018","07:52","DT-8085","Urban","Vegetation","Blow-in/Fall-in NSP Responsibility",65,10.6,2.1465000000000001E-2,2.0249999999999999E-3,"No"]
[null,"13-01-2018","10:14","22PC308 TOWNSHIP","Rural Short","Unknown","Unknown",256,21.05,0.119464,5.6750000000000004E-3,"No"]
[null,"14-01-2018","04:30","DT-10598","Rural Short","Weather",null,11,98.08,2.3918999999999999E-2,2.4399999999999999E-4,"No"]
[null,"14-01-2018","05:12","REC-10022","Rural Long","Asset Failure","HV",540,558.62,347.12658199999998,0.62140399999999996,"No"]
[null,"14-01-2018","15:00","DT-7113","Urban","Unknown","Unknown",152,66.349999999999994,0.31419000000000002,4.7349999999999996E-3,"No"]
[null,"14-01-2018","16:42","DT-6031","Urban","Third Party","Other",35,84.27,9.1882000000000005E-2,1.09E-3,"No"]
[null,"14-01-2018","22:32","DT-3483","Rural Short","Overloads",null,96,102.67,0.218498,2.1280000000000001E-3,"No"]
[null,"14-01-2018","22:52","11WN22 LUDMILLA","Rural Short","Weather",null,1307,41.1,1.190869,2.8975000000000001E-2,"No"]
[null,"15-01-2018","06:33","REC-10049","Rural Long","Unknown","Unknown",39,16.52,0.74125399999999997,4.4879000000000002E-2,"No"]
[null,"15-01-2018","07:18","DT-6485","Rural Short","Weather",null,5,77.27,8.5649999999999997E-3,1.11E-4,"No"]
[null,"15-01-2018","14:29","22LG29 JINDALEE","Rural Short","Network Business","Network Error",7,3.25,5.04E-4,1.55E-4,"No"]
[null,"15-01-2018","15:07","11PA25 PINELANDS","Urban","Weather",null,5,119.72,1.8648000000000001E-2,1.56E-4,"No"]
[null,"15-01-2018","15:37","11FB08 MOORING BASIN","Urban","Weather",null,220,395.08,2.707821,6.8539999999999998E-3,"No"]
[null,"15-01-2018","17:22","22LG29 JINDALEE","Rural Short","Weather",null,7,17.48,2.7130000000000001E-3,1.55E-4,"No"]
[null,"15-01-2018","17:28","DT-2482","Urban","Asset Failure","HV",0,77.2,0,0,"No"]
[null,"15-01-2018","18:00","NMI-25000654413","Rural Short","Third Party","Unauthorised Access",1,62.45,1.384E-3,2.1999999999999999E-5,"No"]
[null,"15-01-2018","18:12","REC-10027","Rural Short","Weather",null,175,18.37,7.1254999999999999E-2,3.8800000000000002E-3,"No"]
[null,"15-01-2018","21:33","SEC-0060","Rural Short","Asset Failure","HV",56,221.3,0.27473599999999998,1.2409999999999999E-3,"No"]
[null,"16-01-2018","08:40","DT-0264","Rural Short","Planned",null,3,152.41999999999999,null,null,"No"]
[null,"16-01-2018","08:46","NMI-25000412497","Rural Short","Network Business","Network Error",1,69.73,1.5460000000000001E-3,2.1999999999999999E-5,"No"]
[null,"16-01-2018","09:00","DT-8446","Rural Short","Planned",null,1,120.2,null,null,"No"]
[null,"16-01-2018","09:05","DT-1046","Urban","Planned",null,34,180.33,null,null,"No"]
[null,"16-01-2018","10:22","DT-1315","Rural Short","Weather",null,1,114.55,2.539E-3,2.1999999999999999E-5,"No"]
[null,"16-01-2018","12:58","NMI-25000313745","Rural Short","Asset Failure","LV",1,135.02000000000001,2.993E-3,2.1999999999999999E-5,"No"]
[null,"16-01-2018","14:39","NMI-25000717013","Rural Short","Third Party","Unauthorised Access",1,56.23,1.2470000000000001E-3,2.1999999999999999E-5,"No"]
[null,"16-01-2018","15:47","11RG02 GOLF","Urban","Unknown","Unknown",940,18.23,0.53395199999999998,2.9284000000000001E-2,"No"]
[null,"16-01-2018","15:47","11LG07 ARALUEN","Urban","Unknown","Unknown",696,19.5,0.422817,2.1683000000000001E-2,"No"]
[null,"16-01-2018","15:47","11LG15 LARAPINTA","Rural Short","Unknown","Unknown",1049,20.2,0.46975699999999998,2.3255000000000001E-2,"No"]
[null,"16-01-2018","22:40","11BE18 PORT","Rural Short","Weather",null,6,15.42,2.0509999999999999E-3,1.3300000000000001E-4,"No"]
[null,"17-01-2018","07:17","DT-2746","Rural Short","Weather",null,1,142.55000000000001,3.16E-3,2.1999999999999999E-5,"No"]
[null,"17-01-2018","08:30","SWH-7547","Rural Short","Weather",null,57,4.4000000000000004,5.5599999999999998E-3,1.2639999999999999E-3,"No"]
[null,"17-01-2018","08:45","DT-8431","Rural Short","Planned",null,1,84.77,null,null,"No"]
[null,"17-01-2018","09:01","NMI-25000390068","Rural Short","Asset Failure","LV",1,56.63,1.256E-3,2.1999999999999999E-5,"No"]
[null,"17-01-2018","09:27","DT-0286","Rural Short","Planned",null,19,104.33,null,null,"No"]
[null,"17-01-2018","11:02","DT-8432","Rural Short","Planned",null,0,76.23,null,null,"No"]
[null,"17-01-2018","13:12","DT-6855","Rural Short","Animal","Animal Impact",1,80.55,1.786E-3,2.1999999999999999E-5,"No"]
[null,"17-01-2018","16:42","DT-6990","Rural Long","Weather",null,1,82.83,9.5320000000000002E-2,1.1509999999999999E-3,"No"]
[null,"17-01-2018","16:53","66 CH-PC","N/A","Network Business","Network Error",0,26.28,null,null,"No"]
[null,"17-01-2018","17:56","REC-10049","Rural Long","Weather",null,39,17.329999999999998,0.77790599999999999,4.4879000000000002E-2,"No"]
[null,"17-01-2018","18:15","REC-10049","Rural Long","Weather",null,39,16.18,0.72629500000000002,4.4879000000000002E-2,"No"]
[null,"18-01-2018","09:07","DT-10735","Rural Short","Planned",null,7,244.37,null,null,"No"]
[null,"18-01-2018","09:12","DT-2270","Urban","Planned",null,1,122.27,null,null,"No"]
[null,"18-01-2018","14:03","NMI-25000466881","Urban","Asset Failure","LV",1,64.819999999999993,2.019E-3,3.1000000000000001E-5,"No"]
[null,"18-01-2018","14:27","11BE03 TDZ","Rural Short","Weather",null,72,16.07,2.5645000000000001E-2,1.596E-3,"No"]
[null,"18-01-2018","19:31","DT-2039","Rural Short","Asset Failure","HV",37,29.6,2.4279999999999999E-2,8.1999999999999998E-4,"No"]
[null,"19-01-2018","07:42","NMI-25000473597","Rural Short","Animal","Animal Impact",1,86.67,1.921E-3,2.1999999999999999E-5,"No"]
[null,"19-01-2018","09:00","DT-8430","Rural Short","Planned",null,1,99.18,null,null,"No"]
[null,"19-01-2018","10:50","DT-1778","Rural Short","Planned",null,6,172.33,null,null,"No"]
[null,"19-01-2018","11:15","DT-8204","Rural Short","Planned",null,2,52.17,null,null,"No"]
[null,"19-01-2018","12:35","NMI-25000189799","Rural Short","Network Business","Network Error",1,65.87,1.4599999999999999E-3,2.1999999999999999E-5,"No"]
[null,"19-01-2018","15:50","REC-10007","Rural Short","Weather",null,165,2.35,8.5959999999999995E-3,3.6579999999999998E-3,"No"]
[null,"19-01-2018","17:22","66 HC-WN 2","N/A","Weather",null,0,14.78,null,null,"No"]
[null,"20-01-2018","04:09","P-0213-SADA","Rural Short","Third Party","Other",0,94.78,0,0,"No"]
[null,"20-01-2018","08:37","DT-2666","Rural Short","Planned",null,1,113.07,null,null,"No"]
[null,"21-01-2018","09:25","66 MR-SY","Rural Short","Weather",null,418,15.25,0.141316,9.2669999999999992E-3,"No"]
[null,"21-01-2018","23:52","DT-0262","Rural Short","Weather",null,24,87.95,4.6794000000000002E-2,5.3200000000000003E-4,"No"]
[null,"22-01-2018","04:37","REC-10036","Rural Short","Weather",null,6,508.62,6.7653000000000005E-2,1.3300000000000001E-4,"No"]
[null,"22-01-2018","09:28","NMI-25000437295","Urban","Planned",null,1,46.38,null,null,"No"]
[null,"22-01-2018","09:30","DT-6205","Rural Short","Unknown","Unknown",9,63.83,1.2736000000000001E-2,2.0000000000000001E-4,"No"]
[null,"22-01-2018","10:29","DT-3205","Rural Short","Unknown","Unknown",4,78.12,6.927E-3,8.8999999999999995E-5,"No"]
[null,"22-01-2018","11:09","NMI-25000886718","Urban","Third Party","Other",1,78.87,2.457E-3,3.1000000000000001E-5,"No"]
[null,"22-01-2018","13:39","NMI-25000817761","Rural Short","Asset Failure","LV",1,60.43,1.34E-3,2.1999999999999999E-5,"No"]
[null,"22-01-2018","19:12","DT-1913","Rural Short","Asset Failure","HV",3,97.08,6.4570000000000001E-3,6.7000000000000002E-5,"No"]
[null,"23-01-2018","07:59","NMI-25000112883","Rural Short","Asset Failure","LV",1,90.53,2.0070000000000001E-3,2.1999999999999999E-5,"No"]
[null,"23-01-2018","08:53","DT-6125","Rural Short","Planned",null,11,75.2,null,null,"No"]
[null,"23-01-2018","09:30","DT-1981","Rural Short","Planned",null,93,220.72,null,null,"No"]
[null,"23-01-2018","09:43","DT-9563","Rural Short","Planned",null,0,44.28,null,null,"No"]
[null,"23-01-2018","10:14","NMI-25020110414","Urban","Network Business","Network Error",1,48.37,1.5070000000000001E-3,3.1000000000000001E-5,"No"]
[null,"23-01-2018","11:19","DT-8418","Rural Short","Planned",null,1,65.17,null,null,"No"]
[null,"23-01-2018","12:02","NMI-25000498933","Urban","Vegetation","Grow-in NSP Responsibility",1,265.77999999999997,8.2799999999999992E-3,3.1000000000000001E-5,"No"]
[null,"23-01-2018","17:12","DT-6232","Urban","Network Business","Switching and Protection Error",42,27.57,3.6069999999999998E-2,1.3079999999999999E-3,"No"]
[null,"23-01-2018","17:40","11RG20 WILLS","Urban","Asset Failure","HV",713,115.8,2.5722109999999998,2.2213E-2,"No"]
[null,"23-01-2018","17:52","DT-0630","Rural Short","Unknown","Unknown",1,175.52,3.8909999999999999E-3,2.1999999999999999E-5,"No"]
[null,"24-01-2018","08:32","DT-2626","Urban","Planned",null,50,201,null,null,"No"]
[null,"24-01-2018","11:15","DT-0303","Rural Short","Planned",null,7,194.53,null,null,"No"]
[null,"25-01-2018","09:24","DT-9560","Rural Short","Planned",null,1,57,null,null,"No"]
[null,"25-01-2018","10:50","DT-9558","Rural Short","Planned",null,1,52.18,null,null,"No"]
[null,"25-01-2018","16:41","REC-10049","Rural Long","Weather",null,39,21.62,0.97013799999999994,4.4879000000000002E-2,"No"]
[null,"25-01-2018","17:57","DT-6719","Rural Short","Animal","Animal Impact",1,88.5,1.9620000000000002E-3,2.1999999999999999E-5,"No"]
[null,"26-01-2018","01:18","NMI-25000393878","Urban","Asset Failure","LV",1,105.13,3.2750000000000001E-3,3.1000000000000001E-5,"No"]
[null,"26-01-2018","03:51","REC-10027","Rural Short","Weather",null,175,14.3,5.5478E-2,3.8800000000000002E-3,"No"]
[null,"26-01-2018","07:57","DT-0220","Rural Short","Asset Failure","LV",2,173.63,7.6990000000000001E-3,4.3999999999999999E-5,"No"]
[null,"26-01-2018","12:17","REC-10049","Rural Long","Weather",null,39,16.73,0.75097800000000003,4.4879000000000002E-2,"No"]
[null,"26-01-2018","17:05","11RG01 GAP","Rural Short","Network Business","Switching and Protection Error",812,28,0.50403500000000001,1.8001E-2,"No"]
[null,"27-01-2018","02:55","DT-2707","Rural Short","Weather",null,88,103.2,0.20133000000000001,1.951E-3,"No"]
[null,"27-01-2018","03:04","NMI-25000387789","Rural Short","Asset Failure","LV",1,69.069999999999993,1.531E-3,2.1999999999999999E-5,"No"]
[null,"27-01-2018","07:29","DT-2047","Urban","Weather",null,9,86.72,2.4313999999999999E-2,2.7999999999999998E-4,"No"]
[null,"27-01-2018","07:40","DT-2291","Urban","Vegetation","Blow-in/Fall-in NSP Responsibility",13,133.83000000000001,5.4202E-2,4.0499999999999998E-4,"No"]
[null,"27-01-2018","09:50","NMI-25000159396","Rural Short","Asset Failure","LV",1,63.45,1.407E-3,2.1999999999999999E-5,"No"]
[null,"27-01-2018","11:14","DT-10341","Rural Long","Unknown","Unknown",1,461.72,0.53132000000000001,1.1509999999999999E-3,"No"]
[null,"27-01-2018","12:39","NMI-25000606785","Urban","Third Party","Unauthorised Access",1,100.13,3.1199999999999999E-3,3.1000000000000001E-5,"No"]
[null,"27-01-2018","15:29","NMI-25000608244","Rural Short","Asset Failure","LV",1,497.23,1.1023E-2,2.1999999999999999E-5,"No"]
[null,"27-01-2018","17:01","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",209,23,0.10656599999999999,4.633E-3,"No"]
[null,"27-01-2018","21:54","DT-2442","Rural Short","Weather",null,7,126.12,1.9571000000000002E-2,1.55E-4,"No"]
[null,"27-01-2018","23:41","DT-0136","Rural Short","Network Business","Network Error",1,199.93,4.4320000000000002E-3,2.1999999999999999E-5,"No"]
[null,"28-01-2018","02:47","11WN04 BULLOCKY POINT","Urban","Weather",null,323,19.62,0.19739499999999999,1.0063000000000001E-2,"No"]
[null,"28-01-2018","04:32","REC-10036","Rural Short","Weather",null,6,237.95,3.1650999999999999E-2,1.3300000000000001E-4,"No"]
[null,"28-01-2018","07:53","REC-10018","Rural Short","Weather",null,0,13.43,0,0,"No"]
[null,"28-01-2018","10:00","22KA10 MATARANKA 1","Rural Long","Planned",null,303,184.4,null,null,"No"]
[null,"28-01-2018","12:17","DT-10788","Rural Short","Weather",null,4,150.43,1.3339999999999999E-2,8.8999999999999995E-5,"No"]
[null,"28-01-2018","18:31","11CP4307 BELYUEN","Rural Short","Weather",null,1,15.78,3.5E-4,2.1999999999999999E-5,"No"]
[null,"28-01-2018","18:55","11WN02 FANNIE BAY","Urban","Weather",null,1480,75.569999999999993,3.4841790000000001,4.6107000000000002E-2,"No"]
[null,"28-01-2018","19:01","11WH02 BLESSER CREEK","Rural Short","Weather",null,56,121.92,0.15135499999999999,1.2409999999999999E-3,"No"]
[null,"28-01-2018","19:08","22SY03 VIRGINIA","Rural Short","Weather",null,1180,425.82,11.139125,2.6159000000000002E-2,"No"]
[null,"28-01-2018","19:14","GCR-0013","Rural Short","Weather",null,158,221.18,0.77473999999999998,3.503E-3,"No"]
[null,"28-01-2018","19:16","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,949,637.82000000000005,13.41864,2.1038000000000001E-2,"No"]
[null,"28-01-2018","19:21","REC-10037","Rural Short","Weather",null,27,20.25,1.2121E-2,5.9900000000000003E-4,"No"]
[null,"28-01-2018","20:06","11CP4306 WAGAIT","Rural Short","Weather",null,299,10.199999999999999,6.7611000000000004E-2,6.6290000000000003E-3,"No"]
[null,"28-01-2018","20:35","22SY12 NOONAMAH","Rural Short","7 - STPIS Exclusion (3.3)(a)",null,908,234.12,null,null,"No"]
[null,"28-01-2018","21:30","DT-0694","Rural Short","Asset Failure","HV",13,408.05,0.117599,2.8800000000000001E-4,"No"]
[null,"28-01-2018","21:55","DT-10346","Rural Long","Unknown","Unknown",3,456.55,1.576122,3.4520000000000002E-3,"No"]
[null,"29-01-2018","03:35","22SY03 VIRGINIA","Rural Short","Asset Failure","HV",1180,5,0.130797,2.6159000000000002E-2,"No"]
[null,"29-01-2018","05:56","DT-2893","Urban","Weather",null,49,124.12,0.189467,1.5269999999999999E-3,"No"]
[null,"29-01-2018","07:12","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,949,15.28,0.32153700000000002,2.1038000000000001E-2,"No"]
[null,"29-01-2018","09:24","DT-0588","Rural Short","Weather",null,2,183.3,8.1270000000000005E-3,4.3999999999999999E-5,"No"]
[null,"29-01-2018","10:03","DT-0694","Rural Short","Asset Failure","HV",13,187.17,5.3941000000000003E-2,2.8800000000000001E-4,"No"]
[null,"29-01-2018","10:25","22WD102 WICKHAM","Urban","Weather",null,8,290.43,7.2384000000000004E-2,2.4899999999999998E-4,"No"]
[null,"29-01-2018","10:26","11WN24 PARAP","Urban","Weather",null,1262,20.18,0.79352500000000004,3.9315999999999997E-2,"No"]
[null,"29-01-2018","11:45","REC-10001","Rural Short","Asset Failure","HV",32,1.72,1.2179999999999999E-3,7.0899999999999999E-4,"No"]
[null,"29-01-2018","11:50","NMI-25000606010","Urban","Third Party","Other",1,44.5,1.3860000000000001E-3,3.1000000000000001E-5,"No"]
[null,"29-01-2018","13:03","REC-10036","Rural Short","Weather",null,6,18.32,2.4359999999999998E-3,1.3300000000000001E-4,"No"]
[null,"29-01-2018","13:27","22SY15 DARWIN RIVER","Rural Short","Weather",null,817,17.829999999999998,0.32299899999999998,1.8112E-2,"No"]
[null,"29-01-2018","16:09","NMI-25000588940","Urban","Asset Failure","LV",1,150.37,4.6839999999999998E-3,3.1000000000000001E-5,"No"]
[null,"29-01-2018","17:05","22SY02 MCMINNS","Rural Short","Weather",null,1238,107.17,2.9412150000000001,2.7445000000000001E-2,"No"]
[null,"30-01-2018","01:34","DT-3145","Urban","Asset Failure","HV",92,139.38,0.39949099999999999,2.8660000000000001E-3,"No"]
[null,"30-01-2018","01:38","DT-3145","Urban","Weather",null,92,112.2,0.32157999999999998,2.8660000000000001E-3,"No"]
[null,"30-01-2018","04:10","DT-3145","Urban","Weather",null,92,80.83,0.231679,2.8660000000000001E-3,"No"]
[null,"30-01-2018","06:36","DT-3403","Rural Short","Weather",null,0,245.2,0,0,"No"]
[null,"30-01-2018","06:40","DT-3264","Urban","Asset Failure","HV",0,170.82,0,0,"No"]
[null,"30-01-2018","06:46","DT-3145","Urban","Asset Failure","HV",92,95.92,0.27490999999999999,2.8660000000000001E-3,"No"]
[null,"30-01-2018","08:31","NMI-25000404593","Urban","Asset Failure","LV",1,259.3,8.0780000000000001E-3,3.1000000000000001E-5,"No"]
[null,"30-01-2018","09:08","DT-3264","Urban","Asset Failure","HV",0,32.950000000000003,0,0,"No"]
[null,"30-01-2018","14:02","DT-3145","Urban","Asset Failure","HV",92,62.37,0.17875099999999999,2.8660000000000001E-3,"No"]
[null,"30-01-2018","17:46","11WS08 CULLEN","Urban","Weather",null,703,17.05,0.37341200000000002,2.1901E-2,"No"]
[null,"30-01-2018","17:54","11BE03 TDZ","Rural Short","Weather",null,72,3.67,5.8529999999999997E-3,1.596E-3,"No"]
[null,"30-01-2018","18:43","NMI-25000754015","Rural Long","Asset Failure","LV",1,61.05,7.0252999999999996E-2,1.1509999999999999E-3,"No"]
[null,"30-01-2018","19:00","DT-2706","Rural Short","Weather",null,79,57.53,0.100761,1.751E-3,"No"]
[null,"30-01-2018","19:06","NMI-25000312887","Urban","Asset Failure","LV",1,4.07,1.27E-4,3.1000000000000001E-5,"No"]
[null,"30-01-2018","19:55","GCR-0763","Rural Long","Weather",null,123,121.47,17.192634999999999,0.141542,"No"]
[null,"30-01-2018","19:56","22MT07 ACACIA","Rural Short","Asset Failure","HV",196,146.05000000000001,0.634606,4.3449999999999999E-3,"No"]
[null,"31-01-2018","03:17","11BE14 ROBERTSON","Urban","Asset Failure","HV",4,46.52,5.7970000000000001E-3,1.25E-4,"No"]
[null,"31-01-2018","09:17","DT-9553","Rural Short","Planned",null,1,107.38,null,null,"No"]
[null,"31-01-2018","10:42","11CP4307 BELYUEN","Rural Short","Weather",null,1,15.57,3.4499999999999998E-4,2.1999999999999999E-5,"No"]
[null,"31-01-2018","13:31","DT-2155","CBD","Asset Failure","HV",123,9.52,0.314664,3.3064999999999997E-2,"No"]
[null,"31-01-2018","14:31","22BA04 TOWN","Rural Short","Weather",null,383,15.48,0.131465,8.4910000000000003E-3,"No"]
[null,"31-01-2018","14:41","DT-0168","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",76,106.53,0.17949200000000001,1.6850000000000001E-3,"No"]
[null,"31-01-2018","17:14","22RG04 BREWER 2","Rural Short","Weather",null,209,18.350000000000001,8.5022E-2,4.633E-3,"No"]
[null,"31-01-2018","20:56","DT-0252","Rural Short","Asset Failure","HV",18,33.1,1.3207999999999999E-2,3.9899999999999999E-4,"No"]
[null,"31-01-2018","23:01","NMI-25000756372","Rural Short","Asset Failure","LV",1,12785.88,0.28344999999999998,2.1999999999999999E-5,"No"]
[null,"31-01-2018","23:05","SWH-0362","Rural Short","Network Business","Network Error",8,14.52,2.575E-3,1.7699999999999999E-4,"No"]
[null,"01-02-2018","00:16","DT-2351","CBD","Planned",null,29,236.3,null,null,"No"]
[null,"01-02-2018","06:57","DT-2148","Urban","7 - STPIS Exclusion (3.3)(a)",null,2,172.6,null,null,"No"]
[null,"01-02-2018","09:13","DT-10006","Rural Short","Planned",null,13,162.30000000000001,null,null,"No"]
[null,"01-02-2018","09:35","DT-9559","Rural Short","Planned",null,2,102.27,null,null,"No"]
[null,"01-02-2018","10:09","DT-10024","Rural Short","Unknown","Unknown",0,193.98,0,0,"No"]
[null,"01-02-2018","11:41","FH-0225","Rural Short","Unknown","Unknown",1,99.05,2.196E-3,2.1999999999999999E-5,"No"]
[null,"01-02-2018","14:19","NMI-25000391924","Urban","Asset Failure","LV",1,92.93,2.895E-3,3.1000000000000001E-5,"No"]
[null,"01-02-2018","16:48","NMI-25010122699","Rural Short","Network Business","Switching and Protection Error",1,93.18,2.0660000000000001E-3,2.1999999999999999E-5,"No"]
[null,"01-02-2018","16:57","NMI-25000399420","Rural Short","Asset Failure","LV",1,46.9,1.0399999999999999E-3,2.1999999999999999E-5,"No"]
[null,"02-02-2018","14:04","11CA23 MOIL","Rural Short","Asset Failure","HV",895,71.22,1.4130290000000001,1.9841000000000001E-2,"No"]
[null,"02-02-2018","21:56","NMI-25000522238","Rural Short","Asset Failure","LV",1,68.88,1.5269999999999999E-3,2.1999999999999999E-5,"No"]
[null,"03-02-2018","16:13","DT-0329","Rural Short","Weather",null,9,286.52999999999997,5.7168999999999998E-2,2.0000000000000001E-4,"No"]
[null,"03-02-2018","16:22","DT-0329","Rural Short","Asset Failure","HV",9,341.12,6.8059999999999996E-2,2.0000000000000001E-4,"No"]
[null,"03-02-2018","19:01","DT-0806","Rural Short","Unknown","Unknown",1,493.53,1.0940999999999999E-2,2.1999999999999999E-5,"No"]
[null,"04-02-2018","08:41","11BE03 TDZ","Rural Short","Planned",null,22,280.27,null,null,"No"]
[null,"04-02-2018","08:54","NMI-25000402564","Rural Short","Asset Failure","LV",1,67.75,1.5020000000000001E-3,2.1999999999999999E-5,"No"]
[null,"04-02-2018","10:08","22SY06 WHITEWOOD","Urban","Unknown","Unknown",4,16.12,2.0079999999999998E-3,1.25E-4,"No"]
[null,"04-02-2018","15:23","11AR05 BELLAMACK 1","Urban","Asset Failure","HV",1151,84.6,3.0335709999999998,3.5858000000000001E-2,"No"]
[null,"04-02-2018","18:47","22SY11 HERBERT","Rural Short","Weather",null,1808,121.07,4.852544,4.0082E-2,"No"]
[null,"04-02-2018","18:55","22WD102 WICKHAM","Urban","Weather",null,8,28.23,7.0369999999999999E-3,2.4899999999999998E-4,"No"]
[null,"04-02-2018","19:04","11WN22 LUDMILLA","Rural Short","Asset Failure","HV",1307,346.82,10.04898,2.8975000000000001E-2,"No"]
[null,"04-02-2018","20:19","NMI-25000383226","Rural Short","Weather",null,1,177.9,3.9439999999999996E-3,2.1999999999999999E-5,"No"]
[null,"04-02-2018","23:02","NMI-25000799463","Rural Short","Asset Failure","LV",1,136.97,3.0360000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-02-2018","04:19","NMI-25000199757","Rural Short","Asset Failure","LV",1,194.28,4.3070000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-02-2018","05:23","DT-0607","Rural Short","Unknown","Unknown",13,139.83000000000001,4.0300000000000002E-2,2.8800000000000001E-4,"No"]
[null,"05-02-2018","13:37","REC-10017","Rural Short","Weather",null,75,15.2,2.5273E-2,1.663E-3,"No"]
[null,"05-02-2018","16:41","NMI-25000580057","Rural Short","Asset Failure","LV",1,51.47,1.1410000000000001E-3,2.1999999999999999E-5,"No"]
[null,"06-02-2018","07:20","NMI-25000114600","Rural Short","Asset Failure","LV",1,41.92,9.2900000000000003E-4,2.1999999999999999E-5,"No"]
[null,"06-02-2018","07:22","NMI-25000330427","Urban","Asset Failure","LV",1,114.5,3.5669999999999999E-3,3.1000000000000001E-5,"No"]
[null,"06-02-2018","08:00","DT-0210","Rural Short","Planned",null,9,47,null,null,"No"]
[null,"06-02-2018","09:02","DT-0217","Rural Short","Asset Failure","HV",1,170.8,3.7859999999999999E-3,2.1999999999999999E-5,"No"]
[null,"06-02-2018","10:13","DT-0804","Rural Short","Unknown","Unknown",1,127.93,2.836E-3,2.1999999999999999E-5,"No"]
[null,"06-02-2018","12:12","DT-8282","Rural Short","Unknown","Unknown",19,54.75,2.3061000000000002E-2,4.2099999999999999E-4,"No"]
[null,"06-02-2018","12:55","DT-6276","Rural Short","Animal","Animal Impact",1,71.97,1.5950000000000001E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","04:24","REC-10030","Rural Long","Animal","Animal Impact",18,138.38,2.8663979999999998,2.0712999999999999E-2,"No"]
[null,"07-02-2018","08:30","DT-1706","Rural Short","Planned",null,9,164.55,null,null,"No"]
[null,"07-02-2018","10:09","22RG04 BREWER 2","Rural Short","Unknown","Unknown",209,15.97,7.3979000000000003E-2,4.633E-3,"No"]
[null,"07-02-2018","11:14","DT-6741","Rural Short","Weather",null,1,199.38,4.4200000000000003E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","11:26","NMI-25000756200","Rural Short","Asset Failure","LV",1,118.6,2.6289999999999998E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","12:08","22HD403 MIDDLE POINT","Rural Short","Asset Failure","HV",42,59.93,5.5803999999999999E-2,9.3099999999999997E-4,"No"]
[null,"07-02-2018","12:19","DT-0217","Rural Short","Weather",null,1,81.099999999999994,1.7979999999999999E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","12:41","NMI-25000629091","Rural Short","Asset Failure","LV",1,92.02,2.0400000000000001E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","13:03","DT-0136","Rural Short","Asset Failure","LV",1,404.07,8.9580000000000007E-3,2.1999999999999999E-5,"No"]
[null,"07-02-2018","19:48","NMI-25000518016","Urban","Asset Failure","LV",1,131.6,4.1000000000000003E-3,3.1000000000000001E-5,"No"]
[null,"07-02-2018","21:10","NMI-25000408173","Urban","Asset Failure","LV",1,237.32,7.3930000000000003E-3,3.1000000000000001E-5,"No"]
[null,"08-02-2018","13:52","22HD403 MIDDLE POINT","Rural Short","Weather",null,42,2.3199999999999998,2.1570000000000001E-3,9.3099999999999997E-4,"No"]
[null,"08-02-2018","14:47","NMI-25000112059","Rural Short","Weather",null,1,34.700000000000003,7.6900000000000004E-4,2.1999999999999999E-5,"No"]
[null,"09-02-2018","13:04","NMI-25020114001","Urban","Asset Failure","LV",1,126.08,3.9280000000000001E-3,3.1000000000000001E-5,"No"]
[null,"10-02-2018","08:02","DT-2418","Rural Short","Planned",null,1,276.87,null,null,"No"]
[null,"10-02-2018","08:34","DT-2560","Urban","Planned",null,58,207,null,null,"No"]
[null,"10-02-2018","09:46","NMI-25010195241","Urban","Asset Failure","LV",1,103.48,3.2239999999999999E-3,3.1000000000000001E-5,"No"]
[null,"10-02-2018","15:32","DT-10725","Rural Short","Unknown","Unknown",1,177.52,3.9350000000000001E-3,2.1999999999999999E-5,"No"]
[null,"11-02-2018","08:00","DT-2418","Rural Short","Planned",null,1,225.23,null,null,"No"]
[null,"11-02-2018","08:01","11BE03 TDZ","Rural Short","Planned",null,22,275.02999999999997,null,null,"No"]
[null,"11-02-2018","10:50","22HD403 MIDDLE POINT","Rural Short","Weather",null,42,149.87,0.139541,9.3099999999999997E-4,"No"]
[null,"11-02-2018","16:04","NMI-25010210132","Rural Short","Weather",null,1,114.07,2.529E-3,2.1999999999999999E-5,"No"]
[null,"11-02-2018","17:58","22BR101 BR-SD 1","Rural Short","Unknown","Unknown",280,16,9.9317000000000003E-2,6.2069999999999998E-3,"No"]
[null,"11-02-2018","17:58","22BR102 BOREFIELDS","Rural Short","Unknown","Unknown",29,17,1.0928999999999999E-2,6.4300000000000002E-4,"No"]
[null,"11-02-2018","17:58","22BR104 HERMANNSBURG","Rural Short","Unknown","Unknown",16,17,6.0299999999999998E-3,3.5500000000000001E-4,"No"]
[null,"11-02-2018","17:58","DT-8611","Rural Short","Asset Failure","HV",15,251.95,8.3781999999999995E-2,3.3300000000000002E-4,"No"]
[null,"11-02-2018","17:58","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",209,14.78,6.8496000000000001E-2,4.633E-3,"No"]
[null,"12-02-2018","07:15","DT-0946","Rural Short","Unknown","Unknown",10,95.47,2.1163999999999999E-2,2.22E-4,"No"]
[null,"12-02-2018","12:58","22SY03 VIRGINIA","Rural Short","Weather",null,1180,112.12,2.932909,2.6159000000000002E-2,"No"]
[null,"12-02-2018","16:16","NMI-25000770905","Rural Short","Asset Failure","LV",1,256.02,5.6759999999999996E-3,2.1999999999999999E-5,"No"]
[null,"12-02-2018","20:28","DT-2560","Urban","Asset Failure","LV",58,67.55,0.122057,1.807E-3,"No"]
[null,"13-02-2018","08:04","DT-1674","Rural Short","Planned",null,9,123,null,null,"No"]
[null,"13-02-2018","08:31","DT-6120","Rural Short","Planned",null,3,113.27,null,null,"No"]
[null,"13-02-2018","13:09","DT-0877","Rural Short","Weather",null,1,49.12,1.0889999999999999E-3,2.1999999999999999E-5,"No"]
[null,"13-02-2018","14:13","66 WN-DA","N/A","Weather",null,0,9.48,null,null,"No"]
[null,"13-02-2018","14:26","11WN13 GOYDER","Urban","Network Business","Network Error",577,28.12,0.50541499999999995,1.7975999999999999E-2,"No"]
[null,"13-02-2018","17:35","NMI-25000837775","Rural Long","Weather",null,1,1440.12,1.657211,1.1509999999999999E-3,"No"]
[null,"13-02-2018","21:10","DT-10372","Rural Long","Unknown","HV",1,274.87,0.31630200000000003,1.1509999999999999E-3,"No"]
[null,"13-02-2018","22:01","DT-10371","Rural Long","Asset Failure","HV",2,127.4,0.293211,2.3010000000000001E-3,"No"]
[null,"13-02-2018","23:11","NMI-25000653803","Rural Short","Asset Failure","LV",1,193.62,4.2919999999999998E-3,2.1999999999999999E-5,"No"]
[null,"14-02-2018","00:52","DT-10371","Rural Long","Weather",null,2,197.23,0.453932,2.3010000000000001E-3,"No"]
[null,"14-02-2018","05:58","DT-0535","Rural Short","Weather",null,18,89.78,3.5826999999999998E-2,3.9899999999999999E-4,"No"]
[null,"14-02-2018","06:38","SWH-6069","Rural Long","Weather",null,177,15.18,3.092578,0.203682,"No"]
[null,"14-02-2018","08:52","REC-10049","Rural Long","Unknown","Unknown",39,236.63,10.619908000000001,4.4879000000000002E-2,"No"]
[null,"14-02-2018","09:44","SWH-2156","Rural Short","Network Business","Network Error",18,13.35,5.3270000000000001E-3,3.9899999999999999E-4,"No"]
[null,"14-02-2018","11:47","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",209,18.43,8.5407999999999998E-2,4.633E-3,"No"]
[null,"14-02-2018","17:44","NMI-25000757819","Rural Short","Asset Failure","LV",1,108.7,2.4099999999999998E-3,2.1999999999999999E-5,"No"]
[null,"15-02-2018","09:00","DT-0121","Rural Short","Planned",null,1,122.18,null,null,"No"]
[null,"15-02-2018","14:07","DT-2040","Rural Short","Network Business","Network Error",54,17.02,2.0371E-2,1.1969999999999999E-3,"No"]
[null,"15-02-2018","15:48","NMI-25000161148","Rural Short","Planned",null,1,28.45,null,null,"No"]
[null,"15-02-2018","16:41","22BR101 BR-SD 1","Rural Short","Asset Failure","HV",280,316.43,1.9642040000000001,6.2069999999999998E-3,"No"]
[null,"15-02-2018","16:42","22TC07 THREE WAYS","Rural Short","Weather",null,596,17.170000000000002,0.22681899999999999,1.3213000000000001E-2,"No"]
[null,"15-02-2018","17:03","22TC07 THREE WAYS","Rural Short","Weather",null,596,30.15,0.398364,1.3213000000000001E-2,"No"]
[null,"15-02-2018","21:20","DT-8280","Urban","Weather",null,72,77.28,0.17335100000000001,2.2430000000000002E-3,"No"]
[null,"16-02-2018","06:21","DT-1263","Rural Short","Unknown","Unknown",84,74.12,0.13802,1.8619999999999999E-3,"No"]
[null,"16-02-2018","10:09","PSPT130547","Rural Short","Asset Failure","LV",1,124.6,2.7620000000000001E-3,2.1999999999999999E-5,"No"]
[null,"16-02-2018","12:52","FH-6397","Rural Short","Animal","Animal Impact",1,45.05,9.990000000000001E-4,2.1999999999999999E-5,"No"]
[null,"16-02-2018","13:20","PSPT133138","Rural Short","Asset Failure","LV",1,97.18,2.1540000000000001E-3,2.1999999999999999E-5,"No"]
[null,"16-02-2018","13:51","SEC-22EV0134","Rural Short","Weather",null,107,84.02,0.199295,2.372E-3,"No"]
[null,"16-02-2018","17:55","NMI-25000426134","Urban","Asset Failure","LV",1,70.95,2.2100000000000002E-3,3.1000000000000001E-5,"No"]
[null,"16-02-2018","20:23","NMI-25000642961","Urban","Asset Failure","LV",1,355.58,1.1077999999999999E-2,3.1000000000000001E-5,"No"]
[null,"17-02-2018","07:30","DT-2116","Rural Short","Planned",null,1,267,null,null,"No"]
[null,"18-02-2018","01:13","DT-6298","Rural Short","Unknown","Unknown",0,70.83,0,0,"No"]
[null,"18-02-2018","07:53","22HD403 MIDDLE POINT","Rural Short","Asset Failure","HV",42,82,7.6350000000000001E-2,9.3099999999999997E-4,"No"]
[null,"18-02-2018","08:30","DT-2392","Rural Short","Planned",null,3,180,null,null,"No"]
[null,"18-02-2018","09:10","DT-2241","Urban","Planned",null,7,165.32,null,null,"No"]
[null,"18-02-2018","18:59","DT-6123","Rural Short","Weather",null,8,98.07,1.7392000000000001E-2,1.7699999999999999E-4,"No"]
[null,"18-02-2018","19:42","DT-2582","Rural Short","Unknown","Unknown",2,78.400000000000006,3.4759999999999999E-3,4.3999999999999999E-5,"No"]
[null,"19-02-2018","08:20","NMI-25000416136","Urban","Third Party","Other",1,46.78,1.457E-3,3.1000000000000001E-5,"No"]
[null,"19-02-2018","10:28","22TC09 WARREGO","Rural Short","Planned",null,2,227.48,null,null,"No"]
[null,"19-02-2018","11:20","DT-6062","Rural Short","Unknown","Unknown",2,42.38,1.879E-3,4.3999999999999999E-5,"No"]
[null,"19-02-2018","12:40","NMI-25000182705","Rural Short","Asset Failure","LV",1,46.83,1.0380000000000001E-3,2.1999999999999999E-5,"No"]
[null,"19-02-2018","14:16","NMI-25000640594","Rural Short","Asset Failure","LV",1,46.95,1.041E-3,2.1999999999999999E-5,"No"]
[null,"19-02-2018","18:36","22PA202 HOWARD SPRINGS","Rural Short","Weather",null,949,23.22,0.48844100000000001,2.1038000000000001E-2,"No"]
[null,"20-02-2018","08:30","DT-6104","Rural Short","Planned",null,12,223,null,null,"No"]
[null,"20-02-2018","08:30","66 MR-SY","Rural Short","Planned",null,209,143.78,null,null,"No"]
[null,"20-02-2018","08:38","DT-6296","Rural Short","Planned",null,96,251.2,null,null,"No"]
[null,"20-02-2018","09:04","DT-0303","Rural Short","Planned",null,7,248.08,null,null,"No"]
[null,"20-02-2018","09:13","DT-1225","Urban","Planned",null,203,167.45,null,null,"No"]
[null,"20-02-2018","09:35","DT-6062","Rural Short","Unknown","Unknown",2,36.799999999999997,1.632E-3,4.3999999999999999E-5,"No"]
[null,"20-02-2018","16:18","NMI-25000321311","Urban","Asset Failure","LV",1,40.6,1.2650000000000001E-3,3.1000000000000001E-5,"No"]
[null,"20-02-2018","17:46","FH-6485","Rural Short","Weather",null,18,54.55,2.1767999999999999E-2,3.9899999999999999E-4,"No"]
[null,"20-02-2018","19:18","NMI-25000118718","Urban","Asset Failure","LV",1,70.08,2.183E-3,3.1000000000000001E-5,"No"]
[null,"21-02-2018","09:06","DT-0087","Rural Short","Planned",null,13,126.22,null,null,"No"]
[null,"21-02-2018","09:10","DT-10495","Rural Short","Planned",null,1,170.75,null,null,"No"]
[null,"21-02-2018","10:08","DT-6062","Rural Short","Unknown","Unknown",2,65.680000000000007,2.9120000000000001E-3,4.3999999999999999E-5,"No"]
[null,"21-02-2018","19:13","DT-3205","Rural Short","Unknown","Unknown",4,131,1.1617000000000001E-2,8.8999999999999995E-5,"No"]
[null,"21-02-2018","23:00","DT-1223-1","CBD","Planned",null,42,255,null,null,"No"]
[null,"22-02-2018","00:02","DT-2876","Urban","Planned",null,31,45,null,null,"No"]
[null,"22-02-2018","07:17","DT-6277","Rural Long","Weather",null,2,82.43,0.18972,2.3010000000000001E-3,"No"]
[null,"22-02-2018","08:56","REC-10036","Rural Short","Unknown","Unknown",6,23.13,3.0769999999999999E-3,1.3300000000000001E-4,"No"]
[null,"22-02-2018","08:57","DT-0810","Rural Short","Weather",null,1,171.82,3.8089999999999999E-3,2.1999999999999999E-5,"No"]
[null,"22-02-2018","08:59","22HD402 LAMBELLS","Rural Short","Planned",null,57,220.28,null,null,"No"]
[null,"22-02-2018","09:20","22SY11 HERBERT","Rural Short","Planned",null,130,314.89999999999998,null,null,"No"]
[null,"22-02-2018","19:28","DT-2039","Rural Short","Asset Failure","LV",37,348.28,0.28568100000000002,8.1999999999999998E-4,"No"]
[null,"22-02-2018","22:45","NMI-25000605036","Urban","Asset Failure","LV",1,163.9,5.1060000000000003E-3,3.1000000000000001E-5,"No"]
[null,"23-02-2018","09:08","DT-0159","Rural Short","Unknown","Unknown",2,215.13,9.5390000000000006E-3,4.3999999999999999E-5,"No"]
[null,"23-02-2018","20:08","DT-8544","Rural Short","Unknown","Unknown",41,71.45,6.4943000000000001E-2,9.0899999999999998E-4,"No"]
[null,"24-02-2018","01:39","NMI-25000834525","Rural Short","Weather",null,1,101.87,2.258E-3,2.1999999999999999E-5,"No"]
[null,"24-02-2018","07:56","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,104,10.050000000000001,null,null,"No"]
[null,"24-02-2018","07:56","22TC02 TCK EAST","Urban","3 - STPIS Exclusion (3.3)(a)",null,726,9.83,null,null,"No"]
[null,"24-02-2018","07:56","22TC07 THREE WAYS","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,596,30.48,null,null,"No"]
[null,"24-02-2018","07:56","22TC08 TCK WEST","Urban","3 - STPIS Exclusion (3.3)(a)",null,254,44.13,null,null,"No"]
[null,"24-02-2018","07:56","22TC09 WARREGO","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,4,44.62,null,null,"No"]
[null,"25-02-2018","08:30","11PA23 GEORGINA","Urban","Planned",null,21,479.98,null,null,"No"]
[null,"25-02-2018","08:30","DT-1375","CBD","Planned",null,14,177.45,null,null,"No"]
[null,"25-02-2018","19:24","NMI-25000347081","Rural Long","Weather",null,1,224.92,0.258822,1.1509999999999999E-3,"No"]
[null,"26-02-2018","07:25","PSPT127252","Rural Short","Network Business","Switching and Protection Error",1,116.95,2.5929999999999998E-3,2.1999999999999999E-5,"No"]
[null,"26-02-2018","09:51","PSPT109974","CBD","Third Party","Other",1,226.8,6.0968000000000001E-2,2.6899999999999998E-4,"No"]
[null,"26-02-2018","09:57","DT-1653","Rural Short","Planned",null,10,69.05,null,null,"No"]
[null,"26-02-2018","23:52","DT-6486","Rural Short","Weather",null,1,124.18,2.7529999999999998E-3,2.1999999999999999E-5,"No"]
[null,"27-02-2018","09:16","DT-2448","Rural Short","Planned",null,56,184.45,null,null,"No"]
[null,"27-02-2018","09:17","DT-2460","Rural Short","Planned",null,89,184.87,null,null,"No"]
[null,"27-02-2018","11:05","DT-2482","Urban","Vegetation","Blow-in/Fall-in NSP Responsibility",0,2,0,0,"No"]
[null,"27-02-2018","11:29","NMI-25000754277","CBD","Third Party","Other",1,156.47999999999999,4.2064999999999998E-2,2.6899999999999998E-4,"No"]
[null,"27-02-2018","18:17","DT-0109","Rural Short","Animal","Animal Impact",17,65.430000000000007,2.4660000000000001E-2,3.77E-4,"No"]
[null,"27-02-2018","19:41","DT-0359","Rural Short","Unknown","Unknown",2,166.23,7.3699999999999998E-3,4.3999999999999999E-5,"No"]
[null,"27-02-2018","22:59","DT-1369","CBD","Planned",null,7,188.45,null,null,"No"]
[null,"28-02-2018","08:37","DT-1727","Rural Short","Planned",null,8,307.73,null,null,"No"]
[null,"28-02-2018","09:02","11WN02 FANNIE BAY","Urban","Planned",null,264,369.93,null,null,"No"]
[null,"28-02-2018","21:48","DT-10823","Rural Short","Unknown","Unknown",1,105.75,2.3440000000000002E-3,2.1999999999999999E-5,"No"]
[null,"01-03-2018","01:06","FH-0169","Rural Short","Asset Failure","HV",0,136.44999999999999,0,0,"No"]
[null,"01-03-2018","01:40","22HD402 LAMBELLS","Rural Short","Asset Failure","HV",94,10,2.0839E-2,2.0839999999999999E-3,"No"]
[null,"01-03-2018","09:30","DT-0260","Rural Short","Planned",null,42,93.23,null,null,"No"]
[null,"01-03-2018","09:35","22SY12 NOONAMAH","Rural Short","Planned",null,76,274.52,null,null,"No"]
[null,"01-03-2018","13:04","11AR05 BELLAMACK 1","Urban","Asset Failure","HV",1098,4.5,0.15393000000000001,3.4207000000000001E-2,"No"]
[null,"01-03-2018","14:08","DT-3215","Rural Short","Asset Failure","HV",1,20.100000000000001,4.46E-4,2.1999999999999999E-5,"No"]
[null,"01-03-2018","15:53","DT-1193","Urban","Unknown","Unknown",99,126.67,0.39066600000000001,3.0839999999999999E-3,"No"]
[null,"02-03-2018","09:05","DT-0101","Rural Short","Planned",null,19,105.7,null,null,"No"]
[null,"02-03-2018","10:32","DT-10008","Rural Short","Unknown","Unknown",8,44.72,7.9310000000000005E-3,1.7699999999999999E-4,"No"]
[null,"02-03-2018","10:48","22KA22 KATHERINE","Urban","Animal","Animal Impact",1544,14.18,0.68223500000000004,4.8100999999999998E-2,"No"]
[null,"02-03-2018","11:19","22BR101 BR-SD 1","Rural Short","Unknown","Unknown",278,17,0.104771,6.1630000000000001E-3,"No"]
[null,"02-03-2018","11:19","22BR102 BOREFIELDS","Rural Short","Unknown","Unknown",8,16,2.8379999999999998E-3,1.7699999999999999E-4,"No"]
[null,"02-03-2018","11:19","22BR104 HERMANNSBURG","Rural Short","Unknown","Unknown",46,15,1.5297E-2,1.0200000000000001E-3,"No"]
[null,"02-03-2018","11:19","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",209,14.55,6.7415000000000003E-2,4.633E-3,"No"]
[null,"02-03-2018","19:47","NMI-25000276843","Urban","Asset Failure","LV",1,72.88,2.271E-3,3.1000000000000001E-5,"No"]
[null,"03-03-2018","10:44","NMI-25000550133","Rural Short","Network Business","Network Error",1,70.88,1.5709999999999999E-3,2.1999999999999999E-5,"No"]
[null,"03-03-2018","17:20","NMI-25010240376","Rural Short","Asset Failure","LV",1,101.85,2.258E-3,2.1999999999999999E-5,"No"]
[null,"03-03-2018","17:21","DT-6153","Rural Long","Weather",null,14,719,11.583429000000001,1.6109999999999999E-2,"No"]
[null,"03-03-2018","17:21","DT-6179","Rural Long","Weather",null,1,719,0.82738800000000001,1.1509999999999999E-3,"No"]
[null,"03-03-2018","23:38","DT-8499","Rural Short","Overloads",null,67,229.3,0.34058500000000003,1.485E-3,"No"]
[null,"04-03-2018","08:47","DT-1317","Rural Short","Planned",null,9,111,null,null,"No"]
[null,"04-03-2018","10:31","DT-6610","Rural Short","Weather",null,2,97.93,4.3420000000000004E-3,4.3999999999999999E-5,"No"]
[null,"05-03-2018","10:02","DT-2427","Rural Short","Planned",null,79,276.77999999999997,null,null,"No"]
[null,"05-03-2018","13:28","NMI-25000823346","Rural Short","Asset Failure","HV",1,119.15,2.6410000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-03-2018","17:11","NMI-25000486699","Rural Short","Third Party","Other",1,62.47,1.3849999999999999E-3,2.1999999999999999E-5,"No"]
[null,"05-03-2018","19:35","FH-6127","Rural Short","Unknown","Unknown",31,99.43,6.8335000000000007E-2,6.87E-4,"No"]
[null,"05-03-2018","20:53","NMI-25000674286","Urban","Asset Failure","LV",1,136,4.2370000000000003E-3,3.1000000000000001E-5,"No"]
[null,"06-03-2018","09:04","DT-6711","Rural Short","Planned",null,2,95.18,null,null,"No"]
[null,"07-03-2018","06:26","DT-6271","Rural Short","Unknown","Unknown",2,54.85,2.4320000000000001E-3,4.3999999999999999E-5,"No"]
[null,"07-03-2018","08:47","11CA23 MOIL","Rural Short","Planned",null,88,226.77,null,null,"No"]
[null,"07-03-2018","08:54","22MT07 ACACIA","Rural Short","Planned",null,45,250.15,null,null,"No"]
[null,"07-03-2018","09:00","DT-2613","Urban","Planned",null,85,219.07,null,null,"No"]
[null,"07-03-2018","16:52","22SY04 DUNDEE","Rural Long","Asset Failure","HV",527,115.1,69.801726000000002,0.60644399999999998,"No"]
[null,"07-03-2018","19:00","NMI-25000115481","Rural Short","Asset Failure","LV",1,157.33000000000001,3.4880000000000002E-3,2.1999999999999999E-5,"No"]
[null,"07-03-2018","20:51","REC-10049","Rural Long","Weather",null,39,16.27,0.73003499999999999,4.4879000000000002E-2,"No"]
[null,"08-03-2018","08:30","DT-2983","Rural Short","Planned",null,76,208.32,null,null,"No"]
[null,"08-03-2018","08:40","DT-1324","Rural Short","Planned",null,5,247.77,null,null,"No"]
[null,"08-03-2018","09:00","DT-1998","Urban","Planned",null,127,159.52000000000001,null,null,"No"]
[null,"08-03-2018","09:01","22HD403 MIDDLE POINT","Rural Short","Planned",null,32,175.08,null,null,"No"]
[null,"08-03-2018","09:49","22PC308 TOWNSHIP","Rural Short","Asset Failure","HV",192,49.93,0.21253900000000001,4.2560000000000002E-3,"No"]
[null,"08-03-2018","11:33","PSPT128947","Rural Short","Asset Failure","LV",1,48.25,1.07E-3,2.1999999999999999E-5,"No"]
[null,"08-03-2018","17:06","DT-6411","Rural Short","Unknown","Unknown",1,75.55,1.6750000000000001E-3,2.1999999999999999E-5,"No"]
[null,"09-03-2018","14:27","NMI-25000743593","Rural Short","Asset Failure","LV",1,55.77,1.2359999999999999E-3,2.1999999999999999E-5,"No"]
[null,"09-03-2018","18:09","DT-10138","Rural Short","Unknown","Unknown",1,141.27000000000001,3.1319999999999998E-3,2.1999999999999999E-5,"No"]
[null,"09-03-2018","19:36","DT-1932","Urban","Overloads",null,113,58.42,0.205648,3.5200000000000001E-3,"No"]
[null,"09-03-2018","20:44","DT-0265","Rural Short","Asset Failure","HV",21,201.25,9.3691999999999998E-2,4.66E-4,"No"]
[null,"10-03-2018","05:12","22KA19 TINDAL 1","Rural Short","Weather",null,245,5.23,2.8424000000000001E-2,5.4310000000000001E-3,"No"]
[null,"10-03-2018","09:05","DT-1927","Urban","Planned",null,1,218.17,null,null,"No"]
[null,"10-03-2018","09:20","22KA19 TINDAL 1","Rural Short","Weather",null,245,19.87,0.107904,5.4310000000000001E-3,"No"]
[null,"10-03-2018","11:12","NMI-25000492219","Urban","Asset Failure","LV",1,109.08,3.398E-3,3.1000000000000001E-5,"No"]
[null,"11-03-2018","08:47","DT-1054","Urban","Planned",null,27,282,null,null,"No"]
[null,"11-03-2018","18:27","DT-6186","Rural Short","Animal","Animal Impact",2,67.92,3.0109999999999998E-3,4.3999999999999999E-5,"No"]
[null,"11-03-2018","18:45","66 MR-SY","Rural Short","Weather",null,345,12.28,9.3947000000000003E-2,7.6480000000000003E-3,"No"]
[null,"12-03-2018","01:29","DT-0220","Rural Short","Unknown","Unknown",2,177.75,7.8810000000000009E-3,4.3999999999999999E-5,"No"]
[null,"12-03-2018","08:00","DT-8059","Urban","Planned",null,0,49.7,null,null,"No"]
[null,"12-03-2018","11:03","DT-3332","Rural Short","Network Business","Network Error",1,12.03,2.6699999999999998E-4,2.1999999999999999E-5,"No"]
[null,"12-03-2018","14:15","NMI-25000399628","Urban","Weather",null,1,80.930000000000007,2.5209999999999998E-3,3.1000000000000001E-5,"No"]
[null,"12-03-2018","19:06","DT-0664","Rural Short","Weather",null,9,434.63,8.6719000000000004E-2,2.0000000000000001E-4,"No"]
[null,"13-03-2018","09:02","SEC-22EV0134","Rural Short","Planned",null,130,148.28,null,null,"No"]
[null,"13-03-2018","09:14","22MT07 ACACIA","Rural Short","Planned",null,9,256.27,null,null,"No"]
[null,"13-03-2018","14:50","DT-1907","Rural Short","Network Business","Network Error",1,10.220000000000001,2.2599999999999999E-4,2.1999999999999999E-5,"No"]
[null,"14-03-2018","08:30","DT-1687","Rural Short","Planned",null,9,162.53,null,null,"No"]
[null,"14-03-2018","09:20","DT-10184","Rural Short","Planned",null,0,204.83,null,null,"No"]
[null,"14-03-2018","09:35","22SY02 MCMINNS","Rural Short","Planned",null,140,151.9,null,null,"No"]
[null,"14-03-2018","20:24","11CA16 NAKARA","Urban","Planned",null,91,156.4,null,null,"No"]
[null,"14-03-2018","21:01","11BE13 KORMILDA","Rural Short","Planned",null,109,149.97,null,null,"No"]
[null,"15-03-2018","08:30","DT-1663","Rural Short","Planned",null,9,180.25,null,null,"No"]
[null,"15-03-2018","10:16","DT-0137","Rural Short","Animal","Animal Impact",6,121.33,1.6139000000000001E-2,1.3300000000000001E-4,"No"]
[null,"15-03-2018","15:22","22PA202 HOWARD SPRINGS","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",949,73.88,1.554387,2.1038000000000001E-2,"No"]
[null,"15-03-2018","16:36","SWH-0092","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",350,292,2.265673,7.7590000000000003E-3,"No"]
[null,"15-03-2018","18:43","DT-0404","Rural Short","Network Business","Network Error",2,44,1.951E-3,4.3999999999999999E-5,"No"]
[null,"16-03-2018","07:57","DT-8059","Urban","Planned",null,0,119.87,null,null,"No"]
[null,"16-03-2018","09:10","11CA16 NAKARA","Urban","Planned",null,160,294.93,null,null,"No"]
[null,"16-03-2018","09:22","NMI-25000752644","Urban","Network Business","Network Error",1,123.35,3.8430000000000001E-3,3.1000000000000001E-5,"No"]
[null,"16-03-2018","11:29","22BA04 TOWN","Rural Short","Planned",null,1,101.13,null,null,"No"]
[null,"16-03-2018","16:42","NMI-25000136306","Rural Short","Asset Failure","LV",1,534.91999999999996,1.1859E-2,2.1999999999999999E-5,"No"]
[null,"16-03-2018","21:26","NMI-25000115268","Urban","Asset Failure","LV",1,154.19999999999999,4.8040000000000001E-3,3.1000000000000001E-5,"No"]
[null,"17-03-2018","00:10","NMI-25000161452","Urban","Weather",null,1,3712,0.11564199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000162509","Urban","Weather",null,1,6624,0.20636199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000303688","Urban","Weather",null,1,3727,0.11611,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000306278","Urban","Weather",null,1,2077,6.4706E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000325871","Urban","Weather",null,1,6338,0.19745199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000344749","Urban","Weather",null,1,2077,6.4706E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000402738","Urban","Weather",null,1,3742,0.116577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000423840","Urban","Weather",null,1,3742,0.116577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000431176","Urban","Weather",null,1,8228,0.256332,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000440045","Urban","Weather",null,1,4012,0.124988,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000483547","Urban","Weather",null,1,3938,0.122683,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000531554","Urban","Weather",null,1,6728,0.20960200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000603865","Urban","Weather",null,1,6293,0.19605,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000607353","Urban","Weather",null,1,6714,0.20916499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000607361","Urban","Weather",null,1,6278,0.19558200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000639059","Urban","Weather",null,1,5273,0.164273,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000644420","Urban","Weather",null,1,6624,0.20636199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000669659","Urban","Weather",null,1,2362,7.3584999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000790713","Urban","Weather",null,1,5047,0.15723200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000810669","Urban","Weather",null,1,2077,6.4706E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000853780","Urban","Weather",null,1,1207,3.7601999999999997E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000868250","Urban","Weather",null,1,4012,0.124988,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000879803","Urban","Weather",null,1,6728,0.20960200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","00:10","NMI-25000888927","Urban","Weather",null,1,6624,0.20636199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000172036","Urban","Weather",null,1,780,2.4299999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000175205","Urban","Weather",null,1,4771,0.14863399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000303012","Urban","Weather",null,1,780,2.4299999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000404966","Urban","Weather",null,1,7684,0.23938400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000571312","Urban","Weather",null,1,780,2.4299999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000690573","Urban","Weather",null,1,7712,0.240257,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000763278","Urban","Weather",null,1,7684,0.23938400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000781694","Urban","Weather",null,1,4502,0.14025399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:02","NMI-25000794224","Urban","Weather",null,1,4786,0.14910100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:38","NMI-25000139927","Urban","Weather",null,1,1899,5.9160999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:38","NMI-25000501284","Urban","Weather",null,1,3340,0.10405300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:38","NMI-25000546452","Urban","Weather",null,1,3354,0.104489,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:38","NMI-25000707540","Urban","Weather",null,1,4667,0.145394,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000110658","Rural Short","Weather",null,1,9638,0.21366499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000110772","Rural Short","Weather",null,1,13841,0.30684099999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000110830","Rural Short","Weather",null,1,12160,0.26957500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000110947","Rural Short","Weather",null,1,6263,0.138845,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000112067","Rural Short","Weather",null,1,13299,0.29482599999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000112124","Rural Short","Weather",null,1,9113,0.20202600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000112644","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000113254","Rural Short","Weather",null,1,3607,7.9963999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000113899","Rural Short","Weather",null,1,9503,0.210672,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000114915","Rural Short","Weather",null,1,12309,0.27287800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000116142","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000116606","Rural Short","Weather",null,1,10841,0.24033399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000117073","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000117560","Rural Short","Weather",null,1,9159,0.203046,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000117825","Rural Short","Weather",null,1,6622,0.14680299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000118022","Rural Short","Weather",null,1,6622,0.14680299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000118682","Rural Short","Weather",null,1,7718,0.1711,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000120359","Rural Short","Weather",null,1,10842,0.24035599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000123963","CBD","Weather",null,1,4837,1.3002689999999999,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","01:55","NMI-25000126446","Urban","Weather",null,1,3202,9.9753999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000127071","Urban","Weather",null,1,3682,0.114708,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000129176","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000134340","Rural Short","Weather",null,1,9099,0.20171600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000134845","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000135223","Urban","Weather",null,1,3787,0.117979,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000135249","Urban","Weather",null,1,5212,0.16237299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000135506","Urban","Weather",null,1,6532,0.20349500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000135926","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000137179","CBD","Weather",null,1,4762,1.280108,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","01:55","NMI-25000137618","Urban","Weather",null,1,12774,0.39795599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000139357","Urban","Weather",null,1,6232,0.19414899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000139372","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000139489","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000139992","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000140844","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000141901","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000142252","CBD","Weather",null,1,3427,0.92123699999999997,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","01:55","NMI-25000142559","Urban","Weather",null,1,10842,0.33776800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000142822","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000143697","Urban","Weather",null,1,6203,0.193246,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000144102","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000144614","Urban","Weather",null,1,3982,0.124054,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000144836","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000145487","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000146148","Rural Short","Weather",null,1,7613,0.16877300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000146741","Urban","Weather",null,1,6232,0.19414899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000146774","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000146782","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000147269","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000148044","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000148688","Urban","Weather",null,1,6412,0.19975699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149010","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149330","Urban","Weather",null,1,8063,0.25119200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149645","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149686","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149843","Urban","Weather",null,1,3742,0.116577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149869","Urban","Weather",null,1,6442,0.20069200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000149892","Urban","Weather",null,1,9023,0.28109899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000150091","Urban","Weather",null,1,6397,0.19928999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000150133","Urban","Weather",null,1,8063,0.25119200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000150182","Rural Short","Weather",null,1,13449,0.298151,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000150803","Urban","Weather",null,1,11951,0.37231700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000151207","Urban","Weather",null,1,11875,0.36994899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000151726","Urban","Weather",null,1,3382,0.105362,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000153324","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000153423","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000153457","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000153498","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000153886","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154091","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154298","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154554","Rural Short","Weather",null,1,10945,0.24263999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154811","Urban","Weather",null,1,6548,0.20399400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154902","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000154926","Rural Short","Weather",null,1,2272,5.0368000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000155288","Urban","Weather",null,1,6697,0.20863599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000155387","Urban","Weather",null,1,10490,0.32680100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000155395","Urban","Weather",null,1,7884,0.245615,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000155429","Urban","Weather",null,1,10841,0.33773599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000155611","Urban","Weather",null,1,5167,0.160971,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000156278","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000156510","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000156534","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000156674","Urban","Weather",null,1,6292,0.196019,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157250","Rural Short","Weather",null,1,4777,0.105901,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157517","Urban","Weather",null,1,7763,0.24184600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157671","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157770","Rural Short","Weather",null,1,8183,0.18140899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157862","Urban","Weather",null,1,11201,0.34895199999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157937","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000157953","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000158084","Urban","Weather",null,1,7763,0.24184600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000158430","Rural Short","Weather",null,1,9023,0.20003099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000158515","Urban","Weather",null,1,12324,0.38393699999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000158654","Rural Short","Weather",null,1,7989,0.17710799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000159256","Urban","Weather",null,1,11111,0.34614800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000159355","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000159703","Urban","Weather",null,1,2197,6.8444000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000159810","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160019","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160033","Urban","Weather",null,1,11979,0.37318899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160230","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160289","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160495","Rural Short","Weather",null,1,6592,0.14613799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160529","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160537","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160545","Rural Short","Weather",null,1,2392,5.3027999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160628","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160769","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160802","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000160842","Urban","Weather",null,1,10490,0.32680100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161023","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161098","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161122","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161164","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161535","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161569","Urban","Weather",null,1,8078,0.25165900000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161576","Urban","Weather",null,1,6862,0.21377599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161719","Rural Short","Weather",null,1,2287,5.0701000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161873","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000161899","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162193","Rural Short","Weather",null,1,11934,0.26456499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162268","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162301","Urban","Weather",null,1,5122,0.15956899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162390","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162466","Urban","Weather",null,1,6532,0.20349500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162549","Rural Short","Weather",null,1,5047,0.111887,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162707","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162806","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000162895","Rural Short","Weather",null,1,13360,0.296178,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000163142","Rural Short","Weather",null,1,6652,0.14746799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000163331","Urban","Weather",null,1,6382,0.198822,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000163828","Rural Short","Weather",null,1,7673,0.170103,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164019","Rural Short","Weather",null,1,6592,0.14613799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164082","Urban","Weather",null,1,8063,0.25119200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164181","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164406","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164495","Rural Short","Weather",null,1,6562,0.14547299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164660","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000164776","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000165569","Rural Short","Weather",null,1,9023,0.20003099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000165602","Rural Short","Weather",null,1,4822,0.10689899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000166146","Rural Short","Weather",null,1,6337,0.140485,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000166212","Rural Short","Weather",null,1,12085,0.26791300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000166277","Rural Short","Weather",null,1,6667,0.14780099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000166765","Rural Short","Weather",null,1,10765,0.238649,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000166856","Urban","Weather",null,1,6337,0.19742000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000167135","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000167176","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000167457","Rural Short","Weather",null,1,3443,7.6327999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000167663","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168083","Urban","Weather",null,1,10841,0.33773599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168223","Rural Short","Weather",null,1,6337,0.140485,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168397","Rural Short","Weather",null,1,6157,0.13649500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168421","Rural Short","Weather",null,1,6427,0.14248,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168661","Rural Short","Weather",null,1,8092,0.179392,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000168736","Rural Short","Weather",null,1,12040,0.26691500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000169117","Urban","Weather",null,1,9233,0.28764099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000169247","Rural Short","Weather",null,1,6307,0.13982,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000169833","Urban","Weather",null,1,11904,0.37085299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000170270","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000170635","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000170692","Urban","Weather",null,1,9053,0.28203400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000171097","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000171107","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000171344","Urban","Weather",null,1,11979,0.37318899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000171690","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000171817","Urban","Weather",null,1,11979,0.37318899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000172028","Urban","Weather",null,1,4867,0.15162500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000172219","Urban","Weather",null,1,3592,0.111904,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000172267","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000173975","Urban","Weather",null,1,9053,0.28203400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000174040","Urban","Weather",null,1,11979,0.37318899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000174247","Urban","Weather",null,1,9083,0.282968,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000174874","Urban","Weather",null,1,11920,0.37135099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000175097","Urban","Weather",null,1,5077,0.158167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000175849","Urban","Weather",null,1,6548,0.20399400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000176020","Urban","Weather",null,1,5062,0.15770000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000176419","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000176797","Urban","Weather",null,1,7989,0.248886,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000176938","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000178586","Rural Short","Weather",null,1,3352,7.4311000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000179238","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000179881","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000181525","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000183792","Rural Short","Weather",null,1,9428,0.209009,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000183891","Urban","Weather",null,1,2017,6.2837000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000184741","Rural Short","Weather",null,1,13689,0.30347200000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000184873","Rural Short","Weather",null,1,13464,0.29848400000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000185204","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000187217","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000187298","Rural Short","Weather",null,1,10841,0.24033399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000187316","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000187605","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000191368","Rural Short","Weather",null,1,3607,7.9963999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000197586","Rural Short","Weather",null,1,4777,0.105901,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000199450","Rural Short","Weather",null,1,4822,0.10689899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000201744","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000208367","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000211990","Rural Short","Weather",null,1,6248,0.138512,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000213094","Urban","Weather",null,1,2167,6.7510000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000213333","Rural Short","Weather",null,1,5032,0.111554,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000213929","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000214309","Rural Short","Weather",null,1,13704,0.30380400000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000222037","Rural Short","Weather",null,1,13404,0.297153,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000223507","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000223521","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000223539","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000225329","Urban","Weather",null,1,3787,0.117979,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000226392","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000229676","Urban","Weather",null,1,13719,0.427396,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000229684","Urban","Weather",null,1,13719,0.427396,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000230338","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000230593","Urban","Weather",null,1,3682,0.114708,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000230932","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000232399","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000232795","Urban","Weather",null,1,5273,0.164273,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000233463","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000236145","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000236153","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238041","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238067","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238132","Urban","Weather",null,1,2092,6.5172999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238297","Urban","Weather",null,1,11920,0.37135099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238370","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238479","Urban","Weather",null,1,5347,0.166578,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238537","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000238810","Urban","Weather",null,1,4762,0.14835400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000239246","Urban","Weather",null,1,4867,0.15162500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000240108","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000240116","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000240527","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000241483","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000242357","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000242365","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000242646","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000243230","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000243248","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000243289","Urban","Weather",null,1,11920,0.37135099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000243842","Rural Short","Weather",null,1,4897,0.10856200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000244287","Rural Short","Weather",null,1,7673,0.170103,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000244493","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000245475","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000245717","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000245723","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000245955","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000246177","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000248255","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000248882","Urban","Weather",null,1,10841,0.33773599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000250312","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000250328","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000250336","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000250344","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000250385","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000251500","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000251518","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000251672","Rural Short","Weather",null,1,7688,0.170435,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000251815","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000251821","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000252728","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000252736","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000252803","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000255326","Urban","Weather",null,1,3563,0.111,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000256696","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000257612","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000257644","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000257652","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000257693","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000259709","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000259723","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000260212","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000260228","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000260483","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262140","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262208","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262222","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262230","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262339","Rural Short","Weather",null,1,6488,0.14383299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262545","Rural Short","Weather",null,1,6488,0.14383299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262604","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262644","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000262711","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263206","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263220","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263404","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263412","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263428","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000263444","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000264154","Urban","Weather",null,1,3757,0.117044,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000264335","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000264369","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000264915","Urban","Weather",null,1,12279,0.38253500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000269038","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000272544","Rural Short","Weather",null,1,6532,0.14480799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000273304","Rural Short","Weather",null,1,6562,0.14547299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000273823","Rural Short","Weather",null,1,6532,0.14480799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000273831","Rural Short","Weather",null,1,10870,0.240977,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000274326","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000274581","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000274599","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000274609","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000274631","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000280367","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000281614","Urban","Weather",null,1,2017,6.2837000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000291613","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000292700","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000292724","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000292740","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000294085","Rural Short","Weather",null,1,2167,4.8039999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000295463","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000296405","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000296726","Urban","Weather",null,1,3742,0.116577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000297351","Rural Short","Weather",null,1,10989,0.243615,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000298608","Urban","Weather",null,1,3667,0.11423999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000300488","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000300506","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000301362","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000301577","Rural Short","Weather",null,1,10720,0.237652,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000301825","Urban","Weather",null,1,3563,0.111,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000302609","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000302617","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000303332","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000303904","Urban","Weather",null,1,9608,0.29932399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000304439","Urban","Weather",null,1,10720,0.33396700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000304520","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000304744","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000305379","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000305486","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000305651","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000306089","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000306286","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000306817","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000310660","Rural Short","Weather",null,1,5062,0.11222,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000312053","Urban","Weather",null,1,10701,0.33337499999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000312820","Urban","Weather",null,1,6232,0.19414899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000313885","Rural Short","Weather",null,1,6608,0.14649300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000313911","Rural Short","Weather",null,1,6518,0.14449799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000314199","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000314462","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000314776","Rural Short","Weather",null,1,10841,0.24033399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000314826","Urban","Weather",null,1,2017,6.2837000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000315818","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000315824","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000316120","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000317233","Rural Short","Weather",null,1,6697,0.14846599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000317282","Urban","Weather",null,1,6217,0.19368199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000317431","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000318280","Rural Short","Weather",null,1,13689,0.30347200000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000320148","Urban","Weather",null,1,10433,0.32502599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000321369","Urban","Weather",null,1,6562,0.20443,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000321567","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000321963","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000322051","Urban","Weather",null,1,11920,0.37135099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000322812","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000323297","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000326301","Rural Short","Weather",null,1,13719,0.30413699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000326390","Urban","Weather",null,1,6488,0.202125,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000327827","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000328528","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000328627","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000330089","Rural Short","Weather",null,1,7673,0.170103,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000331368","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000332316","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000334022","Rural Short","Weather",null,1,4852,0.10756400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000335302","Rural Long","Weather",null,1,13795,15.874568,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000336127","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000336928","Rural Short","Weather",null,1,10720,0.237652,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000337396","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000337446","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000338569","Rural Short","Weather",null,1,8273,0.18340400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000339808","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000343460","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000344582","Urban","Weather",null,1,9307,0.28994700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000347684","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000347750","Urban","Weather",null,1,3682,0.114708,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000347819","Urban","Weather",null,1,3682,0.114708,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000349014","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000349599","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000350797","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000351639","Rural Long","Weather",null,1,9443,10.866512999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000352544","Rural Short","Weather",null,1,9293,0.20601700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000353799","Rural Long","Weather",null,1,9503,10.935558,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000355409","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000355878","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000357899","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000358015","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000358096","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000359359","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000359367","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000359432","Urban","Weather",null,1,10682,0.332783,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000362683","Urban","Weather",null,1,9307,0.28994700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000363327","Urban","Weather",null,1,6217,0.19368199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000363590","Urban","Weather",null,1,5108,0.159133,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000364598","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000366553","Rural Short","Weather",null,1,9608,0.21299999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000367526","Urban","Weather",null,1,7884,0.245615,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000369977","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000370647","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000371579","Rural Short","Weather",null,1,4852,0.10756400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000371793","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000372328","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000372674","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000373979","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000374564","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000377369","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000380654","Rural Short","Weather",null,1,4897,0.10856200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000381158","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000381370","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000381967","Rural Short","Weather",null,1,7718,0.1711,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000382236","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000382426","Urban","Weather",null,1,3652,0.113773,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000382666","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000384191","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000384357","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000384620","Rural Short","Weather",null,1,9099,0.20171600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000384976","Urban","Weather",null,1,11111,0.34614800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000385019","Rural Short","Weather",null,1,9008,0.19969899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000385230","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000385495","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000386477","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000386923","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000387006","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000387269","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000388508","Urban","Weather",null,1,13360,0.41621200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000389091","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000389968","Rural Long","Weather",null,1,12175,14.010357000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000390851","Rural Short","Weather",null,1,6502,0.14414299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000391734","Urban","Weather",null,1,5273,0.164273,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000391742","Urban","Weather",null,1,5273,0.164273,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000393878","Urban","Weather",null,1,6188,0.19277900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000395379","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000395395","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000395413","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000395859","Urban","Weather",null,1,6532,0.20349500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000396196","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000397796","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000398183","Rural Short","Weather",null,1,9428,0.209009,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000399158","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000402530","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000402714","Urban","Weather",null,1,4927,0.15349399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000402720","Urban","Weather",null,1,3652,0.113773,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000403182","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000404338","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000404346","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000405008","Rural Short","Weather",null,1,8092,0.179392,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000405502","Rural Short","Weather",null,1,9083,0.20136100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000405880","Rural Short","Weather",null,1,6248,0.138512,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000406194","Urban","Weather",null,1,9307,0.28994700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000408173","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000409923","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000410602","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000410725","Rural Short","Weather",null,1,13404,0.297153,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000411096","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000412654","Rural Short","Weather",null,1,13569,0.300811,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000413124","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000414009","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000414477","Rural Short","Weather",null,1,6412,0.142148,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000414917","Rural Short","Weather",null,1,13434,0.297819,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000415939","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000416509","Rural Short","Weather",null,1,9608,0.21299999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000417554","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000418018","Urban","Weather",null,1,11111,0.34614800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000418180","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000419766","Urban","Weather",null,1,6488,0.202125,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000420120","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000420204","Urban","Weather",null,1,9653,0.30072599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000421291","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000423477","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000423767","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000424351","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000425053","Rural Short","Weather",null,1,13704,0.30380400000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000425061","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000425291","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000425341","Urban","Weather",null,1,6188,0.19277900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000426110","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000426380","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000426456","Urban","Weather",null,1,9593,0.29885699999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000426794","Rural Short","Weather",null,1,6307,0.13982,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000428799","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000428809","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000429087","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000429979","Urban","Weather",null,1,10701,0.33337499999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000431861","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000431894","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000432081","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000433286","Rural Short","Weather",null,1,6562,0.14547299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000434441","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000434459","Urban","Weather",null,1,6577,0.204897,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000434623","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000434789","Rural Long","Weather",null,1,10998,12.655925999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000436068","Rural Short","Weather",null,1,6562,0.14547299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000437642","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000437733","Rural Short","Weather",null,1,12054,0.26722499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000438021","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000438939","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000440029","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000440128","Urban","Weather",null,1,9307,0.28994700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000441092","Urban","Weather",null,1,13434,0.418518,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000441422","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000442287","Rural Short","Weather",null,1,7989,0.17710799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000442759","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000442965","Urban","Weather",null,1,9593,0.29885699999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000443063","Rural Short","Weather",null,1,3427,7.5972999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000444094","Rural Short","Weather",null,1,10841,0.24033399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000445281","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000445365","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000445456","Urban","Weather",null,1,9248,0.288109,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000447865","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000449985","Rural Short","Weather",null,1,2227,4.9369999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000450936","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000451629","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000451645","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000451876","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000452534","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000452591","Rural Short","Weather",null,1,11934,0.26456499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000452766","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000453334","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000454028","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000454714","Rural Short","Weather",null,1,9038,0.20036399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000456099","Urban","Weather",null,1,6562,0.20443,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000456742","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000456775","Urban","Weather",null,1,3532,0.11003499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000457252","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000457757","Urban","Weather",null,1,3352,0.10442700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000458242","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000458301","Urban","Weather",null,1,3742,0.116577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000459003","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000459218","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000459224","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000459951","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000460240","Rural Short","Weather",null,1,3457,7.6637999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000460380","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000460422","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000462335","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000463185","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000463466","Rural Short","Weather",null,1,13464,0.29848400000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000463565","Rural Short","Weather",null,1,12339,0.27354299999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000464168","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000466246","Rural Short","Weather",null,1,11201,0.24831500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000466361","Rural Short","Weather",null,1,5753,0.12753800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000466980","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000469653","Rural Short","Weather",null,1,6352,0.140818,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000469835","Urban","Weather",null,1,4927,0.15349399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000469942","Rural Short","Weather",null,1,12324,0.27321099999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000472847","Rural Short","Weather",null,1,4927,0.109227,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000476286","Urban","Weather",null,1,11111,0.34614800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000476799","Rural Short","Weather",null,1,13554,0.300479,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000477440","Urban","Weather",null,1,5152,0.16050300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000477608","Urban","Weather",null,1,6638,0.20679800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000477945","Rural Short","Weather",null,1,9099,0.20171600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000478555","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000478679","Urban","Weather",null,1,3307,0.10302500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000478761","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000478943","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000479982","Urban","Weather",null,1,4852,0.15115700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000480082","Urban","Weather",null,1,12279,0.38253500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000480743","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000480784","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000480792","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000481023","Urban","Weather",null,1,7884,0.245615,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000481287","Urban","Weather",null,1,5138,0.16006699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000481634","Rural Short","Weather",null,1,7778,0.172431,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000482301","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000483705","Urban","Weather",null,1,11951,0.37231700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000483860","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000483935","Urban","Weather",null,1,6548,0.20399400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000484124","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000484414","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000484891","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000484933","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000485017","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000485031","Urban","Weather",null,1,13674,0.42599500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000485313","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000485592","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000485800","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000486047","Rural Short","Weather",null,1,3412,7.5641E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000489099","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000490215","Rural Short","Weather",null,1,11934,0.26456499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000490874","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000491435","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000491568","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000493091","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000493371","Rural Short","Weather",null,1,5753,0.12753800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000493470","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000497281","Rural Short","Weather",null,1,9608,0.21299999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000497456","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000497497","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000498776","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000498784","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000499767","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000499790","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000500304","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000500476","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000500799","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000502330","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000502760","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000506647","Rural Short","Weather",null,1,9053,0.20069600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000506960","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000507041","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000510808","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000511226","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000511747","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000512644","Urban","Weather",null,1,11920,0.37135099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000513197","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000513361","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000513610","Rural Short","Weather",null,1,13689,0.30347200000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000515978","Rural Short","Weather",null,1,10842,0.24035599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000516951","Urban","Weather",null,1,5062,0.15770000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000519920","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000520275","Urban","Weather",null,1,4927,0.15349399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000521218","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000521596","Rural Short","Weather",null,1,9503,0.210672,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000521860","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000521992","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000522668","Urban","Weather",null,1,6337,0.19742000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000523039","Rural Short","Weather",null,1,4822,0.10689899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000523114","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000523303","Urban","Weather",null,1,2047,6.3770999999999994E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000524283","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000524978","Urban","Weather",null,1,9083,0.282968,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000525281","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000525430","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000525778","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000526132","Rural Short","Weather",null,1,9053,0.20069600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000526297","Urban","Weather",null,1,3607,0.112371,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000526693","Urban","Weather",null,1,7884,0.245615,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000528079","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000529176","Urban","Weather",null,1,13795,0.42976399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000530449","Rural Short","Weather",null,1,7613,0.16877300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000530522","Rural Short","Weather",null,1,3637,8.0629000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000530564","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000530754","Urban","Weather",null,1,8318,0.25913599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000531050","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000531190","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000531968","Rural Short","Weather",null,1,12369,0.27420899999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000531975","Rural Short","Weather",null,1,5182,0.11488,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000533716","Rural Short","Weather",null,1,4927,0.109227,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000534358","Rural Short","Weather",null,1,12369,0.27420899999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000535034","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000535488","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000537658","Urban","Weather",null,1,3563,0.111,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000537939","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000539794","Rural Short","Weather",null,1,6488,0.14383299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000540003","Rural Short","Weather",null,1,4822,0.10689899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000540380","Rural Short","Weather",null,1,9023,0.20003099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000540679","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000543531","Urban","Weather",null,1,10841,0.33773599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000544927","Rural Short","Weather",null,1,6307,0.13982,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000546287","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000547680","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000547698","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000548373","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000549091","Rural Short","Weather",null,1,11904,0.26390000000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000550190","Urban","Weather",null,1,2002,6.2370000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000551040","Rural Short","Weather",null,1,2287,5.0701000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000551973","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000552771","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000553714","Rural Short","Weather",null,1,6532,0.14480799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000554280","Rural Short","Weather",null,1,6367,0.14115,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000554348","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000554554","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000554605","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000555239","Rural Short","Weather",null,1,4897,0.10856200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000555255","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000555512","Urban","Weather",null,1,6382,0.198822,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000555585","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556115","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556352","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556360","Urban","Weather",null,1,9083,0.282968,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556542","Urban","Weather",null,1,7763,0.24184600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556740","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000556809","Urban","Weather",null,1,6532,0.20349500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000557473","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000557509","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000557721","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000557862","Rural Short","Weather",null,1,11979,0.26556299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000558398","Rural Short","Weather",null,1,6712,0.14879800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000558416","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000558489","Urban","Weather",null,1,9233,0.28764099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000558729","Rural Short","Weather",null,1,12190,0.27023999999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000559082","Rural Short","Weather",null,1,5182,0.11488,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000559586","Rural Short","Weather",null,1,13674,0.30313899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000561741","Rural Short","Weather",null,1,12234,0.27121600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000562367","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000562796","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000565858","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000567449","Urban","Weather",null,1,7568,0.23577100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000567655","Rural Short","Weather",null,1,6697,0.14846599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000567894","Urban","Weather",null,1,12279,0.38253500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000568934","Urban","Weather",null,1,2197,6.8444000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000568983","Urban","Weather",null,1,7553,0.23530300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000569066","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000569801","Urban","Weather",null,1,5108,0.159133,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000570207","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000570958","Rural Short","Weather",null,1,9038,0.20036399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000570966","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000571071","Urban","Weather",null,1,12071,0.37605499999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000571089","Urban","Weather",null,1,6488,0.202125,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000571659","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000571849","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000571908","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000572093","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000572274","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000572373","Urban","Weather",null,1,5077,0.158167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000572813","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000573280","Urban","Weather",null,1,9563,0.29792200000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000573760","Rural Short","Weather",null,1,9188,0.20368900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000573968","Urban","Weather",null,1,6203,0.193246,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000574841","Urban","Weather",null,1,13719,0.427396,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000575071","Urban","Weather",null,1,11111,0.34614800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000575601","Rural Short","Weather",null,1,6427,0.14248,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000576441","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000577240","Urban","Weather",null,1,5062,0.15770000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000577563","Urban","Weather",null,1,6712,0.20910300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000577893","Urban","Weather",null,1,11951,0.37231700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000578100","Urban","Weather",null,1,5152,0.16050300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000578735","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000579156","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000579345","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000580065","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000581047","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000582273","Urban","Weather",null,1,3967,0.123586,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000582323","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000582976","Urban","Weather",null,1,5032,0.15676499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000583140","Rural Short","Weather",null,1,7673,0.170103,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000583173","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000583181","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000583289","Rural Short","Weather",null,1,9053,0.20069600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000583297","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000584576","Rural Short","Weather",null,1,5753,0.12753800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000586160","Rural Short","Weather",null,1,13719,0.30413699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000586481","Urban","Weather",null,1,4897,0.152559,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000587371","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000587884","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000588958","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000592280","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000592777","Rural Short","Weather",null,1,7538,0.16711000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000592785","Rural Short","Weather",null,1,5077,0.112552,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000593635","Urban","Weather",null,1,9428,0.29371599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000593643","Rural Long","Weather",null,1,11277,12.976985000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000594393","Rural Short","Weather",null,1,2227,4.9369999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000594916","Urban","Weather",null,1,9608,0.29932399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000596647","Urban","Weather",null,1,6667,0.207701,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000596829","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000596845","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000597685","Rural Short","Weather",null,1,13689,0.30347200000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000598668","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000600020","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000600105","Urban","Weather",null,1,9038,0.28156599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000600441","Urban","Weather",null,1,6652,0.207234,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000600540","Rural Short","Weather",null,1,10854,0.240623,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601176","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601457","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601465","Urban","Weather",null,1,10701,0.33337499999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601746","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601912","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000601936","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000602109","Urban","Weather",null,1,13330,0.41527799999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000602221","Rural Short","Weather",null,1,12324,0.27321099999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000602429","Urban","Weather",null,1,2092,6.5172999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000602801","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603121","Urban","Weather",null,1,5047,0.15723200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603147","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603534","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603633","Urban","Weather",null,1,11904,0.37085299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603766","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603799","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000603956","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000604401","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000604474","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000604573","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000605143","Rural Short","Weather",null,1,4822,0.10689899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000605300","Rural Short","Weather",null,1,9263,0.20535200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000605324","Rural Short","Weather",null,1,12339,0.27354299999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000605409","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000606083","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000606389","Rural Short","Weather",null,1,7673,0.170103,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000606439","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000606686","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000608731","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000608864","Urban","Weather",null,1,9563,0.29792200000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609160","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609202","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609226","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609234","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609608","Urban","Weather",null,1,3652,0.113773,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000609895","Rural Short","Weather",null,1,11979,0.26556299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000610112","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000610367","Urban","Weather",null,1,9053,0.28203400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000611273","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000611281","Urban","Weather",null,1,11875,0.36994899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000613285","Urban","Weather",null,1,9608,0.29932399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000614978","Rural Short","Weather",null,1,9203,0.20402100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000616487","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000617435","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000617857","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000619480","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000620570","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000620606","Urban","Weather",null,1,10842,0.33776800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000620761","Urban","Weather",null,1,9443,0.294184,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000621604","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622402","Urban","Weather",null,1,10842,0.33776800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622519","Urban","Weather",null,1,9563,0.29792200000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622574","Urban","Weather",null,1,9563,0.29792200000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622582","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622717","Urban","Weather",null,1,8063,0.25119200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622780","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000622897","Urban","Weather",null,1,13299,0.41431200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000623094","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000624380","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000624794","Rural Short","Weather",null,1,6397,0.141815,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000625166","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000625693","Rural Short","Weather",null,1,3502,7.7635999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000626254","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000626287","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000626404","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000627284","Urban","Weather",null,1,4762,0.14835400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000627350","Rural Short","Weather",null,1,7688,0.170435,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000627573","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000628060","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000628358","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000629101","Rural Short","Weather",null,1,9233,0.20468700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000629330","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000629785","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000630075","Urban","Weather",null,1,6608,0.20586299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000632954","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000633241","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000633754","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000635024","Urban","Weather",null,1,7974,0.248419,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000636163","Rural Short","Weather",null,1,12219,0.27088299999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000636170","Urban","Weather",null,1,12114,0.37739499999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000636956","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000637458","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000637763","Rural Short","Weather",null,1,9233,0.20468700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000641122","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000641164","Rural Short","Weather",null,1,9233,0.20468700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000641171","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000641305","Rural Short","Weather",null,1,12071,0.26760200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000641957","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000642458","Urban","Weather",null,1,7778,0.242313,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000644118","Rural Short","Weather",null,1,6608,0.14649300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000644315","Rural Short","Weather",null,1,13374,0.29648799999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000644438","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000644703","Urban","Weather",null,1,5122,0.15956899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000645206","Rural Short","Weather",null,1,6592,0.14613799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000645345","Rural Short","Weather",null,1,13434,0.297819,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000645551","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000647169","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000647472","Rural Short","Weather",null,1,6638,0.14715800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000648637","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000648950","Urban","Weather",null,1,8273,0.25773400000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000649172","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000650024","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000650073","Rural Long","Weather",null,1,12175,14.010357000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","01:55","NMI-25000650544","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000651115","Urban","Weather",null,1,8078,0.25165900000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000651633","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000651690","Rural Short","Weather",null,1,6172,0.136827,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000652516","Rural Short","Weather",null,1,13330,0.29551300000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000653083","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000653265","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000654346","Urban","Weather",null,1,6188,0.19277900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000655435","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000655849","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000656211","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000656540","Rural Short","Weather",null,1,6157,0.13649500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000657687","Urban","Weather",null,1,4867,0.15162500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000657729","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000659866","Rural Short","Weather",null,1,13719,0.30413699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000660626","Urban","Weather",null,1,3697,0.115175,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000662357","Urban","Weather",null,1,3337,0.10396,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000662489","Urban","Weather",null,1,7989,0.248886,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000662705","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000662844","Rural Short","Weather",null,1,11201,0.24831500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000663612","Urban","Weather",null,1,9503,0.29605300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000664858","Rural Short","Weather",null,1,3727,8.2624000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000667125","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000667488","Urban","Weather",null,1,9443,0.294184,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000667538","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000667605","Rural Short","Weather",null,1,6337,0.140485,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000669476","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000669766","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000669809","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000670534","Urban","Weather",null,1,6532,0.20349500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000670817","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000671383","Rural Short","Weather",null,1,4867,0.10789700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000673627","Rural Short","Weather",null,1,10842,0.24035599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000673859","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000674312","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000674542","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000674591","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000675095","Urban","Weather",null,1,2092,6.5172999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000675350","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000675573","Rural Short","Weather",null,1,8183,0.18140899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000675914","Rural Short","Weather",null,1,10765,0.238649,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000676589","Rural Short","Weather",null,1,8092,0.179392,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000677001","Urban","Weather",null,1,9053,0.28203400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000678394","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000679179","Rural Short","Weather",null,1,3352,7.4311000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680015","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680402","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680475","Rural Short","Weather",null,1,13360,0.296178,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680574","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680699","Rural Short","Weather",null,1,6682,0.14813299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680772","Urban","Weather",null,1,6592,0.20536499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680816","Urban","Weather",null,1,9128,0.28437000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000680939","Rural Short","Weather",null,1,8318,0.18440200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000681112","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000681664","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000681755","Rural Short","Weather",null,1,12309,0.27287800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000681879","Rural Short","Weather",null,1,6697,0.14846599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000682082","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000682505","Urban","Weather",null,1,6217,0.19368199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000683866","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000684277","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000685086","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000686084","Rural Short","Weather",null,1,4867,0.10789700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000687081","Rural Short","Weather",null,1,4852,0.10756400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000688261","Rural Short","Weather",null,1,6427,0.14248,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000688849","Urban","Weather",null,1,5287,0.16470899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000689276","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000689599","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000690235","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000690797","Rural Short","Weather",null,1,12324,0.27321099999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000691621","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000692429","Rural Short","Weather",null,1,6667,0.14780099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000694095","Urban","Weather",null,1,1942,6.0499999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000694599","Rural Short","Weather",null,1,4867,0.10789700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000695670","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000697279","Rural Short","Weather",null,1,6532,0.14480799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000699268","Rural Short","Weather",null,1,5302,0.11754000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000699333","Urban","Weather",null,1,7763,0.24184600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000699341","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000699400","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000699905","Urban","Weather",null,1,3772,0.117511,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000700134","Urban","Weather",null,1,4822,0.150223,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000700753","Urban","Weather",null,1,11951,0.37231700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000701545","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000702871","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000703945","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000704134","Urban","Weather",null,1,9053,0.28203400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000704142","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000705941","Rural Short","Weather",null,1,12896,0.28589199999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000706444","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000707186","Rural Short","Weather",null,1,13360,0.296178,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000707623","Rural Short","Weather",null,1,7553,0.16744300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000707708","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000708516","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000709447","Urban","Weather",null,1,11875,0.36994899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000709546","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000709554","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000709562","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000710389","Urban","Weather",null,1,13719,0.427396,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000710613","Urban","Weather",null,1,9083,0.282968,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000711296","Rural Short","Weather",null,1,12190,0.27023999999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000711585","Rural Short","Weather",null,1,12384,0.27454099999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000712558","Rural Short","Weather",null,1,6352,0.140818,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000712847","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000712914","Urban","Weather",null,1,4837,0.15068999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000713878","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000714514","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000714562","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000716989","Urban","Weather",null,1,10765,0.33536899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000718745","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000719578","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000720149","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000720966","Rural Short","Weather",null,1,9307,0.20632700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000722233","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000722960","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000723034","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000724123","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000724486","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000725237","Rural Short","Weather",null,1,9653,0.21399799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000726532","Urban","Weather",null,1,13464,0.41945199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000727547","Rural Short","Weather",null,1,10433,0.23128899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000728264","Rural Short","Weather",null,1,12309,0.27287800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000728727","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000728974","Rural Short","Weather",null,1,6442,0.142813,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000730503","Rural Short","Weather",null,1,10720,0.237652,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000730543","Urban","Weather",null,1,13360,0.41621200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000730683","Rural Short","Weather",null,1,9608,0.21299999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000730858","Rural Short","Weather",null,1,7974,0.17677599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000731442","Urban","Weather",null,1,9623,0.29979099999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000731632","Urban","Weather",null,1,11875,0.36994899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000732051","Rural Short","Weather",null,1,10989,0.243615,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000732521","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000732761","Urban","Weather",null,1,6292,0.196019,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000733166","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000734460","Urban","Weather",null,1,10841,0.33773599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000735822","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000736862","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000737629","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000738215","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000741251","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000742876","Rural Short","Weather",null,1,6608,0.14649300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000743874","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000745095","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000745105","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000748108","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000748733","Urban","Weather",null,1,5287,0.16470899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000749154","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000749228","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000751045","Urban","Weather",null,1,5062,0.15770000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000751291","Rural Short","Weather",null,1,13299,0.29482599999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000754848","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000755177","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000755234","Rural Short","Weather",null,1,10841,0.24033399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000755814","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000756969","Urban","Weather",null,1,10945,0.340976,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000757066","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000757362","Urban","Weather",null,1,5273,0.164273,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000757486","Rural Short","Weather",null,1,9413,0.208677,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000758107","Rural Short","Weather",null,1,3637,8.0629000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000758641","Urban","Weather",null,1,11979,0.37318899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000758948","Urban","Weather",null,1,9413,0.29324899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000759467","Rural Short","Weather",null,1,6682,0.14813299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000759730","Rural Short","Weather",null,1,6458,0.14316799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000759896","Rural Short","Weather",null,1,7688,0.170435,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000760573","Urban","Weather",null,1,10956,0.34131899999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000761036","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000761655","Rural Short","Weather",null,1,13735,0.30449100000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000763916","Urban","Weather",null,1,3563,0.111,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000764350","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000764888","Rural Short","Weather",null,1,6562,0.14547299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000766488","Rural Short","Weather",null,1,6532,0.14480799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000767353","Urban","Weather",null,1,10479,0.326459,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000768039","Urban","Weather",null,1,7628,0.23763999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000770565","Urban","Weather",null,1,9142,0.284806,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000770895","Rural Short","Weather",null,1,8092,0.179392,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000771860","Rural Short","Weather",null,1,5062,0.11222,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000773293","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000773501","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000774796","Urban","Weather",null,1,12160,0.378828,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000774978","Urban","Weather",null,1,3427,0.106763,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000776264","Rural Short","Weather",null,1,6697,0.14846599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000777016","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000777360","Rural Short","Weather",null,1,6652,0.14746799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000782724","Rural Short","Weather",null,1,9503,0.210672,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000783178","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000784522","Rural Short","Weather",null,1,12384,0.27454099999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000785562","Rural Short","Weather",null,1,13464,0.29848400000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000786198","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000787047","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000788210","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000788770","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000790614","Rural Short","Weather",null,1,10479,0.23230899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000791132","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000791628","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000792096","Urban","Weather",null,1,3592,0.111904,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000794027","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000794051","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000794705","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000794911","Urban","Weather",null,1,3412,0.106296,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000795406","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000795414","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000795792","Rural Short","Weather",null,1,6502,0.14414299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000798366","Rural Short","Weather",null,1,13449,0.298151,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000799280","Urban","Weather",null,1,6217,0.19368199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000800307","Rural Short","Weather",null,1,10735,0.237984,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000800792","Rural Short","Weather",null,1,7688,0.170435,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000801262","Rural Short","Weather",null,1,12027,0.266627,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000803150","Urban","Weather",null,1,9083,0.282968,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000803778","Urban","Weather",null,1,3817,0.118913,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000804644","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000805725","Rural Short","Weather",null,1,8123,0.18007899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000806285","Urban","Weather",null,1,2212,6.8912000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000807894","Rural Short","Weather",null,1,5753,0.12753800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000808942","Urban","Weather",null,1,7688,0.239509,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000809018","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000816350","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000816855","Rural Short","Weather",null,1,9023,0.20003099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000819049","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000819931","Urban","Weather",null,1,10490,0.32680100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000820377","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000820542","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000822119","Rural Short","Weather",null,1,4897,0.10856200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000823395","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000823734","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000823999","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000824115","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000825161","Urban","Weather",null,1,3637,0.113306,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000826457","Urban","Weather",null,1,7613,0.23717199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000830351","Rural Short","Weather",null,1,6412,0.142148,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000830410","Rural Short","Weather",null,1,7718,0.1711,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000833428","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000833569","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000834681","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000835152","Rural Short","Weather",null,1,3337,7.3978000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000835481","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000836266","CBD","Weather",null,1,4837,1.3002689999999999,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","01:55","NMI-25000836357","Rural Short","Weather",null,1,10945,0.24263999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000837066","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000838492","Urban","Weather",null,1,8049,0.25075500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000838948","Rural Short","Weather",null,1,11860,0.26292500000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000843016","Rural Short","Weather",null,1,8109,0.17976900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000843865","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000844789","Urban","Weather",null,1,2287,7.1248000000000006E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000844987","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000845522","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000845985","Urban","Weather",null,1,6502,0.20256099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000847436","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000847931","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000849367","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000849481","Urban","Weather",null,1,4867,0.15162500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000849770","Rural Short","Weather",null,1,7688,0.170435,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000850440","Urban","Weather",null,1,8063,0.25119200000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000851638","Rural Short","Weather",null,1,3727,8.2624000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000852353","Urban","Weather",null,1,7673,0.239042,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000852873","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000857625","Urban","Weather",null,1,10735,0.33443400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000857930","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000858054","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000858062","Rural Short","Weather",null,1,10678,0.23672099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000858566","Urban","Weather",null,1,6292,0.196019,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000858797","Urban","Weather",null,1,9563,0.29792200000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000860274","Rural Short","Weather",null,1,10750,0.238317,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000862393","Urban","Weather",null,1,4897,0.152559,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000862880","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000863178","Rural Short","Weather",null,1,9023,0.20003099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000863896","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000865538","Urban","Weather",null,1,9307,0.28994700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000867070","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000867252","Urban","Weather",null,1,3622,0.11283799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000869786","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000871256","Urban","Weather",null,1,10479,0.326459,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000872179","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000874786","Urban","Weather",null,1,3502,0.1091,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000878878","Urban","Weather",null,1,7959,0.24795200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000879447","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000879811","Urban","Weather",null,1,9608,0.29932399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000882292","Urban","Weather",null,1,10678,0.33265800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000882558","Rural Short","Weather",null,1,12054,0.26722499999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000886823","Rural Short","Weather",null,1,6548,0.14516299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000888555","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000889462","Rural Short","Weather",null,1,3217,7.1318000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000889826","Urban","Weather",null,1,3443,0.107262,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000889925","Urban","Weather",null,1,12279,0.38253500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000889982","Rural Short","Weather",null,1,7884,0.17478099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000890271","Urban","Weather",null,1,10989,0.34234700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000891592","Urban","Weather",null,1,9159,0.28533599999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000892128","Rural Short","Weather",null,1,2212,4.9037999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000893299","Rural Short","Weather",null,1,8049,0.17843800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000893497","Rural Short","Weather",null,1,5182,0.11488,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000894553","Rural Short","Weather",null,1,7959,0.17644299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25000900873","Rural Short","Weather",null,1,8318,0.18440200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25009901525","Rural Short","Weather",null,1,7748,0.171766,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","01:55","NMI-25009903307","Urban","Weather",null,1,5257,0.163775,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000144309","Urban","Weather",null,1,7776,0.24225099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000152680","Urban","Weather",null,1,7531,0.23461799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000341905","Urban","Weather",null,1,6454,0.20106499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000366363","Urban","Weather",null,1,453,1.4113000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000487085","Urban","Weather",null,1,453,1.4113000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000487093","Urban","Weather",null,1,3589,0.11181000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000494932","Urban","Weather",null,1,8930,0.278202,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000509749","Urban","Weather",null,1,7719,0.24047499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000627105","Urban","Weather",null,1,7719,0.24047499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000629777","Urban","Weather",null,1,8930,0.278202,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000675789","Urban","Weather",null,1,8930,0.278202,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:14","NMI-25000856315","Urban","Weather",null,1,7719,0.24047499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","03:25","NMI-25000565949","Urban","Weather",null,1,6218,0.193713,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000159537","Urban","Weather",null,1,3329,0.10371,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000238727","Urban","Weather",null,1,2069,6.4457E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000243256","Urban","Weather",null,1,2249,7.0064000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000352263","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000413636","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000449169","Urban","Weather",null,1,3494,0.108851,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000453995","Urban","Weather",null,1,2069,6.4457E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000460035","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000594155","Urban","Weather",null,1,2054,6.3990000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000612116","Urban","Weather",null,1,2054,6.3990000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000634661","Urban","Weather",null,1,6406,0.19957,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000706197","Urban","Weather",null,1,4589,0.14296400000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000709694","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000832118","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","04:03","NMI-25000891584","Urban","Weather",null,1,7591,0.236487,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000161634","Rural Short","Weather",null,1,6333,0.14039599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000161866","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000178727","Rural Short","Weather",null,1,9244,0.20493,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000262181","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000262248","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000262594","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000280341","Rural Short","Weather",null,1,4922,0.109116,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000323140","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000376669","Rural Short","Weather",null,1,4906,0.108761,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000409189","Rural Short","Weather",null,1,586,1.2991000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000417506","Rural Short","Weather",null,1,6363,0.14106099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000463879","Rural Short","Weather",null,1,9052,0.20067399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000464539","Rural Short","Weather",null,1,9052,0.20067399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000552006","Rural Short","Weather",null,1,6333,0.14039599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000648968","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000673692","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000726518","Rural Short","Weather",null,1,2191,4.8571999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000730840","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000780688","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000812169","Rural Short","Weather",null,1,4922,0.109116,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","05:01","NMI-25000848335","Rural Short","Weather",null,1,6423,0.14239199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000150257","Urban","Weather",null,1,10426,0.32480799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000153522","Urban","Weather",null,1,1937,6.0345000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000153779","Urban","Weather",null,1,10426,0.32480799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000155932","Urban","Weather",null,1,8824,0.27489999999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000157112","Urban","Weather",null,1,8089,0.252002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000294754","Urban","Weather",null,1,1937,6.0345000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000305918","Urban","Weather",null,1,7503,0.23374600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000364531","Urban","Weather",null,1,11704,0.364622,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000364557","Urban","Weather",null,1,8763,0.27299899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000389209","Urban","Weather",null,1,6227,0.193994,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000419773","Urban","Weather",null,1,9138,0.28468199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000422875","Urban","Weather",null,1,10411,0.32434000000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000426836","Urban","Weather",null,1,7609,0.23704800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000482616","Urban","Weather",null,1,7353,0.229073,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000523618","Urban","Weather",null,1,9153,0.28514899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000531728","Urban","Weather",null,1,8763,0.27299899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000541604","Urban","Weather",null,1,9348,0.29122399999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000568736","Urban","Weather",null,1,10426,0.32480799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000568785","Urban","Weather",null,1,10403,0.32409100000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000576599","Urban","Weather",null,1,10403,0.32409100000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000609648","Urban","Weather",null,1,8763,0.27299899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000613723","Urban","Weather",null,1,9138,0.28468199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000642953","Urban","Weather",null,1,1937,6.0345000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","06:30","NMI-25000666359","Urban","Weather",null,1,9138,0.28468199999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000135645","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000149322","Urban","Weather",null,1,6109,0.19031699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000153615","Rural Short","Weather",null,1,12934,0.28673399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000154407","Rural Short","Weather",null,1,2987,6.6219E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000154439","Rural Short","Weather",null,1,2912,6.4556000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000154587","Rural Short","Weather",null,1,6453,0.14305699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000155018","Urban","Weather",null,1,4338,0.13514399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000155833","Urban","Weather",null,1,1637,5.0998000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000158281","Rural Short","Weather",null,1,4712,0.10446,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000159505","Rural Short","Weather",null,1,7548,0.16733200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000160173","Rural Short","Weather",null,1,7173,0.15901799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000161404","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000161701","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000175601","Rural Short","Weather",null,1,11508,0.25512099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000184353","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000184626","Rural Short","Weather",null,1,4667,0.103463,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000224834","Rural Short","Weather",null,1,8813,0.19537599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000229750","CBD","Weather",null,1,7217,1.9400539999999999,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","09:00","NMI-25000235476","Urban","Weather",null,1,4532,0.14118800000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000236161","Urban","Weather",null,1,4773,0.14869599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000240404","Rural Short","Weather",null,1,8885,0.19697200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000245970","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000264376","Urban","Weather",null,1,5808,0.18093999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000311386","Rural Short","Weather",null,1,12934,0.28673399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000341374","Rural Short","Weather",null,1,9003,0.19958799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000351201","Urban","Weather",null,1,10023,0.312253,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000364029","Rural Short","Weather",null,1,8943,0.19825799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000375488","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000403407","Rural Short","Weather",null,1,9122,0.20222599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000404900","Urban","Weather",null,1,16174,0.50387899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000419155","Rural Short","Weather",null,1,8885,0.19697200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000423832","Urban","Weather",null,1,4682,0.14586099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000440945","Urban","Weather",null,1,5748,0.17907100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000457327","Urban","Weather",null,1,10414,0.324434,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000460903","Rural Short","Weather",null,1,4682,0.103795,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000469554","Rural Short","Weather",null,1,8885,0.19697200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000474231","Urban","Weather",null,1,11597,0.36128900000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-2500048325","Rural Short","Weather",null,1,12934,0.28673399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000485329","Rural Short","Weather",null,1,9093,0.20158300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000490611","Rural Short","Weather",null,1,6453,0.14305699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000494552","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000497992","Urban","Weather",null,1,7563,0.23561499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000500930","Rural Short","Weather",null,1,7158,0.15868599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000501839","Urban","Weather",null,1,4502,0.14025399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000507644","Rural Short","Weather",null,1,9003,0.19958799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000507685","Urban","Weather",null,1,16174,0.50387899999999997,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000515887","Rural Short","Weather",null,1,5883,0.13042000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000521885","Rural Short","Weather",null,1,6062,0.13438900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000530423","Urban","Weather",null,1,10414,0.324434,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000531421","Rural Short","Weather",null,1,9003,0.19958799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000532758","Rural Short","Weather",null,1,7472,0.16564699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000536890","Rural Short","Weather",null,1,13156,0.29165600000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000548714","Urban","Weather",null,1,5898,0.18374399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000548928","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000550613","CBD","Weather",null,1,7217,1.9400539999999999,2.6899999999999998E-4,"Yes"]
[null,"17-03-2018","09:00","NMI-25000553004","Urban","Weather",null,1,6184,0.19265399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000568613","Rural Short","Weather",null,1,10773,0.23882700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000568950","Rural Short","Weather",null,1,8943,0.19825799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000577761","Urban","Weather",null,1,7427,0.231378,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000584602","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000605571","Urban","Weather",null,1,10339,0.32209700000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000605714","Urban","Weather",null,1,10143,0.31599100000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000610838","Rural Short","Weather",null,1,14406,0.31936700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000611662","Rural Short","Weather",null,1,7158,0.15868599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000613640","Rural Short","Weather",null,1,7548,0.16733200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000622889","Urban","Weather",null,1,7638,0.237951,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000627375","Urban","Weather",null,1,7638,0.237951,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000629506","Urban","Weather",null,1,1862,5.8007999999999997E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000631536","Rural Short","Weather",null,1,4712,0.10446,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000632518","Rural Short","Weather",null,1,11478,0.25445600000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000635999","Rural Short","Weather",null,1,12934,0.28673399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000672010","Urban","Weather",null,1,5808,0.18093999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000681432","Rural Short","Weather",null,1,8913,0.19759199999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000681499","Rural Short","Weather",null,1,8885,0.19697200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000685185","Rural Short","Weather",null,1,14615,0.32400000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000693916","Urban","Weather",null,1,1637,5.0998000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000694046","Rural Short","Weather",null,1,4712,0.10446,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000698673","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000712243","Rural Short","Weather",null,1,12934,0.28673399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000733264","Rural Short","Weather",null,1,7158,0.15868599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000741178","Urban","Weather",null,1,3002,9.3522999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000764623","Urban","Weather",null,1,14705,0.45811400000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000772345","Urban","Weather",null,1,467,1.4548999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000777948","Rural Short","Weather",null,1,8885,0.19697200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000787848","Urban","Weather",null,1,6107,0.19025500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000796460","Urban","Weather",null,1,8813,0.274557,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000797756","Rural Short","Weather",null,1,557,1.2348E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000808182","Urban","Weather",null,1,5808,0.18093999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000808793","Rural Short","Weather",null,1,11478,0.25445600000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000812670","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000814742","Urban","Weather",null,1,6303,0.19636100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000826498","Urban","Weather",null,1,14540,0.45297399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000831325","Rural Short","Weather",null,1,15785,0.34993800000000003,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000842215","Urban","Weather",null,1,4487,0.13978599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000843411","Rural Short","Weather",null,1,8813,0.19537599999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000856090","Rural Short","Weather",null,1,4727,0.104793,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000878714","Urban","Weather",null,1,13444,0.41882900000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:00","NMI-25000886294","Urban","Weather",null,1,9336,0.29085,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:30","NMI-25000454472","Rural Long","Weather",null,1,3167,3.6444190000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","09:40","NMI-25000112842","Rural Short","Weather",null,1,3217,7.1318000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000185195","Rural Short","Weather",null,1,8948,0.19836799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000187034","Rural Short","Weather",null,1,8842,0.196018,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000189484","Rural Short","Weather",null,1,6127,0.13583000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000322191","Rural Short","Weather",null,1,7584,0.16813,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000384828","Rural Short","Weather",null,1,12909,0.28617999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000448302","Rural Short","Weather",null,1,8738,0.193713,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000491948","Rural Short","Weather",null,1,8963,0.19870099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000519797","Rural Short","Weather",null,1,8768,0.194378,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000573265","Rural Short","Weather",null,1,12865,0.28520400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000614499","Rural Short","Weather",null,1,7494,0.166135,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000614616","Rural Short","Weather",null,1,7419,0.16447200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000655857","Rural Short","Weather",null,1,7494,0.166135,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000703598","Rural Short","Weather",null,1,8783,0.19470999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:40","NMI-25000717210","Rural Short","Weather",null,1,7494,0.166135,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000145082","Urban","Weather",null,1,10498,0.32705099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000351615","Urban","Weather",null,1,10558,0.32891999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000376958","Urban","Weather",null,1,10348,0.322378,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000518575","Urban","Weather",null,1,10498,0.32705099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000573520","Urban","Weather",null,1,8819,0.27474399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000574379","Urban","Weather",null,1,6043,0.18826100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000624885","Urban","Weather",null,1,7587,0.23636299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000652779","Urban","Weather",null,1,10348,0.322378,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000690095","Urban","Weather",null,1,10498,0.32705099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000750195","Urban","Weather",null,1,11776,0.366865,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:20","NMI-25000824817","Urban","Weather",null,1,10498,0.32705099999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:29","NMI-25000808470","Rural Short","Weather",null,1,170,3.7690000000000002E-3,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000142582","Rural Short","Weather",null,1,5990,0.13279299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000309751","Rural Short","Weather",null,1,8957,0.19856799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000410444","Rural Short","Weather",null,1,3097,6.8657999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000477210","Rural Short","Weather",null,1,4175,9.2555999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000590286","Rural Short","Weather",null,1,4579,0.10151200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000631099","Rural Short","Weather",null,1,8693,0.192715,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000632375","Urban","Weather",null,1,5719,0.17816799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000751509","Rural Short","Weather",null,1,3096,6.8635000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000752842","Rural Short","Weather",null,1,3096,6.8635000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000755945","Rural Short","Weather",null,1,3096,6.8635000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000775380","Rural Short","Weather",null,1,7128,0.15802099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:00","NMI-25000848731","Rural Short","Weather",null,1,5585,0.12381399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:40","NMI-25000508361","Rural Short","Weather",null,1,5543,0.12288300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","11:56","NMI-25000200670","Rural Short","Weather",null,1,7117,0.157777,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:10","NMI-25000313976","Urban","Weather",null,1,7522,0.23433799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","12:26","NMI-25000605548","Rural Short","Weather",null,1,5827,0.12917899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000176946","Rural Short","Weather",null,1,5995,0.13290299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000181533","Rural Short","Weather",null,1,8822,0.195575,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000267099","Rural Short","Weather",null,1,7307,0.16198899999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000322507","Rural Short","Weather",null,1,1554,3.4451000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000334312","Rural Short","Weather",null,1,1554,3.4451000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000347413","Rural Short","Weather",null,1,6999,0.15516099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000462780","Rural Short","Weather",null,1,1554,3.4451000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000671095","Rural Short","Weather",null,1,4465,9.8985000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000730866","Rural Short","Weather",null,1,1554,3.4451000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","12:40","NMI-25000769242","Rural Short","Weather",null,1,8822,0.195575,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:02","NMI-25000445828","Rural Short","Weather",null,1,4335,9.6102999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:02","NMI-25000646907","Rural Short","Weather",null,1,7247,0.160659,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:02","NMI-25000742595","Rural Short","Weather",null,1,4415,9.7876000000000005E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:05","NMI-25000591054","Rural Short","Weather",null,1,11339,0.25137399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000156916","Rural Short","Weather",null,1,11423,0.25323699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000255105","Rural Short","Weather",null,1,11480,0.2545,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000292916","Rural Short","Weather",null,1,14119,0.313004,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000309248","Rural Short","Weather",null,1,8837,0.195908,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000357386","Rural Short","Weather",null,1,11480,0.2545,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000368906","Rural Short","Weather",null,1,14135,0.313359,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000394265","Rural Short","Weather",null,1,14075,0.312029,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000504625","Rural Short","Weather",null,1,4367,9.6811999999999995E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000565197","Rural Short","Weather",null,1,7488,0.16600200000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000638521","Rural Short","Weather",null,1,9828,0.21787699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000732687","Rural Short","Weather",null,1,11423,0.25323699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:30","NMI-25000834311","Rural Short","Weather",null,1,13024,0.28872900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:35","NMI-25000379471","Rural Long","Weather",null,1,4259,4.9010360000000004,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","13:35","NMI-25000389520","Rural Long","Weather",null,1,2774,3.1921750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","13:42","NMI-25000689062","Rural Long","Weather",null,1,1372,1.5788260000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","14:00","NMI-25000137007","Urban","Weather",null,1,2972,9.2589000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000152847","Urban","Weather",null,1,5567,0.173432,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000227225","Rural Short","Weather",null,1,9953,0.22064800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000229593","Urban","Weather",null,1,5942,0.185115,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000230603","Urban","Weather",null,1,2957,9.2120999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000400966","Urban","Weather",null,1,4352,0.13558100000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000423899","Urban","Weather",null,1,8358,0.260382,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000424392","Urban","Weather",null,1,5567,0.173432,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000452121","Urban","Weather",null,1,5942,0.185115,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000477382","Urban","Weather",null,1,1157,3.6045000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000505006","Urban","Weather",null,1,2972,9.2589000000000005E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000514450","Urban","Weather",null,1,5942,0.185115,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000555651","Urban","Weather",null,1,6903,0.21505299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000624126","Urban","Weather",null,1,3047,9.4924999999999995E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000690789","Urban","Weather",null,1,6963,0.216923,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000701883","Urban","Weather",null,1,1547,4.8195000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000706080","Urban","Weather",null,1,1382,4.3054000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000715346","Urban","Weather",null,1,2927,9.1187000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000716147","Urban","Weather",null,1,1547,4.8195000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000727331","Urban","Weather",null,1,2702,8.4177000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000779004","Urban","Weather",null,1,5942,0.185115,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000788359","Urban","Weather",null,1,6903,0.21505299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000827974","Urban","Weather",null,1,6903,0.21505299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:00","NMI-25000883472","Rural Short","Weather",null,1,11599,0.25713799999999998,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:15","NMI-25000396385","Rural Short","Weather",null,1,5882,0.13039799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:15","NMI-25000679731","Rural Short","Weather",null,1,8749,0.19395699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000174066","Urban","Weather",null,1,5405,0.16838500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000176211","Urban","Weather",null,1,4322,0.13464599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000257297","Urban","Weather",null,1,9107,0.28371600000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000319461","Urban","Weather",null,1,4322,0.13464599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000398745","Urban","Weather",null,1,7382,0.22997600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000401823","Urban","Weather",null,1,2882,8.9785000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000402696","Urban","Weather",null,1,4502,0.14025399999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000404643","Urban","Weather",null,1,4322,0.13464599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000446406","Urban","Weather",null,1,1128,3.5140999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000498289","Urban","Weather",null,1,9047,0.28184700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000568760","Urban","Weather",null,1,1128,3.5140999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000662713","Urban","Weather",null,1,2882,8.9785000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:30","NMI-25000680798","Urban","Weather",null,1,4307,0.13417899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:33","NMI-25000308309","Urban","Weather",null,1,1441,4.4892000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:33","NMI-25000504682","Urban","Weather",null,1,1441,4.4892000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:40","NMI-25000627342","Rural Short","Weather",null,1,6923,0.153476,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000140043","Urban","Weather",null,1,9899,0.30839,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000144679","Urban","Weather",null,1,5769,0.179725,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000148706","Urban","Weather",null,1,5438,0.16941300000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000166871","Urban","Weather",null,1,6894,0.21477299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000171155","Urban","Weather",null,1,10166,0.31670799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000173587","Urban","Weather",null,1,6909,0.21523999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000176764","Urban","Weather",null,1,12655,0.39424900000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000274657","Urban","Weather",null,1,7270,0.22648699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000302599","Urban","Weather",null,1,5723,0.17829200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000303373","Urban","Weather",null,1,11141,0.347082,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000316162","Urban","Weather",null,1,9899,0.30839,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000418066","Urban","Weather",null,1,5453,0.169881,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000425333","Urban","Weather",null,1,3983,0.124085,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000449655","Urban","Weather",null,1,6894,0.21477299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000449738","Urban","Weather",null,1,8259,0.25729800000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000457772","Urban","Weather",null,1,11096,0.34568100000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000480513","Urban","Weather",null,1,8259,0.25729800000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000491352","Urban","Weather",null,1,7180,0.22368299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000527625","Urban","Weather",null,1,7180,0.22368299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000527908","Urban","Weather",null,1,2664,8.2992999999999997E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000549678","Urban","Weather",null,1,7180,0.22368299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000582844","Urban","Weather",null,1,5723,0.17829200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000603435","Urban","Weather",null,1,7180,0.22368299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000608533","Urban","Weather",null,1,10062,0.31346800000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000620126","Urban","Weather",null,1,9700,0.30219000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000622343","Urban","Weather",null,1,7105,0.22134599999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000624142","Urban","Weather",null,1,12655,0.39424900000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000631314","Urban","Weather",null,1,1208,3.7634000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000674773","Urban","Weather",null,1,10177,0.31705,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000681037","Urban","Weather",null,1,6894,0.21477299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000681374","Urban","Weather",null,1,8274,0.25776500000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000698293","Urban","Weather",null,1,6894,0.21477299999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000706858","Urban","Weather",null,1,9899,0.30839,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000719033","Urban","Weather",null,1,8259,0.25729800000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000738207","Urban","Weather",null,1,5723,0.17829200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000746845","Urban","Weather",null,1,7270,0.22648699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000777667","Urban","Weather",null,1,10177,0.31705,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000812267","Urban","Weather",null,1,9899,0.30839,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:54","NMI-25000878571","Urban","Weather",null,1,9899,0.30839,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","14:58","NMI-25000442626","Rural Short","Weather",null,1,7176,0.159085,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:58","NMI-25000480967","Rural Short","Weather",null,1,5794,0.12844700000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:58","NMI-25000646970","Rural Short","Weather",null,1,5884,0.130442,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","14:58","NMI-25000791919","Rural Short","Weather",null,1,12516,0.27746700000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000313448","Rural Short","Weather",null,1,5293,0.117341,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000611309","Rural Short","Weather",null,1,5293,0.117341,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000647508","Rural Short","Weather",null,1,9600,0.21282300000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000658529","Rural Short","Weather",null,1,4018,8.9075000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000773138","Rural Short","Weather",null,1,4018,8.9075000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:05","NMI-25000811476","Rural Short","Weather",null,1,5293,0.117341,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000170117","Urban","Weather",null,1,4028,0.12548699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000223515","Urban","Weather",null,1,9727,0.30303099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000227607","Urban","Weather",null,1,2632,8.1995999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000260063","Urban","Weather",null,1,4028,0.12548699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000428641","Urban","Weather",null,1,9713,0.302595,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000460299","Urban","Weather",null,1,9727,0.30303099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000529431","Urban","Weather",null,1,9713,0.302595,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000586136","Urban","Weather",null,1,4028,0.12548699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000607832","Urban","Weather",null,1,4028,0.12548699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000654320","Urban","Weather",null,1,7177,0.22359000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000735327","Urban","Weather",null,1,4028,0.12548699999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000750848","Urban","Weather",null,1,5723,0.17829200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000819378","Urban","Weather",null,1,9727,0.30303099999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:10","NMI-25000855844","Urban","Weather",null,1,5407,0.16844799999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","16:50","NMI-25000114816","Rural Short","Weather",null,1,12809,0.28396300000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:50","NMI-25000401360","Rural Short","Weather",null,1,8518,0.188836,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","16:50","NMI-25000432669","Rural Short","Weather",null,1,8518,0.188836,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000157838","Urban","Weather",null,1,4013,0.12501899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000159289","Urban","Weather",null,1,4100,0.12773000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000159990","Urban","Weather",null,1,5927,0.18464700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000262982","Urban","Weather",null,1,2838,8.8414000000000006E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000367534","Urban","Weather",null,1,4013,0.12501899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000391172","Rural Long","Weather",null,1,8653,9.9574219999999993,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","17:00","NMI-25000445150","Urban","Weather",null,1,9063,0.28234500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000456958","Urban","Weather",null,1,9063,0.28234500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000620471","Urban","Weather",null,1,1053,3.2805000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000623029","Urban","Weather",null,1,2943,9.1685000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000629348","Urban","Weather",null,1,2838,8.8414000000000006E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000747769","Urban","Weather",null,1,4446,0.13850899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000758492","Urban","Weather",null,1,9063,0.28234500000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:00","NMI-25000874349","Rural Long","Weather",null,1,11059,12.726122,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","17:00","NMI-25000876527","Rural Long","Weather",null,1,10009,11.517837,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","17:04","NMI-25000335524","Urban","Weather",null,1,6018,0.18748200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:04","NMI-25000544011","Urban","Weather",null,1,6018,0.18748200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:04","NMI-25000567143","Urban","Weather",null,1,6018,0.18748200000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","17:13","NMI-25000535316","Rural Short","Weather",null,1,995,2.2058000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:13","NMI-25000569165","Rural Short","Weather",null,1,7397,0.16398399999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:13","NMI-25000683287","Rural Short","Weather",null,1,2421,5.3671000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:13","NMI-25000699053","Rural Short","Weather",null,1,4000,8.8676000000000005E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:30","NMI-25000487259","Rural Short","Weather",null,1,8298,0.18395800000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","17:38","NMI-25000136099","Urban","Weather",null,1,2874,8.9535000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","18:12","NMI-25000860127","Urban","Weather",null,1,8261,0.25735999999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000165840","Rural Short","Weather",null,1,8310,0.184225,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000175740","Rural Short","Weather",null,1,5400,0.119713,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000176722","Rural Short","Weather",null,1,5580,0.12370299999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000248117","Rural Short","Weather",null,1,3900,8.6458999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000314173","Rural Short","Weather",null,1,7186,0.159307,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000359517","Rural Short","Weather",null,1,1260,2.7932999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000361175","Rural Short","Weather",null,1,8176,0.181254,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000459134","Rural Short","Weather",null,1,7186,0.159307,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000493968","Rural Short","Weather",null,1,3900,8.6458999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000526784","Rural Short","Weather",null,1,5535,0.122706,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000567135","Rural Short","Weather",null,1,3900,8.6458999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000572465","Rural Short","Weather",null,1,3900,8.6458999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000573316","Rural Short","Weather",null,1,2460,5.4536000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000592182","Rural Short","Weather",null,1,9977,0.22117999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000592629","Rural Short","Weather",null,1,8566,0.18990000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000713358","Rural Short","Weather",null,1,4756,0.105436,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000726178","Rural Short","Weather",null,1,5145,0.11405999999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000776967","Rural Short","Weather",null,1,7186,0.159307,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000798714","Rural Short","Weather",null,1,1260,2.7932999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000816292","Rural Short","Weather",null,1,3900,8.6458999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","18:32","NMI-25000870927","Rural Short","Weather",null,1,5655,0.12536600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000161009","Urban","Weather",null,1,5331,0.16608000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000161543","Urban","Weather",null,1,5331,0.16608000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000164420","Urban","Weather",null,1,5331,0.16608000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000632789","Urban","Weather",null,1,5331,0.16608000000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000638927","Urban","Weather",null,1,1275,3.9720999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","19:02","NMI-25000744048","Urban","Weather",null,1,5354,0.166796,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000190502","Rural Short","Weather",null,1,3759,8.3333000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000446513","Rural Short","Weather",null,1,8156,0.18081,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000571411","Rural Short","Weather",null,1,5259,0.116587,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000638448","Rural Short","Weather",null,1,6952,0.15411900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000725971","Rural Short","Weather",null,1,5259,0.116587,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","20:39","NMI-25000800711","Rural Short","Weather",null,1,6952,0.15411900000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000110574","Rural Short","Weather",null,1,3651,8.0938999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000441102","Urban","Weather",null,1,5058,0.15757499999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000458037","Urban","Weather",null,1,7532,0.234649,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000530720","Urban","Weather",null,1,707,2.2026E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000611547","Rural Short","Weather",null,1,3651,8.0938999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000638794","Urban","Weather",null,1,707,2.2026E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000639487","Urban","Weather",null,1,10128,0.31552400000000003,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000681291","Urban","Weather",null,1,677,2.1090999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000854656","Urban","Weather",null,1,2569,8.0033999999999994E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:31","NMI-25000868268","Urban","Weather",null,1,2580,8.0376000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","21:45","NMI-25000163654","Rural Short","Weather",null,1,9664,0.21424099999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","21:45","NMI-25000449787","Rural Short","Weather",null,1,5254,0.116476,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","21:45","NMI-25000856059","Rural Short","Weather",null,1,4037,8.9496000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000158507","Urban","Weather",null,1,9644,0.30044500000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000162094","Urban","Weather",null,1,7998,0.249167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000334732","Urban","Weather",null,1,8174,0.25464999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000482862","Urban","Weather",null,1,7998,0.249167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000694821","Urban","Weather",null,1,7998,0.249167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:35","NMI-25000733370","Urban","Weather",null,1,7998,0.249167,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","22:50","NMI-25000426497","Rural Short","Weather",null,1,4948,0.109692,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","22:50","NMI-25000484370","Rural Short","Weather",null,1,3613,8.0097000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","22:50","NMI-25000597513","Rural Short","Weather",null,1,4948,0.109692,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","22:50","NMI-25000802697","Rural Short","Weather",null,1,3613,8.0097000000000002E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:02","NMI-25000453532","Rural Short","Weather",null,1,7891,0.17493600000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000149546","Urban","Weather",null,1,9494,0.29577199999999998,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000149934","Urban","Weather",null,1,3852,0.120004,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000155437","Urban","Weather",null,1,6657,0.20738999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000157037","Urban","Weather",null,1,2531,7.8850000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000353550","Urban","Weather",null,1,6657,0.20738999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","23:51","NMI-25000661483","Urban","Weather",null,1,6657,0.20738999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018",null,null,"Rural Short","Weather",null,1870,null,null,4.1456E-2,"Yes"]
[null,"17-03-2018","07:36","DT-0134","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0161","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0172","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0173","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0174","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0176","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0177","Rural Short","Weather",null,8,1730,0.30681900000000001,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0178","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0179","Rural Short","Weather",null,10,1730,0.38352399999999998,2.22E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0180","Rural Short","Weather",null,44,1730,1.687506,9.7499999999999996E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0181","Rural Short","Weather",null,5,1730,0.19176199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0183","Rural Short","Weather",null,5,1730,0.19176199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0184","Rural Short","Weather",null,15,1730,0.57528599999999996,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0185","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0216","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0220","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0225","Rural Short","Weather",null,4,1730,0.15340999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0311","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0332","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0333","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0358","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0365","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0411","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0412","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0415","Rural Short","Weather",null,6,1730,0.23011400000000001,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0420","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0421","Rural Short","Weather",null,23,1730,0.88210500000000003,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0423","Rural Short","Weather",null,16,1730,0.61363800000000002,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0448","Rural Short","Weather",null,5,1730,0.19176199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","07:36","DT-0455","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0463","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0464","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0474","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0475","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0487","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0488","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0489","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0496","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0558","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0561","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","07:36","DT-0566","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0567","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0583","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0584","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0585","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0586","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0587","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0588","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0589","Rural Short","Weather",null,4,1730,0.15340999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0590","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","07:36","DT-0591","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0592","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0597","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0603","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0613","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0614","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0630","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0643","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0649","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0653","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0654","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0657","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0673","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0677","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0679","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0695","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0696","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0831","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0852","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0877","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0879","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0881","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","07:36","DT-0920","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0931","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-0932","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10041","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10072","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10075","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","07:36","DT-10138","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10163","Rural Short","Weather",null,18,1730,0.69034300000000004,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","07:36","DT-10198","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10228","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10242","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10256","Rural Short","Weather",null,2,1730,7.6704999999999995E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10258","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10468","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10521-1","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","07:36","DT-10552","Rural Short","Weather",null,3,1730,0.11505700000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10560","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10561","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10715","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10725","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10738","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10766","Rural Short","Weather",null,1,1730,3.8351999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","DT-10787","Rural Short","Weather",null,278,1730,10.661967000000001,6.1630000000000001E-3,"Yes"]
[null,"17-03-2018","08:10","DT-1267","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1268","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1269","Rural Short","Weather",null,5,6235,0.69111900000000004,1.11E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1293","Rural Short","Weather",null,1,4370,9.6879000000000007E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1294","Rural Short","Weather",null,6,4370,0.58127200000000001,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1295","Rural Short","Weather",null,5,4370,0.48439300000000002,1.11E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1296","Rural Short","Weather",null,10,6235,1.3822380000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1297","Rural Short","Weather",null,17,6235,2.3498049999999999,3.77E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1298","Rural Short","Weather",null,11,4370,1.0656650000000001,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1299","Rural Short","Weather",null,2,4370,0.19375700000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1302","Rural Short","Weather",null,8,4370,0.77502899999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1303","Rural Short","Weather",null,12,4370,1.1625430000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1314","Rural Short","Weather",null,7,4370,0.67815000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1315","Rural Short","Weather",null,1,4370,9.6879000000000007E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1324","Rural Short","Weather",null,5,4370,0.48439300000000002,1.11E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1325","Rural Short","Weather",null,1,4370,9.6879000000000007E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1326","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1327","Rural Short","Weather",null,8,4370,0.77502899999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1328","Rural Short","Weather",null,1,4370,9.6879000000000007E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1506","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-1771","Rural Short","Weather",null,24,4370,2.3250860000000002,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","08:10","DT-1907","Rural Short","Weather",null,2,4370,0.19375700000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2158","Rural Short","Weather",null,11,6235,1.520462,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2221","Rural Short","Weather",null,3,4370,0.29063600000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2230","Rural Short","Weather",null,6,6235,0.82934300000000005,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2243","Rural Short","Weather",null,7,4370,0.67815000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2248","Rural Short","Weather",null,2,6235,0.27644800000000003,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2256","Rural Short","Weather",null,1,14917,0.33069500000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2262","Rural Short","Weather",null,7,6235,0.96756699999999995,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2301","Rural Short","Weather",null,7,4370,0.67815000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2344","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2345","Rural Short","Weather",null,3,6235,0.41467100000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2347","Rural Short","Weather",null,1,14917,0.33069500000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2352","Rural Short","Weather",null,1,6235,0.13822400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2478","Rural Short","Weather",null,455,6235,62.891837000000002,1.0087E-2,"Yes"]
[null,"17-03-2018","08:10","DT-2604","Rural Short","Weather",null,3,4370,0.29063600000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2629","Rural Short","Weather",null,17,4370,1.646936,3.77E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2631","Rural Short","Weather",null,13,4370,1.259422,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2683","Rural Short","Weather",null,7,4370,0.67815000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2684","Rural Short","Weather",null,7,4370,0.67815000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2685","Rural Short","Weather",null,5,6235,0.69111900000000004,1.11E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2751","Rural Short","Weather",null,11,6235,1.520462,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2756","Rural Short","Weather",null,12,4370,1.1625430000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:10","DT-2779","Rural Short","Weather",null,4,6235,0.55289500000000003,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2817","Rural Short","Weather",null,2,4370,0.19375700000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-2903","Rural Short","Weather",null,19,4370,1.8406929999999999,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:10","DT-3025","Rural Short","Weather",null,455,6235,62.891837000000002,1.0087E-2,"Yes"]
[null,"17-03-2018","08:10","DT-3083","Rural Short","Weather",null,23,6235,3.1791480000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","08:10","DT-3142","Rural Short","Weather",null,2,6235,0.27644800000000003,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:10","DT-3256","Rural Short","Weather",null,455,4370,44.079763999999997,1.0087E-2,"Yes"]
[null,"17-03-2018","08:10","DT-3297","Rural Short","Weather",null,87,6235,12.025472000000001,1.9289999999999999E-3,"Yes"]
[null,"17-03-2018","08:10","DT-3346","Rural Short","Weather",null,45,6235,6.220072,9.9799999999999997E-4,"Yes"]
[null,"17-03-2018","08:10","DT-3445","Rural Short","Weather",null,2,6235,0.27644800000000003,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0074","Rural Short","Weather",null,18,3249,1.2964880000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0075","Rural Short","Weather",null,19,3249,1.3685160000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0076","Rural Short","Weather",null,15,3249,1.0804069999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0077","Rural Short","Weather",null,20,3249,1.4405429999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0078","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0079","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0080","Rural Short","Weather",null,8,3249,0.57621699999999998,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0081","Rural Short","Weather",null,7,3249,0.50419000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0119","Rural Short","Weather",null,16,3249,1.152434,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0120","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0121","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0124","Rural Short","Weather",null,23,3249,1.6566240000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0127","Rural Short","Weather",null,15,3249,1.0804069999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0128","Rural Short","Weather",null,24,3249,1.7286509999999999,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0129","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0130","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0131","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0132","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0133","Rural Short","Weather",null,18,3249,1.2964880000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0201","Rural Short","Weather",null,14,3249,1.0083800000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0202","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0203","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0234","Rural Short","Weather",null,14,3249,1.0083800000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0235","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0238","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0240","Rural Short","Weather",null,21,3249,1.51257,4.66E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0241","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0243","Rural Short","Weather",null,40,3249,2.8810850000000001,8.8699999999999998E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0255","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0260","Rural Short","Weather",null,42,3249,3.0251399999999999,9.3099999999999997E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0286","Rural Short","Weather",null,19,3249,1.3685160000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0307","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0384","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0389","Rural Short","Weather",null,8,3249,0.57621699999999998,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0418","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0431","Rural Short","Weather",null,28,3249,2.0167600000000001,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0432","Rural Short","Weather",null,66,3249,4.7537909999999997,1.4630000000000001E-3,"Yes"]
[null,"17-03-2018","08:49","DT-0476","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0477","Rural Short","Weather",null,21,3249,1.51257,4.66E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0490","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0495","Rural Short","Weather",null,19,3249,1.3685160000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0511","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0518","Rural Short","Weather",null,34,3249,2.4489230000000002,7.54E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0534","Rural Short","Weather",null,20,3249,1.4405429999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0535","Rural Short","Weather",null,18,3249,1.2964880000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0536","Rural Short","Weather",null,21,3249,1.51257,4.66E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0547","Rural Short","Weather",null,14,3249,1.0083800000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0548","Rural Short","Weather",null,15,3249,1.0804069999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0565","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0568","Rural Short","Weather",null,23,3249,1.6566240000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0571","Rural Short","Weather",null,12,3249,0.86432600000000004,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0580","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0610","Rural Short","Weather",null,8,3249,0.57621699999999998,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0611","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0626","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0627","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0639","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0640","Rural Short","Weather",null,15,3249,1.0804069999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0641","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0655","Rural Short","Weather",null,8,3249,0.57621699999999998,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0660","Rural Short","Weather",null,10,3249,0.72027099999999999,2.22E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0678","Rural Short","Weather",null,20,3249,1.4405429999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0692","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0715","Rural Short","Weather",null,13,3249,0.93635299999999999,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0716","Rural Short","Weather",null,7,3249,0.50419000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0729","Rural Short","Weather",null,6,3249,0.43216300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0785","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0786","Rural Short","Weather",null,19,3249,1.3685160000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0787","Rural Short","Weather",null,19,3249,1.3685160000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0788","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0789","Rural Short","Weather",null,18,3249,1.2964880000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0790","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-0820","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0823","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0834","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0849","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-0861","Rural Short","Weather",null,1271,3249,91.546487999999997,2.8177000000000001E-2,"Yes"]
[null,"17-03-2018","08:49","DT-0907","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10010","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10019","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10055","Rural Short","Weather",null,13,3249,0.93635299999999999,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10064","Rural Short","Weather",null,7,3249,0.50419000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10065","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10066","Rural Short","Weather",null,6,3249,0.43216300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10067","Rural Short","Weather",null,7,3249,0.50419000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10068","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10069","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10070","Rural Short","Weather",null,7,3249,0.50419000000000003,1.55E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10071","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10130","Rural Short","Weather",null,6,3249,0.43216300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10232","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10233","Rural Short","Weather",null,10,3249,0.72027099999999999,2.22E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10234","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10235","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10266","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10387","Rural Short","Weather",null,8,3249,0.57621699999999998,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10425","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10428","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10429","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10430","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10431","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10432","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10433","Rural Short","Weather",null,6,3249,0.43216300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10434","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10437","Rural Short","Weather",null,11,3249,0.79229799999999995,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10440","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10441","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10465","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10546","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10550","Rural Short","Weather",null,1,3249,7.2026999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10562","Rural Short","Weather",null,17,3249,1.224461,3.77E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10593","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10671","Rural Short","Weather",null,3,3249,0.216081,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10672","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10673","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10674","Rural Short","Weather",null,6,3249,0.43216300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10675","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10676","Rural Short","Weather",null,5,3249,0.36013600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10677","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10678","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10721","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10737","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10742","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10776","Rural Short","Weather",null,1271,3249,91.546487999999997,2.8177000000000001E-2,"Yes"]
[null,"17-03-2018","08:49","DT-10788","Rural Short","Weather",null,4,3249,0.288109,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:49","DT-10804","Rural Short","Weather",null,9,3249,0.64824400000000004,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:49","DT-10832","Rural Short","Weather",null,2,3249,0.14405399999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0045","Rural Short","Weather",null,18,6065,2.4201920000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0046","Rural Short","Weather",null,15,6065,2.016826,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0047","Rural Short","Weather",null,8,5925,1.0508109999999999,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0048","Rural Short","Weather",null,5,5925,0.65675700000000004,1.11E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0049","Rural Short","Weather",null,3,5925,0.39405400000000002,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0055","Rural Short","Weather",null,28,10476,6.5027929999999996,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0083","Rural Short","Weather",null,29,10836,6.9664799999999998,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0084","Rural Short","Weather",null,10,6595,1.4620470000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0085","Rural Short","Weather",null,11,1715,0.41821799999999998,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0086","Rural Short","Weather",null,16,1715,0.60831800000000003,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0087","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0088","Rural Short","Weather",null,20,1715,0.76039699999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0089","Rural Short","Weather",null,39,1715,1.482775,8.6499999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0091","Rural Short","Weather",null,1352,1715,51.402855000000002,2.9973E-2,"Yes"]
[null,"17-03-2018","08:55","DT-0092","Rural Short","Weather",null,4,1715,0.15207899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0093","Rural Short","Weather",null,4,1715,0.15207899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0094","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0095","Rural Short","Weather",null,10,1715,0.38019900000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0096","Rural Short","Weather",null,27,1715,1.0265359999999999,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0097","Rural Short","Weather",null,37,1715,1.4067350000000001,8.1999999999999998E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0099","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0101","Rural Short","Weather",null,18,11495,4.5869910000000003,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0102","Rural Short","Weather",null,20,1715,0.76039699999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0103","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0104","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0105","Rural Short","Weather",null,4,1715,0.15207899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0106","Rural Short","Weather",null,9,1715,0.34217900000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0107","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0108","Rural Short","Weather",null,9,1715,0.34217900000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0109","Rural Short","Weather",null,17,1715,0.64633799999999997,3.77E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0110","Rural Short","Weather",null,12,1715,0.45623799999999998,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0125","Rural Short","Weather",null,22,6247,3.0467770000000001,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0135","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0200","Rural Short","Weather",null,14,10476,3.2513969999999999,3.1E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0204","Rural Short","Weather",null,33,5925,4.3345969999999996,7.3200000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0215","Rural Short","Weather",null,15,1715,0.57029799999999997,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0218","Rural Short","Weather",null,32,1715,1.2166360000000001,7.0899999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0236","Rural Short","Weather",null,19,5925,2.4956770000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0237","Rural Short","Weather",null,28,5925,3.6778400000000002,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0251","Rural Short","Weather",null,5,1715,0.19009899999999999,1.11E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0282","Rural Short","Weather",null,6,1715,0.22811899999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0302","Rural Short","Weather",null,19,5925,2.4956770000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0320","Rural Short","Weather",null,27,5925,3.5464880000000001,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0321","Rural Short","Weather",null,3,1715,0.11405999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0390","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0414","Rural Short","Weather",null,4,11495,1.019331,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0428","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0456","Rural Short","Weather",null,18,7470,2.9808460000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0461","Rural Short","Weather",null,3,1715,0.11405999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0472","Rural Short","Weather",null,22,10174,4.9620470000000001,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0498","Rural Short","Weather",null,21,1715,0.79841700000000004,4.66E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0499","Rural Short","Weather",null,20,1715,0.76039699999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0530","Rural Short","Weather",null,11,1715,0.41821799999999998,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0546","Rural Short","Weather",null,28,1715,1.0645560000000001,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0574","Rural Short","Weather",null,1,6595,0.146205,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0575","Rural Short","Weather",null,12,6595,1.754456,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0576","Rural Short","Weather",null,8,6595,1.169637,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0577","Rural Short","Weather",null,9,6595,1.315842,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0578","Rural Short","Weather",null,9,6595,1.315842,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0599","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0605","Rural Short","Weather",null,8,11495,2.0386630000000001,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0624","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0625","Rural Short","Weather",null,3,1715,0.11405999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0636","Rural Short","Weather",null,19,1715,0.72237700000000005,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0637","Rural Short","Weather",null,18,1715,0.68435800000000002,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0659","Rural Short","Weather",null,15,10174,3.3832140000000002,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0680","Rural Short","Weather",null,12,1715,0.45623799999999998,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0691","Rural Short","Weather",null,3,1715,0.11405999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0694","Rural Short","Weather",null,13,6595,1.9006609999999999,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0717","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0718","Rural Short","Weather",null,9,1715,0.34217900000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0719","Rural Short","Weather",null,17,1715,0.64633799999999997,3.77E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0720","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0721","Rural Short","Weather",null,7,1715,0.26613900000000001,1.55E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0743","Rural Short","Weather",null,15,1715,0.57029799999999997,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0816","Rural Short","Weather",null,7,1715,0.26613900000000001,1.55E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0821","Rural Short","Weather",null,13,1715,0.49425799999999998,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0822","Rural Short","Weather",null,10,5925,1.3135140000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0841-1","Rural Short","Weather",null,12,1715,0.45623799999999998,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0841-2","Rural Short","Weather",null,12,1715,0.45623799999999998,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0872","Rural Short","Weather",null,14,1715,0.53227800000000003,3.1E-4,"Yes"]
[null,"17-03-2018","08:55","DT-0908","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-0934","Rural Short","Weather",null,12,6595,1.754456,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10015","Rural Short","Weather",null,10,6595,1.4620470000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10097","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10098","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10113","Rural Short","Weather",null,12,4445,1.1824939999999999,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10272","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10285","Rural Short","Weather",null,1,5925,0.131351,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10319","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10446","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10472","Rural Short","Weather",null,10,6065,1.3445510000000001,2.22E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10520","Rural Short","Weather",null,7,4445,0.68978799999999996,1.55E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10569","Rural Short","Weather",null,6,5925,0.78810899999999995,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10590","Rural Short","Weather",null,2,7431,0.32947599999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10611","Rural Short","Weather",null,0,1715,0,0,"Yes"]
[null,"17-03-2018","08:55","DT-10621","Rural Short","Weather",null,7,5925,0.91946000000000006,1.55E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10622","Rural Short","Weather",null,4,5925,0.52540600000000004,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10623","Rural Short","Weather",null,4,5925,0.52540600000000004,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10629","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10657","Rural Short","Weather",null,2,1715,7.6039999999999996E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10658","Rural Short","Weather",null,5,1715,0.19009899999999999,1.11E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10659","Rural Short","Weather",null,31,1715,1.1786160000000001,6.87E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10660","Rural Short","Weather",null,4,1715,0.15207899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10661","Rural Short","Weather",null,3,1715,0.11405999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10662","Rural Short","Weather",null,1,1715,3.8019999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10663","Rural Short","Weather",null,16,1715,0.60831800000000003,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10664","Rural Short","Weather",null,5,1715,0.19009899999999999,1.11E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10666","Rural Short","Weather",null,9,6595,1.315842,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10687","Rural Short","Weather",null,2,5895,0.26137300000000002,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10688","Rural Short","Weather",null,5,1715,0.19009899999999999,1.11E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10693","Rural Short","Weather",null,31,1715,1.1786160000000001,6.87E-4,"Yes"]
[null,"17-03-2018","08:55","DT-10717","Rural Short","Weather",null,4,1715,0.15207899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10739","Rural Short","Weather",null,1352,1715,51.402855000000002,2.9973E-2,"Yes"]
[null,"17-03-2018","08:55","DT-10749","Rural Short","Weather",null,3,5925,0.39405400000000002,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10775","Rural Short","Weather",null,1,6595,0.146205,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:55","DT-10781","Rural Short","Weather",null,16,1715,0.60831800000000003,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0050","Rural Short","Weather",null,2,2923,0.12959999999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0052","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0053","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0054","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0056","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0057","Rural Short","Weather",null,24,2923,1.5552010000000001,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0058","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0059","Rural Short","Weather",null,24,2923,1.5552010000000001,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0063","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0064","Rural Short","Weather",null,25,2923,1.620001,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0065","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0066","Rural Short","Weather",null,18,2923,1.166401,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0067","Rural Short","Weather",null,22,2923,1.4256009999999999,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0068","Rural Short","Weather",null,11,2923,0.71279999999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0069","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0070","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0071","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0072","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0073","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0082","Rural Short","Weather",null,24,2923,1.5552010000000001,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0126","Rural Short","Weather",null,13,2923,0.84240000000000004,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0217","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0227-2","Rural Short","Weather",null,36,2923,2.3328009999999999,7.9799999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0250","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0252","Rural Short","Weather",null,18,2923,1.166401,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0259","Rural Short","Weather",null,33,2923,2.138401,7.3200000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0283","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0306","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0308","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0325","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0347","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0369","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0370","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0371","Rural Short","Weather",null,27,2923,1.749601,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0372","Rural Short","Weather",null,33,2923,2.138401,7.3200000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0373","Rural Short","Weather",null,17,2923,1.1016010000000001,3.77E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0385","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0391","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0409","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0422","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0441","Rural Short","Weather",null,27,2923,1.749601,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0442","Rural Short","Weather",null,23,2923,1.4904010000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0451","Rural Short","Weather",null,21,2923,1.3608009999999999,4.66E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0466","Rural Short","Weather",null,19,2923,1.231201,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0467","Rural Short","Weather",null,20,2923,1.296001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0468","Rural Short","Weather",null,18,2923,1.166401,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0469","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0484","Rural Short","Weather",null,23,2923,1.4904010000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0486","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0491","Rural Short","Weather",null,18,2923,1.166401,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0502","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0503","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0504","Rural Short","Weather",null,28,2923,1.8144009999999999,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0505","Rural Short","Weather",null,31,2923,2.0088010000000001,6.87E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0514","Rural Short","Weather",null,26,2923,1.684801,5.7600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0519","Rural Short","Weather",null,17,2923,1.1016010000000001,3.77E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0520","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0521","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0537","Rural Short","Weather",null,17,2923,1.1016010000000001,3.77E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0538","Rural Short","Weather",null,21,2923,1.3608009999999999,4.66E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0542","Rural Short","Weather",null,20,2923,1.296001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0543","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0557","Rural Short","Weather",null,13,2923,0.84240000000000004,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0569","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0570","Rural Short","Weather",null,22,2923,1.4256009999999999,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0593","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0607","Rural Short","Weather",null,13,2923,0.84240000000000004,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0616","Rural Short","Weather",null,11,2923,0.71279999999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0617","Rural Short","Weather",null,20,2923,1.296001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0632","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0633","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0634","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0635","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0645","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0646","Rural Short","Weather",null,20,2923,1.296001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0676","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0688","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0709","Rural Short","Weather",null,18,2923,1.166401,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0710","Rural Short","Weather",null,14,2923,0.90720000000000001,3.1E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0723","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0726","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0730","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0817-1","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0844","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0845","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0846","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0873","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0874","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0875","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0915","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0916","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0922","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0925","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0926","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0927","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0935","Rural Short","Weather",null,2,2923,0.12959999999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-0936","Rural Short","Weather",null,11,2923,0.71279999999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0937","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0938","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0939","Rural Short","Weather",null,13,2923,0.84240000000000004,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0940","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0941","Rural Short","Weather",null,16,2923,1.0368010000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0942","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0943","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0944","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0945","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-0946","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10006","Rural Short","Weather",null,13,2923,0.84240000000000004,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10007","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10008","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10009","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10017","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10032","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10033","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10048","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10073","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10114","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10115","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10116","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10117","Rural Short","Weather",null,11,2923,0.71279999999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10119","Rural Short","Weather",null,10,2923,0.64800000000000002,2.22E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10120","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10164","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10165","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10166","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10167","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10204","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10207","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10250","Rural Short","Weather",null,17,2923,1.1016010000000001,3.77E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10251","Rural Short","Weather",null,25,10203,5.6547590000000003,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10270","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10273","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10312","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10324","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10325","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10326","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10327","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10385","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10388","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10399","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10411","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10427","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10466","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10501","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10504","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10505","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10506","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10507","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10508","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10509","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10540","Rural Short","Weather",null,7,2923,0.4536,1.55E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10542","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10544","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10553","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10557","Rural Short","Weather",null,15,2923,0.972001,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10575","Rural Short","Weather",null,4,2923,0.25919999999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10576","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10577","Rural Short","Weather",null,9,2923,0.58320000000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10578","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10579","Rural Short","Weather",null,5,2923,0.32400000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10603","Rural Short","Weather",null,6,2923,0.38879999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10618","Rural Short","Weather",null,12,2923,0.77759999999999996,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10648","Rural Short","Weather",null,3,2923,0.19439999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10650","Rural Short","Weather",null,8,2923,0.51839999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","08:57","DT-10708","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10709","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10710","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10711","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10719","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10720","Rural Short","Weather",null,2,2923,0.12959999999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10724","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10767","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","DT-10768","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10769","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","08:57","DT-10795","Rural Short","Weather",null,1,2923,6.4799999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","08:57","MX5203511","Rural Short","Weather",null,1870,2923,121.17606600000001,4.1456E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0112","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0113","Rural Short","Weather",null,13,3387,0.97612399999999999,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0114","Rural Short","Weather",null,22,3387,1.651902,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0115","Rural Short","Weather",null,22,3387,1.651902,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0116","Rural Short","Weather",null,18,3387,1.351556,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0117","Rural Short","Weather",null,16,3387,1.2013830000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0140","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0186","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0187","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0188","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0189","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0190","Rural Short","Weather",null,20,3387,1.5017290000000001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0192","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0206","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0211","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0213","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0214","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0228","Rural Short","Weather",null,12,3387,0.90103800000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0239","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0249","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0253","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0266","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0270","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0272","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0289","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0290","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0291","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0292","Rural Short","Weather",null,20,3387,1.5017290000000001,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0293","Rural Short","Weather",null,14,3387,1.05121,3.1E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0300","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0304","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0305","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0313","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0314","Rural Short","Weather",null,19,3387,1.4266430000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0315","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0316","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0331","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0337","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0338","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0339","Rural Short","Weather",null,19,3387,1.4266430000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0340","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0341","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0342","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0343","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0357","Rural Short","Weather",null,8,3387,0.600692,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0368","Rural Short","Weather",null,6,3387,0.450519,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0377","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0378","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0379","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0380","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0381","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0382","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0383","Rural Short","Weather",null,6,3387,0.450519,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0386","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0387","Rural Short","Weather",null,6,3387,0.450519,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0388","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0394","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0397","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0398","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0402","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0424","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0425","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0434","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0436","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0449","Rural Short","Weather",null,6,3387,0.450519,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0473","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0494","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0501","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0506","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0510","Rural Short","Weather",null,14,3387,1.05121,3.1E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0527","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0531","Rural Short","Weather",null,57,3387,4.279928,1.2639999999999999E-3,"Yes"]
[null,"17-03-2018","09:03","DT-0532","Rural Short","Weather",null,30,3387,2.2525940000000002,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0533","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0549","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0556","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0559","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0564","Rural Short","Weather",null,13,3387,0.97612399999999999,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0579","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0604","Rural Short","Weather",null,8,3387,0.600692,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0619","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0638","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0642-1","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0644","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0650","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0651","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0652","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0682","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0683","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0690","Rural Short","Weather",null,3,3387,0.22525899999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0713","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0714","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0724","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0727","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0735","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0869","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0876","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0878","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0887","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0900","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0901","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0902","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0903","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-0904","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0918","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0921","Rural Short","Weather",null,848,4437,83.412519000000003,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-0923","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-0924","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10022","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10023","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10118","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10168","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10169","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10170","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10171","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10172","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10173","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10261","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10268","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-10269","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10284","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10392","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10393","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10396","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-10412","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10421","Rural Short","Weather",null,6,3387,0.450519,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10435","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-10436","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10458","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10459","Rural Short","Weather",null,11,3387,0.82595099999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10460","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10469","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10523","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10548","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10586","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10600","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10619","Rural Short","Weather",null,2,3387,0.150173,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10646","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10649","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10723","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10735","Rural Short","Weather",null,7,3387,0.52560499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10740","Rural Short","Weather",null,9,3387,0.67577799999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10771","Rural Short","Weather",null,1,3387,7.5086E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10780","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-10796","Rural Short","Weather",null,5,3387,0.37543199999999999,1.11E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10797","Rural Short","Weather",null,848,3387,63.673316999999997,1.8799E-2,"Yes"]
[null,"17-03-2018","09:03","DT-10798","Rural Short","Weather",null,4,3387,0.300346,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:03","DT-10807","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:03","DT-10834","Rural Short","Weather",null,10,3387,0.750865,2.22E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0017","Rural Short","Weather",null,2,1746,7.7413999999999997E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0018","Rural Short","Weather",null,5,1746,0.19353600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0020","Rural Short","Weather",null,21,1746,0.81284900000000004,4.66E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0022","Rural Short","Weather",null,1,10191,0.22592400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0023","Rural Short","Weather",null,1,6450,0.14299000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0024","Rural Short","Weather",null,19,6450,2.7168130000000001,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0025","Rural Short","Weather",null,17,6450,2.4308329999999998,3.77E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0026","Rural Short","Weather",null,26,6450,3.7177440000000002,5.7600000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0027","Rural Short","Weather",null,11,6450,1.572892,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0028","Rural Short","Weather",null,24,8873,4.720936,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0029","Rural Short","Weather",null,6,1746,0.232243,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0030","Rural Short","Weather",null,3,1746,0.116121,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0031","Rural Short","Weather",null,23,5235,2.66926,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0033","Rural Short","Weather",null,19,5235,2.205041,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0034","Rural Short","Weather",null,20,10191,4.5184870000000004,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0035","Rural Short","Weather",null,1,5235,0.11605500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0037","Rural Short","Weather",null,17,5235,1.9729319999999999,3.77E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0038","Rural Short","Weather",null,35,9124,7.0794540000000001,7.76E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0039","Rural Short","Weather",null,16,6201,2.1995209999999998,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0040","Rural Short","Weather",null,22,6201,3.0243419999999999,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0041","Rural Short","Weather",null,19,6201,2.6119309999999998,4.2099999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0042","Rural Short","Weather",null,24,6201,3.2992819999999998,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0043","Rural Short","Weather",null,24,6201,3.2992819999999998,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0044","Rural Short","Weather",null,18,6201,2.4744609999999998,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0219","Rural Short","Weather",null,8,1746,0.30965700000000002,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0256","Rural Short","Weather",null,2,6450,0.28598000000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0261","Rural Short","Weather",null,29,4431,2.8486929999999999,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0262","Rural Short","Weather",null,24,9124,4.8544830000000001,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0264","Rural Short","Weather",null,1,10191,0.22592400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0265","Rural Short","Weather",null,1,13851,0.30706299999999997,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0285","Rural Short","Weather",null,33,9124,6.6749140000000002,7.3200000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0334","Rural Short","Weather",null,20,6450,2.8598029999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0335","Rural Short","Weather",null,27,6450,3.8607339999999999,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0336","Rural Short","Weather",null,24,6450,3.4317639999999998,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0344","Rural Short","Weather",null,26,9124,5.259023,5.7600000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0345","Rural Short","Weather",null,28,9124,5.6635629999999999,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0346","Rural Short","Weather",null,35,9124,7.0794540000000001,7.76E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0393","Rural Short","Weather",null,45,5235,5.2224659999999998,9.9799999999999997E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0419","Rural Short","Weather",null,1,10191,0.22592400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0450","Rural Short","Weather",null,29,6450,4.1467150000000004,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0458","Rural Short","Weather",null,16,1746,0.61931400000000003,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0471","Rural Short","Weather",null,32,6450,4.575685,7.0899999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0512","Rural Short","Weather",null,1,10191,0.22592400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0522","Rural Short","Weather",null,5,6450,0.714951,1.11E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0551","Rural Short","Weather",null,17,6450,2.4308329999999998,3.77E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0628","Rural Short","Weather",null,6,6450,0.85794099999999995,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0629","Rural Short","Weather",null,7,6450,1.000931,1.55E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0711","Rural Short","Weather",null,3,1746,0.116121,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0732","Rural Short","Weather",null,9,6201,1.237231,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0733","Rural Short","Weather",null,16,6201,2.1995209999999998,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0745","Rural Short","Weather",null,6,5235,0.69632899999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0818","Rural Short","Weather",null,12,4431,1.1787700000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0819","Rural Short","Weather",null,7,6201,0.96229100000000001,1.55E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0850","Rural Short","Weather",null,13,1746,0.50319199999999997,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0851","Rural Short","Weather",null,4,1746,0.15482799999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:09","DT-0886","Rural Short","Weather",null,6,1746,0.232243,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0899","Rural Short","Weather",null,8,6201,1.099761,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-0919","Rural Short","Weather",null,7,8873,1.3769400000000001,1.55E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10155","Rural Short","Weather",null,5,6201,0.68735000000000002,1.11E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10191","Rural Short","Weather",null,2,1746,7.7413999999999997E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10196","Rural Short","Weather",null,1020,13851,313.20431000000002,2.2612E-2,"Yes"]
[null,"17-03-2018","09:09","DT-10197","Rural Short","Weather",null,3,1746,0.116121,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10208","Rural Short","Weather",null,7,1746,0.27095000000000002,1.55E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10255","Rural Short","Weather",null,5,1746,0.19353600000000001,1.11E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10283","Rural Short","Weather",null,2,1746,7.7413999999999997E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10318","Rural Short","Weather",null,1,6450,0.14299000000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10383","Rural Short","Weather",null,1,10191,0.22592400000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10500","Rural Short","Weather",null,8,8873,1.573645,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10582","Rural Short","Weather",null,2,1746,7.7413999999999997E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10583","Rural Short","Weather",null,1020,1746,39.481245000000001,2.2612E-2,"Yes"]
[null,"17-03-2018","09:09","DT-10594","Rural Short","Weather",null,1,5235,0.11605500000000001,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10625","Rural Short","Weather",null,1,1746,3.8706999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10667","Rural Short","Weather",null,0,6581,0,0,"Yes"]
[null,"17-03-2018","09:09","DT-10695","Rural Short","Weather",null,24,11956,6.3612659999999996,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:09","DT-10696","Rural Short","Weather",null,1,1746,3.8706999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10743","Rural Short","Weather",null,4,5235,0.46421899999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:09","DT-10745","Rural Short","Weather",null,1020,13851,313.20431000000002,2.2612E-2,"Yes"]
[null,"17-03-2018","09:09","DT-10779","Rural Short","Weather",null,1020,1746,39.481245000000001,2.2612E-2,"Yes"]
[null,"17-03-2018","09:21","DT-0137","Rural Short","Weather",null,6,4541,0.60401700000000003,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0138","Rural Short","Weather",null,17,4541,1.711382,3.77E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0139","Rural Short","Weather",null,13,4541,1.3087040000000001,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0287","Rural Short","Weather",null,10,4541,1.0066949999999999,2.22E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0288","Rural Short","Weather",null,11,4541,1.1073649999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0433","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0563","Rural Short","Weather",null,2,4541,0.20133899999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0600","Rural Short","Weather",null,4,4541,0.40267799999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0601","Rural Short","Weather",null,4,4541,0.40267799999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0602","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0608","Rural Short","Weather",null,2,4541,0.20133899999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0618","Rural Short","Weather",null,5,4541,0.50334800000000002,1.11E-4,"Yes"]
[null,"17-03-2018","09:21","DT-0684","Rural Short","Weather",null,102,4541,10.268288999999999,2.261E-3,"Yes"]
[null,"17-03-2018","09:21","DT-0685","Rural Short","Weather",null,2,4541,0.20133899999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0693","Rural Short","Weather",null,3,4541,0.30200900000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0712","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0736","Rural Short","Weather",null,3,4541,0.30200900000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0856","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0883","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0884","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0885","Rural Short","Weather",null,1,4541,0.10067,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:21","DT-0947","Rural Short","Weather",null,3,4541,0.30200900000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:21","DT-10485","Rural Short","Weather",null,2,4541,0.20133899999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-1278","Rural Short","Weather",null,27,4289,2.5672389999999998,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","09:31","DT-1279","Rural Short","Weather",null,18,4289,1.711492,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","09:31","DT-1282","Rural Short","Weather",null,36,4289,3.4229850000000002,7.9799999999999999E-4,"Yes"]
[null,"17-03-2018","09:31","DT-1291","Rural Short","Weather",null,2,4289,0.190166,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-1292","Rural Short","Weather",null,1,4289,9.5083000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-1305","Rural Short","Weather",null,1,4289,9.5083000000000001E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-1307","Rural Short","Weather",null,5,10169,1.127183,1.11E-4,"Yes"]
[null,"17-03-2018","09:31","DT-1997","Rural Short","Weather",null,6,4289,0.57049700000000003,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2107","Rural Short","Weather",null,14,4289,1.331161,3.1E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2169","Rural Short","Weather",null,8,3929,0.69681700000000002,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2249","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2313","Rural Short","Weather",null,243,4289,23.105148,5.3870000000000003E-3,"Yes"]
[null,"17-03-2018","09:31","DT-2362","Rural Short","Weather",null,1,5609,0.124346,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2369","Rural Short","Weather",null,7,3929,0.60971399999999998,1.55E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2372","Rural Short","Weather",null,4,5609,0.49738399999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2374","Rural Short","Weather",null,25,5609,3.1086499999999999,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2375","Rural Short","Weather",null,6,5609,0.74607599999999996,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2392","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2405","Rural Short","Weather",null,2,3929,0.174204,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2428","Rural Short","Weather",null,243,4289,23.105148,5.3870000000000003E-3,"Yes"]
[null,"17-03-2018","09:31","DT-2444","Rural Short","Weather",null,7,3929,0.60971399999999998,1.55E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2451","Rural Short","Weather",null,1,10169,0.225437,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2513","Rural Short","Weather",null,5,3929,0.43551000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2514","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2540","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2541","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2542","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2543","Rural Short","Weather",null,6,3929,0.52261199999999997,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2551","Rural Short","Weather",null,85,3929,7.4036759999999999,1.884E-3,"Yes"]
[null,"17-03-2018","09:31","DT-2586","Rural Short","Weather",null,4,3929,0.348408,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2595","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2611","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2623","Rural Short","Weather",null,4,5609,0.49738399999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2680","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2740","Rural Short","Weather",null,1,5609,0.124346,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2747","Rural Short","Weather",null,4,3929,0.348408,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2748","Rural Short","Weather",null,5,3929,0.43551000000000001,1.11E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2827","Rural Short","Weather",null,29,4289,2.7574040000000002,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2833","Rural Short","Weather",null,8,5609,0.99476799999999999,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2834","Rural Short","Weather",null,7,5609,0.87042200000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2863","Rural Short","Weather",null,25,4289,2.3770730000000002,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","09:31","DT-2869","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2900","Rural Short","Weather",null,3,4289,0.28524899999999997,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2905","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2934","Rural Short","Weather",null,85,3929,7.4036759999999999,1.884E-3,"Yes"]
[null,"17-03-2018","09:31","DT-2949","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-2956","Rural Short","Weather",null,85,3929,7.4036759999999999,1.884E-3,"Yes"]
[null,"17-03-2018","09:31","DT-3166","Rural Short","Weather",null,9,5609,1.1191139999999999,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:31","DT-3167","Rural Short","Weather",null,2,5609,0.248692,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3169","Rural Short","Weather",null,2,3929,0.174204,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3179","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3186","Rural Short","Weather",null,2,3929,0.174204,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3301","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3304","Rural Short","Weather",null,2,3929,0.174204,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3328","Rural Short","Weather",null,3,3929,0.26130599999999998,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3387","Rural Short","Weather",null,1,3929,8.7101999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:31","DT-3462","Rural Short","Weather",null,243,4289,23.105148,5.3870000000000003E-3,"Yes"]
[null,"17-03-2018","09:31","DT-3463","Rural Short","Weather",null,243,4289,23.105148,5.3870000000000003E-3,"Yes"]
[null,"17-03-2018","09:31","DT-3464","Rural Short","Weather",null,3,4289,0.28524899999999997,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:33","DT-1233","Urban","Weather",null,69,4287,9.2153340000000004,2.15E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1234","Urban","Weather",null,94,4287,12.554223,2.928E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1246","Urban","Weather",null,64,4287,8.5475560000000002,1.9940000000000001E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1247","Urban","Weather",null,92,5102,14.623010000000001,2.8660000000000001E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1249","Urban","Weather",null,42,4287,5.6093339999999996,1.3079999999999999E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1250","Urban","Weather",null,89,4287,11.886445,2.7729999999999999E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1251","Urban","Weather",null,62,4287,8.2804450000000003,1.9319999999999999E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1252","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-1253","Urban","Weather",null,135,7769,32.674382000000001,4.2059999999999997E-3,"Yes"]
[null,"17-03-2018","09:33","DT-1414","Urban","Weather",null,4,4287,0.53422199999999997,1.25E-4,"Yes"]
[null,"17-03-2018","09:33","DT-1909","Urban","Weather",null,3,4287,0.400667,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2207","Urban","Weather",null,3,4287,0.400667,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2217","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2303","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2765","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2771","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-2821","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-3155","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-3193","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-3217","Urban","Weather",null,31,10167,9.818899,9.6599999999999995E-4,"Yes"]
[null,"17-03-2018","09:33","DT-3319","Urban","Weather",null,1,4287,0.13355600000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:33","DT-3456","Urban","Weather",null,804,4287,107.37867199999999,2.5048000000000001E-2,"Yes"]
[null,"17-03-2018","09:35","DT-1277","Rural Short","Weather",null,11,3145,0.76693699999999998,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:35","DT-1280","Rural Short","Weather",null,28,3145,1.9522040000000001,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","09:35","DT-1281","Rural Short","Weather",null,17,3145,1.1852659999999999,3.77E-4,"Yes"]
[null,"17-03-2018","09:35","DT-1283","Rural Short","Weather",null,7,3145,0.48805100000000001,1.55E-4,"Yes"]
[null,"17-03-2018","09:35","DT-1284","Rural Short","Weather",null,376,3145,26.215305000000001,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-1285","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1304","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1306","Rural Short","Weather",null,26,3145,1.8127599999999999,5.7600000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-1308","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1309","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1779","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1781","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1919","Rural Short","Weather",null,4,3925,0.34805399999999997,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1983","Rural Short","Weather",null,4,3145,0.27888600000000002,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:35","DT-1985","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2045","Rural Short","Weather",null,13,3145,0.90637999999999996,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2057","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2093","Rural Short","Weather",null,11,3145,0.76693699999999998,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2121","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2122","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2167","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2184","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2224","Rural Short","Weather",null,5,3925,0.43506699999999998,1.11E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2226","Rural Short","Weather",null,5,3925,0.43506699999999998,1.11E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2274","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2295","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2307","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2359","Rural Short","Weather",null,12,3145,0.83665900000000004,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2401","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2407","Rural Short","Weather",null,12,3145,0.83665900000000004,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2408","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2442","Rural Short","Weather",null,7,6209,0.96353200000000006,1.55E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2459","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2469","Rural Short","Weather",null,16,3145,1.115545,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2470","Rural Short","Weather",null,4,3145,0.27888600000000002,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2471","Rural Short","Weather",null,2,3145,0.13944300000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2473","Rural Short","Weather",null,63,3145,4.3924580000000004,1.397E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2474","Rural Short","Weather",null,36,3145,2.509976,7.9799999999999999E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2531","Rural Short","Weather",null,376,12925,107.736987,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2535","Rural Short","Weather",null,28,3145,1.9522040000000001,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2567","Rural Short","Weather",null,376,6209,51.755431000000002,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2581","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2640","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2646","Rural Short","Weather",null,1,10165,0.22534799999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2660","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2671","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2675","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2727","Rural Short","Weather",null,376,6209,51.755431000000002,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2728","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2799","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-2803","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2828","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2844","Rural Short","Weather",null,21,3145,1.464153,4.66E-4,"Yes"]
[null,"17-03-2018","09:35","DT-2854","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2878","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2886","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2895","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2958","Rural Short","Weather",null,1,6209,0.13764699999999999,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-2972","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-3015","Rural Short","Weather",null,376,3145,26.215305000000001,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-3016","Rural Short","Weather",null,376,3145,26.215305000000001,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-3020","Rural Short","Weather",null,64,3925,5.5688570000000004,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","09:35","DT-3021","Rural Short","Weather",null,14,3925,1.2181869999999999,3.1E-4,"Yes"]
[null,"17-03-2018","09:35","DT-3022","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3023","Rural Short","Weather",null,12,3145,0.83665900000000004,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-3045","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3056","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3057","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3074","Rural Short","Weather",null,2,3925,0.17402699999999999,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3092","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3131","Rural Short","Weather",null,15,3145,1.0458229999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","09:35","DT-3133","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3168","Rural Short","Weather",null,3,3145,0.20916499999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3215","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3222","Rural Short","Weather",null,1,3925,8.7012999999999993E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3227","Rural Short","Weather",null,3,3925,0.26103999999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:35","DT-3275","Rural Short","Weather",null,9,3145,0.627494,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:35","DT-3350","Rural Short","Weather",null,376,3145,26.215305000000001,8.3359999999999997E-3,"Yes"]
[null,"17-03-2018","09:35","DT-3390","Rural Short","Weather",null,1,3145,6.9722000000000006E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:37","DT-1070","Urban","Weather",null,30,3143,2.9374750000000001,9.3499999999999996E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1071","Urban","Weather",null,9,3143,0.88124199999999997,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1072","Urban","Weather",null,1,3143,9.7916000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:37","DT-1083","Urban","Weather",null,14,3143,1.370822,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1085","Urban","Weather",null,20,3143,1.9583159999999999,6.2299999999999996E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1086","Urban","Weather",null,31,3143,3.0353910000000002,9.6599999999999995E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1102","Urban","Weather",null,30,3143,2.9374750000000001,9.3499999999999996E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1103","Urban","Weather",null,6,3143,0.58749499999999999,1.8699999999999999E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1104","Urban","Weather",null,1,3143,9.7916000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:37","DT-1105","Urban","Weather",null,7,3143,0.68541099999999999,2.1800000000000001E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1106","Urban","Weather",null,14,3143,1.370822,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","09:37","DT-1768","Urban","Weather",null,4,3143,0.39166299999999998,1.25E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2136","Urban","Weather",null,1,3143,9.7916000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:37","DT-2142","Urban","Weather",null,13,3143,1.2729060000000001,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2182","Urban","Weather",null,15,5388,2.5178349999999998,4.6700000000000002E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2236","Urban","Weather",null,19,3143,1.860401,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2255","Urban","Weather",null,13,3143,1.2729060000000001,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2563","Urban","Weather",null,21,3143,2.0562320000000001,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2600","Urban","Weather",null,27,3143,2.6437270000000002,8.4099999999999995E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2963","Urban","Weather",null,1,3143,9.7916000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:37","DT-2964","Urban","Weather",null,14,3143,1.370822,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","09:37","DT-2987","Urban","Weather",null,21,3143,2.0562320000000001,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","09:37","DT-3202","Urban","Weather",null,4,3143,0.39166299999999998,1.25E-4,"Yes"]
[null,"17-03-2018","09:37","DT-3204","Urban","Weather",null,38,3143,3.7208009999999998,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","09:37","DT-3209","Urban","Weather",null,17,3143,1.664569,5.2999999999999998E-4,"Yes"]
[null,"17-03-2018","09:37","DT-3236","Urban","Weather",null,21,3143,2.0562320000000001,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0118","Rural Short","Weather",null,28,4402,2.7324609999999998,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0122","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0123","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0153","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0154","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0155","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0157","Rural Short","Weather",null,1,4402,9.7587999999999994E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0198","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0205","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0207","Rural Short","Weather",null,14,3312,1.027933,3.1E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0208","Rural Short","Weather",null,12,3312,0.88108500000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0209","Rural Short","Weather",null,12,3312,0.88108500000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0210","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0221","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0222","Rural Short","Weather",null,13,3312,0.95450900000000005,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0223","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0226","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0229","Rural Short","Weather",null,16,3312,1.1747810000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0230","Rural Short","Weather",null,15,3312,1.1013569999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0231","Rural Short","Weather",null,15,3312,1.1013569999999999,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0258","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0267","Rural Short","Weather",null,17,3312,1.2482040000000001,3.77E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0279","Rural Short","Weather",null,9,3312,0.66081400000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0280","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0281","Rural Short","Weather",null,24,3312,1.7621709999999999,5.3200000000000003E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0284","Rural Short","Weather",null,13,3312,0.95450900000000005,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0295","Rural Short","Weather",null,13,3312,0.95450900000000005,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0296","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0297","Rural Short","Weather",null,25,3312,1.8355950000000001,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0298","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0299","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0303","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0312","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0319","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0322","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0324","Rural Short","Weather",null,12,3312,0.88108500000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0326","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0327","Rural Short","Weather",null,17,3312,1.2482040000000001,3.77E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0328","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0329","Rural Short","Weather",null,9,3312,0.66081400000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0330","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0354","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0355","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0359","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0366","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0374","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0375","Rural Short","Weather",null,16,3312,1.1747810000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0399","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0401","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0405","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0410","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0430","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0446","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0447","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0453","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0492","Rural Short","Weather",null,20,3312,1.4684759999999999,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0509","Rural Short","Weather",null,9,3312,0.66081400000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0554","Rural Short","Weather",null,12,3312,0.88108500000000001,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0595","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0622","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0667","Rural Short","Weather",null,9,3312,0.66081400000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0668","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0669","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0697","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0704","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0705","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0706","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0722","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0744","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0793","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0794","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0795","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0796","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0836","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0837","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0838","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0839","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0854","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0855","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0860","Rural Short","Weather",null,16,3312,1.1747810000000001,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0871","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0891","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0906","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-0928","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0933","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-0949","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10001","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10002","Rural Short","Weather",null,14,3312,1.027933,3.1E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10003","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10004","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10005","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10020","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10021","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10056","Rural Short","Weather",null,8,3312,0.58738999999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10057","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10058","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10059","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10060","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10061","Rural Short","Weather",null,9,3312,0.66081400000000001,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10062","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10086","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10087","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10088","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10099","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10100","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10101","Rural Short","Weather",null,10,3312,0.73423799999999995,2.22E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10102","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10103","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10104","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10179","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10180","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10181","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10182","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10183","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10184","Rural Short","Weather",null,931,3312,68.357541999999995,2.0639000000000001E-2,"Yes"]
[null,"17-03-2018","09:38","DT-10185","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10186","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10262","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10263","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10264","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10265","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10274","Rural Short","Weather",null,931,3312,68.357541999999995,2.0639000000000001E-2,"Yes"]
[null,"17-03-2018","09:38","DT-10328","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10409","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10413","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10417","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10467","Rural Short","Weather",null,931,3312,68.357541999999995,2.0639000000000001E-2,"Yes"]
[null,"17-03-2018","09:38","DT-10489","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10492","Rural Short","Weather",null,931,3312,68.357541999999995,2.0639000000000001E-2,"Yes"]
[null,"17-03-2018","09:38","DT-10495","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10498","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10595","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10596","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10597","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10598","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10601","Rural Short","Weather",null,7,3312,0.51396600000000003,1.55E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10602","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10605","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10606","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10607","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10608","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10609","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10610","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10628","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10633","Rural Short","Weather",null,11,3312,0.80766199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10641","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10642","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10653","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10654","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10655","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10685","Rural Short","Weather",null,1,3312,7.3424000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10706","Rural Short","Weather",null,3,3312,0.22027099999999999,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10778","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10785","Rural Short","Weather",null,2,3312,0.14684800000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-10826","Rural Short","Weather",null,6,3312,0.44054300000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10837","Rural Short","Weather",null,5,3312,0.36711899999999997,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-10838","Rural Short","Weather",null,4,3312,0.29369499999999998,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","09:38","DT-1260","Rural Short","Weather",null,70,4282,6.6449410000000002,1.552E-3,"Yes"]
[null,"17-03-2018","09:38","DT-1261","Rural Short","Weather",null,136,5047,15.216635999999999,3.0149999999999999E-3,"Yes"]
[null,"17-03-2018","09:38","DT-1264","Rural Short","Weather",null,1,4282,9.4927999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-1415","Rural Short","Weather",null,6,4282,0.56956600000000002,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:38","DT-1470","Rural Short","Weather",null,5,4282,0.47463899999999998,1.11E-4,"Yes"]
[null,"17-03-2018","09:38","DT-2456","Rural Short","Weather",null,1,4282,9.4927999999999998E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:38","DT-2656","Rural Short","Weather",null,3,4282,0.28478300000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:38","DT-2823","Rural Short","Weather",null,8,4282,0.75942200000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:38","DT-3446","Rural Short","Weather",null,980,4282,93.029173999999998,2.1725999999999999E-2,"Yes"]
[null,"17-03-2018","09:41","DT-1054","Urban","Weather",null,31,1589,1.5345960000000001,9.6599999999999995E-4,"Yes"]
[null,"17-03-2018","09:41","DT-1056","Urban","Weather",null,20,1589,0.990062,6.2299999999999996E-4,"Yes"]
[null,"17-03-2018","09:41","DT-1057","Urban","Weather",null,44,1589,2.1781359999999999,1.371E-3,"Yes"]
[null,"17-03-2018","09:41","DT-1059","Urban","Weather",null,1,13108,0.408362,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-1060","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-1101","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-1200","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-1201","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-1961","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2051","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2140","Urban","Weather",null,3,1589,0.148509,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2232","Urban","Weather",null,27,1589,1.336584,8.4099999999999995E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2311","Urban","Weather",null,23,1589,1.138571,7.1699999999999997E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2312","Urban","Weather",null,47,1589,2.3266460000000002,1.464E-3,"Yes"]
[null,"17-03-2018","09:41","DT-2329","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2330","Urban","Weather",null,50,1589,2.475155,1.5579999999999999E-3,"Yes"]
[null,"17-03-2018","09:41","DT-2411","Urban","Weather",null,6,4399,0.822268,1.8699999999999999E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2412","Urban","Weather",null,7,1589,0.346522,2.1800000000000001E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2413","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2414","Urban","Weather",null,444,1589,21.979375999999998,1.3832000000000001E-2,"Yes"]
[null,"17-03-2018","09:41","DT-2415","Urban","Weather",null,18,1589,0.89105599999999996,5.6099999999999998E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2430","Urban","Weather",null,21,1589,1.0395650000000001,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2431","Urban","Weather",null,11,1589,0.54453399999999996,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2432","Urban","Weather",null,9,1589,0.44552799999999998,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2439","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2476","Urban","Weather",null,10,1589,0.495031,3.1199999999999999E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2499","Urban","Weather",null,12,1589,0.59403700000000004,3.7399999999999998E-4,"Yes"]
[null,"17-03-2018","09:41","DT-2752","Urban","Weather",null,3,1589,0.148509,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2753","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2840","Urban","Weather",null,444,1589,21.979375999999998,1.3832000000000001E-2,"Yes"]
[null,"17-03-2018","09:41","DT-2846","Urban","Weather",null,38,1589,1.8811180000000001,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","09:41","DT-2911","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-2933","Urban","Weather",null,2,1589,9.9005999999999997E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:41","DT-3093","Urban","Weather",null,14,1589,0.69304299999999996,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","09:41","DT-3130","Urban","Weather",null,3,1589,0.148509,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:41","DT-3225","Urban","Weather",null,444,1589,21.979375999999998,1.3832000000000001E-2,"Yes"]
[null,"17-03-2018","09:41","DT-3238","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-3273","Urban","Weather",null,19,1589,0.94055900000000003,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","09:41","DT-3359","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:41","DT-3360","Urban","Weather",null,1,1589,4.9502999999999998E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:44","DT-0276","Urban","Weather",null,1,2012,6.2681000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:44","DT-0277","Urban","Weather",null,1,2012,6.2681000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:44","DT-0681","Urban","Weather",null,2,2012,0.125362,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:44","DT-0905","Urban","Weather",null,4,2012,0.250724,1.25E-4,"Yes"]
[null,"17-03-2018","09:44","DT-10313","Urban","Weather",null,4,4756,0.59266600000000003,1.25E-4,"Yes"]
[null,"17-03-2018","09:44","DT-10555","Urban","Weather",null,4,2012,0.250724,1.25E-4,"Yes"]
[null,"17-03-2018","09:44","DT-10580","Urban","Weather",null,4,2012,0.250724,1.25E-4,"Yes"]
[null,"17-03-2018","09:44","DT-10707","Urban","Weather",null,2,2012,0.125362,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:50","DT-1312","Urban","Weather",null,1,3130,9.7511E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:50","DT-2482","Urban","Weather",null,2,3130,0.195022,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:50","DT-3139","Urban","Weather",null,1,3130,9.7511E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:50","DT-3441","Urban","Weather",null,2,3130,0.195022,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:51","DT-1041","Urban","Weather",null,8,3739,0.931867,2.4899999999999998E-4,"Yes"]
[null,"17-03-2018","09:51","DT-1042","Urban","Weather",null,96,3739,11.182404,2.9910000000000002E-3,"Yes"]
[null,"17-03-2018","09:51","DT-1043","Urban","Weather",null,85,3739,9.9010870000000004,2.6480000000000002E-3,"Yes"]
[null,"17-03-2018","09:51","DT-1045","Urban","Weather",null,125,3739,14.560422000000001,3.8939999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-1046","Urban","Weather",null,34,3739,3.9604349999999999,1.059E-3,"Yes"]
[null,"17-03-2018","09:51","DT-1047","Urban","Weather",null,10,3739,1.1648339999999999,3.1199999999999999E-4,"Yes"]
[null,"17-03-2018","09:51","DT-1048","Urban","Weather",null,185,3739,21.549424999999999,5.7629999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-1053","Urban","Weather",null,33,3739,3.8439519999999998,1.0280000000000001E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2165","Urban","Weather",null,1,3739,0.116483,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:51","DT-2239","Urban","Weather",null,183,3739,21.316458000000001,5.7010000000000003E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2289","Urban","Weather",null,78,3739,9.0857039999999998,2.4299999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2298","Urban","Weather",null,59,3739,6.8725189999999996,1.838E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2504","Urban","Weather",null,1,3739,0.116483,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:51","DT-2736","Urban","Weather",null,1,3739,0.116483,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:51","DT-2796","Urban","Weather",null,11,3739,1.281317,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","09:51","DT-2829","Urban","Weather",null,41,3739,4.7758190000000003,1.2769999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2830","Urban","Weather",null,25,3739,2.9120840000000001,7.7899999999999996E-4,"Yes"]
[null,"17-03-2018","09:51","DT-2843","Urban","Weather",null,82,3739,9.5516369999999995,2.555E-3,"Yes"]
[null,"17-03-2018","09:51","DT-2877","Urban","Weather",null,13,3739,1.514284,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","09:51","DT-2906","Urban","Weather",null,54,3739,6.2901020000000001,1.6819999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-3141","Urban","Weather",null,26,3739,3.0285679999999999,8.0999999999999996E-4,"Yes"]
[null,"17-03-2018","09:51","DT-3291","Urban","Weather",null,55,3739,6.4065859999999999,1.7129999999999999E-3,"Yes"]
[null,"17-03-2018","09:51","DT-3299","Urban","Weather",null,79,3739,9.2021870000000003,2.4610000000000001E-3,"Yes"]
[null,"17-03-2018","09:51","DT-3313","Urban","Weather",null,21,3739,2.446151,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","09:51","DT-3343","Urban","Weather",null,92,3739,10.716471,2.8660000000000001E-3,"Yes"]
[null,"17-03-2018","09:51","DT-3428","Urban","Weather",null,2,3739,0.23296700000000001,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:52","DT-1076","Rural Short","Weather",null,21,2403,1.1187149999999999,4.66E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1077","Rural Short","Weather",null,17,2403,0.90562600000000004,3.77E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1078","Rural Short","Weather",null,18,2403,0.95889899999999995,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1079","Rural Short","Weather",null,16,2403,0.85235399999999995,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1080-1","Rural Short","Weather",null,34,2403,1.811253,7.54E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1107","Rural Short","Weather",null,5,2403,0.26636100000000001,1.11E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1108","Rural Short","Weather",null,6,2403,0.319633,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1109","Rural Short","Weather",null,12,2403,0.639266,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-1110","Rural Short","Weather",null,2,2403,0.106544,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-1111","Rural Short","Weather",null,267,2403,14.223663,5.9189999999999998E-3,"Yes"]
[null,"17-03-2018","09:52","DT-1270","Rural Short","Weather",null,1,2403,5.3272E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-1778","Rural Short","Weather",null,6,10148,1.349826,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2058","Rural Short","Weather",null,7,2403,0.37290499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2067","Rural Short","Weather",null,30,2403,1.5981639999999999,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2131","Rural Short","Weather",null,1,2403,5.3272E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-2238","Rural Short","Weather",null,34,2403,1.811253,7.54E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2363","Rural Short","Weather",null,1,2403,5.3272E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-2536","Rural Short","Weather",null,8,2403,0.42617699999999997,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2587","Rural Short","Weather",null,267,2403,14.223663,5.9189999999999998E-3,"Yes"]
[null,"17-03-2018","09:52","DT-2730","Rural Short","Weather",null,7,2403,0.37290499999999999,1.55E-4,"Yes"]
[null,"17-03-2018","09:52","DT-2800","Rural Short","Weather",null,267,2403,14.223663,5.9189999999999998E-3,"Yes"]
[null,"17-03-2018","09:52","DT-2849-1","Rural Short","Weather",null,2,2403,0.106544,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-2849-2","Rural Short","Weather",null,2,2403,0.106544,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-2917","Rural Short","Weather",null,1,2403,5.3272E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-3027","Rural Short","Weather",null,1,2403,5.3272E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:52","DT-3224","Rural Short","Weather",null,30,2403,1.5981639999999999,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","09:52","DT-3267","Rural Short","Weather",null,3,2403,0.15981600000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:54","DT-1994","Rural Short","Weather",null,3,2228,0.148178,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2100","Rural Short","Weather",null,46,2228,2.2720579999999999,1.0200000000000001E-3,"Yes"]
[null,"17-03-2018","09:54","DT-2160","Rural Short","Weather",null,36,2228,1.778132,7.9799999999999999E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2166","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2218","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2219","Rural Short","Weather",null,2,2228,9.8784999999999998E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2220","Rural Short","Weather",null,3,2228,0.148178,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2222","Rural Short","Weather",null,22,2228,1.0866370000000001,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2227","Rural Short","Weather",null,46,2228,2.2720579999999999,1.0200000000000001E-3,"Yes"]
[null,"17-03-2018","09:54","DT-2246","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2508","Rural Short","Weather",null,15,2228,0.74088900000000002,3.3300000000000002E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2509","Rural Short","Weather",null,27,2228,1.333599,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2582","Rural Short","Weather",null,2,2228,9.8784999999999998E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2601","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2679","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2749","Rural Short","Weather",null,29,2228,1.4323840000000001,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2767","Rural Short","Weather",null,23,2228,1.136029,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","09:54","DT-2935","Rural Short","Weather",null,2,2228,9.8784999999999998E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2943","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-2945","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-3048","Rural Short","Weather",null,2,2228,9.8784999999999998E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-3177","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-3232","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:54","DT-3246","Rural Short","Weather",null,274,2228,13.533564,6.0740000000000004E-3,"Yes"]
[null,"17-03-2018","09:54","DT-3268","Rural Short","Weather",null,1,2228,4.9392999999999999E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","09:55","DT-10744","Urban","Weather",null,5,4265,0.66435100000000002,1.56E-4,"Yes"]
[null,"17-03-2018","09:55","DT-1112","Urban","Weather",null,2,4265,0.26573999999999998,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:55","DT-1113","Urban","Weather",null,14,4265,1.8601829999999999,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","09:55","DT-1272","Urban","Weather",null,471,4265,62.581856000000002,1.4673E-2,"Yes"]
[null,"17-03-2018","09:55","DT-1273","Urban","Weather",null,471,4265,62.581856000000002,1.4673E-2,"Yes"]
[null,"17-03-2018","09:55","DT-1274","Urban","Weather",null,44,4817,6.6029470000000003,1.371E-3,"Yes"]
[null,"17-03-2018","09:55","DT-1275","Urban","Weather",null,1,4817,0.15006700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-1276","Urban","Weather",null,17,4817,2.551139,5.2999999999999998E-4,"Yes"]
[null,"17-03-2018","09:55","DT-1413","Urban","Weather",null,1,4817,0.15006700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-1769","Urban","Weather",null,1,4265,0.13286999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-2110","Urban","Weather",null,4,4817,0.60026800000000002,1.25E-4,"Yes"]
[null,"17-03-2018","09:55","DT-2149","Urban","Weather",null,4,4265,0.53148099999999998,1.25E-4,"Yes"]
[null,"17-03-2018","09:55","DT-2192","Urban","Weather",null,2,4265,0.26573999999999998,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:55","DT-2252","Urban","Weather",null,1,4817,0.15006700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-2293","Urban","Weather",null,22,4817,3.3014739999999998,6.8499999999999995E-4,"Yes"]
[null,"17-03-2018","09:55","DT-2539","Urban","Weather",null,3,4265,0.39861099999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:55","DT-2555","Urban","Weather",null,1,4817,0.15006700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-2894","Urban","Weather",null,139,4265,18.468955000000001,4.3299999999999996E-3,"Yes"]
[null,"17-03-2018","09:55","DT-3062","Urban","Weather",null,1,4265,0.13286999999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-3063","Urban","Weather",null,4,4265,0.53148099999999998,1.25E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3064","Urban","Weather",null,13,4265,1.727312,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3065","Urban","Weather",null,13,4265,1.727312,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3066","Urban","Weather",null,19,4265,2.5245329999999999,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3067","Urban","Weather",null,4,4265,0.53148099999999998,1.25E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3068","Urban","Weather",null,18,4265,2.3916629999999999,5.6099999999999998E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3069","Urban","Weather",null,2,4265,0.26573999999999998,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:55","DT-3143","Urban","Weather",null,1,4817,0.15006700000000001,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:55","DT-3194","Urban","Weather",null,471,4265,62.581856000000002,1.4673E-2,"Yes"]
[null,"17-03-2018","09:55","DT-3260","Urban","Weather",null,38,4265,5.049067,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","09:55","DT-3260-1","Urban","Weather",null,38,4265,5.049067,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","09:55","DT-3311","Urban","Weather",null,19,4265,2.5245329999999999,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","09:55","DT-3391","Urban","Weather",null,2,4265,0.26573999999999998,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:55","DT-3447","Urban","Weather",null,29,4265,3.8532350000000002,9.0300000000000005E-4,"Yes"]
[null,"17-03-2018","09:56","DT-1001","Urban","Weather",null,2,3967,0.247173,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","09:56","DT-1002","Urban","Weather",null,35,3967,4.3255239999999997,1.09E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1003","Urban","Weather",null,57,3967,7.0444250000000004,1.776E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1004","Urban","Weather",null,8,13237,3.2990439999999999,2.4899999999999998E-4,"Yes"]
[null,"17-03-2018","09:56","DT-1005","Urban","Weather",null,1,13237,0.41238000000000002,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:56","DT-1008","Urban","Weather",null,67,3967,8.2802889999999998,2.0869999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1018","Urban","Weather",null,68,9064,19.201595000000001,2.1180000000000001E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1022","Urban","Weather",null,92,9064,25.978629000000002,2.8660000000000001E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1024","Urban","Weather",null,106,3967,13.100159,3.3019999999999998E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1159","Urban","Weather",null,1627,4384,222.21128999999999,5.0687000000000003E-2,"Yes"]
[null,"17-03-2018","09:56","DT-1160","Urban","Weather",null,3,4384,0.40973199999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:56","DT-1161","Urban","Weather",null,33,3967,4.0783509999999996,1.0280000000000001E-3,"Yes"]
[null,"17-03-2018","09:56","DT-1965","Urban","Weather",null,94,3967,11.617122,2.928E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2089","Urban","Weather",null,41,9064,11.577432,1.2769999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2202","Urban","Weather",null,38,3967,4.6962830000000002,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2223","Urban","Weather",null,1627,13237,670.94298900000001,5.0687000000000003E-2,"Yes"]
[null,"17-03-2018","09:56","DT-2388","Urban","Weather",null,86,3967,10.628431000000001,2.679E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2522","Urban","Weather",null,75,3967,9.2689800000000009,2.3370000000000001E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2606","Urban","Weather",null,41,3967,5.067043,1.2769999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2627","Urban","Weather",null,12,3967,1.4830369999999999,3.7399999999999998E-4,"Yes"]
[null,"17-03-2018","09:56","DT-2636","Urban","Weather",null,40,3967,4.9434560000000003,1.2459999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2637","Urban","Weather",null,49,3967,6.0557340000000002,1.5269999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2672","Urban","Weather",null,301,3967,37.199508000000002,9.3769999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2901","Urban","Weather",null,1,4384,0.136577,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:56","DT-2946","Urban","Weather",null,74,3967,9.1453939999999996,2.3050000000000002E-3,"Yes"]
[null,"17-03-2018","09:56","DT-2991","Urban","Weather",null,147,3967,18.167200999999999,4.5799999999999999E-3,"Yes"]
[null,"17-03-2018","09:56","DT-3017","Urban","Weather",null,1,3967,0.123586,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:56","DT-3026","Urban","Weather",null,3,3967,0.37075900000000001,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","09:56","DT-3095","Urban","Weather",null,1627,3967,201.07508000000001,5.0687000000000003E-2,"Yes"]
[null,"17-03-2018","09:56","DT-3148","Urban","Weather",null,4,13237,1.6495219999999999,1.25E-4,"Yes"]
[null,"17-03-2018","09:56","DT-3181","Urban","Weather",null,1,3967,0.123586,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","09:56","DT-3349","Urban","Weather",null,9,3967,1.1122780000000001,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","10:02","DT-1225","Urban","Weather",null,1,3172,9.8819000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:02","DT-1226","Urban","Weather",null,164,5256,26.853921,5.1089999999999998E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1227","Urban","Weather",null,83,5352,13.838936,2.5860000000000002E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1228","Urban","Weather",null,144,3172,14.229976000000001,4.4860000000000004E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1229","Urban","Weather",null,13,3172,1.284651,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","10:02","DT-1230","Urban","Weather",null,66,3172,6.5220719999999996,2.0560000000000001E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1231","Urban","Weather",null,94,3172,9.2890119999999996,2.928E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1235","Urban","Weather",null,68,10769,22.813545999999999,2.1180000000000001E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1236","Urban","Weather",null,90,3172,8.8937349999999995,2.8040000000000001E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1238","Urban","Weather",null,29,4948,4.4702950000000001,9.0300000000000005E-4,"Yes"]
[null,"17-03-2018","10:02","DT-1239","Urban","Weather",null,68,3172,6.7197110000000002,2.1180000000000001E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1242","Urban","Weather",null,91,3172,8.9925540000000002,2.8349999999999998E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1243","Urban","Weather",null,40,3172,3.9527709999999998,1.2459999999999999E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1244","Urban","Weather",null,90,3172,8.8937349999999995,2.8040000000000001E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1350","Urban","Weather",null,131,3172,12.945325,4.0810000000000004E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1441","Urban","Weather",null,86,3172,8.4984579999999994,2.679E-3,"Yes"]
[null,"17-03-2018","10:02","DT-1987","Urban","Weather",null,61,3172,6.0279759999999998,1.9E-3,"Yes"]
[null,"17-03-2018","10:02","DT-2265","Urban","Weather",null,76,3172,7.5102650000000004,2.3679999999999999E-3,"Yes"]
[null,"17-03-2018","10:02","DT-2724","Urban","Weather",null,39,3172,3.853952,1.2149999999999999E-3,"Yes"]
[null,"17-03-2018","10:02","DT-3075","Urban","Weather",null,1,3172,9.8819000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:02","DT-3170","Urban","Weather",null,1,3172,9.8819000000000004E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:02","DT-3455","Urban","Weather",null,79,6660,16.391165000000001,2.4610000000000001E-3,"Yes"]
[null,"17-03-2018","10:06","DT-0158","Rural Short","Weather",null,12,3307,0.87975499999999995,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0159","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0160","Rural Short","Weather",null,2,15819,0.70138299999999998,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0194-1","Rural Short","Weather",null,5,3307,0.36656499999999997,1.11E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0194-2","Rural Short","Weather",null,5,3307,0.36656499999999997,1.11E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0508","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0513","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0515","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:06","DT-0516","Rural Short","Weather",null,4,3307,0.29325200000000001,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0524","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0525","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0526","Rural Short","Weather",null,5,3307,0.36656499999999997,1.11E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0528","Rural Short","Weather",null,18,3307,1.3196330000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0594","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0606","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0666","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0670","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0671","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0672","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0792","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0880","Rural Short","Weather",null,5,3307,0.36656499999999997,1.11E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0894","Rural Short","Weather",null,11,3307,0.80644199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0895","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0896","Rural Short","Weather",null,8,3307,0.58650400000000003,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0897","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0898","Rural Short","Weather",null,11,3307,0.80644199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0912","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-0913","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-0914","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10016","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:06","DT-10038","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:06","DT-10192","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10193","Rural Short","Weather",null,11,3307,0.80644199999999999,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:06","DT-10202","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-10203","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10257","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10317","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10391","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10407","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10416","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10420","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10438","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10461","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10462","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10474","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:06","DT-10475","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10476","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10478","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10479","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10480","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10482","Rural Short","Weather",null,4,3307,0.29325200000000001,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10517-1","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10518-1","Rural Short","Weather",null,4,3307,0.29325200000000001,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10547","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10564","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10587","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10588","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10589","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-10644","Rural Short","Weather",null,1,3307,7.3313000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10668","Rural Short","Weather",null,2,3307,0.14662600000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10669","Rural Short","Weather",null,3,3307,0.219939,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:06","DT-10670","Rural Short","Weather",null,6,3307,0.43987799999999999,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:06","DT-10800","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:06","DT-10825","Rural Short","Weather",null,205,3307,15.029152,4.5450000000000004E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1029","Urban","Weather",null,58,3110,5.6194899999999999,1.807E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1030","Urban","Weather",null,137,3110,13.273622,4.2680000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1032","Urban","Weather",null,61,3110,5.9101530000000002,1.9E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1033","Urban","Weather",null,11,3110,1.0657650000000001,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:10","DT-1034","Urban","Weather",null,111,3110,10.754541,3.4580000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1099","Rural Short","Weather",null,18,4250,1.6959299999999999,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","10:10","DT-1147","Rural Short","Weather",null,52,4250,4.8993529999999996,1.1529999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1148","Rural Short","Weather",null,1,4250,9.4217999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:10","DT-1185","Rural Short","Weather",null,5,11660,1.292454,1.11E-4,"Yes"]
[null,"17-03-2018","10:10","DT-1186","Rural Short","Weather",null,98,4250,9.2333949999999998,2.173E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1836","Rural Short","Weather",null,51,4250,4.8051339999999998,1.1310000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-1999","Urban","Weather",null,1,3110,9.6888000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:10","DT-2193","Rural Short","Weather",null,20,4250,1.884366,4.4299999999999998E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2253","Urban","Weather",null,27,3110,2.6159690000000002,8.4099999999999995E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2317","Rural Short","Weather",null,6,4250,0.56530999999999998,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2515","Urban","Weather",null,38,3110,3.6817350000000002,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2608","Rural Short","Weather",null,31,4250,2.9207679999999998,6.87E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2650","Urban","Weather",null,38,3110,3.6817350000000002,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2682","Urban","Weather",null,90,3110,8.7198980000000006,2.8040000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2720","Rural Short","Weather",null,72,4250,6.7837189999999996,1.596E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2721","Rural Short","Weather",null,58,4250,5.4646629999999998,1.286E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2722","Rural Short","Weather",null,47,4250,4.428261,1.042E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2726","Urban","Weather",null,41,3110,3.9723980000000001,1.2769999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2739","Urban","Weather",null,24,3110,2.3253059999999999,7.4799999999999997E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2755","Urban","Weather",null,115,3110,11.142092,3.5829999999999998E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2766","Rural Short","Weather",null,1412,4250,133.036269,3.1302999999999997E-2,"Yes"]
[null,"17-03-2018","10:10","DT-2770","Urban","Weather",null,36,3110,3.487959,1.122E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2862","Urban","Weather",null,17,3110,1.647092,5.2999999999999998E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2870","Rural Short","Weather",null,60,4250,5.6530990000000001,1.33E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2879","Urban","Weather",null,55,3110,5.3288260000000003,1.7129999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2915","Urban","Weather",null,21,3110,2.034643,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2919","Rural Short","Weather",null,43,4250,4.0513880000000002,9.5299999999999996E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2920","Rural Short","Weather",null,1412,4250,133.036269,3.1302999999999997E-2,"Yes"]
[null,"17-03-2018","10:10","DT-2921","Rural Short","Weather",null,107,4250,10.08136,2.372E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2922","Rural Short","Weather",null,51,4250,4.8051339999999998,1.1310000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2923","Rural Short","Weather",null,155,4250,14.60384,3.4359999999999998E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2924","Rural Short","Weather",null,102,4250,9.6102690000000006,2.261E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2925","Rural Short","Weather",null,114,4250,10.740888999999999,2.5270000000000002E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2926","Rural Short","Weather",null,64,4250,6.029973,1.4189999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2929","Rural Short","Weather",null,86,4250,8.1027760000000004,1.9070000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2930","Rural Short","Weather",null,63,4250,5.9357540000000002,1.397E-3,"Yes"]
[null,"17-03-2018","10:10","DT-2931","Rural Short","Weather",null,44,4250,4.1456059999999999,9.7499999999999996E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2938","Urban","Weather",null,14,3110,1.3564290000000001,4.3600000000000003E-4,"Yes"]
[null,"17-03-2018","10:10","DT-2951","Rural Short","Weather",null,1,4250,9.4217999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:10","DT-2954","Urban","Weather",null,54,3110,5.2319389999999997,1.6819999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3028","Rural Short","Weather",null,1,4250,9.4217999999999996E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:10","DT-3218","Urban","Weather",null,33,3110,3.1972960000000001,1.0280000000000001E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3226","Urban","Weather",null,16,3110,1.5502039999999999,4.9799999999999996E-4,"Yes"]
[null,"17-03-2018","10:10","DT-3239","Urban","Weather",null,50,3110,4.8443880000000004,1.5579999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3282","Urban","Weather",null,21,3110,2.034643,6.5399999999999996E-4,"Yes"]
[null,"17-03-2018","10:10","DT-3296","Urban","Weather",null,145,3110,14.048724,4.5170000000000002E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3310","Urban","Weather",null,2,3110,0.193776,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:10","DT-3312","Urban","Weather",null,44,3110,4.2630610000000004,1.371E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3330","Rural Short","Weather",null,9,4250,0.84796499999999997,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","10:10","DT-3442","Urban","Weather",null,54,3110,5.2319389999999997,1.6819999999999999E-3,"Yes"]
[null,"17-03-2018","10:10","DT-3443","Rural Short","Weather",null,1412,4250,133.036269,3.1302999999999997E-2,"Yes"]
[null,"17-03-2018","10:10","DT-3443-1","Rural Short","Weather",null,1412,4250,133.036269,3.1302999999999997E-2,"Yes"]
[null,"17-03-2018","10:11","DT-1012","Urban","Weather",null,5,1449,0.22570799999999999,1.56E-4,"Yes"]
[null,"17-03-2018","10:11","DT-1013","Urban","Weather",null,34,1449,1.5348139999999999,1.059E-3,"Yes"]
[null,"17-03-2018","10:11","DT-1014","Urban","Weather",null,126,1449,5.6878409999999997,3.9249999999999997E-3,"Yes"]
[null,"17-03-2018","10:11","DT-1015","Urban","Weather",null,139,1449,6.2746810000000002,4.3299999999999996E-3,"Yes"]
[null,"17-03-2018","10:11","DT-1154","Urban","Weather",null,1,1449,4.5142000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:11","DT-1155","Urban","Weather",null,1,1449,4.5142000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:11","DT-1156-1","Urban","Weather",null,360,1449,16.250973999999999,1.1214999999999999E-2,"Yes"]
[null,"17-03-2018","10:11","DT-1156-2","Urban","Weather",null,2,1449,9.0283000000000002E-2,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:11","DT-1911","Urban","Weather",null,15,1449,0.67712399999999995,4.6700000000000002E-4,"Yes"]
[null,"17-03-2018","10:11","DT-2212","Urban","Weather",null,1,1449,4.5142000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:11","DT-2861","Urban","Weather",null,1,1449,4.5142000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:11","DT-2867-1","Urban","Weather",null,1,1449,4.5142000000000002E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:11","DT-2867-2","Urban","Weather",null,360,1449,16.250973999999999,1.1214999999999999E-2,"Yes"]
[null,"17-03-2018","10:11","DT-3457","Urban","Weather",null,3,1449,0.13542499999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:11","DT-3457-1","Urban","Weather",null,3,1449,0.13542499999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:11","DT-3457-2","Urban","Weather",null,3,1449,0.13542499999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:14","DT-10025","Rural Long","Weather",null,9,4726,48.945914999999999,1.0357E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10026","Rural Long","Weather",null,10,4726,54.384349999999998,1.1507E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10027","Rural Long","Weather",null,14,4726,76.138090000000005,1.6109999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10029","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10031","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10036","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10037","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10039","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10040","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10042","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10043","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10044","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10045","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10046","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10047","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10049","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10050","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10051","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10052","Rural Long","Weather",null,582,4726,3165.1691599999999,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10054","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10063","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10085","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10089","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10090","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10093","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10094","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10095","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10096","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10105","Rural Long","Weather",null,2,5716,13.155351,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10106","Rural Long","Weather",null,3,5716,19.733025999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10107","Rural Long","Weather",null,36,5716,236.79631800000001,4.1426999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10108","Rural Long","Weather",null,35,5716,230.21864199999999,4.0275999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10109","Rural Long","Weather",null,13,5716,85.509781000000004,1.4959999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10110","Rural Long","Weather",null,20,5716,131.55350999999999,2.3015000000000001E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10111","Rural Long","Weather",null,23,5716,151.28653600000001,2.6467000000000001E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10112","Rural Long","Weather",null,30,5716,197.330265,3.4521999999999997E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10121","Rural Long","Weather",null,8,4726,43.507480000000001,9.2060000000000006E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10122","Rural Long","Weather",null,18,4726,97.891829999999999,2.0712999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10123","Rural Long","Weather",null,11,4726,59.822785000000003,1.2658000000000001E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10124","Rural Long","Weather",null,23,4726,125.084005,2.6467000000000001E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10125","Rural Long","Weather",null,9,4726,48.945914999999999,1.0357E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10126","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10127","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10129","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10139","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10140","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10141","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10142","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10143","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10146","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10147","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10148","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10149","Rural Long","Weather",null,2,4251,9.7836590000000001,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10150","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10151","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10152","Rural Long","Weather",null,3,4726,16.315304999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10154","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10156","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10157","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10158","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10159","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10174","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10175","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10176","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10178","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10187","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10188","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10190","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10194","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10195","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10199","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10200","Rural Long","Weather",null,5,4461,25.667434,5.7540000000000004E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10201","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10205","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10206","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10210","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10212","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10214","Rural Long","Weather",null,1,5776,6.6467200000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10215","Rural Long","Weather",null,1,5776,6.6467200000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10216","Rural Long","Weather",null,2,5776,13.293441,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10217","Rural Long","Weather",null,2,5776,13.293441,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10218","Rural Long","Weather",null,1,5776,6.6467200000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10219","Rural Long","Weather",null,1,5776,6.6467200000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10220","Rural Long","Weather",null,4,5776,26.586881000000002,4.6030000000000003E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10221","Rural Long","Weather",null,1,5776,6.6467200000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10222","Rural Long","Weather",null,2,5776,13.293441,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10223","Rural Long","Weather",null,2,5776,13.293441,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10224","Rural Long","Weather",null,4,5776,26.586881000000002,4.6030000000000003E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10225","Rural Long","Weather",null,582,5776,3868.3912540000001,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10240","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10252","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10253","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10276","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10277","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10278","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10282","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10286","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10287","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10288","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10289","Rural Long","Weather",null,582,11721,7849.9677789999996,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10290","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10291","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10292","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10293","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10294","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10295","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10296","Rural Long","Weather",null,2,11721,26.975833999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10297","Rural Long","Weather",null,3,11721,40.463751000000002,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10298","Rural Long","Weather",null,2,11721,26.975833999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10299","Rural Long","Weather",null,2,11721,26.975833999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10300","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10301","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10302","Rural Long","Weather",null,4,11721,53.951669000000003,4.6030000000000003E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10303","Rural Long","Weather",null,2,14608,33.620252999999998,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10304","Rural Long","Weather",null,1,11721,13.487916999999999,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10305","Rural Long","Weather",null,2,11721,26.975833999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10315","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10322","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10329","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10335","Rural Long","Weather",null,582,5841,3911.924051,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10336","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10337","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10338","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10339","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10340","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10341","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10342","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10343","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10344","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10345","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10346","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10347","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10348","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10349","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10350","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10351","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10352","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10353","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10354","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10355","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10356","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10357","Rural Long","Weather",null,582,5841,3911.924051,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10358","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10359","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10360","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10361","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10362","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10363","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10364","Rural Long","Weather",null,582,5841,3911.924051,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10365","Rural Long","Weather",null,2,5841,13.443038,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10366","Rural Long","Weather",null,3,5841,20.164556999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10367","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10368","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10369","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10370","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10371","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10372","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10373","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10374","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10375","Rural Long","Weather",null,5,4461,25.667434,5.7540000000000004E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10376","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10377","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10378","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10379","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10380","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10381","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10382","Rural Long","Weather",null,582,4461,2987.6892979999998,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10394","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10395","Rural Long","Weather",null,3,4726,16.315304999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10397","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10398","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10400","Rural Long","Weather",null,1,5841,6.7215189999999998,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10401","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10402","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10418","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10419","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10426","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10442","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10444","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10445","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10447","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10448","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10449","Rural Long","Weather",null,3,4726,16.315304999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10450","Rural Long","Weather",null,3,5716,19.733025999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10451","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10452","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10453","Rural Long","Weather",null,2,5716,13.155351,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10454","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10455","Rural Long","Weather",null,3,5716,19.733025999999999,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10456","Rural Long","Weather",null,2,5716,13.155351,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10457","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10486","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10487","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10488","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10491","Rural Long","Weather",null,3,4461,15.400460000000001,3.4520000000000002E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10543","Rural Long","Weather",null,2,4726,10.87687,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10545","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10549","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10554","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10568","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10570","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10572","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10581","Rural Long","Weather",null,1,4251,4.8918299999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10624","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10627","Rural Long","Weather",null,1,5716,6.5776750000000002,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10647","Rural Long","Weather",null,18,13096,271.26352100000003,2.0712999999999999E-2,"Yes"]
[null,"17-03-2018","10:14","DT-10651","Rural Long","Weather",null,1,4461,5.1334869999999997,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10741","Rural Long","Weather",null,2,4461,10.266973999999999,2.3010000000000001E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10750","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10751","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10752","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10753","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10754","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10755","Rural Long","Weather",null,582,4251,2847.044879,0.66973499999999997,"Yes"]
[null,"17-03-2018","10:14","DT-10756","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10757","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10758","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10759","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10760","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10761","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10762","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10808","Rural Long","Weather",null,0,4251,0,0,"Yes"]
[null,"17-03-2018","10:14","DT-10822","Rural Long","Weather",null,1,4726,5.4384350000000001,1.1509999999999999E-3,"Yes"]
[null,"17-03-2018","10:14","DT-10829","Rural Long","Weather",null,0,4726,0,0,"Yes"]
[null,"17-03-2018","10:23","DT-1006","Rural Short","Weather",null,58,3369,4.3318700000000003,1.286E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1007","Rural Short","Weather",null,49,3369,3.6596829999999998,1.0859999999999999E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1010","Rural Short","Weather",null,99,3369,7.3940539999999997,2.1949999999999999E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1011","Rural Short","Weather",null,79,3369,5.9003059999999996,1.751E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1088","Rural Short","Weather",null,28,3369,2.0912480000000002,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","10:23","DT-1089","Rural Short","Weather",null,68,3369,5.0787440000000004,1.5070000000000001E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1090","Rural Short","Weather",null,184,5442,22.198457000000001,4.0790000000000002E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1091","Rural Short","Weather",null,76,8777,14.787887,1.6850000000000001E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1092","Rural Short","Weather",null,22,5427,2.6468479999999999,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","10:23","DT-1094","Rural Short","Weather",null,25,3369,1.8671850000000001,5.5400000000000002E-4,"Yes"]
[null,"17-03-2018","10:23","DT-1162","Rural Short","Weather",null,74,3369,5.5268689999999996,1.6410000000000001E-3,"Yes"]
[null,"17-03-2018","10:23","DT-1833","Rural Short","Weather",null,30,3369,2.2406229999999998,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","10:23","DT-1924","Rural Short","Weather",null,1,3369,7.4687000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:23","DT-1940","Rural Short","Weather",null,98,3369,7.3193669999999997,2.173E-3,"Yes"]
[null,"17-03-2018","10:23","DT-2035","Rural Short","Weather",null,61,3369,4.5559320000000003,1.3519999999999999E-3,"Yes"]
[null,"17-03-2018","10:23","DT-2053","Rural Short","Weather",null,36,3369,2.6887470000000002,7.9799999999999999E-4,"Yes"]
[null,"17-03-2018","10:23","DT-2123","Rural Short","Weather",null,26,3369,1.941873,5.7600000000000001E-4,"Yes"]
[null,"17-03-2018","10:23","DT-2147","Rural Short","Weather",null,1,3369,7.4687000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:23","DT-2214","Rural Short","Weather",null,14,3369,1.0456240000000001,3.1E-4,"Yes"]
[null,"17-03-2018","10:23","DT-2306","Rural Short","Weather",null,2,3369,0.14937500000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:23","DT-2486","Rural Short","Weather",null,60,3369,4.4812450000000004,1.33E-3,"Yes"]
[null,"17-03-2018","10:23","DT-2585","Rural Short","Weather",null,99,3369,7.3940539999999997,2.1949999999999999E-3,"Yes"]
[null,"17-03-2018","10:23","DT-2802","Rural Short","Weather",null,1414,3369,105.608007,3.1347E-2,"Yes"]
[null,"17-03-2018","10:23","DT-2957","Rural Short","Weather",null,27,3369,2.0165600000000001,5.9900000000000003E-4,"Yes"]
[null,"17-03-2018","10:23","DT-3002","Rural Short","Weather",null,4,3369,0.29875000000000002,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:23","DT-3060","Rural Short","Weather",null,1,3369,7.4687000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:23","DT-3195","Rural Short","Weather",null,16,3369,1.1949989999999999,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","10:23","DT-3263","Rural Short","Weather",null,8,3369,0.597499,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:23","DT-3342","Rural Short","Weather",null,63,3369,4.7053070000000004,1.397E-3,"Yes"]
[null,"17-03-2018","10:23","DT-3382","Rural Short","Weather",null,1,3369,7.4687000000000003E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:34","DT-1036","Urban","Weather",null,3,1776,0.16598599999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:34","DT-1049","Urban","Weather",null,26,1776,1.4385490000000001,8.0999999999999996E-4,"Yes"]
[null,"17-03-2018","10:34","DT-1050","Urban","Weather",null,11,1776,0.60861699999999996,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:34","DT-1173","Urban","Weather",null,66,1776,3.6517029999999999,2.0560000000000001E-3,"Yes"]
[null,"17-03-2018","10:34","DT-1175","Urban","Weather",null,117,1776,6.4734730000000003,3.6449999999999998E-3,"Yes"]
[null,"17-03-2018","10:34","DT-1176","Urban","Weather",null,5,1776,0.276644,1.56E-4,"Yes"]
[null,"17-03-2018","10:34","DT-1177","Urban","Weather",null,2,1776,0.11065800000000001,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:34","DT-2042","Urban","Weather",null,69,1776,3.8176890000000001,2.15E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2047","Urban","Weather",null,9,1776,0.49795899999999998,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2066","Urban","Weather",null,22,1776,1.2172339999999999,6.8499999999999995E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2141","Urban","Weather",null,3,1776,0.16598599999999999,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:34","DT-2234","Urban","Weather",null,56,1776,3.098414,1.745E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2245","Urban","Weather",null,11,1776,0.60861699999999996,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2290","Urban","Weather",null,53,1776,2.9324279999999998,1.6509999999999999E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2364","Urban","Weather",null,1,1776,5.5329000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:34","DT-2441","Urban","Weather",null,1,1776,5.5329000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:34","DT-2450","Urban","Weather",null,47,1776,2.6004550000000002,1.464E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2538","Urban","Weather",null,11,1776,0.60861699999999996,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2570","Urban","Weather",null,15,1776,0.829932,4.6700000000000002E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2609","Urban","Weather",null,43,1776,2.37914,1.34E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2635","Urban","Weather",null,18,1776,0.995919,5.6099999999999998E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2798","Urban","Weather",null,1,1776,5.5329000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:34","DT-2847","Urban","Weather",null,12,1776,0.66394600000000004,3.7399999999999998E-4,"Yes"]
[null,"17-03-2018","10:34","DT-2893","Urban","Weather",null,52,1776,2.8770989999999999,1.6199999999999999E-3,"Yes"]
[null,"17-03-2018","10:34","DT-2907","Urban","Weather",null,48,1776,2.6557840000000001,1.495E-3,"Yes"]
[null,"17-03-2018","10:34","DT-3001","Urban","Weather",null,1,1776,5.5329000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:34","DT-3013","Urban","Weather",null,5,1776,0.276644,1.56E-4,"Yes"]
[null,"17-03-2018","10:34","DT-3140","Urban","Weather",null,1,1776,5.5329000000000003E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:34","DT-3156","Urban","Weather",null,6,1776,0.33197300000000002,1.8699999999999999E-4,"Yes"]
[null,"17-03-2018","10:34","DT-3276","Urban","Weather",null,24,1776,1.3278920000000001,7.4799999999999997E-4,"Yes"]
[null,"17-03-2018","10:34","DT-3339","Urban","Weather",null,140,1776,7.7460360000000001,4.3620000000000004E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1187","Urban","Weather",null,64,2635,5.2537459999999996,1.9940000000000001E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1189","Urban","Weather",null,64,2635,5.2537459999999996,1.9940000000000001E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1190","Urban","Weather",null,100,2635,8.2089780000000001,3.1150000000000001E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1191","Urban","Weather",null,106,2635,8.7015170000000008,3.3019999999999998E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1192","Urban","Weather",null,1,2635,8.2089999999999996E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:35","DT-1193","Urban","Weather",null,100,2635,8.2089780000000001,3.1150000000000001E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1194","Urban","Weather",null,52,2635,4.268669,1.6199999999999999E-3,"Yes"]
[null,"17-03-2018","10:35","DT-1772","Urban","Weather",null,1,2635,8.2089999999999996E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:35","DT-2597","Urban","Weather",null,71,2635,5.8283750000000003,2.212E-3,"Yes"]
[null,"17-03-2018","10:35","DT-2778","Urban","Weather",null,1,2635,8.2089999999999996E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:44","DT-2064","Rural Short","Weather",null,2,3109,0.137847,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:44","DT-2086","Rural Short","Weather",null,5,3109,0.34461700000000001,1.11E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2094","Rural Short","Weather",null,5,3109,0.34461700000000001,1.11E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2095","Rural Short","Weather",null,23,3109,1.58524,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2096","Rural Short","Weather",null,23,3109,1.58524,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2097","Rural Short","Weather",null,28,3109,1.9298569999999999,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2098","Rural Short","Weather",null,22,3109,1.516316,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2170","Rural Short","Weather",null,16,3109,1.102776,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2171","Rural Short","Weather",null,13,3109,0.89600500000000005,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2172","Rural Short","Weather",null,34,3109,2.3433980000000001,7.54E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2173","Rural Short","Weather",null,30,3109,2.067704,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2174","Rural Short","Weather",null,30,3109,2.067704,6.6500000000000001E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2175","Rural Short","Weather",null,22,3109,1.516316,4.8799999999999999E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2176","Rural Short","Weather",null,35,3109,2.4123220000000001,7.76E-4,"Yes"]
[null,"17-03-2018","10:44","DT-2210","Rural Short","Weather",null,4,3109,0.27569399999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:44","DT-3254","Rural Short","Weather",null,7,3109,0.482464,1.55E-4,"Yes"]
[null,"17-03-2018","10:45","DT-1025","Rural Short","Weather",null,155,3976,13.662322,3.4359999999999998E-3,"Yes"]
[null,"17-03-2018","10:45","DT-1026","Rural Short","Weather",null,111,3976,9.7839849999999995,2.4610000000000001E-3,"Yes"]
[null,"17-03-2018","10:45","DT-1028","Rural Short","Weather",null,2,3976,0.176288,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:45","DT-1061","Rural Short","Weather",null,2,3976,0.176288,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:45","DT-1095","Rural Short","Weather",null,56,3976,4.9360650000000001,1.2409999999999999E-3,"Yes"]
[null,"17-03-2018","10:45","DT-1097","Rural Short","Weather",null,39,3976,3.4376159999999998,8.6499999999999999E-4,"Yes"]
[null,"17-03-2018","10:45","DT-1098","Rural Short","Weather",null,104,3976,9.1669769999999993,2.3059999999999999E-3,"Yes"]
[null,"17-03-2018","10:45","DT-1136","Rural Short","Weather",null,47,3976,4.1427680000000002,1.042E-3,"Yes"]
[null,"17-03-2018","10:45","DT-1883","Rural Short","Weather",null,101,3976,8.9025449999999999,2.2390000000000001E-3,"Yes"]
[null,"17-03-2018","10:45","DT-2002","Rural Short","Weather",null,108,3976,9.5195530000000002,2.3939999999999999E-3,"Yes"]
[null,"17-03-2018","10:45","DT-2124","Rural Short","Weather",null,3,3976,0.264432,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:45","DT-2237","Rural Short","Weather",null,101,3976,8.9025449999999999,2.2390000000000001E-3,"Yes"]
[null,"17-03-2018","10:45","DT-2300","Rural Short","Weather",null,1,3976,8.8144E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:53","DT-1044","Urban","Weather",null,63,3097,6.0784140000000004,1.9629999999999999E-3,"Yes"]
[null,"17-03-2018","10:53","DT-1197","Urban","Weather",null,2,3097,0.192966,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:53","DT-1198","Urban","Weather",null,2,3097,0.192966,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:53","DT-1835","Urban","Weather",null,261,3097,25.181999000000001,8.1309999999999993E-3,"Yes"]
[null,"17-03-2018","10:53","DT-2083","Urban","Weather",null,3,3097,0.28944799999999998,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:53","DT-2105","Urban","Weather",null,2,3097,0.192966,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:53","DT-2132","Urban","Weather",null,1,3097,9.6482999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:53","DT-2133","Urban","Weather",null,1,3097,9.6482999999999999E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:53","DT-2134","Urban","Weather",null,261,3097,25.181999000000001,8.1309999999999993E-3,"Yes"]
[null,"17-03-2018","10:53","DT-2228","Urban","Weather",null,261,3097,25.181999000000001,8.1309999999999993E-3,"Yes"]
[null,"17-03-2018","10:53","DT-2283","Urban","Weather",null,82,10297,26.304682,2.555E-3,"Yes"]
[null,"17-03-2018","10:53","DT-2503","Urban","Weather",null,19,3097,1.833172,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","10:53","DT-2561","Urban","Weather",null,261,3097,25.181999000000001,8.1309999999999993E-3,"Yes"]
[null,"17-03-2018","10:53","DT-2941","Urban","Weather",null,2,3097,0.192966,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:53","DT-2950","Urban","Weather",null,6,3097,0.57889699999999999,1.8699999999999999E-4,"Yes"]
[null,"17-03-2018","10:53","DT-3265","Urban","Weather",null,38,3097,3.6663450000000002,1.1839999999999999E-3,"Yes"]
[null,"17-03-2018","10:55","DT-1037","Urban","Weather",null,9,3065,0.85937300000000005,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","10:55","DT-1051","Urban","Weather",null,170,4723,25.013552000000001,5.2960000000000004E-3,"Yes"]
[null,"17-03-2018","10:55","DT-1052","Urban","Weather",null,2,3065,0.190972,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:55","DT-1178","Urban","Weather",null,29,3065,2.7690890000000001,9.0300000000000005E-4,"Yes"]
[null,"17-03-2018","10:55","DT-1764","Urban","Weather",null,9,3065,0.85937300000000005,2.7999999999999998E-4,"Yes"]
[null,"17-03-2018","10:55","DT-1986","Urban","Weather",null,44,3065,4.2013769999999999,1.371E-3,"Yes"]
[null,"17-03-2018","10:55","DT-2168","Urban","Weather",null,2,3065,0.190972,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:55","DT-2723","Urban","Weather",null,8,3065,0.76388699999999998,2.4899999999999998E-4,"Yes"]
[null,"17-03-2018","10:55","DT-2768","Urban","Weather",null,86,3065,8.2117819999999995,2.679E-3,"Yes"]
[null,"17-03-2018","10:55","DT-2842","Urban","Weather",null,1,4723,0.14713899999999999,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:55","DT-2953","Urban","Weather",null,1,3065,9.5486000000000001E-2,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:55","DT-2994","Urban","Weather",null,18,4723,2.6484939999999999,5.6099999999999998E-4,"Yes"]
[null,"17-03-2018","10:55","DT-3244","Urban","Weather",null,146,3065,13.940932999999999,4.548E-3,"Yes"]
[null,"17-03-2018","10:55","DT-3244-1","Urban","Weather",null,146,3065,13.940932999999999,4.548E-3,"Yes"]
[null,"17-03-2018","10:55","DT-3248","Urban","Weather",null,36,3065,3.4374899999999999,1.122E-3,"Yes"]
[null,"17-03-2018","10:55","DT-3248-1","Urban","Weather",null,36,3065,3.4374899999999999,1.122E-3,"Yes"]
[null,"17-03-2018","10:55","DT-3277","Urban","Weather",null,2,3065,0.190972,6.2000000000000003E-5,"Yes"]
[null,"17-03-2018","10:55","DT-3287","Urban","Weather",null,15,4723,2.2070780000000001,4.6700000000000002E-4,"Yes"]
[null,"17-03-2018","10:56","DT-1016","Urban","Weather",null,93,4204,12.180192999999999,2.8969999999999998E-3,"Yes"]
[null,"17-03-2018","10:56","DT-1017","Urban","Weather",null,61,5095,9.6823890000000006,1.9E-3,"Yes"]
[null,"17-03-2018","10:56","DT-1020","Urban","Weather",null,29,4204,3.7981250000000002,9.0300000000000005E-4,"Yes"]
[null,"17-03-2018","10:56","DT-1021","Urban","Weather",null,112,4204,14.668619,3.4889999999999999E-3,"Yes"]
[null,"17-03-2018","10:56","DT-1023","Urban","Weather",null,22,4204,2.8813360000000001,6.8499999999999995E-4,"Yes"]
[null,"17-03-2018","10:56","DT-1027","Urban","Weather",null,159,4204,20.824200000000001,4.9529999999999999E-3,"Yes"]
[null,"17-03-2018","10:56","DT-1163","Urban","Weather",null,1,4204,0.13097,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:56","DT-1179","Urban","Weather",null,11,4204,1.4406680000000001,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:56","DT-1962","Urban","Weather",null,34,4204,4.4529740000000002,1.059E-3,"Yes"]
[null,"17-03-2018","10:56","DT-1963","Urban","Weather",null,117,4204,15.323468,3.6449999999999998E-3,"Yes"]
[null,"17-03-2018","10:56","DT-2137","Urban","Weather",null,3,4204,0.39290900000000001,9.2999999999999997E-5,"Yes"]
[null,"17-03-2018","10:56","DT-2371","Urban","Weather",null,13,4204,1.7026079999999999,4.0499999999999998E-4,"Yes"]
[null,"17-03-2018","10:56","DT-2394","Urban","Weather",null,76,4204,9.9537060000000004,2.3679999999999999E-3,"Yes"]
[null,"17-03-2018","10:56","DT-2549","Urban","Weather",null,57,4204,7.4652789999999998,1.776E-3,"Yes"]
[null,"17-03-2018","10:56","DT-2550","Urban","Weather",null,48,4204,6.2865510000000002,1.495E-3,"Yes"]
[null,"17-03-2018","10:56","DT-2809","Urban","Weather",null,17,4204,2.2264870000000001,5.2999999999999998E-4,"Yes"]
[null,"17-03-2018","10:56","DT-2868","Urban","Weather",null,1,4204,0.13097,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:56","DT-2892","Urban","Weather",null,19,4204,2.488426,5.9199999999999997E-4,"Yes"]
[null,"17-03-2018","10:56","DT-2961","Urban","Weather",null,7,4204,0.91678899999999997,2.1800000000000001E-4,"Yes"]
[null,"17-03-2018","10:56","DT-2966","Urban","Weather",null,28,4204,3.6671550000000002,8.7200000000000005E-4,"Yes"]
[null,"17-03-2018","10:56","DT-2971-1","Urban","Weather",null,82,4204,10.739525,2.555E-3,"Yes"]
[null,"17-03-2018","10:56","DT-2971-2","Urban","Weather",null,82,4204,10.739525,2.555E-3,"Yes"]
[null,"17-03-2018","10:56","DT-3046","Urban","Weather",null,60,4204,7.8581890000000003,1.869E-3,"Yes"]
[null,"17-03-2018","10:56","DT-3059","Urban","Weather",null,1,4204,0.13097,3.1000000000000001E-5,"Yes"]
[null,"17-03-2018","10:56","DT-3094","Urban","Weather",null,31,4204,4.0600639999999997,9.6599999999999995E-4,"Yes"]
[null,"17-03-2018","10:56","DT-3145","Urban","Weather",null,100,4204,13.096981,3.1150000000000001E-3,"Yes"]
[null,"17-03-2018","10:56","DT-3243","Urban","Weather",null,47,4204,6.1555809999999997,1.464E-3,"Yes"]
[null,"17-03-2018","10:56","DT-3286","Urban","Weather",null,23,4204,3.0123060000000002,7.1699999999999997E-4,"Yes"]
[null,"17-03-2018","10:56","DT-3430","Urban","Weather",null,11,4204,1.4406680000000001,3.4299999999999999E-4,"Yes"]
[null,"17-03-2018","10:56","DT-3431","Urban","Weather",null,1413,5524,243.16682800000001,4.4019999999999997E-2,"Yes"]
[null,"17-03-2018","10:57","DT-10656","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-10765","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-1317","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-1318","Rural Short","Weather",null,16,3103,1.1006469999999999,3.5500000000000001E-4,"Yes"]
[null,"17-03-2018","10:57","DT-1319","Rural Short","Weather",null,13,3103,0.89427599999999996,2.8800000000000001E-4,"Yes"]
[null,"17-03-2018","10:57","DT-1320","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-1321","Rural Short","Weather",null,18,3103,1.2382280000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-1518","Rural Short","Weather",null,44,3103,3.02678,9.7499999999999996E-4,"Yes"]
[null,"17-03-2018","10:57","DT-1921","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-1957","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-1984","Rural Short","Weather",null,50,3103,3.4395229999999999,1.108E-3,"Yes"]
[null,"17-03-2018","10:57","DT-2054","Rural Short","Weather",null,18,3103,1.2382280000000001,3.9899999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2088","Rural Short","Weather",null,14,3103,0.96306599999999998,3.1E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2135","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2153","Rural Short","Weather",null,9,3103,0.61911400000000005,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2159","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2273","Rural Short","Weather",null,8,3103,0.55032400000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2284","Rural Short","Weather",null,12,3103,0.82548600000000005,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2305","Rural Short","Weather",null,10,3103,0.68790499999999999,2.22E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2308","Rural Short","Weather",null,29,3103,1.994923,6.4300000000000002E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2324","Rural Short","Weather",null,11,3103,0.75669500000000001,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2337","Rural Short","Weather",null,28,3103,1.9261330000000001,6.2100000000000002E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2348","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2452","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2480","Rural Short","Weather",null,497,3103,34.188858000000003,1.1018E-2,"Yes"]
[null,"17-03-2018","10:57","DT-2481","Rural Short","Weather",null,10,3103,0.68790499999999999,2.22E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2487","Rural Short","Weather",null,8,3103,0.55032400000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2488","Rural Short","Weather",null,8,3103,0.55032400000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2489","Rural Short","Weather",null,11,3103,0.75669500000000001,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2490","Rural Short","Weather",null,5,3103,0.34395199999999998,1.11E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2491","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2492","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2497","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2524","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2525","Rural Short","Weather",null,5,3103,0.34395199999999998,1.11E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2526","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2565","Rural Short","Weather",null,5,3103,0.34395199999999998,1.11E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2568","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2602","Rural Short","Weather",null,11,3103,0.75669500000000001,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2725","Rural Short","Weather",null,10,3103,0.68790499999999999,2.22E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2737","Rural Short","Weather",null,4,3103,0.27516200000000002,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2775","Rural Short","Weather",null,14,3103,0.96306599999999998,3.1E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2801","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2838","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2866","Rural Short","Weather",null,8,3103,0.55032400000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2939","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-2942","Rural Short","Weather",null,12,3103,0.82548600000000005,2.6600000000000001E-4,"Yes"]
[null,"17-03-2018","10:57","DT-2973","Rural Short","Weather",null,497,3103,34.188858000000003,1.1018E-2,"Yes"]
[null,"17-03-2018","10:57","DT-2974","Rural Short","Weather",null,497,3103,34.188858000000003,1.1018E-2,"Yes"]
[null,"17-03-2018","10:57","DT-3043","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3101","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3102","Rural Short","Weather",null,23,3103,1.5821810000000001,5.1000000000000004E-4,"Yes"]
[null,"17-03-2018","10:57","DT-3203","Rural Short","Weather",null,8,3103,0.55032400000000004,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-3259","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3295","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3295-2","Rural Short","Weather",null,3,3103,0.206371,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3305","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3395","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3403","Rural Short","Weather",null,497,3103,34.188858000000003,1.1018E-2,"Yes"]
[null,"17-03-2018","10:57","DT-3432","Rural Short","Weather",null,11,3103,0.75669500000000001,2.4399999999999999E-4,"Yes"]
[null,"17-03-2018","10:57","DT-3436","Rural Short","Weather",null,2,3103,0.13758100000000001,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3437","Rural Short","Weather",null,1,3103,6.8790000000000004E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","10:57","DT-3438","Rural Short","Weather",null,6,3103,0.41274300000000003,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","11:23","DT-2260","Rural Short","Weather",null,0,3101,0,0,"Yes"]
[null,"17-03-2018","11:23","DT-351","Rural Short","Weather",null,0,3101,0,0,"Yes"]
[null,"17-03-2018","11:23","DT-352","Rural Short","Weather",null,0,3101,0,0,"Yes"]
[null,"17-03-2018","11:23","DT-353","Rural Short","Weather",null,0,3101,0,0,"Yes"]
[null,"17-03-2018","13:11","DT-0141","Rural Short","Weather",null,3,4314,0.28691100000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0142","Rural Short","Weather",null,2,4314,0.191274,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0143","Rural Short","Weather",null,1,4314,9.5637E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0145","Rural Short","Weather",null,3,4314,0.28691100000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0146","Rural Short","Weather",null,3,4314,0.28691100000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0147","Rural Short","Weather",null,2,4314,0.191274,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0148","Rural Short","Weather",null,2,4314,0.191274,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0242","Rural Short","Weather",null,1,12869,0.28529300000000002,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0263","Rural Short","Weather",null,1,4314,9.5637E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0416","Rural Short","Weather",null,2,4314,0.191274,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0457","Rural Short","Weather",null,8,4314,0.76509700000000003,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","13:11","DT-0596","Rural Short","Weather",null,1,4314,9.5637E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0598","Rural Short","Weather",null,3,4314,0.28691100000000003,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","13:11","DT-0826","Rural Short","Weather",null,1,4314,9.5637E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-10035","Rural Short","Weather",null,2,4314,0.191274,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","13:11","DT-10689","Rural Short","Weather",null,38,4314,3.6342110000000001,8.4199999999999998E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0164","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0165","Rural Short","Weather",null,9,2196,0.43814799999999998,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0167","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0168","Rural Short","Weather",null,78,2196,3.7972869999999999,1.7290000000000001E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0169","Rural Short","Weather",null,79,2196,3.8459699999999999,1.751E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0170","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0171","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0318","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0348","Rural Short","Weather",null,73,2196,3.553871,1.6180000000000001E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0364","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0367","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0427","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0435","Rural Short","Weather",null,8,2196,0.38946500000000001,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0437","Rural Short","Weather",null,6,2196,0.292099,1.3300000000000001E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0438","Rural Short","Weather",null,7,2196,0.34078199999999997,1.55E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0452","Rural Short","Weather",null,4,2196,0.19473299999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0478","Rural Short","Weather",null,3,2196,0.14604900000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0479","Rural Short","Weather",null,8,2196,0.38946500000000001,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0480","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0481","Rural Short","Weather",null,4,2196,0.19473299999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0482","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0483","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0485","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0560","Rural Short","Weather",null,3,2196,0.14604900000000001,6.7000000000000002E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0612","Rural Short","Weather",null,8,2196,0.38946500000000001,1.7699999999999999E-4,"Yes"]
[null,"17-03-2018","23:20","DT-0797","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0798","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0799","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0800","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0801","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0802","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0803","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0804","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0805","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0806","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0807","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0808","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0809","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0810","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0811","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0812","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0813","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0824","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0825","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0832","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0835","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0840","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0848","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0859","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0917","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-0929","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-0948","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10018","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10024","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10030","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10092","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10128","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10144","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10153","Rural Short","Weather",null,5,2196,0.24341599999999999,1.11E-4,"Yes"]
[null,"17-03-2018","23:20","DT-10189","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10230","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10231","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10280","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10281","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10314","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10320","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10330","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10414","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10422","Rural Short","Weather",null,4,2196,0.19473299999999999,8.8999999999999995E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10423","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10424","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10496","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10497","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10514","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10541","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10565","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10566","Rural Short","Weather",null,5,2196,0.24341599999999999,1.11E-4,"Yes"]
[null,"17-03-2018","23:20","DT-10612","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10613","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10614","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10615","Rural Short","Weather",null,2,2196,9.7365999999999994E-2,4.3999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10616","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10617","Rural Short","Weather",null,394,2196,19.181165,8.7349999999999997E-3,"Yes"]
[null,"17-03-2018","23:20","DT-10645","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10679","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10686","Rural Short","Weather",null,9,2196,0.43814799999999998,2.0000000000000001E-4,"Yes"]
[null,"17-03-2018","23:20","DT-10690","Rural Short","Weather",null,7,2196,0.34078199999999997,1.55E-4,"Yes"]
[null,"17-03-2018","23:20","DT-10691","Rural Short","Weather",null,5,2196,0.24341599999999999,1.11E-4,"Yes"]
[null,"17-03-2018","23:20","DT-10692","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10722","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10726","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","23:20","DT-10786","Rural Short","Weather",null,1,2196,4.8682999999999997E-2,2.1999999999999999E-5,"Yes"]
[null,"17-03-2018","07:36","22MT06 LAKE BENNETT","Rural Short","Asset Failure","Subtransmission",257,1729,9.8508689999999994,5.6969999999999998E-3,"Yes"]
[null,"17-03-2018","08:04","22SY02 MCMINNS","Rural Short","Weather",null,1206,15,0.40103800000000001,2.6735999999999999E-2,"Yes"]
[null,"18-03-2018","19:34","NMI-25010228131","Urban","Unknown","Unknown",1,807.07,2.5142999999999999E-2,3.1000000000000001E-5,"No"]
[null,"19-03-2018","04:43","REC-10029","Rural Long","Unknown","Unknown",39,24.02,1.0778479999999999,4.4879000000000002E-2,"No"]
[null,"19-03-2018","19:35","22SY03 VIRGINIA","Rural Short","Network Business","Network Error",1244,40.85,1.1265719999999999,2.7577999999999998E-2,"No"]
[null,"20-03-2018","00:19","22SY03 VIRGINIA","Rural Short","Weather",null,1244,15.38,0.42424600000000001,2.7577999999999998E-2,"No"]
[null,"20-03-2018","11:32","DT-6860","Rural Short","Animal","Animal Impact",2,93.55,4.1479999999999998E-3,4.3999999999999999E-5,"No"]
[null,"20-03-2018","16:55","NMI-25000699739","Rural Short","Unknown","Unknown",1,26.65,5.9100000000000005E-4,2.1999999999999999E-5,"No"]
[null,"20-03-2018","18:56","22SY03 VIRGINIA","Rural Short","Weather",null,1244,469.2,12.939717999999999,2.7577999999999998E-2,"No"]
[null,"20-03-2018","19:18","NMI-25010141832","Rural Short","Vegetation","Grow-in NSP Responsibility",1,87.85,1.9480000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-03-2018","21:41","11BE13 KORMILDA","Rural Short","Network Business","Switching and Protection Error",326,1.1299999999999999,8.1910000000000004E-3,7.2269999999999999E-3,"No"]
[null,"20-03-2018","23:44","22SY03 VIRGINIA","Rural Short","Weather",null,1244,18.37,0.506521,2.7577999999999998E-2,"No"]
[null,"21-03-2018","00:04","22HD403 MIDDLE POINT","Rural Short","Weather",null,33,128.58000000000001,9.4069E-2,7.3200000000000001E-4,"No"]
[null,"21-03-2018","12:36","11BE13 KORMILDA","Rural Short","Asset Failure","HV",326,2.17,1.5658999999999999E-2,7.2269999999999999E-3,"No"]
[null,"21-03-2018","14:33","11BE04 MCMILLANS","Rural Short","Asset Failure","HV",426,4.2699999999999996,4.0294000000000003E-2,9.4439999999999993E-3,"No"]
[null,"21-03-2018","20:50","11WN03 MARRANGA","Urban","Network Business","Network Error",416,57.72,0.74800299999999997,1.2959999999999999E-2,"No"]
[null,"22-03-2018","18:21","11CA12 MARRARA","Urban","Network Business","Network Error",671,36.229999999999997,0.75742399999999999,2.0903999999999999E-2,"No"]
[null,"22-03-2018","21:36","22KA19 TINDAL 1","Rural Short","Unknown","Unknown",245,22.43,0.12184499999999999,5.4310000000000001E-3,"No"]
[null,"23-03-2018","02:59","22KA19 TINDAL 1","Rural Short","Unknown","Unknown",245,21.17,0.114965,5.4310000000000001E-3,"No"]
[null,"23-03-2018","05:21","22KA19 TINDAL 1","Rural Short","Unknown","Unknown",245,17.8,9.6679000000000001E-2,5.4310000000000001E-3,"No"]
[null,"23-03-2018","08:40","22KA19 TINDAL 1","Rural Short","Unknown","Unknown",245,118.18,0.64190199999999997,5.4310000000000001E-3,"No"]
[null,"23-03-2018","11:52","22KA19 TINDAL 1","Rural Short","Animal","Animal Impact",245,5.22,2.8334000000000002E-2,5.4310000000000001E-3,"No"]
[null,"23-03-2018","15:23","11WN02 FANNIE BAY","Urban","Network Business","Network Error",1330,42,1.7402409999999999,4.1433999999999999E-2,"No"]
[null,"24-03-2018","07:56","11CA12 MARRARA","Urban","7 - STPIS Exclusion (3.3)(a)",null,671,23.2,null,null,"No"]
[null,"24-03-2018","11:14","DT-6103","Rural Short","Unknown","Unknown",1,79.63,1.7650000000000001E-3,2.1999999999999999E-5,"No"]
[null,"24-03-2018","13:31","22SY03 VIRGINIA","Rural Short","Weather",null,1244,12.88,0.3553,2.7577999999999998E-2,"No"]
[null,"25-03-2018","11:03","NMI-25010147274","Urban","Asset Failure","LV",1,269.12,8.3840000000000008E-3,3.1000000000000001E-5,"No"]
[null,"25-03-2018","16:51","11BE16 ANULA","Rural Short","Asset Failure","HV",992,98.98,2.1768079999999999,2.1992000000000001E-2,"No"]
[null,"27-03-2018","02:51","22KA06 TINDAL 2","Rural Short","Weather",null,245,15.75,8.5544999999999996E-2,5.4310000000000001E-3,"No"]
[null,"27-03-2018","11:36","FH-6000","Rural Short","Unknown","Unknown",13,562.58000000000004,0.162135,2.8800000000000001E-4,"No"]
[null,"27-03-2018","22:52","11PA15 MOULDEN","Urban","Asset Failure","HV",1649,132.62,6.8128250000000001,5.1372000000000001E-2,"No"]
[null,"28-03-2018","06:28","11PA23 GEORGINA","Urban","Unknown","Unknown",362,15.7,0.17705799999999999,1.1278E-2,"No"]
[null,"28-03-2018","09:10","NMI-25000837924","Urban","Asset Failure","LV",1,243.15,7.5750000000000001E-3,3.1000000000000001E-5,"No"]
[null,"28-03-2018","09:27","NMI-25000684293","Rural Short","Unknown","Unknown",1,149.5,3.3140000000000001E-3,2.1999999999999999E-5,"No"]
[null,"28-03-2018","10:24","NMI-25000557846","Rural Short","Asset Failure","HV",1,117.68,2.6090000000000002E-3,2.1999999999999999E-5,"No"]
[null,"29-03-2018","06:08","DT-6943","Rural Short","Unknown","Unknown",9,57.77,1.1526E-2,2.0000000000000001E-4,"No"]
[null,"29-03-2018","10:40","NMI-25000688880","Rural Short","Asset Failure","LV",1,83.93,1.861E-3,2.1999999999999999E-5,"No"]
[null,"29-03-2018","10:42","DT-2646","Rural Short","Network Business","Network Error",8,78.819999999999993,1.3978000000000001E-2,1.7699999999999999E-4,"No"]
[null,"29-03-2018","15:30","DT-1746","Urban","Asset Failure","HV",121,61.92,0.2334,3.7699999999999999E-3,"No"]
[null,"30-03-2018","04:46","DT-6671","Rural Short","Unknown","Unknown",0,56.42,0,0,"No"]
[null,"30-03-2018","08:55","DT-0742","Rural Short","Animal","Animal Impact",8,246.03,4.3635E-2,1.7699999999999999E-4,"No"]
[null,"30-03-2018","18:51","NMI-25000161220","Rural Short","Asset Failure","LV",1,146.53,3.248E-3,2.1999999999999999E-5,"No"]
[null,"31-03-2018","04:35","REC-10029","Rural Long","Unknown","Unknown",39,8.15,0.36576500000000001,4.4879000000000002E-2,"No"]
[null,"31-03-2018","13:05","11PA15 MOULDEN","Urban","Network Business","Switching and Protection Error",1649,20.100000000000001,1.0325839999999999,5.1372000000000001E-2,"No"]
[null,"31-03-2018","14:26","DT-1626","Rural Short","Asset Failure","HV",10,50.67,1.1232000000000001E-2,2.22E-4,"No"]
[null,"31-03-2018","16:37","REC-10049","Rural Long","Unknown","Unknown",39,257.3,11.547411,4.4879000000000002E-2,"No"]
[null,"31-03-2018","18:39","NMI-25000689490","Urban","Asset Failure","LV",1,94.47,2.9429999999999999E-3,3.1000000000000001E-5,"No"]
[null,"31-03-2018","19:31","DT-1021","Urban","Asset Failure","HV",104,37.380000000000003,0.12112100000000001,3.2399999999999998E-3,"No"]
[null,"01-04-2018","11:20","22TC01 ALI CURUNG","Rural Long","Network Business","Network Error",48,2.17,0.11967800000000001,5.5236E-2,"No"]
[null,"01-04-2018","16:44","22SY11 HERBERT","Rural Short","Asset Failure","HV",1849,37.03,1.5180149999999999,4.0991E-2,"No"]
[null,"01-04-2018","20:35","22SY03 VIRGINIA","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",1244,61.68,1.701119,2.7577999999999998E-2,"No"]
[null,"01-04-2018","21:48","DT-1686","Rural Short","Asset Failure","LV",9,350.15,6.9861999999999994E-2,2.0000000000000001E-4,"No"]
[null,"03-04-2018","02:27","GCR-22RH6500","Rural Long","Unknown","Unknown",5,15.83,9.1101000000000001E-2,5.7540000000000004E-3,"No"]
[null,"03-04-2018","09:13","NMI-25020116195","Rural Short","Asset Failure","LV",1,120.63,2.6740000000000002E-3,2.1999999999999999E-5,"No"]
[null,"03-04-2018","16:21","NMI-25000783698","Rural Short","Asset Failure","LV",1,317.10000000000002,7.0299999999999998E-3,2.1999999999999999E-5,"No"]
[null,"03-04-2018","16:35","DT-0108","Rural Short","Asset Failure","HV",9,241.1,4.8105000000000002E-2,2.0000000000000001E-4,"No"]
[null,"03-04-2018","17:46","NMI-25000649841","Urban","Third Party","Other",1,107.52,3.3500000000000001E-3,3.1000000000000001E-5,"No"]
[null,"04-04-2018","21:17","DT-2080","Urban","Asset Failure","HV",1,105.03,3.2720000000000002E-3,3.1000000000000001E-5,"No"]
[null,"05-04-2018","08:57","22TC01 ALI CURUNG","Rural Long","Planned",null,48,49,null,null,"No"]
[null,"05-04-2018","09:51","22TC01 ALI CURUNG","Rural Long","Planned",null,3,36,null,null,"No"]
[null,"06-04-2018","09:55","NMI-25000786207","Rural Short","Asset Failure","LV",1,86.98,1.928E-3,2.1999999999999999E-5,"No"]
[null,"06-04-2018","12:37","DT-10024","Rural Short","Unknown","Unknown",0,221.95,0,0,"No"]
[null,"06-04-2018","18:21","22BA05 MANTON","Rural Short","Weather",null,11,15.15,3.6939999999999998E-3,2.4399999999999999E-4,"No"]
[null,"06-04-2018","23:54","NMI-25000113065","Rural Short","Asset Failure","LV",1,178.58,3.9589999999999998E-3,2.1999999999999999E-5,"No"]
[null,"07-04-2018","07:59","DT-8040","Rural Short","Animal","Animal Impact",33,47.65,3.4860000000000002E-2,7.3200000000000001E-4,"No"]
[null,"07-04-2018","08:30","DT-6122","Urban","Unknown","Unknown",1,46.85,1.4599999999999999E-3,3.1000000000000001E-5,"No"]
[null,"07-04-2018","20:18","22SY15 DARWIN RIVER","Rural Short","Weather",null,884,111.77,2.190337,1.9597E-2,"No"]
[null,"07-04-2018","23:51","NMI-25020110208","Urban","Asset Failure","LV",1,53.93,1.6800000000000001E-3,3.1000000000000001E-5,"No"]
[null,"08-04-2018","07:37","DT-8292","Urban","Planned",null,15,278.52,null,null,"No"]
[null,"08-04-2018","14:15","DT-2293","Urban","Asset Failure","LV",22,34.57,2.3691E-2,6.8499999999999995E-4,"No"]
[null,"09-04-2018","10:17","DT-6409","Rural Short","Animal","Animal Impact",0,102.82,0,0,"No"]
[null,"09-04-2018","13:09","11PA08 YARRAWONGA","Rural Short","Asset Failure","HV",447,123.3,1.221848,9.9100000000000004E-3,"No"]
[null,"09-04-2018","13:15","NMI-25000351754","Rural Long","Unknown","Unknown",1,137.16999999999999,0.15784400000000001,1.1509999999999999E-3,"No"]
[null,"09-04-2018","13:45","11PA25 PINELANDS","Urban","Asset Failure","HV",4,73.28,9.1319999999999995E-3,1.25E-4,"No"]
[null,"09-04-2018","18:10","PSPT145710","Rural Short","Third Party","Other",1,93,2.062E-3,2.1999999999999999E-5,"No"]
[null,"10-04-2018","07:54","22TC09 WARREGO","Rural Short","Planned",null,1,318,null,null,"No"]
[null,"10-04-2018","13:20","DT-6415","Rural Short","Animal","Animal Impact",1,71.22,1.5790000000000001E-3,2.1999999999999999E-5,"No"]
[null,"10-04-2018","14:09","DT-0159","Rural Short","Unknown","Unknown",2,46.83,2.0760000000000002E-3,4.3999999999999999E-5,"No"]
[null,"10-04-2018","16:22","NMI-25010215329","Urban","Asset Failure","LV",1,47.68,1.4859999999999999E-3,3.1000000000000001E-5,"No"]
[null,"10-04-2018","19:04","DT-6409","Rural Short","Animal","Animal Impact",0,38.880000000000003,0,0,"No"]
[null,"11-04-2018","09:48","DT-2492","Rural Short","Planned",null,2,172.32,null,null,"No"]
[null,"11-04-2018","11:48","DT-1800","Rural Short","Asset Failure","HV",45,140.27000000000001,0.139931,9.9799999999999997E-4,"No"]
[null,"11-04-2018","11:48","DT-1799","Rural Short","Asset Failure","HV",9,160.27000000000001,3.1976999999999998E-2,2.0000000000000001E-4,"No"]
[null,"11-04-2018","15:35","DT-1800","Rural Short","Asset Failure","HV",8,15.47,2.7430000000000002E-3,1.7699999999999999E-4,"No"]
[null,"12-04-2018","01:04","DT-1295","Rural Short","Unknown","Unknown",5,143.32,1.5886000000000001E-2,1.11E-4,"No"]
[null,"12-04-2018","11:25","NMI-25000431332","Rural Long","Vegetation","Blow-in/Fall-in NSP Responsibility",1,224.82,0.25870700000000002,1.1509999999999999E-3,"No"]
[null,"12-04-2018","11:26","DT-6124","Rural Long","Animal","Animal Impact",1,40.369999999999997,4.6452E-2,1.1509999999999999E-3,"No"]
[null,"12-04-2018","17:52","FH-6303","Rural Short","Animal","Animal Impact",0,54.92,0,0,"No"]
[null,"12-04-2018","22:40","DT-2129","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",1,43.9,9.7300000000000002E-4,2.1999999999999999E-5,"No"]
[null,"13-04-2018","07:23","DT-2250","Rural Short","Unknown","Unknown",1,50.42,1.1180000000000001E-3,2.1999999999999999E-5,"No"]
[null,"13-04-2018","10:03","DT-1001","Urban","Planned",null,2,120.3,null,null,"No"]
[null,"13-04-2018","18:09","NMI-25000886542","Rural Short","Third Party","Other",1,35.729999999999997,7.9199999999999995E-4,2.1999999999999999E-5,"No"]
[null,"14-04-2018","12:13","DT-0474","Rural Short","Unknown","Unknown",1,90.33,2.003E-3,2.1999999999999999E-5,"No"]
[null,"14-04-2018","15:08","DT-6610","Rural Short","Vegetation","Grow-in NSP Responsibility",2,93.53,4.1469999999999996E-3,4.3999999999999999E-5,"No"]
[null,"15-04-2018","08:31","DT-6260",null,"Unknown","Unknown",0,116.6,null,null,"No"]
[null,"15-04-2018","19:19","NMI-25000691960","Rural Short","Asset Failure","LV",1,94.02,2.0839999999999999E-3,2.1999999999999999E-5,"No"]
[null,"15-04-2018","20:35","DT-1297","Rural Short","Unknown","Unknown",16,155.53,5.5168000000000002E-2,3.5500000000000001E-4,"No"]
[null,"17-04-2018","09:02","DT-3380","Rural Short","Planned",null,152,345,null,null,"No"]
[null,"17-04-2018","11:04","NMI-25000647417","Rural Short","Asset Failure","LV",1,53.58,1.188E-3,2.1999999999999999E-5,"No"]
[null,"17-04-2018","18:14","DT-3004","Rural Short","Network Business","Network Error",217,57.45,0.27637299999999998,4.8110000000000002E-3,"No"]
[null,"18-04-2018","07:47","22BR101 BR-SD 1","Rural Short","Unknown","Unknown",278,15,9.2444999999999999E-2,6.1630000000000001E-3,"No"]
[null,"18-04-2018","07:47","22BR102 BOREFIELDS","Rural Short","Unknown","Unknown",8,15,2.66E-3,1.7699999999999999E-4,"No"]
[null,"18-04-2018","07:47","22BR104 HERMANNSBURG","Rural Short","Unknown","Unknown",46,15,1.5297E-2,1.0200000000000001E-3,"No"]
[null,"18-04-2018","07:47","22BR103 BR-SD 2","Rural Short","Unknown","Unknown",209,15.33,7.1043999999999996E-2,4.633E-3,"No"]
[null,"18-04-2018","09:28","REC-10033","Rural Short","Asset Failure","HV",1,28.22,6.2600000000000004E-4,2.1999999999999999E-5,"No"]
[null,"18-04-2018","09:33","DT-2133","Urban","Planned",null,1,204.33,null,null,"No"]
[null,"18-04-2018","11:11","DT-0382","Rural Short","Network Business","Network Error",5,7.12,7.8899999999999999E-4,1.11E-4,"No"]
[null,"18-04-2018","18:51","DT-3004","Rural Short","Network Business","Network Error",217,47.83,0.23011100000000001,4.8110000000000002E-3,"No"]
[null,"18-04-2018","23:04","DT-3002","Rural Short","Asset Failure","LV",3,88.28,5.8710000000000004E-3,6.7000000000000002E-5,"No"]
[null,"19-04-2018","00:10","DT-0216","Rural Short","Unknown","Unknown",1,363.1,8.0499999999999999E-3,2.1999999999999999E-5,"No"]
[null,"19-04-2018","08:40","DT-1538","Rural Short","Planned",null,10,310.27,null,null,"No"]
[null,"19-04-2018","09:00","22SY11 HERBERT","Rural Short","Planned",null,420,130.9,null,null,"No"]
[null,"19-04-2018","14:44","DT-3004","Rural Short","Network Business","Network Error",217,34.549999999999997,0.166209,4.8110000000000002E-3,"No"]
[null,"19-04-2018","16:27","NMI-25000679541","Urban","Asset Failure","LV",1,111.9,3.4859999999999999E-3,3.1000000000000001E-5,"No"]
[null,"19-04-2018","18:56","NMI-25000114162","Rural Short","Asset Failure","LV",1,129.38,2.8679999999999999E-3,2.1999999999999999E-5,"No"]
[null,"19-04-2018","22:58","DT-0216","Rural Short","Animal","Animal Impact",1,241.55,5.3550000000000004E-3,2.1999999999999999E-5,"No"]
[null,"20-04-2018","16:12","NMI-25000449480","Rural Short","Third Party","Other",1,72.42,1.6050000000000001E-3,2.1999999999999999E-5,"No"]
[null,"20-04-2018","17:13","DT-8145","Rural Short","Animal","Animal Impact",8,36.049999999999997,6.3940000000000004E-3,1.7699999999999999E-4,"No"]
[null,"21-04-2018","18:07","DT-0601","Rural Short","Unknown","Unknown",4,211.4,1.8745999999999999E-2,8.8999999999999995E-5,"No"]
[null,"21-04-2018","21:13","22MK103 CORROBOREE","Rural Short","Third Party","Vehicle impact",64,143.03,0.20293800000000001,1.4189999999999999E-3,"No"]
[null,"22-04-2018","08:32","DT-1309","Rural Short","Unknown","Unknown",1,92,2.0400000000000001E-3,2.1999999999999999E-5,"No"]
[null,"23-04-2018","05:50","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,48,13.5,null,null,"No"]
[null,"23-04-2018","08:17","DT-6045","Rural Short","Unknown","Unknown",2,75.900000000000006,3.3649999999999999E-3,4.3999999999999999E-5,"No"]
[null,"23-04-2018","10:13","DT-1665","Rural Short","Planned",null,10,135.32,null,null,"No"]
[null,"23-04-2018","11:03","NMI-25000894321","Urban","Asset Failure","LV",1,86.17,2.6840000000000002E-3,3.1000000000000001E-5,"No"]
[null,"23-04-2018","12:00","NMI-25000428261","Rural Short","Asset Failure","LV",1,137.69999999999999,3.0530000000000002E-3,2.1999999999999999E-5,"No"]
[null,"23-04-2018","23:51","FH-7116-1","Rural Long","Unknown","Unknown",7,124.98,1.0067699999999999,8.0549999999999997E-3,"No"]
[null,"24-04-2018","08:36","DT-1700","Rural Short","Planned",null,9,242.23,null,null,"No"]
[null,"24-04-2018","08:41","22TC01 ALI CURUNG","Rural Long","Planned",null,48,103.37,null,null,"No"]
[null,"24-04-2018","08:47","DT-6074","Rural Short","Planned",null,1,137.9,null,null,"No"]
[null,"25-04-2018","09:28","DT-8553","Rural Short","Animal","Animal Impact",17,44.42,1.6739E-2,3.77E-4,"No"]
[null,"25-04-2018","19:51","22TC01 ALI CURUNG","Rural Long","Unknown","Unknown",48,22.22,1.227158,5.5236E-2,"No"]
[null,"25-04-2018","19:51","22TC07 THREE WAYS","Rural Short","Unknown","Unknown",591,20.53,0.26902500000000001,1.3102000000000001E-2,"No"]
[null,"25-04-2018","19:51","22TC09 WARREGO","Rural Short","Unknown","Unknown",1,24.18,5.3600000000000002E-4,2.1999999999999999E-5,"No"]
[null,"26-04-2018","09:00","22PC308 TOWNSHIP","Rural Short","Planned",null,2,236.68,null,null,"No"]
[null,"26-04-2018","09:42","22BA04 TOWN","Rural Short","7 - STPIS Exclusion (3.3)(a)",null,347,48.63,null,null,"No"]
[null,"26-04-2018","18:04","DT-0608","Rural Short","Unknown","Unknown",2,351.47,1.5583E-2,4.3999999999999999E-5,"No"]
[null,"27-04-2018","00:15","DT-1996","Urban","Planned",null,5,144.25,null,null,"No"]
[null,"27-04-2018","00:20","REC-10029","Rural Long","Animal","Animal Impact",39,178.78,8.0236479999999997,4.4879000000000002E-2,"No"]
[null,"27-04-2018","04:22","22KA03 FLORINA","Rural Short","Unknown","Unknown",250,14.55,8.0640000000000003E-2,5.5420000000000001E-3,"No"]
[null,"27-04-2018","08:39","22TC01 ALI CURUNG","Rural Long","Planned",null,48,84.03,null,null,"No"]
[null,"27-04-2018","09:00","22BR102 BOREFIELDS","Rural Short","Planned",null,8,254.6,null,null,"No"]
[null,"27-04-2018","09:24","DT-6844","Rural Short","Overloads",null,1,105.58,2.3410000000000002E-3,2.1999999999999999E-5,"No"]
[null,"27-04-2018","14:43","DT-0677","Rural Short","Unknown","Unknown",1,383.72,8.5070000000000007E-3,2.1999999999999999E-5,"No"]
[null,"28-04-2018","09:02","DT-1736","Rural Short","Planned",null,46,212.33,null,null,"No"]
[null,"29-04-2018","05:43","DT-6943","Rural Short","Unknown","Unknown",9,55.03,1.098E-2,2.0000000000000001E-4,"No"]
[null,"29-04-2018","09:39","DT-0106","Rural Short","Unknown","Unknown",9,181.5,3.6213000000000002E-2,2.0000000000000001E-4,"No"]
[null,"30-04-2018","12:26","DT-0602","Rural Short","Unknown","Unknown",1,106.83,2.3679999999999999E-3,2.1999999999999999E-5,"No"]
[null,"30-04-2018","13:57","DT-0610","Rural Short","Unknown","Unknown",7,23.95,3.7169999999999998E-3,1.55E-4,"No"]
[null,"30-04-2018","20:47","66 BE-HC 1","N/A","Unknown","Unknown",0,88.07,null,null,"No"]
[null,"01-05-2018","07:58","DT-6844","Rural Short","Unknown","Unknown",1,246.57,5.4660000000000004E-3,2.1999999999999999E-5,"No"]
[null,"01-05-2018","09:00","DT-2400","Rural Short","Planned",null,65,255.3,null,null,"No"]
[null,"02-05-2018","00:43","REC-10032","Rural Long","Unknown","Unknown",216,120.37,29.918527000000001,0.24856200000000001,"No"]
[null,"02-05-2018","03:47","DT-6270","Rural Short","Unknown","Unknown",6,60.65,8.0669999999999995E-3,1.3300000000000001E-4,"No"]
[null,"02-05-2018","22:24","NMI-25000690095","Urban","Asset Failure","LV",1,117.3,3.6540000000000001E-3,3.1000000000000001E-5,"No"]
[null,"03-05-2018","03:27","FH-6528","Rural Short","Animal","Animal Impact",60,47.7,6.3448000000000004E-2,1.33E-3,"No"]
[null,"03-05-2018","08:30","DT-1601","Rural Short","Planned",null,10,447.75,null,null,"No"]
[null,"04-05-2018","00:18","REC-10032","Rural Long","Unknown","Unknown",216,114.03,28.344304000000001,0.24856200000000001,"No"]
[null,"04-05-2018","01:08","NMI-25000311460","Rural Short","Asset Failure","LV",1,118.83,2.6340000000000001E-3,2.1999999999999999E-5,"No"]
[null,"04-05-2018","09:40","DT-1299","Rural Short","Unknown","Unknown",2,110.95,4.9189999999999998E-3,4.3999999999999999E-5,"No"]
[null,"04-05-2018","10:24","DT-8346","Rural Short","Unknown","Unknown",1,69.87,1.549E-3,2.1999999999999999E-5,"No"]
[null,"04-05-2018","15:54","NMI-25000842149","Urban","Asset Failure","LV",1,190.8,5.9439999999999996E-3,3.1000000000000001E-5,"No"]
[null,"04-05-2018","17:54","NMI-25000471973","Rural Long","Asset Failure","LV",1,402.03,0.46263900000000002,1.1509999999999999E-3,"No"]
[null,"05-05-2018","06:58","REC-10014","Rural Short","Unknown","Unknown",2,161.1,7.143E-3,4.3999999999999999E-5,"No"]
[null,"05-05-2018","07:28","DT-6498","Rural Short","Unknown","Unknown",1,66.599999999999994,1.4760000000000001E-3,2.1999999999999999E-5,"No"]
[null,"05-05-2018","15:08","NMI-25000661491","Rural Short","Asset Failure","LV",1,91.03,2.0179999999999998E-3,2.1999999999999999E-5,"No"]
[null,"06-05-2018","04:58","66 HC-AR","N/A","Animal","Animal Impact",0,429,null,null,"No"]
[null,"06-05-2018","08:37","11BE09 JAIL","Rural Short","Planned",null,212,95.4,null,null,"No"]
[null,"06-05-2018","09:02","22RG13 BREWER 1","Rural Short","Planned",null,24,168.95,null,null,"No"]
[null,"06-05-2018","09:10","DT-2211","Rural Short","Planned",null,1,276.17,null,null,"No"]
[null,"06-05-2018","11:07","DT-2229","Urban","Planned",null,4,148.93,null,null,"No"]
[null,"07-05-2018","00:57","22PA202 HOWARD SPRINGS","Rural Short","Unknown","Unknown",989,14.95,0.32778099999999999,2.1925E-2,"No"]
[null,"07-05-2018","10:16","11CP4307 BELYUEN","Rural Short","Unknown","Unknown",1,14.62,3.2400000000000001E-4,2.1999999999999999E-5,"No"]
[null,"07-05-2018","10:32","DT-6107","Rural Short","Animal","Animal Impact",6,86.98,1.157E-2,1.3300000000000001E-4,"No"]
[null,"07-05-2018","16:35","FH-6397","Rural Short","Animal","Animal Impact",1,75.72,1.6789999999999999E-3,2.1999999999999999E-5,"No"]
[null,"07-05-2018","17:41","NMI-25000536270","Rural Short","Asset Failure","LV",1,101.77,2.2560000000000002E-3,2.1999999999999999E-5,"No"]
[null,"08-05-2018","01:46","66 LE-CA","N/A","Animal","Animal Impact",0,142.75,null,null,"No"]
[null,"08-05-2018","06:06","22KA09 PINE CREEK","Rural Short","Unknown","Unknown",116,14.13,3.6345000000000002E-2,2.5720000000000001E-3,"No"]
[null,"08-05-2018","09:31","DT-6802","Rural Long","Planned",null,1,85.33,null,null,"No"]
[null,"08-05-2018","12:46","DT-6742","Rural Short","Unknown","Unknown",1,269.12,5.9659999999999999E-3,2.1999999999999999E-5,"No"]
[null,"09-05-2018","10:32","11WB01 PARLIAMENT","CBD","Network Business","Switching and Protection Error",1,38.130000000000003,1.0251E-2,2.6899999999999998E-4,"No"]
[null,"09-05-2018","10:32","11WB02 WEST LANE","CBD","Network Business","Switching and Protection Error",73,39.520000000000003,0.77546099999999996,1.9623999999999999E-2,"No"]
[null,"09-05-2018","10:32","11WB03 BENNETT","CBD","Network Business","Switching and Protection Error",329,29.07,2.570681,8.8441000000000006E-2,"No"]
[null,"09-05-2018","10:32","11FB03 FB-WB","CBD","Network Business","Switching and Protection Error",0,38.479999999999997,0,0,"No"]
[null,"09-05-2018","11:11","DT-1400","CBD","Asset Failure","HV",9,79,0.19112899999999999,2.4190000000000001E-3,"No"]
[null,"09-05-2018","22:32","DT-1031","Urban","Asset Failure","LV",243,80.08,0.60625700000000005,7.5700000000000003E-3,"No"]
[null,"10-05-2018","08:06","DT-6939","Urban","Planned",null,49,366,null,null,"No"]
[null,"10-05-2018","08:42","DT-1600","Rural Short","Planned",null,9,291,null,null,"No"]
[null,"11-05-2018","08:36","DT-6844","Rural Short","Planned",null,1,196.2,null,null,"No"]
[null,"11-05-2018","12:55","11CA16 NAKARA","Urban","Unknown","Unknown",1462,15.32,0.69762199999999996,4.5546999999999997E-2,"No"]
[null,"11-05-2018","18:39","REC-10036","Rural Short","Third Party","Other",7,93.65,1.4533000000000001E-2,1.55E-4,"No"]
[null,"12-05-2018","11:13","DT-6891","Rural Short","Animal","Animal Impact",0,29.22,0,0,"No"]
[null,"12-05-2018","12:34","SWH-0021","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",114,664.9,1.68038,2.5270000000000002E-3,"No"]
[null,"12-05-2018","12:34","22SY02 MCMINNS","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",1206,92.1,2.4623699999999999,2.6735999999999999E-2,"No"]
[null,"13-05-2018","09:20","NMI-25000594667","Rural Short","Asset Failure","LV",1,99.78,2.212E-3,2.1999999999999999E-5,"No"]
[null,"13-05-2018","09:21","DT-1986","Urban","Planned",null,42,400.2,null,null,"No"]
[null,"13-05-2018","11:22","DT-6671","Rural Short","Unknown","Unknown",0,31.82,0,0,"No"]
[null,"13-05-2018","11:22","FH-6303","Rural Short","Unknown","Unknown",0,87.33,0,0,"No"]
[null,"14-05-2018","10:01","NMI-25000655625","Rural Long","Unknown","LV",1,102.07,0.117453,1.1509999999999999E-3,"No"]
[null,"14-05-2018","12:59","NMI-25000565394","Rural Short","Asset Failure","LV",1,129.88,2.879E-3,2.1999999999999999E-5,"No"]
[null,"14-05-2018","13:23","REC-10036","Rural Short","Unknown","Unknown",7,14.4,2.235E-3,1.55E-4,"No"]
[null,"14-05-2018","15:51","DT-10543","Rural Long","Animal","Animal Impact",2,457.88,1.053817,2.3010000000000001E-3,"No"]
[null,"15-05-2018","10:05","11WN13 GOYDER","Urban","Third Party","Other",556,37.93,0.65705899999999995,1.7321E-2,"No"]
[null,"15-05-2018","10:25","NMI-25000604518","Urban","Asset Failure","LV",1,152.72,4.7580000000000001E-3,3.1000000000000001E-5,"No"]
[null,"16-05-2018","01:27","DT-1057","Urban","7 - STPIS Exclusion (3.3)(a)",null,36,352,null,null,"No"]
[null,"16-05-2018","01:27","11WN11 BISHOP","Urban","7 - STPIS Exclusion (3.3)(a)",null,371,20.72,null,null,"No"]
[null,"16-05-2018","09:16","GCR-22HD514","Rural Short","Planned",null,0,266.32,null,null,"No"]
[null,"17-05-2018","09:19","DT-0130","Rural Short","Planned",null,17,201,null,null,"No"]
[null,"17-05-2018","09:25","22SY02 MCMINNS","Rural Short","Planned",null,88,195,null,null,"No"]
[null,"17-05-2018","14:45","NMI-25000508668","Rural Short","Asset Failure","LV",1,201.7,4.4710000000000001E-3,2.1999999999999999E-5,"No"]
[null,"17-05-2018","15:50","NMI-25000493579","Rural Short","Animal","Animal Impact",1,236.65,5.2459999999999998E-3,2.1999999999999999E-5,"No"]
[null,"18-05-2018","00:24","22KA22 KATHERINE","Urban","Planned",null,10,163,null,null,"No"]
[null,"18-05-2018","16:00","11CA16 NAKARA","Urban","7 - STPIS Exclusion (3.3)(a)",null,1462,35.979999999999997,null,null,"No"]
[null,"18-05-2018","17:53","DT-8415","Rural Short","Animal","Animal Impact",3,28.9,1.9220000000000001E-3,6.7000000000000002E-5,"No"]
[null,"18-05-2018","19:23","REC-10022","Rural Long","Animal","Animal Impact",540,198.6,123.41081699999999,0.62140399999999996,"No"]
[null,"19-05-2018","01:34","DT-6012","Urban","Planned",null,0,201.13,null,null,"No"]
[null,"19-05-2018","10:43","REC-10036","Rural Short","Vegetation","Blow-in/Fall-in NSP Responsibility",7,434.02,6.7351999999999995E-2,1.55E-4,"No"]
[null,"19-05-2018","17:50","REC-10040","Rural Short","Unknown","Unknown",12,15.58,4.1460000000000004E-3,2.6600000000000001E-4,"No"]
[null,"20-05-2018","10:27","DT-6008","Urban","Unknown","Unknown",85,95.78,0.25363999999999998,2.6480000000000002E-3,"No"]
[null,"21-05-2018","00:25","22KA22 KATHERINE","Urban","Planned",null,49,220,null,null,"No"]
[null,"21-05-2018","00:27","DT-6515","Urban","Planned",null,0,217.92,null,null,"No"]
[null,"21-05-2018","08:26","DT-8137","Rural Short","Unknown","Unknown",19,175.27,7.3824000000000001E-2,4.2099999999999999E-4,"No"]
[null,"21-05-2018","11:20","PSPT121430","Rural Short","Asset Failure","LV",1,29.22,6.4800000000000003E-4,2.1999999999999999E-5,"No"]
[null,"21-05-2018","13:53","NMI-25000373014","Rural Short","Asset Failure","LV",1,225.95,5.0090000000000004E-3,2.1999999999999999E-5,"No"]
[null,"21-05-2018","18:29","NMI-25000746085","Rural Short","Third Party","Other",1,219.12,4.8580000000000003E-3,2.1999999999999999E-5,"No"]
[null,"22-05-2018","00:01","DT-0070","Rural Short","Unknown","Unknown",14,182.62,5.6677999999999999E-2,3.1E-4,"No"]
[null,"22-05-2018","14:11","DT-10127","Rural Long","Unknown","Unknown",1,353.92,0.40726899999999999,1.1509999999999999E-3,"No"]
[null,"22-05-2018","16:32","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,48,7,null,null,"No"]
[null,"22-05-2018","16:32","22TC09 WARREGO","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,7,null,null,"No"]
[null,"23-05-2018","15:38","FH-6397","Rural Short","Unknown","Unknown",1,89.85,1.9919999999999998E-3,2.1999999999999999E-5,"No"]
[null,"23-05-2018","22:08","DT-6117","Urban","Planned",null,50,29,null,null,"No"]
[null,"24-05-2018","00:15","DT-6012","Urban","Planned",null,0,170.2,null,null,"No"]
[null,"24-05-2018","08:09","DT-2009","Urban","Planned",null,104,200.17,null,null,"No"]
[null,"24-05-2018","08:59","DT-0577","Rural Short","Network Business","Network Error",9,7.17,1.4300000000000001E-3,2.0000000000000001E-4,"No"]
[null,"24-05-2018","10:04","DT-6944","Rural Short","Network Business","Network Error",9,23.73,4.7349999999999996E-3,2.0000000000000001E-4,"No"]
[null,"24-05-2018","17:27","NMI-25010177685","Rural Short","Third Party","Other",1,42.13,9.3400000000000004E-4,2.1999999999999999E-5,"No"]
[null,"24-05-2018","17:35","22RG13 BREWER 1","Rural Short","Unknown","Unknown",374,14.17,0.11745899999999999,8.2909999999999998E-3,"No"]
[null,"25-05-2018","08:44","NMI-25000454340","Rural Short","Asset Failure","LV",1,47.58,1.0549999999999999E-3,2.1999999999999999E-5,"No"]
[null,"26-05-2018","11:07","DT-0608","Rural Short","Animal","Animal Impact",2,106.25,4.7109999999999999E-3,4.3999999999999999E-5,"No"]
[null,"27-05-2018","04:35","REC-10032","Rural Long","Vegetation","Blow-in/Fall-in NSP Responsibility",216,161.47,40.134407000000003,0.24856200000000001,"No"]
[null,"27-05-2018","07:17","DT-6284",null,"Vegetation","Blow-in/Fall-in NSP Responsibility",15,306,null,null,"No"]
[null,"27-05-2018","08:32","11BE19 HIDDEN VALLEY","Urban","Planned",null,70,296,null,null,"No"]
[null,"28-05-2018","11:28","REC-10002","Rural Short","Third Party","Other",17,3.32,1.25E-3,3.77E-4,"No"]
[null,"28-05-2018","12:13","11LG16 BRAITLING","Rural Short","Network Business","Network Error",1660,10.050000000000001,0.36984600000000001,3.6801E-2,"No"]
[null,"28-05-2018","12:24","DT-8331","Rural Short","Asset Failure","HV",5,203,2.2502000000000001E-2,1.11E-4,"No"]
[null,"28-05-2018","14:43","DT-0160","Rural Short","Unknown","Unknown",2,319.60000000000002,1.417E-2,4.3999999999999999E-5,"No"]
[null,"28-05-2018","17:24","NMI-25000599889","Urban","Third Party","Other",1,112.38,3.5010000000000002E-3,3.1000000000000001E-5,"No"]
[null,"29-05-2018","03:41","22HD403 MIDDLE POINT","Rural Short","Animal","Animal Impact",33,188.98,0.13825599999999999,7.3200000000000001E-4,"No"]
[null,"29-05-2018","10:21","DT-1765","Urban","Asset Failure","LV",6,29.25,5.4669999999999996E-3,1.8699999999999999E-4,"No"]
[null,"29-05-2018","11:30","22TC09 WARREGO","Rural Short","Planned",null,1,10.35,null,null,"No"]
[null,"29-05-2018","11:38","DT-6122","Urban","Network Business","Network Error",1,80.37,2.5040000000000001E-3,3.1000000000000001E-5,"No"]
[null,"30-05-2018","08:50","22BR103 BR-SD 2","Rural Short","Planned",null,201,151,null,null,"No"]
[null,"31-05-2018","08:41","NMI-25010238980","Urban","Network Business","Switching and Protection Error",1,138.80000000000001,4.3239999999999997E-3,3.1000000000000001E-5,"No"]
[null,"31-05-2018","09:05","22PA202 HOWARD SPRINGS","Rural Short","Planned",null,271,308.27,null,null,"No"]
[null,"31-05-2018","12:11","DT-2336","Urban","Network Business","Network Error",60,14.73,2.7539999999999999E-2,1.869E-3,"No"]
[null,"01-06-2018","16:54","DT-10038","Rural Short","Unknown","Unknown",0,106.67,0,0,"No"]
[null,"03-06-2018","09:00","22SY03 VIRGINIA","Rural Short","Planned",null,25,160.97999999999999,null,null,"No"]
[null,"03-06-2018","09:03","DT-6334","Rural Short","Unknown","Unknown",4,98.63,8.7460000000000003E-3,8.8999999999999995E-5,"No"]
[null,"03-06-2018","13:05","DT-0024","Rural Short","Unknown","Unknown",19,92.15,3.8815000000000002E-2,4.2099999999999999E-4,"No"]
[null,"03-06-2018","19:34","NMI-25000167274","Rural Short","Asset Failure","LV",1,143.38,3.179E-3,2.1999999999999999E-5,"No"]
[null,"03-06-2018","21:18","22TC09 WARREGO","Rural Short","3 - STPIS Exclusion (3.3)(a)",null,1,17.28,null,null,"No"]
[null,"03-06-2018","21:18","22TC01 ALI CURUNG","Rural Long","3 - STPIS Exclusion (3.3)(a)",null,48,15.25,null,null,"No"]
[null,"04-06-2018","08:31","NMI-25000568942","Urban","Asset Failure","LV",1,72.88,2.271E-3,3.1000000000000001E-5,"No"]
[null,"04-06-2018","11:55","66PC301 COSMO HOWLEY","Rural Short","Unknown","Unknown",5,17.95,1.99E-3,1.11E-4,"No"]
[null,"04-06-2018","17:05","REC-10048","Rural Short","Animal","Animal Impact",0,150.05000000000001,0,0,"No"]
[null,"05-06-2018","09:05","DT-0494","Rural Short","Planned",null,10,9.1300000000000008,null,null,"No"]
[null,"05-06-2018","22:00","DT-6018","Urban","Planned",null,18,365.95,null,null,"No"]
[null,"06-06-2018","09:44","11ML02 LARRAKEYAH","Urban","Planned",null,99,115.88,null,null,"No"]
[null,"07-06-2018","06:42","DT-2627","Urban","Unknown","Unknown",12,120.55,4.5067000000000003E-2,3.7399999999999998E-4,"No"]
[null,"07-06-2018","14:21","DT-8183","Rural Short","Planned",null,0,96,null,null,"No"]
[null,"08-06-2018","23:37","11WN04 BULLOCKY POINT","Urban","Asset Failure","HV",298,52.1,0.48368499999999998,9.2840000000000006E-3,"No"]
[null,"09-06-2018","05:17","DT-6333","Rural Short","Unknown","Unknown",3,93.45,6.215E-3,6.7000000000000002E-5,"No"]
[null,"09-06-2018","07:22","FH-6219","Rural Short","Unknown","Unknown",2,156.78,6.9509999999999997E-3,4.3999999999999999E-5,"No"]
[null,"09-06-2018","08:01","11WN11 BISHOP","Urban","Unknown","Unknown",371,229,2.6467800000000001,1.1558000000000001E-2,"No"]
[null,"09-06-2018","15:15","PT-10089","Rural Short","Third Party","Unauthorised Access",0,79.7,0,0,"No"]
[null,"10-06-2018","02:51","DT-6065","Urban","Animal","Animal Impact",5,57.98,9.0320000000000001E-3,1.56E-4,"No"]
[null,"10-06-2018","15:06","NMI-25000773723","Rural Short","Third Party","Other",1,74.150000000000006,1.6440000000000001E-3,2.1999999999999999E-5,"No"]
[null,"10-06-2018","16:08","DT-0608","Rural Short","Animal","Animal Impact",2,166.33,7.3749999999999996E-3,4.3999999999999999E-5,"No"]
[null,"10-06-2018","16:21","NMI-25000391750","Urban","Asset Failure","LV",1,43.5,1.3550000000000001E-3,3.1000000000000001E-5,"No"]
[null,"12-06-2018","02:25","FH-6197-2","Urban","Asset Failure","HV",1,47.33,1.475E-3,3.1000000000000001E-5,"No"]
[null,"12-06-2018","04:56","DT-0852","Rural Short","Unknown","Unknown",1,236.35,5.2399999999999999E-3,2.1999999999999999E-5,"No"]
[null,"12-06-2018","08:30","DT-1654","Rural Short","Planned",null,9,149.35,null,null,"No"]
[null,"12-06-2018","12:57","NMI-25000682792","Rural Short","Asset Failure","LV",1,131.47999999999999,2.9150000000000001E-3,2.1999999999999999E-5,"No"]
[null,"12-06-2018","16:27","DT-6742","Rural Short","Animal","Animal Impact",1,1.1000000000000001,2.4000000000000001E-5,2.1999999999999999E-5,"No"]
[null,"12-06-2018","17:35","NMI-25000548647","Rural Short","Asset Failure","LV",1,373.82,8.2869999999999992E-3,2.1999999999999999E-5,"No"]
[null,"12-06-2018","19:46","DT-2370","Rural Short","Asset Failure","LV",67,133.69999999999999,0.19858799999999999,1.485E-3,"No"]
[null,"12-06-2018","20:42","PSPT100100","Rural Short","Vegetation","Grow-in NSP Responsibility",1,224.32,4.973E-3,2.1999999999999999E-5,"No"]
[null,"13-06-2018","06:32","22KA18 GORGE","Rural Short","Unknown","Unknown",204,14.8,6.6933000000000006E-2,4.522E-3,"No"]
[null,"13-06-2018","09:46","11RG01 GAP","Rural Short","Planned",null,82,6.27,null,null,"No"]
[null,"13-06-2018","10:03","DT-10159","Rural Long","Animal","Animal Impact",2,433.27,0.99716099999999996,2.3010000000000001E-3,"No"]
[null,"14-06-2018","07:35","DT-6521","Rural Short","Animal","Animal Impact",1,93.17,2.065E-3,2.1999999999999999E-5,"No"]
[null,"14-06-2018","08:00","22KA10 MATARANKA 1","Rural Long","Planned",null,258,139.94999999999999,null,null,"No"]
[null,"14-06-2018","08:43","NMI-25000512019","Urban","Asset Failure","LV",1,65.599999999999994,2.0439999999999998E-3,3.1000000000000001E-5,"No"]
[null,"14-06-2018","09:03","DT-1947","Rural Short","Planned",null,51,257.52,null,null,"No"]
[null,"14-06-2018","16:53","DT-6610","Rural Short","Unknown","Unknown",2,45.37,2.0110000000000002E-3,4.3999999999999999E-5,"No"]
[null,"15-06-2018","03:42","22KA18 GORGE","Rural Short","Unknown","Unknown",204,16.37,7.4018E-2,4.522E-3,"No"]
[null,"15-06-2018","12:00","NMI-25000115045","Rural Short","Asset Failure","LV",1,125.1,2.7729999999999999E-3,2.1999999999999999E-5,"No"]
[null,"15-06-2018","14:04","DT-8318","Rural Short","Network Business","Network Error",61,7.5,1.0142E-2,1.3519999999999999E-3,"No"]
[null,"15-06-2018","17:43","NMI-25000402696","Urban","Asset Failure","LV",1,134.41999999999999,4.1879999999999999E-3,3.1000000000000001E-5,"No"]
[null,"17-06-2018","02:18","NMI-25020118364","Urban","Third Party","Unauthorised Access",1,41.03,1.2780000000000001E-3,3.1000000000000001E-5,"No"]
[null,"17-06-2018","09:50","NMI-25000152807","Rural Short","Asset Failure","LV",1,55.42,1.2290000000000001E-3,2.1999999999999999E-5,"No"]
[null,"18-06-2018","08:43","22PA202 HOWARD SPRINGS","Rural Short","Unknown","Unknown",989,2.42,5.2985999999999998E-2,2.1925E-2,"No"]
[null,"18-06-2018","09:11","DT-0745","Rural Short","Asset Failure","HV",1,119.27,2.6440000000000001E-3,2.1999999999999999E-5,"No"]
[null,"18-06-2018","09:26","DT-0031","Rural Short","Asset Failure","HV",22,78.58,3.8327E-2,4.8799999999999999E-4,"No"]
[null,"18-06-2018","10:10","DT-0745","Rural Short","Animal","Animal Impact",1,17.149999999999999,3.8000000000000002E-4,2.1999999999999999E-5,"No"]
[null,"19-06-2018","09:14","22PA202 HOWARD SPRINGS","Rural Short","Planned",null,271,339.17,null,null,"No"]
[null,"19-06-2018","11:45","DT-7502","Rural Long","Planned",null,1,46.25,null,null,"No"]
[null,"19-06-2018","23:13","DT-6012","Urban","Planned",null,0,164,null,null,"No"]
[null,"20-06-2018","12:25","DT-2250","Rural Short","Asset Failure","LV",1,57.23,1.2689999999999999E-3,2.1999999999999999E-5,"No"]
[null,"20-06-2018","22:30","DT-2202","Urban","Planned",null,37,227.77,null,null,"No"]
[null,"21-06-2018","09:37","DT-2653","Rural Short","Planned",null,0,193.32,null,null,"No"]
[null,"21-06-2018","10:06","DT-10188","Rural Long","Planned",null,1,107.15,null,null,"No"]
[null,"21-06-2018","12:12","22PA202 HOWARD SPRINGS","Rural Short","Network Business","Network Error",989,36.630000000000003,0.80319200000000002,2.1925E-2,"No"]
[null,"22-06-2018","08:53","DT-0160","Rural Short","Unknown","Unknown",2,89.2,3.9550000000000002E-3,4.3999999999999999E-5,"No"]
[null,"22-06-2018","09:58","DT-0931","Rural Short","Planned",null,1,61.2,null,null,"No"]
[null,"22-06-2018","12:47","11DA24 CITY VALLEY","Urban","Asset Failure","HV",1004,44.25,1.3840619999999999,3.1278E-2,"No"]
[null,"24-06-2018","08:32","DT-2444","Rural Short","Planned",null,7,186,null,null,"No"]
[null,"24-06-2018","10:03","NMI-25000157177","Rural Short","Asset Failure","LV",1,124.07,2.7499999999999998E-3,2.1999999999999999E-5,"No"]
[null,"24-06-2018","11:41","REC-10002","Rural Short","Animal","Animal Impact",17,134.47999999999999,5.0682999999999999E-2,3.77E-4,"No"]
[null,"25-06-2018","03:55","REC-10022","Rural Long","Weather",null,540,15.28,9.4971230000000002,0.62140399999999996,"No"]
[null,"25-06-2018","08:22","NMI-25000343164","Rural Short","Third Party","Other",1,40.299999999999997,8.9300000000000002E-4,2.1999999999999999E-5,"No"]
[null,"26-06-2018","08:35","DT-6669","Urban","Asset Failure","LV",70,49.55,0.108056,2.1810000000000002E-3,"No"]
[null,"26-06-2018","09:00","DT-2881","Urban","Planned",null,53,96.32,null,null,"No"]
[null,"26-06-2018","09:02","11CA12 MARRARA","Urban","Planned",null,15,315.12,null,null,"No"]
[null,"26-06-2018","09:48","DT-3254","Rural Short","Network Business","Network Error",7,9.2200000000000006,1.4300000000000001E-3,1.55E-4,"No"]
[null,"26-06-2018","10:08","DT-2094","Rural Short","Network Business","Network Error",5,6.75,7.4799999999999997E-4,1.11E-4,"No"]
[null,"26-06-2018","10:20","DT-2097","Rural Short","Network Business","Network Error",25,9.7799999999999994,5.4219999999999997E-3,5.5400000000000002E-4,"No"]
[null,"26-06-2018","10:34","DT-2098","Rural Short","Network Business","Network Error",24,7.6,4.0439999999999999E-3,5.3200000000000003E-4,"No"]
[null,"26-06-2018","10:48","DT-2173","Rural Short","Network Business","Network Error",27,10.08,6.0359999999999997E-3,5.9900000000000003E-4,"No"]
[null,"26-06-2018","11:02","DT-2170","Rural Short","Network Business","Network Error",16,8.67,3.0739999999999999E-3,3.5500000000000001E-4,"No"]
[null,"26-06-2018","11:16","DT-2172","Rural Short","Network Business","Network Error",34,9.9700000000000006,7.5119999999999996E-3,7.54E-4,"No"]
[null,"26-06-2018","11:30","DT-2171","Rural Short","Network Business","Network Error",13,9.0299999999999994,2.6029999999999998E-3,2.8800000000000001E-4,"No"]
[null,"26-06-2018","11:44","DT-2174","Rural Short","Network Business","Network Error",29,6.25,4.0179999999999999E-3,6.4300000000000002E-4,"No"]
[null,"26-06-2018","11:55","DT-2175","Rural Short","Network Business","Network Error",21,8.0299999999999994,3.7399999999999998E-3,4.66E-4,"No"]
[null,"26-06-2018","12:07","DT-2176","Rural Short","Network Business","Network Error",35,12.07,9.3629999999999998E-3,7.76E-4,"No"]
[null,"26-06-2018","12:24","DT-2210","Rural Short","Network Business","Network Error",4,8.0500000000000007,7.1400000000000001E-4,8.8999999999999995E-5,"No"]
[null,"26-06-2018","12:35","DT-2096","Rural Short","Network Business","Network Error",22,6.77,3.3E-3,4.8799999999999999E-4,"No"]
[null,"26-06-2018","14:38","DT-0042","Rural Short","Network Business","Network Error",22,29.52,1.4396000000000001E-2,4.8799999999999999E-4,"No"]
[null,"27-06-2018","05:07","NMI-25000638687","Rural Short","Asset Failure","LV",1,150.72999999999999,3.3419999999999999E-3,2.1999999999999999E-5,"No"]
[null,"27-06-2018","11:19","NMI-25000458978","Rural Short","Asset Failure","LV",1,227.18,5.0359999999999997E-3,2.1999999999999999E-5,"No"]
[null,"28-06-2018","00:26","REC-10022","Rural Long","Unknown","Unknown",540,156.93,97.518986999999996,0.62140399999999996,"No"]
[null,"28-06-2018","15:12","NMI-25000334817","Urban","Asset Failure","LV",1,120.5,3.754E-3,3.1000000000000001E-5,"No"]
[null,"29-06-2018","09:36","DT-6279","Rural Long","Asset Failure","HV",0,208.3,0,0,"No"]
[null,"30-06-2018","01:07","REC-10022","Rural Long","Unknown","Unknown",540,16.149999999999999,10.035672999999999,0.62140399999999996,"No"]
[null,"28-06-2018","00:26","REC-10022","Rural Long","Unknown","Unknown",540,156.93,97.518986999999996,0.62140399999999996,"No"]
[null,"28-06-2018","15:12","NMI-25000334817","Urban","Asset Failure","LV",1,120.5,3.754E-3,3.1000000000000001E-5,"No"]
[null,"29-06-2018","09:36","DT-6279","Rural Long","Asset Failure","HV",0,208.3,0,0,"No"]
[null,"30-06-2018","01:07","REC-10022","Rural Long","Unknown","Unknown",540,16.149999999999999,10.035672999999999,0.62140399999999996,"No"]

{"sheet":"Amendments","index":22,"n_rows":3,"n_cols":4,"rows_kept":3,"cut":false,"hidden":false,"merged":[[1,1,1,3]]}
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" resubmits this Regulatory Reporting Statement, please use this worksheet to identify amendments made to data resubmitted to the AER.\")","v":"If Power and Water resubmits this Regulatory Reporting Statement, please use this worksheet to identify amendments made to data resubmitted to the AER."}]
[null,"NSP data amendments"]
[null,"Worksheet","Table/Cell","Reason for amendment"]